{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Specifications"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Specifications","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"merged":[[1,1,1,4],[2,1,5,1],[2,2,5,2],[2,3,4,3],[2,4,4,4],[6,1,6,4],[11,1,11,4]],"flags":["formulas_cached_only"]}
[]
[null,"PLATFORM SUPPLY VESSEL "]
[null,"SPECIFICATIONS","PETROSA REQUIREMENT ","Importance of Specification","TO BE COMPLETED BY TENDERER"]
[]
[]
[]
[]
[null,"Type of vessel","Platform Supply Vessel"]
[null,"Dynamic Positioning","DP 2","Disqualitying Factor"]
[null,"Clear Wooden Deck Sace (space to be reachable by crane)"," Minimum  400 sq m free deck space","Disqualitying Factor"]
[null,"FRC/Rescue boat solas(minimum 2 off for 15 persons each) 1x DAVIT lifting arrangement)","Vessel should be equipped with :\n• Minimum 1 X 6 man  FRC's \n\n","Disqualitying Factor"]
[null,"Other requirements"]
[null,"Class","DNV + 1A1, AUTR DP ( or similar, ABS or Lloyds Register classes)","Supplier to provide information"]
[null,"IT CONNECTIVITY","Transmit and receive Word/Excell/emails","Supplier to provide information"]
[null,"SAT, RADIO COMMS","SAT C and normal marine comms, equiped with aeronautical radios for comms with chopper","Supplier to provide information"]
[null,"Deck Crane","As per vessel spec","Supplier to provide information"]
[null,"Fire fighting monitors (Minimum requirement)","2 x Fire fighting monitors with capacity to deliver water and foam to spray from vessel allowing to disperse Condensate / Light Oil and/or extinguish any burning Condensate on sea surface; Minimum 100 cubes/hour @ 70m height and to provide boundry cooling to the Platform if required","Supplier to provide information"]
[null,"Liquid Cargo discharging capacity","As per vessel spec","Supplier to provide information"]
[null,"Fire Fighting Equipment (Minimum requirement)","2 x Firewater Pumps with capacity to deliver water and foam at acceptable pressure and volume to Fire fighting monitors that will be able to disperse Condensate / Light Oil and/or extinguish any burning Condensate on sea surface; Minimum 1500 cubes/hour @+-120m height","Supplier to provide information"]
[null,"Vessel must be able to perforrm 24 hour operations during entire contractual period with sufficient number and qualified staff","Minimum safety manning requirement by flag status","Supplier to provide information"]
[null,"FUEL"," discharge rate of 30m3/h minimum","Supplier to provide information"]
[null,"WATER","Minimum 50m3/h minimum","Supplier to provide information"]
[null,"Ship owner to ensure that the crew meet the safety standard for training, certificates and watches","IMDG, safe stowing and lashing of cargo, rigging, first aid","Supplier to provide information"]
[null,"Compliance with policies and procedures","Vessels to familiarize with PetroSA offshore conditions and ensure marine,emergency,waste procedure/policies are complied with","Supplier to provide information"]
[null,"Deck crew English speaking","Key personel minimum","Supplier to provide information"]