{"text_format":"3","workbook":"xlsx","n_sheets":12,"sheets":["SANS 1200_Ps & Gs","Removal of undesirable vegetati","Segmented Paving","Earthworks","Concrete Bus Lane Repairs","Lay-bys","Fencing","Maintenance of Bus Stations","Installation of Bus Shelters","Installation of Bus Stop Signs","Raised NMT","Plant & Equipment"],"not_rendered":{"defined_names":12},"read":"whole","date_system":"1900"}

{"sheet":"SANS 1200_Ps & Gs","index":0,"n_rows":47,"n_cols":7,"rows_kept":47}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200",1,"CONTRACTOR'S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS"]
[null,"1.1","Fixed Charges"]
[null,"1.1.1","Contractual requirements: Insurance of works, and public liability","Prov Sum",1,null,"Rate Only"]
[null,"1.1.2","Site establishment: Provide and erect site offices, ablutions, fencing, signage, and temporary utilities","Prov Sum",1,null,"Rate Only"]
[null,"1.1.3.","Mobilization: Transport and setup of plant, equipment, and personnel to site","Prov Sum",1,null,"Rate Only"]
[null,"1.1.4","Demobilization: Removal of all temporary facilities and site reinstatement at completion","Prov Sum",1,null,"Rate Only"]
[]
[null,"1.2","Time-Related Charges"]
[null,"1.2.1","Supervision and administration: Site agent, foremen, and office staff","month",1,null,"Rate Only"]
[null,"1.2.2","Time-related insurances and securities: Ongoing premiums","month",1,null,"Rate Only"]
[null,"1.2.3","Security and watching: 24-hour site guarding and access control","month",1,null,"Rate Only"]
[null,"1.2.4","Community Liaison Officer (CLO): Appointment and services for community engagement, meetings, and dispute resolution.","month",1,null,"Rate Only"]
[]
[null,"1.3","Provisional Sums"]
[null,"1.3.1","Training programs: Skills development, safety induction, and labor training (including allowances for local hires).","Prov Sum",1,null,"Rate Only"]
[null,"1.3.2","Contingencies: Unforeseen time-related obligations (e.g., delays, additional CLO activities).","Prov Sum",1,null,"Rate Only"]
[]
[null,2,"DAYWORKS SCHEDULE"]
[null,"2.1","PERSONNEL"]
[null,"2.1.1","Unskilled","hr",1,null,"Rate Only"]
[null,"2.1.2","Semi-skilled","hr",1,null,"Rate Only"]
[null,"2.1.3","Skilled","hr",1,null,"Rate Only"]
[null,"2.1.4","Ganger","hr",1,null,"Rate Only"]
[null,"2.1.5","Flagmen","hr",1,null,"Rate Only"]
[null,"2.1.6","Skilled Artisan","hr",1,null,"Rate Only"]
[]
[null,"2.2","Labour outside normal working hours (a) Outside normal working hrours and Saturdays"]
[null,"2.2.1","Unskilled","hr",1,null,"Rate Only"]
[null,"2.2.2","Semi-skilled","hr",1,null,"Rate Only"]
[null,"2.2.3","Skilled","hr",1,null,"Rate Only"]
[null,"2.2.4","Ganger","hr",1,null,"Rate Only"]
[null,"2.2.5","Flagmen","hr",1,null,"Rate Only"]
[null,"2.2.6","Sundays and public hrolidays (i) Unskilled","hr",1,null,"Rate Only"]
[null,"2.2.7","Semi-skilled","hr",1,null,"Rate Only"]
[null,"2.2.8","Skilled","hr",1,null,"Rate Only"]
[null,"2.2.9","Ganger","hr",1,null,"Rate Only"]
[null,"2.2.10","Flagmen","hr",1,null,"Rate Only"]
[]
[null,3,"OCCUPATIONAL HEALTH AND SAFETY ACT"]
[null,"3.1","Health and Safety plan","Lump Sum",1,null,"Rate Only"]
[null,"3.2","Implementation of health and safety plan","month",1,null,"Rate Only"]
[null,"3.3","Preventive and/ or mitigation measures","Prov Sum",1,null,"Rate Only"]
[null,"3.4","Contractor's handling costs, profit and all other charges in respect of subitem and C1.2.6.2 above","%",{"v":0.1,"d":"10%"},null,"Rate Only"]
[]
[null,4,"ACCOMMODATION OF VEHICULAR TRAFFIC"]
[null,"4.1","Accommodation of traffic and maintaining temporary deviations (including provision of flagman and all relevent temporary signs)","month",1,null,"Rate Only"]

{"sheet":"Removal of undesirable vegetati","index":1,"n_rows":13,"n_cols":7,"rows_kept":13}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200 C",5,"REMOVAL OF UNDESIRABLE VEGETATION: PHYSICAL ERADICATION"]
[null,"5.1","Eradication of undesirable vegetation"]
[null,"5.1.1","Annual eradication Various road sections as descibed under C3.1.2.1 : Description of site Tree felling on instruction ","ha",1,null,"Rate only"]
[null,"(i)","Girth 151 mm to 500 mm","No",1,null,"Rate only"]
[null,"(ii)","Girth 501 mm to 1000 mm","No",1,null,"Rate only"]
[null,"(iii)","Girth 1 001 mm to 2000 mm","No",1,null,"Rate only"]
[null,"(iv)","Girth 2 001 mm to 4000 mm","No",1,null,"Rate only"]
[null,"(v)","Girth larger than 4000 mm","No",1,null,"Rate only"]
[null,"5.1.2","Additional eradication of undesirable vegetation on instruction of the Department of Transport Rustenburg local Municipality Project Manager/ Technician","ha",1,null,"Rate only"]
[]
[null,"5.2","COLLECTION AND REMOVAL OF DEBRIS AND LITTER"]
[null,"5.2.1","Clearing of the road reserve (a) Urban roads: Various road sections as descibed under C3.1.2.1: Description of site","month",1,null,"Rate Only"]

{"sheet":"Segmented Paving","index":2,"n_rows":11,"n_cols":7,"rows_kept":11}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200 MJ",6,"SEGMENTED PAVING"]
[null,"6.1","Concrete block paving"]
[null,"6.1.1","80mm Tan Concrete Interlocking Paver","m²",1,null,"Rate Only"]
[null,"6.1.2","60mm Tan Concrete Interlocking Paver","m²",1,null,"Rate Only"]
[null,"6.1.3","25mm bedding coarse river sand","m²",1,null,"Rate Only"]
[null,"6.1.4","Cast in-situ concrete edge and intermediate beams","m³",1,null,"Rate Only"]
[]
[null,"6.2","Provision and application of approved herbicide and ant poison"]
[null,"6.2.1","Provision of materials","prime cost sum",1,null,"Rate Only"]
[null,"6.2.2","Contractors charges and profit added to the prime cost sum","%",{"v":0.15,"d":"15%"},null,"Rate Only"]

{"sheet":"Earthworks","index":3,"n_rows":10,"n_cols":7,"rows_kept":10}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200 D",7,"Earthworks"]
[null,"7.1","Bulk excavation in soft material for foundations (up to 2 m deep, including trimming sides)","m³",1,null,"Rate Only"]
[null,"7.2","Extra over Item 1.2 for intermediate excavation (pickable but requiring mechanical aid).","m³",1,null,"Rate Only"]
[null,"7.3","Restricted excavation for strip footings (trenches <1.5 m wide; backfill not included)","m³",1,null,"Rate Only"]
[null,"7.4","Import and place G5 fill material from commercial sources, compacted in 150 mm layers to 95% Mod AASHTO density","m³",1,null,"Rate Only"]
[null,"7.5","Backfill around concrete structures with excavated material, compacted to 93% density","m³",1,null,"Rate Only"]
[null,"7.6","Disposal of surplus excavated material off-site (haul up to 5 km).","m³",1,null,"Rate Only"]
[null,"7.8","Compaction testing: Density tests at 1 per 500 m³","No.",1,null,"Rate Only"]
[null,"7.9","Dewatering excavations (provisional; pumps and sumps as needed).","Prov Sum",1,null,"Rate Only"]

{"sheet":"Concrete Bus Lane Repairs","index":4,"n_rows":12,"n_cols":7,"rows_kept":12}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200 G",8,"CONCRETE BUS LANE REPAIRS"]
[null,"8.1","Break out and remove existing damaged concrete, including disposal off-site","m³",1,null,"Rate Only"]
[null,"8.2","Repair layworks (prepare and clean surfaces for new concrete bonding)","m²",1,null,"Rate Only"]
[null,"8.3","Stabilisation of subbase (import and compact G5 material to 95% Mod AASHTO density)","m³",1,null,"Rate Only"]
[null,"8.4","Supply and apply stabilisation agent (e.g., cementitious binder for subbase)","t",1,null,"Rate Only"]
[null,"8.5","Supply and install reinforcing steel (bars/fabric per design, including bending and fixing)","kg",1,null,"Rate Only"]
[null,"8.6","Install dowels in existing sleeves (drill and grout as required for joint continuity)","No",1,null,"Rate Only"]
[null,"8.7","Cast 25 MPa concrete (structural grade, including mixing, placing, compacting, and formwork; comply with slump 70-120 mm)","m³",1,null,"Rate Only"]
[null,"8.8","Form expansion joints (including fillers and sealants)","m",1,null,"Rate Only"]
[null,"8.9","Curing of concrete (apply approved compound or ponding for min. 3-6 days based on conditions)","m²",1,null,"Rate Only"]
[null,"8.10","Testing of concrete (compressive strength samples per SANS 5863, including lab fees)","No",1,null,"Rate Only"]

{"sheet":"Lay-bys","index":5,"n_rows":13,"n_cols":7,"rows_kept":13}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200 D",10,"LAY-BYS"]
[null,"10.1","Excavation for lay-by shaping, including disposal of surplus material","m³",1,null,"Rate Only"]
[null,"10.2","Import and compact fill material to 95% Mod AASHTO density for contoured areas, ensuring no ponding","m³",1,null,"Rate Only"]
[null,"10.3","Trimming and shaping of lay-by surface (machine method), to ±150 mm tolerance with ridges on slopes","m²",1,null,"Rate Only"]
[null,"10.4","Trimming and shaping (hand method) in confined areas","m²",1,null,"Rate Only"]
[null,"10.5","Supply and spread topsoil (150 mm thick), Engineer-approved","m³",1,null,"Rate Only"]
[null,"10.6","Apply fertilizers and soil improvement agents for vegetation establishment","ha",1,null,"Rate Only"]
[null,"10.7","Grassing of lay-by verges (hydroseeding or sodding) for erosion protection","m²",1,null,"Rate Only"]
["SANS 1200 MJ; SANS 1058","10.8","Install segmented paving for lay-by surface (e.g., 80 mm interlocking blocks on sand bedding)","m²",1,null,"Rate Only"]
["SANS 2001-CC1; SANS 1200 G","10.9","Construct edge beams or kerbs for lay-by boundaries (cast in-situ concrete, 20 MPa)","m³",1,null,"Rate Only"]
["SANS 1200 DK","10.10","Provision for erosion protection (e.g., stone pitching on slopes)","m²",1,null,"Rate Only"]
[null,"10.11","Testing and quality control (e.g., compaction tests, material sampling)","Prov Sum",1,null,"Rate Only"]

{"sheet":"Fencing","index":6,"n_rows":10,"n_cols":7,"rows_kept":10}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 2001-CG1",9,"FENCING"]
[null,"9.1","Supply and install 2.4 m high ClearVu or similar high-security mesh fencing panels (e.g., 2480 mm wide), including galvanizing for corrosion resistance","No",1,null,"Rate Only"]
[null,"9.2","Supply and install fence posts (60x40 mm rectangular steel tubing, 2.7 m long for 2.4 m above ground), set in concrete","No",1,null,"Rate Only"]
[null,"9.3","Cast 25 MPa concrete bases for fence posts (e.g., 300x300x600 mm deep), including excavation and compaction","m³",1,null,"Rate Only"]
[null,"9.4","Supply and install metal fixators (security bolts and nuts for panel-to-post connection)","No",1,null,"Rate Only"]
[null,"9.5","Supply and install lockable gate (1.71 m x 1.07 m, matching ClearVu panels), including hinges and locking mechanism","No",1,null,"Rate Only"]
[null,"9.6","Apply reflective tape or warning signs to fencing for visibility (e.g., “Construction Site - No Entry”)","No",1,null,"Rate Only"]
[null,"9.7","Testing and quality control of materials (e.g., steel coating, concrete strength)","Prov Sum",1,null,"Rate Only"]
[null,"9.8","Maintenance and inspection of fencing during construction period to ensure stability and security","Lump Sum",1,null,"Rate Only"]

{"sheet":"Maintenance of Bus Stations","index":7,"n_rows":19,"n_cols":7,"rows_kept":19}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 10400-B ",11,"Maintenance of Existing Bus Stations"]
[null,"11.1","Remove existing ceiling brandering, including disposal of debris","m²",1,null,"Rate Only"]
[null,"11.2","Supply and install new ceiling brandering (timber or steel, as specified), ensuring fire resistance","m²",1,null,"Rate Only"]
[null,"11.3","Remove existing paint by hand or machine sanding on steel columns","m²",1,null,"Rate Only"]
[null,"11.4","Remove existing paint by hand or machine sanding on data bands","m²",1,null,"Rate Only"]
[null,"11.5","Apply two coats of superior quality, low sheen, washable pure acrylic emulsion paint (e.g., Plascon Daring Lime G1-A1-1) on walls","m²",1,null,"Rate Only"]
[null,"11.6","Apply two coats of superior quality, low sheen, washable pure acrylic emulsion paint (e.g., Plascon Phantom Ship 60) on concrete benches","m²",1,null,"Rate Only"]
[null,"11.7","Apply one coat water-based metal primer, one coat universal undercoat, and two coats pure gloss enamel paint (e.g., Plascon Phantom Ship 60) on steel columns","m²",1,null,"Rate Only"]
[null,"11.8","Apply one coat water-based metal primer, one coat universal undercoat, and two coats pure gloss enamel paint (e.g., Plascon Wake Up Orange O5-A1-1) on data bands","m²",1,null,"Rate Only"]
[null,"11.9","Apply one coat water-based metal primer, one coat universal undercoat, and two coats pure gloss enamel paint (e.g., Plascon Phantom Ship 60) on roof sheeting, steel beams, and rafters","m²",1,null,"Rate Only"]
[null,"11.10","Supply and install 200W LED floodlights (IP66, 220-240V), including testing for compliance","No",1,null,"Rate Only"]
[null,"11.11","Supply and install steel wire armored 3-core 4 mm² cables, including connections and testing","m",1,null,"Rate Only"]
[null,"11.12","Supply and install 1 lever 1-way switch with cover plate, including testing","No",1,null,"Rate Only"]
[null,"11.13","Supply and install 4x4 slimline socket (white, 18017/101), including testing","No",1,null,"Rate Only"]
[null,"11.14","Clean existing gutters, removing debris and obstructions","m",1,null,"Rate Only"]
[null,"11.15","Reseal gutters and treat for rust (e.g., abrasive blasting, anti-corrosion coating)","m",1,null,"Rate Only"]
[null,"11.16","Testing and quality control (e.g., paint adhesion, electrical compliance, concrete repairs)","Prov Sum",1,null,"Rate Only"]
[null,"11.17","Temporary barriers and signage during maintenance to ensure public safety","Lump Sum",1,null,"Rate Only"]

{"sheet":"Installation of Bus Shelters","index":8,"n_rows":18,"n_cols":7,"rows_kept":18}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 2001-CG1; SANS 1431; SANS 121",12,"Installation of Bus Shelters"]
[null,"12.1","Supply and install IPE section steel columns (including stub columns with chamfered edges), galvanized","kg",1,null,"Rate Only"]
[null,"12.2","Supply and install steel rafters welded to IPE columns, galvanized","kg",1,null,"Rate Only"]
[null,"12.3","Supply and install steel purlins welded between rafters, galvanized","kg",1,null,"Rate Only"]
[null,"12.4","Supply and install steel base plates welded to stub columns, galvanized","kg",1,null,"Rate Only"]
[null,"12.5","Supply and install steel brackets/cleats for tube fixation, galvanized","kg",1,null,"Rate Only"]
[null,"12.6","Supply and install 100 mm diameter steel tubes for seats, galvanized","m",1,null,"Rate Only"]
[null,"12.7","Supply and install KLIP-LOK 406 (or similar) roof sheeting (orange, 0.50 mm thick), including fixings","m²",1,null,"Rate Only"]
[null,"12.8","Supply and install galvanized steel roof fixings, per manufacturer specifications","set",1,null,"Rate Only"]
[null,"12.9","Supply and install perforated steel panels (10 mm diameter holes), galvanized or coated","m²",1,null,"Rate Only"]
[null,"12.10","Supply and install perforated steel seats welded to tubes, galvanized or coated","No",1,null,"Rate Only"]
[null,"12.11","Supply and install perforated steel fascia with flat bar surround, galvanized or coated","m",1,null,"Rate Only"]
[null,"12.12","Supply and install angle iron frame for signage panel, galvanized","No",1,null,"Rate Only"]
[null,"12.13","Supply and install map information board, compliant with SARTSM specifications","No",1,null,"Rate Only"]
[null,"12.14","Supply and install advertising board frame, galvanized","No",1,null,"Rate Only"]
[null,"12.15","Install tactile paving for accessibility to shelter entrance","m²",1,null,"Rate Only"]
[null,"12.16","Testing and quality control (e.g., concrete strength, weld quality, coating durability)","Prov Sum",1,null,"Rate Only"]

{"sheet":"Installation of Bus Stop Signs","index":9,"n_rows":11,"n_cols":7,"rows_kept":11}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 2001-CG1; SANS 1431; SANS 121",13,"Installation of Bus Stop Signs"]
[null,"13.1","Excavation for sign pole bases (300x300x320 mm deep), including disposal of surplus material","m³",1,null,"Rate Only"]
[null,"13.2","Cast 25 MPa concrete bases for sign poles (300x300x320 mm), including formwork and curing","m³",1,null,"Rate Only"]
[null,"13.3","Supply and install steel tubing poles (75x75x2 mm, 2.55 m above ground), galvanized, including base plates","No",1,null,"Rate Only"]
[null,"13.4","Supply and install steel frame for sign board, galvanized, attached to pole","No",1,null,"Rate Only"]
[null,"13.5","Supply and install Yarona Bus Stop Signs with names (double-sided, high-intensity retroreflective sheeting, per SARTSM specs)","No",1,null,"Rate Only"]
[null,"13.6","Apply reflective tape (2 bands, high-intensity grade, per SARTSM specs) to poles for visibility","No",1,null,"Rate Only"]
[null,"13.7","Labour for installation of bus stop signs, including pole erection and concrete encasement","No",1,null,"Rate Only"]
[null,"13.8","Supply and install tactile paving for accessibility at bus stop sign location","m²",1,null,"Rate Only"]
[null,"13.9","Testing and quality control (e.g., concrete strength, retroreflectivity, pole stability)","Prov Sum",1,null,"Rate Only"]

{"sheet":"Raised NMT","index":10,"n_rows":13,"n_cols":7,"rows_kept":13}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 784; SANS 10400-S ",14,"Raised NMT"]
[null,"14.1","Excavation for platform subbase (150 mm deep), including disposal of surplus material","m³",1,null,"Rate Only"]
[null,"14.2","Supply and compact 150 mm G7 subbase material from commercial source, to 95% Mod AASHTO density","m³",1,null,"Rate Only"]
[null,"14.3","Supply and compact 150 mm G5 base material from commercial source, to 95% Mod AASHTO density","m³",1,null,"Rate Only"]
[null,"14.4","Supply and spread 20 mm coarse river sand bedding for pavers","m³",1,null,"Rate Only"]
[null,"14.5","Supply and install 65 mm Onyx modular concrete paving blocks (25 MPa), laid in herringbone pattern","m²",1,null,"Rate Only"]
[null,"14.6","Supply and install warning tactile paving (e.g., precast concrete or polyurethane blister tiles, 4-5 mm domes, 30% luminance contrast) at kerb ramps and platform edges","m²",1,null,"Rate Only"]
[null,"14.7","Supply and install directional tactile paving (e.g., polyurethane or stainless steel linear bars) to guide to bus stop sign","m²",1,null,"Rate Only"]
[null,"14.8","Supply and install kerb ramps (max 1:12 slope) with 25 MPa concrete, including formwork and curing","m³",1,null,"Rate Only"]
[null,"14.9","Apply approved herbicide and ant poison to paving joints to prevent vegetation growth","Prov Sum",1,null,"Rate Only"]
[null,"14.10","Testing and quality control (e.g., paver strength, TGSI dimensions, subbase compaction)","Prov Sum",1,null,"Rate Only"]
[null,"14.11","Maintenance of tactile paving and pavers (e.g., cleaning, joint resanding, tile replacement) for 12 months","Lump Sum",1,null,"Rate Only"]

{"sheet":"Plant & Equipment","index":11,"n_rows":19,"n_cols":7,"rows_kept":19}
["SANS Reference","Item No.","Description","Unit","QTY","Rate","Amount"]
["SANS 1200 A",15,"Plant and Equipment /Construction equipment"]
[null,"15.1","TLB - Tractor, loader, backhroe (0.5m3 bucket)","hr",1,null,"Rate Only"]
[null,"15.2","Grader (CAT 140 G or similar)","hr",1,null,"Rate Only"]
[null,"15.3","Compactor (Bomag BW 90)","hr",1,null,"Rate Only"]
[null,"15.4","Dewatering pump including generators and accessories (500l/min)","hr",1,null,"Rate Only"]
[null,"15.5","Mobile concrete mixers (150l)","hr",1,null,"Rate Only"]
[null,"15.6","Centremount cranes (20ton)","hr",1,null,"Rate Only"]
[null,"15.7","Mechanical broom","hr",1,null,"Rate Only"]
[null,"15.8","Portable generator set","hr",1,null,"Rate Only"]
[null,"15.9","Tipper Trucks","hr",1,null,"Rate Only"]
[null,"15.10","3 to 5 ton capacity","hr",1,null,"Rate Only"]
[null,"15.11","More than 5 ton capacity","hr",1,null,"Rate Only"]
[null,"15.12","Suitable truck/bus for transporting labourers (40 seater)","hr",1,null,"Rate Only"]
[null,"15.13","Safety vehicle for pre-marking purposes","hr",1,null,"Rate Only"]
[null,"15.14","Compressor (air) including hoses and tools (up to 10m3/min)","hr",1,null,"Rate Only"]
[null,"15.15","Water truck (5 000 litre)","hr",1,null,"Rate Only"]
[null,"15.16","Flat bed truck (6 ton)","hr",1,null,"Rate Only"]
[null,"15.17","Light delivery vehicle (LDV)","hr",1,null,"Rate Only"]