{"text_format":"3","workbook":"xlsx","n_sheets":20,"sheets":["AllDays","Bakgoma","Burgersfort","Fetakgomo","Ga-Phaahla","Giyani","Groblersdal","Lebowakgomo","Mapodile","Marapong","Marblehall","Mogwadi","Moletjie","Mookgophong","Morebeng","Mutale","Phatantswane","Phokwane","Seshego","Vhembe"],"read":"whole","date_system":"1900"}

{"sheet":"AllDays","index":0,"n_rows":32,"n_cols":3,"rows_kept":32,"merged":[[0,0,0,2],[2,0,2,2],[16,0,16,2],[27,0,27,2]]}
["ALL DAYS Library"]
["Product Name /Model /Description","DOQ ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",20]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",20]
["45deg ADAPTER PLATE for COMPACT ","EACH",20]
["TRUNKING FRAME 50 x 50 ","EACH",20]
["25 X 50 BLANK ","EACH",20]
["New Electrical Normal Power Point complete. ","EACH",30]
["Power Skirting 2 Compartment Supply & Install ","P/M",60]
["Brash Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",2]
["Triple output kettle cord PC power cable ","EACH",20]
["Extra Flyleads ","EACH",15]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Electrical 2 Pin 5 A Power outlet ","EACH",8]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",22]
["UTP Labelling ","EACH",84]
["Power Plugs Testing, Fixing and Labelling ","EACH",17]
["Relocate wall mounted cabinet with all equipment inside to New Server room (includes power, Patch panels, Brash panels, UPS, Surge protector and Air Conditioner.) ","P/H",2]
["Convert Red Power Plugs to Normal Power Plugs ","EACH",5]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",2]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
[]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Bakgoma","index":1,"n_rows":28,"n_cols":3,"rows_kept":28,"merged":[[0,0,0,2],[2,0,2,2],[15,0,15,2],[23,0,23,2]]}
["BAKGOMA Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",5]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Electrical 2 Pin 5 A Power outlet ","EACH",5]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",38]
["UTP Labelling ","EACH",94]
["Existing Cabling to be Maintained","EACH",54]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",2]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Burgersfort","index":2,"n_rows":49,"n_cols":4,"rows_kept":49,"merged":[[11,0,11,3],[25,0,25,3]]}
["Item","Description","DOQ","QTY"]
[null,"Limpopo LSAC: BURGERSFORT LIBRARY"]
[1,"Test & Repair / replace flash mount and surface mount wall boxes","EACH",45]
[2,"1 Meter Cat 5e / 6 Patch Lead","EACH",45]
[3,"CAT 6 Surface mount Data Point complete with 3m fly lead and patch lead for WiFi AP, WIFI/APS Connectors","EACH",1]
[4,"yt2 Surface mount trunking","P/M","9m"]
[5,"Switch 24 PORT POE","EACH",1]
[6,"Internal Ceiling mount access point","EACH",1]
[7,"BRUSH PANEL SHORT BASE METAL","EACH",2]
[8,"24 PORT PATCH PANEL CAT 6e LOADED","EACH",2]
[9,"Smart-UPS, 2000 Watts /3 KVA, Input 230V /Output 230V, Interface Port USB, Rack mounted","EACH",1]
["2. OFFICE 51"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead","EACH",10]
[{"$f":"A13+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER","EACH",10]
[{"$f":"A14+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP","EACH",10]
[{"$f":"A15+1","v":4},"Cover Plate P/O 50x50 E/O","EACH",10]
[{"$f":"A16+1","v":5},"Collar 50x50","EACH",10]
[{"$f":"A17+1","v":6},"Euromod Half Blank White","EACH",10]
[7,"Electrical Normal Power Point  complete, excl CB.","EACH",6]
[8,"Electrical Dedicated Power Point  complete, excl CB.","EACH",6]
[9,"Cover 2 X 4 Vert White 16 Amp","EACH",6]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2","EACH",6]
[11,"Plugtop 16 Amp Red","EACH",6]
[12,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","P/M","100m"]
[13,"Power Pole all including Core, Ceiling Flange, Floor location pad, Jack & Assembly","EACH",1]
["2. OFFICE 52"]
[1,"Krone UTP CAT6 Data Point complete with 3m flylead and patchlead","EACH",10]
[{"$f":"A27+1","v":2},"ADAPTER 22.5 X 45 LEGRAND HK SHUTTER","EACH",10]
[{"$f":"A28+1","v":3},"KEYSTONE RJ45 KM8 C6 WHITE STP","EACH",10]
[{"$f":"A29+1","v":4},"Cover Plate P/O 50x50 E/O","EACH",10]
[{"$f":"A30+1","v":5},"Collar 50x50","EACH",10]
[{"$f":"A31+1","v":6},"Euromod Half Blank White","EACH",10]
[7,"Electrical Normal Power Point  complete, excl CB.","EACH",6]
[8,"Electrical Dedicated Power Point  complete, excl CB.","EACH",6]
[9,"Cover 2 X 4 Vert White 16 Amp","EACH",6]
[10,"Cover Socket 2 X 4 Vert Red Ded 16 Amp For MS2","EACH",6]
[11,"Plugtop 16 Amp Red","EACH",6]
[12,"Cable Surfex 2.5 X 2 Core + Earth Dedicated plugs & normal plugs","P/M","100m"]
[13,"Power Pole all including Core, Ceiling Flange, Floor location pad, Jack & Assembly","EACH",1]
[null,"SUNDRIES/ Infrasrtucture"]
[{"$f":"A40+1","v":1},"Tape Brother White 9mm / BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE","EACH",4]
[2,"BRADY \"0\" - \"9\" 37/STRIP BLACK/WHITE","EACH",2]
[{"$f":"A42+1","v":3},"Insulation Tape - Black","EACH",2]
[4,"Silicone","EACH",1]
[null,"Documentation"]
[1,"UTP Test Results (ALL LAN POINTS)","EACH",1]
[{"$f":"A46+1","v":2},"Manufacturer Data Point Certification ","EACH",1]
[3,"COC - Electrical Certification ","EACH",1]
[4,"Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Fetakgomo","index":3,"n_rows":31,"n_cols":3,"rows_kept":31,"merged":[[0,0,0,2],[2,0,2,2],[12,0,12,2],[18,0,18,2],[26,0,26,2]]}
["FETAKGOMO  Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m length)","P/M",10]
["Sundries and Consumables "]
["Brush Panel ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",68]
["UTP Labelling ","EACH",136]
["Power Plugs Testing, Fixing and Labelling ","EACH",52]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V","EACH",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Ga-Phaahla","index":4,"n_rows":30,"n_cols":3,"rows_kept":30,"merged":[[0,0,0,2],[2,0,2,2],[17,0,17,2],[25,0,25,2]]}
["GA-PHAAHLA Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",2]
["Electrical 2 Pin 5 A Power outlet ","EACH",2]
["Power Skirting 2 Compartment Supply & Install (2,4 / 3.0m) lenght","P/M",12]
["Sundries and Consumables ",null,1]
["Brush Panel ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
["Existing Cabling to be Maintained"]
["TP Testing and Fixing ","EACH",62]
["UTP Labelling ","EACH",124]
["Power Plugs Testing, Fixing and Labelling ","EACH",78]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Giyani","index":5,"n_rows":33,"n_cols":3,"rows_kept":33,"merged":[[0,0,0,2],[2,0,2,2],[17,0,17,2],[28,0,28,2]]}
["Giyani Public Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patch lead","EACH",34]
["New 45deg ADAPTER PLATE for COMPACT ","EACH",34]
["New RJ 45 WHITE SHUTTER CAT 6 ","EACH",34]
["New TRUNKING FRAME 50 X 50 ","EACH",34]
["New UTP Labelling ","EACH",68]
["New Electrical Dedicated Power Point complete, excl CB ","EACH",34]
["New Electrical 2 Pin 5 A Power outlet. ","EACH",15]
["Wire, Electrical, Surfex, 2.5 Mm2 ","EACH",1]
["New Electrical Normal Power Point complete ","EACH",34]
["15a Standard Plug top ","EACH",34]
["5-way PSU for cabinet ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Brush Panel ","EACH",2]
["New 25 X 50 BLANK ","EACH",34]
["Existing Cabling to be Maintained"]
["Move/Re-route Existing UTP Points to New Cabinet ","EACH",24]
["UTP Testing and Labelling ","EACH",24]
["15a Dedicated Plug top ","EACH",34]
["Power Plugs Testing and fixing ","EACH",48]
["Power Skirting 2 compartment ","EACH",4]
["Cabinet Cleaning and Cable tying ","P/H",1]
["Testing and repair/or Replacement of 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","P/H",1]
["Testing and repair/or replacement of 230 APC Smart-UPS XL 2200VA RM 3U 230V ","P/H",1]
["Cabinet Cleaning and Cable tying","P/H",1]
["3 Year On call Site Warranty, Maintenance and Support for the service rendered"]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Groblersdal","index":6,"n_rows":31,"n_cols":3,"rows_kept":31,"merged":[[0,0,0,2],[2,0,2,2],[10,0,10,2],[20,0,20,2],[26,0,26,2]]}
["GROBLERSDAL Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",31]
["UTP Labelling ","EACH",82]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Power Plugs Testing, Fixing and Labelling ","EACH",46]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["Testing and/or Replacement of 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Service and repair LG air conditioner","P/H",1]
["OTHERS"]
["Brush Panel ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
[]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Lebowakgomo","index":7,"n_rows":32,"n_cols":3,"rows_kept":32,"merged":[[0,0,0,2],[2,0,2,2],[12,0,12,2],[18,0,18,2],[27,0,27,2]]}
["LEBOWAKGOMO Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",5]
["Electrical 2 Pin 5 A Power outlet ","EACH",2]
["Power Skirting 2 Compartment Supply & Install 2,4m or 3m lenght0","P/M",12]
["Sundries and Consumables "]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",15]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",67]
["UTP Labelling ","EACH",134]
["Power Plugs Testing, Fixing and Labelling ","EACH",68]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying","P/H",1]
[]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Mapodile","index":8,"n_rows":35,"n_cols":3,"rows_kept":35,"merged":[[0,0,0,2],[2,0,2,2],[17,0,17,2],[30,0,30,2]]}
["MAPODILE  Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m or 3m lrnght)","EACH",4]
["Sundries and Consumables ",null,1]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",15]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
[]
["Existing Cabling to be Maintained"]
[" Electrical Normal Power Point complete. ","EACH",53]
["Electrical Dedicated Power Point complete ","EACH",20]
["Electrical 2 Pin 5 A Power outlet ","EACH",8]
["UTP Testing and Fixing ","EACH",35]
["UTP Labelling ","EACH",90]
["Power Plugs Testing, Fixing and Labelling ","P/H",4]
["Convert Red Power Plugs to Normal Power Plugs ","EACH",10]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",2]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying","P/H",1]
["Service of 1200 BTU air conditioner ","P/H",2]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Marapong","index":9,"n_rows":31,"n_cols":3,"rows_kept":31,"merged":[[0,0,0,2],[2,0,2,2],[9,0,9,2],[17,0,17,2],[26,0,26,2]]}
["MARAPONG Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["Sundries and Consumables "]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",5]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Electrical 2 Pin 5 A Power outlet ","EACH",5]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",38]
["UTP Labelling ","EACH",76]
["Power Plugs Testing, Fixing and Labelling ","P/H",3]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
[]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Marblehall","index":10,"n_rows":32,"n_cols":3,"rows_kept":32,"merged":[[0,0,0,2],[2,0,2,2],[11,0,11,2],[20,0,20,2],[27,0,27,2]]}
["MARBLE-HALL  Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",50]
["UTP Labelling ","EACH",120]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Power Plugs Testing, Fixing and Labelling ","EACH",48]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["Testing and/or Replacement of 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["OTHERS"]
["Power Skirting 2 Compartment Supply & Install ","P/M",60]
["Sundries and Consumables ",null,1]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",2]
["Triple output kettle cord PC power cable ","EACH",20]
["Extra Flyleads ","EACH",15]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Mogwadi","index":11,"n_rows":31,"n_cols":3,"rows_kept":31,"merged":[[0,0,0,2],[2,0,2,2],[10,0,10,2],[17,0,17,2],[26,0,26,2]]}
["Mogwadi Library"]
["PRODUCT NAME/ MODEL ","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",20]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",20]
["45deg ADAPTER PLATE for COMPACT ","EACH",20]
["TRUNKING FRAME 50 x 50 ","EACH",20]
["25 X 50 BLANK ","EACH",30]
["New Electrical Normal Power Point complete. ","EACH",30]
["Power Skirting 2 Compartment Supply & Install ","P/M",60]
["Sundries and Consumables "]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",2]
["Triple output kettle cord PC power cable ","EACH",20]
["Extra Flyleads ","EACH",15]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",25]
["UTP Labelling ","EACH",45]
["Power Plugs Testing, Fixing and Labelling ","EACH",41]
["Convert Red Power Plugs to Normal Power Plugs ","EACH",7]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit, Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Moletjie","index":12,"n_rows":30,"n_cols":3,"rows_kept":30,"merged":[[0,0,0,2],[2,0,2,2],[11,0,11,2],[17,0,17,2],[25,0,25,2]]}
["Moletjie Library"]
["PRODUCT NAME/ MODEL ","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete. ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m / 3,0 m length)","P/M",12]
["Sundries and Consumables "]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
["Electrical 2 Pin 5 A Power outlet ","EACH",2]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",32]
["UTP Labelling ","EACH",84]
["Power Plugs Testing, Fixing and Labelling ","EACH",35]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit, Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Mookgophong","index":13,"n_rows":31,"n_cols":3,"rows_kept":31,"merged":[[0,0,0,2],[2,0,2,2],[11,0,11,2],[17,0,17,2],[26,0,26,2]]}
["MOOKGOPHONG  Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m / 3,0m length)","P/M",12]
["Sundries and Consumables "]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",15]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",70]
["UTP Labelling ","EACH",160]
["Power Plugs Testing, Fixing and Labelling ","EACH",50]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
[]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Morebeng","index":14,"n_rows":30,"n_cols":3,"rows_kept":30,"merged":[[0,0,0,2],[2,0,2,2],[14,0,14,2],[25,0,25,2]]}
["Morebeng Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m / 3,0 m length)","P/M",12]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
["Existing Cabling to be Maintained"]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["UTP Testing and Fixing ","EACH",37]
["UTP Labelling ","EACH",94]
["Power Plugs Testing, Fixing and Labelling ","EACH",32]
["Sundries and Consumables ",null,1]
["Brush Panel ","EACH",2]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Mutale","index":15,"n_rows":29,"n_cols":3,"rows_kept":29,"merged":[[0,0,0,2],[2,0,2,2],[14,0,14,2],[24,0,24,2]]}
[" MUTALE LIBRARY"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["New RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["New 45deg ADAPTER PLATE for COMPACT ","EACH",10]
["New TRUNKING FRAME 50 x 50 ","EACH",10]
["New 25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m / 3,0m length)","P/M",12]
["Sundries and Consumables ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Brush Panel ","EACH",2]
["Existing Cabling to be Maintained"]
["Convert Red Power Plugs to Normal Power Plugs ","EACH",18]
["UTP Testing and Fixing ","EACH",64]
["UTP Labelling ","EACH",148]
["Power Plugs Testing and Fixing ","EACH",128]
["Relocate 27U Floor standing cabinet with all equipment inside to New Server room (includes power, Patch panels, Brash panels, UPS, Surge protector, Air Conditioner, UTP and power cabling.)","P/H",3]
["Relocate 1 x network point at Audio Visual room. ","P/H",1]
["Testing and repair/or Replacement of 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V","P/H",1]
["Testing and repair/or replacement of 230 APC Smart-UPS XL 2200VA RM 3U 230V ","P/H",1]
["Cabinet Cleaning and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Phatantswane","index":16,"n_rows":30,"n_cols":3,"rows_kept":30,"merged":[[0,0,0,2],[2,0,2,2],[11,0,11,2],[16,0,16,2],[25,0,25,2]]}
["PHATANTSWANE Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["ew insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m /3,0m length)","P/M",12]
["Sundries and Consumables "]
["Brush Panel ","EACH",2]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",26]
["UTP Labelling ","EACH",72]
["Power Plugs Testing, Fixing and Labelling ","EACH",63]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Phokwane","index":17,"n_rows":35,"n_cols":3,"rows_kept":35,"merged":[[0,0,0,2],[2,0,2,2],[11,0,11,2],[17,0,17,2],[30,0,30,2]]}
["PHOKWANE Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",0]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["25 X 50 BLANK ","EACH",10]
["New Electrical Normal Power Point complete. ","EACH",10]
["New Electrical Dedicated Power Point complete ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m / 3,0m length)","P/M",12]
["Sundries and Consumables "]
["Brush Panel ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Flyleads ","EACH",10]
[]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",70]
["UTP Labelling ","EACH",140]
["Power Plugs Testing, Fixing and Labelling ",null,61]
["Relocate 27U Floor standing cabinet with all equipment inside to New Server room (includes power, Patch panels, Brash panels, UPS, Surge protector.) ","P/H",3]
["Relocate 1 x network point at Audio Visual room. ","P/H",1]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Add 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["Service of 1200 BTU air conditioner ","P/H",2]
[]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Seshego","index":18,"n_rows":27,"n_cols":3,"rows_kept":27,"merged":[[0,0,0,2],[2,0,2,2],[12,0,12,2],[22,0,22,2]]}
["SESHEGO  Library"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patchlead ","EACH",10]
["RJ 45 WHITE SHUTTER CAT 6e ","EACH",10]
["Power Skirting 2 Compartment Supply & Install (2,4m / 3,0m length)","P/M",12]
["Brush Panel ","EACH",1]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Triple output kettle cord PC power cable ","EACH",10]
["Extra Fly-leads ","EACH",10]
["45deg ADAPTER PLATE for COMPACT ","EACH",10]
["TRUNKING FRAME 50 x 50 ","EACH",10]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",51]
["UTP Labelling ","EACH",122]
["Electrical Normal Power Point complete. ","EACH",30]
["Electrical 2 Pin 5 A Power outlet ","EACH",10]
["Power Plugs Testing, Fixing and Labelling ","EACH",80]
["Cabinet Cleaning, mounting existing switches, modems and Cable tying ","P/H",1]
["Testing and/or Replacement of 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V ","P/H",1]
["Supply and installation of 4000VA UPS or Repair 230 APC Smart-UPS XL 2200VA RM 3U 230V ","EACH",1]
["Testing, Repair and /or replacement of cabinet Fan and cabinet power plugs","P/H"]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]

{"sheet":"Vhembe","index":19,"n_rows":32,"n_cols":3,"rows_kept":32,"merged":[[0,0,0,2],[2,0,2,2],[17,0,17,2],[27,0,27,2]]}
["VHEMBE DISTRICT LIBRARY"]
["Product Name /Model /Description","DOQ","QTY"]
["New Installations"]
["New insulation-displacement connector UTP CAT6e Data Point complete with flylead and patch lead ","EACH",10]
["New 45deg ADAPTER PLATE for COMPACT ","EACH",10]
["New RJ 45 WHITE SHUTTER CAT 6 ","EACH",10]
["New TRUNKING FRAME 50 X 50 ","EACH",10]
["New Electrical Dedicated Power Point complete, excl CB ","EACH",10]
["New 15a Dedicated Plug top ","EACH",10]
["New Wire, Electrical, Surfex, 2.5 Mm2 p/meter","EACH",100]
["New Electrical Normal Power Point complete ","EACH",10]
["15a Standard Plug top ","EACH",10]
["Power Skirting (2,4m / 3,0m length)","P/M",12]
["INSULATION-DISPLACEMENT CONNECTOR 24 PORT KM8 CAT 6e LOADED ","EACH",1]
["Brush Panel","EACH",2]
["Sundries and Consumables","EACH",1]
["New 25 X 50 BLANK ","EACH",10]
["Existing Cabling to be Maintained"]
["UTP Testing and Fixing ","EACH",26]
["UTP Labelling ","EACH",72]
["Convert Red Power Plugs to Normal Power Plugs ","EACH",25]
["Power Plugs Testing and fixing ","EACH",58]
["Test/Repair/Replace Cooling 18000 BTU air-conditioner including installation ","P/H",3]
["Cabinet Cleaning and Cable tying ","P/H",1]
["Testing and repair/or Replacement of 2U Electrical Surge & Lighting Protection / Complete System for One V11/X.21 Interface / Unit Includes Equipment AC Power Surge Protector (Phase 3), AC Feed Power Trip-Switch & 15A Feed Socket for Cabinet, Optical Isolation Barrier & Surge Protection on V","P/H",1]
["Testing and repair/or replacement of 230 APC Smart-UPS XL 2200VA RM 3U 230V ","P/H",1]
["Electrical 2 Pin 5 A Power outlet. ","EACH",15]
["DOCUMENTATION"]
["UTP Test Results (ALL LAN POINTS)","EACH",1]
["Manufacturer Data Point Certification ","EACH",1]
["COC - Electrical Certification ","EACH",1]
["Schematic Layout Of Network (4 PRINTOUTS)","EACH",4]