{"text_format":"3","workbook":"xlsx","n_sheets":8,"sheets":["Washers","Nuts","Bolts","Absorbents","Cloth&Cable ties","Welding electrodes","Filters","Rods"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Washers","index":0,"n_rows":156,"n_cols":6,"rows_kept":156}
["Material","Text","Unit","Quantity","Price","Total"]
["0001151","WASHER, FLAT: NOMINAL SIZE: M12; INSIDE DIAMETER: 6 MM; OUTER SIZE: 12 MM; THICKNESS: 0.8 MM; MATERIAL: BRASS; 0BA NOMINAL SIZE","EA",166,null,{"$f":"D2*E2","v":0}]
["0034497","WASHER: TYPE: MAIN STEAM CONTROL VALVE","EA",50,null,{"$f":"D3*E3","v":0}]
["0087519","WASHER, LOCK: INSIDE DIAMETER: 24.8 MM; OUTSIDE DIAMETER: 35.7 MM; THICKNESS: 4.8 MM; NOMINAL SIZE: M24; MATERIAL: SPRING STL; TYPE: HELICAL SPRING; GRADE 4.6","EA",50,null,0]
["0087531","WASHER, FLAT: NOMINAL SIZE: 2BA; INSIDE DIAMETER: 5 MM; OUTER SIZE: 10 MM; THICKNESS: 0.75 MM; MATERIAL: BRASS; PERIPHERAL SHAPE STYLE: RD","EA",50,null,0]
["0087533","WASHER, FLAT: NOMINAL SIZE: 4BA; INSIDE DIAMETER: 4 MM; OUTER SIZE: 9 MM; THICKNESS: 1 MM; MATERIAL: BRASS; PERIPHERAL SHAPE STYLE: RD","EA",70,null,0]
["0087685","WASHER, FLAT: NOMINAL SIZE: M30; INSIDE DIAMETER: 33 MM; OUTER SIZE: 57 MM; THICKNESS: 4 MM; MATERIAL: MS BLACK","KG",250,null,0]
["0089164","WASHER, FLAT: NOMINAL SIZE: M12; INSIDE DIAMETER: 13 MM; OUTER SIZE: 30 MM; THICKNESS: 3 MM; MATERIAL: DIN 6796; SUPPL P/N: EC/12/TW; CONSISTING OF ONE TRAN AND TWO WASHERS PER SET","EA",50,null,0]
["0089546","WASHER, LOCK: TYPE: KEY; FLUID/DRIVE SCOOP","EA",50,null,0]
["0089590","WASHER, FLAT: NOMINAL SIZE: M33; BR","EA",50,null,0]
["0089603","WASHER, FLAT: NOMINAL SIZE: M16; INSIDE DIAMETER: 17 MM; OUTER SIZE: 38.6 MM; THICKNESS: 3.4 MM; MATERIAL: STL; REFERENCE NO: ST HD 609-2-14","EA",50,null,0]
["0089615","WASHER, LOCK: INSIDE DIAMETER: 61 MM; OUTSIDE DIAMETER: 86 MM; THICKNESS: 1.5 MM; NOMINAL SIZE: 60 MM; MATERIAL: STL; TYPE: INTERNAL TOOTH; GRADE: HT; SPECIFICATION: ISO 9001; SUPPL P/N: MB12; TYPE SKF ONLY","EA",50,null,0]
["0089647","WASHER: TYPE: GUIDE; SUPPL P/N: UMC 508","EA",50,null,0]
["0089648","WASHER: INSIDE DIAMETER: 52 IN; COUP 1-2IN TAB","EA",50,null,0]
["0089649","WASHER, TAB: INSIDE DIAMETER: 3 IN; OUTSIDE DIAMETER: 8 IN","EA",50,null,0]
["0089665","WASHER, LOCK: INSIDE DIAMETER: 13 MM; SUPPL P/N: 002; IT A41","EA",50,null,0]
["0089666","WASHER, LOCK: SUPPL P/N: F15","EA",50,null,0]
["0089670","WASHER, THRUST: INSIDE DIAMETER: 100 MM; THICKNESS: 2.31 MM; REFERENCE NO: DU 7L; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0089677","WASHER, LOCK: TYPE: SPRING; REFERENCE NO: 039","EA",50,null,0]
["0089678","WASHER, THRUST: 45-3 NB PART 115; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0089679","WASHER, THRUST: 45-3 N4B PART 11; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0089680","WASHER: TYPE: INSULATING; INSIDE DIAMETER: 10 MM; OUTSIDE DIAMETER: 20 MM; MATERIAL: TUFNOL","EA",50,null,0]
["0089681","WASHER, LOCK: THICKNESS: 5 MM; NOMINAL SIZE: 13 MM; TCHER L/MO","EA",50,null,0]
["0089682","WASHER: TYPE: CONICAL; SUPPL P/N: D3C-D5C","EA",50,null,0]
["0089693","WASHER, TAB: TYPE: BELLVILLE","EA",50,null,0]
["0089715","WASHER, LOCK: SUPPL P/N: 869010-2900","EA",50,null,0]
["0089725","WASHER, LOCK: (SETS)ITEM 119-121","EA",50,null,0]
["0089943","WASHER: TYPE: PIN CAP, MONO PUMP; INSIDE DIAMETER: 10 MM; OUTSIDE DIAMETER: 20 MM; THICKNESS: 2 MM; MATERIAL: STL; SUPPL P/N: 1150603103; 3100; REFERENCE NO: 1150603101","EA",50,null,0]
["0091833","WASHER, FLAT: INSIDE DIAMETER: 15 MM; OUTER SIZE: 28 MM; THICKNESS: 5 MM","EA",50,null,0]
["0091834","WASHER, FLAT: INSIDE DIAMETER: 15 MM; OUTER SIZE: 20 MM","EA",50,null,0]
["0091835","WASHER, FLAT: INSIDE DIAMETER: 12 MM; OUTER SIZE: 28 MM; THICKNESS: 5 MM","EA",50,null,0]
["0091836","WASHER, FLAT: STEAM CONT TURBINE","EA",50,null,0]
["0091837","WASHER, FLAT: NOMINAL SIZE: M10; TURBINE","EA",50,null,0]
["0091839","WASHER, LOCK: INSIDE DIAMETER: 11 MM","EA",50,null,0]
["0091842","WASHER, LOCK: KSB OIL PUMP","EA",50,null,0]
["0091844","WASHER: INSIDE DIAMETER: 19 MM; OUTSIDE DIAMETER: 38.5 MM; THICKNESS: 3.25 MM","EA",50,null,0]
["0091846","WASHER: TYPE: H2 PLANT BB TENSION; INSIDE DIAMETER: 1 IN","EA",50,null,0]
["0091847","WASHER, FLAT: NOMINAL SIZE: 1 IN; H2 PLANT BB GEE","EA",50,null,0]
["0091855","WASHER, TAB: STE DRAINAGE PUMP","EA",50,null,0]
["0091860","WASHER, LOCK: INSIDE DIAMETER: 13 MM; OUTSIDE DIAMETER: 35 MM; THICKNESS: 1.5 MM; NOMINAL SIZE: 12 MM; MATERIAL: STL; TYPE: BELLEVILLE; GRADE: HT; SPECIFICATION: ISO 9001; SUPPL P/N: 44-76; MODEL NO: HPT32-25-4STG","EA",50,null,0]
["0091861","WASHER: INSIDE DIAMETER: 7/8 IN; OUTSIDE DIAMETER: 1-3/4 IN; THICKNESS: 3/16 IN; MATERIAL: BRASS","EA",50,null,0]
["0094581","WASHER, SEALING: INSIDE DIAMETER: 21 MM; OUTSIDE DIAMETER: 31 MM; THICKNESS: 4 MM; MATERIAL: RUBBER","EA",50,null,0]
["0094593","WASHER, SEALING: INSIDE DIAMETER: 47 MM; OUTSIDE DIAMETER: 60 MM; THICKNESS: 9.5 MM; MATERIAL: RUBBER","EA",50,null,0]
["0101818","WASHER, SEALING: INSIDE DIAMETER: 50 MM; OUTSIDE DIAMETER: 90 MM; THICKNESS: 5 MM; MATERIAL: RUBBER","EA",50,null,0]
["0102247","WASHER, FLAT: MATERIAL: RUBBER; HC25352","EA",50,null,0]
["0102248","WASHER, FLAT: MATERIAL: RUBBER; HC28462","EA",50,null,0]
["0102249","WASHER, FLAT: MATERIAL: RUBBER; ADS400112","EA",50,null,0]
["0102250","WASHER, FLAT: MATERIAL: RUBBER; HC86721 41M","EA",50,null,0]
["0102252","WASHER: TYPE: DOMED; INSIDE DIAMETER: 3/4 IN; REFERENCE NO: HCP16611","EA",50,null,0]
["0102335","WASHER: INSIDE DIAMETER: 38 MM; OUTSIDE DIAMETER: 75 MM; MATERIAL: KLINGERIT","EA",50,null,0]
["0102347","WASHER: TYPE: JOINT; SUPPL P/N: 22616","EA",50,null,0]
["0102361","WASHER, SEALING: MANUF P/N: 825050; FLYGHT MODEL B 2050 PUMP","EA",50,null,0]
["0113411","WASHER, SEALING: USIT RING; FOR OIL DRAIN PLUG PART NO. 97 FOR A SIEMENS TYPE3AC - ANS/1250-350/ 13.8 6.6 KV O.C.B","EA",50,null,0]
["0225473","WASHER, FLAT: NOMINAL SIZE: M20; INSIDE DIAMETER: 21 MM; OUTER SIZE: 32 MM; THICKNESS: 2 MM; MATERIAL: MS; GRADE: 4.6; SPECIFICATION: SABS 135","EA",500,null,0]
["0225474","WASHER, LOCK: INSIDE DIAMETER: 21 MM; OUTSIDE DIAMETER: 28 MM; THICKNESS: 3 MM; NOMINAL SIZE: M20; MATERIAL: STL; TYPE: SPRING; SPECIFICATION: SABS 135","EA",50,null,0]
["0225475","WASHER, FLAT: NOMINAL SIZE: M24; INSIDE DIAMETER: 25 MM; OUTER SIZE: 38 MM; THICKNESS: 2 MM; MATERIAL: STL; GRADE: 4.6; SPECIFICATION: SABS 135","EA",50,null,0]
["0230008","WASHER, SEALING: DRAWING NO: IM.19 REV 1; REFERENCE NO: 16; FOR USE ON BURNER GUN ASSEMBLY SEAL","EA",60,null,0]
["0230009","WASHER, SEALING: DRAWING NO: IM.19 REV 1; REFERENCE NO: 18; FOR USE ON BURNER GUN ASSEMBLY SEAL","EA",80,null,0]
["0230175","WASHER, FLAT: INSIDE DIAMETER: 8 MM; OUTER SIZE: 16 MM; THICKNESS: 1 MM; MATERIAL: MS; FOR MAINTENANCE","EA",50,null,0]
["0230384","WASHER: TYPE: COMPRESSION; DRAWING NO: 40/81033/2103 REV 1; FOR USE ON 8.5E BALL MILL","EA",61,null,0]
["0231333","WASHER, LOCK: TYPE: SOOTBLOWER; SUPPL P/N: 869016-2900","EA",50,null,0]
["0231335","WASHER, LOCK: TYPE: SOOTBLOWER; SUPPL P/N: 901098-0005","EA",50,null,0]
["0231767","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 869006-2900","EA",50,null,0]
["0231779","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 327882-1123","EA",50,null,0]
["0231781","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 869068-0012","EA",50,null,0]
["0231785","WASHER, LOCK: TYPE: SOOTBLOWER; SUPPL P/N: 869016-3200","EA",50,null,0]
["0231789","WASHER, LOCK: NOMINAL SIZE: 3/8 IN; TYPE: SPRING SPLIT; SUPPL P/N: 869016-2700; FOR USE ON SOOTBLOWER","EA",50,null,{"$f":"D67*E67","v":0}]
["0231791","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 869068-0013","EA",50,null,0]
["0231806","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 879005-5600","EA",50,null,0]
["0231825","WASHER: TYPE: SOOTBLOWER; MATERIAL: CORK; SUPPL P/N: 390799-0117","EA",50,null,0]
["0231922","WASHER: TYPE: VALVE GUIDE; SUPPL P/N: 301167-2114; FOR USE ON SOOTBLOWER","EA",50,null,0]
["0231924","WASHER: TYPE: PACKING; SUPPL P/N: 302027-0116; FOR USE ON SOOTBLOWER","EA",50,null,0]
["0231947","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 869011-2700; FOR AUXILIARY SUPPORT ASSEMBLY","EA",50,null,0]
["0231948","WASHER: TYPE: SOOTBLOWER; SUPPL P/N: 869068-0026; FOR AUXILIARY SUPPORT ASSEMBLY","EA",50,null,0]
["0231968","WASHER, LOCK: TYPE: SOOTBLOWER; SUPPL P/N: 869016-2600; FOR ITEM 111 LANCE DRIVE ASSEMBLY","EA",50,null,0]
["0233043","WASHER, FLAT: INSIDE DIAMETER: 1-1/2 IN; GRADE: 8.8; REFERENCE NO: 1700; FOR USE ON BOILER 2 MILL; STANDARD","EA",190,null,0]
["0233063","WASHER, LOCK: INSIDE DIAMETER: 5/8 IN; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",50,null,0]
["0233064","WASHER, LOCK: INSIDE DIAMETER: 3/4 IN; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",70,null,0]
["0233065","WASHER, LOCK: INSIDE DIAMETER: 1/2 IN; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER MILL","EA",50,null,0]
["0233066","WASHER, LOCK: INSIDE DIAMETER: 1 IN; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",70,null,0]
["0233067","WASHER, LOCK: INSIDE DIAMETER: 2 IN; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER MILL","EA",50,null,0]
["0233069","WASHER, LOCK: INSIDE DIAMETER: 20 MM; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",200,null,0]
["0233070","WASHER, LOCK: INSIDE DIAMETER: 30 MM; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",50,null,0]
["0233071","WASHER, LOCK: INSIDE DIAMETER: 24 MM; TYPE: SPRING; GRADE: 8.8; CAT NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",70,null,0]
["0233072","WASHER, LOCK: INSIDE DIAMETER: 12 MM; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",50,null,0]
["0233073","WASHER, LOCK: INSIDE DIAMETER: 10 MM; TYPE: SPRING; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",80,null,0]
["0233074","WASHER, FLAT: INSIDE DIAMETER: 5/8 IN; REFERENCE NO: 1700; FOR USE ON BOILER 2 MILL; SANS, GRADE 8.8","EA",50,null,0]
["0233075","WASHER, FLAT: INSIDE DIAMETER: 3/4 IN; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",60,null,0]
["0233076","WASHER, FLAT: INSIDE DIAMETER: 1/2 IN; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER MILL","EA",50,null,0]
["0233077","WASHER, FLAT: INSIDE DIAMETER: 1 IN; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",100,null,0]
["0233078","WASHER, FLAT: INSIDE DIAMETER: 1-1/2 IN; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER MILL","EA",50,null,0]
["0233079","WASHER, FLAT: INSIDE DIAMETER: 1 IN; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",1200,null,0]
["0233080","WASHER, FLAT: INSIDE DIAMETER: 30 MM; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",70,null,0]
["0233081","WASHER, FLAT: INSIDE DIAMETER: 2 IN; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER MILL","EA",50,null,0]
["0233082","WASHER, FLAT: INSIDE DIAMETER: 16 MM; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",1700,null,0]
["0233083","WASHER, FLAT: INSIDE DIAMETER: 12 MM; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",1500,null,0]
["0233084","WASHER, FLAT: INSIDE DIAMETER: 10 MM; GRADE: 8.8; REFERENCE NO: SANS 1700; FOR USE ON BOILER 2 MILL","EA",320,null,0]
["0233143","WASHER, LOCK: INSIDE DIAMETER: 1-1/2 IN; TYPE: SPRING; REFERENCE NO: 1700; FOR USE ON BOILER 2 MILL; SANS; GRADE: 8.8","EA",50,null,0]
["0233619","WASHER, SEALING: NOMINAL SIZE: 15 MM; INSIDE DIAMETER: 16 MM; OUTSIDE DIAMETER: 20 MM; THICKNESS: 1.6 MM; MATERIAL: CU; FOR USE ON BOILER MILL REFURBISHMENT","EA",50,null,0]
["0233622","WASHER, FLAT: NOMINAL SIZE: 5.6 MM; INSIDE DIAMETER: 6.6 MM; OUTER SIZE: 12.4 MM; THICKNESS: 2 MM; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE; BLACK CUT","EA",160,null,0]
["0233623","WASHER, LOCK: INSIDE DIAMETER: 6.5 MM; OUTSIDE DIAMETER: 9.9 MM; THICKNESS: 1.6 MM; NOMINAL SIZE: 5.5 MM; MATERIAL: MS; TYPE: SPRING; GRADE: 4.6; FOR MAINTENANCE USE; SHAPE SQUARE","EA",50,null,0]
["0233628","WASHER, FLAT: INSIDE DIAMETER: 10 MM; MATERIAL: MS; GRADE: 4; FOR MAINTENANCE USE; BLACK CUT; ( 11.3 X 20.5 X 2 )","EA",350,null,0]
["0233629","WASHER, LOCK: INSIDE DIAMETER: 10.4 MM; OUTSIDE DIAMETER: 16 MM; THICKNESS: 2.5 MM; NOMINAL SIZE: 9.4 MM; MATERIAL: MS; TYPE: SPRING; GRADE: 4.6; FOR MAINTENANCE USE; SHAPE SQUARE","EA",150,null,0]
["0233635","WASHER, FLAT: NOMINAL SIZE: 11.4 MM; INSIDE DIAMETER: 12.4 MM; OUTER SIZE: 18 MM; THICKNESS: 2.5 MM; MATERIAL: MS; FOR MAINTENANCE USE; SHAPE SQUARE","EA",50,null,0]
["0233636","WASHER, FLAT: NOMINAL SIZE: 17 MM; INSIDE DIAMETER: 18 MM; OUTER SIZE: 29.9 MM; THICKNESS: 3 MM; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE; BLACK CUT","EA",930,null,0]
["0233637","WASHER, LOCK: INSIDE DIAMETER: 16.6; OUTSIDE DIAMETER: 24.4 MM; THICKNESS: 3.5 MM; NOMINAL SIZE: 15.6 MM; MATERIAL: MS; TYPE: SPRING; GRADE: 4.6; FOR MAINTENANCE USE; SHAPE SQUARE","EA",330,null,0]
["0233644","WASHER, FLAT: NOMINAL SIZE: 17 MM; INSIDE DIAMETER: 18 MM; OUTER SIZE: 29.9 MM; THICKNESS: 3 MM; MATERIAL: MS; GRADE: 8.8; FOR MAINTENANCE USE; BLACK CUT","EA",120,null,0]
["0233647","WASHER, LOCK: INSIDE DIAMETER: 10.4 MM; OUTSIDE DIAMETER: 16 MM; THICKNESS: 2.5 MM; NOMINAL SIZE: 9.4 MM; MATERIAL: MS; TYPE: SPRING; FOR MAINTENANCE USE; SHAPE SQUARE; GRADE: 8.8","EA",50,null,0]
["0233653","WASHER, FLAT: NOMINAL SIZE: 12.8 MM; INSIDE DIAMETER: 13.8 MM; OUTER SIZE: 23.7 MM; THICKNESS: 2 MM; MATERIAL: MS; FOR MAINTENANCE USE; BLACK CUT, GRADE 4.6","EA",50,null,0]
["0233673","WASHER, FLAT: INSIDE DIAMETER: 20 MM; MATERIAL: MS; GRADE: 4; FOR MAINTENANCE USE; BLACK CUT","EA",50,null,0]
["0233674","WASHER, LOCK: INSIDE DIAMETER: 20 MM; MATERIAL: MS; TYPE: SPRING; GRADE: 4; FOR MAINTENANCE USE; SHAPE SQUARE","EA",50,null,0]
["0233679","WASHER, FLAT: INSIDE DIAMETER: 24 MM; MATERIAL: MS; GRADE: 4; FOR MAINTENANCE USE; SHAPE SQUARE","EA",150,null,0]
["0233680","WASHER: INSIDE DIAMETER: 24 MM; MATERIAL: MS; GRADE: 4; FOR MAINTENANCE USE, BLACK CUT","EA",50,null,0]
["0234933","WASHER, FLAT: NOMINAL SIZE: 1-1/2 IN; INSIDE DIAMETER: 1-9/16 IN; OUTER SIZE: 3-1/2 IN; THICKNESS: 3/16 IN; MATERIAL: MS; DRAWING NO: FC 407 REV 1; REFERENCE NO: KA 308; FOR ASH HOPPER DOORS, UNITS 1, 2, 3, 4 AND 6; AS PER DRAWING","EA",68,null,0]
["0240322","WASHER: TYPE: CONTROL VALVE HP; INSIDE DIAMETER: 10.5 MM; OEM P/N: 5121-061, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51200-0017/ 061 REV 1; FOR HP CONTROL VALVE DV 2 - 6, UNITS 1 - 4","EA",50,null,0]
["0247950","WASHER, THRUST: MATERIAL: STL; REQUIRED FOR USE ON ID FANS, BOILERS 1, 5 AND 6, 9-1/2 IN SIROCCO RING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0249585","WASHER, FLAT: NOMINAL SIZE: M16; INSIDE DIAMETER: 17 MM; OUTER SIZE: 30 MM; THICKNESS: 3 MM; MATERIAL: STL; SUPPL P/N: 0607-1; BUFFALO B520 RFL RECLAIM FE EDER","EA",50,null,0]
["0250737","WASHER: NOMINAL SIZE: 1 IN; OUTSIDE DIAMETER: 2 IN; MATERIAL: MS; DRAWING NO: FB7869/47-411A REV 1; REQUIRED FOR USE ON HOPKINSON SOOTBLOWER ROLLER S, UNITS 2, 3 & 4; HOIST","EA",70,null,0]
["0251182","WASHER, SEALING: NOMINAL SIZE: 1/8 IN; INSIDE DIAMETER: 7 MM; OUTSIDE DIAMETER: 14 MM; THICKNESS: 2 MM; MATERIAL: MS PASSIVATED; GRADE: 4.6; DRAWING NO: IM23 REV 1; REQUIRED FOR USE ON OIL BLOCK AT BURNERS, UNITS 1 - 6","EA",50,null,0]
["0251193","WASHER, SEALING: NOMINAL SIZE: 1/2 IN; INSIDE DIAMETER: 21 MM; OUTSIDE DIAMETER: 28.5 MM; THICKNESS: 3 MM; MATERIAL: MS PASSIVATED; GRADE: 4.6; DRAWING NO: IM23 REV 1; REQUIRED FOR USE ON OIL BLOCK, BURNERS UNITS 1 - 6","EA",50,null,0]
["0252387","WASHER: INSIDE DIAMETER: 25/32 IN; OUTSIDE DIAMETER: 1-1/2 IN; THICKNESS: 1/8 IN; MATERIAL: MS; GRADE: 4.6; SUPPL P/N: DN190L; REQUIRED FOR USE AT A SH HOPPER, UNIT 1, 2, 3, 4 & 6","EA",50,null,0]
["0501371","WASHER: TYPE: CUP; NOMINAL SIZE: M16; INSIDE DIAMETER: 18 MM; OUTSIDE DIAMETER: 39 MM; THICKNESS: 4.2 MM; MATERIAL: MILD CARBON STEEL; SPECIFICATION: DIN6796; FOR USE IN TRANSFORMER HIGH VOLTAGE BUSHING","EA",100,null,0]
["0501372","WASHER: TYPE: CUP; NOMINAL SIZE: M12; INSIDE DIAMETER: 13 MM; OUTSIDE DIAMETER: 29 MM; THICKNESS: 3 MM; MATERIAL: BRASS; SPECIFICATION: DIN6796; FOR USE ON EXCITATION LINKS","EA",800,null,0]
["0555647","WASHER, TAB: TYPE: TAB LOCKING; OEM P/N: 2490-007, OEM: GE STEAM POWER SERVICE; DRAWING NO: SZ 50001464 REV 0; FOR USE ON HP TURBINE CENTRELINE; NOZZLE BOX ASSEMBLY SPARES FOR UNIT'S 1-6; AS PER OEM DRAWING","EA",50,null,0]
["0630832","WASHER: TYPE: RETAINING; INSIDE DIAMETER: 9.5 MM; OUTSIDE DIAMETER: 25.5 MM; THICKNESS: 10.8 MM; MATERIAL: ALLOY STEEL; GRADE: 24CRMO5; OEM P/N: 2480-042, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24800-0065; REFERENCE NO: SZ50003461","EA",50,null,0]
["0630851","WASHER: TYPE: INSERT SPHERICAL; NOMINAL SIZE: 15 MM; INSIDE DIAMETER: 3 MM; OUTSIDE DIAMETER: 15 MM; THICKNESS: 10.4 MM; MATERIAL: STL ALLOY; OEM P/N: 3750-904, OEM: GE STEAM POWER SERVICE; REFERENCE NO: SZT-42-24901-00014","EA",50,null,0]
["0632271","WASHER, SPHERICAL MALE: NOMINAL SIZE: 100 MM; INSIDE DIAMETER: 20 MM; OUTER SIZE: 100 MM; THICKNESS: 35 MM; MATERIAL: STL ALLOY; OEM P/N: SZT-42-24101-00033; DRAWING NO: 2410/007 REV 0","EA",50,null,0]
["0632273","WASHER, SPHERICAL MALE: NOMINAL SIZE: 52 MM; INSIDE DIAMETER: 13 MM; OUTER SIZE: 52 MM; THICKNESS: 27.9 MM; MATERIAL: STL ALLOY; OEM P/N: SZT-42-51201-00002; DRAWING NO: 2410/025 REV 0","EA",50,null,0]
["0632279","WASHER, SPHERICAL MALE: NOMINAL SIZE: 33 MM; INSIDE DIAMETER: 10 MM; OUTER SIZE: 33 MM; THICKNESS: 19.5 MM; MATERIAL: STL ALLOY; OEM P/N: SZT-42-26801-00004; DRAWING NO: 2410/038 REV 0","EA",50,null,0]
["0632280","WASHER, LOCK: INSIDE DIAMETER: 13 MM; OUTSIDE DIAMETER: 30 MM; THICKNESS: 1.2 MM; NOMINAL SIZE: 13 MM; MATERIAL: STL ALLOY; TYPE: LOCKING; OEM P/N: SZ50001465; DRAWING NO: 2450/019 REV 0","EA",50,null,0]
["0639910","WASHER: TYPE: BEARING; INSIDE DIAMETER: 1-1/2 IN; OUTSIDE DIAMETER: 3-1/4 IN; THICKNESS: 5 MM; MATERIAL: MILD STEEL; SPECIFICATION: HOPKINSONS 7020; SPECIFICATION: Y30042003","EA",50,null,{"$f":"D131*E131","v":0}]
["0715559","WASHER, FLAT: NOMINAL SIZE: M16; INSIDE DIAMETER: 16 MM; OUTER SIZE: 34 MM; THICKNESS: 2,5 MM; MATERIAL: COPPER; PERIPHERAL SHAPE STYLE: ROUND; SPECIFICATION: TW 1/5; REFERENCE NO: BS2874 CZ121; TRANSITION WASHER: CORROROSION RESISTANT COPPER ALLOY, SURFACE PERNETRATING, GREASE PROTECTED TRANSITION WASHER.","EA",1400,null,0]
["0723220","WASHER, LOCK: INSIDE DIAMETER: 5.1 MM; OUTSIDE DIAMETER: 8.8 MM; THICKNESS: 1.6 MM; NOMINAL SIZE: M5; MATERIAL: STEEL; TYPE: SPRING; OEM P/N: 5161-343, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51600-0187; REFERENCE NO: SZ50002701; FOR HP CONTROL CV SERVOMOTOR","EA",50,null,0]
["0723221","WASHER, LOCK: INSIDE DIAMETER: 6.1 MM; OUTSIDE DIAMETER: 9.9 MM; THICKNESS: 2 MM; NOMINAL SIZE: M6; MATERIAL: STEEL; TYPE: SPRING; OEM P/N: 5161-344, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51600-0187; REFERENCE NO: SZ50001506; FOR HP CONTROL CV SERVOMOTOR","EA",50,null,0]
["0723222","WASHER, LOCK: INSIDE DIAMETER: 10.2 MM; OUTSIDE DIAMETER: 16 MM; THICKNESS: 2.5 MM; NOMINAL SIZE: M10; MATERIAL: STEEL; TYPE: SPRING; OEM P/N: 5161-346, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51600-0187; REFERENCE NO: SZ50001508; FOR HP CONTROL CV SERVOMOTOR","EA",50,null,0]
["0723223","WASHER, LOCK: INSIDE DIAMETER: 12.2 MM; OUTSIDE DIAMETER: 18 MM; THICKNESS: 2.5 MM; NOMINAL SIZE: M12; MATERIAL: STEEL; TYPE: SPRING; OEM P/N: 5161-347, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51600-0187; REFERENCE NO: SZ50001509; FOR HP CONTROL CV SERVOMOTOR","EA",50,null,0]
["0737745","WASHER, LOCK: INSIDE DIAMETER: 9.5 MM; OUTSIDE DIAMETER: 25.5  MM; THICKNESS: 10.8 MM; NOMINAL SIZE: 25.5 MM; MATERIAL: STEEL ALLOY; TYPE: RETAINING; GRADE: 24CRMOV55; OEM P/N: 2480-036, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24800-0065; FOR HP GLAND CARRIER","EA",50,null,0]
["0757435","WASHER, LOCK: INSIDE DIAMETER: 31 MM; OUTSIDE DIAMETER: 45 MM; THICKNESS: 1.5 MM; NOMINAL SIZE: M30; MATERIAL: STEEL; TYPE: TAB; GRADE: 10CR13; OEM P/N: 2480-009, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24800-0065; FOR HP GLAND CARRIER","EA",50,null,0]
["0757438","WASHER: TYPE: INSERT; INSIDE DIAMETER: 28 MM; MATERIAL: STEEL; GRADE: 24CRMO5; OEM P/N: 2460-045, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0005; FOR HP DIAPHRAGM CARRIER 3","EA",50,null,0]
["0757439","WASHER: TYPE: INSERT; INSIDE DIAMETER: 38 MM; MATERIAL: STEEL; GRADE: 24CRMO5; OEM P/N: 2460-006, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0003; FOR HP DIAPHRAGM CARRIER 1","EA",50,null,0]
["0758070","WASHER: TYPE: SELF TAPPING SCREWS; INSIDE DIAMETER: 6 MM; OUTSIDE DIAMETER: 26 MM; THICKNESS: <1 MM; MATERIAL: EPDM RUBBER; OEM P/N: EUREKA 200 X EPDM BONDED WASHERS 6 X 26 MM; 200 X EPDM BONDED WASHERS","EA",50,null,0]
["0760273","WASHER: TYPE: BEARING; INSIDE DIAMETER: 13 MM; OUTSIDE DIAMETER: 24 MM; THICKNESS: 2.5 MM; MATERIAL: STEEL; OEM P/N: 4920-010, OEM: GE STEAM POWER SERVICE","EA",50,null,0]
["0760274","WASHER: TYPE: BEARING; INSIDE DIAMETER: 13 MM; OUTSIDE DIAMETER: 24 MM; THICKNESS: 2.5 MM; MATERIAL: STEEL; OEM P/N: 4921-010, OEM: GE STEAM POWER SERVICE","EA",50,null,0]
["0760275","WASHER, LOCK: INSIDE DIAMETER: 17 MM; OUTSIDE DIAMETER: 36 MM; THICKNESS: 1.2 MM; MATERIAL: STEEL; TYPE: EXTERNAL TAB; OEM P/N: 4920-007, OEM: GE STEAM POWER SERVICE; FOR BEARING","EA",50,null,0]
["0760276","WASHER, LOCK: INSIDE DIAMETER: 21 MM; OUTSIDE DIAMETER: 42 MM; THICKNESS: 1.6 MM; MATERIAL: STEEL; TYPE: EXTERNAL TAB; OEM P/N: 4921-007, OEM: GE STEAM POWER SERVICE","EA",50,null,0]
["0760277","WASHER, LOCK: INSIDE DIAMETER: 13 MM; OUTSIDE DIAMETER: 24 MM; THICKNESS: 2.5 MM; MATERIAL: STEEL; TYPE: BEARING; OEM P/N: 4922-010, OEM: GE STEAM POWER SERVICE","EA",50,null,0]
["0760278","WASHER, LOCK: INSIDE DIAMETER: 21 MM; OUTSIDE DIAMETER: 42 MM; THICKNESS: 1.6 MM; MATERIAL: STEEL; TYPE: EXTERNAL TAB; OEM P/N: 4922-007, OEM: GE STEAM POWER SERVICE; FOR BEARING","EA",50,null,0]
["0760280","WASHER, LOCK: INSIDE DIAMETER: 17 MM; OUTSIDE DIAMETER: 36 MM; THICKNESS: 1.2 MM; MATERIAL: STEEL; OEM P/N: 3790-042, OEM: GE STEAM POWER SERVICE; FOR LP DIAPHRAGM ASSEMBLY; WITH A NOSE","EA",50,null,0]
["0760281","WASHER, SPHERICAL MALE: INSIDE DIAMETER: 38 MM; MATERIAL: STEEL; GRADE: 21CRMOV57; OEM P/N: 2410-030, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012; FOR HP OUTER CASING; INSERT","EA",50,null,0]
["0760282","WASHER, LOCK: INSIDE DIAMETER: 25 MM; OUTSIDE DIAMETER: 60 MM; THICKNESS: 2.5 MM; MATERIAL: STEEL; GRADE: 5CRNI189; OEM P/N: 3940-016, OEM: GE STEAM POWER SERVICE; DRAWING NO: E42.39450-0011; FOR HP/LP DIAPHRAGM SUSPENSION","EA",50,null,0]
["0760283","WASHER: TYPE: BELLEVILLE; INSIDE DIAMETER: 61 MM; OUTSIDE DIAMETER: 150 MM; THICKNESS: 5 MM; MATERIAL: SPRING STEEL; OEM P/N: 4511-008, OEM: GE STEAM POWER SERVICE; DRAWING NO: E42.45130-1007","EA",50,null,0]
["0760284","WASHER, LOCK: INSIDE DIAMETER: 8.4 MM; OUTSIDE DIAMETER: 22 MM; THICKNESS: 0.75 MM; MATERIAL: STEEL; TYPE: LONG TAB; OEM P/N: 4930-033, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.49300-6011; FOR THRUST BEARING","EA",50,null,0]
["0760285","WASHER, SPHERICAL MALE: INSIDE DIAMETER: 28 MM; MATERIAL: STEEL; GRADE: 24CRMO5; OEM P/N: 2410-051, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012; FOR HP OUTER CASING, INSERT","EA",50,null,0]
["0762002","WASHER: TYPE: M16; INSIDE DIAMETER: 16 MM; OUTSIDE DIAMETER: 20 MM; THICKNESS: 0.79 MM; MATERIAL: STAINLESS STEEL","EA",50,null,0]
[]
[{"$nulls":4},"Sub-total"]

{"sheet":"Nuts","index":1,"n_rows":214,"n_cols":6,"rows_kept":214}
["Material","Text","Unit","Quantity","Price","Total"]
["0001154","NUT, HEX: DIAMETER: 2BA; THREAD: 0.0319 IN; NUT HEIGHT: 11/64 IN; MATERIAL: BRASS; GRADE: C10100; SPECIFICATION: BS 57; REFERENCE NO: 2BA; (PRECISION TYPE),DIMENSIONS: 0,324INCH ACROSS FLATS. 0.167INCH THICK,TABLE 6","EA",70,null,{"$f":"D2*E2","v":0}]
["0001155","NUT, HEX: DIAMETER: 0BA; THREAD: 1 MM; NUT HEIGHT: 7/32 IN; MATERIAL: BRASS; GRADE: C10100; SPECIFICATION: BS 57 TABLE 6","EA",162,null,{"$f":"D3*E3","v":0}]
["0046383","NUT, LOCK: RING AND SCREWS 4/5 MEDIVANE PUMP SA 2533 COOLING WATER PUMPS","EA",50,null,0]
["0047625","NUT: TYPE: SHAFT NDE RH; DIAMETER: 88 MM; THREAD: 1.5 MM; MATERIAL: STL; MODEL NO: HCD6N/8; REFERENCE NO: 217A; 119-903-017-014; FOR 50 PCT KSB PUMP","EA",50,null,0]
["0057156","NUT, HEX: DIAMETER: M10; THREAD: 1.5 MM; NUT HEIGHT: 8 MM; MATERIAL: STL WROUGHT; GRADE: 4.6; STEAM PIPE BACK","EA",50,null,0]
["0057158","NUT, LOCK: DIAMETER: M20; LOCKING METHOD: SELF LOCKING; THREAD: 1.75 MM; MATERIAL: WS; NUT HEIGHT: 9.5 MM; GRADE: 4.6; STEAM PIPE BACK","EA",50,null,0]
["0078295","NUT, ASSEMBLY: DEFLECTOR BLEAD STM EMER/S","EA",50,null,0]
["0087146","NUT, COUPLING: DIAMETER: 1/2 IN; THREAD: 13UNC; HEIGHT: 1-5/8 IN; MATERIAL: STL; REFERENCE NO: 327858-1123; TRIP STUD FOR USE WITH DIAMOND POWER RETRACTABLE SOOTBLOWER TYPE IK545","EA",50,null,0]
["0087468","NUT, HEX: DIAMETER: 1/4 IN; THREAD: 20BSW; NUT HEIGHT: 1/4 IN; MATERIAL: BRASS","EA",58,null,0]
["0087559","NUT, HEX: DIAMETER: 4BA; THREAD: 0.66 MM; NUT HEIGHT: 9/64 IN; MATERIAL: BRASS; GRADE: C10100; SPECIFICATION: BS 57 TABLE 6; REFERENCE NO: 4BA","EA",80,null,0]
["0087565","NUT, HEX: DIAMETER: M10; THREAD: 1.5 MM; NUT HEIGHT: 8 MM; MATERIAL: BRASS","EA",50,null,0]
["0087574","NUT, HEX: DIAMETER: 1/4 IN; THREAD: 20BSW; NUT HEIGHT: 7/32 IN; MATERIAL: MS; GRADE: 8.8; SPECIFICATION: BS 1083-1965 TABLE 5; MEDIUM FIT","EA",50,null,0]
["0087577","NUT, HEX: DIAMETER: 3/8 IN; THREAD: 16BSW; NUT HEIGHT: 5/16 IN; MATERIAL: MS; SPECIFICATION: BS 1083 TABLE 5; FINISHED THREAD MEDIUM FIT,GRADE A","EA",108,null,0]
["0087578","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 12BSW; NUT HEIGHT: 7/16 IN; MATERIAL: MS GR A; SPECIFICATION: BS 1083; FINISHED","EA",50,null,0]
["0087579","NUT, HEX: DIAMETER: 5/8 IN; THREAD: 11BSW; NUT HEIGHT: 9/16 IN; MATERIAL: MS GR A; SPECIFICATION: BS 1083; FINISHED","EA",62,null,0]
["0087580","NUT, HEX: DIAMETER: 7/8 IN; THREAD: 9BSW; NUT HEIGHT: 27/32 IN; MATERIAL: MS; GRADE: 4.5; SPECIFICATION: BS 1083 TABLE 5; GRADE A; WASHER FACED AND CHAMFERED; MEDIUM FIT","EA",160,null,0]
["0087581","NUT, HEX: DIAMETER: 1 IN; THREAD: 8BSW; NUT HEIGHT: 7/8 IN; MATERIAL: MS GR A; SPECIFICATION: BS 1083 TABLE 5; WASHER FACED AND CHAMFERED","EA",50,null,0]
["0087585","NUT, HEX: DIAMETER: 7/8 IN; THREAD: BSW; MATERIAL: BRASS; DIM - 1,300 IN W ACROSS FLAT S 0,750 IN THK PRECISION TYPE","EA",50,null,0]
["0087586","NUT, HEX: DIAMETER: 5/16 IN; THREAD: 18BSW; NUT HEIGHT: 1/4 IN; MATERIAL: BRASS","EA",50,null,0]
["0087588","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 12BSW; NUT HEIGHT: 7/16 IN; MATERIAL: BRASS","EA",50,null,0]
["0087589","NUT, HEX: DIAMETER: 5/8 IN; THREAD: 11BSW; NUT HEIGHT: 17/32 IN; MATERIAL: BRASS","EA",50,null,0]
["0087590","NUT, HEX: DIAMETER: 3/4 IN; THREAD: 10BSW; NUT HEIGHT: 11/16 IN; MATERIAL: BRASS","EA",50,null,0]
["0087597","NUT, HEX: DIAMETER: 3/4 IN; THREAD: 12BSF; NUT HEIGHT: 11/16 IN; MATERIAL: MS GR A; SPECIFICATION: BS 1083; WASHER FACED AND CHAMFERED","EA",50,null,0]
["0087616","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 13UNC; NUT HEIGHT: 1/2 IN; MATERIAL: HTS GR 40","EA",50,null,0]
["0087621","NUT, HEX: DIAMETER: 7/16 IN; THREAD: 14BSW; NUT HEIGHT: 3/8 IN; MATERIAL: MS; SPECIFICATION: BS 1083-1965 TABLE 5; PRECISION, MEDIUM FIT, GRADE A","EA",50,null,0]
["0087624","NUT, HEX: DIAMETER: 3/4 IN; THREAD: 10BSW; NUT HEIGHT: 21/32 IN; MATERIAL: MS; SPECIFICATION: BS 1083 TABLE 5; PRECISION, MEDIUM FIT, GRADE A","EA",50,null,0]
["0087628","NUT, HEX: DIAMETER: 1-1/8 IN; THREAD: 7BSW; NUT HEIGHT: 27/32 IN; MATERIAL: MS GR A; SPECIFICATION: BS 1083 TABLE 5; PRECISION, FACED AND CHAMFERED, MEDIUM FIT","EA",150,null,0]
["0087630","NUT, HEX: DIAMETER: 1-1/4 IN; THREAD: 7BSW; NUT HEIGHT: 1-1/6 IN; MATERIAL: MS GR A; SPECIFICATION: BS 1083 TABLE 5; PRECISION, FACED AND CHAMFERED, MEDIUM FIT","EA",83,null,0]
["0087632","NUT, HEX: DIAMETER: 1-1/2 IN; THREAD: BSW; MATERIAL: STL FINISHED","EA",62,null,0]
["0087637","NUT, HEX: DIAMETER: M12; THREAD: 1.75 MM; NUT HEIGHT: 10 MM; MATERIAL: MS BLACK; GRADE: 4.6; SPECIFICATION: SABS 1143","KG",50,null,0]
["0087638","NUT, HEX: DIAMETER: M16; THREAD: 2 MM; NUT HEIGHT: 13 MM; MATERIAL: MS BLACK; GRADE: 4.6; SPECIFICATION: SABS 1143","KG",50,null,0]
["0087640","NUT, HEX: DIAMETER: M24; THREAD: 3 MM; NUT HEIGHT: 18 MM; MATERIAL: MS BLACK; SPECIFICATION: SABS 1143","KG",-126,null,0]
["0087641","NUT, HEX: DIAMETER: M30; THREAD: 3.5 MM; NUT HEIGHT: 24 MM; MATERIAL: MS BLACK; GRADE: 4.6; SPECIFICATION: SABS 1143-1977","KG",50,null,0]
["0087669","NUT, HEX: DIAMETER: 3/4 IN; THREAD: 12BSF; NUT HEIGHT: 11/16 IN; MATERIAL: HTS GR 40; GRADE: 8.8; REFERENCE NO: IF0005-8","EA",50,null,0]
["0087670","NUT, HEX: DIAMETER: 7/8 IN; THREAD: 12BSF; NUT HEIGHT: 3/4 IN; MATERIAL: HTS GR 40; GRADE: 8.8; REFERENCE NO: IF0005A9","EA",50,null,0]
["0087671","NUT, HEX: DIAMETER: 1 IN; THREAD: 10BSF; NUT HEIGHT: 5/8 IN; MATERIAL: HTS","EA",50,null,0]
["0087673","NUT, HEX: DIAMETER: 1-3/4 IN; THREAD: BSF; MATERIAL: STL; FINISHED","EA",50,null,0]
["0087677","NUT, HEX: DIAMETER: 7/8 IN; THREAD: 9BSW; NUT HEIGHT: 3/4 IN; MATERIAL: HTS","EA",50,null,0]
["0087679","NUT, HEX: DIAMETER: M16; THREAD: 2 MM; NUT HEIGHT: 12.5 MM; MATERIAL: HTS; GRADE: 8; SPECIFICATION: SABS 136","EA",50,null,0]
["0087681","NUT, HEX: DIAMETER: M20; THREAD: 2.5 MM; NUT HEIGHT: 17 MM; MATERIAL: HTS; GRADE: 8.8; SPECIFICATION: DIN 934","EA",660,null,0]
["0087689","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 16BSF; NUT HEIGHT: 7/16 IN; MATERIAL: HTS GR 40; GRADE: 8.8; SPECIFICATION: DIN 931; REFERENCE NO: VERBUSP","EA",50,null,0]
["0087691","NUT, HEX: DIAMETER: 5/8 IN; THREAD: 11BSW; NUT HEIGHT: 14.2 MM; MATERIAL: HTS; GRADE: 8.8; SPECIFICATION: DIN 934","EA",50,null,0]
["0088617","NUT: TYPE: GLAND; CLYDE SOOTBLOWER","EA",50,null,0]
["0088619","NUT: VALVE CLYDE S/BL","EA",50,null,0]
["0088673","NUT, CAP: DIAMETER: 1-1/8 IN; THREAD: 12 TPI; HEIGHT: 1-1/8 IN; MATERIAL: BRASS; SUPPL P/N: 302032-0119; DAIMOND POWER, PACKING SOOTBLOWER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",51,null,0]
["0088834","NUT, ADAPTOR: DIAMETER: 70 MM; LOCKING METHOD: LOCK WASHER; THREAD: 2 MM; MATERIAL: STL; SUPPL P/N: KM14","EA",50,null,0]
["0088872","NUT: TYPE: GLAND; 8IN HP BLED STM VALVE","EA",50,null,0]
["0088873","NUT: TYPE: GLAND; 10 IN HP BLED STEAM VALVE","EA",50,null,0]
["0089143","NUT, HEX: DIAMETER: 3BA; NUT HEIGHT: 3.8 MM; MATERIAL: BRASS","EA",50,null,0]
["0089444","NUT, TUBE FITTING: TYPE: HEX; DIAMETER: 6 MM; MATERIAL: STAINLESS STEEL; SUPPL P/N: SS-6M2-1; SS-6M2-1","EA",50,null,0]
["0089446","NUT, HEX: DIAMETER: M12; THREAD: 1.75 MM; NUT HEIGHT: 17 MM; MATERIAL: STAINLESS STEEL; SUPPL P/N: SS-12M2-1; REFERENCE NO: SS-12M2-1","EA",50,null,0]
["0089609","NUT, LOCK: DIAMETER: M10; LOCKING METHOD: NYLOCK; THREAD: 1.5 MM; MATERIAL: STL GALV; TYPE: HEX; GRADE: 8; SELF","EA",50,null,0]
["0089621","NUT, HEX: DIAMETER: M24; THREAD: 3 MM; NUT HEIGHT: 19 MM; MATERIAL: HTS; GRADE: 8.8","EA",50,null,0]
["0089651","NUT, HEX: DIAMETER: 1/4 IN; MATERIAL: BRASS; 16B","EA",50,null,0]
["0089652","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 32B; MATERIAL: BRASS; ETO","EA",50,null,0]
["0089653","NUT, TUBE FITTING: TYPE: FLARED; MATERIAL: BRASS","EA",50,null,0]
["0089654","NUT, TUBE FITTING: TYPE: FLARED; DIAMETER: 1/4 IN; MATERIAL: STL","EA",350,null,0]
["0089655","NUT: DIAMETER: M20","EA",90,null,0]
["0089656","NUT: TYPE: CAPSULE; THREAD: 24 MM","EA",124,null,0]
["0089657","NUT: DIAMETER: M30","EA",50,null,0]
["0089658","NUT, SLOTTED: DIAMETER: M30","EA",50,null,0]
["0089659","NUT, SLOTTED: DIAMETER: M36","EA",50,null,0]
["0089660","NUT, SLOTTED: DIAMETER: M48","EA",50,null,0]
["0089661","NUT, SLOTTED: DIAMETER: M64","EA",50,null,0]
["0089662","NUT, SLOTTED: DIAMETER: M80","EA",50,null,0]
["0089663","NUT, SLOTTED: DIAMETER: M100","EA",50,null,{"$f":"D67*E67","v":0}]
["0089664","NUT, SLOTTED: DIAMETER: M120","EA",50,null,0]
["0089672","NUT, CAP: DIAMETER: M24; AM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0089683","NUT, TUBE FITTING: MATERIAL: SS GR 316; SUPPL P/N: B10-0-316","EA",50,null,0]
["0089684","NUT, LOCK: ITEM 38","EA",50,null,0]
["0089685","NUT, LOCK: TYPE: IMPELLER","EA",50,null,0]
["0089686","NUT: TYPE: SHAFT","EA",50,null,0]
["0089687","NUT: TYPE: PLUNGER; SUPPL P/N: 400521","EA",50,null,0]
["0089689","NUT: TYPE: SHAFT BOTTOM; SUPPL P/N: C5017; C5018","EA",50,null,0]
["0089691","NUT: SUPPL P/N: X1060T4","EA",50,null,0]
["0089708","NUT: TYPE: PROPELLER SHAFT","EA",50,null,0]
["0089709","NUT, LOCK: THREAD: LH; TYPE: SPECIAL; IT 28","EA",110,null,0]
["0089716","NUT, HEX: DIAMETER: M27; HP-LP PIPE FLANGE","EA",50,null,0]
["0089720","NUT, LOCK: SUPPL P/N: 920.7","EA",50,null,0]
["0089721","NUT, LOCK: TYPE: SHAFT; SUPPL P/N: 921","EA",50,null,0]
["0089722","NUT: TYPE: SHAFT; ITEM 12","EA",50,null,0]
["0089723","NUT: TYPE: CLAMPING; LOESCHE MILL","EA",50,null,0]
["0089726","NUT: SUPPL P/N: 4190B; GORMAN PUMP IMPELLER","EA",50,null,0]
["0089734","NUT: DIAMETER: M16; DRAWING NO: DIN 934 REV 1","EA",50,null,0]
["0090052","NUT, HEX: DIAMETER: 3/4 IN; THREAD: 10BSW; NUT HEIGHT: 5/8 IN; MATERIAL: HTS; GRADE: 8.8; SPECIFICATION: DIN 934","EA",50,null,0]
["0090191","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 12BSW; MATERIAL: SS GR 316; SPECIFICATION: BS 1083-1965; PRECISION WASHER FACED AND CHAMFERRED MEDIUM FIT","EA",50,null,0]
["0090438","NUT: TYPE: SHAFT DRIVE END; DIAMETER: 90 MM; THREAD: LH 2 MM; MATERIAL: BRASS; MODEL NO: HCD6N/8; REFERENCE NO: 119-903-017-013; 217; FOR 50 PCT KSB PUMP","EA",50,null,0]
["0090499","NUT: TYPE: IMPELLER; DIAMETER: 2 IN; THREAD: 11 TPI; MATERIAL: STAINLESS STEEL; SPECIFICATION: ISO 9001; MATERIAL GRADE: HT; APPLICATION: BOOSTER; SUPPL P/N: 31.13; MODEL NO: NPTX(D)48-25; REFERENCE NO: 104-604-755-001; FOR USE ON SULZER SFP BOOSTER PUMP","EA",50,null,0]
["0090993","NUT, SLOTTED: TYPE: CASTLE, ROUND; THREAD: M100-6 MM; MATERIAL: STEEL 56T5CM100; GRADE: N204; OEM P/N: 2450-010, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24500-0026 REV 1; 2450-010 REV 0; 06-13772-4112 REV 0; FOR HP INNER CASING","EA",70,null,0]
["0091003","NUT, SLOTTED: TYPE: CASTLE ROUND; DIAMETER: 64 MM; THREAD: 5.5 MM; MATERIAL: STL 56T5CM64 GR N204; OEM P/N: 2650-012, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.26500-0018; 06.13772-4108; IP INNER CASING","EA",50,null,0]
["0091231","NUT, HEX: DIAMETER: 1/2 IN; THREAD: 13UNC; NUT HEIGHT: 7/16 IN; MATERIAL: HTS; REFERENCE NO: 863015-2900; OUTSIDE SIZE OF NUT TO 19MM SPANNER FOR LONG LANCE SOOTBLOWER GLAND FOLLOWER; TYPE IK 545B","EA",50,null,0]
["0091504","NUT, TUBE FITTING: TYPE: GLAND; DIAMETER: M10; MATERIAL: STAINLESS STEEL; SUPPL P/N: SS10M2-1","EA",50,null,0]
["0091830","NUT, HEX: PLAIN","EA",50,null,0]
["0091831","NUT, HEX: PLAIN","EA",50,null,0]
["0091832","NUT: DIAMETER: M42; THREAD: 3 MM; TURBINE","EA",50,null,0]
["0091840","NUT, SLOTTED: TYPE: CASTLE; SPINNER; EM/STP VALVE","EA",50,null,0]
["0091841","NUT, HEX: KSB OIL PUMP SHAFT","EA",50,null,0]
["0091843","NUT, LOCK: KSB OIL PUMP","EA",50,null,0]
["0091845","NUT, HEX: DIAMETER: 3/4 IN; THREAD: BSW; H2 PLANT BB 6EN","EA",50,null,0]
["0091848","NUT: DIAMETER: 2 IN; SUPPL P/N: 217A; SHAFT HOP C-OFF","EA",50,null,0]
["0091849","NUT: SUCT&DISCHARGE CASING","EA",50,null,0]
["0091850","NUT: TYPE: SLEEVE; MATHER & PLATT WATER PUMP 5/6 STRAGLON MEDIVANE PUMP NO 1871/2/3/4","EA",50,null,0]
["0091851","NUT: WITHDRAWAL SPA BILGE PUMP","EA",50,null,0]
["0091852","NUT, LOCK","EA",50,null,0]
["0091854","NUT, LOCK: STE 3V DRAINAGE/PUMP","EA",50,null,0]
["0091857","NUT, SLOTTED: TYPE: SHAFT; DIAMETER: 72 MM; THREAD: 10 TPI; MATERIAL: STL; GRADE: HT; NUT HEIGHT: 24 MM; SPECIFICATION: ISO 9001; SUPPL P/N: 31.15.1; MODEL NO: NPTX(D)48-25; REFERENCE NO: 104-604-751-200; FOR USE ON SFP BOOSTER PUMP","EA",50,null,0]
["0091863","NUT, HEX: DIAMETER: 1-3/4 IN; THREAD: BSW; FINISHED","EA",50,null,0]
["0091864","NUT, HEX: DIAMETER: 1/2 IN; SUPPL P/N: 3SW Z","EA",50,null,0]
["0091865","NUT, HEX: DIAMETER: 2-1/2 IN; THREAD: BSF; MATERIAL: STL; FINISHED","EA",90,null,0]
["0091866","NUT, HEX: DIAMETER: 1/2 IN; THREAD: BSW; MATERIAL: HTS","EA",50,null,0]
["0091868","NUT, HEX: DIAMETER: 5/8 IN; THREAD: BSW; MATERIAL: SS GR 316","EA",50,null,0]
["0091869","NUT, LOCK: THREAD: 7/16-BSF; MATERIAL: STL; TYPE: HEX","EA",50,null,0]
["0129720","NUT: DOUBLE; BROWN BOVERI GENERATOR TYPE WT28H-090-HF3 RPM 3000","EA",50,null,0]
["0136302","NUT, CONDUIT LOCK: TYPE: TUBING; DIAMETER: M20; MATERIAL: STL PROCAST BLACK","EA",71,null,0]
["0136303","NUT, CONDUIT LOCK: TYPE: THINWALL; DIAMETER: M25; MATERIAL: STL","EA",50,null,0]
["0186201","NUT: TYPE: ADJUSTING; DIAMETER: 2-3/8 IN; THREAD: 12 TPI; MATERIAL: SS GR 316; SUPPL P/N: 395124-1128; DIAMOND POWER","EA",160,null,0]
["0227400","NUT, HEX: DIAMETER: M10; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT; DIAMETER: 17 MM","EA",269,null,0]
["0227401","NUT, HEX: DIAMETER: M12; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT; DIAMETER: 19 MM","EA",74,null,0]
["0227402","NUT, HEX: DIAMETER: M16; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT; DIAMETER: 24 MM","EA",70,null,0]
["0227403","NUT, HEX: DIAMETER: M20; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT; DIAMETER: 30 MM","EA",280,null,0]
["0229783","NUT, CAP: SUPPL P/N: B081207; DRAWING NO: IM20 REV 1; OIL BURNER EQUIPMENT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",52,null,0]
["0230171","NUT, HEX: DIAMETER: M6; NUT HEIGHT: 5 MM; MATERIAL: BRASS; FOR MAINTENANCE","KG",50,null,0]
["0230172","NUT: DIAMETER: M12; MATERIAL: MS; FOR MAINTENANCE","KG",66,null,0]
["0230178","NUT, HEX: DIAMETER: M8; NUT HEIGHT: 10 MM; MATERIAL: MS; FOR MAINTENANCE","KG",50,null,0]
["0231334","NUT, LOCK: SUPPL P/N: 901099-0005; FOR SOOTBLOWER","EA",50,null,0]
["0231595","NUT: SUPPL P/N: HG800-007; SPARES FOR HOPKINSON SOOTBLOWERS UNIT 2, 3 AND 4","EA",50,null,0]
["0231768","NUT, LOCK: LOCKING METHOD: JAM; SUPPL P/N: 863008-2900; FOR USE ON SOOTBLOWER","EA",50,null,0]
["0231786","NUT, HEX: SUPPL P/N: 301237-6115; FOR USE ON SOOTBLOWER","EA",50,null,0]
["0231788","NUT, LOCK: LOCKING METHOD: JAM; SUPPL P/N: 863007-6000; FOR USE ON SOOTBLOWER","EA",50,null,0]
["0231793","NUT: TYPE: SOOTBLOWER; SUPPL P/N: 863014-2700","EA",464,null,{"$f":"D131*E131","v":0}]
["0231941","NUT: TYPE: SOOTBLOWER; DIAMETER: 3/8 IN; THREAD: UNC; MATERIAL: STL; APPLICATION: IR2 SCREW TUBE AND PACKING ASSY; SUPPL P/N: 863015-2700","EA",140,null,0]
["0233624","NUT, HEX: DIAMETER: M6; THREAD: 1 MM; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",50,null,0]
["0233630","NUT, HEX: DIAMETER: M10; THREAD: 1.5 MM; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",50,null,0]
["0233638","NUT, HEX: DIAMETER: M16; THREAD: 2 MM; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",50,null,0]
["0233639","NUT, LOCK: DIAMETER: M16; LOCKING METHOD: SELF LOCKING; THREAD: 2 MM; MATERIAL: HTS; GRADE: 8.8; FOR MAINTENANCE USE","EA",64,null,0]
["0233643","NUT, HEX: DIAMETER: M16; THREAD: 2 MM; MATERIAL: HTS; GRADE: 8.8; FOR MAINTENANCE USE","EA",50,null,0]
["0233646","NUT, HEX: DIAMETER: M10; THREAD: 1.5 MM; MATERIAL: HTS; GRADE: 8.8; FOR MAINTENANCE USE","EA",50,null,0]
["0233649","NUT, HEX: DIAMETER: 5/8 IN; THREAD: BSW; MATERIAL: HTS; GRADE: 8.8; FOR MAINTENANCE USE, THREADS: 0.8MM","EA",50,null,0]
["0233652","NUT, HEX: DIAMETER: 1/2 IN; THREAD: BSW; MATERIAL: HTS; GRADE: 8.8; FOR MAINTENANCE USE, THREADS: 0.7MM","EA",50,null,0]
["0233675","NUT, HEX: DIAMETER: M20; THREAD: 2.5 MM; MATERIAL: MS; GRADE: 4; FOR MAINTENANCE USE","EA",50,null,0]
["0233676","NUT, LOCK: DIAMETER: M20; LOCKING METHOD: SELF LOCKING; THREAD: 2.5 MM; MATERIAL: HTS; GRADE: 8; FOR MAINTENANCE USE","EA",50,null,0]
["0233681","NUT, HEX: DIAMETER: M24; THREAD: 3 MM; MATERIAL: MS; GRADE: 4; FOR MAINTENANCE USE","EA",50,null,0]
["0233682","NUT, LOCK: DIAMETER: M24; LOCKING METHOD: SELF LOCKING; THREAD: 3 MM; MATERIAL: HTS; GRADE: 8; FOR MAINTENANCE USE","EA",50,null,0]
["0237151","NUT, SLOTTED: TYPE: HEX; DIAMETER: 125 MM; THREAD: M125-8; MATERIAL: NICR20TIAL; SPECIFICATION: DIN 2510; OEM P/N: 2450-021, OEM: GE STEAM POWER SERVICE; DRAWING NO: E42.99896-7406 REV 1; HP INNER CASING","EA",50,null,0]
["0238852","NUT: TYPE: VALVE; DIAMETER: M12; MATERIAL: SS GR 316; SUPPL P/N: 230388; REQUIRED FOR MILLS, UNITS 1, 2, 3, 4/6","EA",50,null,0]
["0239901","NUT: TYPE: STUFFING BOX; SUPPL P/N: 4013486; 31.38; MODEL NO: HPTPOM32-25-4STG; FOR USE ON SULZER FEED PUMP","EA",50,null,0]
["0239903","NUT, COUPLING: SUPPL P/N: 31.97; 104-600-977-001; MODEL NO: HPTPOM32-25-4STG; NDE, FOR USE ON SULZER FEED PUMP","EA",50,null,0]
["0240323","NUT, HEX: DIAMETER: M10; DRAWING NO: B42.51200-0017 REV 1; REQUIRED FOR HP CONTROL VALVE DV 2-6, GROUP NO 5121, UNITS 1-4","EA",50,null,0]
["0240326","NUT, HEX: DIAMETER: M12; THREAD: 1.5 MM; DRAWING NO: D42.59256-0073 REV 1; REQUIRED FOR CONTROL VALVE COUPLING STEM LOCK, GROUP NO 5126","EA",50,null,0]
["0240354","NUT: TYPE: MAIN STUD; MODEL NO: HCD6N/8; REFERENCE NO: 112; FOR USE ON 50PCT KSB ELECTRIC FEED PUMP","EA",50,null,0]
["0244218","NUT: DIAMETER: M12; SUPPL P/N: 7120-062; REQUIRED FOR USE ON UNITS 1 - 6 EMERGENCY STOP VALVE HEAT SHIELD; AS PER O.E.M. SPECIFICATIONS; STANDARD PITCH","EA",50,null,0]
["0249584","NUT: TYPE: BUFFALO B520 RFL RECLAIM FEEDER; DIAMETER: M16; MATERIAL: STL; SUPPL P/N: NL 16","EA",60,null,0]
["0249653","NUT, LOCK: DIAMETER: M140; THREAD: TR 60 X 3; MATERIAL: GS45 CAST; TYPE: CLAMPING; DRAWING NO: 3.1516.00.0605 REV 1; REQUIRED FOR USE ON UNIT 5, LOESCHE MILLING PLANT, HT 210","EA",50,null,0]
["0250166","NUT, LOCK: DIAMETER: 7/8 IN; LOCKING METHOD: DOUBLE LOCK; THREAD: BSF; MATERIAL: MS; NUT HEIGHT: 1-1/4 IN; TYPE: HOPKINSONS SOOTBLOWERS, U1-5/6; DRAWING NO: DWSA10Q290 REV 1; SQUARE SHAFT","EA",63,null,0]
["0251827","NUT: DIAMETER: 5/8 IN; THREAD: BSF; MATERIAL: MS; REFERENCE NO: DWSA10Q39 2; FOR USE ON POPPET VALVE ON SOOTBLOWERS, UNITS 1-4 /6","EA",50,null,0]
["0252380","NUT: TYPE: CLAMP; DIAMETER: 50 MM; THREAD: UNC; MATERIAL: MS; SUPPL P/N: DN; REQUIRED FOR USE AT ASH HOPPER ACCESS DOOR, UNIT 1-4/6; GRADE 4.6","EA",66,null,0]
["0252894","NUT: DIAMETER: M16; MATERIAL: CS; SPECIFICATION: BS 970; DRAWING NO: BABCOCK 3255/0014 REV 1; REQUIRED FOR USE ON PF BURNER, UNIT 1 TO 6, MACHINED","EA",50,null,0]
["0253387","NUT, HEX: DIAMETER: 5/8 IN; THREAD: BSF; MATERIAL: CS; SUPPL P/N: POPPET001; REQUIRED FOR USE ON POPPET VALVE BOTTOM AT SOOTBLOWER, UNIT 1 TO 6","EA",50,null,0]
["0253388","NUT, HEX: DIAMETER: 1/2 IN; THREAD: BSF; MATERIAL: CS; SUPPL P/N: FB7869/4-516C 0; REQUIRED FOR USE ON POPPET VALVE TOP AT SOOTBLOWER, UNIT 1-6","EA",50,null,0]
["0256020","NUT, LOCK: DIAMETER: M6; LOCKING METHOD: NYLOCK; MATERIAL: STL; NUT HEIGHT: 6 MM; TYPE: HEX; GRADE: 8","EA",50,null,0]
["0256021","NUT, LOCK: DIAMETER: M8; LOCKING METHOD: NYLOCK; MATERIAL: STL; NUT HEIGHT: 8 MM; TYPE: HEX; GRADE: 8","EA",36,null,0]
["0256022","NUT, LOCK: DIAMETER: M12; LOCKING METHOD: NYLOCK; MATERIAL: STL; NUT HEIGHT: 12 MM; TYPE: HEX; GRADE: 8","EA",18,null,0]
["0501160","NUT, HEX: DIAMETER: M20; MATERIAL: X19CRMOVNBN113; REQUIRED FOR H.P.GOVERNOR VALVES; UNITS 1 - 6; AS PER ALSTOM SERVICES O.E.M.REQUIREMENTS; GROUP 5120; ITEM 063","EA",50,null,0]
["0501655","NUT, HEX: DIAMETER: M8; THREAD: 1.25 MM; NUT HEIGHT: 6.5 MM; MATERIAL: BRASS; REQUIRED FOR USE ON PANELS AND CONNECTIONS; ACROSS FLATS 13 MM","EA",50,null,0]
["0527285","NUT: TYPE: ANNULAR; DIAMETER: 495 MM; THREAD: M400-4; MATERIAL: X22CRMOV12-1; APPLICATION: HP NOZZLE BOX; OEM P/N: 2490-051, OEM: GE STEAM POWER SERVICE; 2350-007, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.23550-0051-0054 REV 0; F42.29296-0006 REV 0","EA",50,null,0]
["0569475","NUT, COUPLING: DIAMETER: 54 MM; THREAD: M36; HEIGHT: 186 MM; MATERIAL: EN8; MANUF P/N: J05F24/27PNB; PIN C/W; FOR USE ON CONVEYOR 24A-C COUPLING HALVES BETWEEN GEARBOX AND DRIVE PULLEY","EA",50,null,0]
["0607974","NUT, SLOTTED: DIAMETER: 48 MM; THREAD: M48-5; MATERIAL: STEEL ALLOY; GRADE: 21CRMOV57V; OEM P/N: 2460-009, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0003; FOR HP DIAPHRAGM CARRIER 1","EA",50,null,0]
["0607977","NUT, SLOTTED: TYPE: HP DIAPHRAGM CARRIER 10/11; DIAMETER: 42 MM; THREAD: METRIC; MATERIAL: 34CRNIMO6V; NM42; GROUP NO: 2460; ITEM 030; ALSTOM SPARES","EA",50,null,0]
["0607980","NUT, SLOTTED: TYPE: HP DIAPHRAGM STG 10/11/12/13; DIAMETER: 36 MM; THREAD: METRIC; MATERIAL: 34CRNIMO6V; ALSTOM SPARES; GROUP NO: 2460 AND ITEM 048","EA",50,null,0]
["0620786","NUT: TYPE: FASTENING; DIAMETER: 3/4 IN; THREAD: BSF; MATERIAL: MILD STEEL; MANUF P/N: Y20004180; REFERENCE NO: 2148-457","EA",50,null,0]
["0620803","NUT: TYPE: FASTENING; DIAMETER: 60 MM; THREAD: BSF; MATERIAL: BRASS; MATERIAL GRADE: BRASS; MANUF P/N: Y30039924; REFERENCE NO: 34326-405; TORSION BAR END NUT ITEM 137","EA",50,null,0]
["0622559","NUT: TYPE: TURBINE; DIAMETER: 72 MM; THREAD: M72; MATERIAL: ALLOY; OEM P/N: 1730/004; FOR USE ON LP ROTOR UNIT 1 TO 4","EA",50,null,0]
["0622563","NUT: TYPE: INNER CASING; DIAMETER: 120 MM; THREAD: M120; MATERIAL: ALLOY; APPLICATION: HP INNER CASING; OEM P/N: 2450-014, OEM: GE STEAM POWER SERVICE","EA",50,null,0]
["0622564","NUT: TYPE: RING; DIAMETER: 390 MM; THREAD: M310; MATERIAL: ALLOY; OEM P/N: 2490/009; FOR USE ON HP CASING ASSEMBLY","EA",50,null,0]
["0622565","NUT: TYPE: PIPE; DIAMETER: M48; THREAD: M48; MATERIAL: ALLOY; OEM P/N: 8110/094; FOR USE ON LIVE STEAM INLET PIPES","EA",50,null,0]
["0628349","NUT: TYPE: SLOTTED; DIAMETER: 120 MM; THREAD: METRIC; MATERIAL: STL ALLOY; OEM P/N: 2410-011, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012 REV 0; REFERENCE NO: SZT-42-99996-00575","EA",50,null,0]
["0628354","NUT: TYPE: SLOTTED; DIAMETER: 64 MM; THREAD: METRIC; MATERIAL: STL ALLOY; OEM P/N: 2410-028, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012 REV 0; REFERENCE NO: SZT-42-99996-00579","EA",50,null,0]
["0628355","NUT: TYPE: SLOTTED; DIAMETER: 48 MM; THREAD: METRIC; MATERIAL: STL ALLOY; OEM P/N: 2410-033, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012 REV 0; REFERENCE NO: SZT-42-99996-00443","EA",50,null,0]
["0628357","NUT: TYPE: SLOTTED; DIAMETER: 42 MM; THREAD: METRIC; MATERIAL: STL ALLOY; OEM P/N: 2460-030, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0004 REV 0; REFERENCE NO: SZT-42-99996-00492","EA",50,null,0]
["0630472","NUT, SLOTTED: TYPE: CASTLE; DIAMETER: 72 MM; THREAD: M72; MATERIAL: STL ALLOY; OEM P/N: 1330 / 005","EA",50,null,0]
["0631427","NUT: TYPE: VALVE; DIAMETER: 171.6 MM; THREAD: 4TPI; MATERIAL: MILD STEEL; MANUF P/N: Y30042761 35751-104; DRAWING NO: F5128/5#527 REV 0","EA",50,null,0]
["0631432","NUT: TYPE: VALVE; DIAMETER: ID 58.3 X OD 76.1 X THK 21.2 MM; THREAD: 14TPI; MATERIAL: STAINLESS STEEL; MANUF P/N: Y30041418 35185-436; DRAWING NO: F5128/5#36 REV 0","EA",50,null,0]
["0632202","NUT, SLOTTED: TYPE: CONTROL VALVE; DIAMETER: 64 MM; THREAD: M64; MATERIAL: STEEL ALLOY; GRADE: 56T5V; OEM P/N: 5120-047, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51200-0041; GROOTVLEI 5120-047; REFERENCE NO: SZT-42-99996-00135; CASTLE; HP CV1-6 UNIT 1-6","EA",50,null,0]
["0632278","NUT: TYPE: SLOTTED; DIAMETER: M48; THREAD: 48 MM; MATERIAL: STL ALLOY; OEM P/N: SZT-42-99996-00197; DRAWING NO: 2410/036 REV 0","EA",50,null,0]
["0639766","NUT: TYPE: VALVE SAFETY; DIAMETER: 3/4 IN; THREAD: RH; MATERIAL: STL; SPECIFICATION: Y30042761","EA",50,null,0]
["0639767","NUT: TYPE: VALVE SAFETY; DIAMETER: 3/4 IN; THREAD: RH; MATERIAL: MS; SPECIFICATION: Y20004180","EA",50,null,0]
["0639853","NUT: TYPE: SCREW LOCKING; DIAMETER: 1-1/4 IN; THREAD: RH; MATERIAL: MS; SPECIFICATION: Y30041551","EA",50,null,0]
["0639890","NUT: TYPE: COVEL; DIAMETER: 25 MM; THREAD: RH; MATERIAL: STL; SPECIFICATION: HOPKINSONS 7020; APPLICATION: SAFETY VALVE; SPECIFICATION: Y30089653","EA",50,null,0]
["0639908","NUT: TYPE: SPINDLE; DIAMETER: 50 MM; THREAD: RH; MATERIAL: STL; SPECIFICATION: HOPKINSONS 7020; SPECIFICATION: Y30041535","EA",50,null,0]
["0639939","NUT: TYPE: VALVE; DIAMETER: 2 IN; THREAD: RH; MATERIAL: STL; SPECIFICATION: HOPKINSONS 7020; SPECIFICATION: Y30041418","EA",50,null,0]
["0713650","NUT: TYPE: HEXAGON; THREAD: M27; MATERIAL: STAINLESS STEEL DIN934; APPLICATION: HP/LP CROSSOVER PIPES; OEM P/N: 8160-133, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-133; 42.81600-0003","EA",50,null,0]
["0713651","NUT: TYPE: HEXAGON; THREAD: M20; MATERIAL: DIN2510; APPLICATION: HP/LP CROSSOVER PIPES; OEM P/N: 8160-172, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-172; 42.81600-0003","EA",50,null,0]
["0713652","NUT: TYPE: HEXAGON; THREAD: M20; MATERIAL: DIN2510; APPLICATION: HP/LP CROSSOVER PIPES; OEM P/N: 8160-193, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-193; 42.81600-0003","EA",50,null,0]
["0713653","NUT: TYPE: HEXAGON; THREAD: M20; MATERIAL: DIN2510; APPLICATION: HP/LP CROSSOVER PIPES; OEM P/N: 8160-192, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-192; 42.81600-0003","EA",50,null,{"$f":"D195*E195","v":0}]
["0713654","NUT: TYPE: HEXAGON; THREAD: TM20; MATERIAL: STEEL; MATERIAL GRADE: 56T5; APPLICATION: HP/LP CROSSOVER PIPES; OEM P/N: 8160-140, OEM: GE STEAM POWER SERVICE; 8160-193, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-140; 42.81600-0003; 8160-193","EA",50,null,0]
["0713655","NUT: TYPE: HEXAGON; THREAD: NM20; MATERIAL: STEEL; MATERIAL GRADE: 56T5; APPLICATION: HP/LP CROSSOVER PIPES; OEM P/N: 8160-141, OEM: GE STEAM POWER SERVICE; 8160-192, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-141; 42.81600-0003; 8160-192","EA",50,null,0]
["0757611","NUT, SLOTTED: THREAD: M36-4; MATERIAL: STEEL ALLOY; OEM P/N: 2460-048, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0005; FOR HP DIAPHRAGM CARRIER 3","EA",50,null,0]
["0757703","NUT, CAP: THREAD: M30-3.5; MATERIAL: STEEL; GRADE: 56T5V; OEM P/N: 2480-012, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24800-0065; FOR HP GLAND CARRIER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0758048","NUT: TYPE: M16; THREAD: METRIC - COARSE; MATERIAL: STAINLESS STEEL","EA",50,null,0]
["0759240","NUT, HEX: DIAMETER: 12 MM; THREAD: M12-1.75; MATERIAL: STAINLESS STEEL; OEM P/N: 4921-011, OEM: GE STEAM POWER SERVICE; FOR JOURNAL BEARING","EA",50,null,0]
["0759242","NUT, HEX: DIAMETER: 12 MM; THREAD: M12-1.75; MATERIAL: STAINLESS STEEL; OEM P/N: 4930-024, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.49300-6011; FOR THRUST BEARING","EA",50,null,0]
["0759243","NUT, HEX: DIAMETER: 30 MM; THREAD: M30-3.5; MATERIAL: STEEL; GRADE: 56T5V; OEM P/N: 4511-026, OEM: GE STEAM POWER SERVICE; DRAWING NO: E42.45130-1007","EA",50,null,0]
["0759245","NUT, CAP: DIAMETER: 24 MM; THREAD: M24-3; MATERIAL: STEEL; GRADE: 24CRMO5V; OEM P/N: 2410-057, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012; FOR HP OUTER CASING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0759246","NUT, CAP: DIAMETER: 24 MM; THREAD: M24-3; MATERIAL: STEEL; GRADE: 24CRMO5V; OEM P/N: 2410-047, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012; FOR HP OUTER CASING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0759247","NUT, HEX: DIAMETER: 12 MM; THREAD: M12-1.75; MATERIAL: STAINLESS STEEL; OEM P/N: 4922-011, OEM: GE STEAM POWER SERVICE; FOR JOURNAL BEARING","EA",50,null,0]
["0759263","NUT, SLOTTED: TYPE: CASTLE; DIAMETER: 100 MM; THREAD: M100-6; MATERIAL: STEEL; GRADE: 56T5V; OEM P/N: 2450-008, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24500-0006; FOR HP INNER CASING","EA",50,null,0]
["0759266","NUT: TYPE: SHAFT; DIAMETER: 48 MM; THREAD: M48-5; MATERIAL: STEEL; APPLICATION: MAIN OIL PUMP; OEM P/N: 8510-012, OEM: GE STEAM POWER SERVICE; DRAWING NO: A42.85109-0003; 85 X 25","EA",50,null,0]
["0759267","NUT, HEX: DIAMETER: 18 MM; THREAD: M18-1.5; MATERIAL: STEEL; GRADE: X20CR13V; OEM P/N: 9136-014, OEM: GE STEAM POWER SERVICE; FOR INNER CASING TEMP MEASUREMENT","EA",50,null,0]
["0759268","NUT, HEX: DIAMETER: 12 MM; THREAD: M12-1.75; MATERIAL: STEEL; GRADE: X20CR13V; OEM P/N: 9136-013, OEM: GE STEAM POWER SERVICE; FOR INNER CASING TEMP MEASUREMENT","EA",50,null,0]
["0759340","NUT, SLOTTED: TYPE: CASTLE; DIAMETER: 64 MM; THREAD: M64; MATERIAL: STEEL; GRADE: 56T5V; OEM P/N: 5120-055, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51200-0041; FOR HP CV UNIT 5 AND 6","EA",50,null,0]
["0759344","NUT, HEX: DIAMETER: 20 MM; THREAD: M20-2.5; MATERIAL: STEEL; GRADE: 56T5V; OEM P/N: 5120-066, OEM: GE STEAM POWER SERVICE; FOR HP CV UNIT 5 AND 6","EA",50,null,0]
[]
[{"$nulls":4},"Sub-total"]

{"sheet":"Bolts","index":2,"n_rows":291,"n_cols":6,"rows_kept":291}
["Material","Text","Unit","Quantity","Price","Total"]
["0001985","BOLT, ANCHOR: TYPE: RAW LOOSE; DIAMETER: M6; THREAD LENGTH: 50 MM; MATERIAL: STL; LENGTH: 58 MM; THREAD: 1 MM; REFERENCE NO: C19; 48MM SHIELD LENGTH INDLUCING NUT, 12MM MAXIMUM FIXING THICKNESS, DRILL SIZE 12MM","EA",276,null,{"$f":"D2*E2","v":0}]
["0001986","BOLT, ANCHOR: TYPE: RAW LOOSE; DIAMETER: M10; THREAD LENGTH: 75 MM; MATERIAL: STL; LENGTH: 75 MM; THREAD: 1.5 MM; REFERENCE NO: E19; SIZE 60 MM SHIELD LENGTH, 20 MM FIXING THICKNESS, 1.5 MM PITCH, RECOMMENDED DRILL SIZE 18MM","EA",168,null,{"$f":"D3*E3","v":0}]
["0001987","BOLT, ANCHOR: TYPE: RAWL; DIAMETER: M8; THREAD LENGTH: 58 MM; MATERIAL: STL; LENGTH: 65 MM; LOOSE BOLT TYPE, 0MM MIN TO 10MM MAX FIXING THICKNESS, 60MM MIN DEPTH OF HOLE, DRILL SIZE: 14MM, ANCHOR SIZE: DIA 13 X LG 50","EA",166,null,0]
["0025946","BOLT, ASSEMBLY: TYPE: COUPLING; NOMINAL DIAMETER: 31 MM; LENGTH: 114 MM; NUT QUANTITY: 1; BSW","EA",50,null,0]
["0025949","BOLT, ASSEMBLY: NOMINAL DIAMETER: M32; LENGTH: 146 MM; NUT QUANTITY: 1; FLEX COUPLING","EA",50,null,0]
["0025950","BOLT, ASSEMBLY: TYPE: COUPLING; NOMINAL DIAMETER: M27; LENGTH: 130 MM; NUT QUANTITY: 1; FLEX","EA",50,null,0]
["0025953","BOLT: TYPE: COUPLING; DIAMETER: M20; LENGTH: 106 MM; FLEX","EA",50,null,0]
["0025954","BOLT, ASSEMBLY: TYPE: B; NOMINAL DIAMETER: M12; LENGTH: 88 MM; SUPPL P/N: 50-8-5634; FLEX COUPLING PINS COMPLETE WITH NUTS AND WASHERS","EA",50,null,0]
["0039651","BOLT, ANCHOR: TYPE: RAWL; DIAMETER: M8; THREAD LENGTH: 65 MM; MATERIAL: STL; LENGTH: 65 MM; THREAD: 1.25 MM","EA",86,null,0]
["0080624","BOLT, MACHINE: DIAMETER: 3/8 IN; LENGTH: 1 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: BRASS; THREAD: BSW; TYPE: ANCHOR","EA",50,null,0]
["0080679","BOLT, MACHINE: DIAMETER: M10; LENGTH: 50 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: COARSE; SPECIFICATION: SABS 135-1985 TABLE 9; FREE FIT","EA",50,null,0]
["0080748","BOLT, MACHINE: DIAMETER: M20; LENGTH: 45 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS","EA",50,null,0]
["0080929","BOLT, MACHINE: DIAMETER: M6; LENGTH: 80 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS","EA",63,null,0]
["0080946","BOLT, MACHINE: DIAMETER: M12; LENGTH: 150 MM; HEAD: HEX; MATERIAL: STL","EA",50,null,0]
["0082134","BOLT, MACHINE: DIAMETER: M8; LENGTH: 20 MM; HEAD: HEX; MATERIAL: BRASS","EA",50,null,0]
["0082182","BOLT, MACHINE: DIAMETER: M10; LENGTH: 20 MM; HEAD: HEX","EA",50,null,0]
["0083583","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 50 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 50 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; COARSE THREAD FREE FIT, ISOMETRIC; SPECIFICATION: SABS135","KG",731,null,0]
["0083584","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 65 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 40 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; BOLT PROTECTIVE COATING: BLACK; SOLE SOURCE: CLYDE BERGEMANN AFRICA PTY LTD; SPECIFICATION: SABS 135","KG",390,null,0]
["0083585","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 40 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 25 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION SABS 135","KG",212.368,null,0]
["0083586","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 90 MM; HEAD: HEX; MATERIAL: MS; THREAD: 2 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",350,null,0]
["0083599","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 50 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 33 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",50,null,0]
["0083600","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 55 MM; HEAD: HEX; MATERIAL: MS; THREAD: 2.5 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS135","KG",100,null,0]
["0083601","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 65 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 50 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",146,null,0]
["0083603","BOLT, MACHINE: DIAMETER: 3/8 IN; LENGTH: 1-1/2 IN; HEAD: HEX; MATERIAL: BRASS; THREAD: 16BSW; SPECIFICATION: BS 1083; COPPER ALLOY, 56000PSI TS MIN, THREAD IN ACCORDANCE WITH BS84 CLASS 2A","EA",50,null,0]
["0083604","BOLT, MACHINE: DIAMETER: 3/8 IN; LENGTH: 2 IN; HEAD: HEX; MATERIAL: BRASS; THREAD: 16BSW-2A; SPECIFICATION: BS 1083; COPPER ALLOY; 56000PSI TS MIN, THREAD IN ACCORDANCE WITH BS84","EA",50,null,0]
["0083608","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1/2 IN; LENGTH: 3 IN; HEAD: HEX; MATERIAL: BRASS; THREAD: 12BSW; NUT QUANTITY: 1; IN ACCORDANCE WITH BS 84 CLASS 2A; SPECIFICATION: BS1083","EA",82,null,0]
["0083609","BOLT, MACHINE","EA",50,null,0]
["0083610","BOLT, MACHINE","EA",50,null,0]
["0083611","BOLT, MACHINE: DIAMETER: 5/8 IN; LENGTH: 3 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSW; FOR USE ON AUXILIARY PLANT, 112000 PSI TS MIN 89600 PSI YS MIN PROOF LOAD: 85120 PSI MIN, DOUBLE HEAT TREATED, THREAD TO B584 MEDIUM","EA",50,null,0]
["0083612","BOLT, MACHINE","EA",50,null,0]
["0083614","BOLT, MACHINE: DIAMETER: 5/8 IN; LENGTH: 4 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSW","EA",50,null,0]
["0083615","BOLT, MACHINE","EA",50,null,0]
["0083616","BOLT, MACHINE","EA",50,null,0]
["0083617","BOLT, MACHINE","EA",50,null,0]
["0083618","BOLT, MACHINE","EA",50,null,0]
["0083619","BOLT, MACHINE","EA",50,null,0]
["0083620","BOLT, MACHINE: DIAMETER: 7/8 IN; LENGTH: 2-1/2 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSW","EA",50,null,0]
["0083621","BOLT, MACHINE: DIAMETER: 7/8 IN; LENGTH: 3-3/4 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSW","EA",50,null,0]
["0083622","BOLT, MACHINE: DIAMETER: 7/8 IN; LENGTH: 4-1/2 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSW; THREAD LENGTH: 2-1/2 IN","EA",50,null,0]
["0083624","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 25 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 22 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",50,null,0]
["0083626","BOLT, ASSEMBLY: TYPE: FINISHED; NOMINAL DIAMETER: M20; LENGTH: 60 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS BLACK; THREAD LENGTH: 50 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; TYPE THREADED, SPECIFICATION SABS 135","KG",50,null,0]
["0083629","BOLT, ASSEMBLY","EA",50,null,0]
["0083630","BOLT, ASSEMBLY","EA",55,null,0]
["0083631","BOLT, MACHINE","EA",50,null,0]
["0083632","BOLT, MACHINE","EA",50,null,0]
["0083633","BOLT, MACHINE","EA",50,null,0]
["0083634","BOLT, MACHINE","EA",50,null,0]
["0083635","BOLT, MACHINE","EA",50,null,0]
["0083636","BOLT, MACHINE","EA",50,null,0]
["0083637","BOLT, MACHINE","EA",50,null,0]
["0083638","BOLT, MACHINE","EA",50,null,0]
["0083639","BOLT, MACHINE","EA",50,null,0]
["0083640","BOLT, MACHINE","EA",50,null,0]
["0083641","BOLT, ASSEMBLY","EA",50,null,0]
["0083642","BOLT, MACHINE: DIAMETER: 7/8 IN; LENGTH: 4.68 IN; MATERIAL: STL; THREAD: BSW; SHOULDER","EA",50,null,0]
["0083643","BOLT, MACHINE: DIAMETER: 1-1/4 IN; LENGTH: 7-3/4 IN; MATERIAL: STL; THREAD: BSW; SHOULDER","EA",50,null,0]
["0083644","BOLT, MACHINE: DIAMETER: 1-3/4 IN; LENGTH: 11.62 IN; MATERIAL: STL; THREAD: BSW; SHOULDER","EA",50,null,0]
["0083673","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 90 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD LENGTH: 50 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: HTS; NUT GRADE: 8.8; SPECIFICATION: SABS 136","EA",50,null,0]
["0083681","BOLT, MACHINE: DIAMETER: 3/8 IN; LENGTH: 2 IN; HEAD: HEX; GRADE: S; MATERIAL: HTS; THREAD: 16UNC-2A, BS 1580; SPECIFICATION: SABS 646; BS 1768; 50-60 TS","EA",50,null,0]
["0083683","BOLT, MACHINE: DIAMETER: 5/8 IN; LENGTH: 2 IN; HEAD: HEX; GRADE: S; MATERIAL: HTS; THREAD: 11UNC-2A, BS 1580; 50-60 TS","EA",50,null,0]
["0083684","BOLT, MACHINE: DIAMETER: 3/4 IN; LENGTH: 2 IN; HEAD: HEX; MATERIAL: HTS; THREAD: UNC","EA",50,null,0]
["0083692","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1-1/2 IN; LENGTH: 6-1/2 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSW; NUT MATERIAL: HTS","EA",62,null,0]
["0083716","BOLT, MACHINE: DIAMETER: M24; LENGTH: 150 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: 3 MM; SPECIFICATION: DIN 931; 65/75 TON","EA",50,null,0]
["0083946","BOLT: DIAMETER: M20; LENGTH: 100 MM; MATERIAL: GR EN8; CONDENSOR","EA",50,null,0]
["0083975","BOLT, ASSEMBLY: TYPE: COUPLING; NOMINAL DIAMETER: M12; LENGTH: 36 MM; HEAD: HEX; MATERIAL: STL; THREAD: 1.75 MM; NUT QUANTITY: 1; TAPERLOCK WITH WASHER","EA",50,null,0]
["0084025","BOLT: TYPE: POWER PISTON HP BLED VALVE","EA",50,null,{"$f":"D67*E67","v":0}]
["0084119","BOLT, ASSEMBLY: NOMINAL DIAMETER: M30; LENGTH: 110 MM; HEAD: HEX; MATERIAL: MS; THREAD: 3.5 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; ISO METRIC,COARSE THREAD FREE FIT,BEARING THE SABS MARK OF APPROVAL; SPECIFICATION: SABS135","EA",50,null,0]
["0084210","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 60 MM; HEAD: HEX; MATERIAL: MS; THREAD: 2 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; ISO METRIC, COARSE THREAD FREE FIT, TO THE LATEST EDITION OF SABS135 AND BEARING THE SABS MARK OF APPROVAL; SPECIFICATION: SABS135","KG",146,null,0]
["0084331","BOLT, MACHINE: DIAMETER: M24; LENGTH: 80 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: STL; THREAD: 3 MM; TYPE: VALVE; OEM P/N: 7360-109; 7160-109; FOR EMERGENCY STOP VALVE SERVO; TYPE: VALVE","EA",50,null,0]
["0084378","BOLT, MACHINE","EA",50,null,0]
["0084388","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1/2 IN; LENGTH: 1-1/2 IN; HEAD: HEX; MATERIAL: MS; THREAD: 16BSF; NUT QUANTITY: 1; SOLE SOURCE: CLYDE BERGEMANN AFRICA PTY LTD; SPECIFICATION: BS1083","EA",50,null,0]
["0084417","BOLT, MACHINE","EA",50,null,0]
["0084418","BOLT, MACHINE","EA",50,null,0]
["0084419","BOLT, MACHINE","EA",50,null,0]
["0084420","BOLT, MACHINE","EA",55,null,0]
["0084421","BOLT, MACHINE","EA",50,null,0]
["0084422","BOLT, MACHINE","EA",50,null,0]
["0084423","BOLT, MACHINE","EA",50,null,0]
["0084424","BOLT, ASSEMBLY","EA",50,null,0]
["0084426","BOLT, MACHINE: DIAMETER: 3/4 IN; LENGTH: 6 IN; HEAD: HEX; MATERIAL: HTS; THREAD: BSF","EA",50,null,0]
["0084427","BOLT, MACHINE","EA",50,null,0]
["0084428","BOLT, MACHINE","EA",50,null,0]
["0084429","BOLT, MACHINE","EA",50,null,0]
["0084430","BOLT, MACHINE","EA",50,null,0]
["0084431","BOLT, MACHINE","EA",50,null,0]
["0084432","BOLT, MACHINE","EA",50,null,0]
["0084433","BOLT, MACHINE","EA",50,null,0]
["0084434","BOLT, MACHINE: DIAMETER: 1 IN; LENGTH: 6 IN; HEAD: HEX; MATERIAL: MS BRIGHT; THREAD: 10BSF; SPECIFICATION: BS 1083-1965; 28 TON F/IN SQ TS MEDIUM FIT","EA",50,null,0]
["0084536","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 45 MM; HEAD: HEX; MATERIAL: MS; THREAD LENGTH: 25 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; BOLT PROTECTIVE COATING: BLACK; COARSE THREATED, FREE FIT, SPECIFICATION: SABS 135","KG",101,null,0]
["0084539","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 85 MM; HEAD: HEX; MATERIAL: MS; THREAD: 2.5 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK","KG",175,null,0]
["0084563","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M10; LENGTH: 50 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 30 MM; THREAD: 1.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",155,null,0]
["0084565","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M10; LENGTH: 75 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 28 MM; THREAD: 1.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",75,null,0]
["0084571","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 25 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 25 MM; THREAD: 1.75 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; BOLT PROTECTIVE COATING: BLACK; COARSE THREAD FREE FIT; SPECIFICATION: SABS 135","KG",160,null,0]
["0084572","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 40 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 30 MM; THREAD: 1.75 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",75,null,0]
["0084573","BOLT, ASSEMBLY: NOMINAL DIAMETER: M12; LENGTH: 45 MM; HEAD: HEX; MATERIAL: MS; THREAD: 1.75 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS135: 1985","KG",1135,null,0]
["0084575","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 65 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 33 MM; THREAD: 1.75 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",139,null,0]
["0084578","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 100 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 35 MM; THREAD: 1.75 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",125,null,0]
["0084582","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 150 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS BLACK; THREAD LENGTH: 35 MM; THREAD: 1.75 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION SABS 135, COARSE THREAD FREE FIT","KG",50,null,0]
["0084589","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 75 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 38 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",335,null,0]
["0084590","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 100 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 40 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",450,null,0]
["0084593","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M16; LENGTH: 150 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 45 MM; THREAD: 2 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION SABS 135","KG",50,null,0]
["0084600","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 75 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 48 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",600,null,0]
["0084601","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 100 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 55 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",170,null,0]
["0084603","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 125 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 50 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS1 35","KG",150,null,0]
["0084605","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 150 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 55 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",151,null,0]
["0084613","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M24; LENGTH: 100 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 57 MM; THREAD: 3 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; COARSE THREAD FREE FIT.; SPECIFICATION: SABS 135","KG",980,null,0]
["0084614","BOLT, ASSEMBLY: NOMINAL DIAMETER: M24; LENGTH: 115 MM; HEAD: HEX; MATERIAL: MS; THREAD: 3 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",100,null,0]
["0084618","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M6; LENGTH: 25 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 23 MM; THREAD: 1 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",109.25,null,0]
["0084620","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M6; LENGTH: 40 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 20 MM; THREAD: 1 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",123,null,0]
["0084684","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M24; LENGTH: 50 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 40 MM; THREAD: 3 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS 135","KG",50,null,0]
["0084685","BOLT, ASSEMBLY: NOMINAL DIAMETER: M24; LENGTH: 65 MM; HEAD: HEX; MATERIAL: MS; THREAD: 3 MM; NUT QUANTITY: 1; BOLT PROTECTIVE COATING: BLACK; SPECIFICATION: SABS135","KG",50,null,0]
["0084686","BOLT, ASSEMBLY: NOMINAL DIAMETER: M30; LENGTH: 75 MM; HEAD: HEX; MATERIAL: MS; THREAD: 3.5 MM; BOLT PROTECTIVE COATING: BLACK; NUTS IN 25KG BAGS","KG",100,null,0]
["0084706","BOLT: TYPE: HP CYLINDER; DIAMETER: M48; LENGTH: 209 MM; HP OUTER CYLINDER, C-W MEASURING INSERT STUDS","EA",50,null,0]
["0084707","BOLT: DIAMETER: M48; LENGTH: 275 MM; C-W MEASURING INSERT","EA",50,null,0]
["0084709","BOLT: DIAMETER: M64; LENGTH: 364 MM; C-W MEASURING INSERT STUD, BOX 1 AND 2","EA",50,null,0]
["0084712","BOLT: TYPE: HP INNER CYLINDER; C-W MEASURING INSERT, HRZ72 JOINT P/S, SPECIAL STUDS, 100M X 664.5MM","EA",50,null,0]
["0084714","BOLT, MACHINE: DIAMETER: M120; SUPPL P/N: 011 ITA1; HEADED","EA",50,null,0]
["0084717","BOLT: TYPE: FIXING; DIAMETER: M12; LENGTH: 115 MM","EA",50,null,0]
["0084718","BOLT, MACHINE: DIAMETER: M24; LENGTH: 135 MM; KM","EA",50,null,0]
["0084719","BOLT: TYPE: IMPELLER","EA",50,null,0]
["0084723","BOLT: TYPE: SUSPENSION; LODGE COTTRELL PRECIPITATOR","EA",50,null,0]
["0084724","BOLT, MACHINE: DIAMETER: M20; LENGTH: 125 MM; HEAD: HEX","EA",50,null,0]
["0085049","BOLT, MACHINE: DIAMETER: 1 IN; LENGTH: 4 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: BSF","EA",50,null,0]
["0085428","STUD: TYPE: BOLT; DIAMETER: M80; THREAD: 6 MM; LENGTH: 480 MM; MATERIAL: STEEL; THREAD LENGTH: 160 MM; OEM P/N: 2450-016, OEM: GE STEAM POWER SERVICE; DRAWING NO: 2450-016 REV 0; 06.06386-6202 REV 0; FOR HP INNER CASING","EA",50,null,0]
["0085436","BOLT, MACHINE: DIAMETER: 7/8 IN; LENGTH: 4 IN; HEAD: SQ; GRADE: 8.8; MATERIAL: HTS; THREAD: 9BSW","EA",50,null,0]
["0085496","BOLT, MACHINE: DIAMETER: M12; LENGTH: 65 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: 1.75 MM; SPECIFICATION: DIN 931","EA",62,null,0]
["0085674","BOLT, MACHINE","EA",50,null,0]
["0085676","BOLT, MACHINE: DIAMETER: M30; LENGTH: 48 MM; FEEDBACK VALVE","EA",50,null,0]
["0085677","BOLT, MACHINE: DIAMETER: M34; LENGTH: 12 MM; FEEDBACK VALVE","EA",50,null,0]
["0085678","BOLT, ASSEMBLY: NOMINAL DIAMETER: M6; LENGTH: 15 MM; HEAD: HEX; MATERIAL: MS BRIGHT; FEED BK VALVE, HEAD WITH NUTS FITTED IN","EA",50,null,{"$f":"D131*E131","v":0}]
["0085679","BOLT: TYPE: MAIN STEAM EMERGENCY VALVE","EA",50,null,0]
["0085681","BOLT, MACHINE: DIAMETER: 1-1/2 IN; LENGTH: 7 IN; HEAD: HEX; MATERIAL: STL; THREAD: BSW; SPECIALS BRAND, MACHINED","EA",54,null,0]
["0085682","BOLT, MACHINE: DIAMETER: M24; LENGTH: 60 MM; HEAD: HEX; MATERIAL: HTS; H/RND","EA",50,null,0]
["0085683","BOLT, MACHINE","EA",50,null,0]
["0108587","BOLT, ANCHOR: TYPE: RAWL; DIAMETER: M12; MATERIAL: STL; LENGTH: 90 MM; THREAD: 1.75 MM; SUPPL P/N: G20; REFERENCE NO: LH1290; 20MM DRILL SIZE, 19MM X 73MM ANCHOR SIZE, TYPE: LOOSE BOLT","EA",90,null,0]
["0108762","BOLT: LENGTH: 100 MM; HEAD: RD; MATERIAL: STL; PROTECTIVE COATING: GALV; PAD, (101.6MM LONG ACCEPTABLE )","EA",134,null,0]
["0183410","BOLT: TYPE: LINER; DIAMETER: M12; LENGTH: 35 MM; FOR USE ON PA AND SEAL AIR FANS,BOILER 8-10","EA",59,null,0]
["0224512","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 90 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: STL; NUT QUANTITY: 1; NUT MATERIAL: HTS; NUT GRADE: 8.8; C\\W 2 WASHERS; SPECIFICATION SABS135","EA",615,null,0]
["0224513","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 100 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: STL; THREAD: 2.5 MM; NUT QUANTITY: 1; NUT MATERIAL: HTS; NUT GRADE: 8.8; WASHER; SPECIFICATION: SABS135 AND 2 WASHERS","EA",250,null,0]
["0225472","BOLT, MACHINE: DIAMETER: M20; LENGTH: 120 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: STL; THREAD: 2.5 MM; SPECIFICATION: SABS 135; TYPE: GENERAL PURPOSE","KG",100,null,0]
["0225665","BOLT, MACHINE: DIAMETER: M12; LENGTH: 50 MM; HEAD: HEX; GRADE: 4.8; MATERIAL: MS; THREAD: 1.75 MM; SPECIFICATION: SABS 136; PROTECTIVE COATING: BLACK; TYPE: GENERAL PURPOSE","KG",325,null,0]
["0227262","BOLT, T: DIAMETER: M20; LENGTH: 120 MM; MATERIAL: STAINLESS STEEL; FOR USE ON SLUICE PUMP","EA",50,null,0]
["0227397","BOLT: DIAMETER: M16; LENGTH: 75 MM; HEAD: HEX; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT","EA",50,null,0]
["0227398","BOLT, MACHINE: DIAMETER: M20; LENGTH: 125 MM; HEAD: HEX; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT","EA",65,null,0]
["0227399","BOLT, MACHINE: DIAMETER: M20; LENGTH: 150 MM; HEAD: HEX; MATERIAL: SS GR 316; FOR USE ON COMMON PLANT","EA",62,null,0]
["0230391","BOLT, EYE: TYPE: COLLAR; DIAMETER: 3/4 IN; MATERIAL: STL DROP FORGED; DRAWING NO: 3/7418/71 REV 1; FOR 8.5E BALL MILL","EA",52,null,0]
["0230812","BOLT, MACHINE: DIAMETER: M12; HEAD: SQ; REFERENCE NO: RS 120 A; BALL DIAMETER 20MM, USED AS A 1- PHASE EARTHING DEVICE; TYPE: EARTH BALL","EA",50,null,0]
["0231777","BOLT: TYPE: SHOULDER; DIAMETER: 1.14 AF IN; LENGTH: 3.3/8 IN; HEAD: HEX; GRADE: DPSC M32; MATERIAL: CARBON STEEL; SUPPL P/N: 309428-0116; THREADED 3/4 - 10 FOR 1.1/4 INCH; SHOULDER DIA 0.9925 INCH +/-O.OO25 INCH; FOR USE ON IK545 CAM AND ARM ASSY ON SOOTBLOWER","EA",50,null,0]
["0233033","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 5/8 IN; LENGTH: 1-3/4 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; FOR USE ON BOILER 2 MILL, WITH WASHER, SANS1700; THREADS 2 PITCH","EA",50,null,0]
["0233035","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 3/4 IN; LENGTH: 1-3/4 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: 2.5 MM; NUT QUANTITY: 1; FOR USE ON BOILER 2 MILL, WITH WASHER, SANS 1700","EA",50,null,0]
["0233040","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 1 IN; LENGTH: 2-1/4 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: 3 MM; NUT QUANTITY: 1; FOR USE ON BOILER 2 MILL, SANS1700","EA",70,null,0]
["0233041","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 1 IN; LENGTH: 3-1/4 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; FOR USE ON BOILER 2;, WITH WASHER, SANS1700; THREADS: 3 PITCH","EA",50,null,0]
["0233045","BOLT: DIAMETER: M16; LENGTH: 45 MM; GRADE: 8.8; SPECIFICATION: SANS 1700; FOR USE ON BOILER 2 MILL, SANS 1700","EA",50,null,0]
["0233047","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 55 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; NUT GRADE: 8.8; C\\W 2 WASHERS","EA",350,null,0]
["0233048","BOLT, ASSEMBLY: NOMINAL DIAMETER: M30; LENGTH: 100 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; COME WITH TWO WASHERS","EA",273,null,0]
["0233049","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 60 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; C\\W 2 WASHERS","EA",170,null,0]
["0233052","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 1-1/2 IN; LENGTH: 5-1/2 IN; GRADE: 8.8; FOR USE ON BOILER 2 MILL, WITH 2 FLAT WASHER, SANS1700","EA",50,null,0]
["0233053","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 2 IN; LENGTH: 4-1/2 IN; GRADE: 8.8; FOR USE ON BOILER 2 MILL, WITH FLAT WASHER, SANS1700","EA",50,null,0]
["0233055","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 50 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; COME WITH TWO WASHERS","EA",410,null,0]
["0233056","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 70 MM; HEAD: HEX; GRADE: 8.8; NUT MATERIAL: HTS; C\\W 2 WASHERS","EA",50,null,0]
["0233057","BOLT, ASSEMBLY: NOMINAL DIAMETER: M12; LENGTH: 40 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE MILL, FOR USE ON BOILER 2 MILL, 2 FLAT WASHER AND SPRING WASHER, SANS 1700","EA",575,null,0]
["0233058","BOLT, ASSEMBLY: NOMINAL DIAMETER: M10; LENGTH: 30 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; SPECIFICATION SABS136, FOR USE ON BOILER 2 MILL, WITH 2 FLAT WASHER AND SPRING WASHER, SANS 1700","EA",620,null,0]
["0233059","BOLT, ASSEMBLY: NOMINAL DIAMETER: M12; LENGTH: 80 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; FOR USE ON BOILER 2 MILL, 2 WASHER AND SPRING WASHER","EA",50,null,0]
["0233060","BOLT, ASSEMBLY: NOMINAL DIAMETER: M12; LENGTH: 50 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE MILL, FOR USE ON BOILER 2 MILL, 2 FLAT WASHER AND SPRING WASHER, SANS 1700","EA",450,null,0]
["0233061","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 90 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: STL; NUT QUANTITY: 1; NUT MATERIAL: STL; C\\W 2 FLAT WASHERS","EA",1850,null,0]
["0233062","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 70 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; NUT GRADE: 8.8; C\\W 2 WASHERS","EA",450,null,0]
["0233618","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: 5/8 IN; LENGTH: 1-3/4 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; FOR USE ON BOILER MILL REFURBISHMENT, THREADS: 0.8MM","EA",50,null,0]
["0233621","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M6; LENGTH: 15 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1 MM; NUT QUANTITY: 1; FOR USE ON BOILER MILL REFURBISHMENT","KG",99,null,0]
["0233625","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M10; LENGTH: 15 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1.5 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",450,null,0]
["0233626","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M10; LENGTH: 30 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1.5 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",50,null,0]
["0233627","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M10; LENGTH: 45 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1.5 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",985,null,0]
["0233631","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 20 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1.75 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",70,null,0]
["0233633","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 45 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1.75 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",185,null,0]
["0233640","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 40 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 2.5 MM; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE","EA",626,null,0]
["0233641","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 55 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD LENGTH: 40 MM; THREAD: 2.5 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",50,null,0]
["0233654","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 45 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; C/W TWO WASHERS","EA",450,null,0]
["0233655","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 50 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; C/W TWO WASHERS","EA",2410,null,0]
["0233656","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 70 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; NUT MATERIAL: HTS; NUT GRADE: 8.8; C/W TWO WASHERS","EA",449,null,0]
["0233657","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 60 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; C/W TWO WASHERS","EA",6150,null,0]
["0233658","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 40 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE, C/W TWO WASHERS","EA",1280,null,0]
["0233659","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 35 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE, C/W TWO WASHERS","EA",1547,null,0]
["0233660","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 30 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE, C/W TWO WASHERS","EA",325,null,0]
["0233661","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 30 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; FOR MAINTENANCE USE, C/W TWO WASHERS","EA",537,null,0]
["0233662","BOLT, ASSEMBLY: NOMINAL DIAMETER: M12; LENGTH: 35 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, SPECIFICATION SABS 136, FOR MAINTENANCE USE, WITH 2 WASHER AND SPRING WASHER","EA",2240,null,0]
["0233663","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M12; LENGTH: 40 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 1.75 MM; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; FOR MAINTENANCE USE, C/W TWO WASHERS","EA",50,null,0]
["0233664","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 65 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE, C/W TWO WASHERS","EA",100,null,0]
["0233665","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 95 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE, C/W TWO WASHERS","EA",720,null,0]
["0233666","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 35 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE, C/W TWO WASHERS","EA",450,null,0]
["0233670","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: 1/2 IN; HEAD: HEX; GRADE: 4.6; THREAD: 0.7 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE, C/W TWO WASHERS","EA",50,null,0]
["0233671","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 80 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 2.5 MM; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE","EA",650,null,0]
["0233672","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M20; LENGTH: 100 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 2.5 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",110,null,0]
["0233677","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M24; LENGTH: 60 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 3 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",50,null,0]
["0233678","BOLT, ASSEMBLY: NOMINAL DIAMETER: M24; LENGTH: 80 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 3 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","EA",50,null,0]
["0233689","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 120 MM; HEAD: HEX; MATERIAL: MS; THREAD: 2.5 MM; NUT QUANTITY: 1; TYPE GENERAL PURPOSE, FOR MAINTENANCE USE","KG",150,null,{"$f":"D195*E195","v":0}]
["0233690","BOLT, ASSEMBLY: TYPE: GENERAL PURPOSE; NOMINAL DIAMETER: M24; LENGTH: 120 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 3 MM; NUT QUANTITY: 1; FOR MAINTENANCE USE","KG",200,null,0]
["0233691","BOLT, ASSEMBLY: TYPE: MILL; NOMINAL DIAMETER: 5/8 IN; LENGTH: 1 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; FOR USE ON BOILER; REFURBISHMENT, C/W WASHER; THREADS: 0.8MM","EA",50,null,0]
["0234770","BOLT, ASSEMBLY: TYPE: RETAINING; NOMINAL DIAMETER: 3/4 IN; LENGTH: 3 IN; HEAD: HEX; MATERIAL: HTS; NUT QUANTITY: 1; DRAWING NO: FC 572 REV 1; FC 572 REV B REV 1; REFERENCE NO: KA 1832; WASHER AS PER DRAWING, REQUIRED FOR UNITS 1, 2, 3, 4 AND 6 ASH HOPPER DOORS","EA",50,null,0]
["0234941","BOLT, ASSEMBLY: TYPE: FIXING; NOMINAL DIAMETER: 3/8 IN; LENGTH: 3-1/2 IN; HEAD: HEX; MATERIAL: HTS; NUT QUANTITY: 1; SUPPL P/N: FC 407 C; DRAWING NO: FC 407 REV 1; FOR ASH HOPPER DOORS, UNITS 1, 2, 3, 4 AND 6, C/W WASHER","EA",50,null,0]
["0234944","BOLT, ASSEMBLY: TYPE: FIXING; NOMINAL DIAMETER: 3/4 IN; LENGTH: 3 IN; HEAD: HEX; MATERIAL: HTS; NUT QUANTITY: 1; SUPPL P/N: FC 407 F; DRAWING NO: FC 407 REV 1; FOR ASH HOPPER DOORS, UNITS 1, 2, 3, 4 AND 6, C/W WASHER","EA",50,null,0]
["0235997","BOLT, ASSEMBLY: TYPE: DOOR; NOMINAL DIAMETER: 5/8 IN; LENGTH: 1-3/4 IN; MATERIAL: BRASS; NUT QUANTITY: 1; DRAWING NO: KA 1773 REV 1; FOR USE ON ASH HOPPER DOOR, UNITS 1, 2, 3, 4 AND 6","EA",56,null,0]
["0235999","BOLT, MACHINE: DIAMETER: 5/8 IN; LENGTH: 1-3/4 IN; HEAD: 5 Q; MATERIAL: BRASS; DRAWING NO: ON 190 A REV 1; TYPE: DOOR; FOR USE ON ASH HOPPER DOOR, UNITS 1, 2, 3, 4 AND 6","EA",50,null,0]
["0236000","BOLT, ASSEMBLY: TYPE: DOOR; NOMINAL DIAMETER: 1/2 IN; LENGTH: 1-1/2 IN; MATERIAL: BRASS; NUT QUANTITY: 1; DRAWING NO: ON 190 C REV 1; FOR USE ON ASH HOPPER DOOR, UNITS 1, 2, 3, 4 AND 6","EA",50,null,0]
["0236003","BOLT, ASSEMBLY: TYPE: DOOR; NOMINAL DIAMETER: 3/4 IN; LENGTH: 3-1/4 IN; MATERIAL: BRASS; DRAWING NO: ON 190 F REV 1; FOR USE ON ASH HOPPER;, UNITS 1, 2, 3, 4 AND 6, COMPLETE WITH LOCK WASHER","EA",50,null,0]
["0236397","BOLT, ASSEMBLY: NOMINAL DIAMETER: M12; LENGTH: 70 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; SPECIFICATION: SABS136; FOR USE ON MILLS, WITH 2 WASHER, SPRING WASHER","EA",50,null,0]
["0236398","BOLT, ASSEMBLY: NOMINAL DIAMETER: M20; LENGTH: 110 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; SPECIFICATION: SABS136; FOR USE ON MILLS, WITH 2 WASHERS, SPRING WASHER","EA",500,null,0]
["0236399","BOLT, ASSEMBLY: NOMINAL DIAMETER: M16; LENGTH: 65 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; C\\W 2 WASHERS","EA",386,null,0]
["0236400","BOLT, ASSEMBLY: NOMINAL DIAMETER: M24; LENGTH: 60 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; NUT QUANTITY: 1; SPECIFICATION: SABS136; TYPE: MILL; COME WITH 2 WASHERS","EA",90,null,0]
["0236401","BOLT, ASSEMBLY: NOMINAL DIAMETER: 3/4 IN; LENGTH: 1-1/2 IN; HEAD: HEX; MATERIAL: HTS; THREAD: 10 TPI; NUT QUANTITY: 1; SPECIFICATION SABS136; FOR USE ON MILLS, WITH FLAT WASHER, SPRING WASHER","EA",100,null,0]
["0236402","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1 IN; LENGTH: 2 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: 8 TPI; NUT QUANTITY: 1; SPECIFICATION: SABS136; TYPE: MILL; WITH FLAT WASHER, SPRING WASHER","EA",86,null,0]
["0236403","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1/2 IN; LENGTH: 1-1/2 IN; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; THREAD: 12BSW; NUT QUANTITY: 1; SPECIFICATION: SABS136; TYPE: MILL; WITH FLAT WASHER, SPRING WASHER","EA",50,null,0]
["0236404","BOLT, ASSEMBLY: NOMINAL DIAMETER: M10; LENGTH: 80 MM; HEAD: HEX; MATERIAL: HTS; THREAD: 1.5 MM; NUT QUANTITY: 1; SPECIFICATION: SABS136; TYPE: MILL; WITH FLAT WASHER, SPRING WASHER","EA",90,null,0]
["0238846","BOLT, ASSEMBLY: NOMINAL DIAMETER: M24; LENGTH: 70 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: HTS; SUPPL P/N: NOV0024A1; COME WITH TWO WASHERS","KG",75,null,0]
["0239962","BOLT: TYPE: COUPLING; SUPPL P/N: MS 15/M393; MODEL NO: M/P8INX8INX24IN; FOR USE ON COUPLING REFERENCE 21795P-1 GV, TO BE SUPPLIED IN SETS OF SIX BOLTS AND BUSHES PACKED AS A SET AND CLEARY MARKED, FOR USE ON 100 PCT CONDENSATE EXTRACTION PUMP","EA",50,null,0]
["0240249","SET: TYPE: COUPLING BOLT; COMPRISING: BUSHES RUBBER; FLAT WASHER; NUT; SPRING WASHER; SUPPL P/N: MS 15/M393; FOR 100PCT CONDENSATE EXTRACTION PUMP","EA",50,null,0]
["0240372","BOLT: TYPE: STEM LOCK; DRAWING NO: F42.592595-0196 REV 1; FOR CONTROL VALVE COUPLING, GROUP NO.5126, UNITS 1-4, 6","EA",50,null,0]
["0240957","BOLT: TYPE: TURNING GEAR; DRAWING NO: C42.94303-0007 REV 1; REQUIRE FOR LATCHES ON MAIN TURBINE BARRING, RENK SSS-D7, GROUP 9439","EA",50,null,0]
["0241385","BOLT: TYPE: COUPLING; DRAWING NO: F42.592595-0104 REV 1; REQUIRED FOR CONTROL VALVE STEM LOCK, GROUP NO 5126, UNIT 5","EA",50,null,0]
["0247368","BOLT, ASSEMBLY: NOMINAL DIAMETER: 7/8 IN; LENGTH: 3-1/2 IN; DRAWING NO: D2861 REV 1; REQUIIRED FOR USE ON FD FANS, BOILERS 1 TO 4 & 6, RVC ROLLER COMPLETE WITH NUT & WASHER, AS PER DRAWING","EA",50,null,0]
["0247743","BOLT, ASSEMBLY: TYPE: RETAINING; NOMINAL DIAMETER: M5; LENGTH: 40 MM; HEAD: HEX; MATERIAL: STL; THREAD LENGTH: 38 MM; THREAD: 5 MM; NUT MATERIAL: STL; REQUIRED FOR USE TO TIGHTEN THE LUGS ON MOTOR TERMINALS, COMPLETE WITH NUTS AND WASHERS, WASHER OD 9MM X ID 5.5MM X THK 1 MM","EA",87,null,0]
["0248597","BOLT: TYPE: TABLE HOLD DOWN; DIAMETER: M48; LENGTH: 470 MM; MATERIAL: EN9; REQUIRED FOR USE ON UNIT 5, LOESCHE MILLING PLANT","EA",50,null,0]
["0248919","BAR: TYPE: BUFFALO BOLT; MANUF P/N: 3427-150-165C; FOR BS20 RFL RECLAIM FEEDER","KG",50,null,0]
["0251492","BOLT, MACHINE: DIAMETER: M20; LENGTH: 25 MM; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: 2.5 MM; THREAD LENGTH: 20 MM","KG",75,null,0]
["0252304","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1/2 IN; LENGTH: 1-1/2 IN; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; NUT QUANTITY: 1; SUPPL P/N: FC591B; THREAD UNC; REQUIRED FOR USE AT ASH HOPPERS, UNIT 1, 2, 3, 4 & 6","EA",50,null,0]
["0252305","BOLT, ASSEMBLY: TYPE: NOZZLE; NOMINAL DIAMETER: 3/4 IN; LENGTH: 2 IN; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; NUT QUANTITY: 1; SUPPL P/N: FC591C; THREAD UNC; REQUIRED FOR USE AT ASH HOPPERS, UNIT 1, 2, 3, 4 & 6","EA",61,null,0]
["0252332","BOLT, ASSEMBLY: TYPE: COVER PLATE; NOMINAL DIAMETER: 3/4 IN; LENGTH: 1-3/4 IN; GRADE: 4.6; MATERIAL: MS; THREAD: UNC; NUT QUANTITY: 1; SUPPL P/N: FC591E; REQUIRED FOR USE AT ASH HOPPERS, UNIT 1, 2, 3, 4 & 6, NUT HRH","EA",65,null,0]
["0252376","BOLT, ASSEMBLY: TYPE: NOZZLE; NOMINAL DIAMETER: 3/4 IN; LENGTH: 2-1/4 IN; GRADE: 4.6; MATERIAL: MS; THREAD: UNC; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; SUPPL P/N: AH552C; REQUIRED FOR USE AT ASH HOPPERS, UNIT 1, 2, 3, 4 & 6","EA",50,null,0]
["0252377","BOLT, ASSEMBLY: TYPE: ROD; NOMINAL DIAMETER: 3/8 IN; LENGTH: 3-1/2 IN; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: UNC; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; SUPPL P/N: KA1819BOLT; REQUIRED FOR USE AT ASH HOPPERS, UNIT 1, 2, 3, 4 & 6","EA",50,null,0]
["0252379","BOLT, EYE: DIAMETER: 16 MM; SHANK LENGTH: 120 MM; THREAD LENGTH: 100 MM; MATERIAL: MS; GRADE: 4.6; SUPPL P/N: DB; THREAD UNC; REQUIRED FOR USE A T ASH HOPPER ACCESS DOOR","EA",50,null,0]
["0252381","BOLT, ASSEMBLY: NOMINAL DIAMETER: 3/4 IN; LENGTH: 2-3/4 IN; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: UNC; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; SUPPL P/N: DN190H~BOLT; REQUIRED FOR USE AT ASH HOPPER, UNIT 1, 2, 3, 4 & 6","EA",50,null,0]
["0252384","BOLT, ASSEMBLY: NOMINAL DIAMETER: 1/2 IN; LENGTH: 1-1/4 IN; HEAD: HEX; GRADE: 4.6; MATERIAL: MS; THREAD: UNC; NUT QUANTITY: 1; NUT MATERIAL: MS; NUT GRADE: 4.6; SUPPL P/N: DN190I; REQUIRED FOR USE AT ASH HOPPER, UNIT 1, 2, 3, 4 & 6","EA",50,null,0]
["0253509","BOLT, MACHINE: DRAWING NO: F42.33794-5116 REV 1; REQUIRED FOR NOZZLE SEGMENT ASSEMBLY, GROUP 3370, ITEM 008","EA",50,null,0]
["0254881","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; LENGTH: 40 MM; HEAD: SOCKET HEX; GRADE: 12.9; MATERIAL: STL ALLOY; THREAD LENGTH: 30 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",200,null,0]
["0254882","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; LENGTH: 80 MM; HEAD: SOCKET HEX; GRADE: 12.9; MATERIAL: STL ALLOY; THREAD LENGTH: 30 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",60,null,0]
["0254883","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; LENGTH: 30 MM; HEAD: SOCKET HEX; GRADE: 12.9; MATERIAL: STL ALLOY; THREAD LENGTH: 30 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",50,null,0]
["0254884","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; LENGTH: 60 MM; HEAD: SOCKET HEX; GRADE: 12.9; MATERIAL: STL ALLOY; THREAD LENGTH: 30 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",159,null,0]
["0254885","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; LENGTH: 50 MM; HEAD: SOCKET HEX; GRADE: 12.9; MATERIAL: STL ALLOY; THREAD LENGTH: 30 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",70,null,0]
["0254896","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; HEAD: HEX; MATERIAL: MS; THREAD LENGTH: 40 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",835,null,0]
["0254897","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; HEAD: HEX; MATERIAL: MS; THREAD LENGTH: 30 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",50,null,0]
["0254898","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; HEAD: HEX; MATERIAL: MS; THREAD LENGTH: 50 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",50,null,0]
["0254899","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; HEAD: HEX; MATERIAL: MS; THREAD LENGTH: 60 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",215,null,0]
["0254900","BOLT, ASSEMBLY: NOMINAL DIAMETER: M8; HEAD: HEX; MATERIAL: MS; THREAD LENGTH: 80 MM; THREAD: 1.25 MM; NUT QUANTITY: 1; NUT MATERIAL: EN8; NUT GRADE: 8; PROTECTIVE COATING: BLACK; WITH MILD STEEL FLAT WASHER","EA",44,null,0]
["0254901","BOLT, U: NOMINAL SIZE: 26.7 MM; DIAMETER: M10; LOAD RATING: 695 KG; INSIDE LENGTH: 53 MM; THREAD LENGTH: 30 MM; THREAD: 1.5 MM; MATERIAL: MS; INSIDE WIDTH: 28 MM; GRADE: 4.8; PROTECTIVE COATING: ZN PLTD; REFERENCE NO: G.C.3538 2; COMPLETE WITH TWO NUTS/TWO WASHERS","EA",83,null,0]
["0254902","BOLT, U: NOMINAL SIZE: 33.4 MM; DIAMETER: M10; LOAD RATING: 695 KG; INSIDE LENGTH: 60 MM; THREAD LENGTH: 30 MM; THREAD: 1.5 MM; MATERIAL: MS; INSIDE WIDTH: 36 MM; GRADE: 4.8; PROTECTIVE COATING: ZN PLTD; REFERENCE NO: G.C.3538 6; COMPLETE WITH TWO NUTS/TWO WASHERS","EA",85,null,0]
["0254903","BOLT, U: NOMINAL SIZE: 42.2 MM; DIAMETER: M10; LOAD RATING: 695 KG; INSIDE LENGTH: 69 MM; THREAD LENGTH: 30 MM; THREAD: 1.5 MM; MATERIAL: MS; INSIDE WIDTH: 44 MM; GRADE: 4.8; PROTECTIVE COATING: ZN PLTD; REFERENCE NO: G.C.3539 3; COMPLETE WITH TWO NUTS/TWO WASHERS","EA",125,null,0]
["0254904","BOLT, U: NOMINAL SIZE: 48.3 MM; DIAMETER: M10; LOAD RATING: 695 KG; INSIDE LENGTH: 75 MM; THREAD LENGTH: 30 MM; THREAD: 1.5 MM; MATERIAL: MS; INSIDE WIDTH: 50 MM; GRADE: 4.8; PROTECTIVE COATING: ZN PLTD; REFERENCE NO: G.C.3539 6; COMPLETE WITH TWO NUTS/TWO WASHERS","EA",104,null,0]
["0254905","BOLT, U: NOMINAL SIZE: 60.3 MM; DIAMETER: M10; LOAD RATING: 695 KG; INSIDE LENGTH: 87 MM; THREAD LENGTH: 30 MM; THREAD: 1.5 MM; MATERIAL: MS; INSIDE WIDTH: 62 MM; GRADE: 4.8; PROTECTIVE COATING: ZN PLTD; REFERENCE NO: G.C.3540 3; COMPLETE WITH TWO NUTS/TWO WASHERS","EA",160,null,0]
["0501163","BOLT: DIAMETER: M64; LENGTH: 350 MM; MATERIAL: X19CRMOVNBN111; OEM P/N: 5120-064, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51200-0041 REV 0; REFERENCE NO: SZT-42-99995-01094; REQUIRED FOR TURBINE HP GOVERNOR VALVES, UNITS 1 - 6, AS PER ALSTOM SERVICES O.E.M. REQUIREMENTS","EA",50,null,0]
["0501167","BOLT: DIAMETER: M20; LENGTH: 80 MM; MATERIAL: X19CRRMOUNBN112; GROUP 5120; ITEM 062; REQUIRED FOR USE ON H.P. GOVERNOR VALVES; UNITS 1 - 6","EA",50,null,0]
["0555632","BOLT: TYPE: NOZZLE BOX ASSEMBLY; OEM P/N: 3390-106, OEM: GE STEAM POWER SERVICE; DRAWING NO: SZT 4299993-00592 REV 0; LOCKING BOLTS FOR USE ON HP TURBINE CENTRELINE; SPARES UNIT'S 1-6; AS PER OEM DRAWING","EA",79,null,0]
["0568582","BOLT, ASSEMBLY: TYPE: TRANSFORMER DROPPERS; NOMINAL DIAMETER: M12; LENGTH: 50 MM; HEAD: HEX; GRADE: 8.8; MATERIAL: MILD STEEL; THREAD LENGTH: 46 MM; THREAD: 1.2 MM; NUT QUANTITY: 1; NUT MATERIAL: MILD STEEL; NUT GRADE: 8.8; PROTECTIVE COATING: GALV; SPECIAL FEATURES: FULL THREAD; BOLT PROTECTIVE COATING: GALV; NUT PROTECTIVE COATING: GALV","EA",50,null,0]
["0600935","BOLT: TYPE: STUD; DIAMETER: M20; LENGTH: 80 MM; HEAD: HEX; MATERIAL: X19CRMOVNBN112; BOLT KM 20X80; GROUP NO:5120; ITEM 062; FOR USE ON HP CONTROL VALVE DV3-6","EA",50,null,0]
["0607968","BOLT: TYPE: HP CASING EXTRACTION; DIAMETER: M24; LENGTH: 160 MM; HEAD: HEX; MATERIAL: 30CRMOV9V; E1E2UE3; GROUP NO: 2410; ITEM 052; ALSTOM SPARES","EA",50,null,0]
["0607975","BOLT: TYPE: HP SHAFT GLAND; DIAMETER: 30 MM; LENGTH: 130 MM; HEAD: HEX; MATERIAL: X19CRMOVNBN111; M30 X 130; ALSTOM SPARES; GROUP NO: 2480; ITEM 010","EA",50,null,0]
["0607976","BOLT: TYPE: HP SHAFT GLAND; DIAMETER: 30 MM; LENGTH: 225 MM; HEAD: HEX; MATERIAL: X19CRMOVNBN111; THREAD: METRIC; M30 X 225; ALSTOM SPARES; GROUP NO: 2480; ITEM 011","EA",50,null,0]
["0607978","BOLT: TYPE: HP DIAPHRAGM CARRIER STG 12/15; DIAMETER: 36 MM; LENGTH: 165 MM; HEAD: HEX; MATERIAL: 34CRNIMO6V; THREAD: METRIC; GROUP NO: 2460; ITEM 066; ALSTOM SPARES","EA",50,null,0]
["0607979","BOLT: TYPE: HP DIAPHRAGM CARRIER STG 14/15; DIAMETER: 36 MM; LENGTH: 235 MM; HEAD: HEX; MATERIAL: 34CRNIMO6V; THREAD: METRIC; ALSTOM SPARES; GROUP NO: 2460; ITEM 067","EA",50,null,0]
["0620802","BOLT: TYPE: STUD; DIAMETER: 1-1/8 IN; LENGTH: 6-1/2 IN; HEAD: HEX; MATERIAL: STL 60; THREAD: BSP; THREAD LENGTH: 40 MM; MANUF P/N: Y30039127; REFERENCE NO: 34245-130; B7 7028 BTC","EA",50,null,0]
["0620806","STUD: TYPE: BOLT; DIAMETER: 3/4 IN; THREAD: BSF; LENGTH: 4-1/2 IN; MATERIAL: STL 60; THREAD LENGTH: 4-1/2 IN; MANUF P/N: Y30039081; REFERENCE NO: 34242-145; 3/4 INCH X 4-1/2 INCH LONG","EA",50,null,{"$f":"D259*E259","v":0}]
["0628066","BOLT: TYPE: STUD; DIAMETER: M24; LENGTH: 135 MM; HEAD: TWO FLATS; THREAD: METRIC; OEM P/N: 3750 / 907; DRAWING NO: C42.377900-0002 REV 0","EA",50,null,0]
["0628182","BOLT, CARRIAGE: DIAMETER: 36 MM; LENGTH: 177 MM; THREAD: METRIC; MATERIAL: STL ALLOY; GRADE: 8.8; OEM P/N: 2460-066, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0006; REFERENCE NO: SZT-42-99995-00975; APPLICATION: HP DIAPHRAGM CARRIER IV; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","EA",50,null,0]
["0628313","BOLT: TYPE: EMERGENCY STOP VALV; DIAMETER: 18 MM; LENGTH: 38 MM; GRADE: 21CRMOV511V; MATERIAL: STEEL ALLOY; OEM P/N: 7120-015, OEM: GE STEAM POWER SERVICE; DRAWING NO: A42.71200-0007; GROOTVLEI 7120-015; HP TURBINE","EA",50,null,0]
["0628379","STUD: TYPE: BOLT; DIAMETER: M24; THREAD: METRIC; LENGTH: 160 MM; MATERIAL: STL ALLOY; OEM P/N: 2410-052, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012 REV 0; REFERENCE NO: SZT-42-99995-00970","EA",50,null,0]
["0628383","STUD: TYPE: BOLT; DIAMETER: M24; THREAD: METRIC; LENGTH: 125 MM; MATERIAL: STL ALLOY; OEM P/N: 2410-055, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24100-0012 REV 0; REFERENCE NO: SZT-42-99995-00972","EA",50,null,0]
["0628429","BRACKET: TYPE: BOLT, SUPPORT; MATERIAL: HEAT RESISTANT; DIMENSIONS: 30 X 220 MM; APPLICATION: CASING; OEM P/N: 2490/057; DRAWING NO: B42.24900-0006 REV 0; REFERENCE NO: SZT-42-99994-00033","EA",50,null,0]
["0630762","BOLT, MACHINE: DIAMETER: 48 MM; LENGTH: 274 MM; HEAD: FLAT; GRADE: 8.8; MATERIAL: STL ALLOY; THREAD: 3.5 MM; TYPE: HP TURBINE; OEM P/N: 2460-007, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0003 REV 0; REFERENCE NO: SZT-42-99995-00973; HP DIAPHRAGM CARRIER I","EA",50,null,0]
["0630847","BOLT: TYPE: STUD; DIAMETER: M24; LENGTH: 110 MM; HEAD: HEX; MATERIAL: STL ALLOY; THREAD: 24 MM; OEM P/N: 3350-906, OEM: GE STEAM POWER SERVICE; REFERENCE NO: SZT-42-99995-00980","EA",50,null,0]
["0632270","BOLT: TYPE: STUD; DIAMETER: M100; LENGTH: 500 MM; HEAD: TWO FLAT; MATERIAL: STL ALLOY; THREAD: 100 MM; OEM P/N: SZT-42-99995-01228; DRAWING NO: 2410-014 REV 0","EA",50,null,0]
["0632272","BOLT: TYPE: STUD; DIAMETER: 120 MM; LENGTH: 800 MM; HEAD: TWO FLAT; MATERIAL: STL ALLOY; THREAD: 120 MM; OEM P/N: SZT-42-99995-01224; DRAWING NO: 2410/008 REV 0","EA",50,null,0]
["0632274","BOLT: TYPE: STUD; DIAMETER: M64; LENGTH: 285 MM; HEAD: TWO FLAT; MATERIAL: STL ALLOY; THREAD: 64 MM; OEM P/N: SZT-42-99995-01230; DRAWING NO: 2410/026 REV 0","EA",50,null,0]
["0632275","BOLT: TYPE: STUD; DIAMETER: M48; LENGTH: 195 MM; HEAD: TWO FLAT; MATERIAL: STL ALLOY; THREAD: 48 MM; OEM P/N: SZT-42-99995-01227; DRAWING NO: 2410/031 REV 0","EA",50,null,0]
["0632276","BOLT: TYPE: STUD; DIAMETER: M48; LENGTH: 195 MM; HEAD: TWO FLAT; MATERIAL: STL ALLOY; THREAD: 48 MM; OEM P/N: SZT-42-99995-01226; DRAWING NO: 2410/034 REV 0","EA",50,null,0]
["0632546","BRACKET: TYPE: BOLT; MATERIAL: STL ALLOY HEAT RESISTANT; DIMENSIONS: M30 X 149 MM; SPECIFICATION: CASING ASSEMBLY; APPLICATION: HP TURBINE , HP CASING CASING ASSEMBLY; OEM P/N: 2490-065, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24900-0014 REV 0; REFERENCE NO: SZT-42-99994-00039","EA",50,null,0]
["0632547","BRACKET: TYPE: BOLT; MATERIAL: STL ALLOY HEAT RESISTANT; DIMENSIONS: M30 X 187 MM; SPECIFICATION: CASING ASSEMBLY; APPLICATION: HP TURBINE, HP CASING CASING ASSEMBLY; OEM P/N: 2490-066, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.24900-0014 REV 0; REFERENCE NO: SZT-42-99994-00034","EA",50,null,0]
["0693020","BOLT: DIAMETER: M64; LENGTH: 350 MM; HEAD: TWO FLAT; OEM P/N: 5120-064, OEM: GE STEAM POWER SERVICE; FOR HP CONTROL VALVE CV1 UNIT 1-4","EA",50,null,0]
["0713700","STUD: TYPE: BOLT; DIAMETER: 20 MM; THREAD: M20; LENGTH: 130 MM; MATERIAL: STEEL; OEM P/N: 8160-138, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-138; 42.81600-0003; HP/LP CROSSOVER PIPES","EA",50,null,0]
["0713704","STUD: TYPE: BOLT; DIAMETER: 20 MM; THREAD: M20; LENGTH: 130 MM; MATERIAL: DIN2510; OEM P/N: 8160-191, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-191; 42.81600-0003; HP/LP CROSSOVER PIPES","EA",50,null,0]
["0713705","BOLT, MACHINE: DIAMETER: M27; LENGTH: 140 MM; HEAD: HEXAGON; GRADE: D5; MATERIAL: TOOL STEEL; THREAD: 3 MM; TYPE: HP/LP CROSSOVER PIPES; OEM P/N: 8160-132, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-132; 42.81600-0003; DIN931","EA",50,null,0]
["0713706","BOLT, MACHINE: DIAMETER: M27; LENGTH: 85 MM; HEAD: HEXAGON; GRADE: D5; MATERIAL: TOOL STEEL; THREAD: 3 MM; TYPE: HP/LP CROSSOVER PIPES; OEM P/N: 8160-134, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-134; 42.81600-0003; DIN931","EA",50,null,0]
["0713707","BOLT, MACHINE: DIAMETER: M33; LENGTH: 80 MM; HEAD: HEXAGON; GRADE: D5; MATERIAL: TOOL STEEL; THREAD: 3.5 MM; TYPE: HP/LP CROSSOVER PIPES; OEM P/N: 8160-131, OEM: GE STEAM POWER SERVICE; DRAWING NO: 8160-131; 42.81600-0003; DIN931","EA",50,null,0]
["0723211","BOLT: TYPE: MACHINE; DIAMETER: 10 MM; LENGTH: 35 MM; HEAD: HEX; MATERIAL: STEEL; THREAD: M10; OEM P/N: 5161-348, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.51600-0187; REFERENCE NO: SZ50011687; FOR HP CONTROL CV SERVOMOTOR","EA",50,null,0]
["0737730","STUD: TYPE: EXPANSION BOLT; DIAMETER: 36 MM; THREAD: M36-4; LENGTH: 165 MM; MATERIAL: STEEL; THREAD LENGTH: 72 MM; GRADE: 34CRMONI6V; OEM P/N: 2460-027, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0004; FOR HP DIAPHRAGM CARRIER 2","EA",50,null,0]
["0737867","STUD: TYPE: BOLT; DIAMETER: 36 MM; THREAD: M36-4; LENGTH: 165 MM; MATERIAL: STEEL; THREAD LENGTH: 36+36 MM; GRADE: 34CRMONI6V; OEM P/N: 2460-046, OEM: GE STEAM POWER SERVICE; DRAWING NO: C42.24650-0005; FOR HP DIAPHRAGM CARRIER 3","EA",50,null,0]
["0744879","BOLT: TYPE: DRIVE PINION; DIAMETER: 19 MM; LENGTH: 70/95 MM; HEAD: HEXAGON; MATERIAL: GR8.8-4.6; OEM P/N: GVLBLR1&6AH92N; DRAWING NO: Z1292","EA",50,null,0]
["0744937","BOLT: TYPE: RVC ROLLER; DIAMETER: 22 MM; LENGTH: 102 MM; HEAD: HEXAGON; MATERIAL: GR4.6; OEM P/N: GVLBLR5FD13; DRAWING NO: D3068","EA",50,null,0]
["0744962","BOLT: TYPE: ROLLER; DIAMETER: 22 MM; LENGTH: 89 MM; HEAD: HEXAGON; MATERIAL: WHITE FINISHED BOLT; OEM P/N: GVLBLR1-4&6FD14; DRAWING NO: D2866","EA",50,null,0]
["0758056","BOLT: TYPE: M16; DIAMETER: 16 MM; LENGTH: 110; HEAD: HEXAGON; MATERIAL: STAINLESS STEEL; THREAD: METRIC - COARSE","EA",50,null,0]
["0758148","STUD: TYPE: BOLT; DIAMETER: 33 MM; THREAD: M33-3.5; LENGTH: 165 MM; MATERIAL: STEEL; GRADE: 21CRMOV511; OEM P/N: 7120-058, OEM: GE STEAM POWER SERVICE; DRAWING NO: A42.71200-0007; FOR HP EMERGENCY STOP VALVE (STEAM SIDE)","EA",50,null,0]
["0759192","BOLT, MACHINE: DIAMETER: 20 MM; LENGTH: 17 MM; HEAD: HEXAGON; GRADE: STEEL; MATERIAL: MST50-2; THREAD: M20-2.5; OEM P/N: 4930-041, OEM: GE STEAM POWER SERVICE; DRAWING NO: B42.49300-6011; FOR THRUST BEARING","EA",50,null,0]
[]
[{"$nulls":4},"Sub-total"]

{"sheet":"Absorbents","index":3,"n_rows":13,"n_cols":6,"rows_kept":13}
["Material no.","Material","Unit","Quantity","Price","Total"]
["0052897 ","BREATHER: TYPE: TRFR OIL 1350 L; MATERIAL: SILICA GEL; WEIGHT: 0.5 KG; DIMENSIONS: DIA 114 X LG 279 MM; SIZE A","EA",20,null,{"$f":"D2*E2","v":0}]
["0159776 ","ABSORBENT: TYPE: OIL; FORM: CUSHION; 10 CUSHIONS PER BAG; DRIZIT BRAND ONLY; SIZE: SQ 500MM X THK 75MM","EA",120,null,{"$f":"D3*E3","v":0}]
["0159839 ","ABSORBENT: TYPE: OIL; FORM: FIBER LOOSE; CONTAINER CAPACITY: 10 KG; CONTAINER: BAG; SUPPL P/N: DRIZIT; REQUIRED A MATERIAL SAFETY DATA SHEET WITH EVERY DELIVERY","EA",3420,null,0]
["0159852 ","ABSORBENT: TYPE: OIL; FORM: CUSHION; CONTAINER CAPACITY: 1 KG; CONTAINER: BAG; PACKED 10; PACKAGE POLYTHENE, SHELF LIFE INDEFINITE; SIZE: 500MM SQUARE X 100MM THK","EA",500,null,0]
["0159853 ","ABSORBENT: TYPE: OIL; FORM: BOOM; DIMENSIONS: WD 180 MM X LG 4 M","EA",350,null,0]
["0159865 ","ABSORBENT: TYPE: OIL; FORM: BOOM; DIMENSIONS: DIA 250 MM X LG 2 M; FIBRE SORB CEMENT; TO BE PACKED INDIVIDUALLY","EA",220,null,0]
["0162896","DESICCANT: TYPE: SILICA GEL; CONTAINER: DRUM PLASTIC 1 KG; MESH: 0.25-6.3 MM; GRANULAR IMPREGNATED WITH COBALT CHLORIDE; INDICATING BLUE CRYSTALS ACCORDING TO BS3523 1991 OR EQUIVALENT; CHEMICAL AND PHYSICAL PROPERTIES: MOISTURE CONTENT 2 PCT/M/M MAX; PH 3.5 MIN; WATER SOLUBLE SULPHATES 1.0 PCT/M/M MAX; ABSORPTIVE CAPACITY 23 PCT/M/M MIN; PARTICLE SIZE PARTICLES LESS THAN 0.25M 0.25PCT/M/M; PARTICLES GREATER THAN 6.3 0/M/M; COBALT CHLORIDE 0.5 PCT/M/M MIN FRIABILITY AND DUST 0.5 PCT/M/M; 125 MICRO M MAX","KG",1180,null,0]
["0175741","ABSORBENT: TYPE: SORB NATURAL OIL SPILL; FORM: CLEANSORB PEAT; CONTAINER CAPACITY: 25 KG; CONTAINER: BAG; REFERENCE NO: L0668; CLEAN SORB PEAT ABSORBENT;IDEAL FOR HYDRO CARBON SPILL ON LAND OR WATER; COST EFFECTIVE AND EASY TO USE; 1KG ABSORB TO 13L OIL; SUITABLE FOR MOST CLEAN UPS ABSORBS COMPLETELY ON CORRECT-24HR SPILL CLEAN UP;DRIZIT ENVIROMENTAL","EA",20,null,0]
["0224087 ","CHEMICAL: TYPE: DEGREASER; FORM: LIQUID; CONTAINER CAPACITY: 25 L; CONTAINER: DRUM PLASTIC; SPECIFICATION: DRIZIT BRAND; TYPE: DE BOND; FOR OIL SPILL CLEANING, SOLVENT, NON TOXIC AND ENVIRONMENTAL FRIENDLY, MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT","EA",460,null,0]
["0250312 ","BREATHER: TYPE: SILICA GEL; MATERIAL: GLASS; DIMENSIONS: WD 100 X LG 420 MM; CONNECTION: 20 MM FNPT; FOR TRANSFORMERS WITH 8800 L OIL CAPACITY","EA",70,null,0]
[]
[{"$nulls":4},"Sub-total"]

{"sheet":"Cloth&Cable ties","index":4,"n_rows":16,"n_cols":6,"rows_kept":16}
["Material no.","Description","Unit","Quantity","Price","Total"]
["0011460","TIE, CABLE: TYPE: SELF LOCKING; DIAMETER RANGE: 50 MM; WIDTH: 4.7 MM; LENGTH: 200 MM; MATERIAL: PLASTIC; STRENGTH: 15 KG; COLOR: BLACK; MANUF P/N: T50R; REFERENCE NO: T50R; INSULOK TYPE, 1EA = 100 TIES","EA",23514,null,{"$f":"D2*E2","v":0}]
["0011461","TIE, CABLE: TYPE: SELF LOCKING; DIAMETER RANGE: 18 MM; WIDTH: 2.5 MM; LENGTH: 104 MM; MATERIAL: NYLON; STRENGTH: 15 KG; COLOR: BLACK; SUPPL P/N: T18R; BRAND INSULOK TYPE, 100 PER PACKET","EA",9960,null,{"$f":"D3*E3","v":0}]
["0011501","TIE, CABLE: TYPE: SELF LOCKING; DIAMETER RANGE: 109 MM; WIDTH: 4.7 MM; LENGTH: 395 MM; MATERIAL: NYLON; STRENGTH: 32 KG; COLOR: BLACK; SUPPL P/N: T50L; BRAND INSULOK, PLASTIC, 100 PER PACKET","EA",13810,null,0]
["0016878","CLOTH, KNITTED: FIBER MATERIAL: COTTON; WIDTH: 290 MM; COLOR: WHITE; TYPE MUTTON; PLAIN, IN 1 KG ROLL","KG",283,null,0]
["0102263","CLOTH: WIDTH: 50.8 MM; LENGTH: 30 M; MATERIAL: GLASS FIBER TEFLON COATED; REFERENCE NO: 128A","M",10,null,0]
["0102355","CLOTH: TYPE: OIL; THICKNESS: 0.006 IN","KG",10,null,0]
["0109556","CLOTH, ABRASIVE: TYPE: SANDING; FLINT/EMERY GRADE DESIGNATOR: FINE; OVERALL WIDTH: 1.71 M; LENGTH: 10 M; ABRASIVE MATERIAL: NYLON LOFTED; SUPPLIER NOTE THE ITEM SHALL BE SUPPLIED IN ROLLS, IF NOT THE ITEM WILL BE REJECTED AND SEND BACK ON YOUR COSTS","EA",11,null,0]
["0135747","CLOTH, GLASS: WIDTH: 1 M; LENGTH: 10 M; THICKNESS: 3 MM; MATERIAL: FIBER; JOINTS PA FANS AND MILLS","M",10,null,0]
["0159673","CLOTH: TYPE: GENERAL PURPOSE; WIDTH: 350 MM; LENGTH: 600 MM; MATERIAL: RAYON FIBER VISCOSE 100 PCT; COLOR: WHITE; REFERENCE NO: 063834BLUE; 063818; 065953; 063859PINK; DAY-LEE, MANUFACTURED WITH SMALL PERFORATIONS, PACKED 50 PER PACK AND 10 PACKETS PER CASE ( PACK OF 50 =50 EA ) (1 BOX = 500 EA )","EA",30,null,0]
["0159679","CLOTH: TYPE: CLEANING COLORED GRADE; MATERIAL: LIGHTKNIT; STERILIZED CLEAN, FAST,: CLK , NOT 100 PCT COTTON; SIZE: 25 KG BUNDLES","KG",8245,null,0]
["0247770","CLOTH, GLASS: TRADE NAME: SYNTHO-GLASS SG25; WIDTH: 50 MM; LENGTH: 1.5 M; MATERIAL: GLASS FIBER; REPAIR, PIPE LEAKS, REQUIRED FOR USE ON COOLING WATER, OIL & GAS PIPES; TECHNICAL DATA SHEETS TO BE SUPPLIED AT DELIVERY","EA",13,null,0]
["0247771","CLOTH, GLASS: TRADE NAME: SYNTHO-GLASS SG39; WIDTH: 76 MM; LENGTH: 2.7 M; MATERIAL: GLASS FIBER; REPAIR, PIPE LEAKS, REQUIRED FOR USE ON COOLING WATER, OIL & GAS PIPES; TECHNICAL DATA SHEETS TO BE SUPPLIED AT DELIVERY","EA",17,null,0]
["0578725","CLOTH: TYPE: WIPING; WIDTH: 180 MM; LENGTH: 180 MM; MATERIAL: SILICON TREATED COTTON; COLOR: WHITE; PACKAGE TYPE: BAG PLASTIC; USED FOR DIFFERENT APPLICATIONS IN THE PLANT","EA",10,null,0]
[]
[{"$nulls":4},"Total Excl. VAT"]

{"sheet":"Welding electrodes","index":5,"n_rows":32,"n_cols":6,"rows_kept":32}
["Material no.","Description","Unit","Quantity","Price","Total"]
["0000182 ","ELECTRODE, WELDING: SIZE: 3.15 MM; AWS CLASS: A5.1-91; E6013; CONTAINER: BOX 5 KG; REFERENCE NO: 070-003; AC OR DC CURRENT","KG","180",null,{"$f":"D2*E2","v":0}]
["0000196 ","DISK, CUTTING: OUTSIDE DIAMETER: 230 MM; ARBOR SIZE: 22.23 MM; THICKNESS: 3 MM; GRIT: A80; ABRASIVE MATERIAL: AL OXIDE; SPEED: 6600 RPM; BOND/BACKING: RESINOID; USAGE DESIGN: FIRE BRICKS/STONE; REFERENCE NO: 230BN22G230SM22-23WC24V5BFW; SUPPL P/N: 80EHT230-2C24PS","EA","110",null,{"$f":"D3*E3","v":0}]
["0000197 ","DISK, CUTTING: OUTSIDE DIAMETER: 230 MM; ARBOR SIZE: 22.23 MM; THICKNESS: 3.2 MM; GRIT: 24; ABRASIVE MATERIAL: AL OXIDE; SPEED: 6640 RPM; BOND/BACKING: RESINOID; USAGE DESIGN: STL; REFERENCE NO: RA24T5BFW","EA","61",null,0]
["0000198 ","DISK, GRINDING: DIAMETER: 230 MM; ARBOR SIZE: 22.23 MM; SPEED: 6643 RPM; ABRASIVE MATERIAL: AL OXIDE; BOND/BACKING: RESINOID; USAGE DESIGN: STL; SHAPE: RD; REFERENCE NO: A24-R5-BFW TP27; 230BD 64; A24R5BFW; TP27; REINFORCED; DEPRESSED CENTRE; SIZE 6MM THICK; 80/S MAX","EA","20",null,0]
["0035106 ","ELECTRODE, WELDING: SIZE: DIA 6 MM; MATERIAL: ARC-AIR-CARBON CU COATED; REFERENCE NO: 75107","EA","20",null,0]
["0035107 ","ELECTRODE, WELDING: SIZE: DIA 8 X LG 305 MM; MATERIAL: CARBON CU COATED; CONTAINER: BOX 50; SUPPL P/N: COUGING; 216; DELIVERY WILL NOT BE ACCEPTED IF HAZARDOUS CHEMICAL DATA SHEET IS NOT SUPPLIED WITH EVERY DELIVERY","EA","20",null,0]
["0035127 ","ELECTRODE, WELDING: SIZE: DIA 4.8 MM; MATERIAL: BRZ; CONTAINER: PACK 5 KG; REFERENCE NO: M15; GENERAL PURPOSE","KG","20",null,0]
["0035132 ","ELECTRODE, WELDING: SIZE: 2.5 MM; AWS CLASS: E6013; MATERIAL: MS; CONTAINER: BOX 5 KG; SUPPL P/N: 075-002; VITEMAX, TEST CERTIFICATE TO BE SUPPLIED WITH EVERY CONSIGNMENT, DELIVERY WILL NOT BE ACCEPTED IF HAZARDOUS CHEMICAL DATA SHEET IS NOT SUPPLIED WITH EVERY DELIVERY","KG","20",null,0]
["0035152 ","ELECTRODE, WELDING: SIZE: 3.2 MM; MANUF P/N: 075-833; SUPPL P/N: XYRON 244; FERROLOID 4","KG","30",null,0]
["0035296 ","ELECTRODE, WELDING: SIZE: 4 MM; AWS CLASS: A5.1-81; E7018-1; MATERIAL: STL LOW HYDROGEN COATED; CONTAINER: BOX 4 KG; SUPPL P/N: 075/284; TEST CERTIFICATE TO BE SUPPLIED WITH EVERY CONSIGNEMENT, DELIVERY WILL NOT BE ACCEPTED IF HAZARDOUS CHEMICAL DATA SHEET IS NOT SUPPLIED WITH EVERY DELIVERY","KG","20",null,0]
["0036025 ","DISK, CUTTING: OUTSIDE DIAMETER: 115 MM; ARBOR SIZE: 22.2 MM; THICKNESS: 2.5 MM; GRIT: 30; ABRASIVE MATERIAL: AL OXIDE; SPEED: 13300 RPM; BOND/BACKING: FIBER; USAGE DESIGN: MASONRY/STONE; REFERENCE NO: 1608600276; ABRASIVE REINFORCED, RECESSED CENTRE","EA","125",null,0]
["0036028 ","DISK, GRINDING: DIAMETER: 230 MM; ARBOR SIZE: 22.23 MM; SPEED: 6600 RPM; ABRASIVE MATERIAL: SIC; BOND/BACKING: RESINOID; USAGE DESIGN: STL; REFERENCE NO: 80E230-6-A24SG; 80M/S; ONLY PFERD BRAND ACCEPTABLE FOR SAFETY REASONS; SIZE 6MM","EA","20",null,0]
["0036029 ","DISK, CUTTING: OUTSIDE DIAMETER: 230 MM; ARBOR SIZE: 22.23 MM; THICKNESS: 3.2 MM; GRIT: C24; ABRASIVE MATERIAL: SILICON CARBIDE; SPEED: 6600 RPM; BOND/BACKING: RESINOID; USAGE DESIGN: BRICK/CERAMICS/CONCRETE/NON-FERROUS METAL/STONE/WALL AND WALL CHASING; REFERENCE NO: 80EHT 230-2 C24SG; REINFORCED; ONLY PHERD BRAND ACCEPTABLE FOR SAFETY REASONS","EA","25",null,0]
["0036039 ","DISK, GRINDING: DIAMETER: 115 MM; ARBOR SIZE: 22.23 MM; GRIT: MOS80; SPEED: 13300 RPM; ABRASIVE MATERIAL: AL OXIDE; BOND/BACKING: RESINOID; SHAPE: RD; REFERENCE NO: E115-6A24PS; DEPRESSED CENTRE; SIZE 6 MM","EA","83",null,0]
["0036065 ","DISK, GRINDING: DIAMETER: 100 MM; ARBOR SIZE: 16 MM; GRIT: 24; SPEED: 15300 RPM; ABRASIVE MATERIAL: AL OXIDE; BOND/BACKING: FIBER; SHAPE: 27; SUPPL P/N: E100-4A24RSG; E100-4A24 R SG; SIZE 4MM","EA","50",null,0]
["0137551 ","ELECTRODE: MANUF P/N: 337609550; EIL; PT100 TEPERATURE COMPENSATOR ,7600 SERIES","EA","20",null,0]
["0137552 ","ELECTRODE: TYPE: MICRO; MATERIAL: CERAMIC; DIMENSIONS: 2.25 M; TEMPERATURE RANGE: -5 TO 100 DEG C; SUPPL P/N: 331360200; 7600 SERIES","EA","20",null,0]
["0137553 ","ELECTRODE: TYPE: TOUGHENED INDUSTRIAL; MATERIAL: GLASS; DIMENSIONS: LG 2.25 M; TEMPERATURE RANGE: 0-100 DEG C; PH RANGE: 0-14; SUPPL P/N: H331073070; REFERENCE NO: 7600","EA","20",null,0]
["0151174 ","ELECTRODE: TYPE: PH COMBINATION; MANUF P/N: 33-1912-400; MODEL NO: 2867; WITH CO-AX CLASS BNC CONNECTOR 6 METER EIL","EA","20",null,0]
["0229248 ","DISK, ABRASIVE: TYPE: SANDING; GRIT: 40; OUTSIDE DIAMETER: 115 MM; ARBOR SIZE: 22.33 MM; ABRASIVE MATERIAL: AL OXIDE; ADHESIVE BACKING: RESIN; BACKING MATERIAL: CLOTH X-WEIGHT; REFERENCE NO: PFC115-22 A-PLUS; FOR USE BY MAINTENANCE; POLIFAN","EA","20",null,0]
["0229249 ","DISK, CUTTING: OUTSIDE DIAMETER: 115 MM; ARBOR SIZE: 22.23 MM; THICKNESS: 2.4 MM; GRIT: A30; ABRASIVE MATERIAL: AL OXIDE; BOND/BACKING: RESIN; USAGE DESIGN: STL; TYPE SANDING; FOR USE BY MAINTENANCE; REINFORCED CUT-OFF DISC","EA","20",null,0]
["0230074 ","ELECTRODE: TYPE: INNER; DRAWING NO: CREDFELD CE-1549-LT300S REV 1; CE-1549-LT300S REV 1; REFERENCE NO: 11, 12, 14 & 16; COMPLETE, FOR USE ON GAS/AIR IGNITOR","EA","77",null,0]
["0230078 ","ELECTRODE: TYPE: AIR/GAS IGNITOR; DRAWING NO:  REV 1; CREDFELD CE-1549-LT300S REV 1; MODEL NO: LT300; REFERENCE NO: 12; SPARK GAP END","EA","20",null,0]
["0243509 ","DISK: TYPE: STACK; DIAMETER: ID 50 X OD 100 X HT 77 MM; MATERIAL: INCONEL 718; SUPPL P/N: 528702004; REFERENCE NO: 50567-000-01","EA","20",null,0]
["0244040 ","ELECTRODE: TYPE: PACK BOILER; MATERIAL: STL; DIMENSIONS: LG 455 MM; APPLICATION: BOILER THE200; SUPPL P/N: 185660; AS PER ATTACHED SPARE PART SPREADSHEET, TO BE STORED IN DRY WEATHER PROTECTED CONDITION","EA","20",null,0]
["0545126 ","ELECTRODE, WELDING: SIZE: 4 MM; AWS CLASS: A5; MATERIAL: MS; CONTAINER: 5 KG","KG","50",null,0]
["0550726 ","ELECTRODE, WELDING: SIZE: 2.5 MM; AWS CLASS: A5.1 E6013; MATERIAL: VITEMAX; CONTAINER: 5 KG; SPECIFICATION: ENISO2560E350RC11; MANUF P/N: W075002; A PREMIUM GRADE, GENERAL PURPOSE RUTILE ELECTRODE SUITABLE FOR WELDING MILD STEEL; NOTE: MATERIAL SAFETY DATE SHEET REQUIRE WITH DELIVERY","KG","70",null,0]
["0550761","ELECTRODE, WELDING: SIZE: 2.5 MM; AWS CLASS: A5.1 E7018-1HB; MATERIAL: HYDROGEN; CONTAINER: 4 KG; SPECIFICATION: ENISO2560AE424B12H10; MANUF P/N: W075282; A PREMIUM GRADE SUITABLE FOR WELDING C-MN AND LOW ALLOY STEELS;NOTE: MATERIAL SAFETY DATA SHEET REQUIRE WITH DELIVERY","KG","108",null,0]
["0705531","DISK: TYPE: INSULATION; DIAMETER: ID 32 X OD 55 MM; MATERIAL: H.POPB II RIGID LAMINATED SHEET, HARD PAPER, PF/CP 1; OEM P/N: W 205527P0008; DRAWING NO: W 090033 REV B","EA","20",null,0]
[]
[{"$nulls":4},"Sub-total"]

{"sheet":"Filters","index":6,"n_rows":85,"n_cols":6,"rows_kept":85}
["Material no","Description","Unit","Quantity","Price","Total"]
["0000393","FILTER, ELEMENT: TYPE: 1ST STG CYLINDER HEAD GROUP; WORTHINGTON AIR COOLED RECIPROCATING COMPRESSOR H/SAB/SABC/SBB; MANUF P/N: CA-74-PL; SUPPL P/N: FLR-308","EA",40,null,{"$f":"D2*E2","v":0}]
["0000585","FILTER, ELEMENT: TYPE: OIL; DIMENSIONS: DIA 60 X HT 50 MM; REFERENCE NO: FLR305; USED ON OIL PUMP ON THE WORTHINTON AIR COOLED COMPRESSOR TYPE -H; 7 PLATE ASSEMBLY","EA",40,null,{"$f":"D3*E3","v":0}]
["0024435","FILTER, FUEL: SUPPL P/N: 26560017","EA",40,null,0]
["0024517","FILTER, OIL: APPLICATION: HITACHI GEARBOX","EA",40,null,0]
["0024778","FILTER, ELEMENT: TYPE: COALESCING; MANUF P/N: 180S; SUPPL P/N: S090; MAXIMUM WORKING TEMPERATURE 50 DEG C MIN WORKING TEMPERATURE 1.5 DEG CEL INITIAL PRESSURE DROP 0.1 BAR INITIAL PRESSURE DROP WITH ELEMENT SATURATED WITH OIL 0.275-0.40 BAR RECOMMENDED PRESSURE 0.7-1.05 BAR","EA",40,null,0]
["0024779","FILTER, ELEMENT: MATERIAL: CERAMIC; MANUF P/N: Q120; 360Q; MAXIMUM WORKING TEMPERATURE 65 DEG C MIN WORKING TEMP 1.5 DEG CEL NORMAL OPERATING PRESSURE DROP 0.2-1.25 BAR MAXIMUM PRESSURE DROP 0.7 -1.05 BAR","EA",40,null,0]
["0024780","FILTER, ELEMENT: TYPE: HYPER, COALESCING; SUPPL P/N: P090; MODEL NO: 180P; MAX WORKING TEMP 50 DEG C; MIN WORKING TEMP 1.5 DEG C; INITIAL PRESSURE DROP 0.085 BAR; INITIAL PRESSURE DROP WITH ELEMENT SATURATED WITH OIL 0.170 BAR; MAX RECOMMENDED PRESSURE DROP 0.70-1.05 BAR","EA",40,null,0]
["0024781","FILTER, ELEMENT: TYPE: HYPER; MATERIAL: CERAMIC; MANUF P/N: Q-090; Q090; MAXIMUM WORKING TEMP 65 DEG C","EA",40,null,0]
["0024908","FILTER, ELEMENT: TYPE: AIR; DIMENSIONS: 69 X 26 X 3","EA",40,null,0]
["0024910","FILTER: TYPE: SUCTION; SUPPL P/N: SU25F16","EA",40,null,0]
["0024913","FILTER, ELEMENT: TYPE: AIR MICRON; SUPPL P/N: 25583-/47","EA",41,null,0]
["0024914","FILTER, AIR: MICRON: 0.2 UM; APPLICATION: SAFETY VALVE HOPKINSONS SEVCO LOADING; REFERENCE NO: 25583-16-02; 25583-166","EA",41,null,0]
["0024916","FILTER, OIL: SUPPL P/N: 2654407","EA",40,null,0]
["0024917","FILTER, ELEMENT: TYPE: AIR CLEANER","EA",40,null,0]
["0025089","FILTER, FLUID: TYPE: COM BOILER 6 STEAM","EA",40,null,0]
["0025091","FILTER, ELEMENT: MANUF P/N: P11-9372","EA",40,null,0]
["0039978","FILTER, ELEMENT: TYPE: WASHABLE; DIMENSIONS: WD 300 X LG 600 X THK 50 MM; MANUF P/N: WP 77; WP77; AIR CONDITIONER TURBINE CONTROL PANELS","EA",40,null,0]
["0041865","FILTER, OIL: TYPE: DISCHARGE; REFERENCE NO: FLR296; FOR USE WITH WORTHINGTON COMPRESSORS TYPE H, MODEL SAABC","EA",40,null,0]
["0043355","FILTER, AIR: TYPE: AIRCON KLEENFLO BAG PL","EA",56,null,0]
["0046341","FILTER, ELEMENT: TYPE: PIPE LINE; DRAWING NO: D7344/1 REV 1","EA",40,null,0]
["0050146","FILTER: MATERIAL: COTTON; SUPPL P/N: NW50; SET","EA",40,null,0]
["0050147","FILTER, FLUID: TYPE: COOLANT PLANT; SUPPL P/N: G7882; IT411","EA",40,null,0]
["0050149","FILTER, ELEMENT: TYPE: PRE; MANUF P/N: 11-7443; SUPPL P/N: SMP18-1002; DA18-307; ARM","EA",40,null,0]
["0050150","FILTER, ELEMENT: MECHANICAL","EA",40,null,0]
["0050151","FILTER, ELEMENT: FILTERING RETENTION: 64 UM; SUPPL P/N: 30BG","EA",40,null,0]
["0050156","FILTER, OIL: TYPE: DUAL; MODEL NO: PSOWI; COMPLETE WITH SWITCHOVER HANDLE; 32 L/MIN; UNDRILLED FLANGES","EA",40,null,0]
["0053214","FILTER, AIR: DIMENSIONS: 302 X 490 MM; J12","EA",40,null,0]
["0053215","FILTER, ELEMENT: TYPE: DISPOSABLE, PLEATED, SUPER VEE; DIMENSIONS: SQ 20 X 2 IN; SUPPL P/N: E70802/8; J12 PRECI","EA",40,null,0]
["0053216","FILTER, ELEMENT: TYPE: WASHABLE, AIR; DIMENSIONS: WD 500 X LG 500 MM; MATERIAL: POLY PLEAT; REFERENCE NO: PSA 500","EA",50,null,0]
["0053217","FILTER, ELEMENT: TYPE: WASHABLE PLEATED; DIMENSIONS: WD 394 X LG 495 X THK 48 MM; MATERIAL: POLYESTER; MANUF P/N: WP-77; VOKE MULTIVEE PREC AIR","EA",58,null,0]
["0053218","FILTER, ELEMENT: TYPE: WASHABLE PLEATED PANEL; DIMENSIONS: SQ 490 X THK 48 MM; REFERENCE NO: WP 77","EA",40,null,0]
["0053219","FILTER, ELEMENT: TYPE: DISPOSABLE, PLEATED; DIMENSIONS: WD 508 X LG 635 X HT 50.8 MM; MANUF P/N: C96205/9","EA",40,null,0]
["0071373","FILTER, AIR: BR","EA",40,null,0]
["0102357","GLAND, PACKING: TYPE: MICROWIRE FILTER N7500B; SUPPL P/N: 6400113; 450LA22; DRAWING NO: B6400113 REV 1","EA",40,null,0]
["0160432","FILTER, BAG: MATERIAL: TERRYLENE VELTED; REFERENCE NO: V10 HB; 10 DLM; 10 BAGS PER SET; FLUE GAS PLANT","EA",40,null,0]
["0160434","FILTER: TYPE: UNIVEE; GAS BOOSTER PLANT","EA",40,null,0]
["0160435","FILTER, GAS: TYPE: BOX; BOOSTER PLANT","EA",40,null,0]
["0216341","FILTER, AIR: DIMENSIONS: ID 64 X OD 115 X LG 253 MM; SUPPL P/N: 5306091; REFERENCE NO: C11-100; EMISSION MONITOR CARTRIDGE TYPE OMD41","EA",40,null,0]
["0218733","FILTER, ELEMENT: TYPE: COALESCER CARTRIDGE; DIMENSIONS: ID 89 X OD 152 X LG 733 MM; MATERIAL: PAPER PLEATED; FILTERING RETENTION: 10 UM; SUPPL P/N: A.4-727; FOR USE ON MAIN TURBINE AND BFPT COALESCER LUBE OIL PURIFIER SYSTEMS; CA28; MANUFACTURE NAME AND PART NUMBER TO BE MARKED ON END CAPS; ITEM TO BE PACKED AND SEALED IN PLASTIC BAGS AND CARTON; APPLICATION: LOP; PLEATED PAPER CORE; COMPOSED OF CELLULOSE PAPER AND FABRIC SUPPORT; COALESCER BED COMPOSED OF FIBREGLASS MATS AND SYNTHETIC SUPPORTING FABRIC WITH KNITTED OUTER SOCK","EA",60,null,0]
["0221729","FILTER, ELEMENT: DIMENSIONS: ID 169 X OD 189 X LG 320 MM; MATERIAL: HYDROPHOBIC TEFLON; FILTERING RETENTION: 25 UM; SUPPL P/N: FE0213B; FOR USE ON THE LOP 18 OIL PURIFIERS; (GREEN)","EA",50,null,0]
["0225869","FILTER, OIL: MATERIAL: PAPER; MICRON: 3 UM; SUPPL P/N: 85052769; FOR USE ON INGERSOLL RAND COMPRESSOR ML 16055","EA",40,null,0]
["0225870","FILTER, AIR: MATERIAL: PAPER; MICRON: 3 UM; SUPPL P/N: 39708466; FOR USE ON INGERSOLL RAND COMPRESSOR ML 16055","EA",40,null,0]
["0226621","FILTER: TYPE: INLET; DIMENSIONS: 16 X 20 X 1 IN; MATERIAL: PAPER; SEAL AIR FAN","EA",42,null,0]
["0227629","FILTER, AIR: TYPE: PANEL; DIMENSIONS: SQ 600 X THK 50 MM; MATERIAL: FIBER; MICRON: 0.3 UM; FOR USE ON HVAC SYSTEM, WV 250","EA",40,null,0]
["0229983","FILTER, ELEMENT: DIMENSIONS: WD 41 X LG 161 MM; MATERIAL: SS MESH; FOR USE ON DUAL FILTER LUBRICATION SET ON MILLS AND FEEDERS; FILTRATION SIZE 80 MICRON","EA",380,null,0]
["0231608","FILTER, AIR: TYPE: PRIMARY WASHABLE PANEL; DIMENSIONS: SQ 600 X THK 100 MM; SUPPL P/N: WV 350; ARRESTANCE 90PCT, DIFFERENTIAL AT RATED FLOW 60 PA, FINAL DIFFERENTIAL PRESSURE 250 PA, DUST HOLDING CAPACITY 232G","EA",66,null,0]
["0231609","FILTER, AIR: TYPE: PRIMARY WASHABLE PANEL; DIMENSIONS: 400 X 600 X 100 MM; EFFICIENCY: 90 PCT; SUPPL P/N: WV 350; DIFFERENTIAL AT RATED FLOW 60 PA, FINAL DIFFERENTIAL PRESSURE 250 PA, DUST HOLDING CAPACITY 185G","EA",40,null,0]
["0231610","FILTER, ELEMENT: TYPE: AIR SECONDARY WASHABLE; DIMENSIONS: SQ 600 X WD 300 MM; SUPPL P/N: CC-85PCT; DUST SPOT, ARRESTANCE 99 PCT, RATED FLOW 3400 CU/M/H, INITIAL PRESSURE LOSS 60 PA, FINAL PRESSURE LOSS 600 PA, DUST HOLDING CAPACITY 680G; EFFICIENCY: 85 PCT","EA",42,null,0]
["0231611","FILTER, AIR: TYPE: SECONDARY WASHABLE; DIMENSIONS: 400 X 600 X 300 MM; EFFICIENCY: 85 PCT; SUPPL P/N: CC-85%; ARRESTANCE 99PCT; RATED AIRFLOW 3400 CU/M/H, INITIAL PRESSURE LOSS 60 PA, FINAL PRESSURE LOSS 600 PA, DUST HOLDING CAPACITY 450G","EA",40,null,0]
["0233098","FILTER, ELEMENT: TYPE: CANDLE; MATERIAL: STAINLESS STEEL; FILTERING RETENTION: 30 UM; SUPPL P/N: 2.62.9.270.500.10/100; FOR BFPT LUBE OIL UNIT, EACH HOUSING, X 2 TAKES 26 ELEMENTS, FAB NO; 119637/12 UNIT 1 TO 4","EA",40,null,0]
["0233099","FILTER, ELEMENT: TYPE: CANDLE; MATERIAL: STAINLESS STEEL; FILTERING RETENTION: 20 UM; SUPPL P/N: 2.62.9.270.500.10/100; FOR MAIN TURBINE CONTROL UNIT, EACH HOUSING X 2 TAKES 25, FAB NO: 116957/1983","EA",40,null,0]
["0233100","FILTER, ELEMENT: TYPE: CANDLE; MATERIAL: STAINLESS STEEL; FILTERING RETENTION: 20 UM; SUPPL P/N: 2.62.9.220.250.08/80; FOR BFPT CONTROL OIL UNIT, EACH HOUSING X 2 TAKES 18, FAB NO: 116957/1983 UNIT 1 TO 4","EA",40,null,0]
["0233101","FILTER, ELEMENT: TYPE: CANDLE; MATERIAL: STAINLESS STEEL; FILTERING RETENTION: 30 UM; SUPPL P/N: 2.62.9.355.750.25/250; FOR MAIN TURBINE LUBE OIL UNIT, EACH HOUSING X 2 TAKES 52, FAB NO:119637/12","EA",66,null,0]
["0233753","FILTER, AIR: TYPE: WASHABLE; DIMENSIONS: SQ 495 X THK 100 MM; MATERIAL: FIBER; MICRON: 100 UM; SUPPL P/N: BN464.06.2008; FOR USE ON GENERATOR, EXCITER AND SLIPRINGS","EA",150,null,0]
["0237363","FILTER, AIR: TYPE: INTAKE; DIMENSIONS: SQ 289 X THK 12 MM; MATERIAL: FIBER; MICRON: 10 UM; REFERENCE NO: 3183.100; TO BE USE ON GENERATOR AND TURBINE PLANT, AVR, SK 3326207","EA",256,null,0]
["0240231","FILTER, ELEMENT: DIMENSIONS: LG 60 IN; FILTERING RETENTION: 10 UM; SUPPL P/N: HFU660GF100H13; CARTRIDGE, MEDIA - GF MATERIAL, USE ON UNIT 5 CONDENSATE SYSTEM, PALL HIGH FLOW ULTI PLEAT, INDUSTRIAL STYLE, ABSOLUTE","EA",40,null,0]
["0240246","FILTER, ELEMENT: MATERIAL: PAPER; FILTERING RETENTION: 10 UM; REFERENCE NO: PI33111 SMX 10 7.768.033.3; REQUIRED FOR 50PCT E.F.P. LUBE OIL SYSTEM","EA",130,null,0]
["0240296","FILTER, OIL: MATERIAL: CI; MICRON: 200 UM; REFERENCE NO: 4275; REQUIRED FOR USE ON FUEL PLANT, 6 IN DIN FLANGED","EA",40,null,0]
["0243430","FILTER, ELECTRONIC: TYPE: DPI; POTENTIAL: 220 V; FREQUENCY: 50-60 HZ; CURRENT: 18 A; SUPPL P/N: 5003/045; REQUIRED FOR USE ON G. E. 400 V PANELS, IN CONJUNCTION WITH DPI TYPE 5003/382","EA",40,null,0]
["0246019","FILTER, OIL: SUPPL P/N: HBLN55148501; FKG1N GENERATOR CIRCUIT BREAKER","EA",20,null,0]
["0247254","FILTER, ELEMENT: MATERIAL: PAPER OR INTERPOR FLEECE; SUPPL P/N: 311571; FOR USE ON ID FANS, BOILERS 1, 5 AND 6","EA",20,null,0]
["0247255","FILTER: TYPE: DUAL; DIMENSIONS: ID 163 X OD 230 X LG 324 MM; MATERIAL: GGG 40.3; MICRON: 10 UM; SUPPL P/N: 313906; REQUIRED FOR USE ON ID FANS, BOILERS 1, 5 AND 6","EA",20,null,0]
["0248480","FILTER, ELEMENT: DIMENSIONS: ID 80 X OD 175 X LG 135 MM; MATERIAL: PAPER/STL; SUPPL P/N: P92-2669; REQUIRED FOR USE ON PYRO PURGE FANS, UNITS 1, 2 AND 4, MOUNTING PLATE AND BOLT","EA",340,null,0]
["0249652","FILTER, AIR: TYPE: SILENCER SHORT; DIMENSIONS: DIA 3/8 X LG 2 IN; MATERIAL: BRZ SINTERED; SHAPE: TAPER; MANUF P/N: MEC2921-3/8; FOR USE ON FABRIC FILTER PLANT 220 SERIES PULSE VALVES, UNITS 1, 5 AND 6","EA",718,null,0]
["0251877","FILTER, ELECTRONIC: TYPE: INPUT; POTENTIAL: 185-265 V; FREQUENCY: 50 HZ; CURRENT: 3 A; MANUF P/N: 857781; REFERENCE NO: M F53N-230V; 3BHE 003523 R0030; REQUIRED FOR USE ON ECS POWER SUPPLY CIRCUIT(GROOTVLEI); FOR POWER PACK(DUVHA)","EA",20,null,0]
["0253282","FILTER, OIL: MATERIAL: BETAMICRON 4; MICRON: 10 UM; SUPPL P/N: 0330R010BN4HC; FOR USE ON FEED PUMP CONTROL OIL SYSTEM, UNIT 1 TO 6, ELEMENT FOR NORMAL RUNNING PLANT, ABSOLUTE, GLASS FIBRE DISPOSABLE, HYDAC","EA",20,null,{"$f":"D67*E67","v":0}]
["0253283","FILTER, OIL: TYPE: DISPOSABLE; MATERIAL: METAL FIBER; MICRON: 10 UM; SUPPL P/N: 0330R010V; REQUIRED FOR USE ON FLUSHING OF FEED PUMP CONTROL OIL SYSTEM, UNIT 1 TO 6, ABSOLUTE, HYDAC, CLEANABLE ELEMENT","EA",46,null,0]
["0253284","FILTER, OIL: MATERIAL: BETAMICRON 4; MICRON: 10 UM; SUPPL P/N: 0660R010BN4HC; REQUIRED FOR MAIN TURBINE CONTROL OIL SYSTEM, NORMAL RUNNING PLAN T, UNIT 1 TO 6, GLASS FIBRE DISPOSABLE ELEMENT, MICRON ABSOLUTE, HYDAC","EA",91,null,0]
["0253285","FILTER, OIL: TYPE: DISPOSABLE; MATERIAL: METAL FIBER; MICRON: 10 UM; SUPPL P/N: 0660R010V; REQUIRED FOR USE IN FLUSHING MAIN TURBINE CONTROL OIL SYSTEM, UNIT 1 TO 6, CLEANABLE, HYDAC","EA",26,null,0]
["0256049","FILTER, AIR: MATERIAL: ALUMINIUM; APPLICATION: BURNER SYSTEM MANUAL DRAIN; SUPPL P/N: 1.321.006; SPECIFICATION ZAMAK BODY, 3/8 IN BSP THREADED POR T, MAXIMUM INLET PRESSURE 1.8 MPA, FLOW RATE @ 0.63 MPA, 3100 NI/MIN","EA",20,null,0]
["0501333","FILTER: DIMENSIONS: HT 121 MM; MATERIAL: PAPER; MICRON: 15; MEDIUM: DUST; MANUF P/N: TC-AG108GF; REQUIRED FOR UNIT 1 PYROS ONLY","EA",30,null,0]
["0528998","FILTER, OIL: TYPE: CARTRIDGE; DIMENSIONS: ID 89 X OD 152 X LG 733 MM; MATERIAL: HYDROPHOBIC MESH; MICRON: 25; APPLICATION: OIL PURIFIER; MANUF P/N: 60.644-727/D; FOR USE ON LOP SERIES OIL PURIFIERS; MANUFACTURES NAME AND PART NUMBER TO BE MARKED ON END CAPS; GREEN SUPPORTED BY METAL SCREEN","EA",47,null,0]
["0555669","FILTER, OIL: TYPE: HYDRAULIC; DIMENSIONS: ID 40.2 X OD 78 X LG 398 MM; MATERIAL: WIRE MESH; MICRON: 25; PRESSURE RATING: 25 BAR; MANUF P/N: 04000DN025W/HC; USED ON THE MILLS","EA",68,null,0]
["0555673","FILTER, OIL: DIMENSIONS: ID 22 X OD 47 X LG 152.7 MM; MATERIAL: FIBER INORGANIC; MICRON: 10; PRESSURE RATING: 25 BAR; MANUF P/N: 0110D010BN4HC; USED ON MILLS","EA",28,null,0]
["0557942","FILTER, ELEMENT: MATERIAL: STAINLESS STEEL; FILTERING RETENTION: 140 UM; MODEL NO: SS-4F-K4-140; REQUIRED BY CHEMICAL SERVICES; SWAGELOK 727098001, ADDED UOM","EA",20,null,0]
["0579698","FILTER: TYPE: PARTICULATE DISC; DIMENSIONS: DIA 110 X DP 10 MM; MATERIAL: POLYESTER; POLYPROPYLENE; MICRON: 99; MEDIUM: LEGIONELLA; SPECIFICATION: EN143:2000 P2; MANUF P/N: 2125 P2; REFERENCE NO: M1860; CONTAINS ADVANCED ELECTRET MEDIA FOR MAXIMAL FILTRATION EFFICIENCY AND LIGHT WEIGHT; LOW BREATHING RESISTANCE; DURABLE WATER RESISTANT AND FLAME RETARDANT; BAYONET FITTING ENSURES PRECISE AND SAFER LOCKING; CAN BE USED ON HALF AND FULL FACE MASKS; ABLE TO BE USED FOR PROTECTION FROM MECHANICALLY AND/OR THERMALLY GENERATED PARTICULATES SUCH AS DUSTS; MISTS; WELDING FUMES; SMOKES AND BIOLOGICAL AGENTS SUCH AS LEGIONELLA; Q FEVER AND ANTHRAX; DISC FILTER 2125 IS CAPABLE OF PROVIDING PROTECTION AGAINST PARTICLES AT LEVELS UP TO TEN TIMES THE EXPOSURE STANDARD ON A HALF FACE MASK AND UP TO FIFTY TIMES THE EXPOSURE STANDARD ON A FULL FACE MASK; UNIQUE IDENTIFIER: 240-44175132","EA",104,null,0]
["0610127","FILTER: TYPE: MARSHALLING CABINET; DIMENSIONS: SQ 221 X THK 12 MM; MATERIAL: CHEMICAL FIBER; MICRON: 10; MEDIUM: DUST; MANUF P/N: SK3182100-PU","EA",1020,null,0]
["0661231","FILTER, OIL: TYPE: ROTARY SCREW COMPRESSOR; DIMENSIONS: OD 108 X HT 262 MM; MATERIAL: PAPER; MICRON: 6-80; PRESSURE RATING: 8.5 BAR; SUPPL P/N: 85052769; ML160; 918 CPM","EA",58,null,0]
["0661234","FILTER, AIR: TYPE: INTAKE; DIMENSIONS: ID 15.59 X OD 26.69 X HT 12.7 CM; MATERIAL: WOOD PULP PAPER; MICRON: 5-10; EFFICIENCY: 98 PCT; SHAPE: CIRCULAR; SUPPL P/N: 39728466; ML160; 918 CFM AT 8.5 BAR; CORRUGATED","EA",92,null,0]
["0762240","FILTER, OIL: TYPE: ATHALON FILTER ELEMENT; DIMENSIONS: L=536, ID=63.5, OD=79 MM; MATERIAL: VITON; MICRON: 5; SUPPL P/N: 2021-07; REFERENCE NO: UE310AP20Z","EA",20,null,0]
[501161,"STOPPER: DIMENSIONS: 7/8 IN; MATERIAL: BRASS & CHLOROPENE; APPLICATION: TUBE PLUGGING & SEALING; MANUF P/N: 7/8\"X3B78; THE PLUG TUBE MUST BE TESTED UNDER PRESSURE AND VIBRATION TO 150PSI AND 200 DEGREES F, MATERIAL CERTIFICATE SUPPLIED AT DELIVERY","EA",6000,null,0]
[501164,"STOPPER: DIMENSIONS: DIA 23 X LG 82 MM; MATERIAL: RUBBER; APPLICATION: TUBE PLUGGING; STANDARD: 50-55 SHORE A; MANUF P/N: RKES 12/13/200; REQUIRED FOR COOLING TOWER 6, MATERIAL BLACK NITRILE, TENSILE STRENGTH 13 TO 16 MPA, ELONGATION @ BREAK 400% TO 500%, TEMPERATURE RANGE 40 - 120 DEGREES, 30 MM FLANGED X 5 MM, 6 MM HOLES X 45 MM DEEP, STOPPERS TO BE MOULDED AND MATERIAL CERTIFICATE SUPPLIED AT DELIVERY","EA",1000,null,0]
[]
[{"$nulls":4},"Total Excl. VAT"]

{"sheet":"Rods","index":7,"n_rows":41,"n_cols":6,"rows_kept":41}
["Material","Description","Unit","Quantity","Price","Total"]
["0000181","ROD, WELDING: DIAMETER: 1.6 MM; LENGTH: 750 MM; MATERIAL: MS; CONTAINER: BUNDLE 1 KG; SUPPL P/N: 000-040; ROD, WELDING; DIAMETER 1.6 MM, LENGTH 750 MM, MATERIAL MS, CONTAINER BUNDLE 1 KG, PART NUMBER: 000-040~ROD,WLDG;000-040,DIA 1.6 MM,LG 750 MM","KG",50,null,{"$f":"D2*E2","v":0}]
["0029459 ","ROD: TYPE: PUSH; SUPPL P/N: 31131-126","EA",50,null,{"$f":"D3*E3","v":0}]
["0035141 ","ROD, BRAZING: TYPE: EASY FLOW; DIAMETER: 3 MM; LENGTH: 600 MM; MATERIAL: SILVER ALLOY; CONTAINER: BAG PLASTIC 100 G; SUPPL P/N: 001-202","EA",50,null,0]
["0035151","ROD, WELDING: DIAMETER: 4 MM; LENGTH: 360 MM; MATERIAL: STL; CONTAINER: BOX 5 KG; SUPPL P/N: EC 4023; DELIVERY WILL NOT BE ACCEPTED IF HAZARDOUS CHEMICAL DATA SHEET IS NOT SUPPLIED WITH EVERY DELIVERY; EUTEC TRODE","KG",50,null,0]
["0046318","ROD: TYPE: COUPLING; MATERIAL: STAINLESS STEEL; APPLICATION: PUMP END D908; MANUF P/N: 2600 580; SUPPL P/N: 115090-26-3; DETAIL DESCRIPTION","EA",50,null,0]
["0085233","ROD, THREADED: DIAMETER: 10 MM; THREAD: 1.5 MM; LENGTH: 1 M; MATERIAL: MS; FULL","EA",80,null,0]
["0085234 ","ROD, THREADED: DIAMETER: 12 MM; THREAD: 1.75 MM; LENGTH: 1 M; MATERIAL: MS; FULL THREAD","EA",200,null,0]
["0085235 ","ROD, THREADED: DIAMETER: 16 MM; LENGTH: 1 M; MATERIAL: MS; FULL","EA",150,null,0]
["0085236 ","ROD, THREADED: DIAMETER: 20 MM; LENGTH: 1 M; MATERIAL: MS; FULL","EA",70,null,0]
["0086679 ","ROD, THREADED: DIAMETER: 3/4 IN; LENGTH: 168 IN","EA",75,null,0]
["0086680 ","ROD, THREADED: DIAMETER: 3/4 IN; LENGTH: 180 IN","EA",50,null,0]
["0086681 ","ROD, THREADED: DIAMETER: 3/4 IN; LENGTH: 126 IN","EA",50,null,0]
["0086682","ROD, THREADED: DIAMETER: 7/8 IN; LENGTH: 225 IN","EA",55,null,0]
["0086684 ","ROD, THREADED: DIAMETER: 1-1/8 IN; LENGTH: 420 IN","EA",50,null,0]
["0086685 ","ROD, THREADED: DIAMETER: 11-3/8 IN; LENGTH: 265 IN","EA",50,null,0]
["0086686 ","ROD, THREADED: DIAMETER: 1-1/2 IN; LENGTH: 375 IN","EA",50,null,0]
["0086687 ","ROD, THREADED: DIAMETER: 5/8 IN; LENGTH: 113 IN","EA",50,null,0]
["0135233 ","ROD: TYPE: INSULATING; DIMENSIONS: DIA 6 MM X LG 1 M; MATERIAL: TUFNOL; REFERENCE NO: TUFN0LCARP; CARP","KG",50,null,0]
["0135234 ","ROD, INSULATION: SIZE: DIA 9 MM; MATERIAL: TUFNOL CARP","KG",50,null,0]
["0230814 ","ROD, GROUND: LENGTH: 1.7 M; REFERENCE NO: MGV 100 DC; EARTH STICK","EA",50,null,0]
["0232798 ","ROD, INSULATION: SIZE: OD 2 IN X LG 2 FT; MATERIAL: TUFNOL; SUPPL P/N: 033-002-01; FOR USE ON MIGI RAPPER","EA",50,null,0]
["0233683 ","ROD, THREADED: DIAMETER: 6 MM; THREAD: 1 MM; LENGTH: 3 M; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",70,null,0]
["0233684 ","ROD, THREADED: DIAMETER: 10 MM; THREAD: 1.5 MM; LENGTH: 3 M; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",80,null,0]
["0233685 ","ROD, THREADED: DIAMETER: 12 MM; THREAD: 1.75 MM; LENGTH: 3 M; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",80,null,0]
["0233686 ","ROD, THREADED: DIAMETER: 16 MM; THREAD: 2 MM; LENGTH: 3 M; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",80,null,0]
["0233687 ","ROD, THREADED: DIAMETER: 20 MM; THREAD: 2.5 MM; LENGTH: 3 M; MATERIAL: MS; GRADE: 4.6; FOR MAINTENANCE USE","EA",80,null,0]
["0233688 ","ROD, THREADED: DIAMETER: 24 MM; THREAD: 3 MM; LENGTH: 3 M; MATERIAL: MS; FOR MAINTENANCE USE","EA",130,null,0]
["0234795 ","ROD: DRAWING NO: FC 572 REV B REV 1; FC 572 REV 1; REFERENCE NO: KA 1830","EA",55,null,0]
["0247956 ","ROD: TYPE: PULL END; DIMENSIONS: DIA 40 MM X LG 2.158 M; MATERIAL: STL GR B ASTM A106; APPLICATION: PA FAN; DRAWING NO: C1.013.00622 REV 1; REQUIRED FOR USE ON BOILERS 1 TO 4 AND 6, SCHEDULE 80; COMPLETE WITH WASHER AND SCREW","EA",50,null,0]
["0250358 ","ROD: TYPE: CONNECTING; DIMENSIONS: DIA 1/4 X LG 1-3/4 IN; MATERIAL: STL; APPLICATION: SOOTBLOWER; DRAWING NO: FB7869/20-542 REV 1; REQUIRED FOR VALVE GEAR ASSEMBLY; COMPLETE WITH NUT FOR USE AT HOPKINSONS; UNITS 1 TO 6","EA",50,null,0]
["0250360","ROD: TYPE: CONNECTING; DIMENSIONS: DIA 1/4 X LG 8-1/2 IN; MATERIAL: STL; APPLICATION: SOOTBLOWER; DRAWING NO: FB7869/20-542A REV 1; REQUIRED FOR USE ON HOPKINSONS; UNITS 1 TO 6; COMPLETE WITH LEFT HAND NUT","EA",50,null,0]
["0252340 ","ROD: TYPE: COUPLING; MATERIAL: STL GR EN8; APPLICATION: MONO PUMP 91M; SUPPL P/N: 14320; VAAL DAM","EA",50,null,0]
["0252378 ","ROD: TYPE: TELL TALE; DIMENSIONS: DIA 13 X LG 826 MM; MATERIAL: MS; APPLICATION: ASH HOPPER; SUPPL P/N: KA267/1; UNIT 1, 2, 3, 4 AND 6","EA",50,null,0]
["0252891","ROD: TYPE: ADJUSTING; DIMENSIONS: DIA 16 X LG 300 MM; MATERIAL: CS ASTM A193; 70211/B838/34575/0015 0; REQUIRED FOR SECONDARY SWIRLER ON PF BURNER; UNIT 1 TO 6","EA",50,null,0]
["0571825 ","ROD, THREADED: DIAMETER: 10 MM; THREAD: M10; LENGTH: 1 M; MATERIAL: SS GR 316","EA",69,null,0]
["0571826 ","ROD, THREADED: DIAMETER: 12 MM; THREAD: M12; LENGTH: 1 M; MATERIAL: SS GR 316","EA",63,null,0]
["0571827 ","ROD, THREADED: DIAMETER: 16 MM; THREAD: M16; LENGTH: 1 M; MATERIAL: SS GR 316","EA",104,null,0]
["0571828 ","ROD, THREADED: DIAMETER: 20 MM; THREAD: M20; LENGTH: 1 M; MATERIAL: SS GR 316","EA",50,null,0]
[]
[{"$nulls":4},"Sub-total"]