{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":54,"n_cols":2,"rows_kept":54}
["001007048","WASHER, FLAT; INSIDE DIAMETER: 13 MM, OUTSIDE DIAMETER: , THICKNESS: 2.5 MM, MATERIAL: STEEL, SIZE DESIGNATION: M12, FINISH: ELECTROPLATED, PERIPHERAL SHAPE STYLE: ROUND; STANDARD: SABS 1149, LA; SABS 1149"]
["001007061","WASHER, FLAT; INSIDE DIAMETER: M16, OUTSIDE DIAMETER: 17 MM, THICKNESS: 3 MM, MATERIAL: STEEL, MATERIAL GRADE: 2, FINISH: ELECTROPLATED, PERIPHERAL SHAPE STYLE: ROUND; SABS 1149 TABLE 3; 95KG"]
["001007073","WASHER, FLAT; INSIDE DIAMETER: 21 MM, OUTSIDE DIAMETER: 37 MM, THICKNESS: 3 MM, MATERIAL: STEEL, SIZ E: 59 KG, FINISH: BLACK, PERIPHERAL SHAPE STYLE: ROUND; STANDARD: SABS1149, LA"]
["001007101","WASHER, FLAT; INSIDE DIAMETER: 39 MM, OUTSIDE DIAMETER: 66 MM, THICKNESS: 5 MM, MATERIAL: STEEL, SIZ ADE: 2, FINISH: BLACK, PERIPHERAL SHAPE STYLE: ROUND;  MATERIAL NUMBER : 001007101; UNIT OF ISSUE KG 49/LATEST TABLE 3: NORMAL"]
["001010294","PIN SPLIT             1.6 X 20"]
["001010423","PIN SPLIT 3.2mm dia x 20mm nominal len STEEL"]
["001010512","PIN, COTTER SPLIT; MATERIAL: STEEL, DIAMETER: 4 MM, LENGTH: 40 MM, FINISH: ELECTROPLATED; JOURNAL JACKS DUFF-NORTON 35 TON NO 3510 -C-2 SABS 796/LATEST DIN 94/LATEST NO.3510-C-2 35 TON S-2-18"]
["001010649","PIN SPLIT SABS 796/LATEST 6.3mm dia x 32mm NOMINAL LEN STEEL"]
["001010738","PIN SPLIT 8x40"]
["001010763","PIN, COTTER SPLIT; MATERIAL: STEEL, DIAMETER: 8 MM, LENGTH: 63 MM, PACKAGE TYPE: BOX 100; N.B FOR LOCOMOTIVES DURBAN; NB NB: FOR CAPITAL PARK PLANT 1418 - SUPPLY IN BOXES/BATCHES/PACKETS OF 100"]
["001010839","PIN, COTTER SPLIT; MATERIAL: STEEL, DIAMETER: 10 MM, LENGTH: 56 MM; SABS796; NB: FOR CAPITAL PARK PLANT 1418 - SUPPLY IN BOXES/BATCHES/PACKETS OF 100"]
["001010840","PIN, COTTER SPLIT; MATERIAL: STEEL, DIAMETER: 10 MM, LENGTH: 63 MM;  E/PLATED; PLEASE NOTE FOR LOCOM"]
["001010852","PIN, COTTER SPLIT; MATERIAL: STEEL, DIAMETER: 10 MM, LENGTH: 80 MM;  NB: FOR CAPITAL PARK PLANT 1418 ETS"]
["001014307","BOLT ASSEMBLY; HEX HEAD M16X180MM & NUT 3/KG ELECTRO-PLATED"]
["001016116","NUT, SELF-LOCKING; MATERIAL: STEEL, THREAD SERIES: M10, LOCKING FEATURE: NYLOC, SURFACE TREATMENT: G 10M2S1, PRECISION, NORNAL THICKNESS"]
["001016128","NUT, SELF-LOCKING; MATERIAL: STEEL, THREAD SERIES: M12, LOCKING FEATURE: NYLOC, SURFACE TREATMENT: ZINC PLATED; HEXAGON PRECISION, DIN 985"]
["001016141","NUT, SELF-LOCKING; THREAD SERIES: M24, LOCKING FEATURE: NYLOC, SURFACE TREATMENT: PLATED; HEXAGON BS4929/1"]
["001030530","BOLT ASSEMBLY; WITH NUT; HEX M8X40 25/KG"]
["001033090","NUT, SELF-LOCKING; THREAD DIAMETER: M16, MATERIAL: STEEL, THREAD SERIES: METRIC, LOCKING FEATURE: NY CE TREATMENT: ZINC PLATED, WIDTH ACROSS FLATS: 24 MM, NUT HEIGHT: 15.3 MM, PACKAGE TYPE: BOX 100; SP 10M5,10M2S1; NB: FOR CAPITAL PARK PLANT 1418 - SUPPLY ONLY  IN BOXES AND BATCHES OF 100"]
["001046256","RIVET, LOCKBOLT; TYPE: HUCKBOLT, BOLT DIAMETER: 19 MM, MATERIAL: CARBON STEEL, HEAD SHAPE: ROUND, GRIP RANGE: 24 TO 31 MM, BOLT PROTECTIVE COATING: BLACK; P/N: C50LR-BR24-16RDHD 19-24RT, AVLOCK INTERNATIONAL ROCHDALE; MANUFACTURER: AVLOCK INTERNATIONAL ROCHDALE; RDHD 19-24RT"]
["001046268","PIN-RIVET TYPE GROOVED HUCKBOLT MATERIAL CARBON STEEL DIAMETER 19-31 RT HEAD STYLE ROUND P/N: C50LR-BR24-20RDHD (19-31RT) HUCK 31MM-37MM; 19-31 RT"]
["001048178","STUD PLAIN 3/8 X 1 1/4 INS BSW **NTBR** AT PLANT 1301 ONLY SEE ITEM 001048191, 001000834"]
["001049010","RIVET, LOCKBOLT; TYPE: HUCKBOLT, BOLT DIAMETER: 19 MM, MATERIAL: CARBON STEEL, HEAD SHAPE: ROUND, GR TECTIVE COATING: BLACK; P/N: C50LR-BR24-12, HUCK; MANUFACTURER: AVLOCK INTERNATIONAL; 19-18 RT"]
["001049046","RIVET, LOCKBOLT; TYPE: HUCKBOLT, BOLT DIAMETER: 19 MM, MATERIAL: CARBON STEEL, HEAD SHAPE: ROUND, GRIP RANGE: 37 TO 44 MM, BOLT PROTECTIVE COATING: BLACK; 19-37RT"]
["001049248","COLLAR, PIN-RIVET TYPE LOCK DIMENSIONS DIA 12.7 MM P/N: LC-2R16G UNKNOWN 13S"]
["001049261","COLLAR, LOCK PIN P/N: LC-2R24G 19S UNKNOWN SPEC.SAE 1113 LATEST"]
["001052178","RIVET, LOCKBOLT; TYPE: HUCKBOLT, BOLT DIAMETER: 12.7 MM, MATERIAL: STEEL, HEAD SHAPE: ROUND, GRIP RA TECTIVE COATING: BLACK PLAIN; P/N: C50LR-BR16-24, HUCK; SUPPLIER: AVLOCK INTERNATIONAL; 13-37 RT; PU"]
["001061804","NUT, SELF-LOCKING; THREAD DIAMETER: M20, MATERIAL: STEEL, THREAD SERIES: METRIC, LOCKING FEATURE: NY ZED, PACKAGE TYPE: BAG 100; HEXAGON BS4924 PRT1, PLEASE NOTE: FOR LOCOMOTIVES DURBAN; NB: FOR CAPITA OXES/BATCHES/PACKETS OF 100"]
["001113809","SCREW, MACHINE; DIAMETER: M16, LENGTH: 50 MM, MATERIAL: STEEL, MATERIAL GRADE: 8.8, HEAD STYLE: HEXA GON SOCKET, THREAD SERIES: METRIC; BLACK STEEL"]
["001113812","SCREW, MACHINE; DIAMETER: M12, LENGTH: 55 MM, MATERIAL: STEEL, MATERIAL GRADE: 8.8, HEAD STYLE: HEXA GON SOCKET, THREAD SERIES: METRIC; BLACK STEEL"]
["001669623","PIN, COTTER SPLIT; MATERIAL: STEEL, DIAMETER: 10 MM, LENGTH: 45 MM, FINISH: ZINC PLATED;  SPECIFICAT"]
["001700277","BOLT HEX HEAD HIGH TENSILE M12X50 GRADE 8.8 DELIVERY TO GERMISTON: BOLTS(GR8.8) TO BE PACKED IN A CLEAR PLASTIC BAG WITH 10EA/BAG."]
["001803230","WASHER, FLAT; INSIDE DIAMETER: 8 MM, OUTSIDE DIAMETER: 16 MM, THICKNESS: 1 MM, MATERIAL: STEEL, SIZE APE STYLE: ROUND"]
["062003673","STUD, PLAIN; DIAMETER: 5/8 IN, STUD OVERALL LENGTH: 170 MM, MATERIAL: STEEL, THREAD SERIES: BSW, SPE N: 74520 B69271/2, WABCO"]
["068084311","CLIP, SPRING TENSION TYPE RETAIN ANCHOR PACKAGE TYPE BAG 50 HS BOGIE, MK5 RETAIN ANCHOR CME68_084311_420_C DRAWING NO: CME 68/084311-420 REV B FOR GERMISTON PLANT ORDERS ONLY: THE SUPPLIER IS RESPONSIBLE TO INFORM THE ENGINEERING MANAGER IN TRANSNET ENGINEERING GERMISTON FOR APPROVAL OF FIRST SAMPLE ITEM BEFORE PROCEEDING WITH THE REST OF THE PRODUCTION ORDER; THE SUPPLIER MAY NOT REQUEST FOR THE FIRST SAMPLE ITEM TO BE APPROVED IF SUPPLYING THE SAME ITEM THAT HAS BEEN PREVIOUSLY APPROVED WITH THE SAME DRAWING REVISION; IF THE DRAWING HAS BEEN REVISED, AN APPROVAL WILL BE REQUIRED; THE SUPPLIER WILL BE RESPONSIBLE TO MODIFY ALL DELIVERED INCORRECT MATERIALS IF THE FIRST SAMPLE ITEM WAS NOT APPROVED BY PRODUCT DEVELOPMENT SECTION; FIRST COMPLETED AND SIGNED OFF SAMPLE ITEM TO BE MARKED BY TRANSNET ENGINEERING INSPECTOR."]
["301028439","NUT, SELF-LOCKING; THREAD SERIES: M8, LOCKING FEATURE: NYLOC, SURFACE TREATMENT: PLATED; HEXAGON BS"]
["301028714","NUT, SELF-LOCKING; THREAD SERIES: M6, LOCKING FEATURE: NYLOC, SURFACE TREATMENT: PLATED; HEXAGON BS"]
["301109512","RIVET, SOLID; TYPE: SNAP HEAD, SHANK DIAMETER: M6, LENGTH: 16 MM, RIVET MATERIAL: STEEL;  BRAKE BLOC"]
["301109897","NUT, HEXAGON; NUT STYLE: PLAIN, THREAD DIAMETER: 5/8 IN, MATERIAL: STEEL, SPECIAL FEATURES: ZINC PLATED; PLAIN"]
["301111676","BOLT HEX M10X30  ISUED IN EACH"]
["301112388","WASHER, FLAT; INSIDE DIAMETER: 14 MM, OUTSIDE DIAMETER: 30 MM, THICKNESS: 3 MM, MATERIAL: STEEL, SIZ TURES: ELECTROPLATED, FINISH: ZINC PLATED, PERIPHERAL SHAPE STYLE: ROUND"]
["301112523","BOLT; HIGH TENSILE, HEX HEAD, M10 X 50MM"]
["301112563","BOLT HIGH TENSILE M20X110"]
["301200006","SETSCREW;  HEX M8X40 BLACK 8,8"]
["301201445","NUT, HEXAGON; PLAIN STEEL; M10; ISSUED IN EACH; SABS135"]
["301201518","WASHER FLAT M10 STEEL ISSUED IN EACH"]
["301201520","WASHER FLAT M16 STEEL ISSUED IN EACH"]
["301201521","WASHER FLAT M30 STEEL ISSUED IN EACH"]
["301201524","WASHER, BEVEL TYPE TAPER SIZE DESIGNATION M20 WASHER MATERIAL STEEL ISSUED IN EACH"]
["301201530","WASHER, FLAT SIZE DESIGNATION M27 FINISH BLACK"]
["301201552","COLLAR, PIN-RIVET TYPE LOCK DIMENSIONS DIA 19 MM P/N: 3LC-2R24G AVLOCK INTERNATIONAL (19F)"]
["368029091","BOLT, EYE; TYPE: BRAKE RELEASE SPRING, THREAD DIAMETER: 16 MM, EYE DIAMETER: 16 MM, MATERIAL: STEEL, HREAD SERIES: METRIC, THREAD PITCH: 1.95 MM, SHANK LENGTH: 170 MM, SPECIAL FEATURES: 3.2 MM HOLE"]
["801068200","RIVET, BLIND TYPE POP SHANK DIAMETER 4.8 MM LENGTH 15 MM RIVET MATERIAL STAINLESS STEEL 10M3, 10M5, 10M2S1"]
["914400445","BOLT HEX HEAD M10x35 GRADE: 8.8"]