{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["3-TON BATTERY-OPERATED PALLET T"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"3-TON BATTERY-OPERATED PALLET T","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"merged":[[0,0,0,7],[1,0,1,7],[2,0,3,7],[6,3,6,7],[20,3,20,7],[23,3,23,7],[27,3,27,7]]}
["ANNEXURE A. : TECHNICAL SPECIFICATION"]
["THE APPOINTMET OF A SERVICE PROVIDER TO PROVIDE ONCE OFF SUPPLY AND DELIVERY OF 3-TON BATTERY-OPERATED PALLET TRUCKS WHICH INCLUDES MAINTENANCE TO GAUTENG MEDICAL SUPPLIES DEPOT"]
["Note:                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                              a. The Product Specification in MS Excel format that is attached below must be completed and submitted in its original format.\nb.Bidders will score a weighting of ‘2’ or ‘1’ depending on the weighting requirement per line item. Where a bid is non-compliant with the specification/s of that line item the bid will be scored ‘0’. \nc. The scoring of the bids:\ni.Weights:                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                     \n-Each specification will have a weight of 1, or a 2, which indicates the level of importance, as follows: \n- A specification (line item) with a weight of 2 is a specification with a very high level of importancy that should be complied with.                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                \n- A specification (line item) with a 1 weight is a specification with a standard level of importance \nd. Bidders are required to indicate compliance/non-compliance with the specification by typing 'YES/NO' on each line item on column C.\ne. In the case where a bidder indicated ‘No’ in column ‘C’ and an equivalent or better option is provided, bidders must type ‘Yes’ on column D. Details of the equivalent/better option must be provided on column E. Bidders must note that where an equivalent or better option is provided, a weighting of ‘1’ will be allocated irrespective of the stated weighting requirement in that line item.\nf. Bidders must score a minimum threshold of 31 out 35 to qualify for the next stage of evaluation.\ng. Bidder to provide reference to brochure (page number) / technical data sheet / Any supporting documents on column G.                                                                                                                                                                                                                                                                                                                                                                                                                                "]
[]
["A","B",null,"C","D","E","F","G"]
["Item no.","Technical Specification","Weighting","Comply (Yes/No)","Provide Equivalent/Better          (if applicable)","Comments on Equivalent/Better","Details of Product Offer                                           (Provide your answers in this Column. You are advised to be straight to the point)","Reference to Brochure / Technical Data Sheet (verification) /  Supporting Document"]
["A"]
["A.1","Electric Pallet truck (Pedestrian Type) ",2]
["A.2","Battery-Operated (lithium) 24V-48V/300Ah-500Ah",2]
["A.3","Rated Capacity: minimum of 3000kg and minimum of 3 Ton",2]
["A.4","Driving Wheels: Polyurethane",1]
["A.5","Lift Height: minimum of 140mm or higher",2]
["A.6","Fork Length: 1200mm",2]
["A.7","Fork Width: minimum of 685mm to 700mm",1]
["A.8","Fork Height: minimum 54mm to 56mm (the truck must enter and exit pallets easily)",2]
["A.9","Travel Speed: 10 -12 km/h",2]
["A.10","Service Brake Type: Electromagnetic ",2]
["A.11","Battery Voltage / Nominal Capacity: 24V-48V/300Ah-500Ah",2]
["A.12","Type Of Drive Control: AC",2]
["A.13","Horn: functional ",1]
["B","Performance: "]
["B.1","AC system to offer strong power (drive motor of 0.8 to 2.0kW and lift motor of 1.0 to 2.2kW)",2]
["B.2","Low noise but durable hydraulic unit  </= 65 dB, good quality cylinder pressure tested to 250 bar  ",2]
["C","Safety:"]
["C.1","Emergency reverse belly button to protect the operator from getting hurt.",2]
["C.2","Emergency disconnector which will cut off the power source to avoid accidents when truck goes out of control.",2]
["C.3","Anti-rolling back brake that will keep the truck from skidding down when truck is out of control or when travelling on ramp.",2]
["D","Operation:"]
["D.1","Electric power steering for smooth and comfortable operation in small areas.",2]
[null,"Minimum threshold requirement ",31]