{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Preliminary & General","Building","Summary"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Preliminary & General","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[54,0,54,5]]}
["Item No","LIC","Description","Unit","Quantity","Rate","AMOUNT"]
["SABS",null,"GENERAL (SMALL WORKS)"]
["1200AA"]
[]
[8.3,null,"SCHEDULED FIXED-CHARGE AND VALUE-RELATED ITEMS"]
[]
["8.3.1",null,"Contractual requirements",{"v":1,"d":"1.00"},{"v":1,"d":"1.00"}]
[]
["8.3.2",null,"Establishment of facilities on the site"]
[]
[null,null,"a) Facilities required by Engineer"]
["PSAB 1 ",null,"Contract sign boards","No",1]
[]
["PSAB 3 ",null,"Celluar phone"," Sum",1]
[]
[null,null,"b) Facilities required by Contractor","Sum",1]
[]
["8.3.3",null,"General responsibilities and other fixed charge obligations","Sum",1]
[]
["8.3.4",null,"Removal of site establishment","Sum",1]
[]
["PSA 1",null,"Compliance with the OHS Act regulations","Sum",1]
[]
[]
[8.4,null,"SCHEDULED TIME-RELATED ITEMS"]
[]
["8.4.1",null,"Contractual requirements","Sum",1]
[]
["8.4.2",null,"Operation and Maintenance of Facilities on Site"]
[]
[null,null,"a) Facilities required by Engineer","Sum",1]
[]
[null,null,"b) Facilities required by Contractor","Sum",1]
[]
["8.4.3",null,"General responsibilities and other time related obligations","Sum",1]
[]
["8.4.4",null,"Community Liaison Officer","Prov Sum",1,null,{"v":30000,"d":"30,000.00"}]
["8.4.5",null,"Overheads and profit on item 8.4.4","%"]
[]
["8.4.6",null,"Allowance for PSC Meeting sit in","Prov Sum",1,null,{"v":15000,"d":"15,000.00"}]
["8.4.7",null,"Overheads and profit on item 8.4.6","%"]
{"$rows_empty":13}
["Total Carried to Summary "]

{"sheet":"Building","index":1,"n_rows":1810,"n_cols":7,"rows_kept":1810,"merged":[[76,0,76,5],[84,3,85,3],[179,0,179,5],[237,0,237,5],[259,2,260,2],[341,0,341,5],[344,0,344,5],[373,0,373,5],[376,0,376,5],[431,0,431,5],[434,0,434,5]]}
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[2,null,"EX CAVATION,ETC"]
[]
["2.1",null,"Site clearance etc:"]
[]
["2.1.1",null,"Allow for clearing the area of the site to be built upon of all grass,weeds,shrubs,trees with trunks not exceeding 200mm girth,debris,etc.,including grubbing up all roots, scoffing up as required and cart away all vegetation and debris.","ha",1]
[]
["2.2",null,"Bulk Excacvation"]
[]
["2.2.1",null,"Excavate to reduce levels in open face and ","m³",20]
[null,null,"deposit on site in spoil heaps"]
[]
["2.3",null,"Excavate in earth not exceeding 2m deep:"]
["2.3.1",null,"Trenches.","m³",38]
[]
["2.3.2",null,"Bases.","m³",1]
[]
["2.3.3",null,"Reduced levels under floors.","m³",29]
[]
["2.3.4",null,"Toilet pit.","m³",15]
[]
["2.4",null,"Excavation in earth exceeding 2m and not exceeding 4m deep:"]
[]
["2.4.1",null,"Trenches.","m³",1]
[]
["2.4.2",null,"Toilet pit.","m³",1]
[]
["2.6",null,"Extra over trench and hole excavations in"]
[null,null,"earth for excavation in :"]
[]
["2.6.1",null,"Soft rock.","m³",12]
[]
["2.6.2",null,"Hard rock.","m³",5]
[]
["2.7",null,"Extra over all excavations for carting away:"]
[]
["2.7.1",null,"Surplus material from excavations and/or stock","m³",58]
[null,null,"piles on site to a dumping site to be located"]
[null,null,"by the contractor."]
[]
["Total summary  carried to next page"]
[]
["Total summary carried from previous page"]
["2.8",null,"Risk of collapse of excavations:"]
[]
["2.8.1",null,"Sides of trench and hole excavations not","m2",155]
[null,null,"exceeding 1.5m deep"]
[]
["2.8.2",null,"Sides of trench and hole excavations ","m2",9]
[null,null,"exceeding 1.5m deep."]
[]
["2.9",null,"keeping excvavations free of water;"]
[]
["2.9.1",null,"Keeping excavations free from mud and all",null,"item"]
[null,null,"water including subterranean sources."]
[]
["2.10",null,"EARTH FILLING,ETC."]
[]
[null,null,"Earth filling obtained from the excavation"]
[null,null,"and/or prescribed  stock piles on site"]
[null,null,"compacted to 95% Mod. AASHTO density:"]
[]
["2.10.1",null,"Backfilling to trenches,holes.etc","m³",21]
[]
["2.10.2",null,"Under floors,steps,pavings,etc","m³",8]
[]
["2.11",null,"Earth filing supplied by the contractor "]
[null,null,"compacted to 95% Mod AASHTO density:"]
[]
["2.11.1",null,"Under floors,steps,pavings,etc","m³",54]
[]
["2.12",null,"Coarse river sand filling supplied by the"]
[null,null,"contractor"]
[]
["2.12.1",null,"Under floors etc. (Provisional)","m³",4]
[]
["Total summary  carried to next page"]
[]
[]
["Total summary carried from previous page"]
[]
["2.14",null,"Compaction of surfaces:"]
[]
["2.14.1",null,"Compaction of ground surface under floors etc ","m2",113]
[null,null,"including scarifying for a depth of 150mm,"]
[null,null,"breaking down oversize material,adding suitable"]
[null,null,"where necessary and compacting to 93% Mod"]
[null,null,"AASHTO density."]
[]
["2.15",null,"Prescribed density tests on filling:"]
[]
["2.15.1",null,"Allow for compaction tests by an approved"]
[null,null,"laboratory to determine density of filling"]
[null,null,"material.","No",2]
{"$rows_empty":40}
["Total carried to summary"]
[]
[]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[3,null,"CONCRETE,FORMWORK AND "]
[null,null,"REINFORCEMENT"]
[]
[null,null,"UNREINFORCED CONCRETE CAST AGAINST"]
[null,null,"EXCAVATION SURFACES"]
[]
["3.1",null,"15MPa/20mm concrete:"]
[]
["3.1.1",null,"Footings to walls (Provisional).","m³",8]
[]
["3.2",null,"20MPa/20mm concrete:"]
[]
["3.2.1",null,"Surface beds on waterproofing.","m³",7]
[]
["3.2.2",null,"Surface beds cast in panels  on waterproofing","m³",2]
[]
["3.2.3",null,"Bases (Provisional)","m³",1]
[]
["3.3",null,"25MPa/20mm concrete:"]
[]
["3.3.1",null,"Footings to walls (Provisional).","m³",3]
[]
["3.3.2",null,"Surfaces beds.","m³",1]
[]
["3.4",null,"REINFORCED CONCRETE CAST FORMWORK"]
[]
[null,null,"25MPa/20mm concrete:"]
[]
["3.4.1",null,"Slabs,including beams and inverted beams.","m³",1]
[]
["3.5",null,"CONCRETE TESTS"]
[]
[null,null,"Test blocks:"]
[]
["3.5.1",null,"Making and testing set of three 150x150x150mm"]
[null,null,"concrete strengtrh test cubes (Provisional).","No",4]
[]
[]
[]
[]
[]
["Total summary  carried to next page"]
[]
[]
["Total summary carried from previous page"]
[]
["3.6",null,"Finishing top surfaces of concrete "]
[null,null,"smooth with a wood float:"]
[]
["3.6.1",null,"Surface beds,slabs,etc.","m2",2]
[]
["3.6.2",null,"Surface beds to falls.","m2",17]
[]
["3.7",null,"Finishing top of concrete to an evenly "]
[null,null,"ribbed non-slip surface (broom finish):"]
[]
["3.7.1",null,"Suirface beds to falls.","m2",24]
[]
["3.8",null,"ROUGH FORMWORK (DEGREE OF ACCURACY"]
[null,null,"III) (CPAP Work Group No 111):"]
[]
[null,null,"Permanent Formwork to sides and soffits:"]
[]
["3.8.1",null,"Slabs propped up not exceeding 3.5m high.","m2",3]
[]
[null,null,"Extra on permanent boxing or blocking"]
[null,null,"in or boxing out to form:"]
[]
["3.8.2",null,"120mm Diameter opening through 125mm thick","No",3]
[null,null,"slab (Provisi0onal)."]
[]
["3.8.3",null,"235mm Diameter opening through 125mm thick","No",3]
[null,null,"slab"]
[]
[null,null,"Smooth formwork to sides:"]
[]
["3.8.4",null,"Edges,risers,ends and reveals not exceeding","m",30]
[null,null,"300mm high or wide."]
[]
["3.9",null,"MOVEMENT JOINTS ETC"]
[]
[null,null,"Expansion joints with bitumen "]
[null,null,"impregnated softboard between vertical "]
[null,null,"concrete or brick surfaces:"]
[]
["3.9.1",null,"10mm Joints not exceeding 300mm high ","m",40]
[null,null,"(Provisional)."]
[]
["3.10",null,"Approved polysulphide sealing compound"]
[null,null,"including backing cord,bond breaker,"]
[null,null,"primer etc"]
[]
["3.10.1",null,"10x10mmm In Vertical expansion joints between","m",40]
[null,null,"concrete and brick surfaces,including"]
[null,null,"raking out expansion joint filler as necessary"]
[null,null,"(Provisional)."]
[]
[]
[]
["Total summary  carried to next page"]
[]
[]
["Total summary carried from previous page"]
[]
[null,null,"Vertical construction joints through"]
[null,null,"concrete including thick cement"]
[null,null,"slurry to one face.:"]
[]
[1,null,"Surface beds not exceeding 300mm thick.","m",16]
[]
[null,null,"REINFORCEMENT (PROVISIONAL)"]
[]
[null,null,"Fabric reinforcerment:"]
[]
[2,null,"REF.193 fabric reinforcement in concrete","m2",70]
[null,null,"surface beds,slabs,etc."]
[]
[3,null,"10mm Diameter bars.","kg",58]
{"$rows_empty":36}
["Total carried to summary"]
[]
[]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[4,null,"PRECAST CONCRETE"]
[]
["4.1",null,"'Windblok modular precast concrete"]
[null,null,"window surrounds etc.finished smooth"]
[null,null,"on exposed surfaces,including bedding,"]
[null,null,"bedding and pointing:"]
[]
["4.1.1",null,"590 x 590 x 260 Type WB 260 window ","No",52]
[null,null,"surround."]
[]
["4.2",null,"PRECAST CONCRETE COPINGS ETC"]
[]
[null,null,"Precast concrete finished smooth on"]
[null,null,"exposed surfaces including bedding,"]
[null,null,"jointing and pointing:"]
[]
["4.2.1",null,"750 mm Diameter concrete manhole ring 1000mm","No",2]
[null,null,"long set vertically on prepared filling(elsewhere"]
[null,null,"measured) and filling with mass concrete"]
[null,null,"(elsewhere measured) as base for veranda"]
[null,null,"pole (measured elsewhere)."]
[]
["4.3",null,"BLOCKWORK IN FOUNDATION (PRVOVISIONAL)"]
[]
[null,null,"Blockwork in foundations is to be concrete metric modular masonry units of 7MPa nominal compressive strength in mortar composed of 6 parts (by volume) of sand 1 part (by volume) of cement:"]
["4.3.1",null,"140mm Block walls.","m2",44]
[]
[null,null,"Blockwork in superstructure is to be"]
[null,null,"concrete metric modular masonry units"]
[null,null,"of 7MPa nominal compressive strength"]
[null,null,"in mortar composed of 6 parts (by volume) of sand and 1 part (by volume)"]
[null,null,"of cement:"]
[]
["4.3.2",null,"140mm Block walls.","m2",9]
[]
["4.4",null,"BRICKWORK IN FOUNDATION (PROVISIONAL)"]
[null,null,"Brickwork of NFX bricks (14 Mpa nominal compressive srength) in Class I mortar:"]
[]
["4.4.1",null,"One brick walls.","m2",148]
[]
["4.4.2",null,"Mass brickwork in piers.","m³",1.4]
[]
[]
[]
[]
["Total summary  carried forward"]
[]
[]
["Total carried forward from previous page"]
[null,null,"Brickwork of NFP bricks (14MPa nominal compressive strength) in Class II mortar:"]
["4.4.3",null,"Half brick walls in beamfilling.","m2",13]
[]
["4.4.4",null,"One brick walls.","m2",110]
[]
["4.4.5",null,"Mass brickwork in piers.","m³",1]
[]
["4.6",null,"BRICKWORK AND BLOCKWORK SUNDRIES"]
[]
[null,null,"Weepholes,openings etc."]
[]
["4.6.1",null,"Form hole size 50 x 200mm thick through 140mm","No",47]
[null,null,"block wall."]
[]
["4.6.2",null,"Form weep hole size 100 x 250mm thick","No",4]
[null,null,"through 140mm face block wall."]
[]
["4.6.3",null,"Form window opening size 190 x 190mm high","No",4]
[null,null,"(half block) through 140mm face block."]
[]
["4.7",null,"Bagging and sealing the outer face of"]
[null,null,"the inner skin of walls with 1:3 cement"]
[null,null,"and sand mixture and seal with two coats ''Brixeal'' bitumen emulsion waterproofing coating:"]
[]
["4.7.1",null,"To walls (Provisional).","m2",110]
[]
[]
[]
["Total summary  carried to next page"]
[]
[]
["Total carried forward from previous page"]
[]
["4.8",null,"Brickwork reinforcement:"]
[]
["4.8.1",null,"75 mm wide reinforcement built in ","m",58]
[null,null,"horizontally."]
[]
["4.8.2",null,"150mm Wide reinforcement built in horizontally","m",447]
[]
["4.8.3",null,"Ditto,but in foundations (Provisional).","m",678]
[]
["4.8.4",null,"110 x 75 mm Lintels in lengths not exceeding 3m.","m",13]
[]
[null,null,"Turning pieces:"]
[]
["4.8.5",null,"200mm Wide turning piece ito lintels etc","m",5]
[]
[null,null,"Galvanished wire ties etc :"]
[]
["4.8.6",null,"4mm Diameter roof tie 1500mm long with one ","No",18]
[null,null,"end fixed to timber and other built into brickwork"]
[null,null,"or concrete."]
[]
[null,null,"Cramps.ties etc :"]
[]
["4.8.7",null,"30 x 2mm Galvanized roof tie 1500mm long with"]
[null,null,"one end fixed to timber and other built inton "]
[null,null,"brickwork or concrete."]
[]
[null,null,"Air bricks etc ;"]
[]
["4.8.8",null,"30 X 160mm Cement vermin proof air brick."]
[]
["4.9",null,"FACE BLOCKWORK"]
[]
[null,null,"Face blockwork is to be approved ''earth''"]
[null,null,"coloured modular masonry blocks pointed"]
[null,null,"with square ruled recessed horizontal"]
[null,null,"and vertical joints."]
[]
["4.9.1",null,"140mm Block walls pointed on both sides.","m2",53]
[]
["4.9.2",null,"140mm Block walls pointed on both sides in","m2",3]
[null,null,"beamfilling"]
[]
["4.9.3",null,"Extra over blockwork for face blockwork","m2",11]
[null,null,"externally."]
[]
["4.9.4",null,"Fair raking cutting.","m",7]
[]
[]
[]
[]
[]
[]
["Total summary  carried to next page"]
[]
[]
["Total carried forward from previous page"]
[]
[null,null,"Facebricks (FBS) prime cost R3 500.00"]
[null,null,"per thousand exclusive VAT delivered "]
[null,null,"to the site pointed with square ruled "]
[null,null,"recessed horizontal and vertical joints:"]
[]
["4.9.5",null,"Extra over brickwork for face brickwork ","m2",141]
[null,null,"externally."]
[]
["4.9.6",null,"Ditto,but foundations (Provisional).","m2",21]
[]
["4.9.7",null,"Fair raking cutting","m",22]
[]
[null,null,"Brick-on-edge header course coping,sills"]
[null,null,"etc with recessed joints on all exposed"]
[null,null,"faces:"]
[]
["4.9.8",null,"220mm Wide header course to top of one brick","m",14]
[null,null,"wall bedded and jointed in cement mortar and"]
[null,null,"pointed on top and both sides as described."]
[]
["4.9.9",null,"220mm Wide lintel pointed on face and 110mm","m",2]
[null,null,"soffit."]
[]
["4.9.10",null,"220mm Wide lintel pointed on face and 220mm","m",4]
[null,null,"soffit."]
{"$rows_empty":29}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[5,null,"MASONRY"]
[]
["5.1",null,"DAMPINGPROOFING OF WALLS AND FLOORS"]
[]
[null,null,"One layer of 250 micron 'USB GREEN'"]
[null,null,"water sheeting sealed at laps with "]
[null,null,"Gunplas Pressure Sensitive Tape:"]
[]
["5.1.1",null,"Under surface beds.","m2",107]
[]
[null,null,"One layer of 375 micron embosed "]
[null,null,"dampcourse waterproof sheeting below"]
[null,null,"walls,sills,etc:"]
[]
["5.1.2",null,"Below walls,sills,etc.","m2",19]
[]
[null,null,"Clear Neutral silicone Sealant:"]
[]
["5.1.3",null,"In joint sealing and pointing all round external","m",51]
[null,null,"window and door frames."]
{"$rows_empty":35}
["Total summary carried to next page"]
[]
[]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[6,null,"WATERPROOFING"]
[]
[null,null,"RIBBED SHEETING AND ACCESSORIES"]
[]
[null,null,"0.58mm Nominal thickness corrugate iron"]
[null,null,"roof sheets with silicone polyster top"]
[null,null,"finish or colomet equal,colour ''blue'' to"]
[null,null,"one side ans standard grey backing coat "]
[null,null,"to other side etc. with 275g/m2 galvanising"]
[null,null,"to both sides with one and a half"]
[null,null,"corrugation side lap including fixing to"]
[null,null,"timber purlins at approximately 1,00mm"]
[null,null,"centres including all screws,bolts"]
[null,null,"washers,etc. strictly in accordance with"]
[null,null,"manufactturer's specification"]
[]
["6.1",null,"Roof covering with pitch not exceeding ","m2",261]
[null,null,"50 degrees,"]
[]
[null,null,"0,8mm Nominal thickness ditto,but"]
[null,null,"flashings:"]
[]
["6.1.1",null,"Ridge 460mm girth with minimum 230mm","m",10]
[null,null,"laps,fixed to roof "]
[]
["6.1.2",null,"Extra on last,for closed end.","No",2]
{"$rows_empty":29}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[7,null,"ROOF COVERING,ETC"]
[]
["7.1",null,"ROOFS ETC"]
[]
[null,null,"Sawn softwood:"]
[null,null,"x"]
["7.1.1",null,"38 x 114mm Wall plate.","m",58]
[]
["7.1.2",null,"38 x 228mm Gang boarding.(Provisional)","m",10]
[]
["7.1.3",null,"50 x 76mm Purlins.","m",82]
[]
["7.1.4",null,"50 x 76mm Sprockets average 350mm long,brass","No",100]
[null,null,"screwed to purlins."]
[]
[null,null,"Wrought softwood:"]
[]
["7.1.5",null,"38 x 114mm Rafters.","m",25]
[]
["7.1.6",null,"50 x 76mm Purlins.","m",59]
[]
["7.1.7",null,"50 x 76mm Bearer fascia support (Provisional)","m",58]
[]
[null,null,"Sundries:"]
[]
["7.1.8",null,"MiTekeCo hurricane clip fixed using Permfix nails","No",74]
[null,null,"or bolts through pre-drilled holes."]
[]
["7,1.9",null,"Fix only bolt through average 50mm softwood ","No",30]
[null,null,"including drilling hole."]
[]
["7.1.10",null,"Fix only bolt through average 50mm softwood","No",21]
[null,null,"including drilling hole."]
[]
["7.1.11",null,"Fix only bolt through average 70mm softwood","No",17]
[null,null,"including drilling hole."]
[]
[null,null,"Laminated S.A.pine:"]
[]
["7.1.12",null,"75 x 115mm beam.","m",29]
[]
["7.1.13",null,"75 x 150mm beam.","m",271]
{"$rows_empty":14}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[8,null,"CARPENTRY AND JOINERY"]
[]
["8.1",null,"PREFABRICATED ROOF TRUSSES,ETC."]
[]
["8.1.1",null,"Double pitched roof truss 9638mm span ","No",31]
[null,null,"between plates to 25 degree pitch with 600mm"]
[null,null,"eaves overhang both ends."]
[]
["8.1.2",null,"Allow for bracing,cross bracing,connecting,",null,"Item"]
[null,null,"fixing brackets,hurricane clips,etc.,as required"]
[null,null,"for fixing in position of roof trusses as "]
[null,null,"described in accordance with the"]
[null,null,"manufacturer's instructions."]
[]
["8.1.3",null,"12 x 225mm Fascia board three times drilled,and ","m",116]
[null,null,"brass screwed to and including 38 x 50 x 114"]
[null,null,"mm long S.A.Pine cleats twice brass screwed to"]
[null,null,"rafter foot includng galvanised steel H-profile"]
[null,null,"jointing strips,screws,holes etc."]
[]
["8.1.4",null,"Extra on last for splay cut end.","No",4]
[]
["8.1.5",null,"85 x 275 x 6mm Barge board drilled and brass","m",32]
[null,null,"screwed to purlin end including galvanised"]
[null,null,"steel H-profile jointing strips,screws,holes etc."]
[]
["8.2",null,"BEADS,ARCHITRAVES,ETC"]
[]
[null,null,"Wrought merant:"]
[]
["8.2.1",null,"19 x 70mm Skirting fixed to walls incluiding ","m",131]
[null,null,"19mm quandrant bead planted on."]
[]
[null,null,"PINNING BOARDS"]
[]
[null,null,"Bitumen impregnated fibre board:"]
[]
["8.2.1",null,"12mm Insulation board backing plugged and","m2",7]
[null,null,"glued to wall including all square cutting"]
[null,null,"and waste."]
[]
[null,null,"Wrought meranti:"]
[]
["8.2.2",null,"22 x 44mm  Rebated and chamfered ","m",19]
[null,null,"surrounds plugged and screwed to wall at not"]
[null,null,"exceeding 500mm centers,including screws,"]
[null,null,"holes,plugs,etc."]
[]
["8.2.3",null,"22 x 44mm Twice rebated and chamfered ","m",4]
[null,null,"transomes plugged and screwed to wall at not"]
[null,null,"exceeding 500mm centres,including screws,"]
[null,null,"holes,plugs,etc."]
[]
[]
[]
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[9,null,"CEILINGS,PARTITIONS & ACCESS "]
[null,null,"FLOORING"]
[]
["9.1",null,"NAILED UP CEILINGS"]
[]
[null,null,"4mm Fibre-cement boards with 6 x 32mm"]
[null,null,"wrought meranti coverstrips over joints:"]
[]
["9.1.1",null,"Ceilings including 38 x 50mm sawn softwood","m2",261]
[null,null,"brandering at joints,ends of sheets and at"]
[null,null,"light fiitings,etc."]
[]
["9.1.2",null,"Extra over Fibre-cement ceiling for forming trap","No",1]
[null,null,"door size 630 x 630mm in clear formed with"]
[null,null,"38 x 50 mm sawn S.A.pine framing covered "]
[null,null,"with ceiling boarding and set in 38 x 76mm"]
[null,null,"wrought S.A.pine rebated kerb,including"]
[null,null,"trimmers."]
[]
[null,null,"Paper covered polystyrene cornice,or"]
[null,null,"equal approved,plugged to walls ncluding"]
[null,null,"nitres,etc.:"]
[]
["9.1.3",null,"75mm Covered cornice.","m",131]
[]
[null,null,"Non-combustible polyester thermal "]
[null,null,"insulation of density of not less than "]
[null,null,"kg/m³ :"]
[]
["9.1.4",null,"100mm Insulation in blanket form closely fitted","m2",261]
[null,null,"and laid on top of bandering between roof"]
[null,null,"timbers etc."]
{"$rows_empty":24}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[10,null,"FLOOR COVERING,WALL LININGS,Etc."]
[]
[]
["10.1",null,"VINYL FLOOR COVERING,WALL LININGS,"]
[null,null,"ETC."]
[]
[null,null,"300 X 300 X 2.5mm semi-flexible reinforced"]
[null,null,"vinyl quartz floor tiles,or equal approved,"]
[null,null,"laid to manufacturers specification in"]
[null,null,"patterns to coulour of Architects choiuce:"]
[]
["10.1.1",null,"On smooth screeded floors.","m2",261]
[]
["10.2",null,"POLISH,SEALERS,ETC"]
[]
[null,null,"Clean by stripping and sealing and apply"]
[null,null,"three coats water based copolymer"]
[null,null,"emulsion or other approved sealer:"]
[]
["10.2.1",null,"On vinyl flooring.","m2",261]
{"$rows_empty":36}
["Total carried summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[11,null,"IRONMONGERY"]
[]
["11.1",null,"Locks :"]
[]
["11.1.1",null,"Padlock with three keys (Union 3142).","No",12]
[]
[null,null,"BATHROOM FIITTINGS ETC."]
[]
[null,null,"Longarms:"]
[]
["11.1.2",null,"32 mm Diameter polished hardwood longarm ","No",1]
[null,null,"1.2m long fiited with polished brass pole hook,"]
[null,null,"secured in one chromium plated spring clip"]
[null,null,"screwed to and including small polished "]
[null,null,"hardwood block plugged to wall and fitted on"]
[null,null,"hardwood base size 88 x 88mm countersunk"]
[null,null,"for rod plugged to floor,including quandrant"]
[null,null,"planted on."]
[]
[null,null,"Sundries :"]
[]
["11.1.3",null,"50mm Plasic key tag.","No",16]
[]
["11.1.4",null,"40 x 40 x 5mm Thick black acrylic door number ","No",16]
[null,null,"plate with two numbers size 25mm high,"]
[null,null,"engraved with arial font and painted white,fixed"]
[null,null,"to door frame or wall with chromium plated"]
[null,null,"domeheaded screws."]
[]
[null,null,"Sign plates :"]
[]
["11.1.5",null,"152 x 152 x 2mm Anodised silver engraved sign","No",4]
[null,null,"with Fire Extinguisher Pictogram E06,fixed to "]
[null,null,"wall or door (Union AL5066E-06/2AS)."]
[]
["10.2.7",null,"152 x 152 x 2mm Anodised silver engraved sign","No",1]
[null,null,"with Directional Pictogram E08,fixed to wall or "]
[null,null,"door (Union AL5066E-08/2AS)."]
[]
["10.2.8",null,"152 x 152 x 2mm Anoised silver engraved sign","No",2]
[null,null,"with Male/Female Pictogram E10/E11,fixed to"]
[null,null,"wall or door (Union AL5066E-10/11/2AS)."]
{"$rows_empty":14}
["Total summary carried forward "]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[12,null,"METALWORK"]
[]
["12.1",null,"SUNDRY BRASS WORK:"]
[]
[null,null,"Brass:"]
[]
["12.1.1",null,"4 x 30mm Weatherbar set in concrete flush with","m",2]
[null,null,"floor finish one side."]
[]
[null,null,"ALUMINIUM WINDOWS"]
[]
[null,null,"All windows to be approved by the Architects"]
[null,null,"prior installation."]
[]
[null,null,"Natural anodized aluminium windows,"]
[null,null,"factory glazed with 6.38mm laminated "]
[null,null,"safety glass with clip-on glazing beads,"]
[null,null,"with neoprene seals and fixed with"]
[null,null,"minimum three lugs per side in "]
[null,null,"accordance with manufaccturer's "]
[null,null,"instruction :"]
[]
["12.1.2",null,"Window type Winblock WVAT 66 opening ","No",24]
[null,null,"section,complete with galvanized and powder"]
[null,null,"coated burglar bars."]
[]
["12.1.3",null,"Window type Winblock WVAT 66 fixed section,","No",28]
[null,null,"complete with galvanized and powder coated"]
[null,null,"burglar bars."]
[]
[null,null,"Natural anodized aluminium doors,factory"]
[null,null,"glazed with 6.38mm laminated safety"]
[null,null,"glass with clip-on glazing beads,with"]
[null,null,"neoprene seals and fixed in accordance"]
[null,null,"with manufacturer's intructions;"]
[]
["12.1.4",null,"Double entrance door and frame size","No",2]
[null,null,"1870 x 2032mm high,Type D1,in two equal "]
[null,null,"leaves,glazed with 6.38mm clear laminated"]
[null,null,"safety glass o,including all ironmongery,all as "]
[null,null,"indicated on Architects' drawing No.0805/D001,"]
[null,null,"attached to these bill of quantities."]
[]
["12.2",null,"GALVANIZED GATES"]
[]
[null,null,"Hot Dipped Galvanised Steel Gates :"]
[]
[null,null,"Note : the contractor is to check on site "]
[null,null,"measurements before placing of order."]
{"$rows_empty":7}
["Total summary carried forward to next page"]
["Total summary carried forward from previous page"]
[]
[]
["12.2.1",null,"Security gates size 900 x 2.097mm high of","No",1]
[null,null,"60 x 40 x 2mm hollow square section frame,"]
[null,null,"with two 40 x 6mm horizontal supports with"]
[null,null,"19mm holes drilled for and including six 19mm"]
[null,null,"diameter vertical rods,the whole gate fitted "]
[null,null,"inside a 40 x 60 x 2mm gate surround,with three"]
[null,null,"25mm diameter x 80mm long hinges welded to"]
[null,null,"25 x 3 x 200mm lugs built into concrete block"]
[null,null,"walls complete with two 55 x 40 x 8mm padlock"]
[null,null,"plates for locking and door hook,all as indicated"]
[null,null,"on Engineers Drawing No.J26075/009/0, "]
[null,null,"attached to these bills of quantities."]
[]
["12.2.2",null,"Double yard gate size 1,475 x 2100mm high","No",2]
[null,null,"formed of 32 x 32 x 1.6mm hollow square"]
[null,null,"section framing to detail,with VEM 6320 H"]
[null,null,"'Valmex'' expanded metal mesh welded to "]
[null,null,"inside frame,with 12mm solid rods welded"]
[null,null,"horizontally,with stainless steel shackle for "]
[null,null,"locking mechanism,with 38 x 38 x 10mm thick"]
[null,null,"plates as hinges with rounded ends to one side"]
[null,null,"and hole for 18mm diameter pin hung on pair of"]
[null,null,"socketted and pinned hinges with pin 18mm in "]
[null,null,"diameter and bolted to brickwall,with 200mm"]
[null,null,"locking bolt welded on,or other Architect "]
[null,null,"approved hinges,all as indicated on Architetc's"]
[null,null,"drawing No.0805/GS/001,atached to these bills"]
[null,null,"of quantities."]
[]
["12.2.3",null,"Entrance double gate size 2,130 x 2,125mm high","No",2]
[null,null,"formed of 32 x 32 x 1.6mm hollow square "]
[null,null,"section framing to detail,with VEM 6320 H"]
[null,null,"'Valmex'' expanded metal mesh welded to "]
[null,null,"inside frame,with 10 x 30mm flat bar shaped to"]
[null,null,"detail and 12mm solid rods welded horizontally"]
[null,null,"with stainless steel shackle for locking"]
[null,null,"mechanism,with 38 x 38 x 10mm thick plates as "]
[null,null,"hinges with rounded ends to one side and hole"]
[null,null,"for 18mm diameter pin hung on pair of socketted"]
[null,null,"and pinned hinges with 18mm in diameter and"]
[null,null,"bolted to brick wall,with 200mm locking bolt"]
[null,null,"welded on,or other Architect approved hinges,"]
[null,null,"all as indicated on Architect's Drawing "]
[null,null,"No.0805/GS/002,attached to these bills of"]
[null,null,"quantities."]
{"$rows_empty":9}
["Total summary carried forward to next page"]
["Total summary carried forward from previous page"]
[]
["12.3",null,"Hot Dipped Galvanised Steel Doors ;"]
[]
["12.3.1",null,"Door size 760 x 1,680mm high,prepainted","No"]
[null,null,"'golden brown'' formed of 19 x 19mm tubulor"]
[null,null,"steel framing and middle ledge welded"]
[null,null,"at angles and interaections,covered on one "]
[null,null,"side with 0,6mm galvanised sheeting pressed to"]
[null,null,"shape with edges lapped around and rivetted to"]
[null,null,"frame at 300mm centers,with slot for and"]
[null,null,"including barrel bolt,the gate fitted with and"]
[null,null,"including 25mm diameter x 2120mm long pivot"]
[null,null,"pipe support welded on,with 150 x 75 x 3mm"]
[null,null,"bottom bearing bolted to floor with 3 x 6mm"]
[null,null,"diameter bolts,including top cap bearing bush,"]
[null,null,"washers,bottom bearing bush and finishing"]
[null,null,"smooth on all exposed edges,complete with"]
[null,null,"all fixing brackets,bolts etc."]
[]
["12.4",null,"SUNDRY GALVANISED STEELWORK"]
[]
[null,null,"Purpose made roof supports,columns etc."]
[]
["12.4.1",null,"50 x 6mm Rafter bracket 300mm girth twice","No"]
[null,null,"bent with fishtail,set in concrete pier,including"]
[null,null,"holes for fixing."]
[]
["12.4.2",null,"75mm Outside diameter x 6.51kg/m tubular","No"]
[null,null,"column 3,085mm long with 150 x 150 x 10mm "]
[null,null,"thick x 375mm girth channel-shaped bracket"]
[null,null,"eight times holed for bolts(elsewhere measured)"]
[null,null,"welded on inlcuding setting up in position and "]
[null,null,"embedding bottom end in concrete."]
[null,null,"embedding bottom end in concrete."]
[]
["12.4.3",null,"75 x 3mm Thick three times bent T-shaped roof","No",9]
[null,null,"truss bracket 375mm girth,three times holed for"]
[null,null,"bolts (Bolts and holes elsewhere measured)."]
[]
[null,null,"Sundries :"]
[]
["12.4.4",null,"Bolts.","kg",6]
[]
["12.5",null,"CHALKBOARDS"]
[]
[null,null,"Approved chalkboards to comply with"]
[null,null,"CKS-36-1980 standard specification:"]
[]
["12.5.1",null,"Set of two standard Vitreous enamel magnetic"]
[null,null,"chalkboards with aluminium chalkrail including "]
[null,null,"seting up and fixing to walls complete and"]
[null,null,"securing bottom of each board with two fixig"]
[null,null,"brackets in accordance with the manufacturer's"]
[null,null,"intructions,size 4,800 x 1,140 mm high overall.","Sets","Rate only"]
[]
[]
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[13,null,"PLASTERING"]
[]
["13.1",null,"SCREEDS"]
[]
[null,null,"3 : 1 Cement plaster screeds steel "]
[null,null,"trowelled on concrete:"]
[]
["13.1.1",null,"25mm thick on floors.","m2",69]
[]
[null,null,"GRANOLITHIC"]
[]
[null,null,"Untinted granolithic on concrete :"]
[]
["13.1.2",null,"20mm Thick on floors and landings.","m2",15]
[]
["13.1.3",null,"20mm Thick on treads and risers of door","m2",1]
[null,null,"thresholds including reedings."]
[]
["13.1.4",null,"100 x 100mm Coved triangular fillets against","m",28]
[null,null,"walls,etc."]
[]
["13.2",null,"INTERNAL PLASTER"]
[]
[null,null,"Cement plaster brickwork :"]
[]
["13.2.1",null,"On walls.","m2",81]
[]
["13.2.2",null,"In narrow widths.","m2",{"v":0.3,"d":"0"}]
[]
[null,null,"Cement plaster on concrete."]
[]
["13.2.3",null,"On walls (Provisional).","m2",103]
[]
["13.2.4",null,"On floors with upper surface to falls and ","m2",5]
[null,null,"currents (Provisional)."]
{"$rows_empty":21}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[14,null,"PLUMBING & DRAINAGE (Provisional)"]
[]
["14.1",null,"RAINWATER DISPOSAL (PROVISIONAL) :"]
[]
[null,null,"0.8 mm Galvanised sheet iron with "]
[null,null,"Colomet finish one side :"]
[]
["14.1.1",null,"150 x 125 x 150mm High eaves gutter fixed to","m",27]
[null,null,"falls in continuos lengths at not exceeding "]
[null,null,"600mm centres with and including approved "]
[null,null,"gutter brackets."]
[]
["14.1.2",null,"Extra over eaves gutter for stopped end.","No",6]
[]
["14.1.3",null,"Extra over eaves gutter for 100 x 75mm pipe.","No",3]
[]
["14.1.4",null,"100 x 75mm Rainwater pipes fixed to walls","m",12]
[null,null,"with and including approved holderbats at"]
[null,null,"900mm centres."]
[]
["14.1.5",null,"Extra over rainwater pipe for  bend.","No",16]
[]
["14.1.6",null,"Extra over rainwater pipe for shoe.","No",2]
[]
["14.2",null,"Rainwater tanks :"]
[]
["14.2.1",null,"5000 Litre polyethylene rotomoulded vertical","No",4]
[null,null,"water storage tank complete with lid,with"]
[null,null,"suitable adaptor for outlet and setting in position"]
[null,null,"on concrete tankstand(elsewhere measured) "]
[null,null,"and tying down with 4mm diameter galvanised"]
[null,null,"wire wrapped twice around centre of tank"]
[null,null,"and secured to each corner of tank stand with"]
[null,null,"a double strand of 4mm diameter galvanised"]
[null,null,"wire embedded into concrete.(Note: tanks to be "]
[null,null,"filled with water before Practical Completion)."]
[]
["14.3",null,"Upvc Soil pipes (SABS 791-1986) :"]
[]
["14.3.1",null,"110mm Pipes vertically or ramped to cleaning","m",3]
[null,null,"eyes etc in and including trenches not "]
[null,null,"exceeding 1000mm deep."]
[]
["14.3.2",null,"110mm Pipe laid in ground not exceeding ","m",30]
[null,null,"1000mm deep including all excavations in earth"]
[null,null,"bedding cradle and blanket fill of selected"]
[null,null,"granular material,main fill compacting in layers"]
[null,null,"not exceeding 150mm thick,adjust moisture"]
[null,null,"content to optimum and compact to a density"]
[null,null,"of 90% Modified AASHTO in drain trenches"]
[null,null,"including carting off surplus displaced material."]
[]
[null,null,"Extra over Upvc pipes for fitrtings :"]
[]
["14.3.3",null,"110 mm bend.","No",2]
[]
[]
["Total summary carried forward to next page"]
["Total summary brought forward from previous page"]
[]
["14.3.4",null,"110mm Access bend.","No",2]
[]
["14.3.5",null,"110mm Access Junction.","No",2]
[]
["14.3.6",null,"110mm Access junction.","No",4]
[]
[null,null,"Sundries :"]
[]
["14.3.7",null,"Unreinforced concrete (15MPa) encasing to ","m³",{"v":0.1,"d":"0"}]
[null,null,"horizontal pipe."]
[]
["14.4",null,"Manholes,gulley traps,etc :"]
[]
["14.4.1",null,"Precast concrete cover slab size 950 x 900 x ","No",3]
[null,null,"75mm thick with opening for manhole cover and"]
[null,null,"frame and opening for 120mm diameter vent pipe"]
[null,null,"including hinged cast iron double seal manhole"]
[null,null,"cover and frame,size 450 x 600mm,in "]
[null,null,"accordance with SABS 558,coated with an"]
[null,null,"approved preservative solution before leaving"]
[null,null,"manufacturer and bedded in 1 : 3 cement mortar"]
[null,null,"and sealed in tallow,all set on top of chamber"]
[null,null,"(elsewhere measured)."]
[]
[null,null,"Gratings,cover,etc :"]
[]
["14.4.2",null,"Lifting key for manhole cover.","No",1]
[]
["14.5",null,"Testing :"]
[]
["14.5.1",null,"Testing drainage pipe system.","Prov. Sum",1]
["14.6"]
[null,null,"SANITARY FITTINGS"]
[]
[null,null,"Polyethylene fittings ;"]
[]
["14.6.1",null,"Atlas Plastic rotomoulded polyethylene VIP pit","No",3]
[null,null,"pedestal, or equal approved,size 370 x 500mm"]
[null,null,"high (code: 224AP) with foot piece and VIP 200"]
[null,null,"inlet funnel (code:224AP),inserted into precast"]
[null,null,"concrete cover slab of pit(elsewhere specified)"]
[null,null,"with a removal plug,with and including four 6mm"]
[null,null,"diameter x 50mm long expansion bolts,"]
[null,null,"including heavy duty white double flap seat"]
[null,null,"fixed to pedestal."]
{"$rows_empty":10}
["Total summary carried forward to next page"]
["Total summary carried brought from previous page"]
[]
["14.6.2",null,"Atlas Plastics rotomoulded polyethylene Christy","No",1]
[null,null,"wash hand basin (code: 382AP) 570mm x 395"]
[null,null,"mm wide,or equal approved,with 2 tapholes and"]
[null,null,"40mm waste outlet,plugged and screwed to the"]
[null,null,"wall with galvanised screws and brackets."]
[]
["14.7",null,"WASTE UNIONS ETC"]
[]
[null,null,"Waste unions etc:"]
[]
["14.7.1",null,"32mm Code 301 chrome plated basin waste","No",1]
[null,null,"union."]
[]
["14.8",null,"Taps etc :"]
[]
["14.8.1",null,"Rubber 32 x 40mm Plain basin P-taps.","No",1]
[]
[null,null,"TAPS,VALVES,ETC"]
[]
[null,null,"Piller taps ;"]
[]
["14.8.2",null,"15mm chrome pushbutton demand pillar tap","No",1]
[null,null,"flanged backnut,manufactured in accordance"]
[null,null,"to SABS 1808-66:2005."]
[]
[null,null,"Sundries,etc:"]
[]
["14.8.3",null,"Standard 15mm stainless steel braided female","No",1]
[null,null,"swivel connection piece 350mm long."]
[]
["14.9",null,"SANITARY PLUMBING"]
[]
[null,null,"Upvc piping ( SABS 967-1987) :"]
[]
["14.9.1",null,"40mm Waste piping fixed to walls.","m",1]
[]
["14.9.2",null,"50mm Ditto.","m",3]
[]
["14.9.3",null,"110mm Ditto","m",13]
[]
[null,null,"Extra For:"]
[]
["14.9.4",null,"Plastic or copper wire gauze fly screen glued","No",3]
[null,null,"to top of 110mm pipes as directed on site."]
[]
[null,null,"Extra over Upvc piping for :"]
[]
["14.9.5",null,"50mm bend.","No",1]
[]
["14.9.6",null,"50 to 40mm Reducer.","No",1]
[]
["14.9.7",null,"50mm Access bend.","No",1]
[]
[]
[]
["Total summary carried forward to next page"]
["Total summary carried brought from previous page"]
[]
["14.9.8",null,"50mm Accesss bend with anti-syphon horn.","No",1]
[]
["14.9.9",null,"50mm Junction.","No",1]
[]
["14.9.10",null,"110mm Bend.","No",2]
[]
["14.9.11",null,"110mm Access junction.","No",3]
[]
["14.9.12",null,"110mm Double reducing junction.","No",2]
[]
["1.10",null,"Tesing:"]
["14.10.1",null,"Testing waste water pipe system.","Prov. Sum",1]
[]
[null,null,"WATER SUPPLIES"]
[]
[null,null,"Polypropylene pipes with thermoplastic"]
[null,null,"couplings:"]
[]
["14.10.2",null,"15mm Pipes fixed to walls.","m",4]
[]
["14.10.3",null,"22mm Ditto.","m",5]
[]
["14.10.4",null,"28mm Ditto.","m",4]
[]
[null,null,"Extra over polypropylene pipes for "]
[null,null,"thermoplastic fittings:"]
[]
["14.10.5",null,"15mm Fittings.","No",5]
[]
["14.10.6",null,"22mm Fittings.","No",5]
[]
["14.10.7",null,"28mm Fittings.","No",3]
[]
["14.11",null,"Testing :"]
[]
["14.11,1",null,"Testing water supply pipe system.","Prov. Sum",1]
[]
[null,null,"Sundry work in connection with all"]
[null,null,"plumbing:"]
[]
["14.11.2",null,"Form hole in 150mm blockwall not exceeding","No",1]
[null,null,"50mm diameter including making good."]
[]
["14.11.3",null,"Form hole in 220mm brickwall not exceeding","No",2]
[null,null,"100mm diameter including making good."]
{"$rows_empty":9}
["Total summary carried forward to next page"]
["Total summary carried brought from previous page"]
[]
["14.12",null,"FIRE APPLIANCES ETC."]
[]
[null,null,"Portable fire extinguishers:"]
[]
["14.12.1",null,"4.5 kg carbondioxide portable chemical fire","No",1]
[null,null,"extinguisher complete with full load,wall hook"]
[null,null,"and bracket,bracket fixed to and including 25mm"]
[null,null,"Wrot Meranti backboard,size 250 x 500mm"]
[null,null,"high with chamfered edges,varnish and fixed"]
[null,null,"to wall."]
{"$rows_empty":45}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[15,null,"PAINTWORK"]
[]
["15.1",null,"Prepare and apply two coats pure acrylic"]
[null,null,"roof paint on:"]
[]
["15.1.1",null,"Fascia and barge boards.","m2",38]
[]
["15.2",null,"Prepare and prime nail heads and apply"]
[null,null,"one coat plaster primer thinned 5 parts"]
[null,null,"to 1 part Mineral Turpentine and paint"]
[null,null,"with two coats pure acrylic paint on:"]
[]
["15.2.1",null,"Ceilings and cornices.","m2",261]
[]
["15.3",null,"Prepare and apply one undercoat and"]
[null,null,"paint with two coats premium quality"]
[null,null,"pure acrylic  PVA on:"]
[]
["15.3.1",null,"Interior walls.","m2",239]
[]
["15.4",null,"Prepare and apply one undercoat and"]
[null,null,"paint with two coats premium quality"]
[null,null,"pure acrylic sheen PVA on:"]
[]
["15.4.1",null,"Interior toilet walls (Provisional).","m2",43]
[]
["15.5",null,"Scrub surface with degreaser,rinse"]
[null,null,"thoroughly with tap water,and apply one"]
[null,null,"coat sealer and two coats epoxy paint on:"]
[]
["15.5.1",null,"Interior toilet walls (Provisional).","m2",25]
[]
["15.5.2",null,"On concrete floated or screeded floors","m2",14]
[null,null,"(Provisional)"]
[]
["15.6",null,"ON BRICK SURFACES"]
[]
[null,null,"Clean down with spirits of salts solution"]
[null,null,"and apply two coats silicone-based brick"]
[null,null,"dressing on:"]
[]
["15.6.1",null,"Facings (External).","m2",184]
[]
[null,null,"ON WOOD "]
[]
[null,null,"Prepare and apply one coat wood primer,"]
[null,null,"one undercoat and two coats superior"]
[null,null,"quality smooth gloss enamel on:"]
[]
["15.6.2",null,"General surfaces of timbers at eaves.","m2",58]
[]
[null,null,"Prepare and apply one coat wood primer,"]
[null,null,"one undercoat and two coats superior"]
[null,null,"quality smooth eggshell enamel on:"]
[]
[]
["Total summary carried to next page"]
["Total summary carried from previous page"]
[]
["15.7",null,"Prepare and apply one coat wood primer,"]
[null,null,"one undercoat and two coats superior"]
[null,null,"quality smooth eggshell enamel on:"]
[]
["15.7.1",null,"Skirtings,rails,ect not exceeding 300mm girth.","m",131]
[]
["15.8",null,"Prepare and apply three coats "]
[null,null,"polyurethane matt varnish on:"]
[]
["15.8.1",null,"General surfaces.","m2",6]
[]
["15.8.2",null,"Skirting,rails,etc not exceeding 300mm girth.","m",1]
[]
["15.9",null,"Three coats exterior quality penetrating"]
[null,null,"wood preservative."]
[]
["15.9.1",null,"Roof timbers eaves and verges.","m2",78]
[]
["15.10",null,"ON METAL"]
[]
[null,null,"Clean down thoroughly with galvanised"]
[null,null,"iron cleaner,wash down with water,prime"]
[null,null,"with one coat galvanised metal primer and"]
[null,null,"finish with two coats superior universal"]
[null,null,"non drip enamel on:"]
[]
["15.10.1",null,"Exterior gates,grilles,burglar screens,","m2",22]
[null,null,"balustrades,etc. (both sides measured over"]
[null,null,"the full flat area)."]
{"$rows_empty":25}
["Total carried to summary"]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[]
[16,null,"STORMWATER CHANNELS"]
[]
[16.1,null,"Insitu concrete channels:"]
[]
["16,1,1",null,"600 x 150mm 20MPa open concrete stormwater","m",14]
[null,null,"channel with 560 x 60mm deep 'V' channel,on"]
[null,null,"suitable 150mm subbase material compacted to"]
[null,null,"93% Mod A.A.S.H.T.O.density,including all "]
[null,null,"necessary excavations,formwork,compaction,"]
[null,null,"grading,carting away,etc."]
[]
["16,1,2",null,"Extra over for angles,intersections,ends,","No",8]
[null,null,"dressing into sides of catchpits,etc"]
[]
["16,1,3",null,"900 x 150mm 20MPa open stormwater channel","m",48]
[null,null,"with 860 x 90mm deep 'V' channel,on suitable"]
[null,null,"150mm subbase material compacted to 93% Mod"]
[null,null,"A.A.S.H.T.O.density including all necessary"]
[null,null,"excavations,formwork compaction,grading,"]
[null,null,"carting away,etc."]
[]
["16,1,4",null,"Extra over for angles,intersections,ends,","No",9]
[null,null,"dressing into sides of catchpits,etc."]
[]
["16,1,5",null,"Extra over for widening concrete to form","No",1]
[null,null,"spreader 1800mm wide extreme for a length"]
[null,null,"of 600mm and bedding 120mm stone pitching in"]
[null,null,"concrete spaced at 200mm centre spacings"]
[null,null,"to falls including brushing concrete between"]
[null,null,"stones."]
[]
[16.2,null,"Gabions and Reno Mataresses:"]
[]
["16,2,1",null,"Form Gabion size 1000 x 1800 x 500mm deep","No",1]
[null,null,"using 50mm galvanized diamond mesh stitched"]
[null,null,"closed and lined with u14 Bidum and filled with "]
[null,null,"100mm stones including necessary excavating,"]
[null,null,"carting away etc."]
[]
[16.3,null,"SOAK AWAY"]
[]
[null,null,"Site clearance etc:"]
[]
["16.39.1",null,"Allow for clearing the area of the site to be built","m2",4]
[null,null,"upon of all grass,weeds,shrubs,trees with"]
[null,null,"trunks not exceeding 200mm girth,debris,etc.,"]
[null,null,"including up all roots,scoffling up as required"]
[null,null,"and cart away all vegetation and debris."]
[]
["16.40",null,"Excavation in earth not exceeding "]
[null,null,"2m deep:"]
[]
["16.40.1",null,"Drain soakaway.","m³",3]
[]
[]
["Total summary carried to next page"]
["Total summary carried from previous page"]
[]
["16.41",null,"Extra over bulk excavation in earth"]
[null,null,"for excavation in:"]
[]
["16.41.1",null,"Soft rock.","m³",{"v":0.3,"d":"0"}]
[]
["16.41.2",null,"Hard rock.","m³",{"v":0.2,"d":"0"}]
[]
["16.42",null,"Extra over all excavations for carting away:"]
[]
["16.42.1",null,"Surplus material from excavations and/or stock ","m³",1]
[null,null,"piles on site to a dumping site to be located by"]
[null,null,"the contractor."]
[]
[null,null,"Risk of collapse of excavations:"]
[]
["16.42.2",null,"Sides of trench and hole excavations not","m2",6]
[null,null,"exceeding 1.5m deep."]
[]
[null,null,"Keeping excavations free of water"]
[]
["16.42.3",null,"Keeping excavations free from mud and all"]
[null,null,"water including subterranean sources.",null,"Item"]
[]
[null,null,"Topsoil:"]
[]
["16.42.4",null,"Topsoil carted  on top of Bidum (elsewhere)","m³",{"v":0.2,"d":"0"}]
[null,null,"spread and levelled."]
[]
["16.43",null,"Earth filling supplied by the contractor and"]
[null,null,"lightly compact:"]
[]
["16.43.1",null,"Imported crusher dust or courses river sand.","m³",{"v":0.1,"d":"0"}]
[]
["16.43.2",null,"Selected 38mm graded stone in drain soakawy.","m³",3]
[]
[null,null,"Bidum"]
[]
["16.43.3",null,"Kaymat U24 laid in french drain soakaway.","m2",11]
[]
[null,null,"Drainage:"]
[]
["16.43.4",null,"110mm Diameter perforated piping laid in","m",2]
[null,null,"drain soakaway."]
[]
[null,null,"Extra over perforated piping:"]
[]
["16.43.5",null,"110mm Bend.","No",2]
[]
["16.44",null,"Testing:"]
[]
["16.44.1",null,"Allow for testing all drains,and water supples","Prov. Sum",0]
[null,null,"to the satisfaction of the Principal Agent.all"]
[null,null,"defective work is to be out and replaced at the"]
[null,null,"Contractor's expense."]
[]
["Total summary carried to next page"]
["Total summary carried from previous page"]
[null,null,"FENCING (PROVISIONAL)"]
[]
[null,null,"Clearing of  site:"]
[]
[null,null,"Allow for clearing site for the width of 1,000mm","m",200]
[null,null,"where fencing runs are to be erected including"]
[null,null,"removing trees,shrubs etc.not exceeding "]
[null,null,"200mm girth,grubbing up roots and roughly"]
[null,null,"levelling."]
[]
[null,null,"Galvanised posts:"]
[]
[null,null,"60mm Diameter galvanised steel intermediate","No",70]
[null,null,"fencing post,2,100mm long fitted with a pressed"]
[null,null,"steel mushroom cap,post fitted with 150 x 150 "]
[null,null,"x 3mm flange  plate welded to bottom and "]
[null,null,"embedded in 300 x 300 x 600mm mass concrete"]
[null,null,"(15 Mpa) base."]
[]
[null,null,"100mm Ditto as end post,fitted with one 60mm","No ",10]
[null,null,"diameter galvanised steel stay set raking and"]
[null,null,"with top end flattered and twice bolted through"]
[null,null,"post with M8 galvanised bolts,with post and "]
[null,null,"stay both embedded in mass concrete (15MPa)"]
[null,null,"bases as last."]
[]
[null,null,"100mm Ditto as straining or corner post,but ","No",4]
[null,null,"fitted with two 60mm diameter galvanised"]
[null,null,"steel raking stays."]
[]
[null,null,"150mm Ditto as gate post,but fitted with one","No",2]
[null,null,"60mm diameter galvanised steel raking stay,with"]
[null,null,"post and stay both embedded in 400 x 400 x"]
[null,null,"600mm mass concrete (15MPa) bases"]
[null,null,"(Provisional)"]
[null,null,"with top end flattered and twice bolted through"]
[null,null,"post with M8 galvanised bolts,with post and "]
[null,null,"stay both embedded in mass concrete (15MPa)"]
[null,null,"bases as last."]
[]
[null,null,"100mm Ditto as straining or corner post,but ","No",4]
[null,null,"fitted with two 60mm diameter galvanised"]
[null,null,"steel raking stays."]
[]
[null,null,"150mm Ditto as gate post,but fitted with one","No",2]
[null,null,"60mm diameter galvanised steel raking stay,with"]
[null,null,"post and stay both embedded in 400 x 400 x"]
[null,null,"600mm mass concrete (15MPa) bases"]
[null,null,"(Provisional)"]
[]
[]
[]
[]
[]
[]
["Total summary carried to next page"]
[]
["Total summary carried from previous page"]
[]
[null,null,"Fencing:"]
[]
[null,null,"Fencing formed of 50 x 100 x 2.5mm diameter","m",200]
[null,null,"galavnised weldmesh 1,600 m high with"]
[null,null,"vertical wires facing outwards secured with"]
[null,null,"'howgring'' clips or 1.6mm galvanised binding"]
[null,null,"wire at 300 mm centres to top and bottom"]
[null,null,"straining wires and 700 mm centres to four"]
[null,null,"intermediate straining wires (straining wires"]
[null,null,"elsewhere measured) including holes through"]
[null,null,"posts."]
[]
[null,null,"Six strands of 4mm galvanised straining wires","m",200]
[null,null,"secured to fencing posts with doubled 2mm"]
[null,null,"galvanised wire inserted through hole in post"]
[null,null,"and turned a minimum of four turns around"]
[null,null,"straining wire and attached to straining frame"]
[null,null,"at one end with not less than four turns and"]
[null,null,"the other end to straining bolts"]
[null,null,"(elsewhere measured)."]
[]
[null,null,"Sundries:"]
[]
[null,null,"12 mm Diameter galvanised mild steel straining","No",100]
[null,null,"eye bolt with hook,threaded portion and two"]
[null,null,"nuts washers,including hole through post."]
[]
[null,null,"Ablution facilities","sum",{"v":200000,"d":"200,000"},{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
{"$rows_empty":26}
["Total summary carried to next page"]
[]
["Item No","Ref","Description","Unit","Quantity","Rate","AMOUNT"]
[17,null,"PROVISIONAL SUMS"]
[]
[17.1,null,"Allowance for furniture","Sum",null,null,{"v":150000,"d":"150,000.00"}]
[]
[17.2,null,"ADDITIONAL SERVICES"]
[]
[17.3,null,"Engineering Survey","Sum",null,null,{"v":20000,"d":"20,000.00"}]
[]
[17.4,null,"Overheards and profit on item 17.4"]
[]
[17.5,null,"Geotechnical Investigations","Sum",null,null,{"v":30000,"d":"30,000.00"}]
[]
[17.6,null,"Overheards and profit on item 17.5"]
[]
[17.7,null,"Environmental Issues","Sum",null,null,{"v":10000,"d":"10,000.00"}]
[]
[17.8,null,"Overheards and profit on item 17.7"]
[]
[17.9,null,"OHS Compliance","Sum",null,null,{"v":50000,"d":"50,000.00"}]
[]
[18,null,"Overheards and profit on item 17.9"]
[]
[18.01,null,"EMP Compilation","Sum",null,null,{"v":80000,"d":"80,000.00"}]
[]
[18.02,null,"Overheards and profit on item 18.01","%"]
[]
[18.03,null,"Social Facilitation","Sum",null,null,{"v":100000,"d":"100,000.00"}]
[]
[18.04,null,"Overheads and profit on item 18.03","%"]
[]
[18.05,null,"Electricity Installation","Sum",null,null,{"v":120000,"d":"120,000.00"}]
[]
[18.06,null,"Overheads and profit on item 18.06","%"]
{"$rows_empty":10}
["Total carried to summary"]

{"sheet":"Summary","index":2,"n_rows":44,"n_cols":3,"rows_kept":44,"merged":[[0,0,0,5],[1,0,1,5],[2,0,2,5]]}
[]
[]
[]
[]
["SECTION","DESCRIPTION","TENDERED SUM"]
[]
[1,"Preliminaries & General"]
[]
[2,"Earthworks (Provisional)"]
[]
[3,"Concrete,Formwork & Reinforcement"]
[]
[4,"Precast Concrete"]
[]
[5,"Masonry"]
[]
[6,"Waterproofing"]
[]
[7,"Roof Covering,Etc."]
[]
[8,"Carpentry & Joinery"]
[]
[9,"Ceilings,Partions & Access Flooring"]
[]
[10,"Floor Covering,Wall Linings,Etc."]
[]
[11,"Ironmongery"]
[]
[12,"Metal work"]
[]
[13,"Plastering"]
[]
[14,"Plumbing & Drainage (Provisional)"]
[]
[15,"Paintwork"]
[]
[16,"External Work (Provisional)"]
[]
[17,"Provisional Sums"]
[18,"SUB-TOTAL (1+2+3+4+5+6+7+8+9+10+11+12+13+14+15+16+17)"]
[19,"CONTIGENCIES @ 10% (10% OF 12)"]
[20,"SUB-TOTAL (19+18)"]
[21,"VAT @ 15% (15% OF 20)"]
[22,"TOTAL CARRIED FORWARD TO FORM OF OFFER (20+21)"]