{"text_format":"3","workbook":"xlsx","n_sheets":20,"sheets":["BILL A","BILL B.1.","BILL B.2.","BILL B.3.","BILL B.4.","BILL B.5.","BILL B.6.","BILL B.7.","BILL B.8.","BILL C","BILL D.1.","BILL D.2.","BILL D.3.","BILL D.4.","BILL D.5.","BILL D.6.","BILL D.7.","BILL D.8.","BILL E","BILL Summary"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"BILL A","index":0,"n_rows":110,"n_cols":10,"rows_kept":110,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON"]
[]
[]
[]
["BillHeader",null,"BILL A",null,"PRELIMINARY AND GENERAL"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Work\nGroup"]
["Section","9b40006d-16bc-4afb-a7c5-f0866eb94df1","A1","","PRELIMINARY AND GENERALS",{"$nulls":4},"Dflt"]
["Label","2d78b9e5-9c3c-4838-9943-273fa815799f","","SANS\n1200 A","SECTION A1 : PRELIMINARY AND GENERALS",{"$nulls":4},"Dflt"]
["Header2","308226ae-eac3-4b37-b786-45476e9a37b9","A1.1","8.3\nPSAB 8.2.1","FIXED-CHARGE ITEMS",{"$nulls":4},"Dflt"]
["Item","c556cb01-9949-487a-89d3-21842e293533","A1.1.1","8.3.1","Contractual Requirements","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4f1f2569-bc48-48b7-9f83-3370b41cb2c7","A1.1.2","Annex C3.6.6     CEMP","Submission of the Environmental Management Plan","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","e5c7026f-0543-4b55-abc9-b3abb35df7de","","8.3.2","Establish Facilities on the Site :",{"$nulls":4},"Dflt"]
["Label","791f8354-70bd-4f8e-a540-ec43d9cd276f","","8.3.2.1     PSAB 8.2","a) Facilities for Engineer",{"$nulls":4},"Dflt"]
["Item","6926309b-25cf-4d64-a25f-058051f9f052","A1.1.3","","Furnished Office","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G16 * H16,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3d54b9cd-a10f-4ff4-a4b3-c8c3680ad915","A1.1.4","","Carport","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","78d78fc3-be95-43c3-b37c-deb724d52912","A1.1.5","","Nameboards ( 2 )","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8697e419-db8d-4103-bfcd-2a400bbbacb7","A1.1.6","","Telephone","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d3310daf-a1c3-4676-b05a-52c62eb54403","A1.1.7","","Survey Assistant & Equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7828468e-a255-4667-b1e9-8fc4d52ded57","A1.1.8","","Computer Equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","631b4177-eeef-499f-97cc-ccb4d2877791","","","b) Facilities for Contractor",{"$nulls":4},"Dflt"]
["Item","65a5757e-3fde-4741-a215-e8a38990feac","A1.1.9","PSA 8.3.2.2 (a)","Offices and storage sheds","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G23 * H23,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a4349e4c-6c34-4165-8065-e0ab052b9c4e","A1.1.10","","Ablution and latrine facilities","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","28edfc2b-73e9-429f-9268-bb561445b795","A1.1.11","","Tools and equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2734cc57-8b7c-47ae-9709-7be57ee8f8ac","A1.1.12","","Water supplies, electric power and communications","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","dc4d3adc-96bd-4ed2-b485-010b3205df75","A1.1.13","","Access","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e122cdf7-ace1-4d00-a667-49b2f07c3fc8","A1.1.14","PSA 8.3.2.2 (h)","Dealing with water","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6d58d1db-a971-4457-83a6-28fefb0d87db","A1.1.15","8.3.4","Remove Engineer's and Contractor's Site establishment on completion","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","c678d523-7770-49c5-bc31-75550ce68329","A1.2","8.4\nPSA 8.2.2\nPSAB 8.2.1","TIME-RELATED ITEMS",{"$nulls":4},"Dflt"]
["Item","db619fd9-4ce3-4bd7-a9d6-c7e0f5e0fae9","A1.2.1","8.4.1","Contractual Requirements","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","bd1a8aac-b2a3-4212-aead-78d2903fba31","","8.4.2","Operate and maintain facilities on the Site:",{"$nulls":4},"Dflt"]
["Label","f387795a-90a3-4610-836b-02f77edc6955","","8.4.2.1     PSAB 8.2","a) Facilities for Engineer for duration of construction (SABS 1200 AB)",{"$nulls":4},"Dflt"]
["Item","aa466c58-511c-4a2b-80bf-0d13e47c749a","A1.2.2","","Furnished Office","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G34 * H34,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7ca6a7d9-1816-45b6-9fdd-4a63969d9ad0","A1.2.3","","Carport","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6cd7bbd6-b6d7-4508-91f9-decb3a87a45b","A1.2.4","","Telephone","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","44420c3a-e2f3-4d08-98f6-0360cc35dfca","A1.2.5","","Survey Assistant & Equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","75b458b7-b7cd-4f99-8728-7df53c92063a","A1.2.6","","Computer Equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","46af0abd-dcb5-43c2-a202-2910b83110be","","8.4.2.2","b) Facilities for Contractor for duration of construction, except where otherwise stated",{"$nulls":4},"Dflt"]
["Item","ed3b9c82-d81e-493a-98f2-3039048cf023","A1.2.7","PSA 8.4.2.2 (a)","Offices and storage sheds","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G40 * H40,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","058389a3-b359-482f-b0ab-e4a32beb31e2","A1.2.8","","Ablution and latrine facilities","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b816b3eb-ad4c-4c59-a70b-aa65141b36a4","A1.2.9","","Tools and equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9c206656-f4e8-46b0-ad75-604d84d48f26","A1.2.10","","Water supplies, electric power and communications","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","22420a8d-8217-42b4-9ab7-f56d53f8b4c9","A1.2.11","PSA 8.4.2.2 (h)","Dealing with water","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b1764cca-b483-46ae-a846-ccbb41eb79d3","A1.2.12","","Access","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3fed6a2e-d84c-4d3d-a570-ed105b0ab52e","A1.2.13","","Construction Equipment","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9758a925-6b2d-4430-8167-0fae1eb20f7a","A1.2.14","8.4.3","Supervision","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","83400b04-f333-4e2e-bd09-f2787d89c1fb","A1.2.15","8.4.4","Company and head office overhead costs","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a1caf69e-f642-4e67-bf40-ae8a5cd952ff","A1.2.16","8.4.5","Other time-related obligations Surveyor","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8dd70258-7d36-4440-a658-b2d5a96f5e15","A1.2.17","","Compliance with the specified environmental requirements","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","4949630b-edf8-48ba-a175-0fb0e3fa9ff8","A1.3","Annex C3.6.5 H&S Spec","Fixed and Time Related Charges associated with complying with the Project Health and Safety Specification:",{"$nulls":4},"Dflt"]
["Sum","0d70e2f6-f371-4003-aab5-f8b05c4176b5","A1.3.1","","Preparation of principal contractor’s site specific health and safety plan, safety file, risk assessments, fall prevention/protection plan, Annexure 2 notification to Dept of Labour, demolition method statement, other method statements requested to be prepared for safety reasons, permits, amendments to safety plan during course of project, traffic management / accommodation plans, and any other legally required health and  safety documentation","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","7120d7dd-f9f2-4aa7-8a27-e3f69f044b58","A1.3.2","","Provision of safety documentation required of the principal contractor for Construction Work Permit application by the safety agent of Dept of Labour, if applicable (note section 2.4 of this safety specification document)","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","1688b6d2-96dd-4ea8-a728-0878ab1a7043","A1.3.3","","Provision of current workman’s compensation cover for employees for the project, and ensuring that contractors appointed have such cover too","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","18cd3a8a-7a6a-48b4-8ef9-ef2ee116df02","A1.3.4","","Health and safety management of principal contractor’s employees, visitors and contractors’ employees on site.","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","62931a19-6582-425d-8dd5-c241a335d332","A1.3.5","","Provision of full time Construction Manager for site, provision of Alternate Construction Manager in absence of Construction Manager and provision of sufficient safety supervision on site","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","25ec49b5-82d7-4f82-b498-aadfe41ef833","A1.3.6","","Provision of full time/ part time SACPCMP registered Construction Health & Safety Officer for site (refer to safety specification for full time / part time requirement) and preparation of safety reports after each safety inspection","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","d60b7a39-228c-4c01-8d24-49bbf5f4dfc9","A1.3.7","","Competence assessment, appointment and required competence and safety training of all principal contractor’s legally required appointments for site","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","1362cfbd-2238-42c5-9d5a-72274f9cf617","A1.3.8","","Maintenance of principal contractor’s construction equipment and equipment on site so as to be in safe condition, including inspection registers, inspections by competent persons, thorough examination certificates, hand over certificates and related documentation ","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","08de36b4-16e3-4557-bb06-ae26349d603c","A1.3.9","","Provision of general safety signage (e.g. first aid, firefighting, traffic safety, excavations, PPE, Assembly Point, noise zones, etc.)","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","8f1a28c5-0f41-41c8-bd00-1af6a345f1ea","A1.3.10","","Provision of medical certificates of fitness for employees on site (Annexure 3)","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","bd512f5b-37f7-41c3-b6c6-21608f4c643b","A1.3.11","","Provision of personal protective equipment (PPE) by principal contractor to employees and, as applicable, visitors to site, incl. \n• reflective vests\n• hard hats\n• protective foot wear \n• hearing protection\n• respiratory protection\n• safety eyewear\n• gloves\n• overalls\n• Safety harnesses and lanyards\n• Sunblock\n• UV Protective clothing / hats / eye wear\n• Protective thermal wear (heat / wind / cold / rain)\n• Protective firefighting clothing\n• Arc flash and electrical protective clothing\n","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","2b997eaf-76ed-42f4-9dd2-7ee522475f4f","A1.3.12","","Provision of Fall Prevention and Protection Equipment including.\n• Rope\n• Lifelines & Self-Retracting Lifelines (SRL)\n• Anchor Points\n• Warning Lines & Area demarcation\n• Fall Arrest Accessories\n• Fall Rescue Equipment\n• Passive Fall Protection Equipment\n• Confined Space Rescue and Retrieval (In elevated work situations)\n• Etc.","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","86d90f31-9a26-40e2-af30-7d0b7889386c","A1.3.13","","Provision of Confined Space work equipment & Training\n• Training\n• Air Monitoring Equipment\n• Ventilation Equipment\n• Entry Equipment\n• Personal Protective Equipment\n• Confined Space Rescue and Retrieval Equipment\n• Communication Equipment\n• Etc.\n","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","24e3254e-c1d7-4c4a-a0ee-2f75325ff0fb","A1.3.14","","Holding of safety meetings with safety representatives and safety officers on site on at least monthly basis","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","cb813b25-70e0-4b86-a6f6-6bbf0d07e198","A1.3.15","","Principal contractor construction safety management attendance at health and safety meetings called by Employer, professional team or safety agent","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","f64f97b0-7bdf-4073-9cfb-ae882157741b","A1.3.16","","Provision of site specific health and safety induction training for all on site","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","2c6d6a44-4616-4717-a869-c6835fa13ad0","A1.3.17","","Conducting of toolbox talks to employees on health and safety issues on a weekly basis","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","62be4cd6-a4e2-4865-999d-dfe7a6db788f","A1.3.18","","Provision of sufficient First Aiders for site as per legal requirements","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","dbaa89f3-ee41-4bdc-8b44-0abf4d9facc1","A1.3.19","","Provision of First Aid Boxes for site as per legal requirements","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","51cfc065-0565-420d-b76e-de8564cf50be","A1.3.20","","Provision of sufficient fire extinguishing equipment for site","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","03171569-d619-47fe-98ef-543648b43bfb","A1.3.21","","Fire drills on site at least 6 monthly basis for duration of project","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","d599123e-a80d-40e0-86d7-e9145d51988b","A1.3.22","","Provision of welfare facilities for site (drinking water, toilets, soap, means of drying hands, toilets paper, sheltered eating areas, etc.)","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","0b067483-ca6f-4332-8e5c-d0edb700063e","A1.3.23","","Provision for safe disposal of waste, spill kits, safe housekeeping and storage practices ","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","f39ed795-be23-452b-8381-dde42418d201","A1.3.24","","Provision of leading edge protection, covers to prevent falls","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","79dd0cce-b47e-45e2-818a-4fc7d1015a92","A1.3.25","","Provision of fencing at site camp and to protect excavations","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","e58a342f-71b7-4fcf-9442-7fad2ad88cf2","A1.3.26","","COVID 19 measures – provision of hand sanitiser, respiratory protection (as required), safety signage, formal and informal communication to all on site and any other measures necessary to contain and detect COVID 19 on site (refer to safety specification)","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","29a82df9-c519-4715-8bf1-7987460557ab","A1.3.27","","Compilation of consolidated Safety File at Close Out stage and handover of file to safety agent in hard copy or digital format","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","6d4fd38b-55eb-4868-8353-a25ce00003cc","A1.3.28","","Supply of safety caps on all exposed re-bar ","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","12c49f85-f898-42f6-a1a1-a82784d9f39a","","","Any other compliance item in site specific safety specification issued by project Employer/ safety agent with potential cost implication",{"$nulls":4},"Dflt"]
["Sum","6264c6cc-360f-4092-832e-14d1ef807866","A1.3.29","","·        Item 1","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H81,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","f84063f4-38f8-46c7-9ef6-6dfe910b2808","A1.3.30","","·        Item 2","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","36ca950a-5b5f-460b-9486-253ed680a6cc","A1.3.31","","·        Item 3","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","49b1af25-aafa-448a-8279-5b23b0682676","A1.3.32","","·        Item 4","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","2c787983-ba69-4b56-9667-2c3b06b3b8c1","A1.3.33","","·        Item 5","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","da51381e-cf6a-4de0-a903-f57b2799efa1","A1.3.34","","Principal contractor’s general compliance with respect to the Occupational Health and Safety Act, Construction and other health and safety Regulations apart from other provisions in this bill.","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","fce77635-ab13-4ad8-81f4-447d4a5e9695","A1.4","8.5","SUMS STATED PROVISIONALLY BY ENGINEER\n",{"$nulls":4},"Dflt"]
["Sum","0930557b-84ae-488a-92b9-ade8a838fbc3","A1.4.1","PSA 8.10","Acceptance testing of material and workmanship called for by the Engineer at a nominated laboratory","Prov.Sum",1,{"v":150000,"d":"150,000.00"},{"$f":"ROUND(H88,2)","v":{"v":150000,"d":"150,000.00"}},"Dflt"]
["Sum","a68ac6e0-b8b4-4611-b3ba-065df51a23d7","A1.4.2","PSA 8.1.2.4","Payment to the Municipality for lowering, routing and diversion of services","Prov.Sum",1,{"v":60000,"d":"60,000.00"},{"v":60000,"d":"60,000.00"},"Dflt"]
["Sum","bfdbc09b-bae5-43ac-8725-d37e2a454a12","A1.4.3","","A complete As-Built survey including all structures, pipework, etc. by a registered land surveyor on completion of works","Prov.Sum",1,{"v":75000,"d":"75,000.00"},{"v":75000,"d":"75,000.00"},"Dflt"]
["Sum","232ef795-a80c-4d4d-a223-f28795c17ffb","A1.4.4","","Mechanical installation for Meyerton WWTW (Nominated Sub-Contractor)","Prov.Sum",1,{"v":30000000,"d":"30,000,000.00"},{"v":30000000,"d":"30,000,000.00"},"Dflt"]
["% Previous","e14476d7-3f05-4b54-8bae-6912dec87a45","A1.4.5","","Overheads, charges and profit on item A1.4.4","%",{"$f":"I91","v":{"v":30000000,"d":"30000 000.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G92 * H92,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","c1855980-c4ec-4d3f-98af-36317495fc70","A1.4.6","","Electrical installation for Meyerton WWTW (Nominated Sub-Contractor)","Prov.Sum",1,{"v":60000000,"d":"60,000,000.00"},{"$f":"ROUND(H93,2)","v":{"v":60000000,"d":"60,000,000.00"}},"Dflt"]
["% Previous","9ba5073d-6c12-4ea8-a0b8-f3d4743cfcc6","A1.4.7","","Overheads, charges and profit on item A1.4.6","%",{"$f":"I93","v":{"v":60000000,"d":"60000 000.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G94 * H94,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6d3582c4-e685-4519-a122-c736689ab2a8","","","Provisional Sums for the provision of access and safety equipment required to gain access to structures for initial inspections and testing by the Structural Engineer / Specialists, including all scaffolding, platforms, safety gear and certification and any other equipment required to safely access all areas of the following structures:",{"$nulls":4},"Dflt"]
["Sum","9d384752-d2cc-4c36-ac52-319b2b25737d","A1.4.8","","Raw Water Pump Station","PSum",1,{"v":50000,"d":"50,000.00"},{"$f":"ROUND(H96,2)","v":{"v":50000,"d":"50,000.00"}},"Dflt"]
["Sum","785c54d2-b62d-4f57-ab04-57b740b158ba","A1.4.9","","Biological Reactor","PSum",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"},"Dflt"]
["Sum","a24897de-788b-4a8a-afec-f7b16615ca99","A1.4.10","","Secondary Sedimentation Tank","PSum",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"},"Dflt"]
["Sum","70fec0c1-58a7-47a0-aceb-7a26eadb1149","A1.4.11","","Buildings, as required","PSum",1,{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"},"Dflt"]
["Sum","14d0c2ba-0e4b-46f8-ac0c-103601bb4075","A1.4.12","","Other structures not listed above, as required","PSum",1,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"},"Dflt"]
["Label","2f1657a4-e466-4fa6-8824-9dfe8b9c5672","","","Tests and Specialist Investigations",{"$nulls":4},"Dflt"]
["Sum","341a77ba-a05d-43c7-a315-2b27b26f90be","A1.4.13","","Tests and specialist investigations deemed necessary by the Contractor as described in PSA 7.5","PSum",1,{"v":1000000,"d":"1,000,000.00"},{"$f":"ROUND(H102,2)","v":{"v":1000000,"d":"1,000,000.00"}},"Dflt"]
["Header2","6bc0bf21-0d47-4f4f-89f3-d15400b5a2cb","A1.5","8.8","TEMPORARY WORKS",{"$nulls":4},"Dflt"]
["Label","10ce6ef9-0d6a-4657-bddf-9722e5d4f293","","8.8.4\nPSA 8.8.4\nPSDB 8.3.5","Existing services",{"$nulls":4},"Dflt"]
["Item","16fe078d-ddb6-46af-9a95-775e253576ac","A1.5.1","SANS 1200D 8.3.8.1(a)","Existing Services: Supply or hire and use of specialist equipment and personnel for the detection of underground services","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G105 * H105,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","18549088-8802-4c09-b432-2facb961c2b4","A1.5.2","SANS 1200D 8.3.8.1(c)","Excavate by hand in soft material to expose unknown existing services","m³",300,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","21c8bf38-a476-47a7-b86e-8c90d595c4a9","A1.5.3","PSA 8.8.7","Clear entire site, including outside and inside of all structures and buildings, of all weeds, builders rubble, dewatering of structures and cut grass on establishment on site by the Contractor on a once off basis, further clearing may be required as instructed by the Engineer. ","ha",12,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","bae9fe9d-8119-4325-a125-d228be8fadd9","A1.6","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","08fce572-a236-47d8-aaf0-d47dd5823b4b","","","CCTV Inspection",{"$nulls":4},"Dflt"]
["Item","4da364be-e449-4a1a-bf3f-5f464af1e8d4","A1.6.1","PSLD 8.2.13","CCTV camera surveys of pipelines upon completion.","m",900,{"v":0,"d":"0.00"},{"$f":"ROUND(G110 * H110,2)","v":{"v":0,"d":"0.00"}},"Dflt"]

{"sheet":"BILL B.1.","index":1,"n_rows":37,"n_cols":10,"rows_kept":37,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.1.",null,"DAYWORKS",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","e9d16f91-07d6-4c71-bb2d-ee9a725b6702","B.1.1","SANS 1200 A & AB\nPSA 8.1.1","DAYWORKS",{"$nulls":4},"Dflt"]
["Label","680e6759-b6e5-4331-9aad-2b2cfb1e4d46","","SANS 1200 A & AB\nPSA 8.1.1","SECTION B.1.1 : DAYWORKS",{"$nulls":4},"Dflt"]
["Header2","0cccdf89-9cf2-4522-b8f7-88f986df3da0","B.1.1.1","8.7\nPSA 8.1.1","LABOUR",{"$nulls":4},"Dflt"]
["Item","30021c28-bb1c-421f-821d-a42820039fe3","B.1.1.1.1","","Foreman","hr",135,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ce39a469-d6df-453e-b7dc-0620dab9e539","B.1.1.1.2","","Steel Fixer","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4d25ae07-567e-4a5e-a890-bc78af42085c","B.1.1.1.3","","Concreter","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d2da1f41-63d6-462a-8543-2aa3b4ecf642","B.1.1.1.4","","Chargehand","hr",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","834b22c0-de51-4173-9a4f-5e62a6c78a32","B.1.1.1.5","","Artisan (Welder, Plumber, etc)","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","973091f4-c447-4c66-a94f-bffcef8633d2","B.1.1.1.6","","Pipe layer","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","056b534b-6bdb-482e-b17f-6cad1d9eb317","B.1.1.1.7","","Semi Skilled Labourer","hr",270,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c280eba9-16e0-4a29-8acd-a5554174bfc4","B.1.1.1.8","","Unskilled Labour","hr",540,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","441ec389-e3d1-46b1-bc01-19df9bf6c8ff","B.1.1.1.9","","Security guard","hr",180,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","80decebd-a609-46d1-a7cb-8513df0347f8","B.1.1.2","","MATERIALS",{"$nulls":4},"Dflt"]
["Sum","eb276cf6-4919-403b-a914-16ae86460624","B.1.1.2.1","","Allow for Materials ","Prov.Sum",1,{"v":105000,"d":"105,000.00"},{"$f":"ROUND(H22,2)","v":{"v":105000,"d":"105,000.00"}},"Dflt"]
["% Previous","de4837af-af98-41c4-8597-5bc6cae0a710","B.1.1.2.2","","Overheads, charges and profit on item B.1.1.2.1 ","%",{"$f":"I22","v":{"v":105000,"d":"105 000.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G23 * H23,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","16122280-086c-430d-8293-3d0928346ff1","B.1.1.3","PSA 8.1.1","CONSTRUCTION EQUIPMENT",{"$nulls":4},"Dflt"]
["Item","4e08feb6-7d8b-4188-8fc6-a5e5a547d7ac","B.1.1.3.1","","Front-end Loader, approx. flywheel power 145 kW","hr",45,{"v":0,"d":"0.00"},{"$f":"ROUND(G25 * H25,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","72b82574-0e26-4eb0-98d0-4cdbf710c33c","B.1.1.3.2","","Back acting excavator, approx. flywheel power 100 kW","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e0f191b9-95c1-412c-8e26-902ff3e1bd6c","B.1.1.3.3","","Hand vibrating compactor, static mass","hr",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f9006655-2fa7-4558-a00e-72ebffaf3824","B.1.1.3.4","","Mobile Crane, 5 tonne at 3m radius","hr",27,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e3f10acb-4db5-4494-9ed3-16ac4f4e96b0","B.1.1.3.5","","Compressor, 10.3 m3/min including tools and hoses","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","61759c1a-2d63-415b-9cef-6e4e19f9dbd4","B.1.1.3.6","","Poker vibrator","hr",54,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bce8188f-9bde-4d1c-833a-dd874ade28f1","B.1.1.3.7","","Concrete Mixer 0.3 m3 dry mix capacity","hr",54,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8c8312f8-496e-40b6-9409-e363cb660243","B.1.1.3.8","","50 mm Water Pump including hoses","hr",180,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","aaf4d8d9-18d6-4e4c-a444-00266827d371","B.1.1.3.9","","Tipper, 10m3 capacity ","hr",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","ac431c08-4f0d-4c1e-83f9-7816e6403647","B.1.1.3.10","","Tipper, 5m3 capacity ","hr",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","2ee1d443-6bd2-4295-b55d-c7362ba195f3","B.1.1.3.11","","Flat bed, 7 tonne capacity","hr",27,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","a081a94a-1f63-4ea2-a849-7fa8d06295c2","B.1.1.3.12","","Flat bed, 5 tonne capacity","hr",27,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","25447814-1f8d-4376-a472-37f51b8c20b3","B.1.1.3.13","","1 tonne LDV","hr",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]

{"sheet":"BILL B.2.","index":2,"n_rows":449,"n_cols":10,"rows_kept":449,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.2.",null,"PIPELINES",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","0254b0ee-15b8-4ce0-94df-dea72177844e","B.2.1","","MEDIUM PRESSURE PIPELINES, WATER RETICULATION AND SEWER RETICULATION",{"$nulls":4},"Dflt"]
["Label","fd628a2f-5a5a-43a6-a27e-6d3b12fcc1a3","","SANS 1200L","SECTION B.2.1 : MEDIUM PRESSURE PIPELINES, WATER RETICULATION AND SEWER RETICULATION",{"$nulls":4},"Dflt"]
["Header2","35fb4397-8bfd-4a13-8167-2d19ac1215cd","B.2.1.1","SANS 1200L","MEDIUM PRESSURE PIPELINES",{"$nulls":4},"Dflt"]
["Header3","e6f52d58-360b-43c0-9882-90bf46cec28d","B.2.1.1.1","SANS 1200DB\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","82b1955f-9f5d-4df1-8a5c-ea5af95cfe2f","B.2.1.1.1.1","8.3.1(a)","Clear vegetation and trees of girth up to 1 m","m",540,{"v":0,"d":"0.00"},{"$f":"ROUND(G13 * H13,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","089064cf-68c1-4d08-a05c-21ceda6837f8","B.2.1.1.1.2","8.3.1(c)\nPSC 8.2.10","Remove topsoil to depth of 150mm","m²",730,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","59294f9f-ac35-4b2c-90e6-dd04b0c85fde","B.2.1.1.1.3","SANS 1200C 8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",100,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","04254307-0a43-4ae9-b25a-c819b400983c","B.2.1.1.2","SANS 1200DB","REMOVAL OF EXISTING PIPE",{"$nulls":4},"Dflt"]
["Label","ab0d3284-01c7-43f5-a424-f63003861f60","","8.3.2(a) PSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","d2417f00-1b1f-4c34-9aa8-2ffe1ff94752","","","Over 900 mm up to 1100 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Rate Only","e08f7da6-c04d-483f-9077-41ee780ebf45","B.2.1.1.2.1","","2,0 m                       3,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","a6be0ad8-7660-444d-a08c-add801722265","B.2.1.1.2.2","","3,0 m                       4,0 m","m",110,{"v":0,"d":"0.00"},{"$f":"ROUND(G20 * H20,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","5d89bd80-3416-4147-b04d-541aa773859e","B.2.1.1.2.3","","4,0 m                       5,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header3","53203344-de5e-445d-81f2-f6703b7c5b1e","B.2.1.1.3","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Item","68b1f28c-f1af-462e-ab64-5df3d1e7138e","B.2.1.1.3.1","","1000mm NB HDPE","m",110,{"v":0,"d":"0.00"},{"$f":"ROUND(G23 * H23,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","28ad1cae-221d-4256-82a7-b47bb3a46da3","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","cbb67c5c-ab0b-49cc-ab72-0e11a90ccfb2","","","Over 100 mm up to 200 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","e9261ec6-8976-4f8b-a44b-603cdc284222","B.2.1.1.3.2","","0,0 m                       1,0 m","m",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G26 * H26,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f4e5bff1-232c-4bc3-ae99-9e1b9b7259ae","B.2.1.1.3.3","","1,0 m                       2,0 m","m",150,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","95b763ed-9f14-461d-85ee-7b19b3a1e5ac","B.2.1.1.3.4","","2,0 m                       3,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","c9b96047-2121-4cda-9807-e5d39b518d95","","","Over 400 mm up to 600 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Rate Only","bb235e43-ef4d-4d02-90c6-58f74f3b4f31","B.2.1.1.3.5","","0,0 m                       1,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","2120ac11-c7bc-4c54-b81b-1a747a2b9aaa","B.2.1.1.3.6","","1,0 m                       2,0 m","m",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b6e750d8-ac2f-4466-8fbd-915b15d3c084","B.2.1.1.3.7","","2,0 m                       3,0 m","m",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e3bb62e9-eddf-49f2-9de6-5125266117b9","B.2.1.1.3.8","","3,0 m                       4,0 m","m",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f1999323-7911-4c56-a553-231f3587bb31","B.2.1.1.3.9","","4,0 m                       5,0 m","m",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","34ae5e7d-13fd-40a7-98b5-960f32a23888","B.2.1.1.3.10","","5,0 m                       6,0 m","m",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0f76c723-2a10-4744-a6f3-441ec1bb1c3a","B.2.1.1.3.11","","6,0 m                       7,0 m","m",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","6d230cd2-2c1f-4d22-9afa-49a958916737","","","Over 600 mm up to 1000 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","e723218a-a448-4f28-9e93-18a158a55ee7","B.2.1.1.3.12","","0,0 m                       1,0 m","m",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G38 * H38,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f745446e-e3a8-4414-b6c0-d1a8c376ee7e","B.2.1.1.3.13","","1,0 m                       2,0 m","m",34,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3fb7734b-93f4-41b8-af95-92219497330a","B.2.1.1.3.14","","2,0 m                       3,0 m","m",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","695bb4d0-dbb5-49d5-89ca-7827dc013669","B.2.1.1.3.15","","3,0 m                       4,0 m","m",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5aa90e47-c22d-4e14-a36e-0533cbd6f03a","B.2.1.1.3.16","","4,0 m                       5,0 m","m",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","25d6d2d2-565e-4f7b-8269-4ec4a6b385c1","B.2.1.1.3.17","","5,0 m                       6,0 m","m",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7fcbb6ba-c347-4550-bc36-154ef0d9dea8","B.2.1.1.3.18","","6,0 m                       7,0 m","m",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","0d5d9066-4299-40cd-a507-83e74821b2a3","","","Over 1000 mm up to 1200 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","4a23b2b8-2561-43b9-9dcf-0c14cf502cb5","B.2.1.1.3.19","","1,0 m                        2,0 m","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G46 * H46,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3708fcd5-5aa9-42c7-ae63-a4b956faaefa","B.2.1.1.3.20","","2,0 m                        3,0 m","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2fb6eb70-ba2f-402c-9d83-cfb59017a86a","B.2.1.1.3.21","","3,0 m                        4,0 m","m",150,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","eafbdc98-c4a5-4c6b-af09-39d29b3d564f","B.2.1.1.3.22","","4,0 m                        5,0 m","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","d58f01e0-c184-48d4-a5ed-65ec275c51e0","B.2.1.1.3.23","","5,0 m                        6,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","88fce282-07bd-4dce-938d-75b7fcf3e20c","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.2.1.1.3.2 to B.2.1.1.3.23 incl. for (provisional):",{"$nulls":4},"Dflt"]
["Item","c3fd4cbf-04cd-4fb6-b5f8-cc83b4b13d36","B.2.1.1.3.24","8.3.2(b)\nPSD 8.3.2(b)","Hard rock excavation","m³",93,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5ffe9d48-b062-4642-aefd-d9b72625ced4","B.2.1.1.3.25","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",35,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","3acb28b9-d2d7-4961-9cd9-a41e8fbda860","B.2.1.1.4","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","4c4292d7-d117-4cce-b038-5f5db9c58169","","8.3.3.1","Make up deficiency in backfill material (Provisional)",{"$nulls":4},"Dflt"]
["Item","e5b66dfd-53b0-48b8-b64b-1a1a3d24579d","B.2.1.1.4.1","8.3.3.1(a)","from other necessary excavations on site","m³",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G56 * H56,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","485be4fb-0339-4870-91fe-676a38e085d1","B.2.1.1.4.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",60,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","f5eefcc1-1e3f-438e-b1a4-432c03f19d4a","B.2.1.1.5","SANS 1200DB","PARTICULAR ITEMS",{"$nulls":4},"Dflt"]
["Label","1138641f-76e4-4877-a7a2-2818df92723b","","8.3.4(a)\nPSD 8.3.15","Shore trench opposite structure or service or in unsuitable excavated materials for depths (Provisional)\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","991fe3cd-f1b3-4cf0-9e4e-9434e644bdaf","B.2.1.1.5.1","","1,0 m                        2,0 m","m",103,{"v":0,"d":"0.00"},{"$f":"ROUND(G60 * H60,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","08a558f0-a86d-4c7a-84a3-9b983663701a","B.2.1.1.5.2","","2,0 m                        3,0 m","m",29,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8bafad76-6ac5-499b-9544-d3e7ec9a78e9","B.2.1.1.5.3","","3,0 m                        4,0 m","m",158,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","58d5e156-8ec8-4ab6-af66-f0f1ffe54e80","B.2.1.1.5.4","","4,0 m                        5,0 m","m",23,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c13db995-0ee1-4d04-8194-bf5b0192b1e1","B.2.1.1.5.5","","5,0 m                        6,0 m","m",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","92505fce-8423-4daa-8b00-d9476a9fcd1d","B.2.1.1.5.6","","6,0 m                        7,0 m","m",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","1f2829cf-4583-4ae1-9893-274d11354c9d","B.2.1.1.6","SANS 1200L","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","1c38152a-eaa9-4db6-ade8-2b04288ebfb4","","8.2.1\nPSL 8.2.1","uPVC pipes Class 9: Supply, handle, lay, and bed, complete with approved spigot and socket joints to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Item","672c3851-0ac1-4c93-8ac5-c6b253995221","B.2.1.1.6.1","","110mm NB","m",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G68 * H68,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","d5e3cee2-26bb-418e-89fb-26b550a5ae3f","B.2.1.1.6.2","","160mm NB","m",150,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","99a6ca45-6fd3-43f8-82c4-e3e35bd390c5","","8.2.1\nPSL 8.2.1","oPVC pipes Class 9: Supply, handle, lay, and bed, complete with approved spigot and socket joints to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Rate Only","d87e5eba-2e81-42ed-9122-57e244ecb82c","B.2.1.1.6.3","","600 mm NB","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","8506bbba-a5d2-433a-b9da-fc72f9b420bd","","PSLD 3.1.2 PSLD 8.2.1","Reinforced concrete pipe Class 100D with cast in HDPE liner : Supply, handle, lay, and bed, complete with approved spigot and socket joints to suit, test, and disinfect (potable water pipelines)",{"$nulls":4},"Dflt"]
["Item","af3c1582-3527-4ec6-8fb1-3eb1d661b0f9","B.2.1.1.6.4","","1050 mm NB","m",125,{"v":0,"d":"0.00"},{"$f":"ROUND(G73 * H73,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5be08aca-4e44-4674-8913-c901fa021ef4","","8.2.1\nPSL 8.2.1","Steel pipes with lining & coating:\nSupply, handle, lay, and bed, complete with approved flexible coupling type joint to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Item","6a7c417a-6fad-4e87-95eb-6e5c920d4438","B.2.1.1.6.5","","400 mm NB x 4.5 mm wall thickness","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G75 * H75,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ed4b156b-8764-47f8-bf66-95f82eeed50c","B.2.1.1.6.6","","500 mm NB x 6 mm wall thickness","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","24393a5d-3b2f-43ec-9ce9-e2095fe5e9ad","B.2.1.1.6.7","","600 mm NB x 4.5 mm wall thickness","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1c01d225-8b4a-4c16-a689-99db09ae1db1","","8.2.1\nPSL 8.2.1","Steel pipes with lining/coating:\nHandle, lay, and bed, complete with approved flexible coupling type joint to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Item","54031833-5369-42cd-9513-5791a8a60a56","B.2.1.1.6.8","","1200 mm NB x 6.0 mm wall thickness","m",85,{"v":0,"d":"0.00"},{"$f":"ROUND(G79 * H79,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","ae2918f9-9868-43f1-a4ff-42616ed9b432","","PSL 8.2.1","Inspection of pipes:",{"$nulls":4},"Dflt"]
["Sum","2fc2889a-1347-4e2a-89f2-f9916856f944","B.2.1.1.6.9","","Inspect pipes, documenting defects, acceptance of pipes etc. (Provisional)","P Sum",1,{"v":100000,"d":"100,000.00"},{"$f":"ROUND(H81,2)","v":{"v":100000,"d":"100,000.00"}},"Dflt"]
["Label","c8327820-8afc-42c1-b57d-c175e8a97e4c","","8.2.15\nPSL 8.2.15","Special wrapping in corrosive soil as per Project Specification PSL3.9.3.8 (Provisional):",{"$nulls":4},"Dflt"]
["Item","37fd67d1-6123-4f94-95dc-0f7a020f842d","B.2.1.1.6.10","","160 mm NB","No",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G83 * H83,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","52f9f082-b6cc-4fc9-8c09-4f7cbfa7dabf","B.2.1.1.6.11","","400 mm NB","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b16575c7-5451-41f9-bb9d-e3d244f0de78","B.2.1.1.6.12","","500 mm NB","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a25e0c1a-4c4f-4294-8aea-679d4b05ba17","B.2.1.1.6.13","","600 mm NB","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","b9aa786d-3917-44f7-b52e-4f355b53ab5c","B.2.1.1.6.14","","1000 mm NB","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","5e4e3e0c-2d35-471d-b2cd-76a3d0030350","B.2.1.1.6.15","","1200 mm NB","No",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G88 * H88,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","f253a062-7030-4826-9bb5-ca01161bc7ff","B.2.1.1.7","SANS 1200L","SPECIALS AND FITTINGS",{"$nulls":4},"Dflt"]
["Label","4fd43687-3536-44b1-8eb6-3f76b3623188","","8.2.2","Extra over items B.2.1.1.6.2 for the supplying, laying and bedding of specials complete with spigot and socket joint couplings to suit uPVC pipe",{"$nulls":4},"Dflt"]
["Label","35567ff0-80b8-44a5-ad4a-74d81470777b","","","Bends uPVC Class 9, of deflection:",{"$nulls":4},"Dflt"]
["Item","13d4f3b0-88b7-44cd-b417-025debe61467","B.2.1.1.7.1","","160 mm, 90 deg.","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G92 * H92,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","17e668c1-192e-47c9-a30c-d2f1b5a7960a","B.2.1.1.7.2","","160 mm, 45 deg.","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e588c6f6-3cca-4da1-a6c4-78bddc779120","B.2.1.1.7.3","","160 mm, 22.5 deg.","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","9af03f41-58c5-4a75-a4d2-75adee47d5f2","","","Tees uPVC Class 9:",{"$nulls":4},"Dflt"]
["Rate Only","c0f55163-50e2-414e-ada3-0462255742d1","B.2.1.1.7.4","","160 mm x 160 mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","a26e122d-78e6-4a90-8161-8ac6d3f98e3c","","","Flange Adaptors, Steel to uPVC:",{"$nulls":4},"Dflt"]
["Item","22ced47e-0ce6-400b-be05-3a3f4d61752a","B.2.1.1.7.5","","150 mm NB","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G98 * H98,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","dd64ae94-f33f-4172-a6b4-78b90e0201e0","","8.2.2","Extra over item B.2.1.1.6.4 for the relaying and rebedding of a HDPE pipe specials, complete with approved flexible couplings to suit HDPE pipe as approved by the Engineer.",{"$nulls":4},"Dflt"]
["Label","524fe2ca-d383-4f97-89b7-b3d3b5e34f93","","","HDPE bends, of deflection:",{"$nulls":4},"Dflt"]
["Rate Only","d778ffae-7f2e-459a-9f9a-d009424e6101","B.2.1.1.7.6","","1000 mm, 90 degrees","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","0d360259-f88e-4bc3-9941-fb66908090e0","B.2.1.1.7.7","","1000 mm, 45 degrees","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","b0dfe80e-c19b-4d41-bf4b-3a2202c6f945","B.2.1.1.7.8","","1000 mm, 22.5 degrees","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","13bd2cf7-83b5-442d-8dae-87bc3721609d","","","Flange Adaptors, Steel to HDPE:",{"$nulls":4},"Dflt"]
["Rate Only","900dd42c-7f26-4a25-95b3-000583b6c32c","B.2.1.1.7.9","","1000 mm NB","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","2ca99060-a6c0-44ed-b875-15732027c0aa","","8.2.2","Extra over item B.2.1.1.6.4 for the supplying, laying and bedding of steel pipe specials with lining & coating cast into concrete where necessary, complete with approved flexible couplings to suit pipes as per Dwg. Nos. J40073/010-201, J40073/010-203 and J40073/010-208:",{"$nulls":4},"Dflt"]
["Rate Only","042f9616-66a2-401b-bb93-b7cd5aec9ed9","B.2.1.1.7.10","","1000 mm NB (J40073/010-201)","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","9e9a85af-0c1b-4ee7-82ad-0c47fbcb5041","B.2.1.1.7.11","","1000 mm NB (J40073/010-203)","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","5ee3db84-e296-4cde-a8c7-2e7f6eb1595c","","8.2.5","Supply and fit, incl. bed, test and disinfect (if for potable water) pipes and specials as per Dwg. No. J40073/010-208 (Short pipe runs only):",{"$nulls":4},"Dflt"]
["Item","d2870f56-858b-4a6f-aa25-922c548d76c1","B.2.1.1.7.12","","Item No. P12-B/1 - 500 mm NB mild steel pipe 90 deg. elbow,\n6 mm wall thickness","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G110 * H110,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","cd7650dd-6252-428d-b7b0-b7f5c411606d","B.2.1.1.7.13","","Item No. P12-B/2 - 500 mm NB mild steel straight pipe,\n6 mm wall thickness","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ee612b2d-d33e-40dd-9918-f85b242dd689","B.2.1.1.7.14","","Item No. P12-B/3 - 500 mm NB mild steel pipe 90 deg. medium radius bend, 6 mm wall thickness, flanged on end","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f83a4e19-a753-4085-a9bd-4c5748e2cad0","B.2.1.1.7.15","","Item No. P12-B/4 - 500 mm NB steel VJ dismantling coupling flanged both end","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","e6f7059b-3b6c-4c2d-81ef-45986115c619","","8.2.5","Supply and fit, incl. bed, test and disinfect (if for potable water) pipes and specials as per Dwg. No. J40073/010-224 (Short pipe runs only):",{"$nulls":4},"Dflt"]
["Item","e60a50ff-6730-4c6a-969e-14d3887a9b14","B.2.1.1.7.16","","Item No. P7-B/1 - 600 mm NB mild steel pipe 90 deg. elbow, 4.5 mm wall thickness","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G115 * H115,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0e6a3b67-c857-4259-abcf-7c447ed19d81","B.2.1.1.7.17","","Item No. P7-B/2 - 600 mm NB mild steel straight pipe, 4.5 mm wall thickness","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e7bfce66-27bc-462c-baa7-7dc0ca56ddfd","B.2.1.1.7.18","","Item No. P7-B/3 - 600 mm NB mild steel pipe 90 deg. medium radius bend, 4.5 mm wall thickness","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4f670b0b-180b-410f-aca8-0c2b1b624552","B.2.1.1.7.19","","Item No. P7-B/4 - 600 mm NB mild steel straight pipe flanged one end, 4.5 mm wall thickness, flanges to be drilled to accommodate oPVC Class 9 stub flange","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","cc75ee3f-f032-44b5-a712-a4072da599f3","B.2.1.1.7.20","","Item No. P7-B/5 - 600 mm NB mild steel backing ring drilled to accommodate oPVC Class 9 stub flange","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","86c0ba29-32d6-4532-a1a9-0fd652f72ea0","B.2.1.1.7.21","","Item No. P7-B/6 - 600 mm NB oPVC Class 9 straight pipe, stub flange on one end","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","81badd09-3f54-4ea2-b6f5-3db4f2607d6e","","8.2.5","Supply and fit, incl. bed, test and disinfect (if for potable water) pipes and specials as per Dwg. No. J40073/010-224 (Short pipe runs only):",{"$nulls":4},"Dflt"]
["Item","380e396c-996d-4245-83a0-5051a9cc055e","B.2.1.1.7.22","","Item P8-B/1 - 1200 mm Steel VJ dismantling coupling flanged both ends","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G122 * H122,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","944d1931-a86b-48c9-afc9-81c4221f6159","","8.2.5","Fit, incl. bed, test and disinfect (if for potable water) pipes and specials as per Dwg. No. J40073/010-224 (Short pipe runs only):",{"$nulls":4},"Dflt"]
["Item","6dac2eb8-4bd6-4758-a1cb-d2b65a135a58","B.2.1.1.7.23","","Item P8-B/3,6&8 - 1200 mm, 45 degrees","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G124 * H124,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2ba7c517-0095-47f3-9ed7-9c214d5c3c8b","","8.2.2","Extra over items B.2.1.1.6.5 to B.2.1.1.6.7 for the supplying, laying and bedding of steel pipe specials, complete with approved flexible couplings to suit steel pipe",{"$nulls":4},"Dflt"]
["Label","8d37e14c-f9a9-4f3a-b598-657499d8b6a8","","","Steel bends, of deflection:",{"$nulls":4},"Dflt"]
["Item","1edebef8-42ca-43a9-ae0d-29027800f594","B.2.1.1.7.24","","400 mm, 90 degrees","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G127 * H127,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","efd848e0-d6c8-4989-ac8e-4c39e64c93bf","B.2.1.1.7.25","","400 mm, 45 degrees","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5e97ac54-06ce-4a4a-8dcb-6c603f5b784b","B.2.1.1.7.26","","400 mm, 22.5 degrees","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","c11be63d-e5cd-4528-8d29-3accdf0505f0","B.2.1.1.7.27","","600 mm, 90 degrees","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","566e53d1-32ee-4580-a777-e9eac766b409","B.2.1.1.7.28","","600 mm, 45 degrees","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G131 * H131,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","812c2ded-bc76-4496-8eee-819d46cf76ed","B.2.1.1.7.29","","600 mm, 22.5 degrees","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","2bbefde7-fadc-40ae-9064-0d40b1691f5e","","","Flange Adaptors, Steel to oPVC:",{"$nulls":4},"Dflt"]
["Rate Only","a8cadf2a-860c-4ad9-afc6-2d05a26ed15d","B.2.1.1.7.30","","600 mm NB","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","3a846ee3-7876-4dd9-9d85-66228249fa19","","","Dismantling Joints, Steel to Steel:",{"$nulls":4},"Dflt"]
["Item","27bd409b-fa86-44de-9814-ebbbcf2450ba","B.2.1.1.7.31","","600 mm NB","No",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G136 * H136,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","e316b154-1038-4a8e-9900-33e63b4e55bc","","","Dismantling Joints, Steel to Steel:",{"$nulls":4},"Dflt"]
["Item","5b3715a8-4663-4f8d-a99e-54f9e402e4c3","B.2.1.1.7.32","","1200 mm NB","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G138 * H138,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","0946f23d-0e49-4d2b-85ae-47be24794126","B.2.1.1.8","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","488149bc-778b-444b-82ec-d0f0a2972e46","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional):",{"$nulls":4},"Dflt"]
["Item","e5171363-992d-4aaf-9376-b4b841d8f9f7","B.2.1.1.8.1","8.2.2.3(a)","Selected granular material (cradle)","m³",265,{"v":0,"d":"0.00"},{"$f":"ROUND(G141 * H141,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4a13e27a-c3b3-434d-bac1-72e0d2cd164f","B.2.1.1.8.2","8.2.2.3(b)","Selected fill material (blanket)","m³",375,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5d3c3571-319b-44f4-a09d-89ff79776ceb","B.2.1.1.8.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",55,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e75b3a01-57ca-4542-aea8-e7bbfbe5336d","B.2.1.1.8.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",185,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","19c297a9-7bb1-4986-9bed-04cd077f36d4","","","Concrete bedding (Provisional):",{"$nulls":4},"Dflt"]
["Item","4e2e4b07-122b-433f-8fa2-c9823b0ffcf1","B.2.1.1.8.5","8.2.3","Strength Concrete: 15 MPa/19 mm","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G146 * H146,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","2ea26ae6-5eb9-4802-bcec-3ea485d22165","B.2.1.1.9","","ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","088a23fc-ef83-4055-ac01-a1cec49c1288","","SANS 1200L\n8.2.11","Anchor/Thrust blocks and pedestals:",{"$nulls":4},"Dflt"]
["Item","d8d59e83-d909-427e-98d2-a7285a987567","B.2.1.1.9.1","","Strength Concrete: 15 Mpa/19 mm ","m³",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G149 * H149,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3058fd6f-ad52-48e7-866a-75f43ddb0264","B.2.1.1.9.2","","Formwork: rough, vertical plane","m²",80,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","77ae9c1f-11f6-4c39-8a72-c3068170a3de","B.2.1.1.9.3","SANS 1200LD 8.2.9\nPSL 8.2.19","Pipeline marker posts","No",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","5ca07349-9e0d-4df1-bc9c-6390a1edcbe3","","SANS 1200LB","Encasing of pipes:",{"$nulls":4},"Dflt"]
["Item","c8a5ced1-785a-4c04-949e-e7eba621c9d6","B.2.1.1.9.4","8.2.4\nPSLB 8.2.4","Strength Concrete: 15 MPa/19 mm","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G153 * H153,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","176b9e40-a9b2-4412-8d92-aca71ea5ca85","B.2.1.1.10","SANS 1200D","EXISTING SERVICES",{"$nulls":4},"Dflt"]
["Label","fc7ced5d-6312-4b55-ae4e-cd9afbe31352","","","Services across and in trenches:",{"$nulls":4},"Dflt"]
["Item","d698ed03-9ce6-4945-bd0e-b8d531ab3123","B.2.1.1.10.1","8.3.8.1(c)","Excavate by hand in soft material to expose existing services","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G156 * H156,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","29685b10-a652-42d7-8151-cb168be038fd","","","Dealing with services:",{"$nulls":4},"Dflt"]
["Sum","6f6f7697-b0df-41b2-b46d-ed5eedc9f8c8","B.2.1.1.10.2","8.3.8.2(b)","Permanent protection of Existing service (Provisional)","P Sum",1,{"v":10000,"d":"10,000.00"},{"$f":"ROUND(H158,2)","v":{"v":10000,"d":"10,000.00"}},"Dflt"]
["Sum","f96d3816-0469-4d5e-8d78-e691aeb9b4db","B.2.1.1.10.3","8.3.8.2(c)","Temporary protection of Existing service (Provisional)","P Sum",1,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"},"Dflt"]
["Label","21d6b17d-d817-4c8c-ba8d-fbff0fb2655e","","SANS 1200DB\n8.3.5(a)\nPSDB 8.3.5","Services that intersect a trench:",{"$nulls":4},"Dflt"]
["Item","a08e1ca9-ac02-41da-91ec-950f2a1778c5","B.2.1.1.10.4","","Cables","No.",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G161 * H161,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4c02f43d-fa79-4e31-89a1-38cf6e5aaa65","B.2.1.1.10.5","","Sewer Rising mains up to 400 mm diam.","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","fee21b6b-c743-4030-ac84-7ef81c65a229","","SANS 1200DB\n8.3.5(b)\nPSDB 8.3.5","Services that adjoin a trench:",{"$nulls":4},"Dflt"]
["Item","6a68261a-ba9b-4097-95ad-470cdab47132","B.2.1.1.10.6","","Cables","m",45,{"v":0,"d":"0.00"},{"$f":"ROUND(G164 * H164,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","770cb41a-5bdb-4397-b65e-24808087ff66","B.2.1.1.10.7","","Sewer Rising mains up to 400 mm diam.","m",100,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","6fa3ceb5-c69b-4c1f-871b-5f6c185fefc1","B.2.1.1.11","1200 LD\n8.2.3","MANHOLES, ETC.",{"$nulls":4},"Dflt"]
["Label","988788a9-14ce-423e-a739-ae00ee24e3fe","","8.2.3\nPSLD\n8.2.3\nPSG 3.5.4","Cast in-situ concrete manholes, with heavy duty concrete lockable lid and\nframe, as per Dwg. No. J40073/010-600, for depths\nover          and          up to",{"$nulls":4},"Dflt"]
["Rate Only","fd16ad48-1e70-401f-815a-73070a725251","B.2.1.1.11.1","","  -                              1.0 m"," No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","39bedd36-081c-4e9a-a860-c611d71ae389","B.2.1.1.11.2","","1,0 m                        2,0 m"," No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","5e35e5c2-de3b-4be5-a7ca-78374f2c442e","B.2.1.1.11.3","","2,0 m                        3,0 m"," No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","1f9bdbcf-4397-4fef-b4b7-0ed0799f0652","B.2.1.1.11.4","","3,0 m                        4,0 m"," No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G171 * H171,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","a5a8bd78-2ccd-403b-ba7d-248f58553c36","B.2.1.1.11.5","","4,0 m                        5,0 m"," No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header3","8d258f6f-faa9-4669-a265-61bbd0cb120e","B.2.1.1.12","SANS 1200LD","SUNDRIES",{"$nulls":4},"Dflt"]
["Sum","9a445ea6-4a8e-4542-867c-fa1b8ac5b97b","B.2.1.1.12.1","8.2.11\nPSLD 8.2.11","Connect to existing splitter box (from BNR) including excavation, backfilling and all necessary specials and fittings etc. inclusive all work to complete connection.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H174,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","223c193d-7bfb-4218-b4d6-e79281438f3e","B.2.1.1.12.2","PSL 8.2.17\nPSL 8.2.20","Connect to existing live (from RAS pump station), 400mm to 500mm dia uPVC pipeline, inclusive all work to complete connection.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G175 * H175,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","056cee46-1f02-4073-8da5-27c2c0515207","B.2.1.1.12.3","8.2.11\nPSLD 8.2.11","Connect to existing splitter box (from SST) including excavation, backfilling and all necessary specials and fittings etc. inclusive all work to complete connection.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H176,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","98309788-a13b-45fc-9a59-9c5999cf4d15","B.2.1.1.12.4","PSL 8.2.17\nPSL 8.2.20","Connect to existing RAS pump station live (from SST), inclusive all work to complete connection.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G177 * H177,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Section","33a29211-81b1-449d-bb96-b31f3508e579","B.2.2","","MEDIUM PRESSURE PIPELINES\n(IRRIGATION PUMP STATION RISING MAIN.",{"$nulls":4},"Dflt"]
["Label","0948484f-9368-4b1c-8fd8-8458111be68c","","SANS 1200L","SECTION B.2.2 : MEDIUM PRESSURE PIPELINES\n(IRRIGATION PUMP STATION RISING MAIN.",{"$nulls":4},"Dflt"]
["Header3","692f5d97-8f5a-4b62-9942-0814dba2a4c6","B.2.2.1","SANS 1200DB\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","754bf4fc-e39c-46cb-a342-91797b7df7d8","B.2.2.1.1","8.3.1(a)","Clear vegetation and trees of girth up to 1 m","m",295,{"v":0,"d":"0.00"},{"$f":"ROUND(G181 * H181,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","cfd3bde9-0af3-42d2-8259-8cead912121f","B.2.2.1.2","8.3.1(c)","Remove topsoil to depth of 150mm","m²",210,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8a13fdd6-314c-43fd-869b-26eb58c1ee56","B.2.2.1.3","SANS 1200C 8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",100,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","86a50562-5d61-47e2-868a-afd262c82b15","B.2.2.2","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Label","1121163b-9e18-43ce-a8b6-416e5c3a4404","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","d16584d2-791e-4292-80f6-5f0d54b4d51b","","","Over 100 mm up to 200 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","fe03f313-8f68-43ab-afbe-31c421c33ae6","B.2.2.2.1","","0,0 m                       1,0 m","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G187 * H187,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9ae37a0e-7adb-4421-9055-17d7a604311f","B.2.2.2.2","","1,0 m                       2,0 m","m",265,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d92b5df4-2312-4bfb-ae02-e878bb82cc77","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.2.2.2.1 to B.2.2.2.2 incl. for (Provisional):",{"$nulls":4},"Dflt"]
["Item","ea8eabc3-9526-4171-9e67-740db70f5948","B.2.2.2.3","8.3.2(b)\nPSD 8.3.2(b)","Hard rock excavation","m³",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G190 * H190,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","49e14f3f-1410-4f89-b089-685eca70c7c3","B.2.2.2.4","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","0637360f-47a3-42a3-bced-4a9741c43e24","B.2.2.3","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","f7e3e266-a37a-4929-a706-938c02a5909d","","8.3.3.1","Make up deficiency in backfill material (Provisional):",{"$nulls":4},"Dflt"]
["Item","73aeb516-e9ec-42c2-aa7c-45f70173543b","B.2.2.3.1","8.3.3.1(a)","from other necessary excavations on site","m³",16,{"v":0,"d":"0.00"},{"$f":"ROUND(G194 * H194,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4c27433d-41e3-41ff-9773-8a30ab86bf77","B.2.2.3.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",12,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","aea5abde-7a96-453a-8a19-7a4954ef1225","B.2.2.4","SANS 1200L","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","901d4d15-764d-4c02-94e7-4a2325c24c49","","8.2.1\nPSL 8.2.1","uPVC pipes Class 9: Supply, handle, lay, and bed, complete with approved spigot and socket joints to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Item","1e01747d-52c0-4da1-a295-522453d46713","B.2.2.4.1","","110mm NB","m",295,{"v":0,"d":"0.00"},{"$f":"ROUND(G198 * H198,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8772f7e0-6662-4291-beab-1042898efd4a","","8.2.15\nPSL 8.2.15","Special wrapping in corrosive soil as per Project Specification PSL3.9.3.8 (Provisional):",{"$nulls":4},"Dflt"]
["Item","aca9678b-ad5b-4971-b90e-f2c54fe6bb38","B.2.2.4.2","","110 mm NB","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G200 * H200,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","8c610b78-3179-4135-8b52-7d5c065f3133","B.2.2.5","SANS 1200L","SPECIALS AND FITTINGS",{"$nulls":4},"Dflt"]
["Label","84d03f69-c983-42c2-a865-24c053df0a02","","8.2.2","Extra over items B.2.2.4.1 for the supplying, laying and bedding of specials complete with spigot and socket joint couplings to suit uPVC pipe",{"$nulls":4},"Dflt"]
["Label","c54df2d2-8c4a-4825-a94e-430966dc8e23","","","Bends uPVC Class 9, of deflection:",{"$nulls":4},"Dflt"]
["Item","699a63bc-f66c-465a-aef7-9abe6a005a45","B.2.2.5.1","","110 mm, 90 deg.","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G204 * H204,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","e26d3614-f2d7-4a1d-8d62-6408613a7048","B.2.2.5.2","","110 mm, 45 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","af0cd1a0-5157-4bbc-97b4-4da925cf7e04","B.2.2.5.3","","110 mm, 22.5 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","201e2dc2-b6f3-4d1d-9641-e4bbcf6eb9ce","","8.2.5","Supply and fit, incl. bed, test and disinfect (if for potable water) pipes and specials as per Dwg. No. J40073/010-220 & J40073/010-224 (Short pipe runs only):",{"$nulls":4},"Dflt"]
["Item","986b31f7-ce69-4bc0-92f7-f42e1eb37f79","B.2.2.5.4","","Item No. P13-B/1 - 90 deg. 100 mm NB mild steel short gusset bend, 4.5 mm wall thickness","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G208 * H208,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c61898ab-5e8c-4f6a-baa6-09a0d8549e36","B.2.2.5.5","","Item No. P13-B/2 - 100 mm NB mild steel straight pipe, 4.5 mm wall thickness","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","74ad3bd7-fb23-4fbc-8e4f-3678c2e7d48e","B.2.2.5.6","","Item No. P13-B/3 - 100 mm NB mild steel straight pipe, 4.5 mm wall thickness","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","34b68874-6e21-43cb-829a-761f6630e2b4","B.2.2.5.7","","Item No. P13-B/4 - 100 mm NB 90 deg. elbow mild steel flanged one end, 4.5 mm wall thickness dimensions to be confirmed by manufacturer","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c967c5d2-d4b4-4071-ae88-c2787af6a954","B.2.2.5.8","","Item No. P13-B/5 - 110 mm NB uPVC Class 9 straight pipe with uPVC to steel flanged coupling at one end","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","66af898d-a883-4b7d-8d02-218dcee68cb5","B.2.2.6","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","d2cac809-1cb3-4967-9601-86c32b197b07","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional):",{"$nulls":4},"Dflt"]
["Item","2de3fc7c-218a-494f-83c7-851ea2941c02","B.2.2.6.1","8.2.2.3(a)","Selected granular material (cradle)","m³",75,{"v":0,"d":"0.00"},{"$f":"ROUND(G215 * H215,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","01d0e8e7-72a7-45cf-839b-d77c65840c09","B.2.2.6.2","8.2.2.3(b)","Selected fill material (blanket)","m³",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","14e23d41-207b-4d61-a86c-a5eb18586bd5","B.2.2.6.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bded807e-88c4-4092-a6fd-47b5423f5c55","B.2.2.6.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",55,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","becbead6-6741-4705-9c85-16d6daf5f38c","B.2.2.7","","ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","8b130e37-0600-4810-adaa-36f085363215","","SANS 1200L\n8.2.11","Anchor/Thrust blocks and pedestals:",{"$nulls":4},"Dflt"]
["Item","c2b9deea-9563-4f60-a952-cc77c4986433","B.2.2.7.1","","Strength Concrete: 15 Mpa/19 mm ","m³",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G221 * H221,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c9d7e6c6-68a4-42b1-8399-f6b1ad358062","B.2.2.7.2","","Formwork: rough, vertical plane","m²",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","cd21cf3a-a702-4895-8565-58b9f7c37d04","B.2.2.7.3","SANS 1200LD 8.2.9\nPSL 8.2.19","Pipeline marker posts","No",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Section","daaa680c-339a-4146-add2-3aa79d176cbc","B.2.3","","WATER RETICULATION (BUILDINGS)",{"$nulls":4},"Dflt"]
["Label","14c780f3-e8cd-48e6-804b-c6dc4084878f","","SANS 1200L","SECTION B.2.3 : WATER RETICULATION (BUILDINGS)",{"$nulls":4},"Dflt"]
["Header3","2fd81b54-40e9-48fe-982a-7aaa19402c2e","B.2.3.1","SANS 1200DB\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","79295f23-a0a8-4d2b-bbe5-07a5724b328b","B.2.3.1.1","8.3.1(a)","Clear vegetation and trees of girth up to 1 m","m",265,{"v":0,"d":"0.00"},{"$f":"ROUND(G227 * H227,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","35fea5d2-9808-4458-8a50-89236aa4a922","B.2.3.1.2","8.3.1(c)","Remove topsoil to depth of 150mm","m²",130,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","55044676-dffb-4cd4-95df-aa8505357455","B.2.3.1.3","SANS 1200C 8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","db248ba7-6c9e-45ad-a632-7574128d443f","B.2.3.2","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Label","e8340adc-e60d-446b-8ae5-d45268967b80","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","1b8f60e7-aea0-41bc-abff-fe90133edf1b","","","Up to 100 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","0a21ff5c-d31c-4f35-b5c8-3ea40f0c7e29","B.2.3.2.1","","0,0 m                       1,0 m","m",225,{"v":0,"d":"0.00"},{"$f":"ROUND(G233 * H233,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","141b3d17-e80c-4ac9-8658-d0c099f0cfdf","B.2.3.2.2","","1,0 m                       2,0 m","m",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","9a7e1492-89a0-4ede-b771-6a7bc3942fc8","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.2.3.2.1 to B.2.3.2.2 incl. for (Provisional):",{"$nulls":4},"Dflt"]
["Item","67ed064a-e71c-49a9-858c-ab9b0f19c154","B.2.3.2.3","8.3.2(b)\nPSD 8.3.2(b)","Hard rock excavation","m³",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G236 * H236,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","214d1346-ad2e-43da-acfd-6d03e780c211","B.2.3.2.4","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","11d3f2b3-2ab5-4732-8a8f-4b36f20bae24","B.2.3.3","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","9aafd257-e17d-4f03-9ac4-8e1f5fa19b86","","8.3.3.1","Make up deficiency in backfill material (Provisional):",{"$nulls":4},"Dflt"]
["Item","5b91db23-0f13-4e4c-923b-d91a85d76f8b","B.2.3.3.1","8.3.3.1(a)","from other necessary excavations on site","m³",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G240 * H240,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a7e9db12-f634-4956-bfe4-ef6e48de0dba","B.2.3.3.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","de9606b9-8c63-44a8-ad0d-6a7aabc2a545","B.2.3.4","SANS 1200L","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","173d5623-3022-468d-8569-97f9f24012c5","","8.2.1\nPSL 8.2.1","HDPE pipes Class 12: Supply, handle, lay, and bed, complete with approved couplings for joints to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Item","9fb07289-c7d8-465e-8ed1-ac8aafa37985","B.2.3.4.1","","25 mm NB","m",155,{"v":0,"d":"0.00"},{"$f":"ROUND(G244 * H244,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1ad7657d-0338-4cff-a84b-20bf579aabbc","B.2.3.4.2","","40 mm NB","m",215,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","36bdfe96-82bc-4522-8638-89beb384e13b","B.2.3.4.3","","75 mm NB","m",265,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","ec9ed358-67eb-4ba2-bb85-3e76da6e2ca6","B.2.3.5","SANS 1200L","SPECIALS AND FITTINGS",{"$nulls":4},"Dflt"]
["Label","ceac1159-4ac2-4e42-b307-ff296705c989","","8.2.2","Extra over items B.2.3.4.1 to B.2.3.4.3 for the supplying, laying and bedding of specials complete with approved joint couplings to suit HDPE pipe",{"$nulls":4},"Dflt"]
["Label","6613f732-43ea-4471-a597-f27ed06c0b68","","","Bends HDPE Class 12, of deflection:",{"$nulls":4},"Dflt"]
["Item","9a4f6891-4111-40c2-b7b2-62589950f299","B.2.3.5.1","","25 mm, 90 deg.","No",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G250 * H250,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","ee604fe4-817d-437e-a824-3c669fa5ab25","B.2.3.5.2","","25 mm, 45 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","3b540e23-e819-4852-9c5c-c8479bbd72ca","B.2.3.5.3","","25 mm, 22.5 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","39434d8f-7b7a-4f5c-b3f4-5e9fd000c556","B.2.3.5.4","","40 mm, 90 deg.","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G253 * H253,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","b6063b61-8a8a-4658-b66f-b87a9d8218b2","B.2.3.5.5","","40 mm, 45 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","079fc358-80ce-4039-a81f-583a4d0a5da3","B.2.3.5.6","","40 mm, 25 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","f960da02-a86b-461f-912f-8161dd83e046","B.2.3.5.7","","75 mm, 90 deg.","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G256 * H256,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","4e4c0295-bf06-41aa-ab00-28f9b5203675","B.2.3.5.8","","75 mm, 45 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","f4b3bad0-c721-4c64-9247-cbc0cf57939d","B.2.3.5.9","","75 mm, 22.5 deg.","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","71fc8c3f-3a72-446e-a06a-2d336e8c6efe","","","Tees HDPE Class 12:",{"$nulls":4},"Dflt"]
["Rate Only","2931c2d7-e5af-4955-862f-c297d201ce32","B.2.3.5.10","","25 mm x 25 mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","39b83e27-03f0-4271-a13f-e251dc8ca744","B.2.3.5.11","","40 mm x 40 mm","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G261 * H261,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f96ad958-f078-4901-854e-96fef3edec9b","B.2.3.5.12","","75 mm x 75 mm","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","c35a17f1-6847-44ad-948c-65d46b1744ef","","","Reducers HDPE Class 12:",{"$nulls":4},"Dflt"]
["Rate Only","72ac0aeb-1a84-4c35-8a47-8dd02c62d050","B.2.3.5.13","","25 mm x 22 mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","de133112-9794-46c1-861e-5f29d9aac625","B.2.3.5.14","","40 mm x 22 mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","bbeec694-7dcc-4511-a6b9-736733ef7cc5","B.2.3.5.15","","40 mm x 25 mm","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G266 * H266,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","afca5a20-cc39-458a-98e4-ed6371947e66","B.2.3.5.16","","75 mm x 25 mm","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9e33ab2b-b054-4e42-86d4-ec5ae26db4f0","B.2.3.5.17","","75 mm x 40 mm","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","96f18112-759e-4b22-9b5b-174b23a9096e","B.2.3.6","SANS 1200L","VALVES",{"$nulls":4},"Dflt"]
["Label","96288b22-0708-4664-ac98-36d4fc805ca4","","8.2.3\n","Supply, in valve box, joint, incl. cut pipes where necessary, test, RSV gate valve left hand closing, non-rising spindle, with cap top",{"$nulls":4},"Dflt"]
["Label","19ca297c-0cf2-4abd-9b81-3e77926e34d3","","","Plain-ended valves including  two steel to HDPE couplings per valve:",{"$nulls":4},"Dflt"]
["Item","72431c4a-4233-46f5-9e21-57d184110848","B.2.3.6.1","","25 mm NB","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G272 * H272,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6512d3d4-4039-4e25-b4ec-cffe005f639c","B.2.3.6.2","","40 mm NB","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2a20a4d5-cf7e-447f-bf0f-a09b1d54b636","B.2.3.6.3","","75 mm NB","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","d8811b84-db98-4291-856d-66c985b49002","B.2.3.7","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","df5c059b-4cf9-4478-8790-3845ae5b4572","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional):",{"$nulls":4},"Dflt"]
["Item","5854ef34-cfbd-46a1-b4b8-e37fcc7bd46d","B.2.3.7.1","8.2.2.3(a)","Selected granular material (cradle)","m³",43,{"v":0,"d":"0.00"},{"$f":"ROUND(G277 * H277,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","d404fa96-6c77-451a-9c3b-3452c381040c","B.2.3.7.2","8.2.2.3(b)","Selected fill material (blanket)","m³",113,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","711f44fd-3e11-47d8-97d8-682fb820da36","B.2.3.7.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",1.3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f1bab008-1ec7-4d7f-9609-eb641cf86d16","B.2.3.7.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","8f024956-32ab-4cb3-859c-1dc7d4af7a0f","B.2.3.8","","ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","5a21aeae-7780-484a-b9ca-9dd159b0a0ad","","SANS 1200L\n8.2.11","Anchor/Thrust blocks and pedestals:",{"$nulls":4},"Dflt"]
["Item","1ef078bd-f2b6-43b1-92b3-84326d94d6b9","B.2.3.8.1","","Strength Concrete: 15 Mpa/19 mm ","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G283 * H283,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9fe95216-2ba3-47c1-b90e-293fb0e303a1","B.2.3.8.2","","Formwork: rough, vertical plane","m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ec4ab196-ef47-4061-bbc4-f8f0d7aef27e","B.2.3.8.3","SANS 1200LD 8.2.9\nPSL 8.2.19","Pipeline marker posts","No",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1ea0f6e1-e3c2-45ef-91eb-0a9e6acc9457","","SANS 1200LB","Encasing of pipes:",{"$nulls":4},"Dflt"]
["Item","25dde4e0-5988-4c73-ae88-acc54ad63322","B.2.3.8.4","8.2.4\nPSLB 8.2.4","Strength Concrete: 15 MPa/19 mm","m³",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G287 * H287,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","ac30a96e-3765-4a42-aab5-1a4f9da63d77","B.2.3.9","SANS 1200D","EXISTING SERVICES",{"$nulls":4},"Dflt"]
["Label","91868c3e-6a76-4aa7-a6c2-8742f971b2a1","","","Services across and in trenches:",{"$nulls":4},"Dflt"]
["Item","306ec300-f51d-4159-a59d-72fe7d43a961","B.2.3.9.1","8.3.8.1(c)","Excavate by hand in soft material to expose existing services","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G290 * H290,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2d1940db-1459-4f87-897c-60a0d27dc262","","SANS 1200DB 8.3.5(a)PSDB 8.3.5","Services that intersect a trench:",{"$nulls":4},"Dflt"]
["Item","0760bc13-280a-458d-abac-f754daa38938","B.2.3.9.2","","Cables","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G292 * H292,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6d725d1f-9ee3-40df-a223-efd03ca08310","B.2.3.9.3","","Sewer mains up to 400 mm diam.","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1d02eec0-7165-4567-b181-ec4099ac2984","","SANS 1200DB 8.3.5(b)\nPSDB 8.3.5","Services that adjoin a trench:",{"$nulls":4},"Dflt"]
["Item","f462974d-745a-4607-8851-509b014ed89b","B.2.3.9.4","","Cables","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G295 * H295,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","d29bcc03-cd65-4973-bc97-850df23948ac","B.2.3.10","","SUNDRIES",{"$nulls":4},"Dflt"]
["Item","ac9d4a9d-29d6-4035-b1ad-7ed2911ac989","B.2.3.10.1","PSL 8.2.18","Supply and install Stand Pipe complete as per Dwg. No. J40073/010-104","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G297 * H297,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","47b840cc-f67b-4719-b78c-d2e1f3ff56c2","B.2.3.10.2","PSL 8.2.17","Connect to existing watermain up to 40mm dia HDPE including excavation, backfilling, supply and install all specials and fittings etc. inclusive all work to complete connection.","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6ece1138-93d9-43de-b4e7-0b05860d6989","B.2.3.10.3","PSL 8.2.17","Connect to existing watermain up to 100mm dia AC including excavation, backfilling, supply and install all specials and fittings etc. inclusive all work to complete connection.","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Section","40ceb9b6-221b-43c7-92b2-bbe678951fb2","B.2.4","SANS 1200LD","SEWER RETICULATION (BUILDINGS)",{"$nulls":4},"Dflt"]
["Label","a3561449-25ef-48a2-976d-d461097f7e25","","SANS 1200LD","SECTION B.2.4 : SEWER RETICULATION (BUILDINGS)",{"$nulls":4},"Dflt"]
["Header3","77753344-8283-43f8-932e-b7df67ffc6f4","B.2.4.1","SANS 1200DB\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","cff12cd7-aab6-4c94-87f7-a751ca01ef28","B.2.4.1.1","8.3.1(a)","Clear vegetation and trees of girth up to 1 m","m",195,{"v":0,"d":"0.00"},{"$f":"ROUND(G303 * H303,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e3abdf3f-a960-458b-ac85-9d4518616c0e","B.2.4.1.2","8.3.1(c)","Remove topsoil to depth of 150mm","m²",145,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5e3db909-7943-401b-a063-ef5f049770ac","B.2.4.1.3","SANS 1200C 8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","84f393a5-db85-49a7-b694-f664cdbe4e2a","B.2.4.2","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Label","ba16210d-aaa7-4fc0-adbb-558a7f863cc1","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","aedc8466-e75b-46bc-a44a-686082427d38","","","Up to 110 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","06eea380-e023-4539-a5d1-3941c5943f78","B.2.4.2.1","","0,0 m                       1,0 m","m",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G309 * H309,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a73c5a74-9e67-4c99-ae67-46adea1597c7","B.2.4.2.2","","1,0 m                       2,0 m","m",35,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","5503ed83-26a4-45bc-946c-b7726df88ae8","B.2.4.2.3","","2,0 m                       3,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","7bea59f5-803e-4524-9f93-3c37750d3205","","","Over 110 up to 300 mm diam. for total trench depth:\nExceeding but not Exceeding",{"$nulls":4},"Dflt"]
["Item","13e3a2e9-2d16-4866-8a51-e4c42e0135f6","B.2.4.2.4","","0,0 m                       1,0 m","m",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G313 * H313,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b24c6aea-9856-4d98-816a-87772052ad41","B.2.4.2.5","","1,0 m                       2,0 m","m",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1e0251a2-5447-424d-94ae-dd0a32da96bc","B.2.4.2.6","","2,0 m                       3,0 m","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","04011983-cbc6-4f5f-8182-a5ea6215b48d","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.2.4.2.1 to B.2.4.2.6 incl. for (Provisional):",{"$nulls":4},"Dflt"]
["Item","2118a8b6-49e0-463a-9a7b-1aebb843504e","B.2.4.2.7","8.3.2(b)\nPSD 8.3.2(b)","Hard rock excavation","m³",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G317 * H317,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a238aadf-0b27-4968-a079-8d656a89ad74","B.2.4.2.8","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","5fcd02ec-b9b8-4a6e-a10d-7529ed563499","B.2.4.3","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","08790bc1-b748-4e63-8c2a-89be2b065b12","","8.3.3.1","Make up deficiency in backfill material (Provisional):",{"$nulls":4},"Dflt"]
["Item","542ff9d2-8d5e-4005-9934-ffc5ecb374bf","B.2.4.3.1","8.3.3.1(a)","from other necessary excavations on site","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G321 * H321,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a64f4c27-3ff8-4dfd-b267-cdc041e392ae","B.2.4.3.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","1ad05ba2-4c6b-44cd-93b9-c8e8fbdb80dc","B.2.4.4","SANS 1200DB","PARTICULAR ITEMS",{"$nulls":4},"Dflt"]
["Label","84d687ef-c395-40af-a67b-31f1169f355e","","8.3.4(a)\nPSD 8.3.15","Shore trench opposite structure or service or in unsuitable excavated materials for depths:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","420d5242-6231-48ab-bfc1-fd1e146d7d60","B.2.4.4.1","","1,0 m                        2,0 m","m",105,{"v":0,"d":"0.00"},{"$f":"ROUND(G325 * H325,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1ffef106-7a93-40f8-886d-44746e8608e3","B.2.4.4.2","","2,0 m                        3,0 m","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","052124fd-1999-4445-a9bd-0610c0a56fef","B.2.4.5","SANS 1200LD","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","fcc8b399-d310-46f1-a04b-59074d27d931","","8.2.1\nPSL 8.2.1","Supply, lay, complete with spigot and socket joint to suit PVC pipe, bed and test PVC sewer pipes with couplings:",{"$nulls":4},"Dflt"]
["Item","056ea558-5897-47ba-8fbb-7a14938016d5","B.2.4.5.1","","110mm diameter class 34","m",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G329 * H329,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","951807d3-c790-4f23-b1f3-b60422794749","B.2.4.5.2","","160mm diameter class 34","m",145,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","f250a11e-4d1e-4b28-ac05-03cf57ead1a4","B.2.4.6","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","9a8cdf86-c5c0-41af-ba60-6f5301c39d1b","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional):",{"$nulls":4},"Dflt"]
["Item","6906bd8b-f72a-4092-ae67-9e666c3df6e0","B.2.4.6.1","8.2.2.3(a)","Selected granular material (cradle)","m³",55,{"v":0,"d":"0.00"},{"$f":"ROUND(G333 * H333,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0f93ee36-8dc2-488a-90be-12e7de6f8005","B.2.4.6.2","8.2.2.3(b)","Selected fill material (blanket)","m³",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1fbcd637-abe4-4105-bd3b-89841ef37c62","B.2.4.6.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","55a844a1-614c-4cdd-8cd3-bc50e82ce8e5","B.2.4.6.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",55,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","e41b978a-3f9e-49e9-869e-548b9aba77ff","B.2.4.7","SANS 1200LD","MANHOLES, ETC.",{"$nulls":4},"Dflt"]
["Label","0bd9d19f-02f2-4a39-b752-98bafd48adb3","","8.2.3\nPSLD 8.2.3","Precast concrete manholes, with Type 1A Heavy Duty polyprop lockable manhole covers and frames, as per Dwg. No. J40073/010-102/0:\nover   and   up to",{"$nulls":4},"Dflt"]
["Item","22637e11-f26d-46de-b0f6-ae96120b75f5","B.2.4.7.1","","0,0 m          1,0 m","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G339 * H339,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","31f0c22a-ed0d-4973-b242-2c00f0eb5e81","B.2.4.7.2","","1,0 m          2,0 m","No",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","97438841-8b25-406f-948f-57c4e6aabf66","B.2.4.7.3","","2,0 m          3,0 m","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","e86a5210-5512-4efe-a56a-1f2af9c318b5","B.2.4.7.4","","3,0 m          4,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header3","a3eebc05-c129-42b1-a577-a1529c494469","B.2.4.8","","EXISTING SERVICES",{"$nulls":4},"Dflt"]
["Label","f69716bb-1566-4c6d-8a6e-bd6d03659390","","SANS 1200D","Services across and in trenches:",{"$nulls":4},"Dflt"]
["Item","935ab9be-50be-4ce8-a2bf-d7d91562f931","B.2.4.8.1","8.3.8.1(c)","Excavate by hand in soft material to expose existing services","m³",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G345 * H345,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","a492de38-8532-4927-819a-93d343701bf1","","SANS 1200DB\n8.3.5(a)\nPSDB 8.3.5","Services that intersect a trench:",{"$nulls":4},"Dflt"]
["Item","cc73a87f-ef9f-4ef2-8fe1-3c7c1f5331ba","B.2.4.8.2","","Cables","No.",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G347 * H347,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","159d2ef7-0f7c-4666-aa63-8c311495198c","B.2.4.8.3","","Water mains up to 400 mm diam.","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","92aae159-d1c6-4ca5-b7c4-e71061d9f72d","","SANS 1200DB\n8.3.5(b)\nPSDB 8.3.5","Services that adjoin a trench:",{"$nulls":4},"Dflt"]
["Item","82df56cf-b245-41df-9882-823629d38a93","B.2.4.8.4","","Cables","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G350 * H350,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","7ad11ca8-4a8b-4480-8bcf-13ab53704c34","B.2.4.9","SANS 1200LD","SUNDRIES",{"$nulls":4},"Dflt"]
["Sum","5feef3ff-f306-4c67-b692-c8a8ef3dd279","B.2.4.9.1","8.2.11\nPSLD 8.2.11","Break into and connect to existing raw water pump station including excavation, backfilling and all necessary specials and fittings etc. complete as indicated on Dwg. No. J40073/010-203","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H352,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Section","b63f5a4d-78cc-4dcd-95fd-3cae3f37f92e","B.2.5","","SEWERS (SUB-SURFACE DRAINS)",{"$nulls":4},"Dflt"]
["Label","d0d7c8b4-8880-4ab7-a157-0561692320e1","","","SECTION B.2.5 : SEWERS (SUB-SURFACE DRAINS)",{"$nulls":4},"Dflt"]
["Header3","c6832d53-e1ac-4c44-88e9-f8850dbf6983","B.2.5.1","SANS 1200DB\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","15943b5f-0563-47cb-b398-a92e8bb23de1","B.2.5.1.1","8.3.1(a)","Clear vegetation and trees of girth up to 1 m","m",105,{"v":0,"d":"0.00"},{"$f":"ROUND(G356 * H356,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","425c1262-b1c2-44b5-9637-d8eb7ac1a247","B.2.5.1.2","8.3.1(c)","Remove topsoil to depth of 150mm","m²",75,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ce1f04f5-b3cd-4be4-a28a-5386459d1b00","B.2.5.1.3","SANS 1200C 8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","4402bcca-5b2d-47d1-ab8d-515576f38692","B.2.5.2","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Label","da410444-7aec-43f8-9d09-7d4c254ebbc4","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","9611ca27-1b7d-45ea-9900-8cbbf00f5113","","","over 100 mm up to 200 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","17f14a61-eb34-4150-90a4-78428b12dfda","B.2.5.2.1","","0,0 m                       1,0 m","m",40,{"v":0,"d":"0.00"},{"$f":"ROUND(G362 * H362,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","c13db7a5-aacd-44f4-82be-b06ef05296ab","B.2.5.2.2","","1,0 m                       2,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","177c1a94-8d0b-46a2-8b96-07bbecdcc36d","B.2.5.2.3","","2,0 m                       3,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","067d09b5-9802-4cb2-b4ca-6ed81cfb6a80","B.2.5.2.4","","3,0 m                       4,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","62eb75d6-959b-4c01-b4e2-bd2664a05027","B.2.5.2.5","","4,0 m                       5,0 m","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G366 * H366,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7853ed82-a9f9-4026-b896-b8113cd01411","B.2.5.2.6","","5,0 m                       6,0 m","m",85,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","94bb09e4-2b6d-40ae-8e85-234c051a8fad","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.2.5.2.1 to B.2.5.2.6 incl. for (Provisional):",{"$nulls":4},"Dflt"]
["Item","bbbe6c4e-8de5-474c-a8c4-4f4774ebfb7d","B.2.5.2.7","8.3.2(b)\nPSD 8.3.2(b)","Hard rock excavation","m³",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G369 * H369,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2507fa69-1b85-4110-a155-079b4d2a858a","B.2.5.2.8","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","5cb78312-59eb-413d-9ed2-040009814539","B.2.5.3","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","c766b3ad-0b72-4aa3-93ea-63bcc838c119","","8.3.3.1","Make up deficiency in backfill material (Provisional):",{"$nulls":4},"Dflt"]
["Item","398856e9-0765-4f46-b6e3-8f65c8b1d315","B.2.5.3.1","8.3.3.1(a)","from other necessary excavations on site","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G373 * H373,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a8113654-9495-4630-880c-01afc3112757","B.2.5.3.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","69844166-8ee3-40fc-b289-641e214b11e7","B.2.5.4","SANS 1200DB","PARTICULAR ITEMS",{"$nulls":4},"Dflt"]
["Label","7aace651-41da-4b2b-bb3d-e6dcfcaed368","","8.3.4(a)\nPSD 8.3.15","Shore trench opposite structure or service or in unsuitable excavated materials for depths:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Rate Only","c280faa9-c2c4-4f89-bc29-903cb94c6cec","B.2.5.4.1","","1,0 m                        2,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","659d40bf-e0b6-467f-8718-6961d559bd7c","B.2.5.4.2","","2,0 m                        3,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","a257a042-5b29-4db3-a9c8-c633cd7865b4","B.2.5.4.3","","3,0 m                        4,0 m","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","1946fa2d-8b1c-4ced-b410-a9eb6420f93b","B.2.5.4.4","","4,0 m                        5,0 m","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G380 * H380,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a391d144-8dfb-460b-9a35-524bb5a050a9","B.2.5.4.5","","5,0 m                        6,0 m","m",85,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","f6dc2408-6429-45f8-8558-a61c03a756d0","B.2.5.5","SANS 1200LD","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","53c52088-468c-49fb-af80-360f7ff2326e","","8.2.1","Supply, handle, lay and bed SABS 791 class 51 normal duty uPVC pipes for sub-surface drains complete with socketed rubber ring-coupled joints:",{"$nulls":4},"Dflt"]
["Item","01eb08ad-d285-4f23-aec8-d16bce0ecea1","B.2.5.5.1","","110 mm internal diameter, unperforated","m",105,{"v":0,"d":"0.00"},{"$f":"ROUND(G384 * H384,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a4f9a357-0aff-45e8-aacc-1c32f6c3f03d","B.2.5.5.2","","110 mm internal diameter, perforated","m",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","fc745de4-c034-495c-a644-8ad8bb47f7de","B.2.5.6","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","bb94595e-f40c-47a0-b0e0-0134c5b826a5","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional):",{"$nulls":4},"Dflt"]
["Item","fa722a72-53ea-4c2a-8bdd-a8a52f7f3ccc","B.2.5.6.1","8.2.2.3(a)","Selected granular material (cradle)","m³",26,{"v":0,"d":"0.00"},{"$f":"ROUND(G388 * H388,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","82eff867-398f-41c6-87ed-d819c20b005e","B.2.5.6.2","8.2.2.3(b)","Selected fill material (blanket)","m³",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","727bef62-63b4-4f43-9d2d-37396983381c","B.2.5.6.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4b863485-3da0-4b60-b0fc-5faf1e340dec","B.2.5.6.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",165,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","948fc341-cfb6-4801-b254-d2e65e32148e","B.2.5.7","SANS 1200LD","MANHOLES, ETC.",{"$nulls":4},"Dflt"]
["Label","43a97e47-8916-4e7f-bd43-2f16aab3ab94","","8.2.3\nPSLD 8.2.3","Precast concrete manholes, with Type 1A Heavy Duty polyprop lockable manhole covers and frames, as per Dwg. No. J40073/010-102/0:\nover   and   up to",{"$nulls":4},"Dflt"]
["Rate Only","018e56d6-d965-454c-a202-a4657a2b814c","B.2.5.7.1","","0,0 m          1,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","ee7a31cc-6f3e-4af9-9778-c412469b48bf","B.2.5.7.2","","1,0 m          2,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","6b91d2f1-9af2-4aed-b690-ea3ccf14a6c3","B.2.5.7.3","","2,0 m          3,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","3890e2f0-41d8-491c-8dbd-95e5c30e81f3","B.2.5.7.4","","3,0 m          4,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","6d02852c-eed7-4010-bd2b-b0b405823e23","B.2.5.7.5","","4,0 m          5,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","e86764ab-45d8-4721-85c6-7bee3ca15245","B.2.5.7.6","","5,0 m          6,0 m","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G399 * H399,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","212b6726-2abd-4f86-a243-715867b6bb7c","B.2.5.7.7","","7,0 m          8,0 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header3","b3df5d2c-0c65-45eb-a38f-2baf255e7a88","B.2.5.8","","EXISTING SERVICES",{"$nulls":4},"Dflt"]
["Label","17019fe1-c37c-42dc-a762-d3072f4725e2","","SANS 1200D","Services across and in trenches:",{"$nulls":4},"Dflt"]
["Item","08e91f0a-3b38-4f48-8193-6b45675a2606","B.2.5.8.1","8.3.8.1(c)","Excavate by hand in soft material to expose existing services","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G403 * H403,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","10aa4f56-0898-420b-81cf-e01651707a10","","","Dealing with services:",{"$nulls":4},"Dflt"]
["Sum","ff3a4413-6079-402b-b593-845d1bdabb51","B.2.5.8.2","8.3.8.2(b)","Permanent protection of Existing service (Provisional)","Prov.Sum",1,{"v":10000,"d":"10,000.00"},{"$f":"ROUND(H405,2)","v":{"v":10000,"d":"10,000.00"}},"Dflt"]
["Sum","cce22814-ceaf-4f68-adb6-3421449a235b","B.2.5.8.3","8.3.8.2(c)","Temporary protection of Existing service (Provisional)","Prov.Sum",1,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"},"Dflt"]
["Label","671cf36d-bafc-40e2-95e6-e52f63d055ec","","SANS 1200DB 8.3.5(a)\nPSDB 8.3.5","Services that intersect a trench:",{"$nulls":4},"Dflt"]
["Item","99535f59-88fb-4173-b054-1ae6d97a9747","B.2.5.8.4","","Cables","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G408 * H408,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f26c1d77-3708-4f90-aba4-94bc7f74d9ab","B.2.5.8.5","","Sewer Rising mains up to 400 mm diam.","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5c2e3d15-76b2-40d7-ab5a-b2349501377c","B.2.5.8.6","","Sewer Rising mains over 400 mm diam.","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","9ea82293-9e04-4bc9-931c-7e08ec25ee81","","SANS 1200 DB 8.3.5(b)\nPSDB 8.3.5","Services that adjoin a trench:",{"$nulls":4},"Dflt"]
["Item","db90aa7c-0062-4adf-8f1f-1958259762ab","B.2.5.8.7","","Cables","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G412 * H412,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","9e1b513c-5df6-4d58-95d6-9a133ca02a76","B.2.5.9","SANS 1200LD","SUNDRIES",{"$nulls":4},"Dflt"]
["Sum","614ac5a8-6cfa-439a-9a69-78045dc19076","B.2.5.9.1","8.2.11\nPSLD 8.2.11","Break into and connect to existing manhole (2 No), Scum Manhole No. 1 including flexible joints as per Typical Dwg. No. J40073/010-102 and make good all benching, inclusive all work to complete connection.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H414,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Section","6051ce4e-8761-4f96-bcaf-f96c181353b3","B.2.6","SANS 1200LD","SEWERS (IRRIGATION PUMP STATION OVER FLOW PIPEWORK)",{"$nulls":4},"Dflt"]
["Label","536cc78a-eec3-4c24-98d1-145bf4a2c719","","SANS 1200LD","SECTION B.2.6 : SEWERS (IRRIGATION PUMP STATION OVER FLOW PIPEWORK)",{"$nulls":4},"Dflt"]
["Header3","1d0cf55b-bd63-4686-9bf6-8ad2a59150d5","B.2.6.1","SANS 1200DB\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","5ee07471-15a2-4c7f-ac19-4fa1a26ed5ef","B.2.6.1.1","8.3.1(a)","Clear vegetation and trees of girth up to 1 m","m",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G418 * H418,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","033e1737-bd06-431c-a406-3f3af0f511f4","B.2.6.1.2","8.3.1(c)","Remove topsoil to depth of 150mm","m²",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b8e9e71a-8576-42d3-ae37-71ba9bf47955","B.2.6.1.3","SANS 1200C 8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","b181e19d-2bf9-4fcd-a80b-eab181c943b3","B.2.6.2","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Label","85089e1c-9ede-40b6-a12b-30eaad986476","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill, compact, and dispose of surplus material, for pipes:",{"$nulls":4},"Dflt"]
["Label","7201237c-31e1-4c32-94b9-4f545e95cc9d","","","over 100 mm up to 200 mm diam. for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","5c29e992-13d5-48f2-93e2-9833300b8f20","B.2.6.2.1","","0,0 m                       1,0 m","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G424 * H424,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7cb30fc3-87de-4d05-b752-ca4bb3f5fb90","B.2.6.2.2","","1,0 m                       2,0 m","m",60,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","85448e0e-dc08-4af1-af67-eb83b9b5bf51","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.2.6.2.1 to B.2.6.2.2 incl. for (Provisional):",{"$nulls":4},"Dflt"]
["Item","4a341035-2d6c-4516-9d8e-1083865eb421","B.2.6.2.3","8.3.2(b)\nPSD 8.3.2(b)","Hard rock excavation","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G427 * H427,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e7c87809-ab88-4092-b4aa-b7a006012852","B.2.6.2.4","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","053a0fad-4200-4cc2-83ba-3fc9018e7bba","B.2.6.3","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","469e6fe2-e274-4417-a447-a5c95bbc37a0","","8.3.3.1","Make up deficiency in backfill material (Provisional):",{"$nulls":4},"Dflt"]
["Item","d52fb626-73e3-4860-ba0d-f78ff0b1bf27","B.2.6.3.1","8.3.3.1(a)","from other necessary excavations on site","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G431 * H431,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","cf6da364-d094-4957-bdfa-69d9c1b77f81","B.2.6.3.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","17015d81-4029-464e-8fb3-15a8325d34bb","B.2.6.4","SANS 1200LD","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","e72b96c0-42b7-48b1-ad59-0c30de64690d","","8.2.1","Supply, lay, complete with spigot and socket joint to suit PVC pipe, bed and test PVC sewer pipes with couplings:",{"$nulls":4},"Dflt"]
["Item","084010fd-b8d3-4806-a054-f37e7289bff4","B.2.6.4.1","","160mm diameter class 34","m",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G435 * H435,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","9338b8b5-7bd6-4dcb-b56d-1d476452402a","B.2.6.4.2","","200mm diameter class 34","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header3","8fceee20-e4c2-49fa-b3b1-aeb7330842bd","B.2.6.5","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","5daa6c6b-92cd-4dd8-b230-e9f853c3479b","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional):",{"$nulls":4},"Dflt"]
["Item","6ea5c82f-9f54-4fc3-a348-5fcfb5ed8f99","B.2.6.5.1","8.2.2.3(a)","Selected granular material (cradle)","m³",18,{"v":0,"d":"0.00"},{"$f":"ROUND(G439 * H439,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ac7b63a0-85f0-44c9-a836-64a17db98dd1","B.2.6.5.2","8.2.2.3(b)","Selected fill material (blanket)","m³",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0e3acf21-e5e0-4fc1-9f09-4ef6296b2dfe","B.2.6.5.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9cc367ae-756d-478c-bbb6-4c767b72169e","B.2.6.5.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","7aac1a56-1070-428b-bac6-a14bd7a631a5","B.2.6.6","","ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","22695043-85e0-410e-928e-e98b34788f9a","","SANS 1200L\n8.2.11","Anchor/Thrust blocks and pedestals:"]
["Item","76617e67-3e70-45e8-b7f7-89e258b9e29a","B.2.6.6.1","","Strength Concrete: 15 Mpa/19 mm ","m³",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G445 * H445,2)","v":{"v":0,"d":"0.00"}}]
["Item","0e7442ab-2cf6-4960-b568-9c2a21915fc1","B.2.6.6.2","","Formwork: rough, vertical plane","m²",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","8fc40870-c966-4269-a916-161be6a75547","B.2.6.6.3","SANS 1200LD 8.2.9\nPSL 8.2.19","Pipeline marker posts","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Header3","9e8a6382-0bdb-4d52-a361-8ad4cf345346","B.2.6.7","","SUNDRIES"]
["Item","40272c03-ac12-4d26-9256-63572169b8e3","B.2.6.7.1","PSLE 8.2.4\nPSLE 8.2.14","Construct outlet structure complete as per Dwg. No. J40073/010-111","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G449 * H449,2)","v":{"v":0,"d":"0.00"}}]

{"sheet":"BILL B.3.","index":3,"n_rows":205,"n_cols":10,"rows_kept":205,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.3.",null,"HEAD OF WORKS",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","e0d41a26-dc3f-4381-952e-ac715f0f603e","B.3.1","","HEAD OF WORKS",{"$nulls":4},"Dflt"]
["Label","f8fcb650-6783-40cc-b07b-14d5c549436e","","","SECTION B.3.1 : HEAD OF WORKS",{"$nulls":4},"Dflt"]
["Header2","34842afa-17a9-43dd-8b6d-e39446d04919","B.3.1.1","SANS 1200C\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","6edc5e14-191b-4f3b-9e48-6147a1eb1ab3","B.3.1.1.1","8.2.4","Reclear surfaces (provisional) (where ordered byEngineer)","m²",1200,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","28a9d824-81fb-44ce-92e2-86133bc5b7fd","B.3.1.1.2","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",320,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","83bc95d1-62bb-4009-b544-6d69d4daba3b","B.3.1.2","SANS 1200D\n8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Item","7a89dbd3-a03f-41df-a768-dd179b666505","B.3.1.2.1","8.3.1.2\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",1.5,{"v":0,"d":"0.00"},{"$f":"ROUND(G15 * H15,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","d0ce64b3-7ecc-442b-9120-53059dbef693","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Item","88527ea8-a50f-4df7-94c1-cd1c7fca19e5","B.3.1.2.2","","Head of Works","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G17 * H17,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","74c362cc-6c53-4e85-8955-af7d16911538","","8.3.9","Extra-over for backfill to 95% MOD AASHTO behind structures for :",{"$nulls":4},"Dflt"]
["Item","e12be120-c0c0-4363-91cf-64a17e4f7af7","B.3.1.2.3","","Head of Works","m³",1360,{"v":0,"d":"0.00"},{"$f":"ROUND(G19 * H19,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","70720877-9640-485c-8abd-d784418cf5db","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","49127732-e106-45a9-8042-ac8aeee1efcb","B.3.1.2.4","","Head of Works","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Header2","d0054782-8c0d-44ab-8368-b4fba1655425","B.3.1.3","SANS 1200D\n8.3.4 / 8.3.9","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","e1f59dd9-571a-45be-8278-eb959ed56db0","B.3.1.3.1","","Extra-over item B.3.1.2.3 for importation of material to complete embankment for the head of Works from commercial sources where necessary: G7 material","m³",1360,{"v":0,"d":"0.00"},{"$f":"ROUND(G23 * H23,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","be255fb2-e14b-4d88-87ed-8039c9389fb8","","SANS 1200D 8.3.7","Additional lateral support  (Provisional) for ensuring the stability of the excavation",{"$nulls":4},"Dflt"]
["Item","115bf3c3-9624-44af-8522-1bc36ad30ac6","B.3.1.3.2","","Head of Works","m²",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G25 * H25,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","436bfeec-0149-4bd6-ad35-cc9241ba5ffd","B.3.1.4","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","b48d6195-63a7-412b-a664-dfb1e2974f93","B.3.1.4.1","8.3.10","Topsoiling","m²",1020,{"v":0,"d":"0.00"},{"$f":"ROUND(G27 * H27,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c2bfa711-cf18-4ebc-8c92-2e63ab7f8a56","B.3.1.4.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc. as necessary and wetting","m²",1020,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","f4ee65b6-2377-4cc5-9515-3a7c994971d4","B.3.1.5","SANS 1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","eb6b3480-75e6-4034-8ac5-7145f1848025","","8.4.2","Blinding layer:\n15 MPa/19 mm concrete:",{"$nulls":4},"Dflt"]
["Item","533ad9e2-77cc-40e7-9a74-c44a8e1c17ab","B.3.1.5.1","","50 mm minimum thickness (Channel and Retaining Wall)","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","248db2c3-ccde-4577-814e-e0aaa67f77ad","B.3.1.5.2","","50 mm minimum thickness\n(Ground Slab)","m²",186,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8db5a00e-723a-4c12-bafb-d86f82e8b387","B.3.1.5.3","","50 mm minimum thickness\n(Ground Slab Grit traps)","m²",65,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2e5d9275-7005-48b9-b8e3-c6d9c295c36a","B.3.1.5.4","","75 mm minimum thickness\n(Inlet)","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","372336f9-512b-4738-a4d2-e756cc2ee813","","8.4.3\nPSG 3.5.4","Strength concrete:\n20 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","99ddd0e8-c96e-43b6-a216-dbfadef8cdd3","B.3.1.5.5","","Benching including any necessary formwork or unformed surfaces to different slopes (In Grit Traps, Flume and Stilling Box)","m³",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G36 * H36,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","24f16752-68ae-4be9-972d-b5adfd787de4","","8.4.3\nPSG 3.5.4","Strength concrete (Inclusive of Crystalline Water Proofing additive):\n15 MPa/19 mm",{"$nulls":4},"Dflt"]
["Item","8a3a30c4-264c-436b-87dd-e5c233f84939","B.3.1.5.6","","Mass concrete fill in channel","m³",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G38 * H38,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8442845c-5ae2-41fe-998f-10292178d23f","","8.4.3\nPSG 3.5.4","Strength concrete (Inclusive of Crystalline Water Proofing additive):\n35 MPa/19 mm",{"$nulls":4},"Dflt"]
["Item","511791f4-b322-4361-854c-ef663c575e45","B.3.1.5.7","","Channel and Retaining Wall","m³",17,{"v":0,"d":"0.00"},{"$f":"ROUND(G40 * H40,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2e729fc7-f2c7-44a2-a9e0-3b24ed1e5f4f","B.3.1.5.8","","Ground Slab","m³",36,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","302bbc57-79e9-40b8-88e3-b407b4e79cc6","B.3.1.5.9","","Ground Slab (Grit Traps)","m³",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ca5501d8-0fdc-4311-aa12-9f5f6104375c","B.3.1.5.10","","Elevated Slab (Grit Traps)","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b1223075-cdce-4fbe-a581-5958e4ccac77","B.3.1.5.11","","Floor slab (Inlet)","m³",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8df023e1-dcaf-4d69-92a3-acfcbd2eb9aa","B.3.1.5.12","","Walls (Super structure)","m³",32,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7181c340-e733-46f8-96e3-8ffafbd33de7","B.3.1.5.13","","Flume","m³",14,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3d8f3c7d-1bca-439a-adb2-8fc34d4ce005","B.3.1.5.14","","Stairs","m³",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a7f28d0c-48c9-4dcd-8e8a-d3e99654be24","B.3.1.5.15","","Corner fillet 100mm x 100mm (Along walls)","m",660,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","78610450-ec9c-417f-b508-a80ce2423a70","B.3.1.5.16","","For Stilling Box (Slab)","m³",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","691852e6-e31a-4a10-b41c-054422702ce1","B.3.1.5.17","","For Stilling Box (Walls)","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","738a3ba0-4f62-45e7-8ce7-abc37c60171e","B.3.1.5.18","","For Stilling Box (Roof Slab)","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","a1bb2fd7-369c-4deb-ab9c-ed2c21f6f3ee","B.3.1.6","SANS 1200G\n8.1.1\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","fb9f61aa-1a48-4055-bd18-a7cde94955f3","","8.2.2","Smooth vertical plane to:",{"$nulls":4},"Dflt"]
["Item","a6c156ca-40bf-4d8d-b3d6-a57cdb2fe6e5","B.3.1.6.1","","Walls (Channel and Retaining)","m²",220,{"v":0,"d":"0.00"},{"$f":"ROUND(G54 * H54,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a25d01ce-c141-40c5-91db-bd0e7468ba6f","B.3.1.6.2","","Walls (Super structure)","m²",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b236806c-a092-4ba6-ab5b-aba3a1849c93","B.3.1.6.3","","Inside of the Parshall flumes to special tolerances","m²",28,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","73b95b49-dfec-4a02-a7d5-2e77e8cbb4db","B.3.1.6.4","","Stairs","m²",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","61f5c295-a615-4480-b23d-6192a8da30fa","","8.2.2","Smooth horizontal plane to:",{"$nulls":4},"Dflt"]
["Item","805e27f5-1139-4c9a-aa5e-89b6b749e12a","B.3.1.6.5","","Elevated slab soffit (Grit traps)","m²",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G59 * H59,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","838178a8-169d-4cc7-8ccd-4bfca59f3589","","8.2.5","Vertical narrow widths up to 300mm wide:",{"$nulls":4},"Dflt"]
["Item","b5397675-3103-457c-acd9-43692d3a72de","B.3.1.6.6","","Channel and Retaining Wall","m",95,{"v":0,"d":"0.00"},{"$f":"ROUND(G61 * H61,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","224a93ef-c10e-438e-80ea-77ef0f80a92f","B.3.1.6.7","","Ground Slab","m",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ab39456e-a2a0-4f60-8e7a-ce64915c00d2","B.3.1.6.8","","Elevated Slab (Grit traps)","m",31,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","36a97cdf-465f-4f15-a69e-9ab6ec75d697","B.3.1.6.9","","Floor Slab (Inlet)","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","9d654573-2d89-4b57-b926-ec76a33b3be7","B.3.1.6.10","","Stair risers","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G65 * H65,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5e2fef08-a59b-4c40-b7a5-3ddd5b32dd06","","8.1.1.2\nPSG 8.1.1.8","Chamfers exceeding 20mm x 20mm and grooves:",{"$nulls":4},"Dflt"]
["Item","7c4c1e54-3e11-4a8d-af47-7b6cda1e18a0","B.3.1.6.11","","Chamfer 25mm x 25mm\n(Ground Slab)","m",39,{"v":0,"d":"0.00"},{"$f":"ROUND(G67 * H67,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b4b28d88-7560-4ff5-92fd-28f33f0fed64","","","Weepholes:",{"$nulls":4},"Dflt"]
["Item","65ce1c67-5d68-4293-ac69-f767aa6e8e2a","B.3.1.6.12","","75mm Weephole at 2m c/c with Bidim wrapped at one end","No",18,{"v":0,"d":"0.00"},{"$f":"ROUND(G69 * H69,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5439a6ee-7e19-4f31-a87c-2b36e56f07d0","","8.2.6","Box out holes/form voids",{"$nulls":4},"Dflt"]
["Label","8a0ba9ea-c9cf-4508-afa3-3a25ee455588","","","Large, other than circular, of area over\n0.1m² and up and including to 0.5m² (de-gritter pump head plinth), up to 0,35 m diam.: depths\nover    and    up to",{"$nulls":4},"Dflt"]
["Item","71f472df-89e1-43a8-b684-64f13d31fd50","B.3.1.6.13","","0 m                0,5 m","No.",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G72 * H72,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cc460c8c-cea4-4465-a01d-aa6a2db36d2e","B.3.1.6.14","","Large, circular, of diameter over 0.7m up\nto and incl. 1.3m",{"$nulls":4},"Dflt"]
["Item","133ae67c-c04e-4132-a776-856b9391c333","B.3.1.6.15","","0 m                0,5 m","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G74 * H74,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5194e386-9743-4977-85c7-b52d86bebc37","","PSG 8.10","Cast pipe with puddle flanges into concrete for Pipes up to and including 1000mm NB through walls and slabs of thickness:\nover    and     up to",{"$nulls":4},"Dflt"]
["Rate Only","3634e1ed-237d-4ea1-9ca5-5909d13550d6","B.3.1.6.16","","0,0 m             0,25 m","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","be3ad879-e46f-4db7-9563-1dc1296e893d","B.3.1.6.17","","0,25 m           0,30 m","No.",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G77 * H77,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","62c41bc6-f9ce-4535-9f1b-70edc89d721c","B.3.1.6.18","","0,30 m           0,45 m","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","520f09fb-33ff-4636-a83f-169ce0e4d2ca","","","",{"$nulls":4},"Dflt"]
["Rate Only","5346ae0d-16cf-4cbe-b2c9-6cc95fe45bfc","B.3.1.6.19","","90mm deep x 250mm wide rebate for sluice gates","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header2","5621175a-42bb-47ff-86dd-aee8e02068e6","B.3.1.7","SANS 1200G\n8.1.2\nPSG 8.1.2","REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","6303864e-cead-4960-80ba-cfc7e764c8e4","","8.1.2.3(a)","Mild steel bars:",{"$nulls":4},"Dflt"]
["Item","70c8174e-e989-499c-b84a-61287e42329b","B.3.1.7.1","","25 mm diameter: Basic price","t",0.55,{"v":0,"d":"0.00"},{"$f":"ROUND(G83 * H83,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","823a8158-95d7-43a1-8bf6-def7f2c9587b","","8.1.2.3(b)","Extra-over item B.3.1.7.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","077c771c-5089-4b89-85f1-db995b03f029","B.3.1.7.2","","8 mm","t",0.4,{"v":0,"d":"0.00"},{"$f":"ROUND(G85 * H85,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","aa8cc6bf-f9b2-4181-b4a5-761c3dc43cd7","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","a309fbde-8317-4ba0-b77b-5dd682a013e7","B.3.1.7.3","","25 mm diameter: Basic price","t",7.35,{"v":0,"d":"0.00"},{"$f":"ROUND(G87 * H87,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","fb7b60ce-2993-40c9-ac91-2bc4cc3cbcf7","","8.1.2.3(b)","Extra-over item B.3.1.7.3 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","c287b98d-07c8-41c3-b943-3644a1b54fd5","B.3.1.7.4","","10 mm","t",1.4,{"v":0,"d":"0.00"},{"$f":"ROUND(G89 * H89,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","73c1a341-c081-4f36-874f-1f0dc1ac5f80","B.3.1.7.5","","12 mm","t",5.8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","a677a16f-0d6b-4e91-8bbb-60cb19ac17f3","","8.1.2.3(c)","High-tensile welded mesh reinforcement:",{"$nulls":4},"Dflt"]
["Item","59ad4f00-b23f-464f-b30e-3e2603f500d8","B.3.1.7.6","","High-tensile welded mesh ref 617","m²",245,{"v":0,"d":"0.00"},{"$f":"ROUND(G92 * H92,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","5c7d2ee4-0860-44a8-ba7e-83160a32a242","B.3.1.8","SANS 1200G\n8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","afce3a9d-c61a-420e-845a-ee4992e4a125","","PSG 8.4","Wood-floated finish",{"$nulls":4},"Dflt"]
["Item","bea4b799-19a4-4ddd-a7a9-cc21c7038902","B.3.1.8.1","","Top ground slab","m²",180,{"v":0,"d":"0.00"},{"$f":"ROUND(G95 * H95,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","47ec7141-fda5-4e5b-b979-fae935bf9f31","B.3.1.8.2","","Top ground slab (Grit Traps)","m²",60,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","27ce1d18-babd-4f03-b023-67ae368e70f3","B.3.1.8.3","","Top retaining wall footing","m²",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","df5386e4-3a1b-494e-9ce0-0279d7a39647","","8.1.1.5\nPSG 8.4","Steel-floated finish",{"$nulls":4},"Dflt"]
["Item","c10bfa63-7bc5-4e53-bd41-5d5fa3c6a115","B.3.1.8.4","","Benching (Grit Traps)","m²",41,{"v":0,"d":"0.00"},{"$f":"ROUND(G99 * H99,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","69a62b39-e78a-4775-98d9-7d2c18dd79da","B.3.1.8.5","","Top of Mass Concrete","m²",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","81225641-b610-47fc-81c2-8e73306648ca","B.3.1.8.6","","Top of Channel Floor","m²",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","e8dac9b9-41d1-49be-b92d-3bf8921f6e76","B.3.1.8.7","","Top of Floor Slab (Inlet)","m²",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G102 * H102,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6403ff91-c853-4539-987b-a2c4e2989ddf","B.3.1.8.8","","Top of Walls (Channel and Retain)","m²",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","567603fb-8f65-4588-b0b9-b0fd20770120","B.3.1.8.9","","Top of Walls (Super Structure)","m²",14,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","64d686f2-7604-46af-8927-327e92e65eb4","B.3.1.8.10","","Top of Flume Walls","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","df01611a-3a24-402b-88b7-2454bc75536d","B.3.1.8.11","","Top of flume bottoms to special finishing tolerances","m²",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e73782da-fd99-40eb-b763-5149d28667ec","B.3.1.8.12","","Corner chamfer 270mm x 270mm (Along walls)","m²",107,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","024ad2dc-2bec-4fa9-aa3a-f3d3ef143e80","","8.1.1.5\nPSG 8.4","Non-skid finish",{"$nulls":4},"Dflt"]
["Item","be760ccb-8f48-4516-8548-2ba304bbd2c5","B.3.1.8.13","","Top Elevated Slab (Grit Traps)","m²",16,{"v":0,"d":"0.00"},{"$f":"ROUND(G109 * H109,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","75acc669-5b42-4744-b61a-3f9cee43a274","B.3.1.8.14","","Concrete stairs","m²",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","76bf131f-b818-40b6-bda1-97fef271f108","B.3.1.8.15","","Conveyor Belt Slab","m²",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","609d52e2-3e22-4dd1-a32c-370686aa6027","B.3.1.8.16","","Stilling Box Roof Slab","m²",5.5,{"v":0,"d":"0.00"},{"$f":"ROUND(G112 * H112,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","8ba1c916-c0bf-49fe-81ad-62a3e0f948af","B.3.1.9","SANS 1200G\n8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Label","af117233-9929-4f95-91d6-bbae05d9e00a","","","Joints in floor slabs complete as shown on Dwg. No. J40073/010-201:",{"$nulls":4},"Dflt"]
["Item","5971cf9d-a286-4f58-be5f-45f606838ffb","B.3.1.9.1","","Jointex (Ground Slab)","m",28,{"v":0,"d":"0.00"},{"$f":"ROUND(G115 * H115,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","bc02858c-acaa-446c-bfa3-ea1c45d786ee","B.3.1.9.2","","Jointex (Ground Slab Between walls and ground slabs at Grit Traps)","m",95,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","63cb9bfd-b979-408f-a142-29ea4c431d4b","B.3.1.9.3","","Joints in the channel floors compete with PVC water stop, 12 mm joint filler and polyurethane sealant","m",22,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","b103ff89-129e-4eac-a877-c9dbd4e8c08a","","","Wall joints complete as shown on Dwg. No. J40073/010-201:",{"$nulls":4},"Dflt"]
["Item","fa7debbe-6b1e-4ccf-a9a7-f2d49d294628","B.3.1.9.4","","Joints in channel wall complete with PVC water stop, 12mm joint filler and polyurethane sealant both sides","m",29,{"v":0,"d":"0.00"},{"$f":"ROUND(G119 * H119,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","98691bae-b709-4a08-87af-43ac3bcf88c1","B.3.1.9.5","","Corner chamfer","m",560,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1b1ab6ca-5f69-4b39-b51d-5aca81f9eb4c","","","Contraction joints:",{"$nulls":4},"Dflt"]
["Item","989d95d2-e472-4724-8e90-79ac9f03d30b","B.3.1.9.6","","Vertical contraction joint in wall complete with waterproofing bandage, bond breaker cord, sealant, drilling for dowels, dowels, and epoxy to set dowels to Detail X of Dwg. No. J40073-010-230","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G122 * H122,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","8b539c5b-a70d-4bf2-bf16-f14a262978ac","B.3.1.10","SANS 1200G\n8.7","GROUTING ",{"$nulls":4},"Dflt"]
["Item","81af2e4f-38e4-4da9-a42b-938b5faf8497","B.3.1.10.1","","Grouting of grooves for channel gates","m³",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G124 * H124,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","b98794cb-7785-4672-80f3-d7a5fadc12bd","B.3.1.11","SANS 1200H and HA","STRUCTURAL STEELWORK",{"$nulls":4},"Dflt"]
["Header3","a89ca4ce-cb4c-4d28-bca6-a4b83cbbc037","B.3.1.11.1","1200H\n8.3.1, 8.3.2, 8.3.3, 8.3.4 and 8.3.5","HANDRAILS",{"$nulls":4},"Dflt"]
["Item","179ebe51-c78e-4960-bbc2-c489411abf74","B.3.1.11.1.1","8.3.7(b)","Supply and Assemble the handrails as per the Dwg. No. J40073/010-105. The rate shall cover the fabrication, corrosion protection and installation of galvanised steel handrails complete with all the necessary cleats, brackets,  gussets, packs, etc. complete as shown on Dwg. No. J40073/010-201","m",175,{"v":0,"d":"0.00"},{"$f":"ROUND(G127 * H127,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ebed051c-fb11-4511-937e-11ff5a323ba9","B.3.1.11.1.2","","Handrail at slope (stairs)","m",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","0b2b23da-2bf1-4736-a5c5-be0842d853e9","B.3.1.12","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","5b3c342b-1050-4cfb-9ce3-f9bb89e50253","","","Water Tightness Testing",{"$nulls":4},"Dflt"]
["Item","58680e51-7f60-40d9-b053-4326585e50b8","B.3.1.12.1","PSG 8.12","Testing for Water Tightness, all inclusive to PSG 7.2.5","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G131 * H131,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","70e50d70-0098-4e12-86e1-29a7c94eac46","B.3.1.12.2","","Break through existing inlet works wall, smooth and seal exposed concrete and reinforcing for rectangular void 1750mm x 1360mm dimension","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","09eb51f8-988d-4474-b62b-fa3df1f2d86c","","","Corrective work to Head of Works",{"$nulls":4},"Dflt"]
["Sum","797a3440-289c-4796-8993-fd57bae37589","B.3.1.12.3","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":1800000,"d":"1,800,000.00"},{"$f":"ROUND(H134,2)","v":{"v":1800000,"d":"1,800,000.00"}},"Dflt"]
["Header2","10ebfe10-dd54-4fca-a94a-309237f458f7","B.3.1.13","","MEDIUM PRESSURE PIPELINES",{"$nulls":4},"Dflt"]
["Header3","268bb012-0690-4b2a-b99f-79df893c3aed","B.3.1.13.1","SANS 1200C\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","1577e4f9-e04e-40c3-b4d1-e0dd9570ae42","B.3.1.13.1.1","8.2.1","Clear and grub Site","m²",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G137 * H137,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ebdccdc1-1216-42dc-9c2a-886d23e9be0c","B.3.1.13.1.2","8.2.10\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",100,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","ab5d50b5-215f-4bf5-93f8-720295debfc3","B.3.1.13.2","SANS 1200DB","EXCAVATION",{"$nulls":4},"Dflt"]
["Label","6d1e7697-37d8-4704-b78f-b15c3f5feeac","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2(b)","Excavate in all materials for trenches backfill, compact, and dispose of surplus material, for pipes: \nover 250 mm up to 450 mm in diameter for total trench depth:\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","0a9c8179-0943-41b9-ac8d-b31e6febf770","B.3.1.13.2.1","","0,0 m                       1,0 m","m",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G141 * H141,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","386306c8-c361-40d7-86e5-faef7ca452d7","B.3.1.13.2.2","","1,0 m                       2,0 m","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","527b9d59-de47-4b4f-a9ef-8ad611c1d0cf","B.3.1.13.2.3","","2,0 m                       3,0 m","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","90d05372-2c5e-483d-99de-66530f1cf157","","8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.3.1.13.2.1 to B.3.1.13.2.3 incl. for (Provisional):",{"$nulls":4},"Dflt"]
["Item","9c6cbd07-f500-4b4f-9bce-b2ce96e07631","B.3.1.13.2.4","8.3.2(b)","Hard rock excavation","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G145 * H145,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6b33593e-7cbc-445a-9b01-03e2577cd0ff","B.3.1.13.2.5","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","611a4212-25d2-483e-94e4-47bd06359914","B.3.1.13.3","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","78bc6374-a7da-4f90-9332-fccee2136fe7","","8.3.3.1","Make up deficiency in backfill material (Provisional)",{"$nulls":4},"Dflt"]
["Item","3c964315-84af-4b2c-8f2f-9d1abf02823b","B.3.1.13.3.1","8.3.3.1(a)","from other necessary excavations on site","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G149 * H149,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b9f83fa1-e803-4380-bc86-d5b25c086984","B.3.1.13.3.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","cecfb771-52b6-4bcc-95e5-6f9f85f2bbe5","B.3.1.13.4","SANS 1200DB","PARTICULAR ITEMS",{"$nulls":4},"Dflt"]
["Label","dd96ed36-e528-4a2d-815f-b25f237bccdb","","8.3.4(a)\nPSD 8.3.15","Shore trench opposite structure or service or in unsuitable excavated materials for depths (Provisional)\nExceeding but not exceeding",{"$nulls":4},"Dflt"]
["Item","d70edc1e-3c48-4ccc-ad00-91836a33c8dd","B.3.1.13.4.1","","1,0 m                        2,0 m","m",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G153 * H153,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f7e1ea85-2a7d-493f-993d-c6a3edfcfa57","B.3.1.13.4.2","","2,0 m                        3,0 m","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","1a4f9682-b8ed-4f9d-9c44-728b812d6905","B.3.1.13.5","SANS 1200L","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","ba80f562-03e5-4864-bc51-9ff4ebb096c2","","8.2.1\nPSL8.2.1","uPVC pipes Class 9: Supply, handle, lay and bed uPVC pipes complete with approved flexible coupling type to suit:",{"$nulls":4},"Dflt"]
["Item","d1e50c22-9fe7-4f73-bac4-d99b88962c98","B.3.1.13.5.1","","315 mm NB","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G157 * H157,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4c1330eb-8403-4a3b-94ba-5e6dc7a7d041","B.3.1.13.5.2","","400 mm NB (Mark 5 and 6)","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","8678a18f-a2fb-4cab-bbe9-45d2af09994e","","8.2.15\nPSL 8.2.15","Special wrapping in corrosive soil as per Project Specification PSL3.9.3.8 (Provisional)",{"$nulls":4},"Dflt"]
["Item","d4963145-a1dd-48ea-8cce-dd4d3b4764b7","B.3.1.13.5.3","","300 mm NB","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G160 * H160,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4a992e0b-323d-4a2f-baaf-8a7c4ff36d3b","B.3.1.13.5.4","","400 mm NB","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","b68e334f-18a9-4a64-b45c-355eaf5b8ecd","","8.2.1\nPSL 8.2.1","Steel pipes with lining & coating:\nSupply, handle, lay, and bed, complete with approved flexible coupling type joint to suit, test, and disinfect:",{"$nulls":4},"Dflt"]
["Item","5decc1a3-fd3a-4b79-9fec-ec56a2bfe355","B.3.1.13.5.5","","Stilling Box: Pipe Item 3: 800NB steel straight puddle pipes, flanged one end only, to SANS 1123 Table 1000/3. Puddle flange 150mm from plain end","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G163 * H163,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","ba6b28ca-ba57-4eaf-98d2-c54da5098381","","","Flange Adaptors Steel to HDPE:",{"$nulls":4},"Dflt"]
["Item","00e5fb7a-d19e-46a3-9ccc-4aff6005ebf2","B.3.1.13.5.6","","900NB HDPE to 800NB steel PN10","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G165 * H165,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","e1938293-d791-4fe9-bb73-56ddbd111c69","B.3.1.13.6","SANS 1200L","SPECIALS AND FITTINGS",{"$nulls":4},"Dflt"]
["Label","bb7e93c1-c2f6-4f31-9a1f-d574458399b5","","8.2.2","Extra over item B.3.1.13.5.1 for the supplying, laying and bedding of specials complete with approved spigot to socket type joint to suit uPVC pipe",{"$nulls":4},"Dflt"]
["Label","ce7e54cd-a5b0-413c-9c0c-0c5232af0d13","","","uPVC bends, of deflection:",{"$nulls":4},"Dflt"]
["Item","7518a38d-d1eb-4674-b7be-7ae985fd1d4e","B.3.1.13.6.1","","315 mm NB, 90 degrees","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G169 * H169,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c0d16755-549c-43e4-a175-c2b6f844d28d","B.3.1.13.6.2","","315 mm NB, 45 degrees","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f9f44342-a3e2-4a22-b348-6277e1bdd150","B.3.1.13.6.3","","315 mm NB, 22.5 degrees","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","ecb8d555-1f57-495e-b6bc-6602c4907aa4","","8.2.2","Extra over item B.3.1.13.5.1 and B.3.1.13.5.2 for the supplying, laying and bedding of steel pipe specials cast into concrete where necessary, complete with approved flexible couplings to suit uPVC pipe as per Dwg. No. J40073/010-201:",{"$nulls":4},"Dflt"]
["Item","b1addb5a-9980-441b-8f53-8ffc3dce76a3","B.3.1.13.6.4","","Item No. P14-B/1 - 300 mm NB","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G173 * H173,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","52c13219-1cc1-4741-bf20-ff10be6e2508","B.3.1.13.6.5","","Item No. P14-B/2 - 300 mm NB","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4926e1e0-a3b5-4503-a621-d46ad751b244","B.3.1.13.6.6","","Item No. P14-B/3 - 400 mm NB","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5b875108-d5e8-43b3-af12-042fc76b2824","B.3.1.13.6.7","","Item No. P14-B/4 - 400 mm NB","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","33198663-cb72-4ecb-90b1-0e9172e5d25f","","","Flange Adaptors Steel to uPVC:",{"$nulls":4},"Dflt"]
["Item","2f0b22f5-e6f9-4149-ae5b-2aa566461e41","B.3.1.13.6.8","","300 mm NB","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G178 * H178,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3d04f559-943b-4dd7-bfd8-10c1096867ca","B.3.1.13.6.9","","400 mm NB","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f63b31c6-2b60-4e44-840a-9a11ba97e726","","","Blank Flanges:",{"$nulls":4},"Dflt"]
["Item","62a9aa07-8098-4c27-99cd-831d09203961","B.3.1.13.6.10","","300 mm NB","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G181 * H181,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","652156cd-d1ca-4e00-9708-eb95c623b6cf","B.3.1.13.6.11","","400 mm NB","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","5772f6e2-2810-44c9-92e2-5fc91f86b406","B.3.1.13.7","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","c7fb8a38-70b5-494a-b425-1d27f3afae26","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional)",{"$nulls":4},"Dflt"]
["Item","05bf989d-6ced-45c9-b311-9e123e26388a","B.3.1.13.7.1","8.2.2.3(a)","Selected granular material (cradle)","m³",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G185 * H185,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","de4420e0-297f-496f-ad36-88297a9bfc99","B.3.1.13.7.2","8.2.2.3(b)","Selected fill material (blanket)","m³",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bade5f0a-7d8d-480b-bfdc-367eab3785d4","B.3.1.13.7.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2e66fca8-d46e-45e7-8187-5a36cbc53366","B.3.1.13.7.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","e3a86021-a4c6-47b6-8b88-f001513431cb","B.3.1.13.8","","ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","4aa8a136-f246-4f1c-9ccb-048764655d14","","SANS 1200L 8.2.11","Anchor/Thrust Blocks, Pedestals",{"$nulls":4},"Dflt"]
["Item","a2973b5c-b0be-4d30-8234-b7e2c8b6138e","B.3.1.13.8.1","","Strength Concrete: 15 Mpa/19 mm ","m³",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G191 * H191,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1846bf64-763b-4963-8b81-0f0287e8a57b","B.3.1.13.8.2","","Formwork: rough, vertical plane","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d3544ee0-cf51-42b7-bf08-b8374064772a","B.3.1.13.8.3","SANS 1200LD 8.2.9\nPSL 8.2.19","Pipeline marker posts","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","e1d5c46f-c2e9-406d-b1f9-ca4b1c7cfc39","B.3.1.13.9","SANS 1200LD","MANHOLES",{"$nulls":4},"Dflt"]
["Label","4f7a1178-3f97-4503-a3f5-72e55d101f3c","","8.2.3\nPSLD 8.2.3 PSG 3.5.4","Precast concrete manholes, with Type 1A Heavy Duty polyprop lockable manhole covers and frames, as per Dwg. No. J40073/010-102/0:\nover   and   up to",{"$nulls":4},"Dflt"]
["Item","29f4eb31-05ad-4f36-b7a6-819d8dd649ce","B.3.1.13.9.1","","0,0 m          1,0 m","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G196 * H196,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","cbcd0b4d-10a0-4099-bc54-833e982df725","B.3.1.13.9.2","","1,0 m          2,0 m","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3e0f8377-a5a0-405f-bdef-f68968d41425","B.3.1.13.9.3","","2,0 m          3,0 m","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","085d19ca-6848-4628-b9b4-06c7bc03aad1","B.3.1.13.9.4","","3,0 m          4,0 m","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","9f09656a-8f16-421e-8c55-df18d5279e0a","B.3.1.13.10","","EXISTING SERVICES"]
["Label","50dacdbb-48cd-4e05-889e-99bde72d891b","","SANS 1200DB\n8.3.5(a)\nPSDB 8.3.5","Services that intersect a trench"]
["Item","a52354b5-3cc7-4a43-aaa3-e5691be37fad","B.3.1.13.10.1","","Sewer Rising mains up to 400 mm dia.","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G202 * H202,2)","v":{"v":0,"d":"0.00"}}]
["Header3","1b4e50ed-d319-4528-bf21-06c6d9fa8afe","B.3.1.13.11","","SUNDRIES"]
["Item","d3e29351-2f35-468c-a4de-956790747372","B.3.1.13.11.1","PSL 8.2.17","Break into existing live 400mm dia AC pipeline, including connection, sewage handling, inclusive all work necessary to complete connection etc.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G204 * H204,2)","v":{"v":0,"d":"0.00"}}]
["Item","40bb9454-d005-4cac-8324-184df3c65368","B.3.1.13.11.2","PSL 8.2.17","Connect to existing live 300mm dia uPVC pipeline, inclusive all work to complete connection.","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]

{"sheet":"BILL B.4.","index":4,"n_rows":105,"n_cols":10,"rows_kept":105,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.4.",null,"BIOLOGICAL REACTOR",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","a16f73c4-e98b-42c3-b05e-7dbd44259934","B.4.1","","BIOLOGICAL REACTOR",{"$nulls":4},"Dflt"]
["Label","482ac830-6d12-4a1f-b461-61f6eeaee9af","","","SECTION B.4.1 : BIOLOGICAL REACTOR",{"$nulls":4},"Dflt"]
["Header2","e79c6f80-6c64-46f5-a315-cfd388f9ff5c","B.4.1.1","SANS\n1200C\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","4e34dc1e-3743-4dfa-b9d9-bce81d909113","B.4.1.1.1","8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",1500,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","965a1dfb-cd7a-4b37-a5ea-ce6861b70c78","B.4.1.1.2","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",240,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","f8ede2a4-a7a6-4731-b96d-0e4a28ebde0d","B.4.1.2","SANS 1200D\n8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Item","d6e9aba6-74fa-444b-a5ad-5bf9f402790b","B.4.1.2.1","8.3.1.2\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G15 * H15,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","fdf21ee7-c6c3-46ec-8e6e-bd0971c47ab0","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Item","f18bc7db-80ee-44b2-b674-7390b54dd1d4","B.4.1.2.2","","Biological Reactor","m³",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G17 * H17,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","00a7a053-d9cf-4b90-9c33-4df3fe187e6c","","8.3.2(a)","Backfill to 95% MOD AASHTO behind structures for :",{"$nulls":4},"Dflt"]
["Item","5e9ed153-4afb-442f-ad84-2c2da9874ac5","B.4.1.2.3","","Biological Reactor","m³",2200,{"v":0,"d":"0.00"},{"$f":"ROUND(G19 * H19,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f947e622-fbeb-4bc5-b2bb-425ba6cfdf64","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","15e335a7-0904-4a7e-b113-1cc673adadd5","B.4.1.2.4","","Biological Reactor","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Header2","94d8e805-3aeb-4e90-b995-4ba3bd03ea46","B.4.1.3","SANS 1200D 8.3.4","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","d85ae2e5-dab7-4ee6-9c9f-ee6e3a15d7c9","B.4.1.3.1","","Extra-over item B.4.1.2.3 for importation of material to complete embankment for the Biological Reactor from commercial sources where necessary: G7 material","m³",2200,{"v":0,"d":"0.00"},{"$f":"ROUND(G23 * H23,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b88abb15-39a6-4193-8c4a-e9cdc8970a4a","","SANS 1200D 8.3.7","Additional lateral support  (Provisional) for ensuring the stability of the excavation",{"$nulls":4},"Dflt"]
["Item","4b415882-1c59-47cc-adcb-1dbd43fe7add","B.4.1.3.2","","Biological Reactor","m²",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G25 * H25,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","5731e092-ee0c-432f-ad27-5d4a1ba0cfc2","B.4.1.4","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","5e4e3c07-6438-4dea-b6dd-12358c5e125e","B.4.1.4.1","8.3.10","Topsoiling","m²",1500,{"v":0,"d":"0.00"},{"$f":"ROUND(G27 * H27,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c4400eb4-90b0-46bc-90a5-8735856b2b4b","B.4.1.4.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc. as necessary and wetting","m²",1500,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","ddbe8e89-35b1-49ce-8a1e-bd3f4cabc534","B.4.1.5","SANS\n1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","0cacb69a-6ac5-4cfa-ac89-abfd0d35389f","","8.4.2","Blinding layer:\n15 MPa/19 mm concrete:",{"$nulls":4},"Dflt"]
["Item","452b2289-05a8-4c73-bff6-33cb63e0e950","B.4.1.5.1","","50 mm minimum thickness (stairs)","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","dc63cd49-7383-4a7a-9a0c-306d226465f1","","8.4.3\nPSG 3.5.4","Strength concrete:\n20 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","6bd35163-5a9e-45fe-aedd-07c7bcc6ebfa","B.4.1.5.2","","Benching to outlet","m³",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G33 * H33,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f85a91d0-1764-41f9-ad53-6391a1c155e9","","8.4.3\nPSG 3.5.4","Strength concrete (Inclusive of Crystalline Water Proofing additive):\n35 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","6fc8352a-fb0f-4cae-a362-f6dc7e2613fc","B.4.1.5.3","","WAS flow collector pipe chamber wall","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5f6fc084-3337-468d-8d0e-f115327c3608","B.4.1.5.4","","Stair Plinths","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","00381d28-edff-4cfb-b83f-5e475646c2ba","B.4.1.6","PSG 8.11","Structural floor screeds",{"$nulls":4},"Dflt"]
["Label","49346d73-aa2e-4870-aee3-a390726ea610","","","35 MPa/19mm concrete:",{"$nulls":4},"Dflt"]
["Item","24f0d099-b79e-4735-922b-f2ab729d9aaf","B.4.1.6.1","","50 mm thick to conical floor slabs","m²",4755,{"v":0,"d":"0.00"},{"$f":"ROUND(G39 * H39,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3e41c6c1-eb76-45e1-949e-a8b95f6d1999","B.4.1.6.2","","Fosroc Nitobond EP slowset or equal approved epoxy based bonding agent and primer to prepared concrete floors to receive screeding","m²",4755,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","74622898-4690-4e76-9923-ccea19d70126","B.4.1.7","SANS 1200G 8.1.1\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","fc7b56c4-3201-4599-a46f-ce38094779ce","","8.2.2","Smooth vertical plane to:",{"$nulls":4},"Dflt"]
["Item","146bb8c9-d2fd-401f-bd24-772133303a75","B.4.1.7.1","","WAS flow collector pipe chamber walls","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G43 * H43,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","77b2cebf-b1af-4a7b-ba48-c9e0fef0aba3","","8.2.5","Narrow widths (over 50 mm up to 300 mm wide):",{"$nulls":4},"Dflt"]
["Label","0b340ab6-86c0-4917-ac32-5ffea402de01","","8.2.2","Smooth vertical to footings:",{"$nulls":4},"Dflt"]
["Item","935fab08-ff53-499f-ab49-c308defb7c87","B.4.1.7.2","","Outlet weir upstand","m",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G46 * H46,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","160924d5-5447-4eee-ba97-11dc37b4f2cf","B.4.1.7.3","","Stair Plinths","m²",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","92e2950a-41ec-4218-a3c3-8e077e7c8d2b","","8.1.1.2\nPSG 8.1.1.8","Chamfers exceeding 20mm x 20mm and grooves:",{"$nulls":4},"Dflt"]
["Item","841b9cfa-b3a1-4c03-aea6-d4ec44097bb2","B.4.1.7.4","","Chamfer 25mm x 25mm (stairs)","m",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G49 * H49,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c310a63d-1e8b-4f2d-8c58-8631d000d82c","","8.2.6","Box out holes/form voids:",{"$nulls":4},"Dflt"]
["Label","bb5a3099-5ec1-4b4b-9123-f1cc93e87399","","","Small, circular (openings for sludge and water pressure relief valves etc) up to and including 0,35 m diameter.: depths\nover    and    up to",{"$nulls":4},"Dflt"]
["Item","9998cabe-c96c-467c-986d-58bf482d9c7a","B.4.1.7.5","","0 m                0,25 m","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","897cc531-57db-4602-9e2f-4065bd443c1e","B.4.1.7.6","","0,25 m         0,50 m","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","05deac0d-1235-46c1-90db-50811a84e294","","8.2.6","Small, other shapes up to 0,1  m² in area (opening for sluice gate): depths:\nover    and     up to",{"$nulls":4},"Dflt"]
["Rate Only","499ab6a8-7663-433a-bf04-5f32ad49fdba","B.4.1.7.7","","0 m                 0,5 m","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","b1002b3d-d1fb-4822-b797-528a5b85a074","B.4.1.7.8","","0,5 m             1,0 m","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","86e36d98-6dba-49f0-a183-99a505c862ad","","8.2.6","Large, other shapes, area over 0,1m² up to and including 1,2  m² in wall thickness: \nover    and    up to",{"$nulls":4},"Dflt"]
["Rate Only","9a0e4f37-9a99-4c64-9e0a-0d41c03d784d","B.4.1.7.9","","0 m                0,5 m","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","ebc9a851-614f-4262-ac86-28d9b4a5b645","","PSG 8.10","Cast pipes with or without puddle flange into concrete for:",{"$nulls":4},"Dflt"]
["Label","33848cd2-76a1-4dfe-aded-a1dee6e8f61e","","","Pipes up to and including 200mm NB through walls and Slabs of thickness: \nover    and    up to",{"$nulls":4},"Dflt"]
["Rate Only","f140bc1a-5be0-4a14-aac6-ba2c7d50a874","B.4.1.7.10","","0 m                0,25 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","0037ad31-26d9-4573-97d3-a298b965aef1","B.4.1.7.11","","0,25 m           0,5 m","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G62 * H62,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","858c3f61-32eb-41bf-b01b-393fc1b18562","","","Pipes up to and including 1200mm NB through walls and slabs of thickness: \nover    and    up to",{"$nulls":4},"Dflt"]
["Item","795cb1c3-b4c2-4ec9-951e-ab60da35e52e","B.4.1.7.12","","0 m                0,25 m","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G64 * H64,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","8cc72401-b603-4f33-81aa-465be1aabe46","B.4.1.7.13","","0,25 m           0,5 m","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header2","f1c70d23-4d9e-48ac-99ea-e4a2250820e3","B.4.1.8","SANS 1200G 8.1.2\nPSG 8.1.2","REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","cc9a6ef0-4198-431f-8686-488a2d8b0916","","8.1.2.3(a)","Mild steel bars:",{"$nulls":4},"Dflt"]
["Item","2a59c429-61f6-4f30-b35a-4e331c7d016a","B.4.1.8.1","","25 mm diameter: Basic price","t",0.06,{"v":0,"d":"0.00"},{"$f":"ROUND(G68 * H68,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5cc199a7-30d1-4a37-8003-f7a206210b8e","","8.1.2.3(b)","Extra-over item B.4.1.8.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","a08f3f44-0f3c-426e-9953-fa74af6496ce","B.4.1.8.2","","8 mm","t",0.06,{"v":0,"d":"0.00"},{"$f":"ROUND(G70 * H70,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","62153f75-7976-4384-b6dd-eeae42ebf5cb","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","07f0a750-4da1-4227-a96d-875d420e28ba","B.4.1.8.3","","25 mm diameter: Basic price","t",1.14,{"v":0,"d":"0.00"},{"$f":"ROUND(G72 * H72,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7f327824-9b6e-4f7c-acb3-3032c613790c","","8.1.2.3(b)","Extra-over item B.4.1.8.3 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","22a7adad-c31b-4869-8893-29ef5c303619","B.4.1.8.4","","10 mm","t",0.35,{"v":0,"d":"0.00"},{"$f":"ROUND(G74 * H74,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","87791498-b417-45dc-af8d-42f75a0b35e0","B.4.1.8.5","","12 mm","t",0.35,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7d4f41a2-765f-417e-a9af-cfa3160f2b35","B.4.1.8.6","","16 mm","t",0.44,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","6f335d29-5d21-410a-b74a-f50e0b2d8182","B.4.1.9","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","bfeadbf8-6041-458b-a147-c933c131ff9b","","8.1.1.5\nPSG 8.4","Steel-float finish:",{"$nulls":4},"Dflt"]
["Item","ab9e5dd6-9a15-479e-b5d1-fddc07976034","B.4.1.9.1","","Benching of WAS outlet","m²",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G79 * H79,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","071dd683-049c-492f-82d4-cd74e8f53db7","B.4.1.9.2","","Top of WAS outlet walls","m²",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","51bb7c40-3204-408e-a0d7-da14cf0ff335","","8.1.1.5\nPSG 8.4","Non-skid surface finish:",{"$nulls":4},"Dflt"]
["Item","41f48fd4-15e8-4954-b39b-bb51638c7a7b","B.4.1.9.3","","Stair Plinths","m²",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G82 * H82,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8332149e-ef3b-47a0-b62a-0fbad92748ca","","8.1.1.5\nPSG 8.4","Power-floated finish:",{"$nulls":4},"Dflt"]
["Item","02eaf513-c6a6-49d0-a182-208e9e94666f","B.4.1.9.4","","Mortar screed to floor slabs","m²",4755,{"v":0,"d":"0.00"},{"$f":"ROUND(G84 * H84,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","31b9bc88-96c5-4d96-9ef8-b9feb384ca60","B.4.1.10","SANS 1200 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Label","edd421db-23d0-4462-ba24-9482aead9f7f","","","Contraction joint in floor slab complete as shown on Dwg. No. J40073/010-207 and detail on Dwg. No. J40073/010-103:",{"$nulls":4},"Dflt"]
["Item","7c7d63f8-c7b0-4e65-bb79-caf91049ed73","B.4.1.10.1","","Joint in Floor:\nIncluding forming of joint, supply and installation (all inclusive) of 2mm Recess, Stainless steel strip and 250mm x 2mm Hypelon bandage","m",300,{"v":0,"d":"0.00"},{"$f":"ROUND(G87 * H87,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b636806e-4cff-409f-bfc1-d10feab92f20","B.4.1.10.2","","Joint in Screed:\nIncluding forming of joint, supply and installation (all inclusive) of 8mm diameter Polycord and Polyurethane sealant","m",300,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","38284820-9abe-4957-b58c-21dc811db3b4","","","Wall joints complete as shown on Dwg. No. J40073/010-207 and detail shown on Dwg. No. J40073/010-103:",{"$nulls":4},"Dflt"]
["Item","51b5889c-75f4-4f84-b6d9-42aadb105a66","B.4.1.10.3","","Joint in Wall (Internal Walls):\nIncluding forming of joint, supply and installation (all inclusive) of 2mm Recess, Stainless steel strip and 250mm x 2mm Hypelon bandage on inside","m",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G90 * H90,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","85945bfa-31cc-4075-ad6c-25e6e6a8ca20","B.4.1.10.4","","Joint in Wall (External Walls):\nIncluding forming of joint, supply and installation (all inclusive) of 2mm Recess, Stainless steel strip and 250mm x 2mm Hypelon bandage on inside and 8mm diameter Polycord and Polyurethane sealant on outside","m",600,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","6aa83f0e-bc38-4724-8ce6-4e3685d6d437","B.4.1.11","SANS 1200H and HA","STRUCTURAL STEELWORK",{"$nulls":4},"Dflt"]
["Label","907106a5-14ad-49ef-8610-672ae0dda462","","PSG 8.10","Supply, install, corrosion protection, testing, etc angles:",{"$nulls":4},"Dflt"]
["Item","599a7d66-743a-4bc4-8ece-ce9902c13b17","B.4.1.11.1","","50 x 50 mm galvanised angles cast into concrete","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G94 * H94,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6110ffcc-351e-4913-827d-695b70f62c3f","","","Installation of galvanized steel staircases:",{"$nulls":4},"Dflt"]
["Sum","15225138-af11-4b70-ac23-2f0c90b5e923","B.4.1.11.2","","Complete Installation of staircases, material provided by others","Prov.Sum",1,{"v":50000,"d":"50,000.00"},{"$f":"ROUND(H96,2)","v":{"v":50000,"d":"50,000.00"}},"Dflt"]
["Header2","8f31de69-8c36-4719-a268-97b0c61292f4","B.4.1.12","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","56bdcf42-ffd7-48d3-843f-2d22af643825","","","Water Tightness Testing:",{"$nulls":4},"Dflt"]
["Item","e7067a58-31f6-4667-814a-d478db98d63a","B.4.1.12.1","PSG 8.12","Testing for Water Tightness, all inclusive to PSG 7.2.5","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G99 * H99,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cf84e280-922b-4333-b547-84968e9e08a9","","","Lowering of BNR Weirs:"]
["Sum","96a1e783-9948-40ca-9421-f2e46df11d3c","B.4.1.12.2","","Lowering of BNR weirs complete and all inclusive as shown on Dwg. No. J40073/010-207 & J40073/010-208","PSum",1,{"v":120000,"d":"120,000.00"},{"$f":"ROUND(H101,2)","v":{"v":120000,"d":"120,000.00"}}]
["Label","df8d86e5-0da7-453b-9885-fb8d06df3227","","","Corrective work to BNR"]
["Sum","0a97ff39-8dfa-4444-b7c5-0f6680bb85a3","B.4.1.12.3","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":5000000,"d":"5,000,000.00"},{"$f":"ROUND(H103,2)","v":{"v":5000000,"d":"5,000,000.00"}}]
["Label","6c49c555-f897-4684-97bc-b155db36b1b4","","","Supply of Lime"]
["Sum","e0f68357-96fc-44f1-8552-8f3d945c1102","B.4.1.12.4","","Provide hydrated lime for disinfecting overflowed sludge","PSum",1,{"v":50000,"d":"50,000.00"},{"$f":"ROUND(H105,2)","v":{"v":50000,"d":"50,000.00"}}]

{"sheet":"BILL B.5.","index":5,"n_rows":178,"n_cols":10,"rows_kept":178,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.5.",null,"SECONDARY SEDIMENTATION TANK",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","f3f40298-8c7b-421c-a61b-732bac7975b7","B.5.1","","SECONDARY SEDIMENTATION TANK",{"$nulls":4},"Dflt"]
["Label","b4292b73-9672-40a2-9309-13eab2bc625c","","","SECTION B.5.1 : SECONDARY SEDIMENTATION TANK",{"$nulls":4},"Dflt"]
["Header2","e4a2e39b-e3b2-4c6f-bec2-8c5845f2683a","B.5.1.1","SANS\n1200C &\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","028f0ed4-3591-46a6-924e-ac995d7f5316","B.5.1.1.1","8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",200,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","f54f4401-1629-4246-98b1-ac772af1e668","B.5.1.1.2","8.2.8","Demolish and remove existing concrete flooring on conical surface","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H13,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","cf6ea9ab-146c-45d1-a97d-81cefbcbd408","B.5.1.1.3","8.2.8","Dismantle and remove existing wall footing reinforcing","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f1bc0121-0577-4b29-8597-b1159314d878","B.5.1.1.4","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G15 * H15,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","85c11371-8f0e-4633-ac68-d9e0bb0b1382","B.5.1.2","SANS 1200D\n8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Rate Only","e4cb973d-2c6e-40b2-b178-6cec2822c411","B.5.1.2.1","8.3.1.2\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","ec235039-fe40-4274-a375-4cdd5d7a9dbc","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Rate Only","ac39b235-8db9-4eaf-9b41-f181ac667802","B.5.1.2.2","","Secondary Sedimentation Tank","m³",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","b87639e2-d1d9-4915-91f0-dd7d00bbc1a5","","8.3.2(a)","Backfill to 95% MOD AASHTO behind structures for :",{"$nulls":4},"Dflt"]
["Item","4e5d69e0-a3f3-4480-a4a9-cb0ea4e01743","B.5.1.2.3","","Secondary Sedimentation Tank","m³",1325,{"v":0,"d":"0.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cd3ecd1a-d6c5-4255-8637-c113728c8e92","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","7d64cb64-4473-4b7c-8907-1531dce675ee","B.5.1.2.4","","SST","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G23 * H23,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Header2","d7aea17b-efeb-428b-9389-133999d7d67e","B.5.1.3","SANS 1200D 8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.5.1.2.2 for excavation in:",{"$nulls":4},"Dflt"]
["Rate Only","aaf5bd18-003d-44d4-af11-6fc79d1eded2","B.5.1.3.1","8.3.2(b)","Hard rock material","m³",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header2","43aeaa4a-ae8d-464e-92d0-f9add8f2e67b","B.5.1.4","SANS 1200D 8.3.4","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","956b21bc-dfda-47b0-bd22-584538af37fe","B.5.1.4.1","","Extra-over item B.5.1.2.3 for importation of material to complete embankment for the Secondary Sedimentation Tank from commercial sources where necessary: G7 material","m³",550,{"v":0,"d":"0.00"},{"$f":"ROUND(G27 * H27,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","33556867-e60c-4a07-8c92-83aba5d5c2df","","8.3.7","Additional lateral support  (Provisional) for ensuring the stability of the excavation",{"$nulls":4},"Dflt"]
["Item","a0657a80-3aa3-4953-9d69-380335edba85","B.5.1.4.2","","Secondary Sedimentation Tank","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G29 * H29,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","b0065dae-a05d-4716-8304-8bbeaf3572a5","B.5.1.5","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","2c4af831-253e-4575-8781-cef752878f81","B.5.1.5.1","8.3.10","Topsoiling","m²",1300,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1244900e-a035-4f4d-ba09-fb8a4216abe6","B.5.1.5.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc as necessary and wetting","m²",1300,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","bf7f0be1-0387-482e-a9d7-ead461ef04c9","B.5.1.6","SANS 1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","ec022311-2fe9-49a8-b972-1fd99ba619f6","","8.4.2","Blinding layer:\n15 MPa/19 mm concrete:",{"$nulls":4},"Dflt"]
["Item","6fd4f971-194e-4976-b853-eb7230e1ebaf","B.5.1.6.1","","75 mm minimum thickness (Footing)","m²",140,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","fde6ef89-a8c1-4df8-974e-5e4584063df8","B.5.1.6.2","","50 mm minimum thickness (Channel)","m²",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","e44e0251-a980-40b1-bcac-2f67a4132731","","8.4.3","Strength Concrete:\n15 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","a672c29d-e649-447a-b71a-b9c76f723840","B.5.1.6.3","","Thrust blocks","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G38 * H38,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5fafd766-4f7e-4371-a4ec-25b7b7ff7e1c","","8.4.3\nPSG 3.5.4","Strength Concrete (Inclusive of Crystalline Water Proofing additive):\n35 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","ace955aa-f700-426a-aa38-0c5f6053cb63","B.5.1.6.4","","Conical floor slab","m³",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G40 * H40,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ee380e00-27c7-4193-99d8-c45852fe26c3","B.5.1.6.5","","Footing slab (Walls)","m³",45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f1f0b568-95b2-42a5-b49f-99fdd5e93302","B.5.1.6.6","","Rotating bridge platform beams, slab and plinth","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3d47f60e-c360-414e-bc83-9ff7c1359e4e","B.5.1.6.7","","Launder slab","m³",28,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ab98768d-0d63-4c87-9efa-fc67722742ed","B.5.1.6.8","","Outlet channel slab","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","eab3a4a0-12bf-4938-af7e-12b31471e607","B.5.1.6.9","","Vertical circular walls ","m³",54,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","00309cdd-879b-49a4-9b53-0ed2844ad51a","B.5.1.6.10","","Launder walls","m³",29,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c1eeb506-3ae5-47dd-94c3-bb38abcf1f17","B.5.1.6.11","","Outlet channel walls","m³",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b2879389-47ce-4d29-b1c2-c7a839ad4130","B.5.1.6.12","","Columns","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","853c736e-0768-44ea-8b3b-ed1da33a1a5d","","","Soilcrete:\n3 MPa:",{"$nulls":4},"Dflt"]
["Item","9b495a97-2f95-47cd-bccc-2a0851ba7c68","B.5.1.6.13","","Mass soilcrete under the SST","m³",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G50 * H50,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","3f1ad6d3-e9ab-49d8-aefe-b810e397e627","","8.4.3\nPSG 3.5.4","Strength Concrete:\n20 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","e8269119-7e9f-4b73-8248-951ac60be368","B.5.1.6.14","","Circular benching ","m³",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","40563ab3-6323-4a69-9b1d-dfd8f092902e","","PSG 8.9","No-fines in NF 19 mm:",{"$nulls":4},"Dflt"]
["Item","36bfee7e-0bb1-4905-832c-f97083653372","B.5.1.6.15","","To underside of floor slab, 75 mm nominal thickness","m³",55,{"v":0,"d":"0.00"},{"$f":"ROUND(G54 * H54,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","f53ef4bd-c0b8-425f-9a6a-2c20e00abbb1","B.5.1.7","PSG 8.11","Structural floor screeds",{"$nulls":4},"Dflt"]
["Label","3150a005-fb34-47f7-8bfe-0fb0b68ee881","","","35 MPa/19mm concrete:",{"$nulls":4},"Dflt"]
["Item","b9a529fb-0b02-4d75-9dbb-5c48adee6f7f","B.5.1.7.1","PSG 8.11","50 mm thick to conical floor slabs","m²",685,{"v":0,"d":"0.00"},{"$f":"ROUND(G57 * H57,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3f3e7c7d-1ad2-457d-b94e-18dc94c94a2a","B.5.1.7.2","","Fosroc Nitobond EP slowset or equal approved epoxy based bonding agent and primer to prepared concrete floors to receive screeding","m²",685,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1c465c4d-6315-49c5-80cd-1f9f01291927","B.5.1.7.3","","Average 35 mm thick to launder slabs","m²",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","4f6f057a-bb7a-4d87-89fc-0975c1604a15","B.5.1.8","SANS 1200G 8.2\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","478c9e46-929e-4321-baf9-430e177a0cf7","","8.2.2","Smooth vertical circular to walls:",{"$nulls":4},"Dflt"]
["Item","66c804f4-fde9-439e-990f-18f640ee1803","B.5.1.8.1","","15250 mm radius","m²",310,{"v":0,"d":"0.00"},{"$f":"ROUND(G62 * H62,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5ea71f43-8bbe-4898-b95f-21a20f7c42ad","B.5.1.8.2","","15000 mm radius","m²",360,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6790ff59-8254-45a1-894e-630f857866cb","B.5.1.8.3","","14600 mm radius","m²",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ecf28828-0418-4ad8-915f-73b31022256d","B.5.1.8.4","","14400 mm radius","m²",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","28b2051b-aa8a-4387-ae9c-09ce9c3c9801","","8.2.2","Smooth vertical plane to:",{"$nulls":4},"Dflt"]
["Item","17393e46-de02-4f35-beba-6cb9cd7b565b","B.5.1.8.5","","Rotating bridge platform beams and slab","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G67 * H67,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","db2fdc26-e1da-4fc1-b631-29cd4fafb455","B.5.1.8.6","","Columns","m²",35,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","849ec4e1-12db-4afe-83cc-e43b0a2786f9","B.5.1.8.7","","Outlet ","m²",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b343b6ed-61d0-4d60-bfa4-993ecda93576","B.5.1.8.8","","Channel","m²",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","2b4a2e30-362e-44d6-9d2c-68cd050513df","","8.2.2","Smooth sloping circular to:",{"$nulls":4},"Dflt"]
["Item","d76828ad-a10f-4303-a47b-d20601898e1a","B.5.1.8.9","","Launder soffit","m²",62,{"v":0,"d":"0.00"},{"$f":"ROUND(G72 * H72,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7b68da6f-3cea-4bad-916c-0e6cb54ba7ce","B.5.1.8.10","8.2.2","Smooth, sloping, plane to fillet soffits of rotating bridge platform","m²",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f78a93b1-06f0-475e-960c-2d84d979e38a","","8.2.2","Smooth horizontal plane to:",{"$nulls":4},"Dflt"]
["Item","cc6bd2cb-114a-43ae-9148-fc183b41a052","B.5.1.8.11","","Rotating bridge platform beam and slab soffits","m²",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G75 * H75,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4b64fb28-4a1e-4fc7-bace-caf6e39ba028","B.5.1.8.12","","Launder outlet soffit","m²",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","44576bb7-df3e-4e87-8b9a-b1e7d045e68e","","8.2.5","Narrow widths (over 50 mm up to 300 mm wide):",{"$nulls":4},"Dflt"]
["Label","c3f4fcdf-bd12-406c-acad-ad44d38a8f07","","8.2.1","Rough vertical circular to footings:",{"$nulls":4},"Dflt"]
["Item","0392c7d1-a7b8-47c0-a387-c1d2bfe64c79","B.5.1.8.13","","15850 mm radius (outside)","m",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G79 * H79,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","447c812f-e9b6-4639-9a05-bea695c2b3b7","","8.2.2","Smooth vertical circular to footings:",{"$nulls":4},"Dflt"]
["Item","89aceb29-266f-49b2-b1b5-cfba239914f3","B.5.1.8.14","","14100 mm radius (inside)","m",90,{"v":0,"d":"0.00"},{"$f":"ROUND(G81 * H81,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","674b3ea1-373e-43b3-a803-ee16608cdf41","B.5.1.8.15","","4050 mm radius (centre outside)","m",26,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3040183d-d4c6-4554-8e0e-b4d42c86e2f6","B.5.1.8.16","","3350 mm radius (centre inside)","m",21,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1bfcaa2c-0828-479b-85f4-cc732c22b5f7","","8.2.2","Smooth vertical circular to:",{"$nulls":4},"Dflt"]
["Item","60766252-0d22-4fc1-8d3d-3f08abbbaf87","B.5.1.8.17","","15300 mm radius (mushroom head)","m",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G85 * H85,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5e29284b-a28e-4fab-b09e-8fc2aaf19649","B.5.1.8.18","","14950 mm radius (mushroom head)","m",95,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7fab63c4-8d74-4509-a0be-6b914496cb73","B.5.1.8.19","","300 mm radius (platform plinth)","m",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","01a37477-001f-4e0a-bcbf-99896274063b","B.5.1.8.20","","400 mm radius (platform plinth)","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","fe6b3683-5946-46da-96fb-344550ff22b7","","8.1.1.2\nPSG 8.1.1.8","Chamfers exceeding 20mm x 20mm and grooves:",{"$nulls":4},"Dflt"]
["Rate Only","e818c1d2-e65c-41ac-a1af-c9e9db67fb5f","B.5.1.8.21","","Chamfer 25mm x 25mm","m",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","bc6ef079-5bcf-40b0-ab95-de207f771ea7","B.5.1.8.22","","Chamfer 50mm x 50mm","m",385,{"v":0,"d":"0.00"},{"$f":"ROUND(G91 * H91,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1a01fa9b-2164-48a0-9d92-62ac3fad0ef6","B.5.1.8.23","","Chamfer 100mm x 100mm","m",95,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","44e6fa02-085f-46f7-b524-49911d2e1f47","","8.2.6","Box Out Holes/Form Voids:",{"$nulls":4},"Dflt"]
["Label","e918cdf9-5a58-43e4-9066-c046826af663","","a)","Small, other than circular, of area up to and including 0.1 m² through slabs of thickness:",{"$nulls":4},"Dflt"]
["Label","b4484bbe-4bb3-4d24-91bb-e2177ff232db","","","Over (m)         Up to and incl. (m)",{"$nulls":4},"Dflt"]
["Item","20d48c74-de62-4b78-80a1-f03d7ba0e78c","B.5.1.8.24",""," 0.0                   0.25","No",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G96 * H96,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","83af585a-a443-409a-bb24-c0bd01bafd16","","8.7(b)","Pockets for holding down bolts of diameter:",{"$nulls":4},"Dflt"]
["Label","b63b47cc-cd47-4d28-9543-1daefcc62208","","","Over (mm)       Up to and incl. (mm)",{"$nulls":4},"Dflt"]
["Rate Only","73624faf-2ac7-4743-97b2-533b7bc2c55d","B.5.1.8.25","","8 mm                        16 mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Rate Only","8ca0138e-8895-42da-9b83-78d91a4a9c73","B.5.1.8.26","","16 mm                      24 mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","707411bb-d471-474e-b105-7cb9212643ec","","PSG 8.10","Casting of pipes/specials into concrete for: ",{"$nulls":4},"Dflt"]
["Label","76cc2eb6-440b-4b80-9d51-ecd52be222ce","","","Pipes up to and including 200 mm NB, through walls and slabs of depth:",{"$nulls":4},"Dflt"]
["Label","c4a0c2c4-0665-41fd-b472-cc8ce3158839","","","Over (m)         Up to and incl. (m)",{"$nulls":4},"Dflt"]
["Item","decb8097-6994-4b76-ad97-e3eaa1d957ef","B.5.1.8.27","","0.00                   0.40  ","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G104 * H104,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","84283595-9b8a-4402-bae5-201f008cbf3c","","","Pipes over 200 mm NB up to and including 600 mm NB, through walls and slabs of depth:",{"$nulls":4},"Dflt"]
["Label","d932879e-bbe8-4464-a8b5-41c1e8570091","","","Over (m)         Up to and incl. (m)",{"$nulls":4},"Dflt"]
["Rate Only","a43a9933-e581-489b-b05e-252c2974e99a","B.5.1.8.28","","0.00                   0.40  ","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","9c9967e1-7f8f-4b8b-8ecc-9a7d9b97fdc8","","","HDPE electrical cable sleeve:",{"$nulls":4},"Dflt"]
["Item","ef988ab1-2875-464d-af48-7eed010f3722","B.5.1.8.29","","63 mm diameter type 4 class 6 ","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G109 * H109,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","55f72e1c-db52-423a-a3a1-e59adbda9aab","B.5.1.9","SANS 1200G 8.1.2\nPSG 8.1.2","REINFORCEMENT ",{"$nulls":4},"Dflt"]
["Label","6e15518e-5ab3-4a37-bc4b-2ddf782ec172","","8.1.2.3(a)","Mild steel bars:",{"$nulls":4},"Dflt"]
["Item","8402e7bf-5adf-4303-ae11-797157c4d381","B.5.1.9.1","","25 mm diameter: Basic price","t",2.13,{"v":0,"d":"0.00"},{"$f":"ROUND(G112 * H112,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b16e59cd-53cc-468a-ab53-84626b103f7c","","8.1.2.3(b)","Extra-over item B.5.1.9.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","72a2c4e2-0035-4351-b13f-c665abe47293","B.5.1.9.2","","8 mm","t",0.64,{"v":0,"d":"0.00"},{"$f":"ROUND(G114 * H114,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b6796741-61c4-4006-9c72-6a501a637f98","B.5.1.9.3","","10 mm","t",1.49,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","190a4c19-6687-4a58-943e-cb2e5eed22c2","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","1d2edcc8-d527-4d2e-8def-c88b59d5300d","B.5.1.9.4","","25 mm diameter: Basic price","t",40.37,{"v":0,"d":"0.00"},{"$f":"ROUND(G117 * H117,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","de2831a0-76c0-47b6-bf1d-819708bcccbf","","8.1.2.3(b)","Extra-over item B.5.1.9.4 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","a6507acc-2612-4656-8c35-ed81975fa0f4","B.5.1.9.5","","10 mm","t",14.13,{"v":0,"d":"0.00"},{"$f":"ROUND(G119 * H119,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","bb64c532-1f19-4ced-a21c-e8f843983c41","B.5.1.9.6","","12 mm","t",16.15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","17009844-3b19-4b8c-b6f5-f326cbd06f0e","B.5.1.9.7","","16 mm","t",8.07,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","61b42083-677e-4e58-8ee6-bcb0ab1aea59","B.5.1.9.8","","20 mm","t",2.02,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","6dfe9b07-7899-4648-9e65-3a678575dd83","","8.1.2.3(c)","High-tensile welded mesh reinforcement:",{"$nulls":4},"Dflt"]
["Item","cacbcaf9-de2c-4274-81e9-be4b0a7f3170","B.5.1.9.9","","High-tensile welded mesh ref 617","m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G124 * H124,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","bbf5be7c-a3e3-4e36-8062-7c143545aaf4","B.5.1.10","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","39252e1f-cbc3-4470-9bdf-0ef7d9c4be2d","","PSG 8.4","Wood-floated finish:",{"$nulls":4},"Dflt"]
["Item","0b237189-61a7-4c88-81b9-18ffb20cfd5f","B.5.1.10.1","","Floor slabs","m²",685,{"v":0,"d":"0.00"},{"$f":"ROUND(G127 * H127,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1e2b4342-7751-4142-8ea8-e7ac054f328a","B.5.1.10.2","","Launder slabs","m²",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","831fea9e-65e8-4783-907d-b32284fa8dd2","B.5.1.10.3","","Benching","m²",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d7b570cb-3a3c-464a-992c-6d58267099e7","","8.1.1.5\nPSG 8.4","Steel-floated finish:",{"$nulls":4},"Dflt"]
["Item","7308c8ed-8b44-478d-8e24-d1a5a256e498","B.5.1.10.4","","Top of walls including for vertical tolerance (SST)","m²",35,{"v":0,"d":"0.00"},{"$f":"ROUND(G131 * H131,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","8658946d-dc38-4bed-bc8c-d0b16f58d270","B.5.1.10.5","","Top of beams, slab and plinth","m²",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2aa6cdc1-1bdf-49ae-8120-900342df64f7","B.5.1.10.6","","Channel Floor","m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ccbd6d1b-3f48-420b-8a2c-8ba84795e838","B.5.1.10.7","","Channel Walls","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","222eb6de-c2bc-4e0b-ac08-882b890769b5","","8.1.1.5\nPSG 8.4","Power-floated finish:",{"$nulls":4},"Dflt"]
["Item","6a1c0f66-7819-4f4d-a8ce-d44ecfaa6eef","B.5.1.10.8","","Mortar screed to conical floor slabs","m²",685,{"v":0,"d":"0.00"},{"$f":"ROUND(G136 * H136,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","f6c986f9-0148-4ba4-893e-09dd12ebca99","B.5.1.11","SANS 1200G 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Label","941885c5-b43a-4e5a-85c8-ccd170b2dfa2","","","Expansion joint type B complete as shown on Dwg. No. J40073/010-213:",{"$nulls":4},"Dflt"]
["Item","d543d030-04c4-4508-835d-8b711dd8017d","B.5.1.11.1","","Joint in Floor:\nIncluding forming of joint, supply and installation (all inclusive) of 250mm Rearguard centre bulb waterstop, 10mm Closed cell high density void former, 2mm Recess, Stainless steel strip and 200mm x 2mm Hypelon bandage","m",210,{"v":0,"d":"0.00"},{"$f":"ROUND(G139 * H139,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","19ce93e0-a554-4384-9c7b-c68317936faa","B.5.1.11.2","","Joint in Screed:\nIncluding forming of joint, supply and installation (all inclusive) of 8mm diameter Polycord and Polyurethane sealant","m",210,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f771ef9c-9f81-4d01-8e5f-8baeb46eb268","","","Contraction joint in conical floor slab complete as shown on Dwg. No. J40073/010-213:",{"$nulls":4},"Dflt"]
["Item","22db0c31-fc22-49ff-945c-c8f981b81543","B.5.1.11.3","","Joint in Floor:\nIncluding forming of joint, supply and installation (all inclusive) of 250mm Rearguard waterstop, 2mm Recess, Stainless steel strip and 200mm x 2mm Hypelon bandage","m",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G142 * H142,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","64753a61-ebb6-40d2-bc08-f28b9539f701","B.5.1.11.4","","Joint in Screed:\nIncluding forming of joint, supply and installation (all inclusive) of 8mm diameter Polycord and Polyurethane sealant","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","756f32c5-01fd-464f-a7bc-403dd9d96591","","","Wall joints complete as shown on Dwg. No. J40073/010-213:",{"$nulls":4},"Dflt"]
["Item","d3b04188-b8b3-4e05-8a4a-84befacf7668","B.5.1.11.5","","Construction Joint in Wall:\nIncluding forming of joint, supply and installation (all inclusive) of 2mm Galvanised water stop","m",95,{"v":0,"d":"0.00"},{"$f":"ROUND(G145 * H145,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","bf9eedec-a8f2-4887-aaf1-9c62b19435e6","B.5.1.11.6","","Isolation Joint in Wall (between wall and launder channel):\nIncluding forming of joint, supply and installation (all inclusive) of 10mm Jointex","m",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","432dd38c-1e1a-4d6b-a960-9bda8d475fff","","","Channel Floor and Wall joints complete as shown on Dwg. No. J40073/010-216:",{"$nulls":4},"Dflt"]
["Item","44163eaa-a2b1-4a31-acc0-93698c4857c8","B.5.1.11.7","","Construction and Contractions Joints in Channel:\nIncluding forming of joint, supply and installation (all inclusive) of Centre bulb waterstop","m",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G148 * H148,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ec943d15-250f-4679-a030-68e80bcb6035","B.5.1.11.8","","Construction Joint in Wall:\nIncluding forming of joint, supply and installation (all inclusive) of 2mm Galvanised water stop","m",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","04b25b3b-4e99-4489-9dd0-ecf13c45675f","B.5.1.12","SANS 1200G 8.7","GROUTING",{"$nulls":4},"Dflt"]
["Label","5b4adeb7-362c-4186-ba58-a015a0535a70","","","Grout column bases and HD bolts as specified:",{"$nulls":4},"Dflt"]
["Item","debe2845-78f9-4350-b9f8-8c2d5901a085","B.5.1.12.1","8.7(a) and (b)","Under bases or beds, nominal thickness not exceeding 50 mm","m³",0.5,{"v":0,"d":"0.00"},{"$f":"ROUND(G152 * H152,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","18e5c3ea-7675-44d7-b8b7-eefa38384f0e","B.5.1.12.2","","Drilling hole for dowels into existing channels","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","50a0e002-df47-4f1b-a06c-8b1ac53ea8ad","B.5.1.12.3","","Apply wet and dry epoxy","m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","5f860b71-dbd5-424b-be32-ad69bcaca605","B.5.1.13","SANS 1200G 8.8","HD bolts etc:",{"$nulls":4},"Dflt"]
["Label","464e2b52-9684-4d94-a25e-cb40814024cc","","","Provide and install HD bolts to details given on Dwg. No. J40073/010-214:",{"$nulls":4},"Dflt"]
["Item","b6d30312-02aa-49e6-a889-4a4e3d954170","B.5.1.13.1","","HD bolts in pockets, void exceeding 0.5 litres but less than 1.0 litres","No",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G157 * H157,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7392b0c2-807f-404d-8090-c31fd2362ac4","B.5.1.13.2","","HD bolts in pockets, void less than 0.5 litres","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","47106106-93a8-4a09-8b41-b15793d0ef2c","B.5.1.14","(Refer SANS 1200 L, LB and LD)","MEDIUM PRESSURE PIPELINES ",{"$nulls":4},"Dflt"]
["Header3","be55ccdb-2aad-4e86-9d98-4a9111a8dad0","B.5.1.14.1","","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","eed00ac3-ffe8-4d17-a6b5-a10ca3b77f30","","L8.2.5","Supply and install pipes, valves and specials (short pipe runs):",{"$nulls":4},"Dflt"]
["Label","d5d809ed-6499-4e4a-b26d-4a33e4b11f8f","","","Inlet pipework:",{"$nulls":4},"Dflt"]
["Rate Only","131d8415-7e0c-4dd4-b1cd-6038f7e95fec","B.5.1.14.1.1","","600 mm, 90 deg. bend duckfoot ms","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","a67e5278-336f-4df1-acb8-e75d0cdcba66","B.5.1.14.1.2","","600 mm x 915 mm NB bellmouth, pe/fl, 4.5 mm wt, ms, 5010 mm f/f","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G164 * H164,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","64823b86-00ac-4393-a448-4061ebaf69ac","","","Scum withdrawal pipework:",{"$nulls":4},"Dflt"]
["Item","87e1e785-7ea1-4efb-971f-c1e07ae680e7","B.5.1.14.1.3","","200 mm NB wall pipe, pe/fl, medium duty, s/s, with thr-fl, 800 mm f/f","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G166 * H166,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","8ab31623-dde1-4fb6-9cb2-65fdfaa11e62","B.5.1.14.2","","VALVES",{"$nulls":4},"Dflt"]
["Label","a5c6a325-64eb-43cf-8270-ac9bf26f2b6a","","","Pressure relief supply and installed in floor of SST:",{"$nulls":4},"Dflt"]
["Item","a71f4747-1289-411a-83d9-bfd12d0fc6dd","B.5.1.14.2.1","","Pressure relief valves complete as shown on Dwg. No. J40073/010-214","No",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G169 * H169,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","a3766fd1-b1b0-47bf-b828-64e109ccbd25","B.5.1.15","","MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Item","38371f21-5975-4db0-bf51-aec87af0ba08","B.5.1.15.1","PSG 8.13","Supply and fix in place 250 µm PVC damp-proof course layer between no-fines concrete layer and floor slabs","m²",755,{"v":0,"d":"0.00"},{"$f":"ROUND(G171 * H171,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","c0e73ef4-0b37-41ce-ac6b-f7cf5b3e2cf0","B.5.1.16","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","cd68b451-9936-4638-8298-bf72a57797ed","","","Water Tightness Testing:"]
["Item","d3675a25-f5b7-41d2-af16-edf1e06b6977","B.5.1.16.1","PSG 8.12","Testing for Water Tightness, all inclusive to PSG 7.2.5","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G174 * H174,2)","v":{"v":0,"d":"0.00"}}]
["Label","48b034ea-abc6-4ed7-a913-05e771f88b29","","","Corrective work to SST:"]
["Sum","c2bf274a-bd1f-4d1c-8c29-6d80188203b9","B.5.1.16.2","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":100000,"d":"100,000.00"},{"$f":"ROUND(H176,2)","v":{"v":100000,"d":"100,000.00"}}]
["Header2","7d9573d8-5c46-4f3a-9236-e12cbbba2d59","B.5.1.17","","SCUM MANHOLES (AT SST)"]
["Item","bbf77f4f-df60-415e-8137-3158009e01e6","B.5.1.17.1","","Scum Manholes at SST:\nComplete partially completed manholes including excavation, backfilling, watertightness testing etc. complete with all pipework, testing all inclusive as shown on Dwg. No. J40073/010-225","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G178 * H178,2)","v":{"v":0,"d":"0.00"}}]

{"sheet":"BILL B.6.","index":6,"n_rows":126,"n_cols":10,"rows_kept":126,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.6.",null,"SLUDGE DRYING BEDS",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","a561e081-4b91-452a-80f1-00a40c95f2f2","B.6.1","","SLUDGE DRYING BEDS",{"$nulls":4},"Dflt"]
["Label","d7ef6b23-f3d3-46e4-bd9d-6820ace4deb1","","","SECTION B.6.1 : SLUDGE DRYING BEDS",{"$nulls":4},"Dflt"]
["Header2","ec9a1182-a8d2-4323-9a58-5d3880c7ad16","B.6.1.1","SANS\n1200C\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","8bdb05ee-edea-4c7f-9a44-f81f57e65f89","B.6.1.1.1","8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",200,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a4e9ed0b-1338-44ed-9fbb-cd6b08c3f449","B.6.1.1.2","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","50a0387e-2172-4063-87ce-b3ae0e323849","B.6.1.2","SANS 1200D 8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Label","29647f0d-ad8d-4906-a9c8-bdc461c9a105","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Rate Only","58ad3d41-a975-4c5b-9567-c9e8e6948c5b","B.6.1.2.1","","Sludge Drying Beds","m³",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Label","8d1b57f2-0650-4691-a282-5e4570205473","","8.3.2(a)","Backfill to 95% MOD AASHTO behind structure for :",{"$nulls":4},"Dflt"]
["Item","6c64f2a0-eca9-4732-8708-958c60f8b5f0","B.6.1.2.2","","Sludge Drying Beds","m³",1260,{"v":0,"d":"0.00"},{"$f":"ROUND(G18 * H18,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b787e2c9-e53c-48d5-83d6-74f7a68e31af","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","44fcc901-a5c1-41c9-9fa7-132be5f2a81e","B.6.1.2.3","","Sludge Drying Beds","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G20 * H20,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Header2","81c86a06-dc0b-4933-a418-9b46f506820a","B.6.1.3","SANS 1200D 8.3.4","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","d2109466-d24d-4e59-8655-16f2f6afc881","B.6.1.3.1","8.3.4(a)","Extra-over item B.6.1.2.2 for importation of material to complete embankment for the Sludge Drying Beds from commercial sources where necessary: G7 material","m³",1260,{"v":0,"d":"0.00"},{"$f":"ROUND(G22 * H22,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","280d8d36-2f9e-4187-83be-4963a811ad82","B.6.1.4","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","46ea3a6e-bb5b-43c2-b28e-02e64465ca2b","B.6.1.4.1","8.3.10","Topsoiling","m²",2840,{"v":0,"d":"0.00"},{"$f":"ROUND(G24 * H24,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ed1ca70d-5d6a-40c6-acc4-80272c2581be","B.6.1.4.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc as necessary and wetting","m²",2840,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","c6d5b1cc-54dd-4da9-bd46-7b07214bcf91","B.6.1.5","SANS\n1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","b86e2fdf-4f18-4593-a83f-92cbf8fef2ef","","8.4.2","Blinding layer in 15 MPa/19 mm concrete",{"$nulls":4},"Dflt"]
["Item","4dcf634b-969a-4de9-8cd4-5cf31a0bdfa5","B.6.1.5.1","","50 mm minimum thickness","m²",95,{"v":0,"d":"0.00"},{"$f":"ROUND(G28 * H28,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","de496827-1255-4579-a1f8-604efdb7ef20","","8.4.3","Strength concrete: 25 MPa/19mm",{"$nulls":4},"Dflt"]
["Item","951e3b67-44e5-4b91-b5a9-178f7f4697c5","B.6.1.5.2","","Ramps","m³",35,{"v":0,"d":"0.00"},{"$f":"ROUND(G30 * H30,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b839fd89-f868-4f2b-bd71-98c4a947f793","","8.4.3","Strength concrete: 35 MPa/19mm to:",{"$nulls":4},"Dflt"]
["Item","609b9958-0ae8-43d2-a596-17ad62f00635","B.6.1.5.3","","Inlet structure","m³",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G32 * H32,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","f804d485-2cd1-4aed-b1a6-b155d9d69969","B.6.1.6","SANS 1200G 8.1.1\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","b01b85e4-7749-4648-80b3-8dbc17f16cb8","","8.2.1","Rough formwork",{"$nulls":4},"Dflt"]
["Item","53be510a-b9b2-4246-9f64-c52975106e43","B.6.1.6.1","","Where ordered by the Engineer","m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6145b1f0-bc9b-40e7-9a76-a561e45e5d60","","8.2.2","Smooth formwork (measured to 150 mm below finished ground level)",{"$nulls":4},"Dflt"]
["Label","51145273-f50d-4df6-925f-5238c81b040f","","","Plane vertical",{"$nulls":4},"Dflt"]
["Item","123e612d-838c-48a6-9e62-618780d5d440","B.6.1.6.2","","Ramps","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G38 * H38,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7e403854-1b08-44e1-be9d-7a00e6f8887d","","8.2.5","Vertical narrow widths up to 300mm wide",{"$nulls":4},"Dflt"]
["Item","5c436a8f-d00f-4e30-8e50-117a4d88cbce","B.6.1.6.3","","Inlet Structure (Stand-up walls)","m",40,{"v":0,"d":"0.00"},{"$f":"ROUND(G40 * H40,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","0fee4a7b-8ad8-4fbd-bcb4-04bf25ad7952","","8.1.1.2\nPSG 8.1.1.8","Chamfers exceeding 20mm x 20mm and grooves",{"$nulls":4},"Dflt"]
["Item","e0a8521f-e63b-4eec-937c-dd7afd033d95","B.6.1.6.4","","Chamfer 25mm x 25mm","m",35,{"v":0,"d":"0.00"},{"$f":"ROUND(G42 * H42,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","699814eb-2328-48b3-a402-7242a80d2dce","B.6.1.7","SANS 1200G 8.1.2","REINFORCEMENT ",{"$nulls":4},"Dflt"]
["Label","7eca58a7-2bfa-45ae-b77e-043999c5a6f9","","8.3.1","Mild Steel Bars:",{"$nulls":4},"Dflt"]
["Item","623e00fa-5ad9-41eb-be54-707a88361175","B.6.1.7.1","8.1.2.1","All diameter bars","t",0.1,{"v":0,"d":"0.00"},{"$f":"ROUND(G45 * H45,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6ad93d36-e8ba-4973-96b9-ec3dbc8cc311","","8.3.1","High-tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","14e8ea0b-3ce4-42f9-a8f2-d76eeed79bad","B.6.1.7.2","8.1.2.1","All diameter bars","t",0.2,{"v":0,"d":"0.00"},{"$f":"ROUND(G47 * H47,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","32a92a8d-9a15-46e5-8ecc-cbceaf196e28","","8.3.2","High-tensile welded mesh reinforcement:",{"$nulls":4},"Dflt"]
["Item","6fb747a8-3ead-46b4-b730-3935fbe19b94","B.6.1.7.3","8.1.2.1","High-tensile welded mesh ref 395","m²",95,{"v":0,"d":"0.00"},{"$f":"ROUND(G49 * H49,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","e101afec-c32f-491d-9198-a11f24769435","B.6.1.8","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","0c62b7fa-ab7b-4b0f-8489-8f6e776a98f6","","PSG 8.4","Wood-floated finish:",{"$nulls":4},"Dflt"]
["Item","dbd10d76-4d74-49c9-9c1b-f7be3174f0bd","B.6.1.8.1","","Ramps","m²",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","bd79b42c-6152-4bb4-ac43-2b6062aeee14","","8.1.1.5\nPSG 8.4","Steel-floated finish",{"$nulls":4},"Dflt"]
["Item","cb541cb5-552f-4f95-b1a3-ac9be163c582","B.6.1.8.2","","Inlet structure (Top of Walls)","m²",7,{"v":0,"d":"0.00"},{"$f":"ROUND(G54 * H54,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","8ded815c-d648-44e4-ada7-16505404e98e","B.6.1.9","SANS 1200G 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Item","afee573f-62af-4988-96d4-a959af10565d","B.6.1.9.1","","Finishing of joints in 300mm thick external walls complete, including preparation, 20mm joint filler and polyurethane sealant both sides, etc.","m",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G56 * H56,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","69f7b5df-03af-4ebe-ac4e-e2f6b3f8f7a1","B.6.1.10","SANS 1200L","MEDIUM PRESSURE PIPELINES",{"$nulls":4},"Dflt"]
["Header3","843029cd-0a32-4b2a-ab80-db94b7468fb8","B.6.1.10.1","SANS 1200DB","EXCAVATION AND BACKFILLING",{"$nulls":4},"Dflt"]
["Label","e50023eb-2cdf-41aa-9bf8-42f813b5b167","","8.3.2 (a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill and compact, including disposal of surplus unsuitable material for pipes up to 200 mm diameter for depths\nover   and   up to",{"$nulls":4},"Dflt"]
["Item","02ac0f23-c9c8-497a-b9f0-44c0ac99b216","B.6.1.10.1.1","","0.0 m          1.0 m","m",460,{"v":0,"d":"0.00"},{"$f":"ROUND(G60 * H60,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","f4bd9786-5aef-4b8e-8847-89fdb6d86206","B.6.1.10.2","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","1045f15a-6519-406a-8708-ab4d1b37e610","","","Make up deficiency in backfill material (Provisional)",{"$nulls":4},"Dflt"]
["Item","04d2b266-1a10-4e19-8f06-5143d2813101","B.6.1.10.2.1","8.3.3.1(a)","from other necessary excavations on site","m³",13,{"v":0,"d":"0.00"},{"$f":"ROUND(G63 * H63,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1d112193-55d1-47ba-b5cc-48906ef12038","B.6.1.10.2.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",13,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","eae7814a-e9cd-415a-aa43-8660f45216aa","B.6.1.10.3","SANS 1200L","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","a2e1d4a8-2058-4d62-a7ea-3d11723a62a4","","8.2.1","HDPE pipes, supply, handle, lay, join by butt welding, bed as for flexible pipe, test.",{"$nulls":4},"Dflt"]
["Item","3240d52e-b7a6-4bc1-8a8f-0883161d077c","B.6.1.10.3.1","","200mm diameter HDPE PE100 PN8","m",460,{"v":0,"d":"0.00"},{"$f":"ROUND(G67 * H67,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","a9290254-db4d-4e43-9c9e-c1b907aaebc5","","8.2.15\nPSL 8.2.15","Special wrapping in corrosive soil as per Project Specification PSL3.9.3.8 (Provisional)",{"$nulls":4},"Dflt"]
["Item","53bc6ced-70c1-4ade-8094-f1b5db9a3f99","B.6.1.10.3.2","","200 mm NB","No",80,{"v":0,"d":"0.00"},{"$f":"ROUND(G69 * H69,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","a7d504e6-3151-45de-9032-6a1cc4da1526","B.6.1.10.4","SANS 1200L","SPECIALS AND FITTINGS",{"$nulls":4},"Dflt"]
["Label","35368fe2-871b-4c98-87e1-b3416a4c2425","","8.2.5","Supply and fit, incl. bed, test and disinfect (if for potable water) pipes and specials: (Short pipe runs only)",{"$nulls":4},"Dflt"]
["Item","f420e0e3-ae40-47d6-8789-f6c521063771","B.6.1.10.4.1","","200mm diameter dismantling adaptor","No",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G72 * H72,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c702057f-c372-40a5-93e6-4226e41d3af6","B.6.1.10.4.2","","200mm diameter, mild steel extension pipe, plain ended. 350mm long.","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","975d9859-f309-4838-84b0-cbd95f46af83","B.6.1.10.4.3","","200mm diameter flange adaptor: Steel/Steel","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5d5e9535-f804-4126-983e-3a6079a4b98b","B.6.1.10.4.4","","200mm diameter, mild steel extension pipe, both ends flanged. 615mm long.","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c0478ae8-d2b6-4ea7-bc59-efa2fecfef98","B.6.1.10.4.5","","200 mm diameter, 90 degree short radius bend, both ends flanged.","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","dc35f70f-8318-43a0-baab-7b6901d7a946","B.6.1.10.4.6","","200mm diameter, mild steel extension pipe, both ends flanged. 285mm long.","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","69c137c7-ccd6-49b5-83a9-4f58a717f9db","B.6.1.10.4.7","","200 mm diameter, 90 degree short radius bend, one end flanged.","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","69d9c216-bee8-4cb2-9b8e-fd8601636e5b","","8.2.2","Supply and place pipes for and all the necessary fittings for clear effluent collection",{"$nulls":4},"Dflt"]
["Item","d932ec53-23eb-4303-9c65-856b84882a8d","B.6.1.10.4.8","","200 mm diameter, 90 degree bend (Electrofusion)","No",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G80 * H80,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b317f3db-35ff-4906-b657-c1e6450258ac","B.6.1.10.4.9","","200 mm diameter, Equal Tee (Electrofusion)","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","71a4da37-0d57-41ba-8974-3feba1de93d7","B.6.1.10.4.10","","200 mm diameter, Flange adaptor: Steel/HDPE","No",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","27e58918-39fd-4116-b161-91d57ce90e3e","B.6.1.10.4.11","","200 mm diameter, Equal Tee, Flanged on main ends and plain ended on take-off","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","28d3ec9b-ffa7-43b2-b675-78bf9c48a873","B.6.1.10.4.12","","200 mm diameter, End cap (Electrofusion)","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","c4a30e5b-0cbf-4cbb-abc0-b33d5cb56de7","B.6.1.10.5","SANS 1200L","VALVES",{"$nulls":4},"Dflt"]
["Label","100632d1-3463-4bac-9648-a1d10a3be318","","8.2.3","Supply, install on concrete support, joint, include cut pipes where necessary, test etc.",{"$nulls":4},"Dflt"]
["Label","7a4adeda-a28d-4c9a-a043-025eedc14f58","","","Flanged valves",{"$nulls":4},"Dflt"]
["Item","410857fe-1657-4ad6-8434-477c478d40c2","B.6.1.10.5.1","","200mm NB diam.","No",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G88 * H88,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","5e2fac68-a0d4-4c7e-81dc-f58629600a9b","B.6.1.10.6","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","4cb8cc5b-3511-4f64-aa97-93eaef790aee","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional)",{"$nulls":4},"Dflt"]
["Item","969c031d-b690-4e34-a235-b88b55b61550","B.6.1.10.6.1","8.2.2.3(a)","Selected granular material (cradle)","m³",155,{"v":0,"d":"0.00"},{"$f":"ROUND(G91 * H91,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e93fb1ce-ded6-41a5-a458-0a404e59de21","B.6.1.10.6.2","8.2.2.3(b)","Selected fill material (blanket)","m³",75,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","29f1ca2c-98ef-49a8-82de-5570092a652c","B.6.1.10.6.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3c37377c-2a07-4215-bfd5-daef500259e7","B.6.1.10.6.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","29e9e45a-9196-4492-bb20-0216da7805e6","B.6.1.10.7","","ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","092ca5e3-54d7-4fc0-9892-01b70284fa93","","SANS 1200L 8.2.11","Anchor/Thrust blocks and pedestals",{"$nulls":4},"Dflt"]
["Item","e29d5cbb-5e15-43a5-8644-0c3eb76ffed0","B.6.1.10.7.1","","Strength Concrete: 15 Mpa/19 mm ","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G97 * H97,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","76deb4e1-d02e-4fd2-9e1f-cc1b27dd2442","B.6.1.10.7.2","","Formwork: rough, vertical plane","m²",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","42ae0f2a-6f0f-48cd-a917-7f3a94281eba","B.6.1.10.7.3","SANS 1200LD 8.2.9\nPSL 8.2.19","Pipeline marker posts","No",14,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","e8b7daea-79d3-46ce-afd6-5acb8bb7401c","B.6.1.11","SANS 1200LD","SEWERS",{"$nulls":4},"Dflt"]
["Header3","2df26139-3117-47cd-89d6-ea4e28ac11b9","B.6.1.11.1","SANS 1200DB","EXCAVATION",{"$nulls":4},"Dflt"]
["Label","3439e233-5f47-4a03-a852-dcc99e5f40e8","","8.3.2(a)\nPSDB 8.1.4\nPSDB 8.3.2","Excavate in all materials for trenches, backfill, compact, and dispose of surplus/unsuitable material for pipes: 160mm diam. for total trench depth:\nExceeding but not Exceeding",{"$nulls":4},"Dflt"]
["Item","4d04be17-b609-4a5c-ba20-d95c9d1e2621","B.6.1.11.1.1","","0,0 m                       1,0 m","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G103 * H103,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0079323b-1d26-4e7b-8988-5f0bd217878c","B.6.1.11.1.2","","1,0 m                       2,0 m","m",235,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","ff4af70e-5411-42de-a08c-e408593b839c","B.6.1.11.2","SANS 1200DB","EXCAVATION ANCILLARIES",{"$nulls":4},"Dflt"]
["Label","67524187-0817-4c7d-9158-7742415aa46b","","","Make up deficiency in backfill material (Provisional)",{"$nulls":4},"Dflt"]
["Item","7fd902d6-c599-419d-9778-6da2a885abb8","B.6.1.11.2.1","8.3.3.1(a)","from other necessary excavations on site","m³",13,{"v":0,"d":"0.00"},{"$f":"ROUND(G107 * H107,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f5d33356-d4ea-4739-a330-b0f52f8a0e6d","B.6.1.11.2.2","8.3.3.1(c)","by importation from commercial sources selected by the Contractor","m³",13,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","866e2d7a-ef4a-44db-8a87-9b37623b0492","B.6.1.11.3","SANS 1200LD","PIPEWORK",{"$nulls":4},"Dflt"]
["Label","07aaeb60-f0ed-4b6d-a925-2d8a334d36fc","","8.2.1","Supply, lay, complete with spigot and socket joint to suit PVC pipe, bed class B and test PVC sewer pipes with couplings",{"$nulls":4},"Dflt"]
["Item","06e14f2c-f90e-49f0-a3d0-767ece5747cf","B.6.1.11.3.1","","160mm diameter class 34","m",265,{"v":0,"d":"0.00"},{"$f":"ROUND(G111 * H111,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","eae527cb-613f-45e8-96be-b66c4bc3e44d","","8.2.2","Extra-over Item B.6.1.11.3.1 for cutting ends of PVC sewer pipes to form closure pieces in pipeline including extra coupling (measured per cut end)",{"$nulls":4},"Dflt"]
["Item","f01c164f-2aea-476f-9343-48834685fa78","B.6.1.11.3.2","","160mm diameter class 34","No",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G113 * H113,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","e87d6e6c-bb42-4c10-87ea-2df9d3288b8b","B.6.1.11.4","SANS 1200LB","PROVISION OF BEDDING",{"$nulls":4},"Dflt"]
["Label","0eb2f741-4f14-4ca2-bda9-eaa6b581871f","","8.2.2\nPSLB 8.2.2 ","Provision of bedding from commercial sources (Provisional)",{"$nulls":4},"Dflt"]
["Item","5c9ea0bd-e460-446b-866b-14111d6235c5","B.6.1.11.4.1","8.2.2.3(a)","Selected granular material (cradle)","m³",45,{"v":0,"d":"0.00"},{"$f":"ROUND(G116 * H116,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c94bc229-5203-4c3b-bb55-08b098628f82","B.6.1.11.4.2","8.2.2.3(b)","Selected fill material (blanket)","m³",75,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d51cfb2b-81f3-42ab-8e0a-661e1f13d717","B.6.1.11.4.3","PSLB 8.2.6","19mm stone bedding where instructed (Provisional)","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d6044855-2440-4ead-a234-485fb851e4fc","B.6.1.11.4.4","PSLB 8.2.6","Geotextile fabric (Bidim A4) where instructed (Provisional)","m²",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","c97e173d-d3c8-48f5-9450-59184995f298","B.6.1.11.5","SANS 1200LD","MANHOLES, ETC.",{"$nulls":4},"Dflt"]
["Label","71c5a29a-f12f-4244-ae6e-1926ad38ecb8","","8.2.3\nPSLD 8.2.3","Precast concrete manholes, with Type 1A Heavy Duty polyprop lockable manhole cover and frame, as per Dwg. No. J40073/010-219:\nover   and   up to"]
["Item","641eff4f-9b21-4abe-ace6-2439ad2c417f","B.6.1.11.5.1","","0,0 m          1,0 m","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G122 * H122,2)","v":{"v":0,"d":"0.00"}}]
["Item","6568dc60-e4ff-43de-8bde-23cd84a26ce3","B.6.1.11.5.2","","1,0 m          2,0 m","No",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Header3","3cf2e2b9-63d7-418c-8ce6-a1bf8cfcf4dd","B.6.1.11.6","SANS 1200LD","SUNDRIES"]
["Item","ec8c9c1c-46bd-47fb-81f8-448331f9496f","B.6.1.11.6.1","SANS 1200LD 8.2.11\nPSLD 8.2.11","Break into and connect to existing manhole at SDB-02 including flexible joints as Dwg. No. J40073/010-219 and make good all benching.","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G125 * H125,2)","v":{"v":0,"d":"0.00"}}]
["Item","f23df048-bee5-4555-b8d0-539701b004d5","B.6.1.11.6.2","","Supply, install precast manhole slabs complete with Type 1A Heavy Duty polyprop lockable manhole cover and frame to fit existing pre-cast concrete manhole rings as per Dwg. No. J40073/010-219","No",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]

{"sheet":"BILL B.7.","index":7,"n_rows":355,"n_cols":10,"rows_kept":355,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.7.",null,"PUMP STATIONS",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","e3f3f83a-455e-4eb0-bedd-f0227493d4f5","B.7.1","","RAW WATER AND IRRIGATION PUMP STATION EARTHWORKS ",{"$nulls":4},"Dflt"]
["Label","4af7bb42-40c3-4e49-9a8f-1b14af39ba75","","","SECTION B.7.1 : RAW WATER AND IRRIGATION PUMP STATION EARTHWORKS ",{"$nulls":4},"Dflt"]
["Header2","c31f9abc-745e-4f0a-a728-d9a81ad44561","B.7.1.1","","EARTHWORKS ",{"$nulls":4},"Dflt"]
["Header3","321c414c-afe7-4272-bd10-0ef37962a8ad","B.7.1.1.1","SANS\n1200C\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","49d55ae2-f5d1-4f29-87ea-f1ffb9e2215c","B.7.1.1.1.1","8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",200,{"v":0,"d":"0.00"},{"$f":"ROUND(G13 * H13,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","abb51ee8-0546-4f85-afd3-9cb1b55bc3a0","B.7.1.1.1.2","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","376e8924-9458-44ec-a70f-9401be3461d4","B.7.1.1.2","SANS 1200D 8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Item","74fc788e-3d0e-4a77-b59c-febc7097cfdb","B.7.1.1.2.1","8.3.1.2\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",407,{"v":0,"d":"0.00"},{"$f":"ROUND(G16 * H16,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","bf8be4dd-aefe-4928-aaa8-4ac7e5c84f6a","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Item","06452aa4-c682-45ae-9a19-33b3be0cabcb","B.7.1.1.2.2","","Raw Water Pump Station","m³",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G18 * H18,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","616fd378-ddbb-40b1-a177-70d6613cda32","B.7.1.1.2.3","","Irrigation Pump Station","m³",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a773544a-f64f-40bc-99ef-fdd239db2126","B.7.1.1.2.4","8.3.3\nPSD 8.1.3","Restricted excavation for foundations and footing in all material and dispose of surplus/unsuitable material as ordered within the free haul distance","m³",60,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","978f625c-023c-4e41-b3af-2c3c8ab3948c","","8.3.2(a)","Backfill (min G7 classified material)to 95% MOD AASHTO behind structures for:",{"$nulls":4},"Dflt"]
["Item","41c78228-ae47-460d-a149-5c53b5e161d1","B.7.1.1.2.5","","Raw Water Pump Station","m³",700,{"v":0,"d":"0.00"},{"$f":"ROUND(G22 * H22,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","30ba779e-11b8-4f85-8d5e-e90e9555868f","B.7.1.1.2.6","","Irrigation Pump Station","m³",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","7010ddff-5312-4bd6-a680-8f99750991b6","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","22afd3bc-1aa8-45b6-b6fa-3b55ffd58d08","B.7.1.1.2.7","","Raw Water Pump Station","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G25 * H25,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Item","a8e12c6a-aafc-4312-87e9-9bf68e776148","B.7.1.1.2.8","","Irrigation Pump Station","Prov.Sum",0,{"v":5000,"d":"5,000.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","a7bc92f4-157c-482d-b187-489aea7dd686","B.7.1.1.3","SANS 1200D 8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.7.1.1.2.2 to B.7.1.1.2.4 for excavation in:",{"$nulls":4},"Dflt"]
["Item","e1a3f923-b754-4780-8258-f567bc09b3fe","B.7.1.1.3.1","8.3.2(b)","Hard rock material","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G28 * H28,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","3a1a4482-2d7c-4127-bc35-26daee162852","B.7.1.1.4","SANS 1200D 8.3.4","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","07a63343-f0fa-48c6-b257-80222574b17d","B.7.1.1.4.1","","Extra-over items B.7.1.1.2.5 to B.7.1.1.2.6 for importation of material to complete embankment for the Raw Water Pump Station and Irrigation Pump Station from commercial sources where necessary: G7 material (Prov.)","m³",975,{"v":0,"d":"0.00"},{"$f":"ROUND(G30 * H30,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","6ab2cc9a-9d00-45cc-bfce-bc442a702f55","B.7.1.1.5","SANS 1200D 8.3.7","ADDITIONAL LATERAL SUPPORT",{"$nulls":4},"Dflt"]
["Label","80a1f484-bd95-41a9-845b-d143f9517273","","8.3.7","Additional lateral support  (Provisional) for ensuring the stability of the excavation:",{"$nulls":4},"Dflt"]
["Item","eae1579d-e1c2-4118-805c-7934c8331da4","B.7.1.1.5.1","","Raw Sewage Pump Station","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G33 * H33,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ae285c24-8d16-42f0-9b14-98c6765f2e68","B.7.1.1.5.2","","Irrigation Pump Station","m²",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","83072b13-b1a1-4d39-9a58-c01b548ed863","B.7.1.1.6","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","6c3aae75-16d5-4493-ba0c-b264553120c0","B.7.1.1.6.1","8.3.10","Topsoiling","m²",407,{"v":0,"d":"0.00"},{"$f":"ROUND(G36 * H36,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f27b4283-3bd1-4235-9fe0-12e6e981227b","B.7.1.1.6.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc as necessary and wetting","m²",402,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Section","e500fdbe-00cc-481b-a2c2-6c18e60e3841","B.7.2","","RAW WATER PUMP STATION",{"$nulls":4},"Dflt"]
["Label","c4c191f6-0832-410f-b446-6cb1596e9c21","","","SECTION B.7.2 : RAW WATER PUMP STATION",{"$nulls":4},"Dflt"]
["Header2","71fc7429-702e-493c-acd5-b70b80d667c7","B.7.2.1","SANS 1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","de1c7e97-7d1b-428d-85cf-77594e1ecf41","","8.4.3","Strength concrete:\n20 MPa/19mm:",{"$nulls":4},"Dflt"]
["Item","e8febb57-874f-47a0-8060-e4d3c5d536d7","B.7.2.1.1","","Benching","m³",21,{"v":0,"d":"0.00"},{"$f":"ROUND(G42 * H42,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6e60a6ed-4cb0-4190-aa55-fd5c835af772","","8.4.3","Strength concrete:\n15 MPa/19mm:",{"$nulls":4},"Dflt"]
["Item","d15993dc-d0e8-404d-8767-a216cb9d303c","B.7.2.1.2","","Thrust blocks and pump plinths","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G44 * H44,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","69c0c634-8c40-429e-921d-dc9649ae1001","","8.4.3","Strength concrete:\n35 MPa/19mm:",{"$nulls":4},"Dflt"]
["Item","93ea1154-a0f0-43d7-9c04-e03b7e4eec14","B.7.2.1.3","","Roof slabs and upstand beams","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G46 * H46,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","589bcd49-fbea-4059-b0fc-4e57fbf0ba3f","B.7.2.1.4","","Access Ramps","m³",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","59436ee4-3b7c-4290-95b6-a3b6fa2d9caf","B.7.2.1.5","","Columns","m³",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","b3099828-4b03-4504-9877-83488ae391ca","","","Screeds:",{"$nulls":4},"Dflt"]
["Item","4abbfa5d-50e4-4ed7-92fb-dc45201070ab","B.7.2.1.6","PSG 8.11","Mortar floor screed (1:3 cement:sand), average 35 mm thick ","m²",190,{"v":0,"d":"0.00"},{"$f":"ROUND(G50 * H50,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","11aeba4c-259c-4ff9-9fcf-aec527263da5","B.7.2.2","SANS 1200G 8.2\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","6dcb6f10-1652-40e2-bf78-fffaccab4994","","8.2.2","Smooth horizontal plane:",{"$nulls":4},"Dflt"]
["Item","2dd30a87-8b85-430a-ada1-c3167e69cc8e","B.7.2.2.1","","Upstand Beam","m²",33,{"v":0,"d":"0.00"},{"$f":"ROUND(G53 * H53,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f03e31fe-8dc0-4758-9582-bbe47e906bd7","B.7.2.2.2","","Column","m²",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","41faff59-29a3-4b0e-a430-66ce1d709c92","B.7.2.2.3","","Sides and beams","m²",39,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","7ec9cbba-f6b7-449a-9a07-81ee790488e6","","8.1.1.2\nPSG 8.1.1.8","Chamfers exceeding 20mm x 20mm and grooves:",{"$nulls":4},"Dflt"]
["Item","27e7f154-3ec0-4f39-96b6-502838f87315","B.7.2.2.4","","Chamfer 25mm x 25mm","m",47,{"v":0,"d":"0.00"},{"$f":"ROUND(G57 * H57,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c738ab83-c50e-4e04-8c73-d3329a0ee20c","B.7.2.2.5","","Sides of access ramps","m",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","b51750c7-792d-4f33-8be6-39be4c93b935","","8.2.6","Box Out Holes/Form Voids:",{"$nulls":4},"Dflt"]
["Label","959fd39d-35af-40ee-a427-a52ad5f00bcd","","PSG 8.10","Casting of pipes/specials into concrete for:",{"$nulls":4},"Dflt"]
["Label","7c771bf2-1845-47ea-85b9-68a127402189","","","Pipes up to and including 450 mm NB through walls of thickness:",{"$nulls":4},"Dflt"]
["Label","b3ea93b6-f154-401c-a910-3585be88cbab","","","Over (m)         Up to and incl (m)",{"$nulls":4},"Dflt"]
["Item","792f8eb8-f222-4461-b15d-78f1b6f1b1b6","B.7.2.2.6",""," 0.00                   0.45","No",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G63 * H63,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f6740af9-50e4-47a9-981c-f64d05fc8629","","","Pipes over 300 mm NB up to and including 600 mm NB through walls and slabs of thickness:",{"$nulls":4},"Dflt"]
["Label","ed5a9485-a8f6-4c4e-91fc-bc8df6fe01dc","","","Over (m)         Up to and incl (m)",{"$nulls":4},"Dflt"]
["Item","2f09fdda-b182-460e-b2d9-6f5a97d01974","B.7.2.2.7",""," 0.00                   0.45","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G66 * H66,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","517f5b9a-93e4-458c-928e-4b50511a2ede","","","Pipes over 600 mm NB up to and including 800 mm NB through walls and slabs of thickness:",{"$nulls":4},"Dflt"]
["Label","35e6f4ff-7a17-4895-8f67-f3b0c2e6f4f3","","","Over (m)          Up to and incl (m)",{"$nulls":4},"Dflt"]
["Item","1d008af3-7c69-4216-a0a8-a21483b1b868","B.7.2.2.8",""," 0.00                    0.45","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G69 * H69,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","572a872c-9af2-429d-8e2c-a2b04de5971e","","","Pipes over 800 mm NB up to and including 1000 mm NB through walls and slabs of thickness:",{"$nulls":4},"Dflt"]
["Label","1144cbd5-a2a6-41ab-a9b8-e9b892eef7e9","","","Over (m)          Up to and incl (m)",{"$nulls":4},"Dflt"]
["Item","ddd8c60a-85cb-4ca0-b22e-d3acd1671c4a","B.7.2.2.9",""," 0.00                    0.50","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G72 * H72,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","5ba36439-685f-4aab-a5e6-4d7fa9f3e88d","B.7.2.3","SANS 1200G 8.1.2\nPSG 8.1.2","REINFORCEMENT ",{"$nulls":4},"Dflt"]
["Label","58a13fbc-448a-4f26-8312-8b1f049314d9","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","43fe4064-05a7-4e85-8705-a64f9df732b1","B.7.2.3.1","","25 mm diameter: Basic price","t",2.7,{"v":0,"d":"0.00"},{"$f":"ROUND(G75 * H75,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5490ec83-c583-4339-b999-e2607e225e11","","8.1.2.3(b)","Extra-over item B.7.2.3.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","449d9884-e47d-430e-a9ec-0e1307c3b3e9","B.7.2.3.2","","10 mm","t",0.26,{"v":0,"d":"0.00"},{"$f":"ROUND(G77 * H77,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","010fa81b-f91d-4972-8e41-8c2883b31455","B.7.2.3.3","","12 mm","t",0.07,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","55afddbb-21e8-44a3-9bb7-041911f00959","B.7.2.3.4","","16 mm","t",0.6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ac977919-b313-4b93-9cbb-a056c50d98df","B.7.2.3.5","","20 mm","t",0.4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","e08cdc64-5d08-4b76-a53b-a4918228e342","B.7.2.4","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","4f8f3c96-0d9c-4857-a4a3-d4ba7b41bcca","","8.1.1.5\nPSG 8.4","Steel-floated finish:",{"$nulls":4},"Dflt"]
["Item","193c03dd-b89a-4ebc-a923-54d91fc1a755","B.7.2.4.1","","Top of upstand beam","m²",43,{"v":0,"d":"0.00"},{"$f":"ROUND(G83 * H83,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","795c6c89-2331-42f8-95ef-e283bd727d2f","B.7.2.5","SANS 1200 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Label","1b64fad5-42b8-430f-8e99-5290b6bd4a8b","","","Expansion joints:",{"$nulls":4},"Dflt"]
["Item","37238dfc-03c0-4753-b994-a8f5eabf357e","B.7.2.5.1","","Joints in screed not exceeding 250mm (at expansion joints in the floor slabs) with 10mm thick any approved filler","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G86 * H86,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0eaf16b0-aa97-4920-9cd8-f15e5d042005","B.7.2.5.2","","Corner fillet","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d0a57cb3-2917-4baa-aa34-6db54192b457","B.7.2.5.3","","Brickwork Control joint at the Column interface","m",95,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3d142094-5aae-4368-857f-0ff0ee380a16","B.7.2.5.4","","Slip joint between brickwork and the roof","m",21,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","15eca808-ec65-470d-9fd1-5fde4bd23366","B.7.2.6","","STRUCTURAL STEELWORK (SUNDRY ITEMS) (Refer SANS 1200 HA)",{"$nulls":4},"Dflt"]
["Label","fc9a9121-987d-4365-9835-3c9315f8b41c","","","Supply and install crawl beam in raw water pump station complete, including supply, fitting, corrosion protection, testing, certification, etc. as shown on Dwg. No. J40073/010-204:",{"$nulls":4},"Dflt"]
["Item","c2926825-769b-4b0d-a181-cb24f2b740ef","B.7.2.6.1","","Crawl Beam","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G92 * H92,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","0a1017d1-e5df-4e9b-ad97-e07807505635","B.7.2.7","","MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Item","4229eb84-a1d5-4202-b376-aedf78330799","B.7.2.7.1","","Calcamite type step irons, staggered at 300 mm c/c ","No",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G94 * H94,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","4d284ab6-9c87-456a-bb0c-b7a585f605cf","B.7.2.8","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","0e7aebb5-904f-4472-8cc1-a3d9614b8b15","","","Water Tightness Testing:",{"$nulls":4},"Dflt"]
["Sum","ab97d4c3-c421-4081-a412-d51f21396a74","B.7.2.8.1","PSG 8.12","Testing for Water Tightness, all inclusive to PSG 7.2.5","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H97,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6d46880b-8102-4ec8-a81b-d3d14ae36104","","","Corrective work to Raw Water Pump Station",{"$nulls":4},"Dflt"]
["Sum","3e92e0e2-64d1-4e85-9ee3-558f39e4fddb","B.7.2.8.2","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":1000000,"d":"1,000,000.00"},{"$f":"ROUND(H99,2)","v":{"v":1000000,"d":"1,000,000.00"}},"Dflt"]
["Header2","d242d36d-b679-48e7-aa50-ab333266cc4a","B.7.2.9","","BUILDING WORKS FOR THE RAW WATER PUMP STATION",{"$nulls":4},"Dflt"]
["Label","59e08530-b65a-42b1-8636-d31fa44fee88","","","Surface preparation:",{"$nulls":4},"Dflt"]
["Item","cf0ceecf-0c4f-47aa-a752-88d6beb9a1c2","B.7.2.9.1","","Brickwork in face (outside face) and stock bricks (inside face) to 230 mm external walls","m²",63,{"v":0,"d":"0.00"},{"$f":"ROUND(G102 * H102,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ec6c3043-6cbb-4f73-91cc-dc74211bacc5","B.7.2.9.2","","Brickforce","m",343,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","170c5179-230e-4050-a1e1-447a52458dc2","B.7.2.9.3","","Hoop iron ties shot onto concrete","No",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","54040bce-91c3-42fc-b158-d73c3e203611","","","Brickwork in stock bricks to:",{"$nulls":4},"Dflt"]
["Item","aec07306-4b24-497b-a57a-10689f8e95f1","B.7.2.9.4","","500 mm wide by 500 mm high louvered vent","No",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G106 * H106,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6df55e53-67aa-4c08-ba5b-82989fc1691c","B.7.2.9.5","","Slate internal window sills (180 mm x 25 mm)","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1483e441-176a-479f-af48-9ab7e2c79f87","B.7.2.9.6","","Brick-on-edge external window sills","m",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","129e54ea-c3d9-4202-880f-9518e0bdf60f","","","Damp proof courses and membranes:",{"$nulls":4},"Dflt"]
["Item","cdf1827c-a865-4815-a637-ce12913633b9","B.7.2.9.7","","375 micron embossed black polyethelene to brickwork 230 mm wide","m",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G110 * H110,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","783d5d15-c226-452e-afe2-336556cb2097","B.7.2.9.8","","Plastering, 12 mm thick to internal brick walls","m²",130,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","12bf13cd-5bbe-4f4a-8369-5fec5edddab4","","","Painting:",{"$nulls":4},"Dflt"]
["Item","46467334-39c3-4122-9e44-2d6b3300ea15","B.7.2.9.9","","Internal plastered surfaces (acrylic emulsion)","m²",225,{"v":0,"d":"0.00"},{"$f":"ROUND(G113 * H113,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","22175121-aacb-4e0f-b53a-ac2450cc2da8","B.7.2.9.10","","Fascias and barge boards (acrylic emulsion","m",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","701ef929-0cba-4e9f-a7aa-88c1812b61cb","","","Doors and windows (including frames and glass):",{"$nulls":4},"Dflt"]
["Item","f9e7fa26-967e-46a7-82b8-fe60880de70a","B.7.2.9.11","","Doors complete including supply, fitting, corrosion protection and painting as per Dwg. No. J40073/010-204","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G116 * H116,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c6a2a672-e2b7-4411-a5eb-fa9b1099778e","B.7.2.9.12","","1200 mm wide x 900 mm high Anodized Aluminium sliding window CAT. No 129 and fitted with obscure glass, flyscreen and burglar bars (similar to installation in Admin Building) to be approved by the Engineer prior to arrival on site.","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","de62cd3e-dd07-4c0b-9ba8-089792a7dfef","B.7.2.9.13","","Ceiling boards and insulation","m²",175,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","790309b2-fc5b-4c28-8451-7f8cebd83749","","","Corrugated Iron Sheeting with Timber trusses roofing to:",{"$nulls":4},"Dflt"]
["Item","2fd8db53-11d6-496f-a6af-e9366d862e13","B.7.2.9.14","","Raw Water Sewage Pump station","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G120 * H120,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","34874d00-269b-40d8-890d-9a003d1a7015","","","Whirly Bird Roof ventilators or similar product for: ",{"$nulls":4},"Dflt"]
["Item","bffcb676-e12c-4701-aa41-f73e0500eced","B.7.2.9.15","","Pump station","No",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G122 * H122,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Section","43e8f79d-f79f-4007-a418-905ad0637a0c","B.7.3","","PUMP STATION (IRRIGATION)",{"$nulls":4},"Dflt"]
["Label","c9e29578-b1e5-48bc-9c82-a3579f20770b","","","SECTION B.7.3 : PUMP STATION (IRRIGATION)",{"$nulls":4},"Dflt"]
["Header2","37865c80-5be1-4d6d-a3ba-b6dd8e86aa6d","B.7.3.1","SANS 1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","72d59f4d-3cfb-4d45-8c28-43b0ba73a8ea","","8.4.2","Blinding layer:\n15 MPa/19 mm concrete:",{"$nulls":4},"Dflt"]
["Item","25e03b14-f6c2-417a-a34a-a76eac81a317","B.7.3.1.1","","50 mm minimum thickness","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G127 * H127,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9d55a11a-1991-4664-afeb-6b837f78a2e2","","8.4.3","Strength concrete:\n15 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","a9e9c7dd-7393-4ebc-8f0d-47c7ec1765a1","B.7.3.1.2","","Thrust blocks and pump plinths","m³",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G129 * H129,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8ce08289-bfb4-4361-8309-a814b0b13bb6","","8.4.3\nPSG 3.5.4","Strength concrete (Inclusive of Crystalline Water Proofing additive):\n35 MPa/ 19mm:",{"$nulls":4},"Dflt"]
["Item","2e6eb868-0718-49b3-ac85-3bcf1e3101b6","B.7.3.1.3","","Floor slabs","m³",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G131 * H131,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","451e1e95-986d-47ae-b2eb-2965f237e8c0","B.7.3.1.4","","Walls ","m³",23,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2e3d5a38-4863-4441-b318-981b1d0b114e","B.7.3.1.5","","Roof slabs","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","6f2ffee5-df9c-46ee-a508-ecc08c767000","","8.4.3","Soilcrete:\n3 MPa:",{"$nulls":4},"Dflt"]
["Item","b53faf40-3d01-4b18-9a85-c35bafeebaba","B.7.3.1.6","","Mass soilcrete as shown on \nDwg. No. J40073/010-220","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G135 * H135,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6ded1b9b-d4e3-4533-b53d-521c7fd843f0","","8.4.3","Strength concrete:\n20 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","92f472a0-8e3f-4977-9927-beff83682f37","B.7.3.1.7","","Benching","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G137 * H137,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","951f66d4-df5b-4ef3-a04e-35fea86b04a2","","","Screeds:",{"$nulls":4},"Dflt"]
["Item","5d2b2495-88ad-4f75-922d-4fa8134504d7","B.7.3.1.8","PSG 8.11","Mortar floor screed (1:3 cement:sand), average 35 mm thick ","m²",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G139 * H139,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","e7b04cf0-f084-46c2-a91d-9f299ea72e0b","B.7.3.2","SANS 1200G 8.2\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","0fc164c3-8c6e-4de6-9306-6a7b42cf5874","","8.2.2","Smooth vertical plane:",{"$nulls":4},"Dflt"]
["Item","48c235bd-b1bf-4a09-82fe-62ad3b16c012","B.7.3.2.1","","Walls","m²",169,{"v":0,"d":"0.00"},{"$f":"ROUND(G142 * H142,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","65c1d1f6-f43a-406e-9f2f-5a4a541e295e","B.7.3.2.2","","Columns","m²",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","953be329-afb9-4cfb-af88-d085b943c037","","8.2.2","Smooth horizontal plane:",{"$nulls":4},"Dflt"]
["Item","98df6ad2-be44-4497-892a-c98e8625f189","B.7.3.2.3","","Soffit of roof slab","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G145 * H145,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","40220ed3-6e6a-4503-8cf0-061834998767","","8.2.5","Vertical narrow widths up to\n300 mm wide:",{"$nulls":4},"Dflt"]
["Item","dbfb4976-68f1-412f-9719-3c8f9b871cdb","B.7.3.2.4","","Edge of footings","m",39,{"v":0,"d":"0.00"},{"$f":"ROUND(G147 * H147,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c706a431-62e0-4cae-9a74-d228986b9bb3","B.7.3.2.5","","Smooth, vertical, plane to roof slabs","m",64,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","c3c7fb5c-751e-4f8a-ae8d-b91c5818b3c9","","8.1.1.2\nPSG 8.1.1.8","Chamfers exceeding 20mm x 20mm and grooves:",{"$nulls":4},"Dflt"]
["Item","796a18a8-440c-407e-9c63-72dade52dd38","B.7.3.2.6","","Chamfer 25 mm x 25 mm","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G150 * H150,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","fba947e7-f2d7-4fd8-8879-922ec6faf333","","8.2.6","Box Out Holes/Form Voids:",{"$nulls":4},"Dflt"]
["Label","41ed53d1-b12b-4fc5-96cf-7c98cfe23b72","","","Small, circular up to 0,35 m diam.:\ndepths\nover     and     up to",{"$nulls":4},"Dflt"]
["Item","6f575b3e-9149-4680-886b-91774b436cc1","B.7.3.2.7","","0 m                  0,5 m","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G153 * H153,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","278ecec3-27ef-425a-8765-f34ebf54cd84","","","Large, other shapes, area 1,0 m² - 1,5 m²:\ndepths\nover     and     up to",{"$nulls":4},"Dflt"]
["Item","2e1364f3-a5f0-4716-adba-b6985ad939f2","B.7.3.2.8","","0 m                  0,5 m","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G155 * H155,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","315fa57b-0f72-4772-a85b-03e0d8bf47b4","","PSG 8.10","Casting of pipes/specials into concrete for:",{"$nulls":4},"Dflt"]
["Label","088ab359-d7f7-4299-bb7b-c58137d50e63","","","Pipes up to and including 450 mm NB through walls:\ndepths\nover     and     up to",{"$nulls":4},"Dflt"]
["Item","935eef5a-f15e-4d3c-94ea-a2a82cd9946e","B.7.3.2.9","","0 m                  0,5 m","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G158 * H158,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","b50ffe68-fe02-478c-887c-b024ecd740e6","B.7.3.3","SANS 1200G 8.1.2\nPSG 8.1.2","REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","68dde8a7-d9de-49ae-8f82-b0962c018d91","","8.1.2.3(a)","Mild steel bars:",{"$nulls":4},"Dflt"]
["Item","b4047174-013b-49e3-b464-d94c1718439f","B.7.3.3.1","","25 mm diameter: Basic price","t",0.062,{"v":0,"d":"0.00"},{"$f":"ROUND(G161 * H161,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","4e654828-da78-4110-8c37-aa8c7c7cd98b","","8.1.2.3(b)","Extra-over item B.7.3.3.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","b4fcf40a-d3d5-414a-be4f-ff675c964399","B.7.3.3.2","","8 mm","t",0.039,{"v":0,"d":"0.00"},{"$f":"ROUND(G163 * H163,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","090a4f77-ebeb-4857-ba07-2d98245bcc95","B.7.3.3.3","","10 mm","t",0.023,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","e97ef532-c7e6-4ae5-b73e-b2344effb5d2","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","44ed974d-587a-45a5-a06b-f18e0622177b","B.7.3.3.4","","25 mm diameter: Basic price","t",7.31,{"v":0,"d":"0.00"},{"$f":"ROUND(G166 * H166,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","ec2ff005-47da-4472-9172-b98e7bd2c7a3","","8.1.2.3(b)","Extra-over item B.7.3.3.4 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","1b16ee79-6a95-4d92-88a9-188f95423f84","B.7.3.3.5","","10 mm","t",0.29,{"v":0,"d":"0.00"},{"$f":"ROUND(G168 * H168,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ef0f6cb3-40f0-4c2c-a6fd-6ab89522656a","B.7.3.3.6","","12 mm","t",3.83,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a60f5c0d-3cef-4672-a9db-2b9c45cb45fb","B.7.3.3.7","","16 mm","t",3.15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","1da59957-bca0-4e98-ae42-afdf5d419ed7","B.7.3.4","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","9ff1fecb-ef03-4b0a-8aa3-027e337f0112","","PSG 8.4","Wood-floated finish:",{"$nulls":4},"Dflt"]
["Item","ded34921-bd7c-4930-a7dc-a57c42122f7e","B.7.3.4.1","","Top of floor slabs","m²",29,{"v":0,"d":"0.00"},{"$f":"ROUND(G173 * H173,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","38f97d89-035d-47d2-a0b1-c4ab2e58a32f","","8.1.1.5\nPSG 8.4","Steel-floated finish:",{"$nulls":4},"Dflt"]
["Item","fa83c8e2-9276-449e-89f7-edda68fe5e6b","B.7.3.4.2","","Top of roof slabs","m²",23,{"v":0,"d":"0.00"},{"$f":"ROUND(G175 * H175,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","e10ba2a7-e20b-40f6-8220-0ecea3128e27","B.7.3.5","SANS 1200G 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Item","e9344096-d7d7-4cfe-ac74-430da6ac5715","B.7.3.5.1","","2 mm thick X 200 mm wide galvanised water stop in walls (overlapping length at least 300 mm)","m",51,{"v":0,"d":"0.00"},{"$f":"ROUND(G177 * H177,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7f595c22-9597-4c23-b449-e728b11806f8","","","Expansion joints:",{"$nulls":4},"Dflt"]
["Item","e7c9fd05-2a49-4bb8-98e7-1061e467d3a2","B.7.3.5.2","","Joints in channel wall complete with PVC water stop, 12mm joint filler and polyurethane sealant both sides","m",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G179 * H179,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","07fb7d1d-ff59-44de-a5e4-849a035eec65","B.7.3.6","SANS 1200H","STRUCTURAL STEELWORK:\nSUNDRY ITEMS",{"$nulls":4},"Dflt"]
["Label","0fe11959-642f-434f-b621-884e086c754f","","8.3.9","Open grid floors:",{"$nulls":4},"Dflt"]
["Label","d2785e07-2c7b-4b5d-bd60-ead4ce67c10a","","","a) Steel floors and steps complete and installed with frames and wall fixings to Dwg. Nos. J40073/010-105 and J40073/010-220:",{"$nulls":4},"Dflt"]
["Item","03936547-c578-44d7-bfae-5461a1a78dff","B.7.3.6.1","","50 x 50 x 5 mm thick galvanised angles cast into slabs (Grating by others)","m",40,{"v":0,"d":"0.00"},{"$f":"ROUND(G183 * H183,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","850c19a9-aec5-4f44-b1d6-1f85d518028a","B.7.3.7","","MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Item","029b13ee-435f-4d58-825a-b909c9d69c68","B.7.3.7.1","","Calcamite type step irons, staggered at 300 mm c/c ","No",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G185 * H185,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","a6767386-0415-4325-a24f-50399798b77c","B.7.3.8","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","c7c65622-19ba-416d-8b5b-616ac3ccfd42","","","Water Tightness Testing:",{"$nulls":4},"Dflt"]
["Item","ed7dd8f3-bc77-49d9-b1f6-f7b7c3af1dca","B.7.3.8.1","PSG 8.12","Testing for Water Tightness, all inclusive to PSG 7.2.5","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G188 * H188,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Section","3d680f8b-31bb-4264-ba3f-b9c60b13e64f","B.7.4","","WASTE ACTIVATED SLUDGE (WAS) PUMP STATION",{"$nulls":4},"Dflt"]
["Label","48f469d2-11f7-4c10-9128-7e016a733099","","","SECTION B.7.4 : WASTE ACTIVATED SLUDGE (WAS) PUMP STATION",{"$nulls":4},"Dflt"]
["Header2","d5963828-a6f2-42e5-a861-52ff02fc825b","B.7.4.1","SANS 1200D","EARTHWORKS",{"$nulls":4},"Dflt"]
["Item","3c1f2e0a-58b1-45ec-a4b9-43dfecb24480","B.7.4.1.1","8.3.1.2 PSC8.2.10\n","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",185,{"v":0,"d":"0.00"},{"$f":"ROUND(G192 * H192,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","41d788e8-2c56-4762-b0bf-a550e21bb496","B.7.4.1.2","8.3.2","Bulk Excavation",{"$nulls":4},"Dflt"]
["Item","812c2e04-5243-4371-8635-8fb188607a17","B.7.4.1.2.1","8.3.2 (a)","Excavate in all materials and use for backfill or dispose as ordered","m³",180,{"v":0,"d":"0.00"},{"$f":"ROUND(G194 * H194,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c6444f19-22f0-422f-8253-a74191f7717c","B.7.4.1.2.2","8.3.2 (b)      PSD8.3.2 (b)","Extra-over items B.7.4.1.2.1 for excavation in hard rock material","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","c39749b4-bd2a-4cdb-a4aa-1997fca255a6","B.7.4.1.3","8.3.3","Restricted Excavation",{"$nulls":4},"Dflt"]
["Item","bb4e333e-9ca1-47ac-942e-774b489b913b","B.7.4.1.3.1","8.3.3 (a)","Excavate for restricted foundations and footings in all materials and use for backfill or dispose","m³",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G197 * H197,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a5737ada-bab9-4b21-a481-ec16ce4aefa4","B.7.4.1.3.2","8.3.3 (b)","Extra-over items B.7.4.1.3.1 for excavation in hard rock material","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","a549a00f-7841-4eac-89db-734577cb2a07","B.7.4.1.4","8.3.4","Importing of Materials",{"$nulls":4},"Dflt"]
["Item","7859d9fe-818f-49da-b143-416042555cc2","B.7.4.1.4.1","","a) Extra-over for importation from commercial sources of G7 subgrade quality material placed in 150 mm layers and compacted to 95% MOD AASHTO density","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G200 * H200,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c593a0ed-1db7-4d9a-9e96-65cfb95c3c70","B.7.4.1.4.2","","a) Extra-over for importation from commercial sources of G5 quality material placed in 150 mm layers and compacted to 98% MOD AASHTO density","m³",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","802d6342-fb1c-4df2-8627-c132daf8124b","B.7.4.1.4.3","","Extra-over on B.7.4.1.3 for stabilizing with 2% cement including supply of cement","m³",31,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","382ebc07-9f7f-4b8a-bf67-04b9e2148dc5","B.7.4.1.4.4","8.3.5","Excavation in all material to provide working space around structure","m²",135,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","2ad9616e-2ae2-41ae-b7d5-a22b8e8ce4a4","B.7.4.1.5","8.3.6","Overhaul",{"$nulls":4},"Dflt"]
["Item","97edd797-5b3d-4eae-9000-3b2084fade73","B.7.4.1.5.1","PSD 8.3.6","a) Limited overhaul","m³",180,{"v":0,"d":"0.00"},{"$f":"ROUND(G205 * H205,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5fefd713-69d2-4b21-9c1a-1d9132c1aca0","B.7.4.1.5.2","","b) Long overhaul","m³.km",150,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4fac0f1d-5237-4147-a5de-bb97fbc3963a","B.7.4.1.5.3","8.3.7             PSD 8.3.15","Additional lateral support for existing structures around Waste Activated Sludge Pump Station","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","4a3f96f4-3bcf-435a-a9df-3ea01109f3a9","B.7.4.1.6","8.3.8","Existing Services",{"$nulls":4},"Dflt"]
["Label","132bc7d9-5b6f-418f-9713-1bf32b297d4c","","8.3.8.1","Location",{"$nulls":4},"Dflt"]
["Item","89abddcf-994b-4c74-a2c1-c751026c947e","B.7.4.1.6.1","","c) Excavate by hand in soft material to expose existing services around Waste Activated Sludge Pump Station","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G210 * H210,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","b13d3460-5802-4dd4-acad-51332f80eca2","B.7.4.1.7","8.3.8.2","Dealing with services that are at risk because of the construction of earthworks",{"$nulls":4},"Dflt"]
["Item","78388b72-e1bd-4a56-be71-31943f74e571","B.7.4.1.7.1","","a) Cables","No",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G212 * H212,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5a29f158-a477-4f35-9654-45c39676ad46","B.7.4.1.7.2","","c) Temporary protection of existing pipes","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a20e88a0-6fc0-424c-ac69-c503acfaef86","B.7.4.1.7.3","8.3.9","Extra-over for backfill or for fill material against structures compacted to 93% MOD AASHTO density","m³",205,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","20c40d73-f0d1-4861-abdc-9a66730890c1","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","b50c8959-a25f-4adc-b44a-4fb4a4e8754c","B.7.4.1.7.4","","WAS Pump Station","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G216 * H216,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Header2","15e0db2d-36b6-4262-ae6d-1abdcebf1b89","B.7.4.2","SANS\n1200 G","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Header3","1ecdb2a8-810f-43b0-9f48-47fbd7e5f224","B.7.4.2.1","8.1.1        PSG 8.1.1      PSG 8.2","Formwork",{"$nulls":4},"Dflt"]
["Header4","7b369e78-3f16-4c6e-8c1a-a263594f6caa","B.7.4.2.1.1","8.2.1","Rough vertical to (below final ground level):",{"$nulls":4},"Dflt"]
["Item","a463aec4-11ab-4059-adbd-31d8d79c5c50","B.7.4.2.1.1.1","","Foundations"," m²",17,{"v":0,"d":"0.00"},{"$f":"ROUND(G220 * H220,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header4","49ee4fd3-bb9b-41b3-8488-9ca77c315d22","B.7.4.2.1.2","8.2.2","Smooth vertical to:",{"$nulls":4},"Dflt"]
["Item","c5f5cc34-3f29-4b88-a0a8-cb4bd38b2201","B.7.4.2.1.2.1","","Walls"," m²",310,{"v":0,"d":"0.00"},{"$f":"ROUND(G222 * H222,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","dccc4051-4ecd-4785-b3b4-c2591b7c2205","B.7.4.2.1.2.2","","Columns"," m²",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1a7f3c47-661a-4ffc-8910-c12ab409ef11","B.7.4.2.1.2.3","","Cable trench walls"," m²",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header4","0363a44e-d791-452d-a952-0819358e4568","B.7.4.2.1.3","8.2.2","Smooth horizontal to:",{"$nulls":4},"Dflt"]
["Sum","fc651b3b-042d-42e7-b672-e9b86e5740ea","B.7.4.2.1.3.1","","Slab soffits"," m²",35,{"v":0,"d":"0.00"},{"$f":"ROUND(H226,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header4","94a95a03-df94-4103-ad31-669d1143e963","B.7.4.2.1.4","8.2.2","Smooth sloped to:",{"$nulls":4},"Dflt"]
["Item","fa054cec-8d36-426e-b0d0-c9651ad48476","B.7.4.2.1.4.1","","Slabs"," m²",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G228 * H228,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header4","20e8be34-8567-43f2-8bd4-ba6fc5d80c6c","B.7.4.2.1.5","8.2.6","Box out holes/form voids for all depths",{"$nulls":4},"Dflt"]
["Item","26abea6d-67c5-4446-a328-3393f8247d0f","B.7.4.2.1.5.1","8.2.6 (a)","Small, circular, of diameter up to and including 0,35 m"," No.",13,{"v":0,"d":"0.00"},{"$f":"ROUND(G230 * H230,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","ff4f967b-4b96-4b30-92e9-7caa2e3060ce","B.7.4.2.1.5.2","8.2.6 (c)","Large, circular, of diameter over 0.35 m"," No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","5c9cb2a3-c49b-4cdf-a59d-537ab00e0ba0","B.7.4.2.1.5.3","8.2.6 (d)\t","Large, other than circular, of area over 0.1 m² and up to and incl. 1.0 m²"," No.",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G232 * H232,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","8e9fc470-73e0-48d7-80d6-17deac69617d","B.7.4.2.2","8.1.2 PSG 8.1.2","Reinforcement",{"$nulls":4},"Dflt"]
["Item","5a1cf8bf-fe5b-4a12-8e05-d6495cc6fa87","B.7.4.2.2.1","8.3.1","Mild steel bars","t",0.6,{"v":0,"d":"0.00"},{"$f":"ROUND(G234 * H234,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","d7ac159c-eff3-4874-9b16-59189f0fa130","B.7.4.2.2.2","8.3.1","High-tensile steel bars","t",11.7,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","7fae1453-2ad3-4579-a1a7-1563119ab4fa","B.7.4.2.3","8.1.3 PSG 8.1.3","Concrete",{"$nulls":4},"Dflt"]
["Header4","b778e6ef-0ca0-44de-984f-da7bd8d02717","B.7.4.2.3.1","8.4.2","Strength concrete: 15 MPa/19 mm",{"$nulls":4},"Dflt"]
["Item","c70b9900-aabd-4ede-9481-94e8dd45af41","B.7.4.2.3.1.1","","Blinding layer 50 mm minimum thickness"," m²",95,{"v":0,"d":"0.00"},{"$f":"ROUND(G238 * H238,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","800fc0f0-eb85-481d-9ad6-8b719b0b1774","B.7.4.2.3.1.2","","Mass concrete benching"," m³",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","9b915923-6d57-4db1-bdbc-b6a8931b69b4","B.7.4.2.3.1.3","","Thrust blocks"," m³",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G240 * H240,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header4","9f777e65-aa31-47be-8ba6-fb9d6ce7e07c","B.7.4.2.3.2","8.4.3\nPSG 3.5.4","Strength concrete (Inclusive of Crystalline Water Proofing additive): 35 MPa/19mm",{"$nulls":4},"Dflt"]
["Item","8a819630-c2e4-42c6-8b06-8069dd005eb4","B.7.4.2.3.2.1","","Foundations","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G242 * H242,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a462e87d-5393-4bae-8651-4c0103fed8b6","B.7.4.2.3.2.2","","Slabs","m³",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d237c26b-d77f-43e0-8685-d2127fe45c88","B.7.4.2.3.2.3","","Walls","m³",41,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1ca9cb09-74ae-498e-b4b8-2000259d8cc3","B.7.4.2.3.2.4","","Sloping slabs","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","eb8dd5fb-ffe9-47fa-8c49-e9ac91412374","B.7.4.2.3.2.5","","Columns","m³",0.5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","46be5ffb-6edf-4ce5-b858-700dd723617d","B.7.4.2.3.2.6","","Cable trench slab","m³",1.5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e6952e08-970d-4721-bc2c-1f0936b94535","B.7.4.2.3.2.7","","Cable trench walls","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Rate Only","9d90bd28-47b2-4c1d-a836-dd0b0b1a139b","B.7.4.2.3.2.8","PSG 8.9","No-Fines Concrete 75mm thickness","m³",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Header4","f912fdd3-5146-493f-abdd-2867dc916cd0","B.7.4.2.3.3","8.4.4  PSG 8.4.4","Unformed surface finishes",{"$nulls":4},"Dflt"]
["Label","faf56343-9703-4c03-a10a-09c9fbc0fcb6","","","Wood-floated finish to:",{"$nulls":4},"Dflt"]
["Item","d9f1b54a-892f-4693-afef-3f03e2868dea","B.7.4.2.3.3.1","","Foundations"," m²",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G252 * H252,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","4a936eda-8b7c-4a93-b946-6e5d29475e5c","","","Steel-floated finish to:",{"$nulls":4},"Dflt"]
["Item","2dc9abe7-f60b-4627-b483-3d5881c4bbca","B.7.4.2.3.3.2","","Slabs"," m²",125,{"v":0,"d":"0.00"},{"$f":"ROUND(G254 * H254,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","45e122e9-8a78-4b71-8f84-b58d16956ca2","B.7.4.2.3.3.3","","Wall tops"," m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","9eecf782-4248-4807-bfda-780608157fa6","B.7.4.2.4","8.5   PSG 8.5","Joints",{"$nulls":4},"Dflt"]
["Item","9b6f352c-1e22-4e30-be44-c56da07ef3f3","B.7.4.2.4.1","","Construction joint at the base of wall, as shown on drg no. J40073-010-06","  m",45,{"v":0,"d":"0.00"},{"$f":"ROUND(G257 * H257,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","bd89b716-2212-4504-8a59-5c3735791e07","B.7.4.2.5","PSG 8.10","Items cast into concrete",{"$nulls":4},"Dflt"]
["Label","c2a44029-1dec-476c-bf98-87a1f8d65678","","","Setting puddle pipes or specials into or through concrete work, incl. for formwork around the pipes and fixing the pipes to the designated lines and levels using ABE Durated expansive cementitious grout (pipes measured elsewhere) for diameters:",{"$nulls":4},"Dflt"]
["Item","36fc43f0-57d1-4906-bf07-7149d3e32e23","B.7.4.2.5.1","","100mm up to 250mm","No",11,{"v":0,"d":"0.00"},{"$f":"ROUND(G260 * H260,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","7de2906b-5bdc-45f8-9d2f-e95c651ab4f2","B.7.4.2.5.2","","300mm up to 750mm","No",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","3373ebef-f3d7-444b-abb2-93fbd4145a1a","B.7.4.2.5.3","","900mm x 900mm manhole cover with frame","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G262 * H262,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","827cf32e-5159-48df-8734-624b6abdb4bf","B.7.4.2.6","","Watertightness test of ",{"$nulls":4},"Dflt"]
["Item","ef90acfa-46f0-4f02-8282-3673aa727efb","B.7.4.2.6.1","PSG 8.12","Waste Activated Sludge sump including provision of water","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G264 * H264,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","a61499af-6a25-4ce5-ac16-3c0b0b8d4ab7","B.7.4.2.6.2","PSG 8.12","Valve chamber including provision of water","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b8c98826-3d6d-49aa-a729-59d664fe532a","B.7.4.2.6.3","PSG 8.17","Slurry coat and curing","m²",260,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","48fb25e0-4e26-43dc-957b-30bb12116c67","B.7.4.2.6.4","PSG 8.13","Bond breaker: 250 micron DPC","m²",100,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","388602d9-fa7f-493e-b199-ec1a26d4119e","B.7.4.3","SANS\n1200 HA","STRUCTURAL STEELWORK (SUNDRY ITEMS)",{"$nulls":4},"Dflt"]
["Header3","8baaee80-32d0-4510-a956-62e65c073a61","B.7.4.3.1","8.3.1  PSHA 8.3.1 & 8.3.6\n","Structural steel\n",{"$nulls":4},"Dflt"]
["Label","226ccbe0-2fde-4425-888c-bd45eacb18cd","","","Supply, fabricate, deliver and install structural steelwork for",{"$nulls":4},"Dflt"]
["Item","96a2e9a1-a595-46e0-9d4c-125bde7bf9a8","B.7.4.3.1.1","","203 x 133 x 30kg crawl beam 8.5m long complete including expanding bolts","No\r\n",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G271 * H271,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","c3334f96-809b-4872-87a1-c4df4fea4bd1","B.7.4.3.2","8.3.4  ","Supply and install flooring, complete with frames as shown on drg no. J40073-010-06",{"$nulls":4},"Dflt"]
["Item","91b375fe-f8fa-4730-af63-2af16841a9f1","B.7.4.3.2.1","","Open grid floors, Rectagrid RS40 Type 50x4.5"," m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G273 * H273,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","681a3957-2f34-4a25-9070-9d96bb34ce8f","B.7.4.3.2.2","8.3.2 ","Supply and install handrails complete as shown on J40073-010-105","m",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e815e5fa-1b41-4804-b845-7374af2bc2ce","B.7.4.3.2.3","PSHA 8.3","Supply and install pipe supports complete as shown on J40073-010-06","No",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","b30e51c9-fd57-44d8-99e7-365afb630128","B.7.4.4","","MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Item","0528a08b-f3cf-492c-9e62-4bbf75f6ed33","B.7.4.4.1","","Supply, deliver and install MEGAFLO subsoil drainage system including excavation, stone fill and geofabric blanket","m",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G277 * H277,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","aea31ee7-807d-47f0-a7d0-5087d5422a55","B.7.4.4.2","","900mm x 900mm polymer concrete manhole cover and frame (Code 119181) cast into concrete as per SANS 1882-2003","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0640994b-8be6-4596-98d3-ec770cbc9247","B.7.4.4.3","","Manhole cover locking mechanism cast into concrete as per drawing","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","653210cd-d7c5-4f76-bdad-f186b30abb63","B.7.4.4.4","","80mm HDG mild steel vent pipe with No. 3 wire mesh welded into opening","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Section","81d3d8a7-f63c-4469-82b3-75380c1f513e","B.7.5","","RAS PUMP STATION ALTERATION",{"$nulls":4},"Dflt"]
["Label","2b0d13fe-4d04-41e1-a945-8b9355ea4339","","","SECTION B.7.5 : RAS PUMP STATION ALTERATION",{"$nulls":4},"Dflt"]
["Header2","b2174c25-e673-4092-a4f8-11b86b8c8724","B.7.5.1","SANS\n1200C\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","246ad1ec-10f2-4e0e-9a4d-2b385576ad7c","B.7.5.1.1","8.2.1","Clear and grub Site","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G284 * H284,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","36843fd1-3ae8-4d45-a479-ce8cdea98873","B.7.5.1.2","8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8ca9685b-fa72-45f3-93bd-7242b7fa3f4e","B.7.5.1.3","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","153fa15a-1566-454e-99a5-aa8cb0d9d273","B.7.5.2","SANS 1200D 8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Item","8e9a92bb-99bd-4161-b62f-7b8b87626db8","B.7.5.2.1","8.3.1.2\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G288 * H288,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9e2a5b85-d185-4031-845d-8defe2c1c132","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Item","6b16717c-ad78-4b86-97a1-fb3bfcc89819","B.7.5.2.2","8.3.3\nPSD 8.1.3","Restricted excavation for foundations and footing in all material and dispose of surplus/unsuitable material as ordered within the free haul distance","m³",45,{"v":0,"d":"0.00"},{"$f":"ROUND(G290 * H290,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c9c5c68f-04af-46cd-bbab-697a437e1f0d","","8.3.2(a)","Backfill (min G7 classified material to 95% MOD AASHTO behind structures for:",{"$nulls":4},"Dflt"]
["Item","16c82496-4a1d-4e9c-a091-64970555f5f6","B.7.5.2.3","","RAS Pump Station","m³",85,{"v":0,"d":"0.00"},{"$f":"ROUND(G292 * H292,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cc7d3679-db92-4a5b-9b7c-01709b35adec","","","Chloradane Heptacor' or 'Aldrin' or similar approved soil insecticide",{"$nulls":4},"Dflt"]
["Item","7a8a9445-95d4-4520-9bf2-5618ee274f65","B.7.5.2.4","","RAS Pump Station","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"$f":"ROUND(G294 * H294,2)","v":{"v":5000,"d":"5,000.00"}},"Dflt"]
["Header3","126146ae-160d-48c6-854b-75909c5e5c9a","B.7.5.2.5","SANS 1200D 8.3.2(b)\nPSD 8.3.2(b)","Extra-over item B.7.5.2.2 for excavation in:",{"$nulls":4},"Dflt"]
["Item","3e4c69bc-ce65-434f-ba98-6f1b8eefc36f","B.7.5.2.5.1","8.3.2(b)","Hard rock material","m³",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G296 * H296,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","da7e35b2-ea43-4771-acc3-0f899279170f","B.7.5.3","SANS 1200D 8.3.4","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","8cf5aaa9-8c8a-45b1-9dc2-5a85d775a0a3","B.7.5.3.1","","Extra-over item B.7.5.2.3 for importation of material under the telescopic valve sump for the RAS Pump Station from commercial sources: G5 material.","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G298 * H298,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","743f0dc8-0f48-466a-a120-8cd1bd6999fa","B.7.5.3.2","","Extra-over item B.7.5.2.3 for importation of material under the telescopic valve sump for the RAS Pump Station from commercial sources: G7 material.","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","de7f22b5-6edc-414e-8a43-4371885eb908","B.7.5.4","SANS 1200D 8.3.7","ADDITIONAL LATERAL SUPPORT",{"$nulls":4},"Dflt"]
["Label","03d12b81-4b15-46c8-964a-21dbd742df20","","8.3.7","Additional lateral support  (Provisional) for ensuring the stability of the excavation:",{"$nulls":4},"Dflt"]
["Item","efcba949-3d25-44b2-ad2d-0fd13a54bdf1","B.7.5.4.1","","RAS Pump Station","m²",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G302 * H302,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","a218348d-46c8-46ca-8c3c-599d4187ec15","B.7.5.5","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","bf604752-61d2-4ec1-95af-147fbc21c696","B.7.5.5.1","8.3.10","Topsoiling","m²",75,{"v":0,"d":"0.00"},{"$f":"ROUND(G304 * H304,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","46a74255-2c0a-4346-8dfa-7de8b5f8c8b9","B.7.5.5.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc as necessary and wetting","m²",75,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","e4bb239a-a96d-4be8-abaa-7d03e5beb2b1","B.7.5.6","SANS 1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","7639e965-c5a8-4553-b7b0-041dceb87d3b","","8.4.2","Blinding layer:\n15 MPa/19 mm concrete:",{"$nulls":4},"Dflt"]
["Item","bcf41333-f88b-4390-92fe-5b11826c86db","B.7.5.6.1","","50 mm minimum thickness","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G308 * H308,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2e299cdd-ab85-416c-b796-8ab3ac88350e","","8.4.3\nPSG 3.5.4","Strength concrete (Inclusive of Crystalline Water Proofing additive):\n35 MPa/ 19mm:",{"$nulls":4},"Dflt"]
["Item","aa642883-fd65-424e-a503-7b74cf0b60ae","B.7.5.6.2","","Floor slabs","m³",7,{"v":0,"d":"0.00"},{"$f":"ROUND(G310 * H310,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","705b7bce-d7dd-4e7c-89bc-8f4bb236c4dc","B.7.5.6.3","","Walls ","m³",9,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","5dc89d58-dc7d-41d7-a5f5-57481479899b","B.7.5.7","SANS 1200G 8.2\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","1783c7ce-361d-4a10-90d1-7b3d04864d47","","8.2.2","Smooth vertical plane:",{"$nulls":4},"Dflt"]
["Item","260d2f9d-df8a-4daa-9377-e326d592db0d","B.7.5.7.1","","Walls","m²",65,{"v":0,"d":"0.00"},{"$f":"ROUND(G314 * H314,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7ce51a38-d7e4-47c0-b141-34118c2fd574","","8.2.6","Box Out Holes/Form Voids:",{"$nulls":4},"Dflt"]
["Label","57fcf5b1-2494-4792-b546-85d0c91fec21","","","Large, circular, of diameter over 0.35m up to and incl. 0.7m.:\ndepths\nover     and     up to",{"$nulls":4},"Dflt"]
["Item","94378f5e-2c96-475e-9580-3da617e3ab7c","B.7.5.7.2","","0 m                  0,3 m","No",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G317 * H317,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","684b7032-2867-4c47-b95b-dc6c597b5d9c","","","Large, other than circular, of area over 0.1m2 and up to and including 1.0m2",{"$nulls":4},"Dflt"]
["Item","d40c4eaa-3179-4a7a-bc39-110a2de961fb","B.7.5.7.3","","0 m                  0,3 m","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G319 * H319,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cb8384bb-6eed-40fd-955c-67fe5ad8c1f1","","PSG 8.10","Casting of pipes/specials into concrete for:",{"$nulls":4},"Dflt"]
["Label","70eee80b-4bcf-4b21-81a6-f76a784598c6","","","Pipes up to and including 450 mm NB through walls:\ndepths\nover     and     up to",{"$nulls":4},"Dflt"]
["Item","517949a9-2bbf-4f45-80e2-ca343ebf528b","B.7.5.7.4","","0 m                  0,35 m","No",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G322 * H322,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","0473edd9-2e11-44fb-a0db-7f1d8b60ba47","B.7.5.8","SANS 1200G 8.1.2\nPSG 8.1.2","REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","e6354c40-5bad-4b82-9bda-174e5e7d843c","","8.1.2.3(a)","Mild steel bars:",{"$nulls":4},"Dflt"]
["Item","26eb7172-2a1c-4001-a603-7a3d5895ffff","B.7.5.8.1","","25 mm diameter: Basic price","t",0.12,{"v":0,"d":"0.00"},{"$f":"ROUND(G325 * H325,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","df431bf5-ca15-48d6-864f-091432736550","","8.1.2.3(b)","Extra-over item B.7.5.8.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","dcb1ff7f-4617-41eb-b6fd-7a58be4f840a","B.7.5.8.2","","8 mm","t",0.06,{"v":0,"d":"0.00"},{"$f":"ROUND(G327 * H327,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","637dda99-ca10-4a7d-9890-cdade5095d04","B.7.5.8.3","","10 mm","t",0.06,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","0ac379b6-e3f4-4a50-968a-53ca20e2b2b3","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","49c453dd-d972-4435-a4f6-f3c582ccc1a2","B.7.5.8.4","","25 mm diameter: Basic price","t",2.3,{"v":0,"d":"0.00"},{"$f":"ROUND(G330 * H330,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","e9157027-bd52-433c-a208-5d959940d057","","8.1.2.3(b)","Extra-over item B.7.5.8.4 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","701e2e9a-945d-45d3-b923-4cab9ffc6d8b","B.7.5.8.5","","10 mm","t",0.7,{"v":0,"d":"0.00"},{"$f":"ROUND(G332 * H332,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0b68a4d3-2f5e-433c-8635-43b4ccc370b8","B.7.5.8.6","","12 mm","t",0.7,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0b122371-c4b8-4a2e-97ec-59f56cb6f733","B.7.5.8.7","","16 mm","t",0.9,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","d2ebeab2-4b79-44aa-87fe-b070b04a003c","B.7.5.9","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","fc3f0170-0962-4c7b-ad7b-245d70c18d09","","PSG 8.4","Wood-floated finish:",{"$nulls":4},"Dflt"]
["Item","443b32e5-f473-4728-b9d8-2944b2067226","B.7.5.9.1","","Top of floor slabs","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G337 * H337,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9f534fb4-b039-4341-a89f-d852c1619e2a","","8.1.1.5\nPSG 8.4","Steel-floated finish:",{"$nulls":4},"Dflt"]
["Item","a5456221-88d5-4383-9b68-10d7dc5f0093","B.7.5.9.2","","Top of walls","m²",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G339 * H339,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","9389e69c-9343-411b-b56b-f41c9a281c5f","B.7.5.10","SANS 1200G 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Item","4eefb01a-e173-41e3-bbb2-a54ad1c79421","B.7.5.10.1","","Waterstop in kicker to Detail 1 of Dwg. No. J40073-010-230","m",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G341 * H341,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7961eccd-d289-44ef-95ab-553bfd833882","","","Contraction joints:",{"$nulls":4},"Dflt"]
["Item","9e881cf8-6ced-49fd-b8ba-21646a956e50","B.7.5.10.2","","Vertical contraction joint in wall complete with waterproofing bandage, bond breaker cord, sealant, drilling for dowels, dowels, and epoxy to set dowels to Detail X of Dwg. No. J40073-010-230","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G343 * H343,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","dbd35c64-53c8-4703-b4f7-96cc66845a6e","B.7.5.11","SANS 1200HA","STRUCTURAL STEELWORK:\nSUNDRY ITEMS",{"$nulls":4},"Dflt"]
["Label","479b1561-50b9-4702-be5e-75b8de6c8e17","B.7.5.11.1","","Structural steel\n",{"$nulls":4},"Dflt"]
["Header2","dcd36aec-00d7-4d43-9792-55acf3c67b5b","B.7.5.12","","Supply and install flooring, complete with frames as shown on  Dwg. No. J40073-010-230",{"$nulls":4},"Dflt"]
["Item","67268e61-3017-484a-9e2c-0eabadb193dd","B.7.5.12.1","8.3.4 PSHA 8.3.6","Open grid floors, Rectagrid RS40 Type 50x4.5"," m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G347 * H347,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","8cecff37-3d45-4163-8c81-fe57fad03b06","B.7.5.12.2","8.3.2 PSHA 8.3.2 & 8.3.6","Supply and install handrails complete as shown on  Dwg. No. J40073-010-230","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","5617cbf3-445f-4bf1-ac47-9c30e7fdb58c","B.7.5.13","","MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Item","9f9aa9ed-83e1-4a39-a0f1-546266714510","B.7.5.13.1","","250 micron black plastic membrane","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G350 * H350,2)","v":{"v":0,"d":"0.00"}}]
["Header2","1d140e11-7ff5-414c-ba75-2be9064d8043","B.7.5.14","","SUNDRIES"]
["Label","576983bb-e447-4db0-9572-94f393bc4ee3","","","Water Tightness Testing:"]
["Item","e6ecd24c-3318-49db-b9f2-04b375e9029c","B.7.5.14.1","PSG 8.12","Testing for Water Tightness, all inclusive to PSG 7.2.5","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G353 * H353,2)","v":{"v":0,"d":"0.00"}}]
["Item","76318c1a-d7df-45ac-bf64-4acde6bf89dc","B.7.5.14.2","","Break through existing concrete sump wall, smooth and seal exposed concrete and reinforcing for octagon void 1000mm x 800mm overall dimension","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","7ddca7ef-11f4-407d-9224-21bcbc0433ae","B.7.5.14.3","","Break through existing sump wall for circular void to fit 400mm NB steel pipe puddle flange for casting purposes.","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]

{"sheet":"BILL B.8.","index":8,"n_rows":76,"n_cols":10,"rows_kept":76,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL B.8.",null,"CHLORINE CONTACT CHANNELS",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","81064ffb-8d20-4c1f-9930-978d2de516f0","B.8.1","","CHLORINE CONTACT CHANNEL",{"$nulls":4},"Dflt"]
["Label","f7f082e3-297c-4e86-afbf-6ae6bd42b476","","","SECTION B.8.1 : CHLORINE CONTACT CHANNEL",{"$nulls":4},"Dflt"]
["Header2","7691380c-1b01-45e3-bc42-e7f92b581ad1","B.8.1.1","","JOINTS",{"$nulls":4},"Dflt"]
["Item","4157a82e-ae24-43f4-ade5-8eae06fdc9b3","B.8.1.1.1","SANS 1200G 8.5\nPSG 8.5","Form Joints in floors complete, including preparation, 10 mm wide x 10 mm deep polyurethane sealant, etc.","m",2000,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","2979b656-aee3-452d-bf15-5fcd9fb343ec","B.8.1.2","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","5bc6a2f9-fab7-4f2a-9666-f29f408c2539","","","Removal of broken concrete dividers and dispose off-site to a registered landfill site(Provisional):",{"$nulls":4},"Dflt"]
["Item","6b16d9e1-6cb6-4129-a926-cd9bc27dee67","B.8.1.2.1","","Concrete dividers (Typical fibro-crete concrete panels)","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G15 * H15,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","bb365ee5-3e24-4804-8f41-e70316016b5b","","","Supply, install, etc. concrete dividers:",{"$nulls":4},"Dflt"]
["Item","39af872f-45e3-4d3b-afb3-1f7ff04256f6","B.8.1.2.2","","Concrete dividers (Typical fibro-crete concrete panels)","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G17 * H17,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Section","c352ce74-cb1d-4a94-99bd-80ff5bffbb16","B.8.2","","CHLORINE CONTACT TANK INFLOW CHANNEL",{"$nulls":4},"Dflt"]
["Label","ddcf31bd-25ee-4e3c-89d4-da440b81a3e1","","","SECTION B.8.2 : CHLORINE CONTACT TANK INFLOW CHANNEL",{"$nulls":4},"Dflt"]
["Header2","2dd25e44-615e-49bc-b726-e1335c19f988","B.8.2.1","SANS\n1200C &\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","b69fdcec-d3dc-4b8e-989c-f148ca7c69f7","B.8.2.1.1","8.2.1","Clear and grub Site","m²",85,{"v":0,"d":"0.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","98809d5f-c547-4cde-8aef-5f910c373d2e","B.8.2.1.2","8.2.4","Reclear surfaces (provisional) (where ordered by Engineer)","m²",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1a84c2f1-2454-4a5b-ae0f-1cbc0aae5aa9","B.8.2.1.3","8.2.9","Cart materials and debris to unspecified sites and dump (provisional)","t.km",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","97ff5113-ff1b-4c2a-8e99-333a3f837a1c","B.8.2.2","SANS 1200D\n8.3.2","EARTHWORKS",{"$nulls":4},"Dflt"]
["Item","741d743b-7678-47a0-8e22-67f7e297ce2b","B.8.2.2.1","8.3.1.2\nPSC 8.2.10","Remove topsoil to nominal depth 150mm, stockpile, and maintain","m²",85,{"v":0,"d":"0.00"},{"$f":"ROUND(G25 * H25,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","978dbc60-e9cb-424d-947a-25ec27acb7a3","","8.3.2(a)\nPSD 8.3.6","Excavate for structures in all materials and dispose of surplus/unsuitable material as ordered within the free haul distance for :",{"$nulls":4},"Dflt"]
["Item","c5129097-ae0c-4da2-b7a7-6d09ebfd2db4","B.8.2.2.2","","Channel","m³",75,{"v":0,"d":"0.00"},{"$f":"ROUND(G27 * H27,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","4b9099cd-55fe-40f5-a21e-1d8a9236ef44","","8.3.2(a)","Backfill to 95% MOD AASHTO behind structures for :",{"$nulls":4},"Dflt"]
["Item","a5b00e3c-08a0-4243-8b46-e71fb440fab1","B.8.2.2.3","","Channel","m³",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G29 * H29,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ddb80835-dfbc-48a9-b4e4-54fc9de94774","B.8.2.2.4","","Rip subgrade to 150mm deep and compact to min 93% MOD AASHTO density.","m³",13,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","a4061438-bddf-4a26-970d-7192fa96057f","B.8.2.3","SANS 1200D 8.3.2(b)\nPSD 8.3.2(b)","Extra-over items B.8.2.2.2 for excavation in:",{"$nulls":4},"Dflt"]
["Item","93058cc7-1aec-479d-8613-8600e5e95b37","B.8.2.3.1","8.3.2(b)","Hard rock material","m³",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G32 * H32,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","7ed22192-4270-4452-a583-161e3a7a4c3d","B.8.2.3.2","SANS 1200D 8.3.4","IMPORTING OF MATERIALS",{"$nulls":4},"Dflt"]
["Item","02476f61-5daa-4cc8-9b22-f8ef6abd1c5c","B.8.2.3.2.1","","Extra-over items B.8.2.2.2 for importation of material  from commercial sources: G7 material compacted to 95% MOD AASHTO density","m³",13,{"v":0,"d":"0.00"},{"$f":"ROUND(G34 * H34,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","5339f438-4e60-4ad1-9d7f-9ac9f52e7c15","B.8.2.4","SANS 1200D","FINISHINGS",{"$nulls":4},"Dflt"]
["Item","29b7b0de-41db-4c1a-b990-8a06d1250d7c","B.8.2.4.1","8.3.10","Topsoiling","m²",140,{"v":0,"d":"0.00"},{"$f":"ROUND(G36 * H36,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f586c21a-c556-49a3-a6a7-48cc8e57464e","B.8.2.4.2","8.3.11","Grassing with instant kikuyu lawn grass. Rate to be inclusive of transport and delivery and offloading costs including for temporary stockpile and double handling etc as necessary and wetting","m²",140,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","c8be42d7-29e3-44d5-ac46-633f1539e746","B.8.2.5","SANS 1200G\n8.1.3\nPSG 8.1.3","CONCRETE (STRUCTURAL)",{"$nulls":4},"Dflt"]
["Label","10b8acd6-cf94-4169-bfd6-0ee6752eba76","","8.4.2","Blinding layer:\n15 MPa/19 mm concrete:",{"$nulls":4},"Dflt"]
["Item","39e56501-1502-4ed0-83bf-f6b14523419e","B.8.2.5.1","","50 mm minimum thickness (Channel)","m²",85,{"v":0,"d":"0.00"},{"$f":"ROUND(G40 * H40,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","dec7ba27-4acc-4f69-b32f-2c3fc2c69163","","8.4.3\nPSG 3.5.4","Strength Concrete (Inclusive of Crystalline Water Proofing additive):\n35 MPa/19 mm:",{"$nulls":4},"Dflt"]
["Item","76b837a4-0160-4957-b7d1-2ee754245862","B.8.2.5.2","","Channel slab","m³",13,{"v":0,"d":"0.00"},{"$f":"ROUND(G42 * H42,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","fbfeed58-32dd-4fa5-83f9-996c71a65040","B.8.2.5.3","","Channel walls","m³",7,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","96cbf36f-503e-4b80-ac25-afd35c6ad4e6","B.8.2.6","SANS 1200G 8.2\nPSG 8.2","FORMWORK",{"$nulls":4},"Dflt"]
["Label","62cb438d-164f-4481-a89a-863af1de6066","","8.2.2","Smooth vertical circular to walls:",{"$nulls":4},"Dflt"]
["Item","1572f2ff-75f4-4358-b678-39d284346519","B.8.2.6.1","","Channel walls to match radii of existing channel (Approx. 9m radius)","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G46 * H46,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9c7017e9-cc7d-448b-934a-f4d2ba1f42f2","","","Smooth vertical plane to:",{"$nulls":4},"Dflt"]
["Item","bb342c55-b7e4-451e-bf58-713fb266e25e","B.8.2.6.2","","Channel walls","m",70,{"v":0,"d":"0.00"},{"$f":"ROUND(G48 * H48,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","1cda77ce-e72e-43e7-880f-853f0d72b8d9","B.8.2.7","SANS 1200G 8.1.2\nPSG 8.1.2","REINFORCEMENT ",{"$nulls":4},"Dflt"]
["Label","1905bd3a-a10a-490c-8b6c-ce1c070d6ad7","","8.1.2.3(a)","Mild steel bars:",{"$nulls":4},"Dflt"]
["Item","84a2b548-7f3b-4b9c-a63e-6671ffcd9f58","B.8.2.7.1","","25 mm diameter: Basic price","t",0.15,{"v":0,"d":"0.00"},{"$f":"ROUND(G51 * H51,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2edb469a-364d-4800-9cd4-61251feea1dd","","8.1.2.3(b)","Extra-over item B.8.2.7.1 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","36e9b176-4c57-4c5b-85d7-87e6d73a9ed9","B.8.2.7.2","","8 mm","t",0.1,{"v":0,"d":"0.00"},{"$f":"ROUND(G53 * H53,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","df0b2225-8843-4211-b60e-a91392737915","B.8.2.7.3","","10 mm","t",0.05,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","258d9df8-7fb6-4f53-b88a-95b1682453d4","","8.1.2.3(a)","High tensile steel bars:",{"$nulls":4},"Dflt"]
["Item","46a085fd-957f-45eb-b6f3-1864b00e2f13","B.8.2.7.4","","25 mm diameter: Basic price","t",2.85,{"v":0,"d":"0.00"},{"$f":"ROUND(G56 * H56,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","3e89de4a-5cc5-4c62-a16b-079040ce5031","","8.1.2.3(b)","Extra-over item B.8.2.7.4 for bars of diameter (Provisional):",{"$nulls":4},"Dflt"]
["Item","f9642a27-02db-4db7-a2a3-a45fb5b24de1","B.8.2.7.5","","10 mm","t",1.4,{"v":0,"d":"0.00"},{"$f":"ROUND(G58 * H58,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f008bec7-e693-4761-a369-3a460debceec","B.8.2.7.6","","12 mm","t",1.45,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","18fe7828-d14a-42a1-be0f-b59f2dad0974","B.8.2.8","SANS 1200G 8.4.4\nPSG 8.4","UNFORMED SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Label","02aed71d-0599-4c24-84d1-ec0114e72b3f","","8.1.1.5\nPSG 8.4","Steel-floated finish:",{"$nulls":4},"Dflt"]
["Item","61130073-e4ba-4cee-ade8-759e33e80207","B.8.2.8.1","","Channel Floor","m²",70,{"v":0,"d":"0.00"},{"$f":"ROUND(G62 * H62,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6f6abfb2-1b0b-4424-8012-2e587e900582","B.8.2.8.2","","Channel Wall top","m²",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","c5d4593c-290a-4078-a91f-f375e451d1b1","B.8.2.9","SANS 1200G 8.5\nPSG 8.5","JOINTS",{"$nulls":4},"Dflt"]
["Label","76ffd576-4cee-48c7-a7a4-c850dc7a6715","","","Channel Floor and Wall joints complete as shown on Dwg. No. J40073/010-216:",{"$nulls":4},"Dflt"]
["Item","ae8137d6-6f2c-444a-ba60-2afade47487a","B.8.2.9.1","","Construction and Contractions Joints in Channel:\nIncluding forming of joint, supply and installation (all inclusive) of Centre bulb waterstop as shown on Dwg. No. J40073/010-216","m",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G66 * H66,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","539076b3-4ff5-40c2-b689-ad54f802230e","B.8.2.9.2","","Construction Joint in Wall:\nIncluding forming of joint, supply and installation (all inclusive) of 2mm Galvanised water stop as shown on Dwg. No. J40073/010-216","m",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bd07ebdf-3dc9-4be2-a21b-8ca081c7bbfa","B.8.2.9.3","","Horizontal contraction joint between existing channel floor and new channel floor complete with waterproofing bandage, bond breaker cord, sealant, drilling for dowels, dowels, and epoxy to set dowels to Detail X of Dwg. No. J40073-010-230","m",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","1aefbc4d-a4b0-4855-aa63-1003dc1f1748","B.8.2.10","","ALTERATIONS",{"$nulls":4},"Dflt"]
["Label","cd68a4bd-1a98-400e-acb3-bc03b6654cac","","","Chlorine Contact Tank and existing Pond Inlets:",{"$nulls":4},"Dflt"]
["Sum","c12be240-8fcb-4b8e-9814-e976f1c9abaf","B.8.2.10.1","","Alterations to the inlets of the existing Chlorine Contact Tank and the Ponds","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H71,2)","v":{"v":0,"d":"0.00"}}]
["Label","47062577-38f7-4a08-a82c-f869e8a0b034","","","Demolition:"]
["Sum","9eecf3f4-c3c9-4933-8532-960cbd986cd4","B.8.2.10.2","","Break down existing concrete channel wall, smooth and seal exposed concrete and reinforcing.","m",5,{"v":0,"d":"0.00"},{"$f":"ROUND(H73,2)","v":{"v":0,"d":"0.00"}}]
["Header2","ea72669a-3ef2-46db-80ec-bde6f9d35a5c","B.8.2.11","","SUNDRY"]
["Item","4b2bbde9-76ff-4852-b281-ffdfbea9de9b","B.8.2.11.1","","Remove and reinstall existing sluice gate.","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G75 * H75,2)","v":{"v":0,"d":"0.00"}}]
["Item","cddba482-d32e-4757-b03e-b170e4d8b776","B.8.2.11.2","","Supply and install complete waterworks sluice gate 600mm high x 1200mm wide.","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]

{"sheet":"BILL C","index":9,"n_rows":107,"n_cols":10,"rows_kept":107,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL C",null,"ROADWORKS",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","24f51acf-24f2-4d45-b9a9-897837c50d0d","C1","","ROADWORKS",{"$nulls":4},"Dflt"]
["Label","b3960db5-0a31-4793-8c17-9cbe06ea2e47","","","SECTION C1 : ROADWORKS",{"$nulls":4},"Dflt"]
["Header2","a97a0c40-1dda-482c-91dc-5ed5e7edeb4f","C1.1","SANS 1200DM","EARTHWORK (ROADS, SUBGRADE)",{"$nulls":4},"Dflt"]
["Header3","dcf19018-dfdd-4976-b7f3-37ec0e33ab7d","C1.1.1","SANS 1200DM\nPSC 8.2","SITE CLEARANCE",{"$nulls":4},"Dflt"]
["Item","dfb3427f-9f54-495d-8763-3da6e0098e04","C1.1.1.1","SANS 1200C 8.2.1","Clear and grub Site","m²",2340,{"v":0,"d":"0.00"},{"$f":"ROUND(G13 * H13,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","14b12112-3ee4-4912-bd76-57a28f6e78c8","C1.1.1.2","8.3.2.(a)\nPSC 8.2.10","Remove topsoil to depth of 150 mm, stockpile and maintain for later use","m²",2340,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","98e399b3-2bfb-4bdd-a732-f6ee71e00e89","C1.1.2","SANS 1200DM","TREATMENT OF ROADBED",{"$nulls":4},"Dflt"]
["Label","2965c2d3-8daa-4c5c-ad5c-c4f32528d638","","8.3.3(a)","Road-bed preparation and compaction of material to 93 % Mod. AASHTO maximum for:",{"$nulls":4},"Dflt"]
["Item","e365e2bc-bc0f-4520-b25f-ffcf79c55cac","C1.1.2.1","","150 mm thickness in roads","m³",355,{"v":0,"d":"0.00"},{"$f":"ROUND(G17 * H17,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","463a514a-59df-4e98-8d6e-1bfe5e02dca4","C1.1.3","SANS 1200DM","EARTHWORKS",{"$nulls":4},"Dflt"]
["Label","e583c36b-a9e5-4046-b46b-93e428a108a4","","8.3.4","Cut to fill:",{"$nulls":4},"Dflt"]
["Item","4bde087c-2b35-4fca-a5d4-faecad1a94a1","C1.1.3.1","","Compact to 90 % Mod. AASHTO maximum density","m³",180,{"v":0,"d":"0.00"},{"$f":"ROUND(G20 * H20,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5f5af920-5bea-4ef3-a2f9-dd03a3c6a981","","","Borrow to fill:",{"$nulls":4},"Dflt"]
["Item","7e997759-b69c-4555-9bd0-8a69caf80cc5","C1.1.3.2","8.3.4","Compact to 90 % Mod. AASHTO maximum density","m³",175,{"v":0,"d":"0.00"},{"$f":"ROUND(G22 * H22,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c7e27f95-5e95-4ecc-9f5e-7c7b8f2dafab","","8.3.6","Extra-over items C1.1.3.1 to C1.1.3.2 inclusive for excavating and breaking down material in:",{"$nulls":4},"Dflt"]
["Item","6afbda9b-dad6-46de-8b21-f6a84dde5bd0","C1.1.3.3","","Hard excavation","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G24 * H24,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5f700c6c-8724-4530-be14-853cbfdaca64","","8.3.7","Cut to spoil from:",{"$nulls":4},"Dflt"]
["Item","72534988-5671-4a93-b625-ecf4081c10dd","C1.1.3.4","","Soft excavation","m³",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G26 * H26,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b74c25b1-9501-413a-8503-8d0062c14110","C1.1.3.5","","Hard excavation","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","ce1aef6c-80ae-41ed-9984-3cf2ae86dddb","C1.1.4","","SURFACE FINISHES",{"$nulls":4},"Dflt"]
["Item","4b8b4360-f261-472d-9c51-ae97c585606c","C1.1.4.1","8.3.13(a)","Topsoiling","m²",540,{"v":0,"d":"0.00"},{"$f":"ROUND(G29 * H29,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ded142df-e9d9-4025-964b-767ed2a27571","C1.1.4.2","8.3.13(b)","Grassing","m²",540,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","aac2b61b-96c5-47b2-a960-cd1fc088b236","C1.2","SANS 1200ME\nPSM 8.1","SUBBASE",{"$nulls":4},"Dflt"]
["Label","96810d5d-7912-4bd6-9bf2-6be5275f9a1e","","","Construct gravel subbase with G7 material from commercial sources compacted to 95 % Mod. AASHTO maximum density:",{"$nulls":4},"Dflt"]
["Item","d65566bc-77b7-40e1-9a33-7f5fb03aaaa8","C1.2.1","","150 mm  thickness in roads","m³",355,{"v":0,"d":"0.00"},{"$f":"ROUND(G33 * H33,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b210dde7-8a8f-46ae-81c6-eed50687d0ba","","1200ME\n8.3.2","Construct shoulders with G7 material from commercial sources compacted to 93 % Mod. AASHTO maximum density:",{"$nulls":4},"Dflt"]
["Item","078785d4-146e-40a5-9026-e883a3dfbfa7","C1.2.2","","150 mm thickness","m³",400,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","57e6fdf5-4668-469c-a65b-c8de35dd3c84","C1.3","SANS 1200MF\nPSM 8.1","BASE",{"$nulls":4},"Dflt"]
["Label","00a26b57-67a8-4e39-a291-00781b321b19","","8.3.3","Construct gravel base with G5 material from commercial sources compacted to 97 % Mod. AASHTO maximum density:",{"$nulls":4},"Dflt"]
["Item","107c2f93-1c01-4d26-8a1b-08252dfef188","C1.3.1","","150 mm  thickness in roads","m³",165,{"v":0,"d":"0.00"},{"$f":"ROUND(G38 * H38,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b3c418b8-648c-4f4e-bb94-250be8c35cfb","","8.3.5","Process base by means of:",{"$nulls":4},"Dflt"]
["Item","d4c6b92d-0eee-4cc4-badc-9f0caf76345e","C1.3.2","","Stabilization","m³",165,{"v":0,"d":"0.00"},{"$f":"ROUND(G40 * H40,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6189c210-c9e5-46fb-a49e-1d9860265524","","8.3.8","Stabilizing agent:",{"$nulls":4},"Dflt"]
["Item","68a0e292-d547-4279-a005-6e0415e42d62","C1.3.3","","Portland cement","t",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G42 * H42,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","714a99f6-6be2-4d09-a600-13be48ba3218","C1.3.4","","Provision and application of water for curing","kl",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","26e29ec9-fa24-4834-bc14-89faf5f14b2e","C1.3.5","","Curing by covering with the subsequent layer","m²",1070,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","577855e1-195c-4bfe-b6f7-65f8466d393c","C1.4","SANS 1200MK\nPSMK 8.1","CONCRETE KERBING AND CHANNELLING",{"$nulls":4},"Dflt"]
["Label","e7d9e8d9-a97c-4b74-8288-464a2d5f3f4e","","8.2.1","Supply, lay, grout, joint and backfill for radii exceeding 20 m to straight:",{"$nulls":4},"Dflt"]
["Item","4a200e10-355f-4106-9e10-815728b5e087","C1.4.1","","(a) Type Figure 7 kerb","m",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G47 * H47,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","639ebabd-2d56-442a-8ea8-6ffdbd14722f","C1.4.2","","(b) Type Figure 8C kerb","m",90,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","283d2730-97f3-4757-aab7-a275be282d55","C1.4.3","","(c) Type Figure 7 kerb and Type C1 channel","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","02e5c23c-c78c-4247-a33e-aca6f09fc87b","C1.4.4","","(d) Type Figure 8C kerb and Type C1 channel","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d84a4d48-85fd-447a-9c39-3a1c14a978ff","","8.2.1","Supply, lay, grout, joint and backfill for radii 5 m to radii 20 m in 300 mm lengths:",{"$nulls":4},"Dflt"]
["Item","afb09cc9-5b83-4e1a-8fce-15b323bd680a","C1.4.5","","(a) Type Figure 7 kerb","m",55,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","fc7cd397-db91-442d-a18f-8ae2e4c0551e","C1.4.6","","(b) Type Figure 8c kerb","m",55,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4bb93011-48d3-4217-a36b-2b7b333e9ced","C1.4.7","8.2.1","Transition kerbs","No",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","1a2c33bf-8776-411b-9668-b03d97af6722","C1.5","SANS 1200MM","ANCILLARY ROADWORKS",{"$nulls":4},"Dflt"]
["Header3","376e306b-0733-4b02-87e1-816c56db41ac","C1.5.1","","PERMANENT TRAFFIC SIGNS",{"$nulls":4},"Dflt"]
["Label","e4f1e711-6756-4362-bf22-9c10c50db125","","8.3.1\nPSMM 8.3.4","Supply and erect permanent road signs and posts, including all bolts & nuts, signs and sign posts, excavations, costing in concrete, backfilling etc.",{"$nulls":4},"Dflt"]
["Item","6ade37a6-9de4-4c6b-b43b-c7dbefa131d8","C1.5.1.1","","Stop sign R1 (600 mm diam.)","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G58 * H58,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3145f79f-6723-4f5a-8204-17571fa1c82a","C1.5.1.2","","Warning sign W401","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1c22c679-1bb8-45bd-a028-e8ce35f5b2d1","C1.5.1.3","","Warning sign W402","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","cf7cf6ea-bfc0-416b-ba94-ee9c6e00d758","C1.5.2","","ROAD MARKINGS",{"$nulls":4},"Dflt"]
["Label","d877c55f-b256-4516-9fb2-7c9522f4938d","","8.4.1","Non-reflectorized paint applied at nominal rate of 0,42 l/m²:",{"$nulls":4},"Dflt"]
["Item","13cf162c-79c9-40e3-bc67-6281633dd882","C1.5.2.1","","(a) White lines RM1, 100W","m",1320,{"v":0,"d":"0.00"},{"$f":"ROUND(G63 * H63,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e74e568b-915a-4ee0-b6d4-8b4ca6bcf5ba","C1.5.2.2","","(b) White lines RTM1, 300W","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2b409fa9-856a-4865-8868-bb5dac650f39","C1.5.2.3","","(c) White characters and symbols","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","44ddbeb3-c337-48bb-b9a0-3a663269206a","","8.4.4","Setting out and premarking of lines (excluding traffic island markings, characters, and symbols:",{"$nulls":4},"Dflt"]
["Item","f0fa37bd-9efb-480c-b879-d4297c80021c","C1.5.2.4","","(a) Stop lines (RTM1)","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G67 * H67,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","31d80534-4461-4cc9-9d89-f04421c8f3c3","C1.5.2.5","","(b) Unbroken lines (RM1)","m",1320,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ad123d0c-2650-4969-95e1-396285f9fbf5","C1.5.2.6","","(c) Symbols","No",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","c36e05af-3b39-47a8-b573-3d859aaa01a4","C1.6","SANS 1200MJ","SEGMENTED PAVING",{"$nulls":4},"Dflt"]
["Header3","62f8a9c1-fa1e-4d9b-98be-0a8ef93f6475","C1.6.1","","PROVIDE EDGE RESTRAINTS",{"$nulls":4},"Dflt"]
["Label","f2a6b911-297c-4868-bbae-79921ff5f4e3","","8.2.1","Supply, lay, grout, joint and backfill for edge restraints as shown on Dwg. No. J40073/010-113:",{"$nulls":4},"Dflt"]
["Item","bf3ade86-6099-474d-8a76-bd518844da20","C1.6.1.1","","Admin, Type SA, 80 mm thickness","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G73 * H73,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","589f1283-8361-4c6a-9893-85a48cf60a6f","C1.6.1.2","","Workshop Buiding, Type SA, 80 mm thickness","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","95ed5c9c-1889-40ec-b979-0b6d1e4b5f28","C1.6.1.3","","MCC Buiding, Type SA, 80 mm thickness","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0233265c-79f1-4015-9500-2e711f819872","C1.6.1.4","","Guardhouse, Type SA, 80 mm thickness","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","93c1a949-6952-4328-a801-704bd8112f18","C1.6.1.5","","Blower Building, Type SA, 80 mm thickness","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1b93518b-dcba-497e-b487-51e4060fbace","","8.2.3","Cut units to fit edge restraints:",{"$nulls":4},"Dflt"]
["Item","f0ffe64e-d324-4f86-80ea-13385061aa37","C1.6.1.6","","Admin, Type SA, 80 mm thickness","m",130,{"v":0,"d":"0.00"},{"$f":"ROUND(G79 * H79,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","83c200d3-5fb8-473b-a37e-9957f571afaa","C1.6.1.7","","Workshop Buiding, Type SA, 80 mm thickness","m",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8b895d9a-2621-453b-ae8a-cbea3f06a395","C1.6.1.8","","MCC Buiding, Type SA, 80 mm thickness","m",60,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","99da924b-4371-466c-be44-ee2294d2fa51","C1.6.1.9","","Guardhouse, Type SA, 80 mm thickness","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0fe95edc-e376-4a8c-a94c-9663b328d4ac","C1.6.1.10","","Blower Building, Type SA, 80 mm thickness","m",230,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","55350a69-0f8d-445c-b984-cc389b3d31eb","C1.6.2","","CONSTRUCT PRECAST CONCRETE SEGMENTED PAVING",{"$nulls":4},"Dflt"]
["Label","f5bea7cd-673f-4360-aaa2-8e582e7b59da","","8.2.2","Supply and Install concrete block paving, including supply, delivery to site, stockpiling, installation, compaction, testing, etc., complete in all areas as shown on Dwg. No. J40073/010-005 and J40073/010-021, pattern to approval:",{"$nulls":4},"Dflt"]
["Item","fc73595e-5efe-4c05-89b9-ae0699d58544","C1.6.2.1","","Road, Type SA, 80 mm thickness","m²",700,{"v":0,"d":"0.00"},{"$f":"ROUND(G86 * H86,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9098bcea-1310-461a-abe5-3d6fe8c2840a","C1.6.2.2","","Admin Parking, Type SA, 80 mm thickness","m²",370,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4ac9b8aa-8abb-4ab7-8fd3-cecf2f93d506","C1.6.2.3","","Admin, Type SA, 80 mm thickness","m²",280,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7bcb5144-b980-40a1-8280-580dc473932f","C1.6.2.4","","Blower Buiding, Type SA, 80 mm thickness","m²",650,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","fbaa0f8a-d9dc-454c-bc34-127574af4943","C1.6.2.5","","Workshop Buiding, Type SA, 80 mm thickness","m²",170,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f27dfab5-97ab-4250-93d5-80cba5f48b00","C1.6.2.6","","MCC Buiding, Type SA, 80 mm thickness","m²",140,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","450fc139-82ad-486b-bc3f-56dd26d89350","C1.6.2.7","","Guardhouse, Type SA, 80 mm thickness","m²",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","51980dc9-f5aa-4766-9014-8d98d34f6d71","C1.7","","STORMWATER DRAINAGE",{"$nulls":4},"Dflt"]
["Header3","273d1540-9cce-4c60-96c3-624fc72b4940","C1.7.1","SANS 1200DB","SITE CLEARANCE AND EXCAVATION",{"$nulls":4},"Dflt"]
["Item","37da4f5e-e13c-46da-a88d-e51a2fdc0864","C1.7.1.1","8.3.1(a)","Clear Site","m²",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G95 * H95,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c76d34ad-9bf9-4190-8f75-283e959be67c","C1.7.1.2","8.3.2(a)","Excavate, select materials, backfill and dispose of surplus/unsuitable material","m³",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","0ff0928d-a872-442a-bdf4-2ca93b476bd5","C1.7.2","SANS 1200LE","CATCHPITS",{"$nulls":4},"Dflt"]
["Label","d4ce0550-70cd-46c4-babd-4ac0d5b42326","","","Construct complete with grid inlets :",{"$nulls":4},"Dflt"]
["Item","0b7194d1-4040-47a7-815f-eb783c2efdcf","C1.7.2.1","PSLE 8.2.4\nPSLE 8.2.14","a) Type to be confirmed on site as shown on Dwg. No. J40073/010-111","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G99 * H99,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","10065088-0de4-4071-92d0-e15dd97bbd8e","C1.7.3","","HEADWALLS",{"$nulls":4},"Dflt"]
["Label","10d75162-9a80-4447-9d5b-9d4e4771ab3e","","PSLE 8.2.4\nPSLE 8.2.14","Construct headwall to Dwg. No. J40073/010-111 including excavation, backfilling and compaction to fit pipes:",{"$nulls":4},"Dflt"]
["Item","de6f3525-233b-46a7-95d6-04de63e876f8","C1.7.3.1","","300 mm NB","No",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G102 * H102,2)","v":{"v":0,"d":"0.00"}}]
["Item","016ad5d8-6206-4e3b-997b-55ce2ccf451a","C1.7.3.2","","300 mm NB (Double)","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Header3","9380b736-d9d3-4319-a49b-6059fca8b8f2","C1.7.4","","MISCELLANEOUS"]
["Label","8392372c-082e-4b77-91ab-327d9caaf543","","","Construct open drains to Dwg. No.  J40073/010-114, complete and all inclusive, including excavation, backfilling, concrete, setting out, etc:"]
["Item","049c5576-2220-485b-9066-e22cf4fdc94b","C1.7.4.1","","Concrete lining: 25 MPa/19 mm, 2,4 m wide and 0,25 m deep","m",230,{"v":0,"d":"0.00"},{"$f":"ROUND(G106 * H106,2)","v":{"v":0,"d":"0.00"}}]
["Item","9eec731f-5250-47d7-bc4e-02ee2379f7ce","C1.7.4.2","","No lining","m",100,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]

{"sheet":"BILL D.1.","index":10,"n_rows":163,"n_cols":10,"rows_kept":163,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.1.",null,"MCC BUILDING",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","c9cc560b-6fa2-4dc9-a00b-c438df2a845a","D.1.1","","MCC BUILDING ",{"$nulls":4},"Dflt"]
["Label","9af9913e-f184-4a3a-af08-1e3fc38cbb81","","JBCC","SECTION D.1.1 : MCC BUILDING ",{"$nulls":4},"Dflt"]
["Sum","d22f2434-863c-42f0-a46e-44ba29d4fcef","D.1.1.1","","Housekeeping (Includes cleaning and organising working area)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H11,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","ab140272-10ac-4607-a21b-ab4018e23b48","D.1.1.2","","EARTHWORKS (PROVISIONAL)",{"$nulls":4},"Dflt"]
["Label","60bace5d-ff2e-4f89-879f-1c6f36e5ce1e","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","ac18515b-11dc-4a2e-be10-7783adee1a2c","","","Note:",{"$nulls":4},"Dflt"]
["Label","573b6822-0181-4676-8ce1-61c76e9d19b7","","","Wherever a trade name for any product has been described in the Priced Document attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained prior to the closing date for submission of tenders.",{"$nulls":4},"Dflt"]
["Label","6845bf37-8be0-4532-9ea9-1ddaf8c1d272","","","if prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for.",{"$nulls":4},"Dflt"]
["Label","11092036-bcf2-49f5-bc7d-712ef56cd35b","","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","d4253f69-f3b2-4f39-ac77-ca5b2d78f5b9","","","Extra over all excavations for carting away:",{"$nulls":4},"Dflt"]
["Item","60d0370f-c9bd-441e-a2e8-639931c9516c","D.1.1.2.1","","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the Contractor","m³",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G19 * H19,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","4325156c-d1a5-40fe-accf-867932c14d70","D.1.1.3","","FILLING, ETC",{"$nulls":4},"Dflt"]
["Label","73110be9-a724-42ad-9e17-226212154d06","","","Backfilling with imported G7 material spread in layers not exceeding 150mm thick under floors, etc and compacted to 97% Mod. AASHTO density",{"$nulls":4},"Dflt"]
["Item","4ec52410-a788-4cb1-a851-f77c1d4c3584","D.1.1.3.1","","Under apron, etc.","m³",7,{"v":0,"d":"0.00"},{"$f":"ROUND(G22 * H22,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","90541736-339c-4480-b222-df53670b0986","D.1.1.4","","CONCRETE, FORMWORK AND REINFORCEMENT  ",{"$nulls":4},"Dflt"]
["Label","503a3b22-499b-42d9-9941-927c2893ac55","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","771d1506-aa1e-422f-b572-8900c48833de","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","e4f237e3-124a-4d93-87c8-0c5f428e7802","","","CONCRETE ",{"$nulls":4},"Dflt"]
["Label","6a00edc8-642f-4ceb-b4b9-489b04c59b79","","","UNREINFORCED CONCRETE ",{"$nulls":4},"Dflt"]
["Label","1407b1cf-2969-4d04-bdc0-66c930fe3105","","","Unreinforced concrete 25MPa at 28 days in ",{"$nulls":4},"Dflt"]
["Item","fd75f202-6da1-46d5-822e-c65b61c67ae6","D.1.1.4.1","","Surface beds (apron slabs)","m³",7,{"v":0,"d":"0.00"},{"$f":"ROUND(G29 * H29,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5dafa638-35ee-45c6-9fb9-1e2d1057c9cd","","","REINFORCED CONCRETE ",{"$nulls":4},"Dflt"]
["Label","637a9d9c-049b-44b3-a2b3-161951f455ec","","","Vibrated reinforced concrete 25MPa at 28 days in ",{"$nulls":4},"Dflt"]
["Item","85ef082c-71ba-4eb3-93cf-ab9d4c4e160a","D.1.1.4.2","","Surface beds (ramps)","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G32 * H32,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f6ce1479-04ce-4763-acd3-cbf09f3706f5","","","CONCRETE SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","cb6df4d9-fc8b-422f-b5cf-177da3076879","","","Finishing top surfaces of concrete smooth with a wood float ",{"$nulls":4},"Dflt"]
["Item","5cde5925-5fe2-45b7-9a6a-e5b6ac9cb46b","D.1.1.4.3","","Surface beds, slabs, etc (apron slabs)","m²",91,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","30f15182-9adc-4089-919e-612ee8e6a70d","","","Finishing top surfaces of concrete to an evenly ribbed non-slip surface (ramps)",{"$nulls":4},"Dflt"]
["Item","c8000778-019e-4e00-a460-77f93724a75b","D.1.1.4.4","","Surface beds, slabs, etc (ramps)","m²",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G37 * H37,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","722a492c-49bb-49ea-b119-a52ba4dd9035","","","FORMWORK ",{"$nulls":4},"Dflt"]
["Label","6c4c27a7-a303-4586-9113-700a92c413dd","","","ROUGH FORMWORK (DEGREE OF ACCURACY III) ",{"$nulls":4},"Dflt"]
["Label","3da66755-1784-4048-8347-6e7e5a8a1fb5","","","MOVEMENT JOINTS, ETC",{"$nulls":4},"Dflt"]
["Label","0a8880f7-e5e5-4b53-94f1-c42d8d604c0a","","","Saw cut joints:",{"$nulls":4},"Dflt"]
["Item","0c7dd71f-7353-4059-aaa2-15b4e6043a20","D.1.1.4.5","","6 x 30mm Saw cut joints in top of concrete","m",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G42 * H42,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c01118a7-385f-4d78-b783-2b47a332963f","","","STEEL REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","756d249c-be67-49f3-ac5c-be6d1c8a999f","","","Fabric reinforcement:",{"$nulls":4},"Dflt"]
["Item","46882287-5cbf-4bf0-a66a-2eacf7ee679f","D.1.1.4.6","","Steel mesh reinforcement reference 311 in concrete slabs, surface beds, etc","m²",17,{"v":0,"d":"0.00"},{"$f":"ROUND(G45 * H45,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","ca7952b4-4f8f-481a-ac76-6c51e20e62b2","D.1.1.5",""," MASONRY ",{"$nulls":4},"Dflt"]
["Label","03a6a55f-0279-4e32-bc70-04b10c2b780a","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","dc8e974f-ca10-49af-a24b-6e317ecf5f19","","","SUPERSTRUCTURE ",{"$nulls":4},"Dflt"]
["Label","a4328511-3e64-4186-bc93-c3cd4ed03317","","","Brickwork of NFP bricks (7 MPa nominal compressive strength) in class II mortar ",{"$nulls":4},"Dflt"]
["Item","b4c25e97-40cb-4ce6-bfd1-69f771426cb0","D.1.1.5.1","","One brick walls ","m²",7,{"v":0,"d":"0.00"},{"$f":"ROUND(G50 * H50,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","8805308a-5e38-4b0f-83f8-0e00b36b990b","D.1.1.5.2","","330mm Solid walls ","m²",7,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","563a0d42-f18f-47d5-b853-4299276e9bd4","","","BRICKWORK SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","c24b585d-500d-4c11-9277-2440fae0c12d","","","Joint forming material in movement joints ",{"$nulls":4},"Dflt"]
["Item","a8fc8e65-3ba1-4d4e-9e0f-a29984f93a4c","D.1.1.5.3","","10mm \"Jointex\" Expanded polystyrene with one tear off strip built in horizontal between brick walls and concrete not exceeding 300mm wide ","m",65,{"v":0,"d":"0.00"},{"$f":"ROUND(G54 * H54,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","fb6c752b-9dc4-49ca-8554-40a2921d60d2","D.1.1.5.4","","10 x 10mm Polysulphide sealant in joints ","m",65,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","09d7ed56-871b-44db-8f0a-9e24d7c1359a","D.1.1.6","","WATERPROOFING ",{"$nulls":4},"Dflt"]
["Label","f1faa789-fe9e-48e7-8a15-77dc796598cb","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","2ca243cd-0b6b-452d-a22a-bbd5e112029c","","","WATERPROOFING TO ROOFS, BASEMENTS, ETC ",{"$nulls":4},"Dflt"]
["Label","7b8b5a28-4c72-405a-8bc4-2f1d59d95e95","","","One layer Derbigum SP4 waterproofing membrane, with 75mm side laps and 100mm end laps, sealed to primed surface to falls and crossfalls by 'torch-fusion' finished with one coat of acrylic primer followed by two coats acrylic paint. Waterproofing to be  installed by an Approved Derbigum Contractor under a ten year guarantee. ",{"$nulls":4},"Dflt"]
["Item","d15965c4-818c-4bdf-9745-43856fc7e76e","D.1.1.6.1","","On walls /cable trenches","m²",46,{"v":0,"d":"0.00"},{"$f":"ROUND(G60 * H60,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","0412f855-191b-42a1-8128-b741e6d9c135","D.1.1.7",""," ROOF COVERINGS ",{"$nulls":4},"Dflt"]
["Label","87e54197-25fe-458b-8b84-7d6c507cdb05","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","090f852c-cb49-469c-91b2-b8deaf533185","","","PROFILED METAL SHEETING AND ACCESSORIES ",{"$nulls":4},"Dflt"]
["Label","5dd64b47-1fd0-4bee-b591-2f5ed3344cde","","","\"Klip-Lok 700\" profile roll-formed in continuous lengths from certified Galvanised steel Z200 0.58mm complying with ISQ 550 (3T) (A653) with a Chromadek Colomet finish to one side and standard backing coat, Papyrus white to other and accessories, fixed to timber purlins in strict accordance with manufacturer's specifications.",{"$nulls":4},"Dflt"]
["Item","5f231299-271d-4801-a70f-cfcb3aa4914b","D.1.1.7.1","","Head wall flashings 375mm girth 2 times bent to suit roof profile ","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G65 * H65,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","71a690fb-8ab8-49dc-a93c-2d078e7c6904","D.1.1.7.2","","Counter flashing 185mm girth 2 times bent ","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b249c484-dc06-49a4-84d3-6af8b1394c8d","D.1.1.7.3","","Insulation boarding in 1200mm widths with longitudinal flap joints, laid over purlins (at approximately 1000mm centres) and fixed concurrent with roof covering, including holes through boards etc ","m²",260,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","86d0b978-cf80-4ab1-8690-601c2bd25763","D.1.1.8","","CARPENTRY AND JOINERY ",{"$nulls":4},"Dflt"]
["Label","85d2cb27-7ba2-44af-ba3f-d99635095c50","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","00b53f49-3786-49fb-b0d5-429af5078da1","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","5cdd35eb-4988-4079-961a-84311e23d748","","","Joinery ",{"$nulls":4},"Dflt"]
["Label","7494b1f7-30e5-4efb-b62c-be1f422f916e","","","Descriptions of frames shall be deemed to include frames, transomes, mullions, rails, etc  ",{"$nulls":4},"Dflt"]
["Label","e1a42147-5a3e-46bb-bda9-703d6519c2ff","","","Descriptions of hardwood joinery shall be deemed to include pelleting of bolt holes ",{"$nulls":4},"Dflt"]
["Label","9ec9e533-a31b-4800-8cb8-9a1dbf4845af","","","Fixing ",{"$nulls":4},"Dflt"]
["Label","400218bd-557b-417b-9d77-35ebefe7f00f","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete  ",{"$nulls":4},"Dflt"]
["Label","1d7c9739-d75f-46c0-b076-41788a062dda","","","EAVES, VERGES, ETC ",{"$nulls":4},"Dflt"]
["Item","651330ef-70d7-46b6-81c8-2e212fb5b766","D.1.1.8.1","","Install missing louvres at the two roof sides ","m²",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G77 * H77,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","641f93a9-3b42-457e-a096-c2379bf69e5e","D.1.1.9","","CEILINGS AND PARTITIONS, ETC ",{"$nulls":4},"Dflt"]
["Label","069d5225-a47a-44aa-b1a0-2f04d07df11e","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","739803c9-043b-4592-93b9-23b589779998","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","29763a93-bc9f-4b0b-9c72-ca44e716f8ee","","","Descriptions ",{"$nulls":4},"Dflt"]
["Label","222ca373-56c7-46d7-958c-9d875bb2e477","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete ",{"$nulls":4},"Dflt"]
["Label","13f3bcd4-237f-4527-be7a-a21fbbf7b24d","","","Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere ",{"$nulls":4},"Dflt"]
["Label","73dc7c07-9e42-4777-abd7-3beae71a04d6","","","Electrical  light  fittings, diffusers, panels, etc generally are \"lay in\"  units  of  the  same dimensions as the suspension grid described  and  allowance  must  be  made  accordingly  for their support  inclusive  of any flexibility insetting out that may be required (ceiling panels have not been deducted and pricing is to take cognisance thereof)  ",{"$nulls":4},"Dflt"]
["Label","cbe443ac-5368-405e-843b-24e939f69b09","","","NAILED-UP CEILINGS ",{"$nulls":4},"Dflt"]
["Label","47011b78-528c-4669-887e-babb658ae718","","","\"Everite\" or equally approved ceiling panels ",{"$nulls":4},"Dflt"]
["Item","aae695e7-5f3e-453b-b0e4-2a1ea8aaf0e1","D.1.1.9.1","","Ceilings of 1200 x 2400 x 6mm thick panels including 38 x 38mm SA Pine brandering at 450mm centres in both directions ","m²",84,{"v":0,"d":"0.00"},{"$f":"ROUND(G87 * H87,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b4109718-30a3-473a-b485-c95b8ba62ea4","","","Gypsum plasterboard cornices ",{"$nulls":4},"Dflt"]
["Item","d944bae4-c092-4c2e-ac46-2c06f91ff9a0","D.1.1.9.2","","75mm Coved cornices ","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G89 * H89,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","4501ac2a-9270-487c-a8ea-46ba96ee7615","D.1.1.10","","PLASTERING ",{"$nulls":4},"Dflt"]
["Label","651bf910-48c3-4fb4-84e7-8e9389d5c3f1","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","8e8c7927-6c84-4355-990c-3ac108efad81","","","INTERNAL PLASTER  ",{"$nulls":4},"Dflt"]
["Item","e2f83119-44f1-40ba-aade-110d89750b91","D.1.1.10.1","","Repair Cracks on plastered wall by using polyfilla or equivalent product that is approved byEngineer.  ","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G93 * H93,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","efbc0e74-db6d-43e5-a927-e0c392079b59","","","One coat 1:5 cement plaster 15mm thick on brickwork or concrete finished with sponge roller",{"$nulls":4},"Dflt"]
["Item","89eebeaa-4ed0-44ac-86b9-6fa485c9d985","D.1.1.10.2","","On walls","m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G95 * H95,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b0857810-b025-4158-8022-480270d81b69","","","Gypsum skim plaster",{"$nulls":4},"Dflt"]
["Item","79f4dfb1-802b-4411-a8b4-0f70356a59f9","D.1.1.10.3","","On ceilings ","m²",245,{"v":0,"d":"0.00"},{"$f":"ROUND(G97 * H97,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","d93982ec-7563-476f-8102-b7122f99128b","","","EXTERNAL PLASTER ",{"$nulls":4},"Dflt"]
["Label","1cf926da-8f15-48af-aac0-6a7715fafe08","","","One coat 1:5 cement plaster 12mm thick on brickwork or concrete finished with a wood trowel ",{"$nulls":4},"Dflt"]
["Item","1a293faf-37a9-4831-8d51-2c1a46a1e2ac","D.1.1.10.4","","On beams ","m²",45,{"v":0,"d":"0.00"},{"$f":"ROUND(G100 * H100,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","5ecdb4ea-40b2-478e-8edd-2034d53ecbba","D.1.1.11","","PLUMBING AND DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","a0e5b611-483e-4440-b006-e9a3a4672cc6","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","8d3af14a-b37f-4ed2-977b-2ea3f39319f2","","","RAINWATER DISPOSAL ",{"$nulls":4},"Dflt"]
["Label","88c2db34-3be4-4111-b492-18971d5cda52","","","\"Watertite\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","54903a64-1564-4edc-91a7-f6003543680b","D.1.1.11.1","","140 x 150mm box gutter x 0.9mm brackets fixed at 500mm centres ","m",70,{"v":0,"d":"0.00"},{"$f":"ROUND(G105 * H105,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Rate Only","c95122d8-ad47-4908-8843-492f6ebac52f","D.1.1.11.2","","Extra over gutter for outlet for 75mm dia. pipe ","No.",0,{"v":0,"d":"0.00"},"Rate Only","Dflt"]
["Item","1855b673-6f49-47b0-bfde-a3179c5468ab","D.1.1.11.3","","75 x 1.27mm Diameter rainwater pipes ","m",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G107 * H107,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","028f62fd-dc27-4b02-ae27-4df9a3d46abc","D.1.1.11.4","","Extra over rainwater pipe for bend ","No.",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b3061b5b-4b40-4abc-8e5a-629b3c62c542","D.1.1.11.5","","Extra over rainwater pipe for shoe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","f5d18833-2a06-4b69-8905-194e134681c8","D.1.1.12","","PAINTWORK ",{"$nulls":4},"Dflt"]
["Label","83ca1342-bb48-4eb5-96d0-c92592ebb37e","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","ef08a7ee-1193-4282-a874-1493ce8558b4","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","41fe5c53-e072-461d-a3b6-997b0146cd8c","","","All colours to be selected by the Architect ",{"$nulls":4},"Dflt"]
["Label","400b6121-cdf5-4e98-b69b-edc1088cfb69","","","Only approved brands of paint shall be permitted ",{"$nulls":4},"Dflt"]
["Label","49be3a46-e6c8-463a-917e-b86592181367","","","All painting measured generally will be in colours with a value of more than 7 on the Munsell system in accordance with the relevant SABS specification. Any painting in colours with a value of 7 or less on the Munsell system shall be given as paintwork in darker colours ",{"$nulls":4},"Dflt"]
["Label","c8b6055b-f7e9-4002-a882-01598b70a210","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","6bf6ce61-51ad-476a-a60d-784cd42b73c7","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Prime with one coat of plaster primer all in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","3c1fa20e-f2dd-43dc-bba2-d3874cf8d54c","D.1.1.12.1","","On walls ","m²",520,{"v":0,"d":"0.00"},{"$f":"ROUND(G118 * H118,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","830d61d7-6670-4003-9611-47df830128bf","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","4a27ab5c-d5de-4339-9e01-758eb83e5b23","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Finish with 2 coats of super acrylic PVA paint or similar approved. All in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","8cd30082-254e-4e6d-8281-3f141b870d04","D.1.1.12.2","","On walls ","m²",520,{"v":0,"d":"0.00"},{"$f":"ROUND(G121 * H121,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","413b2da0-397c-43aa-b861-563311e34c16","","","ON EXTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","253d1b7e-ea64-455d-9dad-6b9a3d7114b0","","","Primer and finish with two coats \"Marmoran Armourbrush\" or equally approved, applied in strict accordance to manufacturer's instructions. ",{"$nulls":4},"Dflt"]
["Item","e2cf4c42-367c-4a37-b167-7149f97a6780","D.1.1.12.3","","On walls / RC beam","m²",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G124 * H124,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8f64126c-7932-43ce-97f0-a459842a79b8","","","ON PLASTERBOARD SURFACES ",{"$nulls":4},"Dflt"]
["Label","9875db75-99f7-48bb-8fbb-6cc3bfcb235a","","","One coat alkali resistant primer and two coats PVA emulsion paint for interior use ",{"$nulls":4},"Dflt"]
["Item","263cfa3b-a133-41f1-a3d0-42aa7531db43","D.1.1.12.4","","Ceilings and cornices  ","m²",243,{"v":0,"d":"0.00"},{"$f":"ROUND(G127 * H127,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","af37b922-de81-4b31-8d85-341ea1b11147","","","ON METAL SURFACES ",{"$nulls":4},"Dflt"]
["Label","92dee1c7-a275-4719-8283-0aa27e78c182","","","One coat \"Namelcote\" zinc chromate primer UC 53, one coat \"Plascon Galvogrip\" metal primer and two coats \"Velvaglo\" polyutherane enamel paint (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","491b88d0-70a9-4912-a7a0-b2d6b6d19e6b","D.1.1.12.5","","On door frames etc ","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G130 * H130,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2efc4f2d-7baa-48dc-aff2-d996487e9deb","D.1.1.12.6","","On doors  (both sides)","m²",36,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","322ebb9b-f275-4066-b60e-decafa43d497","","","ON WOOD SURFACES ",{"$nulls":4},"Dflt"]
["Label","1cc82cf5-87a1-431e-a17f-ec6550883955","","","One coat \"Spick and Span\" Oil based wood primer (UCS2), two coats \"Velvago Polyurethane enamel paint (VLO). (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","34564dad-1db9-4ced-a8e8-9667020c8d4e","D.1.1.12.7","","On doors  (both sides)","No.",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G134 * H134,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","06470377-9699-4eff-a660-3570c42badbc","D.1.1.13","","Cable Trench",{"$nulls":4},"Dflt"]
["Item","5d370b64-9935-49b3-8d5d-c4eefb1b49f5","D.1.1.13.1","","Install the 655mm wide x 6mm VASTRAP with 3 No. 30x8mm plate stiffeners per panel, trench plate panel cover over the cable trench where no MCC and Electrical panels are placed","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G136 * H136,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","7aa44fb6-07ad-4860-bd87-3a85010b24e2","D.1.1.14","","Concrete Works (Apron)",{"$nulls":4},"Dflt"]
["Label","6d2313f4-c8d7-4dc3-bd57-5dc27de6c206","","SANS1200 GA","Concrete (Small Works) - Formwork",{"$nulls":4},"Dflt"]
["Item","117e71d9-50d4-4c91-9069-27e4253f82a3","D.1.1.14.1","8.2.1","Formwork - Rough Finish surface","m²",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G139 * H139,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5d6a22ef-219c-4a0a-b189-7070718ac38c","","SANS1200 GA","Concrete (Small Works) - Steel",{"$nulls":4},"Dflt"]
["Item","80292010-8364-4044-b05d-9a868baae8e9","D.1.1.14.2","8.3.2","High Tensile Welded Mesh Ref 245","m²",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G141 * H141,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","32664219-b848-4b24-be77-8ec8015fc5ba","","SANS1200 GA","Concrete (Small Works) - Concrete",{"$nulls":4},"Dflt"]
["Item","cb7cdc60-051e-4e5e-a48d-01a99ff84571","D.1.1.14.3","8.4.3","20 Mpa, 19mm aggregates Concrete","m³",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G143 * H143,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ad799d2e-1422-41e0-9044-15d11c62498c","D.1.1.14.4","8.4.4","Unformed Wooden floated surface finish ","m²",91,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8c040cb5-3abb-4ca5-a627-8d07c5f9d2ba","D.1.1.14.5","8.5.0","6mm x 30mm deep Saw cut joints from top of concrete","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d8feb7ba-5b4e-4a3f-b507-3dd40006d408","D.1.1.14.6","","Install 10mm Jointex Expanded polystyrene","m",65,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2b47de54-291b-49af-9563-1e41434c60a8","D.1.1.14.7","","Install 10mm x 10mm polysulphide ","m",65,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","84c5e232-401d-4af8-aa87-9e8cef114065","D.1.1.14.8","","Allow R30,000.00 as provision to fix the existing MCC Room door damaged locking mechanism and make good the cracked frame anchorage brickwork.    ","Prov.Sum",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"},"Dflt"]
["Sum","5aca9631-cdba-4557-a946-5122145f9c39","D.1.1.14.9","","Supply and Install all complete fire and signage plan in accordance with the Drawing No. J40073/010 - 406F Rev 1","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H149,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","4b15f8e8-7f0e-4e94-b07c-910468a8e98c","D.1.1.15","","TILING ",{"$nulls":4},"Dflt"]
["Label","279fdfe0-91cb-4f2b-99ff-f8715e61c844","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","977c451e-fb54-4a61-9641-a0f349f0ea52","","","\"Note All tiling shall be fixed to plaster or screed with an approved adhesive; the adhesive shall be as recommended by the manufacturer of the tiles. \"",{"$nulls":4},"Dflt"]
["Label","7a370f92-b391-4bdb-9d9b-ce7eb833efa8","","","FLOOR TILING  -  in accordance with interior finishing schedule Drw. No. 010-406G Rev 0",{"$nulls":4},"Dflt"]
["Item","60b8f883-e718-4dba-8d6b-2835ee667a72","D.1.1.15.1","","Supply and install 40mm Untinted grano  with 1 cement/1 stone chippings / 1 sand mix finished with steel trowel in bays not to exceed 12m2.  Provide ABE or equal SABS approved epoxy paint finish on Grano floors","m²",230,{"v":0,"d":"0.00"},{"$f":"ROUND(G154 * H154,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5f3e98e7-b709-41b5-a400-d31106a1bf19","","","Skirting - Grano ",{"$nulls":4},"Dflt"]
["Item","5b2b905e-3e6a-484b-b268-43b0734c544e","D.1.1.15.2","","19mm thick rounded (1:4 cement mix) grano with V Joints 75 mm above finished floor level.  Skirting to project 6mm from finished wall fall with arris top edge. ","m",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G156 * H156,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","15c08c08-b1b6-40b2-b70b-80bed8452d36","D.1.1.16","","PROVISIONAL SUMS ",{"$nulls":4},"Dflt"]
["Label","486be2e5-29ed-4c4b-b42a-b57b034eceda","","","For preambles see \"Model Preambles for Trades\""]
["Label","7f30741f-2797-4877-9f12-5ace67a24328","","","BUDGETARY ALLOWANCES (Roof Rust Repair, Electrical connection, Water Connection, etc)"]
["Item","e6f177d3-0372-4e9b-ac53-0ff490d4e87c","D.1.1.16.1","","Provide for Provisional Sum for Additional Work as instructed by Engineer","Prov.Sum",1,{"v":400000,"d":"400,000.00"},{"$f":"ROUND(G160 * H160,2)","v":{"v":400000,"d":"400,000.00"}}]
["% Previous","7c24c33f-5b2c-414c-a3ef-d8ccc41c0bea","D.1.1.16.2","","Add for profit and general attendance upon above if required  ","%",{"$f":"I160","v":{"v":400000,"d":"400 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Label","f0cf3e2d-6993-4d2c-96f6-2cf978bc4832","","","Corrective work to structure/building"]
["Sum","688ab4d7-ae44-4777-82c0-a15e6fcbee8b","D.1.1.16.3","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":200000,"d":"200,000.00"},{"$f":"ROUND(H163,2)","v":{"v":200000,"d":"200,000.00"}}]

{"sheet":"BILL D.2.","index":11,"n_rows":191,"n_cols":10,"rows_kept":191,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.2.",null,"BLOWER BUILDING",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","988c4295-cb92-45af-80c9-765241902519","D.2.1","","BLOWER BUILDING",{"$nulls":4},"Dflt"]
["Label","f2a49c96-802f-4ce3-9983-8508de6d090f","","JBCC","SECTION D.2.1 : BLOWER BUILDING",{"$nulls":4},"Dflt"]
["Sum","1c56e4cb-b254-4833-bf20-f5632978c1f2","D.2.1.1","","Housekeeping (Includes cleaning and organising working area)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H11,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","fc244e1d-395e-4798-b846-0119c3ad9c18","D.2.1.2","","EARTHWORKS (PROVISIONAL)",{"$nulls":4},"Dflt"]
["Label","20c966c2-a4ca-4bab-bdd4-a1061335498f","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","730c712b-621f-41fd-810f-f43384e6a29c","","","Note:",{"$nulls":4},"Dflt"]
["Label","37548691-5077-4ea6-9587-255a3c4d0820","","","Wherever a trade name for any product has been described in the Priced Document attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained prior to the closing date for submission of tenders.",{"$nulls":4},"Dflt"]
["Label","924f8fff-250c-46d7-b26b-a685a43bcbae","","","if prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for.",{"$nulls":4},"Dflt"]
["Label","c7e45230-e394-454f-b734-ac92009b9fa4","","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","c7a5abc9-ed6b-4f89-a839-d784f19f5b4b","","","Extra over all excavations for carting away:",{"$nulls":4},"Dflt"]
["Item","c7dcab78-9f15-46e5-ab7b-e2a6487d0d95","D.2.1.2.1","","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the Contractor","m³",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G19 * H19,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","5ca46161-0873-4f91-a4ec-be154e486be3","D.2.1.3","","FILLING, ETC",{"$nulls":4},"Dflt"]
["Label","51ce2108-f6be-4eb7-8ca8-6db28d6edf4c","","","Backfilling with imported G7 material spread in layers not exceeding 150mm thick under floors, etc and compacted to 97% Mod. AASHTO density",{"$nulls":4},"Dflt"]
["Item","87db8f83-1cb9-4264-aa95-a15570c4ed33","D.2.1.3.1","","Under floors, steps, paving, etc.","m³",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G22 * H22,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","397cbefc-90fe-4cec-9cc5-579434d4222b","D.2.1.4","","CONCRETE, FORMWORK AND REINFORCEMENT  ",{"$nulls":4},"Dflt"]
["Label","21f67f3f-a56a-44ce-bbf4-e7016799a845","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","1d6054e9-dcdb-41d7-bcea-bbe96d82d45b","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","6a55b3b1-77a8-43ca-990e-8e6a5a4cf3ee","","","CONCRETE ",{"$nulls":4},"Dflt"]
["Label","d0ff1a23-74d7-4bf3-8691-8f92aa769687","","","UNREINFORCED CONCRETE ",{"$nulls":4},"Dflt"]
["Label","15b3186f-38b5-4c67-8727-7ed22e40ed3b","","","Unreinforced concrete 25MPa at 28 days in ",{"$nulls":4},"Dflt"]
["Item","e5296301-566c-433b-9dda-438617ef56f5","D.2.1.4.1","","Surface beds (apron slabs)","m³",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G29 * H29,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","160cbee8-e208-4e53-8c63-d52d368de5fb","","","REINFORCED CONCRETE ",{"$nulls":4},"Dflt"]
["Label","a26d6744-19a2-4e85-98b1-36863146c7ee","","","Vibrated reinforced concrete 25MPa at 28 days in ",{"$nulls":4},"Dflt"]
["Item","0508eeb1-5b8d-4cd2-b70e-6cd66f41ab8f","D.2.1.4.2","","Surface beds (ramps)","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G32 * H32,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","28c7839a-ee26-4880-aac2-bf81184cd0bd","","","CONCRETE SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","083b6e98-3c3c-46ad-9f2e-4b25db19b2e8","","","Finishing top surfaces of concrete smooth with a wood float ",{"$nulls":4},"Dflt"]
["Item","55311264-30d7-4e94-a1a4-ee4361d0dbf4","D.2.1.4.3","","Surface beds, slabs, etc (apron slabs)","m²",82,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c1be80b9-a5d3-4aeb-bd08-e6397c499974","","","Finishing top surfaces of concrete to an evenly ribbed non-slip surface (ramps)",{"$nulls":4},"Dflt"]
["Item","646522cd-1775-4ed3-858c-a9e8fd750d2e","D.2.1.4.4","","Surface beds, slabs, etc (ramps)","m²",17,{"v":0,"d":"0.00"},{"$f":"ROUND(G37 * H37,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","e9444047-370b-4ee1-9f6c-40e90e28e09e","","","FORMWORK ",{"$nulls":4},"Dflt"]
["Label","4509427e-bf9a-4509-872a-97e55905c7bc","","","ROUGH FORMWORK (DEGREE OF ACCURACY III) ",{"$nulls":4},"Dflt"]
["Label","fa831e10-d7ce-4cca-bac5-ae16848a8a87","","","Rough formwork to sides ",{"$nulls":4},"Dflt"]
["Item","8e39a39c-2b62-41ea-8cac-e938b435080e","D.2.1.4.5","","Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",75,{"v":0,"d":"0.00"},{"$f":"ROUND(G41 * H41,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8df4d0b7-b276-4bde-8784-186707406f66","","","MOVEMENT JOINTS, ETC",{"$nulls":4},"Dflt"]
["Label","d13ea94e-91c4-4469-b628-9913094dbf6a","","","Saw cut joints:",{"$nulls":4},"Dflt"]
["Item","cdb9bff5-9fe0-4909-aea2-7639851df836","D.2.1.4.6","","6 x 30mm Saw cut joints in top of concrete","m",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G44 * H44,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b5dcdbe1-07e8-4c50-bc77-bd2656909212","","","STEEL REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","27929559-0130-42f6-8ed6-36d5bc288ad5","","","Fabric reinforcement:",{"$nulls":4},"Dflt"]
["Item","a83334e4-1585-4c81-a206-d2a9bc0b713e","D.2.1.4.7","","Steel mesh reinforcement reference 311 in concrete slabs, surface beds, etc","m²",17,{"v":0,"d":"0.00"},{"$f":"ROUND(G47 * H47,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","950d5264-5d07-44bd-81e8-3261c772d769","D.2.1.5","","MASONRY ",{"$nulls":4},"Dflt"]
["Label","ff61644f-fb96-4cbc-bad9-23365f692410","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","0257ef71-82bb-440b-815e-de34729cff7d","","","FOUNDATIONS ",{"$nulls":4},"Dflt"]
["Label","52b0709b-44f9-4311-a987-2c29a1ea311d","","","Brickwork of NFX bricks (14 MPa nominal compressive strength) in class I mortar ",{"$nulls":4},"Dflt"]
["Item","5ea76eef-8d14-4b80-b7d8-9117a8de0ea5","D.2.1.5.1","","One brick walls ","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","49abd7d9-9875-4d54-9902-443b0c84279f","","","SUPERSTRUCTURE ",{"$nulls":4},"Dflt"]
["Label","0f6b51b1-38e9-4a28-9323-08d4a10255da","","","Brickwork of NFP bricks (7 MPa nominal compressive strength) in class II mortar ",{"$nulls":4},"Dflt"]
["Item","70e6dc7f-a373-4477-a558-b659bd35b23d","D.2.1.5.2","","Half brick walls ","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G55 * H55,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2af8f254-979d-42f6-b02e-e8cd2ff3afd6","D.2.1.5.3","","One brick walls ","m²",260,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","72419496-352f-4cb5-ae73-60e51b7d7815","D.2.1.5.4","","330mm Solid walls ","m²",28,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","ef037f3d-e40e-4610-af3f-0914ed1cc9b7","","","BRICKWORK SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","f221484f-6ac6-4efc-9b65-aee9a14d7124","","","Joint forming material in movement joints ",{"$nulls":4},"Dflt"]
["Item","45e7b4f0-72b6-4238-ad2d-8385ac43c469","D.2.1.5.5","","10mm \"Jointex\" Expanded polystyrene with one tear off strip built in horizontal between brick walls and concrete not exceeding 300mm wide ","m",130,{"v":0,"d":"0.00"},{"$f":"ROUND(G60 * H60,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3f60fc11-e094-470f-a815-1163de307a64","D.2.1.5.6","","10 x 10mm Polysulphide sealant in joints ","m",130,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","7de1d17f-e522-4192-b7df-f7ea837ae4f3","D.2.1.6","","WATERPROOFING ",{"$nulls":4},"Dflt"]
["Label","a01699b0-0469-4225-a4f5-3df43e5c4f98","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","ec288d01-550f-4caa-8621-f535cbf5443e","","","WATERPROOFING TO ROOFS, BASEMENTS, ETC ",{"$nulls":4},"Dflt"]
["Label","8cfc1fa2-e0e3-473b-b6f9-a97cedeb03fa","","","One layer Derbigum SP4 waterproofing membrane, with 75mm side laps and 100mm end laps, sealed to primed surface to falls and crossfalls by 'torch-fusion' finished with one coat of acrylic primer followed by two coats acrylic paint. Waterproofing to be installed by an Approved Derbigum Contractor under a ten year guarantee. ",{"$nulls":4},"Dflt"]
["Item","0d489b0b-072d-4cac-9af6-fe3274b253c3","D.2.1.6.1","","On walls/Cable Trenches ","m²",46,{"v":0,"d":"0.00"},{"$f":"ROUND(G66 * H66,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","f8d11d94-9408-4a3d-ba24-d9c1dd265a35","D.2.1.7","","ROOF COVERINGS ",{"$nulls":4},"Dflt"]
["Label","1ca76970-1b4e-461f-8507-54190ca19a4a","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","70d7cd33-64d8-4cef-9537-a53ae99e3b3b","","","PROFILED METAL SHEETING AND ACCESSORIES ",{"$nulls":4},"Dflt"]
["Label","85e5abbc-ae5e-41f5-99e3-7e626e4bfeea","","","\"Klip-Lok 700\" profile roll-formed in continuous lengths from certified Galvanised steel Z200 0.58mm complying with ISQ 550 (3T) (A653) with a Chromadek Colomet finish to one side and standard backing coat, Papyrus white to other and accessories, fixed to timber purlins in strict accordance with manufacturer's specifications. ",{"$nulls":4},"Dflt"]
["Item","df5855ca-915e-4647-8345-49cfcb448404","D.2.1.7.1","","Head wall flashings 375mm girth 2 times bent to suit roof profile ","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G71 * H71,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f9c916e7-65d1-433e-a002-f6912ce5a206","D.2.1.7.2","","Counter flashing 185mm girth 2 times bent ","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","83cc7fdf-5f2d-4ae5-94ed-e968d95473ba","D.2.1.7.3","","Insulation boarding in 1200mm widths with longitudinal flap joints, laid over purlins (at approximately 1000mm centres) and fixed concurrent with roof covering, including holes through boards etc ","m²",126,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","f8fce5c3-22bd-4e0a-9e1d-d8ea63fdc23e","D.2.1.8","","CARPENTRY AND JOINERY ",{"$nulls":4},"Dflt"]
["Label","bda88fd9-95cd-427d-9db1-4b18b4ddae5a","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","d200fa24-b5c1-434c-9d55-37419224f546","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","3583915c-e3b6-46f9-ba77-5bee801ece30","","","Joinery ",{"$nulls":4},"Dflt"]
["Label","a7f47eaf-4575-4046-b4dc-a84d8e0b2c3b","","","Descriptions of frames shall be deemed to include frames, transomes, mullions, rails, etc  ",{"$nulls":4},"Dflt"]
["Label","6ff1ddd2-090a-47c6-96fb-7eaf3c920a41","","","Descriptions of hardwood joinery shall be deemed to include pelleting of bolt holes ",{"$nulls":4},"Dflt"]
["Label","46b3eee0-2292-4f9c-96ee-3115912d2ba0","","","Fixing ",{"$nulls":4},"Dflt"]
["Label","101cf34a-560c-47a5-af01-70e4c3af1ce7","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete  ",{"$nulls":4},"Dflt"]
["Label","12762aa1-0ae1-4e31-8195-6e78e5ca9cc7","","","EAVES, VERGES, ETC ",{"$nulls":4},"Dflt"]
["Label","880d95dd-87d1-45b4-b857-8260fb41e0c2","","","\"Everite FC77\" pressed fibre-cement ",{"$nulls":4},"Dflt"]
["Item","c32394ee-5bab-4051-94a1-8b3150db001a","D.2.1.8.1","","15 x 300mm Fascias and barge boards including galvanised steel H-profile jointing strips ","m",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G84 * H84,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","770a761d-a2fe-407f-a91b-01cd5a794aa3","D.2.1.8.2","","Install missing louvres at the two roof sides ","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","11e87d67-dbab-4cde-b89e-c9901543cec2","D.2.1.9","","CEILINGS AND PARTITIONS, ETC ",{"$nulls":4},"Dflt"]
["Label","2ec3235e-2c23-4eb2-9c1e-d07117de7622","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","ce581029-3d7e-4a39-b51c-42572ecbb6e0","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","a84012b3-f4c1-4066-afff-cd7a71fc4b0c","","","Descriptions ",{"$nulls":4},"Dflt"]
["Label","7f6b7088-589a-426a-8474-362d4066c92c","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete ",{"$nulls":4},"Dflt"]
["Label","f2fa3dde-a549-4a0c-a514-34afd34645ed","","","Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere ",{"$nulls":4},"Dflt"]
["Label","d27ebcb5-96d3-4594-a0ec-499c93b49ee8","","","Electrical  light  fittings, diffusers, panels, etc generally are \"lay in\"  units  of  the  same dimensions as the suspension grid described  and  allowance  must  be  made  accordingly  for their support  inclusive  of any flexibility insetting out that may be required (ceiling panels have not been deducted and pricing is to take cognisance thereof)  ",{"$nulls":4},"Dflt"]
["Label","0fa9d97d-d341-49cc-b0a7-72ba93c0e68b","","","NAILED-UP CEILINGS ",{"$nulls":4},"Dflt"]
["Label","4fa09100-6415-4c02-b9a5-485c0c6e182f","","","\"Everite\" or equally approved ceiling panels ",{"$nulls":4},"Dflt"]
["Item","abe7d0ce-200c-4424-bc2c-1bd3b497fd4a","D.2.1.9.1","","Ceilings of 1200 x 2400 x 6mm thick panels including 38 x 38mm SA Pine brandering at 450mm centres in both directions ","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G95 * H95,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","a067d6fc-af67-43cf-a60c-ab814c7f06d6","","","Gypsum plasterboard cornices ",{"$nulls":4},"Dflt"]
["Item","e07edd46-1788-4062-812e-d9e2eae34ac6","D.2.1.9.2","","75mm Coved cornices ","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G97 * H97,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","edc44ceb-ecaa-4280-b45a-198d7db4d726","D.2.1.10","","PLASTERING ",{"$nulls":4},"Dflt"]
["Label","c7575f54-207d-4564-8f86-7b7cefad5d37","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","5a8bda86-a068-4826-80a2-02389f2f00f1","","","GRANOLITHIC ",{"$nulls":4},"Dflt"]
["Label","8810619e-fa41-498a-a043-89e658d62100","","","30MPa untinted granolithic on concrete ",{"$nulls":4},"Dflt"]
["Item","20ccf0f6-5269-489e-a300-756ca5c09477","D.2.1.10.1","","30mm thick on floors to falls and crossfalls ","m²",227,{"v":0,"d":"0.00"},{"$f":"ROUND(G102 * H102,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","605986e5-54e3-4705-964c-4a228815483d","","","INTERNAL PLASTER  ",{"$nulls":4},"Dflt"]
["Item","645e3fdb-b86b-4383-b74c-3f46fefef60d","D.2.1.10.2","","Repair about 2.5m x 0.6m cracked section of the wall above the louvre, below the generator exhaust pipe by removing existing brickwork and reinstate the wall to make good.","m²",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G104 * H104,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","1009ecb4-5d66-4a04-8455-14016d509887","D.2.1.10.3","","Repair Cracks on plastered wall by using polyfilla or equivalent product that is approved by Engineer.  ","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f33f072c-8b47-49ac-99cf-9e0bf79319ff","","","One coat 1:5 cement plaster 15mm thick on brickwork or concrete finished with sponge roller",{"$nulls":4},"Dflt"]
["Item","d59ab6a6-efb7-49b2-bffe-0c7f5c95d4ce","D.2.1.10.4","","On walls","m²",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G107 * H107,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5f706c56-ee88-456f-8e00-f6050e72f6cf","","","Gypsum skim plaster on concrete ",{"$nulls":4},"Dflt"]
["Item","e0e34a92-683c-4b39-950b-7d9851520201","D.2.1.10.5","","On ceilings ","m²",227,{"v":0,"d":"0.00"},{"$f":"ROUND(G109 * H109,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8a9ae2a0-c985-439f-b9da-b8a5bb224b16","","","EXTERNAL PLASTER ",{"$nulls":4},"Dflt"]
["Label","1ba878f3-4657-45b6-8592-ee0d1b8319cf","","","One coat 1:5 cement plaster 12mm thick on brickwork or concrete finished with a wood trowel ",{"$nulls":4},"Dflt"]
["Item","25b92b11-af67-47cd-8f37-f30f3d8a7dab","D.2.1.10.6","","On beams ","m²",41,{"v":0,"d":"0.00"},{"$f":"ROUND(G112 * H112,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","ee4ae5b7-be41-4bf8-bd0e-3a598cae43ad","D.2.1.11","","PLUMBING AND DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","0cef2ddc-3033-44a3-9bdf-969bf688b69e","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","112e7222-2423-4296-a3fe-cf5a95457005","","","RAINWATER DISPOSAL ",{"$nulls":4},"Dflt"]
["Label","85d33c48-93c9-4ea4-b57f-62bcec4073bb","","","\"Watertite\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","1da944b5-f2ce-45e4-970d-7ed7b554c710","D.2.1.11.1","","140 x 150mm box gutter x 0.9mm brackets fixed at 500mm centres ","m",70,{"v":0,"d":"0.00"},{"$f":"ROUND(G117 * H117,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","91504d4c-868f-4468-853d-698ac261d8c2","D.2.1.11.2","","Extra over gutter for outlet for 75mm dia. pipe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","71c8e149-773f-427b-8f76-931b546d0153","D.2.1.11.3","","75 x 1.27mm Diameter rainwater pipes ","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bce79ce6-52f3-4c0e-8cf6-7ea772c88c2c","D.2.1.11.4","","Extra over rainwater pipe for bend ","No.",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d6318fe4-8e88-4e36-b862-33adc67d87b4","D.2.1.11.5","","Extra over rainwater pipe for shoe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","379fdac2-69c6-4f76-a878-8c2785b0976b","D.2.1.12","","PAINTWORK ",{"$nulls":4},"Dflt"]
["Label","d5aa8d22-44fe-4706-bf0d-ecdeae1c128a","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","2c61aaba-3bdf-4bd5-94c4-daae0257a944","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","3c597826-2117-4dc6-aed0-66934a72e7e4","","","All colours to be selected by the Architect ",{"$nulls":4},"Dflt"]
["Label","debf417e-420d-4ada-a9fe-3b30ba5f75a9","","","Only approved brands of paint shall be permitted ",{"$nulls":4},"Dflt"]
["Label","cca893db-c81f-4a18-85d1-21da44ebb36b","","","All painting measured generally will be in colours with a value of more than 7 on the Munsell system in accordance with the relevant SABS specification. Any painting in colours with a value of 7 or less on the Munsell system shall be given as paintwork in darker colours ",{"$nulls":4},"Dflt"]
["Label","67611906-5035-45d3-ae3e-d5e0e553555e","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","76b30efa-dc15-4c01-9927-b700f576dbed","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Prime with one coat of plaster primer all in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","6a3389f9-7db8-4481-ad88-e27c5eafbeea","D.2.1.12.1","","On walls ","m²",255,{"v":0,"d":"0.00"},{"$f":"ROUND(G130 * H130,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f286534a-3c72-496d-abf0-14c64557468f","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","3e65a685-a43d-4223-accf-404b76508a3a","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Finish with 2 coats of super acrylic PVA paint or similar approved. All in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","23fd8d38-8711-4a15-a44f-2f24a185b530","D.2.1.12.2","","On walls ","m²",255,{"v":0,"d":"0.00"},{"$f":"ROUND(G133 * H133,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8c162ca0-ea48-45bc-94df-675bf679bd8b","","","ON EXTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","466fc9de-c102-446b-9caa-f94233282a1a","","","Primer and finish with two coats \"Marmoran Armourbrush\" or equally approved, applied in strict accordance to manufacturer's instructions. ",{"$nulls":4},"Dflt"]
["Item","772b5eb3-ab12-4257-b130-4669f66d5322","D.2.1.12.3","","On walls, RC Beam and Door Reveals","m²",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G136 * H136,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","78317dfb-d354-4446-bec7-fb9b09b151fa","","","ON PLASTERBOARD SURFACES ",{"$nulls":4},"Dflt"]
["Label","130b588d-87f9-48c1-a4c1-68c396081d97","","","One coat alkali resistant primer and two coats PVA emulsion paint for interior use ",{"$nulls":4},"Dflt"]
["Item","3765ceb8-a448-4c7d-9153-6a90864abd5c","D.2.1.12.4","","Ceilings and cornices  ","m²",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G139 * H139,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","994c7d00-939e-4b88-baae-f4ec505cbe97","","","ON METAL SURFACES ",{"$nulls":4},"Dflt"]
["Label","bd9e68ba-d666-4b5a-aece-1b425584c0f6","","","One coat \"Namelcote\" zinc chromate primer UC 53, one coat \"Plascon Galvogrip\" metal primer and two coats \"Velvaglo\" polyutherane enamel paint (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","a9ca0ae2-d0f8-40c8-839b-629c77b2dc8c","D.2.1.12.5","","On door frames etc ","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G142 * H142,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3a23cb98-c924-493c-b627-46aadd5a7e20","D.2.1.12.6","","On doors  (both sides)","m²",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","7521b744-0893-4e1c-a602-57ff98e2c484","","","ON WOOD SURFACES ",{"$nulls":4},"Dflt"]
["Label","ec421db9-6bf6-45bc-a100-708b6f81e830","","","One coat \"Spick and Span\" Oil based wood primer (UCS2), two coats \"Velvago Polyurethane enamel paint (VLO). (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","c42b208b-a3f9-4b0d-98d5-9328dff43af6","D.2.1.12.7","","On doors  (both sides)","No.",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G146 * H146,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","9b0f1855-37bc-4103-8f49-f65ebd10f19b","D.2.1.13","","CRAWL BEAMS ",{"$nulls":4},"Dflt"]
["Item","ed041640-6770-4b92-8f62-9db5673a4511","D.2.1.13.1","","Supply and Install the 3.5m long Crawl Beam Size 203 x133x25 I Beam.  The rate shall include the cost of supply,  and complete installation with 210mm Long Cleat Plate made from 102x133x13Kg/m T bolted to RC beam using 2 M16 Hilti HVU which has chemical bolts at each side all in accordance with the details in Drawing No. J40073/010-408/Rev A 1.  Material: 3CR12 and System: Multi-purpose epoxy; Minimum DFT (250 micron) ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G148 * H148,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c6bd1810-b596-4fe7-8da3-5043bf974edb","D.2.1.13.2","","Cable Trench",{"$nulls":4},"Dflt"]
["Item","47dd7714-5bda-4845-a750-1a75817430db","D.2.1.13.3","","Where the angle iron is missing, trim off faces of the edges of the concrete trench with  concrete grinder and Install the 40 x 40 x 3 Angle Iron  by drilling and fixing the  angle iron fish tail anchors into concrete with suitable product and installing the angle iron to suit the chamfered Edges of cable trench.","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G150 * H150,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e94c55a2-0ada-4da9-b243-bb9cd37468cd","D.2.1.13.4","","Install the 655mm wide x 6mm VASTRAP with 3 No. 30x8mm plate stiffeners per panel, trench plate panel cover over the cable trench where no MCC and Electrical panels are placed","m",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","9cf76c32-fec1-4df3-9a57-317c0dd48710","D.2.1.14","","Concrete Works (Apron)",{"$nulls":4},"Dflt"]
["Label","80a83bb5-f238-4b71-8a27-f203f2615e25","","SANS1200 GA","Concrete (Small Works) - Formwork",{"$nulls":4},"Dflt"]
["Item","bf3109b2-9782-4bb5-bd4c-cabea1627a95","D.2.1.14.1","8.2.1","Formwork - Rough Finish surface","m²",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G154 * H154,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","40892fc3-4fc2-4f9a-936d-3236fe12f8dc","","SANS1200 GA","Concrete (Small Works) - Steel",{"$nulls":4},"Dflt"]
["Item","8f04b9b5-f22d-471d-a4b8-9ade740c6c39","D.2.1.14.2","8.3.2","High Tensile Welded Mesh Ref 245","m²",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G156 * H156,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b390dea6-0a3c-40db-ac07-6f4630689673","","SANS1200 GA","Concrete (Small Works) - Concrete",{"$nulls":4},"Dflt"]
["Item","686299fa-e7ec-455f-8f48-85febbadc64d","D.2.1.14.3","8.4.3","20 Mpa, 19mm aggregates Concrete","m²",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G158 * H158,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7e92048c-c6b8-4961-a9a2-d45d2a4f3c2b","D.2.1.14.4","8.4.4","Unformed Wooden floated surface finish ","m²",64,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","39c2ffcf-899b-4bb4-8204-7b9064575a77","D.2.1.14.5","8.5.","6mm x 30mm deep Saw cut joints from top of concrete","m",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","68e5a3a9-d6e0-4de1-a3ab-6dad7ecfda66","D.2.1.14.6","","Install 10mm Jointex Expanded polystyrene","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","54272262-545f-410a-886f-2c8554c03d1d","D.2.1.14.7","","Install 10mm x 10mm polysulphide ","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","61286c79-c0db-4556-96e4-6934ce8e36e2","D.2.1.15","","Remove and replace all the corroded exterior doors.  The old doors would be the Employer's asset and they would be stored within site at location to be indicated by the Engineer.  The replacement doors will be in accordance with the door schedule indicated in Drawing No. J40073/010 - 404A Rev 6.  Ironmongery: Vermin Proof backing, with a 1.2mm solid steel slats, cabin hooks,  earth strap, shooting bolt housing and 3 point locking system for padlock",{"$nulls":4},"Dflt"]
["Item","f90ec267-8b25-4ee0-8fd3-8f068895092e","D.2.1.15.1","","D1 - Door Leaf : Standard 914 x 2440 mm steel frame Transformer door ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G164 * H164,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2894f507-2165-47b6-88dc-1a95643227ef","D.2.1.15.2","","D2 - Door Leaf : Standard 1830 x 2440 mm steel frame Transformer door ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a0e00c17-32aa-4603-8a0f-d4320522883b","D.2.1.15.3","","Install 40mm thick semi solid hardwood doors with 3.2mm tempered hardboard facings, and two hardwood edge strips, 1.2mm rebated closing stiles (SABS 545) complete with Ironmongery (NB Only Frames already installed)","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","fb3a4630-d68a-4f32-ad36-ba51c4a39646","D.2.1.16","","Remove and replace the existing rusted frames and louvres.  The old material would be the Employer's asset and they would be stored within site at Location to be indicated by the Engineer. The replacement frames and louvres will be in accordance with the window schedule indicated in Drawing No. J40073/010 - 404A Rev 6.   ",{"$nulls":4},"Dflt"]
["Item","c6998e23-e90c-4468-bf02-b474487f5acd","D.2.1.16.1","","LV 1 - 2400mm x 1000mm","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G168 * H168,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e0f57460-25f7-44ba-b06a-27de17bf222d","D.2.1.16.2","","LV 2 - 2400mm x 2000mm","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Sum","9587433d-81cd-4969-a01b-896e1ba4a01f","D.2.1.16.3","","Supply and Install all complete fire and signage plan in accordance with the Drawing No. J40073/010 - 404E Rev 2","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H170,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","d8cd5fdd-cf4c-43cd-aa5a-05f022471b1a","D.2.1.17","","Supply and Install Ironmongery",{"$nulls":4},"Dflt"]
["Item","0c1cc9d6-58d3-4420-b4e6-9f048e3736d7","D.2.1.17.1","","Dorma TH120/BP Stainless Steel Lever handle on 150x150mm back plate with cylinder hole","Set",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G172 * H172,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4bfd8f92-29b4-4818-943c-ea8343f36c83","D.2.1.17.2","","Dorma D036S Euro-Profile Cylinder SASH lock SS","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4d4975f5-df89-42be-81ad-02590b66f3a3","D.2.1.17.3","","Dorma DDC106501 Nickel Plated 65mm Ten Pin Euro-Profile Grand Master-Keyed Double Cylinder","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","63e67666-eee8-4fc9-ae7e-3daff169b7a4","D.2.1.17.4","","Dorma DDS-NP-018 Nickel Plated Floor Stop","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6ef9ea0b-a6b4-4e96-a45e-23b30be68372","D.2.1.17.5","","Stainless Steel Kick Plate 200mm x width of Door, finished size to be checked on site, Grade 304 0.9mm thick drilled and countersunk for screw fixing","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9dedbc7f-a71c-49dc-9e8c-5e712e624ecb","D.2.1.17.6","","Dorma DHC SS 031B Stainless Steel hat and coat hook with rubber buffer","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","e71db5ff-3bc0-4db0-a602-3057adf2fa6d","D.2.1.18","","TILING ",{"$nulls":4},"Dflt"]
["Label","02f9dccd-4f57-416d-9118-b1fe3279ffee","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","6ca4e3af-9ebd-4bae-b9ab-3133fc795072","","","\"Note All tiling shall be fixed to plaster or screed with an approved adhesive; the adhesive shall be as recommended by the manufacturer of the tiles. \"",{"$nulls":4},"Dflt"]
["Label","6a423468-a92a-487f-89fc-cec78398a900","","","FLOOR TILING  -  in accordance with interior finishing schedule Drw. No. 010-404F Rev 0",{"$nulls":4},"Dflt"]
["Item","1ef474d8-9d9b-4a0a-825a-e4276572041d","D.2.1.18.1","","Supply and install 40mm Untinted grano  with 1 cement/1 stone chippings / 1 sand mix finished with steel trowel in bays not to exceed 12m2.  Provide ABE or equal SABS approved epoxy paint finish on Grano floors","m²",101,{"v":0,"d":"0.00"},{"$f":"ROUND(G182 * H182,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","ede89e48-03fd-4daf-9ae3-dcdbf361e090","","","Skirting - Grano ",{"$nulls":4},"Dflt"]
["Item","b48597c0-1d34-4861-8586-329a4ef2b02a","D.2.1.18.2","","19mm thick rounded (1:4 cement mix) grano with V Joints 75 mm above finished floor level.  Skirting to project 6mm from finished wall fall with arris top edge. ","m",77,{"v":0,"d":"0.00"},{"$f":"ROUND(G184 * H184,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","1a84408b-2f0f-44fd-8b63-dee77c7b52d4","D.2.1.19","","PROVISIONAL SUMS ",{"$nulls":4},"Dflt"]
["Label","8e9bb50c-2e9d-4df3-ab22-f68693e7be05","","","For preambles see \"Model Preambles for Trades\""]
["Label","0e0ed129-4d0e-4eed-a410-eac8604cab16","","","BUDGETARY ALLOWANCES (Roof Rust Repair, Electrical connection, Water Connection)"]
["Item","fa72cf89-466a-446e-892d-c2a278584358","D.2.1.19.1","","Provide for Provisional Sum of R1,000,000.00 Additional Work as instructed by Engineer","Prov.Sum",1,{"v":400000,"d":"400,000.00"},{"$f":"ROUND(G188 * H188,2)","v":{"v":400000,"d":"400,000.00"}}]
["% Previous","6cd09d68-a496-4824-a06c-d7230a1c35d4","D.2.1.19.2","","Add for profit and general attendance upon above if required  ","%",{"$f":"I188","v":{"v":400000,"d":"400 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Label","b63fb84b-0e79-4b71-97f0-a248f161d338","","","Corrective work to structure/building"]
["Sum","f1d035f0-cf98-4876-9526-d93428d5cb6b","D.2.1.19.3","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":200000,"d":"200,000.00"},{"$f":"ROUND(H191,2)","v":{"v":200000,"d":"200,000.00"}}]

{"sheet":"BILL D.3.","index":12,"n_rows":300,"n_cols":10,"rows_kept":300,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.3.",null,"WORKSHOP BUILDING",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","81b39000-658f-4493-afff-041080164ec9","D.3.1","","WORKSHOP BUILDING",{"$nulls":4},"Dflt"]
["Label","7e069b24-9720-45e3-aaf3-66971cf06745","","JBCC","SECTION D.3.1 : WORKSHOP BUILDING",{"$nulls":4},"Dflt"]
["Sum","e7c026d4-7572-425e-be85-8ba395e3f8d2","D.3.1.1","","Housekeeping (Includes cleaning and organising working area)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H11,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","da2ef526-9589-4f99-ad8a-c79ad7857471","D.3.1.2","","EARTHWORKS",{"$nulls":4},"Dflt"]
["Label","8d7cf87f-0931-4daf-bca6-bd6add2bf727","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","728dd2cc-e9a7-4af5-8f1b-408eaf7f89a5","","","Note:",{"$nulls":4},"Dflt"]
["Label","914d955e-c798-4527-95ef-2d653af0b7a5","","","Wherever a trade name for any product has been described in the Priced Document attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained prior to the closing for submission of tenders.",{"$nulls":4},"Dflt"]
["Label","1c01c262-8504-4bd0-9607-a2a75a29db79","","","if prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered for.",{"$nulls":4},"Dflt"]
["Label","c9ead7ed-c7f5-43a6-82b6-69163fad23e2","","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","5276e592-d4b3-487a-b903-e1c09efa025e","","","Extra over all excavations for carting away:",{"$nulls":4},"Dflt"]
["Item","a576b220-dee3-4ea0-adfe-8a5f862da3f6","D.3.1.2.1","","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the Contractor","m³",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G19 * H19,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2d828f91-40ff-4b6f-96b2-b3598198ed1c","","","FILLING, ETC",{"$nulls":4},"Dflt"]
["Label","d7e55d3a-d7cf-489b-9c04-483646ccfb56","","","Backfilling with imported G7 material spread in layers not exceeding 150mm thick under floors, etc and compacted to 97% Mod. AASHTO density",{"$nulls":4},"Dflt"]
["Item","69d5711d-6353-4c68-bd4b-c5e5b5414432","D.3.1.2.2","","Under floors, steps, paving, etc.","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G22 * H22,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","46a3782e-24db-4b52-b64d-ffa8b8564dad","D.3.1.3","","CONCRETE, FORMWORK AND REINFORCEMENT  ",{"$nulls":4},"Dflt"]
["Label","d08bdb63-d2af-4443-bbd9-a5b1ccc4a384","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","0cb9570f-d043-4c4a-b099-b08a0249afc6","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","0e64ba2a-d568-4273-81b0-cde5dd536748","","","CONCRETE ",{"$nulls":4},"Dflt"]
["Label","df4e9128-3173-4c29-bc55-a413e9d45f5d","","","UNREINFORCED CONCRETE ",{"$nulls":4},"Dflt"]
["Label","f91a626e-5d9d-4bac-9d80-bbce8c9177a2","","","Unreinforced concrete 25MPa at 28 days in ",{"$nulls":4},"Dflt"]
["Item","5daee81b-07ed-4ca4-9ee5-49ff801df80d","D.3.1.3.1","","Surface beds (apron slabs)","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G29 * H29,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8a9a87a8-732f-4ba2-a824-d2aeded62974","","","REINFORCED CONCRETE ",{"$nulls":4},"Dflt"]
["Label","69012412-0d2c-4282-87b7-1ae1d7094ac6","","","Vibrated reinforced concrete 25MPa at 28 days in ",{"$nulls":4},"Dflt"]
["Item","336ba2b0-f0ce-454a-8300-7f6387335bed","D.3.1.3.2","","Surface beds (ramps)","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G32 * H32,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","1a112253-5f61-4445-a1dd-8d5a5b6abec2","","","CONCRETE SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","47efcd5b-92bb-4380-9212-69f1db2ee78d","","","Finishing top surfaces of concrete smooth with a wood float ",{"$nulls":4},"Dflt"]
["Item","fbcb1527-723e-4dea-97d4-c0e81fd1f735","D.3.1.3.3","","Surface beds, slabs, etc (apron slabs)","m²",33,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","84955703-0142-4244-806e-a6bae45c0719","","","Finishing top surfaces of concrete to an evenly ribbed non-slip surface ",{"$nulls":4},"Dflt"]
["Item","0bc7c1a7-7a6f-40a9-b635-3fa2b481c88d","D.3.1.3.4","","Surface beds, slabs, etc (ramps)","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G37 * H37,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","535c600b-d6a6-40a2-b5e4-471e2caf4a13","","","FORMWORK ",{"$nulls":4},"Dflt"]
["Label","4b413976-d8c0-494b-a1d1-091c5d2d935a","","","ROUGH FORMWORK (DEGREE OF ACCURACY III) ",{"$nulls":4},"Dflt"]
["Label","e48323bc-f612-4361-831a-a947c788962d","","","Rough formwork to sides ",{"$nulls":4},"Dflt"]
["Item","5e03b0cb-5f10-427a-877b-e78cccdef474","D.3.1.3.5","","Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",70,{"v":0,"d":"0.00"},{"$f":"ROUND(G41 * H41,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","d1bf3cfe-8595-4e10-9446-48bb16eae881","","","MOVEMENT JOINTS, ETC",{"$nulls":4},"Dflt"]
["Label","97eab2ea-8572-4fb3-b30b-6660e54f76bd","","","Saw cut joints:",{"$nulls":4},"Dflt"]
["Item","f4c09b07-0d1c-4955-a0ee-7cc12d6484b4","D.3.1.3.6","","6 x 30mm Saw cut joints in top of concrete","m",16,{"v":0,"d":"0.00"},{"$f":"ROUND(G44 * H44,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","4639f452-cdf7-4739-a7cd-50acf9b16119","","","STEEL REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","282ed94e-158c-4f16-87d1-9969a3c213e0","","","Fabric reinforcement:",{"$nulls":4},"Dflt"]
["Item","0ee96c51-1fc0-488b-9ebc-168eb66030b0","D.3.1.3.7","","Steel mesh reinforcement reference 311 in concrete slabs, surface beds, etc","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G47 * H47,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","561570ca-5e70-4e30-af3a-afe57b1f65ea","",""," WATERPROOFING ",{"$nulls":4},"Dflt"]
["Label","3bc72985-a69b-4615-a0f5-02f4dc6d74f3","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","f178378f-31d3-4ca2-8638-fe5f19644561","","","WATER PROOFING TO SHOWERS ",{"$nulls":4},"Dflt"]
["Label","62b2641a-e435-4232-8769-2d9d21c0f4b6","","","Apply \"Tal Superflex I\" or equally approved then reinforce with Tal Superflex membrane, waterproofer and bonding agent applied as per manufacturer's specification ",{"$nulls":4},"Dflt"]
["Item","022ebf83-18c9-45d7-9b34-3bab430119fb","D.3.1.3.8","","On shower walls ","m²",11,{"v":0,"d":"0.00"},{"$f":"ROUND(G52 * H52,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","57c22054-32f3-4d92-997a-2d48a751d28e","D.3.1.3.9","","On shower floors ","m²",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","ebf208a6-969c-4025-98d8-7c47e0abf9ab","","","JOINT SEALANTS ",{"$nulls":4},"Dflt"]
["Item","50843491-4bbd-44e6-94fd-1cdd481c2bee","D.3.1.3.10","","Rake out 10mm softboard 20mm deep, prepare and fill with approved polysulphide sealing compound (colour to be approved by Architect) ","m",80,{"v":0,"d":"0.00"},{"$f":"ROUND(G55 * H55,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","60fedd9d-7226-44ec-8635-0081726e2cf7","D.3.1.3.11","","Polysulphide sealant to 3mm wide saw cut joints ","m",16,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","ba527501-2e35-4f84-9778-43096437da3c","D.3.1.4","","ROOF COVERINGS ",{"$nulls":4},"Dflt"]
["Label","30031a48-413f-485b-bfa4-ec4f6dfd6a52","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","49ea27d1-2c59-480e-ab69-8b23912192a0","","","PROFILED METAL SHEETING AND ACCESSORIES ",{"$nulls":4},"Dflt"]
["Sum","90f5eab5-2221-4d29-9ec0-1c3102f82249","D.3.1.4.1","","Remove about 10m² damaged roof sheeting Ridges, Hip cappings and damaged roof trusses and purlins as instructed by Engineer","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H60,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","fc7503bf-8664-4bab-883e-27b4c9d97538","","","\"Klip-Lok 700\" profile roll-formed in continuous lengths from certified Galvanised steel Z200 0.58mm complying with ISQ 550 (3T) (A653) with a Chromadek Colomet finish to one side and standard backing coat, Papyrus white to other and accessories, fixed to timber purlins in strict accordance with manufacturer's specifications.  ",{"$nulls":4},"Dflt"]
["Item","7547d630-6386-45ac-b2c8-0871f3bf95c0","D.3.1.4.2","","Roof covering with pitches not exceeding 25 degrees","m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G62 * H62,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0f0fbc6e-bf3a-4f70-9fcc-a6e1c58b8726","D.3.1.4.3","","Ridge cappings 550mm girth to suit roof profile","m",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4291f06d-dfa3-474f-ba54-0f9f7a2ca0ce","D.3.1.4.4","","Hip cappings 550mm girth to suit roof profile","m",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b65d15b4-f28f-4c15-9a17-96e4c449e1b4","D.3.1.4.5","","Head wall flashings 375mm girth 2 times bent to suit roof profile ","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d47e54c7-37b3-46bd-b0dd-db113d8d7be1","D.3.1.4.6","","Counter flashing 185mm girth 2 times bent ","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","89914d92-8bc6-4f84-9627-f5e6efa57081","","","ROOF AND WALL INSULATION ",{"$nulls":4},"Dflt"]
["Label","7bbba1aa-22ce-424b-b7ce-08c030435c70","","","25mm Thick \"Sagex Kulite\" rigid laminated expanded polystyrene insulation board with lacquered foil on one side ",{"$nulls":4},"Dflt"]
["Item","68683730-ef0d-4370-9daa-7f68e9d71d13","D.3.1.4.7","","Insulation boarding in 1200mm widths with longitudinal flap joints, laid over purlins (at approximately 1000mm centres) and fixed concurrent with roof covering, including holes through boards etc ","m²",306,{"v":0,"d":"0.00"},{"$f":"ROUND(G69 * H69,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","70fc4bf5-8249-435f-99e8-e4230f82d27f","D.3.1.5","","CARPENTRY AND JOINERY",{"$nulls":4},"Dflt"]
["Label","f2bd6c58-dcd6-4789-9b83-885faeb2ab9a","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","3fc8da6f-8e3f-4538-a145-17d76f054016","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","441df7cc-fdf5-449a-bbfe-662be9b2df37","","","Joinery",{"$nulls":4},"Dflt"]
["Label","bddc1ea7-7010-4ba9-9f8b-3c2a32b65838","","","Descriptions of frames shall be deemed to include frames, trasomes, mullions, rails, etc.",{"$nulls":4},"Dflt"]
["Label","2cf52546-943e-47da-a7e1-b3be5a9b5293","","","Description of hardwood joinery shall be deemed to include pelleting of bolt holes",{"$nulls":4},"Dflt"]
["Label","be4e0a30-6f7f-4023-8d2c-0a7a8b6d1882","","","Fixing",{"$nulls":4},"Dflt"]
["Label","d81f2fe3-4815-4854-9a92-0077828937c5","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete",{"$nulls":4},"Dflt"]
["Label","87260306-2acd-4196-a6a0-1607e9d16de7","","","DOORS, ETC",{"$nulls":4},"Dflt"]
["Label","76b4bbd1-4a03-45f0-9804-6300d0e905d5","","","Wrought meranti doors hung to steel frames",{"$nulls":4},"Dflt"]
["Item","8681d3dd-61da-4025-b306-b500c6d09bde","D.3.1.5.1","","44mm Framed and ledged batten double door 1613 x 2032mm high including 3mm plywood backing on one side and 76 x 32mm weather bars","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G80 * H80,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","131853f1-a6f2-4c71-a954-c5a7d5ed1529","D.3.1.5.2","","Extra for 400 x 400mm opening for metal louvre unit","No.",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","9c6cc82b-6c91-483d-ada4-79f1e2716314","","","EAVES, VERGES, ETC ",{"$nulls":4},"Dflt"]
["Label","4b6faf4c-de2d-4a69-bf76-1be0deaad453","","","\"Everite FC77\" pressed fibre-cement ",{"$nulls":4},"Dflt"]
["Item","9b25bac8-272d-4f98-b974-65eee1d5655a","D.3.1.5.3","","15 x 300mm Fascias and barge boards including galvanised steel H-profile jointing strips ","m",73,{"v":0,"d":"0.00"},{"$f":"ROUND(G84 * H84,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","a76d283d-f263-4cba-a80e-39ecbe60eea0","","","JOINERY SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","d00c9800-420e-42f2-ad18-7d9fb65315df","","","Seats ",{"$nulls":4},"Dflt"]
["Item","da420f93-1df6-47b7-9184-25f46a5cf97b","D.3.1.5.4","","600 x 1000mm long seat, comprising 70 x 22mm meranti timber slats bolted to steel support complete ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G87 * H87,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","75c5f50c-618d-4302-a0e4-de71d045fa78","D.3.1.6","","CEILINGS AND PARTITIONS, ETC ",{"$nulls":4},"Dflt"]
["Label","f00c9ac5-1b50-45ac-8b93-6597c86c732e","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","0aa1e93d-3d68-48f4-99ed-f6b74f3fb123","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","2348f0e3-8609-46d0-97ae-304ab6ad41b6","","","Descriptions ",{"$nulls":4},"Dflt"]
["Label","214df369-312f-4950-9472-b90d15a43d5d","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete ",{"$nulls":4},"Dflt"]
["Label","f9502eb0-1b1c-437d-a060-6adfe2d2c745","","","Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere ",{"$nulls":4},"Dflt"]
["Label","0506e95e-f4a4-4c67-ac99-891a4cbd9536","","","Electrical  light  fittings, diffusers, panels, etc generally are \"lay in\"  units  of  the  same dimensions as the suspension grid described  and  allowance  must  be  made  accordingly  for their support  inclusive  of any flexibility insetting out that may be required (ceiling panels have not been deducted and pricing is to take cognisance thereof)  ",{"$nulls":4},"Dflt"]
["Label","6a24b9cb-0fdf-40a1-857c-ce473fb42770","","","NAILED-UP CEILINGS ",{"$nulls":4},"Dflt"]
["Item","a3f6ea08-e79b-4ab5-a1c3-4d95c8ccbd59","D.3.1.6.1","","Remove damaged ceiling and brandering","m²",0,{"v":0,"d":"0.00"},{"$f":"ROUND(G96 * H96,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","1cef7fa3-6d09-45c3-8488-abc94e92f6e7","","","\"Everite\" or equally approved ceiling panels ",{"$nulls":4},"Dflt"]
["Item","024ec0c0-0814-478b-a86c-c358bbb4c539","D.3.1.6.2","","Install Ceilings of 1200 x 2400 x 6mm thick panels including 38 x 38mm SA Pine brandering at 450mm centres in both directions ","m²",310,{"v":0,"d":"0.00"},{"$f":"ROUND(G98 * H98,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","a2eac2db-c6dd-4356-ac6c-8c6faa784ce3","","","Gypsum plasterboard cornices ",{"$nulls":4},"Dflt"]
["Item","b1089689-1eab-4059-baf4-4b7e5d2429e6","D.3.1.6.3","","75mm Coved cornices ","m",200,{"v":0,"d":"0.00"},{"$f":"ROUND(G100 * H100,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","71a4a1c7-b4f2-4300-93b5-e2093e8107a4","D.3.1.7","","IRONMONGERY ",{"$nulls":4},"Dflt"]
["Label","f4a79dbc-8791-4259-97e4-e5844355f255","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","7491488d-6e12-4582-b608-5eb94c35b36e","","","LOCKS ",{"$nulls":4},"Dflt"]
["Label","f11e217d-b741-4e56-88be-5caf9872234d","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","01c0e68a-9ae2-43b0-aa57-ea3bcaceca39","D.3.1.7.1","","Stainless steel Euro-profile cylinder sash lock (Code: D036S) ","No.",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G105 * H105,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","26039da1-6cad-4177-86a4-3224dac50977","D.3.1.7.2","","Stainless steel Euro-profile cylinder dead lock (Code: D037D) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","01454cba-4dd8-4437-91a9-c6db5be201f3","D.3.1.7.3","","Stainless steel Euro-profile escutcheon (Code: DCE-002) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9e05f93e-8ae9-43f6-942b-39df1c338ed4","D.3.1.7.4","","Nickle plated 65mm bathroom privacy cylinder (Code: DBC0065001) ","No.",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2f1e6e3a-20bf-4a32-9940-256d639f8fb7","D.3.1.7.5","","Nickle plated 65mm ten pin Euro-profile grand master keyed single cylinder (Code: DSC104201) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bee407de-fb04-4713-9df4-2c74f8155d25","D.3.1.7.6","","Nickle plated 65mm ten pin Euro-profile grand master keyed double cylinder (Code: DDC106501) ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1cc70998-723e-4496-872d-008d050a83e5","","","HANDLES ",{"$nulls":4},"Dflt"]
["Label","39b21c91-1283-44aa-8d51-e698723486e8","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","12803075-d8e5-429a-b105-ae67488b5486","D.3.1.7.7","","350 x 32mm Stainless steel \"D\" shaped straight back-to-back pull handles (Code: DPH213) ","Pair",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G113 * H113,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6020e3e6-9023-40f9-bd8e-ed47e98c1ba0","D.3.1.7.8","","Stainless steel lever handle including 150 x 150mm backplate with cylinder hole (Code: TH120/BP) ","Set",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f3f959dc-c635-4870-b2b1-259675333624","","","PUSH PLATES AND KICKING PLATES ",{"$nulls":4},"Dflt"]
["Item","b9ebb380-feb1-4e90-8e53-e3df80139c9a","D.3.1.7.9","","877 x 200mm Stainless steel kick plate ","No.",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G116 * H116,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","d8d1a9d6-2de9-430d-9bd4-6884e9254407","","","LETTERS, NAMEPLATES, ETC ",{"$nulls":4},"Dflt"]
["Label","89d45aa8-e46d-4041-8f48-75d6f4deb370","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","4d86737e-bee1-45a5-83a8-d4f58be339f7","D.3.1.7.10","","150 x 150mm stainless steel male/female/staff sign (Code: DSS-130) ","No.",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G119 * H119,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","42c44950-a2a7-4978-95cd-b6be3340e43e","D.3.1.7.11","","150 x 150mm stainless steel male or female sign (Code: DSS-132) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","b6bdd153-360c-4ddc-b3c6-a2f0928b184b","","","SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","d976a956-d4f5-40aa-94c4-f5b0af2471be","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","633b284b-ee74-439f-88e8-d0f67b60fed1","D.3.1.7.12","","Nickle plated floormounted doorstop (Code: DDS-NP-018) ","No.",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G123 * H123,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c709cd2d-6928-4a1e-a53f-365ca6c2b5d6","D.3.1.7.13","","Stainless steel hat and coat hook with rubber buffer (DHC-SS-031B) ","No.",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","608c9da6-96ef-4910-9bdc-ae3840a61f16","","","\"Halstead\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","2fa0e3c5-98f6-4ffc-8a07-8affc8df5231","D.3.1.7.14","","150mm Satin chrome cabin hook (Code: Halstead 166) ","No.",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G126 * H126,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","aa39d4df-032a-4d46-a9c4-c3962ed9ea78","","","DOOR CLOSERS ",{"$nulls":4},"Dflt"]
["Label","1ba106e3-bbb5-447a-9e46-5d4bf7289090","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","6cee35d0-aac6-459a-85c8-aa376c94cd3c","D.3.1.7.15","","TS91/EN3 Slide channel door closer non-hold open  ","No.",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G129 * H129,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","608e7e91-e891-4482-bb9f-a00544136c19","D.3.1.8","","PLASTERING ",{"$nulls":4},"Dflt"]
["Label","e2f1b525-0985-4eda-b84a-f6719d8fd13b","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","f7a3c162-ee91-47b5-9ad7-ad981e2f8091","","","GRANOLITHIC ",{"$nulls":4},"Dflt"]
["Label","6165d792-5c84-447b-a882-aa06752ab337","","","30MPa untinted granolithic on concrete ",{"$nulls":4},"Dflt"]
["Item","576d09c9-51c0-49ea-93ad-3354e02b823c","D.3.1.8.1","","30mm thick on floors and landings ","m²",200,{"v":0,"d":"0.00"},{"$f":"ROUND(G134 * H134,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7c330304-6cc2-44df-9196-523394eb3407","","","SCREEDS  ",{"$nulls":4},"Dflt"]
["Label","1de0036f-3c27-4eec-aa79-2299627c0220","","","1:3 Cement screeds wood floated, on concrete ",{"$nulls":4},"Dflt"]
["Item","5fce2ee6-b4d6-413c-b0fc-f80a6a064c1a","D.3.1.8.2","","Average 50mm thick on floors to falls and crossfalls ","m²",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G137 * H137,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","ca39cb54-f248-4dba-82c3-af3ac6a48a63","","","INTERNAL PLASTER  ",{"$nulls":4},"Dflt"]
["Label","b9d8ecff-1cca-4f6a-b5b3-911fdcd9463f","","","One coat 1:5 cement plaster 15mm thick on brickwork or concrete finished with sponge roller",{"$nulls":4},"Dflt"]
["Item","bb7b9173-4c14-44e7-995e-828bfa7cbe67","D.3.1.8.3","","On walls","m²",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G140 * H140,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","54304999-168d-4d67-8875-17890a207aef","","","Gypsum skim plaster",{"$nulls":4},"Dflt"]
["Item","c6e30b09-5134-4800-a6a3-0e6d7441078e","D.3.1.8.4","","On ceilings ","m²",306,{"v":0,"d":"0.00"},{"$f":"ROUND(G142 * H142,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b6f147c2-1708-4d09-9a25-176b5b905898","","","EXTERNAL PLASTER ",{"$nulls":4},"Dflt"]
["Label","8d881524-6eec-40ab-88b1-c42365b01625","","","One coat 1:5 cement plaster 12mm thick on brickwork or concrete finished with a wood trowel ",{"$nulls":4},"Dflt"]
["Item","17298150-32c5-451e-9249-91047ea7c69c","D.3.1.8.5","","On walls ","m²",52,{"v":0,"d":"0.00"},{"$f":"ROUND(G145 * H145,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","67a15a8e-8ab5-4334-8b45-9e8e622be46c","D.3.1.9","","TILING ",{"$nulls":4},"Dflt"]
["Label","aaf94ec3-c3f1-4c17-81ac-1bd3449a6c8c","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","22108b28-4a3f-4b58-9289-f67867866bd9","","","\"Note All tiling shall be fixed to plaster or screed with an approved adhesive; the adhesive shall be as recommended by the manufacturer of the tiles. \"",{"$nulls":4},"Dflt"]
["Label","57b87b06-447b-405b-aeb0-e20187fd92db","","","WALL TILING  ",{"$nulls":4},"Dflt"]
["Label","44ac8194-751b-49eb-8f90-d91915ead4ea","","","200 x 200 x 6mm white glazed ceramic tiles fixed with adhesive to plaster (plaster elsewhere measured) and Dove Grey flush pointed with epoxy grout ",{"$nulls":4},"Dflt"]
["Item","7f6eec72-d76a-4b84-9aff-bbcce7a09d1d","D.3.1.9.1","","On walls in isolated panels, splashbacks, etc ","m²",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G151 * H151,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","cb323c9a-98f1-4919-bcc8-2f092a7ece16","D.3.1.9.2","","Attic stock ","m²",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","8df29eb4-b69f-4c42-998c-0ce1d42f2701","","","600 x 300mm or equally approved porcelain tiles fixed with adhesive on screed (elsewhere measured) and flush pointed with epoxy grout tile joint filler. ",{"$nulls":4},"Dflt"]
["Item","d52a9702-6d5b-42c0-b175-93ba8037b791","D.3.1.9.3","","On walls ","m²",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G154 * H154,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","48175bad-5b59-4262-a37b-188922e5e875","D.3.1.9.4","","Attic stock ","m²",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","275291e0-9efc-4026-a9c5-040ce4c3ea14","","","FLOOR TILING  -  in accordance with interior finishing schedule Drw. No. 010-403A Rev 3",{"$nulls":4},"Dflt"]
["Item","46b6b96d-2894-4ea3-8ae8-08ce4a6218dd","D.3.1.9.5","","Supply and install Factory fitted \"Van Dyck Latitude Earth Enduroback\" carpet tiles, colour Pirate Heavy commercial (SABS use class U5)","m²",18,{"v":0,"d":"0.00"},{"$f":"ROUND(G157 * H157,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6a964f2d-7681-4c85-9468-5388d0748e72","D.3.1.9.6","","Supply and install field tile 600mm x 600mm full bodied porcelain tile.   The tile adhesive as per TAL adhesive spec REF:SP5401 and the Grout is TAL \"Wall & Floor Grout\" Dove Grey.  M-Trim 8 x 10mm high stainless steel square edge trim (Code:SQE100), bedded in tile adhesive while tile are laid.  M-Trim 10mm high stainless steel movement joint fitted with 6mm wide Dove Grey polyurethane infill (Code:SMJ100.08) fixed to floors with an approved adhesive","m²",36,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a98293cf-d3a5-43cb-86b0-8f87ce37786e","D.3.1.9.7","","Supply and install 40mm Untinted grano  with 1 cement/1 stone chippings / 1 sand mix finished with steel trowel in bays not to exceed 12m2.  Provide ABE or equal SABS approved epoxy paint finish on Grano floors","m²",216,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f109f8d4-4a37-4253-a8b9-850811a34855","","","Floorworx marmoleum fully flexible linoleum floor sheeting 2m wided x 2.5mm thick manufactured in accordance with en 548, all in accordance with interior finishing schedule Dwg. No. 010-403J:",{"$nulls":4},"Dflt"]
["Item","1c4dde70-aeea-412e-a73b-c18ffa13fb46","D.3.1.9.8","","On floors","m²",32,{"v":0,"d":"0.00"},{"$f":"ROUND(G161 * H161,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","72be479a-c263-4c2b-a5b5-8338996e70fe","D.3.1.9.9","","Skirtings","m",26,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1f5a4750-7d43-4c03-a67d-098c60f04c38","","","Skirtings  - Tiled",{"$nulls":4},"Dflt"]
["Item","476f7256-78ae-413b-8a83-6b559b8899cf","D.3.1.9.10","","to match porcelain floor tiles to a height of 100mm AFFL.  TILE adhesive as per TAL adhesive spec REF:SP6148.  Grout - Tal Wall & Floor Grout colour to match or equal approved;refer to REF:SP6148.  Aluminium cover strip to top of the tile skirting. ","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G164 * H164,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","eea93391-bc1f-4854-ad8a-d9e9120804db","","","Skirting - Grano ",{"$nulls":4},"Dflt"]
["Item","00cf79b0-d521-44c0-8339-c0ae06c1a03f","D.3.1.9.11","","19mm thick rounded (1:4 cement mix) grano with V Joints 75 mm above finished floor level.  Skirting to project 6mm from finished wall fall with arris top edge. ","m",51,{"v":0,"d":"0.00"},{"$f":"ROUND(G166 * H166,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2f8ec016-f3ce-4f24-9a53-9520dd775064","","","Skirting - Meranti",{"$nulls":4},"Dflt"]
["Item","b35b2092-18b8-4aea-830d-4f6b4d74c743","D.3.1.9.12","","76 x 19mm Meranti hollow backed skirting with rounded top edge nailed to brick walls and screwed to wall partitions and with 25mm Meranti quadrant.   To be primed with suitable wood primer and finished with two coats matt enamel. ","m",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G168 * H168,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","df722e7a-0325-4cb1-acf3-cffa3a887f8f","D.3.1.10","","JOINT SEALERS, ETC ",{"$nulls":4},"Dflt"]
["Label","5586ece4-488e-4ef2-aba6-67c0adae70ff","","","Approved polyurethane joint sealant dressed into joint including protecting adjoining surfaces with masking tape ",{"$nulls":4},"Dflt"]
["Item","8bcfe372-a6a7-4c1c-9986-4fff984e2ad2","D.3.1.10.1","","10 x 10mm Sealer in tile joint between floor and wall tiles ","m",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G171 * H171,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5bce2f91-1ef4-4ac2-aa04-bcb58700983f","","","SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","907c1276-b7e9-4171-a276-09d990dd0700","","","M-Trim Natural anodised 10mm high aluminium square edge trim (Code : ASQE100.NA), bedded in tile adhesive while tiles are laid. ",{"$nulls":4},"Dflt"]
["Item","a7d9ee77-a3e8-4965-8a1d-61e3bd8cc22b","D.3.1.10.2","","Aluminium edge trim ","m",50,{"v":0,"d":"0.00"},{"$f":"ROUND(G174 * H174,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","9c346432-2196-4e33-a8e0-b0e7279c254a","D.3.1.11","","PLUMBING AND DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","2d5df7ce-e44b-453c-b1ea-ba2e99790424","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","288b586b-1cc6-4921-a75d-e86957e3d418","","","RAINWATER DISPOSAL ",{"$nulls":4},"Dflt"]
["Label","4c66cdeb-a328-4a7b-824b-3d0c2654e37e","","","\"Watertite\" aluminium ",{"$nulls":4},"Dflt"]
["Item","792141be-f495-433a-9475-1fd8c60c3b55","D.3.1.11.1","","140 x 150mm box gutter x 0.9mm brackets fixed at 500mm centres ","m",80,{"v":0,"d":"0.00"},{"$f":"ROUND(G179 * H179,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","d3dfe6f5-3b0f-4793-bc5a-d38cd0eed536","D.3.1.11.2","","Extra over gutter for outlet for 75mm dia. pipe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c77b069f-f815-4f6a-b56e-217dab9391d7","D.3.1.11.3","","75 x 1.27mm Diameter rainwater pipes ","m",17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5d510433-11d8-4bcf-8701-fcc76203a11a","D.3.1.11.4","","Extra over rainwater pipe for bend ","No.",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9d15270a-25cf-4363-95e3-8c16d7633bd1","D.3.1.11.5","","Extra over rainwater pipe for shoe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","7eaebe1d-4111-4ff0-98dc-2d481aeaa4e0","D.3.1.12","","SOIL DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","25c33c19-46ac-404c-9c81-7685f5291983","","","uPVC soil and vent pipes ",{"$nulls":4},"Dflt"]
["Item","98252e03-ddd7-4781-a5dc-9e2f755befdc","D.3.1.12.1","","32mm Diameter uPVC pipes ","m",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G186 * H186,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","c911593b-b24a-48ba-bac8-178edadbfdaa","D.3.1.12.2","","50mm Diameter uPVC pipes ","m",15,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","69fd75f5-504c-48e3-a4a0-a9d31e751e6b","D.3.1.12.3","","110mm Diameter uPVC pipes  ","m",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d8083876-fcdc-4850-a046-f3196247cd29","","","Extra over uPVC for the following fittings  ",{"$nulls":4},"Dflt"]
["Item","1b791aaa-b5fe-42c0-87f0-f7c778dc556d","D.3.1.12.4","","32mm Bend ","No.",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G190 * H190,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","80571d6c-4675-499d-bc62-ae53815230b1","D.3.1.12.5","","32mm Junction ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7f5a94d1-8e77-4758-aeef-0eed245361d3","D.3.1.12.6","","50mm Bend  ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e7be9242-1f05-4099-a99e-b1f07271138d","D.3.1.12.7","","50mm Reducing Junction ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c85054bb-9a38-43fa-8e63-4dc19ffbd1d6","D.3.1.12.8","","110mm dia Reducing Junction ","No.",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e1cf471e-1930-4838-8e9e-76f16e05fb89","D.3.1.12.9","","110mm Bend ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ddc3fc5d-5a59-484a-a0bc-29fb1e466fee","D.3.1.12.10","","110mm Stubstack ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","098d6bf8-6a83-47f6-accc-cb4355fcdaff","D.3.1.12.11","","110mm Air vent cowl ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7c283745-1cde-4563-ad8f-32da44c07207","D.3.1.12.12","","110mm Vent Cap ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","fe0c89f8-d9c8-4244-bb24-27d2c072574d","D.3.1.12.13","","110mm pan connector ","No.",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","77821c0e-e689-49d1-a6a1-6746894121ad","D.3.1.12.14","","Rodding Eye ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","3621e4eb-2ee0-4d2e-8c4d-b55673ffa15e","","","Testing ",{"$nulls":4},"Dflt"]
["Sum","4271947d-1680-4ade-96ca-d8b584666e40","D.3.1.12.15","","Testing soil drainage system ","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H202,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","887e4a5c-8a90-478f-a612-61d731ec1c5c","D.3.1.13","","WATER SUPPLIES  ",{"$nulls":4},"Dflt"]
["Label","43342272-a866-4e69-9baf-0e6a613ff636","","","Copper pipes to SABS 460/0 fixed to walls, ceilings, drywall cavities, etc ",{"$nulls":4},"Dflt"]
["Item","08243fc5-7a23-4bb5-ade9-ebfab94b3d98","D.3.1.13.1","","15mm Pipes ","m",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G205 * H205,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","03354f25-2ddc-4538-ac73-ffc995b79985","D.3.1.13.2","","20mm Pipes ","m",126,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","fdcf0cbe-e782-4ba4-919a-00545938ebf5","D.3.1.13.3","","22mm Pipes ","m",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","757267a2-10db-4de9-81f3-d7782a67cda3","D.3.1.13.4","","35mm Pipes ","m",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1c69112a-ef0f-419d-bda9-6da305737e48","","","Extra over piping for \"Copcal\" soldered fittings ",{"$nulls":4},"Dflt"]
["Item","4ef75cef-048e-414c-a8c6-b455977dad5c","D.3.1.13.5","","15mm Fittings ","No.",28,{"v":0,"d":"0.00"},{"$f":"ROUND(G210 * H210,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f8763892-bc0d-45b5-9087-f947b974c3cd","D.3.1.13.6","","15mm Reducer ","No.",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2a084651-6529-4807-ba98-4acb47aa51a3","D.3.1.13.7","","20mm Fittings ","No.",24,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","644e120b-107e-4a09-856c-4653d43c3c24","D.3.1.13.8","","20mm Reducer ","No.",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","27f4a8dc-9bc5-4e49-af91-b95111b1d192","D.3.1.13.9","","28mm Fittings ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ecc56e89-27f2-44be-9d6f-815048508341","D.3.1.13.10","","35mm Fittings ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0064171f-b65c-452d-9714-86258b500cce","D.3.1.13.11","","35mm Reducer ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","c9c79da7-b3ab-42a5-bfae-f604d9770594","","","Testing ",{"$nulls":4},"Dflt"]
["Sum","df796d45-b491-4ea5-a8fa-2a520b755057","D.3.1.13.12","","Testing water pipe system ","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H218,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","ba91e938-4cd4-4660-a769-90d54838aedf","D.3.1.14","","SANITARY FITTINGS  ",{"$nulls":4},"Dflt"]
["Label","f3997ba1-2c24-468b-a797-e969f90f610a","","","Supply and fix the following sanitary fittings including assembly forming all joints and connections, bedding, pointing, building in, cutting and pinning, plugging and screwing and making good as necessary  ",{"$nulls":4},"Dflt"]
["Label","57d464db-1934-477a-b500-9956f960c308","","","\"Vaal\" or equally approved ",{"$nulls":4},"Dflt"]
["Label","de537fc2-cb91-4b92-974b-b1e27123ef96","","","Note: Bathroom fittings samples to be provided for approval prior to ordering ",{"$nulls":4},"Dflt"]
["Item","0d91387e-d746-453b-959e-019b1e6d1053","D.3.1.14.1","","Hand Wash Basin -  Vaal Snitaryware Hibiscus Wall mounted basin; Code 7023, two tapholes, including intergrated overflow and chainstay hole bolted to wall and sealed with silicone sealant where basin meets wall; 510x405mm white Vitreous China","No",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G223 * H223,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e65810f1-7889-4587-9078-da279641a154","D.3.1.14.2","","WC Pan -  Vaal Sanitaryware Hibiscus close coupled suite (Code:772656), comprising 90 degree outlet open rim pan (Code:772600\\0 with matching 6/3 litre top dual flush cistern (Code:710740) including lid and fitments and Jazz Thermoset seat (Code:8531Z0) White Vitreaus China","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b5b7dd3b-1dde-4317-b305-93c7e2d2d971","D.3.1.14.3","","Basin Mixer - Cobra Watertech Ledimo 15mm pillar tap with aerator outlet and flanged backnut (Code:LO-214-15) manufactured in accordance with SANS 226:200 Type 1 (BS 5412) Chrome plated","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7d103e68-1fd3-45eb-8db0-4e454c6ed1c7","D.3.1.14.4","","Kitchen Sink - S1 - Franke - Quinline QLX/QLL 611","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","00f4c2f8-2b15-4e45-8664-77eb55ef83ac","D.3.1.14.5","","Sink Mixer - Cobra Watertech Noka 15mm chrome plated deck mounted sink mixer with overarm swivel outlet and adjustable flanges (Code:NA-970) manufactured in accordance with SANS 226:2004 Type 1 (BS 5412)","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6aa43f93-267c-44e9-a730-0622b6f2eea9","D.3.1.14.6","","Paper towel dispenser and bin - Franke Stratos STRX 601 1,2/1.5mm thick satin finished stainless steel paper towel and soap dispenser combination (Code:359770), size 396x134x305mm high with a capacity of 300-400 towels, replace able and refillable 1 litre container and cylinder lock with standard Frankey key, container and cylinder lock with standard Franke key, plugged and screwwed to the wall with stainless steel screws.  ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","cbc087f7-0b33-44c7-9f5a-b8d9f3b93097","D.3.1.14.7","","Toilet paper dispenser - Franke Stratos STRX672 1,2/1.5mm thick satin finished stainless steel double toilet roll dispenser (Code:359716), size 156x141x303mm high for 2 rolls maximum 108mm diameter with spindle system and cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","587b0f0e-2990-4187-b404-50d587d13d19","D.3.1.14.8","","Soap Dispenser - Franke Stratos STRX618 1,2/1.5mm thick satin finished stainless steel soad dispenser (Code:359705), size 100 x 134 x 304mm high with a replaceable and refillable 1 litre container, cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws. ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","46682cff-abef-4767-888a-ade36b7dd677","D.3.1.14.9","","Wall Hung Bowl Urinal - Vaal Sanitaryware Sweetpea Urinal - 565x275x310mm white vitreous China wall mounted top inlet urinal (Code:705126) including 38mm chromium plated domical grating (code:8787Z0) and chromium plated top inlet spreade (Code:7054Z0).","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","79def515-407f-4425-90ad-67e667426a6f","D.3.1.14.10","","Pillar sink mixer - Cobra Watertech Medical Elbow Action - Ref:505-21B pillar tap with blue indice. 1/4 inch turn ceramic disc and flanged back nut;  Chromium Plated; Cobra Watertech (Pty) Ltd","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3e245d80-0c84-4a61-96e2-f347e498061c","D.3.1.14.11","","Flush Valve Grab Rail - Standard grab rails for disabled WC by Chairman industries, 750mm SR2 for back rail.  ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c74cbdd5-51b0-4309-a3b2-4a4f3526859c","D.3.1.14.12","","Cistern back Rail - Standard grab rails for disabled WC by Chairman industries, 750mm SR2A for Cistern back rail. ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f073af39-21dc-4942-b73e-eb00b61e11e3","D.3.1.14.13","","Dogleg side rail - Standard grab rails for disabled WC by Chairman industries, 750mm DL2 dog-leg side rail.  ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d9e043c6-f883-44c1-9771-8974e4e536bb","D.3.1.14.14","","WC Pan - Vaal Sanitaryware Pearl Paraplegic vitreous china floor mounted paraplegic wash-down suite colour white (Code:7300SC) comprising semi close couple 90 degree outlet open rim wash-down pan and matching 9 litre cistern, including lid, fitments and purpose made chromium plated side flush lever, white Vitreous China.","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","63ea47a5-2087-43b0-b00f-e58b59a550d6","D.3.1.14.15","","Staff Mixer - Cobra Watertech Gal 15mm chrome plated single lever undertile bath/shower mixer with classic handle (Code: GA-656), sliding wall flange and stepped blanking plug, manufactured in accordance with SANS 1480:2005 (BS EN 1286).","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2a3f9224-e216-4bb6-a171-bbe72975806a","D.3.1.14.16","","Shower Rose - Cobra Watertech chrome plated Relaxa Plus shower head (Code:28274) with five spray patterns, ball-jointed connector and anti-lime nipples. ","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ae47e708-4121-4933-aab5-f5344084d2df","D.3.1.14.17","","Shower Rail - Cobra Watertech 600mm long Classic shower rail (Code:007-MSR/CP) with sliding handshower holder. ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","25a26660-90f5-489f-b10c-c886a5c21956","D.3.1.14.18","","Shower Rose  Cobra Watertech 110mm diameter Circa handshower (Code:007CI/CP) with 3 spray functions and anti-lime nipples. ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b7ffba0b-411a-4cde-b45d-1c11370f6884","D.3.1.14.19","","Shower Mixer - Cobra Watertech Gala 15mm chrome plated single lever undertile batch/shower mixer with classic handle (Code:GA-656), sliding wall flange and stepped blanking plug, manufactured in accordance with SANS 1480-2005 (BS EN 1286)","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","fca68e39-4ce0-4b08-b304-f528b6da9f63","D.3.1.14.20","","Hinged Bench/Fold up shower seat - Ref XS ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e9d46d70-bb0d-4125-83b2-3bef7a48228a","D.3.1.14.21","","Paper towel dispenser and bin - Franke Stratos STRX 601 1,2/1.5mm thick satin finished stainless steel paper towel and soap dispenser combination (Code:359770), size 396x134x305mm high with a capacity of 300-400 towels, replace able and refillable 1 litre container and cylinder lock with standard Frankey key, container and cylinder lock with standard Franke key, plugged and screwwed to the wall with stainless steel screw","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3db26b24-62e4-4e54-b8ce-85af5662c440","D.3.1.14.22","","Toilet paper dispenser - Franke Stratos STRX672 1,2/1.5mm thick satin finished stainless steel double toilet roll dispenser (Code:359716), size 156x141x303mm high for 2 rolls maximum 108mm diameter with spindle system and cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e167cff5-250c-43ba-b420-93db7d0c9c50","D.3.1.14.23","","Soap Dispenser - Franke Stratos STRX618 1,2/1.5mm thick satin finished stainless steel soad dispenser (Code:359705), size 100 x 134 x 304mm high with a replaceable and refillable 1 litre container, cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws. ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1155f3a0-f9ce-490c-a38d-e6cd2b0c8b84","D.3.1.14.24","","Soap Holder - Franke BHM6P polished stainless steel double arm double arm soap rack (Code:359944), size 163x100mm deep, plugged and screwed to the wall with stainless steel screws. ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9cf1609d-4007-409a-9ab6-59671aee5555","D.3.1.14.25","","Sanitary Bin - Waste bin with hygiene bag dispenser for wall mounting, stainless steel, surface satin finished, front with Inox Plus surface refinement for the reduction of finger marks and better cleaning characteristis (easy to clean), material thickness 1.5mm, curved front cover, approx. 3.8 litre capacity, folding self-closing lid wth piano hinge, removable plastic container inside, incl, stainless steel screws and dowel.  Code STRX614","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","fab24519-b511-4cbf-9af5-f681900d54a0","D.3.1.14.26","","32mm Diameter chromium plated curtain or hanging rail 800mm long including flanged end brackets ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","dcfe890a-a10b-4e98-8263-dfd0a0d77c9e","D.3.1.14.27","","Lab Sink - Vaal Sanitaryware Lab Sink ceramic fireclay laboratory sink colour White (Code:234500), size 435 x 335mm with waste outlet including acid resistant waste fitting (code:8790Z0) fitted underneath opening in workshop surface (by others) on and including two adjustable underslung brackets (code:8109Z0)","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","892df165-a090-415b-9c8b-80e18be8d6d7","D.3.1.14.28","","Mixer - Cobra Watertech 15mm chrome plated wall mounted mixer (Code:515/055-21) with aerated swan neck swivel spout, fixed centre bent inlet connections and elbow action lever, manufactured in accordance with SANS 226:2009 Type 2 (BS 5412)","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0a7b5204-4b5e-41ee-915f-5b82211c8190","D.3.1.14.29","","Emergency shower  - Cobra watertech 15mm chrome plated Prestex shower head (Code:065) with balljoint connector. ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","48fd4e17-fe5f-41c9-baae-4ff2e8524078","D.3.1.14.30","","Shower Mixer - Cobra Watertech 20mm brushed chrome plated metering valve (Code:KM1-00) with non-hold open feature, pull chain assembly and integral shut-off valve, manufactured in accordance with SANS 1808-9:2001.","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","8d819f84-6a91-4e60-9e8b-0b7783b2fa98","","","Valves ",{"$nulls":4},"Dflt"]
["Item","6e70f342-e51a-4556-af1a-a9d7ada9a340","D.3.1.14.31","","20mm Isolating Valve ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G254 * H254,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","d6aba612-72ad-4efd-93da-939432cadb17","D.3.1.14.32","","32mm Isolating Valve ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e5340cf3-bd5a-408e-b96f-5caf08a5c55e","D.3.1.14.33","","40mm Pressure Release Valve ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","46f6728d-fc1e-4fca-80ad-20ba51ea352c","D.3.1.14.34","","FM2.100CP \"Flushmaster\" toilet flush valve ","No.",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","46ef4f04-ed37-4f11-9f75-2f0e2010b0f6","","","TRAPS ETC ",{"$nulls":4},"Dflt"]
["Label","a40f0835-1a07-446c-afa6-952cc0b4a166","","","uPVC ",{"$nulls":4},"Dflt"]
["Item","5885e6f1-892f-4ef9-88a2-a2d95112e30c","D.3.1.14.35","","50mm \"P\" trap ","No.",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G260 * H260,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","889f64d7-86bc-4484-b5a0-bfb081e5dda5","D.3.1.15","","GLAZING ",{"$nulls":4},"Dflt"]
["Label","7cd35591-482e-4a17-95ad-9447b82574b0","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","1e85d04c-b582-4488-b7c2-cded8b153db5","","","TOPS, SHELVES, DOORS, MIRRORS, ETC ",{"$nulls":4},"Dflt"]
["Label","7b18d5e2-f324-4622-86b1-7d68d6ca1522","","","6mm Silvered float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers and sealed to tiles with clear silicone sealant ",{"$nulls":4},"Dflt"]
["Item","4f31afe5-0b49-4ff4-b3ef-0051df79500a","D.3.1.15.1","","Mirror sizes 600 x 985mm high ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G265 * H265,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","ed37a16e-0649-4a4f-95fa-5f57fd2ddabd","D.3.1.16","","PAINTWORK ",{"$nulls":4},"Dflt"]
["Label","aac9256a-df4b-4ef9-85a0-0f8a6ead65af","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","6ee8958f-7915-47cf-8ec4-b3b97d22e5a1","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","0f33e4f0-c4de-4516-864f-cc5a01fc806c","","","All colours to be selected by the Architect ",{"$nulls":4},"Dflt"]
["Label","96ed1e4d-8a6c-4ff4-ba71-e8e4f2f26b8e","","","Only approved brands of paint shall be permitted ",{"$nulls":4},"Dflt"]
["Label","87454763-dd29-4900-bf76-9fda2cb9f7cb","","","All painting measured generally will be in colours with a value of more than 7 on the Munsell system in accordance with the relevant SABS specification. Any painting in colours with a value of 7 or less on the Munsell system shall be given as paintwork in darker colours ",{"$nulls":4},"Dflt"]
["Label","71da9ab9-7efc-43c5-b5ee-f7f41264ca3f","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","43cd9ad2-49fe-46ac-9b82-e256eb79f9c3","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Prime with one coat of plaster primer all in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","2d6f663e-bd78-4f02-869b-14a11e682cf4","D.3.1.16.1","","On walls ","m²",700,{"v":0,"d":"0.00"},{"$f":"ROUND(G274 * H274,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5aaa65ed-3625-4e66-86f7-d2fb8761136e","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","bb27e043-dd00-49db-a31b-aff43fabfe8b","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Finish with 2 coats of super acrylic PVA paint or similar approved. All in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","2cad45e6-6631-499f-a112-5a3f0423df95","D.3.1.16.2","","On walls ","m²",700,{"v":0,"d":"0.00"},{"$f":"ROUND(G277 * H277,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","42c44892-360b-4e5c-8c82-78df2f4a505d","","","ON EXTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","8c2a3d71-5338-44f4-80c5-c6491d2634e4","","","Primer and finish with two coats \"Marmoran Armourbrush\" or equally approved, applied in strict accordance to manufacturer's instructions. ",{"$nulls":4},"Dflt"]
["Item","203c5c26-d88d-4508-9727-7dfdcb1a8dc0","D.3.1.16.3","","On walls  / RC Beams","m²",52,{"v":0,"d":"0.00"},{"$f":"ROUND(G280 * H280,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5a47e6e9-4a03-4235-aaf8-ea11bcbbe89b","","","ON PLASTERBOARD SURFACES ",{"$nulls":4},"Dflt"]
["Label","0ed2501f-9d04-4352-a45f-53b5e83f7dde","","","One coat alkali resistant primer and two coats PVA emulsion paint for interior use ",{"$nulls":4},"Dflt"]
["Item","1980d0e4-7521-483e-8dc9-a457fb499f34","D.3.1.16.4","","Ceilings and cornices  ","m²",507,{"v":0,"d":"0.00"},{"$f":"ROUND(G283 * H283,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","a4593709-30e1-4bb3-a793-b0c683ebf8f1","","","ON METAL SURFACES ",{"$nulls":4},"Dflt"]
["Label","5b14c917-345e-4cd8-871a-9eaf43f271b1","","","One coat \"Namelcote\" zinc chromate primer UC 53, one coat \"Plascon Galvogrip\" metal primer and two coats \"Velvaglo\" polyutherane enamel paint (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","97d3c664-4226-4627-9e2c-7dbdf7981b35","D.3.1.16.5","","On door frames etc ","m²",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G286 * H286,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f1820b8b-2bde-4bff-b91e-bbd3e49247fa","","","ON WOOD SURFACES ",{"$nulls":4},"Dflt"]
["Label","013ae262-e8dd-4c91-982a-1a43e17c9c82","","","One coat \"Spick and Span\" Oil based wood primer (UCS2), two coats \"Velvago Polyurethane enamel paint (VLO). (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","0a9e842f-cdb3-4842-9151-e63ac45c139f","D.3.1.16.6","","On doors ","m²",60,{"v":0,"d":"0.00"},{"$f":"ROUND(G289 * H289,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","09319604-96e2-4046-8fee-9f14b17718d0","","","\"Plascon\" or equally approved wood filler BS, One coat \"Spick and Span WoodShield\" diluted with mineral turpentine 25 and 2 coats \"Spick and Span Woodshield\" (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommend",{"$nulls":4},"Dflt"]
["Item","c628e055-1fd5-4d69-8490-ac7cc221466d","D.3.1.16.7","","On doors ","m²",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G291 * H291,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","34a614b8-5c53-4b0b-9673-085f5f8baee0","D.3.1.17","","PROVISIONAL SUMS ",{"$nulls":4},"Dflt"]
["Label","a2cdd826-0493-44f6-9f6b-ab718d166d68","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Item","8c213e29-aee5-4c3e-b484-ea89d82b68d4","D.3.1.17.1","","Supply and Install the 7.8m long Crawl Beam: Size 305 x165x40 I Beam.  The rate shall include the cost of supply,  and complete installation with 210mm Long Cleat Plate made from 152x165x20Kg/m T bolted to RC beam using 2 M16 Hilti HVU which has chemical bolts at each side all in accordance with the details in Drawing No. J40073/010-419/Rev A 1.   Material: 3CR12 and System: Multi-purpose epoxy; Minimum DFT (250 micron) ","No. ",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G294 * H294,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f0eeaad5-8db7-4058-b15c-fef19e9fc6f0","D.3.1.17.2","","Insulation boarding in 1200mm widths with longitudinal flap joints, laid over purlins (at approximately 1000mm centres) and fixed concurrent with roof covering, including holes through boards etc ","m²",338,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Sum","7a15955e-3b4e-4cdc-af1e-5b3fa1303549","D.3.1.17.3","","Fix 1 broken window pane","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H296,2)","v":{"v":0,"d":"0.00"}}]
["Item","fd438e6d-c1b4-40a0-b02d-7d603f058aba","D.3.1.17.4","","Provide the sum of R 250,000,00 (Two Hundred and Fifty Thousand Rand) for mechanical and electrical installation and treatment of corrosion on roof","Prov.Sum",1,{"v":250000,"d":"250,000.00"},{"$f":"ROUND(G297 * H297,2)","v":{"v":250000,"d":"250,000.00"}}]
["% Previous","cb001d61-ce82-4749-8182-3f690b68d747","D.3.1.17.5","","Add for profit and general attendance upon above if required  ","%",{"$f":"I297","v":{"v":250000,"d":"250 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Label","afe65f7e-1085-41a2-9ec8-b8626d729c6b","","","Corrective work to structure/building"]
["Sum","e0873f55-b0ee-4304-8b4f-51b5ce372654","D.3.1.17.6","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":250000,"d":"250,000.00"},{"$f":"ROUND(H300,2)","v":{"v":250000,"d":"250,000.00"}}]

{"sheet":"BILL D.4.","index":13,"n_rows":171,"n_cols":10,"rows_kept":171,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.4.",null,"GUARD HOUSE",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","29b363b1-1c1a-4289-8d0a-e36db51a3720","D.4.1","","GUARD HOUSE",{"$nulls":4},"Dflt"]
["Label","e0775a9f-3cde-461e-8ba5-065ace440636","","JBCC","SECTION D.4.1 : GUARD HOUSE",{"$nulls":4},"Dflt"]
["Sum","3394bbc4-6254-446d-b4d0-03b1715a9028","D.4.1.1","","Housekeeping (Includes cleaning and organising working area)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H11,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","4541a07f-ce72-4b7e-9002-ccd0677bc0e5","D.4.1.2","","IRONMONGERY ",{"$nulls":4},"Dflt"]
["Label","cf7d747d-1324-4030-afda-4215b8453dbd","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","7c4f7273-69b2-4602-8225-e194874189f6","","","LOCKS ",{"$nulls":4},"Dflt"]
["Label","c6c50930-0f73-422a-afae-86a598e9053c","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","b126f101-04c4-47e4-a1a7-6bef0825cb76","D.4.1.2.1","","Stainless steel Euro-profile cylinder sash lock (Code: D036S) ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G16 * H16,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","66ec58d8-ebd0-455d-9643-2e631caf8b8d","D.4.1.2.2","","Stainless steel Euro-profile cylinder dead lock (Code: D037D) ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0938e2df-e158-44f4-ad98-8958a1411ea7","D.4.1.2.3","","Stainless steel Euro-profile escutcheon (Code: DCE-002) ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7113483f-6853-4ae8-94f2-a09b40a96bb7","D.4.1.2.4","","25mm narrow stile deadlock (Code: D045D) ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a4084249-6c7e-43ec-bdb6-509fcc96e661","D.4.1.2.5","","Nickle plated 65mm bathroom privacy cylinder (Code: DBC0065001) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5e1ac7fb-1c8b-4942-8718-0798737aeb30","D.4.1.2.6","","Nickle plated 65mm ten pin Euro-profile grand master keyed single cylinder (Code: DSC104201) ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","93478bcd-8179-44fe-af19-8ac17cc5e5b3","D.4.1.2.7","","Nickle plated 65mm ten pin Euro-profile grand master keyed double cylinder (Code: DDC106501) ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","7f003ab5-2b2f-42f3-87cc-d10d04f48293","","","HANDLES ",{"$nulls":4},"Dflt"]
["Label","ff35defd-a9c6-43b0-92f6-1db06fa3c56e","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","1713e0b1-2d42-418b-92f4-d75315f9ea5d","D.4.1.2.8","","350 x 32mm Stainless steel \"D\" shaped offset back-to-back pull handles (Code: DPH215) ","Pair",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G25 * H25,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9903353f-1953-4fe3-9d59-ef8fd805a2f7","D.4.1.2.9","","Stainless steel lever handle including 150 x 150mm backplate with cylinder hole (Code: TH120/BP) ","Set",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","79bf2a0a-31b4-4e6c-a66e-f2580221f1a7","","","PUSH PLATES AND KICKING PLATES ",{"$nulls":4},"Dflt"]
["Item","fca196d3-caa1-442f-9912-a9529ec229dd","D.4.1.2.10","","877 x 200mm Stainless steel kick plate ","No.",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G28 * H28,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","092706e3-81f7-4279-9a76-416e69f667be","","","LETTERS, NAMEPLATES, ETC ",{"$nulls":4},"Dflt"]
["Label","dd0693f1-ab5c-45a6-9b04-477e7295ba72","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","8b4ba578-fe2f-4d2b-bb9a-df70788b4315","D.4.1.2.11","","150 x 150mm stainless steel male/female/staff sign (Code: DSS-130) ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6add4e6b-5fd2-41f3-b9a2-19f67d2c46fc","D.4.1.2.12","","150 x 150mm stainless steel male or female sign (Code: DSS-132) ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","6964053d-212b-489d-bafa-e843bb33022e","","","SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","958e04c6-6867-4558-b697-df1671383e25","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","55ca8ddf-9124-4176-a8bf-08ce53c55530","D.4.1.2.13","","Nickle plated floormounted doorstop (Code: DDS-NP-018) ","No.",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G35 * H35,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f4ec2e8f-6f52-4daf-b901-1fed2db906ba","D.4.1.2.14","","Stainless steel hat and coat hook with rubber buffer (DHC-SS-031B) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","571cafa6-8ff2-4769-bedd-d0f09569b20d","","","DOOR CLOSERS ",{"$nulls":4},"Dflt"]
["Label","531b3b93-ba84-431b-a1a4-521a2f9b7a58","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","ded31ef3-219b-4266-b383-8928b853e554","D.4.1.2.15","","TS91/EN3 Slide channel door closer non-hold open  ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G39 * H39,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","0349c5fb-7aaa-4615-8176-347774fb6193","D.4.1.3","","PLASTERING ",{"$nulls":4},"Dflt"]
["Label","4016585a-5ca2-4a36-986f-a9ed66612f8d","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","406ff8bf-7bb2-4bbb-af83-96e0d61702d9","","","SCREEDS  ",{"$nulls":4},"Dflt"]
["Label","19769498-e6e8-48a0-8dc7-423645badad6","","","1:3 Cement screeds wood floated, on concrete ",{"$nulls":4},"Dflt"]
["Item","b215e336-0f13-4328-80fa-2e505a50d10b","D.4.1.3.1","","Average 50mm thick on floors to falls and crossfalls ","m²",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G44 * H44,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","e8353fdd-c094-48fa-bc83-98366d7ced38","","","INTERNAL PLASTER",{"$nulls":4},"Dflt"]
["Label","13b5a77f-fb5f-4ef3-b7eb-874ca1642969","","","Gypsum skim plaster",{"$nulls":4},"Dflt"]
["Item","05aec4fa-5c94-4fe6-9952-a8abc5103df3","D.4.1.3.2","","On ceilings","m²",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G47 * H47,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","97cc1d14-ec81-4b51-9a17-b0f4de53de2c","","","PLASTER ",{"$nulls":4},"Dflt"]
["Label","f5e173b2-79a9-4761-9c9e-49bca895e47d","","","One coat 1:5 cement plaster 12mm thick on brickwork or concrete finished with a wood trowel ",{"$nulls":4},"Dflt"]
["Item","04792826-f1a2-40ed-8555-b071311484d1","D.4.1.3.3","","On concrete beams  and walls","m²",15,{"v":0,"d":"0.00"},{"$f":"ROUND(G50 * H50,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","bfd65cfb-c000-4d3d-9004-4308445a1e84","D.4.1.3.4","","Crack repair on plastered surfaces with polyfilla or similar approved product","m²",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","70f1d80c-3dcd-444e-8b81-bd686d92e2bf","","","TILING ",{"$nulls":4},"Dflt"]
["Label","edd409c3-6c55-4b49-a8b8-40bbb091bd4a","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","020b02b6-339e-407f-8cb6-aba29cec6e51","","","\"Note All tiling shall be fixed to plaster or screed with an approved adhesive; the adhesive shall be as recommended by the manufacturer of the tiles. \"",{"$nulls":4},"Dflt"]
["Label","226eae0a-9a14-4f81-ac81-1b057c8d65cb","","","WALL TILING  ",{"$nulls":4},"Dflt"]
["Label","ab0d2f10-6274-4ea5-a2c3-3be34e9f1c84","","","200 x 200 x 6mm white glazed ceramic tiles fixed with adhesive to plaster (plaster elsewhere measured) and Dove Grey flush pointed with epoxy grout ",{"$nulls":4},"Dflt"]
["Item","8dc701a3-fc72-47a9-ab9d-f727ddc9ca51","D.4.1.3.5","","On walls in isolated panels, splashbacks, etc ","m²",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G57 * H57,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0c871a8c-3747-43e9-a8da-39db69e42b09","D.4.1.3.6","","On narrow widths ","m²",0.5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a05678b4-b3f4-410c-b60f-4aea2126b50c","D.4.1.3.7","","Attic stock ","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","86a37790-c195-4058-95fd-e2dcffbf56df","","","FLOOR TILING ",{"$nulls":4},"Dflt"]
["Label","e7638d35-ac65-4226-8028-56e6156c5ead","","","200 x 200mm porcelain floor tiles fixed with adhesive to screed (screed elsewhere) and flush pointed with waterproof grout ",{"$nulls":4},"Dflt"]
["Item","b08e795b-57cc-408f-8ffb-c37fb363d8a0","D.4.1.3.8","","Attic stock ","m²",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G62 * H62,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cb67d9c6-0712-412b-820f-a2b47c9c9f40","","","600 x 300mm or equally approved porcelain tiles fixed with adhesive on screed (elsewhere measured) and flush pointed with epoxy grout tile joint filler. ",{"$nulls":4},"Dflt"]
["Item","ff479d3f-5d84-4ee2-9f76-e27dc00c5d53","D.4.1.3.9","","Skirting 100mm high (of cut tiles 600 x 300mm) ","m",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G64 * H64,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","0b4a3e2c-f0f5-4d93-ab4d-504d1aca3142","D.4.1.3.10","","Attic stock ","m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","f17f18aa-0a84-4ccf-8b17-e07ff4f72c33","","","JOINT SEALERS, ETC ",{"$nulls":4},"Dflt"]
["Label","a2270dcd-7052-4b28-8374-6c9cfeb4e15f","","","Approved polyurethane joint sealant dressed into joint including protecting adjoining surfaces with masking tape ",{"$nulls":4},"Dflt"]
["Item","60e6b7ad-7da2-4ff3-a39e-38e44d9aaae9","D.4.1.3.11","","10 x 10mm Sealer in tile joint between floor and wall tiles ","m",4.5,{"v":0,"d":"0.00"},{"$f":"ROUND(G68 * H68,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","e84d9576-4dff-41d3-b7fd-95fe58255ded","D.4.1.4","","PLUMBING AND DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","bd95d9ea-0951-4848-a6be-2a05a32d25d8","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","9b99bd72-6799-4fcc-bf77-4dd57c2fd112","","","RAINWATER DISPOSAL ",{"$nulls":4},"Dflt"]
["Label","6783eba3-e78b-4cd8-b1c2-e4e34d82470e","","","\"Watertite\" aluminium ",{"$nulls":4},"Dflt"]
["Item","d06a91d9-5d6a-4dea-829b-d8c4521976c6","D.4.1.4.1","","140 x 150mm box gutter x 0.9mm brackets fixed at 500mm centres ","m",26,{"v":0,"d":"0.00"},{"$f":"ROUND(G73 * H73,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","862097d2-7844-4884-b4c0-8d9f6b32fc14","D.4.1.4.2","","Extra over gutter for outlet for 75mm dia. pipe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","864769e5-8f26-41f6-b9a5-e8a412fc864f","D.4.1.4.3","","75 x 1.27mm Diameter rainwater pipes ","m",13,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c72f9b75-0315-4e0a-8957-f639762de47b","D.4.1.4.4","","Extra over rainwater pipe for bend ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","879dad6f-bf7d-409b-abb7-74ff46ba5aad","D.4.1.4.5","","Extra over rainwater pipe for shoe ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","4652228d-dc64-4fd1-9dc7-861ec72f42f5","D.4.1.5","","SOIL DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","e4b66dc1-ce4c-4c00-a626-772f0705b0bb","","","uPVC soil and vent pipes ",{"$nulls":4},"Dflt"]
["Item","0162f009-7770-4cbc-baa4-df80a014013a","D.4.1.5.1","","50mm Diameter uPVC pipes ","m",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G80 * H80,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9698619c-5f07-4551-8865-bb5305f0e13b","D.4.1.5.2","","100mm Diameter uPVC pipes  ","m",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","2618a2ce-ee06-458d-888d-a9e94c96f106","","","Extra over uPVC for the following fittings  ",{"$nulls":4},"Dflt"]
["Item","e2ae60cb-3b6e-4f5c-bef1-df13b91dba43","D.4.1.5.3","","50mm Bend  ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G83 * H83,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6d5a5d65-00c5-474f-9440-817ed2d913ef","D.4.1.5.4","","50mm Reducing Junction ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","abd6f60c-b4df-42fb-bf95-43db18f4442b","D.4.1.5.5","","100mm dia Reducing Junction ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4b7f36b0-8375-4bb1-b5ec-7c9ca0a28edb","D.4.1.5.6","","100mm Bend ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e47d6244-f215-4b05-a5d7-372c082b4942","D.4.1.5.7","","100mm Stubstack ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","dcfc9c2b-c1fa-40e7-8b95-5b91cb728df6","D.4.1.5.8","","100mm Air vent cowl ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","55d20757-7c5e-4c7e-88b7-11a9cdde7392","D.4.1.5.9","","100mm Vent Cap ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bf5c76f0-5ef6-4499-83b3-0eeddbb3b01e","D.4.1.5.10","","100mm pan connector ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1440284c-9b89-4e56-b49a-021ed7e7f832","D.4.1.5.11","","Rodding Eye ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","fa762ef6-0156-4575-9de5-ae9b32a8d544","","","Testing ",{"$nulls":4},"Dflt"]
["Sum","71589f39-15cc-41b1-9114-7a8ced4ab187","D.4.1.5.12","","Testing soil drainage system ","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H93,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","66d83f96-3548-4be5-913c-b87ecda16075","D.4.1.6","","WATER SUPPLIES  ",{"$nulls":4},"Dflt"]
["Label","90edca29-6509-42fd-afef-91f439dac708","","","Copper pipes to SABS 460/0 fixed to walls, ceilings, drywall cavities, etc ",{"$nulls":4},"Dflt"]
["Item","40c0423c-8d8e-413a-a970-b867f93b26c3","D.4.1.6.1","","15mm Pipes ","m",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G96 * H96,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","148deaa1-0458-4ff9-b1f7-f9459fcaaa84","","","Extra over piping for \"Copcal\" soldered fittings ",{"$nulls":4},"Dflt"]
["Item","38731eda-09ff-497f-ab30-3faafca2a8d6","D.4.1.6.2","","15mm Fittings ","No.",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G98 * H98,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","39cd3a5e-666e-4f1f-8c6b-65eca7dec5e3","D.4.1.6.3","","15mm Reducer ","No.",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","6dec9db6-5427-453c-9a14-645701d6cf8e","","","TESTING ",{"$nulls":4},"Dflt"]
["Sum","83c8c2b0-8279-40db-a1a9-5a98796d6671","D.4.1.6.4","","Testing water pipe system ","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H101,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","12724f49-c291-40eb-b9ff-ec493dcfed59","D.4.1.7","","SANITARY FITTINGS  ",{"$nulls":4},"Dflt"]
["Label","dbe76056-dcb7-411d-87fe-32b2a9f818e0","","","Supply and fix the following sanitary fittings including assembly forming all joints and connections, bedding, pointing, building in, cutting and pinning, plugging and screwing and making good as necessary  ",{"$nulls":4},"Dflt"]
["Label","32224b00-1229-499e-bb8b-7abb32870b69","","","\"Vaal\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","6efbbf6e-46b6-483e-9380-995896f99002","D.4.1.7.1","","Hand Wash Basin -  Vaal Snitaryware Hibiscus Wall mounted basin; Code 7023, two tapholes, including integrated overflow and chainstay hole bolted to wall and sealed with silicone sealant where basin meets wall; 510x405mm white Vitreous China","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G105 * H105,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9e8bdb0c-71e9-4f4b-a027-8882455271a4","D.4.1.7.2","","WC Pan -  Vaal Sanitaryware Hibiscus close coupled suite (Code:772656), comprising 90 degree outlet open rim pan (Code:772600\\0 with matching 6/3 litre top dual flush cistern (Code:710740) including lid and fitments and Jazz Thermoset seat (Code:8531Z0) White Vitreaus China","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b5244eae-3bad-40c8-a6a2-a8aca8c9ed0c","D.4.1.7.3","","Kitchen Sink - S1 - Franke - Quinline QLX/QLL 611","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","122fb509-7fd3-4c41-8193-a1ea312c8f68","D.4.1.7.4","","Sink Mixer - Cobra Watertech Noka 15mm chrome plated deck mounted sink mixer with overarm swivel outlet and adjustable flanges (Code:NA-970) manufactured in accordance with SANS 226:2004 Type 1 (BS 5412)","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5abae48b-1248-4288-96e6-20a605685f7d","D.4.1.7.5","","Paper towel dispenser and bin - Franke Stratos STRX 601 1,2/1.5mm thick satin finished stainless steel paper towel and soap dispenser combination (Code:359770), size 396x134x305mm high with a capacity of 300-400 towels, replace able and refillable 1 litre container and cylinder lock with standard Frankey key, container and cylinder lock with standard Franke key, plugged and screwwed to the wall with stainless steel screws.  ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a75f8d47-0a89-4eaf-8166-7cc436672408","D.4.1.7.6","","Toilet paper dispenser - Franke Stratos STRX672 1,2/1.5mm thick satin finished stainless steel double toilet roll dispenser (Code:359716), size 156x141x303mm high for 2 rolls maximum 108mm diameter with spindle system and cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b6b8feb7-9a05-487c-8d32-fdb48fbf616d","D.4.1.7.7","","Soap Dispenser - Franke Stratos STRX618 1,2/1.5mm thick satin finished stainless steel soad dispenser (Code:359705), size 100 x 134 x 304mm high with a replaceable and refillable 1 litre container, cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws. ","No",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","bc6287fc-0d4d-4207-ab8a-be5bbb648961","D.4.1.7.8","","Basin Mixer - Cobra Watertech Ledimo 15mm pillar tap with aerator outlet and flanged backnut (Code:LO-214-15) manufactured in accordance with SANS 226:200 Type 1 (BS 5412) Chrome plated","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","5e1f9e8e-11c9-49fe-9e2d-0b99a6ba07e5","","","TAPS, VALVES, ETC ",{"$nulls":4},"Dflt"]
["Label","65e5ed19-0e05-48e3-9670-6ec8ce39bbf1","","","\"Cobra Watertech\" or equally approved ",{"$nulls":4},"Dflt"]
["Label","ae1bf96b-7d5f-48d2-97ab-f031872aff4c","","","Valves ",{"$nulls":4},"Dflt"]
["Item","ed7060a7-76e2-45b9-b6a3-abe20b1bcc9e","D.4.1.7.9","","20mm Isolating Valve ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G116 * H116,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","7c6dc36c-0501-493c-adc4-8d09da74be5f","D.4.1.7.10","","FM2.100CP \"Flushmaster\" toilet flush valve ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","e5c27d33-3e97-462e-a9f9-6bda398d171a","","","\"Cobra Watertech\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","033dee16-c041-4482-909f-09a3850972e4","D.4.1.7.11","","Cobra Watertech 32mm chrome plated slotted basin waste union (Code: 301-32) install chain and plug to suit ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G119 * H119,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7f8e972a-335c-4255-9729-a3f9366aef4b","","","TRAPS ETC ",{"$nulls":4},"Dflt"]
["Label","8f7f1def-bfcf-4024-9002-f02df6838fb9","","","\"Cobra Watertech\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","87850cfa-b677-471e-9c8f-a4d75bc212ad","D.4.1.7.12","","32mm chrome plated deep seal bottle trap with outlet for 50mm PVC (Code: 345/50). ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G122 * H122,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","7869b159-6715-46bd-97f7-1ed357785e2d","","","uPVC ",{"$nulls":4},"Dflt"]
["Item","c6278877-fb58-419d-963f-4faf922c4e52","D.4.1.7.13","","50mm \"P\" trap ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G124 * H124,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9d4e9635-703c-437f-996a-4f442e3fe016","","","HOT WATER CYLINDERS ",{"$nulls":4},"Dflt"]
["Label","6919b197-a50e-4ceb-8179-97fbd6795c70","","","\"Kwikot\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","1e2c5d21-6d12-4e4f-ad53-caed79c11da7","D.4.1.7.14","","Kwikot 600i Dual 100 litre capacity \"Slimline\" vertically mounted 600Kpa (Code: ESG-100-I). Water heater complete with standard driptray bottom outlet space vacuum breaker, safe valve, pressure reducing valve and stoptap. Position of units in roof space as shown on plan.","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G127 * H127,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","860d717a-8461-4179-91c4-83574d508282","D.4.1.8","","GLAZING ",{"$nulls":4},"Dflt"]
["Label","76aefcb5-98d5-4e7e-900a-4bfcddb3c298","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","ab47c63f-d67b-4a98-9ef0-ca55271eea4c","","","TOPS, SHELVES, DOORS, MIRRORS, ETC ",{"$nulls":4},"Dflt"]
["Label","8d7774a9-e085-4f8f-805f-5fcd69a6982a","","","6mm Silvered float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers and sealed to tiles with clear silicone sealant ",{"$nulls":4},"Dflt"]
["Item","1eb198e5-e01c-4fa2-b9b9-2dcc4fe6a0b8","D.4.1.8.1","","Mirror sizes 600 x 985mm high ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G132 * H132,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","7d779433-2f17-4958-87ce-b2b6df406d54","D.4.1.9","","PAINTWORK ",{"$nulls":4},"Dflt"]
["Label","85cf5167-512b-4a1b-9523-25fb4754214c","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","6c4190a5-a606-4adb-92b6-7240d6ff3550","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","609bb44b-f66c-4449-a71f-6f89746fc7ce","","","All colours to be selected by the Architect ",{"$nulls":4},"Dflt"]
["Label","c711a9db-e80f-4400-8aac-173a5daa3774","","","Only approved brands of paint shall be permitted ",{"$nulls":4},"Dflt"]
["Label","0f9a19a3-b2cb-4887-8393-cf0855e45e62","","","All painting measured generally will be in colours with a value of more than 7 on the Munsell system in accordance with the relevant SABS specification. Any painting in colours with a value of 7 or less on the Munsell system shall be given as paintwork in darker colours ",{"$nulls":4},"Dflt"]
["Label","f5346e3c-77fb-47d7-bbf5-6c79d44865bc","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","1707dc22-a424-48d0-9ff1-f3e7b02455a7","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Prime with one coat of plaster primer all in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","4c9397b2-c7bc-4d8e-9d18-c972cc50bf18","D.4.1.9.1","","On walls ","m²",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G141 * H141,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5a3e0665-9649-4171-a0f0-814e953e2db5","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, finish with 2 coats of super acrylic PVA paint or similar approved. All in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","17c00e3f-7fed-42ef-beb1-ca0ef1c70706","D.4.1.9.2","","On walls ","m²",100,{"v":0,"d":"0.00"},{"$f":"ROUND(G143 * H143,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","212a8ad5-39c2-4496-8b25-eeedb490b0bd","","","ON EXTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","bc8fd5f9-529c-4499-802c-c04aca374fb6","","","Primer and finish with two coats \"Marmoran Armourbrush\" or equally approved, applied in strict accordance to manufacturer's instructions. ",{"$nulls":4},"Dflt"]
["Item","3e21d352-e636-46cd-91d2-512e44f310ec","D.4.1.9.3","","On walls  / RC Beam","m²",11,{"v":0,"d":"0.00"},{"$f":"ROUND(G146 * H146,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2fcdd179-e108-45f5-b557-4c30c8be346e","","","ON PLASTERBOARD SURFACES ",{"$nulls":4},"Dflt"]
["Label","15860cd2-c376-4ded-852b-e24ee8c61dd0","","","Patch up holes in Ceiling with rhynolite or polyfilla.  One coat alkali resistant primer and two coats PVA emulsion paint for interior use ",{"$nulls":4},"Dflt"]
["Item","32a1e763-e155-499e-a6f8-9e4bf3c9ec39","D.4.1.9.4","","Ceilings and cornices  ","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G149 * H149,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","d53ddeb9-2ce7-4f0f-8c12-4cb407daf7fc","","","ON METAL SURFACES ",{"$nulls":4},"Dflt"]
["Label","21bc9c01-7327-4385-92db-3de005f4b2ae","","","One coat \"Namelcote\" zinc chromate primer UC 53, one coat \"Plascon Galvogrip\" metal primer and two coats \"Velvaglo\" polyutherane enamel paint (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","1f14a0dc-d52d-4a36-ae37-10c9619142d5","D.4.1.9.5","","On door frames etc ","m²",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G152 * H152,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","dc0612fe-9ede-4efe-aabc-b751a40c9713","","","ON WOOD SURFACES ",{"$nulls":4},"Dflt"]
["Label","ed4ae2b2-4331-4ea0-97d8-c321a8160b0c","","","One coat \"Spick and Span\" Oil based wood primer (UCS2), two coats \"Velvago Polyurethane enamel paint (VLO). (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","697c1f54-f265-4d1b-8735-08bf91079f05","D.4.1.9.6","","On doors ","m²",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G155 * H155,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8b3a834c-c59a-49a5-9c94-462169696e34","","","ROOFING ",{"$nulls":4},"Dflt"]
["Label","ec34b5b2-66d6-4839-bec6-0e008d9a991b","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","e205f454-de00-4333-b55e-95277f3997ec","","","PROFILED METAL SHEETING AND ACCESSORIES ",{"$nulls":4},"Dflt"]
["Sum","f0cc63a6-376e-4b97-ad97-eb1945d01476","D.4.1.9.7","","Remove all roof sheeting, Ridges and Hip cappings (corroded)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H159,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","16f580ca-ac87-49ba-a33c-d78d4d34f2cb","","","\"Klip-Lok 700\" profile roll-formed in continuous lengths from certified Galvanised steel Z200 0.58mm complying with ISQ 550 (3T) (A653) with a Chromadek Colomet finish to one side and standard backing coat, Papyrus white to other and accessories, fixed to timber purlins in strict accordance with manufacturer's specifications",{"$nulls":4},"Dflt"]
["Item","993a2dd4-147b-4886-b0d8-78c12c5308ae","D.4.1.9.8","","Roof covering with pitches not exceeding 25 degrees","m²",22,{"v":0,"d":"0.00"},{"$f":"ROUND(G161 * H161,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4701f4b3-9c1c-42cb-b563-24ac57c0270e","D.4.1.9.9","","Ridge cappings 550mm girth to suit roof profile","m",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8b7eef06-7fcb-4214-9c89-055dc1b51bdb","D.4.1.9.10","","Hip cappings 550mm girth to suit roof profile","m",7,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b4feea1b-46b6-4484-ba41-3a58326eb1a1","D.4.1.9.11","","Insulation boarding in 1200mm widths with longitudinal flap joints, laid over purlins (at approximately 1000mm centres) and fixed concurrent with roof covering, including holes through boards etc ","m²",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","61706903-4e4e-41fc-b11c-866327e6549c","D.4.1.10","","PROVISIONAL SUMS ",{"$nulls":4},"Dflt"]
["Label","e7127bbf-7861-4fee-ad73-7e5cd38cda10","","","For preambles see \"Model Preambles for Trades\""]
["Label","97ec4bd1-0fb9-4f75-9857-5781724a42b4","","","BUDGETARY ALLOWANCES (Electrical wiring, testing and connection, Water Connection, etc)"]
["Item","0f4a7b3f-4386-4bf5-9204-c874a2aee8dd","D.4.1.10.1","","Provide for Provisional Sum of R50,000.00 Additional Work as instructed by Engineer","Prov.Sum",1,{"v":50000,"d":"50,000.00"},{"$f":"ROUND(G168 * H168,2)","v":{"v":50000,"d":"50,000.00"}}]
["% Previous","77d999f0-cef2-4597-91d0-648dafc07a04","D.4.1.10.2","","Add for profit and general attendance upon above if required  ","%",{"$f":"I168","v":{"v":50000,"d":"50 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Label","4deaf642-3c2e-4e9d-bf08-42cd4266f945","","","Corrective work to structure/building"]
["Sum","82b134ea-a617-4533-8fbf-100a91d70c77","D.4.1.10.3","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":50000,"d":"50,000.00"},{"$f":"ROUND(H171,2)","v":{"v":50000,"d":"50,000.00"}}]

{"sheet":"BILL D.5.","index":14,"n_rows":286,"n_cols":10,"rows_kept":286,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.5.",null,"ADMIN BUILDING",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","7601f183-93b1-4c1d-871d-3de81b35c3b0","D.5.1","","ADMIN BUILDING",{"$nulls":4},"Dflt"]
["Label","e190923c-b754-4ea7-8d0a-780ad8614f69","","JBCC","SECTION D.5.1 : ADMIN BUILDING",{"$nulls":4},"Dflt"]
["Sum","1bcd031c-f7df-4585-8dd6-5df7c0ba9543","D.5.1.1","","Housekeeping (Includes cleaning and organising working area)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H11,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","8d1d6063-a5e0-433a-8e56-5bd1b633e31d","D.5.1.2","","CEILING ",{"$nulls":4},"Dflt"]
["Label","d9b229f6-a6de-4e0e-8048-ffd0b60f3473","","","SUSPENDED CEILINGS ",{"$nulls":4},"Dflt"]
["Label","002aa4a0-387f-4d60-8b80-244ba75cdae0","","","\"BPB Gypsum Donnceil Gyprex\" or equally approved 1200 x  600 x 12.5mm white vinyl ceiling tiles including SQ/T38 white powder coated tee suspension system including main and cross tees, necessary hangers, grids, etc ",{"$nulls":4},"Dflt"]
["Item","b32cc7fa-1a78-4207-a251-cc422ab807a0","D.5.1.2.1","","Ceilings suspended not exceeding 1m below timber purlins at 1500mm centres (passage)","m²",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G15 * H15,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","cea357e1-3a98-47db-8e53-2cb6433ea0d9","","","CORNICES ",{"$nulls":4},"Dflt"]
["Label","1a06ee65-80b8-4f11-b959-0cbd5b730dd3","","","BPB Gypsum \"donn\" shadowline cornices perimeter trims, etc to suspended ceilings ",{"$nulls":4},"Dflt"]
["Item","0d7d441a-d842-4ed7-b72d-6e29bebc7e75","D.5.1.2.2","","Type LSM 25 pre-painted cornices, plugged (passage)","m",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G18 * H18,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","645c4a8c-e7b5-4928-b98b-8929d930ea73","","","NAILED-UP CEILINGS ",{"$nulls":4},"Dflt"]
["Label","2e0d3da1-0b09-46e3-bbc9-1e4ff0886247","","","\"Everite\" or equally approved ceiling panels ",{"$nulls":4},"Dflt"]
["Item","1455fb31-5097-4bf4-93fe-200b4f9cf05d","D.5.1.2.3","","Ceilings of 1200 x 2400 x 6mm thick panels including 38 x 38mm SA Pine brandering at 450mm centres in both directions (kitchen/cleaner store)","m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9eae3063-4054-49cc-94f2-92c657ab9727","","","Gypsum plasterboard cornices ",{"$nulls":4},"Dflt"]
["Item","cf4e7eca-56bb-4443-bf4c-b1545b509db6","D.5.1.2.4","","75mm Coved cornices (kitchen/cleaner store)","m",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G23 * H23,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","8965f1d9-d72e-483e-8b19-b07a00af62ac","D.5.1.3","","IRONMONGERY ",{"$nulls":4},"Dflt"]
["Label","900b654c-cab1-4b96-a0b2-9b9e432ecd68","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","0bef7254-4b5d-411b-b293-fc3e3d4f2176","","","HINGES, BOLTS, ETC ",{"$nulls":4},"Dflt"]
["Label","1e8d5982-5dad-4d1b-a301-fde1f7d4f497","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","886b05f1-0e86-48ff-8d79-c5f269687611","D.5.1.3.1","","Stainless steel adjustable roller bolt (Code: DBC-SS-022) ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G28 * H28,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","1f16382e-df00-4050-b9bd-653e3ae67438","","","LOCKS ",{"$nulls":4},"Dflt"]
["Label","29189b04-a740-4393-9269-af27467d05cf","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","fa5100e1-f68e-4d55-bcdf-027a2e4ef049","D.5.1.3.2","","Stainless steel bathroom/WC dead lock (Code: D032D) ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G31 * H31,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ae8f3259-e6cb-4173-a177-0173bc83e3eb","D.5.1.3.3","","Stainless steel Euro-profile cylinder sash lock (Code: D036S) ","No.",17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f649d55d-daee-4d65-9cc9-32df2c1a1135","D.5.1.3.4","","Stainless steel Euro-profile cylinder dead lock (Code: D037D) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2f2eac1f-0726-4493-804c-36473583dc0b","D.5.1.3.5","","Stainless steel Euro-profile escutcheon (Code: DCE-002) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","584f62a1-4e19-41e3-b31c-cca74f1f8376","D.5.1.3.6","","25mm narrow stile deadlock (Code: D045D) ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0853b926-6f66-4ea6-8772-33e4f6c612e4","D.5.1.3.7","","Nickle plated 65mm bathroom privacy cylinder (Code: DBC0065001) ","No.",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","07e1c475-4009-41b7-9035-56eae0c09904","D.5.1.3.8","","Nickle plated 65mm ten pin Euro-profile grand master keyed single cylinder (Code: DSC104201) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6007e0b4-f248-4455-b41b-62888d744832","D.5.1.3.9","","Nickle plated 65mm ten pin Euro-profile grand master keyed double cylinder (Code: DDC106501) ","No.",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","38e35f5e-58a6-4cd8-a897-caebd6a6600c","","","HANDLES ",{"$nulls":4},"Dflt"]
["Label","ab236ea8-0134-401f-92c2-17ccdf51f4d5","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","067a4e0c-b74f-4606-a04c-ce65b539a958","D.5.1.3.10","","Stainless steel WC indicator with 79mm turn knob for physically impaired (Code: DWC-006) ","Pair",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G41 * H41,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2439db46-754a-410c-ad29-739e1109fbe2","D.5.1.3.11","","150 x 19mm Stainless steel \"D\" shaped straight bolt through pull handles (Code: DPH301C) ","Pair",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3d23e44c-e9a1-4f56-835d-2357c5af5a69","D.5.1.3.12","","350 x 32mm Stainless steel \"D\" shaped offset back-to-back pull handles (Code: DPH215) ","Pair",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","85840945-0927-4b36-8cb1-8e0e376aeef7","D.5.1.3.13","","350 x 32mm Stainless steel \"D\" shaped straight back-to-back pull handles (Code: DPH213) ","Pair",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e37f68ab-2888-4eb2-8cf9-fc8d90aea7df","D.5.1.3.14","","Stainless steel lever handle including 150 x 150mm backplate with cylinder hole (Code: TH120/BP) ","Set",17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","e291bd6a-748f-4c74-88c6-e5f06acb06d6","","","PUSH PLATES AND KICKING PLATES ",{"$nulls":4},"Dflt"]
["Item","53d29cc6-e886-469f-b1ba-b7b4b56436c2","D.5.1.3.15","","712 x 200mm Stainless steel kick plate ","No.",12,{"v":0,"d":"0.00"},{"$f":"ROUND(G47 * H47,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","dde46757-c708-438d-b261-1aa29ab558ec","D.5.1.3.16","","877 x 200mm Stainless steel kick plate ","No.",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","4bbe28da-df94-43e8-a5f2-089f9f45b02a","","","LETTERS, NAMEPLATES, ETC ",{"$nulls":4},"Dflt"]
["Label","7d4aa18e-b543-48bb-82a8-cda03047c73b","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","bb3f4404-f5af-48d7-a68f-c2e89be35b66","D.5.1.3.17","","150 x 150mm stainless steel male/female/staff sign (Code: DSS-130) ","No.",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G51 * H51,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","9cee7cd0-b7da-4951-9579-afd177ca8e0b","D.5.1.3.18","","150 x 150mm stainless steel male or female sign (Code: DSS-132) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","eef06262-91a6-437d-a961-0871f61410a5","D.5.1.3.19","","150 x 150mm stainless steel disabled person sign (Code: DSS-133) ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7e11ea53-1551-4a90-9435-92c631de1250","D.5.1.3.20","","150 x 150mm stainless steel fire hose reel sign (Code: DSS-145) ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","65e8a429-3dd5-486a-bd2d-f97a6d6e9966","","","SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","84bfd1b2-d987-4d99-9b3c-8b9044b78d79","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","4ca50cb4-1d53-476b-8eaf-b09b2950d2c4","D.5.1.3.21","","Nickle plated floormounted doorstop (Code: DDS-NP-018) ","No.",29,{"v":0,"d":"0.00"},{"$f":"ROUND(G57 * H57,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ee65ce7d-3415-4858-bcee-6296d8b6a9f7","D.5.1.3.22","","Double action non hold open floor spring complete with stainless steel cover plate 8021 bottom strap and 8062 top centre for aluminium framed glass door (Code: BTS75R/EN2-5) ","Set",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","81274f42-7056-4ea7-8da6-6d79e0e02e24","D.5.1.3.23","","Stainless steel hat and coat hook with rubber buffer (DHC-SS-031B) ","No.",17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","dc7b30f9-c249-42c2-b4f2-547e2e2aab70","","","DOOR CLOSERS ",{"$nulls":4},"Dflt"]
["Label","e9a7c54a-886c-4a02-814e-174149984dd3","","","\"Dorma\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","33e81fe3-e68d-4db2-85c3-6d5693e619f3","D.5.1.3.24","","TS91/EN3 Slide channel door closer non-hold open  ","No.",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G62 * H62,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b940dd08-c090-4d81-9796-fbc6a35a5a7e","D.5.1.3.25","","TS73N/EN3-4 Parallel arm door closer delayed closing push side fitting ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","3bd47d07-d302-428c-91ad-116b3b1631c6","D.5.1.4","","ROOFING ",{"$nulls":4},"Dflt"]
["Label","fca34711-e2b9-4762-b03b-aa98e4614671","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","82cf5129-d97a-4abd-baee-db9ca6b51d62","","","PROFILED METAL SHEETING AND ACCESSORIES ",{"$nulls":4},"Dflt"]
["Sum","8f84e425-95ac-4e5c-b652-630676bdf6da","D.5.1.4.1","","Remove all roof sheeting, Ridges and Hip cappings (corroded)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H67,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","efec2f37-60e3-48d5-971f-5096caafe8a7","","","\"Klip-Lok 700\" profile roll-formed in continuous lengths from certified Galvanised steel Z200 0.58mm complying with ISQ 550 (3T) (A653) with a Chromadek Colomet finish to one side and standard backing coat, Papyrus white to other and accessories, fixed to timber purlins in strict accordance with manufacturer's specifications.  ",{"$nulls":4},"Dflt"]
["Item","cbdb605f-7686-459d-a8d6-b3635358483c","D.5.1.4.2","","Roof covering with pitches not exceeding 25 degrees","m²",580,{"v":0,"d":"0.00"},{"$f":"ROUND(G69 * H69,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","744b819a-1b42-41d6-a18d-f5baa01e6877","D.5.1.4.3","","Ridge cappings 550mm girth to suit roof profile","m",70,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","6503b80d-96c0-4af9-9303-a77442faa956","D.5.1.4.4","","Hip cappings 550mm girth to suit roof profile","m",40,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","5525b55e-3c84-4ef8-8b55-7865e49c4f21","D.5.1.4.5","","Head wall flashings 375mm girth 2 times bent to suit roof profile ","m",12,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b04cd663-ebaf-404b-ba84-705aa4a77b05","D.5.1.4.6","","Counter flashing 185mm girth 2 times bent ","m",12,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4f613cba-47db-494d-912f-c6f2ed2b2951","D.5.1.4.7","","Insulation boarding in 1200mm widths with longitudinal flap joints, laid over purlins (at approximately 1000mm centres) and fixed concurrent with roof covering, including holes through boards etc ","m²",580,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","19eb2c81-3ba7-4979-a18d-6ffd765b9a01","D.5.1.5","","WATERPROOFING TO ROOFS, and SHOWER FLOORS",{"$nulls":4},"Dflt"]
["Label","d6c4fbc3-d3ec-44b5-92df-e2df8b6be578","","","Two layer Derbigum SP4 waterproofing membrane, with 75mm side laps and 100mm end laps, sealed to primed surface to falls and crossfalls by 'torch-fusion' finished withone coat of acrylic primer followed by two coats acrylic paint. Waterproofing to be installed by an Approved Derbigum Contractor under a ten year guarantee. ",{"$nulls":4},"Dflt"]
["Item","aa788f0d-87ba-492b-b75c-5d9fb3e476ff","D.5.1.5.1","","On flat roofs ","m²",47,{"v":0,"d":"0.00"},{"$f":"ROUND(G77 * H77,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ecfcc8db-1ed8-4882-bf8a-81b9a22941f9","D.5.1.5.2","","On sides of gable and parapet walls ","m²",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c96a620b-6d8f-4fb8-adf8-d219aaa60586","D.5.1.5.3","","Additional membrane at 100mm diameter outlet ","No.",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","65660bb7-bc23-4b63-b3bd-14c74619e3a9","","","Two coats Derbigum Roof Cote Aluminium ",{"$nulls":4},"Dflt"]
["Item","a5701adf-d9d1-4c84-b2a3-60f9f314a73e","D.5.1.5.4","","On flat roofs ","m²",66,{"v":0,"d":"0.00"},{"$f":"ROUND(G81 * H81,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","ee1ff2e9-1f59-4897-a3aa-257a2db41c30","","","WATER PROOFING TO SHOWERS ",{"$nulls":4},"Dflt"]
["Label","c949ea3d-e5f6-4c4c-92e2-20c18c5c5f94","","","Apply \"Tal Superflex I\" or equally approved then reinforce with Tal Superflex membrane, waterproofer and bonding agent applied as per manufacturer's specification ",{"$nulls":4},"Dflt"]
["Item","6e5e831e-c8bf-4b69-8572-258ce1f0f9af","D.5.1.5.5","","On shower floors ","m²",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G84 * H84,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","91e50686-6e58-4eb8-ba31-d2f977475909","","","EAVES, VERGES, ETC ",{"$nulls":4},"Dflt"]
["Label","4b88b239-b4fe-47c7-af02-88c31b3141e9","","","Supply and Install \"Everite FC77\" pressed fibre-cement ",{"$nulls":4},"Dflt"]
["Item","2501d6d6-579e-4b37-b00f-9787b739a9d7","D.5.1.5.6","","15 x 300mm Fascias and barge boards including galvanised steel H-profile jointing strips (provision)","m",103,{"v":0,"d":"0.00"},{"$f":"ROUND(G87 * H87,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","5f955761-93a9-4cb7-9c13-2b319b7583ae","","","JOINERY SUNDRIES ",{"$nulls":4},"Dflt"]
["Label","18dd16ed-a7a3-4cc0-8c2f-55d4a9bd32a2","","","Seats ",{"$nulls":4},"Dflt"]
["Item","bd1f86de-d8c7-41ea-b6aa-5c74078280f1","D.5.1.5.7","","600 x 1000mm long seat, comprising 70 x 22mm meranti timber slats bolted to steel support complete ","No.",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G90 * H90,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","37b8ee2f-0200-40e3-9106-609f84a51c54","D.5.1.6","","PLUMBING AND DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","fbf13f80-971d-4bee-b1f1-a63aee6be5a2","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","dc2ba0f7-11b1-46e3-a305-683dfacfb88f","","","RAINWATER DISPOSAL ",{"$nulls":4},"Dflt"]
["Sum","7f49f473-ce93-43d4-8fdc-9a8347e78f02","D.5.1.6.1","","Remove the installed roof drainage system (gutters and downpipes)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H94,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","23247a1d-9c10-4f0f-8fd4-32c0a5fe9591","","","\"Watertite\" aluminium ",{"$nulls":4},"Dflt"]
["Item","fdd15ba2-34ee-45de-84f4-4804a5b4890b","D.5.1.6.2","","140 x 150mm box gutter x 0.9mm brackets fixed at 500mm centres ","m",109,{"v":0,"d":"0.00"},{"$f":"ROUND(G96 * H96,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","cb121b8a-6b2f-481e-b421-f63a971989fb","D.5.1.6.3","","Extra over gutter for outlet for 75mm dia. pipe ","No.",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4099e358-0b01-446f-ba73-83247eff2538","D.5.1.6.4","","75 x 1.27mm Diameter rainwater pipes ","m",35,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a85eb093-ffa9-4529-bd0e-684eb0f08e77","D.5.1.6.5","","Extra over rainwater pipe for bend ","No.",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","768e7eb7-e08a-4526-9ac5-4e382e7c2ca3","D.5.1.6.6","","Extra over rainwater pipe for shoe ","No.",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","a68a5939-280a-425c-9388-4286d90eac03","","","\"Fulbore\" cast iron outlets ",{"$nulls":4},"Dflt"]
["Item","1baad1eb-abfd-4025-89ec-24bee467addc","D.5.1.6.7","","100mm 90 Degree side outlet ","No.",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G102 * H102,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","22f4d2e7-e0d9-4b9b-a7a6-169a18fa2137","D.5.1.7","","SOIL DRAINAGE ",{"$nulls":4},"Dflt"]
["Label","d082cfa0-cbbe-48ee-b738-eed878b5baa8","","","uPVC soil and vent pipes ",{"$nulls":4},"Dflt"]
["Item","e56797c8-7710-4b8c-bd16-f6b9edaf4d2b","D.5.1.7.1","","50mm Diameter uPVC pipes ","m",40,{"v":0,"d":"0.00"},{"$f":"ROUND(G105 * H105,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f058cc09-75e2-4605-8090-ff39dfb2b54e","D.5.1.7.2","","100mm Diameter uPVC pipes  ","m",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","3733bd80-af97-401e-830a-ffc32a4ad17a","","","Extra over uPVC for the following fittings  ",{"$nulls":4},"Dflt"]
["Item","32ecce5e-0c29-4597-907b-3588d7c9d2dd","D.5.1.7.3","","50mm Bend  ","No.",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G108 * H108,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f9eec732-d99f-4e34-a6f3-3a8eff71580b","D.5.1.7.4","","50mm Reducing Junction ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","27207a04-6d26-426a-a2d3-ee2821c0b7b2","D.5.1.7.5","","100mm dia Reducing Junction ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","630f5a21-81dc-4623-b779-d3735ab89dc7","D.5.1.7.6","","100mm Bend ","No.",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7230f358-a9e3-4372-a4fa-50d9dd37209e","D.5.1.7.7","","100mm Stubstack ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","82976f9f-83ba-43ce-90a8-200a45d27b19","D.5.1.7.8","","100mm Air vent cowl ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9a8e0b5b-8e46-4101-9ff8-18ede0a32ff3","D.5.1.7.9","","100mm Vent Cap ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","83db31c0-c5f5-49f8-a885-1c2350afe791","D.5.1.7.10","","100mm pan connector ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f74cc2b6-5306-4431-b5b6-643b536e1fa9","D.5.1.7.11","","Rodding Eye ","No.",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","abfd3811-c334-42d7-9be0-e3432f1901e4","","","Testing ",{"$nulls":4},"Dflt"]
["Sum","715e31ce-47e3-4f0f-acf8-b03e6924b409","D.5.1.7.12","","Testing soil drainage system ","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H118,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","f7b531f5-e1a9-429c-af24-653363a17f4d","D.5.1.8","","WATER SUPPLIES  ",{"$nulls":4},"Dflt"]
["Label","f5dd6679-0de5-43c5-9f00-55fb5fe93436","","","Copper pipes to SABS 460/0 fixed to walls, ceilings, drywall cavities, etc ",{"$nulls":4},"Dflt"]
["Item","25b7421e-21e5-41f7-a812-908133e9abe1","D.5.1.8.1","","15mm Pipes ","m",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G121 * H121,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e83e190c-80bd-47e1-b0c1-3d432a68da93","D.5.1.8.2","","20mm Pipes ","m",50,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8982f088-b1c2-40fd-b279-6f2200651317","D.5.1.8.3","","22mm Pipes ","m",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e1a7fd89-1e5e-4439-a01b-2208ea820d23","D.5.1.8.4","","35mm Pipes ","m",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","83f824cb-d354-4e54-9c97-8a7121fa9677","","","Extra over piping for \"Copcal\" soldered fittings ",{"$nulls":4},"Dflt"]
["Item","c9bccd22-aa04-424c-aa78-290431a41a0b","D.5.1.8.5","","15mm Fittings ","No.",46,{"v":0,"d":"0.00"},{"$f":"ROUND(G126 * H126,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","b142b2cf-b17b-4f73-a908-b0812514de6a","D.5.1.8.6","","15mm Reducer ","No.",12,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7d9c80ea-9ec5-4cff-a9cf-58effe2cba80","D.5.1.8.7","","20mm Fittings ","No.",44,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4780948f-34ac-4707-ad49-b6b9002d315f","D.5.1.8.8","","20mm Reducer ","No.",17,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","06adf1be-6ab8-42f5-a0fd-fd058a239344","D.5.1.8.9","","28mm Fittings ","No.",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","899435f2-f582-4efd-ab7b-f71c3d552fbc","D.5.1.8.10","","35mm Fittings ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","990976bc-67af-4067-ad19-13abcaae1ef7","D.5.1.8.11","","35mm Reducer ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1ac09070-c0e8-4ebb-8294-2650e5bec8e2","","","TESTING ",{"$nulls":4},"Dflt"]
["Sum","57a371bb-33ab-4b81-95a7-b2972e8fa064","D.5.1.8.12","","Testing water pipe system ","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H134,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","bd522c22-68ac-47ca-bc09-8bdc264ce458","D.5.1.9","","SANITARY FITTINGS  ",{"$nulls":4},"Dflt"]
["Label","9014211c-7941-47b3-b21c-3cf416715501","","","Supply and fix the following sanitary fittings including assembly forming all joints and connections, bedding, pointing, building in, cutting and pinning, plugging and screwing and making good as necessary  ",{"$nulls":4},"Dflt"]
["Label","6ae3a3e3-77fb-4614-b6dc-f489653a1c8a","","","\"Franke\" or equally approved ",{"$nulls":4},"Dflt"]
["Label","ff9ac412-f579-49dd-ac33-ba6eb2a8db0f","","","Male and Female Ablutions",{"$nulls":4},"Dflt"]
["Label","2a8d650e-f690-46f4-96d3-488961d0f676","","","Hand wash basin ",{"$nulls":4},"Dflt"]
["Item","0ac9ac64-1f3a-499c-89a8-bd602a29ba1c","D.5.1.9.1","","15mm chrome plated Gala single lever sink mixer with aerated swivel outlet (Code:GA-670; white; size - 570mmx455mm)","No",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G140 * H140,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","94bc676b-405b-4f52-b1da-b509b5d248d1","D.5.1.9.2","","Basin Mixer: Cobra Watertech Callisto single tap hole mixer with pop-up waste, mounting kit, angle valves with sliding flanges (Code:CL-950)","No",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","60344406-336b-43ea-b565-4957e724043b","D.5.1.9.3","","Wall Hung WC Pan: Vaal Entice 90% outlet back inlet closed rim wall hung pan REF:439600WH with soft close seat; Vitreous China, White","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a1d7e15a-6fef-4d72-8927-c8d80fcde822","D.5.1.9.4","","Geberit Kombifix concealed cistern with front actuated with Tango single flush/stop actuator in white alpin finish, including flush pipe and pan connector, water supply connection with angle stop valve, protection cover for service opening and protection cover for flush pipe, fixed with included fastening materials inside solid wall from 120mm up to 200mm.  WC fixed 450mm from finished floor level.  All with Geberit conditional guarantee.  ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ac89214f-f3e2-4257-beac-d8f8c661b178","D.5.1.9.5","","WC Pan Actuator -  Geberit Tango single flush with flush/stop actuator ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","4c231867-304e-4911-b559-87929480c2e7","D.5.1.9.6","","Wall Hung Bowl Urinal - Vaal Sanitaryware Sweetpea Urinal - 565x275x310mm white vitreous China wall mounted top inlet urinal (Code:705126) including 38mm chromium plated domical grating (code:8787Z0) and chromium plated top inlet spreade (Code:7054Z0).","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","2b0a32a0-6644-43c9-af3f-07dfd837c406","D.5.1.9.7","","Hanger Bracket- Fixed to wall with bracket and sealed with mildew resistant silicone sealant where urinal meets wall. ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f350b9d4-640b-422e-8f10-ca844f08f7be","D.5.1.9.8","","Cobra Watertech exposed urinal chrome plated junior.  Flushmaster flushvalve (code:FJ6-000) with non-hold open feature, wall flange and 20mm \"Ball-o-Stop\" control inlet.  ","No",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","81198445-cebd-4dcd-b03f-8a8b6740d28c","","","Disabled Bathroom ",{"$nulls":4},"Dflt"]
["Item","3bfb30f6-28d4-4ac7-8651-cbe3f3d9faaa","D.5.1.9.9","","Pillar sink mixer - Cobra Watertech Medical Elbow Action - Ref:505-21B pillar tap with blue indice. 1/4 inch turn ceramic disc and flanged back nut;  Chromium Plated; Cobra Watertech (Pty) Ltd","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G149 * H149,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","457331f7-d3ce-4ffb-869e-d7776123dd13","D.5.1.9.10","","Flush Valve Grab Rail - Standard grab rails for disabled WC by Chairman industries, 750mm SR2 for back rail.  ","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","0d4dab72-69f8-4a17-9643-a5551a5208b7","D.5.1.9.11","","Cistern back Rail - Standard grab rails for disabled WC by Chairman industries, 750mm SR2A for Cistern back rail. ","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c46df025-991c-4738-a04c-b836c78c20d3","D.5.1.9.12","","Dogleg side rail - Standard grab rails for disabled WC by Chairman industries, 750mm DL2 dog-leg side rail.  ","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","c99a5af4-3aff-4b1c-bb7e-d86077fa4113","","","Staff Kitchen ",{"$nulls":4},"Dflt"]
["Item","ad8140ca-ba73-4916-bad4-f829cdbe472d","D.5.1.9.13","","Kitchen Sink - S1 Franke - Quinline QLX/QLL 611","No ",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G154 * H154,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","59ca8d73-8acc-4b02-a599-31ae877ca39e","D.5.1.9.14","","Sink Mixer - Cobra Watertech Noka 15mm chrome plated deck mounted sink mixer with overarm swivel outlet and adjustable flanges (Code:NA-970) manu","No ",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","433170ec-3aab-4278-9162-7154de6b1544","","","Staff Showers",{"$nulls":4},"Dflt"]
["Item","a1b8818d-eefe-4813-b360-1dfd34377d6e","D.5.1.9.15","","Staff Mixer - Cobra Watertech Gal 15mm chrome plated single lever undertile bath/shower mixer with classic handle (Code: GA-656), sliding wall flange and stepped blanking plug, manufactured in accordance with SANS 1480:2005 (BS EN 1286).","No",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G157 * H157,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","508f8bb0-8bcf-48fe-a096-2b5f77cbaa38","D.5.1.9.16","","Shower Rose - Cobra Watertech chrome plated Relaxa Plus shower head (Code:28274) with five spray patterns, ball-jointed connector and anti-lime nipples. ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","334439e9-049d-4c0d-8b98-d4ae00ffabf3","","","Disabled Shower Area",{"$nulls":4},"Dflt"]
["Item","ad89a904-197b-4e65-a8a2-ceeff3b6d6dd","D.5.1.9.17","","Shower Rail - Cobra Watertech 600mm long Classic shower rail (Code:007-MSR/CP) with sliding handshower holder. ","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G160 * H160,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e83a864e-a39a-4d70-aee8-d7efb1e7e848","D.5.1.9.18","","Shower Rose  Cobra Watertech 110mm diameter Circa handshower (Code:007CI/CP) with 3 spray functions and anti-lime nipples. ","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b068e4ce-3578-4293-9217-daeef3e9b652","D.5.1.9.19","","Shower Mixer - Cobra Watertech Gala 15mm chrome plated single lever undertile batch/shower mixer with classic handle (Code:GA-656), sliding wall flange and stepped blanking plug, manufactured in accordance with SANS 1480-2005 (BS EN 1286)","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","72b4ed94-595d-4dc5-bc24-7b6a8b152d85","D.5.1.9.20","","Hinged Bench/Fold up shower seat - Ref XS ","No",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","20e82686-2cdd-451d-b233-c0fb4efe81a5","","","Fittings ",{"$nulls":4},"Dflt"]
["Label","c4d359db-9a4a-4512-9a17-e0d59bb085ae","","","Note: samples to be provided for approval prior to ordering ",{"$nulls":4},"Dflt"]
["Item","825fcd4a-3e77-434a-a0a0-ac426b57195b","D.5.1.9.21","","Hand Dryer -  Frankie HF2400 HD, 12/1.5mm thick satin finished stainless steel automatic hands free hand dryer (Code:359961), size 280 x 207 x 245mm high with 2 vandal proof lock screws and key wrench, plugged and screwed to the wall with stainless steel screws, 200W motor connected to 230/240 volt power supply, with 5 year warranty","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G166 * H166,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","3c874b87-05ee-44e1-b678-f93ee85a0011","D.5.1.9.22","","Toilet Paper Dispenser - Franke Stratos STRX672 1,2/1.5mm thick satin finished stainless steel double toilet roll dispenser (Code:359716), size 156 x 141 x 303mm high for 2 rolls maximum 108mm diameter with spindle system and cylinder lock with satandard Franke key, plugged and screwed to the wall with stainless steel screws.  ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","dfb0f179-d536-40ac-af4e-c040a54c358e","D.5.1.9.23","","Paper tower dispenser and bin -  Franke Stratos STRX 601 1, 2/1.5mm thick satin finished stainless steel paper towel and soad dispenser combination","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","b6e9c0ec-1a30-4b48-8663-bce9206e73d8","D.5.1.9.24","","Soap Dispenser - Franke Stratos STRX618 1,2/1.5mm thick satin finished stainless steel soad dispenser (Code:359705), size 100 x 134 x 304mm high with a replaceable and refillable 1 litre container, cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws. ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","ade36355-1dc8-4b54-a9f4-2cacba582b86","D.5.1.9.25","","Toilet paper dispenser - Franke Stratos STRX672 1,2/1.5mm thick satin finished stainless steel double toilet roll dispenser (Code:359716), size 156x141x303mm high for 2 rolls maximum 108mm diameter with spindle system and cylinder lock with standard Franke key, plugged and screwed to the wall with stainless steel screws ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","87ded5b9-a979-47aa-8545-c9f91a609361","D.5.1.9.26","","Paper towel dispenser and bin - Franke Stratos STRX 601 1,2/1.5mm thick satin finished stainless steel paper towel and soap dispenser combination (Code:359770), size 396x134x305mm high with a capacity of 300-400 towels, replace able and refillable 1 litre container and cylinder lock with standard Frankey key, container and cylinder lock with standard Franke key, plugged and screwwed to the wall with stainless steel screws.  ","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3f50cbf9-d379-4719-ab6a-c7e7a0f4eab4","D.5.1.9.27","","Soap Holder - Franke BHM6P polished stainless steel double arm double arm soap rack (Code:359944), size 163x100mm deep, plugged and screwed to the wall with stainless steel screws. ","No",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","084cd971-bf44-41aa-90da-c10229086b84","D.5.1.9.28","","Sanitary Bin - Waste bin with hygiene bag dispenser for wall mounting, stainless steel, surface satin finished, front with Inox Plus surface refinement for the reduction of finger marks and better cleaning characteristis (easy to clean), material thickness 1.5mm, curved front cover, approx. 3.8 litre capacity, folding self-closing lid wth piano hinge, removable plastic container inside, incl, stainless steel screws and dowel.  Code STRX614","No",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d0bda766-7037-494e-9cf7-cd44a1919dfe","D.5.1.9.29","","32mm Diameter chromium plated curtain or hanging rail 800mm long including flanged end brackets ","No",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","118a8e33-66ff-49b5-845e-4c21bc5613fc","D.5.1.9.30","","Steel Lockers - Type GB002 - 1800mm highx 300 width x 450mm depth. Lock type - Cam - 1 way","No",12,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","f5cc9d26-c631-401f-84c9-89f83ba0197a","D.5.1.9.31","","Supply and Install Bench complete with the following: Wrought Hardwood slated seating of 32x90mm chamfered slats at 100mm centres, screwed through 40x40x2mm tubular section triangular steel framework.  Steel framework to be bolted to wall with two R16 Rawl - bolts.  Steel framework to be painted with one coat primer in accordance with SABS Specificaion 1219, one undercoat in accordance with SABS Specification 681, Type II and two coats gloss enamel paint in accordance with SABS Specification 630.  Slatted seating to be stopped with Tinted stopping, sanded down and applied with three coats eggshell varnish to SABS 887, Type 1","No",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","7b7f8fcd-40bc-43cf-82fa-e9b71673a134","","","TAPS, VALVES, ETC ",{"$nulls":4},"Dflt"]
["Label","6f22e11f-2524-4e67-9b3b-e45f4fc20e9d","","","\"Cobra Watertech\" or equally approved ",{"$nulls":4},"Dflt"]
["Label","71604a35-ba86-43e6-927e-c49d2fca5e62","","","Valves ",{"$nulls":4},"Dflt"]
["Item","7ea51f40-30d9-40dd-8d64-203a7acd84c3","D.5.1.9.32","","20mm Isolating Valve ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G180 * H180,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e7818572-dfef-44a9-961c-37a036c8918d","D.5.1.9.33","","32mm Isolating Valve ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","43de5df2-bf4d-4df0-9bd8-6557f17ff021","D.5.1.9.34","","40mm Pressure Release Valve ","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1c9799e5-1aa5-4236-9c80-dd43422bc8dd","D.5.1.9.35","","FM2.100CP \"Flushmaster\" toilet flush valve ","No.",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","19f5f7ed-4bd9-465a-9acb-cebda53dedc2","","","\"Cobra Watertech\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","65d1b8df-21fd-4ca3-98ae-0889bd51d621","D.5.1.9.36","","Cobra Watertech 32mm chrome plated slotted basin waste union (Code: 301-32) install chain and plug to suit ","No.",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G185 * H185,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","d7fca770-062b-43d1-aea6-b51f4a0b7ed1","D.5.1.9.37","","75mm chrome plated shower grating (Code: C-373/1). ","No.",8,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","124f33b0-3515-467d-8ca5-e06783da96ce","","","TRAPS ETC ",{"$nulls":4},"Dflt"]
["Label","b65cf05b-5392-4f66-9837-1f90f5544185","","","\"Cobra Watertech\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","886dd300-c810-4b87-a4d3-f2b238e9578e","D.5.1.9.38","","32mm chrome plated deep seal bottle trap with outlet for 50mm PVC (Code: 345/50). ","No.",9,{"v":0,"d":"0.00"},{"$f":"ROUND(G189 * H189,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","319bcdf7-7a40-4b99-9e04-5d280d94876e","","","uPVC ",{"$nulls":4},"Dflt"]
["Item","633f5ae7-527b-42e2-a53a-901a3df87b76","D.5.1.9.39","","50mm \"P\" trap ","No.",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G191 * H191,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","558b2a26-97b7-4b1f-afda-6216c5581591","","","HOT WATER CYLINDERS ",{"$nulls":4},"Dflt"]
["Label","11c529e2-c017-4bb1-b526-a4d9f8242db0","","","\"Kwikot\" or equally approved ",{"$nulls":4},"Dflt"]
["Item","735c4877-1386-445c-91d1-c6c4efacead5","D.5.1.9.40","","Kwikot 600i Dual 150 litre capacity \"Slimline\" vertically mounted 600Kpa (Code: ESG-150-I). Water heater complete with standard driptray bottom outlet space vacuum breaker, safe valve, pressure reducing valve and stoptap. Position of units in roof space as shown on plan. ","No.",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G194 * H194,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","c9aa829b-8eef-4375-95a2-495399d43ac0","D.5.1.10","","GLAZING ",{"$nulls":4},"Dflt"]
["Label","3174e805-1ebc-4b49-8a02-f6162e0a4f9f","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","1b8a2e12-6b00-4052-bafe-6b36aaa57ff5","","","TOPS, SHELVES, DOORS, MIRRORS, ETC ",{"$nulls":4},"Dflt"]
["Label","4ea4ec37-555f-4775-877e-848a28a313cc","","","6mm Silvered float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers and sealed to tiles with clear silicone sealant ",{"$nulls":4},"Dflt"]
["Item","7c5c4826-b28a-4449-8da4-f52de1ae344c","D.5.1.10.1","","Mirror sizes 600 x 985mm high ","No.",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G199 * H199,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","451d007d-7629-4b51-9f6f-389c34fbebe8","D.5.1.11","","PAINTWORK",{"$nulls":4},"Dflt"]
["Label","1a36fd3a-e9ac-447a-bf06-9b2ab0afc861","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","201d9085-bd93-44d9-a6f5-463fa5eacdae","","","SUPPLEMENTARY PREAMBLES ",{"$nulls":4},"Dflt"]
["Label","c1b879cd-52ca-4c57-9c1d-182839f48fae","","","All colours to be selected by the Architect ",{"$nulls":4},"Dflt"]
["Label","6889efca-ec80-4fe9-846a-282d69951322","","","Only approved brands of paint shall be permitted ",{"$nulls":4},"Dflt"]
["Label","da95d441-1d1d-491c-a243-dc9ad8528642","","","All painting measured generally will be in colours with a value of more than 7 on the Munsell system in accordance with the relevant SABS specification. Any painting in colours with a value of 7 or less on the Munsell system shall be given as paintwork in darker colours ",{"$nulls":4},"Dflt"]
["Label","e9918caa-f47a-4706-94cd-5e1744efc6e5","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","4906e628-5d55-4947-b22a-df1f78e8e446","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, Prime with one coat of plaster primer all in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","05b2f060-6b27-4172-ae93-aba24331bfde","D.5.1.11.1","","Walls ","m²",1014,{"v":0,"d":"0.00"},{"$f":"ROUND(G208 * H208,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","b42ea51c-d5c8-4a84-b4e9-03ada1d67988","","","ON INTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","1c4f2e0b-1065-48fb-8242-9e987303bb5f","","","Clean off dust, remove loose paint, fix cracks with polyfilla or similar approved product, finish with 2 coats of super acrylic PVA paint or similar approved. All in accordance with Manufacturer's detailed specification and recommendation ",{"$nulls":4},"Dflt"]
["Item","1bc2d08a-acbd-43c9-8eb0-db64cfe4a55c","D.5.1.11.2","","Walls ","m²",1014,{"v":0,"d":"0.00"},{"$f":"ROUND(G211 * H211,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","bd5123b3-19b0-4640-8788-d52099f8c327","","","ON EXTERNAL FLOATED PLASTER SURFACES ",{"$nulls":4},"Dflt"]
["Label","5df61f45-5bb7-4861-a578-b85fc7557193","","","Primer and finish with two coats \"Marmoran Armourbrush\" or equally approved, applied in strict accordance to manufacturer's instructions. ",{"$nulls":4},"Dflt"]
["Item","dc12a779-4a0d-42a2-88d3-70a941b88935","D.5.1.11.3","","On walls  / RC Beam","m²",95,{"v":0,"d":"0.00"},{"$f":"ROUND(G214 * H214,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","2f838dcf-1845-44cb-8921-13b05454a9f0","","","TO SOFFITS OF CONCRETE SLABS ",{"$nulls":4},"Dflt"]
["Label","03d3ff86-99ec-446a-a693-33322a2b529b","","","One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior  ",{"$nulls":4},"Dflt"]
["Item","1b995e92-a56a-444f-8bcd-74f032b58a35","D.5.1.11.4","","To concrete soffits of slabs ","m²",30,{"v":0,"d":"0.00"},{"$f":"ROUND(G217 * H217,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ceda19d5-ee91-4500-957f-e435bd702dff","D.5.1.11.5","","On Window Cills and Reveals, Clean off dust from the previously painted areas; remove the loose paint, fix cracks with rhynolite or similar approved product","m²",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","07149a91-2897-4ffe-a429-afb5e7af69b8","","","ON PLASTERBOARD SURFACES ",{"$nulls":4},"Dflt"]
["Label","d76a4ffb-935d-4364-bc50-e7cc8eaa78c4","","","One coat alkali resistant primer and two coats PVA emulsion paint for interior use ",{"$nulls":4},"Dflt"]
["Item","07f5d7a3-a6ea-4496-a3c0-98a296bdf7b4","D.5.1.11.6","","Ceilings and cornices  ","m²",345,{"v":0,"d":"0.00"},{"$f":"ROUND(G221 * H221,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","f2a9c168-7f36-4ab0-bf0b-731ce42c8d75","","","ON METAL SURFACES ",{"$nulls":4},"Dflt"]
["Label","384e0338-98d8-4d4e-b8f5-e5e7661e2d4f","","","One coat \"Namelcote\" zinc chromate primer UC 53, one coat \"Plascon Galvogrip\" metal primer and two coats \"Velvaglo\" polyutherane enamel paint (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","0c4d6f1d-2b1e-4da8-965e-8b29a92fbf11","D.5.1.11.7","","On door frames etc ","m²",40,{"v":0,"d":"0.00"},{"$f":"ROUND(G224 * H224,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","65b6354d-e475-459d-8913-f755f21b1b4b","","","ON WOOD SURFACES ",{"$nulls":4},"Dflt"]
["Label","db527911-b838-4914-9844-8a31257fe43e","","","One coat \"Spick and Span\" Oil based wood primer (UCS2), two coats \"Velvago Polyurethane enamel paint (VLO). (Colour by Architect). All in accordance with Manufacturer's detailed specification and recommendation) ",{"$nulls":4},"Dflt"]
["Item","deef278f-1f93-4b2d-ae67-feebd5dae518","D.5.1.11.8","","On doors  (both sides)","No.",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G227 * H227,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","7750904e-8f0d-4f8d-8cba-bc6bbff30d46","D.5.1.12","","PLASTERING ",{"$nulls":4},"Dflt"]
["Label","138f2491-ed8d-4529-a6b4-f23775433b02","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","fe41bb54-264e-4750-8230-2f8a195d274d","","","SCREEDS  ",{"$nulls":4},"Dflt"]
["Label","442aac88-9bea-4c23-ae9e-da48b94c8e38","","","1:3 Cement screeds wood floated, on concrete ",{"$nulls":4},"Dflt"]
["Item","6fa3c70a-cbd0-4108-98cf-c6759198fadd","D.5.1.12.1","","Average 50mm thick on floors to falls and crossfalls ","m²",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G232 * H232,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","13870015-896c-42f6-93ae-d7aabac54fda","","","INTERNAL PLASTER  ",{"$nulls":4},"Dflt"]
["Label","a3baf378-7adc-49ba-ab7b-2020a31a3f55","","","Gypsum skim plaster",{"$nulls":4},"Dflt"]
["Item","3c0b64fc-8486-40d5-b23b-486a85bb098c","D.5.1.12.2","","On ceilings ","m²",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G235 * H235,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","c1501363-a700-4b52-ace0-8788d67e8884","","","PLASTER ",{"$nulls":4},"Dflt"]
["Label","e2203855-0002-4abb-8219-86eaede28c8b","","","One coat 1:5 cement plaster 12mm thick on brickwork or concrete finished with a wood trowel ",{"$nulls":4},"Dflt"]
["Item","a03393bd-46a9-4f92-a712-766cfe923a36","D.5.1.12.3","","Exterior Concrete beams ","m²",5,{"v":0,"d":"0.00"},{"$f":"ROUND(G238 * H238,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","52eaed19-4211-4170-8d08-7bd0f7019624","D.5.1.12.4","","Interior Walls ","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1834e28c-6f28-46ab-bdc3-442960da9d8d","D.5.1.12.5","","Concrete Repair - chip off honey combs on concrete or defects and patch with proprietary epoxy or equivalent approved product","m²",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","07593ec1-db07-4ff5-863a-05e6eff65156","","","For preambles see \"Model Preambles for Trades\"",{"$nulls":4},"Dflt"]
["Label","4337ab3b-39be-4d8d-a4bb-4cfc368f75bf","","","\"Note: All tiling shall be fixed to plaster or screed with an approved adhesive; the adhesive shall be as recommended by the manufacturer of the tiles. \"",{"$nulls":4},"Dflt"]
["Header2","c2b38709-2135-4363-8a30-effbfa562742","D.5.1.13","","TILING  ",{"$nulls":4},"Dflt"]
["Label","6e609a25-1c12-402c-9a21-f447e834563f","","","WALL TILING  ",{"$nulls":4},"Dflt"]
["Label","29d97fb7-f7a6-47ca-be9b-f0fb2850c9e7","","","200 x 200 x 6mm white glazed ceramic tiles fixed with adhesive to plaster (plaster elsewhere measured) and Dove Grey flush pointed with epoxy grout ",{"$nulls":4},"Dflt"]
["Item","31aa8167-a630-4409-8870-f76fb673899e","D.5.1.13.1","","On walls ","m²",35,{"v":0,"d":"0.00"},{"$f":"ROUND(G246 * H246,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","f49a189c-1e1a-4c87-9aea-0a5335fbf58b","D.5.1.13.2","","On walls in isolated panels, splashbacks, etc ","m²",72,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","a49a7b8d-bfca-41d9-a3e4-3c44dd7952e1","D.5.1.13.3","","On narrow widths ","m²",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","62ecbf75-3e86-456f-9b24-64b002365ce2","D.5.1.13.4","","Attic stock ","m²",41,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d372ed95-4a7e-4b43-a507-9efb18e0304f","","","FLOOR TILING ",{"$nulls":4},"Dflt"]
["Label","186add07-e2e3-41ca-8616-1ef103a0069a","","","200 x 200mm porcelain floor tiles fixed with adhesive to screed (screed elsewhere) and flush pointed with waterproof grout ",{"$nulls":4},"Dflt"]
["Item","df3bf5d3-248a-4a8f-b712-863bfbb204ac","D.5.1.13.5","","On shower floors ","m²",8,{"v":0,"d":"0.00"},{"$f":"ROUND(G252 * H252,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","ae587a54-4388-4a30-8d7d-248eb7be3ac2","D.5.1.13.6","","Attic Stock ","m²",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d80c68eb-3d57-4483-8e69-73d20a704fbe","","","600 x 600mm or equally approved porcelain tiles  (PC Amount R 200/m2) fixed with adhesive on screed (elsewhere measured) and flush pointed with epoxy grout tile joint filler. ",{"$nulls":4},"Dflt"]
["Item","c3d415dd-ec3e-47c8-95cd-6255a263e0ad","D.5.1.13.7","","On floors and landings ","m²",25,{"v":0,"d":"0.00"},{"$f":"ROUND(G255 * H255,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","8b445d9e-6247-478f-a5c1-daef414d145a","D.5.1.13.8","","Skirting 75mm high (of cut tiles 600 x 600mm) ","m",20,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","04e6506a-e59e-4bcc-8605-14dd507f869c","D.5.1.13.9","","Attic stock ","m²",39,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","fd3bb140-40ba-469f-954b-89e4b57822b1","D.5.1.14","","CARPETS, VINYL & SKIRTINGS",{"$nulls":4},"Dflt"]
["Label","bf8ce99b-4bc6-4686-9ca9-5216a3247ff7","","","Factory fitted \"Van Dyck Latitude Earth Enduroback\" carpet tiles, colour Pirate Heavy commercial (SABS use class U5) all in accordance with interior finishing schedule Dwg. No. 010-403J:",{"$nulls":4},"Dflt"]
["Item","75a4d720-b15f-4b29-a096-431dfd03f989","D.5.1.14.1","","On floors","m²",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G260 * H260,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6bd6133d-c8eb-42a9-99a0-ae22d252fbb6","","","76 x 19mm Meranti hollow backed skirting with rounded top edge nailed to brick walls and screwed to wall partitions and with 25mm Meranti quadrant. To be primed with suitable wood primer and finished with two coats matt enamel.",{"$nulls":4},"Dflt"]
["Item","d1e119d9-f58e-4da5-9c29-795205821400","D.5.1.14.2","","Skirtings","m",102,{"v":0,"d":"0.00"},{"$f":"ROUND(G262 * H262,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","bf0bc531-3bf9-45de-82ef-cff13ba42d85","D.5.1.15","","JOINT SEALERS, ETC ",{"$nulls":4},"Dflt"]
["Label","27e06c5d-228c-4183-9336-63e5ea6314a0","","","Approved polyurethane joint sealant dressed into joint including protecting adjoining surfaces with masking tape ",{"$nulls":4},"Dflt"]
["Item","21c936f3-7dba-4fed-94db-7e1e5488b705","D.5.1.15.1","","10 x 10mm Sealer in tile joint between floor and wall tiles ","m",31,{"v":0,"d":"0.00"},{"$f":"ROUND(G265 * H265,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","ad68485b-9608-4231-8c94-c9f590d43a48","D.5.1.16","","INTERIOR DOORS (Refer Door Schedule Architectural Drawing No. J40073/010-402F/Rev 2",{"$nulls":4},"Dflt"]
["Label","efa28179-01d2-42ee-aa53-ee7eb60b3445","","","Install 40mm thick semi solid hardwood doors with 3.2mm tempered hardboard facings, and two hardwood edge strips, 1.2mm rebated closing stiles (SABS 545) complete with Ironmongery (NB Only Frames already installed)",{"$nulls":4},"Dflt"]
["Item","597e0c0c-adac-4a0e-981e-768f8f4208e2","D.5.1.16.1","","Door No. D1 at Female and Male Change Rooms","No. ",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G268 * H268,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","50d6cf0b-5325-4701-86d1-77b0831ce763","D.5.1.16.2","","Door No. D3 at Shower/WC Disabled for Disabled","No. ",2,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","93162f59-221b-4d79-b892-f57a6e67fc87","D.5.1.16.3","","Door No. D6 at Male and Female Shower rooms","No. ",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","61d77751-52cd-41f9-8af0-a567b315d396","D.5.1.16.4","","Door No. D5 at DB, Telkom, FHR, Cleaner and Store Rooms","No. ",4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","4ee085c8-5556-4ce2-a004-83c89d8b5496","","","Shower Cubicles - supply and install frame, door, ironmongery and glazing ",{"$nulls":4},"Dflt"]
["Item","1ec06bf4-b4a5-4573-93ce-ef629538d320","D.5.1.16.5","","Install Aluminium Frame Shopfront, purpose made to dimenstions of Door No. D6.  All aluminium sections to be equal quality and must comply to AAAMSA Specifications and KAL Manufacturing Specifications.  AAAMSA approved Aluminium framed doors with powder coat finish to SABS 999-1986.  Colour: available to architect on request","No. ",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G273 * H273,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","1b5d9ffc-edc0-4da3-b90e-512bc7dbdfb4","D.5.1.17","","EXTERIOR ENTRANCE DOORS",{"$nulls":4},"Dflt"]
["Label","6b07ce7a-4385-4963-adaa-96f92cf3564f","","","Board Room Door SF3",{"$nulls":4},"Dflt"]
["Sum","ef7f897a-4548-42dd-9f26-ea0e4c53f41d","D.5.1.17.1","","Reinstall the door to fit and leave no gap underneath and above the door.","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H276,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","69f3ad73-0f07-4bfe-85d4-c5b7291c8862","","","Foyer/Lobby Doors SF2",{"$nulls":4},"Dflt"]
["Sum","8abd28cb-982a-4282-bced-1ecef4bfe3bd","D.5.1.17.2","","Remove door, break concrete anchoring the door fixing mechanism and reinstall the door or competent concrete in accordance with supplier's details","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H278,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Sum","b50c2247-feb1-4de6-867c-51b655e3d609","D.5.1.17.3","","Supply and Install all complete fire and signage plan in accordance with the Drawing No. J40073/010 - 402U / Rev 1","Sum",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","3483a52a-c8ed-48bb-9d52-5d3e0148da9e","D.5.1.18","","PROVISIONAL SUMS ",{"$nulls":4},"Dflt"]
["Label","d978a735-4b79-4570-8711-b38f0f001d9a","","","For preambles see \"Model Preambles for Trades\""]
["Label","01d4262a-0290-452e-a6d8-45400e7cf713","","","BUDGETARY ALLOWANCES (Completing the Electrical Work and connection, Water Connection, etc)"]
["Item","754f9b4c-eafa-4d7f-85c1-f2ab3310a660","D.5.1.18.1","","Provide for Provisional Sum of R500,000.00 Additional Work as instructed by Engineer","Prov.Sum",1,{"v":500000,"d":"500,000.00"},{"$f":"ROUND(G283 * H283,2)","v":{"v":500000,"d":"500,000.00"}}]
["% Previous","5b07b74c-790a-40a4-ac63-750c6f16ecc9","D.5.1.18.2","","Add for profit and general attendance upon above if required  ","%",{"$f":"I283","v":{"v":500000,"d":"500 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Label","512144cb-8079-4763-83f8-b28bdcf1ea32","","","Corrective work to structure/building"]
["Sum","dee66b9a-9fd2-44b9-8ec9-54fb38dad8fd","D.5.1.18.3","","Corrective works as directed by the Specialist investigations/tests conducted by the Contractor","PSum",1,{"v":350000,"d":"350,000.00"},{"$f":"ROUND(H286,2)","v":{"v":350000,"d":"350,000.00"}}]

{"sheet":"BILL D.6.","index":15,"n_rows":38,"n_cols":10,"rows_kept":38,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.6.",null,"FeCL BUILDING",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","3ef7f517-691b-47bd-a936-e96d17e3560e","D.6.1","","FeCL BUILDING",{"$nulls":4},"Dflt"]
["Label","9478d8c8-8b23-4418-b974-de977640df82","","JBCC","SECTION D.6.1 : FeCL BUILDING",{"$nulls":4},"Dflt"]
["Header2","1df8be04-03d2-4005-9a4c-4bca9f4fff37","D.6.1.1","SANS1200 DA","Earthworks",{"$nulls":4},"Dflt"]
["Item","31a9241e-c77f-41c7-b9b6-760bc3b30bd3","D.6.1.1.1","8.3.1 b)","Excavate in all materials and dispose to designated area","m³",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","bae30df3-59d8-4f5e-905c-a5b0e6d2e706","D.6.1.1.2","8.3.1 c)","1) Extra over for intermediate excavation ","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","44c0a8f7-110b-4e54-b2f0-d56b5b8202eb","D.6.1.1.3","","2) Extra over for hard rock excavation ","m³",3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","28ecd16c-36e7-4a5a-80e4-42f0a3a2c671","","","FILLING, ETC",{"$nulls":4},"Dflt"]
["Label","f9fdaf3e-488b-4cb2-9411-64b9765d09fc","","","Backfilling with imported G7 material spread in layers not exceeding 150mm thick under floors, etc and compacted to 97% Mod. AASHTO density",{"$nulls":4},"Dflt"]
["Item","55f4520a-6c01-4722-8406-b0a3e1fe80e1","D.6.1.1.4","","Under floors, steps, paving, etc.","m³",10,{"v":0,"d":"0.00"},{"$f":"ROUND(G17 * H17,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","29595030-2775-48a3-9d6d-68caea459d61","D.6.1.1.5","","Backfilling with soilcrete (G7 and 2% cement by volume) to underside of blinding concrete","m³",10,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","c8bfc202-8979-4e55-9940-73161357824c","D.6.1.2","","Concrete Works (Apron, Steps, Plinth and Wall)",{"$nulls":4},"Dflt"]
["Label","0ec802c1-1013-4272-b58b-4c1d0891f0c6","","SANS1200 GA","Concrete (Small Works) - Formwork",{"$nulls":4},"Dflt"]
["Item","30a40068-420e-4125-930d-8fdfe8d8c19d","D.6.1.2.1","8.2.1","Formwork - Rough Finish surface","m²",143.6,{"v":0,"d":"0.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","fe0fc13b-f047-4093-a4a8-b7bacdd4908e","D.6.1.2.2","8.2.2","Formwork - Smooth Finish surface","m²",23,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","80bea182-0acb-4baf-ad24-d90addbcc725","","SANS1200 GA","Concrete (Small Works) - Steel",{"$nulls":4},"Dflt"]
["Item","60aab3fc-0224-4613-8ba3-aca61a89fa8c","D.6.1.2.3","8.3.1","Mild tensile steel ","kg",0.2,{"v":0,"d":"0.00"},{"$f":"ROUND(G24 * H24,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","bb1052d0-7beb-4ac3-b153-3538b2dd41d3","D.6.1.2.4","","High tensile steel ","kg",0.6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","03ce0c3e-7635-4195-bfb9-b745b61e0447","D.6.1.2.5","8.3.2","High Tensile Welded Mesh Ref 245","m²",88.35,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","d674b15b-f5ce-4d90-9431-769c884d1eb9","","SANS1200 GA","Concrete (Small Works) - Concrete",{"$nulls":4},"Dflt"]
["Item","f06d5bfe-57cd-4d21-bb87-a3a4d109a4a3","D.6.1.2.6","8.4.2","50mm thick Blinding Concrete (15Mpa,19mm aggregates)","m²",46.23,{"v":0,"d":"0.00"},{"$f":"ROUND(G28 * H28,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","2441f586-7c3b-427d-853b-3f3ecfa19022","D.6.1.2.7","8.4.3","20 Mpa, 19mm aggregates Concrete","m³",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","646581be-4f09-4cf0-86e0-68baaa6e5117","D.6.1.2.8","8.4.4","Unformed Wooden floated surface finish ","m²",87.4,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","32f87a45-bfa3-4b12-8fad-382629f97308","D.6.1.2.9","8.5.0","6mm x 30mm deep Saw cut joints from top of concrete","m",29,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","eefcacc7-95f3-415e-9357-a2a9be7041b7","D.6.1.2.10","","Install 10mm Jointex Expanded polystyrene","m",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","9ae9f2e7-c007-43dc-adcd-7c5953955a33","D.6.1.2.11","","Install 10mm x 10mm polysulphide ","m",30,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","9ac2e78e-bb2b-4e88-8de9-db920c93dfa8","D.6.1.2.12","","Supply and install  25mm HDPE Class 10 potable waterline ","m",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Item","1a3a40bf-cbbb-4893-b13c-7a7dfff8be84","D.6.1.2.13","","Supply and install 25mm heavy duty brass gate valve","No.",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["Header2","d7fd2abb-8cc1-40bd-9d3d-be7284473df8","D.6.1.3","","Supply and install 90 degrees elbow, one end 25mm diameter compression fitting, one end threaded"]
["Item","3bc8f9a7-636c-4b44-90e8-2c2cc6759109","D.6.1.3.1","","Allow R300,000.00 for Mechanical Works ","Prov.Sum",1,{"v":300000,"d":"300,000.00"},{"$f":"ROUND(G37 * H37,2)","v":{"v":300000,"d":"300,000.00"}}]
["% Previous","014c124e-113e-4333-b957-826f34122d68","D.6.1.3.2","","Add for profit and general attendance upon above if required  ","%",{"$f":"I37","v":{"v":300000,"d":"300 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]

{"sheet":"BILL D.7.","index":16,"n_rows":205,"n_cols":10,"rows_kept":205,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
["BillHeader",null,"BILL D.7.",null,"WAS PUMP STATION",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","d6288a3f-c025-4bdd-9e1c-7fd5e3434ae8","D.7.1","","WAS PUMP STATION",{"$nulls":4},"Dflt"]
["Label","fbb3bdcc-7b89-4f0f-8766-e952d4b88182","","JBCC","SECTION D.7.1 : WAS PUMP STATION",{"$nulls":4},"Dflt"]
["Header2","4996f0d2-334b-4604-90b0-154e7352c967","D.7.1.1","JBCC","BILL No. 1 FOUNDATIONS (PROVISIONAL)",{"$nulls":4},"Dflt"]
["Header3","3b63187c-b31f-4c9a-b9bf-10c0d417a94e","D.7.1.1.1","","EARTHWORKS",{"$nulls":4},"Dflt"]
["Label","0d896ffe-8881-47b6-a295-c963837a318b","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","9e4f160c-2c04-4b99-bbb0-2b0d7c493ed7","","","Nature of ground",{"$nulls":4},"Dflt"]
["Label","afab73c5-616c-4450-a075-aa1971e9d94a","","","Use \"assumed to be\" if no trial holes, soils investigations, etc have been carried out - discuss with Engineer. Use \"Trial holes indicate that\" where the ground has been investigated by means of trial holes",{"$nulls":4},"Dflt"]
["Label","7bf02841-9264-48cb-994f-b88e5859557c","","","Nature of ground",{"$nulls":4},"Dflt"]
["Label","e61ece6a-3393-4bd9-96c4-c397984e9e12","","","A soils investigation has been carried out on site by the Engineer and the report is annexed to these bills of quantities. Descriptions of excavations shall be deemed to include all ground conditions classifiable as \"earth\" described in the above report a",{"$nulls":4},"Dflt"]
["Label","4554074a-05e8-4fa7-9215-8ebb54e13066","","","Carting away of excavated material",{"$nulls":4},"Dflt"]
["Label","3c3e10f2-5ea3-486d-86c2-d94c4547b938","","","Descriptions of carting away of excavated material shall be deemed to include loading excavated material onto trucks directly from the excavations or, alternatively, from stock piles situated on the building site",{"$nulls":4},"Dflt"]
["Label","cd7ca05d-50fe-491f-a880-cb9a0090f89b","","","Excavations, Filling, Etc.",{"$nulls":4},"Dflt"]
["Item","783d7b5e-a41e-41be-b578-005419563c36","D.7.1.1.1.1","","Excavate in earth for holes not exceeding 2000mm deep.","m³",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G21 * H21,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","4cd93b72-d019-4ef4-bd37-9746aa152c38","D.7.1.1.1.2","","Extra over excavations in earth to bases and trenches for excavation in soft rock.","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","e2ec5a13-294b-48e7-852e-63d53d71bc3c","D.7.1.1.1.3","","Extra over all excavations for carting away surplus excavated material.","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","1c21ac81-a80b-4774-9a70-0ddfb9131391","D.7.1.1.1.4","","Allow for risk of collapse to sides of trench and base excavations not exceeding 1500mm deep.","m²",5,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","8df17cb4-da42-4ca4-af57-5353b9e732e8","D.7.1.1.1.5","","Earth filling, selected by the Contractor from the excavated material, deposited in layers not exceeding 150mm thick, watered and consolidated to 93% modified AASHTO density in backfilling.","m³",1,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","c8272378-8780-4e27-9938-0b77b96e3244","D.7.1.1.2","","CONCRETE",{"$nulls":4},"Dflt"]
["Label","47088dc9-6e7f-44e1-a369-32972ff229bc","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","c9eee4f1-9b44-4f63-a592-5b50669d10e7","","","Cost of tests",{"$nulls":4},"Dflt"]
["Label","2c350234-0ff1-4e3d-9fde-c3b24f71eae6","","","The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the architect.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the architect.  (Test cubes are measured separately)",{"$nulls":4},"Dflt"]
["Label","de07facf-0aaa-4bb8-a07b-fc18127c8e8d","","","Breeze concrete shall consist of twelve parts clean dry furnace ash, free from coal or other foreign matter, to one part cement (12:1), the ash graded up to particles which will pass a 16,5mm ring from a minimum which fails to pass a 4,75mm mesh.  The finer materials from the screening are to be first mixed with the cement into a mortar and the ash added afterwards and thoroughly incorporated",{"$nulls":4},"Dflt"]
["Label","b3f40671-45ea-40c2-a919-1f95bb047e1c","","","\"Foamcement \" lightwieght concrete",{"$nulls":4},"Dflt"]
["Label","6aa7c15a-f28b-41f3-84e0-116e97998798","","","\"Foamcement\" lightweight concrete is to have a density of 600kg/m3 for the top 50mm and 400kg/m3 for the remaining thickness.  The minimum thickness at outlets, channels, etc shall be 50mm",{"$nulls":4},"Dflt"]
["Label","6df5ae83-8560-4e95-ae1e-c44a4aa6f955","","","\"Celbeton\" lightweight concrete",{"$nulls":4},"Dflt"]
["Label","92471809-a7c7-4a5b-a99e-d30252effb16","","","\"Celbeton\" lightweight concrete is to have a density of 1000kg/m3 for the top 20mm and 480kg/m3 for the remaining thickness.  The minimum thickness at outlets, channels, etc shall be 30mm",{"$nulls":4},"Dflt"]
["Label","cbe1325a-c82d-4956-9dca-9747d70d1521","","","Formwork",{"$nulls":4},"Dflt"]
["Label","f77087d5-d9e6-4e33-9c14-3a839dcc6505","","","Description of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use",{"$nulls":4},"Dflt"]
["Label","615ff159-0c1c-4121-864e-e8a0e4a8e2aa","","","The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself.",{"$nulls":4},"Dflt"]
["Label","47afbb91-13fe-4f0a-975d-e0d37f1ed8d4","","","Formworks to soffits of solid etc shall be deemed to be slabs not exceeding 250mm thick unless otherwise described",{"$nulls":4},"Dflt"]
["Label","1f4b6b3a-13a5-4150-a8af-82513bdba004","","","Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the Engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\"",{"$nulls":4},"Dflt"]
["Label","ca3d5a99-3c21-4279-8018-69303f9ed406","","","Reinforced Cement Concrete (25MPa) In",{"$nulls":4},"Dflt"]
["Item","de869a2a-78a0-45ae-b1a4-0dfb76c8ca12","D.7.1.1.2.1","","Stub Columns.","m³",0.1,{"v":0,"d":"0.00"},{"$f":"ROUND(G41 * H41,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","6d747c23-ab10-466e-80ff-ebce8e0fcee8","D.7.1.1.2.2","","Column bases.","m³",0.3,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header3","c5076de4-b4ec-4ba8-8ea6-10646392f732","D.7.1.1.3","","CONCRETE CAST AGAINST EXCAVATED SURFACES",{"$nulls":4},"Dflt"]
["Label","ef4b4cbc-af17-4647-9b63-bc87fb7773ff","","","Cement Concrete (10MPa) In",{"$nulls":4},"Dflt"]
["Item","810669d7-653b-4897-9253-b22a43d18c24","D.7.1.1.3.1","","Blinding under bases.","m³",0.1,{"v":0,"d":"0.00"},{"$f":"ROUND(G45 * H45,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","98b9c4f2-8a60-4270-bc20-0fc515af4f5e","D.7.1.1.4","","FORMWORK",{"$nulls":4},"Dflt"]
["Label","2d6ede37-b1f1-4556-99fb-b7c718dab4cc","","","Class F1 Formwork To",{"$nulls":4},"Dflt"]
["Item","ba34f79b-51bd-4921-95c2-85e372f6c4a6","D.7.1.1.4.1","","Sides of square or rectangular columns.","m²",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G48 * H48,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","39ea1e21-e3bd-4bf5-b7aa-a5c51de63c61","D.7.1.1.5","","REINFORCEMENT (Provisional)",{"$nulls":4},"Dflt"]
["Label","9b446bf6-e8b1-4559-b03d-be7255294a5c","","","Mild Steel / High Tensile steel Bar Reinforcement To S Concrete.",{"$nulls":4},"Dflt"]
["Item","22e8bf54-ea9c-4948-ba14-bff738e52323","D.7.1.1.5.1","","Reinforcement in foundations: All diameter bars.","t",0.03,{"v":0,"d":"0.00"},{"$f":"ROUND(G51 * H51,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","0309e70d-8ce1-4409-814b-e9fdae6cb0a2","D.7.1.2","JBCC","BILL No. 2 CONCRETE, FORMWORK AND REINFORCEMENT",{"$nulls":4},"Dflt"]
["Label","2783f4a0-9883-4cb4-afde-a0b8b3d15bb9","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","4806dbf2-08c2-4c42-a074-b0c0950b1aed","","","Cost of tests",{"$nulls":4},"Dflt"]
["Label","34d1f6f8-4554-493b-b191-54e9f056507c","","","The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the a",{"$nulls":4},"Dflt"]
["Label","264f3aac-437d-4fe7-a95d-8a55c578795c","","","Breeze concrete shall consist of twelve parts clean dry furnace ash, free from coal or other foreign matter, to one part cement (12:1), the ash graded up to particles which will pass a 16,5mm ring from a minimum which fails to pass a 4,75mm mesh.  The fin",{"$nulls":4},"Dflt"]
["Label","06eb9758-102f-42d3-9edb-dd6b441444ca","","","\"Foamcement \" lightwieght concrete",{"$nulls":4},"Dflt"]
["Label","f9b27c1d-99b9-4a1d-b012-7db9c32e5183","","","\"Foamcement\" lightweight concrete is to have a density of 600kg/m3 for the top 50mm and 400kg/m3 for the remaining thickness.  The minimum thickness at outlets, channels, etc shall be 50mm",{"$nulls":4},"Dflt"]
["Label","afd871c4-5328-4079-a5ec-cc13b72cbd97","","","\"Celbeton\" lightweight concrete",{"$nulls":4},"Dflt"]
["Label","84f19bee-808c-421d-9fca-730f57cbea2b","","","\"Celbeton\" lightweight concrete is to have a density of 1000kg/m3 for the top 20mm and 480kg/m3 for the remaining thickness.  The minimum thickness at outlets, channels, etc shall be 30mm",{"$nulls":4},"Dflt"]
["Label","3bacbce5-0851-47f9-909b-3f5e142d93a2","","","Formwork",{"$nulls":4},"Dflt"]
["Label","8e9b46ea-ab4a-40ad-bd3d-d8e32f59bc52","","","Description of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy re",{"$nulls":4},"Dflt"]
["Label","e648f98b-ff9e-4576-84dd-2ceefaca30ea","","","The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself.",{"$nulls":4},"Dflt"]
["Label","2169b963-2091-41e4-868a-860019cb3895","","","Formworks to soffits of solid etc shall be deemed to be slabs not exceeding 250mm thick unless otherwise described",{"$nulls":4},"Dflt"]
["Label","ff4fd452-1dff-4e4a-972d-e2947d9ea3df","","","Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the Engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall",{"$nulls":4},"Dflt"]
["Header3","3269f865-e66c-4f0d-9e17-4a522b43d67f","D.7.1.2.1","","CONCRETE",{"$nulls":4},"Dflt"]
["Label","583dbb5b-da79-4bd4-8331-e66dfebd5b60","","","Reinforced Cement Concrete (30MPa) In",{"$nulls":4},"Dflt"]
["Item","71ae1459-61ab-440f-b6d1-79a40a238dd6","D.7.1.2.1.1","","30MPa Reinforced concrete in: Ring beams.","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G68 * H68,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","57eaca84-727c-4ec3-b1ee-14b237316361","","","Reinforced Cement Concrete (20MPa) In",{"$nulls":4},"Dflt"]
["Item","6a293a87-cb31-471e-9691-94550e879954","D.7.1.2.1.2","","20MPa Reinforced concrete for apron.","m³",3,{"v":0,"d":"0.00"},{"$f":"ROUND(G70 * H70,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","9e66b83f-b2cf-4f1c-aad8-1f789f8d8430","","","Concrete Sundries",{"$nulls":4},"Dflt"]
["Item","b0b6a1d4-38ec-4b41-8265-1423f4cf3b6b","D.7.1.2.1.3","","10mm Thick bed of non-metallic non-shrink grout size 300 x 300mm including chamfered edge all around.","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G72 * H72,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","b3a981fc-2507-4f3e-a455-ea4b173e7858","D.7.1.2.2","","FORMWORK",{"$nulls":4},"Dflt"]
["Label","315e1cae-3cdb-4ac5-9a75-85fae32899a7","","","Formwork To (Degree of Accuracy I)",{"$nulls":4},"Dflt"]
["Item","65025202-eb4e-4ca9-9647-49e9ed6bbb52","D.7.1.2.2.1","","Formwork to sides of ring beams.","m²",23,{"v":0,"d":"0.00"},{"$f":"ROUND(G75 * H75,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","6575a79a-5354-4170-a17e-aebb388e80e9","","","Permanent Formwork To",{"$nulls":4},"Dflt"]
["Item","b4d6dca1-aa19-4756-9d39-859b24a0a78b","D.7.1.2.2.2","","Soffit of wall beams over 80mm wide cavity of hollow wall. (Provisional)","m",23,{"v":0,"d":"0.00"},{"$f":"ROUND(G77 * H77,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","8171a65b-0bce-44c6-8cc0-ebbcd55312d1","","","Rough formwork to sides",{"$nulls":4},"Dflt"]
["Item","3f0bf1fc-fa93-45fe-ab79-9a51ba68f90e","D.7.1.2.2.3","","Edges, rises, ends and reveals not exceeding 300mm high or wide.","m",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G79 * H79,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","9f981e3c-18ab-4210-9dfd-a3bbd0b3216b","D.7.1.2.3","","CONCRETE SUNDRIES",{"$nulls":4},"Dflt"]
["Label","7e87580e-ffc0-4473-8d43-d9c7082f8dc1","","","Finishing top surfaces of concrete to an evenly ribbed non-slip surface",{"$nulls":4},"Dflt"]
["Item","09f04b7a-347a-4e7a-b415-488b36fa4e23","D.7.1.2.3.1","","Pavings to falls.","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G82 * H82,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","5dbd5ca5-9f02-4958-b59e-0ba882f0bf08","D.7.1.2.4","","REINFORCEMENT (PROVISIONAL)",{"$nulls":4},"Dflt"]
["Label","41b6e4a6-330f-465e-b8a5-259463fd501b","","","Steel Bar Reinforcement To Structural Concrete Work",{"$nulls":4},"Dflt"]
["Item","6db71bfc-d127-47e1-b411-07f369e9bd29","D.7.1.2.4.1","","All Diameter bars. (Provisional)","t",0.45,{"v":0,"d":"0.00"},{"$f":"ROUND(G85 * H85,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","4d535971-820e-4721-8499-b08c8a48bd56","","","Fabric reinforcement",{"$nulls":4},"Dflt"]
["Item","bf1a374f-d632-409a-8ae5-641bf189c190","D.7.1.2.4.2","","Type 193 fabric reinforcement in concrete surface beds.","m²",20,{"v":0,"d":"0.00"},{"$f":"ROUND(G87 * H87,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","2f0c3d82-9b5f-43c1-a0f9-a21037650c53","D.7.1.3","JBCC","BILL No. 3 MASONRY",{"$nulls":4},"Dflt"]
["Label","0fadc944-9e83-44fa-9cfb-a6a3a9a34368","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","ff41a454-99c9-4fd9-833f-94564a72c97c","","","BRICKWORK",{"$nulls":4},"Dflt"]
["Label","465bfe57-4a58-4c1f-8622-9d30feb2360a","","","Sizes in descriptions",{"$nulls":4},"Dflt"]
["Label","aaa0af8e-58cd-4a9a-bf67-9a042540fe27","","","Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick",{"$nulls":4},"Dflt"]
["Label","2d4419d1-5d2c-490f-83b0-46b945ed6660","","","Hollow walls etc",{"$nulls":4},"Dflt"]
["Label","1fecbeb9-1173-418e-ae32-36535b86369e","","","Descriptions of hollow walls shall be deemed to include leaving every fifth perpend of the bottom course of the external skin open as a weep hole.",{"$nulls":4},"Dflt"]
["Label","ee8703cb-6f0f-4d7b-81da-c43c27ea2d30","","","Walls in two skins described as \"bagged and sealed\" shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture and sealed with two coats \"Brixeal\" bitumen emulsion waterproofing coating.",{"$nulls":4},"Dflt"]
["Label","dba76fa8-6094-4566-9038-b15c7ec7d474","","","User note:",{"$nulls":4},"Dflt"]
["Label","aaf40d95-56e4-4f76-9722-fd8fb8f7d4ce","","","The above preamble generally applies for works in hot and humid coastal areas",{"$nulls":4},"Dflt"]
["Label","91ab6051-339a-4d3b-ba0c-ac0edf55cd4b","","","Face bricks",{"$nulls":4},"Dflt"]
["Label","4c38d332-4673-410f-91d2-b6a30b2f709c","","","Bricks shall be ordered timeously to obtain uniformity in size and colour",{"$nulls":4},"Dflt"]
["Label","37b60807-b8e5-4fdf-a478-9999ad9c1ec8","","","Pointing",{"$nulls":4},"Dflt"]
["Label","065553c7-bad5-4f75-bd0b-b63fd8cd56b9","","","Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc",{"$nulls":4},"Dflt"]
["Header3","921055d3-4697-40df-a7c2-a538f3c5b869","D.7.1.3.1","","BRICKWORK",{"$nulls":4},"Dflt"]
["Label","b5815ed4-48f1-4074-af83-62851da07f75","","","Brickwork In Clay Bricks In 1:5 Cement Mortar In",{"$nulls":4},"Dflt"]
["Item","439cc4f0-a43e-4600-ac66-fbcfa0099475","D.7.1.3.1.1","","300mm Cavity wall in two half brick thickness's including butterfly wire ties.","m²",87,{"v":0,"d":"0.00"},{"$f":"ROUND(G104 * H104,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","93d6cafe-36eb-4417-82e3-e61bea1e7537","","","Brickwork Sundries",{"$nulls":4},"Dflt"]
["Item","6f46b47d-2088-4d26-8022-505cb9784023","D.7.1.3.1.2","","Bag down outer face of inner skin of brick wall with 4.1 cement slurry and apply two coats bituminous emulsion including working around ties.","m²",87,{"v":0,"d":"0.00"},{"$f":"ROUND(G106 * H106,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","e63c2294-0057-475e-b825-af6d838f135c","D.7.1.3.1.3","","80 x 75mm Triangular cement mortar fillet in cavity wall including forming weepholes.","m",23,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","b196694f-b03f-4748-83b2-135bf1e3d78c","","","Galvanised Brick Reinforcement",{"$nulls":4},"Dflt"]
["Item","49e140a1-6425-4d12-84d5-aaba3b74cc20","D.7.1.3.1.4","","Brick reinforcement 150mm wide. (Provisional).","m",348,{"v":0,"d":"0.00"},{"$f":"ROUND(G109 * H109,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","41a5d86c-d7f9-467f-8e79-2cbf4ba8c345","","","Ties, Cramps, Etc.",{"$nulls":4},"Dflt"]
["Item","1dde77f6-15ae-4718-9fb2-6c012dd4eea7","D.7.1.3.1.5","","2 x 30mm Galvanised hoop iron tie 750mm long with one end cast 340mm deep into ring beam and other end wrapped around rafter and spiked to plate.","No",14,{"v":0,"d":"0.00"},{"$f":"ROUND(G111 * H111,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","769dfe3f-ab94-43b6-b564-c915979a2c19","D.7.1.3.2","","FACE BRICKWORK",{"$nulls":4},"Dflt"]
["Label","c713fe7b-c6a6-4b7f-8bfd-16ea884a75b8","","","Face Bricks (PC Amount Of R 5800.00 Per Thousand) Pointed With Ruled-In Vertical And Horizontal Joints",{"$nulls":4},"Dflt"]
["Item","956752ba-6296-4339-a9b6-803b7fa470e1","D.7.1.3.2.1","","Extra over brickwork for face brickwork.","m²",87,{"v":0,"d":"0.00"},{"$f":"ROUND(G114 * H114,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","0b88d2f2-a1e5-4229-a087-ce69fdb6ce88","D.7.1.3.3","","SUNDRIES",{"$nulls":4},"Dflt"]
["Label","11ec030f-4eec-4253-81ef-5e80ca02a7a2","","","Core drilling",{"$nulls":4},"Dflt"]
["Item","7118b58f-7af3-4321-98f9-a572334a496b","D.7.1.3.3.1","","Core drilling hole exceeding 200mm and not exceeding 250mm diameter through 300mm thick reinforced brickwall","No",2,{"v":0,"d":"0.00"},{"$f":"ROUND(G117 * H117,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","3ed8191d-fa98-494d-8793-e6ab0d898cee","D.7.1.4","JBCC","BILL NO. 4 ROOF COVERINGS, ETC.",{"$nulls":4},"Dflt"]
["Header3","f9c2d049-2197-410f-a8bc-ac94cb58e543","D.7.1.4.1","","PROFILED METAL SHEETING AND ACCESSORIES",{"$nulls":4},"Dflt"]
["Label","340cf89e-862a-4e9a-98c5-9da57b258aa5","","","GRS  \"Klip-Lok 406\" colour coated both sides 0,8mm aluminium finish roof sheeting, fixed to timber purlins including KL65 clips and class 3 fasteners in strict accordance with manufacturer's specifications by a GRS approved contractor (Elsewhere Measured.",{"$nulls":4},"Dflt"]
["Item","92d9bcf2-35b0-49fd-9c26-faf894788ca8","D.7.1.4.1.1","","Roof covering with pitch not exceeding 25 degrees with side and end laps sealed with 12 x 25mm closed cell bitumen impregnated polyurethane foam strips and seam stitched.","m²",61,{"v":0,"d":"0.00"},{"$f":"ROUND(G121 * H121,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","813b1ef6-c98e-4e70-a30e-63f9623442c8","D.7.1.4.1.2","","Extra over roof covering for 80 degree bullnose to 820mm radius","m",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","d566f7b0-092b-4260-b005-771a74ad7926","D.7.1.4.1.3","","Extra over roof covering for 90 degree bullnose to 820mm radius","m",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","3f47b63a-9db7-4d41-af6b-a299a790bf2f","D.7.1.4.1.4","","Side cladding with side and end laps sealed with 12 x 25mm closed bitumen impregnated polyurethane foam strips and seam stitched.","m²",25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","7db4d2b1-d63f-411d-9f6e-34d3949782fe","D.7.1.4.1.5","","Drip flashing 450mm girth.","m",11,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","64ad4ee6-31fc-42fd-82ec-6169ad935914","D.7.1.4.1.6","","Drip flashing 450mm girth.","m",19,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Item","c9bb4c56-4554-491b-8586-434027e20623","D.7.1.4.1.7","","Standard Drip Flashing 231mm girth 3 (Three) times bent.","m",13,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","971c01ff-d1cd-4ae3-a78e-a261ae94fc2b","D.7.1.5","JBCC","BILL No. 5 CARPENTRY AND JOINERY",{"$nulls":4},"Dflt"]
["Label","4c6f5d6f-8b77-4429-8a95-278996c07a96","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","0b62d0f6-1ec7-4542-b76b-0cafb76cdcb7","","","Particle board:",{"$nulls":4},"Dflt"]
["Label","7887c6a0-7235-4741-968c-a0dde6f1129c","","","Particle board shall comply with the following specifications: a) SABS 1300 Particle board: exterior and flooring type b) SABS 1301 Particle board: interior type",{"$nulls":4},"Dflt"]
["Label","a8feb18b-2cb3-41b4-b933-5e10071c493e","","","Joinery:",{"$nulls":4},"Dflt"]
["Label","233863cf-afb9-4011-9d78-b97e53698a55","","","Descriptions of frames shall be deemed to include frames, transomes, mullions, rails, etc",{"$nulls":4},"Dflt"]
["Label","da2b9e0b-8184-4f9c-9389-75ca537d0445","","","Descriptions of hardwood joinery shall be deemed to include pelleting of bolt holes",{"$nulls":4},"Dflt"]
["Label","60db1536-f3d0-420a-83a8-6f676b27351b","","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete",{"$nulls":4},"Dflt"]
["Label","eb03b377-dedc-4410-84ee-b284f44c873a","","","Decorative laminate finish:",{"$nulls":4},"Dflt"]
["Label","f19ab986-cf19-41e8-b34f-3e8d1f7495b0","","","Laminate finish shall be glued under pressure.  Edge strips shall be butt jointed at junctions with adjacent similar finish",{"$nulls":4},"Dflt"]
["Header3","932cfe6f-6064-49f9-a8ed-c6dd3e829ff2","D.7.1.5.1","","CARPENTRY",{"$nulls":4},"Dflt"]
["Label","d0ffd20c-13fc-47cb-8b06-3cb6872ee674","","","ROOFS, ETC.",{"$nulls":4},"Dflt"]
["Label","500de119-028b-4e4f-bdc5-510662f2134e","","","The Following In Roofs",{"$nulls":4},"Dflt"]
["Label","7f6c930a-b43b-438a-804c-bd971f8d19e5","","","Wrot Pine",{"$nulls":4},"Dflt"]
["Item","1729f327-193a-4a75-9b09-ead249e8df7a","D.7.1.5.1.1","","50 x 76mm Purlin.","m",120,{"v":0,"d":"0.00"},{"$f":"ROUND(G142 * H142,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","8c35b225-402d-4c59-9b62-be8b2efa2702","D.7.1.5.2","","TIMBER ROOF TRUSSES",{"$nulls":4},"Dflt"]
["Label","50b86143-d572-479e-83d7-2aac53a180de","","","Plate nailed timber roof truss construction",{"$nulls":4},"Dflt"]
["Label","de1de1db-bff0-4495-9a16-e1fb81bb228c","","","The following is applicable in respect of roof trusses:",{"$nulls":4},"Dflt"]
["Label","3314b1b5-d85d-4c1f-9f10-390504212ef5","","","Trusses at 15Â­Â° pitch",{"$nulls":4},"Dflt"]
["Item","c4b559db-0a80-4a8e-8277-64e11d55b5cf","D.7.1.5.2.1","","SSAP Double curved truss built up with a combination of a Bow string, Mono truss and Bull nose end truss size approximately 4500mm span x 2550mm high extreme overall.(Provisional).","No",7,{"v":0,"d":"0.00"},{"$f":"ROUND(G147 * H147,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","913bc213-8345-4410-8beb-8cf59e902d98","","","Sawn South African Pine",{"$nulls":4},"Dflt"]
["Item","170a57cf-028a-419a-a6ce-29f35619e6e5","D.7.1.5.2.2","","38 x 114mm wall plates.","m",23,{"v":0,"d":"0.00"},{"$f":"ROUND(G149 * H149,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","a3c43754-4c73-4246-93bb-b2f72cf14927","D.7.1.6","JBCC","BILL No. 6 STRUCTURAL STEEL",{"$nulls":4},"Dflt"]
["Label","54a2b1b9-2955-45e3-9579-6be9e188396b","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","bbc7123e-578f-4f4f-be07-9c9222947925","","","Descriptions",{"$nulls":4},"Dflt"]
["Label","0cd93948-c008-406b-b167-403bd2023ced","","","Descriptions of bolts shall be deemed to include nuts and washers",{"$nulls":4},"Dflt"]
["Label","ce06b839-73cd-49db-a04c-50a7649c9694","","","Descriptions of L-shaped and U-shaped anchor bolts shall be deemed to include bending, threading, nuts and washers and embedding in concrete",{"$nulls":4},"Dflt"]
["Label","7250187b-4365-4038-b026-7801a9471589","","","Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete",{"$nulls":4},"Dflt"]
["Label","718e599b-f7af-40bf-ae7a-85e981d3b0a2","","","Descriptions of L-shaped and U-shaped anchor bolts shall be deemed to include bending, threading, nuts and washers and embedding in concrete. Where anchor bolts are described as embedded in sides or soffits of concrete it shall be deemed to include holes ",{"$nulls":4},"Dflt"]
["Label","99d0fe36-88f9-4dca-a961-79ca42479bba","","","Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete.",{"$nulls":4},"Dflt"]
["Header3","a61dc573-afb4-4e13-915b-bc919937169b","D.7.1.6.1","","STEEL COLUMNS AND BEAMS",{"$nulls":4},"Dflt"]
["Label","960cb1c4-6036-4d90-b12c-d2890fee28d2","","","Galvanised Welded Columns In Single Lengths With Flat Section Base, Top, Bearer And Connection Plates Bolted To Concrete Stub Columns (Elsewhere measured)",{"$nulls":4},"Dflt"]
["Item","d2cd7ed7-80fa-443a-85d1-de80fbe49170","D.7.1.6.1.1","","152 x 152mm x 23kg/m H-section columns.","t",0.2,{"v":0,"d":"0.00"},{"$f":"ROUND(G160 * H160,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Label","77dad370-dabc-467d-8681-d490ae8cdcd2","","","Galvanised Welded Beams In Single Lengths With Flat Section Bearer And Connection Plates Bolted to steel column",{"$nulls":4},"Dflt"]
["Item","7fda02a7-783b-4b63-af4f-577c993450be","D.7.1.6.1.2","","152 x 152mm x 23kg/m H-section beams","t",0.02,{"v":0,"d":"0.00"},{"$f":"ROUND(G162 * H162,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","5d152edd-6f6e-4afb-95f7-fbbbeac17706","D.7.1.6.1.3","","203 x 133mm x 25kg/m I-section beams.","t",0.25,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1648b776-7e66-4b0d-9540-cecf4eec6dab","","","Bolts To Columns, Beams, Etc",{"$nulls":4},"Dflt"]
["Item","1d6d842e-6b9b-4495-8508-f0cfabe87a82","D.7.1.6.1.4","","20mm Diameter H.D bolts 500mm long embedded 400mm deep into concrete and including 80 x 80 x 10mm thick end plate.","No",4,{"v":0,"d":"0.00"},{"$f":"ROUND(G165 * H165,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","17c4d736-ebee-48ed-be2f-fead19371e82","D.7.1.6.1.5","","High tensile friction grip bolts with nuts and washers.","t",0.06,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Header2","8ddafcdc-86e7-4edb-8d1f-325d85718263","D.7.1.7","JBCC","BILL No. 7 METALWORK",{"$nulls":4},"Dflt"]
["Label","1975b67b-6f0e-40f2-a03d-16d40f4b4551","","","SUPPLEMENTARY PREAMBLES",{"$nulls":4},"Dflt"]
["Label","84704efe-428e-4d15-9d39-f2ec28a83afd","","","Descriptions",{"$nulls":4},"Dflt"]
["Label","eca6c540-8f6c-4b57-b8b2-d22f8fd2eb7a","","","Descriptions of bolts shall be deemed to include nuts and washers",{"$nulls":4},"Dflt"]
["Label","c073d97a-61c1-4d89-8bd0-f7d603dee440","","","Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete",{"$nulls":4},"Dflt"]
["Label","5d26c414-607f-4f16-bb6a-78c75b961569","","","Metalwork described as\"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described",{"$nulls":4},"Dflt"]
["Header3","14d07a7f-13d1-4550-ab35-4a1299fc5027","D.7.1.7.1","","PRESSED STEEL COMBINATION DOORS AND FRAMES",{"$nulls":4},"Dflt"]
["Label","05840973-77c6-424e-9621-008e409aea11","","","Pre-galvanised pressed steel transformer room doors and frames",{"$nulls":4},"Dflt"]
["Item","c2b2476a-bc77-45fa-87ce-c12161ab1398","D.7.1.7.1.1","","Door type D01 size 2064 x 4250mm high including frames, ironmongery and louvres complete as per Architects door schedule attached.","No",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G175 * H175,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","e2f4ccd2-5c2a-403c-ac1d-e42a1a5c6a28","D.7.1.8","JBCC","BILL No. 8 PLASTERING",{"$nulls":4},"Dflt"]
["Label","9d317d91-41d0-4d7d-b7d8-5162215213a3","","","INTERNAL PLASTER",{"$nulls":4},"Dflt"]
["Item","4eeba20b-c777-483f-9784-e719e8bb22a6","D.7.1.8.1","","1:5 Cement Plaster On Brickwork On Walls","m²",89,{"v":0,"d":"0.00"},{"$f":"ROUND(G178 * H178,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","c0404a61-d791-44e9-9909-4f6ee312a939","D.7.1.9","JBCC","BILL No. 9 PAINTWORK",{"$nulls":4},"Dflt"]
["Label","1fa25ea9-dfbd-4f90-ad00-04e4d95e949e","","","PREPARATORY WORK TO EXISTING WORK",{"$nulls":4},"Dflt"]
["Label","7d53ebba-4f99-4b01-b1de-ff15e011e2f0","","","Previously painted plastered surfaces",{"$nulls":4},"Dflt"]
["Label","f1409b02-0c56-4d5b-b480-f78f03ef5de2","","","Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth",{"$nulls":4},"Dflt"]
["Label","2ff34f77-4940-4a8c-a735-344f9afb418b","","","Previously painted metal surfaces",{"$nulls":4},"Dflt"]
["Label","a24a209b-f637-490f-9ab2-532e112b833d","","","Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal",{"$nulls":4},"Dflt"]
["Label","ed053689-5a63-4fa1-88ad-33e7f6f22c5e","","","Previously painted wood surfaces",{"$nulls":4},"Dflt"]
["Label","d5c716f6-a6cb-4a1e-92ae-dfde22a1bf1f","","","Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth",{"$nulls":4},"Dflt"]
["Header3","72b6d337-7d3e-4d9d-965b-25ecf367c0b0","D.7.1.9.1","","PAINT ON PLASTER, FIBRE REINFORCED CEMENT, ETC.",{"$nulls":4},"Dflt"]
["Label","60b1fbc5-bd3b-41ef-a77b-53ce4f87650c","","","Prepare And Apply One Coat Plascon Plaster Primer And Two Coats Plascon Wall & All On",{"$nulls":4},"Dflt"]
["Item","86e45cf5-96b3-47ad-995f-f4e7e016462f","D.7.1.9.1.1","","Plastered walls.","m²",89,{"v":0,"d":"0.00"},{"$f":"ROUND(G189 * H189,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header3","edf90e27-8562-4a19-8e6f-765b1eaee4b8","D.7.1.9.2","","PAINT ON DOORS AND FRAMES",{"$nulls":4},"Dflt"]
["Label","cc68b969-5937-4dde-bde4-7513a837c313","","","Prepare and Apply 1 coat Plascon Metalcare Galvanised Iron Primer, 1 coat Plascon Universal Undercoat and 2 coats Plascon Velvaglo Enamel",{"$nulls":4},"Dflt"]
["Item","1ac8eebf-e7f9-488e-92f6-b97b92a53616","D.7.1.9.2.1","","Doors","m²",18,{"v":0,"d":"0.00"},{"$f":"ROUND(G192 * H192,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Item","424fa825-5acc-4bac-b90f-70e9d43aa45c","D.7.1.9.2.2","","Door frames.","m²",6,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},"Dflt"]
["Label","1fdeaac1-d900-4eba-bde3-b5607f608ded","","","Prepare and apply 2 coats bitumen emulsion paint",{"$nulls":4},"Dflt"]
["Item","528b9d3d-d53c-48e7-82fd-fc7604567f88","D.7.1.9.2.3","","Door frames.","m²",6,{"v":0,"d":"0.00"},{"$f":"ROUND(G195 * H195,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","e758cea5-36a5-435f-9fff-bfb791a84ff5","D.7.1.10","JBCC","BILL No. 10 PROVISIONAL SUMS",{"$nulls":4},"Dflt"]
["Label","a7385756-7f9a-4b57-aa83-85841dba816c","","","Attention is directed to the relevant sections of the Model Preambles for Trades which forms a part of this Bill and must be read in conjunction herewith.",{"$nulls":4},"Dflt"]
["Label","4f2dadc0-686b-4fb4-b3d4-03225bfa1b30","","","THE FOLLOWING NOMINATED SUB-CONTRACT AMOUNTS ARE FOR WORK TO BE CARRIED OUT BY NOMINATED SUB-CONTRACTORS AS INSTRUCTED BY Engineer",{"$nulls":4},"Dflt"]
["Label","7da6b058-dbe2-4702-9d33-4cc2ea13aa39","","","Note:  The following Provisional Sums are net and do not include any discount for the Main Contractor.  ----------------",{"$nulls":4},"Dflt"]
["Sum","3bb5ca10-5446-460d-8f2f-8a82b52f5f14","D.7.1.10.1","","Provide the sum of R22 000.00 (Twenty Two Thousand) for Electrical  Installation to RAS Building","Prov.Sum",1,{"v":22000,"d":"22,000.00"},{"$f":"ROUND(H200,2)","v":{"v":22000,"d":"22,000.00"}}]
["% Previous","78dffcbc-a95a-4448-a6d2-633a2a4615a8","D.7.1.10.2","","Allow for profit if required. ","%",{"$f":"I200","v":{"v":22000,"d":"22 000.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G201 * H201,2)","v":{"v":0,"d":"0.00"}}]
["% Previous","d1755721-f530-4c99-bcdd-1817b6d12ea9","D.7.1.10.3","","Allow for general attendance on ditto. ","%",{"$f":"I200","v":{"v":22000,"d":"22 000.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Item","48b307e9-71de-4865-9705-5462de84314f","D.7.1.10.4","","Allow for gantry hook installation complete.","Prov.Sum",1,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
["Label","fc5db830-9f4d-4c83-b9cc-4d5ca63fa597","","","THE FOLLOWING MONETARY PROVISIONS ARE TO BE OMITTED FROM THE CONTRACT SUM  BY THE ENGINEER AND USED AS DIRECTED BELOW"]
["Item","6297827e-6b81-4c8b-92a7-55d1e4dec0f4","D.7.1.10.5","","Provide the sum of R30 000.00 (Thirty Thousand) for Contingencies, to be deducted in whole or part if not required.","Prov.Sum",1,{"v":30000,"d":"30,000.00"},{"$f":"ROUND(G205 * H205,2)","v":{"v":30000,"d":"30,000.00"}}]

{"sheet":"BILL D.8.","index":17,"n_rows":30,"n_cols":10,"rows_kept":30,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":8},"v","Dflt"]
["BillHeader",null,"BILL D.8.",null,"MISCELLANEOUS (BUILDINGS)",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","bcf99866-94d8-4d5d-b694-99c34c04767c","D.8.1","","MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Label","f274bcf3-a301-4121-bcb0-59584d0c9aaf","","","SECTION D.8.1 : MISCELLANEOUS",{"$nulls":4},"Dflt"]
["Header2","a955e0a4-1b18-43cd-a9c5-472444b27cdb","D.8.1.1","","BLOWER BUILDING",{"$nulls":4},"Dflt"]
["Label","cb0fe47d-31c7-470a-b7bf-b16b1c96703d","","","Supply and install crawl beam in blower building complete, including supply, fitting, corrosion protection, testing, certrification, etc. as shown on Dwg. No. J40073/010-408",{"$nulls":4},"Dflt"]
["Item","9d1d2410-a630-46c2-9e37-eca4cca421f6","D.8.1.1.1","","Crawl Beam","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G13 * H13,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","f9c5953d-9cee-4bb5-a4a0-cd31977188f2","D.8.1.2","","SEPTIC TANK",{"$nulls":4},"Dflt"]
["Label","a81c4400-f1e5-4456-ade9-b9caa36b1a28","","","Construct septic tank complete, including excavation, backfilling, testing, etc complete as shown on Dwg. No. J40073/010-226",{"$nulls":4},"Dflt"]
["Item","eb9ec7ac-7216-4730-8d10-ceb0e911eb97","D.8.1.2.1","","Septic Tank","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G16 * H16,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","10cf81eb-5b48-4dcf-9fbb-8a4ef98d4221","D.8.1.3","","SIGNAGE",{"$nulls":4},"Dflt"]
["Label","4e366c36-098e-44f4-b7fa-e439414fb366","","","Mandatory and Prohibitive signage, supply, install etc. to all buildings",{"$nulls":4},"Dflt"]
["Sum","1e7215e7-3b74-4962-9018-7c75d8275143","D.8.1.3.1","PSA 8.9","Signage (Provisional)","Prov.Sum",1,{"v":250000,"d":"250,000.00"},{"$f":"ROUND(H19,2)","v":{"v":250000,"d":"250,000.00"}},"Dflt"]
["Header2","b23ee940-85cf-42e7-9e6c-5dcd5ec8345f","D.8.1.4","","ELECTRICAL INSTALLATIONS",{"$nulls":4},"Dflt"]
["Label","7501854e-2bdb-4129-8005-b99fcba6a5a6","","","Complete Electrical installations to the following buidlings (Provisional):",{"$nulls":4},"Dflt"]
["Sum","74ae5a4f-a65e-48a4-a01a-a01f23897497","D.8.1.4.1","","Admin building (Provisional)","Prov.Sum",1,{"v":8000,"d":"8,000.00"},{"$f":"ROUND(H22,2)","v":{"v":8000,"d":"8,000.00"}},"Dflt"]
["Sum","f6da271d-76dd-4f40-b194-e6d471d1e984","D.8.1.4.2","","Workshop building (Provisional)","Prov.Sum",1,{"v":14000,"d":"14,000.00"},{"v":14000,"d":"14,000.00"},"Dflt"]
["Sum","0cabb22c-0673-4d0c-b8e8-571964bf983f","D.8.1.4.3","","MCC building (Provisional)","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"v":5000,"d":"5,000.00"},"Dflt"]
["Sum","d3611dd1-ac77-4506-933a-4d3333676e23","D.8.1.4.4","","Blower Building (Provisional)","Prov.Sum",1,{"v":5000,"d":"5,000.00"},{"v":5000,"d":"5,000.00"}]
["Sum","6880da86-c8be-4e28-be31-7d63322caae3","D.8.1.4.5","","Raw Sewage pump station (Provisional)","Prov.Sum",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
["Header2","e189e88b-fe15-4210-a417-8d9eaa3a7cd1","D.8.1.5","","ARCHITECTURAL FINISHES"]
["Sum","dad1fe3d-bebd-4348-b249-7230b08deca7","D.8.1.5.1","","Architectural finishes to the buildings (Provisional)","Prov.Sum",1,{"v":350000,"d":"350,000.00"},{"$f":"ROUND(H28,2)","v":{"v":350000,"d":"350,000.00"}}]
["Header2","47939e3c-7848-4a9d-b67d-7755b2a69f82","D.8.1.6","","CORRECTIVE WORK TO BUILDINGS"]
["Sum","ff2e11c3-d3be-47d0-909a-2b6b81c305f8","D.8.1.6.1","","Corrective work to buildings due to deterioration of exposed, unfinished works as directed by the Engineer (Provisional)","Sum",1,{"v":500000,"d":"500,000.00"},{"$f":"ROUND(H30,2)","v":{"v":500000,"d":"500,000.00"}}]

{"sheet":"BILL E","index":18,"n_rows":21,"n_cols":10,"rows_kept":21,"merged":[[2,4,3,8]]}
[]
[{"$nulls":3},"Bid No:","RW10404061/23",{"$nulls":4},"Work\nGroup"]
[{"$nulls":3},"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON",{"$nulls":4},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":9},"Dflt"]
[{"$nulls":8},"v","Dflt"]
["BillHeader",null,"BILL E",null,"SOCIO ECONOMIC DEVELOPMENT",{"$nulls":4},"Dflt"]
["Item Type","GUID","Item Ref","Payment\nRefers","Description","Unit","Quantity","Rate","Amount\nR","Dflt"]
["Section","1304ae26-2caa-4c51-96c2-27362b39f9d2","E1","","SOCIO ECONOMIC DEVELOPMENT",{"$nulls":4},"Dflt"]
["Header2","711e6cff-b9db-4022-9b5b-64f4d29db76a","E1.1","","SKILLS DEVELOPMENT PROGRAM",{"$nulls":4},"Dflt"]
["Sum","089935b4-dc0b-41f4-bb72-47c7baad4a1f","E1.1.1","","Accredited training programme are targeted which will provide the beneficiaries with significant and recognised credit value in accordance with the National Qualification Framework (NQF) (2.5% of Project Value - Sub Total A) (Provisional)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H11,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["% Previous","508e388f-5bff-4ab7-a054-313c6a19ad4c","E1.1.2","","Contractors mark-up on Item E1.1.1","%",{"$f":"I11","v":{"v":0,"d":" 0.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G12 * H12,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","925310dc-f481-4f2c-a6ee-9f647a1e40e2","E1.2","","SOCIAL RESPONSIBILITY PROGRAM",{"$nulls":4},"Dflt"]
["Sum","9d1edb40-aa97-4df2-8905-911358b42a02","E1.2.1","","Social Responsibility programs aimed at community development (1.5% of Project Value - Sub Total A) (Provisional)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H14,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["% Previous","ec24a40f-3a09-439d-ae2d-989fd66c3e3e","E1.2.2","","Contractors mark-up on Item E1.2.1","%",{"$f":"I14","v":{"v":0,"d":" 0.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G15 * H15,2)","v":{"v":0,"d":"0.00"}},"Dflt"]
["Header2","b3127690-43ac-40bb-859f-1b6404ce68d6","E1.3","","COMMUNITY LIAISON OFFICER"]
["Item","c9c181b1-5b58-498b-a06b-3d43d3200b84","E1.3.1","Contract Part C3 Scope of Work, C3.5.2.4 Community Participation","Community Liaison Officer for the duration of Construction. A key component in aiding the realisation of the SED objectives is effective community liaising with all the relevant role-players, structures, civic organisations and the community at large. (Provisional)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(G17 * H17,2)","v":{"v":0,"d":"0.00"}}]
["% Previous","dbb33036-6016-4042-9870-2de31e3eb05b","E1.3.2","","Contractors mark-up on Item E1.3.1","%",{"$f":"I17","v":{"v":0,"d":" 0.00"}},{"v":0,"d":"0.0%"},{"v":0,"d":"0.00"}]
["Header2","e6870126-0a8d-4e16-859c-d9325c3e8ceb","E1.4","","PARTICIPATION OF LOCAL ENTERPRISES"]
["Sum","0020c8c7-f9df-4c1c-9a06-8a4bd1e197e4","E1.4.1","","Work allocated to local enterprises (inclusive of P&G's and SHEQ) (Minimum 5% of Project Value) (Sub-Total A) (Provisional)","Sum",1,{"v":0,"d":"0.00"},{"$f":"ROUND(H20,2)","v":{"v":0,"d":"0.00"}}]
["% Previous","fbc42330-8e08-4c59-b170-1e8681b8def4","E1.4.2","","Contractors mark-up on Item E1.4.1","%",{"$f":"I20","v":{"v":0,"d":" 0.00"}},{"v":0,"d":"0.0%"},{"$f":"ROUND(G21 * H21,2)","v":{"v":0,"d":"0.00"}}]

{"sheet":"BILL Summary","index":19,"n_rows":80,"n_cols":9,"rows_kept":80,"merged":[[2,2,5,4]]}
[]
[null,"Bid No:","RW10404061/23"]
[null,"Description","TENDER FOR THE UPGRADE OF MEYERTON WASTEWATER TREATMENT WORKS BY 15 ML/DAY AT MEYERTON"]
[]
[]
[{"$nulls":8},"v"]
["BILL Summary"]
[]
["Section\nNumber","Description","Amount"]
["BILL A","PRELIMINARY AND GENERAL"]
["A1","PRELIMINARY AND GENERALS",{"$f":"SUM('BILL A'!I9:I110)","v":{"v":91535000,"d":"91,535,000.00"}}]
[null,"BILL A TOTAL:",{"$f":"SUM('BILL A'!I9:I110)","v":{"v":91535000,"d":"91,535,000.00"}}]
["BILL B.1.","DAYWORKS"]
["B.1.1","DAYWORKS",{"$f":"SUM('BILL B.1.'!I9:I37)","v":{"v":105000,"d":"105,000.00"}}]
[null,"BILL B.1. TOTAL:",{"$f":"SUM('BILL B.1.'!I9:I37)","v":{"v":105000,"d":"105,000.00"}}]
["BILL B.2.","PIPELINES"]
["B.2.1","MEDIUM PRESSURE PIPELINES, WATER RETICULATION AND SEWER RETICULATION",{"$f":"SUM('BILL B.2.'!I9:I177)","v":{"v":120000,"d":"120,000.00"}}]
["B.2.2","MEDIUM PRESSURE PIPELINES\r\n(IRRIGATION PUMP STATION RISING MAIN.",{"$f":"SUM('BILL B.2.'!I178:I223)","v":{"v":0,"d":"0.00"}}]
["B.2.3","WATER RETICULATION (BUILDINGS)",{"$f":"SUM('BILL B.2.'!I224:I299)","v":{"v":0,"d":"0.00"}}]
["B.2.4","SEWER RETICULATION (BUILDINGS)",{"$f":"SUM('BILL B.2.'!I300:I352)","v":{"v":0,"d":"0.00"}}]
["B.2.5","SEWERS (SUB-SURFACE DRAINS)",{"$f":"SUM('BILL B.2.'!I353:I414)","v":{"v":20000,"d":"20,000.00"}}]
["B.2.6","SEWERS (IRRIGATION PUMP STATION OVER FLOW PIPEWORK)",{"$f":"SUM('BILL B.2.'!I415:I449)","v":{"v":0,"d":"0.00"}}]
[null,"BILL B.2. TOTAL:",{"$f":"SUM('BILL B.2.'!I9:I449)","v":{"v":140000,"d":"140,000.00"}}]
["BILL B.3.","HEAD OF WORKS"]
["B.3.1","HEAD OF WORKS",{"$f":"SUM('BILL B.3.'!I9:I205)","v":{"v":1805000,"d":"1,805,000.00"}}]
[null,"BILL B.3. TOTAL:",{"$f":"SUM('BILL B.3.'!I9:I205)","v":{"v":1805000,"d":"1,805,000.00"}}]
["BILL B.4.","BIOLOGICAL REACTOR"]
["B.4.1","BIOLOGICAL REACTOR",{"$f":"SUM('BILL B.4.'!I9:I105)","v":{"v":5225000,"d":"5,225,000.00"}}]
[null,"BILL B.4. TOTAL:",{"$f":"SUM('BILL B.4.'!I9:I105)","v":{"v":5225000,"d":"5,225,000.00"}}]
["BILL B.5.","SECONDARY SEDIMENTATION TANK"]
["B.5.1","SECONDARY SEDIMENTATION TANK",{"$f":"SUM('BILL B.5.'!I9:I178)","v":{"v":105000,"d":"105,000.00"}}]
[null,"BILL B.5. TOTAL:",{"$f":"SUM('BILL B.5.'!I9:I178)","v":{"v":105000,"d":"105,000.00"}}]
["BILL B.6.","SLUDGE DRYING BEDS"]
["B.6.1","SLUDGE DRYING BEDS",{"$f":"SUM('BILL B.6.'!I9:I126)","v":{"v":5000,"d":"5,000.00"}}]
[null,"BILL B.6. TOTAL:",{"$f":"SUM('BILL B.6.'!I9:I126)","v":{"v":5000,"d":"5,000.00"}}]
["BILL B.7.","PUMP STATIONS"]
["B.7.1","RAW WATER AND IRRIGATION PUMP STATION EARTHWORKS ",{"$f":"SUM('BILL B.7.'!I9:I37)","v":{"v":5000,"d":"5,000.00"}}]
["B.7.2","RAW WATER PUMP STATION",{"$f":"SUM('BILL B.7.'!I38:I122)","v":{"v":1000000,"d":"1,000,000.00"}}]
["B.7.3","PUMP STATION (IRRIGATION)",{"$f":"SUM('BILL B.7.'!I123:I188)","v":{"v":0,"d":"0.00"}}]
["B.7.4","WASTE ACTIVATED SLUDGE (WAS) PUMP STATION",{"$f":"SUM('BILL B.7.'!I189:I280)","v":{"v":5000,"d":"5,000.00"}}]
["B.7.5","RAS PUMP STATION ALTERATION",{"$f":"SUM('BILL B.7.'!I281:I355)","v":{"v":5000,"d":"5,000.00"}}]
[null,"BILL B.7. TOTAL:",{"$f":"SUM('BILL B.7.'!I9:I355)","v":{"v":1015000,"d":"1,015,000.00"}}]
["BILL B.8.","CHLORINE CONTACT CHANNELS"]
["B.8.1","CHLORINE CONTACT CHANNEL",{"$f":"SUM('BILL B.8.'!I9:I17)","v":{"v":0,"d":"0.00"}}]
["B.8.2","CHLORINE CONTACT TANK INFLOW CHANNEL",{"$f":"SUM('BILL B.8.'!I18:I76)","v":{"v":0,"d":"0.00"}}]
[null,"BILL B.8. TOTAL:",{"$f":"SUM('BILL B.8.'!I9:I76)","v":{"v":0,"d":"0.00"}}]
["BILL C","ROADWORKS"]
["C1","ROADWORKS",{"$f":"SUM('BILL C'!I9:I107)","v":{"v":0,"d":"0.00"}}]
[null,"BILL C TOTAL:",{"$f":"SUM('BILL C'!I9:I107)","v":{"v":0,"d":"0.00"}}]
["BILL D.1.","MCC BUILDING"]
["D.1.1","MCC BUILDING ",{"$f":"SUM('BILL D.1.'!I9:I163)","v":{"v":630000,"d":"630,000.00"}}]
[null,"BILL D.1. TOTAL:",{"$f":"SUM('BILL D.1.'!I9:I163)","v":{"v":630000,"d":"630,000.00"}}]
["BILL D.2.","BLOWER BUILDING"]
["D.2.1","BLOWER BUILDING",{"$f":"SUM('BILL D.2.'!I9:I191)","v":{"v":600000,"d":"600,000.00"}}]
[null,"BILL D.2. TOTAL:",{"$f":"SUM('BILL D.2.'!I9:I191)","v":{"v":600000,"d":"600,000.00"}}]
["BILL D.3.","WORKSHOP BUILDING"]
["D.3.1","WORKSHOP BUILDING",{"$f":"SUM('BILL D.3.'!I9:I300)","v":{"v":500000,"d":"500,000.00"}}]
[null,"BILL D.3. TOTAL:",{"$f":"SUM('BILL D.3.'!I9:I300)","v":{"v":500000,"d":"500,000.00"}}]
["BILL D.4.","GUARD HOUSE"]
["D.4.1","GUARD HOUSE",{"$f":"SUM('BILL D.4.'!I9:I171)","v":{"v":100000,"d":"100,000.00"}}]
[null,"BILL D.4. TOTAL:",{"$f":"SUM('BILL D.4.'!I9:I171)","v":{"v":100000,"d":"100,000.00"}}]
["BILL D.5.","ADMIN BUILDING"]
["D.5.1","ADMIN BUILDING",{"$f":"SUM('BILL D.5.'!I9:I286)","v":{"v":850000,"d":"850,000.00"}}]
[null,"BILL D.5. TOTAL:",{"$f":"SUM('BILL D.5.'!I9:I286)","v":{"v":850000,"d":"850,000.00"}}]
["BILL D.6.","FeCL BUILDING"]
["D.6.1","FeCL BUILDING",{"$f":"SUM('BILL D.6.'!I9:I38)","v":{"v":300000,"d":"300,000.00"}}]
[null,"BILL D.6. TOTAL:",{"$f":"SUM('BILL D.6.'!I9:I38)","v":{"v":300000,"d":"300,000.00"}}]
["BILL D.7.","WAS PUMP STATION"]
["D.7.1","WAS PUMP STATION",{"$f":"SUM('BILL D.7.'!I9:I205)","v":{"v":62000,"d":"62,000.00"}}]
[null,"BILL D.7. TOTAL:",{"$f":"SUM('BILL D.7.'!I9:I205)","v":{"v":62000,"d":"62,000.00"}}]
["BILL D.8.","MISCELLANEOUS (BUILDINGS)"]
["D.8.1","MISCELLANEOUS",{"$f":"SUM('BILL D.8.'!I9:I30)","v":{"v":1232000,"d":"1,232,000.00"}}]
[null,"BILL D.8. TOTAL:",{"$f":"SUM('BILL D.8.'!I9:I30)","v":{"v":1232000,"d":"1,232,000.00"}}]
["BILL E","SOCIO ECONOMIC DEVELOPMENT"]
["E1","SOCIO ECONOMIC DEVELOPMENT",{"$f":"SUM('BILL E'!I9:I21)","v":{"v":0,"d":"0.00"}}]
[null,"BILL E TOTAL:",{"$f":"SUM('BILL E'!I9:I21)","v":{"v":0,"d":"0.00"}}]
[]
[null,"TENDER AMOUNT",{"$f":"+C12+C15+C23+C26+C29+C32+C35+C42+C46+C49+C52+C55+C58+C61+C64+C67+C70+C73+C76","v":{"v":104209000,"d":"104,209,000.00"}}]
[null,"ALLOWANCE FOR VAT AT 15%",{"$f":"C78*15%","v":{"v":15631350,"d":"15,631,350.00"}}]
[null,"TOTAL TENDER SUM",{"$f":"C79+C78","v":{"v":119840350,"d":"119,840,350.00"}}]