{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Threaded Rods","Deviation Schedule","Test Schedule"],"not_rendered":{"external_links":2,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Threaded Rods","index":0,"n_rows":104,"n_cols":7,"rows_kept":104,"merged":[[0,1,0,6],[1,3,1,5],[2,3,2,5],[2,7,2,9],[3,3,3,5],[4,3,4,5],[5,3,5,5],[7,4,7,5],[8,4,8,5],[9,4,9,5],[11,1,11,6],[12,1,12,6],[13,2,13,4],[14,2,14,3],[15,2,15,3],[16,2,16,3],[21,2,21,3],[22,3,22,4],[34,2,34,3],[44,8,44,9],[48,2,48,3],[63,2,63,3],[74,2,74,3],[77,2,77,3],[80,2,80,4],[81,2,81,4],[89,1,89,6],[90,1,90,6],[91,1,91,6],[93,2,93,6],[94,1,94,6],[96,0,96,1],[98,1,98,3],[98,5,98,6],[103,1,103,3],[103,5,103,6]],"flags":["formulas_cached_only"]}
[null,"ESKOM TENDER E2719DXLIMOU"]
[{"$nulls":3},"Technical Schedules A and B for:"]
[{"$nulls":3},"DDT-3015 - THREADED RODS WITH NUTS, WASHERS AND BONDING CLIPS(ASSEMBLED)"]
[{"$nulls":3},"NB! UNIQUE SHEDULES ARE TO BE COMPLETED PER SAP NUMBER LISTED BELOW"]
[{"$nulls":3},"NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS AND DOCUMENTS"]
[]
[]
[{"$nulls":3},"SAP Number","Technical Description "]
[{"$nulls":3},"0163865","ROD,THD:M20-2.5-6G;LG 600 MM"]
[]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[null,1,2,null,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"General information"]
[null,1.1,"Purchasing details"]
[null,"1.1.1",null,"Sap No","Select SAP number from list above",163865]
[null,"1.1.2",null,"Eskom drawing number",null,"D-DT-3015","xxxxxxxxxx"]
[null,"1.1.3",null,"Quantity of units required","Quantity","Batch Order"]
[]
[null,2,"Requirements",null,null,"Required"]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Manufacturer","Manufacturer name","Yes"]
[null,"2.1.2",null,"Supplier","Suppliers name","Yes"]
[null,"2.1.3",null,"Country of origin","Where manufactured.","Yes"]
[null,"2.1.4",null,"Local content","%","Yes"]
[null,"2.1.5",null,"Manufacturer's Product Code","Specify Code","Yes"]
[null,"2.1.6",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","Yes"]
[null,2.2,"·","Identification"]
[null,"2.2.1",null,"Manufacturer's Physical identification mark on product (Indelible marking)",null,"Yes"]
[null,2.3,"·","Supply"]
[null,"2.3.1",null,"Item supplied with curved washers, round flat washers, spring washers(Eskom D-DT 3014),hex nuts (Eskom D-DT 3173) and bonding clips (Eskom D-DT 3033) as required per SAP number.",null,"Yes"]
[]
[null,3,"Threaded Rods",null,null,"Required"]
[null,3.1,"·","Mechanical Properties"]
[null,"3.1.1",null,"Material Grade",null,"Grade 070M20 Steel"]
[null,3.2,"·","Compliance to all dimensions and requirements per SAP number (Buyer's Guide drawing DDT 3015)"]
[null,"3.2.1",null,"Diameter","mm","Yes"]
[null,"3.2.2",null,"Length","mm","Yes"]
[null,"3.2.3",null,"Chamfer","mm/deg","Yes"]
[null,"3.2.4",null,"Thread size / pitch","","Yes"]
[null,3.3,"·","Galvanising (If and as required per SAP number)."]
[null,"3.3.1",null,"Average minimum galvanizing coating thickness on product body to SANS 121. (Hot dip galvanising.)","SANS 121","Yes"]
[null,"3.3.2",null,"Corrosion specification - SANS 2081","SANS 2081","Yes"]
[null,3.4,"·","Electro Plating (If and as required per SAP number)."]
[null,"3.4.1",null,"Electro plated to SANS 2081 (ZINC).","SANS 2081 (ZINC)","Yes"]
[]
[null,4,"Nuts, washers and bonding clips."]
[null,4.1,"·","Nuts and washers"]
[null,"4.1.1",null,"Material - 240-47172520 [7.2.5 a)]","At least grade 6.8","Yes"]
[null,"4.1.2",null,"Galvanising - SANS 121 - 240-47172520 [7.2.5 a)]","SANS 121","Yes"]
[null,4.2,"·","Bonding clips"]
[null,"4.2.1",null,"Material - According to SAP number requirement - D-DT 3033","Mild steel or tinned copper or aluminium alloy.","Yes"]
[null,"4.2.2",null,"Galvanising - (Where required) - SANS 121 - D-DT 3033","SANS 121","Yes"]
[null,"4.2.3",null,"Hot dipped tinning - (Where required) - D-DT    3033","Coating thickness: 4 – 12 Microns","Yes"]
[null,"4.2.4",null,"Dimensions and hole size - D-DT 3033:"]
[null,"4.2.4.1",null,"Working length.","50mm","Yes"]
[null,"4.2.4.2",null,"Overall width.","40mm","Yes"]
[null,"4.2.4.3",null,"Inside diameter of loop.","7mm","Yes"]
[null,"4.2.4.4",null,"Material thickness","2mm","Yes"]
[null,"4.2.4.5",null,"Hole diameter.","22mm","Yes"]
[]
[null,5,"Testing",null,null,"Required","Report Number"]
[null,5.1,null,"Test Reports (where applicable)."]
[null,"5.1.1",null,"Thread pull test according to SANS 1700","Type test","YES"]
[null,"5.1.2",null,"Hot dip galvanizing (SANS 121)","Type and sample tests","YES"]
[null,"5.1.3",null,"Visual examination (SANS 61284)","Type tests","YES"]
[null,"5.1.4",null,"Dimensional and material verification (SANS 61284)","Type and sample tests","YES"]
[null,"5.1.5",null,"Hardness test (ASTM E92)","Type tests","YES"]
[null,"5.1.6",null,"Charpy V-Notch impact test (ASTM E23)","Type tests","YES"]
[null,"5.1.7",null,"Tensile test (ASTM E8)","Type tests","YES"]
[null,"5.1.8",null,"Torque test","Type tests","YES"]
[]
[null,6,"Packaging",null,null,"Required"]
[null,6.1,"·","Packaging"]
[{"$nulls":3},"As required per SAP number (DDT 3015)","DDT 3015","Yes"]
[null,7,"Quality Assurance",null,null,"Required"]
[null,7.1,null,"Quality Plan (including handling of non-conformances etc)","Quality plan.","Yes"]
[]
[null,8,"Documentation/ Samples (to be submitted with tender)"]
[null,null,"Note: All documentation to be provided in electronic format.",null,null,"Required"]
[null,8.1,"·","Required documentation:"]
[null,"8.1.1",null,"All documentation (drawings, letters, plans,gaurantees, test reports etc) as required above.","If required","YES"]
[]
[null,9,"·","Samples",null,"Required"]
[null,9.1,null,"One assembled sample to be supplied.","One","Yes"]
[]
[]
[null,"DEVIATION SCHEDULE MUST BE COMPLETED AND SIGNED."]
[null,"IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED THAT THE SUPPLIER AND MANUFACTURER FULLY"]
[null," COMPLIES WITH THE REQUIREMENTS OF THE ESKOM SPECIFICATION/S."]
[]
[null,null,"ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER / MANUFACTURER DETAILS"]
[]
[null,null,"         "]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":45,"n_cols":6,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,8,2,10],[3,0,3,6],[3,7,3,13],[3,14,3,20],[3,21,3,27],[3,28,3,34],[3,35,3,41],[3,42,3,48],[3,49,3,55],[3,56,3,62],[3,63,3,69],[3,70,3,76],[3,77,3,83],[3,84,3,90],[3,91,3,97],[3,98,3,104],[3,105,3,111],[3,112,3,118],[3,119,3,125],[3,126,3,132],[3,133,3,139],[3,140,3,146],[3,147,3,153],[3,154,3,160],[3,161,3,167],[3,168,3,174],[3,175,3,181],[3,182,3,188],[3,189,3,195],[3,196,3,202],[3,203,3,209],[3,210,3,216],[3,217,3,223],[3,224,3,230],[3,231,3,237],[3,238,3,244],[3,245,3,251],[3,252,3,255],[4,0,4,6],[4,7,4,13],[4,14,4,20],[4,21,4,27],[4,28,4,34],[4,35,4,41],[4,42,4,48],[4,49,4,55],[4,56,4,62],[4,63,4,69],[4,70,4,76],[4,77,4,83],[4,84,4,90],[4,91,4,97],[4,98,4,104],[4,105,4,111],[4,112,4,118],[4,119,4,125],[4,126,4,132],[4,133,4,139],[4,140,4,146],[4,147,4,153],[4,154,4,160],[4,161,4,167],[4,168,4,174],[4,175,4,181],[4,182,4,188],[4,189,4,195],[4,196,4,202],[4,203,4,209],[4,210,4,216],[4,217,4,223],[4,224,4,230],[4,231,4,237],[4,238,4,244],[4,245,4,251],[4,252,4,255],[5,0,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,0,35,6],[36,0,36,6],[40,1,40,2],[44,1,44,2]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation Schedule"]
["DDT-3015 - THREADED RODS WITH NUTS, WASHERS AND BONDING CLIPS(ASSEMBLED)"]
[]
["SAP No:  163865"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item(SAP no)","Clause","Description of Deviation"]
{"$rows_empty":27}
["ESKOM TENDER E2719DXLIMOU"]
[]
["SUPPLIER SIGNATURES"]
[]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[0,1,0,4],[1,1,1,4],[2,1,2,4],[3,0,3,6],[17,1,17,2],[18,1,18,4],[19,1,19,4],[22,1,22,2],[26,1,26,2]],"flags":["formulas_cached_only"]}
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"DDT-3015 - THREADED RODS WITH NUTS, WASHERS AND BONDING CLIPS(ASSEMBLED)"]
[null,"The test reports are required for the selected SAP number listed on this sheet"]
["SAP NO:  163865"]
[]
[null,1,2,3,4]
[null,"Item ","Description","Standard","Report No."]
[null,null,"Threaded Rods"]
[null,"4.1.1","Thread pull test according to SANS 1700 (Type test).","SANS 1700"]
[null,"4.1.2","Hot dip galvanizing - SANS 121 - (Type and sample test).","SANS 121 and 240-75655504 - [3.9.4.13.1]"]
[null,"4.1.3","Visual examination - SANS 61284 - (Type and sample test).","SANS 61284"]
[null,"4.1.4","Dimensional and material verification - SANS 61284 - (Type and sample test).","SANS 61284"]
[null,"4.1.5","Hardness test - ASTM E92 - (Type test).","ASTM E92 and 240-75883830 - [3.2.2.4]"]
[null,"4.1.6","Charpy V-Notch impact test - ASTM E23 - (Type test).","ASTM E23 and 240-75883830 - [3.2.2.2]"]
[null,"4.1.7","Tensile test - ASTM E8 - (Type test).","ASTM E8"]
[null,"4.1.8","Torque test - (Type test)."]
[]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,"Sign",null,null,"Date"]