BOQ FOR REPLACEMENT OF DAMAGED EAVES CEILING TO STP MAIN BUILDING
Item no	Description	Unit	Qty	Rate	Amount
NOTES:
Submission of a safety file is compulsory only to the appointed bidder. No work will be executed until this requirement is met.
Preliminaries and General
1	Allow for preliminaries and general for the duration of the project (contractors will be required to breakdown their preliminaries items)	item	1
2	Scaffolding, carting away of access material Provision of scaffolding to be used during the removal and installation of new ceiling	Item	1
Preparation and submission of a health and safety file
3	Prepare and submit a safety file as per the appendix from SENTECH Safety office (the file will be submitted by the successful bidder after appointment to the office of the OHS Specialist). Demolitions and Alterations	Item	1
4	Carefully remove existing gutters and downpipes (set downpipes aside for re-use. supply new gutters size 75mm x 100mm x 0.4mm	m	170
5	Replace damaged ceiling on eaves and cornices (quadrant beads). Ceiling on eaves to be suitable for exterior and moisture resistance board.	M2	297
6	CEILING KU BAND Remove existing damaged ceiling bords, branderings and supply new ceiling boards. Supply branderings 38mm x 38mm with nails and including all sundries KU and Main Building.	M2 M	18 170
7	Supply and fix facia boards to match the existing	M	20
CARPENTRY AND JOINERY
PAINTWORK TO EXISTING WORKS
Prepare and brush to remove all loose contaminants and apply two coats paint:
8	On ceilings, facias and barge boards (with water damages / new ceiling)	M2	315
Apply one coats 'High Gloss Alkyd Enamel' paint on steel:
9	On down pipes and gutters	m	80
Carried to Summary

LIST OF SIMILAR PROJECTS

Project Name	Client Name	Client Contactable Reference	Project Duration
Name: Contact No:	From	To
Name: Contact No:
Name: Contact No:
Name: Contact No:
Name: Contact No:
Name: Contact No:
Name: Contact No:
Name: Contact No: