{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Schedule A B CT SB2"],"not_rendered":{"external_links":2,"defined_names":106},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Schedule A B CT SB2","index":0,"n_rows":78,"n_cols":13,"rows_kept":78,"merged":[[16,0,16,5],[17,0,17,5]],"flags":["formulas_cached_only"]}
[" TECHNICAL SPECIFICATION FOR Calibration 9103/9140 Field Dry-Well "]
[]
[null,"Appendix A: Technical Schedules"]
["Schedule A and Schedule B provide technical details against tendered equipment/Supplier’s statement of compliance or non-compliance. The tenderer is requested "]
["to complete this Schedule A/B as part of the tender submission data package."]
[]
["When completing the Schedule A/B, the tenderer is requested to take cognisance of the following:"]
[]
["It is expected of the tenderer to state clearly, for each clause that requires a statement of compliance in the Schedule A/B, either “Comply” or “Do Not Comply”. "]
["The Tenderer shall provide detailed evidence for each answer specifically stating the exact location of the evidence in the supporting documentation i.e document "]
["name and reference, page number, paragraph number."]
[]
["If a clause in the Schedule A/B requires information only, e.g. describe application etc. The tenderer is at liberty to provide any information deemed appropriate."]
[]
["SCHEDULE A : PURCHASER'S PARTICULAR REQUIREMENT                     SCHEDULE B: THE TENDERER'S COMPLIANCE"]
["Technical scoring methodology: "]
["COMPLIANT  [Meet the technical requirement(s) AND,  No foreseen technical risk(s) in meeting technical requirements  &Manual technical specification manual submitted]"]
["NON-COMPLIANT [Does not meet the technical requirement(s) AND/OR Unacceptable technical risk(s) AND/OR;  Unacceptable exceptions AND/OR;  Unacceptable conditions]  "]
[]
[]
[]
["Clause No","Description of Clause","Schedule A \n(Purchaser's Particular Requirement)","Weight","Schedule B Compliance","Clause Score","Total Score","Schedule B Compliance","Clause Score","Total Score","Schedule B Compliance","Clause Score","Total Score"]
[4,"FUNCTIONAL REQUIREMENTS","Stated for Information only"]
[4.1,"9103 Specifications  requirements","Stated for Information only "]
[null,"The device shall meet the following :","State Compliance"]
["4.1.1","Range: –25°C to 140°C (–13°F to 284°F) at 23°C ambient","State Compliance",3]
["4.1.2","Accuracy: ±0.25°C (holes greater than 1/4\" [6.35mm]:±1°C)","State Compliance",3]
["4.1.3","Mains fuses :2 x T 2.0 AH 250 V (high-breaking capacity wire fuse 5 x 20 mm)","State Compliance",3]
["4.1.4","Stability: ±0.02°C at –25°C ±0.04°C at 140°C","State Compliance",3]
["4.1.5","Well-to-well uniformity ±0.1°C between similarly sized wells","State Compliance",3]
["4.1.6","Heating times 18 minutes from ambient to 140°C","State Compliance",3]
["4.1.7","Cooling times 20 minutes from ambient to –25°C","State Compliance",3]
["4.1.8","Stabilization time 7 minutes","State Compliance",3]
["4.1.9","Immersion depth 124 mm (4.875 in)","State Compliance",3]
["4.1.10","Computer interface RS-232 included with free Interface-it software (Model 9930)","State Compliance",3]
["4.1.11","Inserts Insert A, B, C, or D included (specify when ordering)","State Compliance",3]
["4.1.12","Power 115 V AC (±10%), 1.3 A or 230 V AC (±10%), 0.7 A, switchable, 50/60 Hz, 150 W","State Compliance",3]
["4.1.13","Size (W x H x D) 143 x 261 x 245 mm (5.63 x 10.25 x 9.63 in)","State Compliance",3]
["4.1.14","Weight 5.7 kg (12 lb)","State Compliance",2]
["4.1.15","NIST-traceable certificate Data at –25°C, 0°C, 25°C, 50°C, 75°C, 100°C, and 140°","State Compliance",3]
[4.2,"9140 Specifications  requirements","Stated for Information only "]
[null,"The device shall meet the following :","State Compliance"]
["4.1.1","Range: 35°C to 350°C (95°F to 662°F)","State Compliance",3]
["4.1.2","Accuracy: ±0.5°C (holes greater than 1/4\" [6.35mm]: ±1°C)","State Compliance",3]
["4.1.3","Mains fuses :2 x T 2.0 AH 250 V (high-breaking capacity wire fuse 5 x 20 mm)","State Compliance",3]
["4.1.4","Stability:±0.03°C at 50°C ±0.05°C at 350°C","State Compliance",3]
["4.1.5","Well-to-well uniformity ±0.1°C with similarly sized wells","State Compliance",3]
["4.1.6","Heating times 12 minutes from ambient to 350°C","State Compliance",3]
["4.1.7","Cooling times 15 minutes from 350°C to 100°C","State Compliance",3]
["4.1.8","Stabilization time 7 minutes","State Compliance",3]
["4.1.9","Immersion depth 124 mm (4.875 in)","State Compliance",3]
["4.1.10","Computer interface RS-232 included with free Interface-it software (Model 9930)","State Compliance",3]
["4.1.11","Inserts Insert A, B, C, or D included (specify when ordering)","State Compliance",3]
["4.1.12","Power 115 V AC (±10%), 4.4 A or 230 V AC (±10%), 2.2 A, switchable, 50/60 Hz, 500 W","State Compliance",3]
["4.1.13","Size (W x H x D)152 x 86 x 197 mm (6 x 3.375 x 7.75 in)","State Compliance",3]
["4.1.14","Weight 2.7 kg (6 lb)","State Compliance",2]
["4.1.15","NIST-traceable certificate Data at 50°C, 100°C, 150°C, 200°C, 250°C, 300°C, and 350°C","State Compliance",3]
[5,"General Specification","Stated for Information only                 "]
[5.1,"Software License","Stated for Information only                 "]
["5.1.1","The Supplier shall provide an enterprise software license, if any, for all software provided with the Calibration 9103/9140 Field Dry-Well for use by the Purchaser.","State Compliance         ",3]
[5.2,"Documentation","Stated for Information only                 "]
["5.2.1","The Supplier shall supply a complete set of documentation. Such documentation shall enable Purchaser’s personnel to perform maintenance on the Calibration 9103/9140 Field Dry-Well . The documentation shall include the following:","State Compliance          "]
["5.2.1.1","Manuals","State Compliance          ",2]
["5.2.2","Manuals shall include the following:","State Compliance          "]
["5.2.2.1","Hard copy of  manuals with all the mechanical, electrical and environmental specifications of  the unit","State Compliance          ",1]
["5.2.3","All documents shall be supplied in English Language.","State Compliance          ",1]
["5.2.4","All documents shall be supplied in a digital format and hard copy format and shall be available on the internet.","State Compliance          ",1]
[5.6,"Quality Assurance","Stated for Information only                 "]
["5.6.1","Eskom’s Quality Assurance requirements as specified in ISO 9001:2015 are applicable.","State Compliance          ",1]
[]
[]
[null,"Signature:   ________________________________"]
[]
[null,"Print Name: ________________________________"]
[]
[null,"Company:   ________________________________"]
[]
[null,"Date:          ________________________________"]