{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["T5BD","T5BS"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"T5BD","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[3,3,3,6],[4,4,4,5],[48,0,48,6]]}
[]
[]
[]
["Vehicle Job Description:",null,null,"Required to carrying Goods, equipment and passengers up to a GVM of 19000 kg on all types of road surfaces with up to 80% off road usage.."]
["T5BD \nDual wheel\n ",null,null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to compleate"]
["Vehicle Type Required:",null,"RATING","Medium Truck 4x4 >16000 <19000GVM (Duel wheel application)","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)",1,null,"To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD)",1,null,"To be Standard"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM",2,null,"To be Standard"]
["ABS BRAKES",2,null,"To be Standard"]
["POWER STEERING",2,null,"To be Standard"]
["DAY RUN LIGHTS INSTALLED",1,null,"To be Standard"]
["TWO EMMERGENCY TRIANGLES",1,null,"To be Standard"]
["IMMOBILISER (Factory Warranty)",1,null,"To be Standard"]
["ALARM (Factory Warranty)",1,null,"To be Standard"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)",1,null,"To be Standard"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ",2,null,"To be Standard"]
["ENGINE PROTECTION DEVICE ",2,null,"To be Standard"]
["TRAILER BRAKE CONTROL",1,null,"To be Standard"]
["AIR CHARGE LINE TO THE FRONT",1,null,"To be Standard"]
["REVERSE ALARM/BEEPER",1,null,"To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT",1,null,"To be Standard"]
["VEHICLE CONFIGURATION :",2,null,"Medium Truck 4x4 >16000 <19000GVM (Duel wheel application)"]
["TRACTION: ",1,null,"4x4"]
["Diesel Powered (Normally aspirated or Turbo)",1,null,"YES"]
["Power Rating - Kw",2,null,"160Kw"]
["Torque Rating - NM",2,null,"850Nm"]
["Permissible Front axle rating “ Max.”",1,null,"7500kg"]
["Permissible Rear axle rating “ Max.”",1,null,"9000kg"]
["D/T Rating “Min.”",1,null,"21000Kg"]
["Wheel base “ Max.”",1,null,"4500mm and 4800mm "]
["Chassis to facilitate the fitting of 18Tm hydraulic crane ",2,null,"YES"]
["Automatic Gearbox",1,null,"YES"]
["Fully synchromesh Gearbox",1,null,"YES"]
["Independent transfer box (4x4)",1,null,"YES"]
["Gear ratio: Top gear 1:1 ",1,null,"YES"]
["Gear ratio: Lowest gear higher than 8:1",1,null,"YES"]
["Top speed of  vehicle max 100kmph (determine by gear ratio, no electronic speed limiters allowed)",1,null,"YES"]
["Power assisted Steering",1,null,"YES"]
["Seat Belts: SABS approved",2,null,"YES"]
["Tyres (Size) 11 R 22.5. (up to 80% off road usage) Compatible diff ratio",1,null,"YES"]
["Number of gears, manual",1,null,"YES"]
["Mud-flaps: Factory fitted",1,null,"YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE",2,null,"Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km",1,null,"Specify"]
["Acceptance / Acceptance",50,{"$f":"SUM(C7:C45)","v":0}]
["Name of Evaluator : ",{"$nulls":3},"Signature :"]
["Name of Verifier",{"$nulls":3},"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",null,null,100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",null,null,50]
["Original Equipment manufacturer (OEM) or registered dealer",null,null,20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",null,null,20]
["Proof of after sales service and repairs (OEM Service Level Agreement) ",null,null,10]

{"sheet":"T5BS","index":1,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[3,3,3,6],[4,4,4,5],[48,0,48,6]]}
[]
[]
[]
["Vehicle Job Description:",null,null,"Required to carrying Goods, equipment and passengers up to a GVM of 19000 kg on all types of road surfaces with up to 80% off road usage.."]
["T5BS \nSingle Wheel\n ",null,null,"Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to compleate"]
["Vehicle Type Required:",null,"RATING","Medium Truck 4x4 >16000 <19000GVM (Single Wheel application)","Comply (YES/No)","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)",1,null,"To be Standard"]
["RADIO/CD PRICE FITTED (IF NOT STD)",1,null,"To be Standard"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM",2,null,"To be Standard"]
["ABS BRAKES",2,null,"To be Standard"]
["POWER STEERING",2,null,"To be Standard"]
["DAY RUN LIGHTS INSTALLED",1,null,"To be Standard"]
["TWO EMMERGENCY TRIANGLES",1,null,"To be Standard"]
["IMMOBILISER (Factory Warranty)",1,null,"To be Standard"]
["ALARM (Factory Warranty)",1,null,"To be Standard"]
["WHEEL BASE EXTENTION IF NEEDED (PRICE FITTED IF NOT STD)",1,null,"To be Standard"]
["PTO Suitable for a 21Tm crane (PRICE FITTED IF NOT STD) ",2,null,"To be Standard"]
["ENGINE PROTECTION DEVICE ",2,null,"To be Standard"]
["TRAILER BRAKE CONTROL",1,null,"To be Standard"]
["AIR CHARGE LINE TO THE FRONT",1,null,"To be Standard"]
["REVERSE ALARM/BEEPER",1,null,"To be Standard"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT",1,null,"To be Standard"]
["VEHICLE CONFIGURATION :",2,null,"Medium Truck 4x4 >16000 <19000GVM (Single Wheel application)"]
["TRACTION: ",1,null,"4x4"]
["Diesel Powered (Normally aspirated or Turbo)",1,null,"YES"]
["Power Rating - Kw",2,null,"160Kw"]
["Torque Rating - NM",2,null,"850Nm"]
["Permissible Front axle rating “ Max.”",1,null,"7500kg"]
["Permissible Rear axle rating “ Max.”",1,null,"8000kg"]
["D/T Rating “Min.”",1,null,"21000Kg"]
["Wheel base “Min and Max.”",1,null,"4500mm and 4800mm "]
["Chassis to facilitate the fitting of 18Tm hydraulic crane ",2,null,"YES"]
["Automatic Gearbox",1,null,"YES"]
["Fully synchromesh Gearbox",1,null,"YES"]
["Independent transfer box (4x4)",1,null,"YES"]
["Gear ratio: Top gear 1:1 ",1,null,"YES"]
["Gear ratio: Lowest gear higher than 8:1",1,null,"YES"]
["Top speed of  vehicle max 100kmph (determine by gear ratio, no electronic speed limiters allowed)",1,null,"YES"]
["Power assisted Steering",1,null,"YES"]
["Seat Belts: SABS approved",2,null,"YES"]
["Tyres (Size) 1400R20 Steel radial Tyres (Michelin XZL)  (up to 80% off road usage) Compatible diff ratio",1,null,"YES"]
["Number of gears, manual",1,null,"YES"]
["Mud-flaps: Factory fitted",1,null,"YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE",2,null,"Specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km",1,null,"Specify"]
["Acceptance / Acceptance",50,{"$f":"SUM(C7:C45)","v":0}]
["Name of Evaluator : ",{"$nulls":3},"Signature :"]
["Name of Verifier",{"$nulls":3},"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Technical Evaluation Criteria",null,null,100]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",null,null,50]
["Original Equipment manufacturer (OEM) Letter or registered dealer",null,null,20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",null,null,20]
["Proof of after sales service and repairs (OEM Service Level Agreement) ",null,null,10]