{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":4,"n_cols":6,"rows_kept":4,"merged":[[0,0,0,5]]}
["Annexure A – Schedule of Compliance for Live Line Services 420-520mm Conductor Carts"]
["Item","Description of Equipment","Schedule A - Returnable by Tenderer","Datasheet/Specification (Yes/No)","Certificate\n(Yes/No or N/A)","Compliant/Non-Compliant"]
[1,"CART: TYPE: CONDUCTOR; DIMENSIONS: WD 786 X LG 975 X HT 1156 MM; CAPACITY: 300 KG; DRAWING NO: LLD-AS-001; SPECIFICATION: SANS 3834-2: 2006; SANS 3834-5: 2006; ASSEMBLED; WHEEL SPACING LENGTH RANGE: 420–520 MM WITHOUT MIDDLE WHEELS; CERTIFY WELDS AND CAPACITY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Provide Correct Evidence & State Compliance (Material data sheets, Specifications or Certifications of items listed on drawing sheet)."]
[2,"CART: TYPE: CONDUCTOR; DIMENSIONS: WD 786 X LG 975 X HT 1728 MM; CAPACITY: 300 KG; DRAWING NO: LLD-AS-003; SPECIFICATION: SANS 3834-2: 2006; SANS 3834-5: 2006; ASSEMBLED; WHEEL SPACING LENGTH RANGE: 420–520 MM WITHOUT MIDDLE WHEELS; WITH TOP WHEEL BUNDLE SUPPORT; CERTIFY WELDS AND CAPACITY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","Provide Correct Evidence & State Compliance (Material data sheets, Specifications or Certifications of items listed on drawing sheet)."]