{"text_format":"3","workbook":"xls","n_sheets":20,"sheets":["1-1 BILL NO. 1","1-2 BILL NO. 2","1-3 BILL NO. 3","1-4 BILL NO. 4","1-5 BILL NO. 5","1-6 BILL NO. 6","1-7 BILL NO. 7","1-8 BILL NO. 8","1-9 BILL NO. 9","1-10 BILL NO.10","1-11 BILL NO. 11","1-12 BILL NO. 12","1-13 BILL NO. 13","1-14 BILL NO. 14","1-15 BILL NO. 15","1-16 BILL NO. 16","1-17 BILL NO. 17","1-18 BILL NO. 18","1-19 BILL NO. 19","1-20 Summary"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1-1 BILL NO. 1","index":0,"n_rows":6,"n_cols":7,"rows_kept":6,"flags":["formulas_cached_only"]}
["04:05:23","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["18","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"",""]
["18","","PRELIMINARIES","H1",{"v":0,"d":"0.0"},"",""]
["18","1/1","A1.0\tDefinitions and Interpretation (Clause 1.0)  F: ___________ V: ____________ T:____________ ","Item",{"v":1,"d":"1.00"},"",""]

{"sheet":"1-2 BILL NO. 2","index":1,"n_rows":82,"n_cols":7,"rows_kept":82,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE"]
["19","","BILL NO. 2","H1",{"v":0,"d":"0.0"},"",""]
["19","","ALTERATIONS (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"",""]
["19","","(CPAP WORK GROUP 102 UNLESS OTHERWISE STATED)","H2",{"v":0,"d":"0.0"},"",""]
["19","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"",""]
["19","","TEMPORARY BARRIERS, SCREENS, ETC","H2",{"v":0,"d":"0.0"},"",""]
["19","","Temporary barriers, screens, etc including removal.","H3",{"v":0,"d":"0.0"},"",""]
["19","2/1","Dry wall barrier 2700mm high formed of galvanised steel channel section rails and studs covered on one side, with 12,7mm gypsum board panels and finished with two coats interior quality PVA emulsion paint on one side including corners, ends, etc.","m",75,"",""]
["19","2/2","Dry wall barrier 3000mm high formed of galvanised steel channel section rails and studs covered on one side, with 12,7mm gypsum board panels and finished with two coats interior quality PVA emulsion paint on one side including corners, ends, etc.","m",75,"",""]
["19","2/3","Dry wall barrier 3500mm high formed of galvanised steel channel section rails and studs covered on one side, with 12,7mm gypsum board panels and finished with two coats interior quality PVA emulsion paint on one side including corners, ends, etc.","m",75,"",""]
["19","2/4","Security and safety warning tapes and signage to enclose the Works where necessary","Item",{"v":1,"d":"1.00"},"",""]
["19","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"",""]
["19","","Breaking down and removing brickwork including finishes etc (in accordance with Engineers instruction)","H3",{"v":0,"d":"0.0"},"",""]
["19","2/5","Half brick wall internally","m2",122,"",""]
["19","","Taking down Faggots","H3",{"v":0,"d":"0.0"},"",""]
["19","2/6","Taking down faggots from balcony","m2",86,"",""]
["20","","Taking out doors, windows, etc including thresholds, sills, etc and handing to employer (building up openings elsewhere)","H3",{"v":0,"d":"0.0"},"",""]
["20","2/7","Timber single door and frame not exceeding 2,5m2 from half brick wall","No",27,"",""]
["20","2/8","Remove existing sunscreens 3990 x 2103mm width overall fixed from one brick wall.","m2",16,"",""]
["20","","Taking down and removing roofs, floors, ceilings, partitions, etc and cart away unless otherwise described","H3",{"v":0,"d":"0.0"},"",""]
["20","2/9","Double roman concrete roof tile","m2",998,"",""]
["20","2/10","Corrugated iron roof covering and purlins","m2",257,"",""]
["20","2/11","Plasterboard ceilings including  timber brandering, insulation, etc.","m2",240,"",""]
["20","2/12","Rainwater gutters complete with fixings","m",245,"",""]
["20","2/13","Rainwater downpipes complete with fixings","m",13,"",""]
["20","2/14","Timber moulded cornices (Provisional)","m",250,"",""]
["20","","Taking out and removing joinery fittings etc and cart away","H3",{"v":0,"d":"0.0"},"",""]
["20","2/15","Rectangular kitchen floor cupboards1200x 600 x 650mm high.","No",1,"",""]
["20","","Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screeds, plaster, etc and cart away","H3",{"v":0,"d":"0.0"},"",""]
["20","2/16","Vinyl tiles from floors","m2",169,"",""]
["20","","Hacking up/off and removing ceramic,clay tile floor and wall finishes including removing mortar bed or backing and cart away","H3",{"v":0,"d":"0.0"},"",""]
["20","2/17","Ceramic tiles to floors","m2",174,"",""]
["20","2/18","Clay tiles to verandah floors.","m2",415,"",""]
["21","","Taking out and removing piping, sanitary fittings, etc including disconnecting piping from fittings and making good floor and wall finishes (making good tiling and paintwork elsewhere) and handover to Employer","H3",{"v":0,"d":"0.0"},"",""]
["21","2/19","Viterous china wash hand double basin complete with water supplies and drainage","No",16,"",""]
["21","2/20","Viterious china single wash hand basin complete water supplies and drainage","No",15,"",""]
["21","2/21","Vitreous china WC suite complete with water supplies and drainage","No",25,"",""]
["21","2/22","male urinal system with drainage","No",4,"",""]
["21","2/23","Taking out and remove 5100 x 2105mm steel barglar bars,  make good on balcony and set aside for reuse","No",4,"",""]
["21","","Repair structural crack in plastered brick or concrete surfaces by hacking out plaster 150mm wide, opening crack completely, repairing underlay brickwork/concrete, fixing chicken wire mesh over crack, filling with \"Crackfiller\" ,etc and leave it ready for painting (painting elsewhere measured):","H3",{"v":0,"d":"0.0"},"",""]
["21","2/24","Escape staircase prepare cracked surface on the internal wall to receive approved epoxy crack sealer, apply 2 coats of enamel paint, colour to match existing","m2",92,"",""]
["21","","Vacuum and clean with system cleaner. Allow to dry as per specialist.","H3",{"v":0,"d":"0.0"},"",""]
["21","2/25","On carpet floors","m2",2277,"",""]
["21","","Ceramic tiles.Use approved non-abrasive cleaning agent and mild cleaner.","H3",{"v":0,"d":"0.0"},"",""]
["21","2/26","On walls","m2",707,"",""]
["21","2/27","On floors","m2",148,"",""]
["21","","Red clay tiles.Use an approved non-abrasive cleaning agent and mild cleaner.","H3",{"v":0,"d":"0.0"},"",""]
["21","2/28","On floors and landings","m2",415,"",""]
["22","","Light blasting for removal of efflorescence.Allow surface to dry well and use a stiff brush,then wash with water.","H4",{"v":0,"d":"0.0"},"",""]
["22","2/29","On external face brick walls","m2",636,"",""]
["22","","BUILDING UP OPENING","H2",{"v":0,"d":"0.0"},"",""]
["22","","Brickwork in NFP bricks in class II mortar in building up openings.","H3",{"v":0,"d":"0.0"},"",""]
["22","2/30","half brick walls. (Provisional)","m2",20,"",""]
["22","2/31","One brick walls. (Provisional)","m2",45,"",""]
["22","","VERANDA FLOOR DRAIN","H3",{"v":0,"d":"0.0"},"",""]
["22","","PREPARATORY WORK TO EXISTING SURFACES","H2",{"v":0,"d":"0.0"},"",""]
["22","2/32","Prepare existing veranda floor to receive new carpet tiles (elsewhere measured)","m2",415,"",""]
["22","2/33","Strip existing waterproofing and prepare slab to receive new torched on waterproofing (elsewhere measured)","m2",73,"",""]
["22","2/34","Prepare underside of balcony slab to receive new finish","m2",86,"",""]
["22","","MAKING GOOD OF FINISHES ETC","H2",{"v":0,"d":"0.0"},"",""]
["22","2/35","Making good defects in existing screeded floors with \"Pavelite\"","m2",589,"",""]
["22","2/36","Floor screeds in patches","m2",7,"",""]
["22","2/37","Walls where 110mm thick brick walls are removed","m",26,"",""]
["22","2/38","Floors where 110 brick walls removed","m",44,"",""]
["22","2/39","Walls in patches","m2",4,"",""]
["22","","Making good staircase and landings including balustrades","H3",{"v":0,"d":"0.0"},"",""]
["22","2/40","Brush off any lose rust using wire brush, wipe cleaning with methylated spirit, prepare with metal( rust inhibitive primer) and apply 2 coats of acrylic gloss enamel paint.","m2",365,"",""]
["23","","Breaking out for and forming openings through brick walls for new doors and frames including necessary precast concrete lintels and making good plaster on one side and into reveals and face brickwork on other side and into reveals and with ? concretethresholds with steel trowelled finish (new doors and frames and making good paintwork elsewhere)","H3",{"v":0,"d":"0.0"},"",""]
["23","2/41","Opening 3800 x 3700mm high through one brick wall","No",1,"",""]
["23","2/42","Opening for door with steel frame 1350 x 2040mm high overall through one brick wall","No",2,"",""]
["23","","Sundries","H2",{"v":0,"d":"0.0"},"",""]
["23","","Wash down with sugar soap, allow to dry and apply one coats brick seal","H3",{"v":0,"d":"0.0"},"",""]
["23","2/43"," On external face brick walls","m2",523,"",""]
["23","2/44","All veranda floor drain must be cleaned and flushed","No",3,"",""]
["23","","Fumigation","H2",{"v":0,"d":"0.0"},"",""]
["23","","Roof ","H3",{"v":0,"d":"0.0"},"",""]
["23","2/45","Roof to be fumigated according to SANS 10204:2006 regulations or latest additions","m2",998,"",""]
["23","","Cleaning and unblocking of box gutters and donwpipes","H3",{"v":0,"d":"0.0"},"",""]
["23","2/46","250 x 250 mm Aluminium box gutters in the executive block","m",86,"",""]
["23","2/47","Aluminium down pipes complete in the executive block","m",26,"",""]

{"sheet":"1-3 BILL NO. 3","index":2,"n_rows":43,"n_cols":7,"rows_kept":43,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["24","","BILL NO. 3","H1",{"v":0,"d":"0.0"},"",""]
["24","","MASONRY (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"",""]
["24","","(CPAP WORK GROUP NO. 116)","H2",{"v":0,"d":"0.0"},"",""]
["24","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"",""]
["24","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"",""]
["24","","BRICKWORK","H2",{"v":0,"d":"0.0"},"",""]
["24","","Sizes in descriptions","H3",{"v":0,"d":"0.0"},"",""]
["24","","Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick","",{"v":0,"d":"0.0"},"",""]
["24","","Hollow walls etc ","H3",{"v":0,"d":"0.0"},"",""]
["24","","Descriptions of hollow walls shall be deemed to include leaving every fifth perpend of the bottom course of the external skin open as a weep hole. ","",{"v":0,"d":"0.0"},"",""]
["24","","Walls in two skins described as \"bagged and sealed\" shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture and sealed with two coats \"Brixeal\" bitumen emulsion waterproofing coating.","",{"v":0,"d":"0.0"},"",""]
["24","","User note: ","H3",{"v":0,"d":"0.0"},"",""]
["24","","The above preamble generally applies for works in hot and humid coastal areas","",{"v":0,"d":"0.0"},"",""]
["24","","Face bricks ","H3",{"v":0,"d":"0.0"},"",""]
["24","","Bricks shall be ordered timeously to obtain uniformity in size and colour","",{"v":0,"d":"0.0"},"",""]
["24","","Pointing ","H3",{"v":0,"d":"0.0"},"",""]
["24","","Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc","",{"v":0,"d":"0.0"},"",""]
["25","","BLOCKWORK","H2",{"v":0,"d":"0.0"},"",""]
["25","","Concrete masonry units","H3",{"v":0,"d":"0.0"},"",""]
["25","","Blocks are to be either solid or hollow modular dense concrete masonry units having a compressive strength of 7 MPa","",{"v":0,"d":"0.0"},"",""]
["25","","Wall ties for blockwork","H3",{"v":0,"d":"0.0"},"",""]
["25","","Wall ties shall be polypropylene \"Permaties\" complying with BS 76377.  Ties for hollow walls shall be of sufficient length to allow not less than 75mm of each end to be built into the blockwork.  Ties are to be spaced at intervals of not more than 1m in the horizontal direction and not more than 400mm staggered in the vertical direction except at openings, vertical joints or ends of walls where they are to be placed vertically above each other","",{"v":0,"d":"0.0"},"",""]
["25","","Blockwork ","H3",{"v":0,"d":"0.0"},"",""]
["25","","Blockwork shall comply with SABS 0145 \"Concrete Masonry Construction\" ","",{"v":0,"d":"0.0"},"",""]
["25","","Surfaces to be plastered shall have joints raked out to a depth of at least 10mm to provide a key.  Cavities of hollow walls shall be kept free of mortar droppings or other undesirable matter. Every second perpend of the bottom course of the external skin of hollow walls shall be left open as a weep hole","",{"v":0,"d":"0.0"},"",""]
["25","","Standard complementary blocks","H3",{"v":0,"d":"0.0"},"",""]
["25","","Descriptions of blockwork shall be deemed to include standard complementary blocks such as corner, three-quarter, half and quarter blocks required in the construction of corners, reveals, jambs, ends, etc to solid and hollow walls and for bonding as necessary","",{"v":0,"d":"0.0"},"",""]
["25","","DECORATIVE BLOCKS","H2",{"v":0,"d":"0.0"},"",""]
["25","","Blocks shall be of approved manufacture, sound, well burnt or cured and uniform and true in size, shape and colour","",{"v":0,"d":"0.0"},"",""]
["26","","SAMPLES","H2",{"v":0,"d":"0.0"},"",""]
["26","","Samples of all masonry building units, except those for walls described as \"load bearing\", shall consist of a minimum of 6 units.  Samples of building units to be used in walls described as \"load bearing\" shall consist of 30 units from every 30 000 units delivered to site","",{"v":0,"d":"0.0"},"",""]
["26","","BRICKWORK IN FOUNDATIONS (PROVISIONAL)","H2",{"v":0,"d":"0.0"},"",""]
["26","","Brickwork of NFP bricks in class II mortar","H3",{"v":0,"d":"0.0"},"",""]
["26","","Load bearing brickwork of 14MPa bricks in class II mortar to SABS 0164","H3",{"v":0,"d":"0.0"},"",""]
["26","3/1","Half brick walls","m2",51,"",""]
["26","3/2","One brick walls","m2",19,"",""]
["26","","BRICKWORK SUNDRIES","H2",{"v":0,"d":"0.0"},"",""]
["26","","Brickwork sundries","H3",{"v":0,"d":"0.0"},"",""]
["26","3/3","230mm Brick cills set sloping and slightly projecting or equally approved match to existing one.Colour to Architect","m",69,"",""]
["26","3/4","10 x 150mm wide slate grey fibre-cement cills in single lengths,set flat and slight or equally approved match to existing one. Colour to Architect.","m",69,"",""]

{"sheet":"1-4 BILL NO. 4","index":3,"n_rows":17,"n_cols":8,"rows_kept":17,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["27","","BILL NO. 4","H1",{"v":0,"d":"0.0"},"","",""]
["27","","WATERPROOFING (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["27","","(CPAP WORK GROUP NO. 120)","H2",{"v":0,"d":"0.0"},"","",""]
["27","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["27","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["27","","All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South African National Standards' (SANS) shall apply ","",{"v":0,"d":"0.0"},"","",""]
["27","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["27","","Waterproofing","H3",{"v":0,"d":"0.0"},"","",""]
["27","","Waterproofing of roofs, basements, etc shall be laid under a ten year guarantee.  Waterproofing to roofs shall be laid to even falls to outlets etc with necessary ridges, hips and valleys. Descriptions of sheet or membrane waterproofing shall be deemed to include additional labour to turn-ups and turn-downs","",{"v":0,"d":"0.0"},"","",""]
["27","","WATERPROOFING TO ROOFS, BASEMENTS, ETC","H2",{"v":0,"d":"0.0"},"","",""]
["27","","Apply bitumein primer.Apply one layer of 4mm torch on waterproofing membrane finished with 2 coats of bitumen aluminium paint done to manufactures specification.","H3",{"v":0,"d":"0.0"},"","",""]
["27","4/1","On concrete roof slab","m2",73,"","",""]
["27","","Protective stone dressing balast","H3",{"v":0,"d":"0.0"},"","",""]
["27","4/2","20-30mm round stone ballast","m2",73,"","",""]

{"sheet":"1-5 BILL NO. 5","index":4,"n_rows":22,"n_cols":8,"rows_kept":22,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["28","","BILL NO. 5","H1",{"v":0,"d":"0.0"},"","",""]
["28","","ROOF COVERINGS ETC (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["28","","(CPAP WORK GROUP NO. 124)","H2",{"v":0,"d":"0.0"},"","",""]
["28","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["28","","SLATES","H2",{"v":0,"d":"0.0"},"","",""]
["28","","Double roman concrete tiles 420 x 332mm laid straight bond to flat slope 35 degrees, fixed to battens at 354mm battens centre on and including Marley or equal approved non permeable undertile membrane","H3",{"v":0,"d":"0.0"},"","",""]
["28","5/1","Roof covering with pitch not exceeding 25 degrees","m2",998,"","",""]
["28","5/2","Ridge capping 550mm girth,to match roofing tiles bedded and pointed in 1:3 cement mortar tinted to match tile colour  ","m",22,"","",""]
["28","5/3","Hip capping 550mm girth, to match roofing tiles bedded and pointed in 1:3 cement mortar tinted to match tile colour  ","m",29,"","",""]
["28","5/4","Hip finial","No",4,"","",""]
["28","5/5","Angle intersection of ridge, with hip including soaker","No",2,"","",""]
["28","5/6","Purpose made tile to end of ridge bedded and pointed in 1:3 cement mortar tinted to match tile colour (Provisional)","No",2,"","",""]
["28","","PROFILED ROOF METAL SHEETING AND ACCESSORIES","H2",{"v":0,"d":"0.0"},"","",""]
["28","","Metal Roof Sheeting","H3",{"v":0,"d":"0.0"},"","",""]
["28","5/7","Brownbuilt 0.6mm klip cover metal roof sheeting on 175x50mm purlins.","m2",257,"","",""]
["28","5/8","Raking cutting to roof sheeting (both sides measured)","m",29,"","",""]
["28","","ROOF AND WALL INSULATION","H2",{"v":0,"d":"0.0"},"","",""]
["29","","\"Sisalation 420\" heavy industrial grade aluminium foil based insulation and match existing one; and equally approved","H3",{"v":0,"d":"0.0"},"","",""]
["29","5/9","Insulation with stapled joints laid over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering including straining wires, etc.","m2",998,"","",""]

{"sheet":"1-6 BILL NO. 6","index":5,"n_rows":58,"n_cols":8,"rows_kept":58,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["30","","BILL NO. 6","H1",{"v":0,"d":"0.0"},"","",""]
["30","","CARPENTRY AND JOINERY (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["30","","(CPAP WORK GROUP NO. 126)","H2",{"v":0,"d":"0.0"},"","",""]
["30","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["30","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["30","","All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South African National Standards' (SANS) shall apply ","",{"v":0,"d":"0.0"},"","",""]
["30","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["30","","All timber roof trusses including nail plated trusses and bolted tusses with lapped members must comply with SABS 0243 ; The design manufacture and erection of timber truss.  The contractor shall submit letters ref TR.1 and TR.2 duly signed by the truss system Engineer, in respect of roof structure ","",{"v":0,"d":"0.0"},"","",""]
["30","","Particle board:","H3",{"v":0,"d":"0.0"},"","",""]
["30","","Particle board shall comply with the following specifications: a) SABS 1300 Particle board: exterior and flooring type b) SABS 1301 Particle board: interior type","",{"v":0,"d":"0.0"},"","",""]
["30","","Joinery:","H3",{"v":0,"d":"0.0"},"","",""]
["30","","Descriptions of frames shall be deemed to include frames, transomes, mullions, rails, etc","",{"v":0,"d":"0.0"},"","",""]
["30","","Descriptions of hardwood joinery shall be deemed to include pelleting of bolt holes","",{"v":0,"d":"0.0"},"","",""]
["31","","Fixing","H3",{"v":0,"d":"0.0"},"","",""]
["31","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete","",{"v":0,"d":"0.0"},"","",""]
["31","","Decorative laminate finish: ","H3",{"v":0,"d":"0.0"},"","",""]
["31","","Laminate finish shall be glued under pressure.  Edge strips shall be butt jointed at junctions with adjacent similar finish","",{"v":0,"d":"0.0"},"","",""]
["31","","ROOF CONSTRUCTION ETC","H2",{"v":0,"d":"0.0"},"","",""]
["31","","Wrought softwood grade CCA H2","H3",{"v":0,"d":"0.0"},"","",""]
["31","6/1","38 x 38mm Battens for concrete tile roof covering","m",1224,"","",""]
["31","","DOORS ETC","H2",{"v":0,"d":"0.0"},"","",""]
["31","","Semi-solid with hardboard facing 13 x 44mm hardwood edge on lock and hinge side","H3",{"v":0,"d":"0.0"},"","",""]
["31","6/2","762 x 2032 High x  44mm thick  (TYPE 1) ","No",22,"","",""]
["31","","Solid with hardboard facing 13 x 44mm hardwood edge on lock and hinge side","H3",{"v":0,"d":"0.0"},"","",""]
["31","6/3","1212 x 2032 High x 44mm Thick (TYPE3)","No",1,"","",""]
["31","","FIRE DOORS (Provisional)","H1",{"v":0,"d":"0.0"},"","",""]
["31","","44mm Class E Semi solid door with hardwood facing and 13 x 44mm hardwood edges ","H3",{"v":0,"d":"0.0"},"","",""]
["31","6/4","762 x 2032 High  (TYPE 1) ","No",13,"","",""]
["31","","44mm Class B Solid laminated double Fire door with hardboard facing ","H3",{"v":0,"d":"0.0"},"","",""]
["31","6/5","2132 x 900 x 44mm Solid hardwood french door with 8 panel lite clear safety glass (elsewhere measured) TYPE 2 ","No",1,"","",""]
["31","6/6","1212 x 2032 High  TYPE 4","No",16,"","",""]
["31","","FRAMED FRAMES ETC","H2",{"v":0,"d":"0.0"},"","",""]
["32","","Wrot meranti","H3",{"v":0,"d":"0.0"},"","",""]
["32","6/7","102 x 69mm Rebated frame for 813 x 2032mm high door","No",6,"","",""]
["32","6/8","100 x 60mm with 44mm rebated frame for 760 x 2032mm high door.","No",20,"","",""]
["32","6/9","120x60mm rebated frame for 915 x2134mm high door. (Provisional)","No",2,"","",""]
["32","6/10","120x60mm double rebated frame for 2032 x1212mm high door. (Provisional)","No",2,"","",""]
["32","6/11","100x60mm rebated frame for 2032 x762mm high door. ","No",22,"","",""]
["32","","FITTINGS","H2",{"v":0,"d":"0.0"},"","",""]
["32","","32mm thick Surinno post formed solid surface counter top,sealed between wall and top with clear silicone sealant. Counter top to be fixed to wall with hollow section 50 x 50 x 2.5mm painted mild steel brackets anchored to brick wall by means of 8mm expansion bolts. Cut steel sections to be sealed off by means of a plastic plug, or neatly welded and ground smooth to receive 3 coats of paint. Paint colour to later specification by Architect . All work to be as Architect's drawing No. 103-001 Rev.00 ","H3",{"v":0,"d":"0.0"},"","",""]
["32","6/12"," Floor cupboard 1120 x 635mm with 38mm post formed formica on particle board including 4 drawers on hidden roller hinges, all to the Architects drawing no.059789/2016/D-C9","No",1,"","",""]
["32","6/13"," Glazed top hung double door cabinet 1120 x 635mm with 38mm solid post formed formica on particle board including 4 drawers on hidden roller hinges, all to the Architects drawing no.059789/2016/D-C9","No",1,"","",""]
["32","6/14","Double sink floor cupboard 1191 x 575mm with 32mm post formed formica, sink cut, 4 drawers, rollers, shelves, all as described on Architect's drawing no. 059789/2016/D-C9","No",2,"","",""]
["32","6/15"," L Shaped floor cupboard 2438 x 1372mm overall with 38mm post formed formica on particle board including 4 drawers on hidden roller hinges, all to the Architects drawing no.059789/2016/D-C9","No",1,"","",""]
["33","","COUNTER","H2",{"v":0,"d":"0.0"},"","",""]
["33","","32mm thick Formica post formed solid surface counter with panelyte top, sealed between wall and top with clear silicone sealant. Counter top to be fixed to wall with hollow section 50 x 50 x 2.5mm painted mild steel brackets anchored to brick wall by means of 8mm expansion bolts. Cut steel sections to be sealed off by means of a plastic plug, or neatly welded and ground smooth to receive 3 coats of paint. Paint colour to later specification by Architect . All work to be as Architect's drawing 059789/2016/D-C9","H3",{"v":0,"d":"0.0"},"","",""]
["33","6/16"," Counter top size 1200 x 635mm wide overall","No",1,"","",""]
["33","","SKIRTINGS","H2",{"v":0,"d":"0.0"},"","",""]
["33","","Wrought hardwood","H3",{"v":0,"d":"0.0"},"","",""]
["33","6/17","100 x 22mm PAR square edge harwood skirting with 15 degrees chamfer to the top (PROVISIONAL)","m",1364,"","",""]
["33","6/18","19 x 69mm Skirting with 19mm quadrant bead","m",177,"","",""]
["33","","EAVES, VERGES, ETC","H2",{"v":0,"d":"0.0"},"","",""]
["33","","\"Everite Nutec\" pressed fibre cement","H3",{"v":0,"d":"0.0"},"","",""]
["33","6/19","15 x 225mm Fascias including galvanised steel jointing strips and 38 x 38mm softwood rafter filler piece 150mm high an 1200mm centres","m",168,"","",""]
["33","6/20","80 x 200mm medium density fibre cement barge board, with aluminium H-Profile barge board joiners","m",19,"","",""]

{"sheet":"1-7 BILL NO. 7","index":6,"n_rows":26,"n_cols":8,"rows_kept":26,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["34","","BILL NO. 7","H1",{"v":0,"d":"0.0"},"","",""]
["34","","CEILINGS, PARTITIONS AND ACCESS FLOORING (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["34","","(CPAP WORK GROUP NO. 129)","H2",{"v":0,"d":"0.0"},"","",""]
["34","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["34","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["34","","All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South Afrcan National Standards' (SANS) shall apply ","",{"v":0,"d":"0.0"},"","",""]
["34","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["34","","Descriptions:","H3",{"v":0,"d":"0.0"},"","",""]
["34","","Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete","",{"v":0,"d":"0.0"},"","",""]
["34","","Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere","",{"v":0,"d":"0.0"},"","",""]
["34","","NAILED UP CEILINGS","H2",{"v":0,"d":"0.0"},"","",""]
["34","","6mm NUTEC ceiling with H-Type joints painted with Plascon polvin white paint","H3",{"v":0,"d":"0.0"},"","",""]
["34","7/1","Ceilings including 38 x 50mm ( on edge) sawn softwood brandering at 400mm centres fully skimmed","m2",393,"","",""]
["34","","ACOUSTIC MINERAL FIBRE CEILING","H2",{"v":0,"d":"0.0"},"","",""]
["35","","600 x 600 x 15mm sand finish square edge acoustic mineral fibre ceiling tiles laid on pre painted exposed tee grid system, with aluminium shadow mould cornice trims.","H3",{"v":0,"d":"0.0"},"","",""]
["35","7/2","Suspended ceiling not exceeding 1m deep below","m2",965,"","",""]
["35","","\"Ornamental Mouldings\" or other and approved","H3",{"v":0,"d":"0.0"},"","",""]
["35","7/3","Aluminium shadow mould cornice trims.","m",1144,"","",""]
["35","","PARTITIONS ETC","H2",{"v":0,"d":"0.0"},"","",""]
["35","","\"Rhinoboard\" 12.5mm partitioning with and including  \"Isover 63 x 600 x 1200mm \"Cavitybatt\" insulation, the wall shall  comprise  62.5mm 'Ultrasteel'  studding formed  of  top  and  bottom  tracks  with vertical studs at maximum 400mm  centres,  friction fitted or pop-riveted to the top and bottom  tracks  with  similar  additional  vertical studs as necessary at  abutments, ends, etc and covered as described with wallboard screwed  to  studding with \"Drywall\" screws at maximum 220mm  centres. Boards are to be butt jointed and finished with 50mm wide scrim tape and \"Readymix D\" jointing compound all in accordance with   the manufacturer's   instructions. ","H3",{"v":0,"d":"0.0"},"","",""]
["35","7/4","Ceramic urinal partition 705mm x 400mm Duravite or equally approved.","m",31,"","",""]
["35","7/5","Extra over partition 3300mm high for vertical abutment","No",19,"","",""]
["35","7/6","Extra over partition 3300mm high for corner","No",11,"","",""]

{"sheet":"1-8 BILL NO. 8","index":7,"n_rows":19,"n_cols":8,"rows_kept":19,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["36","","BILL NO. 8","H1",{"v":0,"d":"0.0"},"","",""]
["36","","FLOOR COVERINGS, PLASTIC LININGS, ETC (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["36","","(CPAP WORK GROUP NO. 130)","H2",{"v":0,"d":"0.0"},"","",""]
["36","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["36","","SUPPLEMENTARY PREAMBLE","H3",{"v":0,"d":"0.0"},"","",""]
["36","","P1  Samples - with reference to all items and colour schemes, samples of all items are to be presented for approval prior to any bulk orders. Please take note that most items will have at least six weeks delivery period, these approvals will only take place at dates of site meetings, the samples need to be approved well in advance to avoid any delays with the lead time on orders.All samples must remain in the sample room for the duration of the contract period.  P2  Mock up rooms - all wall and floor finishes must be prepared in advance as part of a mock up room/rooms and at least a 100m2 of vinyl flooring will serve as a sample floor   NOTE:  Where applicable, all expansion joints in screed to be in accordance with vinyl sheet expansion detail. Complete with EJC50 polyspan joint cover or equal approved. Strip and welding rod colours to Architect's approval   Where applicable, all expansion joints in screed to be in accordance with vinyl sheet expansion detail. Complete with EJC65 polyspan joint cover or equal approved. Strip and welding rod colours to Architect's approval ","",{"v":0,"d":"0.0"},"","",""]
["36","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["37","","All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South Afrcan National Standards' (SANS) shall apply ","",{"v":0,"d":"0.0"},"","",""]
["37","","FLOOR COVERINGS","H2",{"v":0,"d":"0.0"},"","",""]
["37","","300 x 300 x 2.5mm Semi-flexible vinyl tiles laid with welded joints","H3",{"v":0,"d":"0.0"},"","",""]
["37","8/1","On floors","m2",187,"","",""]
["37","","New Carpet floor 500 x 500 x9mm '' Nexus Berber Point 920'' carpet tiles with ( bitumen backing) or equally approved laid in checker pattern including 8mm brass straight edge at door threshold.","H3",{"v":0,"d":"0.0"},"","",""]
["37","8/2","On floors","m2",415,"","",""]
["37","","POLISH, SEALERS, ETC","H2",{"v":0,"d":"0.0"},"","",""]
["37","","Polish, sealers, etc","H3",{"v":0,"d":"0.0"},"","",""]
["37","8/3","Strip, clean and apply three coats non-slip acrylic emulsion floor dressing buffed to an approved finish","m2",187,"","",""]

{"sheet":"1-9 BILL NO. 9","index":8,"n_rows":42,"n_cols":8,"rows_kept":42,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["38","","BILL NO. 9","H1",{"v":0,"d":"0.0"},"","",""]
["38","","IRONMONGERY (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["38","","(CPAP WORK GROUP NO. 132)","H2",{"v":0,"d":"0.0"},"","",""]
["38","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["38","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["38","","Proprietary items","H4",{"v":0,"d":"0.0"},"","",""]
["38","","Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration","",{"v":0,"d":"0.0"},"","",""]
["38","","Finishes to ironmongery","H3",{"v":0,"d":"0.0"},"","",""]
["38","","Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacquered CH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelled AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded","",{"v":0,"d":"0.0"},"","",""]
["38","","HINGES, BOLTS, ETC","H2",{"v":0,"d":"0.0"},"","",""]
["38","","\"Solid\" or equally approved","H3",{"v":0,"d":"0.0"},"","",""]
["38","9/1","WC deadlocks indicator with 79mm turn knob.Doma or equally approved.","No",6,"","",""]
["38","9/2","(100 x 76 x 2mm) x2 s/s sinkless hinges.","No",26,"","",""]
["38","","\"EN-SUITE\" LOCKS","H2",{"v":0,"d":"0.0"},"","",""]
["39","","\"Union\" or equally approved ","H3",{"v":0,"d":"0.0"},"","",""]
["39","","The following locks are to be suitable for master and grand master key operation","",{"v":0,"d":"0.0"},"","",""]
["39","9/3","Three lever lock set,SABS approved (chrome), with satin chrome door arch handle on plate or equally approved match the existing one","No",26,"","",""]
["39","9/4","Union 37651 helping hand indicator bolt.","No",4,"","",""]
["39","","PUSH PLATES AND KICKING PLATES","H2",{"v":0,"d":"0.0"},"","",""]
["39","","\"Union\" or equally approved ","H3",{"v":0,"d":"0.0"},"","",""]
["39","","BATHROOM FITTINGS","H3",{"v":0,"d":"0.0"},"","",""]
["39","9/5","RODX672 Franke toilet roll holder or equally approved","No",26,"","",""]
["39","9/6","RODX611 Franke toilet roll holder","No",4,"","",""]
["39","9/7","STRX611 Franke Sanitary towel disposer or equally approved","No",26,"","",""]
["39","9/8","STRX625 Franke soap dispenser or equally approved ","No",3,"","",""]
["39","9/9","CHRX630 Franke electronic towel dispenser or equally approved ","No",3,"","",""]
["39","9/10","BS610 Franke waste container,perforated,wall mounted or equally approved.","No",3,"","",""]
["39","9/11","CNTX BR Franke  straight grab bar or equally approved ","No",5,"","",""]
["39","9/12","CNTX600 Franke x 3 straight grab bar or equally approved ","No",15,"","",""]
["39","9/13","CNTV450 Franke straight grab bar or equally approved ","No",5,"","",""]
["40","","FIRE SIGNAGE (PROVISIONAL)","H2",{"v":0,"d":"0.0"},"","",""]
["40","9/14","152 X 152 Photoluminous 'Arrow' sign","No",1,"","",""]
["40","9/15","152 X 152 Photoluminous 'Exit' sign","No",10,"","",""]
["40","9/16","152 X 152 Photoluminous 'Fire Extinguisher' sign","No",8,"","",""]
["40","9/17","152 X 152 Photoluminous 'Fire Hose Reel' sign","No",8,"","",""]
["40","9/18","152 X 152 Photoluminous 'Man Running Left' sign","No",16,"","",""]
["40","9/19","152 X 152 Photoluminous 'Man Running Right' sign","No",18,"","",""]
["40","9/20","152 X 152 Photoluminous 'Man Running Down' sign","No",21,"","",""]
["40","9/21","152 x 152 Photoluminous 'Man Running Up' sign ","No",1,"","",""]

{"sheet":"1-10 BILL NO.10","index":9,"n_rows":34,"n_cols":8,"rows_kept":34,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["41","","BILL NO.10","H1",{"v":0,"d":"0.0"},"","",""]
["41","","METALWORK (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["41","","(CPAP WORK GROUP NO. 136)","H2",{"v":0,"d":"0.0"},"","",""]
["41","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["41","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["41","","Descriptions of bolts shall be deemed to include nuts and washers","",{"v":0,"d":"0.0"},"","",""]
["41","","Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete","",{"v":0,"d":"0.0"},"","",""]
["41","","Metalwork described as\"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described","",{"v":0,"d":"0.0"},"","",""]
["41","","WELDED SCREENS, GATES, BURGLAR BARS, ETC","H2",{"v":0,"d":"0.0"},"","",""]
["41","","10mm Hot dipped galvanised steel round bar type NBP1 burglar bars to suit small pane casement type steel windows","H3",{"v":0,"d":"0.0"},"","",""]
["41","","GALVANISED STEEL STAIRS","H2",{"v":0,"d":"0.0"},"","",""]
["41","10/1","8mm \"Vastrap\" plate continuous treads, risers and landing including all required fixings, bolts, etc","m2",19,"","",""]
["41","","STEEL BALUSTRADES","H2",{"v":0,"d":"0.0"},"","",""]
["41","","Hot dipped galvanised Balustrade","H3",{"v":0,"d":"0.0"},"","",""]
["41","10/2","50mm diameter x 2mm thick handrail, 50x50x5mm bottom and top rail and 10x10 solid vertical bars at 100mm centres","m",39,"","",""]
["41","","ALUMINIUM SUNSCREENS","H2",{"v":0,"d":"0.0"},"","",""]
["42","","Aluminium sunscreens/or cantilever hanging must be to Engineers Approval.","H3",{"v":0,"d":"0.0"},"","",""]
["42","10/3","Powder coated aluminium plate -/+50mm, Fixed to wall with 4No.M16 chemical anchors on base plate. Powder coated extruded aluminium elliptical fin blade at varying angles, +/-300L & BT(mm) Fitted between flat plates. Powder coated aluminium rod round bars, +/-30mm.Fitted between flat plates Powder coated aluminium 300H x 20T(mm) base plate.","m2",561,"","",""]
["42","","Aluminium window frame","H3",{"v":0,"d":"0.0"},"","",""]
["42","10/4","5100 x 2105mm Powder coated aluminium window frame. Colour to match existing.","No",11,"","",""]
["42","10/5","3096 x 2105mm Powder coated aluminium window frame.Colour to match existing.","No",3,"","",""]
["42","10/6","2367 x 2105mm Powder coated aluminium window frame.Colour to match existing","No",1,"","",""]
["42","10/7","2546 x 2105mm Powder aluminium window frame. Colour to match existing.","No",1,"","",""]
["42","10/8","2351 x 2105mm Powder coated aluminium window frame.Colour to match existing.","No",1,"","",""]
["42","10/9","2489 x 2105mm Powder coated aluminium window frame.Colour to match existing.","No",1,"","",""]
["42","10/10","2470 x 2105mm Powder coated aluminium window frame.Colour to match existing.","No",1,"","",""]
["42","10/11","3096 x 2105mm Powder coated aluminium window frame.Colour to match existing.","No",2,"","",""]
["42","","Steel Doors","H3",{"v":0,"d":"0.0"},"","",""]
["42","10/12","2032 x 762 steel door","No",13,"","",""]
["42","10/13","2132 x1212 steel door ","No",13,"","",""]
["42","10/14","2132 x 900 steel door","No",1,"","",""]

{"sheet":"1-11 BILL NO. 11","index":10,"n_rows":23,"n_cols":8,"rows_kept":23,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["43","","BILL NO. 11","H1",{"v":0,"d":"0.0"},"","",""]
["43","","PLASTERING (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["43","","(CPAP WORK GROUP NO. 142)","H2",{"v":0,"d":"0.0"},"","",""]
["43","","All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South African National Standards' (SANS) shall apply ","",{"v":0,"d":"0.0"},"","",""]
["43","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["43","","PRICES","H2",{"v":0,"d":"0.0"},"","",""]
["43","","The prices of mouldings, weathering, skirtings, labours, etc. shall include for forming mitres, stops, etc. unless otherwise described.The prices of granolithic described as with grooves forming panels, shall include for lining into panels not exceeding 20m2 in area with the length of any panel not exceeding 20m2 in area with the length of any panel not exceeding 4.5m with v-joints and where described as with margins, shall include for steel trowelled margins generally 100mm wide at the perimeters of areas.The prices of all rendering shall include for working around pipes, balusters, etc.Rates for plaster are to include for all filling to and working around electrical conduits, etc., prior to plastering.","",{"v":0,"d":"0.0"},"","",""]
["43","","SPECIALIST FLOORING","H2",{"v":0,"d":"0.0"},"","",""]
["43","","Polyurethane screed","H3",{"v":0,"d":"0.0"},"","",""]
["43","","SCREEDS","H2",{"v":0,"d":"0.0"},"","",""]
["43","11/1","Self levelling screed","m2",416,"","",""]
["43","","EXTERNAL PLASTER","H2",{"v":0,"d":"0.0"},"","",""]
["43","","One coat cement plaster on brickwork with a wood float smooth finish","H3",{"v":0,"d":"0.0"},"","",""]
["43","11/2","On walls","m2",19,"","",""]
["44","","INTERNAL PLASTER","H2",{"v":0,"d":"0.0"},"","",""]
["44","","One coat cement plaster on brickwork with a wood float smooth finish","H3",{"v":0,"d":"0.0"},"","",""]
["44","11/3","On walls","m2",716,"","",""]
["44","","SKIMMING","H2",{"v":0,"d":"0.0"},"","",""]
["44","","Skimmed concrete soffit finish","H3",{"v":0,"d":"0.0"},"","",""]
["44","11/4","Prepare to receive an approved plaster bonding, apply gyproc rhinolight multi-purpose / cretestone minimum 3mm(or equally approved).","m2",627,"","",""]

{"sheet":"1-12 BILL NO. 12","index":11,"n_rows":12,"n_cols":8,"rows_kept":12,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["45","","BILL NO. 12","H1",{"v":0,"d":"0.0"},"","",""]
["45","","TILING (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["45","","(CPAP WORK GROUP NO. 144)","H2",{"v":0,"d":"0.0"},"","",""]
["45","","The Tenderer is referred to the relevant Clauses in the separate document Model Preambles for Trades (WB20)","",{"v":0,"d":"0.0"},"","",""]
["45","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["45","","FLOOR TILING","H2",{"v":0,"d":"0.0"},"","",""]
["45","","300 x 300 x 5mm Terracotta floor tiles supplied and delivered to site and including for taking delivery, storage, fixed with adhesive to bedding and flush pointed with jointing compound including wastage","H3",{"v":0,"d":"0.0"},"","",""]
["45","12/1","On floors and landings","m2",174,"","",""]
["45","12/2","Skirting 150mm high","m",319,"","",""]

{"sheet":"1-13 BILL NO. 13","index":12,"n_rows":47,"n_cols":8,"rows_kept":47,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["46","","BILL NO. 13","H1",{"v":0,"d":"0.0"},"","",""]
["46","","PLUMBING AND DRAINAGE (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["46","","(CPAP WORK GROUP NO. 145 &146)","H2",{"v":0,"d":"0.0"},"","",""]
["46","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["46","","RAINWATER DISPOSAL","H2",{"v":0,"d":"0.0"},"","",""]
["46","","0.6mm \"Alugutter\" or equally approved standard 127mm OG profile eaves gutter in long lengths fixed by means of pressed aluminium concealed hanger brackets at 600 to 750mm centres complete with any necessary expansion joints","H3",{"v":0,"d":"0.0"},"","",""]
["46","13/1","127 x 96mm Eaves gutters with brackets fixed to fascias to match the existing one","m",245,"","",""]
["46","13/2","76mm Diameter rainwater pipes with brackets plugged to match existing one","m",181,"","",""]
["46","13/3","Extra over eaves gutter for stopped end","No",4,"","",""]
["46","13/4","Extra over eaves gutter for angle","No",8,"","",""]
["46","13/5","Extra over eaves gutter for outlet for 76mm rainwater pipe","No",14,"","",""]
["46","13/6","Extra over 76mm rainwater pipe for bend","No",14,"","",""]
["46","13/7","Extra over 76mm rainwater pipe for shoe","No",14,"","",""]
["46","","\"Franke\" stainless steel or other and approved","H3",{"v":0,"d":"0.0"},"","",""]
["46","13/8","Stainless steel single centre bowl drop-in sink size 600mm x 1200mm. Bowl size 610 x 460 x 230mmdeep with overflow, manufactured in grade 304 (18/10) stainless steel. Tap to be 15mm 102CP demand bib tap. All in accordance to relative SANS","No",3,"","",""]
["46","13/9","Vanity whb. ceramic fireclay oval self-rimming drop-in vanity basin, 595x455mm with three semi-punched tapholes, and chain stay hole through the centre semi-punched taphole.Colour white.Cameo or equally approved.","No",15,"","",""]
["47","13/10","WC.Complete dual flush close-couple bottom in let Bibo toilet mechanism.An universal dual flush mechanism, front flush. Complete with bottom inlet valve & all seals couplers.","No",23,"","",""]
["47","","\"Charlog Plastics\" or other and approved","H3",{"v":0,"d":"0.0"},"","",""]
["47","13/11","Wall hung urinal.Dry waterless air trap and fixing included.Colour white. Duravit or equally approved","No",5,"","",""]
["47","13/12","Paraplegic WC. Atlas raised close-coupled paraplegic pan including cistern mechanism & seat.Ceramic.Colour white.Lecico or equally approved.","No",8,"","",""]
["47","","TRAPS ETC","H2",{"v":0,"d":"0.0"},"","",""]
["47","","uPVC","H3",{"v":0,"d":"0.0"},"","",""]
["47","13/13","Touch-free,electronic control pillar tap,chrome.Cobration-Cobra or equally approved. Full adjustment remote control.Cobration-Cobra or equally approved.","No",11,"","",""]
["47","","TAPS, VALVES, ETC","H2",{"v":0,"d":"0.0"},"","",""]
["47","13/14","Regulating valve","No",14,"","",""]
["47","13/15","15mm Chromium plated raised wall mounted tap code GRO-36273000 including mounting box code GRO-3633700","No",1,"","",""]
["47","","Chromium Plated","H3",{"v":0,"d":"0.0"},"","",""]
["47","13/16","15mm Chromium plated paraplegic taps","No",8,"","",""]
["47","","Toilet and urinal flush valves ","H3",{"v":0,"d":"0.0"},"","",""]
["47","13/17","\"Cobra Watertech\" or eqully approved Flush master junior FJ4.203 toilet flush valve","No",23,"","",""]
["47","13/18","\"Cobra Watertech\" or equally approved Flush master junior FJ8.102 urinal flush valve","No",5,"","",""]
["47","","ELECTRIC WATER HEATERS","H2",{"v":0,"d":"0.0"},"","",""]
["48","","Electrical water heaters","H3",{"v":0,"d":"0.0"},"","",""]
["48","13/19","\"Zip hydroboil\" or equally and approved, model 7.5 /45, 2,5L boiling water unit with stainless steel finish mounted 300mm above the sink bowl.Oveflow to discharge into the sink. Including one \"cobra\" fullway ballcock code 1075-15 fitted to inlet pipe.","No",1,"","",""]
["48","","TESTING","H3",{"v":0,"d":"0.0"},"","",""]
["48","13/20","Allow for testing all water supplies,and Fire Services to the satisfaction of the Technical Director. All detective work is to be taken out and replaced at the Contractor's expense and the whole re-tested until found satisfactory","Item",{"v":1,"d":"1.00"},"","",""]
["48","","FIRE APPLIANCES ETC","H2",{"v":0,"d":"0.0"},"","",""]
["48","13/21","Installation of new standard wall mounted Fire Hose Reels with Ø19mm hose, size 480 x 300mm, 30m long @ 2.0MPa. Installed according to SANS 543, installed as per SANS 1128 and SANS 10105.","No",16,"","",""]
["48","13/22","New 4,5kg Dry Chemical Powder Hand Held Fire Extinguishers  including varnished hardwood backing plate and wall bracket, as per SANS 1522 and SANS 1739. Mounted as per SANS 10105.","No",16,"","",""]
["48","","BUDGETARY ALLOWANCE","H1",{"v":0,"d":"0.0"},"","",""]
["48","","Reticulation and detection of fire equipment ","H3",{"v":0,"d":"0.0"},"","",""]
["48","13/23","Provide a sum of R30 000.00 (Thirty Thousand Rands) for Reticulation and detection for fire equipment","Item",{"v":1,"d":"1.00"},{"v":628745,"d":"628745.00"},{"v":628745,"d":"628745.00"},""]
["48","13/24","Add for profit on the above","%IT","","","",""]
["48","13/25","Allow for attendance","%IT","","","",""]

{"sheet":"1-14 BILL NO. 14","index":13,"n_rows":19,"n_cols":8,"rows_kept":19,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["49","","BILL NO. 14","H1",{"v":0,"d":"0.0"},"","",""]
["49","","GLAZING (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["49","","(CPAP WORK GROUP NO. 150)","H2",{"v":0,"d":"0.0"},"","",""]
["49","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["49","","BILL NO. 16","H1",{"v":0,"d":"0.0"},"","",""]
["49","","SUPPLEMENTARY PREAMBLE","H3",{"v":0,"d":"0.0"},"","",""]
["49","","All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South African National Standards' (SANS) shall apply ","",{"v":0,"d":"0.0"},"","",""]
["49","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["49","","'Franke' model MH600R chronos reflective polished surface mirror or equal approved with concealed fixing installed strictly manufactures specifications.","H3",{"v":0,"d":"0.0"},"","",""]
["49","14/1","CHR601 Frank x2 mirror","No",6,"","",""]
["49","14/2","CHRH601 Frank x1 mirror","No",3,"","",""]
["49","","GLAZING TO WOOD WITH PINNED-ON BEADS (BEADS ELSEWHERE)","H2",{"v":0,"d":"0.0"},"","",""]
["49","","6mm Lite safety glass","H4",{"v":0,"d":"0.0"},"","",""]
["49","14/3","Panes exceeding 0,1m² and not exceeding 0,5m² (Provisional)","m2",7,"","",""]
["49","14/4","Panes exceeding 0,5m² and not exceeding 2m² (Provisional)","m2",102,"","",""]
["49","14/5","Panes exceeding 14m² and not exceeding 16m² (Provisional)","m2",96,"","",""]

{"sheet":"1-15 BILL NO. 15","index":14,"n_rows":49,"n_cols":8,"rows_kept":49,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["50","","BILL NO. 15","H1",{"v":0,"d":"0.0"},"","",""]
["50","","PAINTWORK (PROVISIONAL)","H1",{"v":0,"d":"0.0"},"","",""]
["50","","(CPAP WORK GROUP NO. 152)","H2",{"v":0,"d":"0.0"},"","",""]
["50","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["50","","SUPPLEMENTARY PREAMBLES","H1",{"v":0,"d":"0.0"},"","",""]
["50","","Supplementary Preamble:  1. All SABS Specifications referred to in this document shall be deemed to be omitted and the redesigned and renumbered 'South African National Standards' (SANS) shall apply   SUBSTRATE REQUIREMENTS FOR RESIN FLOORING SYSTEMS (PROS-TRUCT). 1.\tSurface finish required for the application of resin flooring systems should be a minimum of 20mPa cured concrete or screed laid true to line and level, be clean and dry, free of laitance and have a single pass steel trowel finish. PURE CEMENT MUST NOT BE USED as a final finish to the screed. The minimum screed thickness to be 40mm. No concrete curing membranes to be used. 2.\tThe use of products such as cretestone, pavelite and other gypsum based products should not be used as levelling compounds as these are weak and will lead to disbondment of the resin finish. 3.\tMaximum moisture content of the concrete or screed is not to exceed 4% as measured with a moisture meter. Provided there is good ventilation and warm weather, a 40mm screed should dry sufficiently in 8 to 10 days. A 100mm + concrete generally requires 28 days to cure sufficiently.","",{"v":0,"d":"0.0"},"","",""]
["50","","Where trade names are given in the following items, the materials used shall be of the make and type specified, or other approved by the Director ","",{"v":0,"d":"0.0"},"","",""]
["51","","PAINTWORK ETC TO PREVIOUSLY PAINTED WORK","H2",{"v":0,"d":"0.0"},"","",""]
["51","","Previously painted plastered surfaces  Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth  Previously painted metal surfaces  Surfaces shall be thoroughly rubbed and cleaned down. Blistered or peeling paint shall be completely removed down to bare metal  Previously painted wood surfaces  Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth","",{"v":0,"d":"0.0"},"","",""]
["51","","ON PLASTER","H3",{"v":0,"d":"0.0"},"","",""]
["51","","Painted walls.Prepare surface.Apply water-based multi-surface primer.Apply x2 Plascon ''wall &all'' or equally approved.Colour to Architect.","H4",{"v":0,"d":"0.0"},"","",""]
["51","15/1","On internal walls","m2",7834,"","",""]
["51","","Prepare surface apply approved wood primer,apply x2 coats Plascon wall & all or equally approved.Colour to Architect.","H3",{"v":0,"d":"0.0"},"","",""]
["51","15/2","On existing doors","m2",762,"","",""]
["51","15/3","On existing door frames","m2",322,"","",""]
["51","","Contractor must test to determine the original finish with denatured alcohol.Prepare surface to receive x2 coats of original clear finish.","H3",{"v":0,"d":"0.0"},"","",""]
["51","15/4","On existing doors","m2",57,"","",""]
["51","15/5","On existing door frames","m2",13,"","",""]
["51","","PAINTWORK, ETC. TO NEW WORK","H2",{"v":0,"d":"0.0"},"","",""]
["52","","ON PLASTERED SURFACES","H3",{"v":0,"d":"0.0"},"","",""]
["52","","Apply water-based multi-surfaced primer.Apply x2 Plascon ''Wall & All'' or equally approved.Colour to Architect.","H4",{"v":0,"d":"0.0"},"","",""]
["52","15/6","On internal plastered walls","m2",698,"","",""]
["52","15/7","On external plastered walls","m2",19,"","",""]
["52","","ON PLASTER BOARD","H2",{"v":0,"d":"0.0"},"","",""]
["52","","Prepare surface.Apply water-base multi-surface primer.Apply x2 coats of ''Wall &All'' or equally approved.Colour white","H3",{"v":0,"d":"0.0"},"","",""]
["52","15/8","On ceilings and cornices","m2",750,"","",""]
["52","","ON SMOOTH CONCRETE","H2",{"v":0,"d":"0.0"},"","",""]
["52","","Prepare to receive an approved palster bonding.Apply Gyproc Rhinolite multipurpose/Creatastone minimum 3mm(or equally approved).Apply x2 coats of approved acrylic paint.Colour white","H3",{"v":0,"d":"0.0"},"","",""]
["52","15/9","On ceilings and cornices(soffits)","m2",2418,"","",""]
["52","","ON METAL","H2",{"v":0,"d":"0.0"},"","",""]
["52","","Remove pealing paint with approved all purpose paint remover,treat rust with approved treatment,clean with waterbase degreaser,apply approved metal primer,apply x2 coats waterbased enamel paint,all to manufacture specs,colour to Architect","H3",{"v":0,"d":"0.0"},"","",""]
["52","15/10","Window steel frames","m2",673,"","",""]
["52","","Clean surface with approved aquasolve degreaser.Prime with approved etch primer.Apply x2 coats of solvent bases paint.Plascon metal care or equally approved.Colour to Architect.","H3",{"v":0,"d":"0.0"},"","",""]
["52","15/11","Aluminium window frames","m2",360,"","",""]
["53","","Remove pealing paint with approved all purpose paint remover,treat rust with approved treatment.Clean with waterbase degrease,apply approved metal primer,apply x2 coats of waterbased enamel paint,all to manufactures specs.Colour to Architect","H3",{"v":0,"d":"0.0"},"","",""]
["53","15/12","On steel door frames","m2",2,"","",""]
["53","","ON WOOD","H2",{"v":0,"d":"0.0"},"","",""]
["53","","One coat Dark Mahogany Stain, one coat Plascon Woodcare Ultra Varnish (X33/X44) thinned 20% with mineral turpentine (AZH1) by volume. Allow 6 hours to dry. Sand slightly with 220 grit paper to denib. Apply two further coats of Plascon Woodcare Ultra Varnish (X33/X44) unthinned allowing 6 hours of grying between coats or similar approved","H3",{"v":0,"d":"0.0"},"","",""]
["53","15/13","Skirtings, rails, etc not exceeding 300mm girth (PROVISIONAL)","m",1364,"","",""]
["53","","Prepare surface apply approved wood primer,apply x2 coats Plascon wall & all or equally approved.Colour to Architect.","H3",{"v":0,"d":"0.0"},"","",""]
["53","15/14","On new doors","m2",71,"","",""]
["53","15/15","On new door frames","m2",32,"","",""]
["53","","Contractor must test to determine the original finish with denatured alcohol.Prepare surface to receive x2 coats of original clear finish.","H3",{"v":0,"d":"0.0"},"","",""]
["53","","ON SOFFIT","H2",{"v":0,"d":"0.0"},"","",""]
["53","","Concrete soffit finish","H3",{"v":0,"d":"0.0"},"","",""]
["53","15/16","Apply approved oil base primer. Apply 2 coats of approved acrylic paint.","m2",627,"","",""]

{"sheet":"1-16 BILL NO. 16","index":15,"n_rows":12,"n_cols":8,"rows_kept":12,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["54","","BILL NO. 16","H1",{"v":0,"d":"0.0"},"","",""]
["54","","PAPERHANGING","H2",{"v":0,"d":"0.0"},"","",""]
["54","","(CPAP WORK GROUP NO. 152)","H2",{"v":0,"d":"0.0"},"","",""]
["54","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["54","","PAPERHANGING TO EXISTING WORK","H2",{"v":0,"d":"0.0"},"","",""]
["54","","Previously papered plastered surfaces ","H3",{"v":0,"d":"0.0"},"","",""]
["54","","Surfaces shall be thoroughly washed down and allowed to dry completely before any paperhanging is commenced.  Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth.  Bare plaster surfaces shall be painted with a single coat of interior quality PVA emulsion paint","",{"v":0,"d":"0.0"},"","",""]
["54","","Existing wallpaper shall be completely removed and surfaces shall be thoroughly cleaned down. Cracks shall be opened, filled with a suitable filler and finished smooth.  Bare plaster surfaces shall be painted with a single coat of interior quality PVA emulsion paint","",{"v":0,"d":"0.0"},"","",""]
["54","16/1","On previously papered walls and columns ","m2",55,"","",""]

{"sheet":"1-17 BILL NO. 17","index":16,"n_rows":21,"n_cols":8,"rows_kept":21,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["55","","BILL NO. 17","H1",{"v":0,"d":"0.0"},"","",""]
["55","","BUDGETARY ALLOWANCES","H1",{"v":0,"d":"0.0"},"","",""]
["55","","Work for which budgetary allowances are provided will be measured and valued in accordance with the and deducted in whole or in part if not required without any compensation for loss of profit on the said allowances.","",{"v":0,"d":"0.0"},"","",""]
["55","","Executive Block","H3",{"v":0,"d":"0.0"},"","",""]
["55","17/1","Provide the sum of R23 157,26.00 (Twenty Three Thousand One Hundred and Fifty Seven Rands) for New Reception Counter ","Item",{"v":1,"d":"1.00"},23157.26,23157.26,""]
["55","17/2","Profit ","%IT","","","",""]
["55","17/3","Attendance","%IT","","","",""]
["55","17/4","Provide the sum of R335 076 (Three Hundred and Thirty Five Thousand and Sventy Six Rands) for new block C shopfront in ground floor ","Item",{"v":1,"d":"1.00"},{"v":335076,"d":"335076.00"},{"v":335076,"d":"335076.00"},""]
["55","17/5","Profit ","%IT","","","",""]
["55","17/6","Attendance","%IT","","","",""]
["55","","External works","H3",{"v":0,"d":"0.0"},"","",""]
["55","17/7","Provide the sum of R 1 194 853,75 (One Million One hundred and Ninety four thousand, eight hundred and fifty three rands and seventy five cents) for external works","Item",{"v":1,"d":"1.00"},1194853.75,1194853.75,""]
["55","17/8","Profit ","%IT","","","",""]
["55","17/9","Attendance","%IT","","","",""]
["55","","Block A : storm damage based on desktop report","H3",{"v":0,"d":"0.0"},"","",""]
["55","17/10","Provide the sum of R1 079 988 (One Million and Sevety Nine thousan , Nine hundred and Tighty Eight Rands only for the desk top storm damage report on Block A","Item",{"v":1,"d":"1.00"},{"v":1079988,"d":"1079988.00"},{"v":1079988,"d":"1079988.00"},""]
["55","17/11","Profit ","%IT","","","",""]
["55","17/12","Attendance","%IT","","","",""]

{"sheet":"1-18 BILL NO. 18","index":17,"n_rows":548,"n_cols":8,"rows_kept":548,"flags":["formulas_cached_only"]}
["04:05:24","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["56","","BILL NO. 18","H1",{"v":0,"d":"0.0"},"","",""]
["56","","ELECTRICAL INSTALLATION ","H1",{"v":0,"d":"0.0"},"","",""]
["56","","(CPAP WORK GROUP NO. 160)","H2",{"v":0,"d":"0.0"},"","",""]
["56","","The Tenderer is referred to the relevant Clauses in the separate document 'Model Preambles for Trades 2008'","",{"v":0,"d":"0.0"},"","",""]
["56","","SUPPLEMENTRY PREAMBLES","H2",{"v":0,"d":"0.0"},"","",""]
["56","","The SUPLEMENTRY PREAMBLES and all subsequent specifications applicable to the same trade In the preceeding sections of this document, apply equally to this trade","",{"v":0,"d":"0.0"},"","",""]
["56","","All equipment, electrical matreials or methods of installation shall comply fully with SANS 10142 (as ammended)","",{"v":0,"d":"0.0"},"","",""]
["56","","Proprietary items or materials where specified are to be of the brand specified - or other approved by the Head: Works","",{"v":0,"d":"0.0"},"","",""]
["56","","CPAP WORK GROUP","H2",{"v":0,"d":"0.0"},"","",""]
["56","","Unless otherwise stated, all items in this bill will be Work Group 160","",{"v":0,"d":"0.0"},"","",""]
["56","","LV DISTRIBUTION BOARD","H2",{"v":0,"d":"0.0"},"","",""]
["56","","The supply, installation and commissioning of complete distribution boards, including all busbars and switchgear as specified and shown on drawing, and to standard specification.","H3",{"v":0,"d":"0.0"},"","",""]
["56","","Main Distribution Kiosk for Essential Supply as specified on Drawing no. KIOSK-1(E) (NEXT TO INDOOR SUB-STATION)","H4",{"v":0,"d":"0.0"},"","",""]
["56","18/1","Supply ","No",1,"","",""]
["56","18/2","Install","No",1,"","",""]
["57","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-2 (E) (GROUND FLOOR BLOCK C)","H3",{"v":0,"d":"0.0"},"","",""]
["57","18/3","Supply ","No",1,"","",""]
["57","18/4","Install","No",1,"","",""]
["57","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-3 (E) (GROUND FLOOR BLOCK C)","H3",{"v":0,"d":"0.0"},"","",""]
["57","18/5","Supply ","No",1,"","",""]
["57","18/6","Install","No",1,"","",""]
["57","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-4 (E) (FIRST FLOOR BLOCK C)","H3",{"v":0,"d":"0.0"},"","",""]
["57","18/7","Supply","No",1,"","",""]
["57","18/8","Install","No",1,"","",""]
["57","","Sub Distribution Board for Non-essential Supply as specified on Drawing no. DB-5 (E) (FIRST FLOOR BLOCK C)","H3",{"v":0,"d":"0.0"},"","",""]
["57","18/9","Supply","No",1,"","",""]
["57","18/10","Install","No",1,"","",""]
["57","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-6 (E) (THIRD FLOOR BLOCK C)","H3",{"v":0,"d":"0.0"},"","",""]
["57","18/11","Supply ","No",1,"","",""]
["57","18/12","Install","No",1,"","",""]
["57","","Sub Distribution Board for Non-essential Supply as specified on Drawing no. DB-7 (E) (THIRD FLOOR BLOCK C)","H3",{"v":0,"d":"0.0"},"","",""]
["57","18/13","Supply","No",1,"","",""]
["57","18/14","Install","No",1,"","",""]
["58","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-8 (E) (GROUND FLOOR EXECUTIVE BLOCK BLOCK)","H3",{"v":0,"d":"0.0"},"","",""]
["58","18/15","Supply","No",1,"","",""]
["58","18/16","Install","No",1,"","",""]
["58","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-9 (E) (FIRST FLOOR EXECUTIVE BLOCK BLOCK)","H3",{"v":0,"d":"0.0"},"","",""]
["58","18/17","Supply","No",1,"","",""]
["58","18/18","Install","No",1,"","",""]
["58","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-10 (E) (FIRST FLOOR EXECUTIVE BLOCK BLOCK)","H3",{"v":0,"d":"0.0"},"","",""]
["58","18/19","Supply","No",1,"","",""]
["58","18/20","Install","No",1,"","",""]
["58","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-10 (E) (FIRST FLOOR EXECUTIVE BLOCK BLOCK)","H3",{"v":0,"d":"0.0"},"","",""]
["58","18/21","Supply","No",1,"","",""]
["58","18/22","Install","No",1,"","",""]
["58","","Sub Distribution Board for Essential Supply as specified on Drawing no. DB-11 (E) (SECOND FLOOR EXECUTIVE BLOCK BLOCK)","H3",{"v":0,"d":"0.0"},"","",""]
["58","18/23","Supply","No",1,"","",""]
["58","18/24","Install","No",1,"","",""]
["58","18/25","The supply, installation, connecting, testing and commissioning of 11 of 15KVA watt 230 phase UPS with 30 minutes battery back up, spike and lighting protected for the uninterrupted power supply to the offices","No",11,"","",""]
["58","","MAINS CABLING WIRING","H1",{"v":0,"d":"0.0"},"","",""]
["58","","LOW VOLTAGE CABLES","H2",{"v":0,"d":"0.0"},"","",""]
["59","","The supply and installation in horizontal ducting, drawn through cable sleeve in trench or on cable tray and sleeves)","H3",{"v":0,"d":"0.0"},"","",""]
["59","","95mm2 x 4 core ECC KIOSK-1(E)","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/26","Supply ","m",200,"","",""]
["59","18/27","Install","m",200,"","",""]
["59","","Termination for 95mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/28","Supply ","No",16,"","",""]
["59","18/29","Install","No",16,"","",""]
["59","","70mm2 x 4 core ECC DB-2 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/30","Supply","m",300,"","",""]
["59","18/31","Install","m",300,"","",""]
["59","","Termination for 70mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/32","Supply ","No",8,"","",""]
["59","18/33","Install","No",8,"","",""]
["59","","70mm2 x 4 core ECC DB-3 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/34","Supply ","m",300,"","",""]
["59","18/35","Install","m",300,"","",""]
["59","","Termination for 70mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/36","Supply ","No",8,"","",""]
["59","18/37","Install","No",8,"","",""]
["59","","70mm2 x 4 core ECC DB-4 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/38","Supply ","m",60,"","",""]
["59","18/39","Install","m",60,"","",""]
["59","","Termination for 70mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["59","18/40","Supply ","No",8,"","",""]
["60","18/41","Install","No",8,"","",""]
["60","","50mm2 x 4 core ECC DB-5 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/42","Supply ","m",60,"","",""]
["60","18/43","Install","m",60,"","",""]
["60","","Termination for 50mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/44","Supply ","No",8,"","",""]
["60","18/45","Install","No",8,"","",""]
["60","","25mm2 x 4 core ECC DB-12 (E) ","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/46","Supply ","m",60,"","",""]
["60","18/47","Install","m",60,"","",""]
["60","","Termination for 25mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/48","Supply ","No",8,"","",""]
["60","18/49","Install","No",8,"","",""]
["60","","95mm2 x 4 core ECC DB-7 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/50","Supply ","m",60,"","",""]
["60","18/51","Istall","m",60,"","",""]
["60","","Termination for 95mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/52","Supply ","No",16,"","",""]
["60","18/53","Install","m",16,"","",""]
["60","","95mm2 x 4 core ECC DB-8 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/54","Supply ","m",200,"","",""]
["60","18/55","Install","m",200,"","",""]
["60","","Termination for 95mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["60","18/56","Supply ","No",16,"","",""]
["60","18/57","Install","No",16,"","",""]
["61","","95mm2 x 4 core ECC DB-9 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/58","Supply ","m",200,"","",""]
["61","18/59","Install","m",200,"","",""]
["61","","Termination for 95mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/60","Supply ","No",16,"","",""]
["61","18/61","Install","No",16,"","",""]
["61","","70mm2 x 4 core ECC DB-10 (E) ","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/62","Supply ","m",60,"","",""]
["61","18/63","Install","m",60,"","",""]
["61","","Termination for 70mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/64","Supply ","No",8,"","",""]
["61","18/65","Install","No",8,"","",""]
["61","","95mm2 x 4 core ECC DB-11 (E)","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/66","Supply ","m",200,"","",""]
["61","18/67","Install","m",200,"","",""]
["61","","Termination for 90mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/68","Supply ","No",16,"","",""]
["61","18/69","Install","No",16,"","",""]
["61","","25mm2 x 4 core ECC DB-12 (E) ","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/70","Supply ","m",80,"","",""]
["61","18/71","Install","m",80,"","",""]
["61","","Termination for 25mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["61","18/72","Supply ","No",8,"","",""]
["61","18/73","Install","No",8,"","",""]
["62","","16mm2 x 4 core ECC DB-13 (E) ","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/74","Supply ","m",100,"","",""]
["62","18/75","Install","m",100,"","",""]
["62","","Termination for 16mm² x  4 core cable","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/76","Supply ","No",8,"","",""]
["62","18/77"," Install","No",8,"","",""]
["62","","EARTH SPIKE","H3",{"v":0,"d":"0.0"},"","",""]
["62","","1.2m copper coated earth spike at every distribution board","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/78","Supply ","No",13,"","",""]
["62","18/79","Install","No",13,"","",""]
["62","","Cable maker tape (320mm wide)","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/80","Supply ","m",860,"","",""]
["62","18/81","Install","m",860,"","",""]
["62","","110mm diameter (kabelflex sleeve) services","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/82","Supply ","m",1260,"","",""]
["62","18/83","Install","m",1260,"","",""]
["62","","45 degrees slow bends for 110mm dia.sleeve","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/84","Supply ","No",252,"","",""]
["62","18/85","Install","No",252,"","",""]
["62","","50mm diameter (kabelflex sleeve)","H4",{"v":0,"d":"0.0"},"","",""]
["62","18/86","Supply ","m",1039,"","",""]
["62","18/87","Install","m",1039,"","",""]
["63","","45 degrees slow bends for 50mm ","H4",{"v":0,"d":"0.0"},"","",""]
["63","18/88"," Supply ","No",520,"","",""]
["63","18/89","Install","No",520,"","",""]
["63","","The supply and installation of galvanised bosal conduit including cutting, bending, joints and  fixed materials, cast on surface in roofspace","H3",{"v":0,"d":"0.0"},"","",""]
["63","","50mm Ø galvanised conduit","H4",{"v":0,"d":"0.0"},"","",""]
["63","18/90","Supply ","m",100,"","",""]
["63","18/91","Install","m",100,"","",""]
["63","","32mm Ø galvanised conduit","H4",{"v":0,"d":"0.0"},"","",""]
["63","18/92","Supply ","m",90,"","",""]
["63","18/93","Install","m",90,"","",""]
["63","","Excavations for cables in trenches (450 x 600x1000) 3 linear metres equals 1 cubic metre, including cart away, backfilling, risk of collapse ","H4",{"v":0,"d":"0.0"},"","",""]
["63","18/94","Excavate in normal earth measured in linear metres (not cubic metre)","m",1060,"","",""]
["63","18/95","Allow for Soft Rock in above trench","m3",530,"","",""]
["63","18/96","Allow for Hard Rock in above trench","m3",265,"","",""]
["63","","Electrical Manholes","H3",{"v":0,"d":"0.0"},"","",""]
["63","","Supply and build either pre-cast or full wall manhole with heavy duty cover with the following minimum inside dimensions:  - 1200mm x 1200mm  x 600mm ","H4",{"v":0,"d":"0.0"},"","",""]
["63","18/97","Supply","No",2,"","",""]
["63","18/98","Install","No",2,"","",""]
["63","","Telephone Manholes","H3",{"v":0,"d":"0.0"},"","",""]
["64","","Supply and build either pre-cast or full wall manhole with heavy duty cover with the following minimum inside dimensions:  - 600mm x 600mm  x 600mm deep ","H4",{"v":0,"d":"0.0"},"","",""]
["64","18/99","Supply","No",3,"","",""]
["64","18/100","Install","No",3,"","",""]
["64","","Galvanised bosal.","H3",{"v":0,"d":"0.0"},"","",""]
["64","","The supply, installation of conduit. Prices to include cutting, draw boxes, fixing materials tees, bends, saddles, etc. ","H4",{"v":0,"d":"0.0"},"","",""]
["64","18/101","Supply ","m",15840,"","",""]
["64","18/102","Install: cast in concrete, on surface in roof- space, built in brickwork","m",15840,"","",""]
["64","","GENERAL LIGHTING  ","H1",{"v":0,"d":"0.0"},"","",""]
["64","","CONDUIT","H2",{"v":0,"d":"0.0"},"","",""]
["64","","CONDUIT ACCESSORIES","H3",{"v":0,"d":"0.0"},"","",""]
["64","","The supply and installation if drawboxes including locknuts The supply and installation if drawboxes including locknuts","H3",{"v":0,"d":"0.0"},"","",""]
["64","","Lightweight round, deep back or side entry type for 20mm dia conduit cast in concrete or roofspace, average for 1, 2, 3, and 4 ways","H4",{"v":0,"d":"0.0"},"","",""]
["64","18/103","Supply ","No",610,"","",""]
["64","18/104","Install","No",610,"","",""]
["64","","Lightweight round, deep back or side entry dia conduit cast in concrete or roofspace, average for 1, 2, 3,and 4 ways","H4",{"v":0,"d":"0.0"},"","",""]
["64","18/105","Supply ","No",100,"","",""]
["64","18/106","Install","No",100,"","",""]
["65","","Galvanised bosal, 100 x 50 x 50 switch boxes for 20mm dia conduit built into brick-work or cast into concrete (coverplates measured elsewhere)","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/107","Supply ","No",610,"","",""]
["65","18/108","Install","No",610,"","",""]
["65","","3.5 Octagon Box Octagon Single Gang Handy Box white for the Occupancy Sensor","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/109","Supply ","No",264,"","",""]
["65","18/110","Install","No",264,"","",""]
["65","","Equipment and Control Gear","H3",{"v":0,"d":"0.0"},"","",""]
["65","","16A single lever, one way flush mounted rocker type switch with coverplates (red in colour) ","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/111","Supply ","No",132,"","",""]
["65","18/112","Install","No",132,"","",""]
["65","","10A photo cell surface mounted in an empty luminaire","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/113","Supply ","No",9,"","",""]
["65","18/114","Install","No",9,"","",""]
["65","","16A two lever, two way flush mounted rocker type switch with coverplates (red in colour) ","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/115","Supply","No",100,"","",""]
["65","18/116","Install","No",100,"","",""]
["65","","16A one lever, three way flush mounted rocker type switch  with coverplates (red in colour) ","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/117","Supply","No",45,"","",""]
["65","18/118","Install","No",45,"","",""]
["65","","16A one lever, one way downlight flush mounted rocker type switch with coverplates (red in colour) ","H4",{"v":0,"d":"0.0"},"","",""]
["65","18/119","Supply","No",45,"","",""]
["66","18/120","Install","No",45,"","",""]
["66","","16A one lever, two way downlight flush mounted rocker type switch with coverplates (red in colour) ","H4",{"v":0,"d":"0.0"},"","",""]
["66","18/121","Supply","No",45,"","",""]
["66","18/122","Install","No",45,"","",""]
["66","","16A one lever, five way downlight flush mounted rocker type switch with coverplates (red in colour) ","H4",{"v":0,"d":"0.0"},"","",""]
["66","18/123","Supply","No",45,"","",""]
["66","18/124","Install","No",45,"","",""]
["66","","Dimmer switch - 1000w (one lever, one way)","H4",{"v":0,"d":"0.0"},"","",""]
["66","18/125","Supply","No",45,"","",""]
["66","18/126","Install","No",45,"","",""]
["66","","CMR 10 Occupancy Sensor with a coverage pattern of 360 degrees and viewing distance of 8.53 meters when mounted at 2.74 meters while when mounted at 2.13 viewing distance of 9.25 meters. ","H4",{"v":0,"d":"0.0"},"","",""]
["66","18/127","Supply ","No",249,"","",""]
["66","18/128","Install","No",249,"","",""]
["66","","CONDUCTORS","H2",{"v":0,"d":"0.0"},"","",""]
["66","","The supply and installation of PVC insulated single core stranded copper conductors drawn into conduits ","H3",{"v":0,"d":"0.0"},"","",""]
["66","","1. 5mm2   PVC black and red","H4",{"v":0,"d":"0.0"},"","",""]
["66","18/129","Supply ","m",42240,"","",""]
["66","18/130","Install","m",42240,"","",""]
["66","","2. 5mm2   PVC green / yellow earth wire  ","H4",{"v":0,"d":"0.0"},"","",""]
["66","18/131","Supply","No",21120,"","",""]
["66","18/132","Install","No",21120,"","",""]
["67","","ROOF LIGHT SWITCHES","H3",{"v":0,"d":"0.0"},"","",""]
["67","","16A metal clad switch below ceiling mounted at trap door with illuminated \"red\" toggle switch","H4",{"v":0,"d":"0.0"},"","",""]
["67","18/133","Supply ","No",13,"","",""]
["67","18/134","Install","No",13,"","",""]
["67",""," LUMINAIRES","H2",{"v":0,"d":"0.0"},"","",""]
["67","","Supply, take delivery, unpack, test fittings, including installation, materials, connections, fluorescent and incandescent lamps. All lamps shall be Colour as described below with Standard Starters.","H3",{"v":0,"d":"0.0"},"","",""]
["67","","Type A ","H4",{"v":0,"d":"0.0"},"","",""]
["67","18/135","Supply ","No",134,"","",""]
["67","18/136","Install","No",134,"","",""]
["67","","Type B","H4",{"v":0,"d":"0.0"},"","",""]
["67","18/137","Supply ","No",271,"","",""]
["67","18/138","Install","No",271,"","",""]
["67","","Type C","H4",{"v":0,"d":"0.0"},"","",""]
["67","18/139","Supply ","No",15,"","",""]
["67","18/140","Install","No",15,"","",""]
["67","","Type DL","H4",{"v":0,"d":"0.0"},"","",""]
["67","18/141","Supply ","No",131,"","",""]
["67","18/142","Install","No",131,"","",""]
["67","","Type PL","H4",{"v":0,"d":"0.0"},"","",""]
["67","18/143","Supply ","No",160,"","",""]
["67","18/144","Install","No",160,"","",""]
["68","","Type E","H4",{"v":0,"d":"0.0"},"","",""]
["68","18/145","Supply ","No",84,"","",""]
["68","18/146","Install","No",84,"","",""]
["68","","Type F","H4",{"v":0,"d":"0.0"},"","",""]
["68","18/147","Supply ","No",138,"","",""]
["68","18/148","Install","No",138,"","",""]
["68","","Type T","H4",{"v":0,"d":"0.0"},"","",""]
["68","18/149","Supply ","m",28,"","",""]
["68","18/150","Install","No",28,"","",""]
["68","","Type W","H4",{"v":0,"d":"0.0"},"","",""]
["68","18/151","Supply","No",17,"","",""]
["68","18/152","Install","No",17,"","",""]
["68","","EMERGENCY LIGHTING  ","H3",{"v":0,"d":"0.0"},"","",""]
["68","","Supply and install 250x300mm Suspended Double sided illuminated fire escape sign equiped with a battery pack (Lead Acid battery)","H4",{"v":0,"d":"0.0"},"","",""]
["68","18/153","Supply","No",8,"","",""]
["68","18/154","Install","No",8,"","",""]
["68",""," SMALL POWER","H1",{"v":0,"d":"0.0"},"","",""]
["68","","CONDUIT AND  CONDUIT ACCESSORIES SABS APPROVED CONDUIT","H2",{"v":0,"d":"0.0"},"","",""]
["68","","Galvanised bosal. The supply and installation of conduit including cutting, drawboxes and fixing materials  ","H3",{"v":0,"d":"0.0"},"","",""]
["68","","20mm dia","H4",{"v":0,"d":"0.0"},"","",""]
["68","18/155","Supply ","m",5368,"","",""]
["69","","Install: cast in concrete, on surface in roofspace built into brickwork","H4",{"v":0,"d":"0.0"},"","",""]
["69","","25mm dia","H4",{"v":0,"d":"0.0"},"","",""]
["69","18/156","Supply ","m",5368,"","",""]
["69","18/157","Install: cast in concrete, on surface in roofspace built into brickwork","m",1952,"","",""]
["69","18/158","Install: cast in concrete, on surface in roofspace built into brickwork","m",1952,"","",""]
["69","","The supply of drawboxes including locknuts, bushes coverplates, fixing materials when required etc.","H3",{"v":0,"d":"0.0"},"","",""]
["69","","Round box for 20mm","H4",{"v":0,"d":"0.0"},"","",""]
["69","18/159","Supply ","No",924,"","",""]
["69","18/160","Install","No",924,"","",""]
["69","","Round box for 25mm","H4",{"v":0,"d":"0.0"},"","",""]
["69","18/161","Supply","No",96,"","",""]
["69","18/162","Install","No",96,"","",""]
["69","","Galvanised steel, 100 x 100 x 50mm box for 20mm conduit built into brickwork or cast in concrete. (coverplates measured elsewhere)","H4",{"v":0,"d":"0.0"},"","",""]
["69","18/163","Supply ","No",924,"","",""]
["69","18/164","Install","No",924,"","",""]
["69","","Galvanised steel, 100 x 100 x 50mm box for 25mm conduit built into brickwork or cast in concrete (coverplates measured elsewhere)","H4",{"v":0,"d":"0.0"},"","",""]
["69","18/165","Supply ","No",96,"","",""]
["69","18/166","Install","No",96,"","",""]
["69","","CONDUCTORS","H2",{"v":0,"d":"0.0"},"","",""]
["70","","The supply and installation of PVC insulated stranded single core copper conductors drawn into conduits and ducting","H3",{"v":0,"d":"0.0"},"","",""]
["70","","2.5mm2   PVC black and red","H4",{"v":0,"d":"0.0"},"","",""]
["70","18/167","Supply ","m",33176,"","",""]
["70","18/168","Install","m",33176,"","",""]
["70","","4mm2   PVC black and red","H4",{"v":0,"d":"0.0"},"","",""]
["70","18/169","Supply ","m",924,"","",""]
["70","18/170","Install","m",924,"","",""]
["70","","2.5mm2   PVC insulated green/yellow  earth wire","H4",{"v":0,"d":"0.0"},"","",""]
["70","18/171","Supply ","m",16588,"","",""]
["70","18/172","Install","m",16588,"","",""]
["70","","EQUIPMENT AND CONTROL","H3",{"v":0,"d":"0.0"},"","",""]
["70","","The supply and installation of single white round pin switch socket outlets 16A 3 pin flush mounted with coverplates and \"white\" neon lamp to indicate normal available","H4",{"v":0,"d":"0.0"},"","",""]
["70","18/173","Supply ","No",40,"","",""]
["70","18/174","Install","No",40,"","",""]
["70","","The supply and installation of Double white round pin switch socket outlets 16A 3 pin flush mounted with coverplates and \"white\" neon lamp to indicate normal power available","H4",{"v":0,"d":"0.0"},"","",""]
["70","18/175","Supply ","No",36,"","",""]
["70","18/176","Install","No",36,"","",""]
["70","","The supply and installation of red round pin single switch socket outlets 16A 3 pin flush mounted with cover plates and \"red\" to indicate essential power available","H4",{"v":0,"d":"0.0"},"","",""]
["70","18/177","Supply ","No",10,"","",""]
["70","18/178","Install","No",10,"","",""]
["71","","5A switchless socket outlets ","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/179","Supply","No",14,"","",""]
["71","18/180","Install","No",14,"","",""]
["71","","25 Ampere, isolator for cassette room aircon and mid wall split unit (heat pump), including cover ","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/181","Supply ","No",174,"","",""]
["71","18/182","Install","No",174,"","",""]
["71","","20 Ampere, single pole flush dryer complete with including diamond range cover ","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/183","Supply ","No",21,"","",""]
["71","18/184","Install","No",21,"","",""]
["71","","30 Ampere, one lever surface weatherproof isolator for cassette room airconditioner with heat pump, including cover.","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/185","Supply ","No",87,"","",""]
["71","18/186","Install","No",87,"","",""]
["71","","63 Ampere, Tripple pole weatherproof isolator for VRV units including cover.","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/187","Supply ","No",9,"","",""]
["71","18/188","Install","No",9,"","",""]
["71","","16 Amp duplex switch for extract fan including cover","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/189","Supply ","No",66,"","",""]
["71","18/190","Install","No",66,"","",""]
["71","","40 Ampere, single pole flush mounted isolator for hydroboiler complete with including cover  ","H4",{"v":0,"d":"0.0"},"","",""]
["71","18/191","Supply ","No",9,"","",""]
["71","18/192","Install","No",9,"","",""]
["71","","POWER SKIRTING AND  POWER TRUNKING","H2",{"v":0,"d":"0.0"},"","",""]
["72","","The supply and installation of modular pre-galvanised 2 compartment power skirting or power trunking complete with 2 separate clip on steel full length covers length covers silver in colour, Endcap/top end, Inside  Bend, Outside Bend, Corner Riser, Mid Point \"TEE\" Riser etc.","H3",{"v":0,"d":"0.0"},"","",""]
["72","","2 compartment P802 power ducting complete with 55mm cover (subdivisible).","H4",{"v":0,"d":"0.0"},"","",""]
["72","18/193","Supply ","m",678,"","",""]
["72","18/194","Install","m",678,"","",""]
["72","","16A 3 pin round socket outlet white ","H4",{"v":0,"d":"0.0"},"","",""]
["72","18/195","Supply","No",205,"","",""]
["72","18/196","Install","No",205,"","",""]
["72","","16A 3 pin round socket outlet red ","H4",{"v":0,"d":"0.0"},"","",""]
["72","18/197","Supply","No",473,"","",""]
["72","18/198","Install","No",473,"","",""]
["72","","Data Blank cover","H4",{"v":0,"d":"0.0"},"","",""]
["72","18/199","Supply","No",410,"","",""]
["72","18/200","Install","No",410,"","",""]
["72","","Telephone Blank cover","H4",{"v":0,"d":"0.0"},"","",""]
["72","18/201","Supply","No",205,"","",""]
["72","18/202","Install","m",205,"","",""]
["72","","TELEPHONE AND  NETWORK","H1",{"v":0,"d":"0.0"},"","",""]
["72","","CONDUIT ","H2",{"v":0,"d":"0.0"},"","",""]
["72","","All conduits and accessories to be galvanised bosal. The supply and installation of conduit including cutting, bending, joints, settings, fittings, boxes, fixing materials","H3",{"v":0,"d":"0.0"},"","",""]
["73","","25mm galvanised bosal  conduit","H4",{"v":0,"d":"0.0"},"","",""]
["73","18/203","Supply ","m",2000,"","",""]
["73","18/204","Install: cast in concrete, on surface in roof space built into brickwork","m",2000,"","",""]
["73","","32mm galvanised bosal conduit","H4",{"v":0,"d":"0.0"},"","",""]
["73","18/205","Supply ","m",140,"","",""]
["73","18/206","Install","m",140,"","",""]
["73","","CONDUIT ACCESSORIES ","H2",{"v":0,"d":"0.0"},"","",""]
["73","","The suply, installation of drawboxes including locknuts, bushes, coverplates, fixing materials.","H3",{"v":0,"d":"0.0"},"","",""]
["73","","100 x 50 x 50 galvanised bosal drawboxes for 25mm conduit built into wall brick including coverplates ","H4",{"v":0,"d":"0.0"},"","",""]
["73","18/207","Supply ","No",25,"","",""]
["73","18/208","Install","No",25,"","",""]
["73","","100 x 50 x 50mm galvanised draw boxes for 25mm conduit built into brick work with blank coverplates. ( Television point )","H4",{"v":0,"d":"0.0"},"","",""]
["73","18/209","Supply ","No",2,"","",""]
["73","18/210","Install","No",2,"","",""]
["73","","The supply and installation of galvanised steel draw wires drawn into conduit(1.6mm)","H4",{"v":0,"d":"0.0"},"","",""]
["73","18/211","Supply ","m",2140,"","",""]
["73","18/212","Install","m",2140,"","",""]
["73","","The supply and installation of flush board with soft wood backing architrave and hinged door 450 x 450 x 100mm board","H4",{"v":0,"d":"0.0"},"","",""]
["73","18/213","Supply ","No",3,"","",""]
["73","18/214","Install","No",3,"","",""]
["74","","300 x 300 x 100mm board","H4",{"v":0,"d":"0.0"},"","",""]
["74","18/215","Supply ","No",3,"","",""]
["74","18/216","Install","No",3,"","",""]
["74","","AREA  LIGHTING","H1",{"v":0,"d":"0.0"},"","",""]
["74","","LOW VOLTAGE CABLE","H2",{"v":0,"d":"0.0"},"","",""]
["74","","Provide, install,test and commission the following 1 000V ECC/SWA/ECC copper cable. Price shall allow for the installation of cables in cable ducts, through sleeves, conduits, or installation against vertical and horizontal levels (e.g..walls, poles,etc) but shall not include the various cable ends, trenches or the backfilling of trenches.","H3",{"v":0,"d":"0.0"},"","",""]
["74","","6mm² x 4 core ECC","H4",{"v":0,"d":"0.0"},"","",""]
["74","18/217","Supply ","m",240,"","",""]
["74","18/218","Install","m",240,"","",""]
["74","","Terminate and make off the following 1 000V ECC/ SWA/ECC cable in a cable gland onto a gland plate according to the manufacture's instructions. Provide the gland as well as the cores with lugs and bolt onto terminals. The marking of the cable shall also be allowed for. (Note the light fittings are supplied with glands, see detail spec.)","H3",{"v":0,"d":"0.0"},"","",""]
["74","","6mm² x 4 core  terminations","H4",{"v":0,"d":"0.0"},"","",""]
["74","18/219","supply","No",38,"","",""]
["74","18/220","install","No",38,"","",""]
["74","","Provide and install a three-way Pratley box,cores with  lugs and suitable connectors. ","H4",{"v":0,"d":"0.0"},"","",""]
["74","18/221","supply","No",16,"","",""]
["74","18/222","Install","No",16,"","",""]
["74","","Provide and install a four-way Pratley box, cores with lugs and suitable connectors.","H4",{"v":0,"d":"0.0"},"","",""]
["74","18/223","supply","No",16,"","",""]
["75","18/224","install","No",16,"","",""]
["75","","CABLE TRENCHES","H3",{"v":0,"d":"0.0"},"","",""]
["75","","Excavation and back-fill cable trenches as per specification. (Including soft soil layer around cable). The excavation for the perimeter poles are included here.","H4",{"v":0,"d":"0.0"},"","",""]
["75","18/225","Earth","m3",600,"","",""]
["75","18/226","Soft rock","m3",300,"","",""]
["75","18/227","Hard rock","m3",200,"","",""]
["75","","Provide and install cable marker tape above cable, 300mm below finished ground level.","H4",{"v":0,"d":"0.0"},"","",""]
["75","18/228","Supply","m",540,"","",""]
["75","18/229","Install","m",540,"","",""]
["75","","PVC INSULATED CONDUCTOR","H3",{"v":0,"d":"0.0"},"","",""]
["75","","Provide and install the following lenghts of insulated conductor (inside poles) 2.5mm","H4",{"v":0,"d":"0.0"},"","",""]
["75","18/230","Supply","m",3784,"","",""]
["75","18/231","Install","m",3784,"","",""]
["75","","EARTH WIRE","H4",{"v":0,"d":"0.0"},"","",""]
["75","","Supply and install the following lengths of earth wire( inside poles)","H4",{"v":0,"d":"0.0"},"","",""]
["75","18/232","Supply","m",1892,"","",""]
["75","18/233","Install","m",1892,"","",""]
["75","","6mm (to be taped together with the cable at 1.5m intervals)","H4",{"v":0,"d":"0.0"},"","",""]
["75","18/234","Supply","m",240,"","",""]
["75","18/235","Install","m",240,"","",""]
["75","","LIGHT FITTINGS","H4",{"v":0,"d":"0.0"},"","",""]
["76","","Provide ,install and connect completely the following light fittings as described light  fitting schedule in the positions indicated on the drawings. Light fittings shall  be complete  with lamps and shall be approved by the Department ","H3",{"v":0,"d":"0.0"},"","",""]
["76","","Type X","H4",{"v":0,"d":"0.0"},"","",""]
["76","18/236","Supply","No",4,"","",""]
["76","18/237","Install","No",4,"","",""]
["76","","Type J","H4",{"v":0,"d":"0.0"},"","",""]
["76","18/238","Supply","No",10,"","",""]
["76","18/239","Install","No",10,"","",""]
["76","","Photocell","H4",{"v":0,"d":"0.0"},"","",""]
["76","18/240","Supply","No",15,"","",""]
["76","18/241","Install","No",15,"","",""]
["76","18/242","Supply: Galvanised steel light pole to achieve 9.5m above ground.","No",10,"","",""]
["76","18/243"," Install in tarmac to achieve 9.5m above ground level ","No",10,"","",""]
["76","","ACCESS CONTROL","H2",{"v":0,"d":"0.0"},"","",""]
["76","","Supply, Install, Test and commission an access control system complete with a control panel, software electromechanical hardware, electronic hardware and sytem users (ID card)","H3",{"v":0,"d":"0.0"},"","",""]
["76","","GATE CONTROL EQUIPEMENT ","H3",{"v":0,"d":"0.0"},"","",""]
["76","","Supply and Install a boom gate complete with all the necessary equipments . It must have a green button  for opening and a red button for closing ","H4",{"v":0,"d":"0.0"},"","",""]
["76","18/244","Supply","No",2,"","",""]
["76","18/245","Install","No",2,"","",""]
["77","","CCTV","H1",{"v":0,"d":"0.0"},"","",""]
["77","","CCTV  EQUIPMENT ","H2",{"v":0,"d":"0.0"},"","",""]
["77","18/246","Supply and install Indoor Dome Camera complete with an IR illumination, day/night, digital noise reduction and digital Slow shutter.","No",18,"","",""]
["77","18/247","Install","No",18,"","",""]
["77","18/248","Supply and install Indoor Bullet Camera complete with an IR illumination, day/night, digital noise reduction and digital Slow shutter.","No",40,"","",""]
["77","18/249","Install","No",40,"","",""]
["77","18/250","Supply and install Outdoot Bullet Camera complete with an IR illumination, day/night, digital noise reduction and digital Slow shutter.","No",11,"","",""]
["77","18/251","Install","No",11,"","",""]
["77","18/252","Supply and install outdoor PTZ Camera complete with an IR illumination, day/night, digital noise reduction and digital Slow shutter.","No",10,"","",""]
["77","18/253","Install","No",10,"","",""]
["77","","Network switch.","H4",{"v":0,"d":"0.0"},"","",""]
["77","18/254","supply ","No",12,"","",""]
["77","18/255","Install","No",12,"","",""]
["77","","Network Vidoe recorder","H4",{"v":0,"d":"0.0"},"","",""]
["77","18/256","supply ","No",4,"","",""]
["77","18/257","Install","No",4,"","",""]
["77","","MONITORS","H3",{"v":0,"d":"0.0"},"","",""]
["77","","Supply and Install LED monitor complete with 16 channel real channel NVR","H4",{"v":0,"d":"0.0"},"","",""]
["77","18/258","supply ","No",8,"","",""]
["77","18/259","Install","No",8,"","",""]
["78","","CABLES","H2",{"v":0,"d":"0.0"},"","",""]
["78","","Allow for the supply and install of RG59 power cable ","H4",{"v":0,"d":"0.0"},"","",""]
["78","18/260","Supply","m",1264,"","",""]
["78","18/261","Install","m",1264,"","",""]
["78","","CONDUIT","H2",{"v":0,"d":"0.0"},"","",""]
["78","","Conduit and accessories to be Galvanized Bosal. The supply and installation of conduit includes cutting, drawboxes and fixing materials.","H3",{"v":0,"d":"0.0"},"","",""]
["78","","20mm dia","H4",{"v":0,"d":"0.0"},"","",""]
["78","18/262","Supply ","m",832,"","",""]
["78","18/263","Install: cast in concrete, on surface in roofspace built into brickwork","m",832,"","",""]
["78","","CONDUIT ACCESSORIES","H2",{"v":0,"d":"0.0"},"","",""]
["78","","The supply of drawboxes including locknuts, bushes, coverplates, fixing materials when required.  ","H3",{"v":0,"d":"0.0"},"","",""]
["78","","Round box for 20mm","H4",{"v":0,"d":"0.0"},"","",""]
["78","18/264","Supply ","No",230,"","",""]
["78","18/265","Install","No",230,"","",""]
["78","","WIRE BASKET","H3",{"v":0,"d":"0.0"},"","",""]
["78","","Supply and Install P220 wire basket above ceiling ","H4",{"v":0,"d":"0.0"},"","",""]
["78","18/266","Supply ","m",1264,"","",""]
["78","18/267","Install","m",1264,"","",""]
["78","","SLEEVES","H3",{"v":0,"d":"0.0"},"","",""]
["78","","Supply and Install 50mm diameter (kabelflex sleeve)","H4",{"v":0,"d":"0.0"},"","",""]
["78","18/268","Supply","m",395,"","",""]
["78","18/269","Install","m",395,"","",""]
["79","","45 degrees slow bends for 50mm dia.sleeve","H4",{"v":0,"d":"0.0"},"","",""]
["79","18/270","Supply","No",198,"","",""]
["79","18/271","Install","No",198,"","",""]
["79","","Supply and install camera housing, brackets and all connections.","H4",{"v":0,"d":"0.0"},"","",""]
["79","18/272","Supply","No",92,"","",""]
["79","18/273","Install","No",92,"","",""]
["79","18/274","Testing and commissioning of the  complete CCTV ","SUM",1,"","",""]
["79","18/275","Provide marked-up copy \"As built\" record drawings for CCTV.","SUM",1,"","",""]
["79","18/276","Provide training course for CCTV installation ","SUM",1,"","",""]
["79","18/277","Provide complete operating and maintenance manuals for the complete installation","SUM",1,"","",""]
["79","","EARTHING AND LIGHTNING PROTECTION ","H1",{"v":0,"d":"0.0"},"","",""]
["79","","EARTHING","H2",{"v":0,"d":"0.0"},"","",""]
["79","18/278","Earthing and bonding to SANS 10142-1","Item",{"v":1,"d":"1.00"},"","",""]
["79","","TESTING & COMMISIONING ","H4",{"v":0,"d":"0.0"},"","",""]
["79","18/279","Testing of the complete electrical installation in terms of SANS 10142-1 and provision of Certificates of Compliance ","Item",{"v":1,"d":"1.00"},"","",""]
["79","","BONDING OF WATER MAINS AND CABLES","H3",{"v":0,"d":"0.0"},"","",""]
["79","","Bond the proposed water main to the adjacent down conductor. All water pipes, hand basins, sinks, baths, gutters and rain water pipes shall be bonded.","H4",{"v":0,"d":"0.0"},"","",""]
["79","18/280","All external earth wires and cable armouring from the incoming and outgoing cables will be properly crimped into cable lugs and bolted to their respective earth bars.","SUM",1,"","",""]
["79","","LIGHTNING PROTECTION","H2",{"v":0,"d":"0.0"},"","",""]
["79","","Earthrods  ","H3",{"v":0,"d":"0.0"},"","",""]
["80","","Earthrods should ideally be spaced approximately 10m intervals and connected to the earth wire to achieve equal potential bonding 1500mm Copper Earthrods/spikes ","H4",{"v":0,"d":"0.0"},"","",""]
["80","18/281","Supply","No",30,"","",""]
["80","18/282","Install","No",30,"","",""]
["80","","Supply and Install Down Alluminium rod strictly in accordance with the relevant SANS & IEC Specifications","H3",{"v":0,"d":"0.0"},"","",""]
["80","","16mm2 Aluminium Rods","H4",{"v":0,"d":"0.0"},"","",""]
["80","18/283","Supply ","m",250,"","",""]
["80","18/284","Install","m",250,"","",""]
["80","18/285","Terminate","No",25,"","",""]
["80","","Bare Stranded Copper Earth Wire","H2",{"v":0,"d":"0.0"},"","",""]
["80","","Supply and install Bare Stranded Copper wires in trenches  including termination for Equipotential Bonding strictly in accordance with the relevant SANS & IEC Specifications","H3",{"v":0,"d":"0.0"},"","",""]
["80","","35mm2 copper cable","H4",{"v":0,"d":"0.0"},"","",""]
["80","18/286","Supply ","m",120,"","",""]
["80","18/287","Install","m",120,"","",""]
["80","18/288","Terminate","No",10,"","",""]
["80","","Ring Earth Trenching","H3",{"v":0,"d":"0.0"},"","",""]
["80","","Trenching ( 300mm wide X  600mm deep ) and backfilling in compacted layers (300mm),  including bedding and installation of warning tape above cable.","H4",{"v":0,"d":"0.0"},"","",""]
["80","18/289","soft hand pickable soil","m",350,"","",""]
["80","18/290","soil requiring pneumatics tools and aids","m",100,"","",""]
["81","","TESTING","H3",{"v":0,"d":"0.0"},"","",""]
["81","18/291","Test the complete installation including the handing in of the test results (Certificate of Lightning Protection) to the Engineer.","Item",{"v":1,"d":"1.00"},"","",""]
["81","","REMOVAL OF EXISTING MATERIAL ON SITE  LOW VOLTAGE CABLES","H1",{"v":0,"d":"0.0"},"","",""]
["81","","DISCONNECT THE FOLLOWING SUPPLY CABLES","H2",{"v":0,"d":"0.0"},"","",""]
["81","","Price to switch off, disconnet and remove the following existing three or single phase supply cable. Price for digging must be included here. Make safe and tidy afterwards.( All cables must return to client)","H4",{"v":0,"d":"0.0"},"","",""]
["81","18/292","50mm²  -  70mm²","SUM",1,"","",""]
["81","18/293","16mm²  - 35mm²","SUM",1,"","",""]
["81","18/294","6mm²  - 10mm²","SUM",1,"","",""]
["81","","Excavations for cables in trenches (450 x 600x1000) 3 linear  metres equals 1 cubic metre","H4",{"v":0,"d":"0.0"},"","",""]
["81","18/295"," metres equals 1 cubic metre (not cubic metre)","m",200,"","",""]
["81","18/296","Allow for Soft Rock in above trench","m3",70,"","",""]
["81","18/297","Allow for Hard Rock in above trench","m3",30,"","",""]
["81","","CONFIRM CABLE ROUTE","H4",{"v":0,"d":"0.0"},"","",""]
["81","18/298","Price to confirm an existing supply cable route and position on site with a cable detector. Price per visit of one day ","SUM",1,"","",""]
["81","","Price to remove the following flush distribution boards. Disconnect and remove circuit breakers and other switchgear, disconnect conduits etc. ","H4",{"v":0,"d":"0.0"},"","",""]
["81","18/299","Up to 8 way","No",9,"","",""]
["81","18/300","Up to 12 way","No",6,"","",""]
["81","18/301","Up to 18 way","No",5,"","",""]
["82","","As above but for the following surface distribution boards:","H4",{"v":0,"d":"0.0"},"","",""]
["82","18/302","Up to 8 way","No",5,"","",""]
["82","18/303","Up to 18 way","No",7,"","",""]
["82","18/304","Up to 11 way 3phase","No",11,"","",""]
["82","","GENERAL LIGHTING   ","H4",{"v":0,"d":"0.0"},"","",""]
["82","18/305","Price to remove the PVC/ Galvanised conduit, internal and external wiring, wall/surface light switch, wall/surface plugs.","SUM",1,"","",""]
["82","","CONDUIT BOXES","H4",{"v":0,"d":"0.0"},"","",""]
["82","18/306","Price to remove Galvanised bosal, 100 x 50 x 50 switch boxes for 20mm dia conduit built into brick-work or cast into concrete (coverplates measured elsewhere) ","SUM",1,"","",""]
["82","","Equipment and Control Gear","H4",{"v":0,"d":"0.0"},"","",""]
["82","18/307","Galvanised steel, 100 x 100 x 50mm box for 20mm conduit built into brickwork or cast in concrete. (coverplates measured elsewhere)","SUM",1,"","",""]
["82","","LUMINAIRES","H4",{"v":0,"d":"0.0"},"","",""]
["82","18/308","Remove an existing recessed mounted, diffusser, three lamp and return to client.","SUM",1,"","",""]
["82","18/309","Remove an existing surface mounted, open channel, two lamp fluorescent luminaires and return to client. ","SUM",1,"","",""]
["82","18/310","Remove an existing surface mounted fluorescent/ bulkhead type luminaires and return to client.","SUM",1,"","",""]
["82","18/311","Remove an existing pole mounted luminaires (mounted on 6m poles), including additional floodlights and return to client.","SUM",1,"","",""]
["82","18/312","Remove an existing photo cells","SUM",1,"","",""]
["82","","TELEPHONE AND LAN SYSTEM WIRE-WAYS","H3",{"v":0,"d":"0.0"},"","",""]
["83","","CONDUIT ","H4",{"v":0,"d":"0.0"},"","",""]
["83","18/313","Price to remove all conduits and accessories to be PVC. The supply and installation of conduit including cuitting, bending,joints,settings, fittings, boxes, fixing materials","SUM",1,"","",""]
["83","18/314","Price to remove all PVC Slevees","SUM",1,"","",""]
["83","18/315","Price to remove 300 x 300 x 100mm board","SUM",1,"","",""]
["83","","SUNDRY ITEMS","H4",{"v":0,"d":"0.0"},"","",""]
["83","18/316","Allow sum for feature lighting to architects choice","SUM",1,"","",""]
["83","18/317","Provide certificate of compliance for all works","SUM",1,"","",""]

{"sheet":"1-19 BILL NO. 19","index":18,"n_rows":197,"n_cols":8,"rows_kept":197,"flags":["formulas_cached_only"]}
["04:05:25","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["84","","BILL NO. 19","H1",{"v":0,"d":"0.0"},"","",""]
["84","","MECHANICAL WORK","H1",{"v":0,"d":"0.0"},"","",""]
["84","","(CPAP WORK GROUP NO. 170 AND 172 AS APPLICABLE)","H2",{"v":0,"d":"0.0"},"","",""]
["84","","The Tenderer is referred to the relevant Clauses in the separate document ' Model Preambles for Trades 2008' ","",{"v":0,"d":"0.0"},"","",""]
["84","","SUPPLEMENTARY PREAMBLE","H3",{"v":0,"d":"0.0"},"","",""]
["85","","MISCELLANEOUS ITEMS","H2",{"v":0,"d":"0.0"},"","",""]
["85","","Outdoor Unit- Supply and install complete as specified including all fixures and fittings, auxilliaries and ancilliaries and refrigerant for entire system and hail guards. Note the total outdoor load includes the fresh air system load. 2.2.1 56kW Unit","H4",{"v":0,"d":"0.0"},"","",""]
["85","","Indoor Unit- Supply and install complete as specified including all fixures and fittings, control panels, auxilliaries and ancilliaries. Four way cassette units.","",{"v":0,"d":"0.0"},"","",""]
["85","","The system shall have the capability of providing heating or cooling to individual spaces simultaneously as specified and shown on the drawings. ","",{"v":0,"d":"0.0"},"","",""]
["85","","The tender price shall include for the equipment specified below as well as all branch controllers, refrigerant piping, refnet joints, auxilliary and ancilliary equipment etc. for the system to operate as specified.","",{"v":0,"d":"0.0"},"","",""]
["85","","Refrigerant pipe runs shall generally follow the routes shown on the drawings. Also the routes can be diverted where we have obstacles in the pre-designed path.","",{"v":0,"d":"0.0"},"","",""]
["85","","Air conditioning Installation","H2",{"v":0,"d":"0.0"},"","",""]
["85","","VRV - System ","H3",{"v":0,"d":"0.0"},"","",""]
["85","","Outdoor Unit- Supply and install complete as specified including all fixures and fittings, auxilliaries and ancilliaries and refrigerant for entire system and hail guards. Note the total outdoor load includes the fresh air system load.","H4",{"v":0,"d":"0.0"},"","",""]
["85","19/1","56kW","No",8,"","",""]
["85","","Indoor Unit- Supply and install complete as specified including all fixures and fittings, control panels, auxilliaries and ancilliaries. Midwall type indoor units","H4",{"v":0,"d":"0.0"},"","",""]
["85","19/2","1.4 kW","No",84,"","",""]
["85","19/3","2.3 kW","No",18,"","",""]
["86","","Indoor Unit- Supply and install complete as specified including all fixures and fittings, control panels, auxilliaries and ancilliaries. Four way cassette units. Roundflow cassette units","H4",{"v":0,"d":"0.0"},"","",""]
["86","19/4","4.3 kW","No",67,"","",""]
["86","","Medium duty galvanised, perforated cable tray complete with fittings and hangers to manufacturer's specifications","H4",{"v":0,"d":"0.0"},"","",""]
["86","19/5","300mm wide","m",405,"","",""]
["86","19/6","Electrical Installation complete with fittings and fixures","No",32,"","",""]
["86","19/7","Control panel and related switchgear ","No",19,"","",""]
["86","19/8","Wall wired remotes","No",91,"","",""]
["86","","Condensate drains including all fittings and fixtures","H4",{"v":0,"d":"0.0"},"","",""]
["86","19/9","25mm Condensate Drain Pipe","m",376,"","",""]
["86","19/10","32mm Condensate Drain Pipe","m",480,"","",""]
["86","19/11","Small items to complete this installation in full.","Item",{"v":1,"d":"1.00"},"","",""]
["86","","Water Heating ","H3",{"v":0,"d":"0.0"},"","",""]
["86","19/12","Supply and install commission 5 ltrs hydroboil 25-30 cup equivalent W 318mm x D150mm x H 431mm on top of kitchen sink","No",3,"","",""]
["86","19/13","190 ltrs heat pumps complete with all pipe works at the ablution","No",6,"","",""]
["86","","Air Conditioning Installation","H2",{"v":0,"d":"0.0"},"","",""]
["86","","AC Gas & liquid Piping and Fittings","H3",{"v":0,"d":"0.0"},"","",""]
["86","","For purposes of measuring extra over to piping and fittings measured under the system Bills. Supply and install air conditioning gas and liquid piping and fittings for R410A system","H4",{"v":0,"d":"0.0"},"","",""]
["86","19/14","Copper piping ø6.35mm","m",100,"","",""]
["86","19/15","Copper piping ø9.52mm","m",250,"","",""]
["86","19/16","Copper piping ø12.7mm","m",160,"","",""]
["87","19/17","Copper piping ø15.88mm","m",160,"","",""]
["87","19/18","Copper piping ø19.05mm","m",186,"","",""]
["87","19/19","56kW","m",6,"","",""]
["87","19/20","Copper piping ø28.58mm","m",30,"","",""]
["87","19/21","DCM601- intelligent touch Controller with allcomplete accessories","m",67,"","",""]
["87","19/22","Zoning kit BPG-DZKAPP with all complete accessories","m",12,"","",""]
["87",""," Day Works","H3",{"v":0,"d":"0.0"},"","",""]
["87","","Dayworks for items on site  and to be approved by the Engineer prior to implementation","H4",{"v":0,"d":"0.0"},"","",""]
["87","19/23","Qualified Artisan","Hrs",{"v":40,"d":"40.00"},"","",""]
["87","19/24","Semi-skilled labourer","Hrs",{"v":80,"d":"80.00"},"","",""]
["87","19/25","Labourer","Hrs",{"v":160,"d":"160.00"},"","",""]
["87","","HEATING VENTILATION AND AIR CONDITIONING INSTALLATION","H2",{"v":0,"d":"0.0"},"","",""]
["87",""," Fresh Air System","H3",{"v":0,"d":"0.0"},"","",""]
["87","19/26","600x350 Weather Louvre,Natural anodised finish, Filter box and filter+WMS ","No",8,"","",""]
["87","","In Line Fan - FAF 01","H4",{"v":0,"d":"0.0"},"","",""]
["87","19/27","Supply and install in line duct fan, axial inline fan, Duty 500 l/s c/w 2 x 1.5D sound attenuators","No",7,"","",""]
["87","","Wall Mounted extract fans - EF 01, 02,03,04 &05","H4",{"v":0,"d":"0.0"},"","",""]
["87","19/28","Wall mounted extract fans Duty 50 l/s","No",17,"","",""]
["87","19/29","Wall mounted control ON/OFF switches, power & control cables","No",15,"","",""]
["87","19/30","7 days timer controller to the fan","No",21,"","",""]
["87","","Galvanised Sheet Metal Ducting","H3",{"v":0,"d":"0.0"},"","",""]
["88","","Low pressure, uninsulated, galvanised ducting & ancillaries including supports & fixings ","H4",{"v":0,"d":"0.0"},"","",""]
["88","19/31","600x350 wall sleeve","No",8,"","",""]
["88","19/32","Transformation piece 600x350 to dia 400","No",8,"","",""]
["88","19/33","Transformation piece 550x200 to dia 400","No",8,"","",""]
["88","19/34","500x200","m",79,"","",""]
["88","19/35","90 degree bend 500x200","No",7,"","",""]
["88","19/36","Reducer 500x200 to 400x200","No",7,"","",""]
["88","19/37","500x200","m",40,"","",""]
["88","19/38","Reducer 400x200 to 300x200","No",7,"","",""]
["88","19/39","300x200","m",94,"","",""]
["88","19/40","200x150","m",54,"","",""]
["88","19/41","300x150","m",48,"","",""]
["88","19/42","150x150","m",84,"","",""]
["88","19/43","Straight ducting dia 150 mm","m",240,"","",""]
["88","","Stop End","H4",{"v":0,"d":"0.0"},"","",""]
["88","19/44","300x200","No",8,"","",""]
["88","19/45","150x150","No",47,"","",""]
["88","19/46","200x150","No",24,"","",""]
["88","","Spigots","H4",{"v":0,"d":"0.0"},"","",""]
["88","19/47","Galvanised sheet metal spigot 150 mm diam.","No",134,"","",""]
["88","","Balancing Dampers","H4",{"v":0,"d":"0.0"},"","",""]
["88","19/48","Galvanised sheet metal dampers 150 mm diam.","No",137,"","",""]
["89","","Take Off","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/49","Galvanised sheet metal 45 deg. Shoe takeoff 200 x150 mm .","No",24,"","",""]
["89","19/50","Galvanised sheet metal 45 deg. Shoe takeoff 150 x150 mm .","No",49,"","",""]
["89","19/51","Galvanised sheet metal 45 deg. Shoe takeoff 300 x150 mm .","No",20,"","",""]
["89","","Flexible Ducting","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/52","150 mm diam un-insulated flexible ducting.","m",290,"","",""]
["89","","Diffusers & Ventilators","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/53","Supply and install 150 mm diam ceiling disc diffuser with balancing disc.","No",122,"","",""]
["89","19/54","250x250 Door Grille","No",19,"","",""]
["89","","Electrical Connection","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/55","Supply and install power cable to isolator provided by others, in roof space.","No",7,"","",""]
["89","","Hangers & Brackets","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/56","Supply, Install, test, commission and provide 12 month guarantee for all hangers, brackets and etc. for fresh air & extraction ducting all as specified.","No",7,"","",""]
["89","19/57","600x350 Weather Louvre,Natural anodised finish, Filter box and filter+WMS ","No",5,"","",""]
["89","19/58","300 x300 Weather Louvre,Natural anodised finish","No",7,"","",""]
["89","","In Line Fan - FAF 02","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/59","Supply and install in line duct fan, axial inline fan, Duty 650 l/s c/w 2 x 1.5D sound attenuators","No",5,"","",""]
["89","","In Line Fan - EF-07","H4",{"v":0,"d":"0.0"},"","",""]
["89","19/60","Supply and install in line duct fan, axial inline fan, Duty 300 l/s @150Pa c/w 2 x 1.5D sound attenuators","No",10,"","",""]
["90","19/61","Supply and install in line duct fan, axial inline fan, Duty 200 l/s c/w 2 x 1.5D sound attenuators","No",2,"","",""]
["90","19/62","Wall mounted control ON/OFF switches, power & control cables","No",30,"","",""]
["90","19/63","7 days timer controller to the fan","No",30,"","",""]
["90","","Galvanised Sheet Metal Ducting","H4",{"v":0,"d":"0.0"},"","",""]
["90","","Low pressure, uninsulated, galvanised ducting & ancillaries including supports & fixings ","H4",{"v":0,"d":"0.0"},"","",""]
["90","19/64","600x350 wall sleeve","No",5,"","",""]
["90","19/65","300x300 wall sleeve","No",7,"","",""]
["90","19/66","Transformation piece 600x350 to dia 400","No",7,"","",""]
["90","19/67","Transformation piece 600x200 to dia 400","No",5,"","",""]
["90","19/68","Transformation piece 200x200 to dia 200","No",6,"","",""]
["90","19/69","Transformation piece 300x300  to dia 200","No",9,"","",""]
["90","19/70","600x200","m",8,"","",""]
["90","19/71","90 degree bend 500x200","No",11,"","",""]
["90","19/72","90 degree bend 200x200","No",11,"","",""]
["90","19/73","Reducer 500x200 to 300x200","No",5,"","",""]
["90","19/74","300x200","m",60,"","",""]
["90","19/75","Reducer 300x150 to 150x150","No",20,"","",""]
["90","19/76","300x150","m",36,"","",""]
["90","19/77","90 degree bend 500x200","No",{"v":0,"d":"0.0"},"","",""]
["90","19/78","150x150","m",90,"","",""]
["90","19/79","200x150","m",139,"","",""]
["90","19/80","200x200","m",85,"","",""]
["90","19/81","Straight ducting dia 150 mm","m",236,"","",""]
["91","","Stop end","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/82","300x200","No",4,"","",""]
["91","19/83","150x150","No",14,"","",""]
["91","19/84","200x150","No",14,"","",""]
["91","19/85","200x200","No",8,"","",""]
["91","","Take Off","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/86","Galvanised sheet metal 45 deg. Shoe takeoff 200 x150 mm .","No",16,"","",""]
["91","19/87","Galvanised sheet metal 45 deg. Shoe takeoff 300 x150 mm .","No",21,"","",""]
["91","","Spigots","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/88","Galvanised sheet metal spigot 150 mm diam.","No",126,"","",""]
["91","","Flexible Ducting","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/89","150 mm diam un-insulated flexible ducting.","m",260,"","",""]
["91","","Diffusers & Ventilators","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/90","Supply and install 150 mm diam ceiling disc diffuser with balancing disc.","No",119,"","",""]
["91","19/91","250x250 Door Grille","No",30,"","",""]
["91","","Electrical Connection","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/92","Supply and install power cable to isolator provided by others, in roof space.","No",54,"","",""]
["91","","Hangers & Brackets","H4",{"v":0,"d":"0.0"},"","",""]
["91","19/93","Supply, Install, test, commission and provide 12 month guarantee for all hangers, brackets and etc. for fresh air & extraction ducting all as specified.","No",5,"","",""]
["91","","FIRE DETECTION SYSTEM","H1",{"v":0,"d":"0.0"},"","",""]
["92","","Supply, installation and commisioning of analogue addressable fire detection system including all cabling, devices and connections as listed.","H4",{"v":0,"d":"0.0"},"","",""]
["92","19/94","8 Loop Fire Control Panel ","No",1,"","",""]
["92","19/95","4 Loop Fire Control Panel ","No",7,"","",""]
["92","19/96","Battery back up system","No",9,"","",""]
["92","19/97","Addressable Multisensor  (algorithm  based technology)","No",342,"","",""]
["92","19/98","Addressable Sounder","No",63,"","",""]
["92","19/99","Addressable Call Point (Break Glass)","No",35,"","",""]
["92","19/100","Addressable unit monitored outputs for driving sounders C/W mounting box. ","No",41,"","",""]
["92","19/101","Relay ( interface )","No",20,"","",""]
["92","19/102","Teledialer system linked to the Fire department or police station ","SUM",9,"","",""]
["92","19/103","120db 24 V DC evacuation siren C/W mounting brackets and all fixing materials.","No",15,"","",""]
["92","19/104","PH30 Fire cable","m",15320,"","",""]
["92","","Supply and install conduit as specified placed in position for surface mounting on concrete or brickwork, and for surface mounting in ceiling void including bending, jointing, cutting, draw boxes, coupling, inspection bends, bends, tees and saddles  ","H4",{"v":0,"d":"0.0"},"","",""]
["92","19/105","25mm galvanised sprague","m",10080,"","",""]
["92","19/106","Line isolator and base","No",53,"","",""]
["92","19/107","Screwed dome lids for conduit boxes","No",662,"","",""]
["92","19/108","20mm flexible PVC coated conduit (Kopex), in 1 metre lengths","No",517,"","",""]
["93","19/109","8mm flexible PVC coated conduit (Kopex), in 1 metre lengths","No",294,"","",""]
["93","","Supply and install screened conductor (FR20) as specified, for connecting fire panel to line devices and sensors. Conductor  to be into conduit /ducting. ","H4",{"v":0,"d":"0.0"},"","",""]
["93","19/110","Low levelMagnet door hold backmounted @300mmAFFL and 150mm from the end","No",37,"","",""]
["93","19/111","Strobe Worning light","No",12,"","",""]
["93","19/112","1mm sq x 2 core screened cable (loop cable)","m",14580,"","",""]
["93","","STAIRCASE PRESSURIZING FAN & ELEVATOR SHAFT PRESSURIZING FAN","H1",{"v":0,"d":"0.0"},"","",""]
["93","","Supply, installation and commisioning of analogue addressable fire detection system including all cabling, devices and connections as listed.","H4",{"v":0,"d":"0.0"},"","",""]
["93","19/113","Elevator Shaft Pressurizing  Fan  -892 l/s With all accessories necessary to install","No",2,"","",""]
["93","19/114","Staircase Pressuring Fan - 10437 l/s With all accessories necessary to install","No",2,"","",""]
["93","19/115","Automatic Opening Smoke detector Ventilator 40x400","No",16,"","",""]
["93","19/116","Smoke detector","No",12,"","",""]
["93","19/117","Automatic Elevator Shaft Smoke Ventilator System Mounted at roof top of the Elevator Shaft linked  and controlled by Smoke Detector to open","No",2,"","",""]
["93","19/118","Door grills","No",8,"","",""]
["93","19/119","Relay ( interface )","No",2,"","",""]
["93","19/120","32 Way Eletrical controlpanel with Variable speed drive  place next to SPF  and  ESPF postion ( Electrican) to  provide","No",4,"","",""]
["93","19/121","PH30 Fire cable","m",1780,"","",""]
["94","","Supply and install conduit as specified placed in position for surface mounting on concrete or brickwork, and for surface mounting in ceiling void including bending, jointing, cutting, draw boxes, coupling, inspection bends, bends, tees and saddles ","H4",{"v":0,"d":"0.0"},"","",""]
["94","19/122","25mm galvanised sprague","m",600,"","",""]
["94","19/123","Screwed dome lids for conduit boxes","No",24,"","",""]
["94","19/124","20mm flexible PVC coated conduit (Kopex), in 1 metre lengths","No",96,"","",""]
["94","19/125","8mm flexible PVC coated conduit (Kopex), in 1 metre lengths","No",104,"","",""]
["94","19/126","Fire resistance duct 250x450mm square","m",98,"","",""]
["94","19/127","Low levelMagnet door hold backmounted @300mmAFFL and 150mm from the end","No",12,"","",""]
["94","","Installation of Fire Hydrant","H3",{"v":0,"d":"0.0"},"","",""]
["94","19/128","Provision Of Supply and Install fire hydrant in 150m away from the existing Main water line ","SUM",1,"","",""]
["94","","Excavation","H4",{"v":0,"d":"0.0"},"","",""]
["94","19/129","Escavation of 60m and lay 2x 110 sleevs to link executive block, Guard house  and Block C fire pannel","m3",22,"","",""]
["94","19/130","Cutting Tare and Replacement","m3",6,"","",""]
["94","","Fire Protection at the Parking Area","H4",{"v":0,"d":"0.0"},"","",""]
["94","19/131","Supply and Install 9 kg Fire exsitnguishers  at the specified ares at the caparking","No",14,"","",""]
["94","","Excavation","H4",{"v":0,"d":"0.0"},"","",""]
["94","19/132","Escavation of 60m and lay 2x 110 sleevs to link executive block, Guard house  and Block C fire pannel","m3",16,"","",""]
["94","","Sleeves","H4",{"v":0,"d":"0.0"},"","",""]
["94","19/133","110 Dia","m",120,"","",""]

{"sheet":"1-20 Summary","index":19,"n_rows":24,"n_cols":8,"rows_kept":24,"flags":["formulas_cached_only"]}
["04:05:25","."]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["95","1","PRELIMINARIES","Page",18,0,"",""]
["95","2","ALTERATIONS","Page",23,0,"",""]
["95","3","MASONARY","Page",26,0,"",""]
["95","4","WATERPROOFING","Page",27,0,"",""]
["95","5","ROOF COVERING","Page",29,0,"",""]
["95","6","CARPENTRY & JOINERY","Page",33,0,"",""]
["95","7","CEILINGS, PARTITION AND ACCESS FLOORING","Page",35,0,"",""]
["95","8","FLOOR COVERING","Page",37,0,"",""]
["95","9","IRONMONGERY","Page",40,0,"",""]
["95","10","METALWORK","Page",42,0,"",""]
["95","11","PLASTERING","Page",44,0,"",""]
["95","12","TILING","Page",45,0,"",""]
["95","13","PLUMBING AND DRAINAGE","Page",48,0,"",""]
["95","14","GLAZING","Page",49,0,"",""]
["95","15","PAINTING","Page",53,0,"",""]
["95","16","PAPERHANGING","Page",54,0,"",""]
["95","17","PROVISIONAL SUMS","Page",55,0,"",""]
["95","18","Electrical Installation","Page",83,0,"",""]
["95","19","Mechanical Installation","Page",94,0,"",""]
["95","","Sub Total","ST",{"v":0,"d":"0.00"},"","Sub Total",""]
["95","","VAT @ 15%","TAX",{"v":15,"d":"15.00"},"","",""]