Schedule 18 - Decommissioning  
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Decommissioning of existing STPs
[bookmark: _Ref110317663]GENERAL
There are presently a total of seven existing STPs operational in the two areas. Six of these existing STPs shall be decommissioned once the new Conveyance systems and treatment infrastructure are in place and operational.

In the Northern project area (uMdloti) the existing STPs to be decommissioned are:
· Genazzano STP
· Umdloti STP
· Verulam STP
· King Shaka International (KSIA) package STP

In the Southern project area (Umkomaas) the existing STPs to be decommissioned are:
· Umkomaas STP
· Craigieburn STP

Decommissioning of the existing STPs shall include the requirements set out in 2 below.
[bookmark: _Ref110317642]REQUIREMENTS FOR DECOMMISSIONING
Assessment and remediation plan
The Concessionaire shall undertake Environmental Site Assessments for each of the existing STPs that are to be decommissioned and if deemed required shall develop and execute site remediation plans in accordance with the E&S Minimum Requirements and the associated standards. 
Mechanical and electrical equipment
All superfluous mechanical and electrical equipment must be removed, and the municipality must be notified of all power supply points that become redundant.
Reuse of structures
Structures that can be reused for the raw sewage Conveyance systems shall be repurposed accordingly and must be modified and/or adapted as required, made safe for the intended purpose and fenced off from the remainder of the site.

Where existing structures are repurposed, these must be repaired or refurbished to suit their intended purpose and shall be maintained and repaired periodically so that the structure has a remaining useful life of 20 years at the end of the PPP term.
Safety and redundant structures
Redundant structures must be made safe where possible. Given the nature of the sites and structures, this must specifically address requirements to eliminate fall and/or drown hazards and unauthorised entry. Redundant structures that cannot be made safe must be demolished.
Landscaping
Areas where structures are removed or demolished must be planted with suitable ground coverings. Similarly, all areas that are potentially at risk of erosion must be landscaped and planted with suitable ground coverings in a manner that will mitigate the risk of erosion.
Fencing
All redundant STPs shall be fenced and provided with a secured point of access.

Environmental, Social and Health and Safety 
E&S management of decommissioning is addressed under Schedule 13. 
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