{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":3,"rows_kept":34}
["ACQUISITION OF MOBILE RAMPS CHECKLIST"]
[]
[]
["ITEM NUMBER","ITEM","ü  TICK"]
["i.","Proven track record of no less than two (2) years in the supply and delivery of mobile ramps.\n\nThe following must be submitted:"]
[1,"A reference letter relating to the appointment letter/contract. The reference letter shall indicate the following: "]
[2,"Company name, contact person, and confirmation of products supplied. "]
[]
["ii.","Bidders must provide the following information pertaining to the product offered:"]
[1," Product documentation"]
[2,"Concept Drawings"]
[]
["iii.","Bidders must provide detailed technical specifications of the product (mobile ramps) conforming to the following items:"]
[null,"Detailed technical specifications as listed below:"]
[]
[1,"The ramps should be made of durable materials such as aluminium or steel."]
[2,"The ramps should have a secure attachment mechanism to the platform and the train."]
[3,"The ramps should be easy to assemble and disassemble for storage when not in use."]
[4,"The ramps should have wheels for easy transport to different locations on the platform."]
[5]
[6,"The ramps should be designed to fit different platform heights, and train configurations by the requirements outlined in SANS ARP 084 - 1:2009, SANS 10400 Part S 2011."]
[7," The ramps should have handrails on both sides to support and stabilize passengers."]
[8,"The ramps should have a weight capacity of at least 150 kg to accommodate passengers in wheelchairs and their mobility devices."]
[9,"The width of the ramp should be at least 700mm to accommodate the passage of a standard-sized wheelchair."]
[10,"The ramp length should be sufficient to create a slope of no more than 1:12 for the required platform height. The exact length will depend on the specific platform height and train configuration."]
[11,"The height of the handrails should be between 860mm and 960 mm above the ramp surface."]
[12,"The ramps should withstand outdoor weather conditions like rain and excessive heat."]
[" "]
["iv.","SHE FILE CHECKLIST, providing the following items:"]
[null,"1.      Organisational structure"]
[null,"2.      Safety Health and Environmental Plan"]
[null,"3.      Risk assessment"]
[null,"4.    Method statement"]
[null,"5.    Safe working procedure"]