{"text_format":"3","workbook":"xls","n_sheets":10,"sheets":["Cover","P&G's","Inspections","Stabilisation","Access & Env","Foundations","Structural Work","Crossing","Tower labels & Bird Guards","Summary"],"not_rendered":{"external_links":2,"defined_names":14},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Cover","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"merged":[[2,1,2,4],[3,1,3,4],[4,1,4,4],[5,1,5,4],[6,1,6,4],[7,1,7,4],[8,1,8,4],[9,1,9,4],[10,1,10,4],[11,1,11,4],[12,1,12,4],[13,1,13,4],[14,1,14,4],[15,1,15,4],[16,1,16,4],[17,1,17,4],[18,1,18,4],[19,1,19,4],[20,1,20,4],[21,1,21,4],[22,1,22,4],[23,1,23,4],[24,1,24,4],[25,1,25,4],[26,1,26,4],[27,1,27,4],[28,1,28,4],[29,1,29,4],[30,1,30,4],[31,1,31,4],[32,1,32,4],[33,1,33,4]],"flags":["formulas_cached_only"]}
[]
[]
[null,"PROVISIONAL SCHEDULE OF QUANTITIES"]
[]
[null,"FOR "]
[]
[null,"ESKOM TRANSMISSION GRIDS"]
[null,"FRAMEWORK BoQ FOR EMERGENCY PROJECTS"]
[]
[]
[null,"FOR"]
[]
[null,"ESKOM TRANSMISSION"]
[null,"MEGAWATT PARK"]
[null,"MAXWELL DRIVE"]
[null,"SUNNINGHILL"]
[]
[{"$nulls":4}," "]
[]
[]
[]
[]
[]
[null,"Document Prepared by"]
[null,"Asset Management Projects Execution Department"]
[null,"Quantity Surveying Group"]

{"sheet":"P&G's","index":1,"n_rows":212,"n_cols":6,"rows_kept":212,"merged":[[4,0,5,1]],"flags":["formulas_cached_only"]}
["TRANSMISSION PROJECT LINES - FRAMEWORK BoQ"]
[]
["SECTION NO. 1"]
["PRELIMINARY AND GENERAL"]
["Note: The Preliminary & General will be priced/negotiated at the percentage cost of the specific detailed scope per task order "]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SECTION NO. 1"]
[]
[null,"SCHEDULE NO. 1"]
[]
[null,"PRELIMINARY AND GENERAL "]
[null,"(Applicable to the whole of the"]
[null," Works) "]
[]
[null,"FIXED CHARGE ITEMS "]
[]
[1,"Contractual requirements","SUM"]
[]
[null,"Establishment of Facilities on the Site "]
[]
[null,"Facilities for Engineer "]
[]
[2,"Name boards.  (In No. 2)","SUM"]
[]
[null,"Facilities for Contractor "]
[]
[3,"Offices and storage sheds","SUM"]
[]
[4,"Workshops","SUM"]
[]
[5,"Laboratories","SUM"]
[]
[6,"Living accommodation","SUM"]
[]
[7,"Ablution and latrine facilities","SUM"]
[]
[8,"Tools and equipment","SUM"]
[]
[9,"Water supplies, electric power,"]
[null,"communications, dealing with water, and"]
[null,"access","SUM"]
[]
[10,"Dealing with water","SUM"]
[]
[11,"Access","SUM"]
[]
[12,"Plant","SUM"]
[]
[13,"Other fixed charge obligations","SUM"]
[]
[14,"Removal of site establishment","SUM"]
[]
[15,"Complying with Eskom Health and Safety"]
[null,"Specifications","SUM"]
[]
[16,"Complying with the Mine Health and Safety"]
[null,"Specifications","SUM"]
[]
[17,"Complying with Environmental"]
[null,"Management Programme Act and all other"]
[null,"statutory environmental requirements","SUM"]
[]
[18,"Security for the works for duration of the Contract, equivalent to Bidvest.","SUM"]
[]
[]
[19,"Detailed \"as built\" records (as per works information) 3 soft copies and 1 hard copy","SUM"]
[]
[]
[null,"CARRIED FORWARD"]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"BROUGHT FORWARD"]
[]
[null,"TIME RELATED ITEMS "]
[]
[20,"Contractual requirements","SUM"]
[]
[null,"Operation and Maintenance of Facilities on"]
[null," Site, for Duration of Construction, (unless"]
[null," otherwise stated) "]
[]
[null,"Facilities for Engineer "]
[]
[21,"Name boards.  (In No. 2)","SUM"]
[]
[null,"Facilities for Contractor "]
[]
[22,"Offices and storage sheds","SUM"]
[]
[23,"Workshops","SUM"]
[]
[24,"Laboratories","SUM"]
[]
[25,"Living accommodation","SUM"]
[]
[26,"Ablution and latrine facilities ","SUM"]
[]
[27,"Tools and equipment","SUM"]
[]
[28,"Water supplies, electric power,"]
[null," communications, dealing with water, and"]
[null," access","SUM"]
[]
[29,"Dealing with water","SUM"]
[]
[30,"Access","SUM"]
[]
[31,"Plant","SUM"]
[]
[32,"Supervision for duration of construction","SUM"]
[]
[33,"Complying with Eskom Health and Safety"]
[null,"Specifications","SUM"]
[]
[34,"Complying with the Mine Health and Safety"]
[null,"Specifications","SUM"]
[]
[35,"Company and head office overhead costs"]
[null,"for duration of construction","SUM"]
[]
[36,"Other time related obligations","SUM"]
[]
[37,"Complying with Environmental"]
[null,"Management Programme and all other"]
[null,"statutory environmental requirements","SUM"]
[]
[38,"Security for the works for duration of the Contract, equivalent to Bidvest.","SUM"]
[]
[]
[39,"Detailed \"as built\" records (as per works information) 3 soft copies and 1 hard copy","SUM"]
[]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]
[]
[]
[]
[]
["SECTION NO. 2  -"]
["PROVISIONAL"]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SECTION NO. 2."]
[null,"SCHEDULE NO. 1"]
[]
[null,"INSPECTION"]
[null,"Note: This will be used as instructed by the Project Manager and paid with a Site Instruction."]
[]
[null,"Transportation for free issue material due to employers risk: (PROVISIONAL)"]
[]
[1,"Provisional sum, for the collection and delivery of free issue material supplied by Eskom from a predetermined location to site, with a 10 ton flatbed truck including truck hire, driver, etc., complete. (Provisional)","Km",null,null,"Rate only"]
[]
[null,"PROVISIONAL DAYWORKS"]
[]
[null,"Standing Time Due to Employers Risk (Provisional):"]
[null,"Labour "]
[]
[2,"Project Engineer","hr",null,null,"Rate only"]
[]
[3,"Site Engineer","hr",null,null,"Rate only"]
[]
[4,"Design Engineer","hr",null,null,"Rate only"]
[]
[5,"Site Foreman","hr",null,null,"Rate only"]
[]
[6,"Supervisors","hr",null,null,"Rate only"]
[]
[7,"Leadinghands","hr",null,null,"Rate only"]
[]
[8,"Linesman/ Erector","hr",null,null,"Rate only"]
[]
[9,"Semi skilled Labourers","hr",null,null,"Rate only"]
[]
[10,"Unskilled Labourers","hr",null,null,"Rate only"]
[]
[11,"Community Laising Officer (CLO)","month",null,null,"Rate only"]
[]
[12,"Driver Operator","hr",null,null,"Rate only"]
[]
[null,"Transport and Plant"]
[13,"4 x 4 Light vehicle","day",null,null,"Rate only"]
[]
[14,"4 x 4 Light vehicle","km",null,null,"Rate only"]
[]
[15,"8 Ton truck","hr",null,null,"Rate only"]
[]
[16,"8 Ton truck","km",null,null,"Rate only"]
[]
[17,"10 Ton truck","hr",null,null,"Rate only"]
[]
[18,"10 Ton truck","km",null,null,"Rate only"]
[]
[19,"20 Ton Crane Truck","hr sta",null,null,"Rate only"]
[]
[20,"20 Ton Crane Truck","hr wo",null,null,"Rate only"]
[]
[21,"TLB","hr sta",null,null,"Rate only"]
[]
[22,"TLB","hr wo",null,null,"Rate only"]
[]
[23,"Tension stringing equipment set","hr sta",null,null,"Rate only"]
[]
[24,"Tension stringing equipment set","hr wo",null,null,"Rate only"]
[]
[25,"Day shift security guard grade C - unarmed","hr",null,null,"Rate only"]
[]
[26,"Night shift security guard grade C - armed","hr",null,null,"Rate only"]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Inspections","index":2,"n_rows":29,"n_cols":6,"rows_kept":29,"flags":["formulas_cached_only"]}
[]
[]
[null,"SECTION NO. 3 : "]
[]
[null,"INSPECTION"]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"WORKS TO DISMANTLE AS DETAILED IN THE WORKS INFORMATION (240-47172520) AND TECHNICAL SPECIFICATIONS REQUIREMENT."]
[]
[null,"REMOVAL OF EXISTING HARDWARE, INSULATORS AND CONDUCTOR : Contractor to design and submit for approval alternate methods in order to prevent downtime on the line during replacement.  "]
[]
[]
[null,"Conduct visual inspections on all towers affected ensure structural intergrity, and compile/provide report.","tower",null,null,"Rate only"]
[]
[null,"Removal of existing   Phase (3 x) conductors by cutting to collectable sizes. Conductor scrap to be collected by Eskom's approved scrapmetal dealer.","km",null,null,"Rate only"]
[]
[null,"Removal of existing hardware assemblies and insulators","Sum",null,null,"Rate only"]
[]
[null,"Poletop inspection","Sum",null,null,"Rate only"]
[]
[null,"Assessment for conductors","Sum",null,null,"Rate only"]
[]
[null,"Assessmen","Sum",null,null,"Rate only"]
[]
[null,"Damage & slippage","Sum",null,null,"Rate only"]
[]
[null,"Guy wired inspections (rope & fittings)","Sum",null,null,"Rate only"]
[]
[null,"Stub and link","Sum",null,null,"Rate only"]

{"sheet":"Stabilisation","index":3,"n_rows":22,"n_cols":6,"rows_kept":22,"flags":["formulas_cached_only"]}
[]
[]
[null,"SECTION NO. 4 : "]
[]
[null,"STABILISATION"]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"WORKS TO DISMANTLE AS EXECUTION IN THE WORKS INFORMATION (240-47172520) AND TECHNICAL SPECIFICATIONS REQUIREMENT."]
[]
[1,"stolen members - replace / add","Towers",null,null,"rate only"]
[]
[2,"Backstay the unstable towers  - crane to support stabilisation","Towers",null,null,"rate only"]
[]
[3,"Backstay of unstable towers","Towers",null,null,"rate only"]
[]
[4,"Backstay of the conductors on the ground","No",null,null,"rate only"]
[]
[]
[5,"Backstaying of towers to enable dismantling and future connections (backstaying of each phase plus each earthwire) . Preference is given to concrete blocks, sledges and stay wire for backstaying.","No",null,null,"rate only"]
[]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Access & Env","index":4,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[8,0,10,0],[8,1,10,1],[8,3,10,3],[8,4,10,4],[8,5,10,5]],"flags":["formulas_cached_only"]}
[]
[]
[null,"SECTION NO. 5"]
[null,"ACCESS"]
["BILL ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[]
[null,"SCHEDULE NO. 1 - PROVISIONAL"]
[3.1,"BUSH CLEARING : To be carried out in three phases in accordance with TRMSCAAC6, Act 36 of 1947and EPC 32-247 and the Environmental Management Plan, including chemical treatment to prevent regrowth, de-stumping, cutting of felled trees into manageable sizes and stacking on servitude/road edge."]
[]
[]
[1,"Clearance of max. 8m wide strip along centre of servitude as per ESKASABG3 (refer to clause 4.3)","km",null,null,"Rate Only"]
[2,"Clearance around tower sites and guys as per ESKASABG3 (refer to clause 4.3) (Provisional)","Tower",null,null,"Rate Only"]
[3,"Selective trimming or cutting down of indigenous vegetation outside the 8m strip (item 3.1)(refer to clause 4.3)","km",null,null,"Rate Only"]
[4,"Clearance of alien species within the servitude as per Regulation GNR.1048 of 25 May 1984\n","km",null,null,"Rate Only"]
[5,"As per TRMSCAAC6 and EPC 32-247 and the Enviromental Plan, Including chemical treatment to prevent regrowth, de-stumping, cutting of felled trees into mangeable sizes and stacking on servitude/road edge at all tower positons.","sum",null,null,"Rate Only"]
[3.2,"ENVIRONMENTAL AND REHABILITATION REQUIREMENTS"]
[1,"Rehabilitation of damage caused during construction of access and servitude roads. in accordance with the requirements of the  TRMSCAAC6 and EPC 32-247."," km.",null,null,"Rate Only"]
[2,"Rehabilitation of damage caused during construction to tower sites, camp sites, batching plant site, etc. in accordance with the requirements of the TRMSCAAC6 and EPC 32-247.","km",null,null,"Rate Only"]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Foundations","index":5,"n_rows":38,"n_cols":6,"rows_kept":38,"flags":["formulas_cached_only"]}
[]
["SECTION NO. 6 : "]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[]
[]
[null,"SCHEDULE NO. 1"]
[]
[null,"Works to be done as per  technical aspects from 240-57127951 and SAICE Code of Practice (2010)."]
[]
[null,"FOUNDATIONS (PROVISIONAL)"]
[]
[null,"Design and Construct Reinforced concrete  foundation cap for installed micropiles including  excavation, reinforcement steel, formwork, backfilling with approved imported material, compacting to approved density, soil tests, test tubes, setting out, carting away of excavated material to an approved registered dump site, etc., complete:"]
[]
[null,"Foundation Type :"]
[]
[1,"Reinforced concrete foundation \"Type 1\" for tower type  complete as per attached standard specification (per leg).","No.",null,null,"rate only"]
[]
[2,"Reinforced concrete foundation \"Type 2\" for tower type  complete as per attached standard specification (per leg).","No.",null,null,"rate only"]
[]
[3,"Reinforced concrete foundation \"Type 3\" for tower type  complete as per attached standard specification (per leg).","No.",null,null,"rate only"]
[]
[4,"Reinforced concrete foundation \"Type 4\" for tower type  complete as per attached standard specification (per leg).","No.",null,null,"rate only"]
[]
[5,"Reinforced concrete foundation \"Soft Rock\" for tower type  complete as per attached standard specification (per leg).","No",null,null,"rate only"]
[]
[6,"Reinforced concrete foundation \"Hard Rock\" for tower type  complete as per attached standard specification (per leg).","No",null,null,"rate only"]
[]
[null,"SOIL NOMINATION "]
[null,"Nominations of foundation types to be done on site by a Civil Engineer. Civil Engineer to specify which of the foundation types must be used for each structure. ","No",null,null,"rate only"]
[]
[]
[]
[]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Structural Work","index":6,"n_rows":95,"n_cols":6,"rows_kept":95,"flags":["formulas_cached_only"]}
[]
["SECTION NO. 7 : "]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"STRUCTURAL STEEL WORK"]
[null,"Supply and Delivery new tower steel members and accessories to site: including anti climb devices, tower shackles, bolts, etc., complete as per attached standard specification."]
[]
[1,"Steel tower structures ","Tonne",null,null,"rate only"]
[2,"Supply a Steel monopole towers","Tonne",null,null,"rate only"]
[]
[3,"Supply and install complete anti-climb devices include all accessories .","No",null,null,"rate only"]
[]
[4,"Supply and install all the damage tower members.","Kg",null,null,"rate only"]
[5,"Supply  new earthpeak for tower  ( ton weight), completet as per detailed specification","No",null,null,"rate only"]
[]
[]
[null,"Assembly of new towers"]
[]
[6,"Steel tower structures ","No",null,null,"rate only"]
[7,"Supply a Steel monopole towers","No",null,null,"rate only"]
[8,"Supply and install complete anti-climb devices include all accessories .","No",null,null,"rate only"]
[]
[9,"Supply and install all the damage tower members.","No",null,null,"rate only"]
[]
[10,"Supply  new earthpeak for tower  ( ton weight), completet as per detailed specification","No",null,null,"rate only"]
[]
[]
[null,"Erection of new towers"]
[]
[11,"Steel tower structures ","No",null,null,"rate only"]
[12,"Supply a Steel monopole towers","No",null,null,"rate only"]
[13,"Supply and install complete anti-climb devices include all accessories .","No",null,null,"rate only"]
[14,"Supply and install all the damage tower members.","No",null,null,"rate only"]
[15,"Supply  new earthpeak for tower  ( ton weight), completet as per detailed specification","No.",null,null,"rate only"]
[]
[]
[]
[null,"Installation of accessories (Dressing) of towers with earthwire assembly complete: (Material Supplied by Eskom)"]
[]
[16,"Strain assembly with earth conductor accessories to strain towers complete as per attached standard specification .","Towers",null,null,"rate only"]
[17,"Suspension assembly with earth conductor accessories to suspension tower complete as per attached standard specification ","Towers",null,null,"rate only"]
[]
[null,"Installation of accessories (Dressing) of towers with phase conductor assembly complete: (Material Supplied by Eskom)"]
[]
[18,"Dressing of the towers with phase conductor accessories to self supporting towers  complete as per attached standard specification. ","Towers",null,null,"rate only"]
[]
[19,"Dressing of the towers with phase conductor accessories to strain towers  complete as per attached standard specification. ","Towers",null,null,"rate only"]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]
[{"$nulls":5},{"v":0,"d":"0.00"}]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SECTION NO. 6."]
[]
[null,"SCHEDULE NO. 2"]
[]
[]
[null,"Stringing and regulating of Earthwires "]
[]
[1,"Stringing and regulation of 2x19/2.65 earthwire Between towers  (both phases)- route length","M",null,null,"rate only"]
[2,"Ducting of earthing for underpass (including excavation - route length)","M",null,null,"rate only"]
[3,"Joining of existing earthwire to new earthwire (join at existing tower ","No",null,null,"rate only"]
[4,"Installation of vibration dampers on earthwires","No",null,null,"rate only"]
[]
[null,"Stringing and regulation of the phase conductor "]
[]
[5,"Stringing and regulation of the phase conductor - route length","M",null,null,"rate only"]
[]
[6,"Joining of new conductor to existing conductor at existing towers  - cater for installation of new strain assemblies on one side of existing towers. Cater for modification of existing jumpers. Include for dressing of half of existing towers with new hardware.","per phase",null,null,"rate only"]
[]
[7,"Installation of vibration dampers on twin Dinosaur","No",null,null,"rate only"]
[]
[8,"Installation of spacer dampers along spans (45m spacing between spacers)","No",null,null,"rate only"]
[]
[null,"Stringing and regulation of the phase conductor (3x Dinosuar)"]
[]
[9,"Stringing and regulation of the phase conductor between towers - route length","No",null,null,"rate only"]
[]
[10,"Joining of new conductor to existing conductor at existing towers ( phases ) - cater for installation of new strain assemblies on one side of existing towers. Cater for modification of existing jumpers. Include for dressing of half of existing towers with new hardware.","No. phase",null,null,"rate only"]
[]
[]
[12,"Installation of spacer dampers along spans (45m spacing between spacers)","No",null,null,"rate only"]
[]
[null,"Testing requirements (to be done before stringing commences)."]
[]
[13,"Tension testing on the phase conductor with dead ends.","each",null,null,"rate only"]
[]
[14,"Tension testing on the earthwire with dead ends .","each",null,null,"rate only"]
[]
[15,"Testing of concrete cubes ","each",null,null,"rate only"]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Crossing","index":7,"n_rows":21,"n_cols":6,"rows_kept":21,"flags":["formulas_cached_only"]}
[]
["SECTION NO. 8"]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"Crossings:"]
[]
[1,"Allow all the necessary requirements for highway Crossings - supply and install safety net support structure (30m long x 16m width),including all the accessories and SANRAL cost.","No.",null,null,"rate only"]
[]
[2,"Allow all the necessary requirements for  Major Road Crossings (- supply and install safety net support structure (30m long x 16m width),including all the accessories.","No.",null,null,"rate only"]
[]
[3,"Allow all the necessary requirements for railway Crossings - supply and install safety net support structure (30m long x 16m width),including all the accessories.","No.",null,null,"rate only"]
[]
[4,"Allow all the necessary requirements for Live Line Crossings- 22kV.","No.",null,null,"rate only"]
[5,"Allow all the necessary requirements for Live Line Crossings- 132kV.","No.",null,null,"rate only"]
[6,"Allow all the necessary requirements for Live Line Crossings- 400kV."]
[7,"Allow all the necessary requirements for conveyor, HDPE pipeline, sewer pipe, dam crossing.","No.",null,null,"rate only"]
[8,"Allow all the necessary requirements for Live Line Crossings- 400kV.","No.",null,null,"rate only"]
[9,"Allow for dropping of 22kV Line for crossing purposes and re-instate the line to its original state.","No.",null,null,"rate only"]
[]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Tower labels & Bird Guards","index":8,"n_rows":30,"n_cols":6,"rows_kept":30,"flags":["formulas_cached_only"]}
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SECTION NO. 9"]
[]
[null,"TOWER LABELLING "]
[]
[null,"Supply Line Labels:"]
[]
[1,"Supply Line tower labels as per attached standard specification.","No",null,null,"rate only"]
[2,"Tower identification labels","No",null,null,"rate only"]
[3,"Line crossing labels","No",null,null,"rate only"]
[]
[null,"Installion of line labels:"]
[]
[4,"Dead line installation of line labels, tower identification labels and line crossing labels","No",null,null,"rate only"]
[5,"Live line installation of line labels- for existing portions of lines","No",null,null,"rate only"]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SECTION NO. 10."]
[]
[9.2,"Supply and install Bird Guardss:"]
[]
[1,"Supply and install Bird guards, complete including brackets and all required accessories (on strain towers or suspension tower)","M",null,null,"rate only"]
[2,"Aircraft warning devices (on earth wires) ","No",null,null,"rate only"]
[3,"Supply and install Bird diverters - large spirals 350mm dia (on earth wires)-stagered balck and white as per spec.","No",null,null,"rate only"]
[]
[null,"SUB TOTAL   -  CARRIED TO SUMMARY"]

{"sheet":"Summary","index":9,"n_rows":61,"n_cols":4,"rows_kept":61,"merged":[[1,0,1,1]],"flags":["formulas_cached_only"]}
[]
["FINAL SUMMARY - TRANSMISSION LINES PROJECT",null,null,"ESKOM ESTIMATE"]
["SCHEDULE","DESCRIPTIONS","AMOUNT","AMOUNT"]
[]
[]
[null,"SECTION 1 - PRELIMINARY AND GENERAL"]
[]
[1,"Preliminaries  (Fixed  Items)",null,{"$error":"#REF!"}]
[]
[1,"Preliminaries  ( Time Related Items)"]
[]
[null,"SECTION 2 . PROVISIONAL ITEM "]
[]
[2,"Provisional Day Works",null,{"$error":"#REF!"}]
[]
[null,"SECTION NO. 3  -  "]
[]
[3,"Inspections",null,{"$error":"#REF!"}]
[]
[]
[null,"SECTION NO. 4  - "]
[]
[4,"Stabilisation",null,{"$error":"#REF!"}]
[]
[]
[null,"SECTION 5. "]
[]
[5,"Steel Structural Works - Towers",null,{"$error":"#REF!"}]
[]
[6,"Stringing and regulating of Earthwires "]
[]
[]
[]
[null,"SECTION NO. 6 : "]
[]
[7,"Crossings",null,{"$error":"#REF!"}]
[]
[]
[null,"SECTION NO.  : 7"]
[]
[8,"Civil Works",null,{"$error":"#REF!"}]
[]
[9,"Site clearance:"]
[]
[10,"Supply and Install additional earthing"]
[]
[11,"Cameras, Video monitoring "]
[]
[]
[]
[null,"SECTION NO.  : 8"]
[]
[12,"Supply and Installation Line Labels:",null,{"$error":"#REF!"}]
[]
[13,"Supply and install Bird Guardss:",null,{"$error":"#REF!"}]
[]
[]
[]
[{"$nulls":3},{"$error":"#REF!"}]
[]
[null,"CONTRACT AMOUNT",null,{"$error":"#REF!"}]