eskom holdings SOC ltd

Contract No. _________
Kusile Power Station Supply and Delivery of Non-Critical Pumps for a Period of Five (5) Years on an As and When Required Basis

Part 2: Pricing Data

NEC3 Supply Contract
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C2.1 Pricing assumptions
1. How goods and services are priced and assessed for payment
Clause 11 in NEC3 Supply Contract, (SC3) core clauses states:

	Identified and defined terms
	11

11.2
	(11) The Prices are the amounts stated in the price column of the Price Schedule.  Where a quantity is stated for an item in the Price Schedule, the Price is calculated by multiplying the quantity by the rate.


	
	
	(12) The Price Schedule is the price schedule unless later changed in accordance with this contract.



	Assessing the amount due
	50.2
	The amount due is
· the Price for each lump sum item in the Price Schedule which the Supplier has completed, 
· where a quantity is stated for an item in the Price Schedule, an amount calculated by multiplying the quantity which the Supplier has completed by the rate,
· plus other amounts to be paid to the Supplier,

· less amounts to be paid by or retained from the Supplier.
Any tax which the law requires the Purchaser to pay to the Supplier is included in the amount due.




This confirms that the Supply Contract is a priced contract where the Prices are derived from a list of items of goods and services which can be priced as lump sums or as expected quantities of goods and services multiplied by a rate, or a mix of both.
2. Function of the Price Schedule
Clause 53.1 states: “Information in the Price Schedule is not Goods Information”.  This confirms that instructions to do work or how it is to be done are not included in the Price Schedule but in the Goods Information.  This is further confirmed by Clause 20.1 which states, “The Supplier Provides the Goods and Services in accordance with the Goods Information”. Hence the Supplier does not Provide the Goods and Services in accordance with the Price Schedule.   The Price Schedule is only a pricing document.  
3. Preparing the price schedule
Items in the price schedule may have been inserted by the Purchaser and the tendering supplier should insert any additional items which he considers necessary.  Whichever party provides the items in the price schedule the total of the Prices is assumed to be fully inclusive of everything necessary to Provide the Goods and Services as described at the time of entering into this contract.

It will be assumed that the tendering supplier has 
· Read Pages 8, 11, 12 and Appendix 5 of the SC3 Guidance Notes before preparing the price schedule;
· Included in his Prices and rates for correction of Defects (core clause 43.1) as there is no compensation event for this unless the Defect is due to a Supplier’s risk;
· Spread the cost of doing work he chooses not to list as separate items in the price schedule across other Prices and rates in order to fulfil the obligation to Provide the Goods and Services for the tendered total of the Prices; 
· Understood that there is no adjustment to lump sum prices in the price schedule if the amount, or quantity, of work within that lump sum item later turns out to be different to that which the Supplier estimated at time of tender. The only basis for a change to the Prices is as a result of a compensation event per clause 60.1;
· Understood that the Supplier does not have to allow in his Prices and rates for matters that may arise as a result of a compensation event.
3.1. Format of the price schedule
Entries in the first four columns in the price schedule in section C2.2 are made either by the Purchaser or the tendering supplier. 

If the Supplier is to be paid an amount for the item which is not adjusted if the quantity of work in the item changes, the tendering supplier enters the amount in the Price column only, the Unit, Quantity and Rate columns being left blank.

If the Supplier is to be paid an amount for the item which is the rate for the item multiplied by the quantity completed, the tendering Supplier enters the rate which is then multiplied by the Quantity to produce the Price, which is also entered.
If the Supplier is to be paid an amount for an item proportional to the length of time for which the goods and services are provided, a unit of time is stated in the Unit column and the length of time (as a quantity of the stated units of time) is stated in the Quantity column.

C2.2 the price schedule
	ITEM NO.
	MATERIAL NO.
	DESCRIPTION
	UOM
	QTY
	RATE
	AMOUNT

	 
	 
	
	 
	 
	 
	 

	 
	 
	ITEM 1
	 
	 
	 
	 

	1
	 
	PRELIMINARIES AND GENERAL
	 
	 
	 
	 

	 
	 
	
	 
	 
	 
	 

	1.1
	 
	Safety file 
	Once off
	1
	 
	 

	1.2
	 
	Medicals - Entry (Per Person)
	Per Person
	5
	 
	 

	1.3
	 
	Medicals - Exit (Per Person)
	Per Person
	1
	 
	 

	1.4
	 
	Police Clearance Certification (Per Person)
	Per Person
	5
	 
	 

	1.5
	 
	PPE
	Per Person
	5
	 
	 

	1.6
	 
	12 Tonne truck Diesel 
	Per Day
	120
	 
	 

	 
	 
	
	 
	 
	 
	 

	 
	 
	Total Item 1 (Preliminary & General) carried to Summary:
	 
	 
	 
	 

	 
	 
	
	 
	 
	 
	 

	 
	 
	ITEM 2
	 
	 
	 
	 

	2
	 
	SUPPLY AND DELIVER OF NON CRITICAL PUMPS
	 
	 
	 
	 

	 
	 
	
	 
	 
	 
	 

	 
	 
	
	 
	 
	 
	 

	ITEM NO.
	MATERIAL NO.
	DESCRIPTION
	OEM PART NO.
	QTY
	 
	 

	1
	571870
	PUMP: TYPE: PERISTALTIC; SIZE: 1/8 IN; CAPACITY: 1 L/HR; SPEED: 50 RPM; RATING: 50 KPA; DRIVER: MOTOR; SPECIFICATION: JSR 25; POTENTIAL: 220 V; CASING MATERIAL: STEEL; APPLICATION: CONDENSATE WATER; SUPPL P/N: 32. 00510
	SUPPL P/N: 32. 00510
	12
	 
	 

	2
	576757
	PUMP, CENTRIFUGAL: NPSH: 0.24 BAR; CAPACITY: 5-60 L/S; TOTAL HEAD: 130 KPA; SIZE: 160 MM; SPEED: 460 R/S; STAGE: 1; DRIVER: INDUCTION MOTOR - 3.8KW; 400V; 4 POLE; 1435RPM; W21 112M; TYPE: TRANSFORMER OIL CIRCULATION PUMP; SPECIFICATION: IEC34-1; MOUNT: FLANGE; SUPPL P/N: VMOA 100 218-C A C 3 F; REFERENCE NO: 107839-1
	SUPPL P/N: VMOA 100 218-C A C 3 F | REFERENCE NO: 107839-1
	3
	 
	 

	3
	620120
	CONTROL; SUPPLIED WITH OEM MANUAL; DATA SHEET; GENERAL ARRANGEMENT DRAWINGS AND SPARE PARTS LIST HORIZONTAL; REFERENCE NO: 10/035574; DIRECTLY COUPLED TO A 90 W; 1 PHASE; IP65/F; ELECTRIC MOTOR AND A MECHANICAL DIAPHRAGM PUMP, DIAPHRAGM: TYPE: FERRIC CHLORIDE DOSING; SIZE: 20 X 20 MM; CAPACITY: 115 L/HR; SPEED: 120 RPM; RATING: 3 BAR; MOUNT:
	REFERENCE NO: 10/035574
	2
	 
	 

	4
	620430
	PUMP, CENTRIFUGAL: NPSH: 1.62 M; CAPACITY: 32 L/S; TOTAL HEAD: 12.2 M; SIZE: 152 X 152 MM; SPEED: 1020 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: RAW SEWAGE; MOUNT: HORIZONTAL; SHAFT DIAMETER: 38.1 MM; REFERENCE NO: 0212091425-259N; TO BE SUPPLIED WITH OEM MANUAL; DATA SHEET; GENERAL ARRANGEMENT DRAWINGS AND SPARE PARTS LIST
	REFERENCE NO: 0212091425-259N
	2
	 
	 

	5
	620431
	PUMP, CENTRIFUGAL: NPSH: 2.4 M; CAPACITY: 130 M3/HR; TOTAL HEAD: 12 M; SIZE: 125 X 100 MM; SPEED: 1450 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: FILTER SUPPLY; MOUNT: HORIZONTAL; SHAFT DIAMETER: 38.1 MM; REFERENCE NO: 9372521-547; TO BE SUPPLIED WITH OEM MANUAL; DATA SHEET; GENERAL ARRANGEMENT DRAWINGS AND SPARE PARTS LIST
	REFERENCE NO: 9372521-547
	2
	 
	 

	6
	620970
	PUMP, CENTRIFUGAL: NPSH: 3.4 M; CAPACITY: 135 M3/HR; TOTAL HEAD: 90 M; SIZE: 125 X 80 MM; SPEED: 2970 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: ISO 5199/EN 25199; MOUNT: HORIZONTAL; DRAWING NO: 0.90/37310 REV 0; MODEL NO: LSN-125-80-S1VV1-7502; APPLICATION: FLY ASH CONDITIONING WATER SUPPLY; SUPPLY DATA SHEET ON DELIVERY; GENERAL ARRANGEMENT DRAWING; OPERATING AND MAINTENANCE MANUAL; DESIGN AND DRAWINGS REFER TO ESKOM DOCUMENT NUMBER: 203-9618
	MODEL NO: LSN-125-80-S1VV1-7502 | DRAWING NO: 0.90/37310 REV 0
	5
	 
	 

	7
	623393
	PUMP, CENTRIFUGAL: NPSH: 3.8 M; CAPACITY: 1100 M3/HR; TOTAL HEAD: 64.4 M; SIZE: 300 X 250 MM; SPEED: 1473 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: CPK250-500; MOUNT: HORIZONTAL; REFERENCE NO: 506367/9; ON EVERY DELIVERY THE ITEM SHOULD HAVE THE FOLLOWING SUPPORTING DOCUMENTS: DRAWINGS; DATASHEET AND MANUAL
	REFERENCE NO: 506367/9
	18
	 
	 

	8
	623394
	PUMP, CENTRIFUGAL: NPSH: 1.5 M; CAPACITY: 40 M3/HR; TOTAL HEAD: 30 M; SIZE: 65 X 40 MM; SPEED: 2890 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MEGA-CHEM 40-160; MOUNT: HORIZONTAL; REFERENCE NO: 396.094/5; ON EVERY DELIVERY THE ITEM SHOULD HAVE THE FOLLOWING SUPPORTING DOCUMENTS: DRAWINGS; DATASHEET AND MANUAL
	REFERENCE NO: 396.094/5
	2
	 
	 

	9
	623397
	PUMP, CENTRIFUGAL: NPSH: 1.2 M; CAPACITY: 35 M3/HR; TOTAL HEAD: 41.3 M; SIZE: 65 X 40 MM; SPEED: 2930 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MEGA-CHEM 40-160; MOUNT: HORIZONTAL; REFERENCE NO: 396.060/1; ON EVERY DELIVERY THE ITEM SHOULD HAVE THE FOLLOWING SUPPORTING DOCUMENTS: DRAWINGS; DATASHEET AND MANUAL
	REFERENCE NO: 396.060/1
	2
	 
	 

	10
	623400
	PUMP, CENTRIFUGAL: NPSH: 2 M; CAPACITY: 300 M3/HR; TOTAL HEAD: 20.4 M; SIZE: 200 X 150 MM; SPEED: 1465 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 150-315; MOUNT: HORIZONTAL; REFERENCE NO: 396.111/2
	REFERENCE NO: 396.111/2
	2
	 
	 

	11
	623401
	PUMP, CENTRIFUGAL: NPSH: 4.8 M; CAPACITY: 120 M3/HR; TOTAL HEAD: 40.8 M; SIZE: 100 X 125 MM; SPEED: 2940 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 80-160; MOUNT: HORIZONTAL; REFERENCE NO: 396.109/10
	REFERENCE NO: 396.109/10
	2
	 
	 

	12
	623402
	FOLLOWING SUPPORTING DOCUMENTS: DRAWINGS; DATASHEET AND MANUAL ELECTRIC MOTOR; SPECIFICATION: CPK200-500; MOUNT: HORIZONTAL; REFERENCE NO: 506385/7; ON EVERY DELIVERY THE ITEM SHOULD HAVE THE PUMP, CENTRIFUGAL: NPSH: 3.8 M; CAPACITY: 560.5 M3/HR; TOTAL HEAD: 83.7 M; SIZE: 200 X 250 MM; SPEED: 1485 RPM; STAGE: 1; DRIVER:
	REFERENCE NO: 506385/7
	3
	 
	 

	13
	623403
	PUMP, CENTRIFUGAL: NPSH: 2.17 M; CAPACITY: 230.06 M3/HR; TOTAL HEAD: 26.3 M; SIZE: 200 X 150 MM; SPEED: 1482 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MCP200-150 315VD; MOUNT: HORIZONTAL; REFERENCE NO: 9972457229/200
	REFERENCE NO: 9972457229/200
	2
	 
	 

	14
	623407
	PUMP, CENTRIFUGAL: NPSH: 4.6 M; CAPACITY: 450 M3/HR; TOTAL HEAD: 32 M; SIZE: 200 X 150 MM; SPEED: 1580 RPM; STAGE: 1; DRIVER: DIESEL ENGINE; SPECIFICATION: ETA 150-315(J); MOUNT: HORIZONTAL; SUPPL P/N: 203-30156; REFERENCE NO: 9972286854/100
	SUPPL P/N: 203-30156 | REFERENCE NO: 9972286854/100
	6
	 
	 

	15
	623409
	PUMP, CENTRIFUGAL: NPSH: 7 M; CAPACITY: 160 M3/HR; TOTAL HEAD: 10.2 M; SIZE: 125 X 100 MM; SPEED: 1440 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 100-200; MOUNT: HORIZONTAL; REFERENCE NO: 369.092/3
	REFERENCE NO: 369.092/3
	2
	 
	 

	16
	623426
	PUMP, CENTRIFUGAL: NPSH: 5.3 M; CAPACITY: 1120 M3/HR; TOTAL HEAD: 18.4 M; SIZE: 350 MM; SPEED: 985 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MEGA-NORM 350-400; MOUNT: HORIZONTAL; REFERENCE NO: C03764/5; ON EVERY DELIVERY THE ITEM SHOULD HAVE THE FOLLOWING SUPPORTING DOCUMENTS: DRAWINGS; DATASHEET AND MANUAL
	REFERENCE NO: C03764/5
	2
	 
	 

	17
	624128
	NO: 254373 RPM; RATING: PN16; DRIVER: ELECTRIC MOTOR; APPLICATION: FUEL OIL LP SYSTEM; MOUNT: FLANGE; SUPPL P/N: KV-1500.EXB-003936; REFERENCE PUMP, ROTARY: TYPE: STOP SCREW; PORT SIZE: 200 X 150 MM; CAPACITY: 14171 L/MIN AT 60 DEG C; 1520 L/MIN AT 30 DEG C; SPEED: 1450
	PN16 | SUPPL P/N: KV-1500.EXB-003936
	3
	 
	 

	18
	624129
	PUMP, ROTARY: TYPE: STOP SCREW; PORT SIZE: 80 MM; CAPACITY: 8.9 M3/HR AT 120 DEG C; 9.7 M3/HR AT 30 D EG C; SPEED: 1426 RPM; RATING: PN16; DRIVER: ELECTRIC MOTOR; APPLICATION: DRAIN FUEL OIL TANK; MOUNT: FLANGE; SUPPL P/N: KV-160.EXA-004051; REFERENCE NO: 254795
	PN16 | SUPPL P/N: KV-160.EXA-004051 | REFERENCE NO: 254795
	3
	 
	 

	19
	633904
	PUMP, CENTRIFUGAL: NPSH: 6 M; CAPACITY: 17 M3/HR; TOTAL HEAD: 98.5 M; SIZE: 100 MM; SPEED: 2919 RPM; STAGE: 7; TYPE: MULTI STG; MOUNT: VERTICAL; SUPPL P/N: CR-15-7-A-F-A-E-HQQE; OPERATING PRESSURE: 10 BAR; SUCTION AND DISCHARGE PORTS ON SAME LEVEL AND IN ONE LINE ENABLING INSTALLATION IN A HORIZONTAL ONE-PIPE SYSTEM
	SUPPL P/N: CR-15-7-A-F-A-E-HQQE
	2
	 
	 

	20
	633905
	PUMP, CENTRIFUGAL: NPSH: 100 FT; CAPACITY: 200 M3/HR; TOTAL HEAD: 98.5 M; SIZE: 230 X 110.5 MM; SPEED: 2950 RPM; STAGE: 5; TYPE: MULTI STG SPLIT CASE; MOUNT: HORIZONTAL; SUPPL P/N: MPA100.2/2A-SA311A-9002; OPERATING PRESSURE: 40 BAR; ENSURE THE TEST REPORTS AND DATASHEETS ARE ATTACHED WITH THE PUMP ON DELIVERY
	SUPPL P/N: MPA100.2/2A-SA311A-9002
	3
	 
	 

	21
	634527
	HYDRA-CELL D/G-10 SERIES PUMP, DIAPHRAGM: TYPE: AIR; SIZE: 1 X 3/4 IN; CAPACITY: 28 L/MIN; SPEED: 1450 RPM; RATING: 25 BARS; MOUNT: BOLTED BASE; BELT WASH;
	 
	3
	 
	 

	22
	634750
	PUMP, CENTRIFUGAL: NPSH: 9.2-3.2 M; CAPACITY: 300.7/100 M3/HR; TOTAL HEAD: 30 M; SIZE: 200 X 150 MM; SPEED: 1475 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR 400 V 37 KW IP65; 1500 RPM; TYPE: END SUCTION; SPECIFICATION: ETA-CX-150-315; MOUNT: HORIZONTAL; SHAFT DIAMETER: 42 MM; SUPPL P/N: ST.250408; ITEM DATA SHEET IS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: ST.250408
	5
	 
	 

	23
	635210
	PUMP: TYPE: HP POTABLE PUMP IN LP SERVICES; SIZE: DIA 368 X LG 570 MM; CAPACITY: 120 M3/HR; SPEED: 2950 RPM; RATING: 16 BAR; SUPPL P/N: 080-065-250 080-065-250; DIFFERENTIAL HEAD: 90 M; MATERIAL: CAST IRON; CASING; BRONZE IMPELLER; CR STL SHAFT; ETA 080-065-250 AT 2950 RPM; FLUID TEMPERATURE AT 20 DEG C; BARESHAFT PUMP ONLY; CLOSED IMPELLER TYPE; SEALING ARRANGEMENT; MECHANICAL SEAL; EXTERNAL COATING; RAL 6010 GREEN; FULL SIZE IMPELLER; BALANCING CERTIFICATE ACCORDING TO ISO 1940; OIL FILLED BEARING HOUSING WITH SIGHT GLASS; IDENTIFICATION LABEL; PUMP MAKE; MODEL; SERIAL NUMBER; IMPELLER SIZE; HEAD FLOW; ENSURE NAME PLATE IS FILLED IN; PUMP DRAWING TO BE PROVIDED WITH QUOTE DURING TENDER STAGE
	SUPPL P/N: 080-065-250 080-065-250
	3
	 
	 

	24
	635452
	PUMP: TYPE: HYDROCELL; SIZE: 1 X 3/4 IN; CAPACITY: 30.6 L/MIN; SPEED: 1450 RPM; RATING: 24 BAR; DRIVER: ELECTRIC MOTOR; SPECIFICATION: D10-X; POTENTIAL: 400 VAC; CASING MATERIAL: PLASTIC; APPLICATION: WATER; MODEL NO: D10XKBTHFEHA; OIL TYPE: 10W30; OIL CAPACITY: 1.05 L; GLAND SEAL FLUSH; BRASS HEAD; BUNA- DIAPHRAGM; MAXIMUM INLET PRESSURE: 17 BAR; BI-DIRECTIONAL TAPERED ROLLER BEARINGS 7/8 IN; SHAFT DIA: 500 MACRONS MAXIMUM SOLID SIZE; VALVE SEAT: SS 17-4
	MODEL NO: D10XKBTHFEHA
	5
	 
	 

	25
	636710
	IMPELLER DIA: MAX 330 MM; DESIGNED 313.6 MM; IMPELLER SHAFT: 270 MM; POWER: 55.9 KW ELECTRIC MOTOR; TYPE: END SUCTION; MOUNT: VERTICAL; MODEL NO: LS200-350 S1VL1; WORKING PRESSURE: 3.2 BAR; IMPELLER TYPE: RADIAL; PUMP, CENTRIFUGAL: NPSH: 10 M; CAPACITY: 248.4 M3/HR; TOTAL HEAD: 31 M; SIZE: 200 X 250 MM; SPEED: 1475 RPM; STAGE: 1; DRIVER:
	MODEL NO: LS200-350 S1VL1
	2
	 
	 

	26
	638984
	PUMP, ASSEMBLY: TYPE: HOPPER FOG; APPLICATION: LIMESTONE DUST SUPPRESSION SYSTEM; IMPELLER BEARINGS; SHAFT; SEALS AND ALL OTHER PARTS; 4KW; 70BAR; 26LPM AT 1440RPM
	 
	5
	 
	 

	27
	639114
	PUMP, DIAPHRAGM: TYPE: CONTROLLABLE; SIZE: 5 MM; CAPACITY: 7 L/HR; SPEED: 150 RPM; RATING: 10 BARS; MANUF P/N: C409.2-7,0(E); REFERENCE NO: 00QLF30 AP001
	MANUF P/N: C409.2-7,0(E) | REFERENCE NO: 00QLF30 AP001
	2
	 
	 

	28
	639235
	PUMP: TYPE: DISPLACEMENT; SIZE: 19 X 15 MM; CAPACITY: 12 L/MIN; SPEED: 1800 RPM; RATING: 1518.75 KPA; APPLICATION: GEARBOX OIL INTERNAL GEAR PUMP; SUPPL P/N: 109-F461001; SHW INTERGRATED PUMP WITH EXTERNAL SUCTION PRESSURE LINES
	SUPPL P/N: 109-F461001
	2
	 
	 

	29
	642430
	PUMP, ROTARY: TYPE: SCREW INSERT; PORT SIZE: 200 X 150 MM; CAPACITY: 25.30 KGS AT 31 BARG; SPEED: 1489 RPM; RATING: PN40; DRIVER: MOTOR; APPLICATION: FUEL OIL HP PUMP; MOUNT: VERTICAL; SUPPL P/N: CCGV-2250.ECEZP.50009; HOUSING P235GH; OPERATING TEMP: 150 DEG C
	PN40 | SUPPL P/N: CCGV-2250.ECEZP.50009
	3
	 
	 

	30
	642496
	PUMP, ASSEMBLY: TYPE: DOUBLE GEAR; APPLICATION: MILLS HYDRAULIC OIL PUMP SYSTEM; SUPPL P/N: 3510532; REFERENCE NO: PGE104-2200/1100-RBR1/1N-3900; SQUARE FLANGE
	SUPPL P/N: 3510532 | REFERENCE NO: PGE104-2200/1100-RBR1/1N-3900
	5
	 
	 

	31
	644961
	SPECIFICATION: MVT 274-300; REFERENCE NO: 1302-003 PUMP: TYPE: LIQUID RING VACUUM; SIZE: 4 X 4 IN; CAPACITY: 561 M3/HR; SPEED: 970 RPM; RATING: 33 MBAR ABS; DRIVER: ELECTRIC MOTOR;
	SPECIFICATION: MVT 274-300
	3
	 
	 

	32
	645239
	PUMP, ROTARY: TYPE: HYDRAULIC, SCREW; PORT SIZE: DN80; CAPACITY: 92 DM3/S; SPEED: 2900 RPM; RATING: 40 BARS; SPECIFICATION: L3MF60/120; OEM P/N: HTGD485981P0012
	OEM P/N: HTGD485981P0012
	2
	 
	 

	33
	648334
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 5 L/HR; SPEED: 29 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.09 KW; SPECIFICATION: DMH 251; SUPPL P/N: 957-386-56; REFERENCE NO: 1000.000.0-1/P4; PUMP BODY MATERIAL: AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-386-56 | REFERENCE NO: 1000.000.0-1/P4
	2
	 
	 

	34
	648351
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 24 L/HR; SPEED: 120 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.09 KW; SPECIFICATION: DMH 251; SUPPL P/N: 957-386-61; REFERENCE NO: 1000.000.0-1/P14; PUMP BODY MATERIAL: AL; HEAD: SS; DIAPHRAGM: PTFE; VALVE BODY: 316L; VALVE BALL: 316L; VALVE SEAT: 316L; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-386-61 | REFERENCE NO: 1000.000.0-1/P14
	2
	 
	 

	35
	648352
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 46 L/HR; SPEED: 120 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.09 KW; SPECIFICATION: DMH 252; SUPPL P/N: 957-386-59; REFERENCE NO: 1000.000.0-1/P8; PUMP BODY MATERIAL: AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-386-59 | REFERENCE NO: 1000.000.0-1/P8
	2
	 
	 

	36
	648353
	EVERY DELIVERY AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON DRIVER: ELECTRIC MOTOR 0.09 KW; SPECIFICATION: DMH 252; SUPPL P/N: 957-386-62; REFERENCE NO: 1000.000.0-1/P12; PUMP BODY MATERIAL: PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 37 L/HR; SPEED: 96 N/M; RATING: 10 BAR;
	SUPPL P/N: 957-386-62 | REFERENCE NO: 1000.000.0-1/P12
	2
	 
	 

	37
	648354
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 38 L/HR; SPEED: 96 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.09 KW; SPECIFICATION: DMH 252; SUPPL P/N: 957-386-58; REFERENCE NO: 1000.000.0-1/P7; PUMP BODY MATERIAL: AL; HEAD; PVDF; DIAPHRAGM: PTFE; VALVE BODY: PVDF; VALVE BALL: PTFE; VALVE SEAT: PTFE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-386-58 | REFERENCE NO: 1000.000.0-1/P7
	2
	 
	 

	38
	648355
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 11/4 X 11/4 IN; STYLE: ONE; CAPACITY: 67 L/HR; SPEED: 96 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.18 KW; SPECIFICATION: DMH 253; SUPPL P/N: 957-386-63; REFERENCE NO: 1000.000.2-3/P15/16; PUMP BODY MATERIAL: AL; HEAD; PVDF; DIAPHRAGM: PTFE; VALVE BODY: PVDF; VALVE BALL: PTFE; VALVE SEAT: PTFE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-386-63 | REFERENCE NO: 1000.000.2-3/P15/16
	4
	 
	 

	39
	648356
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 143 L/HR; SPEED: 75 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.55 KW; SPECIFICATION: DMH 254; SUPPL P/N: 957-335-12; REFERENCE NO: 1000.000.0-1/P28; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-335-12 | REFERENCE NO: 1000.000.0-1/P28
	2
	 
	 

	40
	648357
	DELIVERY PVDF; DIAPHRAGM: PTFE; VALVE BODY: PVDF; VALVE BALL: PTFE; VALVE SEAT: PTFE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-370-96; REFERENCE NO: 1000.000.0-1/P17; PUMP BODY MATERIAL: AL; HEAD; PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 1500 L/HR; SPEED: 146 N/M; RATING: 4 BAR; DRIVER:
	SUPPL P/N: 957-370-96 | REFERENCE NO: 1000.000.0-1/P17
	2
	 
	 

	41
	648358
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 1150 L/HR; SPEED: 146 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-364-14; REFERENCE NO: 1000.000.0-1/P26; PUMP BODY MATERIAL: AL; HEAD; PVDF; DIAPHRAGM: PTFE; VALVE BODY: PVDF; VALVE BALL: PTFE; VALVE SEAT: PTFE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-364-14 | REFERENCE NO: 1000.000.0-1/P26
	2
	 
	 

	42
	648359
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 1150/2 L/HR; SPEED: 146 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 1.5 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-370-97; REFERENCE NO: 1000.000.0-1/P18+25; PUMP BODY MATERIAL: AL; HEAD: SS; DIAPHRAGM: PTFE; VALVE BODY: 316 L; VALVE BALL: 316 L; VALVE SEAT: 316 L; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-370-97 | REFERENCE NO: 1000.000.0-1/P18+25
	4
	 
	 

	43
	648364
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 440 L/HR; SPEED: 56 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-382-17; REFERENCE NO: 1000.000.0-1/P9; PUMP BODY MATERIAL: AL; HEAD; PVDF; DIAPHRAGM: PTFE; VALVE BODY: PVDF; VALVE BALL: PTFE; VALVE SEAT: PTFE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-382-17 | REFERENCE NO: 1000.000.0-1/P9
	2
	 
	 

	44
	648365
	DELIVERY PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PP; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-386-55; REFERENCE NO: 1000.000.0-1/P3; PUMP BODY MATERIAL: AL; HEAD: PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 750 L/HR; SPEED: 73 N/M; RATING: 4 BAR; DRIVER:
	SUPPL P/N: 957-386-55 | REFERENCE NO: 1000.000.0-1/P3
	2
	 
	 

	45
	648366
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32; STYLE: ONE; CAPACITY: 440 L/HR; SPEED: 56 N/M; RATING: 4 BAR; DRIVER: ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 967-249-72/957-386-57; REFERENCE NO: 1000.000.0-1/P2/5; PUMP BODY MATERIAL: AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 967-249-72/957-386-57 | REFERENCE NO: 1000.000.0-1/P2/5
	4
	 
	 

	46
	655099
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 1150 L/HR; SPEED: 146 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-126-58; REFERENCE NO: 1000-0000-1/1; PUMP BODY MATERIAL: AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-126-58 | REFERENCE NO: 1000-0000-1/1
	2
	 
	 

	47
	655100
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 5/8 X 5/8 IN; STYLE: ONE; CAPACITY: 1151 L/HR; SPEED: 146 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 1.1 KW; SPECIFICATION: DMH 257; SUPPL P/N: 957-386-60; REFERENCE NO: 1000-0000-1/10; PUMP BODY MATERIAL: AL; HEAD: SS; DIAPHRAGM: PTFE; VALVE BODY: 316 L; VALVE BALL: 316 L; VALVE SEAT: 316 L; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-386-60 | REFERENCE NO: 1000-0000-1/10
	2
	 
	 

	48
	655101
	REQUIRED ON EVERY DELIVERY MATERIAL: AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS DRIVER: ELECTRIC MOTOR 0.18 KW; SPECIFICATION: DMH 253; SUPPL P/N: 957-316-63; REFERENCE NO: 1000-0000-2-3/13-14; PUMP BODY PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: 11/4 X 11/4 IN; STYLE: ONE; CAPACITY: 66.5 L/HR; SPEED: 96 N/M; RATING: 10 BAR;
	SUPPL P/N: 957-316-63 | REFERENCE NO: 1000-0000-2-3/13-14
	4
	 
	 

	49
	655102
	PUMP, RECIPROCATING: TYPE: DIAPHRAGM DOSING; SIZE: DN32 MM; STYLE: ONE; CAPACITY: 143 L/HR; SPEED: 75 N/M; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR 0.55 KW; SPECIFICATION: DMH 254; SUPPL P/N: 957-250-65/957-263-95; REFERENCE NO: 1000-0000-1/6-27; PUMP BODY MATERIAL: AL; HEAD: PVC; DIAPHRAGM: PTFE; VALVE BODY: PVC; VALVE BALL: GLASS; VALVE SEAT: PE; DATA SHEET; DRAWINGS AND MANUALS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 957-250-65/957-263-95 | REFERENCE NO: 1000-0000-1/6-27
	4
	 
	 

	50
	655305
	SET: TYPE: SCREW PUMP BEARING BALL SET; APPLICATION: ANTIFRICTION FUEL OIL AND PROPANE PLANT; SUPPL P/N: SP-KUS-F2-16011
	SUPPL P/N: SP-KUS-F2-16011
	3
	 
	 

	51
	659390
	PUMP, CENTRIFUGAL: NPSH: 2.6 M; CAPACITY: 30 M3/HR; TOTAL HEAD: 9.9 M; SIZE: 3 X 2 IN; SPEED: 1450 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: HORIZONTAL; SPECIFICATION: NEPO-80-50-200; DRAWING NO: 68249 REV 0; ON EVERY DELIVERY PLEASE PROVIDE DRAWINGS; DATA SHEET AND MANUAL; ONLY PUMP REQUIRED
	DRAWING NO: 68249 REV 0
	2
	 
	 

	52
	659397
	SHEET AND MANUAL; ONLY PUMP REQUIRED MOTOR; TYPE: HORIZONTAL; SPECIFICATION: NEPO-80-50-200; DRAWING NO: 68250 REV 0; ON EVERY DELIVERY PLEASE PROVIDE DRAWINGS; DATA PUMP, CENTRIFUGAL: NPSH: 2.6 M; CAPACITY: 30 M3/HR; TOTAL HEAD: 7.3 M; SIZE: 3 X 2 IN; SPEED: 1450 RPM; STAGE: 1; DRIVER: ELECTRIC
	DRAWING NO: 68250 REV 0
	2
	 
	 

	53
	659398
	PUMP, CENTRIFUGAL: NPSH: 2.5 M; CAPACITY: 21 M3/HR; TOTAL HEAD: 8.8 M; SIZE: 3 X 2 IN; SPEED: 1450 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: HORIZONTAL; SPECIFICATION: NEPO-80-50-200; DRAWING NO: 68248 REV 0; ON EVERY DELIVERY PLEASE PROVIDE DRAWINGS; DATA SHEET AND MANUAL; ONLY PUMP REQUIRED
	DRAWING NO: 68248 REV 0
	2
	 
	 

	54
	659839
	PUMP, RECIPROCATING: TYPE: DOSING; SIZE: 1 IN; STYLE: ONE; CAPACITY: 310 L/HR; SPEED: 97 RPM; RATING: 20 BARS; SPECIFICATION: RF410.2-310KM; SUPPL P/N: WP353636
	SUPPL P/N: WP353636
	12
	 
	 

	55
	659840
	PUMP, CENTRIFUGAL: NPSH: 0; CAPACITY: 45 M3/HR; TOTAL HEAD: 9 M; SIZE: 80 X 65 MM; SPEED: 1468 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: HORIZONTAL; SPECIFICATION: NKG80-65-160/177; REFERENCE NO: B99071359-P116130002; DRAWINGS; DATASHEET AND MANUAL REQUIRED ON EVERY DELIVERY; PUMP ONLY REQUIRED
	REFERENCE NO: B99071359-P116130002
	2
	 
	 

	56
	659841
	PUMP, CENTRIFUGAL: NPSH: 0.24 M; CAPACITY: 40 M3/HR; TOTAL HEAD: 1 M; SIZE: 2 X 2 IN; SPEED: 2900 RPM; STAGE: 1; TYPE: HORIZONTAL; SPECIFICATION: DB22; MODEL NO: DB22P-E-FF-5-25; REFERENCE NO: 131741-I14; DRAWINGS; DATASHEET AND MANUAL REQUIRED ON EVERY DELIVERY; PUMP ONLY REQUIRED
	MODEL NO: DB22P-E-FF-5-25 | REFERENCE NO: 131741-I14
	2
	 
	 

	57
	662122
	PUMP, CENTRIFUGAL: NPSH: 5.79 M; CAPACITY: 165.2 CM/HR; TOTAL HEAD: 58.3 M; SIZE: 125 X 100 MM; SPEED: 2960 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 125-100-250; MOUNT: HORIZONTAL; SHAFT DIAMETER: 32 MM
	SPECIFICATION: 125-100-250
	2
	 
	 

	58
	662175
	EVERY DELIVERY SENSING; DIRECTION OF ROTATION: CLOCKWISE FROM SHAFT END; MOUNTING FLANGE: SAEJ744-4HOLE; DATASHEET C/W PUMP CURVE REQUIRED ON MAX PRESSURE: 400BAR; CHARGE: W/C CHARGE PUMP; OPERATION: OPEN CIRCUIT; DISPLACEMENT: 260M3; CONTROL: PRESSURE CONTROL WITH LOAD P/N: A11VLO260DRS/11R-NSD12N00-S; REFERENCE NO: 27338386; AXIAL PISTOL UNIT: SWASHPLATE DESIGN; VARIABLE; NOMINAL PRESSURE: 350BAR; PUMP, ASSEMBLY: TYPE: HYDRAULIC AXIAL PISTOL VARIABLE PUMP A11VLO; APPLICATION: DRUM RECLAIMER RAKE HYDRAULIC POWER PACK; SUPPL
	P/N: A11VLO260DRS/11R-NSD12N00-S | REFERENCE NO: 27338386
	4
	 
	 

	59
	662399
	PUMP: TYPE: PRESSURE COMPENSATED; SIZE: 100 X 32 MM; CAPACITY: 23 M3/MIN; SPEED: 1420 RPM; RATING: 10 BAR; DRIVER: ELECTRIC MOTOR; POTENTIAL: 380 VACS; CASING MATERIAL: CI; APPLICATION: TERRACE CONVEYOR HYDRAULIC DRIVE AND CYLINDER EXTENSION SYSTEM; SUPPL P/N: 2570-00-03-05
	SUPPL P/N: 2570-00-03-05
	4
	 
	 

	60
	662402
	PUMP: TYPE: ELECTRO PROPORTIONAL CLOSED LOOP; SIZE: 100 MM; CAPACITY: 230 M3/MIN; SPEED: 1420 RPM; RATING: 20 BARS; DRIVER: ELECTRIC MOTOR; SPECIFICATION: TH-CD-2570-00-03; POTENTIAL: 380 VACS; CASING MATERIAL: CI; APPLICATION: TERRACE CONVEYOR HYDRAULIC DRIVE AND CYLINDER EXTENSION SYSTEM; SUPPL P/N: 2570-00-03-08
	SUPPL P/N: 2570-00-03-08
	5
	 
	 

	61
	662556
	BRACKET: TYPE: PUMP MOUNTING; MATERIAL: STL; DIMENSIONS: LG 100 MM; SPECIFICATION: TH-CD-2572-00-02; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SUPPL P/N: 2572-00-02-10
	SUPPL P/N: 2572-00-02-10
	4
	 
	 

	62
	662557
	PUMP: TYPE: ELECTRO PROPORTIONAL CLOSED LOOP; SIZE: 120 X 90 MM; CAPACITY: 230 M3/MIN; SPEED: 1420 RPM; RATING: 20 BARS; DRIVER: ELECTRIC MOTOR; SPECIFICATION: TH-CD-2572-00-02; POTENTIAL: 400 VACS; CASING MATERIAL: CAST STEEL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SUPPL P/N: 2572-00-02-08
	SUPPL P/N: 2572-00-02-08
	5
	 
	 

	63
	662558
	SUPPL P/N: 2572-00-02-05 SPECIFICATION: TH-CD-2572-00-02; POTENTIAL: 380 VACS; CASING MATERIAL: CAST STEEL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; PUMP: TYPE: FIXED DISPLACEMENT; SIZE: 80 MM; CAPACITY: 0-266 L/MIN; SPEED: 1222 RPM; RATING: 20 BARS; DRIVER: ELECTRIC MOTOR;
	SUPPL P/N: 2572-00-02-05 SPECIFICATION: TH-CD-2572-00-02
	5
	 
	 

	64
	662570
	PUMP: TYPE: FIXED DISPLACEMENT; SIZE: 100 MM; CAPACITY: 176 L/MIN; SPEED: 1480 RPM; RATING: 36 MPA; DRIVER: ELECTRIC MOTOR; SPECIFICATION: TH-CD-2572-00-02; POTENTIAL: 380 VAC; CASING MATERIAL: CAST STEEL; APPLICATION: LIMESTONE HYDRAULIC FEEDER DRIVE; SUPPL P/N: 2572-00-02-31
	SUPPL P/N: 2572-00-02-31
	5
	 
	 

	65
	662656
	PUMP: TYPE: ANION; SIZE: 80 X 110 MM; CAPACITY: 176 L/MIN; SPEED: 1440 RPM; RATING: 0-6 MPA; DRIVER: BULL GEAR; SPECIFICATION: TH-CD-2599-00-00; POTENTIAL: 400 VAC; CASING MATERIAL: CAST STEEL; APPLICATION: ASH HANDLING LUBRICATION SYSTEM; SUPPL P/N: 2599-00-00-10
	SUPPL P/N: 2599-00-00-10
	5
	 
	 

	66
	662714
	PUMP: TYPE: LOAD SENSING; SIZE: 1 IN; CAPACITY: 0-365 M3/HR; SPEED: 1189 RPM; RATING: PN10; SPECIFICATION: TH-CD-2592-00-03; CASING MATERIAL: CI; APPLICATION: LIMESTONE; SUPPL P/N: 2592-00-03-16
	PN10 | SUPPL P/N: 2592-00-03-16
	5
	 
	 

	67
	665479
	DEVICE: TYPE: BOOSTER PUMP-A; APPLICATION: STACKER HYDRAULIC SYSTEM 0 1EAD41 AP003; SUPPL P/N: 0973 0 07404-1-29; SPECIFICATION: 0973 0 07404-1
	SUPPL P/N: 0973 0 07404-1-29
	5
	 
	 

	68
	665481
	DEVICE: TYPE: BOOSTER PUMP-B; APPLICATION: STACKER HYDRAULIC SYSTEM 0 1EAD41 AP004; SUPPL P/N: 0973 0 07404-1-30; SPECIFICATION: 0973 0 07404-1
	SUPPL P/N: 0973 0 07404-1-30
	5
	 
	 

	69
	675381
	PUMP: TYPE: VACUUM; SIZE: 20 X 25 MM; CAPACITY: 18.9 M3/HR; SPEED: 1405 RPM; RATING: 0.005 MBAR; SPECIFICATION: WK1-100622; APPLICATION: SEAL OIL SYSTEM; OEM P/N: WK4-101771P0001; SUPPL P/N: D16B - EX; DRAWING NO: MKQ11AN001 REV 0; LEYBOLD TRIVAC
	OEM P/N: WK4-101771P0001 | SUPPL P/N: D16B - EX | DRAWING NO: MKQ11AN001 REV 0
	7
	 
	 

	70
	675871
	PUMP, CENTRIFUGAL: CAPACITY: 10 M3/HR; TOTAL HEAD: 8 M; SIZE: 40/40; SPEED: 1420 RPM; STAGE: 1; OEM P/N: GME9789236P0002; DRAWING NO: GME9789236P0002 REV 0; WK4-101680R0040-13 REV 0; CO2 EXP DEVICE, NIT 32/160
	OEM P/N: GME9789236P0002 | DRAWING NO: GME9789236P0002 REV 0
	5
	 
	 

	71
	676398
	PUMP, CENTRIFUGAL: NPSH: 5.22 M; CAPACITY: 0.5 M3/HR; TOTAL HEAD: 15.75 M; SIZE: 1 IN; SPEED: 2840 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: HIGH PRESSURE; SPECIFICATION: V F002/02 B2D13ES00325AW; MOUNT: VERTICAL; SUPPL P/N: 796008; PUMP AND MOTOR MUST BE SUPPLIED AS AN ASSEMBLY; DRAWINGS; DATASHEET; CERTIFICATE AND ALL MANUALS IS REQUIRED ON EVERY DELIVERY
	SUPPL P/N: 796008
	2
	 
	 

	72
	679658
	PUMP, CENTRIFUGAL: NPSH: 5.52 M; CAPACITY: 125 M3/HR; TOTAL HEAD: 98 M; SIZE: 80 X 50 MM; SPEED: 2622 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: ANSI B73.1; MOUNT: HORIZONTAL; SUPPL P/N: ETN84-85; REFERENCE NO: 3196 LTI; DENSITY RANGE 1000-1200 KG/M3; PH: 5–8; SITE ALTITUDE: 1504 MASL
	SUPPL P/N: ETN84-85 | REFERENCE NO: 3196 LTI
	2
	 
	 

	73
	682783
	PUMP, ASSEMBLY: TYPE: WATER; APPLICATION: LOW TEMPERATURE COOLING CIRCUIT FOR ENGINE MODEL 20V4000G63L; SUPPL P/N: X52420300001; REFERENCE NO: 528102903
	SUPPL P/N: X52420300001 | REFERENCE NO: 528102903
	3
	 
	 

	74
	690213
	PUMP, CENTRIFUGAL: NPSH: 0.5 M; CAPACITY: 6000 IPH; TOTAL HEAD: 5 M; SIZE: 25 MM; SPEED: 2720 RPM; STAGE: 1; DRIVER: MOTOR; SPECIFICATION: CTM 25-8 P; REFERENCE NO: 1310-4290
	REFERENCE NO: 1310-4290
	1
	 
	 

	75
	691843
	PUMP, ROTARY: TYPE: REVERSIBLE LOBE; PORT SIZE: 10 IN; CAPACITY: 391/440 M3/HR; SPEED: 490/540 RPM; RATING: 330 KPA; DRIVER: ELECTRIC MOTOR WITH GEAR; TOTAL HEAD: 25/07 M; SPECIFICATION: VX186-368QD; MOUNT: HORIZONTAL; PLEASE THE FOLLOWING WITH DRAWINGS, DATA SHEET, TEST CERTIFICATE, PERFOMANCE CURVES AND MANUAL
	SPECIFICATION: VX186-368QD
	6
	 
	 

	76
	693237
	PUMP, CENTRIFUGAL: NPSH: 2 M; CAPACITY: 25 M3/HR; TOTAL HEAD: 30 M; SIZE: 50 X 32 MM; SPEED: 2880 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 32-160; MOUNT: HORIZONTAL; SUPPL P/N: 2125900X0X
	SUPPL P/N: 2125900X0X
	4
	 
	 

	77
	698141
	PUMP, CENTRIFUGAL: NPSH: 72 M3/HR; CAPACITY: 120 M3/HR; TOTAL HEAD: 7.2 M; SIZE: DISCHARGE DIAMETER: 113 MM; SUCTION DIAMETER: 80 MM; SPEED: 1400 RPM; STAGE: TWO; DRIVER: MOTOR; TYPE: SUBMISSIBLE; OEM P/N: NP3069MT-1 ADAPTIVE 433; MOTOR NUMBER: N3069.16013-10-4BB-W; 1.3 KW; INSTALLATION TYPE: P-SEMI PERMANENT, WET, SELF CLEANING, SEMI-OPEN CHANNEL IMPELLER, IDEAL FOR PUMPING IN WATER WASTE
	OEM P/N: NP3069MT-1 ADAPTIVE 433
	5
	 
	 

	78
	703878
	PUMP, ASSEMBLY: TYPE: SCREW; APPLICATION: OIL; SUPPL P/N: 30-50-ALU-HC
	SUPPL P/N: 30-50-ALU-HC
	1
	 
	 

	79
	706911
	PUMP, ASSEMBLY: TYPE: HIGH PRESSURE CENTRIFUGAL; APPLICATION: WATER CANNONS; SUPPL P/N: MTC-A-65/6A-05.1/10.81; REFERENCE NO: 9971660934/000300/05; FLOW RATE: 50.40M3/H; HEIGHT: 290.43M; SPEED: 2975MIN; MAT. NO: 01190081; ZN 3823-219
	SUPPL P/N: MTC-A-65/6A-05.1/10.81 | REFERENCE NO: 9971660934/000300/05
	1
	 
	 

	80
	707139
	A; CUSAPPA OIL COOLING PUMP INCLUDED REFERENCE PLP20.31.5DO-0351-LGE/GD-N 22.5 CC/REV; CHARGE PUMP INPUT 16/32 18 TEETH SPLINE AND OUTPUT 16/32 9 TEETH SPLINE; CHARGE PUMP MOUNTINGS INPUT / OUTPUT SIDE SAE SPLINE; INPUT SHAFT ON MAIN PUMP ANSI B92.1; 39.5 MM USABLE SPLINE LENGTH; OD 34.5 MM; OUTPUT 16/32 18 TEETH SPLINED; CHARGE PUMP RELIEF VALVE SETTING 150 BAR; INTERNAL GEAR CHARGE PUMP WITH EXTERNAL SUCTION AND ADDITIONAL GEAR OIL COOLING PUMP; 21 TEETH 16/32 PRESSURE 250 BAR; ELECTRO HYDRAULICS CONTROL SOLENOIDS 24V; REVERSIBLE DIRECTION; FORWARD RELIEF VALVE SETTING 300 BAR; REVERSE APPLICATION: HYDRAULIC DRIVE; MOUNT: FLANGE SAE C; POWER 98 KW AND TORQUE 305 NM AT CONTINIOUS SPEED 3100 RPM ON CONTINIOUS PUMP, ROTARY: TYPE: HYDRAULIC; PORT SIZE: 1 IN; CAPACITY: 75 CM2; SPEED: VARIOUS; RATING: 420 BAR; DRIVER: ELECTRIC MOTOR;
	 
	1
	 
	 

	81
	707723
	PUMP, CENTRIFUGAL: NPSH: 1.8 M; CAPACITY: 55 M3/HR; TOTAL HEAD: 83 M; SIZE: 80 X 50 MM; SPEED: 2960 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: SUCTION END; SPECIFICATION: DIN 24256; DIN EN 22858; MOUNT: FLANGE B1; SHAFT DIAMETER: 55 MM; SUPPL P/N: KRC-50/250-308/GN; REFERENCE NO: 1293781/01-1293786/01; IMPELLER SIZE: 253 MM; TOP-DISCHARGE; DATASHEET INCLUDE PUMP CURVE AND TEST CERTIFICATE TO BE INCLUDED IN EVERY DELIVERY; EVERY ITEM SHOULD BE DELIVERED WITH THE LATEST DOCUMENT REVISIONS
	SUPPL P/N: KRC-50/250-308/GN | REFERENCE NO: 1293781/01-1293786/01
	1
	 
	 

	82
	708340
	PUMP, ROTARY: TYPE: HYDRAULIC; PORT SIZE: 1-1/2 IN; CAPACITY: 260 R/KWHR; SPEED: 1800 RPM; RATING: 260 R/KWHR; APPLICATION: PISTON; SPECIFICATION: ISO 9001; MOUNT: FLANGE (4) HOLE; MANUF P/N: 4102885.4; DRAWING NO: AL-5344-00-001 REV 0; REFERENCE NO: 0.84/10540/2; DRUM RECLAIMER - R6280; 11026064
	MANUF P/N: 4102885.4 | REFERENCE NO: 0.84/10540/2 | DRAWING NO: AL-5344-00-001 REV 0
	1
	 
	 

	83
	709509
	PUMP, CENTRIFUGAL: NPSH: 3 M; CAPACITY: 385 M3/HR; TOTAL HEAD: 50.9 M; SIZE: 200 X 150 MM; SPEED: 985 RPM; STAGE: 1; DRIVER: MOTOR; TYPE: SLURRY; SPECIFICATION: 8/6 EE-AH; SHAFT DIAMETER: 80 MM
	 
	1
	 
	 

	84
	711764
	PUMP: TYPE: ROTARY GEAR; SIZE: 1 IN; CAPACITY: 50 L/MIN; SPEED: 1440 RPM; RATING: 1.1 KW; DRIVER: ELECTRIC MOTOR; APPLICATION: RECIRCULATION PUMP LUBE OIL; SUPPL P/N: HGBX-100L
	SUPPL P/N: HGBX-100L
	1
	 
	 

	85
	713073
	PUMP, CENTRIFUGAL: NPSH: 2.51 M; CAPACITY: 170 M3/HR; TOTAL HEAD: 83 M; SIZE: 51.86 KW; SPEED: 2970 RPM; STAGE: SINGLE; DRIVER: MOTOR 7.5 KW; TYPE: KRC-100B/250-308/GN; SPECIFICATION: KRC; MOUNT: BASE PLATE; SUPPL P/N: 1289603/03; REFERENCE NO: 1289603/03-2 4 0LCL21/22; KRC 100B/250-308/GN; SINGLE STAGE: Q 170M3/H; HEAD 74.5 M; POWER 51.86 KW; TS 100 DEGREE CELCIUS; PT 30 BAR; PS 20 BAR; WEIGHT 150 KG; AP001; SINGLE STAGE; PS 20
	SUPPL P/N: 1289603/03 | REFERENCE NO: 1289603/03-2 4 0LCL21/22
	1
	 
	 

	86
	717906
	PUMP, CENTRIFUGAL: NPSH: 0 M; CAPACITY: 25200 L/HR; TOTAL HEAD: 25 M; SIZE: 165 X 25 MM; SPEED: 2684 RPM; STAGE: 1; DRIVER: MOTOR; TYPE: SLURRY; REFERENCE NO: AH400227
	REFERENCE NO: AH400227
	1
	 
	 

	87
	717907
	PUMP, CENTRIFUGAL: NPSH: 1.6 M; CAPACITY: 24000 L/HR; TOTAL HEAD: 40 M; SIZE: 200 X 40 MM; SPEED: 2900 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR 7.5 KW 2P; TYPE: SLURRY; REFERENCE NO: SR11010021-1NP185
	REFERENCE NO: SR11010021-1NP185
	1
	 
	 

	88
	717908
	PUMP, ASSEMBLY: TYPE: VACUUM; APPLICATION: DEWATERING GYPSUM
	 
	1
	 
	 

	89
	718025
	TYPE: SLURRY; REFERENCE NO: WP51825 PUMP, CENTRIFUGAL: NPSH: 3 M; CAPACITY: 385 M3/HR; TOTAL HEAD: 46 M; SIZE: 8/6 EE-AH MM; SPEED: 985 RPM; STAGE: 1; DRIVER: MOTOR;
	REFERENCE NO: WP51825 PUMP, CENTRIFUGAL: NPSH: 3 M
	1
	 
	 

	90
	718290
	PUMP: TYPE: SHAFT; SIZE: DN 4 X 6 MM; CAPACITY: 290 ML/MIN; SPEED: 5 RPM; RATING: 5 W; DRIVER: MOTOR; POTENTIAL: 115/230 V; FURNISHED ITEMS: HAS A CABLE WITH 3 WIRE CONNECTION; CASING MATERIAL: ALLUMINIUM / STEEL; APPLICATION: RECIPROCATING PUMP USED AT SMOKE STACK COOLER; SUPPL P/N: 83234954; V=115/230, HZ=50/60 COIL; POWER / RATING: 5 W; SUPPLIERS TO PROVIDE TECHNICAL DATASHEET
	SUPPL P/N: 83234954
	1
	 
	 

	91
	719006
	PUMP, CENTRIFUGAL: NPSH: 4.9 M; CAPACITY: 110 M3/HR; TOTAL HEAD: 30 M; SIZE: 100 X 80 MM; SPEED: 1460 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR 22 KW; 1460 RPM; TYPE: SLURRY; SPECIFICATION: ROWA-UV80.32-TMU 160L4-250
	 
	1
	 
	 

	92
	721434
	PUMP, CENTRIFUGAL: NPSH: 1.1 M; CAPACITY: 15 M3/HR; TOTAL HEAD: 70 M; SIZE: 50 X 32 MM; SPEED: 2935 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; MOUNT: VERTICAL; SHAFT DIAMETER: 42 MM; MODEL NO: LSN50-32-250-S1VL11102
	MODEL NO: LSN50-32-250-S1VL11102
	1
	 
	 

	93
	721507
	PUMP, CENTRIFUGAL: NPSH: 4.5 M; CAPACITY: 720 M3/HR; TOTAL HEAD: 66 M; SIZE: 200 X 250 MM; SPEED: 1485 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: DRAINAGE; SPECIFICATION: ISO 5199/EN 25199; MOUNT: HORIZONTAL; SHAFT DIAMETER: 55 MM; MODEL NO: LS-200-500-S2VL1-20004
	MODEL NO: LS-200-500-S2VL1-20004
	5
	 
	 

	94
	723403
	PUMP: TYPE: 2 STAGE; SIZE: DN 125; CAPACITY: 208 M3/HR; SPEED: 1470 RPM; RATING: 16 BARS; SUPPL P/N: TP 125-420/4-A -F-B-BQQE;
	SUPPL P/N: TP 125-420/4-A -F-B-BQQE
	1
	 
	 

	95
	724325
	PUMP: TYPE: SUBMERSIBLE DRAINAGE; SIZE: HT 1180 X WD 900 X DIA 610; CAPACITY: 576 M3/HR; SPEED: 2965 RPM; RATING: 148-400 A; DRIVER: ELECTRIC MOTOR; POTENTIAL: 95 KW; FURNISHED ITEMS: FLOAT SWITCH; CASING MATERIAL: CI; APPLICATION: DIRTY WATER; SUPPL P/N: PD524400-INT; DN 100-150; MAIN BEARING: TWO SINGLE-ROW ANGULAR CONTACT BALL BEARINGS. SUPPORT BEARING: CYLINDRICAL SINGLE-ROW ROLLER BEARING WITH C3 CLEARANCE. CASTED PARTS: CAST IRON, MOTOR SHAFT: SS, IMPELLER: HARD-ON, DIFFUSERS: NITRATE RUBBER, SCREWS AND NUTS: SS
	SUPPL P/N: PD524400-INT
	5
	 
	 

	96
	728149
	PUMP, ROTARY: TYPE: GEAR; PORT SIZE: 19 X 13 MM; CAPACITY: 25.5 L/MIN; SPEED: 1500 MM; RATING: 7.5 KW; SPECIFICATION: ISO; SUPPL P/N: GHP2-D-25; GHP2-D-25
	SUPPL P/N: GHP2-D-25
	6
	 
	 

	97
	729091
	PUMP: TYPE: HP BYPASS HYDRAULIC; SIZE: 95 MM; CAPACITY: 19 M3; SPEED: 1800 RPM; RATING: PN 280; SUPPL P/N: D951Z2205/A; DRAWING NO: HZ-R18A1-RKP019SM; 19 CCM/REV
	PN 280 | SUPPL P/N: D951Z2205/A | DRAWING NO: HZ-R18A1-RKP019SM
	1
	 
	 

	98
	729474
	PUMP, CENTRIFUGAL: NPSH: 15.1 M; CAPACITY: 212.7 CM3/HR; TOTAL HEAD: 18.1 M; SIZE: DN80; SPEED: 2900 RPM; STAGE: PN 10; DRIVER: 5.5 KW; SUPPL P/N: 00PPG000032300; MODEL NO: VEROTWIN-DPL 80/145-5,5/2
	PN 10 | SUPPL P/N: 00PPG000032300 | MODEL NO: VEROTWIN-DPL 80/145-5,5/2
	1
	 
	 

	99
	729480
	PUMP, CENTRIFUGAL: NPSH: 12.7 M; CAPACITY: 84.1 CM3/HR; TOTAL HEAD: 15 M; SIZE: DN65; SPEED: 2900 RPM; STAGE: PN 10; DRIVER: 2.2KW; TYPE: VEROTWIN-DPL 65/120(111.5)-2,2/2; SUPPL P/N: 00PPG00005100; MODEL NO: VEROTWIN-DPL 65/120(111.5)-2,2/2
	PN 10 | SUPPL P/N: 00PPG00005100 | MODEL NO: VEROTWIN-DPL 65/120(111.5)-2,2/2
	1
	 
	 

	100
	729519
	SUPPL P/N: NK 80-200/211 A2F2AE-SBQQE; MODEL NO: B99263422P117190001 PUMP, CENTRIFUGAL: NPSH: 8 M; CAPACITY: 86 CM3/HR; TOTAL HEAD: 16 M; SIZE: 211 MM; SPEED: 1475 RPM; STAGE: PN 16; DRIVER: 7.5 KW;
	SUPPL P/N: NK 80-200/211 A2F2AE-SBQQE | PN 16 | MODEL NO: B99263422P117190001 PUMP, CENTRIFUGAL: NPSH: 8 M
	1
	 
	 

	101
	729520
	PUMP, CENTRIFUGAL: NPSH: 2.3 M; CAPACITY: 92 CM3/HR; TOTAL HEAD: 54 M; SIZE: 397 MM; SPEED: 1479 RPM; STAGE: PN 16; DRIVER: 30KW; SUPPL P/N: NK80-400/397 A2F2BE-SBQQE; MODEL NO: B99315768P117370003
	PN 16 | SUPPL P/N: NK80-400/397 A2F2BE-SBQQE | MODEL NO: B99315768P117370003
	1
	 
	 

	102
	729524
	PUMP, CENTRIFUGAL: NPSH: 3.26 M; CAPACITY: 191 CM3/HR; TOTAL HEAD: 30.9 M; SIZE: 340 MM; SPEED: 1470 RPM; STAGE: PN 16; DRIVER: 22KW; SUPPL P/N: TP 125-340/4 A-F-B-BAQE; MODEL NO: A98858623P218030002
	PN 16 | SUPPL P/N: TP 125-340/4 A-F-B-BAQE | MODEL NO: A98858623P218030002
	1
	 
	 

	103
	729526
	PUMP, CENTRIFUGAL: NPSH: 4.08 M; CAPACITY: 290 CM3/HR; TOTAL HEAD: 41 M; SIZE: 450 MM; SPEED: 1480 RPM; STAGE: PN 16; DRIVER: 45KW; SUPPL P/N: TP 150-450/4 A-F-B-BAQE; MODEL NO: A97927106P317010001
	PN 16 | SUPPL P/N: TP 150-450/4 A-F-B-BAQE | MODEL NO: A97927106P317010001
	1
	 
	 

	104
	729527
	PUMP, CENTRIFUGAL: NPSH: 3.81 M; CAPACITY: 317 CM3/HR; TOTAL HEAD: 46 M; SIZE: 520 MM; SPEED: 1485; STAGE: PN 16; DRIVER: 55 KW; SUPPL P/N: TP 150-520/4 A-F-B-BAQE; MODEL NO: A97927105P316310
	PN 16 | SUPPL P/N: TP 150-520/4 A-F-B-BAQE | MODEL NO: A97927105P316310
	1
	 
	 

	105
	731037
	PUMP: TYPE: FOAM INDUCTION MOTOR PUMP; SIZE: FD6000-09S1-03-290; CAPACITY: 500-6000; SPEED: 1440 RPM; RATING: 3 PCT ADMIXTURE; DRIVER: MOTOR; CASING MATERIAL: FPM CUAL 10NI5FE5; SUPPL P/N: FD6000/3-PP-S; PTFE 1.4571; KERAMIK; ALMG3SI; STAHL; APPLICATION: FIRE WATER SYSTEM; UNIT TO COME AS COMPLETE ASSEMBLY PARTS: WATER MOTOR (CAST AL, HC COATED), PROPORTIONING PUMP (SS); PIPEWORK (SS) AND SUPPORT FRAME AS SHOWN IN MANUAL
	SUPPL P/N: FD6000/3-PP-S
	1
	 
	 

	106
	731845
	PUMP: TYPE: EXTERNAL GEAR; CAPACITY: 11.3 CM3/REV; SPEED: 3000 RPM; RATING: 250 BARS; DRIVER: ELECTRIC MOTOR; CASING MATERIAL: ALUMINIUM; APPLICATION: HYDRAULIC SYSTEM; SUPPL P/N: MNR0510525009; REFERENCE NO: AZPF11011RCB20MB;
	SUPPL P/N: MNR0510525009 | REFERENCE NO: AZPF11011RCB20MB
	1
	 
	 

	107
	750947
	APPLICATION: BFP MIN-FLOW SKID HPU; SPECIFICATION: ISO; SUPPL P/N: 752-00-009; MODEL NO: ALP2-D-9 PUMP, ROTARY: TYPE: GEAR PUMP; PORT SIZE: 13 X 13 MM; CAPACITY: 9.1 L/MIN; SPEED: 4000 RPM; RATING: 4 KW; DRIVER: MOTOR;
	SUPPL P/N: 752-00-009 | MODEL NO: ALP2-D-9 PUMP, ROTARY: TYPE: GEAR PUMP
	4
	 
	 

	108
	751347
	PUMP: TYPE: HYDRA-CELL D10; SIZE: ¾” 28 L/MIN; CAPACITY: 28 L/MIN; SPEED: 1410 RPM; RATING: 8.26/4.75 A; APPLICATION: COURSE ASH CONVEYOR WASH BOX
	 
	4
	 
	 

	109
	761800
	PUMP, CENTRIFUGAL: NPSH: 4.3 M; CAPACITY: 180 M3/HR; TOTAL HEAD: 67 M; SIZE: 125 X 80 MM; SPEED: 2965 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: LSN125-80 250 S1VL1; MOUNT: HORIZONTAL; SUPPL P/N: 61220402
	SUPPL P/N: 61220402
	3
	 
	 

	110
	762297
	PUMP, ASSEMBLY: TYPE: MAIN PUMPS ASSEMBLY; APPLICATION: HYDRAULIC PUMP FOR COAL STACKER; OEM P/N: 2625-ACH-SP-054; DRAWING NO: ACH-2625-054; REFERENCE NO: ACH-SP-054; TORQUE 0.88 NM; MOUNTING SAE J744; WEIGHT 40KG, ROTATION CLOCKWISE/COUNTERCLOCKWISEFLANGE SIZE 25.4MM; SHAFT SPLINED; INPUT SPEED 4250RPM; PRESSURE 0.7BAR, SENSOR VOLT 4.5V-8.5VTEMPERATURE RANGE -40 TO 110˚C; CURRENT 12 -20 MA
	OEM P/N: 2625-ACH-SP-054 | REFERENCE NO: ACH-SP-054 | DRAWING NO: ACH-2625-054
	4
	 
	 

	111
	675656
	PUMP: TYPE: H2 SEAL OIL; SIZE: 150 MM; CAPACITY: 320-18 MM2/S; SPEED: 1450 RPM; RATING: 4 BAR; SPECIFICATION: WK1-100622; APPLICATION: SEAL OIL SYSTEM; OEM P/N: WK4-101676P0001; MANUF P/N: 675656; PACKAGE NO: MKW42AP001; MKW46AP001
	MANUF P/N: 675656;
	6
	 
	 

	112
	675382
	PUMP: TYPE: VACUUM SEAL OIL; SIZE: 20 MM; CAPACITY: 120 L/MIN; SPEED: 950 RPM; RATING: 10 BAR; SPECIFICATION: WK1-100622; APPLICATION: GENERATOR AUX SEAL OIL SYSTEM; OEM P/N: SNGS-120-E-R-42-U12.1-W32 -ATEX; WK4-101675P0001; DRAWING NO: WK1-100622/MKW36AP001
	OEM P/N: SNGS-120-E-R-42-U12.1-W32 -ATEX; WK4-101675P0001; DRAWING NO: WK1-100622/MKW36AP001
	3
	 
	 

	113
	774992
	PUMP: TYPE: KNF DIAPHRAM VACCUM PM29994-86; SIZE: N/A; CAPACITY: 2.5 BAR; SPEED: 6.5 L/MIN; RATING: 115/230 V; CASING MATERIAL: VITON (PVDF); OEM P/N: PU4292-N811; FREQUENCY: 50 HZ; 1.5/0.75A; 60W; MAX FLOW RATE: 5-6 NI/MIN
	 
	1
	 
	 

	114
	766504
	PUMP: TYPE: ROTARY DRUM; SIZE: 41 MM; CAPACITY: 0 TO 80 L/MIN; SPEED: 3000 RPM; RATING: 0 TO 6 BAR; SUPPL P/N: L0122-206; MODEL NO: PVDF 41-L-SL-1200MM ; USE IN CHEMICAL TRANSFER FROM 1000L FLOWBINS OF SODIUM HYPOCHLORITE 12-15% COMPLETE WITH ALL ACCESSORIES.E. HOUSING: PVDF, IMPELLER: ETFE, DRIVE SHAFT: HASTELLOY C (HC-4)(2.4610). INCLUDE STORAGE BRACKET HOSE CONNECTION: 25MM HOSE TAIL, G 1¼” MALE THREADED. HOSE: VERSACHEM -UHMWPE -25MM, LENGTH-10M. CLAMP HOSE STEPLESS 35.8-39.0 MOTOR: MA II5-S 575W, 230V, ENCLOSURE: IP54-EXTREMLY HARSH ENVIRONMENTS & FUMING LIQUIDS. NOZZLE PVDF/FPM- 1” HOSE CON
	 
	1
	 
	 

	115
	766503
	PUMP: TYPE: ROTARY DRUM PUMP; SIZE: 41 MM; CAPACITY: 0 TO 80 L/MIN; SPEED: 3000 RPM; RATING: 0 TO 6 BAR; SUPPL P/N: L0151-158; MODEL NO: RE SS 41-L-MS-1200MM; USE IN CHEMICAL TRANSFER FROM 1000L FLOWBINS OF SULPHURIC ACID 98% & PHOSPHORIC ACID 85% WITH ALL ACCESSORIES. HOUSING: STAINLESS STEEL; IMPELLER: ETFE, DRIVE SHAFT: STAINLESS STEEL (1.4571), INCLUDE STORAGE BRACKET HOSE CONNECTION: 25MM HOSE TAIL, G 1¼” MALE THREADED. HOSE: VERSACHEM -UHMWPE -25MM, LENGTH-10M. CLAMP HOSE STEPLESS 35.8-39.0 MOTOR: MA II5-S 575W, 230V, ENCLOSURE: IP54-EXTREMLY HARSH ENVIRONMENTS & FUMING LIQUIDS. NOZZLE PVDF/FPM- 1” HOSE CON.
	 
	1
	 
	 

	116
	675381
	PUMP: TYPE: VACUUM; SIZE: 20 X 25 MM; CAPACITY: 18.9 M3/HR; SPEED: 1405 RPM; RATING: 0.005 MBAR; SPECIFICATION: WK1-100622; APPLICATION: SEAL OIL SYSTEM; OEM P/N: WK4-101771P0001; SUPPL P/N: D16B - EX; DRAWING NO: MKQ11AN001 REV 0; LEYBOLD TRIVAC
	 
	12
	 
	 

	117
	676225
	STATOR: TYPE: WATER PUMP; MANUF P/N: CHN-B80-250/01G-W20; WK4-101721P0001; DRAWING NO: WK4-101677R0010/26, 32 REV C; REFERENCE NO: CNH-B80-250; COOLING WATER UNIT
	 
	6
	 
	 

	118
	675657
	PUMP: TYPE: AIR SEAL OIL; SIZE: 150 MM; CAPACITY: 210 L/MIN; SPEED: 2900 RPM; RATING: 12 BAR; SPECIFICATION: WK1-100622; APPLICATION: GENERATOR AUX SEAL OIL SYSTEM; OEM P/N: WK4-101674P0001; MANUF P/N: 675657; PACKAGE NO: MKW21AP001; MKW22AP001; MKW23AP001
	 
	6
	 
	 

	119
	623403
	PUMP, CENTRIFUGAL: NPSH: 2.17 M; CAPACITY: 230.06 M3/HR; TOTAL HEAD: 26.3 M; SIZE: 200 X 150 MM; SPEED: 1482 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MCP200-150 315VD; MOUNT: HORIZONTAL; REFERENCE NO: 9972457229/200
	 
	1
	 
	 

	120
	725753
	PUMP, CENTRIFUGAL: NPSH: 13.2 M; CAPACITY: 2040 M3/HR; TOTAL HEAD: 220 M; SIZE: 450 X 350 MM; SPEED: 1485 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR U500/160 6600 V 4P 1800 KW; 1485 RPM; TYPE: DOUBLE SUCTION HORIZONTAL SPLIT CASING; MOUNT: HORIZONTAL; SHAFT DIAMETER: 120 MM
	 
	2
	 
	 

	121
	585006
	MKW36: PUMP; P/N WK4-101675P0001
PUMP: TYPE: SCREW; SIZE: 65 X 50 MM; CAPACITY: 120 L/MIN; SPEED: 950 RPM; RATING: 10.5 BAR; DRIVER: ELECTRIC MOTOR; CASING MATERIAL: EN-GJS-400-15; APPLICATION: SEAL OIL; MANUF P/N: SNGS120ER42U12.1-W32/DS41A
	 
	6
	 
	 

	122
	634487
	MKW42/46: PUMP; P/N WK4-101676P0001
PUMP: TYPE: SCREW; SIZE: 65 X 50 MM; CAPACITY: 55.9-57.6 L/MIN; SPEED: 1450 RPM; RATING: 4 BAR; DRIVER: MOTOR; APPLICATION: H2 SEAL OIL; SUPPL P/N: SNGS80ER36U12.1-W32/DS35A
	 
	6
	 
	 

	123
	762659
	PUMP, CENTRIFUGAL: NPSH: 1.9 M; CAPACITY: 171 M3/HR; TOTAL HEAD: 40.87 M; SIZE: 125 X 100 MM; SPEED: 1475 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 100-400; MOUNT: HORIZONTAL; REFERENCE NO: 396.100/2
	REFERENCE NO: 396.100/2
	3
	 
	 

	124
	762675
	PUMP, CENTRIFUGAL: NPSH: 2.6 M; CAPACITY: 330 M3/HR; TOTAL HEAD: 56 M; SIZE: 200 X 150 MM; SPEED: 1480 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: HORIZONTAL; SPECIFICATION: LS150-500 S1VV1; MOUNT: HORIZONTAL; REFERENCE NO: 60353805
	REFERENCE NO: 60353805
	4
	 
	 

	125
	721951
	PUMP, CENTRIFUGAL: NPSH: 2.3 M; CAPACITY: 385 M3/HR; TOTAL HEAD: 10.02 M; SIZE: 200 X 250 MM; SPEED: 960 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: 200-315; MOUNT: HORIZONTAL; REFERENCE NO: C03627/9
	SPECIFICATION: 200-315
	3
	 
	 

	126
	687431
	PUMP, CENTRIFUGAL: NPSH: 1.2 M; CAPACITY: 171 M3/HR; TOTAL HEAD: 75.6 M; SIZE: 200 X 150 MM; SPEED: 1480 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: CPK150-500; MOUNT: HORIZONTAL; REFERENCE NO: 506388/90
	SPECIFICATION: CPK150-500
	3
	 
	 

	127
	693239
	PUMP, CENTRIFUGAL: NPSH: 4.28 M; CAPACITY: 98.59 M3/HR; TOTAL HEAD: 58.32 M; SIZE: 100 MM; SPEED: 2948 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: SUBMERSIBLE; SPECIFICATION: KRTD 80-315/372 UG1-S; MODEL NO: UGI449273
	SPECIFICATION: KRTD 80-315/372 UG1-S
	2
	 
	 

	128
	761799
	PUMP, CENTRIFUGAL: NPSH: 5.52 M; CAPACITY: 120.03 M3/HR; TOTAL HEAD: 107.8 M; SIZE: 100 X 65 MM; SPEED: 2985 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MCP100-065 315VD; MOUNT: HORIZONTAL; SUPPL P/N: 2135903615
	SPECIFICATION: MCP100-065 315VD
	3
	 
	 

	129
	757041
	PUMP: TYPE: LIQUID RING VACUUM; SIZE: 5 X 5 IN; CAPACITY: 900 M3/HR; SPEED: 970 RPM; RATING: 33 MBAR ABS; DRIVER: ELECTRIC MOTOR; SPECIFICATION: MVT 410-260
	SPECIFICATION: MVT 410-260
	3
	 
	 

	130
	620425
	AERATOR: TYPE: SURFACE; MODEL NO: K1.8-NA5NA; MATERIAL: SS 304L; FOR USE AT SEWAGE TREATMENT PLANT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).
	MODEL NO: K1.8-NA5NA
	3
	 
	 

	131
	620447
	COMPRESSOR, AIR: CAPACITY: 29.10 M3/HR; DISCHARGE PRESSURE: 10 BAR; POTENTIAL: 400 VAC; POWER: 4 KW; CURRENT: 10 A; DRIVER: V-BELT; VOLUME CAPACITY: 200 L; REFERENCE NO: 1676420001; 004134; TO BE SUPPLIED WITH OEM MANUAL; DATA SHEET; GENERAL ARRANGEMENT DRAWINGS AND SPARE PARTS LIST; 17.13 SCFM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).
	GA 5-11
	2
	 
	 

	132
	772681
	PUMP, CENTRIFUGAL: NPSH: 2.3 M; CAPACITY: 17 M3/HR; TOTAL HEAD: 21.5 M; SIZE: 2x1 1/4 IN; SPEED: 2900 RPM; STAGE: 1; DRIVER: ELECTRIC MOTOR; TYPE: HORIZONTAL; SPECIFICATION: NEPO-50-32-160; SHAFT DIAMETER: 24; DRAWING NO: 67981; SERIAL NO. 13.0437/1; ON EVERY DELIVERY, PLEASE PROVIDE DRAWINGS, DATA SHEET AND MANUAL
	SPECIFICATION: NEPO-50-32-160
	2
	 
	 

	133
	TBC
	rated flow:10m3/hr, rated head:27.1 m, CM10-2 A-R-A-V-AQQV
	 
	6
	 
	 

	134
	TBC
	rated flow:10m3/hr, rated head:40.5 m, CM10-3 A-R-A-V-AQQV
	 
	6
	 
	 

	135
	TBC
	rated flow:3.1m3/hr, rated head:41.5 m, CM10-3 A-R-E-AOOE F-A-A-N
	 
	2
	 
	 

	136
	643443
	PUMP, CENTRIFUGAL: SIZE: DN32; STAGE: SINGLE; DRIVER: ELECTRIC MOTOR; OEM P/N: NIT32-160/01U5A-W4-19/200; GAS COOLING SYSTEM
	 
	2
	 
	 

	137
	585005
	PUMP: TYPE: SCREW; SIZE: 80 X 65 MM; CAPACITY: 210 L/MIN; SPEED: 2900 RPM; RATING: 13.8 BAR; DRIVER: ELECTRIC MOTOR; CASING MATERIAL: EN-GJS-400-15; APPLICATION: SEAL OIL; MANUF P/N: SNGS210ER40U12.1-W32/DS38A
	 
	2
	 
	 

	138
	681526
	PUMP, FUEL: TYPE: DIESEL; FLOW RATE: 0.35 L/S; PRESSURE RATING: 1.5 BAR; INLET SIZE: 83 MM; CONNECTION TYPE: BOLT; SPECIAL FEATURES: O-RING 00429083000; APPLICATION: LOW PRESSURE DELIVERY PUMP FOR ENGINE MODEL 20V4000G63L; SUPPL P/N: X52808100004; REFERENCE NO: 528102903
	 
	2
	 
	 

	139
	682784
	PUMP, FUEL: TYPE: HAND PRIMING; FLOW RATE: 0.35 L/S; PRESSURE RATING: 1.5 BAR; INLET SIZE: 30 MM; CONNECTION TYPE: THD; SPECIAL FEATURES: O-RING 00429083000; APPLICATION: DIESEL FUEL ENGINE TYPE 20V4000G63L; SUPPL P/N: X54808800001; REFERENCE NO: 528102903
	 
	3
	 
	 

	140
	682785
	PUMP, FUEL: TYPE: HP FUEL; FLOW RATE: 0.35 L/S; PRESSURE RATING: 1800 BAR; INLET SIZE: 130 MM; CONNECTION TYPE: BOLT; SPECIAL FEATURES: O-RING 700429130003; APPLICATION: ENGINE MODEL 20V4000G63L; SUPPL P/N: X59507300003; REFERENCE NO: 528102903
	 
	3
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