{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["BOQ","SUMMARY","TOTAL PROJECT AMOUNT"],"read":"whole","date_system":"1900"}

{"sheet":"BOQ","index":0,"n_rows":71,"n_cols":7,"rows_kept":71,"merged":[[65,0,65,5]]}
["ANNEXURE B: BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["A","SABS 1200 A","SCHEDULE A : PRELIMINARY AND GENERAL"]
[]
["A1","8.3","FIXED-CHARGE ITEMS"]
[]
["A1.1","8.3.1     ","Contractual Requirements, safety file, induction and  access card.","Sum",{"v":1,"d":"1.0"}]
[]
["A1.12",null,"Site establishment","Sum",{"v":1,"d":"1.0"}]
[]
["A1.13","8.3.4     ","Removal of site establishment","Sum",{"v":1,"d":"1.0"}]
[]
["A2","8.4","TIME-RELATED ITEMS"]
[]
["A2.1","8.4.1     ","Contractual Requirements","Sum",{"v":0,"d":"0.0"}]
[]
[null,"8.4.2","Operate and maintain facilities on the Site:","Sum ",{"v":0,"d":"0.0"}]
[null,"8.4.2.2","Facilities for Contractor for duration of construction, except where otherwise stated"]
["A2.6","(a)","Offices and storage sheds","Sum",{"v":0,"d":"0.0"}]
["A 2.10","(c)","Tools and equipment","Sum",{"v":0,"d":"0.0"}]
["A 2.11","(d)","Water supplies, electric power and communication","Sum",{"v":0,"d":"0.0"}]
["A 2.12","(e)","Dealing with water","Sum",{"v":0,"d":"0.0"}]
["A 2.13","(f)","Access","Sum",{"v":0,"d":"0.0"}]
{"$rows_empty":7}
[null,null,"Total carried over to Summary page "]
["ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
["B","SABS 1200 C","SCHEDULE B : PLACEMENT OF NEW SCREED AND WATERPROOFING"]
["B1"]
["B1.1",null,"Clean gutters and unblock downpipes. Size of gutter is +/- 700mm and downpipe size dimetre is 110mm","m",{"v":1,"d":"  1"}]
[]
[null,null,"DEMOLITIONS, REMOVALS AND ALTERATIONS"]
[null,null,"Removal of 50mm Screed on floors. Remove existing flat roof waterproofing to receive new (elsewhere)\nand prepare screed as per manufacturer's instruction","m2",{"v":1,"d":"  1"}]
[]
["B1.2",null,"Remove old water proofing membrane including old joint sealant and clean surface to receive sand cement screed","m2",{"v":1,"d":"  1"}]
[]
[null,null,"JOINT SEALANTS ETC"]
[null,null,"Silicone sealing compound including backing cord, bond breaker,\nprimer, etc"]
["B1.2",null,"Apply new flexible joint sealant to existing constructions.","m",{"v":1,"d":"  1"}]
[null,null,"6 x 10mm In saw cut joints in floors","m",{"v":1,"d":"  1"}]
[null,null,"6 x 15mm In expansion joints in soffits including raking out\nexpansion joint filler as necessary","m",{"v":1,"d":"  1"}]
[]
["B1.3",null,"Supply and place new 20-30MPa at 28 days sand cement screed minimum thickness 40mm with 1:50 fall. Construction joints to enclose a maximum area of 9m2. ","m3",{"v":1,"d":"  1"}]
[]
[null,null,"Waterproofing:"]
[null,null,"For Preambles see the Model Preambles for Trades 2008 edition\npublished by the Association of South African Quantity Surveyors"]
[]
[null,null,"Concrete Roof Waterproofing"]
["B1.4",null,"Clean down the entire concrete roof completely throughout, removing all loose particles, dust and debris. Apply joint sealant material where applicable. Install 4mm dual waterproofing membrane on the roof and side cladding. Make sure that there is no water ponding and air pockets at completion.\nPLEASE REFER TO ITEM 4.1 (SCOPE OF WORK) for a complete specification.","m2",{"v":1,"d":"  1"}]
[]
["B1.5",null,"Apply UV resistant waterproofing paint.  PLEASE REFER TO SECTION 4.1. PROTECTIVE ROOFING PAINT\nTwo coats bituminous aluminium paint\nOn waterproofing to roofs","m2",{"v":1,"d":"  1"}]
[]
[null,null,"Steel roof waterproofing"]
[null,null,"Waterproofing steel roof and flashing.\n\nPLEASE REFER TO SECTION 4.2 (Project Scope) above for a complete specification.","m2",{"v":1,"d":"  1"}]
[]
[null,null,"Paint the steel roof and side flashing with UV resistant waterproofing paint.\nPLEASE REFER TO SECTION 4.2 (Project Scope) above for a complete specification\n","m2",{"v":1,"d":"  1"}]
[]
[]
[]
["Total carried over to Summary page "]
[]
[]
[]
[]
[null,null," "]

{"sheet":"SUMMARY","index":1,"n_rows":35,"n_cols":3,"rows_kept":35}
[]
["SCHEDULE","DESCRIPTION","AMOUNT"]
[]
["A","TOTAL BROUGHT FORWARD FROM SCHEDULE: PRELIMINARY AND GENERAL"]
[]
["B","TOTAL BROUGHT FORWARD FROM SCHEDULE: PLACEMENT OF NEW SCREED AND WATERPROOFING"]
{"$rows_empty":25}
["SUB TOTAL",null,{"$f":"SUM(C4:C11)","v":{"v":0,"d":"R 0.00"}}]
[]
[]
["TOTAL CARRIED FORWARD TO TOTAL PROJECT AMOUNT",null,{"$f":"C32","v":{"v":0,"d":"R 0.00"}}]

{"sheet":"TOTAL PROJECT AMOUNT","index":2,"n_rows":34,"n_cols":3,"rows_kept":34}
[]
["ITEM","DESCRIPTION","AMOUNT"]
[]
[]
[null,"AMOUNT BROUGHT FORWARD FROM SUMMARY"]
{"$rows_empty":25}
["SUB-TOTAL"]
[]
["15% VAT"]
["TOTAL CARRIED FORWARD TO TENDER FORM"]