{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["2.BOQ -Retic","3.TO Process","Sheet"],"not_rendered":{"images":1,"external_links":2,"defined_names":41},"read":"whole","date_system":"1900"}

{"sheet":"2.BOQ -Retic","index":0,"n_rows":443,"n_cols":4,"rows_kept":443,"merged":[[3,3,4,3],[7,1,7,3],[43,1,43,2],[64,1,64,2],[226,1,226,2],[274,2,274,3],[299,1,299,3],[327,1,327,2],[388,1,388,2],[404,1,404,2],[406,1,406,2],[442,1,442,2]]}
["                "]
[null,"NEC3 : RETICULATION (MV & LV) TERM CONTRACT   "]
["BILL"]
[{"$nulls":3},"Contractor's tendered rate"]
["ITEM NO.","DESCRIPTION","UNIT"]
[]
["A","PRELIMINARY AND GENERAL"]
["A.1","0-50km Radius (from nearest CNC to Site and back)"]
["A1.1.1","Establish facilities on site (include all resources required to ensure work to be fully completed)","Sum"]
["A1.1.2","Maintain facilities on site (include all resources required to ensure work to be fully completed)","Weeks"]
["A1.1.3","Security (24/7), two security guards at all times,day shift needs 2 no security officers (Grade D) with bulletproof vests and two way radios.Night shift needs 2 no security officers (Grade C) with bulletproof vests and two way radios. (All security service providers to be registered with PSIRA)_(actual cost - proof of cost e.g. invoice to be submitted when claimed)","per person/12hr shift"]
["A1.1.4","De-establish facilities on site (ensure all items to provide the works be removed and that site is normalised to customers satisfaction)","Sum"]
["A1.2",">50-100km Radius  (from nearest CNC to Site and back)"]
["A1.2.1","Establish facilities on site (include all resources required to ensure work to be fully completed)","Sum"]
["A1.2.2","Maintain facilities on site (include all resources required to ensure work to be fully completed)","Weeks"]
["A1.2.3","Security (24/7), two security guards at all times,day shift needs 2 no security officers (Grade D) with bulletproof vests and two way radios.Night shift needs 2 no security officers (Grade C) with bulletproof vests and two way radios. (All security service providers to be registered with PSIRA)_(actual cost - proof of cost e.g. invoice to be submitted when claimed)","per person/12hr shift"]
["A1.2.4","De-establish facilities on site (ensure all items to provide the works be removed and that site is normalised to customers satisfaction)","Sum"]
["A1.3",">100-150km Radius  (from nearest CNC to Site and back)"]
["A1.3.1","Establish facilities on site (include all resources required to ensure work to be fully completed)","Sum"]
["A1.3.2","Maintain facilities on site (include all resources required to ensure work to be fully completed)","Weeks"]
["A1.3.3","Security (24/7), two security guards at all times,day shift needs 2 no security officers (Grade D) with bulletproof vests and two way radios.Night shift needs 2 no security officers (Grade C) with bulletproof vests and two way radios. (All security service providers to be registered with PSIRA)_(actual cost - proof of cost e.g. invoice to be submitted when claimed)","per person/12hr shift"]
["A1.3.4","De-establish facilities on site (ensure all items to provide the works be removed and that site is normalised to customers satisfaction)","Sum"]
["A1.4",">150-200km Radius  (from nearest CNC to Site and back)"]
["A1.4.1","Establish facilities on site (include all resources required to ensure work to be fully completed)","Sum"]
["A1.4.2","Maintain facilities on site (include all resources required to ensure work to be fully completed)","Weeks"]
["A1.4.3","Security (24/7), two security guards at all times,day shift needs 2 no security officers (Grade D) with bulletproof vests and two way radios.Night shift needs 2 no security officers (Grade C) with bulletproof vests and two way radios. (All security service providers to be registered with PSIRA)_(actual cost - proof of cost e.g. invoice to be submitted when claimed)","per person/12hr shift"]
["A1.4.4","De-establish facilities on site (ensure all items to provide the works be removed and that site is normalised to customers satisfaction)","Sum"]
[null,"Travel and Accommodation"]
["A1.5","Once off rate per km (for site establishment purposes including all vehicles to transport resources etc to complete the works i.e. from contractors' base to nearest CNC including return distance) - Only when site is more than 50km from Contractor Base","km"]
["A1.6","Accommodation (3-Star or less)  - proof of cost e.g. invoice to be submitted when claimed","Cost plus Handling Fee %",{"v":0.05,"d":"5%"}]
["A1.7","Professionally registered Civil Engineer","hr"]
[null,"COMPENSATION RATES (to be used for Compensations Events only) - Schedule of Cost Components"]
[null,"TRANSPORT & EQUIPMENT"]
["A1.8","LDV ","km"]
["A1.9","Truck (2 to 4-ton)","km"]
["A1.10","Truck (8-ton)","km"]
["A1.11","Truck with Crane (8-ton)","km"]
["A1.12","Truck (22-ton) - used on approval from Eskom Representative","km"]
[null,"WORKER RATES"]
["A1.13","Linesman per hour (normal)","hr"]
["A1.14","Labourer per hour (normal)","hr"]
["A1.15","Supervisor per hour (normal)","hr"]
["A1.16","Cable Jointer (Skilled)","hr"]
[null,"TOTAL (P&Gs)"]
["B","GENERAL"]
["B1","Prepare for outages …correct snag list – check safety /quality","each"]
["B2","Excavation of soft soil","m³"]
["B3","Excavation of hard soil / rock","m³"]
["B4","Backfill and compact of holes - normal","m³"]
["B5","Backfill and compact of holes - with sand and cement mixture (labour only)","m³"]
["B6","Importing soil","m³"]
["B7","Rock drilling or Excavate using mechanical boring device i.e. Auger or Excavate using a jack hammer & compressor  (irrespective of depth of hole, each hole to be verified by Eskom's Clerk of Works)  - proof of cost e.g. invoice to be submitted when claimed","Cost plus Handling Fee %",{"v":0.05,"d":"5%"}]
["B8","Adhoc Material – Compensation: only on written instruction from Employer  - proof of cost e.g. invoice to be submitted when claimed (No retention deduction on material)","Cost plus Handling Fee %",{"v":0.05,"d":"5%"}]
["B9","Compliance to Environmental Management Plan and maintenance thereof","each"]
["B10","Health and Safety (in compliance with OH&S Act and Construction Regulations) - specify items to verify cost","each"]
["B11","Health & Safety Plan & maintaining File  ( For Minor Works  & Split Metering Projects  only 10% of the value to be paid)","each"]
["B12","PPE   - proof of cost e.g. invoice to be submitted when claimed","Actual Cost"]
["B13","Temporary labour","hr"]
["B14","Erect goal posts: temporary structure and traffic signs to regulate traffic during construction for all road crossings/railway crossing. (This includes any loss of production during these crossings and ensuring access is maintained to roads and properties as well as any fees by Provincial Traffic Department) ","each"]
["B15","Utilisation of Community Liaison Officer (Contractor to submit time sheet weekly for CLO based on attendance register)","per day"]
["B16","Cart away rubble and excavated soil to a registered dumping site","ton/km"]
["B17","Storage of material (once-off amount for the entire duration of this contract)","sum"]
[null,"All “excess” material must be returned to Eskom stores within 1 week or sooner after completion. Final payment will be withheld until all material is returned."]
["B18","Scrapped material transported to Brackenfell by truck","km"]
[null,"TOTAL (GENERAL)"]
["C","LV WORKS"]
[null,"Excavate, backfill and compact as per Eskom standard and import backfill soil where required for holes and trenches for poles, stays, flying stays and earth electrodes (all material measured elsewhere)","D-DT 0350, 0342"]
["C1","Excavate Holes Depth:1.5 to 2.0m …soft soil","each"]
["C2","Excavate Holes Depth: > 2.0m ...soft soil","each"]
["C3","Excavate Holes Depth:1.5 to 2.0m….hard soil","each"]
["C4","Excavate Holes Depth: > 2.0m…hard soil","each"]
[null,"Layout and fit poles fully at hole position on site to ensure ease of lifting by hand or crane when planting"]
["C5","Layout and fit poles (by crane) 4 - 7m Conc/Wood","each"]
["C6","Layout and fit pole (by crane) 7 - 13m Conc/Wood","each"]
["C7","Layout and fit poles (by hand) 4 - 7m Conc/Wood","each"]
["C8","Layout and fit pole (by hand) 7 -13m Conc/Wood","each"]
[null,"Erect (Plant) Poles ","D-DT 0050 to 0058"]
["C9","Erect (Plant) poles (by crane) 4 - 7m Conc/Wood","each"]
["C10","Erect (Plant) pole (by crane) 7 - 13m Conc/Wood","each"]
["C11","Erect (Plant) poles (by hand) 4 - 7m Conc/Wood","each"]
["C12","Erect (Plant) pole (by hand) 7 -13m Conc/Wood","each"]
["C13","Assemble Struct. LV Insulators/ABC","each"]
[null,"Assemble and Erect Struts and Stays ","D-DT 0341 to 0343"]
["C14","Assemble and Erect Strut (by hand)","each"]
["C15","Assemble and Erect Strut (by crane)","each"]
["C16","Stays: Make-off  Conventional Stays LV","each"]
["C17","Stays: Make-off  Flying Stays LV","each"]
["C18","Install Conventional Stays & Backfill LV","each"]
["C19","Install Flying Stays & Backfill LV","each"]
[null,"Run out, String, tension, regulate and bind in various conductors (inclusive of hardware and accessories)","D-DT 3136"]
["C20","Run out/ String/tension/regulate bind in LV Bare conductor","m"]
["C21","Run out/ String/binding conductor ABC 35mm","m"]
["C22","Run out/ String/binding conductor ABC 70mm","m"]
["C23","Run out/ String/binding conductor ABC 120mm","m"]
["C24","Making off tail ends in pole top box ABC","each"]
["C25","Making off tail ends on transformer ABC","each"]
["C26","Making off of ABC using IPC","set"]
["C27","Morsdorfer Installation","each"]
["C28","Metering LV Installation","each"]
["C29","Install LV Fuse Unit as per Eskom D-DT0030 assembly drawings. (Accessories inclusive of fuse bracket & mounting hardware, fuse holders amd labels)","set"]
["C30","Repair of ABC (Heat Shrinking) remove and replace IPC’s","each"]
[null,"Install on wooden and/or concrete pole a pole mounted distribution box as specified complete with pole mounting brackets(incl.sealing), cable ties, PG clamps, MCBs, neutral , phase and earth bars, insulated copper tails for connecting to LV ABC, IPCs & factory installed cable openings. Included shall be the stainless steel strapping, buckles and terminations of the tails onto LV ABC. Eskom D-DT standrad as amended will apply","D-DT 3055"]
["C31","BOX,POLE TOP DIST 4-WAY 50A D3055 ","each"]
["C32","BOX,POLE TOP DIST 8-WAY 50A D3055 ","each"]
["C33","BOX,POLE TOP DIST 4-WAY 120A D3055 ","each"]
["C34","BOX,POLE TOP DIST 2-WAY 50A D3055 ","each"]
["C35","BOX,POLE TOP SPLIT METER 2-WAY 50A D3055 ","each"]
["C36","BOX,POLE TOP SPLIT METER 4-WAY 50A D3055 ","each"]
["C37","BOX,POLE TOP SPLIT METER 2-WAY 120A D3055 ","each"]
["C38","BOX,POLE TOP SPLIT METER 8-WAY 50A D3055","each"]
[null,"Earthing at end of run and transformer points of LV line. (include trenching, backfill & compact for earthing, bonding, BIL downwire, spikes and connection thereof)"]
["C39","Trenching ","m"]
["C40","Earthing complete @ structure using galvanized kicker pipes","each"]
["C41","Testing of Transformer earthing (Hoenderpoort)","each"]
[null,"Finishing of various types of structures complete for energising"]
["C42","Finishing of LV Structures  Intermediate","each"]
["C43","Finishing of LV Structures  Suspension","each"]
["C44","Finishing of LV Structures  Strain","each"]
["C45","Finishing of LV Structures  Terminal","each"]
[null,"Dismantling / Removal / Demolish LV Overhead Line hardware & attachments"]
["C46","Loosening/slacking of conductor/Rolling up/cut-up/removal conductor ","phase meter"]
["C47","Disassemble LV insulators/ABC attachment and other line hardware","each"]
["C48","Removal of Poles (backfill holes firmly and normalise site)","each"]
["C49","Transport dismantled items to nearest TSC / collection point as arranged by the Employer.","km"]
[null,"Labelling"]
["C50","Label wood pole number (LV Only)","each"]
["C51","Label pole mounted LV fuse/brkr ","each"]
["C52","Print numbering label onto LV pole top box","each"]
["C53","Identify and label service connections in pole top box","each"]
["C54","Print label to kiosk to on kiosk/stubby door (Red circle background)","each"]
["C55","Identify and label feeder cables (Label at both ends)","each"]
["C56","Identify and label LV service connection cables","each"]
["C57","Identify and label customer meters in LV meterbox/meter room","each"]
[null,"Streetlights"]
["C58","Install / mount  Streetlights","each"]
["C59","Install / mount  Streetlight Control Box","each"]
["C60","Repair of ABC (Heat Shrinking) remove and replace IPC’s (as and when required)","each"]
["C61","Install Photocell","each"]
["C62","Testing of Photocell","each"]
["C63","Making off tail ends in pole top box ABC","each"]
["C64","Making off tail ends on transformer ABC","each"]
["C65","Making off of ABC using IPC","each"]
[null,"Service Connections"]
["C66","Installation only of pre-paid energy dispenser units, including SPU back plate ","each"]
["C67","Connect airdac to breaker (inside pole top box), string airdac to brick built house, drill access hole, fit pigtal and switch on","m"]
["C68","Modification only of Pole Top Boxes (4 way and 8 way) with stainless steel strapping","per pole top box"]
["C69","Morsdorfer Installation","set"]
["C70","Conversion (Removal of existing and replace with proposed) Prepaid Energy Dispensary Units (e.g. 20A replaced by 60A). The obsolete pre-paid ED/EC units remain the property of Eskom)","each"]
["C71","Meter shifting 0- 10 in formal house","each"]
["C72","Excavate cable trenches not exceeding 600mm wide and 1000mm deep in the pickable material.  Including backfilling with excavated material and compact","m"]
["C73","Laying of conductor in excavated trenches","m"]
["C74","Upload of PCS file and completion of application form with meter number, date of installation, GPS co-ordinates of meter (brick built) or transformer (informal dwelling/shack) and other relevant technical information still outstanding on application form","per connection"]
["C75","Connect airdac to breaker (inside pole top box), string airdac to 7m pole, Fit screw-in pigtail on 7m pole, string to informal dwelling/shack, fit screw-in pigtail on informal dwelling/shack, installation of sprig (informal dwelling/shack) and switch on","m"]
["C76","Mount meterbox to 7m pole ","each"]
["C77","Connect service cable to meter per dwelling","each"]
["C78","Secure backing board to the dwelling","each"]
["C79","Mount socket outlet to the backing board (as and when required)","each"]
["C80","Connect socket outlet per dwelling (as and when required)","each"]
["C81","Repair of ABC (Heat Shrinking) remove and replace IPC’s (as and when required)","each"]
["C82","Test installation and provide COC","each"]
["C83","Installation of IPC","each"]
["C84","Installation of split meter complete","each"]
[null,"Metering"]
["C85","Assemble & Erect H-poles  ≥9 meter","each"]
["C86","Install equipment metering units","each"]
["C87","Install equipment: load-break switch ","each"]
["C88","Install equipment: links","each"]
["C89","Install equipment: surge arrestors","each"]
["C90","Testing of metering units","each"]
["C91","Making off tail ends in pole top box ABC","each"]
["C92","Making off tail ends on transformer ABC","each"]
["C93","Making off of ABC using IPC","each"]
[null,"Schools and Clinics"]
["C94","Installation of Meter Box on Transformer Pole","each"]
["C95","Distribution Board surface mounted & wired – 6 Way","each"]
["C96","Distribution Board surface mounted & wired – 8 Way","each"]
["C97","Distribution Board surface mounted & wired – 12 Way","each"]
["C98","Distribution Board surface mounted & wired – 18 Way","each"]
["C99","Distribution Board surface mounted & wired – 30 Way","each"]
["C100","Distribution Board surface mounted & wired – 36 Way","each"]
["C101","Install Pre-paid Meter provided by Eskom","each"]
["C102","Ready Board (Apple / Voltex / York)","each"]
["C103","Heineman SA15A SP  60/100A Earth Leakage Relay","each"]
["C104","Heineman SA1-63 SP  MCB-10A","each"]
["C105","Heineman SA1-63 SP  MCB-20A","each"]
["C106","Heineman SA1-63 SP  MCB-40A","each"]
["C107","Heineman SA1-63 SP  MCB-60A","each"]
["C108","Heineman SA1-63 SP  MCB-80A","each"]
["C109","Heineman SA1-63 SP  MCB-100A","each"]
["C110","60A Single pole isolator","each"]
["C111","1,5m 58W Single flourescent fitting + Light","each"]
["C112","1,5m 58W Double flourescent fitting + Lights","each"]
["C113","100W GLS indoor Bulkhead + Light complete","each"]
["C114","100W GLS outdoor Bulkhead + Light complete","each"]
["C115","10A , 250V National Photo-Cell","each"]
["C116","Single Lever 16A Light Switch surface mounted complete","each"]
["C117","Two Way Switch 16A Light Switch surface mounted complete","each"]
["C118","Master Switch for outside lighting","each"]
["C119","15A Double wall plug surface mounted complete","each"]
["C120","15A Double wall plug surface mounted complete (dedicated supply for computer)","each"]
["C121","2 x 1,5mm2 & earth cable for lights (Surfix)","m"]
["C122","2 x 2,5mm2 & earth cable for plugs (Surfix)","m"]
["C123","2 x 4mm2 & earth cable for geysers (Surfix)","m"]
["C124","2 x 6mm2 & earth cable for stoves (Surfix)","m"]
["C125","1,5mm2 PVC insulated Cu wire for lights (tubed buildings)","m"]
["C126","2,5mm2 PVC insulated Cu wire for plugs (tubed buildings)","m"]
["C127","4mm2 PVC insulated Cu wire for geysers (tubed buildings)","m"]
["C128","6mm2 PVC insulated Cu wire for stoves (tubed buildings)","m"]
["C129","6mm2 PVC insulated Cu earthwire","m"]
["C130","10mm2  3 core SWA cable","m"]
["C131","16mm2  4 core SWA cable","m"]
["C132","25mm2  4 core SWA cable","m"]
["C133","10mm2  3 core concentric cable","m"]
["C134","16mm2  3 core concentric cable","m"]
["C135","Trenching and laying of cable, backfill and compact","m"]
["C136","75 x 50 PVC trunking with snap on cover","m"]
["C137","Wood trusses 114 x 38mm for fixing lights","m"]
["C138","Wooden brandering 38 x 38mm for fixing surfix in roof space","m"]
["C139","P2200 Unistrut 1,5m for fixing lights onto steel trusses","m"]
["C140","Supply and install earthspike complete with copper earth","m"]
["C141","Supply and install PVC tubing","m"]
["C142","Supply and install galvanized pipes","m"]
["C143","Supply and install PVC 3 or 4 way boxes complete","m"]
["C144","Testing of the installation and provision of COC","each"]
["C145","Supply and install school siren","each"]
["C146","Completion of necessary documentation – Form 1-S, Documentation form the Employer to be completed in conjunction with COW and co-signed by the Headmaster/mistress","each"]
[null,"TOTAL (LV WORKS)"]
["D","MV OVERHEAD LINE"]
[null,"Excavate, backfill and compact as per Eskom standard and import backfill soil where required for holes and trenches for poles, stays, flying stays and earth electrodes (all material measured elsewhere)","D-DT 0350, 0342"]
["D1","Excavate Holes Depth:1.5 to 2.0m …soft soil","each"]
["D2","Excavate Holes Depth: > 2.0m ...soft soil","each"]
["D3","Excavate Holes Depth:1.5 to 2.0m….hard soil","each"]
["D4","Excavate Holes Depth: > 2.0m…hard soil","each"]
[null,"Layout and fit poles fully at hole position on site to ensure ease of lifting by hand or crane when planting"]
["D5","Layout and fit poles (by crane) 4 - 7m Conc/Wood","each"]
["D6","Layout and fit pole (by crane) 7 - 13m Conc/Wood","each"]
["D7","Layout and fit poles (by crane) >13m Conc/Wood","each"]
["D8","Layout and fit poles (by crane) H-Pole Wood","each"]
["D9","Layout and fit poles (by crane) Double-Pole Sructure Wood","each"]
["D10","Layout and fit poles (by hand) 4 - 7m Conc/Wood","each"]
["D11","Layout and fit pole (by hand) 7 -13m Conc/Wood","each"]
["D12","Layout and fit poles (by hand) >13m Conc/Wood","each"]
["D13","Layout and fit poles (by hand) H-Pole Wood","each"]
["D14","Layout and fit poles (by hand) Double-Pole Sructure Wood","each"]
[null,"Erect (Plant) Poles ","D-DT 0050 to 0058"]
["D15","Erect (Plant) poles (by crane) 4 - 7m Conc/Wood","each"]
["D16","Erect (Plant) pole (by crane) 7 - 13m Conc/Wood","each"]
["D17","Erect (Plant) poles (by crane) >13m Conc/Wood","each"]
["D18","Erect (Plant) pole (by crane) H-Pole Wood","each"]
["D19","Erect (Plant) poles (by crane) Double-Pole Sructure Wood","each"]
["D20","Erect (Plant) poles (by hand) 4 - 7m Conc/Wood","each"]
["D21","Erect (Plant) pole (by hand) 7 -13m Conc/Wood","each"]
["D22","Erect (Plant) poles (by hand) >13m Conc/Wood","each"]
["D23","Erect (Plant) pole (by hand) H-Pole Wood","each"]
["D24","Erect (Plant) poles (by hand) Double-Pole Sructure Wood","each"]
[null,"Assemble and Erect Struts and Stays ","D-DT 0341 to 0343"]
["D25","Assemble and Erect Strut (by hand)","each"]
["D26","Assemble and Erect Strut (by crane)","each"]
["D27","Stays: Make-off  Conventional Stays","each"]
["D28","Stays: Make-off  Flying Stays","each"]
["D29","Install Conventional Stays & Backfill LV","each"]
["D30","Install Flying Stays & Backfill LV","each"]
[null,"Run out, String, tension, regulate and bind in various conductors (inclusive of hardware and accessories)"]
["D31","Run out/ String/tension/regulate bind in MV Bare conductor (Squirrel, Fox, Mink, Acacia, Pine). Greased or ungreased ","m"]
["D32","Run out/ String/tension/regulate bind in MV Bare conductor (Hare, Oak, 0.5Cu & 0.1Cu). Greased or ungreased ","m"]
["D33","Run out/ String/tension/regulate bind in MV Bare conductor (Chickadee). Greased or ungreased ","m"]
["D34","Extra-over: Installation of bird diverters ","each"]
["D35","Extra-over: Installation of vibration dampers ","each"]
["D36","Run out/ String/binding conductor ABC 35mm (inclusive of all attachments to complete the activity)","m"]
["D37","Run out/ String/binding conductor ABC 70mm (inclusive of all attachments to complete the activity)","m"]
["D38","Run out/ String/binding conductor ABC 120mm (inclusive of all attachments to complete the activity)","m"]
["D39","Making off tail ends in pole top box ABC","each"]
["D40","Making off of ABC using IPC","set"]
["D41","Repair of ABC (Heat Shrinking) remove and replace IPC’s","each"]
[null,"Transformers: (Complete installation include earthing)","D-DT 0420 to 0468 & D-DT 1860 to 1868"]
["D42","11-22kV, and 33kV : 16-100kVA Single / 3 Phase","each"]
["D43","11-22kV, and 33kV : 200kVA - 500kVA","each"]
["D44","11-22kV : 1MVA","each"]
[null,"Equipment: (Complete installation include earthing where required)","D-DT 1821 to 1877"]
["D45","Surge Arrestors                                ","set"]
["D46","Cut-out Fuses Complete (Fused)    (D-WC-6498)","set"]
["D47","Load Break Switch D-DT-1857 and D-DT-1858","each"]
["D48","Ground Mounted Regulators D-WC-6478-20-01-00","set of 2 or 3 CANS"]
["D49","Switched/Fixed Shunt Capacitors    D-WC-6447-20-03-00","set"]
["D50","Voltage Regulator Cans – Elevated   D-WC-7216-20-09-00","set of 2 or 3 CANS"]
["D51","Recloser (complete with control box)  D-WC-7343-20-03-01","each"]
["D52","Pole mounted switch-able units","each"]
[null,"Earthing","D-DT 1821 to 1877"]
["D53","Excavate and backfill trenches 400mm wide x 1000mm deep and lay 10mm round cable and make connections complete","m"]
["D54","Installation of earth spikes.","each"]
[null,"Metering and ancillary cabling from installed transformer"]
["D55","16kVA ( Single Phase)","each"]
["D56","25kVA","each"]
["D57","32kVA","each"]
["D58","50kVA","each"]
["D59","100kVA","each"]
["D60","200kVA","each"]
["D61","500kVA","each"]
["D62","1MVA","each"]
[null,"MV & LV Testing (Allowance for complete testing and commissioning of MV Equipment.  Soil resistance test for equipment to be performed as per Eskom Standard and verified by Eskom's Clerk of Works)"]
["D63","MV Earth Electrode Test","each"]
["D64","Transormer LV Earth Electrode Test","each"]
[null,"Labeling of MV equipment"]
["D65","Label pole mounted Trfr. Number","each"]
["D66","Label mounted device number (Fuse, Switch, Link etc.)","each"]
["D67","Label wood pole","each"]
["D68","Label Voltage Regulator","each"]
["D69","Label to pole mounted recloser/sectionaliser/capacitor/switch-able unit","each"]
[null,"Dismantling / Removal / Demolish MV Overhead Line and Equipment"]
["D70","Demolish existing 11 & 22 kV lines complete and transport to nearest TSC / collection point as arranged by the Employer. ( This item includes loosening/slacking of all conductor/rolling-up/cut-up and removal of conductor; Detaching and removal of hardware; complete removal of poles and normalise site)","linear m \n(i.e. running all 3 phases)"]
[null,"Removal of Pole Mounted  & Ground Mounted Transformers/Minisubs :"]
["D71","16kVA-100kVA Pole Mounted Transformer","each"]
["D72",">100-315kVA Pole Mounted Transformer","each"]
["D73","500kVA Pole Mounted Transformer","each"]
["D74","200 to 315kVA Minisub","each"]
["D75","500kVA Minisub","each"]
["D76","1MVA Minisub or Ground Mounted transformer","each"]
[null,"Removal of other equipment :"]
["D77","Voltage Regulators  (3-CAN)","set "]
["D78","Voltage Regulators  (2-CAN)","set "]
["D79","Auto-reclosers with control box / Sectionalisers / Switched or Shunt Capacitors","each"]
["D80","LPU Metering Units","each"]
["D81","Load Break Switch","each"]
["D82","MV links / Isolators","each"]
["D83","Surge Arrestors                                ","set of 3"]
["D84","MV Fuses","set of 3"]
["D85","Remove all types of equipment plinths and dispose thereof at a registered dumping site","each"]
[null,"TOTAL (MV OVERHEAD LINE)"]
["E","MV UNDERGROUND CABLE"]
["E1","Excavate, backfill and compact trenches 1.0m deep x 500mm wide for cables in pickable materials (soft) by hand (including laying of \"danger tape')","m"]
["E2","Excavate, backfill and compact trenches 1.0m deep x 500mm wide for cables in hard materials by hand. (including laying of \"danger tape')","m"]
["E3","Excavate, backfill and compact trenches 1.0m deep x 500mm wide for cables in all materials by machine.(including laying of \"danger tape')","m"]
[null,"laying of Pipes"]
["E4","Supply and lay PVC Pipe (110mm)","m"]
["E5","Supply and lay PVC Pipe (160mm)","m"]
["E6","Supply and lay HDPE Pipe (110mm)","m"]
["E7","Supply and lay HDPE Pipe (160mm)","m"]
[null,"Cable Laying / Termination"]
["E8","Laying of 16-35mm sq LV cable","m"]
["E9","Terminate / Join 16/35mm LV cables","each"]
["E10","Laying of 70-95mm sq LV cable","m"]
["E11","Terminate / Join 70/95mm LV cables","each"]
["E12","Laying of 120mm sq LV cable","m"]
["E13","Terminate / Join 120 LV cables","each"]
["E14","Laying of 25mm sq MV Cable","m"]
["E15","Terminate / Join 25mm sq MV cables","each"]
["E16","Laying of 95mm sq MV Cable","m"]
["E17","Terminate / Join 95mm sq MV cables","each"]
["E18","Laying of 185mm sq MV Cable","m"]
["E19","Terminate / Join 185mm MV cables","each"]
["E20","Laying of 300mm sq Alu MV Cable","m"]
["E21","Terminate / Join 300mm sq Alu MV cables","each"]
["E22","Laying of 630mm sq single-core MV Cable","m"]
["E23","Terminate / Join 630mm sq single-core MV cables","each"]
["E24","MV Cable pressure test","each"]
["E25","Earthing of MV cables","each"]
["E26","Supply and install concrete slab as cable cover  (as per Eskom specification)","each"]
[null,"Supply and installation of plinths for:"]
["E27","Ring Main Units (RMU) D-DT-0863 set 6 pages 1-6","each"]
["E28","Mini Sub Type “A” =< 500kVA  D-DT-0859 set 7 pages 1-2","each"]
["E29","Mini Sub Type “A” = 1000kVA  D-DT-0859 set 7 pages 3-4","each"]
["E30","Mini Sub Type “B” Front Entry Cable  D-DT-0859 set 7 page 6","each"]
["E31","Mini Sub Type “B” Side Entry Cable   D-DT-0859 set 7 page 5","each"]
["E32","LPU metering (CT/VT unit)  D-DT-0861 Set 2 sheets 1-2","each"]
["E33","CW1 Cubical D-DT-1010 Set 2 Sheets 1-2 or similar metering kiosk","each"]
["E34","Stubby Kiosk base complete","each"]
[null,"Installation of equipment:"]
["E35","RMU inclusive of labeling","each"]
["E36","Mini Sub Type “A” inclusive of labeling","each"]
["E37","Mini Sub Type “B” inclusive of labeling","each"]
["E38","LPU metering unit inclusive of labeling","each"]
["E39","CW1  Cubical D-DT-1010 Set 2 Sheets 1-2 or similar metering kiosk (inclusive of labelling)","each"]
["E40","Stubby Kiosk base complete","each"]
[null,"Dismantling / Removal / Demolish MV Cable and Equipment"]
[null,"Removal of Minisubs/RMUs etc :"]
["E41","Ring Main Units (RMU)","each"]
["E42","Mini Sub Type “A” =< 500kVA  ","each"]
["E43","Mini Sub Type “A” = 1000kVA ","each"]
["E44","Mini Sub Type “B” Front Entry Cable  ","each"]
["E45","Mini Sub Type “B” Side Entry Cable   ","each"]
["E46","LPU metering (CT/VT unit)  ","each"]
["E47","CW1 Cubical  or similar metering kiosk","each"]
[null,"Removal of MV Cable (inclusive of Excavations, Rolling-up of cable and backfill & compact trench (normalise site)"]
["E48","Removal of 4-core cable","m"]
["E49","Removal of 25 to 70mm sq 3-core MV cable","m"]
["E50","Removal of 95 to 185mm sq 3-core MV cable","m"]
["E51","Removal of =>300mm sq 3-core MV cable","m"]
["E52","Removal of 630mm sq single-core MV Cable","m"]
[null,"TOTAL (MV UNDERGROUND CABLE)"]
["F","RE-INSTATEMENT"]
[null,"Trench Re-instatement"]
["F1","Light duty road-way (Trench = 0.5-1m wide, 150mm base + 25mm premix)","m"]
["F2","Footway (Trench = 0.5-1m wide, 75mm base + 25mm premix)","m"]
["F3","Footway (Trench = 0.1-1.5m wide, 75mm base + 25mm premix)","m"]
["F4","Heavy duty road-way (Trench = 0.5-1m wide, 225mm base + 40mm premix)","m"]
["F5","Brick paving (labour only)","m²"]
["F6","Concrete paving (labour only)","m²"]
["F7","Kerb (labour only)","m"]
["F8","Channel (labour only)","m"]
["F9","Clear site and take away rubble to nearest dumping site","m³\n"]
["F10","Saw cutting","m"]
["F11","Excavate trenches for layerworks","m³\n"]
[null,"General "]
["F12","Traffic Control","per day"]
[null,"TOTAL (RE-INSTATEMENT)"]
["G","THRUSTBORING"]
[null,"(The items include all labour, plant, material and equipment required to install cable ducting by thrust-boring ducts under existing roadways and surfaced areas.  Also to include transport within 100km radius from Brackenfell office)"]
[null,"Soil Conditions: Normal pickable"]
[null,"Install Cable Ducts -  Supply, join & install the following sizes of PVC cable ducting under raods and surfaced areas by thrust-boring :"]
["G1","160mm diameter PVC duct","m"]
["G2","110mm diameter PVC duct","m"]
["G3","75mm diameter PVC duct","m"]
["G4","63mm diameter PVC duct","m"]
[null,"Install Cable Ducts -  Supply, weld & install the following sizes of HDPE cable ducting under raods and surfaced areas by thrust-boring :"]
["G5","160mm diameter HDPE duct","m"]
["G6","110mm diameter HDPE duct","m"]
["G7","75mm diameter HDPE duct","m"]
["G8","63mm diameter HDPE duct","m"]
[null,"Soil Conditions: Intermediate"]
[null,"Install Cable Ducts -  Supply, join & install the following sizes of PVC cable ducting under raods and surfaced areas by thrust-boring :"]
["G9","160mm diameter PVC duct","m"]
["G10","110mm diameter PVC duct","m"]
["G11","75mm diameter PVC duct","m"]
["G12","63mm diameter PVC duct","m"]
[null,"Install Cable Ducts -  Supply, weld & install the following sizes of HDPE cable ducting under raods and surfaced areas by thrust-boring :"]
["G13","160mm diameter HDPE duct","m"]
["G14","110mm diameter HDPE duct","m"]
["G15","75mm diameter HDPE duct","m"]
["G16","63mm diameter HDPE duct","m"]
[null,"Soil Conditions: Heavy/Rocky"]
[null,"Install Cable Ducts -  Supply, join & install the following sizes of PVC cable ducting under raods and surfaced areas by thrust-boring :"]
["G17","160mm diameter PVC duct","m"]
["G18","110mm diameter PVC duct","m"]
["G19","75mm diameter PVC duct","m"]
["G20","63mm diameter PVC duct","m"]
[null,"Install Cable Ducts -  Supply, weld & install the following sizes of HDPE cable ducting under raods and surfaced areas by thrust-boring :"]
["G21","160mm diameter HDPE duct","m"]
["G22","110mm diameter HDPE duct","m"]
["G23","75mm diameter HDPE duct","m"]
["G24","63mm diameter HDPE duct","m"]
[null,"Transport Rate"]
["G25","Travelling Rate (from base stated in contract)","km"]
[null,"TOTAL (THRUSTBORING)"]

{"sheet":"3.TO Process","index":1,"n_rows":44,"n_cols":20,"rows_kept":44,"merged":[[1,0,1,7],[2,0,2,7],[3,1,3,5],[4,1,4,5],[4,6,12,6],[4,7,12,7],[5,1,5,5],[13,1,13,5],[14,1,14,5],[15,1,15,5],[16,1,16,5],[17,1,17,5],[18,1,18,5],[19,1,19,5],[20,1,20,5],[21,1,21,5],[22,1,22,5],[26,0,26,2],[26,4,26,7],[31,5,32,5],[31,7,32,7],[33,5,33,7],[35,4,36,4],[35,5,36,5],[35,6,36,6],[35,7,36,7],[37,7,39,7],[38,4,39,4],[38,5,39,5],[38,6,39,6],[40,4,41,4],[40,5,41,5],[40,6,41,6],[40,7,41,7],[43,5,43,6]]}
[]
[{"$f":"#REF!","v":{"$error":"#REF!"}}]
["TASK ORDER PROCESS "]
[null,"ACTIVITY",{"$nulls":4},"RESPONSIBLE PERSON","DURATION (working days)  "]
[1,"Project Co-ordinator or other Requestor requests QS for work to be completed via this contract ",{"$nulls":4},"PC / Requestor","As per request",{"$nulls":11},0.1]
[null,"The below mentioned info is required to be populated on task order: ",{"$nulls":17},0]
[null,null,"-      Project Name, Project Number ",{"$nulls":16},0.025]
[null,null,"-      The Task START and COMPLETION Date",{"$nulls":16},0]
[null,null,"-      The Scope of Works"]
[null,null,"-          Project ID and job no with WBS No as noted on SAP for cost payment"]
[null,null,"-          The requestor should state the contact person "]
[null,null,"-          SAP ID of Requestor"]
[null,null,"-          PC requests Contractor to complete all relevant \"REQUIREMENTS for CONSTRUCTION COMPLIANCE\" "]
[2,"PC to arrange a site meeting with the contractor, after sending the BOQ and drawings to the contractor at least  4 days  before the site meeting.",{"$nulls":4},"PC& QS","5 days"]
[3," When all required information is received the QS populates the information on the task order and forwards it to the respective \"Contracts Administrator\" for 45 number creation.",{"$nulls":4},"QS incl Contracts Administrator","3 days"]
[4,"The PC should be copied at all times for any communication regarding the request",{"$nulls":4},"Strict Adherence by all"]
[5,"Once 45 numbers created, the QS insert the 45 number on the task order and forward as a PDF document to the PC and the Contractor",{"$nulls":4},"QS","2 days"]
[6,"Once the task order work is completed the Contractor sends the task order to the Requestor/PC for signatures or confirmation that the PC agrees with the work completed.",{"$nulls":4},"Contractor","2 day"]
[null,"MODIFICATIONS"]
[7,"Should there be changes in design etc to the Task Order, the PC signs for changes and forward it to the QS to modify the task order after Task Order Committee (TOC) approval.",{"$nulls":4},"PC ","2 days"]
[8,"QS sends a request for modification to the Contracts Administrator to load the changes on SAP as shown on the task order.",{"$nulls":4},"QS incl Contracts Administrator","3 days"]
[9,"PC and Contractor signs off the revised Task Order to include approved Modifications",{"$nulls":4},"PC & Contractor","2 days"]
[]
["Note: Minor Works Process to be followed when minor work projects are executed"]
[]
[]
["TASK ORDER APPROVAL PROCESS ",{"$nulls":3},"PAYMENT PROCESS "]
[null,"ACTIVITY","DESCRIPTION",null,null,"ACTIVITY","RESPONSIBLE PERSON","DURATION (working days)  "]
[]
[1,"Submissions to TOC","PC to fully complete and submit the TO Request Form, requesting for a TOC Meeting/Approval",null,1,"On completion of the task order activities as per Milestone, the Contractor to forward Assessment/Task Order assesment of work that was done to Project Co-ordinator (PC) and Clerk of works","Contractor","On completion "]
[2,"Estimate","at TOC meeting we approve in concept and allocate a contractor",null,2,"PC,Clerk of works together with the Contractor agrees to the Task Order Assessment.","PC ,COW and Contractor","1 day"]
[3,"Quote","Quote approved at TOC Meeting",null,3,"PC will then submit the verified signed-off Task order Assessment to the relevant Quantity Surveyor (QS) to  create  a Payment Certificate","PC ","Included in item 2"]
[4,"Re-Quote","A revised quote to be completed by Contractor if TOC request to do so (PC to co-ordinate)"]
[5,"PC to finalise","PC to inform and submit revised Task Order to QS that all decisions at meeting is finalised ",null,null,"NOTE: MODIFICATIONS/CHANGES TO THE ORIGINAL TASK ORDER HAVE TO BE INCLUDED IN THE ASSESSMENT"]
[6,"45-number","Quotation approval at Meeting/adhoc and allows 45-number to be created by Project Controller",null,4,"The QS verifies the claim against the original task order and; \n- send a request to the Contracts Administrator to do the modification in SAP \n- creates the Payment Certificate ","Quantity Surveyor & Contracts administrator","3 days "]
[7,"TO Update","QS to update Task Order and PC to sign together with Contractor to formalise Contract",null,5,"QS prepares a payment certificate  and send the Payment Certificate and the task order assesment to the Project Co-Ordinator to sign it. PC to  send a signed payment certificate and the task order assesment to the  Project Controller to create a Service entry number. ","QS,PC and Project controller","3 days "]
[8,"Modifications","PC to inform QS timeously of any modifications to be submitted to TO Committee"]
[9,"Modification Approval","QS to check modifications for correctness before submission to the TO Committee",null,6,"The Project Controller to process  and create the Service Entry (SE) number and notifies the PC to release the Good Receipt  (GR) number starting with a 50……","Project Controller","2 days "]
[10,"TO MOD Update","QS to update MODS on Task Order as approved by Committee",null,7,"Thereafter, the  PC will populate  the Service Entry (SE) number and Good Receipt (GR) number on the Payment Certificate and sent to the Contractor .","PC"]
[11,"MODS loaded on SAP","Modifications to be loaded on SAP by the Project Controller"]
[12,"Payments ","Payments made on completion of works as informed by PC/COW",null,8,"Once the Contractor has received the payment certificate with the SE and GR number, he will generate the invoice and sign the Payment Certificate and send back a copies to the PC. The invoice and fully signed Payment Certificate will thereafter be submitted by the Contractor directly to Eskom Shared Services via email","Contractor","Complete "]
[13,"Cancellations/Terminations","All Task Order cancellations or Terminations to be ratified by Task Order Committee"]
[]
[{"$nulls":5},"NOTE:   All Modifications will require Task Order Committee (TOC) Approval"]

{"sheet":"Sheet","index":2,"n_rows":14,"n_cols":3,"rows_kept":14,"hidden":true}
[]
[]
[]
[]
[]
[null,"Selection of Drop Down for \"Contractor PA\""]
[]
[null,"Y",0]
[null,"N",1]
[null,null,2]
[null,null,3]
[null,null,4]
[null,null,5]
[null,null,6]