{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["PSC254-BF-TBOQ1"],"not_rendered":{"defined_names":1,"comments":2},"read":"whole","date_system":"1900"}

{"sheet":"PSC254-BF-TBOQ1","index":0,"n_rows":1108,"n_cols":12,"rows_kept":1108}
["COUNTER","ISC","SECTION","BILL","PAGE NO","ITEM NO",{"$nulls":3},"QUANTITY","RATE","AMOUNT"]
[1,115,1,1,1,null,"SECTION NO. 1"]
[]
[2,686,1,1,1,null,"BILL NO. 1"]
[]
[3,33,1,1,1,"C1.2","GENERAL REQUIREMENTS AND PROVISIONS"]
[]
[{"$nulls":5},"C1.2.5.1","Health and Safety Plan",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"J8*K8","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C1.2.5.2","Implementation of health and safety plan                             ",null,"month",{"v":10,"d":"10 "},null,{"$f":"J10*K10","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.2.5.3","Provision of full time Construction Safety Officer               ",null,"month",{"v":10,"d":"10 "},null,{"$f":"J12*K12","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.2.5.4","Submission of the Health and Safety File                                ",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"J14*K14","v":{"v":0,"d":"0.00"}}]
[]
[5,914,1,1,1,"PC1.2.10","Standing time (Plant and Labour)"]
[]
[6,915,1,1,1,null,"(a) Asphalt milling team",null,"hr",null,null,"Rate Only"]
[]
[7,916,1,1,1,null,"(b) Asphalt paving team",null,"hr",null,null,"Rate Only"]
[]
[8,917,1,1,1,null,"(c) Runway marking team",null,"hr",null,null,"Rate Only"]
[]
[9,918,1,1,1,null,"(d) Earthwork team",null,"hr",null,null,"Rate Only"]
[]
[10,919,1,1,1,null,"(e) Electrical team",null,"hr",null,null,"Rate Only"]
[]
[11,920,1,1,1,"PC1.2.11","Airside induction courses and permits",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"J28*K28","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(a) Actual cost for attaining permits",null,"PS",{"v":1,"d":"1 "},{"v":0,"d":"0.00"},{"$f":"J30*K30","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(b) Contractors charge in respect of item C1.2.11 (a) above",null,"%",{"v":0.05,"d":"5.00%"},{"$f":"L30","v":{"v":0,"d":"0.00"}},{"$f":"J32*K32","v":{"v":0,"d":"0.00"}}]
[]
[13,116,1,2,2,null,"SECTION NO. 1"]
[]
[14,687,1,2,2,null,"BILL NO. 2"]
[]
[15,102,1,2,2,"C1.3 ","CONTRACTOR'S SITE ESTABLISHMENT AND GENERAL OBLIGATIONS"]
[]
[{"$nulls":5},"C1.3.1 ","The Contractor's general obligations"]
[]
[{"$nulls":5},"C1.3.1.1 ","Fixed obligations",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"J42*K42","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C1.3.1.2 ","Value-related obligations",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"J44*K44","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C1.3.1.3 ","Time-related obligations",null,"month",{"v":10,"d":"10 "},null,{"$f":"J46*K46","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(a) Mobilisation period",null,"month"]
[]
[16,109,1,2,2,"PC1.3.1.4","Suspension Cost"]
[]
[17,110,1,2,2,null,"(a) De-establishment",null,"No",{"v":1,"d":"1 "},null,{"$f":"J52*K52","v":{"v":0,"d":"0.00"}}]
[]
[18,111,1,2,2,null,"(b) Re-establishment",null,"No",{"v":1,"d":"1 "},null,{"$f":"J54*K54","v":{"v":0,"d":"0.00"}}]
[]
[19,112,1,2,2,null,"(c) Suspension period",null,"month",{"v":3,"d":"3 "},null,{"$f":"J56*K56","v":{"v":0,"d":"0.00"}}]
[]
[20,113,1,2,2,null,"(d) Engineer's cost",null,"PC Sum",{"v":1,"d":"1 "},null,{"$f":"J58*K58","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C1.3.2","Contract sign boards",null,"m2",{"v":9.6,"d":"10 "},null,{"$f":"J60*K60","v":{"v":0,"d":"0.00"}}]
[]
[22,217,1,3,3,null,"SECTION NO. 1"]
[]
[23,688,1,3,3,null,"BILL NO. 3"]
[]
[24,117,1,3,3,"C1.4","FACILITIES FOR THE ENGINEER"]
[]
[25,118,1,3,3,"C1.4.1 ","Site accommodation"]
[]
[26,119,1,3,3,"C1.4.1.1","Offices and conference room",null,"m²",{"v":40,"d":"40 "},null,{"$f":"J70*K70","v":{"v":0,"d":"0.00"}}]
[]
[27,120,1,3,3,"C1.4.1.2","Laboratories",null,"m²",null,null,"Rate Only"]
[]
[28,121,1,3,3,"C1.4.1.3","Open concrete working floors and verandas",null,"m²",null,null,"Rate Only"]
[]
[29,122,1,3,3,"C1.4.1.4","Roofs over open concrete working floors and verandas",null,"m²",null,null,"Rate Only"]
[]
[30,123,1,3,3,"C1.4.1.5","Store rooms inside the laboratory",null,"m²",null,null,"Rate Only"]
[]
[31,124,1,3,3,"C1.4.1.6","Car ports",null,"No",{"v":4,"d":"4 "},null,{"$f":"J80*K80","v":{"v":0,"d":"0.00"}}]
[]
[32,125,1,3,3,"C1.4.1.7","Ablution unit (equipped as specified)",null,"No",{"v":5,"d":"5 "},null,{"$f":"J82*K82","v":{"v":0,"d":"0.00"}}]
[]
[33,126,1,3,3,"C1.4.1.8","Change room with a shower",null,"No",null,null,"Rate Only"]
[]
[34,127,1,3,3,"C1.4.1.9","Kitchen unit (equipped as specified)",null,"No",{"v":1,"d":"1 "},null,{"$f":"J86*K86","v":{"v":0,"d":"0.00"}}]
[]
[35,128,1,3,3,"C1.4.1.10","Type A prefabricated house (equipped as specified)",null,"No",{"v":0,"d":"0 "},null,{"$f":"J88*K88","v":{"v":0,"d":"0.00"}}]
[]
[36,129,1,3,3,"C1.4.1.11","Type B prefabricated house (equipped as specified)",null,"No",{"v":0,"d":"0 "},null,{"$f":"J90*K90","v":{"v":0,"d":"0.00"}}]
[]
[37,130,1,3,3,"C1.4.1.12","Type C prefabricated house (equipped as specified)",null,"No",{"v":0,"d":"0 "},null,{"$f":"J92*K92","v":{"v":0,"d":"0.00"}}]
[]
[38,131,1,3,3,"C1.4.1.13","Rented housing paid for by the Contractor",null,"Prov Sum",{"v":1,"d":"1 "},{"$f":"4*10000*10","v":{"v":400000,"d":"400,000.00"}},{"$f":"J94*K94","v":{"v":400000,"d":"400,000.00"}}]
[]
[39,132,1,3,3,"C1.4.1.14","Contractor's handling costs, profit and all other charges in respect of item C1.4.1.13",null,"%",{"v":0.1,"d":"10%"},{"$f":"SUM(L94:L95)","v":{"v":400000,"d":"400,000.00"}},{"$f":"ROUND(J96*K96,2)","v":{"v":40000,"d":"40,000.00"}}]
[]
[40,133,1,3,3,"C1.4.2","Items measured by area"]
[]
[41,134,1,3,3,"C1.4.2.1","Shelving as specified, complete with brackets",null,"m²",{"v":6,"d":"6 "},null,{"$f":"ROUND(J100*K100,2)","v":{"v":0,"d":"0.00"}}]
[]
[42,135,1,3,3,"C1.4.2.2","Work benches with a concrete slab top",null,"m²",null,null,"Rate Only"]
[]
[43,136,1,3,4,"C1.4.2.3","Work-benches with a wooden top",null,"m²",null,null,"Rate Only"]
[]
[44,137,1,3,4,"C1.4.2.4","Constant-temperature baths of concrete and/or plastered brick",null,"m²",null,null,"Rate Only"]
[]
[45,138,1,3,4,"C1.4.2.5","Concrete footings and pedestals for laboratory equipment",null,"m²",null,null,"Rate Only"]
[]
[46,139,1,3,4,"C1.4.2.6","Roller blinds, opaque type",null,"m²",null,null,"Rate Only"]
[]
[47,140,1,3,4,"C1.4.2.7","Venetian blinds",null,"m²",{"v":8,"d":"8 "},null,{"$f":"ROUND(J112*K112,2)","v":{"v":0,"d":"0.00"}}]
[]
[48,141,1,3,4,"C1.4.2.8","Notice boards",null,"m²",{"v":3,"d":"3 "},null,{"$f":"ROUND(J114*K114,2)","v":{"v":0,"d":"0.00"}}]
[]
[49,142,1,3,4,"C1.4.2.9","White boards",null,"m²",null,null,"Rate Only"]
[]
[50,143,1,3,4,"C1.4.2.10","Galvanised wire mesh fencing for store rooms",null,"m²",null,null,"Rate Only"]
[]
[51,144,1,3,4,"C1.4.2.11","Galvanised wire mesh store room gate with a padlock",null,"m²",null,null,"Rate Only"]
[]
[52,145,1,3,4,"C1.4.3","Items measured by number"]
[]
[53,146,1,3,4,"C1.4.3.1","Office swivel chair",null,"No",null,null,"Rate Only"]
[]
[54,147,1,3,4,"C1.4.3.2","Office chair",null,"No",{"v":12,"d":"12 "},null,{"$f":"ROUND(J126*K126,2)","v":{"v":0,"d":"0.00"}}]
[]
[55,148,1,3,4,"C1.4.3.3","Draughtsman's stool",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J128*K128,2)","v":{"v":0,"d":"0.00"}}]
[]
[56,149,1,3,4,"C1.4.3.4","Laboratory high chair",null,"No",null,null,"Rate Only"]
[]
[57,150,1,3,4,"C1.4.3.5","Office desk with 3 drawers (at least one lockable drawer)",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J132*K132,2)","v":{"v":0,"d":"0.00"}}]
[]
[58,151,1,3,4,"C1.4.3.6","Typist desk (L-shaped)",null,"No",null,null,"Rate Only"]
[]
[59,152,1,3,4,"C1.4.3.7","Drawing table",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J136*K136,2)","v":{"v":0,"d":"0.00"}}]
[]
[60,153,1,3,4,"C1.4.3.8","Conference table",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J138*K138,2)","v":{"v":0,"d":"0.00"}}]
[]
[61,154,1,3,4,"C1.4.3.9","Bookcase",null,"No",null,null,"Rate Only"]
[]
[62,155,1,3,4,"C1.4.3.10","Filing cabinet",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J142*K142,2)","v":{"v":0,"d":"0.00"}}]
[]
[63,156,1,3,4,"C1.4.3.11","General purpose steel cabinet with shelves",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J144*K144,2)","v":{"v":0,"d":"0.00"}}]
[]
[64,157,1,3,4,"C1.4.3.12","Wall mounted pivot plan filing system",null,"No",null,null,"Rate Only"]
[]
[65,158,1,3,5,"C1.4.3.13","220/250 volt power outlet plug point",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J148*K148,2)","v":{"v":0,"d":"0.00"}}]
[]
[66,159,1,3,5,"C1.4.3.14","400/231 volt 3-phase power outlet plug point",null,"No",null,null,"Rate Only"]
[]
[67,160,1,3,5,"C1.4.3.15","Single 1500m, 58 watt fluorescent tube ceiling light",null,"No",{"v":6,"d":"6 "},null,{"$f":"ROUND(J152*K152,2)","v":{"v":0,"d":"0.00"}}]
[]
[68,161,1,3,5,"C1.4.3.16","Single 1500mm, 22 watt LED tube ceiling light",null,"No",null,null,"Rate Only"]
[]
[69,162,1,3,5,"C1.4.3.17","11 watt compact fluorescent bulb ceiling light",null,"No",null,null,"Rate Only"]
[]
[70,163,1,3,5,"C1.4.3.18","7 watt LED bulb ceiling light",null,"No",null,null,"Rate Only"]
[]
[71,164,1,3,5,"C1.4.3.19","Wash-hand basin",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J160*K160,2)","v":{"v":0,"d":"0.00"}}]
[]
[72,165,1,3,5,"C1.4.3.20","Laboratory basin",null,"No",null,null,"Rate Only"]
[]
[73,166,1,3,5,"C1.4.3.21","Extractor fan",null,"No",null,null,"Rate Only"]
[]
[74,167,1,3,5,"C1.4.3.22","Fume cupboard",null,"No",null,null,"Rate Only"]
[]
[75,168,1,3,5,"C1.4.3.23","Fire extinguisher 9,0 kg, dry powder type",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J168*K168,2)","v":{"v":0,"d":"0.00"}}]
[]
[76,169,1,3,5,"C1.4.3.24","Air-conditioning unit",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J170*K170,2)","v":{"v":0,"d":"0.00"}}]
[]
[77,170,1,3,5,"C1.4.3.25","Heater",null,"No",null,null,"Rate Only"]
[]
[78,171,1,3,5,"C1.4.3.26","Concrete specimen curing bath",null,"No",null,null,"Rate Only"]
[]
[79,172,1,3,5,"C1.4.3.27","Waste paper basket",null,"No",null,null,"Rate Only"]
[]
[80,173,1,3,5,"C1.4.3.28","UPS / Voltage stabiliser (2kVa)",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J178*K178,2)","v":{"v":0,"d":"0.00"}}]
[]
[81,174,1,3,5,"C1.4.3.29","A3 / A4 colour printer, copier, scanner",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J180*K180,2)","v":{"v":0,"d":"0.00"}}]
[]
[82,175,1,3,5,"C1.4.3.30","A4 colour printer, copier, scanner",null,"No",null,null,"Rate Only"]
[]
[83,176,1,3,5,"C1.4.3.31","Rain gauge",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J184*K184,2)","v":{"v":0,"d":"0.00"}}]
[]
[84,177,1,3,5,"C1.4.3.32","Minimum/maximum atmospheric temperature gauge",null,"No",null,null,"Rate Only"]
[]
[85,178,1,3,5,"C1.4.3.33","Digital thermometer",null,"No",null,null,"Rate Only"]
[]
[86,179,1,3,5,"C1.4.3.34","Mobile outdoor weather station",null,"No",null,null,"Rate Only"]
[]
[87,180,1,3,5,"C1.4.3.35","3,0m aluminium straight edge complete with two measuring wedges",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J192*K192,2)","v":{"v":0,"d":"0.00"}}]
[]
[88,181,1,3,6,"C1.4.3.36","Measuring wheel",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J194*K194,2)","v":{"v":0,"d":"0.00"}}]
[]
[89,182,1,3,6,"C1.4.3.37","First aid kit",null,"No",{"v":3,"d":"3 "},null,{"$f":"ROUND(J196*K196,2)","v":{"v":0,"d":"0.00"}}]
[]
[90,183,1,3,6,"C1.4.3.38","Standpipe complete with 30m of 19mm dia. heavy duty hose pipe",null,"No",null,null,"Rate Only"]
[]
[{"$nulls":5},"PC1.4.3.39","ACSA approved lime coloured reflective safety  jackets (With lettering)",null,"No",{"v":12,"d":"12 "},null,{"$f":"ROUND(J200*K200,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.4.3.40","Rechargeable 500 000 candlelight halogen lamps",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J202*K202,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.4.3.41","Two-way hand held radio VHF/AM Dittel FSG5 complete with charger, carrying bag with strap and vehicle magnetic antenna including adapter cable",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J204*K204,2)","v":{"v":0,"d":"0.00"}}]
[]
[91,184,1,3,6,"C1.4.4","Prime cost items"]
[]
[92,185,1,3,6,"C1.4.4.1","Cell phones costs, including pro-rata rentals, for calls made in connection with contract administration",null,"PC Sum",{"v":1,"d":"1 "},{"v":35000,"d":"35,000.00"},{"$f":"ROUND(J208*K208,2)","v":{"v":35000,"d":"35,000.00"}}]
[]
[93,186,1,3,6,"C1.4.4.2","Handling costs and profit in respect of item C1.4.4.1",null,"%",{"v":0.1,"d":"10%"},{"$f":"L208","v":{"v":35000,"d":"35,000.00"}},{"$f":"ROUND(J210*K210,2)","v":{"v":3500,"d":"3,500.00"}}]
[]
[94,187,1,3,6,"C1.4.4.3","The provision of a direct independent telephone line for the Engineer, including the monthly rental charges and the cost of business calls",null,"PC Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J212*K212,2)","v":{"v":0,"d":"0.00"}}]
[]
[95,188,1,3,6,"C1.4.4.4","Handling costs and profit in respect of item C1.4.4.3",null,"%",{"v":0,"d":"0%"},null,{"$f":"ROUND(J214*K214,2)","v":{"v":0,"d":"0.00"}}]
[]
[96,189,1,3,6,"C1.4.4.5","The provision of internet connectivity and WiFi data for Engineer\"€™s site staff",null,"PC Sum",{"v":1,"d":"1 "},{"$f":"800*10","v":{"v":8000,"d":"8,000.00"}},{"$f":"ROUND(J216*K216,2)","v":{"v":8000,"d":"8,000.00"}}]
[]
[97,190,1,3,6,"C1.4.4.6","Handling costs and profit in respect of item C1.4.4.5",null,"%",{"v":0.1,"d":"10%"},{"$f":"L216","v":{"v":8000,"d":"8,000.00"}},{"$f":"ROUND(J218*K218,2)","v":{"v":800,"d":"800.00"}}]
[]
[98,191,1,3,6,"C1.4.4.7","The provision of paper and ink for a combination colour printer/copier/scanner",null,"PC Sum",{"v":1,"d":"1 "},{"v":7500,"d":"7,500.00"},{"$f":"ROUND(J220*K220,2)","v":{"v":7500,"d":"7,500.00"}}]
[]
[99,192,1,3,6,"C1.4.4.8","Handling costs and profit in respect of item C1.4.4.7",null,"%",{"v":0.1,"d":"10%"},{"$f":"L220","v":{"v":7500,"d":"7,500.00"}},{"$f":"ROUND(J222*K222,2)","v":{"v":750,"d":"750.00"}}]
[]
[100,193,1,3,6,"C1.4.4.9","The provision of a complete 220/250 volt single phase electrical power installation, including all poles, insulators, wiring, switchboards, mains connections, meters etc.",null,"PC Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J224*K224,2)","v":{"v":0,"d":"0.00"}}]
[]
[101,194,1,3,6,"C1.4.4.10","Handling costs and profit in respect of item C1.4.4.9",null,"%",{"v":0,"d":"0%"},null,{"$f":"ROUND(J226*K226,2)","v":{"v":0,"d":"0.00"}}]
[]
[102,195,1,3,6,"C1.4.4.11","The provision of a complete 440/231 volt three phase electrical power installation, including all poles, insulators, wiring, switchboards, mains connections, meters etc.",null,"No",null,null,"Rate Only"]
[]
[103,196,1,3,7,"C1.4.4.12","Handling costs and profit in respect of item C1.4.4.11",null,"%",{"v":0,"d":"0%"},null,{"$f":"ROUND(J230*K230,2)","v":{"v":0,"d":"0.00"}}]
[]
[104,197,1,3,7,"C1.4.4.13","Provision of a 25 kVA volt three phase electricity generator if electricity from a power supply authority is not available on site",null,"PC Sum",{"v":1,"d":"1 "},{"v":65000,"d":"65,000.00"},{"$f":"ROUND(J232*K232,2)","v":{"v":65000,"d":"65,000.00"}}]
[]
[105,198,1,3,7,"C1.4.4.14","Handling costs and profit in respect of item C1.4.4.13",null,"%",{"v":0.1,"d":"10%"},null,{"$f":"ROUND(J234*K234,2)","v":{"v":0,"d":"0.00"}}]
[]
[106,199,1,3,7,"C1.4.4.15","The provision of all gas installations required at the site offices, laboratories and at the Engineer\"€™s staff accommodation (if required), including gas storage cylinders, tubing, regulators, gas burners and shut-off cocks",null,"PC Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J236*K236,2)","v":{"v":0,"d":"0.00"}}]
[]
[107,200,1,3,7,"C1.4.4.16","Handling costs and profit in respect of item C1.4.4.15",null,"%",{"v":0,"d":"0%"},null,{"$f":"ROUND(J238*K238,2)","v":{"v":0,"d":"0.00"}}]
[]
[108,201,1,3,7,"C1.4.5","Services at site offices, laboratories and site accommodation"]
[]
[109,202,1,3,7,"C1.4.5.1","Fixed costs",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J242*K242,2)","v":{"v":0,"d":"0.00"}}]
[]
[110,203,1,3,7,"C1.4.5.2","Running costs",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J244*K244,2)","v":{"v":0,"d":"0.00"}}]
[]
[111,204,1,3,7,"C1.4.6","Office staff"]
[]
[112,205,1,3,7,"C1.4.6.1","Secretary / receptionist",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J248*K248,2)","v":{"v":0,"d":"0.00"}}]
[]
[113,206,1,3,7,"C1.4.6.2","Technical assistant",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J250*K250,2)","v":{"v":0,"d":"0.00"}}]
[]
[114,207,1,3,7,"C1.4.7","Site inspection transport"]
[]
[115,208,1,3,7,"C1.4.7.1","Provision of a bus, mini-bus or combi van for site inspection purposes (specify type and size of vehicle)",null,"Per day",null,null,"Rate Only"]
[]
[116,209,1,3,7,"C1.4.7.2","Travel on site",null,"km",null,null,"Rate Only"]
[]
[117,210,1,3,7,"C1.4.8","Site security measures for the Engineer's facilities"]
[]
[118,211,1,3,7,"C1.4.8.1","Supply and installation of all required security measures at the Engineer's site offices and laboratories",null,"Lump Sum ",{"v":1,"d":"1 "},null,{"$f":"ROUND(J260*K260,2)","v":{"v":0,"d":"0.00"}}]
[]
[119,212,1,3,7,"C1.4.8.2","Provision of security guards / watchmen and an armed response service at the Engineer's site offices and laboratories",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J262*K262,2)","v":{"v":0,"d":"0.00"}}]
[]
[120,213,1,3,8,"C1.4.8.3","Supply and installation of all required security measures at the Engineer's site accommodation",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J264*K264,2)","v":{"v":0,"d":"0.00"}}]
[]
[121,214,1,3,8,"C1.4.8.4","Provision of security guards / watchmen and an armed response service at the Engineer's site accommodation",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J266*K266,2)","v":{"v":0,"d":"0.00"}}]
[]
[122,215,1,3,8,"C1.4.8.5","Supply and installation of an alarm system at the Engineer's rented accommodation (No. of houses stated \"€¦)",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J268*K268,2)","v":{"v":0,"d":"0.00"}}]
[]
[123,216,1,3,8,"C1.4.8.6","Provision of an armed response service at the Engineer's rented accommodation (No. of houses stated \"€¦)",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J270*K270,2)","v":{"v":0,"d":"0.00"}}]
[]
[125,283,1,4,9,null,"SECTION NO. 1"]
[]
[126,689,1,4,9,null,"BILL NO. 4"]
[]
[127,218,1,4,9,"C1.5 ","ACCOMODATION OF TRAFFIC"]
[]
[128,219,1,4,9,"C1.5.1 ","Accommodation of pedestrian and non-motorised traffic"]
[]
[129,220,1,4,9,"C1.5.1.1","Accommodation of pedestrian and non-motorised traffic",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J280*K280,2)","v":{"v":0,"d":"0.00"}}]
[]
[130,221,1,4,9,"C1.5.1.2","Construction of temporary pedestrian walkways and/or cycle paths:"]
[]
[131,222,1,4,9,null,"(a) Gravel surfaced pedestrian walkways / cycle paths",null,"m²",{"v":0,"d":"0 "},null,{"$f":"ROUND(J284*K284,2)","v":{"v":0,"d":"0.00"}}]
[]
[132,223,1,4,9,null,"(b) Bitumen surfaced pedestrian walkways / cycle paths",null,"m²",{"v":0,"d":"0 "},null,{"$f":"ROUND(J286*K286,2)","v":{"v":0,"d":"0.00"}}]
[]
[133,224,1,4,9,null,"(c) 60mm concrete block paved pedestrian walkways / cycle paths",null,"m²",{"v":0,"d":"0 "},null,{"$f":"ROUND(J288*K288,2)","v":{"v":0,"d":"0.00"}}]
[]
[134,225,1,4,9,"C1.5.2","Accommodation of vehicular traffic",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J290*K290,2)","v":{"v":0,"d":"0.00"}}]
[]
[135,226,1,4,9,"C1.5.3","Liaison with traffic authorities",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J292*K292,2)","v":{"v":0,"d":"0.00"}}]
[]
[136,227,1,4,9,"PC1.5.4","Construction of temporary deviations"]
[]
[137,228,1,4,9,null,"The applicable payment items required for the construction of temporary deviations shall be taken from the relevant chapters and sections in Chapters 1, 3, 5, 9 and 10 and inserted into the Pricing Schedule here. Each payment item for the construction of temporary deviations shall be preceded by the main payment item number C1.5.4 / followed by the payment number for the applicable payment item"]
[]
[138,229,1,4,9,"C1.5.5","Maintenance of temporary deviations"]
[]
[139,230,1,4,9,"C1.5.5.1","Grass cutting",null,"ha",{"v":0,"d":"0 "},null,{"$f":"ROUND(J300*K300,2)","v":{"v":0,"d":"0.00"}}]
[]
[140,231,1,4,9,"C1.5.5.2","Drain cleaning",null,"km",{"v":0,"d":"0 "},null,{"$f":"ROUND(J302*K302,2)","v":{"v":0,"d":"0.00"}}]
[]
[141,232,1,4,9,"C1.5.5.3","Cleaning out culverts",null,"m³",{"v":0,"d":"0 "},null,{"$f":"ROUND(J304*K304,2)","v":{"v":0,"d":"0.00"}}]
[]
[142,233,1,4,10,"C1.5.5.4","Collection of rubbish / litter",null,"km",{"v":0,"d":"0 "},null,{"$f":"ROUND(J306*K306,2)","v":{"v":0,"d":"0.00"}}]
[]
[143,234,1,4,10,"C1.5.5.5","Base patching using crushed stone material stabilised with bitumen emulsion and cement",null,"m³",{"v":0,"d":"0 "},null,{"$f":"ROUND(J308*K308,2)","v":{"v":0,"d":"0.00"}}]
[]
[144,235,1,4,10,"C1.5.5.6","Base and/or surface patching using cold premixed asphalt",null,"kg",{"v":0,"d":"0 "},null,{"$f":"ROUND(J310*K310,2)","v":{"v":0,"d":"0.00"}}]
[]
[145,236,1,4,10,"C1.5.5.7","Base and/or surface patching using hot plant mixed asphalt",null,"kg",{"v":0,"d":"0 "},null,{"$f":"ROUND(J312*K312,2)","v":{"v":0,"d":"0.00"}}]
[]
[146,237,1,4,10,"C1.5.5.8","Replacement of damaged guardrails",null,"m",{"v":0,"d":"0 "},null,{"$f":"ROUND(J314*K314,2)","v":{"v":0,"d":"0.00"}}]
[]
[147,238,1,4,10,"C1.5.5.9","Grading of temporary deviations and existing roads used as detours",null,"kg",{"v":0,"d":"0 "},null,{"$f":"ROUND(J316*K316,2)","v":{"v":0,"d":"0.00"}}]
[]
[148,239,1,4,10,"C1.5.5.10","Watering of temporary deviations and existing roads used as detours",null,"kl",{"v":0,"d":"0 "}]
[]
[149,240,1,4,10,"C1.5.5.11","Other road maintenance work ordered by the Engineer",null,"Item",{"v":0,"d":"0 "},null,{"$f":"ROUND(J320*K320,2)","v":{"v":0,"d":"0.00"}}]
[]
[150,241,1,4,10,"C1.5.5.12","Handling cost, profit and all other charges in respect of item C1.5.6.11",null,"%",{"v":0,"d":"0%"},null,{"$f":"ROUND(J322*K322,2)","v":{"v":0,"d":"0.00"}}]
[]
[151,242,1,4,10,"C1.5.6","Removal of temporary deviations",null,"km",{"v":0,"d":"0 "},null,{"$f":"ROUND(J324*K324,2)","v":{"v":0,"d":"0.00"}}]
[]
[152,243,1,4,10,"C1.5.7","Temporary traffic control facilities"]
[]
[153,244,1,4,10,"C1.5.7.1","Delineators including mounting bases and ballast:"]
[]
[154,245,1,4,10,null,"(a) Single sided, reversible left or right (size indicated)",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J330*K330,2)","v":{"v":0,"d":"0.00"}}]
[]
[155,246,1,4,10,null,"(b) Double sided, reversible left or right (size indicated)",null,"No",null,null,"Rate Only"]
[]
[156,247,1,4,10,"C1.5.7.2","Traffic cones, minimum height 750mm",null,"No",null,null,"Rate Only"]
[]
[157,248,1,4,10,"C1.5.7.3","Flagmen",null,"Man-Shift",{"v":100,"d":"100 "},null,{"$f":"ROUND(J336*K336,2)","v":{"v":0,"d":"0.00"}}]
[]
[158,249,1,4,10,"C1.5.7.4","Traffic controllers",null,"Man-Shift",null,null,"Rate Only"]
[]
[159,250,1,4,10,"C1.5.7.5","Provision of illuminated traffic signs:"]
[]
[160,251,1,4,10,null,"(a) Sign mounted flashing amber lights (2 lights with the specified power supply) mounted on a backing board which is:"]
[]
[161,252,1,4,11,null,"(i) 900mm wide x 150mm high",null,"No",{"v":0,"d":"0 "},null,{"$f":"ROUND(J344*K344,2)","v":{"v":0,"d":"0.00"}}]
[]
[162,253,1,4,11,null,"(ii) 1200mm wide x 200mm high",null,"No",{"v":0,"d":"0 "},null,{"$f":"ROUND(J346*K346,2)","v":{"v":0,"d":"0.00"}}]
[]
[163,254,1,4,11,null,"(b) Flashing LED illuminated arrow board",null,"No",{"v":0,"d":"0 "},null,{"$f":"ROUND(J348*K348,2)","v":{"v":0,"d":"0.00"}}]
[]
[164,255,1,4,11,null,"(c) Illuminated road sign \"€“ R & TR series (1200mm diameter)",null,"No",{"v":0,"d":"0 "},null,{"$f":"ROUND(J350*K350,2)","v":{"v":0,"d":"0.00"}}]
[]
[165,256,1,4,11,null,"(d) Illuminated road sign \"€“ TW series (length of sides indicated)",null,"No",{"v":0,"d":"0 "},null,{"$f":"ROUND(J352*K352,2)","v":{"v":0,"d":"0.00"}}]
[]
[166,257,1,4,11,null,"(e) Mobile variable message sign",null,"No",{"v":0,"d":"0 "},null,{"$f":"ROUND(J354*K354,2)","v":{"v":0,"d":"0.00"}}]
[]
[167,258,1,4,11,null,"(f) Mobile variable message sign with a speed measuring and display capability",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J356*K356,2)","v":{"v":0,"d":"0.00"}}]
[]
[168,259,1,4,11,"C1.5.7.6","Maintenance of illuminated traffic signs:"]
[]
[169,260,1,4,11,null,"(a) Sign mounted flashing amber lights (a pair of two lights mounted on a separate backing board)",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J360*K360,2)","v":{"v":0,"d":"0.00"}}]
[]
[170,261,1,4,11,null,"(b) Flashing LED illuminated arrow board",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J362*K362,2)","v":{"v":0,"d":"0.00"}}]
[]
[171,262,1,4,11,null,"(c) Illuminated road sign \"€“ R & TR series (diameter indicated)",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J364*K364,2)","v":{"v":0,"d":"0.00"}}]
[]
[172,263,1,4,11,null,"(d) Illuminated road sign \"€“ TW series (length of sides indicated)",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J366*K366,2)","v":{"v":0,"d":"0.00"}}]
[]
[173,264,1,4,11,null,"(e) Mobile variable message sign",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J368*K368,2)","v":{"v":0,"d":"0.00"}}]
[]
[174,265,1,4,11,null,"(f) Mobile variable message sign with a speed measuring and display capability",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J370*K370,2)","v":{"v":0,"d":"0.00"}}]
[]
[175,266,1,4,11,"C1.5.7.7","Traffic calming devices:"]
[]
[176,267,1,4,11,null,"(a) 25mm high x 100mm wide asphalt rumble strips",null,"m",{"v":0,"d":"0 "},null,{"$f":"ROUND(J374*K374,2)","v":{"v":0,"d":"0.00"}}]
[]
[177,268,1,4,11,null,"(b) 50mm high x 500m wide asphalt rumble strips",null,"m",{"v":0,"d":"0 "},null,{"$f":"ROUND(J376*K376,2)","v":{"v":0,"d":"0.00"}}]
[]
[178,269,1,4,11,null,"(c) 150mm high x 3m wide asphalt speed control humps",null,"m",{"v":0,"d":"0 "},null,{"$f":"ROUND(J378*K378,2)","v":{"v":0,"d":"0.00"}}]
[]
[179,270,1,4,11,"C1.5.7.8","Traffic control stations",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J380*K380,2)","v":{"v":0,"d":"0.00"}}]
[]
[180,271,1,4,11,"C1.5.7.9","Cleaning of traffic control facilities",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J382*K382,2)","v":{"v":0,"d":"0.00"}}]
[]
[181,272,1,4,12,"C1.5.8","Traffic safety officer",null,"Man-Month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J384*K384,2)*0","v":{"v":0,"d":"0.00"}}]
[]
[182,273,1,4,12,"C1.5.9","Traffic safety vehicle",null,"month",{"v":10,"d":"10 "},null,{"$f":"ROUND(J386*K386,2)","v":{"v":0,"d":"0.00"}}]
[]
[183,274,1,4,12,"C1.5.10","Tow trucks"]
[]
[184,275,1,4,12,"C1.5.10.1","Provision of a tow truck on call for light vehicles weighing less than two tonnes",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J390*K390,2)","v":{"v":0,"d":"0.00"}}]
[]
[185,276,1,4,12,"C1.5.10.2","Provision of a tow truck on call for heavy vehicles weighing two tonnes or more",null,"month",{"v":0,"d":"0 "},null,{"$f":"ROUND(J392*K392,2)","v":{"v":0,"d":"0.00"}}]
[]
[186,277,1,4,12,"C1.5.11","Provision of safety equipment for visitors"]
[]
[187,278,1,4,12,"C1.5.11.1","Provision of reflective safety vests for visitors",null,"No",null,null,"Rate Only"]
[]
[188,279,1,4,12,"C1.5.11.2","Provision of hard hats for visitors",null,"No",null,null,"Rate Only"]
[]
[189,280,1,4,12,"C1.5.12","Additional traffic accommodation facilities ordered by the Engineer:"]
[]
[190,281,1,4,12,"C1.5.12.1","Provision of additional traffic accommodation facilities",null,"Item",{"v":1,"d":"1 "},null,{"$f":"ROUND(J402*K402,2)","v":{"v":0,"d":"0.00"}}]
[]
[191,282,1,4,12,"C1.5.12.2","Handling cost, profit and all other charges in respect of item C1.5.12.1",null,"%",{"v":0,"d":"0%"},null,{"$f":"ROUND(J404*K404,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.5.13","Safety Barriers: "]
[]
[{"$nulls":6},"(a) Provide HDPE plastic mobile road safety barrier, NJ type (2.0m x 1.0m high) taped with yellow reflective tape, two strips on either side",null,"No",{"v":30,"d":"30 "},null,{"$f":"ROUND(J408*K408,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(b) Placing, moving and final removal of HDPE NJ type barriers upon completion of the works ",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J410*K410,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(c) Provide precast concrete temporary barrier, NJ type (2.0m x 0.8m high with 0.6m base) taped with yellow reflective tape, two strips on either side and with two amber flashing lights mounted on each barrier",null,"No",{"v":6,"d":"6 "},null,{"$f":"ROUND(J412*K412,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(d) Placing, moving and final removal of concrete barriers upon completion of the apron works ",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J414*K414,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(e) Provide Taxiway/Runway closure barriers as per drawing complete",null,"No",{"v":6,"d":"6 "},null,{"$f":"ROUND(J416*K416,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(f) Placing, moving and final removal of taxiway/runway closure barriers upon completion of the works ",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J418*K418,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.5.14","Provision of lighting on site for works areas during night work or where instructed",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J420*K420,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.5.15","Provision of mobile flood light tower for the use by the Engineer’s staff for works areas during night work or where instructed",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J422*K422,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"PC1.5.16","Provision of escort services for all project vehicles",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J424*K424,2)","v":{"v":0,"d":"0.00"}}]
[]
[125,283,1,4,9,null,"SECTION NO. 1"]
[]
[126,689,1,4,9,null,"BILL NO. 5"]
[]
[127,218,1,4,9,"C1.7","LOADING AND HAULING"]
[]
[{"$nulls":5},"C1.7.1","Loading"]
[]
[{"$nulls":5},"C1.7.1.1","Loading from stockpile using machines and some hand labour where necessary",null,"m³",7910,null,{"$f":"ROUND(J434*K434,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C1.7.1.2","Loading from heaps or windrows using machines and/some hand labour where necessary",null,"m³"]
[]
[{"$nulls":5},"C1.7.1.3","Loading by hand only from stockpile or heaps when labour enhancement work is specified or it is not possible to use machines",null,"m³"]
[]
[{"$nulls":5},"C1.7.2","Hauling"]
[]
[{"$nulls":5},"C1.7.2.1","Hauling material for use in the Works and off-loading it on the site of the Works:"]
[]
[{"$nulls":6},"(a) Soil, gravel, crushed stone and pavement layer material",null,"m³-km"]
[]
[{"$nulls":6},"(b) Boulders and hard material",null,"m³-km"]
[]
[{"$nulls":5},"C1.7.2.2","Hauling material to spoil and off-loading it at a designated spoil or stockpile area:"]
[]
[{"$nulls":6},"(a) Cleared and grubbed material (organic matter and all other unsuitable or waste material)",null,"m³-km"]
[]
[{"$nulls":6},"(b) Soil and gravel material",null,"m³-km",{"v":20250,"d":"20,250 "},null,{"$f":"ROUND(J452*K452,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"(c) Boulders, hard material and concrete",null,"m³-km"]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L6:L455)","v":{"v":560550,"d":"560,550.00"}}]
[197,669,2,1,14,null,"SECTION NO. 2"]
[]
[198,692,2,1,14,null,"BILL NO. 1"]
[]
[199,293,2,1,14,"C2.1 ","GENERAL REQUIREMENTS AND TRENCHING FOR SERVICES"]
[]
[200,294,2,1,14,"C2.1.2.5 ","Using hand excavation to locate, expose and verify services"]
[]
[201,295,2,1,14,null,"Excavation in soft material situated within the following depth ranges below the  surface level:"]
[]
[202,296,2,1,14,null,"(a) 0.0 m up to 2.0 m",null,"m³",{"v":50,"d":"50 "},null,{"$f":"ROUND(J467*K467,2)","v":{"v":0,"d":"0.00"}}]
[]
[203,297,2,1,14,null,"(b) Exceeding 2.0 m and up to 3.0 m",null,"m³",{"v":25,"d":"25 "},null,{"$f":"ROUND(J469*K469,2)","v":{"v":0,"d":"0.00"}}]
[]
[204,298,2,1,14,null,"(c) Extra over subitem B12.06(a) for excavation in hard material",null,"m³",{"v":10,"d":"10 "},null,{"$f":"ROUND(J471*K471,2)","v":{"v":0,"d":"0.00"}}]
[]
[205,299,2,1,14,"C2.1.7 ","Extra over items C2.1.6, C2.1.8 and C2.1.16 for excavating in:"]
[]
[206,300,2,1,14,"C2.1.7.1 ","Hard material irrespective of depth",null,"m³",{"v":25,"d":"25 "},null,{"$f":"ROUND(J475*K475,2)","v":{"v":0,"d":"0.00"}}]
[]
[207,301,2,1,14,"C2.1.7.2 ","Stabilised material irrespective of depth",null,"m³",{"v":10,"d":"10 "},null,{"$f":"ROUND(J477*K477,2)","v":{"v":0,"d":"0.00"}}]
[]
[208,302,2,1,14,"C2.1.8","Excavations outside the normal trench profile",null,"m³",{"v":10,"d":"10 "},null,{"$f":"ROUND(J479*K479,2)","v":{"v":0,"d":"0.00"}}]
[]
[209,303,2,1,14,"C2.1.9 ","Trench excavation using labour enhanced construction methods"]
[]
[210,304,2,1,14,"C2.1.9.1 ","Trenches up to 1.0 m wide (in soft material)"]
[]
[211,305,2,1,14,null,"(a) Up to 1.0 m deep",null,"m³",{"v":25,"d":"25 "},null,{"$f":"ROUND(J485*K485,2)","v":{"v":0,"d":"0.00"}}]
[]
[212,306,2,1,14,null,"(b) Over 1.0 m and up to 1.5 m deep",null,"m³",{"v":10,"d":"10 "},null,{"$f":"ROUND(J487*K487,2)","v":{"v":0,"d":"0.00"}}]
[]
[213,307,2,1,14,"C2.1.11 ","Backfilling of trenches"]
[]
[214,308,2,1,14,"C2.1.11.1 ","Backfill compacted to 93 % (100 % for sand) of MDD (areas subject to traffic loads) using material"]
[]
[215,309,2,1,14,null,"(a) From the excavated trench material",null,"m³",{"v":25,"d":"25 "},null,{"$f":"ROUND(J493*K493,2)","v":{"v":0,"d":"0.00"}}]
[]
[216,310,2,1,14,null,"(b) From other excavations on Site",null,"m³",{"v":10,"d":"10 "},null,{"$f":"ROUND(J495*K495,2)","v":{"v":0,"d":"0.00"}}]
[]
[217,311,2,1,15,null,"(c) From approved borrow areas",null,"m³",{"v":10,"d":"10 "},null,{"$f":"ROUND(J497*K497,2)","v":{"v":0,"d":"0.00"}}]
[]
[219,671,2,2,16,null,"SECTION NO. 2"]
[]
[220,694,2,2,16,null,"BILL NO. 2"]
[]
[221,312,2,2,16,"C2.4 ","ENERGY AND OTHER SERVICES"]
[]
[222,313,2,2,16,"C2.4.1 ","Bedding for electric power cables using material:"]
[]
[223,314,2,2,16,"C2.4.1.1 ","Selected from the excavated trench material",null,"m³",{"v":50,"d":"50 "},null,{"$f":"ROUND(J507*K507,2)","v":{"v":0,"d":"0.00"}}]
[]
[224,315,2,2,16,"C2.4.1.2 ","Selected from other excavations on site",null,"m³",{"v":30,"d":"30 "},null,{"$f":"ROUND(J509*K509,2)","v":{"v":0,"d":"0.00"}}]
[]
[225,316,2,2,16,"C2.4.1.3 ","Selected from approved borrow areas",null,"m³",{"v":25,"d":"25 "},null,{"$f":"ROUND(J511*K511,2)","v":{"v":0,"d":"0.00"}}]
[]
[226,317,2,2,16,"C2.4.1.4 ","Selected from sources provided by the Contractor",null,"m³",{"v":25,"d":"25 "},null,{"$f":"ROUND(J513*K513,2)","v":{"v":0,"d":"0.00"}}]
[]
[227,318,2,2,16,"C2.4.2 ","Concrete for bedding and encasement for electric power cables"]
[]
[228,319,2,2,16,"C2.4.2.1 ","Concrete bedding (Class C16 / 20-20 concrete)",null,"m³",{"v":15,"d":"15 "},null,{"$f":"ROUND(J517*K517,2)","v":{"v":0,"d":"0.00"}}]
[]
[229,320,2,2,16,"C2.4.2.2 ","Concrete encasement of cables (Class C16 / 20-20 concrete)",null,"m³",{"v":15,"d":"15 "},null,{"$f":"ROUND(J519*K519,2)","v":{"v":0,"d":"0.00"}}]
[]
[230,321,2,2,16,"C2.4.3 ","Cable laying accessories (warning tape, protection slabs, markers etc.)"]
[]
[231,322,2,2,16,"C2.4.3.1 ","Electrical warning tape - Supply and install above all cables a continuous brightly coloured corrosion proof (PVC or PE) electrical warning tape. The tape shall have a minimum thickness of 0.8 mm and a minimum width of 150 mm. The tape shall be yellow, marked with the words \"ELECTRIC CABLE / ELEKTRIESE KABEL\" in red letters at least 70 mm in height. These markings shall not be more than 0.5 m apart. The warning tape shall be installed 400 mm above the cable / cable sleeve in a trench",null,"m",{"v":150,"d":"150 "},null,{"$f":"ROUND(J523*K523,2)","v":{"v":0,"d":"0.00"}}]
[]
[232,323,2,2,16,"C2.4.3.2 ","Concrete slab protection (1000 mm x 300 mm x 60 mm thick - 25Mpa)",null,"m",{"v":30,"d":"30 "},null,{"$f":"ROUND(J525*K525,2)","v":{"v":0,"d":"0.00"}}]
[]
[233,324,2,2,16,"C2.4.3.3 ","Cable markers (Base - 250 mm x 250 mm, Top - 150 mm x 150 mm, Height - 300 mm)",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J527*K527,2)","v":{"v":0,"d":"0.00"}}]
[]
[234,325,2,2,16,"C2.4.4 ","Installation of new services"]
[]
[235,326,2,2,17,"C2.4.4.1 ","PVC Sleeves - Supply and install sleeve pipes including short lengths jointing, sweeping bends, buses, locknuts, etc."]
[]
[236,327,2,2,17,null,"(a) 50 mm diameter HDPE Corrugated   -   Colour BLACK / GREEN / BLUE",null,"m",{"v":50,"d":"50 "},null,{"$f":"ROUND(J533*K533,2)","v":{"v":0,"d":"0.00"}}]
[]
[237,328,2,2,17,null,"(b) 32 mm diameter PVC Conduit",null,"m",{"v":50,"d":"50 "},null,{"$f":"ROUND(J535*K535,2)","v":{"v":0,"d":"0.00"}}]
[]
[238,329,2,2,17,"C2.4.4.2 ","Cabling Medium Voltage - Supply, install and connect Cables and Earth Wires in ground and/or through sleeves/conduit and/or fixed on cable trays/ladders"]
[]
[239,330,2,2,17,null,"(a) Insulated Airfield Lighting Cable XLPE (2.8/5kV) - Single Core - 6 mm\"² - 7 strand tinned annealed copper conductor",null,"m",{"v":100,"d":"100 "},null,{"$f":"ROUND(J539*K539,2)","v":{"v":0,"d":"0.00"}}]
[]
[240,331,2,2,17,null,"(b) Cable Joint for above cable (C2.4.4.2(a))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J541*K541,2)","v":{"v":0,"d":"0.00"}}]
[]
[241,332,2,2,17,"C2.4.4.3 ","Cabling Low Voltage - Supply, install and connect Cables and Earth Wires in ground and/or through sleeves/conduit and/or fixed on cable trays/ladders"]
[]
[242,333,2,2,17,null,"(a) ADB Series Transformer Secondary Cable (600v insulation) - 2.5 mm\"² (AWG 12) x 2-core - special length of 15 m with transformer connector",null,"No",{"v":30,"d":"30 "},null,{"$f":"ROUND(J545*K545,2)","v":{"v":0,"d":"0.00"}}]
[]
[243,334,2,2,17,null,"(b) ADB Series Transformer Secondary Cable (600v insulation) - 2.5 mm\"² (AWG 12) x 2-core",null,"m",{"v":150,"d":"150 "},null,{"$f":"ROUND(J547*K547,2)","v":{"v":0,"d":"0.00"}}]
[]
[244,335,2,2,17,null,"(c) ADB Series Transformer Secondary Cable (600v insulation) - 2.5 mm\"² (AWG 12) x 1-core",null,"m",{"v":600,"d":"600 "},null,{"$f":"ROUND(J549*K549,2)","v":{"v":0,"d":"0.00"}}]
[]
[245,336,2,2,17,null,"(d) ADB Series Transformer Secondary Cable (600v insulation) - 4.0 mm\"² (AWG 10) x 1-core",null,"m",{"v":150,"d":"150 "},null,{"$f":"ROUND(J551*K551,2)","v":{"v":0,"d":"0.00"}}]
[]
[246,337,2,2,17,null,"(e) Cable Joint for 2.5 mm\"² x 2-core cable above (C2.4.4.2(a & b))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J553*K553,2)","v":{"v":0,"d":"0.00"}}]
[]
[247,338,2,2,17,null,"(f) Cable Joint for 2.5 mm\"² x 2-core cable above (C2.4.4.2(c))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J555*K555,2)","v":{"v":0,"d":"0.00"}}]
[]
[248,339,2,2,17,null,"(g) Cable Joint for 2.5 mm\"² x 2-core cable above (C2.4.4.2(d))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J557*K557,2)","v":{"v":0,"d":"0.00"}}]
[]
[249,340,2,2,18,"C2.4.4.4 ","Communication Cabling - Supply and install communication cabling on the airfield where damaged"]
[]
[250,341,2,2,18,null,"(a) 400Hz x 7-core",null,"m",{"v":50,"d":"50 "},null,{"$f":"ROUND(J561*K561,2)","v":{"v":0,"d":"0.00"}}]
[]
[251,342,2,2,18,null,"(b) Joining of communication cable (C2.4.4.4(a)) - per joint",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J563*K563,2)","v":{"v":0,"d":"0.00"}}]
[]
[252,343,2,2,18,"C2.4.5 ","Airfield Ground Lighting (AGL) - Runway & Taxiway"]
[]
[253,344,2,2,18,"C2.4.5.1 ","Remove the following light fittings & equipment and safekeep it to be reinstalled afterwards. All light fittings & equipment need to be numbered on itself and on the drawing(s) to ensure that the light fittings and equipment are reinstalled in the same positions afterwards"]
[]
[254,345,2,2,18,null,"(a) ADB SAFEGATE LED Elevated End Bars Light - Type EREL6GR19SF000 - Green / Red",null,"No",{"v":16,"d":"16 "},null,{"$f":"ROUND(J569*K569,2)","v":{"v":0,"d":"0.00"}}]
[]
[255,346,2,2,18,null,"(b) Transformer for above light fitting (C2.4.5.1(a))",null,"No",{"v":16,"d":"16 "},null,{"$f":"ROUND(J571*K571,2)","v":{"v":0,"d":"0.00"}}]
[]
[256,347,2,2,18,null,"(c) ADB SAFEGATE LED Elevated Runway Edge Light - Type EREL6WW39S0000 - White / White",null,"No",{"v":22,"d":"22 "},null,{"$f":"ROUND(J573*K573,2)","v":{"v":0,"d":"0.00"}}]
[]
[257,709,2,2,18,null,"(d) Transformer for above light fitting (C2.4.5.1(c))",null,"No",{"v":22,"d":"22 "},null,{"$f":"ROUND(J575*K575,2)","v":{"v":0,"d":"0.00"}}]
[]
[258,710,2,2,18,null,"(e) ADB SAFEGATE LED Elevated Runway Edge Light - Type EREL6YW39S0000 - Yellow / White",null,"No",{"v":36,"d":"36 "},null,{"$f":"ROUND(J577*K577,2)","v":{"v":0,"d":"0.00"}}]
[]
[259,711,2,2,18,null,"(f) Transformer for above light fitting (C2.4.5.1(e))",null,"No",{"v":36,"d":"36 "},null,{"$f":"ROUND(J579*K579,2)","v":{"v":0,"d":"0.00"}}]
[]
[260,712,2,2,18,null,"(g) ADB SAFEGATE RELIANCE Elevated Taxiway Edge Light - Type L-861T - Blue",null,"No",{"v":55,"d":"55 "},null,{"$f":"ROUND(J581*K581,2)","v":{"v":0,"d":"0.00"}}]
[]
[261,713,2,2,18,null,"(h) Transformer for above light fitting (C2.4.5.1(g))",null,"No",{"v":55,"d":"55 "},null,{"$f":"ROUND(J583*K583,2)","v":{"v":0,"d":"0.00"}}]
[]
[262,714,2,2,18,null,"(i) ADB SAFEGATE SafeLED Inset 8-inch Stop Bar Light / Holding Point Light - Type SL-IQ1-SB-I-U-W-S-R-1C",null,"No",{"v":64,"d":"64 "},null,{"$f":"ROUND(J585*K585,2)","v":{"v":0,"d":"0.00"}}]
[]
[263,715,2,2,18,null,"(j) Transformer for above light fitting (C2.4.5.1(i))",null,"No",{"v":64,"d":"64 "},null,{"$f":"ROUND(J587*K587,2)","v":{"v":0,"d":"0.00"}}]
[]
[264,716,2,2,18,null,"(k) ADB SAFEGATE LED Inset 12-inch Runway Edge Light - Type FED-2-200-C/CM",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J589*K589,2)","v":{"v":0,"d":"0.00"}}]
[]
[265,717,2,2,19,null,"(l) Transformer for above light fitting (C2.4.5.1(k))",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J591*K591,2)","v":{"v":0,"d":"0.00"}}]
[]
[266,718,2,2,19,null,"(m) ADB Light Base - Deep - L-867 & L-868 (only where instructed by the electrical engineer)",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J593*K593,2)","v":{"v":0,"d":"0.00"}}]
[]
[267,719,2,2,19,null,"(n) ADB Light Base - Shallow - for Inset Lights (only where instructed by the electrical engineer)",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J595*K595,2)","v":{"v":0,"d":"0.00"}}]
[]
[268,720,2,2,19,"C2.4.5.2 ","Reinstall the following light fittings & equipment as per the numbering applied during removal"]
[]
[269,721,2,2,19,null,"(a) ADB SAFEGATE LED Elevated End Bars Light - Type EREL6GR19SF000 - Green / Red",null,"No",{"v":16,"d":"16 "},null,{"$f":"ROUND(J599*K599,2)","v":{"v":0,"d":"0.00"}}]
[]
[270,722,2,2,19,null,"(b) Transformer for above light fitting (C2.4.5.1(a))",null,"No",{"v":16,"d":"16 "},null,{"$f":"ROUND(J601*K601,2)","v":{"v":0,"d":"0.00"}}]
[]
[271,723,2,2,19,null,"(c) ADB SAFEGATE LED Elevated Runway Edge Light - Type EREL6WW39S0000 - White / White",null,"No",{"v":22,"d":"22 "},null,{"$f":"ROUND(J603*K603,2)","v":{"v":0,"d":"0.00"}}]
[]
[272,724,2,2,19,null,"(d) Transformer for above light fitting (C2.4.5.1(c))",null,"No",{"v":22,"d":"22 "},null,{"$f":"ROUND(J605*K605,2)","v":{"v":0,"d":"0.00"}}]
[]
[273,725,2,2,19,null,"(e) ADB SAFEGATE LED Elevated Runway Edge Light - Type EREL6YW39S0000 - Yellow / White",null,"No",{"v":36,"d":"36 "},null,{"$f":"ROUND(J607*K607,2)","v":{"v":0,"d":"0.00"}}]
[]
[274,726,2,2,19,null,"(f) Transformer for above light fitting (C2.4.5.1(e))",null,"No",{"v":36,"d":"36 "},null,{"$f":"ROUND(J609*K609,2)","v":{"v":0,"d":"0.00"}}]
[]
[275,727,2,2,19,null,"(g) ADB SAFEGATE RELIANCE Elevated Taxiway Edge Light - Type L-861T - Blue",null,"No",{"v":55,"d":"55 "},null,{"$f":"ROUND(J611*K611,2)","v":{"v":0,"d":"0.00"}}]
[]
[276,728,2,2,19,null,"(h) Transformer for above light fitting (C2.4.5.1(g))",null,"No",{"v":55,"d":"55 "},null,{"$f":"ROUND(J613*K613,2)","v":{"v":0,"d":"0.00"}}]
[]
[277,729,2,2,19,null,"(i) ADB SAFEGATE SafeLED Inset 8-inch Stop Bar Light / Holding Point Light - Type SL-IQ1-SB-I-U-W-S-R-1C",null,"No",{"v":64,"d":"64 "},null,{"$f":"ROUND(J615*K615,2)","v":{"v":0,"d":"0.00"}}]
[]
[278,730,2,2,19,null,"(j) Transformer for above light fitting (C2.4.5.1(i))",null,"No",{"v":64,"d":"64 "},null,{"$f":"ROUND(J617*K617,2)","v":{"v":0,"d":"0.00"}}]
[]
[279,731,2,2,19,null,"(k) ADB SAFEGATE LED Inset 12-inch Runway Edge Light - Type FED-2-200-C/CM",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J619*K619,2)","v":{"v":0,"d":"0.00"}}]
[]
[280,732,2,2,19,null,"(l) Transformer for above light fitting (C2.4.5.1(k))",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J621*K621,2)","v":{"v":0,"d":"0.00"}}]
[]
[281,733,2,2,19,null,"(m) ADB Light Base - Deep - L-867 & L-868 (only where instructed by the electrical engineer) - Bases to be installed by an expert to ensure that lights will face the correct directions/angles",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J623*K623,2)","v":{"v":0,"d":"0.00"}}]
[]
[282,734,2,2,20,null,"(n) ADB Light Base - Shallow - for Inset Lights (only where instructed by the electrical engineer) - Bases to be installed by an expert to ensure that lights will face the correct directions/angles",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J625*K625,2)","v":{"v":0,"d":"0.00"}}]
[]
[283,735,2,2,20,null,"C2.4.5.3 Handling cost and profit in respect of subitem C2.4.5.2(m & n)",null,"%",{"v":0.1,"d":"10%"},{"$f":"SUM(L623:L625)","v":{"v":0,"d":"0.00"}},{"$f":"ROUND(J627*K627,2)","v":{"v":0,"d":"0.00"}}]
[]
[284,736,2,2,20,"C2.4.5.4 ","Supply and install the following new light fittings & new equipment (only where instructed by the electrical engineer)"]
[]
[285,737,2,2,20,null,"(a) ADB SAFEGATE LED Elevated End Bars Light - Type EREL6GR19SF000 - Green / Red",null,"No",{"v":8,"d":"8 "},null,{"$f":"ROUND(J631*K631,2)","v":{"v":0,"d":"0.00"}}]
[]
[286,738,2,2,20,null,"(b) Transformer for above light fitting (C2.4.5.1(a))",null,"No",{"v":8,"d":"8 "},null,{"$f":"ROUND(J633*K633,2)","v":{"v":0,"d":"0.00"}}]
[]
[287,739,2,2,20,null,"(c) ADB SAFEGATE LED Elevated Runway Edge Light - Type EREL6WW39S0000 - White / White",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J635*K635,2)","v":{"v":0,"d":"0.00"}}]
[]
[288,740,2,2,20,null,"(d) Transformer for above light fitting (C2.4.5.1(c))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J637*K637,2)","v":{"v":0,"d":"0.00"}}]
[]
[289,741,2,2,20,null,"(e) ADB SAFEGATE LED Elevated Runway Edge Light - Type EREL6YW39S0000 - Yellow / White",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J639*K639,2)","v":{"v":0,"d":"0.00"}}]
[]
[290,742,2,2,20,null,"(f) Transformer for above light fitting (C2.4.5.1(e))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J641*K641,2)","v":{"v":0,"d":"0.00"}}]
[]
[291,743,2,2,20,null,"(g) ADB SAFEGATE RELIANCE Elevated Taxiway Edge Light - Type L-861T - Blue",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J643*K643,2)","v":{"v":0,"d":"0.00"}}]
[]
[292,744,2,2,20,null,"(h) Transformer for above light fitting (C2.4.5.1(g))",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J645*K645,2)","v":{"v":0,"d":"0.00"}}]
[]
[293,745,2,2,20,null,"(i) ADB SAFEGATE SafeLED Inset 8-inch Stop Bar Light / Holding Point Light - Type SL-IQ1-SB-I-U-W-S-R-1C",null,"No",{"v":15,"d":"15 "},null,{"$f":"ROUND(J647*K647,2)","v":{"v":0,"d":"0.00"}}]
[]
[294,746,2,2,20,null,"(j) Transformer for above light fitting (C2.4.5.1(i))",null,"No",{"v":15,"d":"15 "},null,{"$f":"ROUND(J649*K649,2)","v":{"v":0,"d":"0.00"}}]
[]
[295,747,2,2,20,null,"(k) ADB SAFEGATE LED Inset 12-inch Runway Edge Light - Type FED-2-200-C/CM",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J651*K651,2)","v":{"v":0,"d":"0.00"}}]
[]
[296,748,2,2,20,null,"(l) Transformer for above light fitting (C2.4.5.1(k))",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J653*K653,2)","v":{"v":0,"d":"0.00"}}]
[]
[297,749,2,2,20,null,"(m) ADB Light Base - Deep - L-867 (only where instructed by the electrical engineer) - Bases to be installed by an expert to ensure that lights will face the correct directions/angles",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J655*K655,2)","v":{"v":0,"d":"0.00"}}]
[]
[298,750,2,2,21,null,"(n) ADB Light Base - Deep - L-868 (only where instructed by the electrical engineer) - Bases to be installed by an expert to ensure that lights will face the correct directions/angles",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J657*K657,2)","v":{"v":0,"d":"0.00"}}]
[]
[299,751,2,2,21,null,"(o) ADB Light Base - Shallow - for Inset Lights (only where instructed by the electrical engineer) - Bases to be installed by an expert to ensure that lights will face the correct directions/angles",null,"No",{"v":20,"d":"20 "},null,{"$f":"ROUND(J659*K659,2)","v":{"v":0,"d":"0.00"}}]
[]
[300,752,2,2,21,"PC2.4.5.5 ","Handling cost and profit in respect of subitem C2.4.5.4(m, n & o)",null,"%",{"v":0.1,"d":"10%"},{"$f":"SUM(L655:L659)","v":{"v":0,"d":"0.00"}},{"$f":"ROUND(J661*K661,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L466:L662)","v":{"v":0,"d":"0.00"}}]
[304,672,3,1,23,null,"SECTION NO. 3"]
[]
[305,695,3,1,23,null,"BILL NO. 1"]
[]
[306,753,3,1,23,"C3.1","DRAINS"]
[]
[307,754,3,1,23,"C3.1.2","Clearing, shaping and disposal of accumulated sediment in existing unlined open drains"]
[]
[308,755,3,1,23,"C3.1.2.1","Using conventional methods",null,"m³",{"v":160,"d":"160 "},null,{"$f":"ROUND(J672*K672,2)","v":{"v":0,"d":"0.00"}}]
[]
[309,756,3,1,23,"C3.1.3 ","Excavation, clearing and disposal of accumulated sediment in existing lined drains and drainage systems"]
[]
[310,757,3,1,23,"C3.1.3.1 ","Using conventional methods (up to 1.5 m):"]
[]
[311,758,3,1,23,null,"(a) Manholes and inlet and outlet structures",null,"m³",{"v":5,"d":"5 "},null,{"$f":"ROUND(J678*K678,2)","v":{"v":0,"d":"0.00"}}]
[]
[312,759,3,1,23,"C3.1.3.2","Using conventional methods (in excess of 1,5m):"]
[]
[313,760,3,1,23,null,"(a) Manholes and inlet and outlet structures",null,"m³",{"v":5,"d":"5 "},null,{"$f":"ROUND(J682*K682,2)","v":{"v":0,"d":"0.00"}}]
[]
[314,761,3,1,23,"C3.1.4 ","Excavation and disposal of material for subsoil drainage systems:"]
[]
[315,762,3,1,23,"C3.1.4.1","Excavating in all materail situated within the following depth ranges below the surface:"]
[]
[316,763,3,1,23,null,"(a) 0.0 m to 1.5 m",null,"m³",{"v":560,"d":"560 "},null,{"$f":"ROUND(J688*K688,2)","v":{"v":0,"d":"0.00"}}]
[]
[317,764,3,1,23,null,"(b) Exceeding 1.5 m and up to 3.0 m",null,"m³",{"v":280,"d":"280 "},null,{"$f":"ROUND(J690*K690,2)","v":{"v":0,"d":"0.00"}}]
[]
[318,765,3,1,23,"C3.1.4.5","Extra over sub-item C3.1.4.1 for excavation through stabilised existing road layers",null,"m³",{"v":84,"d":"84 "},null,{"$f":"ROUND(J692*K692,2)","v":{"v":0,"d":"0.00"}}]
[]
[319,766,3,1,23,"C3.1.7 ","Natural permeable material in subsoil drainage systems (approved crushed stone):"]
[]
[320,767,3,1,23,"C3.1.7.2","Crushed stone obtained from commercial sources (state grade)",null,"m³",{"v":250,"d":"250 "},null,{"$f":"ROUND(J696*K696,2)","v":{"v":0,"d":"0.00"}}]
[]
[321,768,3,1,23,"C3.1.9 ","Pipes in subsoil drainage systems:"]
[]
[322,769,3,1,23,"C3.1.9.1","U-PVC pipes and fittings, normal duty, complete with couplings (160mm perforated or non-perforated as specified in Drawing No. 301695-CIV-DP-010)",null,"m",{"v":840,"d":"840 "},null,{"$f":"ROUND(J700*K700,2)","v":{"v":0,"d":"0.00"}}]
[]
[323,770,3,1,24,"C3.1.10","Polymer film sheeting or similar approved material, for lining subsoil drainage systems:"]
[]
[324,771,3,1,24,"C3.1.11","Geotextiles (Synthetic-fibre filter fabric: Grade 2)",null,"m²",{"v":2440,"d":"2,440 "},null,{"$f":"ROUND(J704*K704,2)","v":{"v":0,"d":"0.00"}}]
[]
[325,772,3,1,24,"C3.1.13","Concrete outlet structures, manhole boxes, junction boxes and cleaning eyes for subsoil drainage systems:"]
[]
[326,773,3,1,24,"C3.1.13.4","Cleaning eyes",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J708*K708,2)","v":{"v":0,"d":"0.00"}}]
[]
[327,774,3,1,24,"C3.1.14","Caps for subsoil drain pipes:"]
[]
[328,775,3,1,24,"C3.1.14.1","Concrete caps",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J712*K712,2)","v":{"v":0,"d":"0.00"}}]
[]
[329,776,3,1,24,"C3.1.15","Repairing or replacing existing drainage systems",null,"Item",{"v":1,"d":"1 "},null,{"$f":"ROUND(J714*K714,2)","v":{"v":0,"d":"0.00"}}]
[]
[330,777,3,1,24,"C3.1.20","Breaking into existing drainage structures and install subsoil drain pipe",null,"No",{"v":4,"d":"4 "},null,{"$f":"ROUND(J716*K716,2)","v":{"v":0,"d":"0.00"}}]
[]
[331,778,3,1,24,"C3.1.21","Clearing of existing subsoil drains"]
[]
[332,779,3,1,24,"C3.1.21.1","Cleaning rod, brush and flushing",null,"m",{"v":1650,"d":"1,650 "},null,{"$f":"ROUND(J720*K720,2)","v":{"v":0,"d":"0.00"}}]
[]
[333,780,3,1,24,"C3.1.22","Test flushing of subsoil drain pipe systems",null,"No",{"v":10,"d":"10 "},null,{"$f":"ROUND(J722*K722,2)","v":{"v":0,"d":"0.00"}}]
[]
[334,781,3,1,24,"C3.1.24","Submission of as built drawings by the Contractor",null,"Item",{"v":1,"d":"1 "},null,{"$f":"ROUND(J724*K724,2)","v":{"v":0,"d":"0.00"}}]
[]
[336,673,3,2,25,null,"SECTION NO. 3"]
[]
[337,696,3,2,25,null,"BILL NO. 2"]
[]
[338,782,3,2,25,"C3.2","CULVERTS"]
[]
[339,783,3,2,25,"C3.2.15","Manholes and catch pits, with prefabricated elements"]
[]
[340,784,3,2,25,"C3.2.15.1","Prefabricated floors (installed at a standard depth of 1,0m):"]
[]
[341,785,3,2,25,null,"(a) Prefabricated floors",null,"No",{"v":3,"d":"3 "},null,{"$f":"ROUND(J736*K736,2)","v":{"v":0,"d":"0.00"}}]
[]
[342,786,3,2,25,"C3.2.15.2","Prefabricated roofs:"]
[]
[343,787,3,2,25,null,"(a) Prefabricated roofs",null,"No",{"v":3,"d":"3 "},null,{"$f":"ROUND(J740*K740,2)","v":{"v":0,"d":"0.00"}}]
[]
[344,788,3,2,25,"C3.2.16","Brickwork (Engineering bricks):"]
[]
[345,789,3,2,25,"C3.2.16.2","230mm thick",null,"m²",{"v":10,"d":"10 "},null,{"$f":"ROUND(J744*K744,2)","v":{"v":0,"d":"0.00"}}]
[]
[346,790,3,2,25,"C3.2.17","Plaster",null,"m²",{"v":10,"d":"10 "},null,{"$f":"ROUND(J746*K746,2)","v":{"v":0,"d":"0.00"}}]
[]
[347,791,3,2,25,"C3.2.18","Benching",null,"m³",{"v":1,"d":"1 "},null,{"$f":"ROUND(J748*K748,2)","v":{"v":0,"d":"0.00"}}]
[]
[348,792,3,2,25,"C3.2.19","Accessories"]
[]
[349,793,3,2,25,"C3.2.19.1","Manhole frames (450 mm x 760 mm Cast Iron frames per SABS 115 h/d product 2904 or similar approved) (Drawing No. 301695-CIV-TD-011 Rev A)",null,"No",{"v":3,"d":"3 "},null,{"$f":"ROUND(J752*K752,2)","v":{"v":0,"d":"0.00"}}]
[]
[350,794,3,2,25,"C3.2.19.2","Inlet grids or covers (450 mm x 760 mm Cast Iron grid per SABS 115 h/d product 2904 or similar approved) (Drawing No. 301695-CIV-TD-011 Rev A)",null,"No",{"v":3,"d":"3 "},null,{"$f":"ROUND(J754*K754,2)","v":{"v":0,"d":"0.00"}}]
[]
[351,795,3,2,25,"C3.2.23","Breaking into existing drainage structures and building in pipes or culverts (PC 700mm diameter)",null,"No",{"v":3,"d":"3 "},null,{"$f":"ROUND(J756*K756,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L671:L757)","v":{"v":0,"d":"0.00"}}]
[355,675,4,1,27,null,"SECTION NO. 4"]
[]
[356,698,4,1,27,null,"BILL NO. 1"]
[]
[357,796,4,1,27,"C4.3 ","EXISTING ROAD MATERIALS"]
[]
[358,797,4,1,27,"C4.3.6","Milling and removal of existing asphalt layers with an average milling depth (Contractor takes ownership)"]
[]
[359,798,4,1,27,"C4.3.6.1","Not exceeding 50mm",null,"m³",{"v":8060,"d":"8,060 "},null,{"$f":"ROUND(J767*K767,2)","v":{"v":0,"d":"0.00"}}]
[]
[360,799,4,1,27,"C4.3.6.2","Exceeding 50mm but not exceeding 100mm",null,"m³",{"v":9290,"d":"9,290 "},null,{"$f":"ROUND(J769*K769,2)","v":{"v":0,"d":"0.00"}}]
[]
[361,800,4,1,27,"C4.3.9","Excavating material by using conventional road construction equipment"]
[]
[362,801,4,1,27,"C4.3.9.2","Crushed stone and macadam materials",null,"m³",{"v":1022,"d":"1,022 "},null,{"$f":"ROUND(J773*K773,2)","v":{"v":0,"d":"0.00"}}]
[]
[363,802,4,1,27,"C4.3.10","Excavating material by using labour enhanced methods of construction"]
[]
[364,803,4,1,27,"C4.3.11","Breaking down a stabilised layer by using conventional road construction equipment",null,"m³",{"v":1022,"d":"1,022 "},null,{"$f":"ROUND(J777*K777,2)","v":{"v":0,"d":"0.00"}}]
[]
[365,804,4,1,27,"C4.3.12","Removing of existing concrete material within the following average depth ranges"]
[]
[366,805,4,1,27,"C4.3.13","Lifting of existing paving blocks (interlocking 60mm thick)"]
[]
[367,806,4,1,27,"C4.3.13.2","Using labour enhanced methods of construction",null,"m²",{"v":6812,"d":"6,812 "},null,{"$f":"ROUND(J783*K783,2)","v":{"v":0,"d":"0.00"}}]
[]
[368,807,4,1,27,"C4.3.15","Stockpiling of road layer materials"]
[]
[369,808,4,1,27,"C4.3.15.1","Asphalt material",null,"m³",{"v":17348,"d":"17,348 "},null,{"$f":"ROUND(J787*K787,2)","v":{"v":0,"d":"0.00"}}]
[]
[370,809,4,1,27,"C4.3.15.2","Crushed stone material",null,"m³",{"v":1022,"d":"1,022 "},null,{"$f":"ROUND(J789*K789,2)","v":{"v":0,"d":"0.00"}}]
[]
[371,810,4,1,27,"C4.3.16","Stacking paving blocks and road edging"]
[]
[372,811,4,1,27,"C4.3.16.1","Paving blocks (interlocking 60mm thick)",null,"No",{"v":370217,"d":"370,217 "},null,{"$f":"ROUND(J793*K793,2)","v":{"v":0,"d":"0.00"}}]
[]
[373,812,4,1,27,"C4.3.18","Excavate non-compliant or excess pavement layer material to spoil in sites designated by the Contractor, material consisting of"]
[]
[374,813,4,1,27,"C4.3.18.2","Crushed stone material",null,"m³",{"v":2044,"d":"2,044 "},null,{"$f":"ROUND(J797*K797,2)","v":{"v":0,"d":"0.00"}}]
[]
[376,676,4,2,28,null,"SECTION NO. 4"]
[]
[377,699,4,2,28,null,"BILL NO. 2"]
[]
[378,814,4,2,28,"C4.4","COMMERCIAL MATERIALS"]
[]
[379,815,4,2,28,"C4.4.2","Commercial materials identified by the Contractor from commercial, private or other non-commercial suppliers"]
[]
[380,816,4,2,28,"C4.4.2.1","Pavement layer material:"]
[]
[381,817,4,2,28,null,"(c) G5A crushed rock/boulder materials",null,"m³",{"v":1022,"d":"1,022 "},null,{"$f":"ROUND(J809*K809,2)","v":{"v":0,"d":"0.00"}}]
[]
[382,818,4,2,28,"C4.4.4","Cementitious stabilising agents"]
[]
[383,819,4,2,28,"C4.4.4.1","Cement",null,"t",{"v":3727.8,"d":"3,727.80"},null,{"$f":"ROUND(J813*K813,2)","v":{"v":0,"d":"0.00"}}]
[]
[384,820,4,2,28,"C4.4.5","Bituminous stabilising agents"]
[]
[385,821,4,2,28,"C4.4.5.2","Emulsion stable grade (Anionic SS60)",null,"t",{"v":2444,"d":"2,444.00"},null,{"$f":"ROUND(J817*K817,2)","v":{"v":0,"d":"0.00"}}]
[]
[386,822,4,2,28,"C4.4.6","Active filler for bituminous stabilisation (Cement)",null,"t",{"v":611,"d":"611.00"},null,{"$f":"ROUND(J819*K819,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L766:L820)","v":{"v":0,"d":"0.00"}}]
[390,677,5,1,30,null,"SECTION NO. 5"]
[]
[391,700,5,1,30,null,"BILL NO. 1"]
[]
[392,823,5,1,30,"C5.3","ROAD PAVEMENT LAYERS"]
[]
[393,824,5,1,30,"C5.3.1","Commercial materials identified by the Employer from commercial, private or other non-commercial suppliers (specify the source/s)",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J828*K828,2)","v":{"v":0,"d":"0.00"}}]
[]
[394,825,5,1,30,"C5.3.2","Construction of pavement layers"]
[]
[395,826,5,1,30,"C5.3.2.1","Construction of layers using conventional construction methods:"]
[]
[396,827,5,1,30,null,"(k) Upper subbase gravel layer (unstabilised) (l150mm) compacted to 97% of MDD",null,"m³",{"v":2044,"d":"2,044 "},null,{"$f":"ROUND(J834*K834,2)","v":{"v":0,"d":"0.00"}}]
[]
[397,828,5,1,30,"C5.3.11","Riding quality measurements:"]
[]
[398,829,5,1,30,"C5.3.11.3","Using an inertial profilometer",null,"km",{"v":75,"d":"75 "},null,{"$f":"ROUND(J838*K838,2)","v":{"v":0,"d":"0.00"}}]
[]
[399,830,5,1,30,"C5.3.12","Surface regularity payment adjustments",null,"Item",{"v":1,"d":"1 "},null,{"$f":"ROUND(J840*K840,2)","v":{"v":0,"d":"0.00"}}]
[]
[401,678,5,2,31,null,"SECTION NO. 5"]
[]
[402,701,5,2,31,null,"BILL NO. 2"]
[]
[{"$nulls":5},"C5.4","STABILISATION"]
[]
[{"$nulls":5},"C5.4.7","Bituminous stabilisation of pavement layers "]
[]
[{"$nulls":5},"C5.4.7.1","Bituminous stabilisation 300 mm of base layer",null,"litre (ℓ)",{"$f":"(((61100)*2000)*3%)/1.05","v":{"v":3491428.5714285714,"d":"3,491,429 "}},null,{"$f":"ROUND(J850*K850,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.4.8","Bituminous stabilisation agent :"]
[]
[{"$nulls":5},"C5.4.8.1","60% anionic emulsion",null,"litre (ℓ)",{"$f":"(((61100)*2000)*3%)/1.05","v":{"v":3491428.5714285714,"d":"3,491,429 "}},null,{"$f":"ROUND(J854*K854,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.4.9","Filler for bituminous stabilisation"]
[]
[{"$nulls":5},"C5.4.9.1","Filler for bituminous stabilisation (cement CEM II (A-L) 32,5N)",null,"Ton",{"$f":"((61100*1%)*1440)/1000","v":{"v":879.84,"d":"880 "}},null,{"$f":"ROUND(J858*K858,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.4.10","Provision and application of water for curing",null,"kl",{"$f":"(61100/0.3)*0.5*3*7/1000","v":{"v":2138.5,"d":"2,139 "}},null,{"$f":"ROUND(J860*K860,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.4.11","Curing by covering with the subsequent layer",null,"m³",{"$f":"(61100/0.3)*0.15","v":{"v":30550,"d":"30,550 "}},null,{"$f":"ROUND(J862*K862,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.4.14","Trial section for a chemically stabilised layer",null,"m³",{"$f":"500*0.15*3.5","v":{"v":262.5,"d":"263 "}},null,{"$f":"ROUND(J864*K864,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.4.15","Trial section for a bituminously stabilised layer (3,5m wide)",null,"m²",{"$f":"500*0.2","v":{"v":100,"d":"100 "}},null,{"$f":"ROUND(J866*K866,2)","v":{"v":0,"d":"0.00"}}]
[]
[401,678,5,2,31,null,"SECTION NO. 5"]
[]
[402,701,5,2,31,null,"BILL NO. 3"]
[]
[403,831,5,2,31,"C5.5","RECONSTRUCTION OF PAVEMENT LAYERS"]
[]
[404,832,5,2,31,"C5.5.1","Compiling and implementing M&U plans for the reconstruction of an existing road pavement",null,"No",{"v":2,"d":"2 "},null,{"$f":"ROUND(J874*K874,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C5.5.4","Sampling of in-situ material for mix design procedure",null,"No",9,null,{"$f":"ROUND(J876*K876,2)","v":{"v":0,"d":"0.00"}}]
[]
[405,833,5,2,31,"C5.5.8","Pre-pulverising material in the existing pavement"]
[]
[406,834,5,2,31,"C5.5.8.2","Crushed stone base (300mm deep)",null,"m³",{"v":61100,"d":"61,100 "},null,{"$f":"ROUND(J880*K880,2)","v":{"v":0,"d":"0.00"}}]
[]
[407,835,5,2,31,"C5.5.9","Temporarily blading layer material to windrow",null,"m³",{"v":61100,"d":"61,100 "},null,{"$f":"ROUND(J882*K882,2)","v":{"v":0,"d":"0.00"}}]
[]
[408,836,5,2,31,"C5.5.10","Roller-pass compaction of an exposed pavement layer"]
[]
[409,837,5,2,31,"C5.5.10.1","Smooth drum vibratory rollers",null,"m²",{"v":407334,"d":"407,334 "},null,{"$f":"ROUND(J886*K886,2)","v":{"v":0,"d":"0.00"}}]
[]
[410,838,5,2,31,"C5.5.11","Watering the exposed pavement layer",null,"kl",{"v":4074,"d":"4,074 "},null,{"$f":"ROUND(J888*K888,2)","v":{"v":0,"d":"0.00"}}]
[]
[411,839,5,2,31,"C5.5.16","In-situ reconstruction of a pavement layer using a recycler to construct a stabilised base layer"]
[]
[412,840,5,2,31,"C5.5.16.1","Chemically stabilised base layer compacted to 100% of MDD:"]
[]
[413,841,5,2,31,null,"(a) Using non-cemented material compacted to 100% of MDD, 150mm thick (Cement stabilized C4)",null,"m³",{"v":1030,"d":"1,030 "},null,{"$f":"ROUND(J894*K894,2)","v":{"v":0,"d":"0.00"}}]
[]
[414,842,5,2,31,"C5.5.16.2","Emulsion stabilised subbase layer compacted to 102% of MDD:"]
[]
[415,843,5,2,31,null,"(a) Using non-cemented material compacted to 102% MDD, 300 mm thick (BSM1)",null,"m³",{"v":61100,"d":"61,100 "},null,{"$f":"ROUND(J898*K898,2)","v":{"v":0,"d":"0.00"}}]
[]
[416,844,5,2,31,"C5.5.20","Material shortfall or make-up material"]
[]
[417,845,5,2,31,"C5.5.20.3","For base layer",null,"m³",{"v":4980,"d":"4,980 "},null,{"$f":"ROUND(J902*K902,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L828:L903)","v":{"v":0,"d":"0.00"}}]
[421,679,6,1,33,null,"SECTION NO. 6"]
[]
[422,702,6,1,33,null,"BILL NO. 1"]
[]
[423,846,6,1,33,"C6.2 ","SEGMENTAL BLOCK PAVING LAYERS"]
[]
[424,847,6,1,33,"C6.2.1","Segmental block paving"]
[]
[425,848,6,1,33,"C6.2.1.1","80mm thick Interlocking block paving (Type S-A - 25MPa)",null,"m²",{"v":6820,"d":"6,820 "},null,{"$f":"ROUND(J913*K913,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C6.2.2","Cast in-situ concrete edge and intermediate beams (150mm x 200mm deep)",null,"m3",{"$f":"350*0.3*0.2","v":{"v":21,"d":"21 "}},null,{"$f":"ROUND(J915*K915,2)","v":{"v":0,"d":"0.00"}}]
[]
[426,849,6,1,33,"C6.2.3","Provision and application of approved herbicide and ant poison"]
[]
[427,850,6,1,33,"C6.2.3.1","Provision of materials",null,"PC Sum",{"v":1,"d":"1 "},{"$f":"(1267463/1000)*2","v":{"v":2534.926,"d":"2,534.93"}},{"$f":"ROUND(J919*K919,2)","v":{"v":2534.93,"d":"2,534.93"}}]
[]
[428,851,6,1,33,"C6.2.3.2","Contractor\"€™s charges and profit added to the prime cost sum",null,"%",{"v":0.1,"d":"10%"},{"$f":"L919","v":{"v":2534.93,"d":"2,534.93"}},{"$f":"ROUND(J921*K921,2)","v":253.49}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L911:L922)","v":{"v":2788.42,"d":"2,788.42"}}]
[430,680,7,1,34,null,"SECTION NO. 7"]
[]
[431,703,7,1,34,null,"BILL NO. 1"]
[]
[432,852,7,1,34,"C7.1","REPLACEMENT OF EXISTING JOINT SEALANT"]
[]
[433,853,7,1,34,"C7.1.1","Replacing of joint sealant in existing concrete pavement as follows:"]
[]
[434,854,7,1,34,"C7.1.1.1","Removal of existing seal and backing material",null,"m",{"v":5900,"d":"5,900 "},null,{"$f":"ROUND(J932*K932,2)","v":{"v":0,"d":"0.00"}}]
[]
[435,855,7,1,34,"C7.1.1.2","Reaming of existing joints (20 mm x 50 mm deep)",null,"m",{"v":5900,"d":"5,900 "},null,{"$f":"ROUND(J934*K934,2)","v":{"v":0,"d":"0.00"}}]
[]
[436,856,7,1,34,"C7.1.1.5","Installation of backing material in saw cut joints (to fit saw cut dimensions)",null,"m",{"$f":"5900","v":{"v":5900,"d":"5,900 "}},null,{"$f":"ROUND(J936*K936,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C7.1.1.6","Installation of cold pour sealant (high elasticity self levelling silicon)",null,"litre (ℓ)",{"$f":"0.02*0.03*5900*1000","v":{"v":3539.9999999999995,"d":"3,540 "}},null,{"$f":"ROUND(J938*K938,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L931:L938)","v":{"v":0,"d":"0.00"}}]
[438,681,8,1,35,null,"SECTION NO. 8"]
[]
[439,704,8,1,35,null,"BILL NO. 1"]
[]
[440,857,8,1,35,"C8.1","PRIME COAT"]
[]
[441,858,8,1,35,"C8.1.1","Prime coat:"]
[]
[442,859,8,1,35,"C8.1.1.2","MC -30 cut-back bitumen",null,"litre (ℓ)",{"v":70000,"d":"70,000 "},null,{"$f":"ROUND(J949*K949,2)","v":{"v":0,"d":"0.00"}}]
[]
[443,860,8,1,35,"C8.1.1.3","Inverted bitumen emulsion",null,"litre (ℓ)",{"v":70000,"d":"70,000 "},null,{"$f":"ROUND(J951*K951,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L948:L952)","v":{"v":0,"d":"0.00"}}]
[445,682,9,1,36,null,"SECTION NO. 9"]
[]
[446,705,9,1,36,null,"BILL NO. 1"]
[]
[447,861,9,1,36,"C9.1","ASPHALT LAYERS"]
[]
[448,862,9,1,36,"C9.1.1","Asphalt mix designs"]
[]
[449,863,9,1,36,"C9.1.1.1","Stone skeletal mixes:"]
[]
[451,865,9,1,36,null,"(d) Ultrathin Friction Courses (UTFC) (Bitumen Rubber binder)",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J964*K964,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":5},"C9.1.1.2","Sand skeletal mixes:"]
[]
[{"$nulls":6},"(a) Continuously graded base or surfacing (EMB; level II)",null,"Lump Sum",{"v":1,"d":"1 "},null,{"$f":"ROUND(J968*K968,2)","v":{"v":0,"d":"0.00"}}]
[]
[452,866,9,1,36,"C9.1.2","Construction of trial sections"]
[]
[453,867,9,1,36,"C9.1.2.1","Asphalt layers (Continously graded Asphalt with 20% reclaimed material, 45mm placed by paver)",null,"m²",{"v":6000,"d":"6,000 "},null,{"$f":"ROUND(J972*K972,2)","v":{"v":0,"d":"0.00"}}]
[]
[454,868,9,1,36,"C9.1.2.2","Removal of trial section where so instructed by the Engineer",null,"m²",{"v":6000,"d":"6,000 "},null,{"$f":"ROUND(J974*K974,2)","v":{"v":0,"d":"0.00"}}]
[]
[455,869,9,1,36,"C9.1.3","Application of bond coat"]
[]
[456,870,9,1,36,"C9.1.3.1","Stable\"€“grade 30% net bitumen emulsion as specified.  Applied with a calibrated distributer",null,"litre (ℓ)",{"v":343880,"d":"343,880 "},null,{"$f":"ROUND(J978*K978,2)","v":{"v":0,"d":"0.00"}}]
[]
[457,871,9,1,36,"C9.1.5.2","Rehabilitation"]
[]
[458,872,9,1,36,null,"(g) Continously graded Asphalt, 45mm placed by paver (20 % reclaimed asphalt)",null,"t",{"v":358460,"d":"358,460.00"},null,{"$f":"ROUND(J982*K982,2)","v":{"v":0,"d":"0.00"}}]
[]
[459,873,9,1,36,null,"(h) Continously graded Asphalt Correction layer, variable thickness (max 20mm) placed by paver (20 % reclaimed asphalt)",null,"t",{"v":2500,"d":"2,500.00"},null,{"$f":"ROUND(J984*K984,2)","v":{"v":0,"d":"0.00"}}]
[]
[460,874,9,1,36,null,"(i) Certified: BRUTFC layer (15mm thickness)",null,"t",{"v":154800,"d":"154,800.00"},null,{"$f":"ROUND(J986*K986,2)","v":{"v":0,"d":"0.00"}}]
[]
[461,875,9,1,36,"C9.1.10","Variation rates"]
[]
[462,876,9,1,36,"C9.1.10.1","Bitumen (AE2)",null,"t",{"v":720,"d":"720.00"},null,{"$f":"ROUND(J990*K990,2)","v":{"v":0,"d":"0.00"}}]
[]
[463,877,9,1,36,"C9.1.10.2","Aggregate",null,"t",{"v":2510,"d":"2,510.00"},null,{"$f":"ROUND(J992*K992,2)","v":{"v":0,"d":"0.00"}}]
[]
[464,878,9,1,37,"C9.1.10.3","Active filler (Hydrated lime)",null,"t",{"v":360,"d":"360.00"},null,{"$f":"ROUND(J994*K994,2)","v":{"v":0,"d":"0.00"}}]
[]
[465,879,9,1,37,"C9.1.13","Coring of asphalt layers"]
[]
[466,880,9,1,37,"C9.1.13.1","100mm diameter",null,"No",{"v":300,"d":"300 "},null,{"$f":"ROUND(J998*K998,2)","v":{"v":0,"d":"0.00"}}]
[]
[467,881,9,1,37,"C9.1.13.2","150mm diameter",null,"No",{"v":100,"d":"100 "},null,{"$f":"ROUND(J1000*K1000,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L963:L1001)","v":{"v":0,"d":"0.00"}}]
[469,683,10,1,38,null,"SECTION NO. 11"]
[]
[470,706,10,1,38,null,"BILL NO. 1"]
[]
[471,882,10,1,38,"C11.7","ROAD MARKINGS AND ROAD STUDS"]
[]
[472,883,10,1,38,"C11.7.1","Road marking:"]
[]
[473,884,10,1,38,"C11.7.1.1","White lines broken or unbroken (300 mm and 600 mm wide water-bourne paint or similar approved)",null,"km",{"v":4.8,"d":"5 "},null,{"$f":"ROUND(J1011*K1011,2)","v":{"v":0,"d":"0.00"}}]
[]
[474,885,10,1,38,"C11.7.1.2","Yellow lines broken or unbroken (300 mm and 600 mm wide water-borne paint or similar approved)",null,"km",{"v":7.5,"d":"8 "},null,{"$f":"ROUND(J1013*K1013,2)","v":{"v":0,"d":"0.00"}}]
[]
[475,886,10,1,38,"C11.7.1.4","White lettering and symbols (Water-borne paint or similar approved)",null,"m²",{"v":5510,"d":"5,510 "},null,{"$f":"ROUND(J1015*K1015,2)","v":{"v":0,"d":"0.00"}}]
[]
[476,887,10,1,38,"C11.7.1.5","Yellow lettering and symbols (Water-borne paint or similar approved)",null,"m²",{"v":344,"d":"344 "},null,{"$f":"ROUND(J1017*K1017,2)","v":{"v":0,"d":"0.00"}}]
[]
[477,888,10,1,38,"C11.7.1.7","Transverse lines, painted island and arrestor bed markings (Water-borne paint or similar approved - any colour)",null,"m²",{"v":1360,"d":"1,360 "},null,{"$f":"ROUND(J1019*K1019,2)","v":{"v":0,"d":"0.00"}}]
[]
[478,889,10,1,38,"C11.7.2","Retro-reflective road marking:"]
[]
[479,890,10,1,38,"C11.7.2.1","White lines broken or unbroken (300 mm and 600 mm wide)",null,"km",{"v":4.8,"d":"5 "},null,{"$f":"ROUND(J1023*K1023,2)","v":{"v":0,"d":"0.00"}}]
[]
[480,891,10,1,38,"C11.7.2.4","White lettering and symbols",null,"m²",{"v":350,"d":"350 "},null,{"$f":"ROUND(J1025*K1025,2)","v":{"v":0,"d":"0.00"}}]
[]
[481,892,10,1,38,"C11.7.5","Variations in rate of application:"]
[]
[482,893,10,1,38,"C11.7.5.1","White paint",null,"litre (ℓ)",{"v":500,"d":"500 "},null,{"$f":"ROUND(J1029*K1029,2)","v":{"v":0,"d":"0.00"}}]
[]
[483,894,10,1,38,"C11.7.5.2","Yellow paint",null,"litre (ℓ)",{"v":210,"d":"210 "},null,{"$f":"ROUND(J1031*K1031,2)","v":{"v":0,"d":"0.00"}}]
[]
[484,895,10,1,38,"C11.7.5.4","Retro-reflective beads",null,"kg",{"v":270,"d":"270 "},null,{"$f":"ROUND(J1033*K1033,2)","v":{"v":0,"d":"0.00"}}]
[]
[485,896,10,1,38,"C11.7.7","Road studs"]
[]
[486,897,10,1,38,"C11.7.8","Setting out and premarking the lines (excluding traffic island markings, lettering and symbols)",null,"km",{"v":17.1,"d":"17 "},null,{"$f":"ROUND(J1037*K1037,2)","v":{"v":0,"d":"0.00"}}]
[]
[487,898,10,1,38,"C11.7.9","Re-establishing the painting unit during the defects notification period and at other instances on instruction of the Engineer",null,"No",{"v":1,"d":"1 "},null,{"$f":"ROUND(J1039*K1039,2)","v":{"v":0,"d":"0.00"}}]
[]
[489,684,10,2,39,null,"SECTION NO. 11"]
[]
[490,707,10,2,39,null,"BILL NO. 2"]
[]
[491,899,10,2,39,"C11.8","LANDSCAPING AND PLANTING PLANTS"]
[]
[492,900,10,2,39,"C11.8.1","Trimming:"]
[]
[493,901,10,2,39,"C11.8.1.1","Machine trimming",null,"m²",{"v":80,"d":"80 "},null,{"$f":"ROUND(J1049*K1049,2)","v":{"v":0,"d":"0.00"}}]
[]
[494,902,10,2,39,"C11.8.1.2","Hand trimming",null,"m²",{"v":40,"d":"40 "},null,{"$f":"ROUND(J1051*K1051,2)","v":{"v":0,"d":"0.00"}}]
[]
[495,903,10,2,39,"C11.8.2","Trimming using machines for trimming or shaping (alternative to subitem C11.8.1.1):"]
[]
[496,904,10,2,39,"C11.8.2.1","Bulldozer",null,"hr",{"v":20,"d":"20 "},null,{"$f":"ROUND(J1055*K1055,2)","v":{"v":0,"d":"0.00"}}]
[]
[497,905,10,2,39,"C11.8.2.2","Motor grader",null,"hr",{"v":20,"d":"20 "},null,{"$f":"ROUND(J1057*K1057,2)","v":{"v":0,"d":"0.00"}}]
[]
[498,906,10,2,39,"C11.8.3","Preparing the areas for grassing:"]
[]
[499,907,10,2,39,"C11.8.3.3","Topsoiling within the road reserve where the following materials are used:"]
[]
[500,908,10,2,39,null,"(a) Topsoil obtained from within the road reserve or borrow areas",null,"m³",{"v":12,"d":"12 "},null,{"$f":"ROUND(J1063*K1063,2)","v":{"v":0,"d":"0.00"}}]
[]
[501,909,10,2,39,"C11.8.4","Grassing"]
[]
[502,910,10,2,39,"C11.8.4.1","Hydroseeding:"]
[]
[{"$nulls":6},"(c) Hydroseeding",null,"ha",0.1,null,{"$f":"ROUND(J1069*K1069,2)","v":{"v":0,"d":"0.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L1010:L1070)","v":{"v":0,"d":"0.00"}}]
[506,685,11,1,41,null,"SECTION NO. 20"]
[]
[507,708,11,1,41,null,"BILL NO. 1"]
[]
[508,911,11,1,41,"C20.1","TESTING MATERIALS AND JUDGEMENT OF WORKMANSHIP"]
[]
[509,912,11,1,41,"PC20.1.6","(a) Provision for testing materials and judgement of workmanship",null,"PC Sum",{"v":1,"d":"1 "},{"v":1900000,"d":"1,900,000.00"},{"$f":"ROUND(J1078*K1078,2)","v":{"v":1900000,"d":"1,900,000.00"}}]
[]
[{"$nulls":6},"(i) Handling cost and profit in respect of item C20.1.6 (a)",null,"%",{"v":0.1,"d":"10%"},{"$f":"K1078","v":{"v":1900000,"d":"1,900,000.00"}},{"$f":"ROUND(J1080*K1080,2)","v":{"v":190000,"d":"190,000.00"}}]
[]
[{"$nulls":6},"Carried to Summary",{"$nulls":3},"R",{"$f":"SUM(L1077:L1081)","v":{"v":2090000,"d":"2,090,000.00"}}]
[]
[{"$nulls":6},"FINAL SUMMARY"]
[]
[511,1,12,1,42,null,"GENERAL",null,"Section",1,null,{"$f":"L456","v":{"v":560550,"d":"560,550.00"}}]
[]
[512,2,12,1,42,null,"SERVICES",null,"Section",2,null,{"$f":"L663","v":{"v":0,"d":"0.00"}}]
[]
[513,3,12,1,42,null,"DRAINAGE",null,"Section",3,null,{"$f":"L758","v":{"v":0,"d":"0.00"}}]
[]
[514,4,12,1,42,null,"EARTHWORKS AND PAVEMENT LAYERS MATERIALS",null,"Section",4,null,{"$f":"L821","v":{"v":0,"d":"0.00"}}]
[]
[515,5,12,1,42,null,"EARTHWORKS AND PAVEMENT LAYERS CONSTRUCTION",null,"Section",5,null,{"$f":"L904","v":{"v":0,"d":"0.00"}}]
[]
[516,6,12,1,42,null,"CONCRETE LAYERS",null,"Section",6,null,{"$f":"L923","v":{"v":2788.42,"d":"2,788.42"}}]
[]
[517,547,12,1,42,null,"MAINTENANCE AND REPAIR CONCRETE LAYERS",null,"Section",7,null,{"$f":"L940","v":{"v":0,"d":"0.00"}}]
[]
[518,7,12,1,42,null,"PRETREATMENT AND REPAIR EXISTING LAYERS",null,"Section",8,null,{"$f":"L953","v":{"v":0,"d":"0.00"}}]
[]
[519,8,12,1,42,null,"ASPHALT LAYERS",null,"Section",9,null,{"$f":"L1002","v":{"v":0,"d":"0.00"}}]
[]
[520,9,12,1,42,null,"ANCILLIARY ROAD WORKS",null,"Section",11,null,{"$f":"L1071","v":{"v":0,"d":"0.00"}}]
[]
[521,10,12,1,42,null,"QUALITY ASSURANCE",null,"Section",20,null,{"$f":"L1082","v":{"v":2090000,"d":"2,090,000.00"}}]
[]
[{"$nulls":6},"Total",{"$nulls":3},"R",{"$f":"SUM(L1085:L1107)","v":{"v":2653338.42,"d":"2,653,338.42"}}]