{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["NOMANGESI-MALUNGA-MLOMO"],"read":"whole","date_system":"1900"}

{"sheet":"NOMANGESI-MALUNGA-MLOMO","index":0,"n_rows":187,"n_cols":8,"rows_kept":187}
["Client ",null,"Winnie Madikizela Mandela Local Municipality"]
[]
["Contract No",null,"WMM-LM 05/02/26/01 MWC"]
[]
["Contract Name",null,"MAINTENANCE OF WARD 18 COMMUNITY HALL "]
[]
["ITEM NO ","PAYMENT",null,"DESCRIPTION","Unit","Quantity","Rate","Amount"]
[null,"SANS 1200 A",null,"SECTION 1:PRELIMINARY AND GENERAL"]
[1,8.3,null,"FIXED-CHANGE ITEMS"]
[1.1,"8.3.1",null,"Contractual Requirements","Sum",1]
[1.2,"8.3.2",null,"Establish Facilities on site :"]
[]
[1.8,8.4,null,"TIME RELATED ITEMS "]
["1.8.1","8.4.1",null,"Contractual Requirements","Sum",1]
[1.9,"8.2.1",null,"CONTRACTUAL REQUIREMENTS including the provision,maintenance and removal of facilities for the engineer as specified and for the contractor"]
[]
["1.9.1","8.2.2",null,"a)Fixed Charges","Sum",1]
[{"$nulls":3},"b)Time-Related Charges","Month",1]
["Total Carried Forward to Summary"]
[]
["ITEM NO","PAYMENT",null,"DESCRIPTION ","Unit","Quantity","Rate","Amount"]
[{"$nulls":3},"RENOVATION TO EXISTING BUILDING "]
[2,null,null,"SECTION2:REMOVAL OF EXISTING WORK"]
[]
[{"$nulls":3},"Allow for protecting all existing work liable to suffer damage(I,e.walls ,finishes,floors,windows,etc)from damage during the building "]
[{"$nulls":3},"operations,alterations,etc,and make good all work damaged with new material to match existing to the approval of the director."]
[]
[2.1,null,null,"Carefully taking out and remove all existing roof sheets,windows,wall finishes including skirting."]
[{"$nulls":3},"cornice and timber doors,frames and ceiling boards from hall and ablution facilities"]
["2.1.2",null,null,"Taking out and remove ceiling boards (only affected areas)","m²",108]
["2.1.5",null,null,"Taking out and remove single door with frame (Toilets)","No",7]
[]
[2.2,null,null,"Carefully taking out,remove painting and clear surface"]
[]
["2.2.1",null,null,"Remove all painting from the walls (Hall inside only and in and out in the toilets)","m²",485]
["Total Carried Forward to Summary"]
[]
["ITEM NO","PAYMENT",null,"DESCRIPTION","Unit","Quantity","Rate","Amount"]
[{"$nulls":3},"RENOVATIONS TO EXISTING BUILDING"]
[3,"SABS1200C",null,"SECTION3:EXCAVATION AND CONCRETE"]
[3.1]
[{"$nulls":3},"Excavation in earth and leveling soilto receive ne concrete aprons,concrete v-drain and concrete pavers"]
["3.1.1",null,null,"Concrete aprons","m³",2]
[3.2,null,null,"FILLING,ETC"]
[{"$nulls":3},"Earth filling obtained from the excavations and or prescribed stock piles on site compacted to 90%mod AASHTO density"]
["3.2.1",null,null,"Backfilling to sides of aprons","m³",2]
[]
["Total Carried Forward to summary"]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,4,null,"SECTION4:CRACKS AND LINKS"]
[]
[null,"4.1.1",null,"Inspect and fix all cracks in toilet and community hall","Sum",1,5000]
[null,"4.1.2",null,"Inspect and fix all Links on Roof sheeting","Sum",1,10000]
[]
[null,"Total Carried Forward to Summary"]
[]
[]
["ITEM NO ","PAYMENT",null,"DESCRIPTION","Unit","Quantity","Rate","Amount"]
[{"$nulls":3},"RENOVATION TO EXISTING BUILDING"]
[{"$nulls":3},"CARPENTRY AND JOINERY"]
[5,"PS15",null,"SECTION5:WINDOWS,DOORS AND CEILING"]
[]
[5.1,null,null,"STEEL WINDOWS"]
["5.1.1",null,null,"W1-Window type Steel - Glazing","no",5]
[]
[5.2,null,null,"DOORS(Supply and Install)"]
[{"$nulls":3},"all doors including cabin hooks,rubber stops,door frames"]
[{"$nulls":3},"finishings and locks"]
[]
["5.2.1",null,null,"Standard 2032x813x44mm framed battern meranti door","no",7]
[{"$nulls":3},"including pressed metal frame to still230 wall,including applicable"]
[{"$nulls":3},"pictograms (D1 AND D2)Rate to include 2coats of varnish,"]
["5.2.2",null,null,"Standard 2032x1613x44mm framed battern merant door ","no",2]
[{"$nulls":3},"including pressed metal frame to still 230 wall,including "]
[{"$nulls":3},"applicable pictogram (D1 AND D2)Rate to include 2coats of "]
[{"$nulls":3},"varnish."]
[]
[5.3,null,null,"Ceiling"]
[]
["5.3.1",null,null,"Supply and install 6.4mm GYPSUM CEILING BOARD to halls","m²",108]
[{"$nulls":3},"including 38x38 brandering and painting"]
[]
["5.3.2",null,null,"Supply and install 19x50mm PLANNED S.A PINE CORNICE:","m",40]
[{"$nulls":3},"Paint as for Ceiling "]
["5.3.3"]
[]
["Total Carried Forward to summary"]
[]
[null,"ITEM NO","PAYMENT ","DESCRIPTION","UNIT","QUANTITY","Rate","Amount"]
[]
[null,6,null,"RENOVATIONS TO EXISTING BUILDING"]
[{"$nulls":3},"SECTION 6: IRONMONONGERY"]
[{"$nulls":3},"PREAMBLE"]
[{"$nulls":3},"For Trade Preamble refer to \"Department of public works : Specification of materials and methods to be used -PW371\""]
[]
[{"$nulls":3},"SUPPLEMENTARY PREAMBLE"]
[{"$nulls":3},"Items material or methods to be specified by trade names or caralogue number only an indication  of the quality"]
[{"$nulls":3},",  item material or methods of similar quality may be used with prio approval from the project lender"]
[null,6.1,null,"HINGES,BOLTS CATCHE, CABIN HOOK ECT"]
[{"$nulls":3},"LOCKS"]
[null,"6.1.1",null,"Three lever mortice locksel","No",6]
[{"$nulls":3},"Door latching (Toilets)","No",14]
[null,6.2,null,"HINGES "]
[null,"6.2.1",null,"100X 75 mm two  bolt bearings bruss butt hinges or similer","No",9]
[]
[null,"Total Carried Forward to summary"]
[]
[]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[{"$nulls":3},"RENOVATION TO EXISTING BUILDING"]
[null,7,"PS10","SECTION 7:PAINTWORK"]
[]
[null,null,"PB1"]
[{"$nulls":3},"PREVIOUSLY PAINTED WALLS are to be throughly"]
[{"$nulls":3},"prepared,seal cracks,etc prior to moving new paint."]
[{"$nulls":3},"Colour to be agreed upon on site"]
[null,7.1,null,"High qualityPure Acrylic emusion with a fully Washable"]
[{"$nulls":3},"Medium Sheen Finish with anti-microhial additive"]
[null,"7.1.1",null,"On internal and External walls","m²",485]
[{"$nulls":3},"Hall internall walls, Toilet Extenal walls and internal walls"]
[null,7.2,null,"ON PREVIUOSLY PAINTED CEILINGS"]
[{"$nulls":3},"Clean and fix Existing Ceiling and prepare for skimming,"]
[{"$nulls":3},"apply 3-6mm coat of Rhinolite as per Manufactures"]
[{"$nulls":3},"instruction Two coats \"plascom Super Acrylic PVA"]
[{"$nulls":3},"(EPL)paint"]
[null,"7.2.1",null,"On Ceilings","m²",108]
[]
[null,7.3,null,"PAINTWORK ON WOOD"]
[]
[{"$nulls":3},"One coat base primer  and two coats internal quality"]
[null,"7.3.1",null,"Paint Prepare and apply paint on single doors ","No",11]
[]
[null,7.4,null,"Scrap down Varnish Repair and make good door and "]
[{"$nulls":3},"frame and prepair to Re-Varnish."]
[null,"7.4.1",null,"Prepair and apply paint on double doors ","No",4]
[]
[null,"7.5.1",null,"Scrap down Varnish Repair and make Window frame "]
[{"$nulls":3},"frame and prepair to Re-Varnish."]
[{"$nulls":3},"Prepair and apply paint on window frames (Toilets)","no ",7]
[null,"Total Carried Forward"]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,8,null,"SECTION 8:BATHROOM FITTINGS"]
[]
[null,"8.1.1",null,"Stainless steel toilet roll holder plugged to wall","No",7]
[{"$nulls":3},"Hand Rail for paraplegic 2pc","No",1]
[null,"Total Carried Forward"]
[]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,9,null,"SECTION9:SECURITY FENCING"]
[]
[null,"9.1.1",null,"Pepair and Fix two panel of fencing","No",2]
[null,"9.1.2",null," Weatherproof Padlock and chain( to be approved by client)"]
[null,"Total Carried Forward",{"$nulls":3},1]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,10,null,"SECTION10:STORMWATER PIPE"]
[]
[null,"10.1.1",null,"Supply and install 110mm vent pipe","No",3]
[null,"10.1.2",null,"Remove and replace fascia board on toilet","m",30]
[null,"Total Carried Forward"]
[]
[{"$nulls":3},"NOMANGESI MALUNGA COMMUNITY HALL-RENOVATION",{"$nulls":3},"WARD 18"]
[]
[{"$nulls":3},"SUMMARY PAGE"]
[]
[null,null,1,"SECTON1:PRELIMINARY AND GENERAL"]
[null,null,2,"SECTION2:REMOVAL OF EXISTING WORK"]
[null,null,3,"SECTION3: EXCAVATION AND CONCRETE"]
[null,null,4,"CRACKS AND LINKS"]
[null,null,5,"SECTION4:WINDOWS, DOORS AND CEILING"]
[null,null,6,"SECTION5:IRONMONGERY"]
[null,null,7,"SECTION6:PAINTWORK"]
[null,null,8,"SECTION7:BATHROOM FITTINGS"]
[null,null,9,"SECTION8:SECURITY FENCING"]
[null,null,10,"SECTION8:STORMWATER PIPE"]
[]
[{"$nulls":3},"Sub-Total  "]
[{"$nulls":3},"Add Contingencies"]
[{"$nulls":3},"Sub - Total A"]
[]
[{"$nulls":3},"Sub-Total  B"]
[{"$nulls":3},"Vat 15%"]
[]
[{"$nulls":3},"GRAND TOTAL"]