{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["ExportTenderItemQu"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"ExportTenderItemQu","index":0,"n_rows":114,"n_cols":12,"rows_kept":114}
["SectionNo","PartCode","ItemNo","Clause","Unit","LongDescr","MaterialFlag","EstimatedRate","EstimatedQty","Value","AdditionalItemFlag","UniqueItemNo"]
[1,"AA",1,"GCC 2015","sum","GENERAL CONDITIONS OF CONTRACT (GCC 2015) READ IN CONJUNCTION WITH THE CONTRACT DATA Fixed Charge obligations",null,0,1,0,null,2669]
[1,"AA",2,"GCC 2015","sum","Time Related obligations",null,0,1,0,null,2670]
[1,"AA",3,"C1.2.3.1","PC Sum","COMMUNITY LIAISON OFFICER.Allow or a CLO to be appointed. (Rate x 8 hrs x 5days x 52 weeks)",null,1,160000,0,null,2671]
[1,"AA",4,"C1.2.3.1","%","% Mark-up for item 3 above",null,0,160000,0,null,2672]
[1,"AA",5,"C1.2.3.2","sum","LOCAL LABOUR Allow for the monthly submission of proof\r\nof employment of local labour",null,0,1,0,null,2673]
[1,"AB",1,"AB.4","sum","Set up contractor's Camp Site / Store yard",null,0,1,0,null,2674]
[1,"AB",2,"AB.5","sum","Supply and erect Contract Notice Board",null,0,1,0,null,2675]
[1,"AB",3,"AB.7","sum","Initial supply of all signs, barricades and delineators",null,0,1,0,null,2676]
[1,"AB",4,"AB.7","sum","Maintenance of all signs, barricades and delineators",null,0,1,0,null,2677]
[1,"AB",5,"PS AB 8","sum","Survey coordination of existing valves, manholes, catchpits,cable duct markers and set out of project on site.",null,0,1,0,null,2678]
[1,"AB",6,"PS AB 9","sum","Survey for 'As-Built' Drawings on completion",null,0,1,0,null,2679]
[1,"AB",7,"PS.11","sum","Site security",null,0,1,0,null,2680]
[1,"AH",1,"AH.14.1","sum","Contractor's initial obligations in respect of the Occupational Health and Safety Act and Construction Regulations",null,0,1,0,null,2681]
[1,"AH",2,"AH.14.2","sum","Contractor's time related obligations in respect of the Occupational Health and Safety Act and Construction Regulations",null,0,1,0,null,2682]
[1,"AH",3,"AH.14.3","sum","Submission of the Health and Safety File",null,0,1,0,null,2683]
[1,"AB",8,"PS.2.3","sum","The contractor is to construct and\r\nremove on completition, any temporary\r\naccesses he may require for his plant,\r\nequipment and materials. This may\r\nconsist of widening and reinstating\r\naccesses as well as the repair of any\r\ndamage.",null,0,1,0,null,2713]
[1,"AB",9,null,"sum","Allow for the following Additional Items which the tenderer requires to be priced separately :-\r\n\r\na)",null,0,1,0,null,2715]
[1,"AB",10,null,"sum","b)",null,0,1,0,null,2716]
[1,"AB",11,null,"sum","c)",null,0,1,0,null,2717]
[1,"AB",12,"PS.AB.10","PC Sum","Allow for Progress Photographs\r\n(Provisional)\r\n(Provisional Sum)",null,1,5000,0,null,2718]
[1,"AB",13,"PS.AB.8","sum","Initial supply of plant, materials, labour\r\nand services required by the contractor",null,0,1,0,null,2719]
[1,"AB",14,"PS.AB.13.1","PC Sum","Supply and Install of prefabricated homes for temporary housing of Informal settlement residnences and supply of material packs for rebuilding",null,1,3000000,0,null,2788]
[1,"AB",15,"PS.AB.13.2","PC Sum","Appointment of Consultant to facilitate temporary housing relocation and settlement transitions",null,1,900000,0,null,2791]
[1,"AB",16,"PS.AB.14.1","PC Sum","Appointment of Environmental Control Officer",null,1,65000,0,null,2793]
[2,"B",1,"AA.B.[.]","m","Removal of 2 m high precast concrete palasade fence and store on site for re-use",null,0,20,0,null,2699]
[2,"B",2,"B.8.5","m","Removal of 1.6 m high wire mesh fence and store on site for re-use",null,0,10,0,null,2701]
[2,"B",3,"B.8.15","m3","Removal of asphalt sidewalks/medians to tip",null,0,150,0,null,2703]
[2,"B",4,"B.8.9","m3","Removal of brickwork to tip",null,0,60,0,null,2704]
[2,"B",5,"B.8.10","m3","Removal of unreinforced concrete",null,0,50,0,null,2705]
[2,"B",6,"B.8.11","m3","Removal of reinforced concrete",null,0,50,0,null,2706]
[2,"B",7,"B.8.2","m2","General clearance and grubbing in private property",null,0,300,0,null,2707]
[2,"B",8,"B.8.15","m2","Removal of interlocking blocks in paved areas to tip",null,0,25,0,null,2708]
[2,"B",9,"PS.B.22","m2","Removal and clearing of informal settlement debris within culvert route to tip",null,0,1500,0,null,2710]
[2,"B",10,"B.8.14","m3","Removal of roadways to tip",null,0,20,0,null,2711]
[2,"B",11,"PS.B.10","sum","Removal of Corridor Shelter on culvert route to store on site and re-use",null,0,1,0,null,2776]
[2,"B",12,"PS.A.5","m","Removal of Steel Emergency Water Conduit to store on site and re use",null,0,20,0,null,2777]
[2,"B",13,"B.8.19","m","Removal of disused pipes, 300 - 500 mm diameter and spoil at tip. Rate to include all haulage",null,0,10,0,null,2789]
[2,"B",14,"B.8.19","m","Removal of disused pipes, 500 - 800 mm diameter and spoil at tip. Rate to include all haulage",null,0,10,0,null,2790]
[2,"B",15,"PS.B.11","no.","Support existing services across culvert route excavation",null,0,10,0,null,2794]
[2,"B",16,"PS.B.10","PC Sum","Removal of solar panel structure on culvert route to store on site and re-use",null,1,150000,0,null,2836]
[2,"B",17,"B.8.4","no.","Removal of trees of girth exceeding 1,5 m",null,0,10,0,null,2837]
[2,"B",18,"B.8.6","PC Sum","Removal of camera concrete post and store on site for re-use",null,1,3000,0,null,2838]
[3,"C",1,"C.8.1 / PS.C.5","m2","Grade 15/19 concrete blinding of thickness 75 mm",null,0,1800,0,null,1130]
[3,"C",2,"C.8.1 / PS.C.4","m3","Supply and Cast Grade 40/19 concrete in culvert base slab (up to C.J. level, including haunches)",null,0,360,0,null,1131]
[3,"C",3,"C.8.1 / PS.C.4","m3","Supply and Cast Grade 40/19 concrete in walls (up to C.J. at roof slab)",null,0,50,0,null,1132]
[3,"C",4,"C.8.1 / PS.C.4","m3","Supply and Cast Grade 40/19 concrete in roof slab",null,0,25,0,null,1133]
[3,"C",5,"C.8.2 / PS.C.1","t","Galvanised Mild steel reinforcement",null,0,10,0,null,1134]
[3,"C",6,"C.8.2 / PS.C.1","t","Galvenised High tensile steel reinforcement",null,0,45,0,null,1135]
[3,"C",7,"C.8.3","m2","Class 1 vertical shuttering for culvert  floor slabs (up to C.J.)",null,0,400,0,null,1136]
[3,"C",8,"C.5.14 / PS.C.5.4","m2","Class 3a vertical shuttering to exposed walls",null,0,105,0,null,1137]
[3,"C",10,"C.8.3","m2","Class 3a horizontal shuttering to soffit of roof slab",null,0,105,0,null,1138]
[3,"C",11,"C.8.3","m2","Class 1 vertical shuttering to edge of roof slab",null,0,100,0,null,1139]
[3,"C",12,"C.8.3","m2","Class 1 vertical shuttering to construction joints (C.J.)",null,0,82,0,null,1140]
[3,"DD",1,"DD.8.2 / PS.DD.1/ PS.DD.2","m3","Excavate in all material for culvert to tip",null,0,3600,0,null,1645]
[3,"DD",2,"DD.8.2 / PS.DD.1/ PS.DD.2","m3","Excavate in all material for culvert to stockpile and reuse",null,0,2400,0,null,2122]
[3,"DD",3,"DD.8.2","m3","Extra over items 1 and 2 for hard material",null,0,10,0,null,2124]
[3,"DD",4,"DD.8.2","m3","Extra over items 1 and 2 for rock",null,0,5,0,null,2125]
[3,"DD",5,"PS.DD.9","sum","cofferdamming and dewatering",null,0,1,0,null,2130]
[3,"DD",6,"DD.8.5","m3","Backfill and compact using imported material 19mm stone from contractor's own source. Rate to include all haulage and royalties (Provisional)",null,0,525,0,null,2647]
[3,"DD",7,"DD.8.3","m3","Backfill and compact using material from stockpile",null,0,2400,0,null,2656]
[3,"C",9,"C.5.14 / PS.C.5.4","m2","Class 1 vertical shuttering to un-exposed (earth face) walls",null,0,150,0,null,2660]
[3,"C",16,"PG.8.7","m","Supply and installation Standard precast Rectangular concrete portal culvert Class 75S - 3000 x 1200 mm  See Drawing Enclosed",null,0,120,0,null,2746]
[3,"C",14,"C.8.1/PS.C.5.4","m2","Class 3 concrete upper surface finish (wood float)",null,0,250,0,null,2749]
[3,"C",17,"C.8.2","m2","Supply and install Hot Dipped Galvanised BRC Messhing (8mm)",null,0,1350,0,null,2769]
[3,"C",18,"C.8.2","m","Supply drill and dowel, Galvanised High Tensile Steel Reinforcement Y20 with min 300mm grouting in standup base",null,0,240,0,null,2771]
[3,"PG",1,"PJ.5.1/PS.PJ.9","sum","Pipe jacking establishment and disestablishment on site",null,0,1,0,null,2780]
[3,"PG",2,"PJ.5.2","m","Supply of concrete pipes to be jacked  of ID500 Class 100DRC Pipes",null,0,200,0,null,2781]
[3,"PG",3,"PG.5.3","m","Supply and Install of Concrete Jacking pipes  ID500 Class 100D RC including interjack stations",null,0,200,0,null,2783]
[3,"PG",4,"PJ.4.1","no.","Interjack stations",null,0,5,0,null,2784]
[3,"PG",5,"DB.8.5","m3","Extra-over for excavation through soft sand",null,0,100,0,null,2785]
[3,"PG",6,"DB.8.5","m3","Extra-over for excavation through rock",null,0,100,0,null,2786]
[3,"C",15,"PG.8.7","m","Supply and installation Standard precast Rectangular concrete portal culvert Class 75S - 3000 x 1800 mm  See Drawing Enclosed",null,0,500,0,null,2792]
[3,"C",19,"C.8.3 / PS.C.9","m2","Class 3a vertical shuttering to un-exposed (earth face) base slab",null,0,350,0,null,2795]
[3,"DD",8,"PG.8.12.1/PS.DD.4","m2","Supply and Lay  Geofabric Grade 10 to wrap around stone bedding (provisional)",null,0,2200,0,null,2797]
[3,"C",20,"C.8.3/ PS.C.9","m2","Class 3a vertical shuttering to exposed walls of pipe encasement (including haunches)",null,0,250,0,null,2799]
[3,"C",21,"C.8.3","m2","Class 3a horizontal shuttering to soffit of pipe encasement slab",null,0,300,0,null,2800]
[3,"C",22,"C.8.1 / PS.C.4","m3","Supply and Cast Grade 40/19 concrete in pipe encasement (including haunches)",null,0,350,0,null,2802]
[3,"C",23,"PS.C.5.4","m2","Class 3a concrete upper surface finish of pipe encasement (Steel float)",null,0,300,0,null,2804]
[3,"C",24,"C.8.2","m2","Steel mesh reinforcement  Ref 193 for pipe encasement",null,0,960,0,null,2805]
[3,"C",13,"C.8.1/PS.C.5.4","m2","Class 4 concrete base surface finish (Steel float)",null,0,2100,0,null,2825]
[3,"C",25,"PS.C.8.5","m","Bitumastic sealant and Geo-textile wrap to joints",null,0,3800,0,null,2826]
[3,"DD",9,"DB.8.9","m3","Prove existing  services by hand excavasion (provisional), where depth is:-- Over 0,0m and not exceeding 1.5m",null,0,50,0,null,2827]
[3,"DD",10,"DB.8.9","m3","Prove existing  services by hand excavasion (provisional), where depth is:-- Over 1,5m and not exceeding 2.0m",null,0,20,0,null,2828]
[3,"C",26,"PS.C.8.4","m2","Bitumastic impregnated soft board for expansion joints",null,0,25,0,null,2831]
[4,"J",1,"J.8.1","sum","Establish bored piling equipment on site",null,0,1,0,null,2735]
[4,"J",3,"J.8.5","m","Construct 400mm diameter CFA piles -\r\nStraight Piles",null,0,30,0,null,2737]
[4,"J",4,"J.8.13","no.","Integrity testing of piles",null,0,10,0,null,2739]
[4,"J",5,"J.8.9","t","Galvanised high tensile steel reinforcement",null,0,1.2,0,null,2743]
[4,"J",6,"J.8.12","no.","Strip head of  400 mm diameter cast in-situ pile",null,0,6,0,null,2744]
[4,"J",2,"J.8.1","sum","Destablish of piling equipment on site",null,0,1,0,null,2766]
[5,"F",1,"PS.F.8.9","PC Sum","(Provisional) Dune Rehabilitation",null,1,20000,0,null,2692]
[5,"F",2,"PS.F.8.10","PC Sum","Supply and install PVC Trash Trap net system at Culvert Entry Point",null,1,6000,0,null,2754]
[6,"PG",1,"PG.8.2","m","Supply and Lay 1500 mm diameter concrete Class 100D Ogee Pipes on concrete plinth",null,0,150,0,null,2747]
[6,"PG",2,"PG.8.2","m","500 mm diameter HDPE 4kn\\m2 strength or stronger structured wall pipe Spigot and Socket",null,0,60,0,null,2806]
[6,"DB",1,"DB.8.5","m","Excavate and backfill in all material where depth is:- - Over 0,0 m and not exceeding 1,5 m",null,0,60,0,null,2807]
[6,"DB",2,"DB.8.10","m","Placing and compacting of flexible pipe bedding for 500 mm dia. pipe",null,0,60,0,null,2808]
[6,"PG",3,"PG.8.2","m","300 mm diameter HDPE 4kn\\m2 strength or stronger structured wall pipe Spigot and Socket",null,0,30,0,null,2809]
[6,"PH",1,"PH.8.2","no.","Manhole type A with light duty concrete cover. Depth :- - Over 0,0 m and not exceeding 1,5 m",null,0,8,0,null,2810]
[6,"DB",3,"DB.8.10","m","Placing and compacting of flexible pipe bedding for 300 mm dia. pipe",null,0,30,0,null,2815]
[6,"DB",4,"DB.8.9","m3","Provision of selected fill for pipe bedding from a commercial or off- site source",null,0,15,0,null,2817]
[6,"PH",2,"PS.PH.8.2","no.","Manhole type A with light duty concrete cover. Depth :- - Over 0,0 m and not exceeding 1,5 m  to be situted installed over cast insitu culvert",null,0,10,0,null,2833]
[6,"PH",3,"PS.PH.8.3","no.","Break into existing concrete manhole/culvert wall for [400 - 600] mm diameter pipe and make good",null,0,6,0,null,2834]
[7,"S",2,"S.8.1","m2","Reinstatement of ground surface",null,0,30,0,null,2697]
[7,"S",3,"S.8.4","m","Reinstatement of 2 m high precast concrete palasade fence",null,0,20,0,null,2757]
[7,"S",4,"S.8.2","m2","Reinstatement of asphalt sidewalk 25mm- Asphalt Private Plant","S202",0,150,0,null,2760]
[7,"S",5,"S.8.2","m2","Reinstatement of paved areas - brick paving",null,0,25,0,null,2761]
[7,"S",6,"S.8.4","m2","Reinstatement of brick retaining walls. Thickness 230 mm",null,0,40,0,null,2762]
[7,"S",7,"S.8.4","m","Reinstatement of wire or plastic coated mesh fence, 1,6 m high",null,0,10,0,null,2763]
[7,"S",8,"S.8.2","m2","Permanent road reinstatement 150 mm sub base 100 mm Asphalt - Asphalt Private Plant","S206",0,60,0,null,2767]
[7,"S",9,"PS.S.8.6","sum","Reinstatement of Corridor Shelter on culvert route",null,0,1,0,null,2819]
[7,"S",10,"PS.S.8.7","m","Reinstatement of Steel Emergency Water Conduit",null,0,20,0,null,2820]
[7,"S",1,"PS.S.10","PC Sum","Reinstatement of solar panel structure above culvert route",null,1,150000,0,null,2839]
[7,"S",11,"PS.S.8.6","PC Sum","Reinstatement of camera concrete post",null,1,5000,0,null,2840]