{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"merged":[[0,0,1,4],[2,0,2,4]]}
["OFFICE STANDARDS -  CEC"]
[]
["09.2023  v00"]
["OFFICE SIZE AND FURNITURE ALLOCATION PER DESIGNATION"]
["ITEM","DESIGNATION","Approximate AREA SIZE","Walls/Screens","FURNITURE"]
[1.1,"CEC Manager/Team Lead","30m² Fully enclosed and lockable","Full height dry wall with full height semi-solid door and 900mm wide vertical view panel adjacent. \nPainted walls.\n75mm high natural aluminium skirting all round \n1 x Accent wall \nStandard carpet tiles","Managerial Desk with fitted roller door pedenza in white HPL\nModesty panel\nFully upholstered high back chair\n2 x mesh back visitor’s chair with leather seat OR\n1 200mm Bamboo vertical veneer or similar approved circular meeting table with\n4 x mesh-back meeting chair with leather seat\n1 x Swing door OR silver roller door cupboard in White HPL OR\n  b. 2 x Roller door credenza in White HPL\nFrost-free standard white single door refrigerator without freezer compartment\nSteel silver powder coated round tapered wastepaper bin"]
[1.2,"All other grades","7,80m² per person Open plan","Open plan office area with deskes banked together to optimize floor space. \nFull height dry wall with full height semi-solid door and 900mm wide vertical view panel adjacent. \nPainted walls.\n75mm high natural aluminium skirting all round \n1 x Accent wall \nStandard carpet tiles","Standard Workstation in white HPL\n500mm high Desk based screens – fabric covered\nMobile pedestal in white HPL\nModesty panel in solitary applications\nMesh-back high back operator's chair with upholstered seat\nSteel silver powder coated round tapered wastepaper bin"]
[1.3,"All Front Office applications/Receptions - serving public","8,50m² Open plan per person but enclosed and proxied overall to prevent public from accessing back of counter and entering offices beyond.  Lockable door with vertical view panel to close off area behind counter.\nOverall : 60m²","Open plan.\nALL perimeter walls to stretch to underside of soffit.\nDry wall partitions between 2 workstations set up side by side.\nFull height dry wall with full height semi-solid doors and 900mm wide vertical view panels adjacent. \nPainted walls.\n75mm high natural aluminium skirting all round \n1 x Accent wallpapered wall \nStandard Carpet tiles behind counter, \nCommercial quality full bodied porcelain floor tiles with 1mm grout in Reception, passages, toilets (if applicable) and high traffic areas.  ","Workstation with extra depth top (custom-made) in White HPL\n1500mm high fabric covered screens between\nMobile pedestal in White HPL per person.\nModesty panel per desk.\nMesh-back high back operator's chair with upholstered seat\nSteel silver powder coated round tapered wastepaper bin\n2 x Mesh-back Visitor's Chairs with upholstered seat per cubicle/person"]
[]
[{"v":2,"d":"2.00"},"ANCILLARY AREAS"]
["ITEM","ROOM TYPE","Approximate AREA SIZE","Walls/Screens","FURNITURE"]
[2.1,"Meeting Room\n8 - 10 Persons","20m² Fully enclosed and lockable","Full height dry wall with full height semi-solid door and 900mm wide vertical view panel adjacent. \nPainted walls.\n75mm high natural aluminium skirting all round \n1 x Accent wallpapered wall \nStandard carpet tiles","Rectangular table in Bamboo vertical veneer or similar approved\n8 - 10 x Meeting chairs upholstered in fabric\nWhiteboard on 1 wall"]
[2.4,"Pause Area","20m² Partially enclosed and highly visible and well lit and ventilated. Walls and portions of walls that are not tiled, to be painted.","Open Plan – semi-closed off or fully enclosed with glazing to contain noise. Must operate on negative pressure to eliminate and prevent food smells permeating office areas. \nGlued down fully flexible vinyl timber trip flooring with 75mm natural aluminium skirting all round.\nFloor unit with doors and drawers - lockable in white HPL frontals with SS Prep bowl.  75mm high aluminium skirting all round floor unit to protect unit from water seepage and damage.\nBlack Zimbabwe or Belfast Granite worktop and 100mm backsplash to span entire length of counter top.\nRunning hot and cold water at prep bowl with single mixer.\nSplash back extra over : 3 rows of 200 x 200mm white ceramic wall tiles above granite splash-back. To span full length of counter top.\nHydroboil over SS prep bowl (for overflow) for drinking purposes (beverages, etc.)\nWater dispenser or filtration system coupled to potable water supply for drinking.\nKitchen type swing bin built in to floor unit.","Washable and durable floor finish e.g. vinyl plank glue down system.\nBlack Zimbabwe or Belfast Granite worktop and 100mm backsplash to span entire length of counter top.\nFloor unit with doors and drawers - lockable in white HPL frontals with SS Prep bowl.  75mm high aluminium skirting all round floor unit to protect unit from water seepage and damage.\nHot and cold water.\nSplash back extra over : 3 rows of 200 x 200mm white ceramic tiles above granite splash-back. To span full length of counter top.\nFrost-free standard white fridge without freezer compartment.\nMicrowave Oven.\nHydroboil over SS prep bowl (for overflow) for drinking purposes (beverages, etc.)\nWater dispenser or filtration system coupled to potable water supply for drinking.\nKitchen type swing bin - preferably hidden.\n900 x 900mm Square Stainless Steel tables on centre mounted aluminium pedestal.\n4 x plastic chairs  in blue, green, white, black or grey with polished steel frame per table - multiples of 4."]
[2.5,"Store Rooms and Filing Rooms","20m² Fully enclosed and lockable","Full height (to underside of soffit) fire proof dry wall with fire proof door wide enough for easy passage of trolleys. No external windows permissible.\nWalls painted on the inside. \nFloor finish - sealed screed or grey stoep paint to screed.\nWell lit all over so that files/goods can be retrieved with ease.\nSome means of fire detection and fire extinguishing.\nAir-conditioned and well ventilated.\nAccess controlled.","Walls painted on the inside. \nFloor finish - sealed screed or grey stoep paint to screed.\nWell lit all over so that files/goods can be retrieved with ease.\nSome means of fire detection and fire extinguishing.\nAir-conditioned and well ventilated.\nAccess controlled."]
[2.6,"ICT Hub & Server Rooms","12m² Fully enclosed and lockable","Full height (to underside of soffit) fire proof dry wall with fire proof door.  No external windows permissible.\nWalls painted on the inside. \nFloor finish - sealed screed or grey stoep paint to screed.\nSome means of fire detection and fire extinguishing.\nAccess controlled.\nSeparate Air-conditioning connected to back-up power supply to keep equipment cool.\nWell lit all over.","Walls painted on the inside. \nFloor finish - sealed screed or grey stoep paint to screed.\nSome means of fire detection and fire extinguishing.\nAccess controlled.\nSeparate Air-conditioning connected to back-up power supply to keep equipment cool.\nWell lit all over."]