{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Cover1","Price Schedule"],"not_rendered":{"images":1,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Cover1","index":0,"n_rows":40,"n_cols":8,"rows_kept":40}
[" "]
{"$rows_empty":8}
[{"$nulls":5},"ENGINEERING AND CONSTRUCTION"]
["  "]
[{"$nulls":5},"30th JULY 2023"]
{"$rows_empty":15}
["CONTRACT NUMBER",{"$nulls":6},": "]
[]
[]
[]
["CONTRACTOR",{"$nulls":6},":"]
[]
[]
["CONTRACT AMOUNT ",{"$nulls":6},":"]
["(Excluding VAT)"]
[]
[]
[]
[{"$nulls":5},"PART 1 of 2"]

{"sheet":"Price Schedule","index":1,"n_rows":70,"n_cols":6,"rows_kept":70}
[null,null,"UOM","QUANTITY","RATE","AMOUNT"]
[null,"PRICE LIST"]
[]
[null,"Supplementary Preambles"]
[]
[null,"Price must include all related expenses, i.e. transport, accommodation etc"]
[]
[null,"For all the  trucks mentioned below, a minimum of two earthing balls must be permanently installed / bonded on to the chassis of the vehicle to facilitate the earth electrode and equipotential footpate / mat"]
[]
[null,"Trucks are to be rented on an ad hoc basis for a period of three(3) years and must be available on short notice (within 24 hours)"]
[]
[null,"Price must include all related expenses, i.e. transport, accommodation etc."]
[]
[null,"Functional Specification"]
[]
[null,"The trucks will be used for the following by the various Business Units across the East Grid:"]
[]
[null,"Transportation of equipment to and from various substations and Eskom Stores in Simmerpan / where needed within SA."]
[]
[null,"For assisting in perfoming tasks within the substation during outages of various\nkinds,"]
[]
[null,"Transporting may include some of the following"]
[]
[null,"1) 5 to 10ton cable drums."]
[]
[null,"2) Wooden Poles"]
[]
[null,"3) Concrete slabs"]
[]
[null,"4) 6m Containers"]
[]
[null,"5) CTs, VTs, Breakes, etc"]
[]
[null,"6) Oil tanks, tools, etc"]
[]
[null,"Stringing conductor and pilot cable"]
[]
[null,"Dressing of poles"]
[]
[null,"Lifting of tower sections"]
[]
[null,"PLANT SPECIFICATIONS"]
[]
[null,"Crane Specification:"]
[]
[null,"Cranes must have an interchangeable certified head attachment to fit hooks and or man baskets. All crane trucks must have earth plates as a permanent fixture to the truck."]
[]
[null,"Crane"]
[]
[1,"Specialized crane with 22/25m reach to erect and dressing of overhead lines","Day",548]
[]
[2,"Specialized crane with 20/24 ton/meter to lift heavy cable drums","Day",548]
[]
[3,"Specialized crane with 15 to 18 ton/meter to move containers and general heavy goods","Day",548]
[]
[null,"Trucks","Day",548]
[]
[4,"10-13Ton 6x2 / 6X4 / 6x6 Truck Min Engine capacity off 184Kw with 6.1M drop sides and container locks with 20Ton/m to 23Ton/m with Min 4 Ext. behind cab mounted crane","Day",548]
[]
[5,"6x6 Trucks – 12 to 14Ton with minimum 6.1m load body with container locks and turf hooks and mounted cranes. Crane to be mounted behind cap will be preferable.","Day",548]
[]
[6,"Truck with 20 - 24Ton/m crane with 4- 5Ext. mounted behind the cab complete with 12M flat deck trailer with container locks and up rights with a minimum loading capacity of 25Tons","Day",548]
[]
[7,"Sky Jack","Day",548]
[]
[null,"SUBTOTAL"]
[]
[null,"VAT @ 15%"]
[]
[null,"TOTAL AMOUNT INCLUSIVE OF VAT"]