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Part 4: Site Information
Core clause 11.2(16) states 
“Site Information is information which
· describes the Site and its surroundings and

· is in the documents which the Contract Data states it is in.”
In Contract Data, reference has been made to this Part 4 of the contract for the location of Site Information.
1. General description

	Site


:
	Kusile Power Station

	Regional Authority
:
	Emalahleni Local Municipality, Mpumalanga Province

	Nearest Towns
:
	Emalahleni – 42km north east of power station

Bronkhorstspruit – 41km south of power station

Delmas – 45km north of power station

There are informal settlements within a 10 km radius of the power station.

	Infrastructure

:
	Kusile Power Station is situated approximately 3km from the N4 highway and is connected to it by means of a tarred road. There is also a secondary tarred road connecting the site with the R545 and D686. 

	Latitude & longitude
:
	

	Landowner

:
	Portions of Horingkraans Farm 

	River catchment
:
	Wilge River

	Regional Climate
	Kusile Power Station is situated in the Mpumalanga Province on the Highveld in the western part of Mpumalanga province on the escarpment, at an average height of 1551 m above sea level.  The winters are generally dry and cold with regular frost and temperatures varying between -7ºC and 23ºC.

The summers are mild with most of the rainfall occurring during this season. Temperatures vary between 12º & 32º C.

	Wind direction
	Data from the Emalahleni weather station shows that Kusile Power Station is sited in such a way that for most of the year (291 days) the wind direction is from the power station in a direction that is North West. 

	Rainfall
	Based on information recorded at the Emalahleni weather station, the average annual rainfall for the Emalahleni area is approximately 691 mm. (Weather Bureau, Pretoria). 


2. Existing buildings, structures, and plant & machinery on the Site
· The Contractor will be required to work with others with whom the Contractor may be required to share the Affected Property. 
· Requirements for liaison with and acceptance from statutory authorities or inspection agencies will be communicated when required
· Any risk arises due to buildings, structures, and plant & machinery on the Site to be communicated with the project manager prior to work commencement.
3. Subsoil information
Not Applicable

4. Hidden services 

Not Applicable

5. Other reports and publicly available information

Not Applicable
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