Soil ripper specification

* Five-point ripper
* Tractor mounted
* Universal three-point linkage system, for easy transportation
* V-frame constructed

 200mm x 150mm x 10mm boxed channel.