{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Kiosk","AIS Combo"],"read":"whole","date_system":"1900"}

{"sheet":"Kiosk","index":0,"n_rows":36,"n_cols":13,"rows_kept":36,"merged":[[0,1,0,12],[1,1,1,12],[3,5,26,11],[35,1,35,2]]}
[null,"MV Outdoor Circuit Breakers forecast over a period of three (4) years"]
[null,"KIOSK CIRCUIT BREAKERS"]
[null,"NO","DESCRIPTION","LOU","NWOU","GAU","FSOU","MOU","NCOU","ECOU","WCOU","KZNOU","QTY"]
[null,1,"BKR:KSK;11 KV;2500 A;25 KA;3;110 VDC",100,40,"nmm",{"$nulls":6},130]
[null,2,"BKR:KSK;11 KV;2500 A 25 KA;3;220 VDC",{"$nulls":9},10]
[null,3,"BKR:KSK;11 KV;2500 A;31.5 KA;3;110 VDC",null,60,{"$nulls":7},50]
[null,4,"BKR:KSK;11 KV;2500 A;31,5 KA;3;220 VDC",{"$nulls":9},10]
[null,5,"BKR:KSK;22 KV;800 A;25 KA;3;110 VDC",140,65,{"$nulls":7},{"$f":"205-80","v":125}]
[null,6,"BKR:KSK;22 KV;800 A;25 KA;3;220 VDC",30,{"$nulls":8},30]
[null,7,"BKR:KSK;22 KV;800 A;31.5 KA;3;110 VDC",18,30,{"$nulls":7},48]
[null,8,"BKR:KSK;22 KV;800 A;31,5 KA;3;220 VDC",6,{"$nulls":8},6]
[null,9,"BKR:KSK;22 KV;1250 A;25 KA;3;110 VDC",null,11,{"$nulls":7},10]
[null,10,"BKR:KSK;22 KV;1250 A;25 KA;3;220 VDC",{"$nulls":9},1]
[null,11,"BKR:KSK;LOW;22 KV;1250 A;25 KA;3;110 VDC",30,30,{"$nulls":7},50]
[null,12,"BKR:KSK;LOW;22 KV;1250 A;25 KA;3;220 VDC",{"$nulls":9},10]
[null,13,"BKR:KSK;22 KV;1250 A;31.5 KA;3;110 VDC",null,20,{"$nulls":7},15]
[null,14,"BKR:KSK;22 KV;1250 A;31,5 KA;3;220 VDC",{"$nulls":9},5]
[null,15,"BKR:KSK;22 KV;1600 A;25 KA;3;110 VDC",{"$nulls":9},10]
[null,16,"BKR:KSK;22 KV;1600 A;25 KA;3;220 VDC",null,20,{"$nulls":7},10]
[null,17,"BKR:KSK;22 KV;1600 A;31.5 KA;3;110 VDC",30,{"$nulls":8},10]
[null,18,"BKR:KSK;22 KV;1600 A;31.5 KA;3;220 VDC",null,15,{"$nulls":7},10]
[null,19,"BKR:KSK;22 KV;2500 A;25 KA;3;110 VDC",{"$nulls":9},10]
[null,20,"BKR:KSK;22 KV;2500 A;25 KA;3;220 VDC",{"$nulls":9},10]
[null,21,"BKR:KSK;22 KV;2500 A;31.5 KA;3;110 VDC",{"$nulls":9},10]
[null,22,"BKR:KSK;22 KV;2500 A;31.5 KA;3;220 VDC",{"$f":"SUM(D4:D22)","v":354},{"$f":"SUM(E4:E22)","v":291},{"$nulls":7},10]
[null,23,"BKR:KSK;33 KV;800 A;25 KA;3;110 VDC",{"$nulls":9},20]
[null,24,"BKR:KSK;33 KV;800 A;25 KA;3;220 VDC ",{"$f":"SUM(D4:D22)","v":354},{"$f":"SUM(E4:E22)","v":291},{"$nulls":7},16]
[null,25,"BKR:KSK;33 KV;1250 A;25 KA;3;110 VDC",{"$nulls":9},15]
[null,26,"BKR:KSK;33 KV;1250 A;25 KA;3;220 VDC",{"$nulls":9},2]
[null,27,"BKR:KSK;33 KV;1250 A;31.5 KA;3;110 VDC",{"$nulls":9},2]
[null,28,"BKR:KSK;33 KV;1250 A;31,5 KA;3;220 VDC",{"$nulls":9},2]
[null,29,"BKR:KSK;33 KV;1600 A;25 KA;3;110 VDC",{"$nulls":9},2]
[null,30,"BKR:KSK;33 KV;1600 A;25 KA;3;220 VDC",{"$nulls":9},2]
[null,31,"BKR:KSK;33 KV;1600 A;31.5 KA;3;110 VDC",{"$nulls":9},2]
[null,32,"BKR:KSK;33 KV;1600 A;31.5 KA;3;220V DC",{"$nulls":9},2]
[{"$nulls":12},{"$f":"SUM(M4:M35)","v":645}]

{"sheet":"AIS Combo","index":1,"n_rows":28,"n_cols":13,"rows_kept":28,"merged":[[0,1,0,12],[1,1,1,12],[2,1,2,12],[27,1,27,2]]}
[]
[null,"MV Outdoor Circuit Breakers forecast over a period of three (4) years"]
[null,"COMBO CIRCUIT BREAKERS"]
[null,1,"BKR:CMB;11 KV;2500 A;25 KA;3;110 VDC",{"$nulls":9},{"$f":"140-50","v":90}]
[null,2,"BKR:CMB;11 KV;2500 A;31.5 KA;3;110 VDC",{"$nulls":9},28]
[null,3,"BKR:CMB;11 KV;2500 A;25 KA;3;220 VDC",{"$nulls":9},20]
[null,4,"BKR:CMB;11 KV;2500 A;31.5 KA;3;220 VDC",{"$nulls":9},20]
[null,5,"BKR:CMB;22 KV;1250 A;25 KA;3;110 VDC",{"$nulls":9},{"$f":"327-160-50-50","v":67}]
[null,6,"BKR:CMB;22 KV;1250 A;25 KA;3;220 VDC",{"$nulls":9},50]
[null,7,"BKR:CMB;22 KV;1250 A;31.5 KA;3;110 VDC",{"$nulls":9},{"$f":"119-50","v":69}]
[null,8,"BKR:CMB;22 KV;1250 A;31.5 KA;3;220 VDC",{"$nulls":9},20]
[null,9,"BKR:CMB;LOW;22 KV;1250 A;25 KA;3;110 VDC",{"$nulls":9},20]
[null,10,"BKR:CMB;LOW;22 KV;1250 A;25 KA;3;220 VDC",{"$nulls":9},20]
[null,11,"BKR:CMB;22 KV;1600 A;25 KA;3;110 VDC",{"$nulls":9},20]
[null,12,"BKR:CMB;22 KV;1600 A;25 KA;3;220 VDC",{"$nulls":9},20]
[null,13,"BKR:CMB;22 KV;1600 A;31.5 KA;3;110 VDC",{"$nulls":9},20]
[null,14,"BKR:CMB;22 KV;1600 A;31.5 KA;3;220 VDC",{"$nulls":9},20]
[null,15,"BKR:CMB;22 KV;2500 A;25 KA;3;110 VDC",{"$nulls":9},20]
[null,16,"BKR:CMB;22 KV;2500 A;25 KA;3;220 VDC",{"$nulls":9},20]
[null,17,"BKR:CMB;22 KV;2500 A;31.5 KA;3;110 VDC",{"$nulls":9},{"$f":"20+40","v":60}]
[null,18,"BKR:CMB;22 KV;2500 A;31.5 KA;3;220 VDC",{"$nulls":9},{"$f":"20+60","v":80}]
[null,19,"BKR:CMB;33 KV;1600 A;31.5 KA;3;110 VDC",{"$nulls":9},63]
[null,20,"BKR:CMB;33 KV;1600 A;25 KA;3;220 VDC",{"$nulls":9},20]
[null,21,"BKR:CMB;33 KV;1600 A;31.5 KA;3;220 VDC",{"$nulls":9},40]
[null,22,"BKR:CMB;33 KV;1600 A;25 KA;3;110 VDC",{"$nulls":9},20]
[null,23,"BKR:CMB;33 KV;2500 A;31.5 KA;3;110 VDC",{"$nulls":9},{"$f":"10+60","v":70}]
[null,24,"BKR:CMB;33 KV;2500 A;31.5 KA;3;220 VDC",{"$nulls":9},{"$f":"10+50","v":60}]
[{"$nulls":12},{"$f":"SUM(M4:M27)","v":937}]