{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Summary Page","Construction","Maintenance","Sheet1"],"not_rendered":{"external_links":1,"defined_names":31,"comments":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Summary Page","index":0,"n_rows":14,"n_cols":6,"rows_kept":14,"merged":[[0,0,0,5],[3,1,3,3],[6,1,6,3],[12,3,12,4],[13,3,13,4],[16,1,16,5]],"flags":["formulas_cached_only"]}
["SUMMARY OF SCHEDULE OF RATES"]
[]
[]
[1,"CONSTRUCTION ",{"$nulls":3},0]
[]
[]
[2,"MAINTENANCE ",{"$nulls":3},0]
[]
[]
[]
[]
[]
[null,"SUB-TOTAL ",null,"excl. VAT",null,0]
[null,"TOTAL",null,"excl. VAT",null,0]

{"sheet":"Construction","index":1,"n_rows":1011,"n_cols":12,"rows_kept":1011,"merged":[[0,0,0,5],[0,6,3,6],[1008,3,1008,4],[1009,3,1009,4],[1010,3,1010,4]],"flags":["formulas_cached_only"]}
["SCHEDULE OF RATES: Public Realm Delivery,\nLandscape Infrastructure and Ancillary Works\n(TO BE READ WITH CLAUSE C3.3: STANDARDS, SPECIFICATIONS AND TECHNICAL REQUIREMENTS). All rates in the Bill of Quantities shall be deemed to include full compensation for compliance with the Contract, including but not limited to: Environmental Management Plan implementation, Community liaison and local labour obligations, Site establishment and consultant facilities, Protection of existing services and infrastructure, Monitoring, reporting and documentation requirements, No separate claims shall be entertained for these obligations. All work shall: Be executed in a professional and workmanlike manner,  Meet SALI accepted industry practices, Be subject to inspection and rejection if non-compliant The Contractor shall be responsible for: Reinstatement of defective work,  Replacement of failed planting, Compliance with environmental and safety requirements"]
["ITEM NO:","ITEM DESCRIPTION","QUANTITY","UNIT","UNIT PRICE (in Rands)","AMOUNT (in Rands)"]
[1,"MISCELLANEOUS"]
["1.1","Preliminaries and General (The Contractor shall be deemed to have included full compensation for all obligations described in this section within the tendered rates unless otherwise provided.)"]
["1.1.1","Site establishment (Establishment of site camp and facilities, Provision of secure storage, fencing and access control, Setting out and protection of benchmarks and pegs, Site reinstatement upon completion, Compliance with Scope, Specifications, Drawings and BOQ, Contractor’s pricing of all obligations under Preliminaries)",{"v":1,"d":"1.00"},"sum",null,0,{"$nulls":5},"```"]
["1.1.2","Initial Health & safety training",{"v":1,"d":"1.00"},"`",null,0]
["1.1.3","Provision of Personal Protective Clothing & Equipment ",{"v":1,"d":"1.00"},"p/p",null,0]
["1.1.4","Provision of a Health and Safety Plan",{"v":1,"d":"1.00"},"each ",null,0]
["1.1.5","Provision of a Occupational Health and Safety File",{"v":1,"d":"1.00"},"each ",null,0]
["1.1.6","Provision of an Environmental File",{"v":1,"d":"1.00"},"each ",null,0]
["1.1.7","Compliance with Environmental Management Plan (EMP)",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.8","Dust suppression and pollution control measures",{"v":1,"d":"1.00"},"month ",null,0]
["1.1.9","Waste management and disposal",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.10","Protection of vegetation and sensitive areas",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.11","Stormwater and erosion control measures",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.12","Compaction density tests in layers not exceeding 150mm thick",{"v":1,"d":"1.00"},"per test",null,0]
["1.1.13","Concrete material strength test (per Pr Eng/ or Pr L Arch request)",{"v":1,"d":"1.00"},"per test",null,0]
["1.1.14","Construction signage Notice Board",{"v":1,"d":"1.00"},"each ",null,0]
["1.1.15","Provision for site's security personnel ",{"v":1,"d":"1.00"},"month ",null,0]
["1.1.16","Site office for Employer’s Representative (fully furnished)",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.17","Provision of meeting facilities (minimum 10 persons)",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.18","Provision of power, water and communication services",{"v":1,"d":"1.00"},"sum",null,0]
["1.1.19","Provision of survey assistance and site support staff",{"v":1,"d":"1.00"},"sum",null,0]
[]
[null,"PLANT & EQUIPMENT CHARGES -  items are for variation purposes only and shall not be included within unit rates where separately measured."]
[1.2,"Machinery/ Plant/ Equipment",{"$nulls":3},0]
["1.2.1","TLB/ Excavator machine ",{"v":1,"d":"1.00"},"day",null,0]
["1.2.2","Skid steer loader",{"v":1,"d":"1.00"},"day",null,0]
["1.2.3","Rammer",{"v":1,"d":"1.00"},"day",null,0]
["1.2.4","Plate Compactor",{"v":1,"d":"1.00"},"day",null,0]
["1.2.5","Motorised grader",{"v":1,"d":"1.00"},"day",null,0]
["1.2.6","Plant Hire: Tipper trucks - Capacity",{"v":1,"d":"1.00"},"day",null,0]
["1.2.7","Walk behind vibrating rollers- Model - Bomag 60 or similar (small)",{"v":1,"d":"1.00"},"day",null,0]
["1.2.8","Concrete mixers - volume 100 litre wet (Small, towable)",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.9","Diesel compressors including hoses and tools Capacity smaller than 200 cfm (small)",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.10","Water pump Capacity bigger than 200 but smaller than 400 litre/min (medium)",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.11","5.5 KVA grinder generator",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.12","15KVA Welder generator",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.13","Bobcat type excavator",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.14","Water tankers Capacity 500 litre (small,towable)",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.15","Water tankers Capacity 8 000 litre (medium)",{"v":1,"d":"1.00"},"hour",null,0]
["1.2.16","Supply plant (equipment/ tool) fuel, operator and operate",{"v":1,"d":"1.00"},"litre",null,0]
[]
[1.3,"Project Team  -  items are for variation purposes only and shall not be included within unit rates where separately measured."]
["1.3.1","CONTRACTS MANAGER ",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.2","SITE AGENT",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.3","FOREMEN",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.4","Health and Safety Officer",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.5","Environmental Control Officer",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.6","Professional Land Surveyor (for setting-out) ",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.7","Irrigation Specialist",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.8","Professional Landscape Architect/ Manager",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.9","Professional Senior Landscape (/Architectural) Technologist",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.10","Professional Landscape (/Architectural) Technologist",{"v":1,"d":"1.00"},"hour",null,0]
["1.3.11","Professional (/Architectural)Technician",{"v":1,"d":"1.00"},"hour",null,0]
[]
[null,"LABOUR CHARGES"]
[1.4," -  items are for variation purposes only and shall not be included within unit rates where separately measured."]
["1.4.1","Skilled labour",{"v":1,"d":"1.00"},"daily",null,0]
["1.4.2","Un-skilled labourer",{"v":1,"d":"1.00"},"daily",null,0]
["1.4.3","Allow the provisional Amount for: Community Liaison Officer Salary",{"v":1,"d":"1.00"},"daily",null,0]
[]
[null,"ALL items from here onwards are to Include ALL costs in each unit rate: Labour, Plant, Materials, Overheads, and Profit"]
[2,"EARTHWORKS & TOPSOIL PREPARATION (Rates shall include: Disposal to approved sites, Protection of services, Erosion control, Stormwater management, Compliance with environmental requirements)"]
[null,"CONSTRUCTION NOTICE BOARD"]
["2.1.1","Supply and install construction notice boards to detail in the construction details",{"v":1,"d":"1.00"},"item",null,0]
[null,"CLEARING OF VEGETATION"]
["2.1.2","Clearing of vegetation - protection of all areas not affected by the works in this contract including all trees to be retained",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.3","Removal of organic plant material to a suitable landfill or compost facility after verification of quantities by the Landscape Architect. Cost to include dumping cost and transport.",{"v":1,"d":"1.00"},"m³",null,0]
["2.1.4","Transport spoil material to unspecified sites and dump (provisional)",{"v":1,"d":"1.00"},"km",null,0]
["2.1.5","Site scarifying (to a depth of 75mm), clearing, grubbing, debushing and removal off site to a nearest licensed landfill facility",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.6","Excavate by hand (using garden tools where possible) to locate and expose existing services (known and unknown)",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.7","Removal of rubble (rock, waste, debirs etc.) and disposal to the nearest appropriate registered landfill facility",{"v":1,"d":"1.00"},"m³",null,0]
["2.1.8","Demolition of an existing foundation/ wall. Reuse the demolished material as infilling material or dispose off to a licensed facility ",{"v":1,"d":"1.00"},"m³",null,0]
["2.1.9","Ex-situ soil provided by the contractor from other sources (including hauling)",{"v":1,"d":"1.00"},"m³",null,0]
["2.1.10","Excavate and prepare tree holes: Each tree hole should be a minimum of 1,5 times the size of the root ball and deep enough to match the interface level between the trunk and the roots as evident on the tree.",{"v":1,"d":"1.00"},"m³",null,0]
["2.1.11","Soil preparation for seeding: Cultivate to a depth of 150-200mm by removing waste, rubble etc and rake to achieve a desired level and smooth surface",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.12","Final Shaping: Preparation, leveling & contouring of in-situ soil. To be shaped to the correct contours to within a tolerance of plus or minus 150mm",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.13","Stormwater control and erosion protection",{"v":1,"d":"1.00"},"sum",null,0]
[]
[null,"GRADING AND SHAPING"]
["2.1.14","Grade and shappe the areas dermacated for new walkway paving, children play area, outdoor gym area, multi-courts and node areas to a depth of 300mm, allowing for stormwater run-off from paved areas and smoothing out sharp level changes.",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.15","Grading and shaping of excavated spoil to create berms on site as agreed with the Landscape Architect",{"v":1,"d":"1.00"},"m²",null,0]
["2.1.16","Berm in situ fill compacted in layers of 250mm to 90% Mod Aashto density. Total 5 layers",{"v":1,"d":"1.00"},"m²",null,0]
[]
[2.2,"Fertilizers & Soil Improvements"]
["2.2.1","Supply, deliver and apply as per supplier specifications: Slow realease planting hydrogel"]
["2.2.2","Organic slow release tree tablet",{"v":1,"d":"1.00"},"each",null,0]
[null,"Fertilizers: import and spread"]
["2.2.3","Fertilizers to all planting areas - 2:3:2 or alternative as specified by Landscape Architect",{"v":1,"d":"1.00"},"kg",null,0]
["2.2.4","Fertilizers to all lawn areas - 5:1:5 or alternative as specified by Landscape Architect",{"v":1,"d":"1.00"},"kg",null,0]
["2.2.5","Bone Meal for Trees and Plants: 50 g/tree hole and 30 g/ plant hole. To be applied to soil with a pH of less than 7 on instruction by the Landscape Architect pending the soil test results. ",{"v":1,"d":"1.00"},"kg",null,0]
[null,"Organic compost: import and spread"]
["2.2.6","Organic compost for planting areas. Compost must be made of pure plant based organics and be free of weed, seeds, harmful salts, soil, sand, animal by-products and pathogens.",{"v":1,"d":"1.00"},"m³",null,0]
[null,"Top soil: import and spread"]
["2.2.7","Screened Ex-situ Topsoil: Must be composed of 15 – 25 % clay, 10% silt and 65 – 75% sand with a minimum of 2% organic material. The soil should be free from harmful salts, weed seeds and rubble of any kind. Sample to be approved by a Landscape Architect prior to importing ",{"v":1,"d":"1.00"},"m³",null,0]
[null,"Potting soil: import and fill"]
["2.2.8","Landscape mix for potted plants & planters  certified by industry associations - 70 % well draining loamy plant medium and 30 % compost (WEED FREE) - Sample to be approved by a Landscape Architect prior to importing",{"v":1,"d":"1.00"},"m³",null,0]
[null,"Lawn dresssing: import and spread"]
["2.2.9","Top dressing of sodded lawn in layers with a maximum thickness of 10 mm, roll and neatly finish",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Mulch: import and spread"]
["2.2.10","Bark/ Organic Mulch varying in size from 25-50mm in size placed to a depth of 50-70mm in all planted areas",{"v":1,"d":"1.00"},"m³",null,0]
["2.2.11","Soil analysis tests: to establish fertility, water holding capacity and suitability of the soil on site",{"v":1,"d":"1.00"},"per test",null,0]
[null,"Tree protection and support:supply and installation"]
["2.2.12","Tree stakes: driven at least 300mm deep into soil and must be CCA treated and be appropriate size in height and not be less than 35mm in diameter. Must be tied to a tree with a tree tier or strips. ",{"v":1,"d":"1.00"},"each",null,0]
[{"$nulls":5},0]
[3,"SOFTSCAPING. Supply, delivery and planting including: Approved plant quality and size, Correct planting procedures, Staking and protection, Watering and establishment care",{"$nulls":3},0]
[3.1,"Trees (200L) - Supply and Plant",{"$nulls":3},0]
["3.1.1","Acokanthera oblongifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.2","Afrocarpus falcatus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.3","Albizia adianthifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.4","Allophylus natalensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.5","Aloidendron barberae",{"v":1,"d":"1.00"},"each",null,0]
["3.1.6","Antidesma venosum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.7","Apodytes dimidiata subsp. dimidiata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.8","Baphia  racemosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.9","Barringtonia racemose",{"v":1,"d":"1.00"},"each",null,0]
["3.1.10","Bersama lucens",{"v":1,"d":"1.00"},"each",null,0]
["3.1.11","Bolusanthus speciosus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.12","Brachylaena discolor",{"v":1,"d":"1.00"},"each",null,0]
["3.1.13","Bridelia micrantha",{"v":1,"d":"1.00"},"each",null,0]
["3.1.14","Buddleja saligna",{"v":1,"d":"1.00"},"each",null,0]
["3.1.15","Burchellia bubalina",{"v":1,"d":"1.00"},"each",null,0]
["3.1.16","Calodendrum capensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.17","Calpurnia aurea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.18","Canthium spinosum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.19","Capparis tomentosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.20","Cassine aethiopica",{"v":1,"d":"1.00"},"each",null,0]
["3.1.21","Cassine papillosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.22","Cavacoa aurea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.23","Celtis africana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.24","Chaetacme aristata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.25","Chionanthus peglerae",{"v":1,"d":"1.00"},"each",null,0]
["3.1.27","Chrysophyllum viridifolium",{"v":1,"d":"1.00"},"each",null,0]
["3.1.28","Cladostemon kirkii",{"v":1,"d":"1.00"},"each",null,0]
["3.1.29","Cleistanthus foveolatus\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.30","Cleistanthus schlechteri",{"v":1,"d":"1.00"},"each",null,0]
["3.1.31","Cola natalensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.32","Combretum erythrophyllum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.33","Combretum kraussii",{"v":1,"d":"1.00"},"each",null,0]
["3.1.34","Combretum molle",{"v":1,"d":"1.00"},"each",null,0]
["3.1.35","Commiphora harveyi",{"v":1,"d":"1.00"},"each",null,0]
["3.1.36","Commiphora neglecta\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.37","Commiphora schimperi\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.38","Commiphora woodii\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.39","Cordyla africana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.40","Cordia caffra",{"v":1,"d":"1.00"},"each",null,0]
["3.1.41","Craibia zimmermannii",{"v":1,"d":"1.00"},"each",null,0]
["3.1.42","Croton gratissimus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.43","Croton sylvaticus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.44","Cryptocarya latifolia\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.45","Cryptocarya myrtifolia\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.46","Cryptocarya woodii",{"v":1,"d":"1.00"},"each",null,0]
["3.1.47","Cryptocarya wyliei",{"v":1,"d":"1.00"},"each",null,0]
["3.1.48","Cunonia capensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.49","Curtisia dentata\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.50","Cussonia nicholsonii\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.51","Cussonia sphaerocephala\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.52","Cussonia spicata\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.53","Cussonia zuluensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.54","Dais cotinifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.55","Deinbollia oblongifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.56","Diospyros inhacaensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.57","Diospyros natalensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.58","Dombeya cymose",{"v":1,"d":"1.00"},"each",null,0]
["3.1.59","Dombeya rotundifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.60","Dombeya tiliacea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.61","Dovyalis caffra",{"v":1,"d":"1.00"},"each",null,0]
["3.1.62","Ekebergia capensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.63","Erythrina crista-galli",{"v":1,"d":"1.00"},"each",null,0]
["3.1.64","Erythrophleum lasianthum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.65","Erythrina latissima",{"v":1,"d":"1.00"},"each",null,0]
["3.1.66","Erythrina lysistemon",{"v":1,"d":"1.00"},"each",null,0]
["3.1.67","Euphorbia evansii\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.68","Euphorbia ingens\n",{"v":1,"d":"1.00"},"each",null,0]
["3.1.69","Euphorbia turicalli",{"v":1,"d":"1.00"},"each",null,0]
["3.1.70","Euclea natalensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.71","Faidherbia albida",{"v":1,"d":"1.00"},"each",null,0]
["3.1.72","Ficus bubu",{"v":1,"d":"1.00"},"each",null,0]
["3.1.73","Ficus ingens",{"v":1,"d":"1.00"},"each",null,0]
["3.1.74","Ficus lutea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.75","Ficus polita",{"v":1,"d":"1.00"},"each",null,0]
["3.1.76","Ficus sur",{"v":1,"d":"1.00"},"each",null,0]
["3.1.77","Ficus tremula",{"v":1,"d":"1.00"},"each",null,0]
["3.1.78","Galpinia transvaalica",{"v":1,"d":"1.00"},"each",null,0]
["3.1.79","Garcinia livingstonei",{"v":1,"d":"1.00"},"each",null,0]
["3.1.80","Gardenia cornuta",{"v":1,"d":"1.00"},"each",null,0]
["3.1.81","Gonioma kamassi",{"v":1,"d":"1.00"},"each",null,0]
["3.1.82","Halleria lucida",{"v":1,"d":"1.00"},"each",null,0]
["3.1.83","Harpephyllum caffrum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.84","Heteropyxis natalensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.85","Hibiscus tiliaceus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.86","Hymenocardia ulmoides",{"v":1,"d":"1.00"},"each",null,0]
["3.1.87","Ilex mitis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.88","Indigofera jucunda",{"v":1,"d":"1.00"},"each",null,0]
["3.1.89","Loxostylis alata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.90","Maerua rosmarinoides",{"v":1,"d":"1.00"},"each",null,0]
["3.1.91","Manilkara discolor",{"v":1,"d":"1.00"},"each",null,0]
["3.1.92","Margaritaria discoidea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.93","Maytenus heterophylla",{"v":1,"d":"1.00"},"each",null,0]
["3.1.94","Maytenus nemorosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.95","Maytenus peduncularis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.96","Maytenus procumbens",{"v":1,"d":"1.00"},"each",null,0]
["3.1.97","Maytenus undata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.98","Metarungia pubinervia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.99","Millettia grandis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.100","Mimusops obovata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.101","Mundulea sericea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.102","Nuxia congesta",{"v":1,"d":"1.00"},"each",null,0]
["3.1.103","Nuxia floribunda",{"v":1,"d":"1.00"},"each",null,0]
["3.1.104","Ochna natalitia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.105","Olea europea subsp.africana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.106","Olea woodiana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.107","Oncoba spinosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.108","Oxyanthus pyriformis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.109","Peltophorum africanum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.110","Pittosporum viridiflorum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.111","Plumeria rubra (Frangipani)",{"v":1,"d":"1.00"},"each",null,0]
["3.1.112","Podocarpus faclcatus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.113","Polygala myrtifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.114","Protorhus longifolia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.115","Ptaeroxylon obliquum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.116","Rauvolfia caffra",{"v":1,"d":"1.00"},"each",null,0]
["3.1.117","Rothmania capensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.118","Rothmania globosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.119","Schotia brachypetala",{"v":1,"d":"1.00"},"each",null,0]
["3.1.120","Schrebera alata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.121","Sclerocarya birrea",{"v":1,"d":"1.00"},"each",null,0]
["3.1.122","Searsia chirindensis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.123","Searsia lucida",{"v":1,"d":"1.00"},"each",null,0]
["3.1.124","Searsia tomentosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.125","Senegalia burkei ",{"v":1,"d":"1.00"},"each",null,0]
["3.1.126","Senegalia nigrescens",{"v":1,"d":"1.00"},"each",null,0]
["3.1.127","Sideroxylon inerme",{"v":1,"d":"1.00"},"each",null,0]
["3.1.128","Spirostachys africana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.129","Strelitzia nicolai",{"v":1,"d":"1.00"},"each",null,0]
["3.1.130","Strychnos decussata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.131","Syzygium cordatum",{"v":1,"d":"1.00"},"each",null,0]
["3.1.132","Syzygium guineense",{"v":1,"d":"1.00"},"each",null,0]
["3.1.133","Tabernaemontana ventricosa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.134","Terminalia catappa",{"v":1,"d":"1.00"},"each",null,0]
["3.1.135","Terminalia phanerophlebia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.136","Trema orientalis",{"v":1,"d":"1.00"},"each",null,0]
["3.1.137","Trichellia dregeana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.138","Trichellia emetica",{"v":1,"d":"1.00"},"each",null,0]
["3.1.139","Trichocladus grandiflorus",{"v":1,"d":"1.00"},"each",null,0]
["3.1.140","Turraea floribunda",{"v":1,"d":"1.00"},"each",null,0]
["3.1.141","Vachellia gerrardii",{"v":1,"d":"1.00"},"each",null,0]
["3.1.142","Vachellia natalitia",{"v":1,"d":"1.00"},"each",null,0]
["3.1.143","Vachellia robusta subsp. Robusta",{"v":1,"d":"1.00"},"each",null,0]
["3.1.144","Vachellia sieberiana var. woodii",{"v":1,"d":"1.00"},"each",null,0]
["3.1.145","Vepris lanceolata",{"v":1,"d":"1.00"},"each",null,0]
["3.1.146","Volkameria glabra",{"v":1,"d":"1.00"},"each",null,0]
["3.1.147","Warburgia salutaris",{"v":1,"d":"1.00"},"each",null,0]
["3.1.148","Xylotheca kraussiana",{"v":1,"d":"1.00"},"each",null,0]
["3.1.149","Ziziphus mucronata",{"v":1,"d":"1.00"},"each",null,0]
[]
[3.2,"Palm Trees (200L) - Supply and Plant"]
["3.2.1","Cocos nucifera",{"v":1,"d":"1.00"},"each",null,0]
["3.2.2","Hyphaene coriacea",{"v":1,"d":"1.00"},"each",null,0]
["3.2.3","Phoenix reclinata",{"v":1,"d":"1.00"},"each",null,0]
["3.2.4","Roystonea regia",{"v":1,"d":"1.00"},"each",null,0]
[]
[3.3,"Fruits and Edible Trees (50L) - Supply and Plant"]
["3.3.1","Avocado tree",{"v":1,"d":"1.00"},"each",null,0]
["3.3.2","Citrus Lemon",{"v":1,"d":"1.00"},"each",null,0]
["3.3.3","Citrus Orange ",{"v":1,"d":"1.00"},"each",null,0]
["3.3.4","Pecan Nut (Ukulinga) ",{"v":1,"d":"1.00"},"each",null,0]
["3.3.5","Mango tree",{"v":1,"d":"1.00"},"each",null,0]
["3.3.6","Apple tree ",{"v":1,"d":"1.00"},"each",null,0]
["3.3.7","Peach tree",{"v":1,"d":"1.00"},"each",null,0]
["3.3.8","Pawpaw tree",{"v":1,"d":"1.00"},"each",null,0]
["3.3.9","Litchi tree",{"v":1,"d":"1.00"},"each",null,0]
["3.3.10","Banana tree",{"v":1,"d":"1.00"},"each",null,0]
[]
[3.4,"Shrubs - Supply and Plant"]
["3.4.1","Acokanthera oppositifolia - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.2","Acokanthera oppositifolia - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.3","Aloe arborescens - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.4","Aloe arborescens - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.5","Aloe chabaudii - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.6","Aloe chabaudii - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.7","Aloe cooperi - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.8","Aloe cooperi - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.9","Aloe ferox - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.10","Aloe ferox - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.11","Aloe maculata - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.12","Aloe maculata - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.13","Aloe marlothii - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.14","Aloe marlothii - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.15","Aloe pluridens - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.16","Aloe pluridens - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.17","Aloe rupestris - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.18","Aloe rupestris - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.19","Aloe thraskii - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.20","Aloe thraskii - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.21","Alsophila dregei - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.22","Alsophila dregei - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.23","Aristea ecklonii - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.24","Aristea ecklonii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.25","Asparagus plumosus - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.26","Asparagus plumosus - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.27","Barleria obtusa - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.28","Barleria obtusa - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.29","Barleria repens - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.30","Barleria repens - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.31","Bauhinia tomentosa - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.32","Bauhinia tomentosa - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.33","Carissa macrocarpa \"Green Carpet\" - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.34","Carissa macrocarpa \"Green Carpet\" - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.35","Carissa macrocarpa - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.36","Carissa macrocarpa - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.37","Chrysanthemoides monilifera - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.38","Chrysanthemoides monilifera - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.39","Combretum bracteosum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.40","Combretum bracteosum - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.41","Combretum microphyllum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.42","Combretum microphyllum - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.43","Cussonia nicholsonii - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.44","Cussonia nicholsonii - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.45","Cussonia sphaerocephala - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.46","Cussonia sphaerocephala - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.47","Deinbllia oblongifolia - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.48","Deinbllia oblongifolia- 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.49","Dicliptera cernua - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.50","Dicliptera cernua - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.51","Diospyros lycioides - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.52","Diospyros lycioides - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.53","Dissotis princeps - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.54","Dissotis princeps - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.55","Distephanus angulifolius - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.56","Distephanus angulifolius - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.57","Dodonaea angustifolia - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.58","Dodonaea angustifolia - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.59","Dombeya tiliacea - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.60","Dombeya tiliacea - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.61","Dovyalis caffra - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.62","Dovyalis caffra - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.63","Dovyalis rhamnoides - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.64","Dovyalis rhamnoides - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.65","Dracaena aletriformis - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.66","Dracaena aletriformis - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.67","Ehretia rigida - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.68","Ehretia rigida - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.69","Encephalartos ferox (Cycad) - Cone Diameter 20cm",{"v":1,"d":"1.00"},"each",null,0]
["3.4.70","Encephalartos ferox (Cycad) - Cone Diameter 40cm",{"v":1,"d":"1.00"},"each",null,0]
["3.4.71","Encephalartos natalensis (Cycad) - Cone diameter 20cm ",{"v":1,"d":"1.00"},"each",null,0]
["3.4.72","Encephalartos natalensis (Cycad) - Cone diameter 40cm ",{"v":1,"d":"1.00"},"each",null,0]
["3.4.73","Encephalartos villosus (Cycad) - Cone diameter 20cm ",{"v":1,"d":"1.00"},"each",null,0]
["3.4.74","Encephalartos villosus (Cycad) - Cone diameter 40cm ",{"v":1,"d":"1.00"},"each",null,0]
["3.4.75","Euphorbia tirucallii 'Sticks on fire' - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.76","Euphorbia tirucallii 'Sticks on fire' - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.77","Euphorbia tirucallii 'Sticks on fire' - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.78","Ficus burtt-davyi - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.79","Ficus burtt-davyi - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.80","Ficus capreifolia - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.81","Ficus capreifolia - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.82","Gomphocarpus physocarpus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.83","Gomphocarpus physocarpus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.84","Grewia flava- 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.85","Grewia flava- 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.86","Grewia occidentalis - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.87","Grewia occidentalis - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.88","Hibiscus calyphyllus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.89","Hibiscus calyphyllus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.90","Hypoestes aristata - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.91","Hypoestes aristata - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.92","Isoglossa woodii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.93","Isoglossa woodii - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.94","Isoglossa cooperi - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.95","Isoglossa cooperi - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.96","Justicia capensis - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.97","Justicia capensis - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.98","Leonotis leonurus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.99","Leonotis leonurus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.100","Mackaya bella - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.101","Mackaya bella - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.102","Maerua rosmarinoides - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.103","Maerua rosmarinoides - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.104","Monanthotaxis caffra - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.105","Monanthotaxis caffra - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.106","Ochna serrulata - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.107","Ochna serrulata - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.108","Ocimum labiatum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.109","Ocimum labiatum - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.110","Osteospermum moniliferum - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.111","Osteospermum moniliferum - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.112","Pavetta lanceolata - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.113","Pavetta lanceolata - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.114","Pavetta revoluta - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.115","Pavetta revoluta - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.116","Pelargonium capitatum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.117","Pelargonium capitatum - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.118","Plectranthus ciliatus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.119","Plectranthus ciliatus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.120","Plectranthus saccatus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.121","Plectranthus saccatus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.122","Plectranthus spicatus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.123","Plectranthus spicatus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.124","Plectranthus ecklonii - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.125","Plectranthus ecklonii - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.126","Plectranthus fruticosus - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.127","Plectranthus fruticosus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.128","Plumbago auriculata 'Royal Cape' - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.129","Plumbago auriculata 'Royal Cape' - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.130","Plumbago auriculata 'Royal Cape' - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.131","Plumbago auriculata f. alba (White Cape Leadwort) - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.132","Plumbago auriculata f. alba (White Cape Leadwort) - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.133","Plumbago auriculata f. alba (White Cape Leadwort) - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.134","Polygala myrtifolia - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.135","Polygala myrtifolia - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.136","Polygala virgata - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.137","Polygala virgata - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.138","Portulacaria afra - 4L ",{"v":1,"d":"1.00"},"each",null,0]
["3.4.139","Portulacaria afra - 10L ",{"v":1,"d":"1.00"},"each",null,0]
["3.4.141","Portulacaria afra - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.142","Psychotria capensis - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.143","Psychotria capensis - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.144","Roses - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.145","Roses - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.146","Ruellia cordata - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.147","Ruellia cordata - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.148","Searsia dentata - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.149","Searsia dentata - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.150","Searsia natalensis - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.151","Searsia  natalensis - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.152","Searsia nebulosa - 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.153","Searsia nebulosa - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.154","Senecio barbetonicus- 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.155","Senecio barbetonicus- 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.156","Senecio oxyodontus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.157","Senecio oxyodontus - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.158","Strelitzia nicolai - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.159","Strelitzia nicolai - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.160","Strelitzia nicolai - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.161","Strelitzia nicolai - 100L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.162","Strelitzia reginae - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.163","Strelitzia reginae - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.164","Strelitzia reginae - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.165","Tecomaria capensis - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.166","Tecomaria capensis - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.167","Tecomaria capensis - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.168","Tephrosia grandiflora - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.169","Tephrosia grandiflora - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.170","Tetradenia riparia - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.171","Tetradenia riparia - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.172","Thunbergia natalensis - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.173","Thunbergia natalensis - 10L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.174","Turraea obtusifolia - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.4.175","Turraea obtusifolia - 20L",{"v":1,"d":"1.00"},"each",null,0]
[]
[3.5,"Groundcovers - Supply and Plant"]
["3.5.1","Agapanthus africanus 'blue' - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.2","Agapanthus africanus 'blue' - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.3","Agapanthus orientalis - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.4","Agapanthus orientalis - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.5","Agapanthus praecox - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.6","Agapanthus praecox - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.7","Aloe greatheadii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.8","Aloe greatheadii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.9","Aptenia cordifolia- 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.10","Aristida junciformis - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.11","Aristida junciformis - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.12","Asparagus densiflorus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.13","Asparagus macowanii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.14","Asystasia gangetica - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.15","Asystasia gangetica - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.16","Bulbine abyssinica- 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.17","Bulbine frutescens - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.18","Bulbine frutescens - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.19","Bulbine latifolia - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.20","Bulbine latifolia - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.21","Canevalia rosea- 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.22","Carex flagellifera - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.23","Carex flagellifera - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.24","Carpobrotus edulis cuttings",{"v":1,"d":"1.00"},"each",null,0]
["3.5.25","Carpobrotus edulis - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.26","Carpobrotus edulis - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.27","Chlorophytum comosum - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.28","Chlorophytum comosum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.29","Chlorophytum comosum 'variegatum' - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.30","Chlorophytum comosum 'variegatum' - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.31","Chlorophytum saundersii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.32","Chlorophytum saundersii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.33","Clivia miniata - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.34","Clivia miniata - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.35","Cotyledon orbiculata- 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.36","Crassula capitella- 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.37","Crassula erosula 'campfire' - 1L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.38","Crassula erosula 'campfire' - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.39","Crassula multicava, 1L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.40","Crassula multicava, 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.41","Crassula ovata- 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.42","Crinum macowanii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.43","Crinum macowanii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.44","Crocosmia aurea - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.45","Crocosmia aurea - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.46","Cyperus prolifer - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.47","Cyperus prolifer - 5L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.48","Cyrtanthus mackenii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.49","Cyrtanthus mackenii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.50","Cyrtanthus sanguineus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.51","Cyrtanthus sanguineus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.52","Delosperma lineare - Plugs",{"v":1,"d":"1.00"},"each",null,0]
["3.5.53","Delosperma lineare - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.54","Dietes bicolor - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.55","Dietes bicolor - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.56","Dietes grandiflora - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.57","Dietes grandiflora - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.58","Dietes iridioides - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.59","Dietes iridioides - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.60","Elegia tectorum - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.61","Elegia tectorum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.62","Gazania rigens plug",{"v":1,"d":"1.00"},"each",null,0]
["3.5.63","Gazania rigens - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.64","Gazania rigens - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.65","Gazania splendens plug",{"v":1,"d":"1.00"},"each",null,0]
["3.5.66","Gazania splendens - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.67","Gazania splendens - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.68","Haemanthus albiflos - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.69","Haemanthus albiflos - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.70","Helichrysum cymosum - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.71","Helichrysum cymosum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.72","Hypoestes forskaolii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.73","Hypoestes forskaolii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.74","Justicia betonica - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.75","Justicia betonica - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.76","Kalanchoe sexangularis- 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.77","Kalanchoe thyrsiflora- 3L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.78","Kniphofia tysonii - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.79","Kniphofia tysonii - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.80","Ledebouria petiolata - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.81","Ledebouria petiolata -4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.82","Merwilla plumbea - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.83","Merwilla plumbea - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.84","Nemesia denticulata - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.85","Nemesia denticulata - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.86","Nymphaea nouchali - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.87","Nymphaea nouchali - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.88","Ophiopogon japonicus 'kyoto' - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.89","Ophiopogon japonicus 'kyoto' - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.90","Oplismenus hirtellus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.91","Oplismenus hirtellus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.92","Osteospermum fruticosum - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.93","Osteospermum fruticosum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.94","Plectranthus verticillatus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.95","Plectranthus verticillatus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.96","Sansevieria hyacinthoides - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.97","Sansevieria hyacinthoides - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.98","Scadoxus puniceus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.99","Scadoxus puniceus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.100","Setaria megaphylla - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.101","Setaria megaphylla - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.102","Tulbaghia violacea 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.103","Tulbaghia violacea 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.104","Tulbaghia violacea \"Silver Lace\" 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.105","Tulbaghia violacea \"Silver Lace\" 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.106","Zantedeschia aethiopica 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.5.107","Zantedeschia aethiopica 4L",{"v":1,"d":"1.00"},"each",null,0]
[]
[3.6,"Creepers - Supply and Plant"]
["3.6.1","Asparagus falcatus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.2","Asparagus falcatus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.3","Grewia occidentalis - 20L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.4","Grewia occidentalis - 50L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.5","Ficus Pumila - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.6","Ipomoea ficifolia - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.7","Ipomoea ficifolia - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.8","Jasminum multipartitum - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.9","Jasminum multipartitum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.10","Momordica balsamina - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.11","Momordica balsamina - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.12","Rhoicissus digitata - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.13","Rhoicissus digitata - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.14","Rhoicissus rhomboidea - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.15","Rhoicissus rhomboidea - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.16","Rhoicissus tomentosa - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.17","Rhoicissus tomentosa - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.18","Senecio deltoieus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.19","Senecio deltoieus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.20","Senecio macroglossus - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.21","Senecio macroglossus - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.22","Senecio tamoides - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.23","Senecio tamoides - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.24","Thunbergia alata - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.6.25","Thunbergia alata - 4L",{"v":1,"d":"1.00"},"each",null,0]
[]
[3.7,"Lawn & Grasses-  Lawn installation including: Soil preparation, \nTurf/seed installation, Initial watering and protection, Establishment maintenance"]
[null,"Grasses - Supply and Plant"]
["3.7.1","Anthericum saunderssiae - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.7.2","Chondropetalum tectorum - 2L",{"v":1,"d":"1.00"},"each",null,0]
["3.7.3","Chondropetalum tectorum - 4L",{"v":1,"d":"1.00"},"each",null,0]
["3.7.4","Cynodon dactylon instant sods.",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.5","Cynodon dactylon sprigging",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.6","Dactyloctenium australe - Berea LM instant sods",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.7","Dactyloctenium australe - Berea LM Sprigging",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.8","Elegia tectorum - 5L",{"v":1,"d":"1.00"},"each",null,0]
[null,"Instant Lawn - Supply and Plant"]
["3.7.9","Pennisetum clandestinum  instant sods",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.10","Pennisetum clandestinum  Sprigging ",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.11","Stenotaphrum secundatum instant sods",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.12","Stenotaphrum secundatum Sprigging",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Veld grass - Hydroseeding"]
["3.7.13","Hydroseeding: Sour Bushveld veldgrass mix",{"v":1,"d":"1.00"},"m²",null,0]
["3.7.14","Hand seeding (Manual):  Sour Bushveld veldgrass mix",{"v":1,"d":"1.00"},"m²",null,0]
[]
[4,"HARDSCAPING (Rates shall include: Subgrade preparation, Compliance with SANS standards, Shop drawings, Testing and certification, Protection of adjacent structures)"]
[4.1,"Paving Base & Subbase"]
["4.1.1","G4 graded crushed stone imported material compacted in 150mm layer to specified density compaction",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.2","G5 imported material compacted in 150mm layer to specified density compaction",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.3","G5 imported material stabilised with cement at a rate of 1 pocket cement per 5m² - premixed and compacted slightly wet in 150mm layer",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.4","G6 imported material compacted in 150mm layer to specified density compaction",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.5","G7 importedd gravel material compacted in 150mm layer to specified density compaction",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.6","Rip and re-compact 150mm layer insitu material compact insitu material to minimum 93% MOD AASHTO density compaction",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.7","Subgrade Compaction to 90% MOD AASHTO density and stabilize with 5% cement prior to compaction if necessary, in layers of 150mm layers",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.8","Subgrade Compaction to 93% MOD AASHTO density in 150mm layers",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.9","Subgrade Compaction to 95% MOD AASHTO density in 150mm layers",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.10","Subgrade Compaction to 98% MOD AASHTO density in 150mm layers",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.11","Bidim geotextile membrane or similar approved",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.12","30mm thick River Sand Bedding - under paving ",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.13","250 micron SABS plastic USB sheeting membrane (to be used under the riversand) ",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.14","Approved herbicide and ant poison prior laying paving ",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.15","Ref 100 steel mesh (or according to PrEng specification) to be laid during insitu cast concrete ",{"v":1,"d":"1.00"},"m²",null,0]
["4.1.16","15Mpa Concrete footing/ foundation ",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.17","20Mpa Concrete footing/ foundation ",{"v":1,"d":"1.00"},"m³",null,0]
["4.1.18","25Mpa Concrete footing/ foundation ",{"v":1,"d":"1.00"},"m³",null,0]
[{"$nulls":5},0]
[4.2,"Paving materials - Supply and install",{"$nulls":3},0]
[null,"Concrete brick pavers"]
["4.2.1","1000x500x50mm thick concrete paver flagtone (pattern and colour varies), wood floated or brush finish surface.  Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.2","1000x500x50mm thick concrete paver flagtone (pattern and colour varies colour varies), exposed aggregate finish surface. Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.3","600x400x100mm Concrete Grass block permeable paver. Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.4","628x228x50mm light duty concrete edge beam (for edging). Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.5","500x500x50mm thick concrete paver blocks, wood floated brush finish (pattern and colour varies). Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.6","500x500x50mm thick concrete paver blocks, exposed aggregate finish (pattern and colour varies). Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.7","500 x 500 x50mm thick amalgamated concrete product, standard, purpose made or special, product to be tested and test certification for skid or non-slip, and concrete strength (no less than 25mpa) will be requested during the duration of the project to maintain quality of product. Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.8","400x300x60mm thick concrete paver block, wood floated brush finish (pattern and colour varies). Including saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.9","400x400x50mm Tactile or Similar approved: with a warning, directional, pedestrian or cycle signage engraved in the tile. ",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.10","300x300x50mm Tactile or Similar approved: with a warning, directional, pedestrian or cycle signage engraved in the tile",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.11","220x220x50mm concrete brick paver (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.12","200x150x75mm bevelled edge concrete brick paver (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.13","200x150x50mm thick concrete paver block (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.14","200x100x80mm thick interlocking concrete brick paver, in herringbone pattern (colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.15","200x100x60mm thick interlocking concrete brick paver, in herringbone pattern (colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.16","200x100x50mm Double Cobble concrete pavers (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.17","105x105x75mm grey concrete cobble pavers (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.18","100x100x50mm grey concrete cobble pavers (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Clay brick pavers"]
["4.2.19","220x108.5x73mm thick Clay Paving Brick (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.20","220x108.5x50mm thick Clay Paving Brick (colour and pattern varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.21","220x110x50mm clay brick (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.22","220x52x50mm thick Clay Paving Brick (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.23","222x106x73mm thick Clay Paving Brick (pattern and colour varies). Include saw cuttings",{"v":2,"d":"2.00"},"m131",null,0]
[null,"Cobble brick pavers:"]
["4.2.24","108.5x108.5x50mm clay cobble pavers (pattern and colour varies). Include saw cuttings",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Flagstone brick pavers:"]
["4.2.25","300x300x40mm thick Flagstone Paving Material on a concrete base/ screed. Colour and pattern varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.26","300x600x40mm thick Flagstone Paving Material on a concrete base/ screed. Colour and pattern varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.27","450x450x40mm thick Flagstone Paving Material on a concrete base/ screed. Colour and pattern varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.28","600x600x40mm thick Flagstone Paving Material on a concrete base/ screed. Colour and pattern varies",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Washed riversand:"]
["4.2.29","Riversand and filling of paving joints. Sweep riversand into paving joint",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Mortar joint:"]
["4.2.30","Mortar joint/ grouting (5-10mm spacing) with a mixture of sand, water and cement grout (2:1) including preparation of ground or filling",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Rubber Surface:"]
["4.2.31","25mm thick (for 800mm free fall height) Rubberizing: to comprise of recycled EPDM rubber granulate with polyurethane binding agent that will be applied on a concrete base. Rubberising to be installed in accordance with The South African Determination of Critical Fall Height Standard (SANS 51177:2010) and SANS1176-1",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.32","30mm thick (for 1000mm free fall height) Rubberizing: to comprise of recycled EPDM rubber granulate with polyurethane binding agent that will be applied on a concrete base. Rubberising to be installed in accordance with The South African Determination of Critical Fall Height Standard (SANS 51177:2010) and SANS1176-1",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.33","40mm thick (for 1200mm free fall height) Rubberizing: to comprise of recycled EPDM rubber granulate with polyurethane binding agent that will be applied on a concrete base. Rubberising to be installed in accordance with The South African Determination of Critical Fall Height Standard (SANS 51177:2010) and SANS1176-1",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.34","50mm thick (for 1500mm free fall height) Rubberizing: to comprise of recycled EPDM rubber granulate with polyurethane binding agent that will be applied on a concrete base. Rubberising to be installed in accordance with The South African Determination of Critical Fall Height Standard (SANS 51177:2010) and SANS1176-1",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.35","80mm thick (for 2300mm free fall height) Rubberizing: to comprise of recycled EPDM rubber granulate with polyurethane binding agent that will be applied on a concrete base. Rubberising to be installed in accordance with The South African Determination of Critical Fall Height Standard (SANS 51177:2010) and SANS1176-1",{"v":1,"d":"1.00"},"m³",null,0]
[null,"In-situ concrete paving /slab:"]
["4.2.36","125mm thick exposed aggregate concrete smooth and polished finish (20 mPA)",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.37","125mm thick insitu cast Concrete, exposed aggregate finish (20 mPA)",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.38","125mm thick insitu cast Concrete, broom brushed finish (20 mPA)",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.39","100mm thick insitu cast Concrete, broom brushed finish (20 mPA)",{"v":1,"d":"1.00"},"m³",null,0]
[null,"Decking:"]
["4.2.40","Treated CCA H4 pine Timber decking: Includes Timber posts on a 20Mpa concrete footing, Slats (70x20mm thick), joist, and beams ",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.41","Treated and sealed with a high-quality water-resistant coating Balau Timber decking: Includes Timber posts on a 20Mpa concrete footing, Slats (70x20mm thick), joist, and beams ",{"v":1,"d":"1.00"},"m²",null,0]
["4.2.42","Polywood/ Composite decking or similar approved: Includes posts on a 20Mpa concrete footing, Slats, joists, and beams",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.43","Dumprock: 75-200mm diameter Dumprock Material in layers of 200mm thick (colour varies). Uniformly spread and packed to the satisfaction of the Landscape Architect. ",{"v":1,"d":"1.00"},"m³",null,0]
[null,"Gravel:"]
["4.2.44","Gravel stones material: 15-25mm diameter in size, laid in 40mm thick layer (colour varies). Uniformly spread to the satisfaction of the landscape architect. ",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.45","Gravel stones material: 5-13mm diameter in size - laid in 40mm thick layer (colour varies). Uniformly spread to the satisfaction of the landscape architect. ",{"v":1,"d":"1.00"},"m³",null,0]
[null,"Mosaic tile artwork:"]
["4.2.46","Mosaic tiles material flooring or on walls - to be cement grouted ",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Artificial lawn/ grass:"]
["4.2.47","Synthetic/ artificial lawn glued on concrete with an approved polyurethane binding agent",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Asphalt surface:"]
["4.2.48","50mm thick layer of hot (or warm) mix Asphalt. The asphalt wearing course mix shall be sand skeleton mix NMPS of 10mm (eThekwini type Sa-S10). Must be installed on a specified compacted sub-surface layer/s.",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.49","35mm thick layer of hot (or warm) mix Asphalt. The asphalt wearing course mix shall be sand skeleton mix NMPS of 10mm (eThekwini type Sa-S10). Must be installed on a specified compacted sub-surface layer/s.",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.50","25mm thick layer of hot (or warm) mix Asphalt. The asphalt wearing course mix shall be sand skeleton mix NMPS of 10mm (eThekwini type Sa-S10). Must be installed on a specified compacted sub-surface layer/s.",{"v":1,"d":"1.00"},"m³",null,0]
["4.2.51","Sawcut asphalt edge to a maximum depth of 50mm thick",{"v":1,"d":"1.00"},"Lm",null,0]
[null,"Edging:"]
["4.2.52","1000x300x150mm thick Figure-1 Concrete Kerb to be laid on a cgrade 20/19 concrete foundation/ haunch",{"v":1,"d":"1.00"},"Lm",null,0]
["4.2.53","1000x230x125mm thick Figure-6 Concrete Kerb to be laid on 425x80mm thick grade 20/19 concrete foundation",{"v":1,"d":"1.00"},"Lm",null,0]
["4.2.54","1000x150x75mm thick Figure-12 Garden Kerb to be laid on a grade 20/19 concrete foundation/ haunch",{"v":1,"d":"1.00"},"Lm",null,0]
[{"$nulls":5},0]
[4.3,"Masonry/ Concrete work – for public realm walls, retaining walls and built furniture",{"$nulls":3},0]
[null,"Retaining wall:"]
["4.3.1","440mm thick, 500mm high Clay brick (brick size 222x106x73mm) insitu WALL with metal ties, recessed joints and bullnosed header course coping. RETAINING WALL must have waterproofing material and weepholes at 3m intervals. Compacted rubble between the walls to toppe with 200mm thick concrete layer",{"v":1,"d":"1.00"},"Lm",null,0]
[null,"Planter box:"]
["4.3.2","230mm thick, 500mm high Clay brick (brick size 222x106x73mm) insitu WALL with metal ties and recessed joints. SEAT/ PLANTERS WALL with waterproofing material, weepholes at 3m intervals also in accordance with the Engineer's specifications.  Brick colour varies",{"v":1,"d":"1.00"},"Lm",null,0]
[null,"Brick wall:"]
["4.3.3","(222x106x73mm) Clay brick (on edge) bullnosed header course. Brick colour varies",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Plaster:"]
["4.3.4","Cement Plaster and paint to walls",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Wall cladding:"]
["4.3.5","150x150mm Stone Cladding Material applied on sand cement mix with a 10mm grouting spaces. Colour of cladding stone varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.3.6","150x300mm Stone Cladding Material applied on sand cement mix with a 10mm grouting spaces. Colour of cladding stone varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.3.7","300x300mm Stone Cladding Material applied on sand cement mix with a 10mm grouting spaces. Colour of cladding stone varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.3.8","300x450mm Stone Cladding Material applied on sand cement mix with a 10mm grouting spaces. Colour of cladding stone varies",{"v":1,"d":"1.00"},"m²",null,0]
["4.3.9","450x450mm Stone Cladding Material applied on sand cement mix with a 10mm grouting spaces. Colour of cladding stone varies",{"v":1,"d":"1.00"},"m²",null,0]
[null,"Gabbion wall:"]
["4.3.10","2000x1000x500mm PVC coated mesh gabion basket. Colour varies",{"v":1,"d":"1.00"},"each ",null,0]
["4.3.11","2000x1000x500mm hot dipped galvanised steel mesh gabion basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.12","2000x1000x500mm hot deep galvanised welded mesh steel (3mm thick) gabion basket ",{"v":1,"d":"1.00"},"each",null,0]
["4.3.13","2000x1000x1000mm PVC coated steel mesh gabion basket. PVC colour varies",{"v":1,"d":"1.00"},"each",null,0]
["4.3.14","2000x1000x1000mm hot dipped galvanised steel mesh gabion basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.15","2000x1000x1000mm hot dipped galvanised welded mesh steel (3-5mm thick) gabion basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.16","2000x1000x300mm hot dipped galvanised welded mesh steel (3-5mm thick) gabion basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.17","2000x1000x300mm PVC coated steel mesh reno mattress basket. PVC colour varies",{"v":1,"d":"1.00"},"each",null,0]
["4.3.18","2000x1000x300mm hot dipped galvanised steel reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.19","2000x1000x300mm hot dipped galvanised welded mesh steel (3-5mm thick) reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.20","3000x1000x300mm PVC coated steel mesh reno mattress basket. PVC colour varies",{"v":1,"d":"1.00"},"each",null,0]
["4.3.21","3000x1000x300mm hot dipped galvanised steel reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.22","3000x1000x300mm hot dipped galvanised welded mesh steel (3-5mm thick) reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.23","6000x2000x170mm PVC coated steel mesh reno mattress basket. PVC colour varies",{"v":1,"d":"1.00"},"each",null,0]
["4.3.24","6000x2000x170mm hot dipped galvanised steel reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.25","6000x2000x170mm hot dipped galvanised welded mesh steel (3-5mm thick) reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.26","6000x2000x300mm PVC coated steel mesh reno mattress basket. PVC colour varies",{"v":1,"d":"1.00"},"each",null,0]
["4.3.27","6000x2000x300mm hot dipped galvanised steel reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
["4.3.28","6000x2000x300mm hot dipped galvanised welded mesh steel (3-5mm thick) reno mattress basket",{"v":1,"d":"1.00"},"each",null,0]
[null,"In-situ concrete wall:"]
["4.3.29","450x450mm high insitu cast off shutter reinforced concrete (25MPA) seating/ retaining wall, smooth finish and 45° chamfer. Footing to be as per the Engineer's Spec.",{"v":1,"d":"1.00"},null,null,0]
[null,"Stone Wall:"]
["4.3.30","Stone wall: Concrete 25/19 (25 mPA) to be used for foundations and variation of various types of rock types, sizes and texture, rocks to have a nominal size of 150 mm – 500 mm. All to approval of the Landscape architect. Foundations to be 400 mm deep x 1100 mm wide, or according to PrEng’s specifications. Length will vary. Wall to be 500 mm double sleeve rock wall with concrete infill between to required height. Heights and lengths will vary. Rock masonry to be of good quality and workmanship to be consistent throughout.",{"v":1,"d":"1.00"},"Lm",null,0]
[null,"Terrace Block wall:"]
["4.3.31","Terrace Block Walls: precast concrete block retaining wall (Loffelstein or similar). Sample to be approved by a landscape architect. Height not to exceed 1.2m. Construct as per manufacturer's recommendation. Excludes bulk earthworks, backfilling, topsoil, base preparation and compaction, foundation and planting. This is measured elsewhere.",{"v":1,"d":"1.00"},"Lm",null,0]
[null,"Coping:"]
["4.3.32","222x106x73mm Clay brick bullnosed header course coping",{"v":1,"d":"1.00"},"each ",null,0]
["4.3.33","1000x300x85mm thick standard precast concrete coping (pyramid shaped). Coping is recessed on both bottom ends ",{"v":1,"d":"1.00"},"each ",null,0]
["4.3.34","1000x470x75mm thick standard precast concrete coping (pyramid shaped). Coping is recessed on both bottom ends ",{"v":1,"d":"1.00"},"each ",null,0]
["4.3.35","1000x300x100mm thick standard precast concrete coping. Pitched to fall on one side. Coping is recessed on one bottom end ",{"v":1,"d":"1.00"},"each ",null,0]
[]
[5,"PUBLIC REALM FURNITURE AND EQUIPMENT - Rates shall include: Supply and delivery; Offloading and storage; Foundations; Anchoring systems; Fixing and installation; Concrete bases; Reinforcement where required; Protective coatings; Surface preparation; Manufacturer warranties; Compliance testing; Safety certification; All labour, plant, materials and incidentals necessary for complete installation.\n\nAll furniture and equipment shall comply with applicable SANS standards, manufacturer specifications and the requirements of the Employer's Agent."]
[5.1,"Furniture)"]
[null,"Bollards:"]
["5.1.1","500mmØ x 500mm high Precast Half Penny Concrete Bollard, smooth finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.2","500mmØ x 500mm high Precast Half Penny Concrete Bollard, vertical surface to be exposed aggregate finish. The top surface of the bollard to be wood floated smooth finish.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.3","450x450x450mm high precast concrete bollard seat (square bollard), smooth finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.4","500mmØ precast concrete Ball bollard, wood floated smooth finis. To be pegged with steel rods into a 500 x 500 x 250mm deep base",{"v":1,"d":"1.00"},"each",null,0]
["5.1.5","500mmØ precast concrete Ball bollard, exposed aggregate finish. To be pegged with steel rods into a 500 x 500 x 250mm deep base",{"v":1,"d":"1.00"},"each",null,0]
["5.1.6","250mmØ x 1200mm high standard precast concrete bollard, smooth finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.7","250mmØ x 1200mm high standard  precast concrete bollard, exposed aggregate finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.8","250x250x810mm high standard metro precast concrete bollard ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.9","100mmØ x 1200mm high hot dipped galvanised steel removable bollard, powder coated finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.10","100mmØ x 1200mm high stainless steel removable bollard",{"v":1,"d":"1.00"},"each",null,0]
["5.1.11","1200mm high and 900mm high above ground level x 300mm Diameter Precast Concrete Water Fountain, exposed aggregate finish with hot dipped galvanized steel tap. Foundations and installation according to spec by PrEng and in compliance with SANS 1808-16.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.12","1200mm high and 900mm high above ground level x 300mm Diameter Precast Concrete Water Fountain, wood floated finish with hot dipped galvanized steel tap. Foundations and installation according to spec by PrEng and in compliance with SANS 1808-16.",{"v":1,"d":"1.00"},"each",null,0]
[null,"Benches:"]
["5.1.13","Steel bench with backrest\n1800x500x500mm high Long Hot Dipped Galvanized steel bench with backrest, manufactured according to SABS regulations.\n- Composed of 3mm thick punched galvanized steel panel sheeting. Legs: Two x 400mm high and 50mm diam. galvanized steel profiles:\na. Standard leg height is to be extended by an extra 300mm in order for it to be planted.\nb. The total leg length should therefore be 700mm high in total in order to accommodate for the installation specifications as set out below.\n- Finish: galvanised steel with polyurethane paint coat; colour as specified and approved by Landscape Architect.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.14","1500mm wide x 450mm high x 100mm thck precast wood floated smooth finish rectangular standard concrete bench. Concrete 30MPa steel reinforced (SANS 920) precast bench, manufactured according to SABS regulations. Top edge to be chamfered by 20 x 20mm all around",{"v":1,"d":"1.00"},"each",null,0]
["5.1.15","1800mm wide x 450mm high x 100mm thick precast wood floated smooth finish rectangular standard concrete bench. Concrete 30MPa steel reinforced (SANS 920) precast bench, manufactured according to SABS regulations. Top edge to be chamfered by 20 x 20mm all around",{"v":1,"d":"1.00"},"each",null,0]
["5.1.16","1500mm wide x 450mm high x 100mm thick exposed aggregate sawcut stone smooth and polished finish precast rectangular standard concrete bench. Concrete 30MPa steel reinforced (SANS 920) precast bench, manufactured according to SABS regulations. Top edge to be chamfered by 20 x 20mm all around",{"v":1,"d":"1.00"},"each",null,0]
["5.1.17","1800mm wide x 450mm high x 100mm thick exposed aggregate sawcut stone smooth and polished finish precast rectangular standard concrete bench. Concrete 30MPa steel reinforced (SANS 920) precast bench, manufactured according to SABS regulations. Top edge to be chamfered by 20 x 20mm all around",{"v":1,"d":"1.00"},"each",null,0]
[null,"Picnic/ Rest Set:"]
["5.1.18","1500mm wide precast wood floated smooth rectangular concrete Picnic/ Rest set table and benches (x2 Benches X1 table). The table should be in 1 piece and have a centralised hole for umbrella placing. ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.19","1800mm wide precast smooth rectangular concrete Picnic/ Rest set table and benches (x2 Benches X1 table). The table should be in 1 piece and have a centralised hole for umbrella placing. ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.20","1500mm wide precast polished concrete Picnic Set  (table with umbrella hole - game board tables could be included Chess & Morabaraba). Picnic/ Rest set to have x2 Benches X1 table per set. The table should be in 1 piece and have a centralised hole for umbrella placing.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.21","1800mm wide precast polished concrete Picnic Set  (table with umbrella hole - game board tables could be included Chess & Morabaraba). Picnic/ Rest set to have x2 Benches X1 table per set. The table should be in 1 piece and have a centralised hole for umbrella placing.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.22","1000mm dia. Smooth round concrete Picnic/ Rest set with 5 seats approved by the Landscape Architect. The table should be in 1 piece.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.23","6-Seater Picnic Set (benches without backrest): All material is 100% plastic recycled picnic set, assembled using stainless steel fixtures",{"v":1,"d":"1.00"},"each",null,0]
["5.1.24","8-Seater Picnic Set (benches without backrest) : All material is 100% plastic recycled picnic set, assembled using stainless steel fixtures",{"v":1,"d":"1.00"},"each",null,0]
["5.1.25","6-Seater Picnic Set (benches with backrest) : All material is 100% plastic recycled picnic set, assembled using stainless steel fixtures",{"v":1,"d":"1.00"},"each",null,0]
["5.1.26","8-Seater Picnic Set (benches with backrest): All material is 100% plastic recycled picnic set, assembled using stainless steel fixtures",{"v":1,"d":"1.00"},"each",null,0]
[null,"Braai Facility:"]
["5.1.27","Braai Stand: 950mm high x 500mm Diameter precast concrete braai stand, 750mm height above ground Exposed Aggregate concrete finish with hot dipped galvanized steel grid finish. Foundation / fixing: To manufacturer’s specification.",{"v":1,"d":"1.00"},"each",null,0]
["5.1.28","Braai Stand: 950mm high x 500mm Diameter precast concrete braai stand, 750mm height above ground wood floated concrete finish with hot dipped galvanized steel grid finish. Foundation / fixing: To manufacturer’s specification.",{"v":1,"d":"1.00"},"each",null,0]
[null,"Litter bin:"]
["5.1.29","700x700x1150mm high (110L) concrete litterbin, wood floated smooth finish with a drainage hole in the bottom. Must be fixed on a concrete footing ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.30","700x700x1150mm high (110L) concrete litterbin, exposed aggregate finish with a drainage hole in the bottom. Must be fixed on a concrete footing ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.31","550x550x1000mm high (165L) concrete litterbin, wood floated smooth finish with a drainage hole in the bottom. Must be fixed on a concrete footing ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.32","550x550x1000mm high (165L) concrete litterbin, exposed aggregate finish with a drainage hole in the bottom. Must be fixed on a concrete footing ",{"v":1,"d":"1.00"},"each",null,0]
[null,"Drinking fountain:"]
["5.1.33","200x400x1180mm high Concrete drinking fountain, Polished concrete & smooth grey finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.34","201x400x1180mm high Concrete drinking fountain, exposed aggregate concrete finish",{"v":1,"d":"1.00"},"each",null,0]
[null,"Outdoor Chess:"]
["5.1.35","5000x5000mm large Chess with 600x600x20mm tiles set on 125mm thick in-situ concrete slab (20MPa). Rate to include base and layerworks.",{"v":1,"d":"1.00"},"sum",null,0]
[null,"Precast concrete planter box:"]
["5.1.36","1200x1200x1200mm high precast concrete planter box, smooth finish",{"v":1,"d":"1.00"},"each",null,0]
["5.1.37","1200x1200x1200mm high precast concrete planter box, exposed aggregate finish with a central hole at the bottom for drainage",{"v":1,"d":"1.00"},"each",null,0]
["5.1.38","700x700x700mm high precast concrete planter box, wood floated smooth finish with a central hole at the bottom for drainage",{"v":1,"d":"1.00"},"each",null,0]
["5.1.39","700x700x700mm high precast concrete planter box, exposed aggregate finish with a central hole at the bottom for drainage",{"v":1,"d":"1.00"},"each",null,0]
["5.1.40","450x450x770mm high precast concrete planter box, wood floated smooth finish with a central hole at the bottom for drainage",{"v":1,"d":"1.00"},"each",null,0]
["5.1.41","450x450x770mm high precast concrete planter box, exposed aggregate finish with a central hole at the bottom for drainage",{"v":1,"d":"1.00"},"each",null,0]
[null,"Game board:"]
["5.1.42","CUSTOM MADE CONCRETE BOARD GAMES PANEL\n(+/-1000/600x600x50mm) fixed with 100mm thick 20MPa in-situ concrete and surrounded by paving on the 14x brick benches. Games: Chess, Diketo & Morabaraba/ Mhele",{"v":1,"d":"1.00"},"each",null,0]
[null,"Rail and Bicycle rack:"]
["5.1.43","57-100mm dia. Single round Galvanised Mild Steel tube custom Handrail spray-painted yellow. Handrail must meet SANS standards and installed as per Manufacturer's specifications",{"v":1,"d":"1.00"},"Lm",null,0]
["5.1.44","1800x1000mm high x 50mm diameter 304 brushed stainless steel 5-Hoop Bicycle Rack, Legs are to be extended by 300mm into the ground. 10mm round galvanised steel anchor to be welded horizontally onto the bottom of each leg to secure into foundation. Stainless steel base plate cover to be provided for on each leg. To be set 300mm of the bicycle rack profiles into 250 x 250 x 330mm deep 15MPa concrete foundations on prepared and compacted subgrade",{"v":1,"d":"1.00"},"each",null,0]
[null,"Tree rings:"]
["5.1.45","1000mm Diameter Concrete Barrier Kerb Tree Ring. Kerb to be laid on a 100mm thick concrete 25Mpa concrete footing/ haunch",{"v":1,"d":"1.00"},"each",null,0]
["5.1.46","1500mm Diameter Concrete Barrier Kerb Tree Ring. Kerb to be laid on a 100mm thick concrete 25Mpa concrete footing/ haunch",{"v":1,"d":"1.00"},"each",null,0]
["5.1.47","1200x1200x60mm thick exposed aggregate concrete finish. 420mm diameter overall central opening. ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.48","1200x1200mm premanufactured hot dipped galvanised tree grid, . Polyurathane paint finish as per the supplier's spec",{"v":1,"d":"1.00"},"each",null,0]
["5.1.49","1060x920x640 high (760L) Standard Precast Single wash concrete trough ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.50","2120x920x640 high (1520L) Standard Precast Double wash concrete trough ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.51","1000x600mm half round pipe precast concrete channel",{"v":1,"d":"1.00"},"each",null,0]
["5.1.52","1220x610x480mm high precast concrete stormwater channel ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.53","1000x460x170mm high precast concrete stormwater channel ",{"v":1,"d":"1.00"},"each",null,0]
["5.1.54","500x650x220mm high precast concrete stormwater channel",{"v":1,"d":"1.00"},"each",null,0]
["5.1.55","1000x340x280mm high precast concrete stormwater channel with rebate for galvanised steel grate",{"v":1,"d":"1.00"},"each",null,0]
["5.1.56","1200x400x150mm high precast concrete embankment chute to be laid on a 60mm thick concrete base",{"v":1,"d":"1.00"},"each",null,0]
[]
[5.2,"Heavy Duty Play equipment & structures to comply with SANS 51176:2010 and all other applicable SABS standards (All apparatus to be Galvanised prior to Powder Coating) to be Flexitop spray painted - Supply and installation including Foundations and anchoring, Manufacturer compliance"]
["5.2.1","4000x12000mm 4-Seater swing",{"v":1,"d":"1.00"},"each",null,0]
["5.2.2","4000x12000mm 3-Seater swing for the disable",{"v":1,"d":"1.00"},"each",null,0]
["5.2.3","1500x5000mm Arching heart shaped seater see-saw",{"v":1,"d":"1.00"},"each",null,0]
["5.2.4","600x2400mm Senior Joywheel roundabout",{"v":1,"d":"1.00"},"each",null,0]
["5.2.5","2100x3750mm Executive Jungle Gym",{"v":1,"d":"1.00"},"each",null,0]
["5.2.6","3000x7500mmx3000mm high Slide",{"v":1,"d":"1.00"},"each",null,0]
["5.2.7","500x4000mm 4-seater Sea-saw Junior",{"v":1,"d":"1.00"},"each",null,0]
["5.2.8","1000x2500mm 4-Seater wheelchair roundabout",{"v":1,"d":"1.00"},"each",null,0]
["5.2.9","1500x1500mm Toddler combination Jungle Gym with Slide and Swing",{"v":1,"d":"1.00"},"each",null,0]
["5.2.10","10500 x 5700mm CCA H4 Treated Wooden Jungle Gym to include Platform x 2, Roof, Swing, Slide, Ladder, Pull–U–Ladder, Combo Net, Bridge, Gladiator Bars, Rope Ladder, Tyre Tower, Fireman's Pole, and Tyre Ladder as per supplier's specification.",{"v":1,"d":"1.00"},"each",null,0]
["5.2.11","1800x6300mm CCA H4 treated Wooden Jungle Gym to include a Platform, Swing, Roof, Slide, and a Ladder as per supplier's specification.",{"v":1,"d":"1.00"},"each",null,0]
[]
[5.3,"Heavy Duty Outdoor gym equipment to comply with SANS 51176:2010 and all other applicable SABS standards (All apparatus to be hot dipped Galvanised prior to Powder Coating) - Supply and Install"]
["5.3.1","Surf Board",{"v":1,"d":"1.00"},"each",null,0]
["5.3.2","Space/Air Walker",{"v":1,"d":"1.00"},"each",null,0]
["5.3.3","Elliptical Cross trainer",{"v":1,"d":"1.00"},"each",null,0]
["5.3.4","Chest and back Massager",{"v":1,"d":"1.00"},"each",null,0]
["5.3.5","4 person Leg press trainer",{"v":1,"d":"1.00"},"each",null,0]
["5.3.6","Bicycle/Spinning bike",{"v":1,"d":"1.00"},"each",null,0]
["5.3.7","Rowing Machine",{"v":1,"d":"1.00"},"each",null,0]
["5.3.8","Pendulum equipment/ waist trainer",{"v":1,"d":"1.00"},"each",null,0]
["5.3.9","Butterfly - for the disabled",{"v":1,"d":"1.00"},"each",null,0]
["5.3.10","Leg Press Trainer - for the disabled",{"v":1,"d":"1.00"},"each",null,0]
["5.3.11","Stepper machine",{"v":1,"d":"1.00"},"each",null,0]
["5.3.12","Dip bars",{"v":1,"d":"1.00"},"each",null,0]
["5.3.13","Double Parallel Bars",{"v":1,"d":"1.00"},"each",null,0]
["5.3.14","Scaling ladder",{"v":1,"d":"1.00"},"each",null,0]
["5.3.15","Wab board",{"v":1,"d":"1.00"},"each",null,0]
["5.3.16","Push-up bars",{"v":1,"d":"1.00"},"each",null,0]
[]
[6,"FENCING & SECURITY - TO COMPLY WITH APPLICABLE SABS STANDARDS - Installation of fencing including: Setting out\nFoundations and posts, Alignment and stability, Protection of adjacent areas"]
[null,"Clear Fence, Gate and Trellis:"]
[6.1,"3048x2400mm high Hot Dipped Galvanised and Powder Coated Invisible Fence Panel with serrated spike top rail or Similar approved installed to Manufacturer's specifications inclusive of all material required to complete the work. Fence to include 3.2m high hollow “H” profiled posts & sundries, Dimensions – 84x62x2mm, All holes to be pre-drilled before hot dip galvanising. Finish – hot dip galvanised and then pvc coated (min. 200 microns) – Green and is to set them in concrete foundations at the appropriate centres to accommodate the fixing of the fence panels and level difference in ground level. Post Foundations: Posts located in open ground are to have 400x400x800 deep 20mPa/19mm stone concrete bases per post. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.2,"1250 x 2100mm high Hot Dipped Galvinised and Powder Coated Standard Pesriatrian Gate (1350mm Post To Post) with invisble fence material. The Gate frame is to be manufactured using square hollow section 38x38x2mm frame with a 38x38x2mm equal angle to be welded to the inside of the square hollow tube gate frame to allow for the fixing of the invisible  fence panel. To be installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"each ",null,0]
[6.3,"4000 x 2100mm high Hot Dipped Galvinised and Powder Coated Standard Pesriatrian Gate (1350mm Post To Post) with invisble fence material. The Gate frame is to be manufactured using square hollow section 38x38x2mm frame with a 38x38x2mm equal angle to be welded to the inside of the square hollow tube gate frame to allow for the fixing of the invisible  fence panel. To be installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"each ",null,0]
[6.4,"2100mm high Hot Dipped Galvanised Invisible Fence and powder coated or Similar approved installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.5,"1200mm high Hot Dipped Galvanised and Powder coated Invisible Fence installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.6,"1800mm high Hot Dipped Galvinised and Powder coated Steel Palisade fence installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.7,"2100mm high Hot Dipped Galvinised and Powder coated Steel Palisade fence installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.8,"2400mm high Concrete Palisade fence installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction ",{"v":1,"d":"1.00"},"Lm",null,0]
[6.9,"3000mm high Concrete Palisade fence installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
["6.10","Hot Dipped Galvanised & powder coated Steel Post & Rail fence - 3 rails, 1000mm high installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.11,"3000mm High Roll Size of sport & playground fence, Hot Dipped Galvanized: Posts@ 3m spacing, 3-4mm wire mesh diameter, mesh size 50 x 50mm; Frame Size 50mm diameter. ",{"v":1,"d":"1.00"},"Lm",null,0]
[6.12,"6000mm High Roll Size of sport & playground fence, plastic coated diamond wire mesh fence: Posts@ 3000mm spacing, 3-4mm wire mesh diameter, mesh size 50X50mm; Frame Size 50mm diameter",{"v":1,"d":"1.00"},"Lm",null,0]
[6.13,"6000mm High Roll Size of sport & playground fence, Hot Dipped Galvanized: Posts@ 3m spacing, 3-4mm wire mesh diameter, mesh size 50X50mm; Frame Size 50mm diameter",{"v":1,"d":"1.00"},"Lm",null,0]
[6.14,"Mesh: All steel materials shall be of good quality, hot dipped galvanized steel. Panel width 3297mm. Wire with aperture size (centres) @ 76.2mm x 25mm. Height 1.2m, with a wire diameter of 3mm\n(length of entire fence 50m). All pipes shall be hot dipped galvanized (one piece without joints). Furnish moisture proof caps for all posts. Zinc coating shall be smooth and essentially free from lumps, globs or points. Miscellaneous material shall be galvanized.",{"v":1,"d":"1.00"},"Lm",null,0]
[6.15,"1800mm high PVC coated diamond mesh fencing  (75x75mm Diamond mesh size and 1.8mm steel thickness) with hot dipped galvanised mild steel fence posts with razor wire flat wrap security head. Posts at 3000mm centres and are to be set in 300x300x500 concrete bases – ensure that the  post protrudes out of the concrete base, to allow for water drainage. ",{"v":1,"d":"1.00"},"Lm",null,0]
[6.16,"2100mm high PVC coated diamond mesh fencing  (75x75mm Diamond mesh size and 1.8mm steel thickness) with hot dipped galvanised mild steel fence posts with razor wire flat wrap security head. Posts at 3000mm centres and are to be set in 300x300x500 concrete bases – ensure that the  post protrudes out of the concrete base, to allow for water drainage. ",{"v":1,"d":"1.00"},"Lm",null,0]
[6.17,"1510 x 905mm CCA H4 treated wooden Trellis Panel.  ",{"v":1,"d":"1.00"},"each ",null,0]
[6.18,"1140 x 1530mm Steel Creeper/ Trellis Panel, Hot dipped galvanised and powder coated with 9 bars for enhanced stability and support, Green (or Black) colour finish. ",{"v":1,"d":"1.00"},"each ",null,0]
[6.19,"800mm high 150mm diameter dome top CCA H4 treated wooden gumpole post set at 1800mm centres with 2x90mm horizontal top and bottom rails set at 500mm apart. Faced with 38mm plastic coated diamond mesh fence and covered with 80% shade cloth  Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
["6.20","1250mm high x150mm diameter dome top CCA H4 treated wooden gumpole post set in concrete footing (set in 500x500x600mm 20Mpa concrete footing) at 1800mm centres with 2x90mm horizontal top and bottom rails set at 500mm apart. Contractor to check distance and make allowances for additional poles for change in topography and direction",{"v":1,"d":"1.00"},"Lm",null,0]
[6.21,"2500x1250mm Chromadek Signage board (Hot dipped galvanised) on a 18mm shutter board backing fixed to cabstrut horizontal support clamped to 100 - 125mm diameter CCA H4 treated gum pole post set in 500x500x600mm 20Mpa concrete footing",{"v":1,"d":"1.00"},"sum",null,0]
[6.22,"2500x1250mmx3mm thick ABS Plastic material Signage board on a shutter board backing set in 500x500x600mm 20Mpa concrete footing. Signage to be on a UV stable 7 year vinyl material.  ",{"v":1,"d":"1.00"},"sum",null,0]
[6.23,"Hot Dipped Galvanised & powder coated Steel Post & Rail fence - 3 rails, 1m high installed to Manufacturer's specifications inclusive of all material required to complete the work. Contractor to check distance and make allowances for additional poles for ",{"v":1,"d":"1.00"},"sum",null,0]
[6.24,"50x50x1250mm high hot deep galvanised steel weld mesh fencing (2.5mm diameter thick) ",{"v":1,"d":"1.00"},"each ",null,0]
[6.25,"50x50x1500mm high hot deep galvanised steel weld mesh fencing (2.5mm diameter thick) ",{"v":1,"d":"1.00"},"each ",null,0]
[6.26,"50x50x1800mm high hot deep galvanised steel weld mesh fencing (2.5mm diameter thick) ",{"v":1,"d":"1.00"},"each ",null,0]
[6.27,"1800mm high hot dipped galvinised pedestrian gate with diamond mesh fence",{"v":1,"d":"1.00"},"Lm",null,0]
[]
[7,"SPORTS  & BALL COURTS - in accordance with relevant SANS standardised specifications and SASR Norms & Standards. All warranty information must be included in the quotation. Final design and drawings to be approved by the Landscape Architect before ordering and/or implementation"]
[7.1,"5-A-Side Soccer Court:"]
["7.1.1","222 x 106 x 73mm Clay face brick walls ",{"v":1,"d":"1.00"},"Lm",null,0]
["7.1.2","7320mm wide and 2440 mm high with 3mm mild steel, hot dip galvanized Standard White Powder coated with different colour options set on a 25Mpa concrete footing",{"v":1,"d":"1.00"},"each",null,0]
["7.1.3","3000m high 100x100x4.5mm nylon soccer netting material",{"v":1,"d":"1.00"},"Lm",null,0]
["7.1.4","40mm thick 20mPA/ 19mm Fibre reinforced concrete with steel trowel finish ",{"v":1,"d":"1.00"},"Lm",null,0]
["7.1.5","Fibregrass 173 with two part poly-urethane adhesive to a 5-A-Side",{"v":1,"d":"1.00"},"m²",null,0]
[null,"rubberising"]
[7.3,"3650x21250mm Multi-Court on hard surface with an artificial synthetic surface installed as per SASR Netball court requirements including marking. Includes prefabricated;\n- Netball goal post per set of 2 including nylon netting.\n- Futsal (Soccer) goal post per set of 2 including goal nets.\n- Volleybal goal post per set.\n- Basketball goal post per set of 2 including nets.",{"v":1,"d":"1.00"},"sum",null,0]
[7.4,"3000mm high, 3mm Galvanised Chain link fencing to Multi-Court fully installed to Manufacturer's specifications inclusive of all material required to complete the work. Fence must be SABS approved.",{"v":1,"d":"1.00"},"Lm",null,0]
[7.5,"100mm thick Coarse River Sand Layer to leveled sand-based soccer field on top of 150mm in-situ sub-base material compacted to 98% MOD-AASHTO. Rate to include 1x (1000m high, 3000m dia) round concrete mounds/domes to play area.",{"v":1,"d":"1.00"},"m²",null,0]
[7.6,"76mmØ x 3mm thick Football goal post and nylon netting material. Goal Posts are 7320mm apart",{"v":1,"d":"1.00"},"sum",null,0]
[7.7,"100x100x3mm thich hot dipped galvanised and powder coated Basket/ nteball post and nylon netting material",{"v":1,"d":"1.00"},"sum",null,0]
[7.8,"20X10m Standard Padel Court: Perimeter ring beam construction\nSubbase Construction with Drainage, Laser cut powder coated steel structure, 400 Wattled LED flood lights, Padel Federation approved sysnthetic turf, Net and Electrical installation (All spec to be as as per the supplier)",{"v":1,"d":"1.00"},"sum ",null,0]
[]
[8,"IRRIGATION - in accordance with relevant SANS standardised specifications and LIA standards. Rates shall include: Testing and commissioning, As-built drawings, Operating manuals, Warranty"]
[8.1,"Turf Valve Irrigation System "]
["8.1.1","Pump station"]
["8.1.1.1","DAB CENT TWIN IMP K70/300T PUMP 380V",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.2","ELECTRICAL PANEL",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.3","SUCTION & DEL FITTINGS",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.4","WATER TANK 10 000LT VERTICAL",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.5","PUMPROOM (1x1m premanufactured fibre glass material)",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.6","CONCRETE FOUNDATION",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.7","FILTERBANK",{"v":1,"d":"1.00"},"each",null,0]
["8.1.1.8","500L PRESSURE VESSEL",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2","Pipes and Turf Valve Fittings",{"$nulls":3},0]
["8.1.2.1","Mainline connection (or similar)",{"v":1,"d":"1.00"},"each ",null,0]
["8.1.2.2","SABS 40mm CL10 HDPE POLY.PIPE",{"v":1,"d":"1.00"},"each ",null,0]
["8.1.2.3","SABS 63mm CL10 HDPE POLY.PIPE",{"v":1,"d":"1.00"},"each ",null,0]
["8.1.2.4","SABS 75mm CL10 HDPE POLY.PIPE 50m",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.5","75mm  EQUAL COUPLING",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.6","40mm  EQUAL COUPLING",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.7","63mm  EQUAL COUPLING",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.8","75mm  EQUAL 90deg ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.9","75mm END CAP",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.10","75mm x 3\"  MALE ADAPTOR",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.11","75mm x 11/2\"  4 BOLTS SADDLE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.12","40mm x 11/2\"  MALE ADAPTOR",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.13","75mm x 63mm  REDUCER TEE-PIECE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.14","63mm END PLUG",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.15","63mm x 11/2\"  MALE ADAPTOR",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.16","75mm x 20MM  4 BOLTS SADDLE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.17","63mm x 20MM  4 BOLTS SADDLE",{"v":1,"d":"1.00"},"Lm",null,0]
["8.1.2.18","40mm x 20MM  TAPPING SADDLE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.19","40mm  END PLUG",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.20","40mm  EQUAL 90deg ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.21","40mm  EQUAL TEE-PIECE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.22","PTFE THREAD SEALING TAPE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.23","20MM TURF-VALVE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.24","20mm  EQUAL PLASTIC SOCKET",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.25","ROUND VALVE BOX 150mm (610)",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.26","20mm SWING JOINT RISER",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.27","20mm 772 DRAGLINE HOSE",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.28","GALV. 20mm X 600mm TUBULAR TRIPOD",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.29","20mm HOSE NIPPLE CONNECTOR",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.30","GALV. 20mm M&F ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.31","TURF VALVE KEY",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.32","20mm FEMALE CONNECTION",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.33","COMPOSITE CLAMP GS12",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.34","BRASS SPRINKLER",{"v":1,"d":"1.00"},"each",null,0]
["8.1.2.35","110mm Sleeve (SABS). To be installed before hardscaping.",{"v":1,"d":"1.00"},"Lm",null,0]
[]
[8.2,"Automatic Irrigation System"]
["8.2.1","MAINLINE & FITTINGS"]
["8.2.1.1","MAINLINE CONNECTION FITTINGS",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.2","40MM BRASS GATE VALVE",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.3","GALV. 40mm BARREL NIPPLE",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.4","40mm x 40  FEMALE TEE",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.5","JUMBO RECTANGULAR VALVE BOX 500mm DEEP",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.6","40mm  EQUAL 90deg ELBOW",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.7","40MM END CAP",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.8","40 MM TEE",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.9","SABS 40mm CL10 HDPE POLY.PIPE 100m",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.1.10","40mm  EQUAL COUPLING",{"v":1,"d":"1.00"},"each ",null,0]
["8.2.2","TURF-VALVES",{"$nulls":3},0]
["8.2.2.1","40mm x 3/4\"  4 BOLTS SADDLE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.2","ROUND VALVE BOX 150mm (610)",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.3","20mm  EQUAL SOCKET",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.4","20MM SWING JOINT",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.5","20MM PLASTIC RISER VALVE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.6","VALVE CLUSTERS",{"v":2,"d":"2.00"},"each",null,0]
["8.2.2.7","25mm F/C GLOBE VALVE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.8","ECONO 25mm PVC BALL VALVE (601/1000)",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.9","25MM MFE POLY ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.10","ROUND VALVE BOX 250mm (910)",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.11","25 X25 MALE ELBOW  FF",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.12","25mm  BARREL NIPPLE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.2.13","40mm x 25MM  TAPPING SADDLE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3","SPRINKLERS",{"$nulls":3},0]
["8.2.3.1","PRO-SPRAY, 4\"POP-UP BODY",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.2","STAND PIPE 15mm x 600mm",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.3","SHRUB ADAPTOR",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.4","MP1 ROTATOR",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.5","MP2 ROTATOR",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.6","MP3 ROTATOR",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.7","MP LEFT CORNER",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.8","MP SIDE STRIP",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.9","MP RIGHT CORNER",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.10","MSB 10F",{"v":1,"d":"1.00"},"each",null,0]
["8.2.3.11","MP CORNER STRIP",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4","SPRAYLINES & FITTINGS",{"$nulls":3},0]
["8.2.4.1","100mt x 25mm CL3 LDPE PIPE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.2","FULLFLOW 25 x 1/2\" FEM ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.3","FULLFLOW 25mm x 1/2\" FEM TEE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.4","FULLFLOW 25mm TEE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.5","FULLFLOW 25mm ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.6","PTFE TYPE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.7","FLEXIBLE SWING PIPE",{"v":1,"d":"1.00"},"each",null,0]
["8.2.4.8","15mm SPIRAL BARB. MALE ELBOW",{"v":1,"d":"1.00"},"each",null,0]
["8.2.5","CONTROL SYSTEM",{"$nulls":3},0]
["8.2.5.1","PRO-C OUTDOOR CONTROLLER",{"v":1,"d":"1.00"},"each",null,0]
["8.2.5.2","PRM3",{"v":1,"d":"1.00"},"each",null,0]
["8.2.5.3","HUNTER SOLAR SYNC",{"v":1,"d":"1.00"},"each",null,0]
["8.2.5.4","CONTROL CABLE 1,5 sq mm",{"v":1,"d":"1.00"},"each",null,0]
["8.2.5.5","314 SCOTCHLOK W/RESISTANT CONNECTOR",{"v":1,"d":"1.00"},"each",null,0]
["8.2.6","CABLE JUNCTION BOXES",{"$nulls":3},0]
["8.2.6.1","Cable junction box 150mm -- [<10 connections]",{"v":1,"d":"1.00"},"no.",null,0]
["8.2.6.2","Cable junction box 250mm -- [>10 connections]",{"v":1,"d":"1.00"},"no.",null,0]
["8.2.6.3","FLUSH AND PRESSURE TEST",{"v":1,"d":"1.00"},"sum",null,0]
["8.2.7","TRENCH/BACKFILL/PROOF/BEDDING",{"$nulls":3},0]
["8.2.7.1","Excavation and backfill -  parent material",{"v":1,"d":"1.00"},"Lm",null,0]
["8.2.7.2","Excavation and backfill - in compacted road /paving layers",{"v":1,"d":"1.00"},"Lm",null,0]
[]
[9,"ESTABLISHMENT MAINTENANCE DURING CONSTRUCTION"]
[9.1,"Maintenance for all landscaping items during construction until final completion.",1,"mths",null,0]
[9.2,"Provide the following items upon Practical completion of all works for use throughout maintenance period. (This equipment remains the propoerty of the client and is to be properly maintained throughout the maintenance period)",{"$nulls":3},0]
["9.2.1","1000L water tank & trailer (if no running water onsite) for establishment irrigation to areas which are not reached by garden taps",1,"each ",null,0]
["9.2.2","30m long heavy duty hose pipes @ all associated fittings incl. hose extension connectors",1,"each ",null,0]
["9.2.3","50m long heavy duty hose pipes @ all associated fittings incl. hose extension connectors",1,"each ",null,0]
["9.2.4","Hot dipped galvinised tripod sprinkler ",1,"each ",null,0]
[{"$nulls":5},0]
[]
[null,"SUB-TOTAL (excl. 15% VAT) ",null,"excl. VAT",null,0]
[]
[null,"TOTAL (excl. 15% VAT) ",null,"incl. VAT",null,0]

{"sheet":"Maintenance","index":2,"n_rows":113,"n_cols":6,"rows_kept":113,"merged":[[0,0,0,5],[110,3,110,4],[111,3,111,4],[112,3,112,4]],"flags":["formulas_cached_only"]}
["SCHEDULE OF RATES: Public Realm Maintenance and Establishment \n(TO BE READ WITH CLAUSE C3.3: STANDARDS, SPECIFICATIONS AND TECHNICAL REQUIREMENTS). Maintenance shall Include reporting and meet performance standards. All rates in the Bill of Quantities shall be deemed to include full compensation for compliance with the Contract, including but not limited to: Environmental Management Plan implementation, Community liaison and local labour obligations, Site establishment and consultant facilities, Protection of existing services and infrastructure, Monitoring, reporting and documentation requirements, No separate claims shall be entertained for these obligations. All work shall: Be executed in a professional and workmanlike manner,  Meet SALI accepted industry practices, Be subject to inspection and rejection if non-compliant The Contractor shall be responsible for: Reinstatement of defective work,  Replacement of failed planting, Compliance with environmental and safety requirements"]
["ITEM NO:","ITEM DESCRIPTION","QUANTITY","UNIT","UNIT PRICE (in Rands)","AMOUNT (in Rands)"]
[]
[1,"Key personnel for maintenance works. Provide rates for labour required on an 'as and when required basis'. Rates are to include transport and management. "]
[1.1,"CONTRACTS MANAGER ",1,"hr",null,0]
[1.2,"SITE AGENT",1,"hr",null,0]
[1.3,"FOREMEN",1,"hr",null,0]
[1.4,"Irrigation Specialist",1,"hr",null,0]
[1.5,"Brush Cutter ",1,"hr",null,0]
[1.6,"Blower operator",1,"hr",null,0]
[1.7,"Pest Control Operator",1,"hr",null,0]
[1.8,"Other skilled labourers",1,"hr",null,0]
[]
[null,"ALL items from here onwards are to Include ALL costs in each unit rate: Labour, Plant, Materials, Overheads, and Profit"]
[2,"Site clearance"]
[2.1,"Unwanted vegetation, stones rubble, and Litter",1,"m³",null,0]
[]
[3,"Trees, Shrus and Groundcovers"]
[3.1,"Tree staking (2x tree stakes & ties per tree)",1,"each",null,0]
[3.2,"Irrigation per tree (5-10 Litres per day)",1,"each",null,0]
[3.3,"Replacing of a tree - 200L",1,"each",null,0]
[]
[3.4,"Pruning:"]
["3.4.1","Groundcovers",1,"each",null,0]
["3.4.2","Shrubs",1,"each",null,0]
["3.4.3","Small tree (1-20cm stem diameter)",1,"each",null,0]
["3.4.4","Medium tree (21-30cm stem diameter)",1,"each",null,0]
["3.4.5","Large tree (31-50cm stem diameter)",1,"each",null,0]
["3.4.6","Extra Large tree (More than 50cm stem diameter)",1,"each",null,0]
[]
[3.5,"Taking out and removing, grubbing up roots and filling in holes"]
["3.5.1","Small tree (1-20cm stem diameter)",1,"each",null,0]
["3.5.2","Medium tree (21-30cm stem diameter)",1,"each",null,0]
["3.5.3","Large tree (31-50cm stem diameter)",1,"each",null,0]
["3.5.4","Extra Large tree (More than 50cm stem diameter)",1,"each",null,0]
[]
[3.6,"Eradication & Control of Invasive Plant Species"]
["3.6.1","Mature trees; Densely Populated; Mixed species",1,"ha",null,0]
["3.6.2","Mature trees; Sparsely Populated; Mixed species",1,"ha",null,0]
["3.6.3","Immature trees; Densely Populated; Mixed species ",1,"ha",null,0]
["3.6.4","Immature trees; Sparsely Populated; Mixed species ",1,"ha",null,0]
[]
[4,"Mowing of turf/ lawns"]
[4.1,"Mowing of Lawn & Edging\nMower blades have to be sharpened regularly and may not be raised more than 20mm. Topdressing on grass must be done",1,"m²",null,0]
[]
[5,"Replacement of dead Lawn"]
[5.1,"Sprigging of grass per/m²",1,"m²",null,0]
[5.2,"Sowing per/m²",1,"m²",null,0]
[]
[6,"Veldgrass areas (Natural areas)"]
[6.1,"Mowing/ Cutting of veldgrass and Weeding",1,"m²",null,0]
[]
[7,"Pest and Disease Control"]
[7.1,"Pest and Disease Control on all the the sites of works",1,"m²",null,0]
[]
[8,"Weeding "]
[8.1,"In veld/ open space by normal cutting process",1,"m²",null,0]
[8.2,"On lawn areas ( not removed by the normal cutting process, but removed regularly by hand. ",1,"m²",null,0]
[8.3," Aquatic weeds (must be removed by hand. and herbicides should not be used in these areas)",1,"m²",null,0]
[8.4,"On paving (in between paving bricks, concrete etc)",1,"m²",null,0]
[]
[9,"Indoor Plants"]
[9.1,"Maintenance & watering of indoor plants\nWipe off all leaf blade surfaces",1,"each",null,0]
[]
[10,"Aeration of plantbeds"]
[10.1,"Provision for aeration of plantbeds on a weekly basis by means of light forking without disturbing plant roots.",1,"m²",null,0]
[]
[11,"Clipping of Hedges",{"$nulls":3},0]
[11.1,"Hedges to be neatly clipped in a square box format at desired height ",1,"Lm",null,0]
[]
[12,"Irrigation (Maintenance)"]
[12.1,"Inspection of the Mechanical and Irrigation System and servicing: The complete mechanical and landscape irrigation system for the site's project inclusive of piping etc is to be inspected and serviced per schedule by an approved competent person representing a LIA registered Irrigation Contractor who will act as a sub contractor to the main contractor and a written report submitted as to the condition of the system. Routine replacement of small parts, repairs to leaks, adjustments of any nature etc as well as damage and losses due to the Contractor’s negligence as well as by others will be considered to be part of the routine maintenance and must be done on an as and when basis immediately upon detection. Under no circumstances will the use of foreign irrigation equipment be used as replacements.",1,"sum",null,0]
[12.2,"Turf valve system: watering by hand where necessary\nSupply of a 25m long hose pipe and 1 sprinkler",1,"daily",null,0]
[12.3,"Automatic system: running and control of automatioc irrigation system ",1,"daily",null,0]
[]
[13,"Fountains and Water Features"]
[13.1,"Inspections, cleaning, desilting, and Litter removal",1,"each",null,0]
[13.2,"Repairs to a broken water feature",1,"each",null,0]
[]
[14,"Drainage"]
[14.1,"Cleaning and unblocking of stormwater and irrigation drains\nRemoval of litter in stormwater drains",1,"sum",null,0]
[]
[15,"Services"]
[15.1,"All manholes to be kept exposed for ease of identification",1,"each",null,0]
[]
[16,"Play equipment area (maintenance only)"]
[16.1,"Repairing of broken play equipment (welding & repaint)",1,"each",null,0]
[16.2,"Replacing of a play equipment ",1,"each",null,0]
[16.3,"Rubberizing of damage areas (Rubberized areas)",1,"m²",null,0]
[16.4,"Raking and replenishing with sand (Play areas with sand)",1,"m³",null,0]
[]
[17,"Repairs to fencing & gates"]
[17.1,"Repairs to a Metal Palisade fence",1,"Lm",null,0]
[17.2,"Repairs to a Concrete Palisade fence",1,"Lm",null,0]
[17.3,"Repairs to a Invisible fence",1,"Lm",null,0]
[17.4,"Repairs to a pedestrian gate",1,"Lm",null,0]
[17.5,"Repairs to a vehicular gate",1,"Lm",null,0]
[17.6,"Supply & Install 2.4m long x 100 diameter gumpole posts",1,"each",null,0]
[17.7,"Supply & Install 2.7m long x 100x55 AA IPE section post with spear\nhead – hot dipped galvanised",1,"each",null,0]
[17.8,"Supply & Install 150mm long x 40x6mm predrilled 12mmslotted holed flat bar fishplates – hot dipped galvanised",1,"each",null,0]
[17.9,"Supply & Install 2.914m long x 50x50x5mm predrilled to receive\npales equal angle crossbar – hot dipped galvanised",1,"each",null,0]
["17.10","Supply & Install 2.050m long x 65x3mm predrilled rolled pale with\nR3 spear top security head and flat bottom – hot dipped galvanised",1,"each",null,0]
["17.11","Sundries for the above: M8 anti vandal shear nut, washers and round\nheaded bolts – electro galvanised",1,"each ",null,0]
[17.12,"Sundries for the above: M12 anti vandal shear nut, washers and round\nheaded bolts – electro galvanised",1,"each ",null,0]
[18,"Painting: fence & gates"]
[18.1,"Supply and application Galvanised iron degreaser",5,"L",null,0]
[18.2,"Supply and application of Etch Prime",5,"L",null,0]
[18.3,"Supply and application of Enamel Paint",5,"L",null,0]
[]
[]
[null,"SUB-TOTAL  (excl. 15% VAT) ",{"$nulls":3},0]
[]
[null,"TOTAL (excl. 15% VAT) ",null,"excl. VAT",null,0]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}