{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Fire Truck 4x4 4500 L","Sheet1"],"not_rendered":{"images":1,"defined_names":8},"read":"whole","date_system":"1900"}

{"sheet":"Fire Truck 4x4 4500 L","index":0,"n_rows":506,"n_cols":7,"rows_kept":506,"merged":[[5,3,5,6],[6,3,6,6],[26,0,28,0],[30,0,31,0],[32,0,35,0],[38,0,39,0],[50,0,52,0],[54,0,57,0],[60,0,61,0],[136,0,139,0],[161,0,162,0],[163,0,169,0],[182,0,184,0],[192,0,193,0],[210,0,213,0],[218,0,220,0],[236,0,237,0],[238,0,239,0],[264,0,267,0],[274,0,275,0],[280,0,282,0],[296,0,298,0],[331,0,332,0],[335,0,336,0],[373,0,377,0],[412,0,417,0],[420,0,421,0],[428,0,429,0],[457,0,458,0],[462,0,464,0]]}
[]
[]
[]
[]
[]
["Make and model of Truck and superstructure:",null,"X"]
["Country of manufacturing:",null,"X"]
[" Standard Features (Minimum requirements)",null,"Critical criteria ","Comply","Provide reason for comply or non-compliance","Indicate where to validate in datasheets / brochures","Eskom technical evaluation comments"]
["Vehicle Job Description",null,null,"Heavy Duty 4x4 Fire Fighting Vehicle Specifications\nThe chassis cab, the super-structure, pump and the electrical system of the fire fighting vehicle must meet every aspect of the National Road Traffic Act  requirements.\nManufacturer's must use latest technology throughout.","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["Overview: Truck Engine and Chassis","Truck "]
["kW output Min.","Truck ","X","309 kW (326 HP)"]
["Nm output Min.","Truck ","X","1100 Nm @ 1200 - 1750 r.p.m (280 HP @ 2300 r.p.m)"]
["Diesel driven","Truck ",null,"Yes - EURO 3 Emission level, Common-Rail with direct injection  - turbo charger"]
["Permissible front axle mass","Truck ",null,"7700 kg minimum"]
["Permissible rear axle mass","Truck ",null,"8000 kg minimum"]
["All-wheel drive","Truck ","X","4x4 with differential locks on front and rear axle. "]
["Wheels","Truck ",null,"Single rear wheel application"]
["Tyres (Size) ","Truck ","X","Tyres (Size) 1400R20 Steel radial Tyres (Michelin XZL)  (up to 80% off road usage) Compatible diff ratio or equivalent"]
["GVM","Truck ","X","Approx. 18000 kg "]
["D/T Rating “Min.”","Truck ",null,"44 000 Kg"]
["Wheelbase “ Max.” Centre front axle to centre of rear axle unit","Truck ",null,"4800 mm (rear overhang not more than 1800 mm)"]
["Semi-Automatic trailer coupling","Truck ",null,"Yes - with electric supply"]
["Airline booster connection (SABS 1207-1985)","Truck ",null,"Yes"]
["Fuel tank","Truck ",null,"Minimum 250 litres"]
["Electrical system","Truck ",null,"24 V with 2 x 12 Volt, 165 Ah batteries"]
["Electrical wiring","Truck ",null,"All electrical wiring is protected from chafing by use of protective looms and grommets where wiring passes through body. All wiring is distributed via lockable distribution boxes. "]
["Regulated battery charger","Truck ",null,"A regulated battery charger with auto eject plug is fitted to the vehicle, for charging the batteries from external 220V source. "]
[null,"Truck ",null,"A battery isolation switch is fitted to completely isolate the battery. "]
[null,"Truck ",null,"No direct connections from batteries will be accepted."]
["Transmission","Truck "]
["Type ","Truck ","X","Fully automatic Gearbox"]
[null,"Truck ",null,"The gear engaged at any given time must be indicated on the display console."]
["Power Take Off (P.T.O.)","Truck ",null,"The power take-off (PTO) controls will be adjacent to the driver in the cab and pump operator's panel."]
[null,"Truck ",null,"Power take-off engagement warning lights shall be installed in the cab instrument panel and pump operator's panel."]
[null,"Truck ",null,"Engagement of the PTO will be possible in order to facilitate the pump and roll function."]
[null,"Truck ",null,"The PTO ratio will be matched to the pump and vehicle engine to ensure the pump's optimum performance is achieved with the engine rpm within the green band."]
["Cooling System","Truck "]
["Cooling system","Truck ",null,"Water forced circulation by pump. Tubular finned radiator with thermostat."]
["\nEngine cooling","Truck ",null,"The engine cooling system will permit continuous stationary running of the engine without overheating when the subsidiary power take-off (PTO) is engaged."]
[null,"Truck ",null,"The system shall also permit the main pump to run continuously without the engine operating temperature exceeding the limits as specified by the engine manufacturer."]
["Engine, Gearbox & PTO oil cooling","Truck ",null,"If necessary, means shall be provided for the cooling of the oil in the engine, gearbox and power take-off."]
["Instrumentation","Truck ",null,"Suitable temperature indicators shall be provided in the cab and pump instrument panels that indicate the temperature of both cooling water and engine systems and shall be appropriately marked with normal operating temperatures parameters."]
["Air system","Truck ",null,"A dry air cleaner of the Cyclopac type or similar will be fitted."]
["Fuel System","Truck "]
["Diesel Driven","Truck ",null,"A fuel tank with a capacity of not less the 180 litres shall be provided. The fuel capacity shall allow for continues pumping operations at maximum capacity for not less than four hours."]
["Fuel Filling","Truck ",null,"A large, clearly marked filling facility will be provided on the exterior of the vehicle."]
["Water separator","Truck ",null,"The fuel system will be fitted with an effective water separator in addition to the normal inline fuel filter."]
["Brake System","Truck "]
["Braking system","Truck ","X","ABS braking system shall be installed that is specifically designed for Fire Brigade service."]
[null,"Truck ",null,"The dimensions and areas of the brake disk / linings are to ensure that the vehicle in its full GVM condition shall comply with all Road Traffic legislative requirements and the minimum figures stipulated by the South African Bureau of Standards. The vehicle braking system shall have the following as a minimum:"]
["Disks & Drums","Truck ",null,"• Full air operated disc/drum brakes shall be installed."]
[null,"Truck ",null,"• Full ABS braking system"]
[null,"Truck ",null,"• Dual braking system, with split circuits front and rear."]
["Air Reservoirs","Truck ",null,"• All air reservoirs will have drain and safety valves suitably protected from damage."]
["Parking Brake","Truck ",null,"• A spring-operated, fail-safe parking emergency brake is required."]
[null,"Truck ",null,"• The parking brake shall be capable of holding the fully laden vehicle stationary on a dry surface gradient of 1:4."]
[null,"Truck ",null,"• An indication lamp will be provided on the instrument panel in the cab to indicate when the parking brake is applied."]
[null,"Truck ","X","• Provision shall be made to allow the mechanical release of the parking brake in the event of low air pressure."]
["Leak rate","Truck ",null,"• The leakage rate, if any, shall still allow for the release of the parking brake after standing for 24 hours. "]
["Steering","Truck "]
[null,"Truck ",null,"A power assisted steering system shall be installed with a suitably sized steering wheel."]
[null,"Truck ","X","Power steering hydraulic - right-hand drive"]
[null,"Truck ",null,"Turning circle ","Specify"]
["Crew Cab","Truck "]
[null,"Truck ",null,"The cab shall be of sufficient size to accommodate Driver, Officer and Crew of four (4) and will be entirely closed."]
["Cab/chassis fixing","Truck ",null,"The cab will be so designed, and so attached to the chassis as to eliminate to the greatest possible extent the risk of injury to the occupants in the event of an accident."]
[null,"Truck ",null,"The crew cab must be of the original chassis Manufacturer, and MUST carry chassis manufacturers approval and comply with all International Automotive Safety Standards."]
[null,"Truck ",null,"Such approvals must accompany tender documents."]
[null,"Truck ",null,"All seating shall be forward facing."]
["4 forward opening doors","Truck ",null,"The cab will be fitted with four (4) forward opening doors."]
["Cab steps","Truck ",null,"There shall be at least three (3) entry steps at every door with step illumination."]
["Cabin Floor","Truck ",null,"Floor need to be covered with a spray on non slip material"]
["Anti-burst door catches","Truck ","X","All door catches will be of the anti-burst type and will be internally recessed to prevent unintentional opening."]
["Door opening","Truck ",null,"Doors shall open to at least 85O from the longitudinal centre of the cab."]
[null,"Truck ",null,"ALL doors to be fitted with reinforced hinge stop / limiter."]
["Cab internal dimentions:Min length","Truck ",null," 2 600 mm"]
["Cab internal dimentions:Min width ","Truck ",null," 2 500 mm"]
["Min  Floor to Ceiling height","Truck ",null," 1 600 mm"]
["Min  Seat to Ceiling height","Truck ",null," 1 380 mm"]
[null,"Truck ",null,"All equipment stowed in the cab must properly mounted and secured to prevent equipment dislodging while the vehicle in motion."]
["Toughened glass","Truck ","X","All glass will be toughened safety glass and each piece shall be permanently marked describing it as such."]
[null,"Truck ",null,"The design of the cab shall be such as to ensure maximum visibility for the driver."]
["Driver's seat","Truck ","X","Air suspension seat, a bucket-type and fully adjustable for weight, height, reach and tilt."]
[null,"Truck ",null,"The officer and crew seats will be forward facing and the crew seats will be provided with a full width crash bar."]
["Crew seats","Truck ",null,"All seats, the driver's backrest and crash bars will be fully upholstered and covered in heavy duty durable materials."]
["SCBA in backrest","Truck ",null,"The backrest of the crew seats will be provided with quick release bracket suitable for carrying Self Contained Breathing Apparatus (SCBA) sets (Drager PA-91 or similar). "]
[null,"Truck ",null,"The bracket will be a rubber plastic construction (no metal) to eliminate damage to composite cylinders when stowed."]
[null,"Truck ",null,"The brackets shall be fitted with quick release collision restraint straps able to withstand a minimum of 10 G forces."]
["SCBA","Koeberg",null,"Note: Four (4) SCBA sets and fitted  in the cab as part of the back rest of crew seats"]
[null,"Koeberg",null,"four (4) spare cylinders to be supplied in fitted in the 1st locker behind the cab on the right hand side"]
[null,"Truck ",null,"All loose equipment carried in the cab will be secured in such a way as to prevent it being dislodged in the event of an accident."]
[null,"Truck ",null,"Access to the cab will be entirely unobstructed and doors will be forward swung on steel hinges with check straps."]
["Crew cab Cab steps","Truck ",null,"Large steps or step walls will be provided for entering or leaving the cab."]
[null,"Truck ",null,"Noise level in the cab will not exceed 80 dba and if necessary, soundproofing materials will be installed to limit noise below this level."]
["Cab mirrors","Truck ",null,"Large exterior and blind-spot mirrors will be provided."]
["Vehicle control in Cab","Truck ","X","All control necessary for the safe operation and control of the vehicle whilst in motion will be within easy reach of the driver with his seat belt fastened."]
["Air-conditioning","Truck ","X","The cab shall be fully air-conditioned with independently  controlled front and rear vents. "]
["Safety requirements","Truck ","X","The crew cab shall meet ECE29 safety requirements. ECE29 refers the European standard for the approval of vehicles with regard to the protection of the occupants of the cab of a commercial vehicle. (More information attached)"]
["Cab Instruments, warning devices and controls:","Truck ",null,"The vehicles cab is fitted with comprehensive range of instruments and controls as standard and shall include;\n\n"]
["Display","Truck ","X","Universal with 9\" LCD display, GPS, Radio, Bluetooth and reverse camera"]
["Rear camera","Truck ","X","Reverse camera to be installed with a full colour display on the display system"]
["VHF Radio","Koeberg",null,"• A VHF two-way radio will be provided by Eskom to be  installed within easy reach of the driver and officer positions in the cab. Radio frequencies will be provided by the end user."]
[null,"Koeberg",null,"• A VHF Radio antenna shall be installed on top of the cab with coaxle trunked to the radio installation."]
["Warning devices, switches and vehicle instrumentation and controls","Truck ",null,"• Parking brake controls with lock and warning light"]
[null,"Truck ",null,"• Battery isolation switch easily accessible to the driver"]
[null,"Truck ",null,"• Fuse or circuit breaker box"]
[null,"Truck ",null,"• Fog lamp switch and warning light indicating lights on"]
[null,"Truck ",null,"• Cab interior lamps and switches"]
[null,"Truck ",null,"• Master locker light switches and warning light on"]
[null,"Truck ",null,"• Windscreen wiper and washer control"]
[null,"Truck ",null,"• Power take engagement warning lamps"]
[null,"Truck ",null,"• Fuel tank contents gauge"]
[null,"Truck ",null,"• Engine coolant temperature gauge and lubricant temperature gauge"]
[null,"Truck ",null,"• Engine oil pressure gauge"]
[null,"Truck ",null,"• Warning lights bar switches"]
[null,"Truck ",null,"• Warning / PA audio system switch"]
[null,"Truck ",null,"• Air reservoirs pressure gauge"]
[null,"Truck ",null,"• Cab heater / demister controls"]
[null,"Truck ",null,"• Air-conditioning controls switches"]
[null,"Truck ",null,"• Speedometer and Odometer registering in kilometres per hour (kph) and kilometres respectively."]
[null,"Truck ",null,"• Engine tachometer"]
[null,"Truck ",null,"• Hour meter for recording of engine running time"]
[null,"Truck ","X","• LED Light mast extended with warning light & buzzer in CAB"]
[null,"Truck ",null,"• Packet (Locker) door \"OPEN\" visual warning light"]
["Vehicle measurement","Truck "]
[null,"Truck ",null,"The design of the vehicle should take the following measurements into consideration;"]
["Approach angle","Truck ","X","• 30 degrees","Specify"]
["Departure angle","Truck ","X","• 30 degrees","Specify"]
["Static side slope stability","Truck ",null,"• 28 degrees","Specify"]
["Max Width of vehicle","Truck ",null,"• 3100mm including mirrors","Specify"]
["Length","Truck ",null,"• 10 584mm","Specify"]
["Max Height--Including monitor","Truck ",null,"• 3 900 mm ","Specify"]
["Bull Bar / Tow Eye / Electric Winch","Truck "]
["Bull Bar","Truck ",null,"Heavy duty diameter seamless 304 grade \"stainless steel\" round tubing bull bar for additional protection of vehicle frontal areas shall be installed."]
["Recovery Hooks","Truck ","X","Two (2) heavy duty tow eyes shall be installed on either side (left and right) in both the front and the rear of the vehicle."]
["Tow hook ","Truck ","X","Self-locking Tow hitch with a 40mm pin to be fitted directly to the chassis, and chassis to be re-inforced for heavy duty towing ."]
["Winch","Truck ","X","An electrically operated winch capable of pulling not less than 7500 kg capacity, fully reversible shall be installed. A snatch block to be provide to sue with the winch during recoveries."]
[null,"Truck ",null,"The winch shall have a minimum of 30 m x 9 mm galvanized aircraft type cable and a replaceable hook. "]
[null,"Truck ",null,"The winch shall be mounted to the chassis frame with an extension centred at the front bumper. "]
[null,"Truck ",null,"A 9 m remote control cable and switch shall be provided."]
["Major fire fighting vehicle components for the fire tender ","Fire "]
["Subframe ",null,"X","Subframe of structrure to be hot dip galvanised"]
["Pump","Fire ","X","• Firefighting pump capable of 4 500 lpm @ 10 bar maximum flow but not less than 4 000 lpm."," "]
["Superstructure","Fire ",null,"• Superstructure with all mounted components"]
["Water tank","Fire ","X","•Non corosive light weight water tank of not less than 3 000 litre usable capacity "]
["Foam tank","Fire ","X","• Non corosive light weight foam tank of 250 litre capacity"]
["Foam mixing","Fire ",null,"• Foam Proportioning unit 0,5%, 1,0% and 3%"]
["Water monitor","Fire ",null,"• Roof foam/water monitor capable of 3 000 - 4 000 lpm @ 10 bar."]
["High pressure hose reels","Fire ","X","• Two (2) x High Pressure Hose Reels (one of either side of vehicle with electric wind) 350 - 400 lpm @ 40 bar."]
["Light mast","Fire ",null,"• Light mast with all round LED floodlights."]
["Fire-fighting superstructure","Fire "]
["Main components found on vehicle superstructure","Fire ",null,"The superstructure is composed of 3 sections mounted independently on the chassis;"]
["Pump compartment","Fire ",null,"• The pump compartment and equipment lockers at the rear of unit."]
["Water and foam tank","Fire ","X","• The water and foam tank in the center"]
["Lockers and compartments","Fire ","X","• The equipment locker just behind the crew cab."]
[null,"Fire ",null,"Modern technologies like bending, gluing and screwing are preferred. "]
[null,"Fire ","X","Where the bodywork manufacturer is not the chassis manufacturer, the ultimate design of the vehicle will be approved by the chassis manufacturer and the end-user."]
[null,"Fire ","X","The design of the vehicle will be such as to facilitate maintenance and repair and to give as low a centre of gravity as practicable."]
[null,"Fire ","X","The vehicle will be systematically proportioned with due consideration to the distribution and nature of the load to be sustained."]
["Rear camara","Fire ","X","A rear facing camara system will be installed with a full colour display located in the driver's cab."]
[null,"Fire ","X","All structural components and materials will be of the highest grade."]
["Materials ","Truck ",null,"Only AA International Quality 6063 T6 and 6261 T6 will be accepted./AA 6063 is an aluminium alloy, \nwith magnesium and silicon as the alloying elements. ... T6 temper 6063 has an ultimate tensile strength of at least 190 MPa (28,000 psi) and yield strength of at least 160 MPa (23,000 psi). ... Nonferrous Alloys and Special-Purpose Materials, Vol 2, ASM Handbook, ASM International, 1990, p.\nFatigue performance of 6261-T6 aluminium alloy - Constant and variable ... Article in International Journal of Fatigue 19(93):109-118 · June 1997 with 52 Reads ... and specimens in which weld `quality' (as assessed by profile, heat affected zone hardness, extent and microstructure) varied. .... Welding of Aluminum Alloys."]
[null,"fire ",null,"All body panels will be painted except where thread bright panels are fitted."]
["Walkways and floors","Fire ",null,"The minimum thickness of all walkways and locker floors shall be over 3  - 4.6 mm."]
[null,"Fire ",null,"Walkways, steps and floors shall be supported by a structural member every 550 - 600 mm."]
[null,"Fire ",null,"All vertical plain or thread bright panels shall be a minimum 2 - 3 mm thick."]
[null,"Fire ",null,"All structural frames shall be of 6063 aluminium tubing and must be full welded at every joint."]
[null,"Fire ","X","No ferrous metal body framework or panels will be accepted."]
[null,"Fire ",null,"A full description of materials and applications must be submitted with tender in a covering letter."]
[null,"Fire ",null,"Any variations to this specification will not be accepted."]
["Lockers and compartments","Fire ",null,"Off Side (righthand side ) and nearside(lefthand side) top locker will have two (2) shelves."]
[null,"Fire ","X","All compartments will be dust and weather resistant and shall have flush fitting locks."]
["Total locker space","Fire ",null,"Total locker capacity should be approximately 6 m3."]
["Locker open warning sensor","Fire ","X","All Roller Shutter doors are to be fitted with \"OPEN POCKET / LOCKER\" warning sensor with light mounted on the driver's console."]
["Locker hold open","Fire ","X","Roller shutters shall be provided with an efficient means to hold the door open when in use."]
["Walk-on fold down locker/step","Fire ","X","Flip-down access steps shall be provided at all lockers, so that upper shelves are easily reachable, including those above the wheel arch (step integrated with arch)."]
[null,"Fire ","X","All flip-down doors will be fitted with double click anti-burst door locks."]
["Roller shutter doors","Fire ",null,"Roller shutter doors shall be fitted with \"Bar Lock\" mechanism for preventing accidental door opening whilst in motion."]
[null,"Fire ","X","All roller shutter doors must be lockable by means of a central operated locking system (Central Locking), the switch situated on the driver's console and fitted with an override system, which can be activated, in the event of air failure."]
[null,"Fire ",null,"Off side top locker will e fitted with a swing-out shelf , nearside bottom locker will be fitted with a pull out drawer of full door width."]
[null,"Fire ",null,"The roller shutter doors will be of an aluminium type."]
["Deck access","Fire ","X","Suitable provision will be made for climbing onto the deck and all grab handles. Locks and hinges will be stainless steel or chromium plated."]
["Decks and floors","Fire ","X","The deck, back step and floor of the crew compartment will be covered with aluminium chequer plate."]
[null,"Fire ","X","Kick plates will be provided where damage to the paint is likely from climbing into or onto the unit."]
[null,"Fire ","X","Special attention should be paid to the mudguard areas Step Tread. Decking, platforms and kick plates will be of aluminium chequer plate."]
["Under cab protection","Fire ","X","Cab and body will be provided with suitable under body protection against rust."]
["Water Supply","Fire "]
["Water tank","Fire ","X","Non corosive light weight  water supply tank with a carrying capacity of not less than 3,000 litre with baffel system shall be installed. "]
["Foam tank","Fire ","X"," A separate foam tank with a capacity of not less than 250 litres of foam concentrate. "]
["Warrenties on Tanks",null,null,"Water tank "]
[{"$nulls":3},"Foam Tank "]
["Pump output requirements","Fire ","X"," A rear mounted, mutli-stage centrifugal fire pump with the following minimum capacities; "]
["A centrifugal multi-stage fire fighting pump","Rhine ","X","Normal Pressure - Not less than 4 500 lpm @ 10 Bar pressure"]
[null,"Rhine ","X","High Pressure - not less than 400 lpm @ 40 Bar "]
[null,"Fire ","X","Around the pump foam proportioning system with a pre-set of 0.5%, 1% and 6% foam mix. (Note: NOT a foam induction system.)"]
["Stowage, Lockers & Bodywork","Fire "]
["Lockers shall be incorporated into the vehicle body and shall be flush mounted.","Fire ",null,"On each side of the vehicle, there must be three (3) lateral storage lockers. "]
[null,"Fire ",null,"The lockers must be equipped with light alloy roller shutters, which prevent any dust entering the compartments."]
["Swing down doors","Fire ",null,"Lower part compartments must have swing down type doors, which can be used as standing on platforms for the firefighters to access gear stowed higher in lockers."]
["Roller shutter doors","Fire ",null,"The roller shutter doors are fully enclosed within structural members and shall not obstruct the clear door opening."]
["Centre of gravity","Fire ",null,"The superstructure is constructed to ensure the lowest possible center of gravity and minimum height for removal of heavy objects from lockers."]
["Locker fold-down for access to higher lockers","Fire ",null," As indicated, the lower part of the equipment rear lockers shut by tailboard flaps which are hinged and used and used as treads for access to the equipment lockers."]
["Non-slip","Fire ",null,"The areas which can be walked on are covered with aluminium tread plate and coated with a non-slip material."]
["LED illumination in lockers","Fire ",null,"Lockers are illuminated by LED strip Illumination in each locker and it is activated by electromagnetic switches on opening locker doors. "]
["Secure mounting","Fire ",null,"Firefighting equipment will be securely mounted in the equipment lockers. "]
["Pump locker","Fire ",null,"The rear pump compartment is also fitted with a lockable roller shutter door and shall be well illuminated."]
["Roof access","Fire ",null,"Access to the roof is obtained via access ladder mounted at the rear of the superstructure on the left side of the vehicle."]
["Fire Fighting Pump","Fire "]
["A multi-stage centrafugal fire fighting pump to be installed and matched with vehicle engine capacity and output.","Fire ","X","A rear mounted multi-stage centrafugal fire fighting pump complying with EN 1028 and UL certification shall be installed. The pump shall be matched with the vehicle engine capcity but shall not be lower than the required specifications."]
["Pump discharge rate","Fire ","X","Centrifugal fire pump with minimum discharge of not less than 4 500 lpm @ 10 bar. "]
["Power Take Off (P.T.O.)","Fire ","X","Power for driving the pump shall be taken from the vehicle engine via a P.T.O. transfer gear box."]
[null,"Fire ","X","The power take-off (PTO) controls will be on the  pump operator's panel."]
[null,"Fire ","X","Power take-off engagement warning lights shall be installed  pump operator's panel."]
[null,"Rhine ","X","Engagement of the PTO will not impair the vehicles ability to pump and roll. "]
["Pump Specifications","Rhine ","X","The firefighting pump shall compy with EN 1028 or NFPA 1901."]
["Type","Fire ","X","Multiple stage centrifugal pump"]
["Volume pump output:","Fire ","X","Not less than 4 500 lpm @ 10 bar."]
["High pressure pump output:","Fire ","X","Not less than 400 l/min at 40 bar"]
["Materials","Fire ","X","Castings (impeller, pump cover, pump housing) are made from sea-water resistant light metal alloy. "]
[null,"Fire ","X","All wet pump components will be of corrosion resistant materials which will be compatible to avoid galvanic effects."]
[null,"Fire ","X","A flexible connection from the tank to the pump inlet, with a straight through pneumatic butterfly valve will be installed between the tank and pump inlet control in an easily accessible position for the operator."]
["Pump drain","Fire ","X","A  drain valve will be provided at the bottom of the pump casing; the control being arrange so as to prevent the cock opening from vibration. "]
["Cooling system","Fire ","X","A suitable cooling system will be incorporated to prevent heating of water in the hose reel lines when the branch nozzle is closed."]
["Controls","Fire ","X","All controls are mounted at the pump operator’s panel and partially in the driver’s cab. "]
["Pump configuration","Fire ","X","Normal pressure and high pressure pump on one shaft."]
["Normal pressure","Fire ","X","1 - stage centrifugal pump"]
["Normal Pressure Performance","Fire ","X","Not less than 4 500 lpm @ 10 bar"]
["High pressure","Fire ","X","4 - stage centrifugal pump "]
["Cooling system","Fire ","X","A suitable cooling system will be incorporated to prevent heating of water in hose reel lines when the branch is closed."]
[null,"Fire "]
["High Pressure Performance","Fire ","X","Not less than to 400 lpm @ 40 bar"]
["Sealing","Fire ",null,"Maintenance free mechanical sealing"]
[]
["Pump suction intake","Rhine ","X","Pump intake/s shall be fitted with 5.5 inch ERT/STORTZ couplers compatable with Koeberg and city of cape town, and a non-ferrous conical strainer/s and blank-cap/s."]
["Pump hydrant intake","Fire ",null,"A three-way collecting head (aluminium type construction) with three 65 mm instantaneous male couplings with non-returnable valves and female blank caps shall be supplied."]
["Tank to pump","Fire ",null," Water Tank fitted with automatic filling control funtion (pneumatic control valve.)"]
["Foam  inlet","Fire ",null,"A foam tank suction inlet and hose shall be provided"]
[null,"Fire ",null,"A foam tank flushing line shall be provided"]
["Water inlet","Fire ",null,"A water tank suction inlet shall be provided"]
[null,"Fire ",null,"Pump to tank shall be via the main panel controls."]
["Suction hoses","Rhine ","X","Four (4) reinforced rubber suction hoses, each at least 2,5 m in length and with an internal diameter of 5,5inch  to suit the pump intake will be provided and shall be properly mounted (stowed) on the vehicle."]
[null,"Fire ",null,"Suction hoses shall be fitted with aluminium Storz/ERT type couplings."]
[null,"Fire ",null,"At least two (2) suitably sizedand robust Storz/ERT coupling spanners with rubber handle grips will be supplied."]
["Strainers","Fire ",null,"A stainless steel strainer and a basket strainer will be provided."]
[null,"Fire ",null,"Suction hoses, strainers and spanners will be accommodated in an accessible position and securely mounted."]
["Water delivery","Fire ",null,"Four (4) controllable delivery outlets with 65 mm (British Standard) instantaneous female type couplings and blank caps with pressure release lugs, 2 on the  left-hand side and 2 on the right-hand side of the pump intake. "]
["Hose Reels","Fire ",null,"Two 19mm high pressure hose reels 45 m long (able to handle maximum capacity) shall be provided on either side of the vehicle. The hose reels shall have electric rewind. Hoses shall be connected with suitably sized storz or compatible coupling to allow for extention or the changing of branches."]
["Monitor Outlet","Fire ",null,"A single direct outlet with extender to the roof-mounted water/foam monitor. Control via remote control."]
["Priming pump","Fire "]
["Auto controlled primer","Fire ",null,"The priming pump will be automatically controlled by the pressure in the pump."]
["Performance Priming Pump","Fire ",null,"3 m suction height in 5 seconds @ normal atmospheric pressure (0,975 bar)"]
["Foam Proportioning Unit","Fire "]
["A foam proportioning system to work as a complete unit (matched) with the installed pump","Rhine ","X","An automatic normal and high pressure around the pump foam proportioning system designed to work seamlessly with the installed fire fighting pumps shall be installed. Please note, NO induction type system will be acceptable.","All options "]
["Design","Fire ","X","Around the pump foam proportioning system"]
["Flow measurement","Fire ","X","Mechanical, water measuring cone. Foam flow will be proportionate to water flow."]
["Metering","Fire ","X","Fully automatic, mechanically controlled, foam agent dosing cone. "]
["Foam agent suction lift","Fire ","X","High external foam suction capacity, 2 m (foam viscosity of 20 cSt) through a 1.5\" suction line. "]
["Foaming agent output","Fire ","X","Not less than 300 lpm"]
["Foam types","Fire ","X","Must be able to handle all standard types of foam agents like Protein - Fluoroprotein as well as Synthetic and AFFF type foams."]
["Admixing rate","Fire ","X","Foam Proportioning at 0,5%, 1,0% and 3%. One rate for High Pressure. Constant admixing - independent of pump output."]
[null,"Fire","X","A foam pump for the argmenting of the foam supply or filling of the foam tank shall be installed and shall be operable from the pump operating compartment."]
["Water tank ","Fire "]
["Water tank materials and capacity","Fire ","X","A polyethylene roto-moulded water tank of not less than 3 000 litres usable capacity and a separate foam tank of not less than 250 litres is required. (Tenderer to state type of materials to be use manufacturing process and tank capacities as well as period of guarantee) "]
["Water capacity","Fire ","X","Not less than 3000 litre usable capacities "]
["Material","Fire ","X","Polyethylene, roto-moulded"]
[null,"Fire ","X","The entire tank must be incorporated in the superstructure of the vehicle."]
[null,"Fire ","X","Note: NO stainless steel construction will be accepted."]
[null,"Fire ","X","All piping and fittings will be of corrosion resistant type materials."]
["Attachment","Fire ","X","The tank shall be attached with Stainless steel straps to a seperate frame and the frame mounte to the chassis with heavy duty rubber mountings to allow movement of the chassis when in off raod conditions.. "]
["Centre of gravity","Fire ","X","The tank shall be mounted in such a manner as to achieve the lowest conveniently possible centre of gravity."]
["Tank design","Fire ","X","Note: NO floating tank designs will be accepted."]
["Easily removable tank","Fire ","X","The tank shall be mounted in such a way that it can be easily removed for repair, without having to remove major body panels. "]
["Manhole cover","Fire ","X","A 500 mm diameter covers with snap closure and removable sieve "]
["Baffle plates","Fire ","X","The tank shall be suitably baffled to prevent surge whilst the vehicle is in motion and piping will be provided with an anti-vortex plate over the connection to the pump."]
["Filling lines","Fire ","X","Two filling lines, one each side, with 65mm male instantaneous coupling and blank cap and pneumatic actuating valve. "]
[null,"Fire ","X","Tank and fill will be fitted with an automatic and system to maintain tank level between 75% and 100% when connected to hydrant/s."]
["Overflow","Fire ","X","Tank overflow system with spillage prevention shall be provided that will prevent the tank from over-pressurising."]
[null,"Fire ","X","The overflow tube will be so positioned and baffled to prevent loss of water, due to surge and tilting."]
[null,"Fire ","X","Any overflow  will discharge behind the rear wheels and beneath the chassis."]
["Draining","Fire ","X","A drain cock at the suction sump shall be provided."]
["Tank level indication","Fire ","X","A suitable LCD water tank contents gauge will be installed at the pump operator's panel and duplicated on both sides of the vehicle with LED lights."]
[null,"Fire ","X","The side content gauges will consist of five (5) 50 mm LED lights (three (3) Green 100%, 75% and 50%) - (One (1) Amber 25%) - (One (1) Red 0%) "]
[null,"Fire ","X","A suitable electronic foam tank contents gauge will be installed at the pump operator's panel."]
["Foam tank","Fire "]
[null,"Fire ","X","The foam tank suitable for transporting and storing all known brands of synthetic or protein based foam compounds shall be integrated in the water tank."]
["Capacity","Fire ","X","Not less than 250 litres of foam concentrate."]
["Material","Fire ","X","Polyethylene, roto-moulded"]
["Manhole cover","Fire ","X","One 500 mm manhole with snap closure and removable sieve "]
["Filling line","Fire ","X","One filling connection with Storz D/suitable coupling, blank cap and sieve"]
["Suction line","Fire ","X","One suction connection for proportioning unit, remote controlled"]
["Overflow","Fire ","X","One line with overflow and aeration / de-aeration unit"]
["Tank indication","Fire ","X","Tank level is displayed on the control unit screens."]
["Deck mounted Water / Foam Monitor ","Fire "]
["Roof mounted water / foam monitor","Fire ","X","A remote controlled Roof Monitor which is of a design that both water and foam can be used shall be installed at the rear above the pump compartment. "]
["Branch","Rhine ","X","Shall be installed with an Akron or TFT type, fully automated and capable of discharging water or foam. Specify types and prices (include specifications) Eskom to decide on type offered.   "]
["Discharge capacity","Fire ","X","The monitor shall be capable of delivering between 3500 and 4000 lpm @ 10 bar."]
["Controls","Fire ","X","Full movement of the monitor rotation and elevation as well as nozzle control (jet-spray or jet-fog) shall be via a remote control system from 0 - full discharge."]
[null,"Fire ","X","The hand control unit must be housed close to the pump in the rear compartment."]
[null,"Fire ","X","Monitor must allow for spray or jet to be continuously adjustable."]
["Rotation","Fire ","X","Up to 300 degrees minimum."]
["Elevation","Fire ","X","From -20O to +70O minimum."]
["Throw range","Fire ","X","Approximately 70 m @ 10 bar"]
["Manual operation","Fire ","X","Manual operation must be capable in the event of system power failure."]
["Controls & Gauges","Fire "]
["Integrated pump and vehicle control system","Rhine ",null,"A fully integrated pump and vehicle ancillary control panel system that controls the entire vehicle shall be installed in the pump compartment and also in the cab."]
["Labelling of gauges and controls","Fire ",null,"The following gauges, controls, valves and equipment located in the pump panel and will be clearly labelled on engraved labels and shall include:"]
[null,"Fire ","X","•  electronic water and foam tank level indicators suitable illuminated"]
[null,"Fire ","X","•  engine revolution counter"]
[null,"Fire ","X","•  engine temperature gauge and warning light"]
[null,"Fire ","X","•  engine oil pressure gauge"]
[null,"Fire ","X","•  compound pressure gauge for both vacuum and incoming pressure - positive side pressure calibrated to 25 bar and negative side calibrated to -1 bar. The gauge sweep will be divided equally between negative and positive. "]
[null,"Fire ","X","•  pressure gauge for high pressure discharge - for High and Low pressure with large diameter calibrated in bar for main pump and hose reels."]
[null,"Rhine ","X","•  controls for foam discharge"]
[null,"Rhine ","X","•  tank to pump control"]
[null,"Rhine ","X","•  tank fill controls (hydrant to tank) and valve switch"]
[null,"Rhine ","X","•  hose reel control valves"]
[null,"Rhine ","X","•  pump inlet and deliveries with shut-off valves"]
[null,"Rhine ","X","•  pump cooling system control"]
[null,"Fire","X","•  pump grease nipples and lubrication ports"]
[null,"Fire ","X","•  pump operating hour meter"]
[null,"Fire ","X","•  light mast control and switches"]
[null,"Fire ","X","•  pump primer controls"]
[null,"Fire ","X","•  locker, deck, scene and pump compartment light indicators and switches"]
[null,"Fire ","X","•  PTO engagement switch with indicator lights"]
[null,"Fire ","X","•  electronic pump speed control with engine emergency stop / start"]
["Engine, Gearbox & PTO oil cooling","Fire ",null,"If necessary, means shall be provided for the cooling of the oil in the engine, gearbox and power take-off."]
["Instrumentation","Fire ","X","Suitable temperature indicators shall be provided in the cab and pump instrument panels that indicate the temperature of both cooling water and engine systems and shall be appropriately marked with normal operating temperatures parameters."]
["High Pressure Hose Reel","Fire "]
["High pressure hose reels","Fire ","X","Two High-pressure hose reel shall be installed. "]
["Position","Fire ","X","Left and Right-hand side in the equipment locker behind the rear wheels."]
["Type","Fire ","X","Hose reel with brake being connected with the centrifugal fire pump."]
["Hose & Branch","Fire ","X","Each Hose Reel shall be equipped with 45 m, non-deformable 19mm diameter delivery hose, coupled to a trigger operated, pistol grip type turbo-branches. "]
[null,"Fire ","X","All components of the hose reels including branch, coupling and hose, shall be capable of +40 bar working pressure."]
["Couplings","Fire ","X","Hoses shall be attached to the drum and at the branch connection, by Storz/equivalent coupling. "]
["Hose Guides","Fire ","X","Each Hose Reel shall be equipped with hose guides to allow hose to be run at approximately right angles to the centre line of the reel."]
["Electric coiling","Fire ","X","Each hose reel will be provided with an electrical and mechanical over-ride rewind mechanism."]
[null,"Fire ","X","Crank handles shall be supplied for mechanical rewinding of the hose onto the hose reel drum in the event of electric rewind failure."]
["Foam tubes","Fire ","X","Branches shall be equipped with air rating foam tubes."," "]
["Control","Fire ","X","Branches shall be capable of full control between jet and spray."]
["Under truck Nozzles","Fire "]
["Under truck Nozzles","Fire ","X"," The under truck nozzles consists of 3 ground spray nozzles in front and 1 ground spray nozzle in front of each of the rear axles.\nThe body/ground protection unit is used at ground fires under the vehicle for protection of the rear and front wheels.Able to operate from inside the cab while driving.\n"]
["Ladder","Fire "]
["Mounting","Fire ",null,"A ladder bracket for the easy removal of the 2-section fireman’s ladder shall be mounted above the superstructure. Ladder to be supplied"]
["Mounting and lowerring mechanism","Fire ",null,"The ladder housing system shall be such that over-reaching shall not be necessary to slip, ship or stow the ladder."]
["Ladder reach","Koeberg",null,"The ladder shall have a reach of not less than 10 m in height."]
[null,"Koeberg",null,"The 7.4m Duo Safety 2 section NFPA ladder, quoted for in the equipment list, will be mounted in the bracket"]
["Roof area"]
["Gantry box",null,null,"Gantry box for 8 x20 litre spare foam drums, Ladder equipment"]
["Roof Light Mast","Fire "]
["5 m Mast Flood-light system","Fire ","X","An pneumatic extendable Light Mast with a minimum height of 5 meters shall be installed. "]
["LED type lights","Fire ","X","The mast shall have 4 x High Power LED Flood Lamps. Each lamp shall have a high output of 7000 lumens and total of 28000 lumens"]
[null,"Fire ","X","The LED lamps must be positioned in such a way that entire surroundings are illuminated."]
["Pole mounting","Fire ","X","The light-pole must be mounted inside the superstructure."]
["Safety features","Fire ","X","The light mast must have the following safety features;"]
[null,"Fire ","X","•  when releasing the hand brake of the Fire Truck, the pole - when extended - will automatically be lowered into the travelling position."]
[null,"Fire ","X","•  the floodlights are automatically switched off as soon as the light pole is lowered."]
[null,"Fire ","X","•  moreover, there is a pilot lamp and warning buzzer in the driver's cabin, showing that the light pole is extended."]
["Power supply","Fire ","X","The light mast will be powered from the vehicle's normal power supply."]
["Plumbing","Fire "]
["Corrosion resistant","Fire ",null,"All water and foam bearing piping’s are corrosion resistant stainless steel 304 and flexible high pressure rubber hose"]
["Warning Device","Fire "]
[null,"Fire ",null,"A slim line LED 1.6 m light bar will be installed on the vehicle roof with the following;"]
["LED lights bar","Fire ",null,"•  8 LED cluster front"]
[null,"Fire ",null,"•  8 LED cluster rear"]
[null,"Fire ",null,"•  6 LED clusters at the corners"]
["PA / Siren","Fire ",null,"A 200-watt Siren/PA system with soft touch control panel which shall include the following;"]
[null,"Fire ",null,"•  control light bar flash patterns and cruise lights"]
[null,"Fire ",null,"•  all siren tones (yelp, wail, phaser, air horn)"]
["Additional lights","Fire ",null,"Separate touch control switches for;"]
[null,"Fire ",null,"•  Additional lights"]
[null,"Fire ",null,"•  emergency lights"]
[null,"Fire ",null,"•  public address volume"]
[null,"Fire ",null,"•  dim LED lights bar for night mode"]
["Flashing Lights","Fire ",null,"10 LED panel flashing lights will be mounted on the vehicle as follows;"]
[null,"Fire ",null,"•  2 Front"]
[null,"Fire ",null,"•  2 Rear"]
[null,"Fire ",null,"•  3 Left side of vehicle"]
[null,"Fire ",null,"•  3 Right side of vehicle"]
["Electrical System","Fire "]
["Electrical distribution board","Fire ",null,"A separate electrical junction box will be fitted for the power supply of all auxiliary equipment allowing for both 12 & 24 volt supplies."]
["Labelling","Fire ",null,"All connections to be clearly labelled."]
["No battery connections","Fire ","x","No direct connections from the batteries will be accepted."]
["LED lighting","Fire ",null,"All interior and compartment lighting will be of the LED type."]
["12/24 volt electrical system","Fire ",null,"The electrical system shall be 24 volt and there shall be two heavy duty batteries with a total capacity of approximately 165AH for each bank."]
["Alternator","Fire ",null,"An alternator will be fitted having one output capable of supplying the full operational electrical load, but with a minimum of 108A, and shall incorporate fully automatic regulation."]
[null,"Fire ",null,"The alternator will have spike protection fitted."]
[null,"Fire ",null,"The system will be fitted with a battery isolator master switch."]
["Battery trays","Fire ",null,"The batteries will rest on corrosion proof trays."]
["Shore supply","Fire ",null,"A shore power supply / battery management system with auto elect function shall be installed so as to allow the vehicle to be connected to an external power (250 VA) for the purpose of charging and maintaining the batteries.(At back of Vehicle)"]
[null,"Fire ",null,"All  components of the electrical system will be of the waterproof type (marine grade )for sufficient carrying capacity to suit the maximum circuit loading and will be colour coded."]
["Circuit breakers","Fire ",null,"All important electrical circuits will have separate fuses or circuit breakers."]
["Common box","Fire ",null,"Either will be suitable indicated and grouped into a common box located in an accessible position."]
["Fuses / breakers","Fire ",null,"Where fuses are employed, there will be provision within the box for carrying spares."]
[null,"Fire ",null,"All auxiliary equipment will be wired through separate fuses."]
["Crew cab 12 volt supply","Fire ",null,"Provision will be made for a regulated 12-volt electrical supply in the crew cab of the vehicle, on the left side, for a two-way radio, 24 to 12 volt step down transformer with minimum 15 A capacity will be fitted. "]
[null,"Fire ",null,"All wiring will be carried in tubing clipped to the chassis in an approved manner."]
[null,"Fire ",null,"A number plate light will also be provided."]
["Hazard lights","Fire ",null,"A four-way hazard flasher system is required and indicator repeater lamps on each side of the cab are preferred."]
[null,"Fire ",null,"In addition, two fog lamps are required."]
["Paintwork, labelling & finish","Fire "]
["Painting requirement and colour scheme","Rhine ",null,"The paint shall be of the best quality of approved manufacturer and will comply with the requirements of the relevant West coast specifications and will be applied strictly in accordance with the manufacturer's instructions by tradesmen skilled in this class of work. "]
["Driver’s cab","Rhine ",null,"Colour closely maching Fire Red RAL 3000 will be used with a v Brilliant White roof above gutter."]
["Superstructure ","Fire ",null,"Colour closely maching, Fire Red RAL 3000"]
["Roller shutters  ","Fire ",null,"Aluminium natural coloured--anodised"]
["Aluminium tread plate","Fire ",null,"Aluminium natural coloured"]
["Equipment lockers inside","Fire ",null,"Heavy duty rust protection paint – white"]
["Aluminium surfaces ","Fire ",null,"All aluminium surfaces shall be anodised."]
["Rims","Fire ",null,"Hot dipped galvanised"]
["Bumpers","Fire ",null,"Grey"]
["Fenders","Fire ",null,"Grey"]
["Controls/instructions","Fire ",null,"Clearly marked by means of labelling in English."]
["Brackets for equipment","Fire ",null,"All equipment supplied will be securely mounted."]
["Finish","Fire ",null,"The vehicle will be free from sharp or jagged edges or corners, loose grab rails or slippery foot surfaces."]
[null,"Fire ",null,"Any materials that may be subject to corrosion shall have a durable corrosion and weather resistant automotive finish."]
[null,"Fire ",null,"All surfaces including cut ends, etc. will receive specified dry film thickness of paint for each coat and successive coats."]
[null,"Fire ",null,"Paint surfaces which are to be over coated will be hard dry before over-coating, unless the manufacturer's specification states otherwise."]
[null,"Fire ",null,"the dry film thickness will be measured using a non-destructive thickness gauge such as the, \"Miko Test\" or equivalent."]
[null,"Fire ",null,"Areas welded on-site will be abrasive basted and/or ground and all contaminants such as flux and weld splutter removed prior to painting."]
["Decals and Eskom Logo","Fire ",null,"Shall be in white high-reflective (SANS) letter, as per end-users instructions."]
["Standard Tools, Accessories and Documents","Fire "]
["Standard equipment to be supplied with the vehicle","Truck",null,"A complete set of tools required for normal maintenance of the vehicle will be included."]
[null,"Truck",null,"One spare wheel with complete with same rim and tyre as fitted to the vehicle will be supplied loose (will not be carried on vehicle). "]
[null,"Truck",null,"One jack, jack handle, wheel spanner and two triangles."]
[null,"Truck",null,"Maintenance booklet for chassis and vehicle engine."]
[null,"Truck",null,"Operation instruction for chassis and vehicle engine."]
["Suction hoses","Fire",null,"•  At least two (2) suitably sized Suction hose  spanners with rubber handle grips will be supplied."]
["Strainers","Fire",null,"•  A stainless steel strainer and a basket strainer will be provided."]
["Fire brigade ladder","Koeberg",null,"•  A 2-section fire brigade extension ladder that complies with the relevant NFPA or EN 1147 requirements shall be supplied and mounted."]
["Additional Operating fire fighting and rescue equipment to be mounted on or in the vehicle","Fire ",null,"Additional Equipment as described shall be supplied by Eskom  and securely mounted with the vehicle's lockers and compartment;"]
[null,"Fire ",null,"• Eight (8) lengths of rubber lined firefighting hose (65 mm x 30 m) with BS 65 mm instantaneous couplings (one male and female) (rolled on the female coupling)."]
["Hoses","Fire ",null,"• Four (4) lengths of rubber lined firefighting hose (45 mm x 30 m) with BS 65 mm instantaneous couplings (one male and one female) (rolled on the female coupling). "]
["Hose bridges","Fire ",null,"• One (1) set (2 x pieces) heavy duty hose bridges."]
[null,"Fire ",null,"• One (1) hooligan rescue tool with metal cutting claw"]
[null,"Fire ",null,"• One (1) 9 kg DCP type stored pressure fire extinguisher with ABC powder on heavy duty vehicles galvanised bracket to be fitted."]
["Ex rated torches","Koeberg",null,"• Six (6) LED Explosion Proof (Zone 0) torches (Adalit L-3000 LED) with high intensity LED's, rechargeable ultra light Li-ion batteries with indication of the remaining time of light duration and low battery warning shall be provided and installed so that torches are charged from the vehicle's power supply. Charges for each torch shall be installed and shall take power from the vehicle."]
["Ventilation fan","Koeberg",null,"• One (1) High Performance PPV fan with petrol driven engine shall be supplied and suitably mounted in the vehicle. Fan shall have a fast smoke evacuation performance, aluminium frame, be capable of rapid deployment, large, smooth-operating wheels and stable vibration dampers. Where possible, an integrated water spray attachment should be incorporated."]
["Spreader","Koeberg",null,"• One (1) combi tool with single coupling complying with NFPA 1936 and DIN EN 13204 shall be supplied and incorporated into the vehicle stowage. Spread tips to comply with EN class; BS 53/800-20"]
["Cutter","Koeberg",null,"• One (1) Combi PLUS with single coupling complying with NFPA 1936 and DIN EN 13204. Cutter tips to comply with EN-class BC 180-H-18 and NFPA=class A7/B9/C7/D9/E9."]
["Rescue cylinder","Koeberg",null,"• Two (2) Battery operated Rescue Cylinders RZ 2-1290 with single coupling complying with NFPA 1936 and DIN EN 13204. To be supplied with two Weber Rescue Cylinder chains."]
[null,"Koeberg",null,"• One (1) battery powered Sill Support to work in conjunction with the Weber Rescue Cylinder."]
["Hand tools","Koeberg",null,"• One (1) metal Fire Broom with wooden handle."]
[null,"Koeberg",null,"• One (1) foam making branch pipe with BS 65 mm male coupling and ball valve shut-off."]
[null,"Koeberg",null,"• One (1) Inline inductor with induction range from 0.5 - 3%."]
[null,"Koeberg",null,"• One battery operated (including  recharge facility ) Rescue Saw with FR-3 blade of 300 mm for concrete, cast iron, masonry, stone, steel or brick."]
[null,"Koeberg",null,"• Two (2) Pick Head Fire Axe Model FA"]
[null,"Koeberg",null,"• One (1) Scoop Shovel"]
[null,"Koeberg",null,"• One (1) Header Fork"]
[null,"Koeberg",null,"• One (1) Broom with stick"]
[null,"Koeberg",null,"• One (1) Crowbar 600 mm long"]
[null,"Koeberg",null,"• One (1) Bolt cutter 750 mm long"]
[null,"Koeberg",null,"• One (1) Large Wood axe"]
[null,"Koeberg",null,"• One (1) Spade"]
["Dividing breeches","Koeberg",null,"• Two (2) Dividing Breeching with Ball type control valves (1 x 65 mm BS instantaneous male inlet to 2 x 65 mm female outlets)"]
["Collecting breeches","Koeberg",null,"• One (1) Collecting Breeching with ball type control valves (BS 2 x 65 mm male coupling to 1 x BS 65 mm instantaneous female couplings)"]
["Branches","Koeberg",null,"• Two (2) Akron type pistol grip turbo firefighting branches with volume and pressure control/shut-off and flush with 65 mm BS instantaneous male couplings."]
["Pike","Koeberg",null,"• One (1) Pike with wooden handle 3 m long."]
["Training","Fire "]
["The suppliers will provide training to the end-user's personnel in a formalised training environment","Fire ",null,"The supplier shall provide training on the full operation of the vehicle and all ancillary equipment to the end-user."]
[null,"Fire ",null,"Training shall form of the hand-over and acceptance testing of the vehicle."]
[null,"Fire ",null,"Training shall be provided for no less than 12 personnel at a suitable venue."]
[null,"Fire ",null,"All training material will be documented and made available to the end-user as part of the vehicle documentation."]
["Certification","certification",null,"The pump shall be certified in accordance with:"]
[null,"certification","x","• EN 1028 FPN 10-4000 (normal pressure)"]
[null,"certification","x","• EN 1028 FPN 40-250 (high pressure)"]
[null,"certification","x","• UL classified in accordance with NFPA 1901 150-1250"]
["ISO manufacturing certificate ","Tender","x","To be submmitted with the tender "]
["The chassis cab, the super-structure, pump and the electrical system of the firefighting vehicle must meet every aspect of the National Road Traffic Act  requirements.","certification"]
["Weight distribution and placement on the unit must ensure safe driving at a speed of 80-90km/h with safe tilt angles at that speed. ","certification","x"]
[" List of  Acceptance tests required ","Rhine ","x","The manufacturer shall prove to the satisfaction of Eskom the functioning and performance of all mechanical, electrical and pnematically operated equipment which will include but not be limited to:\n•  PTO's\n•  Pump inlet/outlet valves with pump test certificates and performance curves.\n•  All ancilliary equipment operations\n•  High pressure hose rewind machines\n•  Flood lights\n•  Vehicle anciliary lights\n•  Full remote operation of the roof monitor system, etc.\n•  Full operation of the foam system and foam tank refilling capability. "]
["Manufacturer certificate ","certification","x"]
["Homologation certificate","certification","x"]
["Pump performance certificates","Rhine ",null,"Pump curves and all pump performance tests certificates for both flow volume and pressure (normal and high) shall be provided by an approved testing authority."]
["Form proportioning performance certificate","Rhine ",null,"A certificate of performance for the foam preportioning system and tank filling pump shall be provided."]
["Brake test certificate","certification","x"]
["Certificate of roadworthiness","certification","x"]
["GENERAL ","Tender"]
["Vehicle to be build in the Cape Peninsula to enable interaction between bodybuilder and Eskom for problem solving. ","Tender","x"]
["Manufacturer's must use latest technology throughout.","Tender"]
["Operation instruction and manuals for fire-fighting superstructure, pumps and all ancillary equipment shall be supplied to the end-user.","Tender"]
["19. Maintenance and parts manual shall be supplied","Tender","x"]
["20. Operator training  for 16 damage controllers","Tender","x"]
["21. Paint process  ---protection for high corrosive conditions at the west coast. ","Tender","x"]
["Vehicle to be registered in Eskom name before delivery.","Tender","x"]
["22. Complete vehicle to be delivered to Eskom Koeberg","Tender","x"]
["Documents to be returned with this completed spread sheet.","Tender","Critical criteria "]
["23. Completed functional specification spread sheet","Tender","x"]
["24. Weight distribution diagram and calculations ","Tender","x"]
["25. Photos/Brochures/ technical data sheets of the unit  to validate information on this spread sheet","Tender","x"]
["26.  Paint spec details (coastal specific)","Tender","x"]
["Certificate for registration as body builder to build fire engines.","Tender","x"]
["27. Proof of dealership / agency from OEM","Tender","x"]
["28. Proof of existing maintenance and repair support structure in the Western Cape","Tender","x"]
["29. Estimate delivery time  from day of order","Tender","x"]
["30. All  qualifying suppliers may be visited as part of the evalaution, please indicate phisical adress of the factory."]
["Please submit basic drawings of the tendered product."]
["Acceptance ","Tender"]
["Acceptance / Acceptance","Tender"]
["Name of End user : ","Tender",null,"Andre van Rooyen ","Signature :"]
["Name of Verifier","Tender",null,"Eddie Cumpsty ","Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom.","Tender"]
["Technical evaluation"]
["Completed Spec sheet to be returned with column E and F filled in",{"v":0.1,"d":"10%"},{"v":0.1,"d":"10%"}]
["0100% Compliance with tech spec ( Critical Criteria)",{"v":0.7,"d":"70%"},{"v":0.7,"d":"70%"}]
["Company profile",{"v":0.1,"d":"10%"},{"v":0.1,"d":"10%"}]
["Manufacturer ,Importer or Builder certificate",{"v":0.1,"d":"10%"},{"v":0.1,"d":"10%"}]
[null,{"v":1,"d":"100%"},{"v":1,"d":"100%"}]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}