{"text_format":"3","workbook":"xlsx","n_sheets":9,"sheets":["Section A (P & Gs) 1200A","Earthworks Pipe Trenches 1200DB","Earthworks_Roads, Subgr 1200DM","Bedding Pipes 1200LB","Stormwater Drainage 1200LE","Subbase 1200ME","Segmented Paving 1200MJ & MM","Kerbing and Channeling 1200MK","Summary"],"not_rendered":{"images":5,"external_links":20,"defined_names":416},"read":"whole","date_system":"1900"}

{"sheet":"Section A (P & Gs) 1200A","index":0,"n_rows":217,"n_cols":8,"rows_kept":217,"merged":[[0,0,0,4],[2,0,2,7],[22,2,22,3],[45,5,45,6],[46,5,46,6],[48,2,48,3],[52,2,52,3],[56,2,56,3],[65,2,65,3],[74,2,74,3],[83,5,83,6],[84,5,84,6],[91,2,91,3],[101,2,101,3],[103,2,103,3],[109,5,109,6],[110,5,110,6],[111,2,111,3],[119,2,119,3],[123,2,123,3],[140,5,140,6],[141,5,141,6],[172,5,172,6],[173,5,173,6],[190,5,190,6],[191,5,191,6],[216,3,216,4]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
["BILL OF QUANTITIES"]
[]
["Item No","Payment Clause",null,"Short Description","Unit","Quantity","Rate","  Amount"]
[]
[null,"SANS\n1200 A","SECTION 1 : PRELIMINARY AND GENERAL"]
[]
["A1",null,"Fixed-charge items"]
[]
["A1.1","8.3.1",".01","Contractual Requirements ","Sum",1]
[]
["A1.2","8.3.2",null,"Establishment of Facilities on Site"]
[]
["A1.2.1","8.3.2.1","Facilities for the Engineer "]
[]
[null,null,".01","Furnished offices and conference room","Sum",1]
[]
[null,null,".02","2 No  Project Name Boards ","Sum",1]
[]
[null,null,".03","Survey equipment","Sum",1]
[]
["A1.2.2","8.3.2.2","Facilities for Contractor:"]
[]
[null,null,".01","Offices, storage sheds, workshops, living accommodation, ablution and toilet facilities, tools and equipment, water supplies, laboratories, electric power, communications, access and plant","Sum",1]
[]
[null,"8.3.2.2",".02","Dealing with water"]
[]
[null,null,"a)","Generally on site","Sum",1]
[]
[null,null,"b)","Channel and river crossings","Sum",1]
[]
["A1.3","8.3.3",".03","Other Fixed Charge Obligations","Sum",1]
[]
["A1.4",null,".04","Accommodation of traffic","Sum",1]
[]
["A1.5","8.3.4",".05","Removal of site establishment","Sum",1]
[]
["A1.6","SPEC AO","Health and safety:"]
[]
["A1.6.1","8.2.1",".01","General safety obligations","Sum",1]
[]
["A1.6.2","8.2.3",".02","Health and safety plan","Sum",1]
[]
["A1.6.3","8.2.4",".03","Construction Safety Officer and other appointments","Sum",1]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
[]
["A1.5",null,"Environmental Compliance"]
[]
[null,null,".01","Preparation and establishment of all procedures required to achieve and ensure compliance with the requirements of the Environmental Management Programme, RoD and all relevant environmental legislations","Sum",1]
[]
["A1.6",null,"HIV/AIDS Awareness"]
[]
[null,null,".01","Compliance with SANS 1921 Part 6 HIV/ AIDS awareness and regulations","Sum",1]
[]
["A1.7",null,"COVID 19 Awareness"]
[null,null,".02","Compliance with COVID 19 national awareness campaigns and the relevant national regulations and laws","Sum",1]
[]
[null,"SANS"]
["A2","1200 A","Time-Related Items"]
[null,"PSA"]
[]
["A2.1","8.4.1",".01","Contractual Requirements","Sum",1]
[]
["A2.2","8.4.2","Operation and Maintenance of facilities on site for duration of construction"]
["A2.2.1","8.4.2.1","Facilities for the Engineer "]
[]
[null,null,".01","Furnished offices and conference room","Sum",1]
[]
[null,null,".02","2 No Project Name Boards ","Sum",1]
[]
[null,null,".03","Use of survey equipment","Sum",1]
[]
["A2.2.2","8.4.2.2","Facilities for Contractor:"]
[]
[null,null,".01","Offices, storage sheds, workshops, living accommodation, ablution and toilet facilities, tools and equipment, water supplies, laboratories, electric power, communications, access and plant","Sum",1]
[]
[null,null,".02","Dealing with water"]
[]
[null,null,"a)","Generally on site","Sum",1]
[]
[null,null,"b)","Channel and river crossings","Sum",1]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
["A2.3","8.4.3",null,"Supervision for duration of contract","Sum",1]
[]
["A2.4","8.4.4",".01","Company and head office overhead costs for the duration of the contract","Sum",1]
[]
["A2.5","8.4.5","Other Time-Related Obligations",null,"Sum",1]
[]
["A2.6",null,"Dealing with Traffic",null,"Sum",1]
[]
["A2.7","SPEC AO","Health and safety:"]
[]
["A2.7.1","8.2.1",".01","General safety obligations","Sum",1]
[]
["A2.7.2","8.2.3",".02","Health and safety plan","Sum",1]
[]
["A2.7.3","8.2.4",".03","Construction Safety Officer and other appointments","Sum",1]
[]
["A2.100",null,"Administration and supervision of mandatory subcontract work including supervision of SMMEs. Payment will be on progress of the SMME work proportional to the contract participation goal ",null,"Sum",1]
[]
["A.2.200",null,"Professional Fees for the delivery of the following milestones:",null,"Sum",1]
[null,null,".01","Stage 1: Inception Report                         in accordance with ECSA Scope of Services Guidelines, Clause 3.2.1","Sum",1]
[null,null,".02","Stage 2: Preliminary Design Report                          in accordance with ECSA Scope of Services Guidelines, Clause 3.2.2","Sum",1]
[null,null,".03","Stage 3: Detailed Design Report                          in accordance with ECSA Scope of Services Guidelines, Clause 3.2.3","Sum",1]
[null,null,".04","Stage 5: Contract administration and Inspection                          in accordance with ECSA Scope of Services Guidelines, Clause 3.2.5","Sum",1]
[null,null,".05","Stage 6: Close-out Report                          in accordance with ECSA Scope of Services Guidelines, Clause 3.2.6","Sum",1]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
["A2.8",null,"Environmental"]
[]
["A2.8.1",null,".01","Preparation and establishment of all procedures required to achieve and ensure compliance with the requirements of the Environmental Management Programme, EA and all relevant environmental legislations","Sum",1]
[]
["A2.8.2",null,".02","Provisional sum for Final environmental rehabilitation by specialised contractor","Prov",1]
[]
[null,null,".03","Contractors' mark up on Item A2.82","%"]
[]
["A2.9",null,"HIV/AIDS Awareness"]
[]
[null,null,".01","Compliance with SANS 1921 Part 6 HIV/ AIDS awareness and regulations","Sum",1]
[]
["A2.10",null,"COVID 19 Awareness"]
[null,null,".02","Compliance with COVID 19 national awareness campaigns and the relevant national regulations and laws","Sum",1]
[]
["A3",null,"Sums stated provisionally "]
[null,"8.5\nSDA8-4"]
["A3.1",null,".01","Alterations to existing services by authorities","Sum",1,{"v":30000,"d":"R30,000.00"},{"v":30000,"d":"R 30,000.00"}]
[null,"SDA8-9"]
["A3.2",null,".02","Contractor's overheads, charges and profit on Item A3.1 (State % and extend as an amount)","%"]
["A3.3",null,null,"Engineer's Disbursements"]
[]
["A3.3.1",null,null,"Allow For Engineer's Representative site travel @1,000 km/month For 12 months","Km",12000,{"v":5,"d":"R5.00"},{"$f":"F134*G134","v":{"v":60000,"d":"R 60,000.00"}}]
[]
["A3.3.2",null,null,"Other Disbursements"]
[]
[null,null,".01","Other disbursements like Engineer's travels, accommodation, office prints, cell phone usage (air time/data), lap top, etc for 12 month period","Sum",1,{"v":800000,"d":"R800,000.00"},{"$f":"F138*G138","v":{"v":800000,"d":"R 800,000.00"}}]
[]
["A3.3.3",null,null,"Contractor's Mark up on Items A3.3.1 and A3.3.2 (state % and extend as amount)","%"]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
["A3.4.1",null,null,"Renumeration for the Community Liaison Officer for the 12 month period","Sum",1,{"v":120000,"d":"120,000.00"}]
["A3.4.2",null,null,"PSC stipend over the 12 month project period","Sum",1,{"v":120000,"d":"R120,000.00"}]
["A3.4.3",null,null,"Contractor's Markup on Items A3.4.1 and A3.4.2","%"]
["A4",null,"Prime Cost items"]
[null,"8.6\nPDA8-5"]
["A4.1",null,".01"," Additional test required by the engineer ","-",1,{"v":40000,"d":"R40,000.00"},{"$f":"G148*F148","v":{"v":40000,"d":"R 40,000.00"}}]
[]
["A4.2",null,".02","Contractor's overheads, charges and profit on Item A4.1 (State % and extend as an amount)","%"]
[]
["A4.3",null,".03","Accommodation for the Engineer's Representative (Prime Cost)","Prov",1,{"v":120000,"d":"R120,000.00"},{"$f":"G152*F152","v":{"v":120000,"d":"R 120,000.00"}}]
[]
["A4.4",null,".04","Contractor's overheads, charges and profit on Item A4.3 (State % and extend as an amount)","%"]
[]
["A4.5",null,".05","Engineer's telephone and other communication  costs including cell phone costs @R450/week (Prime cost)","Prov",1,{"v":15000,"d":"R15,000.00"},{"v":15000,"d":"R 15,000.00"}]
[]
["A4.6",null,".06","Contractor's overheads, charges and profit on Item A4.5 (State % and extend as an amount)","%"]
[{"$nulls":7},0]
["A4.7",null,".07","Provision of accredited on site skills training as outlined in the specification.  Including supervision, salaries and other validated costs","Prov",1,{"v":130000,"d":"R130,000.00"},{"v":130000,"d":"R 130,000.00"}]
[]
["A4.8",null,".08","Contractor's overheads, charges and profit on Item A4.7 (State % and extend as an amount)","%"]
[]
["A6",null,"Daywork (Provisional)"]
[]
["A6.1","8.7\nPDA8-6",".01"," Labour"]
[]
["A6.1.1",null,null,".01 Skilled labour","h",40]
[]
["A6.1.2",null,null,".02 Semi-skilled labour","h",40]
[]
["A6.1.3",null,null,".03 Unskilled labour","h",40]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
["A6.2",null,".02","Materials"]
[]
["A6.2.1",null,null,".01 Allow for net cost of goods or materials actually used",{"v":0.8,"d":"80%"},"PC sum"]
[]
["A6.2.2",null,null,".02 Contractors'' mark up on Item A6.2.1","%",{"v":0.05,"d":"5%"}]
[]
["A6.3",null,".03","Contractor's own plant on Site"]
[]
["A6.3.1",null,null,".01 Allow for all-inclusive cost of using Contractor's own plant on site","-","PC sum"]
["A6.3.2",null,null,".02 Charge required by contractor on the above subitem","%"]
[]
["A6.4",null,".04","Plant hired by the contractor"]
[]
["A6.4.1",null,null,".01 Allow for net cost of hire plant Contractor ","-","PC sum"]
[]
["A6.4.2",null,null,".02 Charge required by contractor on item A6.4.1","%"]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
["A6.4.3",null,null,"Allow provisional sum for survey by surveyor appointed by the Engineer","Prov"]
[]
["A6.4.4",null,null,"Contractor's overheads, charges and profit on Item A6.4.3 (State % and extend as an amount)","%"]
[]
["A6.4.5",null,null,"Two survey assistants for duration of contract","Sum"]
[]
["A8",null,"Existing services"]
[null,"8.8.4"]
["A8.1",null,".01","Location:"]
[]
["A8.1.1",null,null,".01 Locating, protection, alteration and relocation of existing services carried out by authorities","Prov",1,{"v":45000,"d":"R45,000.00"},{"$f":"G203*F203","v":{"v":45000,"d":"R 45,000.00"}}]
[]
["A8.1.2",null,null,".02 Percentage adjustment on Item A8.1.1 for Contractor's overheads and profit (state % and extend as an amount)","%"]
[]
["A8.1.3",null,null,".03 Excavation by hand in soft to expose services","m3",120]
[]
["A9",null,"Survey beacons/pegs"]
[null,"8.8.5"]
["A9.1",null,".01","Search for, record, reference and protect survey stations, bench marks, erf boundary pegs and other reference pegs and expose on completion of Works","Sum",1]
[null,"SDA8-4"]
["A9.2",null,".02","Re-establish erf boundary pegs by a Registered Land Surveyor when pegs have been ordered to be removed for the execution of the Works","Prov",1,{"v":50000,"d":"R50,000.00"},{"v":50000,"d":"R 50,000.00"}]
[]
["A9.3",null,".03","Percentage adjustment on Item A9.2 for Contractor's overheads and profit (State % and extend as an amount)","%"]
[]
[{"$nulls":3}," TOTAL SECTION 1:\n CARRIED TO SUMMARY"]

{"sheet":"Earthworks Pipe Trenches 1200DB","index":1,"n_rows":131,"n_cols":8,"rows_kept":131,"merged":[[0,0,0,4],[5,2,5,3],[9,2,9,3],[48,2,48,3],[49,5,49,6],[50,5,50,6],[54,2,54,3],[61,2,61,3],[63,2,63,3],[67,2,67,3],[77,2,77,3],[87,5,87,6],[88,5,88,6],[90,2,90,3],[92,2,92,3],[99,2,99,3]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
["Item No","Payment Clause",null,"Short Description","Unit","Quantity","Rate","  Amount\n         R           c"]
[null,"SANS\n1200 DB","SECTION 2 : EARTHWORKS TRENCH EXCAVATION"]
[]
["DB 1",null,"Excavation"]
[]
["DB 1.1","8.3.2","Excavate in all materials for trenches, backfill, compact and dispose of surplus material for:"]
[]
[null,null,".01","Stormwater pipes over 400 mm dia and up to 650 mm dia for depths:"]
[]
[{"$nulls":3},"       Over       and      Up to & including"]
[]
[null,null,".01","0,0 m                  1,0 m","m",1890]
[]
[null,null,".02","1,0 m                  2,0 m","m",3150]
[]
[null,null,".03","2,0 m                  3,0 m","m",1260]
[]
[{"$nulls":3},"Stormwater pipes over 650 mm dia and up to 1200 mm dia for depths:"]
[]
[{"$nulls":3},"       Over      and      Up to & including"]
[]
["DB 1.2","8.3.2",null,".01  0,0 m                  1,0 m","m",170]
[]
[{"$nulls":3},".02  1,0 m                  2,0 m","m",255]
[]
[{"$nulls":3},".03   2,0 m                  3,0 m","m",210]
[]
[{"$nulls":3},".04   3,0 m                 4,0 m","m",130]
[]
[{"$nulls":3},".05   4,0 m                 4,5 m","m",85]
[]
["DB 1.3","8.3.2",null,"Extra over Items DB1:"]
[]
[null,null,".01","Intermediate excavation","m3",5400]
[]
[null,null,".02","Hard rock excavation","m3",2150]
[]
[null,null,".03","Hand excavation where ordered by "]
[{"$nulls":3},"the engineer "]
[]
[{"$nulls":3},".0.1 Soft Material ","m3",20]
[]
[{"$nulls":3},".0.2 Intermediate Material ","m3",20]
[]
["DB 1.4","8.3.2","Excavate and dispose of unsuitable material from trench bottom (Provisional)",null,"m3",350]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
[]
["DB 2",null,"Excavation ancillaries"]
[]
["DB 2.1","8.3.3.1","Make up deficiency in backfill material:"]
[]
[null,null,"0.1","From other necessary excavations on Site","m3",100]
[]
[null,null,"0.2","By importation from designated borrow pits","m3",150]
[]
[null,null,"0.3","By importation from commercial or off-site sources selected by Contractor and approved by Engineer","m3",5400]
["DB 2.2","8.3.3.3","Compaction in road reserves",null,"m3",2400]
[]
["DB 2.3","8.3.4","Particular items:"]
[]
[null,null,"0.1","Shore trench opposite structure or service","m",500]
[]
["DB 2.4","8.3.5","Existing services that intersect or adjoin a trench"]
[]
[null,null,"0.1","Services that intersect a trench:"]
[]
[{"$nulls":3},".01  Watermains up to 200 mm dia","No",50]
[]
[null,null,"0.2","Stormwater pipes 300 mm to 600 mm dia","No",2]
[]
[null,null,"0.3","Cables","No",10]
[]
[null,null,"Services that adjoin a trench:"]
[]
[null,null,"0.1","Watermains up to 200 mm dia","m",6500]
[]
[null,null,"0.2","Sewers up to 200 mm dia","m",6500]
[]
[null,null,"0.3","Overhead telephone","m",50]
[]
[null,null,"0.4","Overhead electricity","m",20]
[]
[{"$nulls":5},"Total Carried Forward"]
[{"$nulls":5},"Total Brought Forward"]
[]
["DB 3","1200 DB","Finishing"]
[]
["DB 3.1","8.3.6.1","Reinstate road surfaces complete with all courses:"]
[]
[null,null,"0.1","Gravel roads","m2",25000]
[]
[null,null,"0.2","60 mm brick paved roads","m2",50]
[]
[]
["DB 3.2",null,"Finishes to trenches"]
[null,null,".01","Reinstate topsoil from stockpile to minimum depth of 150 mm","m2",49000]
[]
[null,null,".02","Reinstate natural grass along working strips 5 m wide","m2",35000]
[]
["DB 4","SABS 1200 DK",null,"Gabions and Pitching (Provisional)"]
[]
[null,null,".01","Supply all materials, construct and place gabions and mattresses where ordered:"]
[]
["DB 4.1","8.2.1 a",".02","Surface preparation - Cavities filled with approved excavated rock or material","m²",50]
[]
["DB 4.2","8.2.2",null,"Gabions (Rate to include costs for complete supply of all materials, filling of the cages and construction of the gabions/mattresses):"]
[]
[null,null,".04","6 x 1 x 1m galvanised wire boxes","m³",35]
[]
[null,null,".05","170 mm thick galvanised reno mattresses","m²",15]
[]
[null,null,".06","Geotextile where ordered (Kaymat U24 or similar approved)","m²",35]
[]
[null,null,".07","Extra over Item B28.2 for grade 15/19 concrete screed, 50mm thick to top of mattresses where ordered","m³",{"v":5,"d":"5.0"}]
[]
["DB 4.3","8.2.5",null,"Stone Pitching (Provisional)"]
[]
[null,null,"a) ","300 mm stone pitching. Minimum size 150 mm","m2",90]
{"$rows_empty":7}
[{"$nulls":3},"TOTAL SECTION 2 CARRIED TO SUMMARY"]

{"sheet":"Earthworks_Roads, Subgr 1200DM","index":2,"n_rows":64,"n_cols":9,"rows_kept":64,"merged":[[0,0,0,5],[2,0,2,8],[4,2,4,4],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,2,17,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[22,2,22,4],[23,2,23,4],[24,2,24,4],[26,2,26,4],[27,2,27,4],[28,6,28,7],[29,6,29,7],[30,2,30,4],[31,2,31,4],[32,2,32,4],[35,2,35,4],[37,2,37,4],[41,2,41,4],[43,2,43,4],[45,2,45,4],[46,2,46,4],[47,2,47,4],[48,2,48,4],[50,2,50,4],[51,2,51,4],[52,2,52,4],[53,2,53,4],[54,2,54,4],[55,2,55,4],[56,2,56,4],[57,2,57,4],[58,2,58,4],[60,2,60,4],[61,2,61,4],[62,2,62,4],[63,1,63,5]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
["BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS TO","DESCRIPTION",null,null,"UNIT","QTY","RATE","AMOUNT"]
[null,"SABS","SECTION 3:  EARTHWORKS (ROADS, SUBGRADE)"]
[null,"1200 DM"]
[null,""]
["B1","8.3.2","Preparation of Site:"]
[]
["B1.1",null,"Preparation and stripping of site/removal of topsoil to 200 mm depth, stockpiling and maintaining",null,null,"m³",{"v":11900,"d":"11,900"}]
[]
["B2","8.3.3","Treatment of road-bed"]
[]
["B2.1",null,"a)  200mm thick road-bed preparation and compaction of material to minimum of 93% of modified AASHTO maximum density",null,null,"m3",{"v":11900,"d":"11,900"}]
[]
["B2.2",null,"b)  In-place treatment of road-bed in intermediate or hard rock material by:"]
[]
["B2.2.1",null,"i)  Ripping",null,null,"m³",{"v":1100,"d":"1,100"}]
["B2.2.2",null,"ii) Blasting",null,null,"m³",450]
[]
["B3","8.3.4","Cut to fill, borrow to fill:"]
[]
["B3.1",null,"a)  Compact to 93% of modified AASHTO maximum density",null,null,"m³",{"v":47600,"d":"47,600"}]
[]
["B3.2",null,"b)  Rockfill, process, and compact",null,null,"m³",{"v":11000,"d":"11,000"}]
[]
["B4","8.3.5","Selected layer (subgrade) compacted to 93% of modified AASHTO maximum density",null,null,"m³",{"v":11900,"d":"11,900"}]
[{"$nulls":6},"Total Carried Forward"]
[{"$nulls":6},"Total Brought Forward"]
[]
["B5","8.3.6","Extra over items 8.3.4 and 8.3.5 for excavating and breaking down material in:"]
[]
[null,null,"a)  Intermediate excavation  ",null,null,"m³",{"v":2500,"d":"2,500"}]
[null,null,"b)  Hard excavation          ",null,null,"m³",{"v":1000,"d":"1,000"}]
[]
["B6","8.3.7","Cut to spoil or stockpile from:"]
[]
[null,null,"a)  Soft excavation          ",null,null,"m³",{"v":1500,"d":"1,500"}]
[null,null,"b)  Intermediate excavation  ",null,null,"m³",{"v":2500,"d":"2,500"}]
[null,null,"c)  Hard excavation          ",null,null,"m³",{"v":1200,"d":"1,200"}]
[]
["B7","8.3.8","Removal of oversize material ",null,null,"m³",{"v":1000,"d":"1,000"}]
[]
["B8","8.3.9","Overbreak of excavation in:"]
[]
[null,null,"a)  Intermediate excavation  ",null,null,"m²",500]
[null,null,"b)  Hard excavation",null,null,"m²",500]
[]
["B9","8.3.10","Materials bladed to windrow      ",null,null,"m³",{"v":2500,"d":"2,500"}]
[]
["B10","8.3.11","Extra over items 8.3.2, 8.3.4, or 8.3.5 for temporary stockpiling of material",null,null,"m3",{"v":75000,"d":"75,000"}]
[]
["B11","8.3.12","Overhaul",null,null,"m³.km",{"v":300000,"d":"300,000"}]
[]
["B12","8.3.13","Surface finishes:"]
[]
[null,null,"(a) Topsoiling",null,null,"m²",200]
[]
[null,null,"b) Grassing or other cover  ",null,null,"m²",250]
[]
["B13","8.3.15","Catchwater mounds and channels and mitre banks and channels",null,null,"m3",250]
[]
[null,"TOTAL SECTION 3 CARRIED TO SUMMARY"]

{"sheet":"Bedding Pipes 1200LB","index":3,"n_rows":56,"n_cols":9,"rows_kept":56,"merged":[[0,0,0,5],[2,0,2,8],[4,2,4,4],[5,2,5,4],[7,2,7,4],[8,2,8,4],[11,2,11,4],[13,2,13,4],[15,2,15,4],[16,2,16,4],[18,2,18,4],[21,2,21,4],[23,2,23,4],[25,2,25,4],[26,2,26,4],[28,2,28,4],[30,2,30,4],[32,2,32,4],[34,2,34,4],[36,2,36,4],[38,2,38,4],[40,2,40,4],[41,2,41,4],[43,2,43,4],[47,2,47,4],[48,2,48,4],[49,2,49,4],[53,2,53,4],[54,2,54,4],[55,2,55,6],[56,2,56,4]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
["BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS TO","DESCRIPTION",null,null,"UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SABS","SECTION 4:  BEDDING (PIPES)"]
[null,"1200 LB"]
[]
["G1","8.2.1","Provision of bedding from trench "]
[null,null,"excavation:"]
[]
[null,null,"(a) Selected granular material",null,null,"m³",150]
[]
[null,null,"b)  Selected fill material",null,null,"m³",200]
[]
[]
["G2","8.2.2","Supply only of bedding by importation:"]
[]
["G3","8.2.2.1","From other necessary excavations"]
[null,null,"(provisional):"]
[]
[null,null,"(a)","Selected granular material",null,"m³",250]
[]
[null,null,"(b)","Selected fill material",null,"m³",200]
[]
[]
["G4","8.2.2.2","From borrow pits (provisional):"]
[]
[null,null,"(a)","Selected granular material",null,"m³",250]
[]
[null,null,"(b)","Selected fill material",null,"m³",200]
[]
["G5","8.2.2.3","From commercial sources "]
[]
[null,null,"(a)","Selected granular material",null,"m³",{"v":7800,"d":"7,800"}]
[]
[null,null,"(b)","Selected fill material",null,"m³",{"v":2200,"d":"2,200"}]
[]
["G6","8.2.3","Concrete bedding cradle (20 Mpa/19)",null,null,"m³",15]
[]
[]
["G7","8.2.4","Encasing of pipes in 20 Mpa/19 concrete for:",null,null,"m³",20]
[]
[null,null,"a) 450 mm pipe",null,null,"m3",15]
[null,null,"b) 600 mm pipe",null,null,"m3",20]
[null,null,"c) 1200 mm pipe",null,null,"m3",25]
[]
["G8",null,"Extra over Items G1 to G5 for bedding in water logged trenches"]
[]
[null,null,"a)  100mm agricultural drain pipe",null,null,"m",{"v":1100,"d":"1,100"}]
[null,null,"b) 19 mm stone",null,null,"m3",530]
[null,null,"c) Geotextile Kaymat Fabric",null,null,"m2",{"v":2850,"d":"2,850"}]
[]
[]
[null,null,"TOTAL SECTION 4 CARRIED TO SUMMARY"]

{"sheet":"Stormwater Drainage 1200LE","index":4,"n_rows":39,"n_cols":9,"rows_kept":39,"merged":[[0,0,0,5],[2,0,2,8],[4,2,4,4],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,2,17,3],[25,2,25,4],[33,2,33,4],[38,1,38,6]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
["BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS TO","DESCRIPTION",null,null,"UNIT","QTY","RATE","AMOUNT"]
[null,"SABS","SECTION 5: STORMWATER DRAINAGE"]
[null,"1200 LE"]
[]
["A1","8.2.1","Supply and lay concrete pipe culverts, Type SC, Class 100D with spigot and socket joints on class C bedding:"]
[]
["A1.1",null,"450 mm ND",null,null,"m",{"v":5900,"d":"5,900"}]
["A1.2",null,"600 mm ND",null,null,"m",400]
["A1.3",null,"1200 mm ND",null,null,"m",840]
[]
["A2","8.2.8","Supply and install manholes, catchpits and the like:"]
[]
["A2.1",null,"a)  Single splay side inlet manholes complete including cover as per Drawing CIV-FM003 for depths (steel reinforcement is measured elsewhere):"]
[null,null,"Over ",null,"Up to"]
["A2.1.1",null,"1.0m",null,"1.5 m","No",80]
["A2.1.2",null,"1.5m",null,"2.0m","No",130]
["A2.1.3",null,"2.0m",null,"2.5 m","No",50]
["A2.1.4",null,"2.5 m",null,"3.0 m","No",1]
[]
["A2.1.5",null,"Steel reinforcement (R bars)",null,null,"t",1.8]
[]
["A2.2",null,"b) Precast concrete manholes, excluding inlets, for depths:"]
[null,null,"Over","Up to"]
[]
["A2.2.1",null,"1.0m","1.5 m",null,"No",2]
["A2.2.2",null,"1.5m","2.0m",null,"No",3]
["A2.2.3",null,"2.0m","2.5 m",null,"No",4]
["A2.2.4",null,"2.5 m","3.0 m",null,"No",1]
[]
["A3","8.2.8","c)  Masonry headwall outlet structure for single pipe as per details on Drawing CIV-FM005 for:"]
[null,null,"a) 450 mm pipe",null,null,"No",1]
[null,null,"b) 600 mm pipe",null,null,"No",1]
[null,null,"c) 1200 mm pipe",null,null,"No",2]
[]
[null,"TOTAL SECTION 5 CARRIED TO SUMMARY"]

{"sheet":"Subbase 1200ME","index":5,"n_rows":40,"n_cols":9,"rows_kept":40,"merged":[[0,0,0,5],[2,0,2,8],[4,2,4,4],[5,2,5,4],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
["BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS TO","DESCRIPTION",null,null,"UNIT","QTY","RATE","AMOUNT"]
[null,"SABS","SECTION 6: SUBBASE"]
[null,"1200 ME"]
["C1","8.3.3","Construct 200 mm thick gravel subbase and shoulder layer (G5) compacted to 95% of modified AASHTO density with material from  commercial sources or designated borrow areas",null,null,"m3",{"v":11900,"d":"11,900"}]
[]
["C2","8.3.5","Process subbase material by stabilisation, as when required, and use in the subbase",null,null,"m3",{"v":5950,"d":"5,950"}]
[]
["C3","8.3.8","Stabilizing agent:"]
[]
[null,null,"a) Portland cement           ",null,null,"t",0.5]
[]
[null,null,"b) Portland blast-furnace cement      ",null,null,"t",0.5]
{"$rows_empty":23}
[null,null,"TOTAL SECTION 6 CARRIED TO SUMMARY"]

{"sheet":"Segmented Paving 1200MJ & MM","index":6,"n_rows":30,"n_cols":9,"rows_kept":30,"merged":[[0,0,0,5],[2,0,2,8],[4,2,4,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,2,17,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[24,2,24,4],[29,2,29,6]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
[]
["BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS TO","DESCRIPTION",null,null,"UNIT","QTY","RATE","AMOUNT"]
[null,"SABS","SECTION 7A:  SEGMENTED PAVING"]
[null,"1200 MJ"]
[]
["E1","8.2.1","Provision of edge restraints for 60 mm interlocking brick paved area",null,null,"m",{"v":17000,"d":"17,000"}]
[]
[]
[]
["E2","8.2.2","b)  Construction of paving complete including  supply and lay 60 mm interlocking paving bricks Type S-A, Class 35, including bedding sand, all in compliance with SABS 1058",null,null,"m2",{"v":59500,"d":"59,500"}]
[]
["E3","8.2.3","Cutting units to fill edge restraints:"]
[]
[null,null,"(a) Straight cutting",null,null,"m",200]
[]
[null,null,"(b) Raking cutting",null,null,"m",200]
[]
[null,null,"c)  Circular cutting",null,null,"m",200]
[]
[null,"SABS 1200MM","SECTION 7B: ANCILLARY WORKS"]
[]
["F.1",null,"Allowance for Ancillary Works where ordered, like road markings, road signs, reflectors, guardrails, etc",null,null,"Sum",1,{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
[]
[]
[]
[null,null,"TOTAL SECTIONS 7 CARRIED TO SUMMARY"]

{"sheet":"Kerbing and Channeling 1200MK","index":7,"n_rows":39,"n_cols":9,"rows_kept":39,"merged":[[0,0,0,5],[1,0,1,8],[3,2,3,4],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[10,2,10,4],[12,2,12,4],[13,2,13,4],[14,2,14,4],[15,2,15,4],[16,2,16,4],[17,2,17,4],[18,2,18,4],[19,2,19,4],[20,2,20,4],[21,2,21,4],[22,2,22,4],[23,2,23,4],[24,2,24,4],[25,2,25,4],[26,2,26,4],[27,2,27,4],[28,2,28,4],[29,2,29,4],[30,2,30,4],[31,2,31,4],[32,2,32,4],[33,2,33,4],[34,2,34,4],[35,2,35,4],[36,2,36,4],[37,2,37,4],[38,2,38,6]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
["BILL OF QUANTITIES"]
[]
["ITEM NO","PAYMENT REFERS TO","DESCRIPTION",null,null,"UNIT","QTY","RATE","AMOUNT"]
[null,"SABS","SECTION 8:  KERBING AND CHANNELLING"]
[null,"1200 MK"]
[]
["D1","8.2.2","Concrete kerbing and channelling combined"]
[]
["D1.1",null,"Pre cast side road kerbing to SABS 927 complete, as per details on Drawing CIV_FM002",null,null,"m"]
[]
["D2","8.2.7","Trimming of excavations for concrete-"]
[null,null,"lined open drains in:"]
[]
[null,null,"a) Soft material",null,null,"m²",130]
[]
[null,null,"b) Intermediate material",null,null,"m²",120]
[]
[null,null,"c) Hard material",null,null,"m²",425]
[]
["D3","8.2.8","Cast in-situ 25 Mpa concrete lining to open drains"]
[]
["D3.1",null,"Trapezoidal drain",null,null,"m3",110]
["D3.2",null,"V-drain",null,null,"m3",110]
[]
["D4","8.2.9","Formwork to cast in-situ concrete lining of open drains (smooth surface finish):"]
[]
[null,null,"a)  To sides with formwork on the internal face only",null,null,"m²",150]
[null,null,"b)  To sides with formwork on both internal faces and external faces (each face measured)",null,null,"m2",150]
[null,null,"c) To ends of slabs",null,null,"m²",250]
[]
["D5","8.2.10","Sealed joints in concrete lining of open drains"]
[]
[null,null,"(a) Flexcell and polysulphide sealants",null,null,"m",{"v":8400,"d":"8,400"}]
[]
["D6","8.2.12","Welded steel fabric mesh Ref 395 steel reinforcement",null,null,"t",0.5]
[]
["D7","8.2.13","Sprayed bitumen emulsion primer or Polyethylene sheeting for concrete-lined open drains",null,null,"m2",{"v":17000,"d":"17,000"}]
[null,null,"TOTAL SECTION 8 CARRIED TO SUMMARY"]

{"sheet":"Summary","index":8,"n_rows":19,"n_cols":3,"rows_kept":19,"merged":[[0,0,0,1],[1,0,1,2],[18,0,18,1]]}
["APPOINTMENT OF A TURNKEY/DESIGN AND BUILD FOR CONSTRUCTION OF A 8.50 KM BLOCK PAVED TOWNSHIP ROAD NETWORK AND STORMWATER COLLECTION AND DISPOSAL FACILITIES FOR THE FATENG TSE NTSHO EXTENSION 5, 743 SITES, IN PAUL ROUX, DIHLABENG LOCAL MUNICIPALITY"]
["SUMMARY OF TENDERED AMOUNTS"]
[]
["SECTION","DESCRIPTION","AMOUNT TENDERED"]
["SECTION 1","PRELIMINARY AND GENERAL"]
["SECTION 2","EARTHWORKS PIPE TRENCHES"]
["SECTION 3","EARTHWORKS (ROADS , SUBGRADE)"]
["SECTION 4","STORMWATER PIPE BEDDING"]
["SECTION 5","STORMWATER DRAINAGE"]
["SECTION 6","SUBBASE"]
["SECTION 7","SEGMENTED PAVING AND ANCILLARY WORKS"]
["SECTION 8","KERBING AND CHANNELLING"]
[null,"SUB TOTAL"]
[null,"ADD: ALLOWANCE FOR CONTINGENCIES @ 20%"]
[null,"SUB TOTAL"]
[null,"ADD ALLOWANCE FOR ESCALATION @ 6%"]
[null,"SUB TOTAL"]
[null,"ADD: VAT @ 15%"]
["TOTAL TENDERED AMOUNT INCLUDING VAT AND ALLOWANCES FOR ESCALATION AND CONTINGENCIES"]