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1. Policy, Leadership and Commitment

a) The contractor and or supplier shall have a documented and implemented environmental management system e.g. environmental policy, operational procedures relating to their activities, aspects/impacts register etc.;
b) The contractor shall comply with all Eskom Grootvlei Power Station environmental requirements such as policies, standards and procedures (work instructions);
c) The contractor shall appoint personnel in writing with basic Environmental knowledge who will have the responsibilities of implementing all environmental/SHE requirements on a specific contract;
d) Method statements related to activities that have significant environmental impacts (methodology and approach) illustrating how environmental impacts and risks will be managed.
e) Station Waste management procedure and color coding shall be adhered to at all times.
f) Ensure that all Environmental Requirements are communicated to relevant employees.
g) The contractor and or supplier shall allocate funds for the implementation of environmental requirements.

2. Legal and Other Requirements
a. Adherence to the ‘Duty of Care’ as stipulated in section 28 of the National Environmental Management Act 107 of 2008 and National Environmental Management: Waste Act, 2008 (Act 59 of 2008) 

3. Aspects, Impacts, Objectives and Targets
a. The contractor will need to ensure that all aspects and impacts that can result in negative impacts on the environmental through their operations are identified and documented. 
b. Objectives and targets will need to be established for aspects and impacts that are deemed to be significant. These objectives and targets will need to be documented and conveyed to all contractor personnel.
c. HCRW must be managed in accordance with the Eskom Health Care Risk Waste Management Standard (240-115842952), National Health Act 61 of 2003 GN 1229, and other related documents.

4. Incident Report and Investigation
a. All incidents shall be managed according to Eskom Environmental incident management procedure-240-133087117.
b. Polluter pays principles shall apply to all Contractors. It is the responsibility of the polluter to clean all spillages and for the rehabilitation of the polluted land and the cost associated with that.
c. Emergency Response Procedure which will be implemented in the event of spillage resultant from any accident during the transportation of the hazardous waste.	
d. HCGW and HCRW shall not be disposed of by burning, dumping, or burying in pits or in trenches. 

5. Health Care Risk Waste

a. The contractor shall provide waste receptacle as required for the medical waste to be disposed of 
b. The receptacle must be properly sealed and must be leak proof and puncture proof to prevent possible spillage and resultant pollution during the storage, collection and transport thereof,
c. Medical waste shall be disposed at permitted hazardous waste incineration facility,
d. All health care risk waste is to be disposed of at an appropriate incineration facility having a valid registration certificate issued by the Department of Environmental Affairs in terms of current legislations.
e. All health care risk waste is to be removed from the power station under cover of a waste manifest document as part of the waste tracking and safe system which will ensure proper disposal of the health care risk waste.
f. The contractor shall provide the employer with a certificate of safe disposal per event for all health care risk waste incinerated for his records within 2 weeks of removal from site.

6. The transportation of hazardous waste shall be in accordance with the National Road Traffic Act 93 of 1996 which includes but is not limited to the following:

a. Vehicles transporting Dangerous Goods must be fitted with the necessary Hazchem labels and placards, emergency triangles, dangerous goods operator card, spill response equipment and the correct number and type of fire extinguishers required for the specific load being transported.
b. The transportation of this waste stream by the contractor shall be in accordance with the National Road Traffic Act No 93 of 1996, The hazardous substances Act (Act 15 of 1973), The Occupational, Health and Safety Act (Act 85 of 1993) SANS Code 10228 (Deals with labelling of bulk containers and placarding of the vehicle in accordance with the type of waste being transported).
c. The operator of the Dangerous Goods Vehicle must be issued with a PDP-"D" Professional driving permit code and have this in his possession at all times
d. The Operator of the Dangerous Goods Vehicle must have in the designated space of the dangerous goods vehicle the required Tremcards and relevant dangerous goods declarations.
e. The Operator of the Dangerous Goods Vehicle must have in his possession a document clearly indicating the route to be followed to the incineration facility at which the health care risk waste is to be incinerated.
f. [bookmark: _Hlk164148146]The contractor shall provide the Employer at the start of the contract with a copy of their valid Emergency Response Procedure which will be implemented in the event of spillage resultant from any accident during the transportation of the hazardous waste.
g. The boxes and containers provided by the contractor for the disposal of the health care risk waste must be manufactured from such material strength to ensure that there is no escape of the waste from the containers during collection, transport and disposal process must be suitably marked with appropriate insignia so as to indicate the hazardous content thereof.
h.  Driver / operator must be trained on hazardous waste transportation and emergency response and proof submitted with other requirement,
i. The contractor will provide the employer with a copy of a valid Registration Certificate of the incineration facility used for the destruction of the health care risk waste as well as the permit of the Class H: H waste disposal site used for the disposal of the ash resultant from the incineration process for his records and a map showing the route that will be used.
j.  During the collection of waste, the contractor is to report to the employer first and he (the contractor) will be taken to site to collect the waste.
k. Any spillages that might occur during the loading of the containers must be cleaned by the contractor before leaving the Power station’s premises. 
l. There will be yearly audits for all permitted waste disposal sites which will be headed by the contractor and they will be accompanied by the employer and the contractor site supervisor, after audits the contractor should arrange the meeting between the contractor and the employer to compile an audit report.
m. The contractor must comply with the provision’s pf the Hazardous Chemical Regulations in GNR 1179 of 25/08/1995 (subsequently amended by GNR.930 of 25 June 2023 and GNR.683 of 27 June 2008)

7. Monitoring and Review 
a. Client personnel will conduct regular environmental audits. Contractors are expected to participate and ensure that corrective actions are executed.
b. Eskom Grootvlei Power Station shall issue non-conformances where there are deviations from Grootvlei Power Station Procedures and any other environmental requirements.
a. All environmental system documentation, records, reports etc. shall be made available for review when requested.
