{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["DBSA_MQHAWE"],"read":"whole","date_system":"1900"}

{"sheet":"DBSA_MQHAWE","index":0,"n_rows":8402,"n_cols":7,"rows_kept":8402}
[null,null,"MQHAWE HIGH SCHOOL EXCEL BOQ"]
[]
["PAGE NO","ITEM NO","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[1,null,"SECTION 1","H1"]
[]
[1,null,"PRELIMINARIES","H1"]
[]
[1,null,"BILL NO. 1","H1"]
[]
[1,null,"MEANING OF TERMS \"TENDER / TENDERER\"","H2"]
[]
[1,null,"Any reference to the words \"Tender\" or \"Tenderer\" herein and/or in any other documentation shall be construed to have the same meaning as the words \"Bid\" or \"Bidder\""]
[]
[1,null,"PRELIMINARIES","H2"]
[]
[1,null,"The JBCC Preliminaries Code 2103, May 2005 edition for use with the JBCC Principal Building Agreement Edition 4.1 Code 2101, March 2005 is taken to be incorporated herein. The tenderer is deemed to have referred to these documents for the full intent and meaning of each clause. These clauses are referred to by number and heading only. Where standard clauses or options are not applicable to the contract such modifications or corrections as are necessary are given under each relevant clause. Where an item is not relevant to this specific contract such item is marked \"N/A\" signifying \"Not Applicable\""]
[]
[1,null,"PRICING OF PRELIMINARIES","H2"]
[]
[1,null,"Should Option A, as set out in clause B10.3.1 hereinafter be used for the adjustment of preliminaries then each item priced is to be allocated to one or more of the three categories Fixed, Value Related or Time Related and the respective amounts entered in the spaces provided under each item"]
[]
[1,null,"Items not priced in these Preliminaries shall be deemed to be included elsewhere in these Bills of Quantities"]
[]
[2,null,"SECTION A: JBCC PRINCIPAL BUILDING AGREEMENT","H2"]
[]
[2,null,"DEFINITIONS","H2"]
[]
[2,1,"A1.0   \tDEFINITIONS AND INTERPRETATIONClause 1.0  Clause 1.1 Definition of \"Commencement Date\" is added:","CONT"]
[]
[2,null,"\"COMMENCEMENT DATE\" means the date that the agreement, made in terms of the Form of Offer and Acceptance, comes into effect","CONT"]
[]
[2,null,"Clause 1.1 Definition of \"Construction Guarantee\" is amended by replacing it with the following:","CONT"]
[]
[2,null,"\"CONSTRUCTION GUARANTEE\" means a guarantee at call obtained by the contractor from an institution approved by the employer in terms of the employer's construction guarantee form as selected in the schedule","CONT"]
[]
[2,null,"Clause 1.1 Definition of \"Construction Period\" is amended by replacing it with the following:","CONT"]
[]
[2,null,"\"CONSTRUCTION PERIOD\" means the period commencing on the commencement date and ending on the date of practical completion","CONT"]
[]
[2,null,"Clause 1.1 Definition of \"Corrupt Practice\" is added:","CONT"]
[]
[2,null,"\"CORRUPT PRACTICE\" means the offering, giving, receiving or soliciting of anything of value to influence the action of a public official in the procurement process or in contract execution","CONT"]
[]
[2,null,"Clause 1.1 Definition of \"Fraudulent Practice\" is added:","CONT"]
[]
[3,null,"\"FRAUDULENT PRACTICE\" means a mispresentation of facts in order to influence a procurement process or the execution of a contract to the detriment of any tenderer and includes collusive practice among tenderers (prior to or after the tender submission) designed to establish tender prices at artificial non-competitive levels and to deprive the tenderer of the benefits of free and open competition","CONT"]
[]
[3,null,"Clause 1.1 Definition of \"Interest\" is amended by replacing it with the following:","CONT"]
[]
[3,null,"\"INTEREST\" means the interest rates applicable on this contract, whether specifically indicated in the relevant clauses or not, will be the rate as determined by the Minister of Finance, from time to time, in terms of section 80(1)(b) of the Public Finance Management Act, 1999 (Act No. 1 of 1999)","CONT"]
[]
[3,null,"Clause 1.1 Definition of \"Principal Agent\" is amended by replacing it with the following:","CONT"]
[]
[3,null,"\"PRINCIPAL AGENT\" means the person or entity appointed by the employer and named in the schedule. In the event of a principal agent not being appointed, then all the duties and obligations of a principal agent as detailed in the agreement shall be fulfilled by a representative of the employer as named in the schedule","CONT"]
[]
[3,null,"Clause 1.1 Definition of \"Security\" is amended by replacing it with the following:","CONT"]
[]
[3,null,"\"SECURITY\" means the form of security provided by the employer or contractor, as stated in the schedule, from which the contractor or employer may recover expense or loss","CONT"]
[]
[3,null,"Clause 1.6 is amended by replacing the words \"prepaid registered post, telefax or e-mail\" with \"prepaid registered post or telefax\"","CONT"]
[]
[3,null,"Clause 1.6.4 is amended by replacing it with the following:","CONT"]
[]
[4,null,"No clause  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[4,null,"OBJECTIVE AND PREPARATION","H2"]
[]
[4,2,"A2.0\tOFFER, ACCEPTANCE AND PERFORMANCE  Clause 2.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[4,3,"A3.0\tDOCUMENTS \tClause 3.0Clause 3.2.1 is amended by replacing\"14.1\" with \"14.0\"Clause 3.7 is amended by the addition of the following:  The contractor shall supply and keep a copy of the JBCC Series 2000 Principal Building Agreement and Preliminaries applicable to this contract on the site, to which the employer, principal agent and agents shall have access at all timesClause 3.10 is amended by replacing the second reference to \"principal agent\" with the word \"employer\" \tFixed:____________ Value related:____________ Time related:____________","Item"]
[]
[4,4,"A4.0\tDESIGN RESPONSIBILITY \tClause 4.0Clause 4.3 is amended by replacing it with the following:No clause\tFixed:____________ Value related:____________ Time related:____________","Item"]
[]
[5,5,"A5.0\tEMPLOYER'S AGENTS Clause 5.0 Clause 5.1.2 is amended to include clauses 32.6.3, 34.3, 34.4 and 38.5.8 Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[5,6,"A6.0\tSITE REPRESENTATIVE Clause 6.0 Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[5,7,"A7.0\tCOMPLIANCE WITH REGULATIONS Clause 7.0 \tNote: A separate clause has been included in Section C : Specific Preliminaries of the bills of quantities / lump sum document for the contractor to have the opportunity to price for all the requirements of the Occupational Health and Safety Act, Construction Regulations and Health and Safety SpecificationFixed:____________ Value related:____________ Time related:____________","Item"]
[]
[5,8,"A8.0\tWORKS RISK Clause 8.0 Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[5,9,"A9.0\tINDEMNITIES Clause 9.0 Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[6,10,"A1\tWORKS INSURANCES Clause 1 Clause 1 is amended by the addition of the following clauses:","CONT"]
[]
[6,null,"10.5 Damage to the Works  (a) \tWithout in any way limiting the contractor's obligations in terms of the contract, the contractor shall bear the full risk of damage to and/or destruction of the works by whatever cause during construction of the works and hereby indemnifies and holds harmless the employer against any such damage. The contractor shall take such precautions and security measures and other steps for the protection and security of the works as the contractor may deem necessary","CONT"]
[]
[6,null,"(b)\tThe contractor shall at all times proceed immediately to remove or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works","CONT"]
[]
[6,null,"(c)\tThe employer shall carry the risk of damage to or destruction of the works and materials paid for by the employer that is the result of the excepted risks as set out in 10.6","CONT"]
[]
[6,null,"(d)\tWhere the employer bears the risk in terms of this contract, the contractor shall, if requested to do so, reinstate any damage or destroyed portions of the works and the costs of such reinstatement shall be measured and valued in terms of 32.0 hereof","CONT"]
[]
[7,null,"10.6 Injury to Persons or loss of or damage to Properties  (a)\tThe contractor shall be liable for and hereby indemnifies the employer against any liability, loss, claim or proceeding whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever arising out of or in the course of or caused by the execution of the works unless due to any act or negligence of any person for whose actions the employer is legally liable","CONT"]
[]
[7,null,"(b)\tThe contractor shall be liable for and hereby indemnifies the employer against any liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the employer or any other body or person, arising out of or in the course of or by reason of the execution of the works unless due to any act or negligence of any person for whose actions the employer is legally liable","CONT"]
[]
[7,null,"(c)\tThe contractor shall, upon receiving a contract instruction from the principal agent, cause the same to be made good in a perfect and workmanlike manner at his own cost and in default thereof the employer shall be entitled to cause it to be made good and to recover the cost thereof from the contractor or to deduct the same from amounts due to the contractor","CONT"]
[]
[7,null,"(d)\tThe contractor shall be responsible for the protection and safety of such portions of the premises placed under his control by the employer for the purpose of executing the works until the issue of the certificate of practical completion","CONT"]
[]
[8,null,"(e)\tWhere the execution of the works involves the risk of removal of or interference with support to adjoining properties including land or structures or any structures to be altered or added to, the contractor shall obtain adequate insurance and will remain adequately insured or insured to the specific limit stated in the contract against the death of or injury to persons or damage to such property consequent on such removal or interference with the support until such portion of the works has been completed","CONT"]
[]
[8,null,"(f)\tThe contractor shall at all times proceed immediately at his own cost to remove or dispose of any debris and to rebuild, restore, replace and/or repair such property and to execute the works","CONT"]
[]
[8,null,"10.7 High risk insurance In the event of the project being executed in a geological area classified as a \"High Risk Area\", that is an area which is subject to highly unstable subsurface conditions that might result in catastrophic ground movement evident by sinkhole or doline formation the following will apply:","CONT"]
[]
[8,null,"10.7.1 Damage to the works  The contractor shall, from the commencement date of the works until the date of the certificate of practical completion bear the full risk of and hereby indemnifies and holds harmless the employer against any damage to and/or destruction of the works consequent upon a catastrophic ground movement as mentioned above. The contractor shall take such precautions and security measures and other steps for the protection of the works as he may deem necessary","CONT"]
[]
[8,null,"When so instructed to do so by the principal agent, the contractor shall proceed immediately to remove and/or dispose of any debris arising from damage to or destruction of the works and to rebuild, restore, replace and/or repair the works, at the contractor's own costs","CONT"]
[]
[9,null,"10.7.2 Injury to persons or loss of or damage to property  The contractor shall be liable for and hereby indemnifies and holds harmless the employer against any liability, loss, claim or proceeding arising at any time during the period of the contract whether arising in common law or by statute, consequent upon personal injuries to or the death of any person whomsoever resulting from, arising out of, or caused by a catastrophic ground movement as mentioned above","CONT"]
[]
[9,null,"The contractor shall be liable for and hereby indemnifies the employer against any and all liability, loss, claim or proceeding consequent upon loss of or damage to any moveable or immovable or personal property or property contiguous to the site, whether belonging to or under the control of the employer or any other body or person whomsoever arising out of or caused by a catastrophic ground movement, as mentioned above, which occurred during the period of the contract","CONT"]
[]
[9,null,"10.7.3 It is the responsibility of the contractor to ensure that he has adequate insurance to cover his risk and liability as mentioned in 10.7.1 and 10.7.2. Without limiting the contractor's obligations in terms of the contract, the contractor shall, within twenty-one (21) calendar days of the commencement date but before commencement of the works, submit to the employer proof of such insurance policy, if requested to do so","CONT"]
[]
[9,null,"10.7.4 The employer shall be entitled to recover any and all losses and/or damages of whatever nature suffered or incurred consequent upon the contractor's default of his obligations as set out in 10.7.1; 10.7.2 and 10.7.3. Such losses or damages may be recovered from the contractor or by deducting the same from any amounts still due under this contract or under any other contract presently or hereafter existing between the employer and the contractor and for this purpose all these contracts shall be considered one indivisible whole Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[10,11,"A11.0\tLIABILITY INSURANCES  Clause 11.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[10,12,"A12.0\tEFFECTING INSURANCES  Clause 12.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[10,13,"A13.0\tNo clause","N/A"]
[]
[10,14,"A14.0\tSECURITY  Clause 14.0  Clauses 14.1 - 14.8 are amended by replacing them with the following:","CONT"]
[]
[10,null,"14.1 In respect of contracts with a contract sum up to R1 million, the security to be provided by the contractor to the employer will be a payment reduction of five per cent (5%) of the value certified in the payment certificate (excluding VAT)","CONT"]
[]
[10,null,"14.1.1 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(A)","CONT"]
[]
[10,null,"14.1.2 The employer shall be entitled to recover expense and loss from the payment reduction in terms of 33.0 provided that the employer complies with the provisions of 33.4 in which event the employer's entitlement shall take precedence over his obligations to refund the payment reduction security or portions thereof to the contractor","CONT"]
[]
[11,null,"14.2 In respect of contracts with a contract sum above R1 million, the contractor shall have the right to select the security to be provided in terms of 14.3, 14.4, 14.5, 14.6, or 14.7 as stated in the schedule. Such security shall be provided to the employer within twenty-one (21) calendar days from commencement date. Should the contractor fail to select the security to be provided or should the contractor fail to provide the employer with the selected security within twenty-one (21) calendar days from commencement date, the security in terms of 14.7 shall be deemed to have been selected","CONT"]
[]
[11,null,"14.3 Where security as a cash deposit of ten per cent (10%) of the contract sum (excluding VAT) has been selected:","CONT"]
[]
[11,null,"14.3.1 The contractor shall furnish the employer with a cash deposit equal in value to ten per cent (10%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date","CONT"]
[]
[11,null,"14.3.2 Within twenty-one (21) calendar days of the date of practical completion of the works the employer shall reduce the cash deposit to an amount equal to three per cent (3%) of the contract value (excluding VAT), and refund the balance to the contractor","CONT"]
[]
[11,null,"14.3.3 Within twenty-one (21) calendar days of the date of final completion of the works the employer shall reduce the cash deposit to an amount equal to one per cent (1%) of the contract value (excluding VAT) and refund the balance to the contractor","CONT"]
[]
[11,null,"14.3.4 On the date of payment of the amount in the final payment certificate, the employer shall refund the remainder of the cash deposit to the contractor","CONT"]
[]
[11,null,"14.3.5 The employer shall be entitled to recover expense and loss from the cash deposit in terms of 33.0 provided that the employer complies with the provisions of 33.4 in which event the employer's entitlement shall take precedence over his obligations to refund the cash deposit security or portions thereof to the contractor","CONT"]
[]
[11,null,"14.3.6 The parties expressly agree that neither the employer nor the contractor shall be entitled to cede the rights to the deposit to any third party","CONT"]
[]
[12,null,"14.4 Where security as a variable construction guarantee of ten percent (10%) of the contract sum (excluding VAT) has been selected:","CONT"]
[]
[12,null,"14.4.1 The contractor shall furnish the employer with an acceptable variable construction guarantee equal in value to ten per cent (10%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date","CONT"]
[]
[12,null,"14.4.2 The variable construction guarantee shall reduce and expire in terms of the Variable Construction Guarantee form included in the invitation to tender","CONT"]
[]
[12,null,"14.4.3 The employer shall return the variable construction guarantee to the contractor within fourteen (14) calendar days of it expiring","CONT"]
[]
[12,null,"14.4.4 Where the employer has a right of recovery against the contractor in terms of 33.0, the employer shall issue a written demand in terms of the variable construction guarantee","CONT"]
[]
[12,null,"14.5 Where security as a fixed construction guarantee of five per cent (5%) of the contract sum (excluding VAT) and a five per cent (5%) payment reduction of the value certified in the payment certificate (excluding VAT) has been selected:","CONT"]
[]
[12,null,"14.5.1 The contractor shall furnish a fixed construction guarantee to the employer equal in value to five per cent (5%) of the contract sum (excluding VAT)","CONT"]
[]
[12,null,"14.5.2 The fixed construction guarantee shall come into force on the date of issue and shall expire on the date of the last certificate of practical completion","CONT"]
[]
[12,null,"14.5.3 The employer shall return the fixed construction guarantee to the contractor within fourteen (14) calendar days of it expiring","CONT"]
[]
[12,null,"14.5.4 The payment reduction of the value certified in a payment certificate shall be in terms of 31.8 (A) and 34.8","CONT"]
[]
[13,null,"14.5.5 Where the employer has a right of recovery against the contractor in terms of 33.0, the employer shall be entitled to issue a written demand in terms of the fixed construction guarantee or may recover from the payment reduction or may do both","CONT"]
[]
[13,null,"14.6 Where security as a cash deposit of five per cent (5%) of the contract sum (excluding VAT) and a payment reduction of five per cent (5%) of the value certified in the payment certificate (excluding VAT) has been selected:","CONT"]
[]
[13,null,"14.6.1 The contractor shall furnish the employer with a cash deposit equal in value to five per cent (5%) of the contract sum (excluding VAT) within twenty-one (21) calendar days from commencement date","CONT"]
[]
[13,null,"14.6.2 Within twenty-one (21) calendar days of the date of practical completion of the works the employer shall refund the cash deposit in total to the contractor","CONT"]
[]
[13,null,"14.6.3 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(A)","CONT"]
[]
[13,null,"14.6.4 Where the employer has a right of recovery against the contractor in terms of 33.0, the employer may issue a written notice in terms of 33.4 or may recover from the payment reduction or may do both","CONT"]
[]
[13,null,"14.7 Where security as a payment reduction of ten per cent (10%) of the value certified in the payment certificate (excluding VAT) has been selected:","CONT"]
[]
[13,null,"14.7.1 The payment reduction of the value certified in a payment certificate shall be mutatis mutandi in terms of 31.8(B)","CONT"]
[]
[13,null,"14.7.2 The employer shall be entitled to recover expense and loss from the payment reduction in terms of 33.0 provided that the employer complies with the provisions of 33.4 in which event the employer's entitlement shall take precedence over his obligations to refund the payment reduction or portions thereof to the contractor","CONT"]
[]
[14,null,"14.8 Payments made by the guarantor to the employer in terms of the fixed or variable construction guarantee shall not prejudice the rights of the employer or contractor in terms of this agreement","CONT"]
[]
[14,null,"14.9 Should the contractor fail to furnish the security in terms of 14.2, the employer, in his sole discretion and without notification to the contractor, is entitled to change the contractor's selected form of security to that of a ten per cent (10%) payment reduction of the value certified in the payment certificate (excluding VAT), whereafter 14.7 shall be applicable  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[14,null,"EXECUTION","H2"]
[]
[14,15,"A15.0\tPREPARATION FOR AND EXECUTION OF THE WORKS  Clause 15.0  Clause 15.1.1 is amended by replacing it with:  No clause  Clause 15.1.2 is amended by replacing it with:  The security selected in terms of 14.0","CONT"]
[]
[14,null,"Clause 15.1 is amended by the addition of the following clause:  15.1.4 An acceptable health and safety plan, required in terms of the Occupational Health and Safety Act, 1993 (Act 85 of 1993), within twenty-one (21) calendar days of commencement date","CONT"]
[]
[14,null,"Clause 15.2.1 is amended by replacing it with the following clause:","CONT"]
[]
[14,null,"Give the contractor possession of the site within ten (10) working days of the contractor complying with the terms of 15.1.4  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[15,16,"A16.0\tACCESS TO THE WORKS  Clause 16.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[15,17,"A17.0\tCONTRACT INSTRUCTIONS  Clause 17.0  Clause 17.1.11 is amended by deleting the words \"and the appointment of nominated and selected subcontractors\"  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[15,18,"A18.0\tSETTING OUT OF THE WORKS  Clause 18.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[15,19,"A19.0\tASSIGNMENT  Clause 19.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[15,20,"A2\tNOMINATED SUBCONTRACTORS  Clause 2  Clause 20.1.3 is amended by replacing it with the following:  No clause  Note: See item B9.1 hereinafter for adjustment of attendance on nominated subcontractors executing work allowed for under provisional sums  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[16,21,"A21.0\tSELECTED SUBCONTRACTORS  Clause 21.0  Clause 21 is amended by replacing it with:  No clause  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[16,22,"A22.0\tEMPLOYER'S DIRECT CONTRACTORS  Clause 22.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[16,23,"A23.0\tCONTRACTOR'S DOMESTIC SUBCONTRACTORS  Clause 23.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[16,null,"COMPLETION","H2"]
[]
[16,24,"A24.0\tPRACTICAL COMPLETION  Clause 24.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[16,25,"A25.0\tWORKS COMPLETION  Clause 25.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[17,26,"A26.0\tFINAL COMPLETION  Clause 26.0  Clause 26.1.2 is amended by inserting \"#\" next to 26.1.2  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[17,27,"A27.0\tLATENT DEFECTS LIABILITY PERIOD  Clause 27.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[17,28,"A28.0\tSECTIONAL COMPLETION  Clause 28.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[17,29,"A29.0\tREVISION OF DATE FOR PRACTICAL COMPLETION  Clause 29.0  Clause 29.2.5 is amended by replacing it with:  No clause  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[17,30,"A3\tPENALTY FOR NON-COMPLETION  Clause 3  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[17,null,"PAYMENT","H2"]
[]
[17,31,"A31.0\tINTERIM PAYMENT TO THE CONTRACTOR  Clause 31.0","CONT"]
[]
[18,null,"Clause 31.5.2 is amended by replacing \"14.7.1\" with \"14.0\"","CONT"]
[]
[18,null,"Clause 31.8 is amended by replacing it with the following two alternative clauses:","CONT"]
[]
[18,null,"Alternative A  31.8(A) Where a security is selected in terms of 14.1; 14.5 or 14.6, the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:","CONT"]
[]
[18,null,"31.8(A).1 Ninety-five per cent (95%) of such value in interim payment certificates issued up to the date of practical completion","CONT"]
[]
[18,null,"31.8(A).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of practical completion and up to but excluding the date of final completion","CONT"]
[]
[18,null,"31.8(A).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of final completion and up to but excluding the final payment certificate in terms of 34.6","CONT"]
[]
[18,null,"31.8(A).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate","CONT"]
[]
[18,null,"Alternative B","CONT"]
[]
[18,null,"31.8(B) Where security as a payment reduction in terms of 14.7 has been selected, the value of the works in terms of 31.4.1 and materials and goods in terms of 31.4.2 shall be certified in full. The value certified shall be subject to the following percentage adjustments:","CONT"]
[]
[18,null,"31.8(B).1 Ninety per cent (90%) of such value in interim payment certificates issued up to the date of practical completion","CONT"]
[]
[19,null,"31.8(B).2 Ninety-seven per cent (97%) of such value in interim payment certificates issued on the date of practical completion and up to but excluding the date of final completion","CONT"]
[]
[19,null,"31.8(B).3 Ninety-nine per cent (99%) of such value in interim payment certificates issued on the date of final completion and up to but excluding the final payment certificate in terms of 34.6","CONT"]
[]
[19,null,"31.8(B).4 One hundred per cent (100%) of such value in the final payment certificate in terms of 34.6 except where the amount certified is in favour of the employer. In such an event the payment reduction shall remain at the adjustment level applicable to the final payment certificate","CONT"]
[]
[19,null,"Clause 31.12 is amended by deleting the following:","CONT"]
[]
[19,null,"Payment shall be subject to the employer giving the contractor a tax invoice for the amount due  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[19,32,"A32.0\tADJUSTMENT TO THE CONTRACT VALUE  Clause 32.0  Clauses 32.5.1, 32.5.4 and 32.5.7 are amended by the addition of the following at the end of the sentence:  \"due to no fault of the contractor\"  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[19,33,"A33.0\tRECOVERY OF EXPENSE AND LOSS  Clause 33.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[20,34,"A34.0\tFINAL ACCOUNT AND FINAL PAYMENT  Clause 34.0  Clause 34.1 is amended by removing \"#\" next to 34.1  Clause 34.2 is amended by inserting \"#\" next to 34.2  Clause 34.8 is amended by deleting the words \"where security as a fixed construction guarantee in terms of 14.4 has been selected or where payment reduction has been applied in terms of 14.7.1\"  Clause 34.13 is amended by replacing \"seven (7) calendar days\" with \"twenty-one (21) calendar days\" and deleting the words \"subject to the employer giving the contractor a tax invoice for the amount due\"  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[20,35,"A35.0\tPAYMENT TO OTHER PARTIES  Clause 35.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[21,null,"CANCELLATION","H2"]
[]
[21,36,"A36.0\tCANCELLATION BY EMPLOYER - CONTRACTOR'S DEFAULT \t  Clause 36.0  Clause 36.1 is amended by the addition of the following clauses:  36.1.3 refuses or neglects to comply strictly with any of the conditions of contract  36.1.4 estate being sequestrated, liquidated or surrendered in terms of the insolvency laws in force within the Republic of South Africa  36.1.5 in the judgement of the employer, has engaged in corrupt or fraudulent practices in competing for or in executing the contract  Clause 36.3 is amended by removing the reference to \"No clause\" and replacing the words \"principal agent\" with \"employer\"","CONT"]
[]
[21,null,"Clause 36.0 is amended by the addition of the following clause:","CONT"]
[]
[21,null,"36.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[21,37,"A37.0\tCANCELLATION BY EMPLOYER - LOSS AND DAMAGE  Clause 37.0  Clause 37.3.5 is amended by replacing \"ninety (90)\" with \"one hundred and twenty (120)\"","CONT"]
[]
[22,null,"Clause 37.0 is amended by the addition of the following clause:  37.5 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[22,38,"A38.0\tCANCELLATION BY CONTRACTOR - EMPLOYER'S DEFAULT  Clause 38.0  Clause 38.5.4 is amended by replacing \"ninety (90)\" with \"one hundred and twenty (120)\"  Clause 38.0 is amended by the addition of the following clause:","CONT"]
[]
[22,null,"38.7 Notwithstanding any clause to the contrary, on cancellation of this agreement either by the employer or the contractor; or for any reason whatsoever, the contractor shall on written instruction, discontinue with the works on a date stated and withdraw himself from the site. The contractor shall not be entitled to refuse to withdraw from the works on the grounds of any lien or right of retention or on the grounds of any other right whatsoever  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[23,39,"A39.0\tCANCELLATION - CESSATION OF THE WORKS  Clause 39.0  Clause 39.3.5 is amended by the addition of the following at the end of the sentence:  \"within one hundred and twenty (120) working days of completion of such a report\"  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[23,null,"DISPUTE","H2"]
[]
[23,40,"A4\tDISPUTE SETTLEMENT Clause 4 \tClause 40.2.2 is amended by replacing \"one (1) year\" with \"three (3) years\"  Clause 40.6 is amended by removing the reference to:  No clause \tClause 40.7.1 is amended by replacing \"(10)\" with \"(15)\" and by the addition of the following: \tWhether or not mediation resolves the dispute, the parties shall bear their own costs concerning the mediation and equally share the costs of the mediator and related costs \tFixed:____________ Value related:____________ Time related:____________","Item"]
[]
[23,null,"SUBSTITUTE PROVISIONS","H2"]
[]
[23,41,"A41.0\tSTATE CLAUSES  Clause 41.0  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[24,null,"CONTRACT VARIABLES","H2"]
[]
[24,42,"A42.0\tTHE SCHEDULE (DPW-04EC)  Clause 42.0  Tenderers are referred to the Contract Data DPW-04(EC) for variables pertaining to this contract  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[24,null,"SECTION B: JBCC PRELIMINARIES","H1"]
[]
[24,null,"B1.0\tDEFINITIONS AND INTERPRETATION","H2"]
[]
[24,43,"B1.1\tDefinitions and interpretation  See also clause A1.0 of Section A for additional and/or amended definitions which shall apply equally to this Section  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[24,null,"B2.0\tDOCUMENTS","H2"]
[]
[24,44,"B2.1\tChecking of documents  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[24,45,"B2.2\tProvisional bills of quantities  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[24,46,"B2.3\tAvailability of construction documentation  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[24,47,"B2.4\tInterests of agents  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,48,"B2.5\tPriced documents  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,49,"B2.6\tTender submission  Clause 2.6 is amended by replacing \"JBCC Form of Tender\" with \"Form of Offer and Acceptance DPW-07(EC)\"  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,null,"B3.0\tTHE SITE","H2"]
[]
[25,50,"B3.1\tDefined works area  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,51,"B3.2\tGeotechnical investigation  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,52,"B3.3\tInspection of the site  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,53,"B3.4\tExisting premises occupied  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,54,"B3.5\tPrevious work - dimensional accuracy  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[25,55,"B3.6\tPrevious work - defects  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,56,"B3.7\tServices - known  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,57,"B3.8\tServices - unknown  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,58,"B3.9\tProtection of trees  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,59,"B3.10\tArticles of value  Fixed:____________ Value related:____________ Time related:___________","Item"]
[]
[26,60,"B3.11\tInspection of adjoining properties  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,null,"B4.0\tMANAGEMENT OF CONTRACT","H2"]
[]
[26,61,"B4.1\tManagement of the works  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,62,"B4.2\tProgramme for the works  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,63,"B4.3\tProgress meetings  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[26,64,"B4.4\tTechnical meetings  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,65,"B4.5\tLabour and plant records  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,null,"B5.0\tSAMPLES, SHOP DRAWINGS AND MANUFACTURERS’ INSTRUCTIONS","H2"]
[]
[27,66,"B5.1\tSamples of materials  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,67,"B5.2\tWorkmanship samples  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,68,"B5.3\tShop drawings  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,69,"B5.4\tCompliance with manufacturers' instructions  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,null,"B6.0\tTEMPORARY WORKS AND PLANT","H2"]
[]
[27,70,"B6.1\tDeposits and fees  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,71,"B6.2\tEnclosure of the works  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[27,72,"B6.3\tAdvertising  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,73,"B6.4\tPlant, equipment, sheds and offices  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,74,"B6.5\tMain notice board  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,75,"B6.6\tSubcontractors' notice board  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,null,"B7.0\tTEMPORARY SERVICES","H2"]
[]
[28,76,"B7.1\tLocation  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,77,"B7.2\tWater  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,78,"B7.3\tElectricity  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,79,"B7.4\tTelecommunication facilities  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,80,"B7.5\tAblution facilities  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[28,null,"B8.0\tPRIME COST AMOUNTS","H2"]
[]
[28,81,"B8.1\tResponsibility for prime cost amounts  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,null,"B9.0\tATTENDANCE ON N/S SUBCONTRACTORS","H2"]
[]
[29,82,"B9.1\tGeneral attendance  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,83,"B9.2\tSpecial attendance  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,84,"B9.3\tCommissioning - fuel, water and electricity  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,null,"B1\tFINANCIAL ASPECTS","H2"]
[]
[29,85,"B10.1\tStatutory taxes, duties and levies  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,86,"B10.2\tPayment for preliminaries  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,87,"B10.3\tAdjustment of preliminariesClauses B10.3.1 and B10.3.2 are amended by replacing \"within fifteen (15) working days of taking possession of the site\" with \"when submitting his priced bills of quantities / lump sum document\" Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[29,88,"B10.4\tPayment certificate cash flow  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,null,"B11.0\tGENERAL","H2"]
[]
[30,89,"B11.1\tProtection of the works  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,90,"B11.2\tProtection / isolation of existing / sectionally occupied works  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,91,"B11.3\tSecurity of the works  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,92,"B11.4\tNotice before covering work  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,93,"B11.5\tDisturbance  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,94,"B11.6\tEnvironmental disturbance  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,95,"B11.7\tWorks cleaning and clearing  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,96,"B11.8\tVermin  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[30,97,"B11.9\tOverhand work  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[31,98,"B11.10\tInstruction manuals and guarantees  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[31,99,"B11.11\tAs built information  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[31,100,"B11.12\tTenant installations  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[31,null,"B12.0\tSCHEDULE OF VARIABLES","H2"]
[]
[31,101,"B12.1\tSchedule of variables  Fixed:____________ Value related:____________ Time related:____________","Item"]
[]
[31,null,"This schedule contains all variables referred to in this document and is divided into pre-tender and post-tender categories. The pre-tender category must be completed in full and included in the tender documents. Both the pre-tender and post-tender categories form part of these Preliminaries"]
[]
[31,null,"Spaces requiring information must be filled in, shown as \"not applicable\" or deleted and not left blank. Where choices are offered, the non-applicable items are to be deleted. Where insufficient space is provided the information should be annexed hereto and cross-referenced to the applicable clause of the schedule. Key cross reference clauses are italicised in [ ] brackets"]
[]
[31,null,"12.1\tPRE-TENDER INFORMATION  12.1.1\tProvisional bills of quantities [2.2]\tThe quantities are provisional\t\t\t\t\tYES/NO"]
[]
[31,null,"12.1.2\tAvailability of construction documentation [2.3]\tConstruction documentation is complete\t\t\t\tYES/NO"]
[]
[32,null,"12.1.3\tInterests of agents [2.4]\tDetails: "]
[]
[32,null,"12.1.4\tDefined works area [3.1]\tDetails: "]
[]
[32,null,"12.1.5\tGeotechnical investigation [3.2]\tDetails: "]
[]
[32,null,"12.1.6\tExisting premises occupied [3.4]\tSpecific requirements: "]
[]
[32,null,"12.1.7\tPrevious work - dimensional accuracy [3.5]\tDetails: "]
[]
[32,null,"12.1.8\tPrevious work - defects [3.6]\tDetails: "]
[]
[32,null,"12.1.9\tServices - known [3.7]\tDetails: "]
[]
[32,null,"12.1.10\tProtection of trees [3.9]\tSpecific requirements: "]
[]
[32,null,"12.1.11\tInspection of adjoining properties [3.11]\tSpecific requirements: "]
[]
[32,null,"12.1.12\tEnclosure of the works [6.2]\tSpecific requirements: "]
[]
[33,null,"12.1.13\tOffices [6.4.3]\tSpecific requirements: \tThe contractor shall provide, maintain and remove on completion of the works an office for the exclusive use of the principal agent, minimum size 4 x 3 x 3m high internally, suitably insulated and ventilated, provided with electric lighting and fitted with boarded floor, desk, chair, drawing stool, drawing board and lock-up drawers for drawings. The office shall be kept clean and fit for use at all times"]
[]
[33,null,"12.1.14\tMain notice board [6.5]\tSpecific requirements: \tThe contractor shall provide, erect where directed, maintain and remove on completion of the works a notice board size 3 x 3m as type Drawing GEN 063, constructed of suitable boarding with flat smooth surface and with edging bead 19mm thick round outer edges and projecting 12mm from face of boarding and rounded on front edge. The board shall be securely fixed to hoarding, where hoarding is provided, or fixed to and including a suitable supporting structure of timber or tubular posts and braces. The board is to be painted ivory white and the bead and 12mm wide dividing lines dark green. All wording shall be inscribed in dark green as per the coat of arms for SA. All wording shall be inscribed in dark green painted sans serif lettering"]
[]
[33,null,"12.1.15\tSubcontractors' notice board [6.6]\tA notice board is required\t\t\t\t\tYES/NO \tSpecific requirements: "]
[]
[33,null,"12.1.16\tWater [7.2]\tOption A (by contractor)\t\t\t\t\tYES/NO  \tOption B (by employer - free of charge)\t\t\t\tYES/NO  \tOption C (by employer - metered)\t\t\t\tYES/NO"]
[]
[34,null,"12.1.17\tElectricity [7.3]\tOption A (by contractor)\t\t\t\t\tYES/NO  \tOption B (by employer - free of charge)\t\t\t\tYES/NO  \tOption C (by employer - metered)\t\t\t\tYES/NO"]
[]
[34,null,"12.1.18\tTelecommunications [7.4]\tTelephone\t\t\t\t\t\t\tYES/NO  \tFacsimile\t\t\t\t\t\t\tYES/NO  \tE-mail\t\t\t\t\t\t\t\tYES/NO"]
[]
[34,null,"12.1.19\tAblution facilities [7.5]\tOption A (by contractor)\t\t\t\t\tYES/NO  \tOption B (by employer)\t\t\t\t\t\tYES/NO"]
[]
[34,null,"12.1.20\tProtection of existing/sectionally occupied works [11.2]\tProtection is required\t\t\t\t\t\tYES/NO"]
[]
[34,null,"12.1.21\tSpecial attendance [9.2]\tSubcontractor (1) details:   \tSubcontractor (2) details:   \tSubcontractor (3) details:   \tSubcontractor (4) details: "]
[]
[34,null,"12.1.22\tProtection of the works [11.1]\tSpecific requirements: "]
[]
[35,null,"12.1.23\tDisturbance [11.5]\tSpecific requirements: \tThe contractor shall keep the site, structures, etc well watered during operations to prevent dust and shall provide and erect and remove on completion of the works all necessary temporary dust screens all to the satisfaction of the principal agent"]
[]
[35,null,"12.1.24\tEnvironmental disturbance [11.6]\tSpecific requirements: "]
[]
[35,null,"12.2\tPOST-TENDER INFORMATION"]
[]
[35,null,"12.2.1\tPayment of preliminaries [10.2]\tOption A (prorated)\t\t\t\t\t\tYES/NO  \tOption B (calculated)\t\t\t\t\t\tYES/NO"]
[]
[35,null,"12.2.2\tAdjustment of preliminaries [10.3]\tOption A (three categories)\t\t\t\t\tYES/NO  \tOption B (detailed breakdown)\t\t\t\t\tYES/NO"]
[]
[35,null,"12.2.3\tAdditional agreed preliminaries items \tDetails: "]
[]
[35,null,"SECTION C: SPECIFIC PRELIMINARIES","H1"]
[]
[35,null,"Section C contains specific preliminary items which apply to this contract except where N/A (Not Applicable) appears against an item"]
[]
[36,102,"C1.0\tCONTRACT DRAWINGS* Select relevant paragraph and delete whichever is not applicable depending on whether the contract is based on a bills of quantities or lump sum document* The drawings issued with the tender documents do not comprise the complete set but serve as a guide only for tendering purposes and for indicating the scope of the work to enable the tenderer to acquaint himself with the nature and extent of the works and the manner in which they are to be executed* A full set of drawings is issued with the tender documents indicating the full scope of the work to enable the tenderer to acquaint himself with the nature and extent of the works and the manner in which they are to be executed Should any part of the drawings not be clearly understood by the tenderer he shall, before submitting his tender, obtain clarification in writing from the principal agentFixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[36,103,"C2.0\tGENERAL PREAMBLES  The document \"Specification of Materials and Methods to be used (PW371)\" is obtainable on the Department's website (http://www.publicworks.gov.za/ under \"Consultants Guidelines\"), and shall be read in conjunction with the bills of quantities / lump sum document and be referred to for the full descriptions of work to be done and materials to be used  Fixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[37,104,"C3.0\tTRADE NAMESWherever a trade name for any product has been described in the bills of quantities / lump sum document, the tenderer's attention is drawn to the fact that any other product of equal quality may be used subject to the written approval of the principal agent being obtained prior to the closing date for submission of tenders If prior written approval for an alternative product is not obtained, the product described shall be deemed to have been tendered forFixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[37,105,"C4.0\tIMPORTED MATERIALS AND EQUIPMENT  Where imported items are listed in the tender documents, the tenderer shall provide all the information called for, failing which the price of any such item, materials or equipment shall be excluded from currency fluctuations. (refer to Schedule of Imported Materials and Equipment DPW-23(EC) to be completed by tenderer)  Notwithstanding any provisions elsewhere regarding the adjustment of contract prices, the price of any item, material or equipment listed in terms of this clause shall be excluded from the Contract Price Adjustment Provisions (if applicable)  Fixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[37,106,"C5.0\tVIEWING THE SITE IN SECURITY AREAS  The site is situated in a security area and the tenderer must arrange with the unit commander or other responsible officer to obtain permission to enter the site for tendering purposes  Fixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[38,107,"C6.0\tCOMMENCEMENT OF WORKS IN SECURITY AREAS  As the works falls within a security area the contractor must give the unit commander or other responsible officer notice before commencement of the works. Should the contractor fail to make such arrangements, admission to the site may be refused and any additional costs will be for the contractor's account  Fixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[38,108,"C7.0\tENTRANCE PERMITS TO SECURITY AREAS  As the works falls within a security area the contractor shall obtain entrance permits for his personnel and workmen entering the area and shall comply with all regulations and instructions which may be issued from time to time regarding the protection of persons and property under the control of the Defence Force, Police or chief security officer  Fixed: ____________ Value related:____________ Time related:____________","Item"]
[]
[38,109,"C8.0\tSECURITY CHECK OF PERSONNEL  The principal agent may require the contractor to have his personnel and workmen, or a certain number of them, security classified  In the event of the principal agent requesting the removal of a person or persons from the works for security reasons, the contractor shall do so forthwith and shall thereafter ensure that such person or persons are denied access to the works and the site and/or to any document or information relating to the works  Fixed:____________ Value related:_____________ Time related:____________","Item"]
[]
[39,110,"C9.0\tPROHIBITION ON TAKING OF PHOTOGRAPHS  In terms of article 119 of the Defence Act, 44 of 1957, it is prohibited to sketch or to take photographs of any military site or installation or any building or civil works thereon or to be in possession of a camera or other apparatus used for taking of photographs except when authorized thereto by or on behalf of the Minister  The same prohibition is also applicable to all correctional institutions in terms of article 44.1(e) of the Correctional Services Act 8 of 1959  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[39,111,"C1\tHIV/AIDS AWARENESS  It is required of the contractor to thoroughly study the HIV/AIDS Specification (PW 1544) of the Department that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document. Provision for pricing of HIV/AIDS awareness is made under items C10.1 to C10.5 hereafter and it is explicitly pointed out that all requirements of the aforementioned specification are deemed to be priced hereunder, as the said items represent the only method of measurement and no additional items or extras to the contract in this regard shall be entertained  The contractor must take note that compliance with the HIV/AIDS Specification is compulsory. In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of clause A 31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance. The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment","CONT"]
[]
[40,null,"C10.1\tAWARENESS CHAMPION  Selection, appointment, briefing and making available of an Awareness Champion including provision of all relevant services, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[40,null,"C10.2\tAWARENESS WORKSHOPS  Selection and appointment of a competent Service Provider approved by the principal agent, provision of a Service Provider Workshop Plan and a suitable venue, conducting of awareness workshops by means of traditional and/or modern multi-media techniques, including follow-up courses, making available all tuition material and performing assessment procedures, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[40,null,"C10.3\tPOSTERS, BOOKLETS, VIDEOS, ETC.  Provision, displaying, maintaining and replacing when necessary of four plastic laminated posters, booklets and educational videos, etc. for the duration of the construction period, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[40,null,"C10.4\tACCESS TO CONDOMS  Provision and maintenance of condom dispensers fixed in position, including male and female condoms, replenishing male and female condoms on a daily basis as required for the duration of the construction period, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[41,null,"C10.5\tMONITORING  Monitoring HIV/AIDS awareness of workers, providing the principal agent with access to information including making available all reports, thoroughly completed and reflecting the correct information, for the duration of the construction period and close out, all in accordance with the HIV/AIDS Specification  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[41,112,"C11.0\tOCCUPATIONAL HEALTH AND SAFETY ACT  The contractor shall comply with all the requirements set out in the Construction Regulations, 2003 issued under the Occupational Health and Safety Act, 1993 (Act No 85 of 1993)  It is required of the contractor to thoroughly study the Health and Safety Specification that must be read together with and is deemed to be incorporated under this Section of the bills of quantities / lump sum document  The contractor must take note that compliance with the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is compulsory.  In the event of partial or total non-compliance, the principal agent, notwithstanding the provisions of clause A31.0 of Section A or any other clause to the contrary, reserves the right to delay issuing any progress payment certificate until the contractor provides satisfactory proof of compliance.  The contractor shall not be entitled to any compensation of whatsoever nature, including interest, due to such delay of payment  Provision for pricing of the Occupational Health and Safety Act, Construction Regulations and Health and Safety Specification is made under this clause and it is explicitly pointed out that all requirements of the aforementioned are deemed to be priced hereunder and no additional claims in this regard shall be entertained  Fixed:_____________ Value related:____________ Time related:______________","Item"]
[]
[41,113,"\t\t\t*** Page Feed ***","Item",1]
[]
[]
[]
[45,null,"BILL NO. 1","H1"]
[]
[45,null,"ALTERATIONS (PROVISIONAL)","H1"]
[]
[45,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[45,null,"View site","H4"]
[]
[45,null,"Before submitting his tender the contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[45,null,"Explosives","H4"]
[]
[45,null,"No explosives whatsoever may be used for demolition purposes unless otherwise stated"]
[]
[45,null,"General","H4"]
[]
[45,null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants. He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent"]
[]
[45,null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the principal agent"]
[]
[45,null,"Doors, fanlights, fittings, frames, linings, etc which are to be re-used shall be thoroughly overhauled before refixing including taking off, easing and rehanging, cramping up, re-wedging as required and making good cramps, dowels, etc, and easing, oiling, adjusting and repairing ironmongery as necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described. Re-painting or re-varnishing is given separately"]
[]
[46,null,"Prices for taking out of doors, windows, etc shall include for removal of all beads, architraves, ironmongery, etc"]
[]
[46,null,"Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc and making good floor and wall finishes to match existing"]
[]
[46,null,"Making good of finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[]
[46,null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc)"]
[]
[46,null,"Damage to existing finishes","H4"]
[]
[46,null,"The Contractor will be held responsible for all damage, however caused, to existing finishes and fittings etc. and he must make good all damage at his own expense to the approval of the Principal Agent. Breaking down, demolition and alteration activities and tasks, hacking off of existing plaster, etc. is to be executed with care so as to prevent damage to remaining floor and wall surfaces and finishes (where these are to be retained). Tenders will be deemed to include allowance for any necessary protection of existing surfaces and structures as may be necessary to effect the above, as the cost of repairing damage to existing surfaces and structures will be solely for the Contractors account."]
[]
[46,null,"Removal of materials","H4"]
[]
[46,null,"Where removal is included in the heading, sub-heading or item description, prices shall be deemed to include for the necessary costs in removal and appropriate disposal of materials including but not limited to labour, transportation and disposal costs. No further claims in this regard will be entertained."]
[]
[47,null,"Removal of asbestos material ","H4"]
[]
[47,null,"The removal of asbestos shall be carried out strictly by a certified entity, registered in accordance with the Occupational Health and Safety Act and the Asbestos Regulation.  Asbestos in all forms/building elements that is to be removed, shall be carried out in strict accordance with aforementioned regulation, and a certificate issued by the entity as contemplated in the above, shall be provided per block for the removal thereof, where the term block shall in this context refer to any single, free standing building structure, regardless of size or purpose.  Corresponding disposal certificates shall be issued by the facility at which the asbestos is disposed of, with said facility to, prior to the disposal of any asbestos material provide satisfactory proof that the facility is duly registered and fully compliant in terms of the act, to receive the asbestos material.  Under no circumstances is the contractor nor any of his duly authorised representatives to sell and/or give away asbestos material to any member/s of the school community, the community in general or the public at large. Should this be found to be occurring, the contractor will be held responsible contractually and may further be prosecuted criminally.  The cost for complying with the above, and all requirements of regulation as reflected above is to be priced for in the items for removal of asbestos material. No further claims in this regard will therefore be entertained."]
[]
[48,null,"REMOVAL OF EXISTING WORK","H2"]
[]
[48,null,"Breaking up and removing unreinforced concrete","H4"]
[]
[48,1,"Steps","m3",19]
[]
[48,null,"Breaking up and removing unreinforced concrete","H4"]
[]
[48,2,"100mm Thick surface beds","m2",25]
[]
[48,null,"Breaking down and removing brickwork etc","H4"]
[]
[48,3,"One brick walls","m2",110]
[]
[48,null,"Taking out and removing doors, windows, etc., from brickwork","H4"]
[]
[48,4,"Timber single door and steel door frame not exceeding 2,5m² from one brick wall","No",84]
[]
[48,5,"Servicing of existing steel windows with new hinges, latches, etc","No",282]
[]
[49,null,"Note: Tenderers are referred to the aforegoing supplementary preambles within this trade when pricing the following item (removal of asbestos)","H3"]
[]
[49,null,"Taking down and removal of Asbestos by accepted removers","H4"]
[]
[49,null,"TAKING DOWN AND REMOVE ASBESTOS BY ACCEPTED REMOVERS","H2"]
[]
[49,null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc","H4"]
[]
[49,6,"Pitched roof 10,52 x 4.17 x 1,7m high overall of timber truss and purlins, ceilings, asbestos sheet covering, ceilings and cornices, fascia and barge boards, gutters and rain water pipes","No",1]
[]
[49,7,"Ditto, but pitched roof 15,34 x 7.50 x 1,7m high","No",1]
[]
[49,8,"Ditto, but pitched roof 18,77 x 3.71 x 1,7m high","No",1]
[]
[49,9,"Ditto, but pitched roof 29,60 x 7.50 x 1,7m high","No",1]
[]
[49,10,"Ditto, but pitched roof 30,82 x 7.50 x 1,7m high","No",1]
[]
[49,11,"Ditto, but pitched roof 37,12 x 7.50 x 1,7m high","No",1]
[]
[50,null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc","H4"]
[]
[50,12,"Asbestos roof sheeting  on pitch roof 25,60 x 13.8 x 1,7m high overall from steel and timber purlins","No",1]
[]
[50,null,"Taking out and removing ironmongery","H4"]
[]
[50,13,"Pinning boards approximately 2400 x 1200mm high including fixings, etc., and cart off site","No",29]
[]
[50,14,"Chalkboards approximately 4800 x 1200mm high including fixings, etc., and cart off site","No",28]
[]
[50,null,"Taking out/off and removing sundry metalwork","H4"]
[]
[50,15,"Steel single leaf security gate not exceeding 2,5m² ","No",45]
[]
[50,16,"Steel double leaf security gate exceeding 2,5m² and not exceeding 5m²","No",6]
[]
[50,null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc","H4"]
[]
[50,17,"30mm Screed from floors","m2",1567]
[]
[51,18,"Internal plaster from walls and columns","m2",3327]
[]
[51,19,"External plaster from walls and columns","m2",1369]
[]
[51,null,"Taking out/off and removing glass and mirrors","H4"]
[]
[51,20,"Glass from steel windows, including cleaning out rebates and preparing for new glass (new glass elsewhere)","m2",269]
[]
[51,null,"Taking  out and removing piping, including cutting off as necessary, holderbats and making good floor and wall finishes (making good tiling and paintwork elsewhere)","H4"]
[]
[51,21,"PVC piping not exceeding 50mm diameter","m",65]
[]
[51,22,"PVC piping exceeding 100mm and not exceeding 200mm diameter","m",30]
[]
[51,null,"Taking out and removing sanitary fittings, tanks, geysers, etc, including disconnecting from pipes, traps, etc and making good floor and wall finishes (making good tiling and paintwork elsewhere)","H4"]
[]
[51,23,"Vitreous china wash hand basin","No",16]
[]
[52,24,"Vitreous china WC pan with cistern and flush pipe","No",10]
[]
[52,25,"Plastic toilet seat pedestal","No",20]
[]
[52,null,"Taking out and remove electrical redundant conduits, wiring, etc","H4"]
[]
[52,26,"Conduits, wiring, etc. from all existing blocks and dispose","Item","1.00"]
[]
[52,null,"MAKING GOOD OF FINISHES, ETC","H2"]
[]
[52,null,"Cleaning brickwork","H4"]
[]
[52,27,"Acid cleaning internal face brickwork at dado level with high pressure cleaner and leave walls clean, in perfect condition and re-apply two coats of clear gloss face brick sealer","m2",363]
[]
[52,28,"Acid cleaning external face brickwork with high pressure cleaner and leave walls clean, in perfect condition","m2",1210]
[]
[52,null,"Cleaning roof tiles","H4"]
[]
[52,29,"Pressure cleaning of existing tiled roof","m2",1229]
[]
[53,null,"MAKING GOOD OF EXISTING WORKS","H2"]
[]
[53,30,"Remove and replace damaged tiles","m2",22]
[]
[53,31,"Repairs to existing surface beds, including filling in cracks, with concrete crack injection or any other approved filler, stitching as required, etc","m2",30]
[]
[]
[]
[55,null,"BILL NO. 2","H1"]
[]
[55,null,"EARTHWORKS (PROVISIONAL)","H1"]
[]
[55,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[55,null,"EXCAVATIONS, ETC","H3"]
[]
[55,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[55,1,"Thickening under surface beds, etc.","m3",15]
[]
[55,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[55,2,"Soft rock","m3",3]
[]
[55,3,"Hard rock","m3",3]
[]
[55,null,"Risk of collapse of excavations","H4"]
[]
[55,4,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",3]
[]
[56,null,"Compaction of surfaces","H4"]
[]
[56,5,"Compaction of ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",25]
[]
[56,null,"WEED KILLERS, INSECTICIDES, ETC","H2"]
[]
[56,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[56,6,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",25]
[]
[]
[]
[58,null,"BILL NO. 3","H1"]
[]
[58,null,"CONCRETE, FORMWORK AND REINFORCEMENT (PROVISIONAL)","H1"]
[]
[58,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[58,null,"Cost of tests","H4"]
[]
[58,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[58,null,"Formwork","H4"]
[]
[58,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[58,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[59,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[59,null,"30MPa/19mm concrete","H4"]
[]
[59,1,"Surface beds on waterproofing","m3",19]
[]
[59,null,"TEST CUBES","H2"]
[]
[59,2,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",3]
[]
[59,null,"CONCRETE SUNDRIES","H2"]
[]
[59,null,"Finishing top surfaces of concrete smooth with a steel trowel","H4"]
[]
[59,3,"Surface beds, slabs, etc","m2",25]
[]
[59,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[59,null,"Rough formwork to sides","H4"]
[]
[59,4,"Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",8]
[]
[60,null,"REINFORCEMENT","H2"]
[]
[60,null,"Fabric reinforcement","H4"]
[]
[60,5,"Type 193 fabric reinforcement in concrete surface beds etc","m2",25]
[]
[]
[]
[62,null,"BILL NO. 4","H1"]
[]
[62,null,"ROOF COVERINGS (PROVISIONAL) ","H1"]
[]
[62,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[62,null,"Proprietary items or materials","H3"]
[]
[62,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[62,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[62,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)  ","H4"]
[]
[62,1,"Roof covering with pitches not exceeding 25 degrees","m2",1886]
[]
[62,2,"Ridge cappings 475mm girth","m",168]
[]
[63,null,"ROOF AND WALL INSULATION","H2"]
[]
[63,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[63,3,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required ","m2",1792]
[]
[]
[]
[65,null,"BILL NO. 5","H1"]
[]
[65,null,"CARPENTRY AND JOINERY (PROVISIONAL) ","H1"]
[]
[65,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[65,null,"Fixing","H4"]
[]
[65,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[65,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[65,null,"Joinery","H4"]
[]
[65,null,"Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts "]
[]
[65,null,"ROOFS ETC","H2"]
[]
[65,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H3"]
[]
[65,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[65,null,"Trusses are at maximum 1200mm centres"]
[]
[65,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[65,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[65,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[66,1,"Supply and install prefabricated timber roof truss system complete and in accordance with the Standard Building Regulations. Truss spanning 10,48 x 1,70mm high overall with 700mm eaves projection on both sides ","No",96]
[]
[66,2,"Ditto, but spanning 6,16m","No",22]
[]
[66,null,"Sawn softwood","H4"]
[]
[66,3,"38 x 114mm Wall plates","m",277]
[]
[66,4,"50 x 76mm Purlins","m",1793]
[]
[66,5,"38 x 114mm Bracing","m",298]
[]
[66,null,"Sundries","H4"]
[]
[66,6,"Wrought faces on sawn timbers","m2",42]
[]
[66,7,"Two coats creosote on sawn timbers","m2",42]
[]
[67,null,"EAVES, VERGES, ETC","H3"]
[]
[67,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[67,8,"80 x 200mm Angle section barge boards including galvanised steel H-profile jointing strips  and fix with hot dip galvanised screws and washers","m",223]
[]
[67,9,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",579]
[]
[67,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[67,null,"Wrought meranti doors hung to steel frames","H4"]
[]
[67,10,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",52]
[]
[67,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[67,11,"44mm Door 813 x 2032mm high","No",40]
[]
[68,null,"SKIRTINGS","H2"]
[]
[68,null,"Wrought meranti","H4"]
[]
[68,12,"75 x 19mm skirtings including 19mm quadrant plugged ","m",888]
[]
[]
[]
[70,null,"BILL NO. 6","H1"]
[]
[70,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING (PROVISIONAL) ","H1"]
[]
[70,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[70,null,"Fixing","H4"]
[]
[70,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[70,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[70,null,"Ceilings","H4"]
[]
[70,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[70,null,"Proprietary items or materials","H3"]
[]
[70,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[70,null,"NAILED-UP CEILINGS","H3"]
[]
[70,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips","H4"]
[]
[70,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres ","m2",1646]
[]
[71,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",43]
[]
[71,null,"Nucornice foam plastic cornices","H4"]
[]
[71,3,"75mm Coved cornices","m",1029]
[]
[]
[]
[73,null,"BILL NO. 7","H1"]
[]
[73,null,"FLOOR COVERINGS, WALL LININGS, ETC (PROVISIONAL)","H1"]
[]
[73,null,"FLOOR COVERINGS","H2"]
[]
[73,null,"300 x 300 x 2.5mm Semi flexible vinyl tiles","H4"]
[]
[73,1,"On floors ","m2",1457]
[]
[73,null,"POLISH, SEALERS, ETC","H2"]
[]
[73,2,"Three coats wax polish on vinyl flooring","m2",1457]
[]
[]
[]
[74,null,"BILL NO. 8","H1"]
[]
[74,null,"IRONMONGERY  (PROVISIONAL) ","H1"]
[]
[74,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[74,null,"Proprietary items","H4"]
[]
[74,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[74,null,"Finishes to ironmongery","H4"]
[]
[74,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[74,null,"Proprietary items or materials","H3"]
[]
[74,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[75,null,"HINGES, BOLTS, ETC","H2"]
[]
[75,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[75,1,"WC chrome plated indicator bolt ","No",30]
[]
[75,null,"LOCKS","H2"]
[]
[75,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[75,2,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles ","No",52]
[]
[75,null,"SUNDRIES","H2"]
[]
[75,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[75,3,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",82]
[]
[75,null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC","H2"]
[]
[75,null,"Manufactured by \"Vitrex System\"","H4"]
[]
[75,4,"Standard green enamel megnatic chalkboard overall size 4800 x 1140mm high comprising two fixed panels, each 2400 x 1140mm high, with aluminium chalk rail plugged","No",31]
[]
[76,5,"Pinning board size 2400 x 1200mm high plugged","No",33]
[]
[]
[]
[78,null,"BILL NO. 9","H1"]
[]
[78,null,"METALWORK (PROVISIONAL) ","H1"]
[]
[78,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[78,null,"Descriptions of bolts, anchors, etc","H4"]
[]
[78,null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[]
[78,null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete"]
[]
[78,null,"Items described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described "]
[]
[78,null,"Proprietary items or materials","H3"]
[]
[78,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[78,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[78,null,"Welded screens and gates ","H4"]
[]
[78,1,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix to wall and padlock set, etc.","No",52]
[]
[]
[]
[79,null,"BILL NO. 10","H1"]
[]
[79,null,"PLASTERING (PROVISIONAL) ","H1"]
[]
[79,null,"SCREEDS","H2"]
[]
[79,null,"Screeds steel trowelled, on concrete","H4"]
[]
[79,1,"30mm Thick on floors and landings","m2",1522]
[]
[79,null,"INTERNAL PLASTER","H2"]
[]
[79,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[79,2,"On walls","m2",3327]
[]
[79,3,"On narrow widths","m2",149]
[]
[79,null,"EXTERNAL PLASTER","H2"]
[]
[79,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[79,4,"On walls","m2",1369]
[]
[79,5,"On narrow widths","m2",149]
[]
[]
[]
[80,null,"BILL NO. 11","H1"]
[]
[80,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[80,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[80,null,"Wire gratings","H4"]
[]
[80,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[80,null,"Stormwater channels","H4"]
[]
[80,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[80,null,"PVC-U pipes and fittings","H4"]
[]
[80,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[80,null,"Polypropylene pipes","H4"]
[]
[80,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[80,null,"Fixing of pipes","H4"]
[]
[80,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[81,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[81,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[81,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[81,null,"General","H4"]
[]
[81,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[81,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[81,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[81,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[81,null,"As-built drawings","H4"]
[]
[81,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[81,null,"French drains","H4"]
[]
[81,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[82,null,"uPVC pipes and fittings","H4"]
[]
[82,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[82,null,"RAINWATER DISPOSAL","H2"]
[]
[82,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[82,1,"150mm Half-round roof gutters with beaded front edge","m",562]
[]
[82,2,"100mm Diameter rainwater pipes","m",169]
[]
[82,3,"Extra over gutter for stopped end","No",52]
[]
[82,4,"Extra over gutter for outlet for 100mm pipe","No",60]
[]
[82,5,"Extra over rainwater pipe for bend","No",64]
[]
[82,6,"Extra over rainwater pipe for shoe","No",60]
[]
[83,null,"STORMWATER CHANNELS","H2"]
[]
[83,null,"Earthworks","H4"]
[]
[83,7,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",99]
[]
[83,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[83,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[83,8,"\"V\" drains","m3","98.9"]
[]
[83,9,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",761]
[]
[83,10,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",731]
[]
[83,11,"Type 193 fabric reinforcement in concrete surface beds etc","m2",761]
[]
[83,12,"10 x 150mm Pre-compressed bitumen impregnated foam plastic joint sealing strips between brickwork and concrete","m",675]
[]
[84,null,"SOIL DRAINAGE","H2"]
[]
[84,null,"Normal duty (Class 51) PVC-U sewer and drain pipes","H4"]
[]
[84,13,"110mm Pipes vertically or ramped to cleaning eyes etc (no excavation)","m",30]
[]
[84,14,"110mm Pipes laid in and including trenches not exceeding 1m deep","m",190]
[]
[84,null,"Extra over normal duty (Class 51) PVC-U sewer and drain pipes for fittings","H4"]
[]
[84,15,"110mm Bend","No",8]
[]
[84,16,"110mm Tee","No",1]
[]
[84,17,"110mm Access bend","No",7]
[]
[84,18,"110mm Access tee","No",1]
[]
[84,19,"110mm Rodding eye","No",2]
[]
[85,20,"110mm Straight reducer","No",8]
[]
[85,21,"22mm Socket","No",6]
[]
[85,22,"28mm Socket","No",2]
[]
[85,23,"110mm Pan connector","No",8]
[]
[85,24,"110mm PVC tovent iron connector","No",2]
[]
[85,25,"110mm Vent iron cowl","No",2]
[]
[85,null,"SANITARY FITTINGS","H2"]
[]
[85,null,"\"Vaal\" or other equal and approved","H4"]
[]
[85,26,"School type lavatory wash hand basin fixed to wall","No",16]
[]
[85,27,"Low level school type wc suite comprising pan with double flap heavy duty plastic seat and matching 9 litre cistern with flush pipe","No",10]
[]
[86,null,"Jojo","H4"]
[]
[86,28,"Plastic toilet seat pedestal","No",20]
[]
[86,null,"WASTE UNIONS ETC","H2"]
[]
[86,null,"\"Cobra Watertech\" or other equal and approved","H4"]
[]
[86,29,"32mm 301 CP basin waste union","No",16]
[]
[86,null,"TRAPS ETC","H2"]
[]
[86,null,"UPVC","H4"]
[]
[86,30,"110mm Two way vent valve","No",20]
[]
[86,null,"Rubber","H4"]
[]
[86,31,"50mm \"P\" or \"S\" trap","No",16]
[]
[86,null,"TAPS, VALVES, ETC","H2"]
[]
[86,32,"HDPE/UPVC to transition fitting. Underground copper portion to be denzo wrapped (1m underground)","No",24]
[]
[86,33,"22mm CP fullway isolating Valve with handle nickel plated","No",36]
[]
[87,34,"28mm CP fullway isolating Valve with handle nickel plated","No",10]
[]
[87,35,"15mm 111-15CP pillar tap","No",16]
[]
[87,null,"SANITARY PLUMBING","H2"]
[]
[87,null,"uPVC soil and vent pipes","H4"]
[]
[87,36,"50mm Pipes","m",50]
[]
[87,37,"100mm Pipes","m",30]
[]
[87,null,"Extra over uPVC soil and vent pipes for fittings","H4"]
[]
[87,38,"50mm Bend","No",6]
[]
[87,39,"100mm Bend","No",3]
[]
[87,40,"50mm Access bend","No",4]
[]
[88,41,"100mm Inspection eye","No",3]
[]
[88,42,"50mm Tee","No",2]
[]
[88,43,"50mm Access bend","No",18]
[]
[88,44,"100mm to 50mm reducer","No",3]
[]
[88,45,"50mm Tee junction","No",18]
[]
[88,46,"100mm Tee with junction","No",18]
[]
[88,47,"50mm Vent cowl","No",15]
[]
[88,null,"WATER SUPPLIES","H2"]
[]
[88,null,"Class 1 copper pipes with capillary couplings","H4"]
[]
[88,48,"22mm Pipes","m",45]
[]
[89,49,"28mm Pipes","m",30]
[]
[89,50,"32mm Pipes","m",13]
[]
[89,null,"Extra over Class 1 copper pipes for capillary fittings","H4"]
[]
[89,51,"22mm Fittings","No",50]
[]
[89,52,"28mm Fittings","No",15]
[]
[89,53,"32mm Fittings","No",6]
[]
[89,null,"Testing","H4"]
[]
[89,54,"Testing water pipe system","Item","1.00"]
[]
[]
[]
[91,null,"BILL NO. 12","H1"]
[]
[91,null,"ELECTRICAL WORK (PROVISIONAL)","H1"]
[]
[91,null,"MAIN POWER SUPPLY","H2"]
[]
[91,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[91,null,"Distribution boards etc","H4"]
[]
[91,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[91,null,"Switches, socket outlets, etc","H4"]
[]
[91,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[91,null,"Light fittings","H4"]
[]
[91,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[91,null,"MUNICIPAL CONNECTION","H2"]
[]
[91,null,"CONNECTION","H2"]
[]
[91,1,"Provide the sum of R50 000 (Fifty thousand rand) for municipal connection","Item","1.00"]
[]
[91,null,"Main supply section","H4"]
[]
[91,2,"250A 3 pole MCCB (70kA) - (LV431670, LV429388, 29450)","No",1]
[]
[91,3,"Landis+Gyr E650 Electrical Meter (ZMD300AT/CT E650)","No",1]
[]
[92,null,"Distribution supply section","H4"]
[]
[92,4,"iC60N 63A 4P CB (A9F444363)","No",21]
[]
[92,5,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[92,6,"125A gG Fuse (125NHG00B)","No",3]
[]
[92,7,"ELSL-90W-CW Solar light","No",30]
[]
[92,null,"EXISTING BLOCKS","H2"]
[]
[92,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[92,null,"DISTRIBUTION BOARD DB","H3"]
[]
[92,8,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",11]
[]
[92,9,"iC60N 63A 4P CB (A9F44363)","No",11]
[]
[93,10,"iC60N 32A 4P CB (A9F44432)","No",11]
[]
[93,11,"iC60N 16A DP CB (AF74616)","No",66]
[]
[93,12,"3P (N/O) CONTACTOR (LC1E3210U5)","No",11]
[]
[93,13,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",11]
[]
[93,14,"Surge arrester, 3P+N, 350V (A9L20600)","No",11]
[]
[93,null,"CABLES","H3"]
[]
[93,15,"1.5mm² 3-Core","m",2640]
[]
[93,16,"2.5mm² 3-Core","m",830]
[]
[93,17,"16mm² 3-Core","m",660]
[]
[94,null,"Cable joints","H4"]
[]
[94,18,"1.5mm² 3-Core","No",22]
[]
[94,19,"16mm² 3-Core","No",22]
[]
[94,null,"Cable terminations","H4"]
[]
[94,20,"1.5mm² 3-Core","No",440]
[]
[94,21,"2.5mm² 3-Core","No",440]
[]
[94,22,"16mm² 3-Core","No",22]
[]
[94,null,"EARTH CONDUCTORS","H3"]
[]
[94,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[94,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[94,23,"6mm²","m",660]
[]
[95,null,"SUNDRIES","H3"]
[]
[95,24,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",11]
[]
[96,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[96,null,"CONDUITS ETC","H3"]
[]
[96,null,"Rigid PVC conduits","H4"]
[]
[96,25,"20mm Diameter","m",3470]
[]
[96,null,"PVC conduit accessories","H4"]
[]
[96,26,"Round outlet box for 20mm conduit","No",347]
[]
[96,27,"Deep type (concrete type) round outlet box for 20mm conduit","No",347]
[]
[96,28,"Standard draw box for 20mm conduit","No",347]
[]
[96,29,"50 x 100 x 50mm Outlet box","No",347]
[]
[96,30,"100 x 100 x 50mm Outlet box","No",347]
[]
[96,31,"100 x 100 x 50mm Outlet box with blank cover plate","No",347]
[]
[96,null,"CONDUCTORS","H3"]
[]
[97,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[97,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[97,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[97,32,"1.5mm²","m",3190]
[]
[97,null,"DRAW-WIRES","H3"]
[]
[97,33,"Galvanised steel draw-wires drawn into conduit","m",3190]
[]
[97,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[97,34,"Flush mounted bell push button","No",11]
[]
[97,35,"16A Flush mounted one lever one-way switch unit","No",1]
[]
[97,36,"16A Flush mounted two lever one-way switch unit","No",62]
[]
[97,37,"16A Three pin flush mounted socket outlet with switch, single type","No",83]
[]
[98,null,"LUMINAIRES","H3"]
[]
[98,38,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",264]
[]
[98,39,"1kW 100A Inverter Trolley","No",22]
[]
[98,null,"SUNDRIES","H3"]
[]
[98,40,"Earthing of buildings","Item","11.00"]
[]
[98,41,"Provision of as built drawings","Item","11.00"]
[]
[98,42,"Testing and commissioning the complete electrical installation","Item","11.00"]
[]
[]
[]
[100,null,"BILL NO. 13 ","H1"]
[]
[100,null,"GLAZING (PROVISIONAL)","H1"]
[]
[100,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[100,null,"Float glass","H4"]
[]
[100,null,"The term \"float glass\" is used for monolithic annealed glass "]
[]
[100,null,"GLAZING TO STEEL WITH PUTTY","H2"]
[]
[100,null,"4mm Clear float glass","H4"]
[]
[100,1,"Panes exceeding 0,1m² and not exceeding 0,5m²","m2",285]
[]
[100,null,"TOPS, SHELVES, DOORS, MIRRORS, ETC","H2"]
[]
[100,null,"4mm Silvered float glass copper backed mirrors with polished edges, holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H4"]
[]
[100,2,"Mirror 450 x 600mm high with four screws","No",18]
[]
[]
[]
[101,null,"BILL NO. 14","H1"]
[]
[101,null,"PAINTWORK (PROVISIONAL) ","H1"]
[]
[101,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[101,null,"PREPARATORY WORK TO EXISTING WORK","H3"]
[]
[101,null,"Previously painted plastered surfaces","H4"]
[]
[101,null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth"]
[]
[101,null,"Previously painted metal surfaces ","H4"]
[]
[101,null,"Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal"]
[]
[101,null,"Previously painted wood surfaces","H4"]
[]
[101,null,"Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth"]
[]
[101,null,"PAINT SPECIFICATIONS","H3"]
[]
[101,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[101,null,"COLOURS","H3"]
[]
[101,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[102,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[102,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[102,null,"One coat alkali resistant primer and two coats PVA emulsion paint for interior use","H4"]
[]
[102,1,"Walls","m2",3327]
[]
[102,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[102,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[102,2,"Ceilings and cornices","m2",1646]
[]
[102,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[102,null,"Two coats alkali resistant primer and two coats superior quality acrylic paint for interior and exterior use ","H4"]
[]
[102,3,"Fascias and barge boards, including priming metal jointing strips","m2",214]
[]
[102,null,"ON WOOD SURFACES","H2"]
[]
[102,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[102,4,"Laminated beam","m2",22]
[]
[103,5,"Doors","m2",289]
[]
[103,null,"One coat sanding sealer, two coats \"Wooddoc\" clear vanish","H4"]
[]
[103,6,"Skirting, rails, etc not exceeding 300mm girth","m",871]
[]
[103,null,"ON EXTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[103,null,"One coat alkali resistant primer and two coats PVA emulsion paint for exterior use","H4"]
[]
[103,7,"Walls","m2",1369]
[]
[103,null,"PAINTWORK, ETC TO PREVIOUSLY PAINTED WORK","H2"]
[]
[103,null,"ON METAL SURFACES","H2"]
[]
[103,null,"One coat alkyd based zinc phosphate primer and two coats premium quality polyurethane enamel paint, on steel","H4"]
[]
[103,8,"Door frames","m2",93]
[]
[103,9,"Windows","m2",538]
[]
[]
[]
[105,1,"Alterations (Provisional)","Page",54]
[]
[105,2,"Earthworks (Provisional)","Page",57]
[]
[105,3,"Concrete, Formwork and Reinforcement  (Provisional)","Page",61]
[]
[105,4,"Roof Coverings (Provisional)","Page",64]
[]
[105,5,"Carpentry and Joinery (Provisional)","Page",69]
[]
[105,6,"Ceilings, Partitions and Access Flooring (Provisional)","Page",72]
[]
[105,7,"Floor Coverings, Wall Linings, etc. (Provisional)","Page",73]
[]
[105,8,"Ironmongery (Provisional)","Page",77]
[]
[105,9,"Metalwork (Provisional)","Page",78]
[]
[105,10,"Plastering (Provisional)","Page",79]
[]
[105,11,"Plumbing and Drainage (Provisional)","Page",90]
[]
[105,12,"Electrical work (Provisional)","Page",99]
[]
[105,13,"Glazing (Provisional)","Page",100]
[]
[105,14,"Paintwork (Provisional)","Page",104]
[]
[106,null,"BILL NO. 1","H1"]
[]
[106,null,"EARTHWORKS (PROVISIONAL)","H1"]
[]
[106,null,"SITE CLEARANCE ETC","H2"]
[]
[106,null,"Site clearance","H4"]
[]
[106,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",231]
[]
[106,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[106,null,"EXCAVATIONS, ETC","H2"]
[]
[106,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[106,2,"Trenches","m3",21]
[]
[106,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[106,3,"Soft rock","m3",2]
[]
[106,4,"Hard rock","m3",1]
[]
[106,null,"Extra over all excavations for carting away","H4"]
[]
[106,5,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",21]
[]
[106,null,"Risk of collapse of excavations","H4"]
[]
[106,6,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",126]
[]
[106,null,"Keeping excavations free of water","H4"]
[]
[106,7,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[107,null,"FILLING ETC","H2"]
[]
[107,null,"Compaction of surfaces","H4"]
[]
[107,8,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",121]
[]
[107,null,"WEED KILLERS, INSECTICIDES, ETC ","H2"]
[]
[107,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[107,9,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",121]
[]
[]
[]
[109,null,"BILL NO. 2","H1"]
[]
[109,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[109,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[109,null,"Cost of tests","H4"]
[]
[109,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[109,null,"Formwork","H4"]
[]
[109,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[109,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[110,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[110,null,"30MPa/19mm concrete","H4"]
[]
[110,1,"Ground beams","m3",12]
[]
[110,2,"Trenches","m3",4]
[]
[110,3,"Surface beds","m3",24]
[]
[110,4,"Pavings","m3",4]
[]
[110,null,"TEST CUBES","H2"]
[]
[110,5,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",6]
[]
[110,null,"CONCRETE SUNDRIES","H2"]
[]
[110,null,"Finishing top surfaces of concrete smooth with a wood float","H4"]
[]
[110,6,"Surface beds, slabs, etc","m2",22]
[]
[110,null,"Finishing top surfaces of concrete smooth with a power float","H4"]
[]
[110,7,"Surface beds, slabs, etc","m2",171]
[]
[110,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[110,null,"Rough formwork to sides","H4"]
[]
[110,8,"Edges, risers, ends and reveals not exceeding 300mm high","m",813]
[]
[110,null,"MOVEMENT JOINTS ETC","H2"]
[]
[110,null,"Expansion joints with 12mm bitumen impregnated softboard, including raking out polysolphyte sealant ","H4"]
[]
[110,9,"Not exceeding 300mm high through slabs","m",51]
[]
[111,null,"REINFORCEMENT","H2"]
[]
[111,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[111,10,"Bars in various diameter","t","0.87"]
[]
[111,null,"Fabric reinforcement","H4"]
[]
[111,11,"Type 395 fabric reinforcement in concrete surface beds etc","m2",203]
[]
[]
[]
[113,null,"BILL NO. 3","H1"]
[]
[113,null,"MASONRY ","H1"]
[]
[113,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[113,null,"BRICKWORK","H3"]
[]
[113,null,"Sizes in descriptions","H4"]
[]
[113,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[113,null,"BRICKWORK","H2"]
[]
[113,null,"FOUNDATIONS (PROVISIONAL)","H2"]
[]
[113,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[113,1,"Half brick walls","m2",4]
[]
[113,2,"One brick walls","m2",38]
[]
[113,null,"SUPERSTRUCTURE","H2"]
[]
[113,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[113,3,"Half brick walls","m2",36]
[]
[113,4,"One brick walls in beam filling","m2",6]
[]
[113,5,"One brick walls of two half brick skins with inner skin bagged and sealed","m2",154]
[]
[113,null,"BRICKWORK SUNDRIES","H2"]
[]
[113,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[113,6,"75mm Wide reinformcement built in horizontally","m",102]
[]
[114,7,"150mm Wide reinforcement built in horizontally","m",507]
[]
[114,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[114,8,"110 x 75mm Lintels in lengths not exceeding 3m","m",21]
[]
[114,null,"Galvanised wire ties etc","H4"]
[]
[114,9,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",28]
[]
[114,null,"FACE BRICKWORK","H2"]
[]
[114,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[114,10,"Extra over brickwork for face brickwork in foundation (Provisional)","m2",13]
[]
[114,11,"Extra over brickwork for face brickwork","m2",127]
[]
[114,12,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",21]
[]
[114,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[114,13,"230mm Wide sills set sloping and slightly projecting","m",7]
[]
[]
[]
[116,null,"BILL NO. 4","H1"]
[]
[116,null,"WATERPROOFING","H1"]
[]
[116,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[116,null,"One layer 375 micron embossed polyethylene dampproof course (SANS 952-1985 type B)","H4"]
[]
[116,1,"In walls","m2",14]
[]
[116,null,"One layer 375 micron embossed polyethylene waterproofing sheeting (SANS 952-1985 type A) sealed at laps with pvc self adhesive tape","H4"]
[]
[116,2,"Under surface beds","m2",79]
[]
[]
[]
[117,null,"BILL NO. 5","H1"]
[]
[117,null,"ROOF COVERINGS","H1"]
[]
[117,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[117,null,"Proprietary items or materials","H3"]
[]
[117,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[117,null,"ROOF COVERINGS","H2"]
[]
[117,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[117,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)","H4"]
[]
[117,1,"Roof covering with pitches not exceeding 25 degrees","m2",144]
[]
[117,2,"Ridge cappings 475mm girth ","m",16]
[]
[117,3,"Hip cappings 75mm girth","m",28]
[]
[117,null,"ROOF AND WALL INSULATION","H2"]
[]
[117,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[117,4,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required","m2",144]
[]
[]
[]
[118,null,"BILL NO. 6","H1"]
[]
[118,null,"CARPENTRY AND JOINERY","H1"]
[]
[118,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[118,null,"Fixing","H4"]
[]
[118,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[118,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[118,null,"Joinery","H4"]
[]
[118,null,"Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts "]
[]
[118,null,"ROOFS ETC","H2"]
[]
[118,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H3"]
[]
[118,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[118,null,"Trusses are at maximum 1250mm centres"]
[]
[118,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[118,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[119,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[119,1,"Supply and install prefabricated 17,5 degree roof for single story building in accordance with the Standard Building Regulations:  Roof construction to double pitched roof with two hipped ends 15,42 x 7.92m and 1,70m high overall with 700mm eaves projection on all sides including standard full trusses, Hip trusses, jack trusses, etc at a maximum centres of 1250mm including, wall plates, permanent bracing and 50 x 76mm purlins at a maximum centres of 1250mm for IBR roof covering specified above","No",1]
[]
[119,null,"Wrought laminated Saligna","H4"]
[]
[119,2,"297 x 70mm Beam bolted to brick piers","m",21]
[]
[119,null,"Sundries","H4"]
[]
[119,3,"Wrought faces on sawn timbers","m2",5]
[]
[119,4,"Two coats creosote on sawn timbers","m2",5]
[]
[119,null,"EAVES, VERGES, ETC","H3"]
[]
[119,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[119,5,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",51]
[]
[120,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[120,null,"Wrought meranti doors hung to steel frame","H4"]
[]
[120,6,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",2]
[]
[120,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[120,7,"44mm Door 813 x 2032mm high","No",2]
[]
[120,null,"FITTINGS","H2"]
[]
[120,null,"Kitchen cupboards etc with approved hinges, handles and telescopic drawer sliders, including 32mm thick post-formed top with 0,6mm Decon Laminated in Artic Granite or similar","H4"]
[]
[120,8,"L-Shaped Sink kitchen cupboard overall size 7,51 x 0,9m high with top, sides, bottom, division, shelf, back and hinged doors, dividing framework, drawers etc.","No",1]
[]
[120,null,"Kitchen storage shelving","H4"]
[]
[120,9,"Bulk storage shelving overall size 3,72 x 2,00 x 0,40m","No",1]
[]
[120,10,"Vegetable storage shelving overall size 3,72 x 2,00 x 0,40m","No",1]
[]
[120,11,"Equipment storage shelving overall size 3,49 x 2,00 x 0,40m","No",1]
[]
[]
[]
[122,null,"BILL NO. 7","H1"]
[]
[122,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING ","H1"]
[]
[122,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[122,null,"Fixing","H4"]
[]
[122,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[122,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[122,null,"Ceilings","H4"]
[]
[122,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[122,null,"Proprietary items or materials","H3"]
[]
[122,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[122,null,"NAILED-UP CEILINGS","H2"]
[]
[122,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips ","H4"]
[]
[122,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres","m2",96]
[]
[122,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",4]
[]
[123,null,"Gypsum plasterboard cornices","H4"]
[]
[123,3,"75mm Coved cornices","m",105]
[]
[]
[]
[125,null,"BILL NO. 8","H1"]
[]
[125,null,"IRONMONGERY ","H1"]
[]
[125,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[125,null,"Proprietary items","H4"]
[]
[125,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[125,null,"Finishes to ironmongery","H4"]
[]
[125,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[126,null,"Proprietary items or materials","H3"]
[]
[126,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[126,null,"LOCKS","H2"]
[]
[126,null,"Manufactured by \"Union\"","H4"]
[]
[126,1,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles","No",9]
[]
[126,null,"LETTERS, NAMEPLATES, ETC","H2"]
[]
[126,null,"Manufactured by \"Union\" or other equal and approved","H4"]
[]
[126,2,"150 x 150mm Anodised aluminium plate with toilet symbol ","No",1]
[]
[126,null,"SUNDRIES","H2"]
[]
[126,null,"Manufactured by \"Union\"","H4"]
[]
[126,3,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",9]
[]
[126,null,"BATHROOM FITTINGS","H2"]
[]
[126,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[126,4,"Toilet roll holder, plugged","No",1]
[]
[]
[]
[128,null,"BILL NO. 9","H1"]
[]
[128,null,"METALWORK","H1"]
[]
[128,null,"GALVANISED STEEL HANDRAILS","H2"]
[]
[128,null,"Welded handrails to stair ","H4"]
[]
[128,1,"50 x 50 x 3mm Hollow section continuous rails","No",8]
[]
[128,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[128,null,"Welded screens and gates ","H4"]
[]
[128,2,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock set","No",7]
[]
[128,null,"GALVANISED STEEL WINDOWS, DOORS, ETC","H2"]
[]
[128,null,"Standard school windows with flat burglar bars to opening sashes","H4"]
[]
[128,3,"Window type 1, size 890 x 1250mm high","No",3]
[]
[128,4,"Ditto, but type 4, size 1022 x 654mm high","No",1]
[]
[128,5,"Ditto, but type 5, size 859 x 457mm high","No",2]
[]
[128,null,"STEEL ROLLER SHUTTERS ETC","H2"]
[]
[128,null,"Galvanised steel roller shutters fixed to brickwork or concrete","H4"]
[]
[128,6,"Manual push-up slatted roller shutters for 2500 x 1300mm high opening ","No",1]
[]
[128,7,"Ditto, but for 2500 x 2800mm high opening ","No",1]
[]
[129,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[129,null,"Double rebated frames suitable for half brick walls","H4"]
[]
[129,8,"Frame for door 813 x 2032mm high","No",2]
[]
[129,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[129,9,"Frame for door 813 x 2032mm high","No",7]
[]
[129,null,"GALVANISED STEEL MINOR WORK","H2"]
[]
[129,null,"Galvanised steel post, including fixing accessories to laminated timber beam and concrete floors ","H4"]
[]
[129,10,"100mm Diameter x 2650mm high galvanised mild steel support post including base plates etc. with timber beam over to support roof above (Timber beam elsewhere)","No",8]
[]
[]
[]
[131,null,"BILL NO. 10","H1"]
[]
[131,null,"PLASTERING","H1"]
[]
[131,null,"GRANOLITHIC","H2"]
[]
[131,null,"Untinted granolithic, on concrete","H4"]
[]
[131,1,"30mm Thick on floors and landings","m2",64]
[]
[131,2,"Skirting 80mm high","m",56]
[]
[131,null,"INTERNAL PLASTER","H2"]
[]
[131,null,"Cement plaster wood floated for tiles, on brickwork","H4"]
[]
[131,3,"On walls","m2",26]
[]
[131,null,"Cement plaster wood floated on brickwork","H4"]
[]
[131,4,"On walls","m2",219]
[]
[131,5,"On narrow widths","m2",5]
[]
[]
[]
[132,null,"BILL NO. 11","H1"]
[]
[132,null,"TILING","H1"]
[]
[132,null,"WALL TILING","H2"]
[]
[132,null,"200 x 200 x 5mm White glazed ceramic tiles on brickwork including cement plaster backing (PC sum R160/m² for supply and delivery)","H4"]
[]
[132,1,"On walls","m2",26]
[]
[132,null,"FLOOR TILING","H2"]
[]
[132,null,"200 x 200 x 8mm White matt ceramic tiles on 22mm bedding on concrete flush pointed with epoxy grout (PC sum R160/m² for supply and delivery)","H4"]
[]
[132,2,"On floors and landings","m2",29]
[]
[132,3,"70mm High cut tile skirting ","m",38]
[]
[]
[]
[133,null,"BILL NO. 12","H1"]
[]
[133,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[133,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[133,null,"Wire gratings","H4"]
[]
[133,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[133,null,"Stormwater channels","H4"]
[]
[133,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[133,null,"PVC-U pipes and fittings","H4"]
[]
[133,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[133,null,"Polypropylene pipes","H4"]
[]
[133,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[134,null,"Fixing of pipes","H4"]
[]
[134,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[134,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[134,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[134,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[134,null,"General","H4"]
[]
[134,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[134,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[134,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[134,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[135,null,"As-built drawings","H4"]
[]
[135,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[135,null,"French drains","H4"]
[]
[135,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[135,null,"uPVC pipes and fittings","H4"]
[]
[135,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[135,null,"RAINWATER DISPOSAL","H2"]
[]
[135,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[135,1,"150mm Half-round roof gutters with beaded front edge","m",51]
[]
[135,2,"100mm Diameter rainwater pipes","m",8]
[]
[135,3,"Extra over gutter for angle","No",3]
[]
[135,4,"Extra over gutter for outlet for 100mm pipe","No",2]
[]
[135,5,"Extra over rainwater pipe for bend","No",4]
[]
[136,null,"STORMWATER CHANNELS","H2"]
[]
[136,null,"Earthworks","H4"]
[]
[136,6,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",7]
[]
[136,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[136,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[136,7,"\"V\" drains","m3",7]
[]
[136,8,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",51]
[]
[136,9,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",55]
[]
[136,10,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",51]
[]
[136,11,"10 x 150mm Pre-compressed bitumen impregnated foam plastic joint sealing strips between brickwork and concrete","m",47]
[]
[136,null,"SOIL DRAINAGE","H2"]
[]
[136,null,"Normal duty (Class 51) PVC-U sewer and drain pipes","H4"]
[]
[136,12,"110mm Pipes vertically or ramped to cleaning eyes etc (no excavation)","m",3]
[]
[136,13,"110mm Pipes laid in and including trenches not exceeding 1m deep","m",15]
[]
[136,null,"Extra over normal duty (Class 51) PVC-U sewer and drain pipes for fittings","H4"]
[]
[136,14,"110mm Bend","No",5]
[]
[136,15,"110mm Tee","No",10]
[]
[136,16,"110mm Access bend","No",10]
[]
[137,17,"110mm Access tee","No",20]
[]
[137,18,"110mm Rodding eye","No",5]
[]
[137,19,"28mm Reducer","No",3]
[]
[137,20,"110mm Straight reducer","No",10]
[]
[137,21,"22mm Socket","No",15]
[]
[137,22,"28mm Socket","No",2]
[]
[137,23,"110mm Pan connector","No",5]
[]
[137,24,"110mm PVC tovent iron connector","No",3]
[]
[137,25,"110mm Vent iron cowl","No",2]
[]
[137,null,"SANITARY FITTINGS","H2"]
[]
[137,null,"\"Vaal\" or other equal and approved","H4"]
[]
[137,26,"1200 x 535mm Single centre bowl sink","No",2]
[]
[137,null,"WASTE UNIONS ETC","H2"]
[]
[137,null,"\"Cobra Watertech\" or other equal and approved","H4"]
[]
[137,27,"32mm 301 CP waste union","No",2]
[]
[137,null,"TRAPS ETC","H2"]
[]
[137,null,"Rubber","H4"]
[]
[137,28,"50mm \"P\" or \"S\" trap","No",2]
[]
[137,null,"TAPS, VALVES, ETC","H2"]
[]
[137,29,"PA3.522 \"Masterflo\" pressure control valve with vacuum breaker","No",2]
[]
[137,30,"FJ100CP \"Flushmaster Junior\" urinal flush valve","No",2]
[]
[137,31,"HDPE/UPVC to transition fitting. Underground copper portion to be denzo wrapped (1m underground)","No",1]
[]
[138,32,"22mm CP fullway isolating Valve with handle nickel plated","No",4]
[]
[138,33,"28mm CP fullway isolating Valve with handle nickel plated","No",2]
[]
[138,34,"PA3.132 \"Masterflo\" pressure control valve with vacuum breaker","No",1]
[]
[138,35,"FJ2100CP Cobra Flushmaster Junior flush valve","No",1]
[]
[138,36,"15mm 111-15CP pillar tap","No",4]
[]
[138,null,"SANITARY PLUMBING","H2"]
[]
[138,null,"uPVC soil and vent pipes","H4"]
[]
[138,37,"50mm Pipes","m",15]
[]
[138,null,"Extra over uPVC soil and vent pipes for fittings","H4"]
[]
[138,38,"50mm Bend","No",9]
[]
[138,39,"50mm Access bend","No",18]
[]
[138,40,"50mm Tee","No",14]
[]
[138,41,"50mm Tee junction","No",18]
[]
[138,42,"50mm Vent cowl","No",15]
[]
[138,null,"WATER SUPPLIES","H2"]
[]
[138,null,"Class 1 copper pipes with capillary couplings","H4"]
[]
[138,43,"22mm Pipes","m",35]
[]
[138,44,"28mm Pipes","m",45]
[]
[138,45,"32mm Pipes","m",30]
[]
[138,null,"Extra over Class 1 copper pipes for capillary fittings","H4"]
[]
[138,46,"22mm Fittings","No",25]
[]
[138,47,"28mm Fittings","No",10]
[]
[139,48,"32mm Fittings","No",25]
[]
[139,null,"Testing","H4"]
[]
[139,49,"Testing water pipe system","Item","1.00"]
[]
[139,null,"ELECTRIC WATER HEATERS","H2"]
[]
[139,null,"Kwikot","H4"]
[]
[139,50,"100 Litre \"Megaflo\" floor or wall electric water heater","No",1]
[]
[139,null,"DRIP TRAYS, TANKS, ETC","H2"]
[]
[139,51,"1200 x 900mm Drip tray for water heater, with 100mm high upstand all round with top edge bent over and with 50mm threaded outlet union","No",1]
[]
[139,null,"FIRE APPLIANCES ETC","H2"]
[]
[139,52,"\"Chubb\" hose reel with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket","No",1]
[]
[139,53,"4,5kg Dry chemical powder fire extinguisher","No",1]
[]
[139,54,"80 x 165mm Brass double booster pump connection and \"Y\" piece with cap and chain ","No",1]
[]
[139,null,"Fire hydrant pedestals","H4"]
[]
[139,55,"Unreinforced concrete hydrant pedestal 900mm high, cast around vertical pipe with bottom 300mm below ground, 300 x 300mm square at base and tapering to 200 x 200mm overall octagonal shaped top, including excavation, formwork and two coats of paint to exposed surfaces","No",1]
[]
[140,null,"WATER SUPPLIES TO FIRE APPLIANCES","H2"]
[]
[140,null,"Sans 2-1/2 class medium steel piping black/galvanised","H4"]
[]
[140,56,"50 NB screwed","m",5]
[]
[140,57,"50 NB screwed union","No",4]
[]
[140,58,"50 NB screwed nipple","No",4]
[]
[140,59,"50 NB galvanised SANS62 medium elbow","No",4]
[]
[140,60,"50 NB welded or screwed spcket","No",5]
[]
[140,61,"100 NB Galvanised screw type reducing tee","No",5]
[]
[140,62,"Painting and labelling of all 50NB  screwed fire pipework (25NB) as per SANS 10252 and SANS10140","m",5]
[]
[140,null,"PHOTOLUMINESCENT SIGNS","H2"]
[]
[140,63,"150 x 150mm Sign","No",1]
[]
[140,64,"Provision of fire plan in laminated A3 size","No",1]
[]
[140,65,"Emergency assembly point sign with steel pole and mass concrete base","No",1]
[]
[]
[]
[142,null,"BILL NO. 13","H1"]
[]
[142,null,"ELECTRICAL WORK","H1"]
[]
[142,null,"BLOCK M","H2"]
[]
[142,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[142,null,"Distribution boards etc","H4"]
[]
[142,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[142,null,"Switches, socket outlets, etc","H4"]
[]
[142,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[142,null,"Light fittings","H4"]
[]
[142,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[142,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[142,null,"DISTRIBUTION BOARD DB","H3"]
[]
[142,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[142,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[142,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[142,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[143,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[143,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[143,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[143,null,"CABLES","H3"]
[]
[143,8,"1.5mm² 3-Core","m",240]
[]
[143,9,"2.5mm² 3-Core","m",180]
[]
[143,10,"16mm² 3-Core","m",60]
[]
[143,null,"Cable joints","H4"]
[]
[143,11,"1.5mm² 3-Core","No",2]
[]
[143,12,"16mm² 3-Core","No",2]
[]
[143,null,"Cable terminations","H4"]
[]
[143,13,"1.5mm² 3-Core","No",40]
[]
[143,14,"2.5mm² 3-Core","No",40]
[]
[143,15,"16mm² 3-Core","No",2]
[]
[143,null,"EARTH CONDUCTORS","H3"]
[]
[143,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[143,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[143,16,"6mm²","m",60]
[]
[143,null,"SUNDRIES","H3"]
[]
[143,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[144,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[144,null,"CONDUITS ETC","H3"]
[]
[144,null,"Rigid PVC conduits","H4"]
[]
[144,18,"20mm Diameter","m",420]
[]
[144,null,"PVC conduit accessories","H4"]
[]
[144,19,"Round outlet box for 20mm conduit","No",42]
[]
[144,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",42]
[]
[144,21,"Standard draw box for 20mm conduit","No",42]
[]
[144,22,"50 x 100 x 50mm Outlet box","No",42]
[]
[144,23,"100 x 100 x 50mm Outlet box","No",42]
[]
[144,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",42]
[]
[144,null,"CONDUCTORS","H3"]
[]
[144,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[144,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[144,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[144,25,"1.5mm²","m",290]
[]
[144,null,"DRAW-WIRES","H3"]
[]
[144,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[144,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[144,27,"Flush mounted bell push button","No",1]
[]
[144,28,"16A Flush mounted two lever one-way switch unit","No",9]
[]
[145,29,"16A Three pin flush mounted socket outlet with switch, single type","No",18]
[]
[145,null,"LUMINAIRES","H3"]
[]
[145,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",24]
[]
[145,31,"1kW 100A Inverter Trolley","No",2]
[]
[145,null,"SUNDRIES","H3"]
[]
[145,32,"Earthing of buildings","Item","1.00"]
[]
[145,33,"Provision of as built drawings","Item","1.00"]
[]
[145,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[147,null,"BILL NO. 14 ","H1"]
[]
[147,null,"GLAZING","H1"]
[]
[147,null,"GLAZING TO STEEL WITH PUTTY","H2"]
[]
[147,null,"4mm Clear float glass","H4"]
[]
[147,1,"Panes exceeding 0,1m² and not exceeding 0,5m²","m2",4]
[]
[147,null,"TOPS, SHELVES, DOORS, MIRRORS, ETC","H2"]
[]
[147,null,"4mm Silvered float glass copper backed mirrors with polished edges, holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H4"]
[]
[147,2,"Mirror 450 x 600mm high with four screws","No",1]
[]
[]
[]
[148,null,"BILL NO. 15","H1"]
[]
[148,null,"PAINTWORK","H1"]
[]
[148,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[148,null,"PAINT SPECIFICATIONS","H3"]
[]
[148,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[148,null,"COLOURS","H3"]
[]
[148,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[148,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[148,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[148,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior use","H4"]
[]
[148,1,"Walls","m2",223]
[]
[148,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[148,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[148,2,"Ceilings and cornices","m2",96]
[]
[149,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[149,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[149,3,"Fascias and barge boards, including priming metal jointing strips","m2",24]
[]
[149,null,"ON WOOD SURFACES","H2"]
[]
[149,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[149,4,"Doors","m2",33]
[]
[149,null,"ON METAL SURFACES","H2"]
[]
[149,null,"One coat alkyd based zinc phosphate primer and two coats premium quality polyurethane enamel paint, on steel","H4"]
[]
[149,5,"Door frame","m2",26]
[]
[149,6,"Windows","m2",10]
[]
[]
[]
[151,1,"Earthworks (Provisional)","Page",108]
[]
[151,2,"Concrete, Formwork and Reinforcement","Page",112]
[]
[151,3,"Masonry","Page",115]
[]
[151,4,"Waterproofing","Page",116]
[]
[151,5,"Roof Coverings","Page",117]
[]
[151,6,"Carpentry and Joinery","Page",121]
[]
[151,7,"Ceilings, Partitions and Access Flooring","Page",124]
[]
[151,8,"Ironmongery","Page",127]
[]
[151,9,"Metalwork","Page",130]
[]
[151,10,"Plastering","Page",131]
[]
[151,11,"Tiling","Page",132]
[]
[151,12,"Plumbing and Drainage (Provisional)","Page",141]
[]
[151,13,"Electrical work","Page",146]
[]
[151,14,"Glazing","Page",147]
[]
[151,15,"Paintwork","Page",150]
[]
[152,null,"BILL NO. 1","H1"]
[]
[152,null,"EARTHWORKS","H1"]
[]
[152,null,"SITE CLEARANCE ETC","H2"]
[]
[152,null,"Site clearance","H4"]
[]
[152,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",81]
[]
[152,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[152,null,"EXCAVATIONS, ETC","H2"]
[]
[152,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[152,2,"Latrine pit","m3",93]
[]
[152,3,"Trenches","m3",8]
[]
[152,4,"Holes","m3",2]
[]
[152,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[152,5,"Soft rock","m3",10]
[]
[152,6,"Hard rock","m3",5]
[]
[152,null,"Extra over all excavations for carting away","H4"]
[]
[152,7,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",92]
[]
[152,null,"Risk of collapse of excavations","H4"]
[]
[152,8,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",17]
[]
[153,9,"Sides of trench and hole excavations exceeding 1,5m deep","m2",50]
[]
[153,null,"Keeping excavations free of water","H4"]
[]
[153,10,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[153,null,"FILLING ETC","H2"]
[]
[153,null,"Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 98% Mod AASHTO density","H4"]
[]
[153,11,"Backfilling  behind retaining walls","m3",8]
[]
[153,null,"Compaction of surfaces","H4"]
[]
[153,12,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",55]
[]
[153,null,"WEED KILLERS, INSECTICIDES, ETC ","H2"]
[]
[153,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[153,13,"To bottoms and sides of trenches etc","m2",80]
[]
[]
[]
[155,null,"BILL NO. 2","H1"]
[]
[155,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[155,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[155,null,"Cost of tests","H4"]
[]
[155,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[155,null,"Formwork","H4"]
[]
[155,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[155,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[156,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[156,null,"30MPa/19mm concrete","H4"]
[]
[156,1,"Strip footings","m3",8]
[]
[156,2,"Surface beds","m3",5]
[]
[156,3,"Pavings","m3",4]
[]
[156,4,"Slabs including beams and inverted beams","m3",6]
[]
[156,null,"TEST CUBES","H2"]
[]
[156,5,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",3]
[]
[156,null,"CONCRETE SUNDRIES","H2"]
[]
[156,null,"Finishing top surfaces of concrete smooth with a steel trowel","H4"]
[]
[156,6,"Surface beds, slabs, etc","m2",36]
[]
[156,null,"PERMANENT FORMWORK ","H2"]
[]
[156,null,"1,2mm Galvanised steel permanent decking system to soffits ","H4"]
[]
[156,7,"Decking to slabs with ends laid on brick walls","m2",34]
[]
[156,null,"REINFORCEMENT","H2"]
[]
[156,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[156,8,"Bars in various diameter","t","1.20"]
[]
[156,null,"Fabric reinforcement","H4"]
[]
[156,9,"Type 395 fabric reinforcement in concrete surface beds etc","m2",31]
[]
[]
[]
[158,null,"BILL NO. 3","H1"]
[]
[158,null,"MASONRY ","H1"]
[]
[158,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[158,null,"BRICKWORK","H3"]
[]
[158,null,"Sizes in descriptions","H4"]
[]
[158,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[158,null,"BRICKWORK","H2"]
[]
[158,null,"FOUNDATIONS (PROVISIONAL)","H2"]
[]
[158,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[158,1,"Piers","m3","0.2"]
[]
[158,2,"One brick walls","m2",5]
[]
[158,null,"SUPERSTRUCTURE","H2"]
[]
[158,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[158,3,"Piers","m3",1]
[]
[158,4,"Half brick walls","m2",49]
[]
[158,5,"Half brick walls in beam filling","m2",3]
[]
[158,6,"One brick walls in two half brick skins with inner skin bagged and sealed","m2",158]
[]
[159,null,"BRICKWORK SUNDRIES","H2"]
[]
[159,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[159,7,"75mm Wide reinformcement built in horizontally","m",364]
[]
[159,8,"150mm Wide reinforcement built in horizontally","m",632]
[]
[159,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[159,9,"110 x 75mm Lintels in lengths not exceeding 3m","m",5]
[]
[159,null,"Galvanised wire ties etc","H4"]
[]
[159,10,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",18]
[]
[159,null,"FACE BRICKWORK","H2"]
[]
[159,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[159,11,"Extra over brickwork for face brickwork","m2",132]
[]
[159,12,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",54]
[]
[159,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[159,13,"230mm Wide sills set sloping and slightly projecting","m",5]
[]
[159,null,"DECORATIVE SCREEN WALLS AND GRILLES","H2"]
[]
[159,14,"190 x 190 x 190mm \"LG Green\" or other equal approved grille blocks with bird proof mesh built in","m2",3]
[]
[]
[]
[161,null,"BILL NO. 4","H1"]
[]
[161,null,"WATERPROOFING","H1"]
[]
[161,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[161,null,"One layer 375 micron embossed polyethylene waterproofing sheeting (SANS 952-1985 type A) sealed at laps with pvc self adhesive tape","H4"]
[]
[161,1,"Under surface beds","m2",36]
[]
[161,null,"Two coats bitumen emulsion waterproof coating","H4"]
[]
[161,2,"On bagged brick walls","m2",44]
[]
[]
[]
[162,null,"BILL NO. 5","H1"]
[]
[162,null,"ROOF COVERINGS","H1"]
[]
[162,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[162,null,"Proprietary items or materials","H3"]
[]
[162,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[162,null,"ROOF COVERINGS","H2"]
[]
[162,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[162,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)","H4"]
[]
[162,1,"Roof covering with pitches not exceeding 25 degrees","m2",74]
[]
[162,2,"Ridge cappings 475mm girth ","m",10]
[]
[162,null,"ROOF AND WALL INSULATION","H2"]
[]
[162,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[162,3,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required","m2",74]
[]
[]
[]
[163,null,"BILL NO. 6","H1"]
[]
[163,null,"CARPENTRY AND JOINERY","H1"]
[]
[163,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[163,null,"Fixing","H4"]
[]
[163,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[163,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[163,null,"ROOFS ETC","H2"]
[]
[163,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H2"]
[]
[163,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[163,null,"Trusses are at maximum 1250mm centres"]
[]
[163,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[163,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[163,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[163,1,"Supply and install prefabricated roof truss system complete and in accordance with the Standard Building Regulations. Truss spanning 4.86 x 1.7m high overall with 700mm eaves projection on both sides","No",9]
[]
[164,null,"Sawn softwood","H4"]
[]
[164,2,"38 x 114mm Wall plate","m",20]
[]
[164,3,"50 x 76mm Purlins","m",80]
[]
[164,4,"38 x 114mm Bracing","m",20]
[]
[164,null,"Sundries","H4"]
[]
[164,5,"Wrought faces on sawn timbers","m2",3]
[]
[164,6,"Two coats creosote on sawn timbers ","m2",3]
[]
[164,null,"EAVES, VERGES, ETC","H2"]
[]
[164,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[164,7,"80 x 200mm Angle section barge boards including galvanised steel H-profile jointing strips  and fix with hot dip galvanised screws and washers","m",14]
[]
[164,8,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",20]
[]
[164,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[164,null,"Wrought meranti doors hung to timber frames","H4"]
[]
[164,9,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",3]
[]
[164,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[164,10,"44mm Door 813 x 2032mm high","No",8]
[]
[]
[]
[166,null,"BILL NO. 7","H1"]
[]
[166,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING ","H1"]
[]
[166,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[166,null,"Fixing","H4"]
[]
[166,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[166,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[166,null,"Ceilings","H4"]
[]
[166,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[166,null,"Proprietary items or materials","H3"]
[]
[166,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[166,null,"NAILED-UP CEILINGS","H2"]
[]
[166,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips ","H4"]
[]
[166,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres","m2",29]
[]
[166,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",2]
[]
[167,null,"Gypsum plasterboard cornices","H4"]
[]
[167,3,"75mm Coved cornices","m",72]
[]
[]
[]
[169,null,"BILL NO. 8","H1"]
[]
[169,null,"IRONMONGERY ","H1"]
[]
[169,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[169,null,"Proprietary items","H4"]
[]
[169,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[169,null,"Finishes to ironmongery","H4"]
[]
[169,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[170,null,"Proprietary items or materials","H3"]
[]
[170,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[170,null,"HINGES, BOLTS, ETC","H2"]
[]
[170,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[170,1,"100mm Aluminium butt hinge ","No",22]
[]
[170,2,"WC chrome plated indicator bolt ","No",8]
[]
[170,null,"LOCKS","H2"]
[]
[170,null,"Manufactured by \"Union\"","H4"]
[]
[170,3,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles","No",3]
[]
[170,null,"LETTERS, NAMEPLATES, ETC","H2"]
[]
[170,null,"Manufactured by \"Union\" or other equal and approved","H4"]
[]
[170,4,"150 x 150mm Anodised aluminium plate with female symbol ","No",1]
[]
[170,null,"SUNDRIES","H2"]
[]
[170,null,"Manufactured by \"Union\"","H4"]
[]
[170,5,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",11]
[]
[170,null,"BATHROOM FITTINGS","H2"]
[]
[170,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[170,6,"Toilet roll holder, plugged","No",9]
[]
[]
[]
[172,null,"BILL NO. 9","H1"]
[]
[172,null,"METALWORK","H1"]
[]
[172,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[172,null,"Welded screens and gates ","H4"]
[]
[172,1,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock set","No",2]
[]
[172,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[172,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[172,2,"Frame for door 813 x 2032mm high","No",3]
[]
[172,null,"Double rebated frames suitable for half brick walls","H4"]
[]
[172,3,"Frame for door 813 x 2032mm high","No",8]
[]
[]
[]
[173,null,"BILL NO. 10","H1"]
[]
[173,null,"PLASTERING","H1"]
[]
[173,null,"SCREEDS","H2"]
[]
[173,null,"Screeds steel trowelled, on concrete","H4"]
[]
[173,1,"30mm Thick on floors and landings","m2",29]
[]
[173,null,"INTERNAL PLASTER","H2"]
[]
[173,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[173,2,"On walls","m2",158]
[]
[173,3,"On narrow widths","m2",7]
[]
[173,null,"EXTERNAL PLASTER","H2"]
[]
[173,null,"Cement plaster wood floated, on brickwork","H4"]
[]
[173,4,"On walls","m2",38]
[]
[173,5,"On narrow widths","m2",2]
[]
[]
[]
[174,null,"BILL NO. 11","H1"]
[]
[174,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[174,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[174,null,"Wire gratings","H4"]
[]
[174,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[174,null,"Stormwater channels","H4"]
[]
[174,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[174,null,"PVC-U pipes and fittings","H4"]
[]
[174,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[174,null,"Polypropylene pipes","H4"]
[]
[174,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[175,null,"Fixing of pipes","H4"]
[]
[175,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[175,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[175,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[175,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[175,null,"General","H4"]
[]
[175,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[175,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[175,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[175,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[176,null,"As-built drawings","H4"]
[]
[176,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[176,null,"French drains","H4"]
[]
[176,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[176,null,"uPVC pipes and fittings","H4"]
[]
[176,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[176,null,"RAINWATER DISPOSAL","H2"]
[]
[176,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[176,1,"150mm Half-round roof gutters with beaded front edge","m",16]
[]
[176,2,"100mm Diameter rainwater pipes","m",10]
[]
[176,3,"Extra over gutter for stopped end","m",4]
[]
[176,4,"Extra over gutter for outlet for 100mm pipe","No",2]
[]
[176,5,"Extra over rainwater pipe for bend","No",3]
[]
[177,null,"STORMWATER CHANNELS","H2"]
[]
[177,null,"Earthworks","H4"]
[]
[177,6,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",4]
[]
[177,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[177,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[177,7,"\"V\" drains","m3",4]
[]
[177,8,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",29]
[]
[177,9,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",33]
[]
[177,10,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",29]
[]
[177,11,"10 x 150mm Pre-compressed bitumen impregnated foam plastic joint sealing strips between brickwork and concrete","m",25]
[]
[177,null,"SOIL DRAINAGE","H2"]
[]
[177,null,"Normal duty (Class 51) PVC-U sewer and drain pipes","H4"]
[]
[177,12,"110mm Pipes vertically or ramped to cleaning eyes etc (no excavation)","m",8]
[]
[177,13,"110mm Pipes laid in and including trenches not exceeding 1m deep","m",29]
[]
[177,null,"Extra over normal duty (Class 51) PVC-U sewer and drain pipes for fittings","H4"]
[]
[177,14,"110mm Bend","No",8]
[]
[177,15,"110mm Tee","No",1]
[]
[177,16,"110mm Access bend","No",7]
[]
[178,17,"110mm Access tee","No",1]
[]
[178,18,"110mm Rodding eye","No",2]
[]
[178,19,"110mm Straight reducer","No",8]
[]
[178,20,"22mm Socket","No",6]
[]
[178,21,"28mm Socket","No",2]
[]
[178,22,"110mm Pan connector","No",8]
[]
[178,23,"110mm PVC tovent iron connector","No",2]
[]
[178,24,"110mm Vent iron cowl","No",2]
[]
[178,null,"SANITARY FITTINGS","H2"]
[]
[178,null,"\"Vaal\" or other equal and approved","H4"]
[]
[178,25,"School type lavatory wash hand basin fixed to wall","No",5]
[]
[178,26,"Low level wc suite comprising pan with double flap heavy duty plastic seat and matching 9 litre cistern with flush pipe","No",8]
[]
[178,null,"WASTE UNIONS ETC","H2"]
[]
[178,null,"\"Cobra Watertech\" or other equal and approved","H4"]
[]
[178,27,"32mm 301 CP basin waste union","No",5]
[]
[178,null,"TRAPS ETC","H2"]
[]
[178,null,"UPVC","H4"]
[]
[178,28,"110mm Two way vent valve","No",8]
[]
[178,null,"Rubber","H4"]
[]
[178,29,"50mm \"P\" or \"S\" trap","No",5]
[]
[178,null,"TAPS, VALVES, ETC","H2"]
[]
[178,30,"HDPE/UPVC to transition fitting. Underground copper portion to be denzo wrapped (1m underground)","No",15]
[]
[179,31,"22mm CP fullway isolating Valve with handle nickel plated","No",10]
[]
[179,32,"28mm CP fullway isolating Valve with handle nickel plated","No",10]
[]
[179,33,"15mm 111-15CP pillar tap","No",5]
[]
[179,null,"SANITARY PLUMBING","H2"]
[]
[179,null,"uPVC soil and vent pipes","H4"]
[]
[179,34,"50mm Pipes","m",13]
[]
[179,35,"100mm Pipes","m",15]
[]
[179,null,"Extra over uPVC soil and vent pipes for fittings","H4"]
[]
[179,36,"50mm Bend","No",6]
[]
[179,37,"100mm Bend","No",3]
[]
[179,38,"50mm Access bend","No",4]
[]
[179,39,"100mm Inspection eye","No",3]
[]
[179,40,"50mm Tee","No",2]
[]
[179,41,"50mm Access bend","No",18]
[]
[179,42,"100mm to 50mm reducer","No",3]
[]
[179,43,"50mm Tee junction","No",18]
[]
[179,44,"100mm Tee with junction","No",18]
[]
[179,45,"50mm Vent cowl","No",15]
[]
[180,null,"WATER SUPPLIES","H2"]
[]
[180,null,"Class 1 copper pipes with capillary couplings","H4"]
[]
[180,46,"22mm Pipes","m",33]
[]
[180,47,"28mm Pipes","m",30]
[]
[180,48,"32mm Pipes","m",13]
[]
[180,null,"Extra over Class 1 copper pipes for capillary fittings","H4"]
[]
[180,49,"22mm Fittings","No",50]
[]
[180,50,"28mm Fittings","No",15]
[]
[180,51,"32mm Fittings","No",6]
[]
[180,null,"Testing","H4"]
[]
[180,52,"Testing water pipe system","Item","1.00"]
[]
[]
[]
[182,null,"BILL NO. 12","H1"]
[]
[182,null,"ELECTRICAL WORK","H1"]
[]
[182,null,"BLOCK S","H2"]
[]
[182,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[182,null,"Distribution boards etc","H4"]
[]
[182,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[182,null,"Switches, socket outlets, etc","H4"]
[]
[182,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[182,null,"Light fittings","H4"]
[]
[182,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[182,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[182,null,"DISTRIBUTION BOARD DB","H3"]
[]
[182,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[182,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[182,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[182,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[183,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[183,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[183,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[183,null,"CABLES","H3"]
[]
[183,8,"1.5mm² 3-Core","m",50]
[]
[183,9,"2.5mm² 3-Core","m",10]
[]
[183,10,"16mm² 3-Core","m",60]
[]
[183,null,"Cable joints","H4"]
[]
[183,11,"1.5mm² 3-Core","No",2]
[]
[183,12,"16mm² 3-Core","No",2]
[]
[183,null,"Cable terminations","H4"]
[]
[183,13,"1.5mm² 3-Core","No",40]
[]
[183,14,"2.5mm² 3-Core","No",40]
[]
[183,15,"16mm² 3-Core","No",2]
[]
[183,null,"EARTH CONDUCTORS","H3"]
[]
[183,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[183,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[183,16,"6mm²","m",60]
[]
[183,null,"SUNDRIES","H3"]
[]
[183,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[184,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[184,null,"CONDUITS ETC","H3"]
[]
[184,null,"Rigid PVC conduits","H4"]
[]
[184,18,"20mm Diameter","m",60]
[]
[184,null,"PVC conduit accessories","H4"]
[]
[184,19,"Round outlet box for 20mm conduit","No",6]
[]
[184,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",6]
[]
[184,21,"Standard draw box for 20mm conduit","No",6]
[]
[184,22,"50 x 100 x 50mm Outlet box","No",6]
[]
[184,23,"100 x 100 x 50mm Outlet box","No",6]
[]
[184,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",6]
[]
[184,null,"CONDUCTORS","H3"]
[]
[184,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[184,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[184,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[184,25,"1.5mm²","m",290]
[]
[184,null,"DRAW-WIRES","H3"]
[]
[184,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[184,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[184,27,"Flush mounted bell push button","No",1]
[]
[184,28,"16A Flush mounted two lever one-way switch unit","No",2]
[]
[185,29,"16A Three pin flush mounted socket outlet with switch, single type","No",1]
[]
[185,null,"LUMINAIRES","H3"]
[]
[185,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",5]
[]
[185,31,"1kW 100A Inverter Trolley","No",2]
[]
[185,null,"SUNDRIES","H3"]
[]
[185,32,"Earthing of buildings","Item","1.00"]
[]
[185,33,"Provision of as built drawings","Item","1.00"]
[]
[185,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[187,null,"BILL NO. 13 ","H1"]
[]
[187,null,"GLAZING","H1"]
[]
[187,null,"TOPS, SHELVES, DOORS, MIRRORS, ETC","H2"]
[]
[187,null,"4mm Silvered float glass copper backed mirrors with polished edges, holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H4"]
[]
[187,1,"Mirror 450 x 600mm high with four screws","No",6]
[]
[]
[]
[188,null,"BILL NO. 14","H1"]
[]
[188,null,"PAINTWORK","H1"]
[]
[188,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[188,null,"PAINT SPECIFICATIONS","H3"]
[]
[188,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[188,null,"COLOURS","H3"]
[]
[188,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[188,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[188,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[188,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior use","H4"]
[]
[188,1,"Walls","m2",165]
[]
[188,null,"ON EXTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[188,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[188,2,"Walls","m2",40]
[]
[188,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[188,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[188,3,"Ceilings and cornices","m2",29]
[]
[189,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[189,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[189,4,"Fascias and barge boards, including priming metal jointing strips","m2",9]
[]
[189,null,"ON WOOD SURFACES","H2"]
[]
[189,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[189,5,"Doors","m2",40]
[]
[]
[]
[191,1,"Earthworks (Provisional)","Page",154]
[]
[191,2,"Concrete, Formwork and Reinforcement","Page",157]
[]
[191,3,"Masonry","Page",160]
[]
[191,4,"Waterproofing","Page",161]
[]
[191,5,"Roof Coverings","Page",162]
[]
[191,6,"Carpentry and Joinery","Page",165]
[]
[191,7,"Ceilings, Partitions and Access Flooring","Page",168]
[]
[191,8,"Ironmongery","Page",171]
[]
[191,9,"Metalwork","Page",172]
[]
[191,10,"Plastering","Page",173]
[]
[191,11,"Plumbing and Drainage (Provisional)","Page",181]
[]
[191,12,"Electrical work","Page",186]
[]
[191,13,"Glazing","Page",187]
[]
[191,14,"Paintwork","Page",190]
[]
[192,null,"BILL NO. 1","H1"]
[]
[192,null,"EARTHWORKS","H1"]
[]
[192,null,"SITE CLEARANCE ETC","H2"]
[]
[192,null,"Site clearance","H4"]
[]
[192,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",49]
[]
[192,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[192,null,"EXCAVATIONS, ETC","H2"]
[]
[192,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[192,2,"Latrine pit","m3",58]
[]
[192,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[192,3,"Soft rock","m3",6]
[]
[192,4,"Hard rock","m3",3]
[]
[192,null,"Extra over all excavations for carting away","H4"]
[]
[192,5,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",58]
[]
[192,null,"Risk of collapse of excavations","H4"]
[]
[192,6,"Sides of trench and hole excavations exceeding 1,5m deep","m2",43]
[]
[192,7,"Sides of trench and hole excavations exceeding 1,5m deep","m2",63]
[]
[193,null,"Keeping excavations free of water","H4"]
[]
[193,8,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[193,null,"FILLING ETC","H2"]
[]
[193,null,"Compaction of surfaces","H4"]
[]
[193,9,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",29]
[]
[]
[]
[195,null,"BILL NO. 2","H1"]
[]
[195,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[195,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[195,null,"Cost of tests","H4"]
[]
[195,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[195,null,"Formwork","H4"]
[]
[195,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[195,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[195,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[195,null,"30MPa/19mm concrete","H4"]
[]
[195,1,"Surface beds","m3",5]
[]
[196,2,"Pavings","m3",2]
[]
[196,3,"Slabs including beams and inverted beams","m3",3]
[]
[196,null,"TEST CUBES","H2"]
[]
[196,4,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",2]
[]
[196,null,"CONCRETE SUNDRIES","H2"]
[]
[196,null,"Finishing top surfaces of concrete smooth with a steel trowel","H4"]
[]
[196,5,"Surface beds, slabs, etc","m2",24]
[]
[196,null,"PERMANENT FORMWORK ","H2"]
[]
[196,null,"1,2mm Galvanised steel permanent decking system to soffits ","H4"]
[]
[196,6,"Decking to slabs with ends laid on brick walls","m2",29]
[]
[196,null,"REINFORCEMENT","H2"]
[]
[196,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[196,7,"Bars in various diameter","t","0.42"]
[]
[196,null,"Fabric reinforcement","H4"]
[]
[196,8,"Type 395 fabric reinforcement in concrete surface beds etc","m2",24]
[]
[]
[]
[198,null,"BILL NO. 3","H1"]
[]
[198,null,"MASONRY ","H1"]
[]
[198,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[198,null,"BRICKWORK","H3"]
[]
[198,null,"Sizes in descriptions","H4"]
[]
[198,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[198,null,"BRICKWORK","H2"]
[]
[198,null,"SUPERSTRUCTURE","H2"]
[]
[198,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[198,1,"Half brick walls","m2",14]
[]
[198,2,"Half brick walls in beam filling","m2",2]
[]
[198,3,"One brick walls in two half brick skins with inner skin bagged and sealed","m2",58]
[]
[198,null,"BRICKWORK SUNDRIES","H2"]
[]
[198,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[198,4,"75mm Wide reinformcement built in horizontally","m",64]
[]
[198,5,"150mm Wide reinforcement built in horizontally","m",232]
[]
[198,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[198,6,"110 x 75mm Lintels in lengths not exceeding 3m","m",2]
[]
[199,null,"Galvanised wire ties etc","H4"]
[]
[199,7,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",12]
[]
[199,null,"FACE BRICKWORK","H2"]
[]
[199,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[199,8,"Extra over brickwork for face brickwork","m2",58]
[]
[199,9,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",24]
[]
[199,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[199,10,"230mm Wide sills set sloping and slightly projecting","m",2]
[]
[199,null,"DECORATIVE SCREEN WALLS AND GRILLES","H2"]
[]
[199,11,"190 x 190 x 190mm \"LG Green\" or other equal approved grille blocks with bird proof mesh built in","m2",1]
[]
[]
[]
[201,null,"BILL NO. 4","H1"]
[]
[201,null,"WATERPROOFING","H1"]
[]
[201,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[201,null,"One layer 375 micron embossed polyethylene waterproofing sheeting (SANS 952-1985 type A) sealed at laps with pvc self adhesive tape","H4"]
[]
[201,1,"Under surface beds","m2",23]
[]
[201,null,"Two coats bitumen emulsion waterproof coating","H4"]
[]
[201,2,"On bagged brick walls","m2",58]
[]
[]
[]
[202,null,"BILL NO. 5","H1"]
[]
[202,null,"ROOF COVERINGS","H1"]
[]
[202,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[202,null,"Proprietary items or materials","H3"]
[]
[202,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[202,null,"ROOF COVERINGS","H2"]
[]
[202,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[202,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)","H4"]
[]
[202,1,"Roof covering with pitches not exceeding 25 degrees","m2",44]
[]
[202,2,"Ridge cappings 475mm girth ","m",7]
[]
[202,null,"ROOF AND WALL INSULATION","H2"]
[]
[202,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[202,3,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required","m2",44]
[]
[]
[]
[203,null,"BILL NO. 6","H1"]
[]
[203,null,"CARPENTRY AND JOINERY","H1"]
[]
[203,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[203,null,"Fixing","H4"]
[]
[203,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[203,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[203,null,"ROOFS ETC","H2"]
[]
[203,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H2"]
[]
[203,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[203,null,"Trusses are at maximum 1250mm centres"]
[]
[203,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[203,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[203,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[203,1,"Supply and install prefabricated roof truss system complete and in accordance with the Standard Building Regulations. Truss spanning 3.74 x 1.7m high overall with 700mm eaves projection on both sides","No",7]
[]
[204,null,"Sawn softwood","H4"]
[]
[204,2,"38 x 114mm Wall plate","m",13]
[]
[204,3,"50 x 76mm Purlins","m",57]
[]
[204,4,"38 x 114mm Bracing","m",14]
[]
[204,null,"Sundries","H4"]
[]
[204,5,"Wrought faces on sawn timbers","m2",3]
[]
[204,6,"Two coats creosote on sawn timbers ","m2",3]
[]
[204,null,"EAVES, VERGES, ETC","H2"]
[]
[204,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[204,7,"80 x 200mm Angle section barge boards including galvanised steel H-profile jointing strips  and fix with hot dip galvanised screws and washers","m",13]
[]
[204,8,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",13]
[]
[204,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[204,null,"Wrought meranti doors hung to timber frames","H4"]
[]
[204,9,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",2]
[]
[204,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[204,10,"44mm Door 813 x 2032mm high","No",2]
[]
[]
[]
[206,null,"BILL NO. 7","H1"]
[]
[206,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING ","H1"]
[]
[206,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[206,null,"Fixing","H4"]
[]
[206,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[206,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[206,null,"Ceilings","H4"]
[]
[206,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[206,null,"Proprietary items or materials","H3"]
[]
[206,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[206,null,"NAILED-UP CEILINGS","H2"]
[]
[206,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips ","H4"]
[]
[206,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres","m2",16]
[]
[206,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",2]
[]
[207,null,"Gypsum plasterboard cornices","H4"]
[]
[207,3,"75mm Coved cornices","m",32]
[]
[]
[]
[209,null,"BILL NO. 8","H1"]
[]
[209,null,"IRONMONGERY ","H1"]
[]
[209,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[209,null,"Proprietary items","H4"]
[]
[209,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[209,null,"Finishes to ironmongery","H4"]
[]
[209,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[210,null,"Proprietary items or materials","H3"]
[]
[210,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[210,null,"HINGES, BOLTS, ETC","H2"]
[]
[210,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[210,1,"100mm Aluminium butt hinge ","No",8]
[]
[210,2,"WC chrome plated indicator bolt ","No",2]
[]
[210,null,"LOCKS","H2"]
[]
[210,null,"Manufactured by \"Union\"","H4"]
[]
[210,3,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles","No",2]
[]
[210,null,"LETTERS, NAMEPLATES, ETC","H2"]
[]
[210,null,"Manufactured by \"Union\" or other equal and approved","H4"]
[]
[210,4,"150 x 150mm Anodised aluminium plate with male symbol ","No",1]
[]
[210,null,"SUNDRIES","H2"]
[]
[210,null,"Manufactured by \"Union\"","H4"]
[]
[210,5,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",4]
[]
[210,null,"BATHROOM FITTINGS","H2"]
[]
[210,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[210,6,"Toilet roll holder, plugged","No",2]
[]
[]
[]
[212,null,"BILL NO. 9","H1"]
[]
[212,null,"METALWORK","H1"]
[]
[212,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[212,null,"Welded screens and gates ","H4"]
[]
[212,1,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock set","No",1]
[]
[212,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[212,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[212,2,"Frame for door 813 x 2032mm high","No",2]
[]
[212,null,"Double rebated frames suitable for half brick walls","H4"]
[]
[212,3,"Frame for door 813 x 2032mm high","No",2]
[]
[]
[]
[213,null,"BILL NO. 10","H1"]
[]
[213,null,"PLASTERING","H1"]
[]
[213,null,"SCREEDS","H2"]
[]
[213,null,"Screeds steel trowelled, on concrete","H4"]
[]
[213,1,"30mm Thick on floors and landings","m2",19]
[]
[213,null,"INTERNAL PLASTER","H2"]
[]
[213,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[213,2,"On walls","m2",83]
[]
[213,3,"On narrow widths","m2",3]
[]
[]
[]
[214,null,"BILL NO. 11","H1"]
[]
[214,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[214,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[214,null,"Wire gratings","H4"]
[]
[214,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[214,null,"Stormwater channels","H4"]
[]
[214,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[214,null,"PVC-U pipes and fittings","H4"]
[]
[214,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[214,null,"Polypropylene pipes","H4"]
[]
[214,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[215,null,"Fixing of pipes","H4"]
[]
[215,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[215,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[215,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[215,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[215,null,"General","H4"]
[]
[215,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[215,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[215,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[215,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[216,null,"As-built drawings","H4"]
[]
[216,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[216,null,"French drains","H4"]
[]
[216,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[216,null,"uPVC pipes and fittings","H4"]
[]
[216,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[216,null,"RAINWATER DISPOSAL","H2"]
[]
[216,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[216,1,"150mm Half-round roof gutters with beaded front edge","m",16]
[]
[216,2,"100mm Diameter rainwater pipes","m",10]
[]
[216,3,"Extra over gutter for stopped end","m",4]
[]
[216,4,"Extra over gutter for outlet for 100mm pipe","No",2]
[]
[216,5,"Extra over rainwater pipe for bend","No",3]
[]
[217,null,"STORMWATER CHANNELS","H2"]
[]
[217,null,"Earthworks","H4"]
[]
[217,6,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",4]
[]
[217,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[217,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[217,7,"\"V\" drains","m3",4]
[]
[217,8,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",29]
[]
[217,9,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",33]
[]
[217,10,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",29]
[]
[217,11,"10 x 150mm Pre-compressed bitumen impregnated foam plastic joint sealing strips between brickwork and concrete","m",25]
[]
[217,null,"SOIL DRAINAGE","H2"]
[]
[217,null,"Normal duty (Class 51) PVC-U sewer and drain pipes","H4"]
[]
[217,12,"110mm Pipes vertically or ramped to cleaning eyes etc (no excavation)","m",8]
[]
[217,13,"110mm Pipes laid in and including trenches not exceeding 1m deep","m",29]
[]
[217,null,"Extra over normal duty (Class 51) PVC-U sewer and drain pipes for fittings","H4"]
[]
[217,14,"110mm Bend","No",8]
[]
[217,15,"110mm Tee","No",1]
[]
[217,16,"110mm Access bend","No",7]
[]
[218,17,"110mm Access tee","No",1]
[]
[218,18,"110mm Rodding eye","No",2]
[]
[218,19,"110mm Straight reducer","No",8]
[]
[218,20,"22mm Socket","No",6]
[]
[218,21,"28mm Socket","No",2]
[]
[218,22,"110mm Pan connector","No",8]
[]
[218,23,"110mm PVC tovent iron connector","No",2]
[]
[218,24,"110mm Vent iron cowl","No",2]
[]
[218,null,"SANITARY FITTINGS","H2"]
[]
[218,null,"\"Vaal\" or other equal and approved","H4"]
[]
[218,25,"School type lavatory wash hand basin fixed to wall","No",4]
[]
[218,26,"Low level wc suite comprising pan with double flap heavy duty plastic seat and matching 9 litre cistern with flush pipe","No",4]
[]
[218,27,"Lavatera 70400 1/2 wall urinal with spreader, waste union, and FJT5.5 flushpipe (flush valve elsewhere)","No",4]
[]
[218,null,"WASTE UNIONS ETC","H2"]
[]
[218,null,"\"Cobra Watertech\" or other equal and approved","H4"]
[]
[218,28,"32mm 301 CP basin waste union","No",4]
[]
[218,null,"TRAPS ETC","H2"]
[]
[218,null,"UPVC","H4"]
[]
[218,29,"110mm Two way vent valve","No",4]
[]
[218,null,"Rubber","H4"]
[]
[218,30,"50mm \"P\" or \"S\" trap","No",4]
[]
[219,null,"TAPS, VALVES, ETC","H2"]
[]
[219,31,"FJ100CP \"Flushmaster Junior\" urinal flush valve","No",4]
[]
[219,32,"HDPE/UPVC to transition fitting. Underground copper portion to be denzo wrapped (1m underground)","No",12]
[]
[219,33,"22mm CP fullway isolating Valve with handle nickel plated","No",2]
[]
[219,34,"28mm CP fullway isolating Valve with handle nickel plated","No",2]
[]
[219,35,"15mm 111-15CP pillar tap","No",4]
[]
[219,null,"SANITARY PLUMBING","H2"]
[]
[219,null,"uPVC soil and vent pipes","H4"]
[]
[219,36,"50mm Pipes","m",13]
[]
[219,37,"100mm Pipes","m",15]
[]
[219,null,"Extra over uPVC soil and vent pipes for fittings","H4"]
[]
[219,38,"50mm Bend","No",6]
[]
[219,39,"100mm Bend","No",3]
[]
[219,40,"50mm Access bend","No",4]
[]
[219,41,"100mm Inspection eye","No",3]
[]
[219,42,"50mm Tee","No",2]
[]
[219,43,"50mm Access bend","No",18]
[]
[219,44,"100mm to 50mm reducer","No",3]
[]
[219,45,"50mm Tee junction","No",18]
[]
[219,46,"100mm Tee with junction","No",18]
[]
[219,47,"50mm Vent cowl","No",15]
[]
[220,null,"WATER SUPPLIES","H2"]
[]
[220,null,"Class 1 copper pipes with capillary couplings","H4"]
[]
[220,48,"22mm Pipes","m",33]
[]
[220,49,"28mm Pipes","m",30]
[]
[220,50,"32mm Pipes","m",13]
[]
[220,null,"Extra over Class 1 copper pipes for capillary fittings","H4"]
[]
[220,51,"22mm Fittings","No",50]
[]
[220,52,"28mm Fittings","No",15]
[]
[220,53,"32mm Fittings","No",6]
[]
[220,null,"Testing","H4"]
[]
[220,54,"Testing water pipe system","Item","1.00"]
[]
[]
[]
[222,null,"BILL NO. 12","H1"]
[]
[222,null,"ELECTRICAL WORK","H1"]
[]
[222,null,"BLOCK T","H2"]
[]
[222,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[222,null,"Distribution boards etc","H4"]
[]
[222,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[222,null,"Switches, socket outlets, etc","H4"]
[]
[222,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[222,null,"Light fittings","H4"]
[]
[222,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[222,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[222,null,"DISTRIBUTION BOARD DB","H3"]
[]
[222,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[222,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[222,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[222,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[223,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[223,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[223,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[223,null,"CABLES","H3"]
[]
[223,8,"1.5mm² 3-Core","m",40]
[]
[223,9,"2.5mm² 3-Core","m",10]
[]
[223,10,"16mm² 3-Core","m",60]
[]
[223,null,"Cable joints","H4"]
[]
[223,11,"1.5mm² 3-Core","No",2]
[]
[223,12,"16mm² 3-Core","No",2]
[]
[223,null,"Cable terminations","H4"]
[]
[223,13,"1.5mm² 3-Core","No",40]
[]
[223,14,"2.5mm² 3-Core","No",40]
[]
[223,15,"16mm² 3-Core","No",2]
[]
[223,null,"EARTH CONDUCTORS","H3"]
[]
[223,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[223,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[223,16,"6mm²","m",60]
[]
[223,null,"SUNDRIES","H3"]
[]
[223,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[224,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[224,null,"CONDUITS ETC","H3"]
[]
[224,null,"Rigid PVC conduits","H4"]
[]
[224,18,"20mm Diameter","m",50]
[]
[224,null,"PVC conduit accessories","H4"]
[]
[224,19,"Round outlet box for 20mm conduit","No",5]
[]
[224,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",5]
[]
[224,21,"Standard draw box for 20mm conduit","No",5]
[]
[224,22,"50 x 100 x 50mm Outlet box","No",5]
[]
[224,23,"100 x 100 x 50mm Outlet box","No",5]
[]
[224,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",5]
[]
[224,null,"CONDUCTORS","H3"]
[]
[224,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[224,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[224,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[224,25,"1.5mm²","m",290]
[]
[224,null,"DRAW-WIRES","H3"]
[]
[224,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[224,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[224,27,"Flush mounted bell push button","No",1]
[]
[224,28,"16A Flush mounted two lever one-way switch unit","No",1]
[]
[225,29,"16A Three pin flush mounted socket outlet with switch, single type","No",1]
[]
[225,null,"LUMINAIRES","H3"]
[]
[225,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",4]
[]
[225,31,"1kW 100A Inverter Trolley","No",2]
[]
[225,null,"SUNDRIES","H3"]
[]
[225,32,"Earthing of buildings","Item","1.00"]
[]
[225,33,"Provision of as built drawings","Item","1.00"]
[]
[225,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[227,null,"BILL NO. 13 ","H1"]
[]
[227,null,"GLAZING","H1"]
[]
[227,null,"TOPS, SHELVES, DOORS, MIRRORS, ETC","H2"]
[]
[227,null,"4mm Silvered float glass copper backed mirrors with polished edges, holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H4"]
[]
[227,1,"Mirror 450 x 600mm high with four screws","No",3]
[]
[]
[]
[228,null,"BILL NO. 14","H1"]
[]
[228,null,"PAINTWORK","H1"]
[]
[228,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[228,null,"PAINT SPECIFICATIONS","H3"]
[]
[228,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[228,null,"COLOURS","H3"]
[]
[228,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[228,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[228,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[228,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior use","H4"]
[]
[228,1,"Walls","m2",80]
[]
[228,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[228,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[228,2,"Ceilings and cornices","m2",16]
[]
[228,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[228,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[228,3,"Fascias and barge boards, including priming metal jointing strips","m2",7]
[]
[229,null,"ON WOOD SURFACES","H2"]
[]
[229,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[229,4,"Doors","m2",15]
[]
[]
[]
[231,1,"Earthworks (Provisional)","Page",194]
[]
[231,2,"Concrete, Formwork and Reinforcement","Page",197]
[]
[231,3,"Masonry","Page",200]
[]
[231,4,"Waterproofing","Page",201]
[]
[231,5,"Roof Coverings","Page",202]
[]
[231,6,"Carpentry and Joinery","Page",205]
[]
[231,7,"Ceilings, Partitions and Access Flooring","Page",208]
[]
[231,8,"Ironmongery","Page",211]
[]
[231,9,"Metalwork","Page",212]
[]
[231,10,"Plastering","Page",213]
[]
[231,11,"Plumbing and Drainage (Provisional)","Page",221]
[]
[231,12,"Electrical work","Page",226]
[]
[231,13,"Glazing","Page",227]
[]
[231,14,"Paintwork","Page",230]
[]
[232,null,"BILL NO. 1","H1"]
[]
[232,null,"EARTHWORKS (PROVISIONAL)","H1"]
[]
[232,null,"SITE CLEARANCE ETC","H2"]
[]
[232,null,"Site clearance","H4"]
[]
[232,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",854]
[]
[232,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[232,null,"EXCAVATIONS, ETC","H2"]
[]
[232,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[232,2,"Trenches","m3",23]
[]
[232,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[232,3,"Soft rock","m3",2]
[]
[232,4,"Hard rock","m3",1]
[]
[232,null,"Extra over all excavations for carting away","H4"]
[]
[232,5,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",23]
[]
[232,null,"Risk of collapse of excavations","H4"]
[]
[232,6,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",182]
[]
[232,null,"Keeping excavations free of water","H4"]
[]
[232,7,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[233,null,"FILLING ETC","H2"]
[]
[233,null,"Compaction of surfaces","H4"]
[]
[233,8,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",650]
[]
[233,null,"WEED KILLERS, INSECTICIDES, ETC ","H2"]
[]
[233,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[233,9,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",650]
[]
[]
[]
[235,null,"BILL NO. 2","H1"]
[]
[235,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[235,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[235,null,"Cost of tests","H4"]
[]
[235,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[235,null,"Formwork","H4"]
[]
[235,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[235,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[235,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[235,null,"30MPa/19mm concrete","H4"]
[]
[235,1,"Ground beams","m3",32]
[]
[236,2,"Trenches","m3",3]
[]
[236,3,"Surface beds","m3",78]
[]
[236,4,"Pavings","m3",16]
[]
[236,5,"Slabs including beams and inverted beams","m3",155]
[]
[236,6,"Stairs including landings, beams and inverted beams","m3",2]
[]
[236,null,"TEST CUBES","H2"]
[]
[236,7,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",6]
[]
[236,null,"CONCRETE SUNDRIES","H2"]
[]
[236,null,"Finishing top surfaces of concrete smooth with a wood float","H4"]
[]
[236,8,"Surface beds, slabs, etc","m2",727]
[]
[236,null,"Finishing top surfaces of concrete smooth with a power float","H4"]
[]
[236,9,"Surface beds, slabs, etc","m2",710]
[]
[236,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[236,null,"Rough formwork to sides","H4"]
[]
[236,10,"Edges, risers, ends and reveals not exceeding 300mm high","m",204]
[]
[236,11,"Outer sides of inverted edge beams","m2",138]
[]
[236,12,"Sloping and stepped outer edges of stairs not exceeding 300mm high extreme","m",150]
[]
[236,13,"Stairs with sloping soffits","m2",18]
[]
[236,14,"Slabs exceeding 250mm and not exceeding 500mm thick","m2",414]
[]
[237,null,"MOVEMENT JOINTS ETC","H2"]
[]
[237,null,"Expansion joints with 12mm bitumen impregnated softboard, including raking out polysolphyte sealant ","H4"]
[]
[237,15,"Not exceeding 300mm high through slabs","m",132]
[]
[237,null,"REINFORCEMENT","H2"]
[]
[237,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[237,16,"Bars in various diameter","t","15.89"]
[]
[237,null,"Fabric reinforcement","H4"]
[]
[237,17,"Type 395 fabric reinforcement in concrete surface beds etc","m2",682]
[]
[]
[]
[239,null,"BILL NO. 3","H1"]
[]
[239,null,"MASONRY (PROVISIONAL) ","H1"]
[]
[239,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[239,null,"BRICKWORK","H3"]
[]
[239,null,"Sizes in descriptions","H4"]
[]
[239,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[239,null,"BRICKWORK","H2"]
[]
[239,null,"SUPERSTRUCTURE","H2"]
[]
[239,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[239,1,"Piers","m3",13]
[]
[239,2,"Half brick walls","m2",14]
[]
[239,3,"One brick walls","m2",218]
[]
[239,4,"One brick walls in beam filling","m2",17]
[]
[239,5,"One brick walls of two half brick skins with inner skin bagged and sealed","m2",517]
[]
[239,null,"BRICKWORK SUNDRIES","H2"]
[]
[239,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[239,6,"75mm Wide reinformcement built in horizontally","m",56]
[]
[239,7,"150mm Wide reinforcement built in horizontally","m",3245]
[]
[240,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[240,8,"110 x 75mm Lintels in lengths not exceeding 3m","m",2]
[]
[240,null,"Galvanised wire ties etc","H4"]
[]
[240,9,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",106]
[]
[240,null,"FACE BRICKWORK","H2"]
[]
[240,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[240,10,"Extra over brickwork for face brickwork","m2",517]
[]
[240,11,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",110]
[]
[240,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[240,12,"230mm Wide sills set sloping and slightly projecting","m",97]
[]
[240,null,"DECORATIVE SCREEN WALLS AND GRILLES","H2"]
[]
[240,13,"190 x 190 x 190mm \"LG Green\" or other equal approved grille blocks with bird proof mesh built in","m2",26]
[]
[]
[]
[242,null,"BILL NO. 4","H1"]
[]
[242,null,"WATERPROOFING","H1"]
[]
[242,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[242,null,"One layer 250 micron green polyethylene waterproof sheeting (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape","H4"]
[]
[242,1,"Under surface beds","m2",966]
[]
[242,null,"WATERPROOFING TO ROOFS, BASEMENTS, ETC","H2"]
[]
[242,null,"One layer Derbigum SP4 waterproofing membrane, with 75mm side laps and 100mm end laps, sealed to primed surface to falls and crossfalls by 'torchfusion' finished with two coats Roofcote grey acrylic paint.","H4"]
[]
[242,2,"On flat roofs","m2",113]
[]
[242,3,"On turn-ups and turn-downs exceeding 300mm girth","m2",21]
[]
[]
[]
[243,null,"BILL NO. 5","H1"]
[]
[243,null,"ROOF COVERINGS (PROVISIONAL) ","H1"]
[]
[243,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[243,null,"Proprietary items or materials","H3"]
[]
[243,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[243,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[243,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)  ","H4"]
[]
[243,1,"Roof covering with pitches not exceeding 25 degrees","m2",639]
[]
[243,2,"Ridge cappings 475mm girth","m",48]
[]
[243,3,"Hip cappings 475mm girth","m",47]
[]
[243,4,"Valley gutters 475mm girth","m",16]
[]
[244,null,"ROOF AND WALL INSULATION","H2"]
[]
[244,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[244,5,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required ","m2",639]
[]
[]
[]
[246,null,"BILL NO. 6","H1"]
[]
[246,null,"CARPENTRY AND JOINERY (PROVISIONAL) ","H1"]
[]
[246,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[246,null,"Fixing","H4"]
[]
[246,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[246,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[246,null,"Joinery","H4"]
[]
[246,null,"Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts "]
[]
[246,null,"ROOFS ETC","H2"]
[]
[246,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H3"]
[]
[246,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[246,null,"Trusses are at maximum 1250mm centres"]
[]
[246,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[246,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[247,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[247,1,"Supply and install prefabricated 17,5 degree roof for a U shaped double story building - Block U  in accordance with the Standard Building Regulations:  Roof construction to double pitched roof with two hipped ends 56,87 x 9,35m and 1,70m high overall with 700mm eaves projection on all sides including standard full trusses, Hip-Valley trusses, jack trusses, etc at a maximum centres of 1250mm including, wall plates, permanent bracing and 50 x 76mm purlins at a maximum centres of 1250mm for IBR roof covering specified above","No",1]
[]
[247,null,"Wrought laminated Saligna","H4"]
[]
[247,2,"297 x 70mm Beam bolted to brick piers","m",67]
[]
[247,null,"Sundries","H4"]
[]
[247,3,"Wrought faces on sawn timbers","m2",22]
[]
[247,4,"Two coats creosote on sawn timbers","m2",22]
[]
[247,null,"EAVES, VERGES, ETC","H3"]
[]
[247,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[247,5,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",137]
[]
[248,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[248,null,"Wrought meranti doors hung to steel frame","H4"]
[]
[248,6,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",14]
[]
[248,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[248,7,"44mm Door 813 x 2032mm high","No",2]
[]
[]
[]
[250,null,"BILL NO. 7","H1"]
[]
[250,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING (PROVISIONAL) ","H1"]
[]
[250,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[250,null,"Fixing","H4"]
[]
[250,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[250,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[250,null,"Ceilings","H4"]
[]
[250,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[250,null,"Proprietary items or materials","H3"]
[]
[250,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[250,null,"NAILED-UP CEILINGS","H3"]
[]
[250,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips","H4"]
[]
[250,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres ","m2",498]
[]
[250,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",8]
[]
[251,null,"Nucornice foam plastic cornices","H4"]
[]
[251,3,"75mm Coved cornices","m",342]
[]
[]
[]
[253,null,"BILL NO. 8","H1"]
[]
[253,null,"FLOOR COVERINGS, WALL LININGS, ETC (PROVISIONAL)","H1"]
[]
[253,null,"FLOOR COVERINGS","H2"]
[]
[253,null,"300 x 300 x 2.5mm Semi flexible vinyl tiles","H4"]
[]
[253,1,"On floors ","m2",989]
[]
[253,null,"Vinyl skirtings, nosings, etc","H4"]
[]
[253,2,"70mm High vinyl skirting ","m",518]
[]
[253,null,"POLISH, SEALERS, ETC","H2"]
[]
[253,3,"Three coats wax polish on vinyl flooring ","m2",989]
[]
[]
[]
[254,null,"BILL NO. 9","H1"]
[]
[254,null,"IRONMONGERY  (PROVISIONAL) ","H1"]
[]
[254,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[254,null,"Proprietary items","H4"]
[]
[254,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[254,null,"Finishes to ironmongery","H4"]
[]
[254,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[255,null,"Proprietary items or materials","H3"]
[]
[255,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[255,null,"LOCKS","H2"]
[]
[255,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[255,1,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles ","No",16]
[]
[255,null,"SUNDRIES","H2"]
[]
[255,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[255,2,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",16]
[]
[255,null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC","H2"]
[]
[255,null,"Manufactured by \"Vitrex System\"","H4"]
[]
[255,3,"Pinning board size 1200 x 1200mm high plugged","No",4]
[]
[255,4,"Pinning board size 2400 x 1200mm high plugged","No",12]
[]
[255,5,"Standard green enamel megnatic chalkboard overall size 4800 x 1140mm high comprising two fixed panels, each 2400 x 1140mm high, with aluminium chalk rail plugged","No",12]
[]
[]
[]
[257,null,"BILL NO. 10","H1"]
[]
[257,null,"METALWORK (PROVISIONAL) ","H1"]
[]
[257,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[257,null,"Descriptions of bolts, anchors, etc","H4"]
[]
[257,null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[]
[257,null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete"]
[]
[257,null,"Items described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described "]
[]
[257,null,"Proprietary items or materials","H3"]
[]
[257,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[257,null,"GALVANISED STEEL BALUSTRADES","H2"]
[]
[257,null,"Bolted balustrades to ramp, staircase and walkway including intersections etc.","H4"]
[]
[257,1,"1100mm High raking black epoxy coated galvanised mild steel balustrades fixed/bolted to concrete on ramps, all as detailed on drawing number 1120.19-MQH-GA-2051","m",99]
[]
[257,2,"Ditto, but raking balustrades fixed to concrete and brickwork on staircase","m",35]
[]
[257,3,"Ditto, but horizontal balustrades fixed to concrete and brickwork on walkways","m",43]
[]
[258,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[258,null,"Welded screens and gates ","H4"]
[]
[258,4,"Galvanised mild steel mesh \"green\" screen with creepers, overall size 1,5 x 5m high, fixed to brickwork and concrete slab as detailed on drawing no. 1120.19-MQH-GA-2051","No",7]
[]
[258,5,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock set, etc.","No",14]
[]
[258,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[258,null,"Double rebated frames suitable for half brick walls","H4"]
[]
[258,6,"Frame for door 813 x 2032mm high","No",2]
[]
[258,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[258,7,"Frame for door 813 x 2032mm high","No",14]
[]
[258,null,"GALVANISED STEEL WINDOWS, DOORS, ETC","H2"]
[]
[258,null,"Standard school windows","H4"]
[]
[258,8,"Window size, 900 x 1100mm high","No",108]
[]
[]
[]
[260,null,"BILL NO. 11","H1"]
[]
[260,null,"PLASTERING (PROVISIONAL) ","H1"]
[]
[260,null,"SCREEDS","H2"]
[]
[260,null,"Screeds steel trowelled, on concrete","H4"]
[]
[260,1,"30mm Thick on floors and landings","m2",1214]
[]
[260,null,"GRANOLITHIC","H2"]
[]
[260,null,"Untinted granolithic, on concrete","H4"]
[]
[260,2,"30mm Thick on floors and landings","m2",225]
[]
[260,null,"INTERNAL PLASTER","H2"]
[]
[260,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[260,3,"On walls","m2",980]
[]
[260,4,"On narrow widths","m2",52]
[]
[260,null,"Cement plaster steel trowelled, on concrete","H4"]
[]
[260,5,"On ceilings","m2",788]
[]
[260,6,"On narrow widths","m2",48]
[]
[]
[]
[261,null,"BILL NO. 12","H1"]
[]
[261,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[261,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[261,null,"Wire gratings","H4"]
[]
[261,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[261,null,"Stormwater channels","H4"]
[]
[261,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[261,null,"PVC-U pipes and fittings","H4"]
[]
[261,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[261,null,"Polypropylene pipes","H4"]
[]
[261,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[262,null,"Fixing of pipes","H4"]
[]
[262,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[262,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[262,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[262,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[262,null,"General","H4"]
[]
[262,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[262,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[262,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[262,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[263,null,"As-built drawings","H4"]
[]
[263,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[263,null,"French drains","H4"]
[]
[263,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[263,null,"uPVC pipes and fittings","H4"]
[]
[263,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[263,null,"RAINWATER DISPOSAL","H2"]
[]
[263,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[263,1,"150mm Half-round roof gutters with beaded front edge","m",137]
[]
[263,2,"100mm Diameter rainwater pipes","m",117]
[]
[263,3,"Extra over gutter for outlet for 100mm pipe","No",16]
[]
[263,4,"Extra over rainwater pipe for bend","No",40]
[]
[263,5,"Extra over rainwater pipe for shoe","No",12]
[]
[263,6,"Fullbore cast iron outlet","No",4]
[]
[264,null,"STORMWATER CHANNELS","H2"]
[]
[264,null,"Earthworks","H4"]
[]
[264,7,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",18]
[]
[264,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[264,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[264,8,"\"V\" drains","m3",18]
[]
[264,9,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",140]
[]
[264,10,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",144]
[]
[264,11,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",140]
[]
[264,12,"Expansion joints with 12mm bitumen impregnated softboard between vertical concrete and brick surfaces","m",132]
[]
[264,null,"FIRE APPLIANCES ETC","H2"]
[]
[264,13,"\"Chubb\" hose reel with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket","No",1]
[]
[264,14,"9kg Dry chemical powder fire extinguisher","No",2]
[]
[264,null,"Fire hydrants","H4"]
[]
[264,15,"100mm Fire hydrant \"Storz\" type","No",1]
[]
[264,null,"WATER SUPPLIES TO FIRE APPLIANCES","H2"]
[]
[264,null,"Sans 2-1/2 class medium steel piping black/galvanised","H4"]
[]
[264,16,"25 NB screwed","m",8]
[]
[264,17,"25 NB screwed union","No",5]
[]
[265,18,"50 NB screwed union","No",4]
[]
[265,19,"25 NB barrel nipple screwed","No",6]
[]
[265,20,"25 NB welded or screwed socket/screw type","No",4]
[]
[265,21,"25 NB welded or screwed type elbow","No",2]
[]
[265,22,"50 NB Galvanised screw type reducing tee","No",2]
[]
[265,23,"50/25 NB Screw type reducing tee","No",2]
[]
[265,24,"100 NB Galvanised screw type reducing tee","No",2]
[]
[265,25,"50/25 NB Reducer","No",1]
[]
[265,26,"100/50 NB Concentric SANS62 reducer","No",1]
[]
[265,27,"Painting and labelling of all 50NB  screwed fire pipework (25NB) as per SANS 10252 and SANS10140","m",6]
[]
[265,28,"Painting and labelling of all pipework (25NB) as per SANS 10252 and SANS10140","m",8]
[]
[265,29,"Flashing of pipe work and pressure testing of whole system","Item","1.00"]
[]
[265,30,"Commissioning of complete system ","Item","1.00"]
[]
[265,null,"PHOTOLUMINESCENT SIGNS","H2"]
[]
[265,31,"150 x 150mm Sign","No",3]
[]
[265,32,"Hydrant and arrow sign (290 x 290mm size per sign) with steel pole and mass concrete base","No",2]
[]
[265,33,"Emergency assembly point sign with steel pole and mass concrete base","No",1]
[]
[]
[]
[267,null,"BILL NO. 13","H1"]
[]
[267,null,"ELECTRICAL WORK","H1"]
[]
[267,null,"BLOCK U","H2"]
[]
[267,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[267,null,"Distribution boards etc","H4"]
[]
[267,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[267,null,"Switches, socket outlets, etc","H4"]
[]
[267,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[267,null,"Light fittings","H4"]
[]
[267,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[267,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[267,null,"DISTRIBUTION BOARD DB","H3"]
[]
[267,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[267,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[267,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[267,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[268,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[268,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[268,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[268,null,"CABLES","H3"]
[]
[268,8,"1.5mm² 3-Core","m",1020]
[]
[268,9,"2.5mm² 3-Core","m",320]
[]
[268,10,"16mm² 3-Core","m",60]
[]
[268,null,"Cable joints","H4"]
[]
[268,11,"1.5mm² 3-Core","No",2]
[]
[268,12,"16mm² 3-Core","No",2]
[]
[268,null,"Cable terminations","H4"]
[]
[268,13,"1.5mm² 3-Core","No",40]
[]
[268,14,"2.5mm² 3-Core","No",40]
[]
[268,15,"16mm² 3-Core","No",2]
[]
[268,null,"EARTH CONDUCTORS","H3"]
[]
[268,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[268,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[268,16,"6mm²","m",60]
[]
[268,null,"SUNDRIES","H3"]
[]
[268,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[269,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[269,null,"CONDUITS ETC","H3"]
[]
[269,null,"Rigid PVC conduits","H4"]
[]
[269,18,"20mm Diameter","m",1340]
[]
[269,null,"PVC conduit accessories","H4"]
[]
[269,19,"Round outlet box for 20mm conduit","No",134]
[]
[269,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",134]
[]
[269,21,"Standard draw box for 20mm conduit","No",134]
[]
[269,22,"50 x 100 x 50mm Outlet box","No",134]
[]
[269,23,"100 x 100 x 50mm Outlet box","No",134]
[]
[269,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",134]
[]
[269,null,"CONDUCTORS","H3"]
[]
[269,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[269,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[269,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[269,25,"1.5mm²","m",290]
[]
[269,null,"DRAW-WIRES","H3"]
[]
[269,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[269,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[269,27,"Flush mounted bell push button","No",1]
[]
[269,28,"16A Flush mounted two lever one-way switch unit","No",20]
[]
[270,29,"16A Three pin flush mounted socket outlet with switch, single type","No",32]
[]
[270,null,"LUMINAIRES","H3"]
[]
[270,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",102]
[]
[270,31,"1kW 100A Inverter Trolley","No",2]
[]
[270,null,"SUNDRIES","H3"]
[]
[270,32,"Earthing of buildings","Item","1.00"]
[]
[270,33,"Provision of as built drawings","Item","1.00"]
[]
[270,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[272,null,"BILL NO. 14 ","H1"]
[]
[272,null,"GLAZING (PROVISIONAL)","H1"]
[]
[272,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[272,null,"Float glass","H4"]
[]
[272,null,"The term \"float glass\" is used for monolithic annealed glass "]
[]
[272,null,"GLAZING TO STEEL WITH PUTTY","H2"]
[]
[272,null,"4mm Clear float glass","H4"]
[]
[272,1,"Panes exceeding 0,1m² and not exceeding 0,5m²","m2",107]
[]
[]
[]
[273,null,"BILL NO. 15","H1"]
[]
[273,null,"PAINTWORK (PROVISIONAL) ","H1"]
[]
[273,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[273,null,"PAINT SPECIFICATIONS","H3"]
[]
[273,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[273,null,"COLOURS","H3"]
[]
[273,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[273,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[273,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[273,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior and use","H4"]
[]
[273,1,"Walls","m2",1032]
[]
[273,2,"Ceilings and cornices ","m2",611]
[]
[273,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[273,null,"One coat primer, one universal undercoat and two coats exterior quality \"Cemote\" pva paint","H4"]
[]
[273,3,"Ceilings and cornices ","m2",498]
[]
[274,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[274,null,"Two coats extremely durable UV-resistant, washable pure acrylic emulsion sheen paint","H4"]
[]
[274,4,"Fascias and barge boards, including priming metal jointing strips","m2",65]
[]
[274,null,"ON WOOD SURFACES","H2"]
[]
[274,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[274,5,"Laminated beam","m2",49]
[]
[274,6,"Doors","m2",56]
[]
[274,null,"ON METAL SURFACES","H2"]
[]
[274,null,"One coat alkyd based zinc phosphate primer and two coats premium quality polyurethane enamel paint, on steel","H4"]
[]
[274,7,"Windows","m2",214]
[]
[274,8,"Door frame","m2",21]
[]
[]
[]
[276,1,"Earthworks (Provisional)","Page",234]
[]
[276,2,"Concrete, Formwork and Reinforcement","Page",238]
[]
[276,3,"Masonry ","Page",241]
[]
[276,4,"Waterproofing","Page",242]
[]
[276,5,"Roof Coverings","Page",245]
[]
[276,6,"Carpentry and Joinery ","Page",249]
[]
[276,7,"Ceilings, Partitions and Access Flooring","Page",252]
[]
[276,8,"Floor Coverings, Wall Linings, etc.","Page",253]
[]
[276,9,"Ironmongery ","Page",256]
[]
[276,10,"Metalwork","Page",259]
[]
[276,11,"Plastering","Page",260]
[]
[276,12,"Plumbing and Drainage (Provisional)","Page",266]
[]
[276,13,"Electrical work","Page",271]
[]
[276,14,"Glazing","Page",272]
[]
[276,15,"Paintwork ","Page",275]
[]
[277,null,"BILL NO. 1","H1"]
[]
[277,null,"EARTHWORKS","H1"]
[]
[277,null,"SITE CLEARANCE ETC","H2"]
[]
[277,null,"Site clearance","H4"]
[]
[277,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",543]
[]
[277,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[277,null,"EXCAVATIONS, ETC","H2"]
[]
[277,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[277,2,"Trenches","m3",50]
[]
[277,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[277,3,"Soft rock","m3",5]
[]
[277,4,"Hard rock","m3",3]
[]
[277,null,"Extra over all excavations for carting away","H4"]
[]
[277,5,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",50]
[]
[277,null,"Risk of collapse of excavations","H4"]
[]
[277,6,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",310]
[]
[277,null,"Keeping excavations free of water","H4"]
[]
[277,7,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[278,null,"FILLING ETC","H2"]
[]
[278,null,"Compaction of surfaces","H4"]
[]
[278,8,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",394]
[]
[278,null,"WEED KILLERS, INSECTICIDES, ETC ","H2"]
[]
[278,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[278,9,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",387]
[]
[]
[]
[280,null,"BILL NO. 2","H1"]
[]
[280,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[280,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[280,null,"Cost of tests","H4"]
[]
[280,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[280,null,"Formwork","H4"]
[]
[280,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[280,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[281,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[281,null,"30MPa/19mm concrete","H4"]
[]
[281,1,"Ground beams","m3",31]
[]
[281,2,"Trenches","m3",45]
[]
[281,3,"Surface beds","m3",52]
[]
[281,4,"Pavings","m3",1]
[]
[281,null,"TEST CUBES","H2"]
[]
[281,5,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",6]
[]
[281,null,"CONCRETE SUNDRIES","H2"]
[]
[281,null,"Finishing top surfaces of concrete smooth with a wood float","H4"]
[]
[281,6,"Surface beds, slabs, etc","m2",34]
[]
[281,null,"Finishing top surfaces of concrete smooth with a power float","H4"]
[]
[281,7,"Surface beds, slabs, etc","m2",378]
[]
[281,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[281,null,"Rough formwork to sides","H4"]
[]
[281,8,"Edges, risers, ends and reveals not exceeding 300mm high","m",19]
[]
[281,null,"MOVEMENT JOINTS ETC","H2"]
[]
[281,null,"Expansion joints with 12mm bitumen impregnated softboard, including raking out polysolphyte sealant ","H4"]
[]
[281,9,"Not exceeding 300mm high through slabs","m",125]
[]
[282,null,"REINFORCEMENT","H2"]
[]
[282,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[282,10,"Bars in various diameter","t","2.68"]
[]
[282,null,"Fabric reinforcement","H4"]
[]
[282,11,"Type 395 fabric reinforcement in concrete surface beds etc","m2",406]
[]
[]
[]
[284,null,"BILL NO. 3","H1"]
[]
[284,null,"MASONRY ","H1"]
[]
[284,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[284,null,"BRICKWORK","H3"]
[]
[284,null,"Sizes in descriptions","H4"]
[]
[284,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[284,null,"BRICKWORK","H2"]
[]
[284,null,"SUPERSTRUCTURE","H2"]
[]
[284,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[284,1,"Half brick walls","m2",211]
[]
[284,2,"One brick walls","m2",58]
[]
[284,3,"One brick walls in beam filling","m2",19]
[]
[284,4,"One brick walls of two half brick skins with inner skin bagged and sealed","m2",198]
[]
[284,5,"One brick walls of face brick pointed on both sides","m2",68]
[]
[284,null,"BRICKWORK SUNDRIES","H2"]
[]
[284,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[284,6,"75mm Wide reinformcement built in horizontally","m",739]
[]
[284,7,"150mm Wide reinforcement built in horizontally","m",585]
[]
[285,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[285,8,"110 x 75mm Lintels in lengths not exceeding 3m","m",80]
[]
[285,null,"Galvanised wire ties etc","H4"]
[]
[285,9,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",72]
[]
[285,null,"FACE BRICKWORK","H2"]
[]
[285,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[285,10,"Extra over brickwork for face brickwork","m2",198]
[]
[285,11,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",80]
[]
[285,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[285,12,"230mm Wide sills set sloping and slightly projecting","m",37]
[]
[]
[]
[287,null,"BILL NO. 4","H1"]
[]
[287,null,"WATERPROOFING","H1"]
[]
[287,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[287,null,"One layer 375 micron embossed polyethylene dampproof course (SANS 952-1985 type B)","H4"]
[]
[287,1,"In walls","m2",40]
[]
[287,null,"One layer 250 micron green polyethylene waterproof sheeting (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape","H4"]
[]
[287,2,"Under surface beds","m2",750]
[]
[]
[]
[288,null,"BILL NO. 5","H1"]
[]
[288,null,"ROOF COVERINGS","H1"]
[]
[288,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[288,null,"Proprietary items or materials","H3"]
[]
[288,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[288,null,"ROOF COVERINGS","H2"]
[]
[288,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[288,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)","H4"]
[]
[288,1,"Roof covering with pitches not exceeding 25 degrees","m2",447]
[]
[288,2,"Ridge cappings 475mm girth ","m",29]
[]
[288,3,"Hip cappings 75mm girth","m",30]
[]
[288,4,"Valley gutters 475mm girth","m",6]
[]
[289,null,"ROOF AND WALL INSULATION","H2"]
[]
[289,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[289,5,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required","m2",447]
[]
[]
[]
[291,null,"BILL NO. 6","H1"]
[]
[291,null,"CARPENTRY AND JOINERY","H1"]
[]
[291,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[291,null,"Fixing","H4"]
[]
[291,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[291,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[291,null,"Joinery","H4"]
[]
[291,null,"Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts "]
[]
[291,null,"ROOFS ETC","H2"]
[]
[291,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H3"]
[]
[291,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[291,null,"Trusses are at maximum 1250mm centres"]
[]
[291,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[291,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[292,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[292,1,"Supply and install prefabricated 17,5 degree roof for single story building in accordance with the Standard Building Regulations:  Roof construction to double pitched roof with two hipped ends 38,70 x 9.82m and 1,70m high overall with 700mm eaves projection on all sides including standard full trusses, Hip trusses, jack and valley trusses, etc at a maximum centres of 1250mm including, wall plates, permanent bracing and 50 x 76mm purlins at a maximum centres of 1250mm for IBR roof covering specified above","No",1]
[]
[292,null,"Sundries","H4"]
[]
[292,2,"Wrought faces on sawn timbers","m2",17]
[]
[292,3,"Two coats creosote on sawn timbers","m2",17]
[]
[292,null,"EAVES, VERGES, ETC","H3"]
[]
[292,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[292,4,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",102]
[]
[292,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[292,null,"Wrought meranti doors hung to steel frame","H4"]
[]
[292,5,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",2]
[]
[293,6,"44mm Double leaf framed batten door 1594 x 2032mm high of 44 x 100mm top rail, stiles and rebated meeting stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","No",2]
[]
[293,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[293,7,"44mm Door 813 x 2032mm high","No",18]
[]
[293,null,"FITTINGS","H2"]
[]
[293,null,"Kitchen cupboards etc with approved hinges, handles and telescopic drawer sliders, including 32mm thick post-formed top with 0,6mm Decon Laminated in Artic Granite or similar","H4"]
[]
[293,8,"L-Shaped Kitchen cupboard overall size 4,50 x 0,9m high with top, sides, bottom, division, shelf, back and hinged doors, dividing framework, drawers etc.","No",1]
[]
[293,null,"Kitchen storage shelving","H4"]
[]
[293,9,"Bulk stockroom shelving overall size 5,50 x 2,00 x 0,40m","No",1]
[]
[293,10,"Reception counter overall size 5,50 x 0,50 x 0,90m high with top, sides, bottom, division, shelf, back and hinged doors, dividing framework, drawers etc. ","No",1]
[]
[293,11,"Standard waiting area timber bench size 2,5m long","No",1]
[]
[]
[]
[295,null,"BILL NO. 7","H1"]
[]
[295,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING ","H1"]
[]
[295,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[295,null,"Fixing","H4"]
[]
[295,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[295,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[295,null,"Ceilings","H4"]
[]
[295,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[295,null,"Proprietary items or materials","H3"]
[]
[295,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[295,null,"NAILED-UP CEILINGS","H2"]
[]
[295,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips ","H4"]
[]
[295,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres","m2",309]
[]
[295,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",12]
[]
[296,null,"Gypsum plasterboard cornices","H4"]
[]
[296,3,"75mm Coved cornices","m",324]
[]
[]
[]
[298,null,"BILL NO. 8","H1"]
[]
[298,null,"FLOOR COVERINGS, WALL LININGS, ETC","H1"]
[]
[298,null,"FLOOR COVERINGS","H2"]
[]
[298,null,"300 x 300 x 2.5mm Semi flexible vinyl tiles","H4"]
[]
[298,1,"On floors ","m2",309]
[]
[298,null,"Vinyl skirtings, nosings, etc","H4"]
[]
[298,2,"70mm High vinyl skirting ","m",296]
[]
[298,null,"POLISH, SEALERS, ETC","H2"]
[]
[298,3,"Three coats wax polish on vinyl flooring ","m2",309]
[]
[]
[]
[299,null,"BILL NO. 9","H1"]
[]
[299,null,"IRONMONGERY ","H1"]
[]
[299,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[299,null,"Proprietary items","H4"]
[]
[299,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[299,null,"Finishes to ironmongery","H4"]
[]
[299,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[300,null,"Proprietary items or materials","H3"]
[]
[300,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[300,null,"LOCKS","H2"]
[]
[300,null,"Manufactured by \"Union\"","H4"]
[]
[300,1,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles","No",20]
[]
[300,2,"Solid art 390/313 rebated four lever mortice lockset with and including Satin Chrome Plated handles","No",2]
[]
[300,null,"LETTERS, NAMEPLATES, ETC","H2"]
[]
[300,null,"Manufactured by \"Union\" or other equal and approved","H4"]
[]
[300,3,"150 x 150mm Anodised aluminium plate with toilet symbol ","No",3]
[]
[300,null,"SUNDRIES","H2"]
[]
[300,null,"Manufactured by \"Union\"","H4"]
[]
[300,4,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",24]
[]
[300,null,"BATHROOM FITTINGS","H2"]
[]
[300,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[300,5,"Toilet roll holder, plugged","No",5]
[]
[301,null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC","H2"]
[]
[301,null,"Manufactured by \"Vitrex System\" or other equal and approved ","H4"]
[]
[301,6,"Pinning board size 1200 x 1200mm high plugged","No",11]
[]
[301,7,"Pinning board size 2400 x 1200mm high plugged","No",1]
[]
[]
[]
[303,null,"BILL NO. 10","H1"]
[]
[303,null,"METALWORK","H1"]
[]
[303,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[303,null,"Welded screens and gates ","H4"]
[]
[303,1,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock, etc","No",2]
[]
[303,2,"Double leaf swing hot dipped galvanised mild steel gate, 1880mm x 2125mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including 50mm brass padlock and all other ironmongery to fix on wall","No",2]
[]
[303,null,"GALVANISED STEEL WINDOWS, DOORS, ETC","H2"]
[]
[303,null,"Standard school windows with flat burglar bars to opening sashes","H4"]
[]
[303,3,"Window type 1, size 890 x 1250mm high","No",6]
[]
[303,4,"Ditto, but type 2, size 533 x 654mm high","No",6]
[]
[303,5,"Ditto, but type 3, size 1022 x 1250mm high","No",26]
[]
[303,6,"Ditto, but type 4, size 1022 x 654mm high","No",2]
[]
[303,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[303,null,"Double rebated frames suitable for half brick walls","H4"]
[]
[303,7,"Frame for door 813 x 2032mm high","No",18]
[]
[303,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[303,8,"Frame for door 813 x 2032mm high","No",2]
[]
[304,9,"Ditto, but for door 1594 x 2032mm high","No",2]
[]
[304,null,"STEEL RECORDROOM AND STRONGROOM DOORS, VENTILATORS, ETC","H2"]
[]
[304,null,"\"Chubb\" recordroom doors suitable for 230mm walls fixed to brickwork or concrete","H4"]
[]
[304,10,"Double ended recordroom ventilator","No",4]
[]
[304,11,"\"Chubb\"  recordroom door and frame 900 x 2100mm high overall with a mass of 180kg","No",2]
[]
[]
[]
[306,null,"BILL NO. 11","H1"]
[]
[306,null,"PLASTERING","H1"]
[]
[306,null,"SCREEDS","H2"]
[]
[306,null,"Screeds steel trowelled, on concrete","H4"]
[]
[306,1,"30mm Thick on floors and landings","m2",309]
[]
[306,null,"INTERNAL PLASTER","H2"]
[]
[306,null,"Cement plaster wood floated on brickwork","H4"]
[]
[306,2,"On walls","m2",738]
[]
[306,3,"On ceilings","m2",24]
[]
[306,4,"On narrow widths","m2",20]
[]
[]
[]
[307,null,"BILL NO. 12","H1"]
[]
[307,null,"TILING","H1"]
[]
[307,null,"WALL TILING","H2"]
[]
[307,null,"200 x 200 x 5mm White glazed ceramic tiles on brickwork including cement plaster backing (PC sum R160/m² for supply and delivery)","H4"]
[]
[307,1,"On walls","m2",4]
[]
[]
[]
[308,null,"BILL NO. 13","H1"]
[]
[308,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[308,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[308,null,"Wire gratings","H4"]
[]
[308,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[308,null,"Stormwater channels","H4"]
[]
[308,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[308,null,"PVC-U pipes and fittings","H4"]
[]
[308,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[308,null,"Polypropylene pipes","H4"]
[]
[308,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[309,null,"Fixing of pipes","H4"]
[]
[309,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[309,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[309,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[309,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[309,null,"General","H4"]
[]
[309,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[309,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[309,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[309,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[310,null,"As-built drawings","H4"]
[]
[310,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[310,null,"French drains","H4"]
[]
[310,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[310,null,"uPVC pipes and fittings","H4"]
[]
[310,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[310,null,"RAINWATER DISPOSAL","H2"]
[]
[310,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[310,1,"150mm Half-round roof gutters with beaded front edge","m",102]
[]
[310,2,"100mm Diameter rainwater pipes","m",17]
[]
[310,3,"Extra over gutter for angle","No",10]
[]
[310,4,"Extra over gutter for outlet for 100mm pipe","No",6]
[]
[310,5,"Extra over rainwater pipe for bend","No",12]
[]
[310,6,"Extra over rainwater pipe for shoe","No",6]
[]
[311,null,"STORMWATER CHANNELS","H2"]
[]
[311,null,"Earthworks","H4"]
[]
[311,7,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",13]
[]
[311,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[311,8,"Weed killer in accordance with SANS 5859 under floors etc,","m2",101]
[]
[311,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[311,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[311,9,"\"V\" drains","m3",13]
[]
[311,10,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",101]
[]
[311,11,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",105]
[]
[311,12,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",101]
[]
[311,13,"Expansion joints with 12mm bitumen impregnated softboard between vertical concrete and brick surfaces","m",97]
[]
[311,14,"One layer 250 micron green polyethylene waterproof sheeting (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape under surface bed","m2",101]
[]
[311,null,"SOIL DRAINAGE","H2"]
[]
[311,null,"Normal duty (Class 51) PVC-U sewer and drain pipes","H4"]
[]
[311,15,"110mm Pipes vertically or ramped to cleaning eyes etc (no excavation)","m",10]
[]
[311,16,"110mm Pipes laid in and including trenches not exceeding 1m deep","m",20]
[]
[312,null,"Extra over normal duty (Class 51) PVC-U sewer and drain pipes for fittings","H4"]
[]
[312,17,"22mm Socket","No",2]
[]
[312,18,"110mm Rodding eye","No",4]
[]
[312,19,"110mm Pan connector","No",5]
[]
[312,20,"50mm Vent cowl","No",5]
[]
[312,21,"110mm Vent cowl","No",5]
[]
[312,null,"SANITARY FITTINGS","H2"]
[]
[312,null,"\"Vaal\" or other equal and approved","H4"]
[]
[312,22,"School type lavatory wash hand basin fixed to wall","No",6]
[]
[312,23,"Low level wc suite comprising pan with double flap heavy duty plastic seat and matching 9 litre cistern with flush pipe","No",5]
[]
[312,null,"Rubber","H4"]
[]
[312,24,"50mm \"P\" or \"S\" trap","No",6]
[]
[312,null,"TAPS, VALVES, ETC","H2"]
[]
[312,25,"HDPE/UPVC to transition fitting. Underground copper portion to be denzo wrapped (1m underground)","No",11]
[]
[312,26,"22mm Fullway isolating ball valve with handle nickel plated","No",2]
[]
[312,27,"15mm Stop cock","No",11]
[]
[312,28,"15mm Bib tap","No",6]
[]
[312,null,"SANITARY PLUMBING","H2"]
[]
[312,null,"uPVC soil and vent pipes","H4"]
[]
[312,29,"50mm Pipes","m",30]
[]
[312,30,"110mm Pipes","m",5]
[]
[313,null,"Extra over uPVC soil and vent pipes for fittings","H4"]
[]
[313,31,"50mm Bend","No",16]
[]
[313,32,"110mm Bend with inspection eye","No",5]
[]
[313,33,"50mm Tee with inspection eye","No",6]
[]
[313,34,"110mm Tee with inspection eye","No",5]
[]
[313,35,"110mm to 50mm Reducer","No",6]
[]
[313,null,"WATER SUPPLIES","H2"]
[]
[313,null,"Class 1 copper pipes with capillary couplings","H4"]
[]
[313,36,"22mm Pipes","m",40]
[]
[313,37,"38mm Pipes","m",15]
[]
[313,null,"Extra over Class 1 copper pipes for capillary fittings","H4"]
[]
[313,38,"22mm Fittings","No",14]
[]
[313,null,"Testing","H4"]
[]
[313,39,"Testing water pipe system","Item","1.00"]
[]
[313,null,"FIRE APPLIANCES ETC","H2"]
[]
[313,40,"\"Chubb\" hose reel with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket","No",1]
[]
[313,41,"9kg Dry chemical powder fire extinguisher","No",2]
[]
[313,null,"Fire hydrants","H4"]
[]
[313,42,"100mm Fire hydrant \"Storz\" type","No",1]
[]
[313,null,"WATER SUPPLIES TO FIRE APPLIANCES","H2"]
[]
[313,null,"Sans 2-1/2 class medium steel piping black/galvanised","H4"]
[]
[313,43,"25 NB screwed","m",8]
[]
[313,44,"25 NB screwed union","No",5]
[]
[314,45,"50 NB screwed union","No",4]
[]
[314,46,"25 NB barrel nipple screwed","No",6]
[]
[314,47,"25 NB welded or screwed socket/screw type","No",4]
[]
[314,48,"25 NB welded or screwed type elbow","No",2]
[]
[314,49,"50 NB Galvanised screw type reducing tee","No",2]
[]
[314,50,"50/25 NB Screw type reducing tee","No",2]
[]
[314,51,"100 NB Galvanised screw type reducing tee","No",2]
[]
[314,52,"50/25 NB Reducer","No",1]
[]
[314,53,"100/50 NB Concentric SANS62 reducer","No",1]
[]
[314,54,"Painting and labelling of all 50NB  screwed fire pipework (25NB) as per SANS 10252 and SANS10140","m",6]
[]
[314,55,"Painting and labelling of all pipework (25NB) as per SANS 10252 and SANS10140","m",8]
[]
[314,56,"Flashing of pipe work and pressure testing of whole system","Item","1.00"]
[]
[314,57,"Commissioning of complete system ","Item","1.00"]
[]
[314,null,"PHOTOLUMINESCENT SIGNS","H2"]
[]
[314,58,"150 x 150mm Sign","No",3]
[]
[314,59,"Hydrant and arrow sign (290 x 290mm size per sign) with steel pole and mass concrete base","No",2]
[]
[314,60,"Emergency assembly point sign with steel pole and mass concrete base","No",1]
[]
[]
[]
[316,null,"BILL NO. 14","H1"]
[]
[316,null,"ELECTRICAL WORK","H1"]
[]
[316,null,"BLOCK V","H2"]
[]
[316,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[316,null,"Distribution boards etc","H4"]
[]
[316,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[316,null,"Switches, socket outlets, etc","H4"]
[]
[316,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[316,null,"Light fittings","H4"]
[]
[316,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[316,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[316,null,"DISTRIBUTION BOARD DB","H3"]
[]
[316,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[316,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[316,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[316,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[317,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[317,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[317,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[317,null,"CABLES","H3"]
[]
[317,8,"1.5mm² 3-Core","m",700]
[]
[317,9,"2.5mm² 3-Core","m",410]
[]
[317,10,"16mm² 3-Core","m",60]
[]
[317,null,"Cable joints","H4"]
[]
[317,11,"1.5mm² 3-Core","No",2]
[]
[317,12,"16mm² 3-Core","No",2]
[]
[317,null,"Cable terminations","H4"]
[]
[317,13,"1.5mm² 3-Core","No",40]
[]
[317,14,"2.5mm² 3-Core","No",40]
[]
[317,15,"16mm² 3-Core","No",2]
[]
[317,null,"EARTH CONDUCTORS","H3"]
[]
[317,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[317,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[317,16,"6mm²","m",60]
[]
[317,null,"SUNDRIES","H3"]
[]
[317,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[318,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[318,null,"CONDUITS ETC","H3"]
[]
[318,null,"Rigid PVC conduits","H4"]
[]
[318,18,"20mm Diameter","m",1110]
[]
[318,null,"PVC conduit accessories","H4"]
[]
[318,19,"Round outlet box for 20mm conduit","No",111]
[]
[318,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",111]
[]
[318,21,"Standard draw box for 20mm conduit","No",111]
[]
[318,22,"50 x 100 x 50mm Outlet box","No",111]
[]
[318,23,"100 x 100 x 50mm Outlet box","No",111]
[]
[318,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",111]
[]
[318,null,"CONDUCTORS","H3"]
[]
[318,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[318,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[318,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[318,25,"1.5mm²","m",290]
[]
[318,null,"DRAW-WIRES","H3"]
[]
[318,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[318,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[318,27,"Flush mounted bell push button","No",1]
[]
[318,28,"16A Flush mounted two lever one-way switch unit","No",24]
[]
[319,29,"16A Three pin flush mounted socket outlet with switch, single type","No",41]
[]
[319,null,"LUMINAIRES","H3"]
[]
[319,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",70]
[]
[319,31,"1kW 100A Inverter Trolley","No",2]
[]
[319,null,"SUNDRIES","H3"]
[]
[319,32,"Earthing of buildings","Item","1.00"]
[]
[319,33,"Provision of as built drawings","Item","1.00"]
[]
[319,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[321,null,"BILL NO. 15 ","H1"]
[]
[321,null,"GLAZING","H1"]
[]
[321,null,"GLAZING TO STEEL WITH PUTTY","H2"]
[]
[321,null,"4mm Clear float glass","H4"]
[]
[321,1,"Panes exceeding 0,1m² and not exceeding 0,5m²","m2",54]
[]
[321,null,"TOPS, SHELVES, DOORS, MIRRORS, ETC","H2"]
[]
[321,null,"4mm Silvered float glass copper backed mirrors with polished edges, holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete","H4"]
[]
[321,2,"Mirror 450 x 600mm high with four screws","No",6]
[]
[]
[]
[322,null,"BILL NO. 16","H1"]
[]
[322,null,"PAINTWORK","H1"]
[]
[322,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[322,null,"PAINT SPECIFICATIONS","H3"]
[]
[322,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[322,null,"COLOURS","H3"]
[]
[322,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[322,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[322,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[322,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior use","H4"]
[]
[322,1,"Walls","m2",758]
[]
[322,null,"ON BAGGED BRICKWORK OR CONCRETE SURFACES","H2"]
[]
[322,2,"Ceilings and beams","m2",24]
[]
[322,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[322,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[322,3,"Ceilings and cornices","m2",309]
[]
[323,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[323,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[323,4,"Fascias and barge boards, including priming metal jointing strips","m2",49]
[]
[323,null,"ON WOOD SURFACES","H2"]
[]
[323,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[323,5,"Doors","m2",87]
[]
[323,null,"ON METAL SURFACES","H2"]
[]
[323,null,"One coat alkyd based zinc phosphate primer and two coats premium quality polyurethane enamel paint, on steel","H4"]
[]
[323,6,"Door frames","m2",51]
[]
[323,7,"Windows","m2",108]
[]
[]
[]
[325,1,"Earthworks (Provisional)","Page",279]
[]
[325,2,"Concrete, Formwork and Reinforcement","Page",283]
[]
[325,3,"Masonry","Page",286]
[]
[325,4,"Waterproofing","Page",287]
[]
[325,5,"Roof Coverings","Page",290]
[]
[325,6,"Carpentry and Joinery","Page",294]
[]
[325,7,"Ceilings, Partitions and Access Flooring","Page",297]
[]
[325,8,"Floor Coverings, Wall Linings, etc.","Page",298]
[]
[325,9,"Ironmongery","Page",302]
[]
[325,10,"Metalwork","Page",305]
[]
[325,11,"Plastering","Page",306]
[]
[325,12,"Tiling","Page",307]
[]
[325,13,"Plumbing and Drainage (Provisional)","Page",315]
[]
[325,14,"Electrical work","Page",320]
[]
[325,15,"Glazing","Page",321]
[]
[325,16,"Paintwork","Page",324]
[]
[326,null,"BILL NO. 1","H1"]
[]
[326,null,"EARTHWORKS","H1"]
[]
[326,null,"SITE CLEARANCE ETC","H2"]
[]
[326,null,"Site clearance","H4"]
[]
[326,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",1267]
[]
[326,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[326,null,"EXCAVATIONS, ETC","H2"]
[]
[326,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[326,2,"Trenches","m3",76]
[]
[326,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[326,3,"Soft rock","m3",8]
[]
[326,4,"Hard rock","m3",4]
[]
[326,null,"Extra over all excavations for carting away","H4"]
[]
[326,5,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",76]
[]
[326,null,"Risk of collapse of excavations","H4"]
[]
[326,6,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",443]
[]
[326,null,"Keeping excavations free of water","H4"]
[]
[326,7,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[327,null,"FILLING ETC","H2"]
[]
[327,null,"Compaction of surfaces","H4"]
[]
[327,8,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",702]
[]
[327,null,"WEED KILLERS, INSECTICIDES, ETC ","H2"]
[]
[327,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[327,9,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",702]
[]
[]
[]
[329,null,"BILL NO. 2","H1"]
[]
[329,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[329,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[329,null,"Cost of tests","H4"]
[]
[329,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[329,null,"Formwork","H4"]
[]
[329,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[329,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[330,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[330,null,"30MPa/19mm concrete","H4"]
[]
[330,1,"Ground beams","m3",54]
[]
[330,2,"Trenches","m3",5]
[]
[330,3,"Surface beds","m3",102]
[]
[330,4,"Pavings","m3",5]
[]
[330,null,"TEST CUBES","H2"]
[]
[330,5,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",6]
[]
[330,null,"CONCRETE SUNDRIES","H2"]
[]
[330,null,"Finishing top surfaces of concrete smooth with a wood float","H4"]
[]
[330,6,"Surface beds, slabs, etc","m2",52]
[]
[330,null,"Finishing top surfaces of concrete smooth with a power float","H4"]
[]
[330,7,"Surface beds, slabs, etc","m2",784]
[]
[330,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[330,null,"Rough formwork to sides","H4"]
[]
[330,8,"Edges, risers, ends and reveals not exceeding 300mm high","m",61]
[]
[330,null,"MOVEMENT JOINTS ETC","H2"]
[]
[330,null,"Expansion joints with 12mm bitumen impregnated softboard, including raking out polysolphyte sealant ","H4"]
[]
[330,9,"Not exceeding 300mm high through slabs","m",1940]
[]
[331,null,"REINFORCEMENT","H2"]
[]
[331,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[331,10,"Bars in various diameter","t","5.03"]
[]
[331,null,"Fabric reinforcement","H4"]
[]
[331,11,"Type 395 fabric reinforcement in concrete surface beds etc","m2",827]
[]
[]
[]
[333,null,"BILL NO. 4","H1"]
[]
[333,null,"MASONRY ","H1"]
[]
[333,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[333,null,"BRICKWORK","H3"]
[]
[333,null,"Sizes in descriptions","H4"]
[]
[333,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[333,null,"BRICKWORK","H2"]
[]
[333,null,"SUPERSTRUCTURE","H2"]
[]
[333,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[333,1,"Half brick walls","m2",62]
[]
[333,2,"One brick walls","m2",262]
[]
[333,3,"One brick walls in beam filling","m2",30]
[]
[333,4,"One brick walls of two half brick skins with inner skin bagged and sealed","m2",420]
[]
[333,null,"BRICKWORK SUNDRIES","H2"]
[]
[333,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[333,5,"75mm Wide reinformcement built in horizontally","m",208]
[]
[333,6,"150mm Wide reinforcement built in horizontally","m",2848]
[]
[333,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[333,7,"110 x 75mm Lintels in lengths not exceeding 3m","m",20]
[]
[334,null,"Galvanised wire ties etc","H4"]
[]
[334,8,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",140]
[]
[334,null,"FACE BRICKWORK","H2"]
[]
[334,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[334,9,"Extra over brickwork for face brickwork","m2",450]
[]
[334,10,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",79]
[]
[334,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[334,11,"230mm Wide sills set sloping and slightly projecting","m",73]
[]
[]
[]
[336,null,"BILL NO. 4","H1"]
[]
[336,null,"WATERPROOFING","H1"]
[]
[336,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[336,null,"One layer 250 micron green polyethylene waterproof sheeting (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape","H4"]
[]
[336,1,"Under surface beds","m2",1940]
[]
[]
[]
[337,null,"BILL NO. 5","H1"]
[]
[337,null,"ROOF COVERINGS ","H1"]
[]
[337,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[337,null,"Proprietary items or materials","H3"]
[]
[337,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[337,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[337,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)  ","H4"]
[]
[337,1,"Roof covering with pitches not exceeding 25 degrees","m2",853]
[]
[337,2,"Ridge cappings 475mm girth","m",66]
[]
[337,3,"Hip cappings 475mm girth","m",47]
[]
[337,4,"Valley gutters 475mm girth","m",16]
[]
[338,null,"ROOF AND WALL INSULATION","H2"]
[]
[338,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[338,5,"Insulation sheeting laid taut over purlins and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required ","m2",894]
[]
[]
[]
[340,null,"BILL NO. 6","H1"]
[]
[340,null,"CARPENTRY AND JOINERY ","H1"]
[]
[340,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[340,null,"Fixing","H4"]
[]
[340,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[340,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[340,null,"Joinery","H4"]
[]
[340,null,"Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts "]
[]
[340,null,"ROOFS ETC","H2"]
[]
[340,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H3"]
[]
[340,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[340,null,"Trusses are at maximum 1250mm centres"]
[]
[340,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[340,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[341,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[341,1,"Supply and install prefabricated 17,5 degree roof for a U shaped single story building - Block W  in accordance with the Standard Building Regulations:  Roof construction to double pitched roof with two hipped ends 76,35 x 9,35m and 1,70m high overall with 700mm eaves projection on all sides including standard full trusses, Hip-Valley trusses, jack trusses, etc at a maximum centres of 1250mm including, wall plates, permanent bracing and 50 x 76mm purlins at a maximum centres of 1250mm for IBR roof covering specified above","No",1]
[]
[341,null,"Wrought laminated Saligna","H4"]
[]
[341,2,"297 x 70mm Beam bolted to steel posts","m",58]
[]
[341,null,"Sundries","H4"]
[]
[341,3,"Wrought faces on sawn timbers","m2",29]
[]
[341,4,"Two coats creosote on sawn timbers","m2",29]
[]
[341,null,"EAVES, VERGES, ETC","H3"]
[]
[341,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[341,5,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",179]
[]
[342,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[342,null,"Wrought meranti doors hung to steel frame","H4"]
[]
[342,6,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",7]
[]
[342,null,"Semi-solid flush doors with commercial veneer suitable for painting","H4"]
[]
[342,7,"44mm Door 813 x 2032mm high","No",12]
[]
[]
[]
[344,null,"BILL NO. 7","H1"]
[]
[344,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING ","H1"]
[]
[344,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[344,null,"Fixing","H4"]
[]
[344,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[344,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[344,null,"Ceilings","H4"]
[]
[344,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[344,null,"Proprietary items or materials","H3"]
[]
[344,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[344,null,"NAILED-UP CEILINGS","H3"]
[]
[344,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips","H4"]
[]
[344,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres ","m2",658]
[]
[344,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",12]
[]
[345,null,"Nucornice foam plastic cornices","H4"]
[]
[345,3,"75mm Coved cornices","m",377]
[]
[]
[]
[347,null,"BILL NO. 8","H1"]
[]
[347,null,"FLOOR COVERINGS, WALL LININGS, ETC ","H1"]
[]
[347,null,"FLOOR COVERINGS","H2"]
[]
[347,null,"300 x 300 x 2.5mm Semi flexible vinyl tiles","H4"]
[]
[347,1,"On floors ","m2",658]
[]
[347,null,"Vinyl skirtings, nosings, etc","H4"]
[]
[347,2,"70mm High vinyl skirting ","m",349]
[]
[347,null,"POLISH, SEALERS, ETC","H2"]
[]
[347,3,"Three coats wax polish on vinyl flooring ","m2",658]
[]
[]
[]
[348,null,"BILL NO. 9","H1"]
[]
[348,null,"IRONMONGERY ","H1"]
[]
[348,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[348,null,"Proprietary items","H4"]
[]
[348,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[348,null,"Finishes to ironmongery","H4"]
[]
[348,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[349,null,"Proprietary items or materials","H3"]
[]
[349,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[349,null,"LOCKS","H2"]
[]
[349,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[349,1,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles ","No",19]
[]
[349,null,"SUNDRIES","H2"]
[]
[349,null,"Manufactured by \"Union\" or other equal and approved ","H4"]
[]
[349,2,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",19]
[]
[349,null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC","H2"]
[]
[349,null,"Manufactured by \"Vitrex System\"","H4"]
[]
[349,3,"Pinning board size 1200 x 1200mm high plugged","No",4]
[]
[349,4,"Pinning board size 2400 x 1200mm high plugged","No",5]
[]
[349,5,"Standard green enamel megnatic chalkboard overall size 4800 x 1140mm high comprising two fixed panels, each 2400 x 1140mm high, with aluminium chalk rail plugged","No",5]
[]
[]
[]
[351,null,"BILL NO. 10","H1"]
[]
[351,null,"METALWORK ","H1"]
[]
[351,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[351,null,"Descriptions of bolts, anchors, etc","H4"]
[]
[351,null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[]
[351,null,"Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete"]
[]
[351,null,"Items described as \"holed for bolt(s)\" shall be deemed to exclude the bolts unless otherwise described "]
[]
[351,null,"Proprietary items or materials","H3"]
[]
[351,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[351,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[351,null,"Welded screens and gates ","H4"]
[]
[351,1,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock set, etc.","No",7]
[]
[351,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[351,null,"Double rebated frames suitable for half brick walls","H4"]
[]
[351,2,"Frame for door 813 x 2032mm high","No",2]
[]
[352,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[352,3,"Frame for door 813 x 2032mm high","No",17]
[]
[352,null,"GALVANISED STEEL WINDOWS, DOORS, ETC","H2"]
[]
[352,null,"Standard school windows","H4"]
[]
[352,4,"Window size, 900 x 1100mm high","No",81]
[]
[352,null,"GALVANISED STEEL MINOR WORK","H2"]
[]
[352,null,"Galvanised steel post, including fixing accessories to laminated timber beam and concrete floors ","H4"]
[]
[352,5,"100mm Diameter x 2650mm high galvanised mild steel support post including base plates etc. with timber beam over to support roof above (Timber beam elsewhere)","No",18]
[]
[]
[]
[354,null,"BILL NO. 11","H1"]
[]
[354,null,"PLASTERING ","H1"]
[]
[354,null,"SCREEDS","H2"]
[]
[354,null,"Screeds steel trowelled, on concrete","H4"]
[]
[354,1,"30mm Thick on floors and landings","m2",658]
[]
[354,null,"INTERNAL PLASTER","H2"]
[]
[354,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[354,2,"On walls","m2",905]
[]
[354,3,"On narrow widths","m2",39]
[]
[]
[]
[355,null,"BILL NO. 12","H1"]
[]
[355,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[355,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[355,null,"Wire gratings","H4"]
[]
[355,null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[355,null,"Stormwater channels","H4"]
[]
[355,null,"Descriptions of channels shall be deemed to include necessary excavation, surface preparation, compaction, etc, and disposal of surplus material on site"]
[]
[355,null,"PVC-U pipes and fittings","H4"]
[]
[355,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings"]
[]
[355,null,"Polypropylene pipes","H4"]
[]
[355,null,"Polypropylene pipes 54mm diameter and smaller shall be seamless copper coloured Class 16 pipes jointed with heat welded thermoplastic or where so described compression fittings  Pipes shall be firmly fixed to walls, etc with coloured nylon snap-in pipe clips with provision for accommodating thermal movement and jointed and fixed strictly in accordance with the manufacturer's instructions"]
[]
[356,null,"Fixing of pipes","H4"]
[]
[356,null,"Unless specifically otherwise stated, descriptions of pipes shall be deemed to include fixing to walls, etc, casting in, building in or suspending not exceeding 1m below suspension level"]
[]
[356,null,"Laying, backfilling, bedding, etc of pipes","H4"]
[]
[356,null,"Pipes shall be laid and bedded in accordance with manufacturers' instructions and trenches shall be carefully backfilled "]
[]
[356,null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with the relevant section of SANS 2001"]
[]
[356,null,"General","H4"]
[]
[356,null,"Descriptions of cast iron roof outlets shall be deemed to include joints to pipes and casting into concrete (adaptors for joints to PVC pipes, etc are given separately)  Descriptions of overflow pipes where measured in number, shall be deemed to include joints to cisterns and splay cut ends"]
[]
[356,null,"Descriptions of pipes laid in and including trenches and of inspection chambers, catchpits, etc shall be deemed to include excavation, bedding, backfilling, compaction to a minimum of 93% Mod AASHTO density and disposal of surplus material on site"]
[]
[356,null,"Descriptions of service pipes and flexible connecting pipes shall be deemed to include connections to taps, cisterns, etc and to steel pipes (adaptors for connections to copper pipes, etc are given separately)"]
[]
[356,null,"Descriptions of WC pans, slop hoppers, etc shall be deemed to include for joints to soil pipes (pan connectors are separately measured)"]
[]
[357,null,"As-built drawings","H4"]
[]
[357,null,"Where required, the contractor shall prepare an updated set of as-built drawings.  At completion of the contract the contractor shall hand these drawings to the principal agent for reproducing onto the originals for handing over to the employer (provision for allowance of as-built drawings elsewhere)"]
[]
[357,null,"French drains","H4"]
[]
[357,null,"Descriptions of french drains shall be deemed to include excavation, stone filling graded from 300mm diameter at bottom to 75mm diameter at top, geofabric filter blanket over stone, 300mm earthfilling over and disposal of surplus material on site"]
[]
[357,null,"uPVC pipes and fittings","H4"]
[]
[357,null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings  Soil, waste and vent pipes and fittings shall be solvent weld jointed or sealed with butyl rubber rings "]
[]
[357,null,"RAINWATER DISPOSAL","H2"]
[]
[357,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[357,1,"150mm Half-round roof gutters with beaded front edge","m",137]
[]
[357,2,"100mm Diameter rainwater pipes","m",86]
[]
[357,3,"Extra over gutter for outlet for 100mm pipe","No",16]
[]
[357,4,"Extra over rainwater pipe for bend","No",36]
[]
[357,5,"Extra over rainwater pipe for shoe","No",12]
[]
[358,null,"STORMWATER CHANNELS","H2"]
[]
[358,null,"Earthworks","H4"]
[]
[358,6,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",18]
[]
[358,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[358,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[358,7,"\"V\" drains","m3",18]
[]
[358,8,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",140]
[]
[358,9,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",144]
[]
[358,10,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",140]
[]
[358,11,"Expansion joints with 12mm bitumen impregnated softboard between vertical concrete and brick surfaces","m",132]
[]
[358,null,"FIRE APPLIANCES ETC","H2"]
[]
[358,12,"\"Chubb\" hose reel with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket","No",1]
[]
[358,13,"9kg Dry chemical powder fire extinguisher","No",2]
[]
[358,null,"Fire hydrants","H4"]
[]
[358,14,"100mm Fire hydrant \"Storz\" type","No",1]
[]
[358,null,"WATER SUPPLIES TO FIRE APPLIANCES","H2"]
[]
[358,null,"Sans 2-1/2 class medium steel piping black/galvanised","H4"]
[]
[358,15,"25 NB screwed","m",8]
[]
[358,16,"25 NB screwed union","No",5]
[]
[359,17,"50 NB screwed union","No",4]
[]
[359,18,"25 NB barrel nipple screwed","No",6]
[]
[359,19,"25 NB welded or screwed socket/screw type","No",4]
[]
[359,20,"25 NB welded or screwed type elbow","No",2]
[]
[359,21,"50 NB Galvanised screw type reducing tee","No",2]
[]
[359,22,"50/25 NB Screw type reducing tee","No",2]
[]
[359,23,"100 NB Galvanised screw type reducing tee","No",2]
[]
[359,24,"50/25 NB Reducer","No",1]
[]
[359,25,"100/50 NB Concentric SANS62 reducer","No",1]
[]
[359,26,"Painting and labelling of all 50NB  screwed fire pipework (25NB) as per SANS 10252 and SANS10140","m",6]
[]
[359,27,"Painting and labelling of all pipework (25NB) as per SANS 10252 and SANS10140","m",8]
[]
[359,28,"Flashing of pipe work and pressure testing of whole system","Item","1.00"]
[]
[359,29,"Commissioning of complete system ","Item","1.00"]
[]
[359,null,"PHOTOLUMINESCENT SIGNS","H2"]
[]
[359,30,"150 x 150mm Sign","No",3]
[]
[359,31,"Hydrant and arrow sign (290 x 290mm size per sign) with steel pole and mass concrete base","No",2]
[]
[359,32,"Emergency assembly point sign with steel pole and mass concrete base","No",1]
[]
[]
[]
[361,null,"BILL NO. 13","H1"]
[]
[361,null,"ELECTRICAL WORK","H1"]
[]
[361,null,"BLOCK W","H2"]
[]
[361,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[361,null,"Distribution boards etc","H4"]
[]
[361,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[361,null,"Switches, socket outlets, etc","H4"]
[]
[361,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[361,null,"Light fittings","H4"]
[]
[361,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[361,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[361,null,"DISTRIBUTION BOARD DB","H3"]
[]
[361,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[361,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[361,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[361,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[362,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[362,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[362,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[362,null,"CABLES","H3"]
[]
[362,8,"1.5mm² 3-Core","m",680]
[]
[362,9,"2.5mm² 3-Core","m",610]
[]
[362,10,"16mm² 3-Core","m",60]
[]
[362,null,"Cable joints","H4"]
[]
[362,11,"1.5mm² 3-Core","No",2]
[]
[362,12,"16mm² 3-Core","No",2]
[]
[362,null,"Cable terminations","H4"]
[]
[362,13,"1.5mm² 3-Core","No",40]
[]
[362,14,"2.5mm² 3-Core","No",40]
[]
[362,15,"16mm² 3-Core","No",2]
[]
[362,null,"EARTH CONDUCTORS","H3"]
[]
[362,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[362,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[362,16,"6mm²","m",60]
[]
[362,null,"SUNDRIES","H3"]
[]
[362,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[363,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[363,null,"CONDUITS ETC","H3"]
[]
[363,null,"Rigid PVC conduits","H4"]
[]
[363,18,"20mm Diameter","m",1290]
[]
[363,null,"PVC conduit accessories","H4"]
[]
[363,19,"Round outlet box for 20mm conduit","No",129]
[]
[363,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",129]
[]
[363,21,"Standard draw box for 20mm conduit","No",129]
[]
[363,22,"50 x 100 x 50mm Outlet box","No",129]
[]
[363,23,"100 x 100 x 50mm Outlet box","No",129]
[]
[363,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",129]
[]
[363,null,"CONDUCTORS","H3"]
[]
[363,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[363,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[363,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[363,25,"1.5mm²","m",290]
[]
[363,null,"DRAW-WIRES","H3"]
[]
[363,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[363,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[363,27,"Flush mounted bell push button","No",1]
[]
[363,28,"16A Flush mounted two lever one-way switch unit","No",20]
[]
[364,29,"16A Three pin flush mounted socket outlet with switch, single type","No",61]
[]
[364,null,"LUMINAIRES","H3"]
[]
[364,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",68]
[]
[364,31,"1kW 100A Inverter Trolley","No",2]
[]
[364,null,"SUNDRIES","H3"]
[]
[364,32,"Earthing of buildings","Item","1.00"]
[]
[364,33,"Provision of as built drawings","Item","1.00"]
[]
[364,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[366,null,"BILL NO. 14 ","H1"]
[]
[366,null,"GLAZING","H1"]
[]
[366,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[366,null,"Float glass","H4"]
[]
[366,null,"The term \"float glass\" is used for monolithic annealed glass "]
[]
[366,null,"GLAZING TO STEEL WITH PUTTY","H2"]
[]
[366,null,"4mm Clear float glass","H4"]
[]
[366,1,"Panes exceeding 0,1m² and not exceeding 0,5m²","m2",80]
[]
[]
[]
[367,null,"BILL NO. 15","H1"]
[]
[367,null,"PAINTWORK ","H1"]
[]
[367,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[367,null,"PAINT SPECIFICATIONS","H3"]
[]
[367,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[367,null,"COLOURS","H3"]
[]
[367,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[367,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[367,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[367,null,"One coat alkali resistant primer and two coats superior quality acrylic emulsion paint for interior use","H4"]
[]
[367,1,"Walls","m2",944]
[]
[367,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[367,null,"One coat primer, one universal undercoat and two coats exterior quality \"Cemote\" pva paint","H4"]
[]
[367,2,"Ceilings and cornices ","m2",658]
[]
[368,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[368,null,"Two coats extremely durable UV-resistant, washable pure acrylic emulsion sheen paint","H4"]
[]
[368,3,"Fascias and barge boards, including priming metal jointing strips","m2",83]
[]
[368,null,"ON WOOD SURFACES","H2"]
[]
[368,null,"One coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint","H4"]
[]
[368,4,"Laminated beam","m2",42]
[]
[368,5,"Doors","m2",33]
[]
[368,null,"ON METAL SURFACES","H2"]
[]
[368,null,"One coat alkyd based zinc phosphate primer and two coats premium quality polyurethane enamel paint, on steel","H4"]
[]
[368,6,"Door frames","m2",39]
[]
[368,7,"Windows","m2",160]
[]
[]
[]
[370,1,"Earthworks (Provisional)","Page",328]
[]
[370,2,"Concrete, Formwork and Reinforcement","Page",332]
[]
[370,3,"Masonry ","Page",335]
[]
[370,4,"Waterproofing","Page",336]
[]
[370,5,"Roof Coverings","Page",339]
[]
[370,6,"Carpentry and Joinery ","Page",343]
[]
[370,7,"Ceilings, Partitions and Access Flooring","Page",346]
[]
[370,8,"Floor Coverings, Wall Linings, etc.","Page",347]
[]
[370,9,"Ironmongery ","Page",350]
[]
[370,10,"Metalwork","Page",353]
[]
[370,11,"Plastering","Page",354]
[]
[370,12,"Plumbing and Drainage (Provisional)","Page",360]
[]
[370,13,"Electrical work","Page",365]
[]
[370,14,"Glazing","Page",366]
[]
[370,15,"Paintwork ","Page",369]
[]
[371,null,"BILL NO. 1","H1"]
[]
[371,null,"EARTHWORKS","H1"]
[]
[371,null,"SITE CLEARANCE ETC","H2"]
[]
[371,null,"Site clearance","H4"]
[]
[371,1,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",36]
[]
[371,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[371,null,"EXCAVATIONS, ETC","H2"]
[]
[371,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[371,2,"Trenches","m3",3]
[]
[371,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[371,3,"Soft rock","m3","0.3"]
[]
[371,4,"Hard rock","m3","0.2"]
[]
[371,null,"Extra over all excavations for carting away","H4"]
[]
[371,5,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",3]
[]
[371,null,"Risk of collapse of excavations","H4"]
[]
[371,6,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",24]
[]
[371,null,"Keeping excavations free of water","H4"]
[]
[371,7,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[372,null,"FILLING ETC","H2"]
[]
[372,null,"Compaction of surfaces","H4"]
[]
[372,8,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",22]
[]
[372,null,"WEED KILLERS, INSECTICIDES, ETC ","H2"]
[]
[372,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[372,9,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",22]
[]
[]
[]
[374,null,"BILL NO. 2","H1"]
[]
[374,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H1"]
[]
[374,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[374,null,"Cost of tests","H4"]
[]
[374,null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the principal agent.  The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the principal agent.  (Test cubes are measured separately)"]
[]
[374,null,"Formwork","H4"]
[]
[374,null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[374,null,"Formwork to sides of bases, pile caps, ground beams, etc will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[375,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[375,null,"30MPa/19mm concrete","H4"]
[]
[375,1,"Ground beams","m3",4]
[]
[375,2,"Surface beds","m3",3]
[]
[375,3,"Pavings","m3",1]
[]
[375,null,"TEST CUBES","H2"]
[]
[375,4,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",3]
[]
[375,null,"CONCRETE SUNDRIES","H2"]
[]
[375,null,"Finishing top surfaces of concrete smooth with a wood float","H4"]
[]
[375,5,"Surface beds, slabs, etc","m2",15]
[]
[375,null,"Finishing top surfaces of concrete smooth with a power float","H4"]
[]
[375,6,"Surface beds, slabs, etc","m2",22]
[]
[375,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[375,null,"Rough formwork to sides","H4"]
[]
[375,7,"Edges, risers, ends and reveals not exceeding 300mm high","m",20]
[]
[375,null,"MOVEMENT JOINTS ETC","H2"]
[]
[375,null,"Expansion joints with 12mm bitumen impregnated softboard, including raking out polysolphyte sealant ","H4"]
[]
[375,8,"Not exceeding 300mm high through slabs","m",20]
[]
[376,null,"REINFORCEMENT","H2"]
[]
[376,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[376,9,"Bars in various diameter","t","0.32"]
[]
[376,null,"Fabric reinforcement","H4"]
[]
[376,10,"Type 395 fabric reinforcement in concrete surface beds etc","m2",17]
[]
[]
[]
[378,null,"BILL NO. 3","H1"]
[]
[378,null,"MASONRY","H1"]
[]
[378,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[378,null,"BRICKWORK","H3"]
[]
[378,null,"Sizes in descriptions","H4"]
[]
[378,null,"Where sizes in descriptions are given in brick units, \"one brick\" shall represent the length and \"half brick\" the width of a brick"]
[]
[378,null,"BRICKWORK","H2"]
[]
[378,null,"SUPERSTRUCTURE","H2"]
[]
[378,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[378,1,"Piers","m3","0.2"]
[]
[378,2,"One brick walls","m2",20]
[]
[378,null,"BRICKWORK SUNDRIES","H2"]
[]
[378,null,"2,5mm Galvanised brick reinforcement","H4"]
[]
[378,3,"150m Wide reinforcement built in horizontally","m",50]
[]
[378,null,"Prestressed fabricated concrete lintels including necessary temporary supports","H4"]
[]
[378,4,"110 x 75mm Lintels in lengths not exceeding 3m","m",7]
[]
[378,null,"Galvanised wire ties etc","H4"]
[]
[378,5,"4mm Diameter roof tie 2m girth bent double, with one end built into brickwork and other end fixed to timber","No",18]
[]
[378,null,"Air bricks etc","H4"]
[]
[378,6,"229 x 152mm Clay vermin proof air brick","No",3]
[]
[379,7,"233 x 175mm Foam plastic air vent","No",3]
[]
[379,null,"FACE BRICKWORK","H2"]
[]
[379,null,"\"Corobrick Firelight Satin\" face bricks pointed with recessed horizontal and vertical joints","H4"]
[]
[379,8,"Extra over brickwork for face brickwork","m2",28]
[]
[379,9,"Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",7]
[]
[379,null,"Brick-on-edge header course copings, sills, etc of face bricks, pointed with recessed joints on all exposed faces","H4"]
[]
[379,10,"230mm Wide sills set sloping and slightly projecting","m",4]
[]
[]
[]
[381,null,"BILL NO. 4","H1"]
[]
[381,null,"WATERPROOFING","H1"]
[]
[381,null,"DAMPPROOFING OF WALLS AND FLOORS","H2"]
[]
[381,null,"One layer 375 micron embossed polyethylene dampproof course (SANS 952-1985 type B)","H4"]
[]
[381,1,"In walls","m2",3]
[]
[381,null,"One layer 250 micron green polyethylene waterproof sheeting (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape","H4"]
[]
[381,2,"Under surface beds","m2",9]
[]
[381,null,"SEALING STRIPS, JOINT SEALANTS, ETC","H2"]
[]
[381,null,"Two-part grey polysulphide sealing compound including backing cord, bond breaker, primer, etc","H4"]
[]
[381,3,"12 x 10mm In expansion joints in floors including raking out expansion joint filler as necessary","m",16]
[]
[]
[]
[382,null,"BILL NO. 5","H1"]
[]
[382,null,"ROOF COVERINGS","H1"]
[]
[382,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[382,null,"Proprietary items or materials","H3"]
[]
[382,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[382,null,"ROOF COVERINGS","H2"]
[]
[382,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[382,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing (timber purlins measured elsewhere)","H4"]
[]
[382,1,"Roof covering with pitches not exceeding 25 degrees","m2",20]
[]
[382,2,"Ridge cappings 475mm girth ","m",2]
[]
[382,3,"Hip cappings 475mm girth","m",9]
[]
[382,null,"ROOF AND WALL INSULATION","H2"]
[]
[382,null,"Multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with a mass of not less than 293g/mý and a Class I fire rating in accordance with SANS 0177-3","H4"]
[]
[382,4,"Insulation sheeting laid taut over purlins (at approximately 1200mm centres) and fixed concurrent with roof covering with minimum 150mm stapled laps including galvanised steel straining wires at not exceeding 400mm centres and double-sided tape at edges where required","m2",20]
[]
[]
[]
[383,null,"BILL NO. 6","H1"]
[]
[383,null,"CARPENTRY AND JOINERY","H1"]
[]
[383,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[383,null,"Fixing","H4"]
[]
[383,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[383,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[383,null,"Joinery","H4"]
[]
[383,null,"Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts "]
[]
[383,null,"ROOFS ETC","H2"]
[]
[383,null,"PLATE NAILED TIMBER ROOF TRUSS CONSTRUCTION ETC","H2"]
[]
[383,null,"SUPPLEMENTARY PREAMBLES","H4"]
[]
[383,null,"Trusses are at maximum 1200mm centres"]
[]
[383,null,"Roof covering is 0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to timber purlins with equal spacing. "]
[]
[383,null,"Ceilings are 6,4mm rhinoboard on 38 x 38mm brandering"]
[]
[384,null,"Dimensions in descriptions of trusses are nominal and actual measurements are to be obtained from the architect/engineer and/or taken on site before design or fabrication commences"]
[]
[384,1,"Supply and install prefabricated hip timber roof structure system complete and in accordance with the Standard Building Regulations, including wall plates, purlins, bracing etc. and 700mm eaves projection on all sides. Building size: 3850 x 2400mm wide.","No",1]
[]
[384,null,"Sundries","H4"]
[]
[384,2,"Wrought faces on sawn timbers","m2",4]
[]
[384,3,"Two coats creosote on sawn timbers ","m2",4]
[]
[384,null,"EAVES, VERGES, ETC","H2"]
[]
[384,null,"Medium density plain fibre-cement fascias and barge boards","H4"]
[]
[384,4,"12 x 225mm Medium density fascia boards including galvanised H-profile jointing strips tied with and including hot dipped galvanised screws and washers","m",17]
[]
[384,null,"TIMBER DOORS, WINDOWS, ETC","H2"]
[]
[384,null,"Wrought meranti doors hung to timber frames","H4"]
[]
[384,5,"44mm Framed, ledged and braced batten door 813 x 2032mm high of 40 x110mm wide top rail and stiles, 20 x 150mm middle ledge and braces and 20 x 225mm bottom ledge, filled in with 22mm tongued and grooved V-jointed one side vertical boarding with tongued and grooved joints to top rail and stiles and with inner edges of framing and abutting edges of boarding chamfered to form V-joint","No",1]
[]
[384,null,"FITTINGS","H2"]
[]
[384,6,"Counter/cupboard 2000 x 900mm high with top, sides, bottom, division, shelf, back and hinged doors, dividing framework and drawers etc.","No",1]
[]
[]
[]
[386,null,"BILL NO. 7","H1"]
[]
[386,null,"CEILINGS, PARTITIONS AND ACCESS FLOORING","H1"]
[]
[386,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[386,null,"Fixing","H4"]
[]
[386,null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete"]
[]
[386,null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as \"bolted\", the bolts have been given elsewhere"]
[]
[386,null,"Ceilings","H4"]
[]
[386,null,"Unless otherwise described ceilings shall be deemed to be horizontal "]
[]
[386,null,"Proprietary items or materials","H3"]
[]
[386,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[386,null,"NAILED-UP CEILINGS","H2"]
[]
[386,null,"6,4mm Fibre-cement plain ceiling boards with H-profile galvanised steel jointing strips ","H4"]
[]
[386,1,"Ceilings including 38 x 38mm sawn softwood brandering at 400mm centres","m2",8]
[]
[386,2,"Extra over ceiling for 600 x 600mm trap door of 38 x 38mm wrought softwood rebated framing with one cross brander, covered with ceiling board and fitted flush in opening, including necessary trimmers around","No",1]
[]
[387,null,"Gypsum plasterboard cornices","H4"]
[]
[387,3,"75mm Coved cornices","m",16]
[]
[]
[]
[389,null,"BILL NO. 8","H1"]
[]
[389,null,"FLOOR COVERINGS, WALL LININGS, ETC","H1"]
[]
[389,null,"FLOOR COVERINGS","H2"]
[]
[389,null,"300 x 300 x 2.5mm Semi flexible vinyl tiles","H4"]
[]
[389,1,"On floors ","m2",5]
[]
[389,null,"Vinyl skirtings, nosings, etc","H4"]
[]
[389,2,"70mm High vinyl skirting ","m",8]
[]
[389,null,"POLISH, SEALERS, ETC","H2"]
[]
[389,3,"Three coats wax polish on vinyl flooring ","m2",5]
[]
[]
[]
[390,null,"BILL NO. 9","H1"]
[]
[390,null,"IRONMONGERY","H1"]
[]
[390,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[390,null,"Proprietary items","H4"]
[]
[390,null,"Where applicable the manufacturers' names or product catalogue titles are given in sub-headings preceding the items  Prices are to be based on the specific products/articles specified.  If tenderers wish to offer alternative products/articles for certain items, these items are to be clearly marked and the alternative specification given with supporting brochures etc clarifying the features of the products/articles offered  On request returnable samples are to be provided to the principal agent for consideration"]
[]
[390,null,"Finishes to ironmongery","H4"]
[]
[390,null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list: BS Satin bronze lacqueredCH Chromium plated SC Satin chromium plated SE Silver enamelled GE Grey enamelledAN Anodised natural AS Anodised silver AB Anodised bronze AG Anodised gold ABL Anodised black PB Polished brass PL Polished and lacquered PT Epoxy coated SD Sanded"]
[]
[391,null,"Proprietary items or materials","H3"]
[]
[391,null,"Proprietary items or materials where specified are to be of the brand specified - or other approved - by the Head"]
[]
[391,null,"LOCKS","H2"]
[]
[391,null,"Manufactured by \"Union\"","H4"]
[]
[391,1,"Solid art 390/313 Four Lever mortice lockset with and including Satin Chrome Plated handles","No",1]
[]
[391,null,"SUNDRIES","H2"]
[]
[391,null,"Manufactured by \"Union\"","H4"]
[]
[391,2,"38mm Diameter door stop plugged and screwed to floor with a 50mm long brass screw","No",1]
[]
[]
[]
[393,null,"BILL NO. 10","H1"]
[]
[393,null,"METALWORK","H1"]
[]
[393,null,"GALVANISED STEEL GATES, SCREENS, ETC","H2"]
[]
[393,null,"Welded screens and gates ","H4"]
[]
[393,1,"Single hot dipped galvanised mild steel gate, 980mm x 2032mm formed of 40 x 60 x 3mm hollow sectioned frames and midrail, filled in with 12mm solid square vertical bars at 110mm centres including all ironmongery to fix on wall and padlock set","No",1]
[]
[393,null,"GALVANISED PRESSED STEEL DOOR FRAMES","H2"]
[]
[393,null,"Double rebated frames suitable for one brick walls","H4"]
[]
[393,2,"Frame for door 813 x 2032mm high","No",1]
[]
[393,null,"GALVANISED STEEL WINDOWS, DOORS, ETC","H2"]
[]
[393,null,"Standard school windows with flat burglar bars to opening sashes","H4"]
[]
[393,3,"Window size, 1022 x 949mm high","No",2]
[]
[393,4,"Window size, 1511 x 949mm high","No",1]
[]
[393,null,"FENCING","H2"]
[]
[393,null,"Galvanised pre-painted \"clear Vu\" fence with steel droppers, posts, gates post etc. including galvanised steel bolts, straining, eye bolts, etc.","H4"]
[]
[393,5,"Fence 2,05m high","m",1300]
[]
[393,6,"\"Clear Vu\" gate size 900 x2032mm high to match fencing profile, including hinges, heavy duty lockable bolt and 50mm brass padlock","No",1]
[]
[]
[]
[394,null,"BILL NO. 11","H1"]
[]
[394,null,"PLASTERING","H1"]
[]
[394,null,"SCREEDS","H2"]
[]
[394,null,"Screeds steel trowelled, on concrete","H4"]
[]
[394,1,"30mm Thick on floors and landings","m2",8]
[]
[394,null,"GRANOLITHIC","H2"]
[]
[394,null,"Untinted granolithic, on concrete","H4"]
[]
[394,2,"30mm Thick on floors and landings","m2",3]
[]
[394,null,"INTERNAL PLASTER","H2"]
[]
[394,null,"Cement plaster steel trowelled, on brickwork","H4"]
[]
[394,3,"On walls","m2",17]
[]
[394,4,"On narrow widths","m2",1]
[]
[]
[]
[395,null,"BILL NO. 12","H1"]
[]
[395,null,"PLUMBING AND DRAINAGE (PROVISIONAL)","H1"]
[]
[395,null,"RAINWATER DISPOSAL","H2"]
[]
[395,null,"Seamless aluminium prepainted gutters and rainwater pipes","H4"]
[]
[395,1,"150mm Half-round roof gutters with beaded front edge","m",17]
[]
[395,2,"100mm Diameter rainwater pipes","m",8]
[]
[395,3,"Extra over gutter for outlet for 100mm pipe","No",2]
[]
[395,4,"Extra over rainwater pipe for bend","No",6]
[]
[395,5,"Extra over rainwater pipe for shoe","No",2]
[]
[395,null,"STORMWATER CHANNELS","H2"]
[]
[395,null,"Earthworks","H4"]
[]
[395,6,"Excavate average 125mm deep in earth to form \"V\" drain profile","m3",3]
[]
[395,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[395,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[395,7,"\"V\" drains","m3",3]
[]
[395,8,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",22]
[]
[395,9,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",26]
[]
[396,10,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",22]
[]
[396,11,"10 x 150mm Pre-compressed bitumen impregnated foam plastic joint sealing strips between brickwork and concrete","m",18]
[]
[396,null,"FIRE APPLIANCES ETC","H2"]
[]
[396,12,"9kg Dry chemical powder fire extinguisher","No",2]
[]
[]
[]
[398,null,"BILL NO. 13","H1"]
[]
[398,null,"ELECTRICAL WORK","H1"]
[]
[398,null,"BLOCK X","H2"]
[]
[398,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[398,null,"Distribution boards etc","H4"]
[]
[398,null,"Rates for distribution boards etc are to include for busbars, jumpers, neutral bars, internal wiring and connections, circuit identification markers, control gear labels, circuit legend cards and working drawings"]
[]
[398,null,"Switches, socket outlets, etc","H4"]
[]
[398,null,"Rates for switches, socket outlets, etc are to include for screwing to outlet boxes, connecting up and cover plates"]
[]
[398,null,"Light fittings","H4"]
[]
[398,null,"Rates for light fittings are to include for hanging, fixing and connecting and for lamp holders and fluorescent tubes and lamps of the type and wattage described"]
[]
[398,null,"LOW TENSION DISTRIBUTION","H2"]
[]
[398,null,"DISTRIBUTION BOARD DB","H3"]
[]
[398,1,"Surface type floor mounted distribution board, in two sections (Main supply with electrical meter) and the second section is for distribution supply, 1000mm wide x 200mm deep x 950mm high, fitted with doors and 20mm thick timber board on the inside to cover the full area, the board colour coded and installed in electrical cupboard","No",1]
[]
[398,2,"iC60N 63A 4P CB (A9F44363)","No",1]
[]
[398,3,"iC60N 32A 4P CB (A9F44432)","No",1]
[]
[398,4,"iC60N 16A DP CB (AF74616)","No",6]
[]
[399,5,"3P (N/O) CONTACTOR (LC1E3210U5)","No",1]
[]
[399,6,"QAT-TRDM TIME SWITCH (QAT-TRDM)","No",1]
[]
[399,7,"Surge arrester, 3P+N, 350V (A9L20600)","No",1]
[]
[399,null,"CABLES","H3"]
[]
[399,8,"1.5mm² 3-Core","m",50]
[]
[399,9,"2.5mm² 3-Core","m",30]
[]
[399,10,"16mm² 3-Core","m",60]
[]
[399,null,"Cable joints","H4"]
[]
[399,11,"1.5mm² 3-Core","No",2]
[]
[399,12,"16mm² 3-Core","No",2]
[]
[399,null,"Cable terminations","H4"]
[]
[399,13,"1.5mm² 3-Core","No",40]
[]
[399,14,"2.5mm² 3-Core","No",40]
[]
[399,15,"16mm² 3-Core","No",2]
[]
[399,null,"EARTH CONDUCTORS","H3"]
[]
[399,null,"Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[399,null,"PVC insulated copper earth conductors laid with cables in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres","H4"]
[]
[399,16,"6mm²","m",60]
[]
[399,null,"SUNDRIES","H3"]
[]
[399,17,"Low tension room accessories comprising first aid kit, pair of rubber gloves and notices on door and inside the room complying with the Occupational Health and Safety Act, 1993","No",1]
[]
[400,null,"GENERAL LIGHTING AND POWER","H2"]
[]
[400,null,"CONDUITS ETC","H3"]
[]
[400,null,"Rigid PVC conduits","H4"]
[]
[400,18,"20mm Diameter","m",80]
[]
[400,null,"PVC conduit accessories","H4"]
[]
[400,19,"Round outlet box for 20mm conduit","No",8]
[]
[400,20,"Deep type (concrete type) round outlet box for 20mm conduit","No",8]
[]
[400,21,"Standard draw box for 20mm conduit","No",8]
[]
[400,22,"50 x 100 x 50mm Outlet box","No",8]
[]
[400,23,"100 x 100 x 50mm Outlet box","No",8]
[]
[400,24,"100 x 100 x 50mm Outlet box with blank cover plate","No",8]
[]
[400,null,"CONDUCTORS","H3"]
[]
[400,null,"Bare copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[400,null,"PVC insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[400,null,"Heat resistant silicon insulated stranded copper conductors drawn into conduit, trunking or power skirting","H4"]
[]
[400,25,"1.5mm²","m",290]
[]
[400,null,"DRAW-WIRES","H3"]
[]
[400,26,"Galvanised steel draw-wires drawn into conduit","m",290]
[]
[400,null,"LIGHT SWITCHES, SOCKET OUTLETS, ETC","H3"]
[]
[400,27,"Flush mounted bell push button","No",1]
[]
[400,28,"16A Flush mounted two lever one-way switch unit","No",2]
[]
[401,29,"16A Three pin flush mounted socket outlet with switch, single type","No",3]
[]
[401,null,"LUMINAIRES","H3"]
[]
[401,30,"Lascon V1-100BC/C/Plas economy injection moulded polycarbonate luminaire with 100W GLS lamp","No",5]
[]
[401,31,"1kW 100A Inverter Trolley","No",2]
[]
[401,null,"SUNDRIES","H3"]
[]
[401,32,"Earthing of buildings","Item","1.00"]
[]
[401,33,"Provision of as built drawings","Item","1.00"]
[]
[401,34,"Testing and commissioning the complete electrical installation","Item","1.00"]
[]
[]
[]
[403,null,"BILL NO. 14 ","H1"]
[]
[403,null,"GLAZING","H1"]
[]
[403,null,"GLAZING TO STEEL WITH PUTTY","H2"]
[]
[403,null,"4mm Clear float glass","H4"]
[]
[403,1,"Panes exceeding 0,1m² and not exceeding 0,5m²","m2",3]
[]
[]
[]
[404,null,"BILL NO. 15","H1"]
[]
[404,null,"PAINTWORK","H1"]
[]
[404,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[404,null,"PAINT SPECIFICATIONS","H3"]
[]
[404,null,"All painting shall be done in accordance with manufacturer's specifications unless otherwise described"]
[]
[404,null,"COLOURS","H3"]
[]
[404,null,"Unless otherwise described paintwork on ceilings shall be deemed to be in the \"White\" colour group and paintwork on all other components shall be deemed to be in the \"Pastel\" colour group in accordance with the Natural Colour System (NCS) adopted by the SA National Standards"]
[]
[404,null,"PAINTWORK ETC TO NEW WORK","H2"]
[]
[404,null,"ON INTERNAL FLOATED PLASTER SURFACES","H2"]
[]
[404,null,"One coat alkali resistant primer and two coats PVA emulsion paint for interior use","H4"]
[]
[404,1,"Walls","m2",18]
[]
[404,null,"ON PLASTERBOARD SURFACES","H2"]
[]
[404,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[404,2,"Ceilings and cornices","m2",8]
[]
[405,null,"ON FIBRE-CEMENT BOARD SURFACES","H2"]
[]
[405,null,"One coat primer and two coats superior quality acrylic emulsion paint for interior and exterior use","H4"]
[]
[405,3,"Fascias and barge boards, including priming metal jointing strips","m2",8]
[]
[405,null,"ON WOOD SURFACES","H2"]
[]
[405,null,"Three coats superior quality clear matt varnish","H4"]
[]
[405,4,"Doors","m2",3]
[]
[]
[]
[407,1,"Earthworks (Provisional)","Page",373]
[]
[407,2,"Concrete, Formwork and Reinforcement ","Page",377]
[]
[407,3,"Masonry ","Page",380]
[]
[407,4,"Waterproofing","Page",381]
[]
[407,5,"Roof Coverings","Page",382]
[]
[407,6,"Carpentry and Joinery","Page",385]
[]
[407,7,"Ceilings, Partitions and Access Flooring","Page",388]
[]
[407,8,"Floor Coverings, Wall Linings, etc.","Page",389]
[]
[407,9,"Ironmongery","Page",392]
[]
[407,10,"Metalwork","Page",393]
[]
[407,11,"Plastering ","Page",394]
[]
[407,12,"Plumbing and Drainage (Provisional)","Page",397]
[]
[407,13,"Electrical work","Page",402]
[]
[407,14,"Glazing","Page",403]
[]
[407,15,"Paintwork","Page",406]
[]
[408,null,"BILL NO. 1","H1"]
[]
[408,null,"EXTERNAL WORK","H1"]
[]
[408,null,"TEMPORARY PARKHOMES","H2"]
[]
[408,null,"\"M-Projects\" or other equal approved temporary parkhome unit","H4"]
[]
[408,null,"Rates for the following Parkhomes to include standard windows, burglar bars, curtains and tracks, two tier steps for access, light fittings and green chalk boards:"]
[]
[408,1,"Provide standard classroom size 7000 x 7000mm temporary parkhomes or nearest size on site for rental and maintenance for educational facilities during construction phase including levelling, positioning on site and connection to an electrical supply including issuing of compliance certificates for a period of 30 months and removal after construction period expires.","No",16]
[]
[408,2,"Transport to and from site of parkhomes as per distance between supplier and site","No",16]
[]
[408,null,"Rates for the following Parkhomes to include standard windows, burglar bars, curtains and tracks, two tier steps for access, light fittings,sanitary fittings, water supply and soil drainages piping including connections:"]
[]
[408,3,"Provide standard toilets temporary parkhomes on site for rental and maintenance during construction phase to serve as a \"Teachers toilets\" including levelling, positioning on site and connection to an electrical supply, drainage system, water supply including issuing of compliance certificates for a period of 8 months and removal from site after construction period expires ","No",1]
[]
[408,4,"Transport to and from site of parkhomes as per distance between supplier and site","No",1]
[]
[409,null,"RELOCATING OF EXISTING PARKHOME CLASSROOMS","H2"]
[]
[409,5,"Move/shift existing 7000 x 7000mm classroom park home from one area to another inside the school premises. Distance between the areas is approximately 200m, including levelling and setting up the new area","No",2]
[]
[409,null,"EXTERNAL WORKS","H1"]
[]
[409,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[409,null,"View site","H4"]
[]
[409,null,"Before submitting his tender the contractor shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials contained in the buildings or portions of the buildings to be demolished.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained"]
[]
[409,null,"Explosives","H4"]
[]
[409,null,"No explosives whatsoever may be used for demolition purposes unless otherwise stated"]
[]
[409,null,"General","H4"]
[]
[409,null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants. He shall provide proper protection and provide, erect and remove when directed, any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent"]
[]
[409,null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the principal agent"]
[]
[410,null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items"]
[]
[410,null,"Unless otherwise described all materials are to become the property of the contractor and are to be removed from the site"]
[]
[410,null,"Removal of materials","H4"]
[]
[410,null,"Where removal is included in the heading, sub-heading or item description, prices shall be deemed to include for the necessary costs in removal and appropriate disposal of materials including but not limited to labour, transportation and disposal costs. No further claims in this regard will be entertained."]
[]
[411,null,"Removal of asbestos material ","H4"]
[]
[411,null,"The removal of asbestos shall be carried out strictly by a certified entity, registered in accordance with the Occupational Health and Safety Act and the Asbestos Regulation.  Asbestos in all forms/building elements that is to be removed, shall be carried out in strict accordance with aforementioned regulation, and a certificate issued by the entity as contemplated in the above, shall be provided per block for the removal thereof, where the term block shall in this context refer to any single, free standing building structure, regardless of size or purpose.  Corresponding disposal certificates shall be issued by the facility at which the asbestos is disposed of, with said facility to, prior to the disposal of any asbestos material provide satisfactory proof that the facility is duly registered and fully compliant in terms of the act, to receive the asbestos material.  Under no circumstances is the contractor nor any of his duly authorised representatives to sell and/or give away asbestos material to any member/s of the school community, the community in general or the public at large. Should this be found to be occurring, the contractor will be held responsible contractually and may further be prosecuted criminally.  The cost for complying with the above, and all requirements of regulation as reflected above is to be priced for in the items for removal of asbestos material. No further claims in this regard will therefore be entertained."]
[]
[411,null,"DEMOLITIONS ETC","H1"]
[]
[411,null,"Taking down and removing","H4"]
[]
[411,6,"Security wire fence with pedestrians and vehicles gates including removing fence and gates posts","m",600]
[]
[412,null,"Demolishing and removing","H4"]
[]
[412,7,"Single storey building 620m² on plan and 2,8m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and asbestos roof sheets including carting away of all material","No",1]
[]
[412,8,"Single storey building 91m² on plan and 2,8m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and asbestos roof sheets including carting away of all material","No",1]
[]
[412,9,"Single storey building 180m² on plan and 2,6m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and asbestos roof sheets including carting away of all material","No",1]
[]
[412,10,"Single storey building 146m² on plan and 2,70m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and asbestos roof sheets including carting away of all material","No",1]
[]
[412,11,"Single storey building 146m² on plan and 2,70m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and asbestos roof sheets including carting away of all material","No",1]
[]
[412,12,"Single storey building 20m² on plan and 2,6m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and corrugated roof sheets including carting away of all material","No",1]
[]
[412,13,"Single storey building 4m² on plan and 2,6m high to eaves comprising two gable ends, reinforced concrete foundations and surface bed, 190mm external and internal block walls, timber roof structure and asbestos roof sheets including carting away of all material","No",1]
[]
[413,null,"LANDSCAPING","H1"]
[]
[413,null,"Note: Landscaping to be completed at least three months before final completion of the project for maintenance allowance","H3"]
[]
[413,null,"Excavate in earth and dispose on site","H4"]
[]
[413,14,"Not exceeding 150mm deep to remove humps, form shallow ditches, etc","m2",10400]
[]
[413,null,"Ground preparation","H4"]
[]
[413,15,"Cultivation and preparation of areas to be planted","m2",10400]
[]
[413,null,"Topsoil supplied by the contractor, including spreading and levelling","H4"]
[]
[413,16,"In plant beds, grassed areas and holes for trees, shrubs, etc","m3",1560]
[]
[413,null,"Compost, lime and fertilizer","H4"]
[]
[413,17,"Compost in plant beds, holes for trees, shrubs, etc","m3",832]
[]
[413,null,"Trees","H4"]
[]
[413,18,"Acacia melanoxylon 600mm high","No",15]
[]
[413,null,"Grassing, ground covers, etc","H4"]
[]
[413,19,"\"Kikuyu\" rolls or other similar approved 50mm thick","m2",10400]
[]
[413,null,"Rockery boulders","H4"]
[]
[413,20,"Rockery boulder approximately 400mm diameter supplied by the contractor","No",600]
[]
[413,null,"Maintenance","H4"]
[]
[413,21,"Allow for maintaining landscaping for a period of 2 months, including watering, weeding, cutting, replacing dead plants, etc","Item","1.00"]
[]
[414,null,"ROADWORK, PARKING AREAS AND PAVING","H1"]
[]
[414,null,"DRIVEWAY","H2"]
[]
[414,null,"SUPPLEMENTARY PREAMBLES","H3"]
[]
[414,null,"Testing of material and filling","H4"]
[]
[414,null,"Descriptions of earth filling, compaction, etc shall be deemed to include for all necessary testing required in accordance with the SABS 1200 series"]
[]
[414,null,"Site clearance","H4"]
[]
[414,22,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",562]
[]
[414,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[414,23,"Reduced levels under floors","m3",242]
[]
[414,null,"Extra over bulk excavation in earth for excavation in","H4"]
[]
[414,24,"Soft rock","m3",24]
[]
[414,25,"Hard rock","m3",12]
[]
[414,null,"Extra over all excavations for carting away","H4"]
[]
[414,26,"Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",562]
[]
[414,null,"Earth filling supplied by the contractor under parking areas, roadways, etc","H4"]
[]
[414,27,"Filling of G5 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",73]
[]
[414,28,"Filling of G6 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",73]
[]
[414,29,"Filling of G9 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",84]
[]
[415,30,"Filling of G10 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",84]
[]
[415,null,"Compaction of surfaces","H4"]
[]
[415,31,"Compaction of ground surfaces under pavings etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",562]
[]
[415,32,"Apply \"Weedmaster Turfmaster\" weedkiller (at a rate of 40-45ml to 5 litres of water per 50m²) to surface of ground","m2",562]
[]
[415,null,"Prescribed density tests on filling","H4"]
[]
[415,33,"In-situ dry density test in accordance with method A10(b) of TMH1","No",5]
[]
[415,34,"Maximum dry density and optimum moisture content test in accordance with method A7 of TMH1","No",5]
[]
[415,35,"CBR test in accordance with method A8 of TMH1","No",5]
[]
[415,null,"Bituminous premix road surfacing","H4"]
[]
[415,36,"Prime coat","m2",562]
[]
[415,37,"30mm Thick asphalt surface paving to parking areas, roadways, etc","m2",562]
[]
[415,null,"Precast concrete finished smooth on exposed surfaces, including bedding, jointing and pointing","H4"]
[]
[415,38,"150 x 300mm High kerbs (SANS 927 fig 6) with 150 x 150 x 300mm unreinforced concrete haunching at back of each joint, including excavation, backfilling, etc","m",430]
[]
[416,null,"PARKING & ASSEMBLY AREA","H2"]
[]
[416,null,"SUPPLEMENTARY PREAMBLES","H3"]
[]
[416,null,"Testing of material and filling","H4"]
[]
[416,null,"Descriptions of earth filling, compaction, etc shall be deemed to include for all necessary testing required in accordance with the SABS 1200 series"]
[]
[416,null,"Site clearance","H4"]
[]
[416,39,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",2056]
[]
[416,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[416,40,"Reduced levels under floors","m3",884]
[]
[416,null,"Extra over bulk excavation in earth for excavation in","H4"]
[]
[416,41,"Soft rock","m3",88]
[]
[416,42,"Hard rock","m3",44]
[]
[416,null,"Extra over all excavations for carting away","H4"]
[]
[416,43,"Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",884]
[]
[416,null,"Earth filling supplied by the contractor under parking areas, roadways, etc","H4"]
[]
[416,44,"Bedding river and top soil mix compacted to 93% Mod AASHTO density","m3",82]
[]
[416,45,"Filling of G5 material in accordance with SABS 1200 DM, compacted to 93% Mod AASHTO density","m3",501]
[]
[416,46,"Filling of G6 material in accordance with SABS 1200 DM, compacted to 93% Mod AASHTO density","m3",308]
[]
[416,47,"Filling of G9 material in accordance with SABS 1200 DM, compacted to 93% Mod AASHTO density","m3",206]
[]
[417,null,"Compaction of surfaces","H4"]
[]
[417,48,"Compaction of ground surfaces under pavings etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",2056]
[]
[417,49,"Apply \"Weedmaster Turfmaster\" weedkiller (at a rate of 40-45ml to 5 litres of water per 50m²) to surface of ground","m2",2056]
[]
[417,null,"Prescribed density tests on filling","H4"]
[]
[417,50,"In-situ dry density test in accordance with method A10(b) of TMH1","No",5]
[]
[417,51,"Maximum dry density and optimum moisture content test in accordance with method A7 of TMH1","No",5]
[]
[417,52,"CBR test in accordance with method A8 of TMH1","No",5]
[]
[417,null,"Precast concrete paving of 500 x 500 x 40mm precast concrete paving slabs with smooth finish laid on 50mm thick river sand bed including preparation of ground filling","H4"]
[]
[417,53,"Paving slabs laid with butt joints","m2",2056]
[]
[417,null,"Precast concrete finished smooth on exposed surfaces, including bedding, jointing and pointing","H4"]
[]
[417,54,"150 x 300mm High kerbs (SANS 927 fig 6) with 150 x 150 x 300mm unreinforced concrete haunching at back of each joint, including excavation, backfilling, etc","m",657]
[]
[418,null,"COVERED WALKWAY","H1"]
[]
[418,null,"SITE CLEARANCE","H2"]
[]
[418,null,"Site clearance","H4"]
[]
[418,55,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",1097]
[]
[418,56,"Stripping average 50mm thick layer of top soil and depositing material in prescribed stock piles on site","m2",1097]
[]
[418,null,"EXCAVATION, FILLING, ETC OTHER THAN BULK","H2"]
[]
[418,null,"EXCAVATIONS, ETC","H3"]
[]
[418,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[418,57,"Thickening under surface beds, etc","m3",549]
[]
[418,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[418,58,"Soft rock","m3",55]
[]
[418,59,"Hard rock","m3",27]
[]
[418,null,"Extra over all excavations for carting away","H4"]
[]
[418,60,"Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",549]
[]
[418,null,"Keeping excavations free of water","H4"]
[]
[418,61,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[418,null,"FILLING ETC","H3"]
[]
[418,null,"Earth filling supplied by the contractor under parking areas, roadways, etc","H4"]
[]
[418,62,"Bedding river and top soil mix compacted to 93% Mod AASHTO density","m3",44]
[]
[419,63,"Filling of G5 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",165]
[]
[419,64,"Filling of G6 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",165]
[]
[419,65,"Filling of G9 material in accordance with SABS 1200 DM, compacted to 98% Mod AASHTO density","m3",110]
[]
[419,null,"Compaction of surfaces","H4"]
[]
[419,66,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",1097]
[]
[419,null,"WEED KILLERS, INSECTICIDES, ETC ","H3"]
[]
[419,null,"Weedkiller (active ingredients metalaclor 102,8 g/l, terbitilasien 248,6 g/l and atrasien 248,6 g/l) mixed in the proportion of 100 ml weedkiller to 100 l water and applied at a rate of 10 l/mý","H4"]
[]
[419,67,"Under paving etc","m2",1097]
[]
[419,null,"CONCRETE, FORMWORK AND REINFORCEMENT","H2"]
[]
[419,null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2"]
[]
[419,null,"25MPa/19mm concrete","H4"]
[]
[419,68,"Surface beds","m3",143]
[]
[419,69,"Surface bed thickening","m3",84]
[]
[419,null,"TEST CUBES","H2"]
[]
[419,70,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",18]
[]
[420,null,"CONCRETE SUNDRIES","H2"]
[]
[420,null,"Finishing top surfaces of concrete smooth with a wood float","H4"]
[]
[420,71,"Surface beds, slabs, etc","m2",1075]
[]
[420,null,"ROUGH FORMWORK (DEGREE OF ACCURACY III)","H2"]
[]
[420,null,"Rough formwork to sides","H4"]
[]
[420,72,"Edges, risers, ends and reveals exceeding 300mm high or wide","m2",340]
[]
[420,null,"MOVEMENT JOINTS ETC","H2"]
[]
[420,null,"Expansion joints with 22mm soft board between vertical concrete and brick surface","H4"]
[]
[420,73,"Exceeding 300mm high to edges of surface beds","m2",313]
[]
[420,null,"REINFORCEMENT","H2"]
[]
[420,null,"Fabric reinforcement","H4"]
[]
[420,74,"Type 395 fabric reinforcement in concrete surface beds etc","m2",11]
[]
[420,null,"WATERPROOFING","H2"]
[]
[420,null,"SEALING STRIPS, JOINT SEALANTS, ETC","H2"]
[]
[420,null,"Pre compressed bitumen impregnated foam plastic joint sealing strips","H4"]
[]
[420,75,"22 x 45mm In joints between concrete slab and walls     ","m",122]
[]
[421,null,"ROOF COVERINGS","H2"]
[]
[421,null,"PROFILED METAL SHEETING AND ACCESSORIES","H2"]
[]
[421,null,"0.50mm - G550 AZ150, ColorPlus® Steel IBR with integral stiffening rib steel roof sheeting and accessories with ColorPlus® and ZincAL® finish on one side and protective primer coating on the reverse side fixed to steel purlins or rails","H4"]
[]
[421,76,"Roof covering with pitches not exceeding 25 degrees","m2",1174]
[]
[421,77,"10 x 250 x 8mm Thick formed aluminium fascia/gutter combination","m",803]
[]
[421,null,"GALVANISED STRUCTURAL STEEL WORK","H2"]
[]
[421,78,"50 x 50 x 3mm  Equal angle","t","8.07"]
[]
[421,79,"100 x 50 x 20 x 3mm Cold formed channels","t","8.56"]
[]
[421,80,"50 x 50 x 4Cold formed square hollow","t","1.73"]
[]
[421,81,"M16 Expansion bolts","No",776]
[]
[421,null,"REPAIRS TO COMBI COURT ","H1"]
[]
[421,null,"Breaking up and removing","H4"]
[]
[421,82,"40mm Thick tarmacadam paving","m2",450]
[]
[421,83,"Plastic coated diamond mesh wire fence with steel posts","m",90]
[]
[421,null,"New paving","H4"]
[]
[421,84,"Base course of crushed stone in accordance with SABS 1200 ME compacted to 98% Mod AASHTO density","m3",36]
[]
[422,null,"Compaction of surfaces","H4"]
[]
[422,85,"Compaction of ground surfaces under pavings etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",450]
[]
[422,null,"Bituminous premix road surfacing","H4"]
[]
[422,86,"40mm Thick to parking areas, roadways, etc","m2",450]
[]
[422,87,"1,000 x 180 x 180mm Precast concrete barrier kerb set in ground","m",90]
[]
[422,null,"Paintwork","H4"]
[]
[422,null,"Prepare and apply one coat white reflection road marking paint on bituminous road surfacing, precast concrete paving blocks, etc.","H4"]
[]
[422,88,"80mm Wide lines","m",178]
[]
[422,89,"80mm Wide lines circular on plan","m",44]
[]
[422,null,"Fence enclosure","H4"]
[]
[422,null,"Galvanised plastic coated diamond mesh fence with steel pipe posts, stays, gates etc. including galvanised steel bolts straining eyebolts etc.,site clearance and preparation of ground","H4"]
[]
[422,90,"Fence 2,4m high of four strands 3mm diameter straining wire tied to posts and eye bolts and the vertical height covered with plastic coated diamond wire mesh tied at 450mm centres to each straining wire","m",90]
[]
[422,91,"Extra over 40mm diameter straining and gate posts 2,5m long vertically including base","No",4]
[]
[422,92,"Gate of 40mm diameter framing 800 x 2000mm high vertically with one diagonal brace, the vertical section covered with plastic coated diamond mesh fence including hinges, lockable barrel bolt etc","No",1]
[]
[423,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[423,93,"\"V\" drains","m3",12]
[]
[423,94,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",93]
[]
[423,95,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",186]
[]
[423,96,"Type 193 fabric reinforcement in concrete surface beds etc ","m2",193]
[]
[424,null,"SPORTS FACILITIES ","H1"]
[]
[424,null,"OUT DOOR CHESS","H3"]
[]
[424,null,"Compaction of surfaces","H4"]
[]
[424,97,"Compaction of ground surfaces under floor etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",49]
[]
[424,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[424,98,"Under floors etc including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",49]
[]
[424,null,"25MPa/19mm Concrete","H4"]
[]
[424,99,"Pavings","m3",2]
[]
[424,null,"Finishing top surfaces of concrete smooth with wood float","H4"]
[]
[424,100,"Surface beds, slabs, etc","m2",19]
[]
[424,null,"Rough formwork to sides","H4"]
[]
[424,101,"Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",19]
[]
[424,null,"Fabric reinforcement","H4"]
[]
[424,102,"Type 193 fabric reinforcement in concrete surface beds etc","m2",19]
[]
[424,null,"Precast concrete paving of 600 x 600 x 40mm precast concrete paving slabs with smooth finish laid on 50mm thick river sand bed including preparation of ground filling","H4"]
[]
[424,103,"Paving slabs laid with butt joints","m2",23]
[]
[425,104,"10 x 100mm Bitumen impregnated foam plastic joint sealing between precast concrete slab and concrete paving","m",19]
[]
[425,105,"200 x 305mm Copper alphabet cast into concrete","No",16]
[]
[425,106,"200 x 305mm Copper numeral cast into concrete","No",16]
[]
[425,null,"One coat alkali resistant primer, one universal undercoat and two coats quality Pva paint","H4"]
[]
[425,107,"Undercoat and two finishing coats matt enamel paint, colour black on alternate precast concrete slabs","m2",12]
[]
[425,null,"SEATING AND STAIRS","H1"]
[]
[425,null,"DETAIL 2 ","H2"]
[]
[425,null,"Concrete, Formwork and Reinforcing","H2"]
[]
[425,null,"25MPa/19mm Concrete","H4"]
[]
[425,108,"Steps, urinal steps, cupboard platforms, etc","m3",34]
[]
[425,null,"Concrete sundries","H4"]
[]
[425,109,"Finishing top surfaces of concrete smooth with steel trowel","m2",22]
[]
[425,null,"Rough formwork to sides","H4"]
[]
[425,110,"Edges, risers, ends and reveals exceeding 300mm high or wide","m2",32]
[]
[425,111,"Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",83]
[]
[425,112,"Sloping and stepped outer edges of stairs 580mm high extreme","m",1]
[]
[425,null,"Fabric reinforcement","H4"]
[]
[425,113,"Type 245 fabric reinforcement in concrete surface beds etc","m2",100]
[]
[426,null,"DETAIL 3 ","H2"]
[]
[426,null,"Concrete, Formwork and Reinforcing","H2"]
[]
[426,null,"25MPa/19mm Concrete","H4"]
[]
[426,114,"Steps, urinal steps, cupboard platforms, etc","m3",16]
[]
[426,null,"Concrete sundries","H4"]
[]
[426,115,"Finishing top surfaces of concrete smooth with steel trowel","m2",39]
[]
[426,null,"Rough formwork to sides","H4"]
[]
[426,116,"Edges, risers, ends and reveals exceeding 300mm high or wide","m2",14]
[]
[426,117,"Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",155]
[]
[426,118,"Sloping and stepped outer edges of stairs 580mm high extreme","m",4]
[]
[426,null,"Fabric reinforcement","H4"]
[]
[426,119,"Type 245 fabric reinforcement in concrete surface beds etc","m2",84]
[]
[426,null,"DETAIL 4 & 5 ","H2"]
[]
[426,null,"Concrete, Formwork and Reinforcing","H2"]
[]
[426,null,"25MPa/19mm Concrete","H4"]
[]
[426,120,"Top and sides of seating detail","m3",11]
[]
[426,null,"Concrete sundries","H4"]
[]
[426,121,"Finishing top surfaces of concrete smooth with steel trowel","m2",30]
[]
[427,null,"Smooth formwok (degree of accuracy II)","H4"]
[]
[427,null,"Smooth formwork to sides","H4"]
[]
[427,122,"Walls circular exceeding 1m radius","m2",46]
[]
[427,null,"Permanent formwok","H4"]
[]
[427,null,"1,2mm Flat galvanised steel permanent decking system to sides and soffits","H4"]
[]
[427,123,"Decking to sides and soffits circular exceeding 1m radius","m2",64]
[]
[427,null,"Reinforcement","H4"]
[]
[427,124,"Mild steel and high tensile steel bars curved of various diameters","t","0.94"]
[]
[427,null,"DETAIL 6","H2"]
[]
[427,null,"Concrete, Formwork and Reinforcing","H2"]
[]
[427,null,"25MPa/19mm Concrete","H4"]
[]
[427,125,"Surface blinding under precast concrete","m3",2]
[]
[427,null,"Precast concrete slabs etc","H4"]
[]
[427,126,"600 x 530 x 65mm Thick seat slab with and including 600 x 365 x 65mm thick riser slab","m",222]
[]
[427,null,"GALVANISED STEEL BALUSTRADES (EXTERNAL ON RAMPS &STAIRS)","H1"]
[]
[427,null,"Bolted balustrades to ramp, staircase and walkway including intersections etc.","H4"]
[]
[427,127,"1100mm High black epoxy coated galvanised mild steel balustrades fixed/bolted to concrete on ramps and steps, all as detailed on architect's drawings","m",207]
[]
[428,null,"WATER TANK & BASE SUPPORT ","H1"]
[]
[428,null,"Excavations, etc","H3"]
[]
[428,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[428,128,"Trenches","m3",83]
[]
[428,null,"Extra over trench and hole excavations in earth for excavation in","H4"]
[]
[428,129,"Soft rock","m3",8]
[]
[428,130,"Hard rock","m3",4]
[]
[428,null,"Extra over all excavations for carting away","H4"]
[]
[428,131,"Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",83]
[]
[428,null,"Risk of collapse of excavations","H4"]
[]
[428,132,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",312]
[]
[428,null,"Keeping excavations free of water","H4"]
[]
[428,133,"Keeping excavations free of all water other than subterranean water","Item","1.00"]
[]
[428,null,"Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 90% Mod AASHTO density","H4"]
[]
[428,134,"Backfilling to trenches, holes, etc","m3",83]
[]
[428,135,"Backfilling to under floors, steps, pavings, etc.","m3",80]
[]
[428,null,"Compaction of surfaces","H4"]
[]
[428,136,"Compaction of ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",160]
[]
[429,null,"Soil insecticide in accordance with SANS 5859","H4"]
[]
[429,137,"Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m2",160]
[]
[429,null,"Concrete, Formwork and Reinforcement","H2"]
[]
[429,null,"25MPa/19mm unreinforced concrete","H4"]
[]
[429,138,"Foundation beams","m3",50]
[]
[429,null,"25MPa/19mm reinforced concrete","H4"]
[]
[429,139,"Surface beds","m3",81]
[]
[429,140,"Bottom and sides of V-drains","m3",158]
[]
[429,141,"Galvanised mild still Y10 \"bar\" 250mm high cast into concrete","No",160]
[]
[429,null,"Test cubes","H4"]
[]
[429,142,"Making and testing 150 x 150 x 150mm concrete strength test cube (Provisional)","No",6]
[]
[429,null,"Finishing top surfaces of concrete smooth with a steel trowel","H4"]
[]
[429,143,"Surface beds, slabs, etc","m2",270]
[]
[429,null,"Rough formwork ( Degree of AccuracyII)","H4"]
[]
[429,144,"Edges, risers, ends and reveals not exceeding 300mm high or wide ","m",736]
[]
[429,null,"Reinforcement ","H4"]
[]
[429,145,"Type 193 fabric reinforcement in concrete surface beds etc","m2",638]
[]
[429,146,"Type 395 fabric reinforcement in concrete surface beds etc","m2",270]
[]
[430,null,"Masonry","H2"]
[]
[430,147,"One brick wall of NFX bricks in class II mortar","m2",158]
[]
[430,148,"Extra over brickwork for face brick \"Horizon satin facebrick pointed with recessed and vertical joints\"","m2",158]
[]
[430,149,"Cement mortar surrounding 225mm x average 150mm high around water tank ","m",232]
[]
[430,null,"Plumbing and Drainage (Provisional)","H2"]
[]
[430,null,"Jo-Jo SG1 polyethylene drinking water tank with black lining internally","H4"]
[]
[430,150,"2500Litre circular tank 1,42m diameter x 1,86m high approximately 0,85m above ground level ","No",40]
[]
[430,151,"Set tank on top of tank stand, tie down tank with 6mm galvanised straining wire tied to mild steel \"U\" bar previously cast into concrete, strapped over tank and tied down on the opposite ends ","No",40]
[]
[430,152,"Outlet union for 15mm copper pipe including hole through tank ","No",40]
[]
[430,null,"Load Test","H4"]
[]
[430,153,"Fill tank with drinkable water to 50% of its capacity for a period of 10 days and then inspect for cracks, depression, etc","No",40]
[]
[430,null,"SOIL DRAINAGE","H1"]
[]
[430,null,"PVC pipes","H4"]
[]
[430,154,"110mm Pipes laid in and including trenches not exceeding 1m deep","m",12]
[]
[430,155,"110mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",125]
[]
[430,156,"Backfilling to pipe trenches","m3",157]
[]
[431,null,"Compaction of surfaces","H4"]
[]
[431,157,"Compaction of ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",82]
[]
[431,null,"Filling of coarse river sand supplied by the contractor, consolidated","H4"]
[]
[431,158,"Under pipes etc","m3",4]
[]
[431,null,"Brick inspection chambers including benching and channels (covers elsewhere)","H4"]
[]
[431,159,"1200 x 1200mm Brick manhole not exceeding 750mm deep internally","No",2]
[]
[431,160,"Ditto, but exceeding 750mm and not exceeding 1000mm deep internally","No",3]
[]
[431,161,"Ditto, but exceeding 1000mm and not exceeding 1250mm deep internally","No",2]
[]
[431,162,"Ditto, but exceeding 1250mm and not exceeding 1500mm deep internally","No",2]
[]
[431,163,"Ditto, but exceeding 1500mm and not exceeding 1750mm deep internally","No",1]
[]
[431,164,"Ditto, but exceeding 1750mm and not exceeding 2000mm deep internally","No",2]
[]
[431,165,"Ditto, but exceeding 2000mm and not exceeding 3000mm deep internally","No",1]
[]
[431,null,"Cast iron covers etc","H4"]
[]
[431,166,"450 x 600mm x 72kg Double seal manhole cover and frame","No",13]
[]
[432,null,"STORMWATER DRAINAGE","H2"]
[]
[432,null,"Class 75D concrete pipes with interlocking joints","H4"]
[]
[432,167,"300mm Pipes laid in and including trenches not exceeding 1m deep","m",3]
[]
[432,168,"300mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",210]
[]
[432,169,"450mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",16]
[]
[432,170,"Backfilling to pipe trenches","m3",177]
[]
[432,null,"Compaction of surfaces","H4"]
[]
[432,171,"Compaction of ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density","m2",206]
[]
[432,null,"Filling of coarse river sand supplied by the contractor, consolidated","H4"]
[]
[432,172,"Under pipes etc","m3",10]
[]
[432,null,"Concrete block stormwater soakaway chamber (covers elsewhere)","H4"]
[]
[432,173,"1000 x 1000mm Concrete block manhole not exceeding 1500mm deep internally","No",164]
[]
[432,null,"Cast iron covers etc","H4"]
[]
[432,174,"450 x 600mm x 72kg Double seal manhole cover and frame","No",164]
[]
[432,null,"FENCING","H1"]
[]
[432,null,"Galvanised security fence including site clearance and preparation of ground","H4"]
[]
[432,175,"1,80m Galvanised pre-painted \"clear Vu\" fencing with steel droppers, posts, gates post etc, on flat slope 76.2mm x 12.7mm mesh aperture","m",600]
[]
[433,176,"Continuous hot dipped galvanised high toughene steel spike affixed to panel edge at 150mm intervals using Anti-vandal bolts","m",600]
[]
[433,177,"Standard 1.35 x 1.8m high swinging gate with posts to match clear vu fence","No",1]
[]
[433,178,"Ditto, but 6,05 x 1,8m high sliding gate including spikes","No",1]
[]
[433,null,"SITE/STREET FURNITURE AND EQUIPMENTS ","H1"]
[]
[433,179,"Civic Litter Bin round 760mm high and 495mm diameter, 155kg ","No",18]
[]
[433,180,"Supply and installation of Civic Drinking fountain 1200/850mm high including providing water supply ","No",19]
[]
[434,null,"RETAINING STRUCTURES FORMED OF BRICKWORK","H1"]
[]
[434,null,"SITE CLEARANCE","H2"]
[]
[434,null,"Site clearance","H4"]
[]
[434,181,"Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc and trees not exceeding 200mm girth","m2",260]
[]
[434,null,"BULK EXCAVATION, FILLING, ETC","H2"]
[]
[434,null,"EXCAVATIONS ETC","H3"]
[]
[434,null,"Open face excavation in earth","H4"]
[]
[434,182,"Cut and fill to embankment behind retaining blocks including trimming to slope","m3",660]
[]
[434,183,"Cut to spoil","m3",2040]
[]
[434,184,"Banks to fill","m3",160]
[]
[434,null,"Extra over bulk excavations in earth for excavation in","H4"]
[]
[434,185,"Soft rock","m3",312]
[]
[434,186,"Hard rock","m3",156]
[]
[434,null,"Compaction of surfaces","H4"]
[]
[434,187,"Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 98% Mod AASHTO density","m2",800]
[]
[434,null,"Excavation in earth not exceeding 2m deep","H4"]
[]
[434,188,"Trenches","m3",145]
[]
[434,null,"Risk of collapse of excavations","H4"]
[]
[434,189,"Sides of trench and hole excavations not exceeding 1,5m deep","m2",264]
[]
[435,null,"Earth filling obtained from the excavations and/or prescribed stock piles on site compacted to ?% Mod AASHTO density","H4"]
[]
[435,190,"To form embankments for retaining structures","m3",51]
[]
[435,null,"25MPa/19mm unreinforced concrete","H4"]
[]
[435,191,"Strip footings","m3",61]
[]
[435,192,"Retaining walls","m3",42]
[]
[435,null,"Brickwork of NFP bricks in class II mortar","H4"]
[]
[435,193,"One brick walls","m2",500]
[]
[435,null,"Stormwater concrete V-Drains at the toe of retaining wall ","H4"]
[]
[435,null,"Earthworks","H4"]
[]
[435,194,"Excavate average 150mm deep in earth to form \"V\" drain profile","m3",33]
[]
[435,null,"Concrete, Formwork and Reinforcing","H4"]
[]
[435,null,"25MPa/19mm Reinforced concrete to bottom and sides of \"V\" drain","H4"]
[]
[435,195,"\"V\" drains","m3",33]
[]
[435,196,"Finishing top surface of \"V\" drains smooth with a steel trowel to falls ","m2",220]
[]
[435,197,"Rough formwork (Degree of accuracy III) to edges, risers, ends and reveals not exceeding 300mm high or wide","m",442]
[]
[435,198,"Type 245 fabric reinforcement in concrete surface beds etc ","m2",220]
[]
[435,199,"Channel Type B complete, including excavations","m",18]
[]
[436,null,"Mild and high tensile steel reinforcement to structural concrete work","H4"]
[]
[436,200,"Bars in various diameter","t",10]
[]
[436,null,"RENO MATRESS CONSTRUCTION","H1"]
[]
[436,null,"Mattresses of galvanised wire boxes placed together and filled with broken stone","H4"]
[]
[436,201,"Approximately 300mm thick 3 x 1m Reno mattress properly bonded including excavations, back filing etc all as per the engineer's details","m2",21]
[]
[436,null,"MAKING GOOD OF EXISTING WORKS","H2"]
[]
[436,202,"Jetting and flushing of all pipes and storm water drain system including manholes","Item","1.00"]
[]
[]
[]
[439,null,"BILL NO. 1","H1"]
[]
[439,null,"PROVISIONAL SUMS","H1"]
[]
[439,null,"SUPPLEMENTARY PREAMBLES","H2"]
[]
[439,null,"General","H4"]
[]
[439,null,"Work for which budgetary allowances are provided will be measured and valued in accordance with clause 32 of the Principal Building Agreement and deducted in whole or in part if not required without any compensation for loss or profit on the said allowances"]
[]
[439,null,"Profit","H4"]
[]
[439,null,"Where stated, the contractor may allow for profit if required"]
[]
[439,null,"General attendance on nominated/selected subcontractors","H4"]
[]
[439,null,"The item \"Attendance\" which follows each provisional sum for nominated/selected subcontractors' work, shall be deemed to cover all the contractor's costs incurred in providing free of charge to the nominated/selected subcontractor"]
[]
[439,null,"Asbestos Inspection Authority (AIA)","H4"]
[]
[439,1,"Provide the Provisional Amount of R30,000 (Thirty thousand Rand) nett for Asbestos Inspection Authority (AIA) to be omitted in part or whole as instructed by Principal Agent","Item","1.00"]
[]
[439,2,"Allow for attendance on item above if required","Item","1.00"]
[]
[439,3,"Allow for profit on item above if required","Item","1.00"]
[]
[440,null,"BUDGETARY ALLOWANCES","H2"]
[]
[440,null,"Community Liaison Officer ","H4"]
[]
[440,4,"Provide the Budgetary Amount of R300,000 (Three hundred thousand Rand) nett for Community Liaison Officer's Salary to be omitted in part or whole as instructed by Principal Agent","Item","1.00"]
[]
[440,5,"Provide the Budgetary Amount of R150 000 (One hundred and fifty thousand Rand) nett for the full construction of septic tank, acid neutralising tank  french drain to be measured and priced at Bill rates","Item","1.00"]
[]
[440,6,"Provide the Budgetary Amount of R6000 (Six thousand Rand) nett for the supply and fixing of school name plate and Department of Education, all to the architect details","Item","1.00"]
[]
[]
[]
[442,null,"BILL NO. 1","H1"]
[]
[442,null,"CONTRACT PARTICIPATION GOALS (CPG)","H1"]
[]
[442,null,"Note to tenderers: As CPGs may not provide any bidder a competitive advantage Provisional Amounts and fixed percentages for profit and attendance have been provided, Only the provisional amount will be adjusted once the awarded tender amount and/or the values beneficiaries have been appointed, and the final values have been ascertained"]
[]
[442,null,"Minimum 30% Sub-Contracting","H4"]
[]
[442,1,"Provision is made for 30% subcontacting to SMMEs in the execution of this project as described in C3.1 Project Specifications. This is the contractors allowance for the P & G's for the 30% sub-contractors (SMME's) after tender awards","Item","1.00"]
[]
[442,2,"Allow for profit all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[442,3,"Allow for attendance all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[442,null,"Minimum Targeted Local Building Material Manufacturers","H4"]
[]
[442,4,"Provision is made for the Minimum Targeted Local Building Material Manufacturers CPG in the execution of this project as described in C3.1 Project Specifications. Allowance for monitoring and monthly reporting on material purchased from Local Building Material Manufacturers by main contractor and subcontractors based on determination by Employer taking into account specific project variables","Item","1.00"]
[]
[442,5,"Allow for profit all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[442,6,"Allow for attendance all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[443,null,"Minimum Targeted Local Building Material Suppliers","H4"]
[]
[443,7,"Provision is made for the Minimum Targeted Local Building Material Suppliers CPG in the execution of this project as described in C3.1 Project Specifications. Allowance for monitoring and monthly reporting on material purchased from Local Building Material Suppliers by main contractor and subcontractors based on determination by Employer taking into account specific project variables","Item","1.00"]
[]
[443,8,"Allow for profit all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[443,9,"Allow for attendance all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[443,null,"Minimum Targeted Local Labour Skills Development","H4"]
[]
[443,10,"Provision is made for the Minimum Targeted Local Labour Skills Development CPG in the execution of this project as described in C3.1 Project Specifications. This allowance is for the cost for a suitable qualified and experienced training service provider appointed by the main contractor including monitoring and monthly reporting","Item","1.00"]
[]
[443,11,"Allow for profit all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[443,12,"Allow for attendance all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[443,null,"Minimum Targeted Enterprise Development","H4"]
[]
[443,13,"A  provision amount has been made allowed for the Minimum Targeted Enterprise Development CPG in the execution of this project as described in C3.1 Project Specifications. The provisional amount allowed is for the  appointment of training coordinator, mentor, training service providers and training of the beneficiary enterprises including monitoring and monthly reporting","Item","1.00"]
[]
[443,14,"Allow for profit all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[443,15,"Allow for attendance all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[444,null,"Minimum Targeted Skills Development Goals","H4"]
[]
[444,16,"Provisional amount has been allowed for the Minimum Targeted  Skills Development CPG in the execution of this project as described in C3.1 Project Specifications.  Stipends payable to the beneficiaries appointment of training coordinator appointment of mentor(where applicable) appointment of training service providers other additional costs as per table 3 of the standard monitoring and monthly reporting","Item","1.00"]
[]
[444,17,"Allow for profit all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[444,18,"Allow for attendance all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[444,null,"National Youth Service Training and Development Programme","H4"]
[]
[444,19,"The programme shall be implemented in terms of the Implementation of the National Youth Service Programme under the Expanded Public Works(EPWP)  Training of Youth Workers Travelling during on-site training Appointment of employment youth workers and monthly stipends Provision of Basic Tools for Youth Workers Provision of EPWP Designed Overalls and hard Hats to Youth Workers Appointment of Youth Training Coordinators Liaison with Service Provider Logistics for Exit Workshops","Item","1.00"]
[]
[444,20,"Allow for  monthly reporting based on the Implementation of the EPWP - NYS as per the specifications and all inclusive of associated costs to the contractor for implementation","%","5.00"]
[]
[445,null,"Labour Intensive Participation Goal","H4"]
[]
[445,21,"Labour Intensive Participation Goal -  Allowance for monthly reporting of labour intensive works by main contractor based on determination by Employer taking into account specific project variables. Allowance for monitoring and monthly reporting of works executed by means of Labour Intensive methods by main contractor and subcontractors based on determination by Employer taking into account specific project variables ","Item","1.00"]
[]
[]
[]
[447,1,"Preliminaries","Page",44]
[]
[447,2,"Existing Blocks - [Block A, B, C, D, E, F, G, I, J, L & O]","Page",105]
[]
[447,3,"Block M - New Kitchen Block","Page",151]
[]
[447,4,"Block S - New Female Ablution Block","Page",191]
[]
[447,5,"Block T - New Male Ablution Block","Page",231]
[]
[447,6,"Block U - New Double Storey Classroom Block","Page",276]
[]
[447,7,"Block V - New Administration Block","Page",325]
[]
[447,8,"Block W - New Multi-Purpose Classroom Block","Page",370]
[]
[447,9,"Block X - New Gate House and Bin Area","Page",407]
[]
[447,10,"External Works","Page",438]
[]
[447,11,"Provisional Sums","Page",441]
[]
[447,12,"Contract Participation Goals (CPG)","Page",446]
[]
[447,null,"SUB-TOTAL A","ST"]
[]
[447,null,"Contingencies @ 5% of Sub-total A to be used at Employer's discretion","Item","1.00"]
[]
[447,null,"Budgetary Amount of R2,436,552.97 (Two million four hundred and thirty six thousand five hundred and fifty two rand and ninety seven cents) nett for Escalation","Item","1.00"]
[]
[447,null,"SUB-TOTAL B","ST"]
[]
[447,null,"ADD: VALUE ADDED TAX @15%","TAX","15.00"]
[]
[null,null,"Carried to Form of Tender"]