{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["Summary","Alterations","Electrical & Mechanical","Plumbing & Drainage"],"not_rendered":{"defined_names":7},"read":"whole","date_system":"1900"}

{"sheet":"Summary","index":0,"n_rows":13,"n_cols":3,"rows_kept":13,"merged":[[1,0,1,1],[2,0,2,2]]}
[]
["NRF/SAIAB/58/2023-24"]
["Panel of service providers to provide general building maintenance services at two SAIAB buildings (Gauteng & Eastern Cape) on an ad hoc basis for a period of 3 years"]
[]
["SUMMARY PAGE"]
[]
["ITEM No.","DESCRIPTION","   AMOUNT"]
[""]
[1,"SECTION 1: Alterations",{"$f":"Alterations!E293","v":0}]
[2,"SECTION 2: Electrical and Mechanical",{"$f":"'Electrical & Mechanical'!E629","v":0}]
[3,"SECTION 3: Plumbing and Drainage",{"$f":"'Plumbing & Drainage'!E215","v":0}]
[]
[null,"TOTAL (For Price Evaluation)",{"$f":"SUM(C9:C12)","v":{"v":0,"d":"R0.00"}}]

{"sheet":"Alterations","index":1,"n_rows":293,"n_cols":5,"rows_kept":293,"merged":[[292,0,292,3]]}
[]
["Item No.","Description","Unit","Qty","Amount Including VAT"]
[null,"SCHEDULE NO.1 TO 6"]
[]
["1.1","Brickwork etc."]
["1.1.1","Mass brickwork","m³",1]
["1.1.2","Half brick wall","m²",1]
["1.1.3","One brick wall","m²",1]
["1.1.4","One and a half brick wall","m²",1]
["1.1.5","280mm Hollow walls of two half brick skins","m²",1]
[]
["1.2","Taking out and removing doors, windows, etc. from brickwork to be demolished"]
["1.2.1","Timber single door and frame not exceeding 2,5m²","no",1]
["1.2.2","Timber double door and frame exceeding 2,5m² and not exceeding 5,0m²","no",1]
["1.2.3","Timber single door and steel frame not exceeding 2,5m²","no",1]
["1.2.4","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m²","no",1]
["1.2.5","Timber single door not exceeding 2,5m²","no",1]
["1.2.6","Timber double door exceeding 2,5m² and not exceeding 5,0m²","no",1]
["1.2.7","Steel single door and steel frame not exceeding 2,5m2","no",1]
["1.2.8","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m²","no",1]
["1.2.9","Glazed steel window not exceeding 2,5m²","no",1]
["1.2.10","Glazed steel window exceeding 2,5m² and not exceeding 5.0m²","no",1]
["1.2.11","Glazed aluminium window not exceeding 2,5m²","no",1]
["1.2.12","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m²","no",1]
[]
["1.3","Taking out and removing doors, windows, etc. including thresholds, sills, etc. (building up openings elsewhere)"]
["1.3.1","Timber single door and frame not exceeding 2,5m² from half or one brick wall","no",1]
["1.3.2","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from half or one brick wall","no",1]
["1.3.3","Timber double door and frame not exceeding 2,5m² from half or one brick wall","no",1]
["1.3.4","Timber double door and frame exceeding 2,5m² and not exceeding 5,0m² from half or one brick wall","no",1]
["1.3.5","Timber single door and steel frame not exceeding 2,5m² from half brick wall","no",1]
["1.3.6","Timber single door and steel frame not exceeding 2,5m² from one brick wall","no",1]
["1.3.7","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1]
["1.3.8","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1]
["1.3.9","Steel single door and frame not exceeding 2,5m² from half or one brick wall","no",1]
["1.3.10","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1]
["1.3.11","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1]
["1.3.12","Glazed timber window not exceeding 2,5m² from half or one brick wall","no",1]
["1.3.13","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1]
["1.3.14","Glazed steel window not exceeding 2,5m² from half or one brick  wall","no",1]
["1.3.15","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1]
["1.3.16","Glazed aluminium window not exceeding 2,5m² from half or one brick  wall","no",1]
["1.3.17","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1]
[]
["1.4","Taking down and removing roofs, floors, panelling, ceilings, partitions, etc."]
["1.4.1","Corrugate sheet iron roof covering, valley linings, ridge flashings and timber purlins","m²",1]
["1.4.2","Concrete, Harveytile sheet iron tile, slate, thatch, etc. roof covering, valley linings, ridge, hip cappings, flashings and timber brandering,purlins, etc.","m²",1]
["1.4.3","Pitched corrugated iron roof 10000 x 10000  by not exceeding 2000mm high overall including roof covering, timber trusses, ceilings and cornices, eaves soffit covering, fascias, barge boards, gutters and rainwater pipes ","no",1]
["1.4.4","Timber rafters, beams, etc","m",1]
["1.4.5","Tongued and grooved timber suspended floor including skirting, joists, bearers, etc","m²",1]
["1.4.6","Gypsum plasterboard ceilings including cornices, timber brandering, etc","m²",1]
["1.4.7","Flush plastered gypsum plasterboard suspended ceilings, including cornices, suspension grid, hangers, etc.","m²",1]
["1.4.8","Flush plastered gypsum plasterboard bulkheads, including cornices, suspension grid, hangers, etc.","m²",1]
["1.4.9","Wood panel bulkheads, including cornices, suspension grid, hangers, etc.","m²",1]
["1.4.10","Acoustic tiles suspended ceiling including suspension grid, hangers, etc","m²",1]
["1.4.11","Acoustic tiles suspended ceiling only","m²",1]
["1.4.12","Drywall partitioning 3000mm high including doors, ironmongery, glazed borrowed lights, etc","m",1]
["1.4.13","Carefully cut out rusted or damaged roof sheeting","m²",1]
[]
["1.5","Taking down and removing rainwater goods"]
["1.5.1","100 x 125mm Box gutters including downpipes","m",1]
[]
["1.6","Taking out and removing sundry joinery work"]
["1.6.1","Timber cornices from brickwork","m",1]
["1.6.2","Timber skirting from brickwork","m",1]
["1.6.3","Timber or asbestos cement sills from brickwork","m",1]
["1.6.4","Timber or asbestos cement fascias and barge boards","m",1]
[]
["1.7","Taking out and removing joinery fittings etc"]
["1.7.1","Timber wall cupboard 600 x 300 x 900mm high","no",1]
["1.7.2","Timber wall cupboard 900 x 300 x 900mm high","no",1]
["1.7.3","Timber wall cupboard 1200 x 300 x 900mm high","no",1]
["1.7.4","Timber floor cupboard 600 x 600 x 900mm high","no",1]
["1.7.5","Timber floor cupboard 900 x 600 x 900mm high","no",1]
["1.7.6","Timber floor cupboard 1200 x 600 x 900mm high","no",1]
["1.7.7","Timber sink cupboard 900 x 600 x 900mm high including disconnecting waste pipe and taps","no",1]
["1.7.8","Timber sink cupboard 1200 x 600 x 900mm high including disconnecting waste pipe (new trap and connecting to new waste pipe elsewhere)","no",1]
["1.7.9","Timber sink cupboard 1800 x 600 x 900mm high including disconnecting waste pipe (new trap and connecting to new waste pipe elsewhere)","no",1]
["1.7.10","Timber counter 1200 x 600 x 900mm high","no",1]
["1.7.11","Timber counter 1600 x 600 x 900mm high","no",1]
["1.7.12","Timber counter 1800 x 600 x 900mm high","no",1]
["1.7.13","Timber counter 2400 x 600 x 900mm high","no",1]
[]
["1.8","Take up and remove wooden wall panneling, vinyl wall covering, wall carpeting, waterproofing, etc."]
["1.8.1","Vinyl wall covering including preparing walls for new finishes.","m²",1]
[]
["1.9","Take up and remove wood block floor covering, vinyl floor covering, carpeting, waterproofing, etc."]
["1.9.1","Vinyl tile floor covering including preparing screed for new floor covering.","m²",1]
["1.9.2","Vinyl sheet floor covering with welded joints including preparing screed for new floor covering.","m²",1]
["1.9.3","Carpet sheet floor covering including preparing screed for floor covering","m²",1]
[]
["1.10","Taking out and removing ironmongery"]
["1.10.1","Mortice lock and striking plate from timber door and steel frame","no",1]
["1.10.2","Mortice lock and striking plate from timber door and wooden frame","no",1]
["1.10.3","Mortice lock and rebate conversion set from timber doors","no",1]
["1.10.4","Mortice lock and rebate conversion set from steel doors","no",1]
["1.10.5","Metal striking plate from steel door frame","no",1]
["1.10.6","Metal striking plate from timber door frame","no",1]
["1.10.7","Overhead door closer","no",1]
["1.10.8","150mm Metal cabin hook and eye including chamfered hardwood block","no",1]
["1.10.9","Chromium plated towel rail not exceeding 1000mm long","no",1]
["1.10.11","Chromium plated hat and coat hook","no",1]
["1.10.12","Side hung window catch","no",1]
["1.10.13","Side or top hung window stay","no",1]
[]
["1.11","Taking out/off and removing sundry metalwork"]
["1.11.1","Steel pipe handrail from walls including making good plaster finish","m",1]
["1.11.2","Steel balustrade 900mm high from concrete stairs including making good granolithic finish to kerb","m",1]
["1.11.3","Steel staircase comprising two flights and one landing, 3.5x2.00m overall on plan and rising 3.20m, including supporting columns, balustrades, etc","no",1]
["1.11.4","Steel wire mesh burglar proofing not exceeding 1,0m² bolted to brickwork and making good face brickwork","no",1]
["1.11.5","Steel wire mesh burglar proofing exceeding 1,0m² and not exceeding 2,0m² bolted to brickwork and making good face brickwork","no",1]
["1.11.6","Steel wire mesh burglar proofing exceeding 2,0m² and not exceeding 3,0m² bolted to brickwork and making good face brickwork","no",1]
["1.11.7","Steel single leaf security gate not exceeding 2,5m² ","no",1]
["1.11.8","Steel double leaf security gate exceeding 2,5m² and not exceeding 5,0m²","no",1]
["1.11.9","Sheet metal eaves gutters and rainwater down pipes","m",1]
[]
["1.12","Hacking up/off and removing ceramic tile floor and wall finishers including removing mortar bed or backing and  preparing concrete or brick surfaces for new screed, plaster or tile finishers"]
["1.12.1","Tiles to floors","m²",1]
["1.12.2","Tiles to treads and risers of stairs","m²",1]
["1.12.3","Tiles to walls","m²",1]
["1.12.4","Tile skirting 100mm high","m",1]
[]
["1.13","Taking out and cleaning"]
["1.13.1","Expansion joints not exceeding 300mm deep and prepare to receive new","m",1]
[]
["1.14","Taking out and removing piping, sanitary fittings, etc including disconnecting piping from fittings and making good floor and wall finishes (making good tiling and paintwork elsewhere)"]
["1.14.1","110mm PVC piping including fittings and brackets","m",1]
["1.14.2","75mm PVC piping including fittings and brackets","m",1]
["1.14.3","75mm Galvanised steel piping including fittings and brackets","m",1]
["1.14.4","25mm Galvanised steel piping including fittings and brackets","m",1]
["1.14.5","40mm Galvanised steel piping including fittings and brackets","m",1]
["1.14.6","100mm Cast iron piping including fittings and brackets","m",1]
["1.14.7","15mm Copper piping including fittings and brackets","m",1]
["1.14.8","22mm Copper piping including fittings and brackets","m",1]
["1.14.9","32mm Copper piping including fittings and brackets","m",1]
["1.14.10","Stainless steel wash hand basin","no",1]
["1.14.11","Stainless steel sink and drainer on timber cupboard 900 x 600 x 900mm high","no",1]
["1.14.12","Stainless steel sink and drainer on timber cupboard 1200 x 600 x 900mm high","no",1]
["1.14.13","Stainless steel sink and drainer on timber cupboard 1800 x 600 x 900mm high","no",1]
["1.14.14","Stainless steel wash trough 1200 x 600 x 900mm high","no",1]
["1.14.15","Precast concrete wash trough 1200 x 600 x 900mm high","no",1]
["1.14.16","Vitreous china high level urinal cistern","no",1]
["1.14.17","Vitreous china wash hand basin","no",1]
["1.14.18","Vitreous china WC pan and cistern","no",1]
["1.14.19","Vitreous china WC pan and high level cistern","no",1]
["1.14.20","Vitreous china WC pan with flush valve","no",1]
["1.14.21","Vitreous china wall hung urinal with flush valve","no",1]
["1.14.22","Vitreous china urinal 1200 x 1500mm high including breaking up and removing 400mm wide concrete urinal step","no",1]
["1.14.23","Vitreous china urinal 1200 x 1500mm high and high level cistern including breaking up and removing 400mm wide concrete urinal step","no",1]
[]
[2,"Taking out and removing glass and mirrors"]
["2.1","Glass from steel windows including cleaning out rebates and preparing for new glass","m²",1]
["2.2","Glass from timber windows with beads including cleaning out rebates and preparing for new glass","m²",1]
["2.3","Mirror from wall","m²",1]
["2.4","Mirror from wall, including making good tiling","m²",1]
[]
[3,"Cutting through floors and ceilings"]
["3.1","Cutting through 100mm thick concrete surface bed for 460mm wide concrete wall footing including making good concrete on both sides of new half brick wall.","m",1]
["3.2","Cutting through 100mm thick concrete surface bed for 700mm wide concrete wall footing including making good concrete on both sides of new one brick wall.","m",1]
["3.3","Cutting through gypsum ceiling and brandering for half brick wall including making good on both sides of wall (new cornices elsewhere)","m",1]
["3.4","Cutting through gypsum ceiling and brandering for one brick wall including making good on both sides of wall (new cornices elsewhere)","m",1]
["3.5","Cutting through \"Nutec\" fibre-cement ceiling and brandering for half brick wall including making good on both sides of wall (new cornices elsewhere)","m",1]
["3.6","Cutting through \"Nutec\" fibre-cement ceiling and brandering for one brick wall including making good on both sides of wall (new cornices elsewhere)","m",1]
[]
[4,"Building up openings"]
["4.1","Cutting toothing and bonding new brickwork to existing","m²",1]
[]
["4.2","Preparatory work to existing surfaces"]
["4.2.1","Cutting out joints of existing brickwork to receive plaster.","m²",1]
["4.2.2","Hacking face of existing concrete columns, beams, etc to receive plaster","m²",1]
["4.2.3","Hacking face of existing face brickwork to receive plaster","m²",1]
["4.2.4","Making good defects in existing screeded floors with \"Pavelite\"","m²",1]
["4.2.5","Chasing existing brick / concrete walls ","m",1]
[]
["4.3","Making good finishes e.t.c"]
["4.3.1","Making good brickwork at ends of half brick wall","m",1]
["4.3.2","Making good brickwork at ends of one brick wall","m",1]
["4.3.3","Making good brickwork at ends of one and half brick wall","m",1]
["4.3.4","Making good brickwork to face of wall where half brick cross wall removed","m",1]
["4.3.5","Making good brickwork to face of wall where one brick cross wall removed","m",1]
["4.3.6","Making good brickwork to face of wall where one and half brick cross wall removed","m",1]
["4.3.7","Making good face brickwork at ends of half brick wall","m",1]
["4.3.8","Making good face brickwork at ends of one brick wall","m",1]
["4.3.9","Making good face brickwork at ends of one and half brick wall","m",1]
["4.3.10","Making good face brickwork to face of wall where half brick cross wall removed","m",1]
["4.3.11","Making good face brickwork to face of wall where one brick cross wall removed","m",1]
["4.3.12","Making good face brickwork to face of wall where one and half brick cross wall removed","m",1]
[]
["4.4","Making good \"Rhino\" gypsum board ceiling and brandering."]
["4.4.1","Ceilings in patches","m²",1]
["4.4.2","Ceilings where half brick walls removed","m",1]
["4.4.3","Ceilings where one brick walls removed","m",1]
["4.4.4","Ceilings where one and half brick walls removed","m",1]
[]
["4.5","Making good 300x300x2,0mm Vinyl floor tiles"]
["4.5.1","Floors in patches","m²",1]
["4.5.2","Floors where partitions removed","m",1]
["4.5.3","Floors where half brick walls removed","m",1]
["4.5.4","Floors where one brick walls removed","m",1]
["4.5.5","Floors where one and half brick walls removed","m",1]
[]
["4.6","Making good 3,5mm \"Industrial floor\" flexible vinyl sheeting "]
["4.6.1","Floors in patches","m²",1]
["4.6.2","Floors where partitions removed","m",1]
["4.6.3","Floors where half brick walls removed","m",1]
["4.6.4","Floors where one brick walls removed","m",1]
["4.6.5","Floors where one and half brick walls removed","m",1]
[]
["4.7","Making good screed and 300x300x2,0mm Vinyl floor tiles"]
["4.7.1","Floors in patches","m²",1]
["4.7.2","Floors where partitions removed","m",1]
["4.7.3","Floors where half brick walls removed","m",1]
["4.7.4","Floors where one brick walls removed","m",1]
["4.7.5","Floors where one and half brick walls removed","m",1]
[]
["4.8","Making good screed and 3,5mm \"Industrial floor\" flexible vinyl sheeting "]
["4.8.1","Floors in patches","m²",1]
["4.8.2","Floors where partitions removed","m",1]
["4.8.3","Floors where half brick walls removed","m",1]
["4.8.4","Floors where one brick walls removed","m",1]
["4.8.5","Floors where one and half brick walls removed","m",1]
[]
["4.9","Making good internal cement plaster."]
["4.9.1","Walls in patches","m²",1]
["4.9.2","Walls where half brick walls removed.","m",1]
["4.9.3","Walls where one brick walls removed.","m",1]
["4.9.4","Walls where one and half brick walls removed.","m",1]
["4.9.5","Concrete ceilings in patches","m²",1]
["4.9.6","Concrete ceilings where half brick walls removed","m",1]
["4.9.7","Concrete ceilings where one brick walls removed","m",1]
["4.9.8","Concrete ceilings where one and half brick walls removed","m",1]
["4.9.9","Making good of chased walls","m",1]
[]
["4.10","Making good external cement plaster."]
["4.10.1","Walls in patches","m²",1]
["4.10.2","Walls where half brick walls removed.","m",1]
["4.10.3","Walls where one brick walls removed.","m",1]
["4.10.4","Walls where one and half brick walls removed.","m",1]
[]
["4.11","Making good 200x200x4mm white glazed ceramic tiles"]
["4.11.1","Walls in patches","m²",1]
["4.11.2","Walls where half brick walls removed.","m",1]
["4.11.3","Walls where one brick walls removed.","m",1]
["4.11.4","Walls where one and half brick walls removed.","m",1]
[]
[null,"Supplementary preambles"]
[]
[null,"Waterproofing to roofs, basements, etc shall be laid under a ten year guarantee. Waterproofing to roofs shall be laid to even falls to outlets etc with necessary ridges, hips and valleys. Description of sheet or membrane waterproofing shall be deemed to include additional labour to turn-ups and turndowns"]
[]
[null,"Protective roofing paint"]
["5.1","Two coats bituminous aluminium paint"]
["5.1.1","On waterproofing to roofs","m²",1]
["5.1.2","On waterproofing to box gutters","m²",1]
[]
["5.2","Clear silicon sealant"]
["5.2.1","Between glazed tiles and sanitary fittings","m",1]
["5.2.2","\"The Works\" or equivalent wet surface sealant","m",1]
[]
["5.3","Epoxy"]
[null,"\"EPOXY 319/20\" epoxy floor and wall coating applied in strict accordance with the manufacturer's instructions "]
[]
["5.3.1","On screeded floors","m²",1]
["5.3.2","On screeded seating slabs","m²",1]
[]
["5.4","Fibre Flex membrane free \"Flash Harry\" or equally approved waterproofing"]
["5.4.1","On flat roofs","m²",1]
["5.4.2","On sloping IBR roof sheeeting","m²",1]
["5.4.3","On walls","m²",1]
[]
[6,"Painting"]
[null,"All painting shall be carried out in strict accordance with \"Plascon\" or equally approved specifications"]
[]
["6.1","Two coats solvent based UV resistant clear gloss acrylic brick dressing"]
["6.1.1","On sills, thresholds, etc","m²",1]
["6.1.2","On flush pointed face walls","m²",1]
["6.1.3","On recessed pointed face walls","m²",1]
[]
["6.2","One coat alkaline resistant plaster primer and two coats superior acrylic PVA emulsion paint"]
["6.2.1","On ceilings and cornices","m²",1]
["6.2.2","On drywall partitions","m²",1]
[]
["6.3","One coat water based galvanised iron primer, one coat universal alkyd based undercoat and two coats alkyd based high gloss enamel paint"]
["6.3.1","On corrugated iron profile roof sheeting (measured on flat)","m²",1]
["6.3.2","On IBR profile roof sheeting (measured on flat)","m²",1]
["6.3.3","On eaves gutters","m²",1]
["6.3.4","On rails, bars, pipes etc ","m",1]
["6.3.5","On eaves gutters/rainwater downpipes not exceeding 300mm girth","m",1]
["6.3.6","On rails, bars, pipes etc not exceeding 300mm girth","m",1]
[]
["6.4","Three coats clear polyurethane suede varnish "]
["6.4.1","On doors","m²",1]
["6.4.2","Skirtings, rails, etc. not exceeding 300mm. girth","m",1]
["TOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"$f":"SUM(E6:E292)","v":0}]

{"sheet":"Electrical & Mechanical","index":2,"n_rows":629,"n_cols":5,"rows_kept":629,"merged":[[628,0,628,3]]}
[]
["Item No.","Description","Unit","Qty","Amount Including VAT"]
[null,"SCHEDULE NO.7"]
[]
[null,"ELECTRICAL"]
[]
[null,"EARTHING SYSTEM "]
[]
[null,"Bare Stranded Copper Earth Wire "]
[null,"Supply, delivery and installation of bare stranded copper fixed to cable tray or rack (tray measured elsewhere):"]
["7.1.1","70mm2","m",1]
[]
["7.1.2","50mm2","m",1]
[]
["7.1.3","25mm2","m",1]
[]
["7.1.4","16mm2","m",1]
[]
["7.1.5","10mm2","m",1]
[]
["7.1.6","6mm2","m",1]
[]
["7.1.7","4mm2","m",1]
[]
["7.1.8","2.5mm2","m",1]
[]
[null,"Supply, delivery and installation of termininations including fastening materials and lugs, and the connection to the specified terminal equipment:"]
[]
["7.1.9","70mm2","no",1]
[]
["7.1.10","50mm2","no",1]
[]
["7.1.11","25mm2","no",1]
[]
["7.1.12","16mm2","no",1]
[]
["7.1.13","10mm2","no",1]
[]
["7.1.14","6mm2","no",1]
[]
["7.1.15","4mm2","no",1]
[]
["7.1.16","2.5mm2","no",1]
[]
[null,"LIGHTING AND SMALL POWER "]
[]
[null,"CONDUITS"]
[]
["7.2","PVC CONDUIT"]
[null,"Supply, deliver and install of conduit including bushes, couplings, saddles, bends, wastage etc"]
[]
[null,"Surface mounted to brickwork, concrete, steel, wood, roof  members, etc exceeding 3000mm above floor level "]
[]
["7.2.1","20mm Diameter ","m",1]
[]
["7.2.2","25mm Diameter ","m",1]
[]
["7.2.3","50mm Diameter","m",1]
[]
[null,"Chased and/or fixed in brickwork not exceeding 3000mm above floor level (making good of chase by others) "]
[null," "]
["7.2.4","20mm Diameter ","m",1]
[]
["7.2.5","25mm Diameter ","m",1]
[]
["7.2.6","50mm Diameter","m",1]
[]
["7.3","GALVANISED CONDUIT "]
[null,"Surface mounted to brickwork, concrete, steel, wood, roof  members, etc exceeding 3000mm above floor level "]
[]
["7.3.1","20mm Diameter ","m",1]
[]
["7.3.2","25mm Diameter ","m",1]
[]
[null,"LIGHTING AND SMALL POWER "]
[]
["7.4","CONDUIT BOXES AND FITTINGS "]
[]
["7.4.1","Cover plate for 100mm x 100mm box ","No",1]
[]
["7.4.2","Cover plate for 100mm x 50mm box ","No",1]
[]
["7.5","POWER SKIRTING "]
[null,"Note: "]
[null,"The rates include for splices, joining, drilling, etc"]
[null,"Power skirting complete with cover surface mounted to  brickwork or concrete "]
[]
["7.5.1","One-compartment ","m",1]
[]
["7.5.2","Two-compartment ","m",1]
[]
["7.5.3","16A Normal power sso on power skirting,complete with pre-punched cover","m",1]
[]
["7.5.4","16A Normal power sso on power skirting.complete with pre punched cover.","m",1]
[null," "]
["7.5.5","16A DUO SSO IN Powerskirting","m",1]
[]
["7.5.6","16A Red dedicated","m",1]
[]
["7.5.7","20A DP Isollator c/w cord grip in power skirting","m",1]
[]
["7.5.8","One-compartment end cap ","No",1]
[]
["7.5.9","Two-compartment end cap ","No",1]
[]
["7.5.10","One-compartment 90 degree bend ","No",1]
[]
[]
["7.6","SWITCHES AND PLUGS"]
[null,"Switches, etc complete with cover plate fixed in flush box "]
[]
["7.6.1","16A One-lever one-way switch ","No",1]
[]
["7.6.2","16A Two-lever one-way switch ","No",1]
[]
["7.6.3","16A Three-lever one-way switch ","No",1]
[]
["7.6.4","16A Four-lever one-way switch ","No",1]
[]
["7.6.5","16A One-lever two-way switch ","No",1]
[]
["7.6.6","16A Two-lever two-way switch ","No",1]
[]
["7.6.7","2 Lever / 3 Lever - Grid plate with surround","No",1]
[]
["7.6.8","2x4 Grid Plate with surround","No",1]
[]
["7.6.9","4x4 Grid Plate with surround","No",1]
[]
["7.6.10","16A Three-pin Single switched socket outlet ","No",1]
[]
["7.6.11","16A Three-pin Double switched socket outlet ","No",1]
[]
["7.6.12","Round Three pin socket outlet","No",1]
[]
["7.6.13","Bell push button complete with surround","No",1]
[]
["7.6.14","16A One lever dimmer switch","No",1]
[]
["7.6.15","Single telephone socket outlet (RJ11) complete with surround","No",1]
[]
["7.6.16","Single TV socket outlet complete with surround","No",1]
[]
["7.6.17","16 A 1-way Light switch insert","No",1]
[]
["7.6.18","16 A 2-way Light switch insert","No",1]
[]
["7.6.19","\"4 x 4\" Extension box with spouts","No",1]
[]
["7.6.20","\"4 x 2\" Extension box with spouts","No",1]
[]
["7.6.21","Stove one-way switch ","No",1]
[]
[null,"WIRING"]
[]
[null,"Supply, delivery and installation of cables "]
[]
["7.7","PVC Multicore Armored Cable"]
[]
["7.7.1","4 mm 3-core ","m",1]
[]
["7.7.1a","2.5 mm 3-core ","m",1]
[]
["7.7.1b","2.5 mm 4-core ","m",1]
[]
["7.7.1c","4 mm 4-core ","m",1]
[]
["7.7.1d","6 mm 3-core ","m",1]
[]
["7.7.1e","6 mm 4-core ","m",1]
[]
["7.7.2","10  mm   3-Core ","m",1]
[]
["7.7.3","10  mm   4-Core ","m",1]
[]
["7.7.4","16  mm   3-Core ","m",1]
[]
["7.7.5","16  mm   4-Core ","m",1]
[]
["7.7.5a","25  mm   3-Core ","m",1]
[]
["7.7.5b","25  mm   4-Core ","m",1]
[]
["7.7.6","35  mm  3-Core ","m",1]
[]
["7.7.6a","35  mm  4-Core ","m",1]
[]
["7.7.7","70  mm  3-Core ","m",1]
[]
["7.7.7a","70  mm  4-Core ","m",1]
[]
["7.7.8","95  mm   4-Core ","m",1]
[]
[]
["7.8","Flexible Cable and Cord"]
[]
["7.8.1","1.5mm2 twin rip cord","m",1]
[]
["7.8.2","2.5mm2 twin rip cord","m",1]
[]
["7.8.3","1.5mm2 PVC carb tyre flex 3-core","m",1]
[]
["7.8.4","2.5mm2 PVC carb tyre flex 3-core","m",1]
[]
["7.8.5","4mm2 PVC carb tyre flex 3-core","m",1]
[]
["7.8.6","6mm2 PVC carb tyre flex 3-core","m",1]
[]
["7.8.7","1.5mm2 Suffix Cable 3-core and earth","m",1]
[]
["7.8.8","2.5mm2 Suffix Cable 3-core and earth","m",1]
[]
["7.8.9","4.0mm2 Suffix Cable 3-core and earth","m",1]
[]
["7.8.10","6.0mm2 Suffix Cable 3-core and earth","m",1]
[]
["7.8.11","1.5mm2 Suffix Cable 4-core and earth","m",1]
[]
["7.8.12","2.5mm2 Suffix Cable 2-core and earth","m",1]
[]
["7.8.13","6.0mm2 Suffix Cable 2-core and earth","m",1]
[]
["7.8.14","1.5mm2 Flat twin and earth","m",1]
[]
["7.8.15","2.5mm2 Flat twin and earth","m",1]
[]
["7.8.16","4.0mm2 Flat twin and earth","m",1]
[]
["7.8.17","6.0mm2 Flat twin and earth","m",1]
[]
["7.9","LIGHT FITTINGS"]
[null,"Supply and install luminaires or equipment complete with  lamps, connections, etc mounted in position "]
[]
["7.9.1","2 # 1200mm Surface florescent","No",1]
[]
["7.9.2","2 # 1500mm Surface florescent","No",1]
[]
["7.9.3","2 # 18W Round bulkhead","No",1]
[]
["7.9.4","2 # 18W Square bulkhead ","No",1]
[]
["7.9.5","CFL light fitting for energy lights wall mounted","No",1]
[]
["7.9.6","4FT - CFL CFL Flourescent light for eneregy lights","No",1]
[]
["7.9.7","30W MH Highbay","No",1]
[]
["7.9.8","50W MH Highbay","No",1]
[]
["7.9.9","70W Mecury Vapour Floodlight","No",1]
[]
["7.9.10","400W Mecury Vapour Floodlight","No",1]
[]
["7.9.11","Flourescent lights starters: 220..240v","No",1]
[]
["7.9.12","Photo cells","No",1]
[]
["7.9.13","Poly bulkhead","No",1]
[]
["7.9.14","60W down light","No",1]
[]
["7.9.15","125W Mecury Vapour Reef light","No",1]
[]
["7.9.16","250W HPS Flood Light","No",1]
[]
["7.9.17","400W HPS Flood Light","No",1]
[]
["7.9.18","125W Pole Mounted Street Light","No",1]
[]
["7.9.17a","1000W HPS Flood Light","No",1]
[]
[null,"LED LIGHT FITTINGS"]
[]
[null,"\"BEKA\" OR EQUALLY APPROVED"]
[]
["7.9.17b","LEDflood48/117N1600A1G","No",1]
[]
["7.9.17c","LEDflood60/145N1600A1G","No",1]
[]
["7.9.18a","EC 35.1140-18W LED downlight, C/W LED engine and driver","No",1]
[]
["7.9.19","BEKA T-BAY 4 x FQ53W/940, medium beam complete with lamps","No",1]
[]
["7.9.20","Vapourlux 280 EVG, T5 complete with lamp (Alternative Ecolux 2 x 80W T5)","No",1]
[]
["7.9.21","Ecolux 2 x 58W, electronic ballast complete with lamp","No",1]
[]
["7.9.22","\"Bekabulk\" 12 LED, colour: RAL 7045 Telegrey 1","No",1]
[]
["7.10.","LIGHT BULBS AND GLOBES"]
[]
[null,"Changing light bulbs/globes with energy saving bulbs "]
[]
["7.10.1a","60 W Bulb","no",1]
[]
["7.10.1","100 W Bulb","no",1]
[]
["7.10.2","4FT Florascent bulb","no",1]
[]
["7.10.3","5FT Florascent bulb","no",1]
[]
["7.10.4","8FT Florascent bulb","no",1]
[]
["7.10.5","Ballast 220V DBL 75W","no",1]
[]
["7.10.6","200W Mercury bulb","no",1]
[]
["7.10.7","125W Mercury bulb","no",1]
[]
["7.10.8","400 W Mecury bulb","no",1]
[]
["7.10.9","60W downlight bulb","no",1]
[]
["7.11","LIGHTNING PROTECTION SYSTEMS "]
[null,"Installed in accordance with the latest SANS Codes of Practise 10199 (2004) and 10313 (2008) in conjuction with SANS 62305-1-2-3-4: 2007 and IEC 62305-1-2-3-4 :2006"]
[null,"Conductors, etc "]
[]
["7.11.1","Reinforced concrete bonding terminal ","No",1]
[]
["7.11.2","Earth electrode test joint ","No",1]
[]
["7.11.3","Tail type bonding terminal fixed to concrete reinforcing rods ","No",1]
[]
[]
["7.12","DISTRIBUTION BOARDS "]
[]
[null,"Flushand Surface Mounted Distibution Boards"]
[]
["7.12.1","12-Way Steel Distribution Board, complete with 1 Plastic Cover and 1 Steel Tray (Mini Rail) Flush Mounted","No",1]
[]
["7.12.2","12-Way Steel Distribution Board, complete with 1 Steel Cover and 1 Steel Tray (Mini Rail) Flush Mounted","No",1]
[]
["7.12.3","13-Way DMC Polyester Flush Distibution Board adjustable with plaster Gauge,  1 Polyester Cover and 1 Polyester Tray (Mini Rail) Flush and Surface Mounted","No",1]
[]
["7.12.4","13-Way Surface Mount Distibution Board (Mini Rail) Surface Mounted","No",1]
[]
["7.12.5","20-Way Steel Distribution Board, complete with 1 Steel Cover and 1 Steel Tray (Mini Rail) Flush Mounted","No",1]
[]
["7.12.6","20-Way Steel Distribution Board, complete with 1 Steel Cover and 1 Steel Tray (Mini Rail) Flush Mounted","No",1]
[]
["7.12.7","40-Way Architrave Board (2x20-Way and Tray)","No",1]
[]
["7.12.8","60-Way Architrave Board (3 x 20-Way and Tray)","No",1]
[]
["7.12.9","Labelling of DB Board (per label)","No",1]
[]
["7.13","CIRCUIT BREAKERS"]
[null,"Fully Installed complete to DB including interconnecting cables"]
[null,"Residential - 13mm Hydraulic Magnetic:"]
[null,"Single Pole"]
["7.13.1","5A (3kA) 1-Pole mcb's","No",1]
[]
["7.13.2","10A, 15A, 20A (3kA) 1-Pole mcb's","No",1]
[]
["7.13.3","25A, 30A, 35A, 40A (3kA) 1-Pole mcb's","No",1]
[]
["7.13.4","40A, 50A, 60A (3kA) 1-Pole mcb's","No",1]
[]
["7.13.4a","80A (3kA) 1-Pole mcb's","No",1]
[]
["7.13.4b","100A (3kA) 1-Pole mcb's","No",1]
[]
[null,"Double Pole"]
["7.13.5","5A (3kA) 2-Pole mcb's","No",1]
[]
["7.13.6","10A, 15A, 20A (3kA) 2-Pole mcb's","No",1]
[]
["7.13.7","25A, 30A, 35A, 40A (3kA) 2-Pole mcb's","No",1]
[]
["7.13.8","40A, 50A, 60A (3kA) 2-Pole mcb's","No",1]
[]
["7.13.8a","80A (3kA) 2-Pole mcb's","No",1]
[]
["7.13.8b","100A (3kA) 2-Pole mcb's","No",1]
[]
[null,"Tripple Pole"]
["7.13.8c","5A (3kA) 3-Pole mcb's","No",1]
[]
["7.13.8d","10A, 15A, 20A (3kA) 3-Pole mcb's","No",1]
[]
["7.13.8f","25A, 30A, 35A, 40A (3kA) 3-Pole mcb's","No",1]
[]
["7.13.8g","40A, 50A, 60A (3kA) 3-Pole mcb's","No",1]
[]
[]
[null,"Single Pole and Neutral"]
[]
["7.13.9","5A (3kA) 1-Pole + N mcb's","No",1]
[]
["7.13.10","10A, 15A, 20A, (3kA)  1-Pole + N mcb's","No",1]
[]
["7.13.11","25A, 30A, 35A, 40A, 50A (3kA)  1-Pole + N mcb's","No",1]
[]
["7.13.12","60A (3kA)  1-Pole + N mcb's","No",1]
[]
[null,"Tripple Pole and Neutral"]
[]
["7.13.13","5A, 10A, 15A, 20A, 25A (3kA)  3-Pole + N mcb's","No",1]
[]
["7.13.14","30A, 35A, 40A, 50A (3kA)  1-Pole + N mcb's","No",1]
[]
[null,"Commercial / Industrial- 13mm Hydraulic Magnetic:"]
[null,"Single Pole"]
["7.13.15","5A (6kA) 1-Pole mcb's","No",1]
[]
["7.13.16","10A, 15A, 20A (6kA) 1-Pole mcb's","No",1]
[]
["7.13.17","25A (6kA) 1-Pole mcb's","No",1]
[]
[null,"Double Pole"]
["7.13.18","5A (6kA) 2-Pole mcb's","No",1]
[]
["7.13.19","10A, 15A, 20A (6kA) 2-Pole mcb's","No",1]
[]
["7.13.20","25A  (6kA) 2-Pole mcb's","No",1]
[]
[null,"Tripple Pole"]
["7.13.21","5A (6kA) 3-Pole mcb's","No",1]
[]
["7.13.22","10A, 15A, 20A (6kA) 3-Pole mcb's","No",1]
[]
["7.13.23","25A  (6kA) 3-Pole mcb's","No",1]
[]
[null,"Single Pole and Neutral"]
[]
["7.13.24","5A, 10A, 15A, 20A (6kA) 1-Pole + N mcb's","No",1]
[]
["7.13.25","25A (6kA)  1-Pole + N mcb's","No",1]
[]
[null,"Tripple Pole and Neutral"]
[]
["7.13.26","5A, 10A, 15A, 20A (6kA) 3-Pole + N mcb's","No",1]
[]
["7.13.27","25A (6kA)  3-Pole + N mcb's","No",1]
[]
["7.14","ISOLATORS / SWITCH CONNECTORS"]
[]
["7.14.1","63A (3kA) 1-Pole Isolator","No",1]
[]
["7.14.2","63A (3kA) 2-Pole Isolator","No",1]
[]
["7.14.3","63A (3kA) 3-Pole Isolator","No",1]
[]
["7.14.4","63A (3kA) 4-Pole Isolator","No",1]
[]
["7.14.5","63A (6kA) 1-Pole Isolator","No",1]
[]
["7.14.6","63A (6kA) 2-Pole Isolator","No",1]
[]
["7.14.7","63A (6kA) 3-Pole Isolator","No",1]
[]
["7.14.8","63A (6kA) 4-Pole Isolator","No",1]
[]
["7.14.9","100A (6kA) 1-Pole Isolator","No",1]
[]
["7.14.10","100A (6kA) 2-Pole Isolator","No",1]
[]
["7.14.11","100A (6kA) 3-Pole Isolator","No",1]
[]
["7.14.12","100A (6kA) 4-Pole Isolator","No",1]
[]
["7.15","EARTH LEAKAGE PROTECTION"]
[]
["7.15.1","63A (N/A) 1-Pole + N","No",1]
[]
["7.15.2","63A (3kA) 1-Pole + N","No",1]
[null," "]
["7.15.3","63A (N/A) 3-Pole + N","No",1]
[]
["7.15.4","63A (3kA) 3-Pole + N","No",1]
[]
["7.15.5","63A (6kA) 1-Pole + N","No",1]
[]
["7.15.6","100A (6kA) 1-Pole + N","No",1]
[]
["7.15.7","63A (6kA) 3-Pole + N","No",1]
[]
["7.15.8","80A (6kA) 3-Pole + N","No",1]
[]
["7.15.9","100A (6kA) 1-Pole + N","No",1]
[]
[]
["7.16","CONNECTIONS "]
[]
[null,"NOTE TO USER OF MODEL BILL: "]
[]
["7.17","These items are for connecting geysers, stoves, etc "]
[]
["7.17.1","Geyser connection","no",1]
[]
["7.17.2","Stove connection","no",1]
[]
["7.17.3","Handryer connection","no",1]
[]
["7.17.4","Gate motor connection","no",1]
[]
["7.17.5","Air conditioning connection","no",1]
[]
["7.18","SUNDRIES "]
[]
["7.18.1","Testing and commissioning ","no",1]
[]
["7.18.2","Coc on existing installation ","no",1]
[]
["7.18.3","Coc on new installation ","no",1]
[]
["7.18.4","Cable warning tape placed 150mm above cables in excavations","m",1]
[]
["7.18.5","Fault tracing","no",1]
[]
["7.18.6","Geyser timer ","no",1]
[null," "]
["7.19","ALTERATIONS (Electrical works)"]
[]
[null,"Removal of faulty electrical components and carting off site"]
[]
["7.19.1","Removal of plugs, light switches, sockets etc","no",1]
[]
["7.19.2","Removal of cables and wires","m",1]
[]
["7.19.3","Removal of faulty stove connection, cover up and make good","no",1]
[]
["7.19.4","Removal of faulty Airconditioning connection","no",1]
[]
["7.19.5","Removal of faulty gate motor including base plate","no",1]
[]
["7.20.","GATE MOTORS"]
[null,"Supply and installation of a Gate Motor complete with backup battery, foundation plate, 4m rack, adaptor kit, lightning protection, sensor, intelligent speed control, lockable manual over ride, with two remotes, (electrical installation measured elsewhere). With a 12 months guarantee and 5-year warranty."]
["7.20.1","Centurion D2 or equivalent sliding gate motor  for gates up to 250kg ","no",1]
[]
["7.20.2","Centurion D5 or equivalent sliding gate motor  for gates up to 500kg ","no",1]
[]
["7.20.3","Centurion D10 or equivalent sliding gate motor  for gates up to 1000kg ","no",1]
[]
["7.21","AIR CONDITIONING UNITS"]
[]
[null,"Supply and install BTU Split Unit airconditioner complete, with a standard back to back installation, 2m of copper pipe, cable and drain pipe, an electrical power supply to nearest plug socket, and mounting brackets. Features must include a cooling and heating, minimum temp of 18°C and maximum temp of  30°C. With auto cool, power failure auto restart, electronic touch controls with remote, 12 hour on/off timer. With a 5-year warranty"]
[]
["7.21.1","9 000 BTU","no",1]
[]
["7.21.2","12 000 BTU","no",1]
[]
["7.21.3","18 000 BTU","no",1]
[]
["7.21.4","24 000 BTU","no",1]
[]
["7.21.5","30 000 BTU","no",1]
[]
["7.21.6","36 000 BTU","no",1]
[]
[null,"Supply and install BTU Cassette Unit airconditioner complete, with a standard  installation, 2m of copper pipe, cable and drain pipe, an electrical power supply to nearest plug socket, and mounting brackets. Features must include a cooling and heating, minimum temp of 18°C and maximum temp of  30°C. With auto cool, power failure auto restart, electronic touch controls with remote, 12 hour on/off timer. With a 5-year warranty"]
[]
["7.21.7","13 000 BTU","no",1]
[]
["7.21.8","19 000 BTU","no",1]
[]
["7.21.9","25 000 BTU","no",1]
[]
["7.21.10","36 000 BTU","no",1]
[]
["7.21.11","42000 BTU","no",1]
[]
["7.21.12","51 000 BTU","no",1]
[]
[null,"Supply and install BTU Ceiling / Console split Unit airconditioner complete, with a standard  installation, 2m of copper pipe, cable and drain pipe, an electrical power supply to nearest plug socket, and mounting brackets. Features must include a cooling and heating, minimum temp of 18°C and maximum temp of  30°C. With auto cool, power failure auto restart, electronic touch controls with remote, 12 hour on/off timer. With a 5-year warranty"]
[]
["7.21.13","19 000 BTU","no",1]
[]
["7.21.14","24 000 BTU","no",1]
[]
["7.21.15","35 600 BTU","no",1]
[]
["7.21.16","44 300 BTU","no",1]
[]
["7.21.17","47 900 BTU","no",1]
[]
[null,"Supply and install Window Unit airconditioner complete, with a standard  installation, 2m of copper pipe, cable and drain pipe, an electrical power supply to nearest plug socket, and mounting brackets. Features must include a cooling and heating, minimum temp of 18°C and maximum temp of  30°C. With auto cool, power failure auto restart, electronic touch controls with remote, 12 hour on/off timer. With a 5-year warranty"]
[]
["7.21.18","8 500 BTU","no",1]
[]
["7.21.19","12 000 BTU","no",1]
[]
["7.21.20","18 000 BTU","no",1]
[]
["7.21.21","23 000 BTU","no",1]
[]
[null,"SUNDRIES"]
[null,"Cleaning, Servicing  and re-gas Airconditioner"]
[]
["7.21.22","9 000 BTU, 12 000 BTU, & 18 000 BTU Split units","no",1]
[]
["7.21.23","24 000 BTU, 30 000 BTU, & 36 000 BTU","no",1]
[]
["7.21.24","42 000 BTU & 51 000 BTU","no",1]
[]
["7.22.","ELECTRICAL WORKS - LABOUR RATES"]
[]
[null,"Normal hours"]
[]
["7.22.1","General Labour (R per day)","hr",1]
[]
["7.22.2","Electrician Semi Skilled (R per day)","hr",1]
[]
["7.22.3","Electrician Artisan (R per day)","hr",1]
[]
[null,"After normal hours and Saturdays "]
[]
["7.22.4","General Labour ","hr",1]
[]
["7.22.5","Semi Skilled ","hr",1]
[]
["7.22.6","Electrician Artisan ","hr",1]
[]
[null,"Sundays and holidays"]
[]
["7.22.7","General Labour ","hr",1]
[]
["7.22.8","Semi Skilled ","hr",1]
[]
["7.22.9","Electrician Artisan ","hr",1]
[]
[null,"POWER GENERATOR"]
[]
["7.23","Including service plan for a period of three years @ 4 visits per annum and including 5 year guarantee. Supply, delivery, termination, connection and initial diesel full tank"]
[]
["7.23.1","3-Phase 165kVA diesel Generator.","no",1]
[]
["7.23.2","3-Phase 75kVA diesel Generator.","no",1]
["TOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"$f":"SUM(E11:E628)","v":0}]

{"sheet":"Plumbing & Drainage","index":3,"n_rows":215,"n_cols":5,"rows_kept":215,"merged":[[214,0,214,3]]}
[]
["Item No.","Description","Unit","Qty","Amount Including VAT"]
[]
[null,"SCHEDULE No. 7"]
[]
[null,"PLUMBING AND DRAINAGE"]
[]
[null,"Rates"]
[]
[null,"Rates shall include travel to and from site within a 30km. radius of the Works location, Materials, Labour, Tools, Equipment, Contractors Overheads and Profit except where otherwise stated."]
[]
[null,"Description"]
[]
[null,"Where \"Replace\" or \"Replacing\" appears in this document it shall be deemed to include taking up/out and carting away from site"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"uPVC pipes and fittings"]
[]
[null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings"]
[]
[null,"Soil, waste and vent pipes and fittings shall be solvent weld jointed"]
[]
[null,"uPVC pressure pipes and fittings"]
[]
[null,"Pipes for water supply shall be of the class stated"]
[]
[null,"Pipes of 40mm diameter and smaller shall be plain ended with solvent welded uPVC loose sockets and fittings"]
[]
[null,"Pipes of 50mm diameter and greater shall have sockets and spigots with push-in type integral rubber ring joints.  Bends shall be uPVC and all other fittings shall be cast iron, all with similar push-in type joints"]
[]
[null,"Copper pipes"]
[]
[null,"Pipes shall be hard drawn and half-hard pipes of the class stated.  Class 0 (thin walled hard drawn) pipes shall not be bent.  Class 1 (thin walled half-hard) class 2 (half-hard) and class 3 (heavy walled half-hard) pipes shall only be bent with benders with inner and outer formers.  Fitting to copper waste, vent and anti-syphon pipes, capillary solder fittings and compression fittings shall be \"Cobra Watertech\" type.  Capillary solder fittings shall comply with ISO 2016.  Only compression fittings shall be used in walls or in ground"]
[]
[null,"Reducing fittings"]
[]
[null,"Where fittings have reducing ends or branches they are described as \"reducing\".  In the case of pipes with diameters not exceeding 60mm only the largest end or branch size is given.  Should the contractor wish to use other fittings and bushes or reducers he may do so on the understanding that no claim in this regard will be entertained."]
[]
[null,"In the case of pipes with diameters exceeding 60mm all sizes are given and no claim for extra bushes, reducers, etc will be entertained"]
[]
[null,"Wire gratings"]
[]
[null,"Descriptions of gutter outlets etc shall be deemed to include wire balloon gratings"]
[]
[null,"Exposed concrete surfaces"]
[]
[null,"Exposed surfaces of concrete stormwater channels, cover slabs, inspection eye marker slabs, gully tops, cleaning eye tops, catchpits, inspection chambers, etc shall be finished smooth with plaster"]
[]
[null,"Excavations"]
[]
[null,"No claim for rock excavation will be entertained unless the contractor has timorously notified the Principal Agent thereof prior to backfilling"]
[]
[null,"\"Soft rock\" and \"hard rock\" shall be as defined in \"Earthworks\""]
[]
[null,"Laying, backfilling, bedding, etc of pipes"]
[]
[null,"Pipes shall be laid and bedded and trenches shall be carefully backfilled in accordance with manufacturers' instructions"]
[]
[null,"Where no manufactures' instructions exist pipes shall be laid in accordance with clause 5.1 and 5.2 of each of the following:"]
[null,"SABS 1200   L   :  Medium-pressure pipelines"]
[null,"                   LD  :  Sewers"]
[null,"                   LE  :  Stormwater drainage"]
[null,"Unless otherwise described bedding of rigid pipes shall be class B bedding"]
[]
[]
[null,"Flush pans"]
[]
[null,"Flush pans shall have straight or side outlets and \"P\" or \"S\" traps as necessary"]
[]
[null,"Stainless steel basins, sinks, wash troughs, urinals, etc"]
[]
[null,"Units shall have standard aprons an all exposed edges and tiling keys against walls where applicable"]
[]
[null,"Waste unions"]
[]
[null,"Descriptions of waste unions shall be deemed to include rubber or vulcanite plugs and chains fixed to fittings"]
[]
[]
[8,"CLEAR SEWER AND WASTE WATER BLOCKAGE"]
[]
[null,"Locate blockage, clear sewer pipes by means of rodding distances between access chambers/junctions (referred to as \"Pipe Length\") not exceeding 10m and removing all obstructions, etc. leaving pipes open and free flowing including disposal of all materials causing blockage, excavations and backfilling where required."]
[]
[null,"Pipe length not exceeding 10m Length"]
[]
["8.1","110mm diameter pipe not exceeding 10m","item",1]
[]
["8.2","160mm diameter pipe not exceeding 10m","item",1]
[]
[null,"Pipe length up to 20 m"]
[]
["8.3","110mm diameter pipe, exceeding 10m but not exceeding 20m","item",1]
[]
["8.4","160mm diameter pipe, exceeding 10m but not exceeding 20m","item",1]
[]
[null,"Locate blockage, clear waste pipes by means of rodding distances between access eyes/open end (referred to as \"Pipe Length\") not exceeding 2m and removing all obstructions, etc. leaving pipes open and free flowing including disposal of all materials causing blockage."]
[]
[null,"Pipe length not exceeding 10m Length"]
[]
["8.5","Not exceeding 40mm diameter pipe, not exceeding 10m","item",1]
[]
["8.6","Exceeding 40mm diameter pipe and not exceeding 75mm diameter pipe, not exceeding 10m","item",1]
[]
[null,"Pipe length exceeding 5m not exceeding 10m"]
[]
["8.7","Not exceeding 40mm diameter pipe, exceeding 10m but not exceeding 20m","item",1]
[]
["8.8","Exceeding 40mm diameter pipe and not exceeding 75mm diameter pipe, exceeding 10m but not exceeding 20m","item",1]
[]
[null,"Sundries"]
[]
["8.9","Unblock 'P', 'S' or bottle trap not exceeding 40mm diameter","no",1]
[]
["8.10","Unblock Gulley, WC pan, Trough urinal trap, etc. not exceeding 110mm diameter","no",1]
[]
[]
[null,"REPLACE DAMAGED UNDERGROUND SEWER PIPE AND FITTINGS"]
[]
[null,"Locate, excavate for and replace damage to uPVC drain pipe and / or fittings in landscaped areas including backfilling, compacting, etc. and leave in good working order."]
[]
[null,"Laid in excavations not exceeding 1m deep"]
[]
["8.11","110mm Ø pipe","m",1]
[]
["8.12","160mm Ø pipe","m",1]
[]
[null,"Laid in excavations exceeding 1m and not exceeding 2m deep"]
[]
["8.13","110mm Ø pipe","m",1]
[]
["8.14","160mm Ø pipe","m",1]
[]
[null,"uPVC fittings"]
[]
["8.15","110mm Access lid","no",1]
[]
["8.16","110mm Gulley grate","no",1]
[]
["8.17","110mm Plain bend","no",1]
[]
["8.18","110mm Access bend","no",1]
[]
["8.19","110mm Plain junction","no",1]
[]
["8.20","110mm Access junction","no",1]
[]
["8.21","110mm Rodding eye","no",1]
[]
["8.22","110mm Gulley head and grate","no",1]
[]
["8.23","110mm Gulley 'P' trap","no",1]
[]
["8.24","160mm Access lid","no",1]
[]
["8.25","160mm Plain bend","no",1]
[]
["8.26","160mm Access bend","no",1]
[]
["8.27","160mm Plain junction","no",1]
[]
["8.28","160mm Access junction and cover","no",1]
[]
["8.29","160mm Rodding eye","no",1]
[]
["8.30","160 x 110mm Taper pipe","no",1]
[]
[]
[null,"REPLACE DAMAGED GRATINGS, MANHOLE COVERS, ETC."]
[]
[null,"Carefully break out from concrete existing damaged frame and grating or manhole cover, replace with new including making good all existing finishers and leave in good working order."]
[]
["8.31","560mm Diameter 125mm thick precast concrete removable cover","no",1]
[]
["8.32","450 x 450mm x 28,5kg Type 14B cast iron single seal manhole cover and frame.","no",1]
[]
["8.33","450 x 600mm x 68kg Type 9D cast iron single seal manhole cover and frame.","no",1]
[]
["8.34","530 x 530mm x 67kg Type 12 cast iron single seal manhole cover and frame.","no",1]
[]
["8.35","450 x 600mm x 72kg Type 8A cast iron double seal manhole cover and frame.","no",1]
[]
[null,"PLUMBING WORKS - LABOUR RATES"]
[]
[null,"Normal hours"]
[]
["8.36","General Labour (R per day)","hr",1]
[]
["8.37","Semi Skilled (R per day)","hr",1]
[]
["8.38","Plumbing Artisan (R per day)","hr",1]
[]
[null,"After normal hours and Saturdays "]
[]
["8.39","General Labour ","hr",1]
[]
["8.40","Semi Skilled ","hr",1]
[]
["8.41","Plumbing Artisan ","hr",1]
[]
[null,"Sundays and holidays"]
[]
["8.42","General Labour ","hr",1]
[]
["8.43","Semi Skilled ","hr",1]
[]
["8.44","Plumbing Artisan ","hr",1]
[]
[]
[null,"TESTING AND COMMISIONING"]
[]
["8.45","Leak detection","no",1]
[]
["8.46","Certificate of Compliance for Geyser installations and other new piping installation. (No COC for repair work)","no",1]
[]
["TOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":3},{"$f":"SUM(E86:E213)","v":0}]