{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["RATES- SOUTH-SOUTHWEST-NORTH","YEAR 2","Sheet2"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"RATES- SOUTH-SOUTHWEST-NORTH","index":0,"n_rows":123,"n_cols":14,"rows_kept":123,"merged":[[0,8,0,9],[0,10,0,11],[0,12,0,13],[2,0,2,9],[3,2,3,9],[8,1,8,9],[32,0,32,9],[62,0,62,1],[90,0,90,1]],"flags":["formulas_cached_only"]}
[{"$nulls":8},"YEAR 1",null,"YEAR 2",null,"YEAR 3"]
["ITEM","Payment","Description","Qty"," Rate  ","Amount","Unit","Qty"," Rate  ","Amount"," Rate  ","Amount"," Rate  ","Amount"]
["SECTION A: SOUTH CENTRAL"]
["A1",null,"Section A1: Preliminary and General"]
[]
["A2",null,"Section A2:  Reinstatements: "]
[null,null,"Inspections and Earthworks"]
["A2.1",null,"Rates are to cover for all contractual requirements, site inspections, site establishment, Health and Safety requirements, labour, plant, material and site supervision (Per call out payable to the contractor)",{"$nulls":3},"Sum"]
["A2.1.1","Asphalt Surfaces (Refer to Drawing Nº 1)"]
["A2.1.2",null,"Remove existing backfill material in pipe trenches to 1000mm maximum depth and dispose of as directed by the Engineer or to a designated site",1,null,null,"m³",1]
["A2.1.3",null,"Supply, handle, place and compact to 95% Mod AASHTO, G5 material in 150mm thick layers, up to a depth of 350mm below finished road level. Rate to include for transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["A2.1.4",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["A2.1.5",null,"Supply all material and construct asphalt layer 40mm thick, including tack coat at 0.3 l/m², transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["A2.2",null,"Brick Paved Surfaces (Refer to 1)"]
["A2.2.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["A2.2.3",null,"Ditto item A2.2.2 using imported granular material from commercial sources",1,null,null,"m³",1]
["A2.2.4",null,"Supply and apply weed killer and a 25mm thick overlying sand bed, including all material, transportation, plant, equipment and labour",1,null,null,"m²",1]
["A2.2.5",null,"Lay inter-locking brick paving using existing bricks, including cleaning of bricks, jointing and all plant and labour",1,null,null,"m²",1]
["A2.2.6",null,"Supply, handle and lay inter-locking brick paving, including jointing and all plant and labour",1,null,null,"m²",1]
["A2.2.7",null,"Supply, handle and lay Kerb Type 6 precast concrete kerbing, including all labour, plant and material.",1,null,null,"m",1]
["A2.3",null,"Concrete Surfaces (Refer to Drawing Nº 1):"]
["A2.3.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["A2.3.2",null,"Backfill trenches using selected granular material from stockpile, in 150mm thick layers compacted to 95% Mod AASHTO. Excess or unsuitable backfill material to be disposed of as directed by the Engineer",1,null,null,"m³",1]
["A2.3.3",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["A2.3.4",null,"Supply all material and construct 150mm thick, Grade 25 Mpa/19mm concrete slab, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["A2.4",null,"Boundary walls"]
["A2.4.1",null,"Remove existing damaged building material and dipose to an accredited landfill site. ",1,null,null,"m³",1]
["A2.4.2",null,"Supply all material and construct 300 mm thick, Grade 25 Mpa/19mm concrete foundation, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["A2.4.3",null,"Supply all material and construct maximum 2 m high plastered wall (brickwork) with paint to match the existing colour, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
[null,null,"Price Summary \"Section A\"",17,0,0]
[]
[]
["SECTION B:  AREA NORTH"]
["Item",null,"Description","Qty"," Rate  ","Amount","Unit","Qty"," Rate  ","Amount"," Rate  ","Amount"," Rate  ","Amount"]
[null,null,"Section B1: Preliminary and General"]
["B2",null,"Section B2:  Reinstatements"]
[null,null,"Inspections and Earthworks"]
["B2.1",null,"Rates are to cover for all contractual requirements, site inspections, site establishment, Health and Safety requirements, labour, plant, material and site supervision (Per call out payable to the contractor)",{"$nulls":3}," Sum"]
["B2.1.1",null,"Asphalt Surfaces (Refer to Drawing Nº 1):"]
["B2.1.2",null,"Remove existing backfill material in pipe trenches to 1000mm maximum depth and dispose of as directed by the Engineer or to a designated site",1,null,null,"m³",1]
["B2.1.3",null,"Supply, handle, place and compact to 95% Mod AASHTO, G5 material in 150mm thick layers, up to a depth of 350mm below finished road level. Rate to include for transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["B2.1.4",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["B2.1.5",null,"Supply all material and construct asphalt layer 40mm thick, including tack coat at 0.3 l/m², transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["B2.2",null,"Brick Paved Surfaces (Refer to Drawing Nº 1): "]
["B2.2.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["B2.2.2",null,"Backfill trenches using selected granular material from stockpile, in 150mm thick layers compacted to 95% Mod AASHTO. Excess or unusable backfill material to be disposed of as directed by the Engineer",1,null,null,"m³",1]
["B2.2.3",null,"Ditto item B2.2.2 using imported granular material from commercial sources",1,null,null,"m³",1]
["B2.2.4",null,"Supply and apply weed killer and a 25mm thick overlying sand bed, including all material, transportation, plant, equipment and labour",1,null,null,"m²",1]
["B2.2.5",null,"Lay inter-locking brick paving using existing bricks, including cleaning of bricks, jointing and all plant and labour",1,null,null,"m²",1]
["B2.2.6",null,"Supply, handle and lay inter-locking brick paving, including jointing and all plant and labour",{"$nulls":3},"m²"]
["B2.2.7",null,"Supply, handle and lay Kerb Type 6 precast concrete kerbing, including all labour, plant and material.",1,null,null,"m",1]
["B2.3",null,"Concrete Surfaces (Refer to Drawing Nº 1):"]
["B2.3.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",{"$nulls":3},"m³"]
["B2.3.3",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["B2.3.4",null,"Supply all material and construct 150mm thick, Grade 25 Mpa/19mm concrete slab, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["B2.4",null,"Boundary walls"]
["B2.4.1",null,"Remove existing damaged building material and dipose to an accredited landfill site. ",1,null,null,"m³",1]
["B2.4.2",null,"Supply all material and construct 300 mm thick, Grade 25 Mpa/19mm concrete foundation, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["B2.4.3",null,"Supply all material and construct maximum 2 m high plastered wall (brickwork) with paint to match the existing colour, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
[null,null,"Price Summary \"Section B\""]
[]
[]
["                                               SECTION C:  SOUTH"]
["Item","Payment","Description","Qty"," Rate  ","Amount","Unit","Qty"," Rate  ","Amount"," Rate  ","Amount"," Rate  ","Amount"]
[null,null,"Section C1:  Preliminary and General"]
[null,null,"Inspections and Earthworks"]
["C2.1",null,"Rates are to cover for all contractual requirements, site inspections, site establishment, Health and Safety requirements, labour, plant, material and site supervision (Per call out payable to the contractor)",{"$nulls":3}," Sum"]
[null,null,"Total carried forward"]
["C2.1.1",null,"Asphalt Surfaces (Refer to Drawing Nº 1):"]
["C2.1.2",null,"Remove existing backfill material in pipe trenches to 1000mm maximum depth and dispose of as directed by the Engineer or to a designated site",1,null,null,"m³",1]
["C2.1.3",null,"Supply, handle, place and compact to 95% Mod AASHTO, G5 material in 150mm thick layers, up to a depth of 350mm below finished road level. Rate to include for transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["C2.1.4",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["C2.1.5",null,"Supply all material and construct asphalt layer 40mm thick, including tack coat at 0.3 l/m², transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["C2.2",null,"Brick Paved Surfaces (Refer to Drawing Nº 1):"]
["C2.2.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["C2.2.2",null,"Backfill trenches using selected granular material from stockpile, in 150mm thick layers compacted to 95% Mod AASHTO. Excess or unusable backfill material to be disposed of as directed by the Engineer",1,null,null,"m³",1]
["C2.2.3",null,"Ditto item C2.2.2 using imported granular material from commercial sources",1,null,null,"m³",1]
["C2.2.4",null,"Supply and apply weed killer and a 25mm thick overlying sand bed, including all material, transportation, plant, equipment and labour",1,null,null,"m²",1]
["C2.2.5",null,"Lay inter-locking brick paving using existing bricks, including cleaning of bricks, jointing and all plant and labour",1,null,null,"m²",1]
["C2.2.6",null,"Supply, handle and lay inter-locking brick paving, including jointing and all plant and labour",1,null,null,"m²",1]
["C2.2.7",null,"Supply, handle and lay Kerb Type 6 precast concrete kerbing, including all labour, plant and material.",1,null,null,"m",1]
["C2.3",null,"Concrete Surfaces (Refer to Drawing Nº 1):"]
["C2.3.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["C2.3.3",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["C2.3.4",null,"Supply all material and construct 150mm thick, Grade 25 Mpa/19mm concrete slab, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["C2.4",null,"Boundary walls"]
["C2.4.1",null,"Remove existing damaged building material and dipose to an accredited landfill site. ",1,null,null,"m³",1]
["C2.4.2",null,"Supply all material and construct 300 mm thick, Grade 25 Mpa/19mm concrete foundation, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["C2.4.3",null,"Supply all material and construct maximum 2 m high plastered wall (brickwork) with paint to match the existing colour, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
[null,null,"Price Summary \"Section C\""]
["                                               SECTION C:  SOUTH WEST"]
["Item","Payment","Description","Qty"," Rate  ","Amount","Unit","Qty"," Rate  ","Amount"," Rate  ","Amount"," Rate  ","Amount"]
[null,null,"Section D1:  Preliminary and General"]
[null,null,"Inspections and Earthworks"]
["D2.1",null,"Rates are to cover for all contractual requirements, site inspections, site establishment, Health and Safety requirements, labour, plant, material and site supervision (Per call out payable to the contractor)",{"$nulls":3}," Sum"]
[null,null,"Total carried forward"]
["D2.1.1",null,"Asphalt Surfaces (Refer to Drawing Nº 1):"]
["D2.1.2",null,"Remove existing backfill material in pipe trenches to 1000mm maximum depth and dispose of as directed by the Engineer or to a designated site",1,null,null,"m³",1]
["D2.1.3",null,"Supply, handle, place and compact to 95% Mod AASHTO, G5 material in 150mm thick layers, up to a depth of 350mm below finished road level. Rate to include for transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["D2.1.4",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["D2.1.5",null,"Supply all material and construct asphalt layer 40mm thick, including tack coat at 0.3 l/m², transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["D2.2",null,"Brick Paved Surfaces (Refer to Drawing Nº 1):"]
["D2.2.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["D2.2.2",null,"Backfill trenches using selected granular material from stockpile, in 150mm thick layers compacted to 95% Mod AASHTO. Excess or unusable backfill material to be disposed of as directed by the Engineer",1,null,null,"m³",1]
["D2.2.3",null,"Ditto item C2.2.2 using imported granular material from commercial sources",1,null,null,"m³",1]
["D2.2.4",null,"Supply and apply weed killer and a 25mm thick overlying sand bed, including all material, transportation, plant, equipment and labour",1,null,null,"m²",1]
["D2.2.5",null,"Lay inter-locking brick paving using existing bricks, including cleaning of bricks, jointing and all plant and labour",1,null,null,"m²",1]
["D2.2.6",null,"Supply, handle and lay inter-locking brick paving, including jointing and all plant and labour",1,null,null,"m²",1]
["D2.2.7",null,"Supply, handle and lay Kerb Type 6 precast concrete kerbing, including all labour, plant and material.",1,null,null,"m",1]
["D2.3",null,"Concrete Surfaces (Refer to Drawing Nº 1):"]
["D2.3.1",null,"Remove existing backfill material in pipe trenches to 650mm maximum depth and stock pile on site",1,null,null,"m³",1]
["D2.3.3",null,"Supply all material and construct G2 granular material layer works compacted to 98% Mod AASHTO in 150mm layers, including transportation of material, plant, equipment and labour",1,null,null,"m³",1]
["D2.3.4",null,"Supply all material and construct 150mm thick, Grade 25 Mpa/19mm concrete slab, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["D2.4",null,"Boundary walls"]
["D2.4.1",null,"Remove existing damaged building material and dipose to an accredited landfill site. ",1,null,null,"m³",1]
["D2.4.2",null,"Supply all material and construct 300 mm thick, Grade 25 Mpa/19mm concrete foundation, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
["D2.4.3",null,"Supply all material and construct maximum 2 m high plastered wall (brickwork) with paint to match the existing colour, including transportation of material, plant, equipment and labour",1,null,null,"m²",1]
[null,null,"Price Summary \"Section D\""]
["E",null,"Total from SECTION A"]
["F",null,"Total from SECTION B"]
["G",null,"Total from SECTION C"]
["H",null,"Total from SECTION D"]
[null,null,"TOTAL TO FORM OF TENDER"]

{"sheet":"YEAR 2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet2","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}