**Turbo transfer system Specifications**

* User interface with programmable methods and pre-programmed methods
* Interface notifications – no load detection, power fail, no cassette detection, end of run
* Protocol setting limit – 1-25V with 1V increments
* X 2 blotting cassettes
* Cassettes for transfer to 2 mini gels or one midi gel
* Anode- platinized titanium electrode
* Cathode stainless steel