{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["BOQ","SUMMARY"],"read":"whole","date_system":"1900"}

{"sheet":"BOQ","index":0,"n_rows":1542,"n_cols":5,"rows_kept":1542,"merged":[[2,0,2,4],[181,0,182,0],[181,2,182,2],[181,3,182,3],[181,4,182,4],[345,0,346,0],[345,1,346,1],[345,2,346,2],[345,4,346,4],[1546,1,1546,2],[1547,1,1547,4],[1548,1,1548,4],[1549,1,1549,2],[1550,1,1550,2],[1551,1,1551,2],[1552,1,1552,2],[1553,1,1553,2],[1554,1,1554,4],[1555,1,1555,2],[1556,1,1556,2],[1557,1,1557,2],[1558,1,1558,2],[1559,1,1559,2],[1560,1,1560,4],[1561,1,1561,2],[1562,1,1562,2],[1563,1,1563,4],[1564,1,1564,4],[1565,1,1565,4],[1566,1,1566,2],[1567,1,1567,2],[1569,1,1569,2],[1571,1,1571,2],[1573,1,1573,2],[1575,1,1575,2],[1577,1,1577,2]]}
["                                                                       BILL OF QUANTITIES"]
[]
[" PANEL OF CONTRACTORS FOR URBAN ROADS AND STORMWATER REHABILITATION (RATE ONLY CONTRACT FOR 3 YEARS)"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 1200: GENERAL REQUIREMENTS AND PROVISIONS"]
[]
["B12.01","Protection, removal, re-alignment and replacement of services"]
[]
[null,"a)The removal, protection and replacement of utility services"]
[]
[null,"i)Telkom services","PC Sum",null," RATE ONLY "]
[null,"ii)Eskom services","PC Sum",null," RATE ONLY "]
[null,"iii)Water services ","PC Sum",null," RATE ONLY "]
[]
[null,"b)Handling cost and profit in respect of subitem B12.01(a)(i),"]
[null,"(ii) and (iii)","%",null," RATE ONLY "]
[]
["B12.02","a) Survey required by the Engineer","PC Sum",null," RATE ONLY "]
[]
[null,"b)Handling cost and profit in respect of subitem B12.02(a)","%",null," RATE ONLY "]
[]
["B12.03","Provision of a Community Liaison Officer"]
[]
[null,"a) Wages, salary, allowances, etc ","day",null," RATE ONLY "]
[]
[null,"b)Handling cost and profit in respect of subitem B12.03(a) above","%"]
[]
["B12.04","Environmental Control"]
[null,"a)Allowance for Environmental Control Officer","PC Sum",null," RATE ONLY "]
[]
[null,"b)Handling cost and profit in respect of subitem B12.04(a)","%",null," RATE ONLY "]
{"$rows_empty":13}
[" 1200","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE","AMOUNT"]
[null,"SECTION 1300: CONTRACTOR'S ESTABLISHMENT ON SITE"]
[null,"AND GENERAL OBLIGATIONS"]
[]
["B13.01","The Contractor's general obligations"]
[]
[null,"a)Fixed obligations","lump sum",null," RATE ONLY "]
[]
[null,"b)Value-Related obligations","lump sum",null," RATE ONLY "]
[]
[null,"c)Time-related obligations","month",null," RATE ONLY "]
[]
[]
["B13.02","Health and Safety","Prov Sum",null," RATE ONLY "]
[]
[null,"a) Fixed obligations for the preparation of risk assessments and completing and checking, the project OH & S file, etc.","Sum",null," RATE ONLY "]
[]
[null,"(b) Time related obligations for updating the risk assessments, etc"]
[null,"(i) Updating and amending the risk assessments, safe work procedures, project health and safety plan, and compliance with relevant legislation","Month",null," RATE ONLY "]
[null,"(ii) Safety officer","Month",null," RATE ONLY "]
[]
["B13.03","Contract sign boards","No",null," RATE ONLY "]
[]
[13.04,"Supply safety signage for camp site"]
[]
[null,"(a) Information signboard at entrance to site office","Sum",null," RATE ONLY "]
{"$rows_empty":16}
[1300,"TOTAL CARRIED TO SUMMARY"]
[]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 1400: HOUSING, OFFICES AND LABORATORIES"]
[null,"FOR THE ENGINEER'S SITE PERSONNEL"]
["14.01","The provision of accommodation as specified, including roof, "]
[null,"external and internal walls, windows complete with glazing, doors"]
[null,"with locks and fittings, burglar proofing, painting, floors, fencing,"]
[null,"the provision of a 220/250 volt electrical installation with wiring,"]
[null,"switchboards, etc, water and sewerage installation, and stores,"]
[null,"complete, in accordance with the drawings and specifications,"]
[null,"except for items scheduled elsewhere:"]
[]
[null,"e)Ablution units","No",null," RATE ONLY "]
[]
["14.08","Services:"]
[null,"The provision of water, electricity, low-pressure gas, sewerage,"]
[null,"septic tanks, sewage and rubbish removal, cleaning services,"]
[null,"maintenance and repairs, all as specified in clause 1404, including"]
[null,"the construction and maintenance of the access roads, footpaths,"]
[null,"etc:"]
[]
[null,"a)Services at offices and laboratories:"]
[null,"(i)Fixed costs","lump sum",null," RATE ONLY "]
[null,"(ii)Running costs","month",null," RATE ONLY "]
{"$rows_empty":18}
[" 1400","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 1500: ACCOMMODATION OF TRAFFIC"]
[]
["15.01","Accommodating traffic and maintaining temporary deviations","km",null," RATE ONLY "]
[]
["15.03","Temporary traffic-control facilities:"]
[]
[null,"a)Flagmen","man-day",null," RATE ONLY "]
[]
[null,"b)Portable STOP and GO-RY signs","No",null," RATE ONLY "]
[]
[null,"e)Road Signs, R- and TR- series (1200mm diameter)","No",null," RATE ONLY "]
[]
[null,"f)Road Signs, TW Series (1200mm side)","No",null," RATE ONLY "]
[]
[null,"g) Road signs, STW-, DTG-, TGS- AND TG-series (excluding"]
[null,"delineators and barricades)","m2",null," RATE ONLY "]
[]
[null,"h)Delineators (800mm x 200mm)"]
[]
[null,"i)Single","No",null," RATE ONLY "]
[]
[null,"ii)Mounted back to back","No",null," RATE ONLY "]
[]
[null,"i)Movable barricade / road sign combination (2400 mm wide)","No",null," RATE ONLY "]
[]
[null,"j)Traffic cones (450mm)","No",null," RATE ONLY "]
[]
[null,"m)Two-way communication devices","No",null," RATE ONLY "]
[]
[15.09,"Maintenance of the bituminous surfacing and pavement of"]
[null,"temporary deviations with bituminous surfacing and existing roads"]
[null,"with bituminous surfacing used as temporary deviations","Prov Sum",null," RATE ONLY "]
[]
[15.1,"Accommodation of traffic where the road is constructed in"]
[null,"half-widths","km",null," RATE ONLY "]
[]
[]
[]
[]
[]
[1500,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 1600: OVERHAUL "]
[]
[16.02,"Overhaul on material hauled in excess of ","m³-km",null," RATE ONLY "]
[null,"1.0km (ordinary overhaul)"]
{"$rows_empty":36}
[1600,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 1700: CLEARING AND GRUBBING"]
[null,"Rates shall include all work necessary for the clearing of the surface, the removal of trees and stumps( exluding large) demolishing and disposal of structures and material."]
[]
["17.01","Clearing and grubbing","ha",null," RATE ONLY "]
[]
["17.05","Cleaning out of hydraulic structures:"]
[]
[null,"a)Pipes with an internal diameter up to and including 750mm","m3",null," RATE ONLY "]
[]
[null,"b)Pipes with an internal diameter exceeding 750mm","m3",null," RATE ONLY "]
[]
[null,"c) Box culverts up to and including 1,5m vertical dimension","m3",null," RATE ONLY "]
[]
[null,"d)Box culverts exceeding 1,5m vertical dimension","m3",null," RATE ONLY "]
[]
[null,"e)Pipe Jetting","day",null," RATE ONLY "]
{"$rows_empty":25}
[" 1700"," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 2100: DRAINS"]
[]
["21.01","Excavation for open drains :"]
[]
[null,"a)Excavating soft material situated within the following"]
[null,"depth ranges below the surface level :"]
[]
[null,"i) 0 m up to 1,5 m ","m3",null,"RATE ONLY"]
[null,"ii) 1.5m up to 3.0m ","m3",null,"RATE ONLY"]
[]
[]
["21.02","Clearing and shaping existing open drains","m3",null,"RATE ONLY"]
[]
["21.03","Excavation for subsoil drainage systems :"]
[]
[null,"a)Excavating soft material situated within the following depth"]
[null,"ranges below the surface level:"]
[]
[null,"i)0 m up to 1,5 m ","m3",null,"RATE ONLY"]
[]
[" 21.04","Impermeable backfilling to subsoil drainage systems","m3 ",null,"RATE ONLY"]
[]
[" 21.06","Natural permeable material in subsoil drainage systems "," m3 ",null,"RATE ONLY"]
[null,"(crushed stone)"]
[]
[" 21.07","Natural permeable material in subsoil drainage systems"," m3 ",null,"RATE ONLY"]
[null,"(sand)"]
[]
["21.08","Pipes in subsoil drainage systems "]
[null,"(b) 110mm diameter - Unplasticized PVC pipes and fittings, ","m ",null,"RATE ONLY"]
[null,"normal duty, complete with couplings, perfoRATEd or slotted"]
[]
["21.10","Synthetic-fibre filter fabric"]
[null,"(a) A4 Geotextile Membrane","m² ",null,"RATE ONLY"]
[]
[" 21.13","Concrete caps for subsoil drain pipes"," No",null,"RATE ONLY"]
[]
[" 21.14","Repairing or replacing existing drainage systems"," Prov Sum",null,"RATE ONLY"]
[]
["21.15","Overhaul for martial hauled in excess of 1.0 km","m³-km",null,"RATE ONLY"]
[null,"With 1.0km free haul"]
[]
["21.16","Backfilling existing eroded side drains","m³",null,"RATE ONLY"]
[]
["21.17","Test flushing of pipe subsoil drains","No",null,"RATE ONLY"]
[]
["21.18","Excavation for the clearing of existing drainage manholes"]
[null,"a) Manholes and inlet and outlet structures","m³",null,"RATE ONLY"]
[null,"b) Culvert barrels","m³",null,"RATE ONLY"]
[null,"c) Concrete side drains","m³",null,"RATE ONLY"]
[]
[" 2100","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 2200: PREFABRICATED CULVERTS"]
[]
["22.01","Excavation:"]
[null,"a) Excavating soft material situated within the following"]
[null,"depth ranges below the surface level:"]
[null,"i)0 m up to 1.5 m","m3",null,"RATE ONLY"]
[null,"ii)Exceeding 1,5m and up to 3,0m","m3",null,"RATE ONLY"]
[null,"iii)Exceeding 3.0m and up to 4.5m","m3",null,"RATE ONLY"]
[]
["22.02","Backfilling:"]
[null,"a)Using the excavated material","m3",null,"RATE ONLY"]
[null,"b)Using imported selected material","m3",null,"RATE ONLY"]
[null,"c)Extra over subitems 22.02(a) and (b) for soil cement","m3",null,"RATE ONLY"]
[null,"backfilling (up to and including 3% cement content)"]
[]
[null,"Rates shall include full compensation for supply, testing, delivery, for placing the selected granular material where required and for the insallation, laying and jointing of the culverts structures,manholes and headwalls as specified "]
[]
["22.03","Concrete pipe culverts:"]
[null,"c)On class C bedding, 100D spigot and socket"]
[null,"i)450 mm diameter","m",null,"RATE ONLY"]
[null,"ii)600 mm diameter ","m",null,"RATE ONLY"]
[null,"iii)900 mm diameter ","m",null,"RATE ONLY"]
[null,"iv) 1200 mm diameter ","m ",null,"RATE ONLY"]
[]
["22.05","Portal and Rectangular Culverts:"]
[null,"b) Without prefabricated floor slabs:  "]
[]
[null,"(i) size 1.2m x 1.2m precast concrete rectangular portal culvert  ","No",null,"RATE ONLY"]
[null,"(ii) size 1.5m x 1.5m precast concrete rectangular portal culvert  ","No",null,"RATE ONLY"]
[null,"(iii) size 1.8m x 1.8m precast concrete rectangular portal culvert  ","No",null,"RATE ONLY"]
[null,"(iv) size 2.1m x 2.1m precast concrete rectangular portal culvert  ","No",null,"RATE ONLY"]
[]
["22.09","Prefabricated concrete inlets and outlets culverts (headwalls, wingwalls with apron complete)"]
[]
[null,"i)450 mm diameter","No",null,"RATE ONLY"]
[null,"ii)600 mm diameter ","No",null,"RATE ONLY"]
[null,"iii)900 mm diameter ","No",null,"RATE ONLY"]
[null,"iv) 1200 mm diameter ","No",null,"RATE ONLY"]
[]
["22.12","Removing existing concrete:"]
[null,"a)Plain concrete","m3",null,"RATE ONLY"]
[null,"b)Reinforced concrete","m3",null,"RATE ONLY"]
[]
["22.13","Removing and re-laying existing pipes"]
[]
[null,"On any class bedding, 100D spigot and socket"]
[null,"i)450 mm diameter","m",null,"RATE ONLY"]
[null,"ii)600 mm diameter ","m",null,"RATE ONLY"]
[null,"iii)900 mm diameter ","m",null,"RATE ONLY"]
[null,"iv) 1200 mm diameter ","m ",null,"RATE ONLY"]
[]
[]
["22.17","Manholes, catchpits, precast inlet and outlet structures complete:"]
[null,"a)Manholes",null,null,"RATE ONLY"]
[null,"(i) Depth exceeding 0m up to 1,5m","No"]
[null,"(i) Depth exceeding 1.5m up to 2,5m","No"]
[]
[null,"b)Catchpits"]
[null,"(i)Single sided (single splay)","No",null,"RATE ONLY"]
[null,"(ii)Double sided (double splay)","No",null,"RATE ONLY"]
[]
[null,"c)Headwalls"]
[null,"(i)450 diameter pipe","No",null,"RATE ONLY"]
[null,"(ii)600 diameter pipe","No",null,"RATE ONLY"]
[null,"(iii)900 diameter pipe ","No",null,"RATE ONLY"]
[]
["22.18","a)110mm thick","m²",null,"RATE ONLY"]
[null,"b)220mm thick","m²",null,"RATE ONLY"]
[]
[" 22.20","Benching","m²",null,"RATE ONLY"]
[]
[]
[2200,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 2200: PREFABRICATED CULVERTS"]
[]
["22.21 ","Accessories "]
[null,"(a) Manhole covers including frames (heavy duty)","No ",null,"RATE ONLY"]
[null,"(b) inlet grids ","No",null,"RATE ONLY"]
[null,"(c) step irons ","No",null,"RATE ONLY"]
[]
[" 22.26","Hand excavations to determine position of existing services","m³",null,"RATE ONLY"]
[]
["22.27","Reinstating trenches crossing roads"]
[null,"a) Selected layers "]
[null,"b) subbase"]
[null,"c) base (including prime coat)","m²",null,"RATE ONLY"]
[null,"ii)Exceeding 1,5m and up to 3,0m","m²",null,"RATE ONLY"]
{"$rows_empty":26}
["2200 ","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 2300: CONCRETE KERBING, CONCRETE "]
[null,"CHANNELLING, CHUTES AND DOWNPIPES, AND CONCRETE"]
[null,"LININGS FOR OPEN DRAINS"]
[]
[null,"Rate to include suply, delivery, full length haunching, excavation, base and channel."]
[]
["23.02","Concrete kerbing-channelling combination (30/19 concrete)"]
[null,"a)Barrier kerb and 300mm wide channel (Fig 3)","m",null," RATE ONLY "]
[null,"c)Semi-mountable kerb and 300mm wide channel (Fig 6)","m",null," RATE ONLY "]
[null,"b)Semi-Mountable Kerb only (Fig 7)","m",null," RATE ONLY "]
[null,"c)Mountable kerb (Fig 8)","m",null," RATE ONLY "]
[null,"d) Figure 12 - Mini Precast edge restraint ","m",null," RATE ONLY "]
[]
["23.04","Cast insitu concrete chute "]
[null,"a)Concrete (25/19 concrete)","m",null," RATE ONLY "]
[null,"b)Formwork Class F1 Finish ","m",null," RATE ONLY "]
[]
["23.07","Trimming of excavations for concrete-lined open drains"]
[null,"(a) In soft material ","m2",null," RATE ONLY "]
[null,"(b) In hard material","m2",null," RATE ONLY "]
[]
[" 23.08","Concrete lining for open drains"]
[null,"(a) Cast in situ concrete lining Class 30/19:"]
[null,"(i) For standard V-drain as per drawing SD0601/2","m3",null," RATE ONLY "]
[]
[null,"(b) Class U2 surface finish to side drains","m2",null," RATE ONLY "]
[]
["23.09","Formwork to cast in situ concrete lining for open drains (Class F2 surface finish)"]
[null," (b) To sides with formwork on both internal and external faces","m2",null," RATE ONLY "]
[null,"(c) To ends of slabs","m2",null," RATE ONLY "]
[]
[" 23.10","Sealed joints in concrete linings of open drains"]
[null,"(a) Closed cell expanded polyethylene sealants","m",null," RATE ONLY "]
{"$rows_empty":8}
["2300 ","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 3300: MASS EARTHWORKS"]
[]
["33.01","Cut and borrow to fill including all haulauge (Roadbed preparation and compaction of material)"]
[null,"(a) soft excation excavation","m³",null," RATE ONLY "]
[null,"(b) intermidiate excavation (200 mm - 400mm)","m³",null," RATE ONLY "]
[null,"(b) hard excavation ( exceeding 400 mm)","m³",null," RATE ONLY "]
[]
[]
["33.04","Cut to spoil, including all haulauge (Roadbed preparation and compaction of material)"]
[null,"(a) soft excation excavation","m³",null," RATE ONLY "]
[null,"(b) intermidiate excavation (200 mm - 400mm)","m³",null," RATE ONLY "]
[null,"(b) hard excavation ( exceeding 400 mm)","m³",null," RATE ONLY "]
{"$rows_empty":20}
["3300 ","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 3400: PAVEMENT LAYERS OF "]
[null,"GRAVEL MATERIAL"]
[]
["34.01","Pavement layers constructed from gravel taken from commercial"]
[null,"sources, including haulage:"]
[]
[null,"a) Gravel selected layer compacted to:"]
[null,"(ii) 95% of modified AASHTO density (150mm G7)","m3",null," RATE ONLY "]
[]
[null,"c) Gravel subbase (unstabilised material) compacted to:"]
[null,"(i) 95% of modified AASHTO density:(150mm approved gravel)","m3",null," RATE ONLY "]
[]
[null,"d) Gravel subbase (chemically stabilised material) compacted to:"]
[null,"(i) 97% of modified AASHTO density:"]
[null,"200mm C3 using G5","m3",null," RATE ONLY "]
[]
[{"$nulls":4},"                  -   "]
{"$rows_empty":23}
["3400 ","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 3600: CRUSHED-STONE BASE"]
[]
["36.01","Crushed-stone base:"]
[]
[null,"c) Constructed from type G2 material obtained "]
[null,"from commercial sources and compacted to "]
[null,"85% of bulk density(150mm)","m³",null," RATE ONLY "]
[]
["36.04","Crushed-stone base constructed with material from existing pavements layers (150mm)"]
[]
[null,"b) G2 material compacted to 85% of bulk relative density:"]
[null,"(i) Material from existing uncemented crushed stone layers","m³",null," RATE ONLY "]
{"$rows_empty":29}
["3600 "," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 3800: BREAKING UP EXISTING PAVEMENT LAYERS"]
[]
["38.01","Excavating anf removing existing bituminus material (except milling)"]
[null,"a) Material intended for recycling with an average depth of excavation:"]
[null,"i) Not exceedomg 30mm ","m2",null," RATE ONLY "]
[null,"ii) Exceeding 30mm but not exceeding 60mm","m2",null," RATE ONLY "]
[]
[null,"b) Material to be disposed of the average depth of excavation:"]
[null,"i) Not exceedomg 30mm ","m2",null," RATE ONLY "]
[null,"ii) Exceeding 30mm but not exceeding 60mm","m2",null," RATE ONLY "]
[]
["38.02","Milling out existing bituminous material with an average milling depth (milled out to an approved stockpile):"]
[]
[null,"a) Not exceedomg 30mm ","m³",null," RATE ONLY "]
[null,"b) Exceeding 30mm but not exceeding 60mm","m³",null," RATE ONLY "]
[null,"c) Exceeding 60mm","m³",null," RATE ONLY "]
[]
["38.03","Milling out cemented crushed stone (milled out to an approved stockpile) :"]
[]
[null,"a) Average milling depth not to exceed 50mm"]
[null,"(i) Comprehensive strength of 10 Mpa and less","m³",null," RATE ONLY "]
[null,"(ii) Comprehensive strength of 10 mpa up to and including 20 Mpa","m³",null," RATE ONLY "]
[null,"(ii) Comprehensive strength exceeding 20 Mpa","m³",null," RATE ONLY "]
[]
[null,"b) Average milling depth not to exceed 50mm but not exceeding 100mm"]
[null,"(i) Comprehensive strength of 10 Mpa and less","m³",null," RATE ONLY "]
[null,"(ii) Comprehensive strength of 10 mpa up to and including 20 Mpa","m³",null," RATE ONLY "]
[null,"(ii) Comprehensive strength exceeding 20 Mpa","m³",null," RATE ONLY "]
[]
[null,"c) Average milling depth exceeding 100mm"]
[null,"(i) Comprehensive strength of 10 Mpa and less"]
[null,"(ii) Comprehensive strength of 10 mpa up to and including 20 Mpa"]
[null,"(ii) Comprehensive strength exceeding 20 Mpa"]
[]
["38.04","Excavating and spoiling material from an existing pavement and/or"]
[null,"the underlying fill (to include haulage):"]
[null,"a) Non-cemented material","m³",null," RATE ONLY "]
[null,"b) Cemented material","m³",null," RATE ONLY "]
[null,"c) Cemented crushed stone","m³",null," RATE ONLY "]
[]
["38.08","Sawing or cutting asphalt or cemented pavement layers:"]
[null,"a) Sawing asphalt","m2",null," RATE ONLY "]
[]
[]
["3800 ","TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 4100: PRIME COAT"]
[]
["41.01","Prime Coat:"]
[null,"c) MC-30 cut-back bitumen","l",null," RATE ONLY "]
{"$rows_empty":32}
["4100 "," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[]
[null,"SECTION 4200 : ASPHALT BASE AND SURFACING"]
[]
["42.02","Asphalt surfacing "]
[null,"a) Continuously graded (40mm thick AC)","m2",null," RATE ONLY "]
[]
["42.04","Tack coat of 30% stable-grade emulsion"," l ",null," RATE ONLY "]
{"$rows_empty":33}
["4200 "," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[]
[null,"SECTION 4400 : Single Seals"]
[]
["44.01","Asphalting - Single seals (confirm stone size)"]
[null,"a) Using 13.2 mm aggregate ","m2",null," RATE ONLY "]
[]
["44.02","Bituminious binder variations "]
[null,"f) MC-300 cut-back bitumen"," l ",null," RATE ONLY "]
{"$rows_empty":32}
[4400," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 4500 : Double Seals"]
[]
["45.01","Asphalting - Double seals using "]
[null,"c) 13.2 mm and 6.7 mm aggregate ","m2",null," RATE ONLY "]
[]
["45.02","Bituminious binder variations "]
[null,"b) 80/100 penetration grade bitumen"," l ",null," RATE ONLY "]
[null,"g) MC-300 cut-back bitumen"," l ",null," RATE ONLY "]
{"$rows_empty":31}
[4500," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 4600 : Bituminous Single Seal with Slurry (Cape Seal)"]
[]
["46.01","Bituminous single seal with 19mm aggregate and slurry "]
[null,"a) 6mm Slurry Seal","m2",null," RATE ONLY "]
[null,"b) 8mm Slurry Seal","m2",null," RATE ONLY "]
[null,"c) 10mm Slurry Seal","m2",null," RATE ONLY "]
[null,"d) 12mm Slurry Seal","m2",null," RATE ONLY "]
[]
["46.02","Bituminous single seal with 13.2mm aggregate and slurry "]
[null,"a) 6mm Slurry Seal","m2",null," RATE ONLY "]
[null,"b) 8mm Slurry Seal","m2",null," RATE ONLY "]
[null,"c) 10mm Slurry Seal","m2",null," RATE ONLY "]
[null,"d) 12mm Slurry Seal","m2",null," RATE ONLY "]
[]
["46.09","Supply and application of Geotextile and Anionic Stable 60 emulsion","m2",null," RATE ONLY "]
["46.10","Supply and application of Fog Spray using 50/50 dilution of Stable 60 emulsion","m2",null," RATE ONLY "]
["46.11","Supply and application of Chip and Spray"]
[null,"a)     Single Seal","m2",null," RATE ONLY "]
[null,"b)    Double Seal","m2",null," RATE ONLY "]
{"$rows_empty":19}
[4600," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 4800 : Treatment of an exsisting surface exhibiting certain defects"]
[]
["48.01","Treatment with diluted bituminous emulsion (fog spray)"]
[]
[null,"c) Supply and application of Fog Spray using 50/50 dilution of Stable 60 emulsion","m2",null," RATE ONLY "]
[]
["48.02","Supply and application of Geotextile and Anionic Stable 60 emulsion","m2",null," RATE ONLY "]
[]
["48.14","Supply and application of Chip and Spray"]
[null,"a)     Single Seal","m2",null," RATE ONLY "]
[null,"b)    Double Seal","m2",null," RATE ONLY "]
{"$rows_empty":34}
[4800," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","PREVIOUS RATE ","RATE"]
[null,"SECTION 5100: PITCHING: STONEWORK AND PROTECTION AGAINST EROSION "]
[]
["51.01","Stone Pitching "]
[]
[null,"(b) grouted stone pitching","m²",null,"RATE ONLY"]
{"$rows_empty":30}
["5100 "," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 5200: GABIONS"]
[]
["52.01","Foundation trench excavation and backfilling:"]
[null,"(b) In all other classes of materials","m³",null," RATE ONLY "]
[]
["52.02","Surface preparation for bedding the gabions","m²",null," RATE ONLY "]
[]
["52.03","Gabions"]
[]
[null,"(a) Galvanised gabion boxes (1m x 1m x 2m)","m³",null," RATE ONLY "]
[null,"(b) PVC coated gabion boxes (1m x 1m x 2m)","m³",null," RATE ONLY "]
[null,"(c) Galvanised gabion mattresses by (0,5m x 1m x 2m)","m³",null," RATE ONLY "]
[null,"(d) PVC coated gabion mattresses by (0,5m x 1m x 2m)","m³",null," RATE ONLY "]
[]
["52.04","Filter fabric (A2 or equally approved)","m²",null," RATE ONLY "]
{"$rows_empty":21}
[5200,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 5400: GUARDRAILS"]
[]
["54.01","Guardrails on timber posts"]
[]
[null,"(a) Galvanised ","m",null," RATE ONLY "]
[]
["54.04","End treatments"]
[null,"(a) End Wings","No.",null," RATE ONLY "]
[]
["54.05","Additional guardrail posts"]
[]
[null,"a) Timber","No.",null," RATE ONLY "]
[null,"b) Steel","No.",null," RATE ONLY "]
[]
["54.06","Reflective pates","No.",null," RATE ONLY "]
{"$rows_empty":25}
[5400," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 5700: ROAD MARKINGS"]
[]
["57.02","Retro-reflective road-marking paint"]
[]
[null,"a) White lines (broken or unbroken)"]
[null,"i)100 mm wide","km",null," RATE ONLY "]
[null,"ii)200 mm wide","km",null," RATE ONLY "]
[]
[null,"b) Yellow lines (broken or unbroken)"]
[null,"i)100 mm wide","km",null," RATE ONLY "]
[null,"c)Red lines (broken or unbroken)"]
[null,"i)100 mm wide","km",null," RATE ONLY "]
[]
[null,"d)White lettering and symbols","m2",null," RATE ONLY "]
[]
["57.05","Galvanised Steel Road Studs","No.",null," RATE ONLY "]
[null,"- 100mm x 100mm x 22mm - 2.5mm thick mild steel housing - Hot dip spin galvanized - Shank of 60mm x 12mm y-reinforced steel - Filled with a 2 part 100% solid polyrethane sand filler"]
[]
["57.06","Setting out and premarking the lines (excluding"]
[null,"traffic-island markings, lettering and symbols)","km",null," RATE ONLY "]
{"$rows_empty":21}
["5700 "," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 5800: LANDSCAPING AND PLANTING PLANTS"]
[]
["58.01","Trimming"]
[null,"Tendered rate shall include full compensation for trimming the areas to the specified finishing requirements., including moving material which would be inherent in this process and the removal of surplus material and stones. "]
[]
[null,"a) Machine trimming","m²",null," RATE ONLY "]
[null,"b) Hand trimming ","m²",null," RATE ONLY "]
[]
["58.03","Preparing the areas for grassing:"]
[null,"Rates to include full compensation of ripping, scarifying, excavating and loading the topsoil placing in stockpiles where necessary."]
[]
[null,"a) Ripping ","ha",null," RATE ONLY "]
[null,"b) Scarifying for loosening topsoil","ha",null," RATE ONLY "]
[]
[null,"c) Topsoiling within the road reserve:"]
[null,"i) Topsoil obtained from within road reserve or borrow areas","m³",null," RATE ONLY "]
[null,"ii) Topsoil obtained from other sources","m³",null," RATE ONLY "]
[]
[null,"e) Providing and applying chemical fertilises and /or soil improvement material:"]
[null,"Rates shall include full compensation for furnishing the fertiliser and/ or soil improvement materials, transporting it to the point of use spreading and mixing it into the scarified soil or topsoil, irrespective of method of application"]
[null,"i) Lime","kg",null," RATE ONLY "]
[null,"vi) Other fertilisers and or soil improvement","kg",null," RATE ONLY "]
[]
["58.04","Grassing:"]
[null,"Rates shall include full compensation for procuring all required material, labour equipment and all incidentals. To include excavation, loading, transporting, off-loading, placing and watering the sods, for replanting dead areas, for watering and weeding the grass, for supply and mowing, which may be necessary for the establishing an acceptable cover, and maintaining the grass."]
[]
[null,"a) The planting of grass ((cynodon dactylon, with sufficient root material)","ha",null," RATE ONLY "]
[]
[null,"b) Sodding by using the following types of sodding "]
[null,"i) Nursery sods (commercial)","m²",null," RATE ONLY "]
[null,"ii) Veld sods (with sufficient root material)","m²",null," RATE ONLY "]
[]
[null,"c) Hydroseeding "]
[null,"i) Prividing an approved seed mixture for hydroseeding","kg",null," RATE ONLY "]
[null,"ii) Providing a mulch (organic)","kg",null," RATE ONLY "]
[]
[null,"e) Hand sowing ","m²",null," RATE ONLY "]
[]
["58.09","Trees and shrubs"]
[null,"Rates shall include full compensation for procuring all required material, labour equipment and all incidentals. To include excavating holes to specified dimensions, loading, transporting, off-loading, placing and watering the sods, for replanting dead areas, for watering and weeding the grass, for supply and mowing, which may be necessary for the establishing an acceptable cover, and maintaining the grass."]
[null,"Plants should have 350 mm stem lengths and be well established within the containers. Supply, plant and maintain."]
[null,"a) Providing trees and plants (Bush violet type)","No.",null," RATE ONLY "]
[]
[]
[]
[]
[5800," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 6100 : FOUNDATIONS FOR STRUCTURES"]
[]
[]
["61.08","Foundation fill consisting of "]
[]
[null,"a) Rock fill","m 3",null," RATE ONLY "]
[null,"d) Mass concrete (15/19 MPA)","m 3",null," RATE ONLY "]
{"$rows_empty":23}
[6100,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 6200: FALSEWORK, FORMWAORK AND CONCRETE FINISH"]
[]
["62.01","Formwork to provide to cast in situ concrete"]
[]
[null,"a) F3 surface finish (external facing)","m 2",null," RATE ONLY "]
{"$rows_empty":27}
[6200,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 6300: STEEL REINFORCEMENT FOR STRUCTURES"]
["63.01","a) Steel reinforcement for: 30/19 concrete (wingwalls, bottom,top slab and any concrete structure)"]
[]
[null,"iii) Welded steel fabric (mesh ref 395)","m 2",null," RATE ONLY "]
[null,"iv) Welded steel fabric (mesh ref 617)","m 2",null," RATE ONLY "]
{"$rows_empty":33}
[6300,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"]
[null,"SECTION 6400: CONCRETE STRUCTURES"]
[]
["64.01","Cast in situ concrete"]
[]
[null,"a)Concrete (20/19 concrete)","m 3",null," RATE ONLY "]
[null,"b)Concrete (25/19 concrete)","m 3",null," RATE ONLY "]
[null,"c)Concrete (30/19 concrete)","m 3",null," RATE ONLY "]
{"$rows_empty":35}
[6400,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE","AMOUNT"]
[]
[null,"SECTION 6600: NO-FINES CONCRETE, JOINTS AND PARAPETS AND DRAINAGE FOR STRUCTURES"]
[]
["66.15","Concrete parapets"]
[null,"a)Parapet wall (25/19 concrete)","m 3",null," RATE ONLY "]
[null,"b) Parapet wall (30/19 concrete)","m 3",null," RATE ONLY "]
{"$rows_empty":34}
[6600,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 7100: CONCRETE PAVEMENTS                                                              (Concrete to be 25Mpa/19mm Stone)"]
[]
[]
[71.02,"Concrete Pavement"]
[null,"150mm thickness excluding texturing and curing","m2",null," RATE ONLY "]
[]
[71.04,"Texturing and curing the concrete pavement:"]
[]
[null,"(a) Burlap-dragged and grooved texture","m2",null," RATE ONLY "]
[]
[null,"(b) Curing","m2",null," RATE ONLY "]
[]
[71.06,"Joints:"]
[]
[null,"(a) Expansion joints complete (excluding dowels)","m",null," RATE ONLY "]
[]
[71.07,"Drilling and testing"]
[]
[null,"(b) 150 mm cores drilled from the pavement and tested  for compressive strength","No.",null," RATE ONLY "]
[]
["71.08","Steel reinforcement in concrete pavement:"]
[]
[null,"(c) Welded steel fabric","kg",null," RATE ONLY "]
{"$rows_empty":16}
["7100 "," TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[]
[null,"SECTION 7300: CONCRETE BLOCK PAVING                                                        "]
[]
[null,"Rates to include full compensation for furnishing all materials, suppy, deliverand Placing . Constructiong the bedding layers, laying and compacting all paving blocks and surface. To also include the filling of koints with jointing sand and for all other necessary work to complete the paving"]
[]
["73.01","a) Interlocking Concrete block paving :                                          ",null,null," RATE ONLY "]
[null,"i) Corobrik Burgundy 220x100x60 (clay)","m2"]
[null,"ii) Concrete paving brick 200mm x 100mm x 60mm (concrete)","m2"]
[]
[null,"b) asphalt type "]
[null,"i) Continuously graded (30mm thick AC)","m2",null," RATE ONLY "]
[]
[null,"c) Concrete type surface"]
[null,"i) 20/19 Mpa concrete "]
[null,"ii) 25/19 Mpa concrete "]
[null,"iii) 25/19 Mpa concrete "]
[]
["73.02","Concrete edge and intermediate beams"]
[null,"a) Cast in situ edge restaints","m",null," RATE ONLY "]
[null,"b) precast edge restarints","m",null," RATE ONLY "]
[]
["73.03","Provision of approved herbicide and ant poison:"]
[null,"(a) Provisional Materials","Prov Sum",null," RATE ONLY "]
[]
[null,"(b) Contractor's charges and profit added to the prime cost sum",{"v":0.1,"d":"10%"},null," RATE ONLY "]
{"$rows_empty":25}
[7300,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 7400: PATENTED EARTH RETAINING SYSTEMS"]
[]
["74.01","Patented earth retaining system"]
[]
[null,"a) Löffelstein precast concrete blocks of type L300","m2",null," RATE ONLY "]
[]
[null,"b) Löffelstein precast concrete blocks of type L500","m2",null," RATE ONLY "]
[]
[null,"c) Löffelstein precast concrete blocks of type L500","m2",null," RATE ONLY "]
[]
["74.02","Excavation for concrete bases for earth retaining systems"]
[]
[null,"a) In soft material","m3",null," RATE ONLY "]
[]
[null,"b) Extra over subitem 74,02 (a) for excavation in hard material","m3",null," RATE ONLY "]
[{"$nulls":4}," "]
["74.03","Concrete bases for earth retaining system of 25MPA","m3",null," RATE ONLY "]
[]
["74/21.10","Fibre filter fabric (Bidem)","m2",null," RATE ONLY "]
[]
["74/35.01","Chemical stabilization (500mm Thick) extra over unstabilized compacted layers (G7 Fill)","m3",null," RATE ONLY "]
[]
["74/35.02","Chemical stabilizing agent:"]
[]
[null,"a) Ordinary portland cement","t",null," RATE ONLY "]
{"$rows_empty":18}
[7400,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION 8100: TESTING MATERIALS AND"]
[null,"WORKMANSHIP"]
[]
["81.02","Other special tests requested by the Engineer","Prov Sum",null,"RATE ONLY"]
[]
[null,"a) Handling cost and profit in respect of subitem 81.02 above","%",null,"RATE ONLY"]
[{"$nulls":4},"                  -   "]
{"$rows_empty":33}
[8100,"TOTAL CARRIED TO SUMMARY"]
[]
["ITEM","DESCRIPTION","UNIT","RATE"," AMOUNT "]
[null,"SECTION D1000: DAYWORKS"]
[]
["D1000","Personnel during normal working hours"]
[]
[null,"a) Unskilled labour","hr",null," RATE ONLY "]
[null,"b) Skilled labour","hr",null," RATE ONLY "]
[null,"c) Foreman","hr",null," RATE ONLY "]
[]
[null,"Equipment"]
[]
[null,"a) TLB (up to 52kW)","hr",null," RATE ONLY "]
[]
[null,"c)Self-propelled compactors"]
[]
[null,"i)Vibrating roller up to 1,0 m wide and mass 1,5 t","hr",null," RATE ONLY "]
[]
[null,"ii)Vibrating roller more than 80 kW and mass 8 t","hr",null," RATE ONLY "]
[]
[null,"d)Tipper truck up to 10 cubic metre capacity","hr",null," RATE ONLY "]
[]
[null,"e) Motor grader from 95 kW up to 120 kW and mass 16 t","hr",null," RATE ONLY "]
[]
[null,"f) Excavator 20 ton","hr",null," RATE ONLY "]
{"$rows_empty":17}
["D1000","TOTAL CARRIED TO SUMMARY"]

{"sheet":"SUMMARY","index":1,"n_rows":62,"n_cols":6,"rows_kept":62,"merged":[[1,0,1,5],[2,0,2,5],[3,1,3,4],[4,0,4,4],[5,1,5,4],[6,1,6,4],[7,1,7,4],[8,1,8,4],[9,1,9,4],[10,1,10,4],[11,1,11,4],[12,0,12,4],[13,1,13,4],[14,1,14,4],[15,1,15,4],[16,1,16,4],[17,0,17,4],[18,1,18,4],[19,1,19,4],[20,1,20,4],[21,1,21,4],[22,1,22,4],[23,0,23,4],[24,1,24,4],[25,1,25,4],[26,1,26,4],[27,1,27,4],[29,1,29,4],[30,1,30,4],[31,0,31,4],[32,1,32,4],[33,1,33,4],[34,1,34,4],[35,1,35,4],[36,1,36,4],[37,0,37,4],[38,1,38,4],[39,1,39,4],[40,1,40,4],[41,1,41,4],[42,1,42,4],[43,1,43,4],[44,0,44,4],[45,1,45,4],[46,1,46,4],[47,1,47,4],[48,1,48,4],[49,0,49,4],[50,1,50,4],[51,0,51,4],[52,1,52,4],[53,1,53,4],[54,1,54,4],[55,1,55,4],[56,1,56,4],[57,1,57,4],[58,1,58,4],[59,1,59,4],[60,1,60,4],[61,1,62,4]]}
[]
["PANEL OF ROADS AND STORMWATER REHABILITATION FOR A PERIOD OF 3 YEARS "]
["DESCRIPTION"]
[{"$nulls":5},"AMOUNT"]
["SECTION 1"]
[1200,"General Requirements and Provisions"]
[1300,"Contractor's Establishment on Site and General Obligations"]
[1400,"Housing, offices and laboratories for the engineer's site personnel"]
[1500,"Accommodation of Traffic"]
[1600,"Overhaul"]
[1700,"Clearing and Grubbing"]
[]
["SECTION 2"]
[2100,"Drains"]
[2200,"Prefabricated Culverts"]
[2300,"Concrete Kerbing, Concrete Channelling, Chutes and Downpipes and Concrete Linings for Open Drains"]
[]
["SECTION 3"]
[3300,"Mass Earthworks"]
[3400,"Pavement Layers of Gravel Material"]
[3600,"Crushed-stone base"]
[3800,"Breaking up existing pavement layers"]
[]
["SECTION 4"]
[4100,"Prime Coat"]
[4200,"Asphalt base and surfacing"]
[4400,"Single Seals"]
[4500,"Single Seals"]
[4600,"Bituminous Single Seal with Slurry (Cape Seal)"]
[4800,"Treatment of an exsisting surface exhibiting certain defects"]
[]
["SECTION 5"]
[5100,"Pitching: Stonework and Protection Against Erosion"]
[5200,"Gabions"]
[5400,"Guardrails"]
[5700,"Road Markings"]
[5800,"Landscaping and Planting Plants"]
["SECTION 6"]
[6100,"FOUNDATIONS FOR STRUCTURES"]
[6200,"FALSEWORK, FORMWAORK AND CONCRETE FINISH"]
[6300,"STEEL REINFORCEMENT FOR STRUCTURES"]
[6400,"CONCRETE STRUCTURES"]
[6600,"NO-FINES CONCRETE, JOINTS AND PARAPETS AND DRAINAGE FOR STRUCTURES"]
[]
["SECTION 7"]
[7100,"Concrete pavements"]
[7300,"Concrete block paving"]
[7400,"Patented Earth Retaining Systems"]
[]
["SECTION 8"]
[8100,"Testing Materials and Workmanship"]
["SECTION 9"]
["D1000","Dayworks"]
[]
["A","SUB-TOTAL"]
[]
["B","CONTINGENCIES"]
[]
["C","SUB-TOTAL (A + B)"]
[]
["D","ADD VAT (15%)"]
[null,"TOTAL INCLUDING VAT"]