{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["Section 1","Section 2","Section 3-SHEQ to verify","Section 4-EMS to verify","Section 5","Section 6","Section 7","Section 8","Summary"],"not_rendered":{"images":1,"external_links":1,"defined_names":13},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Section 1","index":0,"n_rows":53,"n_cols":7,"rows_kept":53,"merged":[[1,9,1,11],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[6,1,7,1],[52,0,52,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":4},"Section 1 : P&G Fixed"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[]
[null,"SABS 1200AA","SECTION 1:  PRELIMINARY & GENERAL"]
[null,null,"FIXED CHARGES"]
[]
["1.1","8.3.1","Contractual Requirements"]
[]
["1.1.1",null,"Contractual Requirements","Sum",1,null,0]
[]
["1.2","8.3.2.","Provision of Facilities on Site"]
[]
["1.2.1","a)","Facilities required by Engineer","Sum",1,null,0]
[null,"b)","Facilities required by Contractor","Sum",1,null,0]
[null,null,"a"]
["1.3","8.3.3","General Responsibilities and Other Fixed-term Obligations","Sum",1,null,0]
[]
["1.4","8.3.4","Removal of Site Establishment","Sum ",1,null,0]
[]
["1.5","PSA 8.10","HIV / AIDS awareness"]
[]
["1.5.1",null,"Conduct HIV/AIDS awareness programme workshops on site for not less than 90% of the workers inclusive of all direct and indirect costs","Sum",1,null,0]
[]
["1.5.2",null,"Provide and maintain condom dispenser","Sum",1,null,0]
[]
["1.5.3",null,"Provide and maintain HIV/AIDS awareness posters","Sum",1,null,0]
[]
["1.5.4",null,"Provide information regarding voluntary testing of construction workers and counselling, support and care in a monthly report.","Sum",1,null,0]
[]
["1.6",null,"Quality Control"]
[]
["1.6.1","PS A 8.10","Quality control and all activities necessary to comply with all requirements of the specified quality control system as per PS 5.","Sum",1,null,0]
[]
[1.7,null,"High Voltage Safe Working Procedures"]
[]
["1.7.1","PSA 8.10","Comply with Safe Working Procedures for pipeline construction within High Voltage Transmission Lines Servitude (See TS041 in Specification Rand Water Cathodic Protection System Technical Specification)","Sum",1,null,0]
{"$rows_empty":13}
["SECTION 1 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 2","index":1,"n_rows":41,"n_cols":7,"rows_kept":41,"merged":[[1,9,1,11],[2,2,2,5],[2,9,2,11],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[17,8,17,22],[40,0,40,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 2:  P&G Time Related"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[]
[null,"SABS 1200AA","SECTION 2:  PRELIMINARY & GENERAL \nTIME RELATED ITEMS"]
[]
[2.1,"8.4.1","Contractual Requirements"]
[]
["2.1.1",null,"Contractual Requirements","Sum",1,null,0]
[]
[2.2,"8.4.2","Operation and Maintenance of Facilities on Site"]
[]
["2.2.1","a)","Facilities for Engineer","sum ",1,null,0]
[]
["2.2.2","b)","Facilities for Contractor","sum ",1,null,0]
[]
[2.3,"8.4.3","General Responsibilities and other Time-related Obligations","Sum",1,null,0]
[]
[2.4,null,"HIV / AIDS awareness"]
[]
["2.4.1","PSA 8.10","Conduct HIV/AIDS awareness programme workshops on site for not less than 90% of the workers inclusive of all direct and indirect costs","Sum",1,null,0]
[]
["2.4.2","PSA 8.10","Provide and maintain condom dispenser","Sum",1,null,0]
[]
["2.4.3","PSA 8.10","Provide and maintain HIV/AIDS awareness posters","Sum",1,null,0]
[]
["2.4.4","PSA 8.10","Provide information regarding voluntary testing of construction workers and counselling, support and care in a monthly report.","Sum",1,null,0]
[]
[2.5,null,"Quality Control"]
[]
["2.5.1","PS A 8.10","Quality control and all activities necessary to comply with all requirements of the specified quality control system as per PS 5.","Sum",1,null,0]
[]
[2.6,null,"High Voltage Safe Working Procedures"]
[]
["2.6.1","PSA 8.10","Comply with Safe Working Procedures for pipeline construction within High Voltage Transmission Lines Servitude (See TS041 in Specification Rand Water Cathodic Protection System Technical Specification)","Sum",1,null,0]
[]
[]
[]
["SECTION 2 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 3-SHEQ to verify","index":2,"n_rows":67,"n_cols":7,"rows_kept":67,"merged":[[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[66,0,66,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 3:  Health and Safety"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,"PSAA 8.11","SECTION 3 :  OCCUPATIONAL HEALTH AND SAFETY"]
[]
[3.1," ","Preparation of the Contractor's site specific Health and Safety Plan"," Lump sum",1,null,0]
[]
[3.2,null,"Principal Contractor's initial obligations in respect of the Occupational Health and Safety Act and Construction Regulations"," Lump sum",1,null,0]
[]
[3.3,null,"Principal Contractor's time related obligations in respect of the Occupational Health and Safety Act and Construction Regulations"," Lump sum",1,null,0]
[]
[3.4,null,"Provision of full Personal Protective Equipment (PPE)"," Lump sum",1,null,0]
[]
[3.5,null,"Provision of a full time Construction Health and Safety Officer"," Lump sum",1,null,0]
[]
[3.6,null,"Cost of medical certificates and medical surveillance"]
[]
["3.6.1",null,"(a) Initial (baseline) medical examinations"," Lump sum",1,null,0]
[]
["3.6.2",null,"(b) Periodic and exit examinations"," Lump sum",1,null,0]
[]
["3.6.2",null,"(c) Medical Consultation as and when required with OHP and OMP"," Lump sum",1,null,0]
[]
[3.7,null,"Induction Training","Lump sum",1,null,0]
[]
[3.8,null,"Provision of First Aid Boxes to GSR requirements and other emergency safety equipment such as fire extinguishers.","Lump sum",1,null,0]
[]
[3.9,null,"Transportation of Workers","Lump sum",1,null,0]
[]
[{"v":3.1,"d":"3.10"},null,"Welfare Facilities ","Lump sum",1,null,0]
[]
[3.11,null,"Occupational Hygiene Surveys","Lump sum",1,null,0]
[]
[3.12,null,"Training (OH & S requirements)","Lump sum",1,null,0]
[]
[3.13,null,"Security requirements including the security risk assessment (before site establishment)"]
[]
[3.14,null,"Employee wellness programs","Lump sum",1,null,0]
[]
[3.15,null,"Drug and Alcohol Testing, Policies and Procedures","Lump sum",1,null,0]
[]
[3.16,null,"Barricading","Lump sum",1,null,0]
[]
[3.16,null,"Safety notices and signs","Lump sum",1,null,0]
[]
[3.17,null,"SHE  Incentives","Prov. Sum",1,null,0]
[]
[3.18,null,"Construction work permit application fee","Prov. Sum",1,null,0]
[]
[3.19,null,"Adequate ventilation and lighting during construction","Lump sum",1,null,0]
[]
[{"v":3.2,"d":"3.20"},null,"Submission of the Health and Safety File (hard and soft copies - After tender award and  project completion)","Lump sum",1,null,0]
[]
[3.21,null,"Provision of Client Pr.CHSA (Construction Health & Safety  Agent) registered with SACPCMP for the duration of the project.","Lump sum",1,null,0]
{"$rows_empty":10}
["SECTION 3 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 4-EMS to verify","index":3,"n_rows":52,"n_cols":7,"rows_kept":52,"merged":[[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[51,0,51,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 4:  Environment"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,"PSAA 8.12","SECTION 4 :  ENVIRONMENT"]
[]
[4.1,null,"Signage"]
["4.1.1",null,"Environmental information sign at gate \n(metal - A2 size)","Each",1,null,0]
["4.1.2",null,"Topsoil (corex board with wooden peg A3 size)","Each",4,null,0]
[]
[4.2,"TS 1.26","Storm water deflection berms / cross embankments / erosion control berms for steep slope erosion protection or for the protection of topsoil stockpiles.","  Lump sum",1,null,0]
[]
[4.3,null,"Pollution Prevention"]
["4.3.1",null,"Waste disposal provision at an approved location","  Lump sum",1,null,0]
["4.3.2",null,"Waste bins and receptacles that have water tight lids","Lump sum",1,null,0]
["4.3.3",null,"Spillage kits for all construction vehicles and be easily available on site","Lump sum",1,null,0]
["4.3.4",null,"Drip trays for all vehicles parked overnight ","Lump sum",1,null,0]
[]
[4.4,null,"Administration and documentation","  Lump sum",1,null,0]
[]
[4.5,null,"Fire protection equipment. Two flappers and one fire extinguisher per working head","  Lump sum",1,null,0]
{"$rows_empty":29}
["SECTION 4 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 5","index":4,"n_rows":118,"n_cols":7,"rows_kept":118,"merged":[[1,9,1,11],[2,9,2,11],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[58,6,59,6],[60,1,60,2],[117,0,117,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 5: Dayworks"]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,"SANS","SECTION 5: DAYWORKS"]
[null,"1200A"]
["6.1",8.7,"Labour by class"]
[]
["6.1.1",null,"Unskilled Labourers","hrs",0,null,"Rate Only"]
[]
["6.1.2",null,"Semi Skilled Labourers","hrs",0,null,"Rate Only"]
[]
["6.1.3",null,"Skilled labour","hrs",0,null,"Rate Only"]
[]
["6.2",8.7,"Labour by trade"]
[]
["6.2.1",null,"Construction Hand and Operator","hrs",0,null,"Rate Only"]
[]
["6.2.2",null,"Carpenter","hrs",0,null,"Rate Only"]
[]
["6.2.3",null,"Clerk","hrs",0,null,"Rate Only"]
[]
["6.2.4",null,"Artisans","hrs",0,null,"Rate Only"]
[]
["6.2.5",null,"Foreman","hrs",0,null,"Rate Only"]
[]
["6.2.6",null,"Gangers and Section Leaders","hrs",0,null,"Rate Only"]
[]
["6.2.7",null,"Steel fixer","hrs",0,null,"Rate Only"]
[]
["6.2.8",null,"Bricklayer or Plasterer","hrs",0,null,"Rate Only"]
[]
["6.2.9",null,"Welder","hrs",0,null,"Rate Only"]
[]
["6.3",8.7,"Materials"]
[]
["6.3.1",null,"Provisional sum for cost of material","Sum",0,null,"Rate Only"]
[]
["6.3.2",null,"Contractors mark-up on material","%","Rate Only",null,"Rate Only"]
[]
["6.4",8.7,"Plant"]
[]
[null,null,"Tenderers to insert the hire rate at which each item will be charged, which is to cover all relevant costs of plant hire, including operating crew"]
[]
["6.4.1",null,"Lowbed transport of plant to and from site","t.km",0,null,"Rate Only"]
[]
["6.4.2",null,"Bulldozer and ripper (D6 or equivalent)","hrs",0,null,"Rate Only"]
[]
["6.4.3",null,"Grader (120G or equivalent)","hrs",0,null,"Rate Only"]
[]
["6.4.4",null,"Front end wheel loaders (Cat 950 or similar)","hrs",0,null,"Rate Only"]
[]
[]
[]
[]
[]
[{"$nulls":6},0]
[null,"Carried Forward "]
[null,"Brought Forward",{"$nulls":4},0]
[]
[]
["6.4.5",null,"Back acting excavators (Hitachi EX200 or similar)","hrs",0,null,"Rate Only"]
[]
["6.4.6",null,"T L B","hrs",0,null,"Rate Only"]
[]
["6.4.7",null,"Tractors and drawn trailers and rollers","hrs",0,null,"Rate Only"]
[]
["6.4.8",null,"Compactors (D72Y or equivalent)","hrs",0,null,"Rate Only"]
[]
["6.4.9",null,"Compressors (250CFM or equivalent)","hrs",0,null,"Rate Only"]
[]
["6.4.10",null,"Trucks (7t or equivalent)","hrs",0,null,"Rate Only"]
[]
["6.4.11",null,"Tip Trucks (10t or equivalent)","hrs",0,null,"Rate Only"]
[]
["6.4.12",null,"Water Tanker","hrs",0,null,"Rate Only"]
[]
["6.4.13",null,"Plate Compactor","hrs",0,null,"Rate Only"]
[]
["6.4.14",null,"Light delivery vehicles (1t or equivalent)","km",0,null,"Rate Only"]
[]
["6.4.15",null,"Site Boom","No.",0,null,"Rate Only"]
[]
["6.4.16",null,"Generator","No.",0,null,"Rate Only"]
{"$rows_empty":31}
["SECTION 6 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 6","index":5,"n_rows":87,"n_cols":7,"rows_kept":87,"merged":[[1,9,1,11],[2,9,2,11],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[3,7,4,7],[41,1,42,1],[43,1,44,1],[46,1,46,2],[86,0,86,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 6:  Site Clearance and Rehabilitation"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[]
[null,"SABS 1200C","SECTION 6:  SITE CLEARANCE AND REHABILITATION"]
[]
[6.1,null,"Site Clearance"]
[]
["6.1.1","8.2.1","Clear and grub vegetation and trees of girth up to 0.5 m along the route of the mainline (Within 10 m wide working strip and excluding trees to be relocated) (See PS2.6 & PSC 5.9)","m2",75,null,0]
[]
["6.1.2","8.2.2 ","Clear large trees of girth and designated obstacles (See PS2.6, PSC5.9 & PSC 5.10)"]
[]
["6.1.2.1",null,"a) over 1m and up to and including 2m","no",0,null,0]
[]
["6.1.2.2",null,"b) over 2m m and up to and including 3m","no",0,null,0]
[]
["6.1.2.3",null,"c) over 3m in steps of 1m","no",0,null,"Rate Only"]
[]
[null,"SABS 1200C"]
[6.2,null,"Transportation of debris "]
[]
["6.2.1","8.2.9","Transport debris and materials resulting from site clearing to unspecified location ","m3.km",100,null,0]
[]
[6.3,null,"Remove and Stockpile Topsoil"]
[]
["6.3.1","8.2.10","Remove and stockpile topsoil to a depth of 150mm along the route of the pipeline (within working servitude) and maintain","Sum",1,null,0]
[]
[6.4,"TS1","Fire Breaks"]
[]
["6.4.1",1.24,"Form fire breaks on Engineer's Instruction","m²",38,null,0]
[]
[6.5,"TS1","Rehabilitation"]
[]
["6.5.1","TS 1.26","Restoring the ground surface for the full working area around chambers and over excavated trenches.","m3",6,null,0]
[]
["6.6","SABS 1200DA","Final Grading"]
[]
["6.6.1","PSDA\n5.2.5.1","Grade, shape and compact to final grades the surface around chamber to 150mm depth","m2",38,null,"Rate only"]
[]
["6.7",null,"Topsoiling"]
[]
["6.7.1","PSDA  8.3.6","Place topsoil to a depth of 150mm","m2",38,null,0]
[]
[null,"Carried Forward ",{"$nulls":4},0]
[null,"Brought Forward",{"$nulls":4},0]
[]
["6.8","SANS 1200D","Vegetation Re-establishment"]
[]
["6.8.1","8.3.11","Hydroseeding with appropriate grass seed mix. (Deemed to be inclusive of soil preparation and improvements, materials and labour).","m2",38,null,0]
[]
["6.9","8.3.8.1","Existing services"]
[null,"a)","The supply of specialist equipment for detection.","Sum",1,null,0]
[null,"b)","The use or hire of specialist equipment","Hours",3,null,0]
{"$rows_empty":30}
[{"$nulls":5}," "]
["SECTION 7 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 7","index":6,"n_rows":38,"n_cols":7,"rows_kept":38,"merged":[[1,7,1,8],[2,7,2,8],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[5,1,6,1],[37,0,37,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 7:  Earthworks and Bedding"]
[]
["Item ","Payment","Description","Unit","Qty","Rate","Amount"]
["No.","Refers"]
[null,null,"SECTION 7 :  EARTHWORKS & BEDDING"]
[]
[]
[7.1,"SABS 1200DA","Excavation for Chambers and trenches"]
[]
["7.1.1","PSDA8.3.2(a)","Excavate in all materials and use for backfill    (• In-situ backfill of selected suitable G7 material from excavations, compacted in layers not exceeding 150mm to 93% MOD AASHTO density at -1% to +2% OMC) or dispose as ordered. All haul for this contract shall be regarded as freehaul.  The cost of transportation of all materials will be deemed to be included in the rates and prices tendered.","m³",220,null,0]
[]
["7.1.2","8.3.2(b)","Extra over Item 1.1 for excavation in hard rock.","m³",31,null,0]
[]
[]
[]
["7.1.3","8.3.4.1","Importing of backfill G7 Material compacted in layers not exceeding 150mm in thickness compacted to 93% MOD AASHTO density AT -1% to +2% OMC","m³",59,null,0]
[]
[]
[null,"8.3.4.2","Extra over for 8.3.1(b)","m3",31,null,0]
[]
["7.1.4","8.3.4.2","G5 Material compacted in layers not exceeding 100 mm in thickness compacted to 95% MOD AASHTO density AT -1% to +2% OMC","m³",14,null,0]
[]
["7.1.5","8.3.5","Existing services (exposure, protection and alteration)","Sum","1",null,0]
[]
["7.1.6","8.3.6","Topsoiling","m2",50,null,0]
[]
[null,"8.8","Shoring of excavations","Sum",1,null,0]
[]
["7.1.7","8.3.8","Traffic signs (where applicable)","Sum","1",null,0]
[]
["7.1.8","PSDA 8.3.10","Take and provide photographic records","sum","1",null,0]
[]
[]
[]
[]
[]
["SECTION 8 CARRIED FORWARD TO SUMMARY",{"$nulls":5},0]

{"sheet":"Section 8","index":7,"n_rows":100,"n_cols":7,"rows_kept":100,"merged":[[1,7,1,8],[3,2,4,2],[3,3,4,3],[3,4,4,4],[3,5,4,5],[3,6,4,6],[55,2,56,2],[55,3,56,3],[55,4,56,4],[55,5,56,5],[55,6,56,6],[57,1,57,2],[99,0,99,5]],"flags":["formulas_cached_only"]}
[]
["Installation of a 300 mm meter connection in Pretoriusrand",{"$nulls":5},"Section 8:  Concrete and Steel works "]
[]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[]
[null,null,"SECTION 9: CONCRETE (SMALL WORKS) AND STRUCTURAL STEEL WORKS (SUNDRY ITEMS)"]
[]
[9.1,"SABS\n1200GA","SECTION 9.1: CONCRETE (SMALL WORKS)"]
[]
["9.1.1","8.2","Formwork"]
[]
["9.1.1.1","8.2.2","Smooth Formwork"]
[]
[null,null,"To Walls","m2",182,null,0]
[]
["9.1.1.2","8.2.3","Narrow widths"]
[]
[null,null,"Sides of roof slab (280mm high)","m",29,null,0]
[]
[null,null,"Sides of base slab (450mm high)","m",0,null,0]
[]
["9.1.1.3","8.2.4","Box out Holes / Form Voids"]
[]
[null,null,"a) Box out hole for 500mm x 500mm x 200mm (deep) pump sump","No.",1,null,0]
[null,null,"b) Box out hole for 410mm x 410mm x 400mm (deep)","No.",2,null,0]
[null,null,"c) Box out hole for 60mm x 60mm x 400mm (deep)","No.",1,null,0]
[]
["9.1.2","8.3","Reinforcement"]
[]
["9.1.2.1","8.3.1","Steel bars"]
[]
["9.1.2.1.1",null,"Mild steel reinforcement"]
[null,null,"Base Slab, Walls and Roof Slab","kg",232,null,0]
[]
["9.1.2.1.2",null,"High tensile steel reinforcement"]
[null,null,"Base Slab, Walls and Roof Slab","kg",11420,null,0]
[]
["9.1.3","8.3.2","High tensile welded mesh Ref. 888","m2",6,null,0]
[]
["9.1.4","8.4","Concrete"]
[]
["9.1.4.1","8.4.2","50mm Class 15/19MPa Blinding Layer:","m2",0,null,0]
[]
["9.1.4.2.1","8.4.3","a) Grade 35MPa/19mm:"]
[null,null,"Base Slab and walls","m3",61,null,0]
[]
["9.1.4.2.2",null,"b) Grade 60MPa/19mm:"]
[null,null,"Roof Slab","m3",14,null,0]
[]
["9.1.5","8.4.4","Unformed surface finishes"]
[]
["9.1.5.1",null,"Wood-floated finish to floor and roof slab","m2",59,null,0]
[]
[null,"Carried Forward ",{"$nulls":4},0]
["Item","Payment","Description","Unit","Qty","Rate","Amount"]
["No","Refers"]
[null,"Brought Forward",{"$nulls":4},0]
[]
["9.1.6","8.8","Miscellaneous"]
[]
["9.1.6.1",null,"Cast in PVC sleeves:"]
[]
["9.1.6.2",null,"110mm diameter x 400mm long including vermin proof mesh","No.",6,null,0]
[]
["9.1.6.3",null,"Cast in 50mm diameter x 280mm long PVC sleeves in roof slab for lifting purposes","No.",8,null,0]
[]
["9.1.6.4",null,"Cast in standard Rand Water manhole frame and cover (supplied by Rand Water)","No.",1,null,0]
[]
["9.1.6.5",null,"Supply and cast in standard Rand Water frame and sump cover (as per DGR No. A8879)","No.",1,null,0]
[]
["9.1.6.6",null,"Supply all materials and and install the Steel valve supports as detailed on Rand Water Detail Drg A12210:","No.",2,null,0]
[]
["9.1.6.7",null,"Supply, deliver and install platforms as per manufacture details (as per DRG No. R029197/01 for platform location)","No.",2,null,0]
[]
["9.1.6.8",null,"Water tightness test of all concrete valve chambers (excluding air valves)","Sum ",1,null,0]
[]
["9.1.6.9",null,"Construction of external mass concrete access steps inclusive of handrails for the chamber (Refer to Drawing RA 27329)","No.",1,null,0]
[]
[]
[9.2,"SABS\n1200HA","SECTION 9.2: STRUCTURAL STEELWORK (SUNDRY ITEMS)"]
[]
["9.2.1","8.3","Scheduled Items"]
[]
["9.2.1.1","8.3.3","Ladders complete and installed"]
[]
["9.2.1.1.1",null,"Supply and Install Standard Rand Water Catladder (as per DRG No. A7406) "]
[]
[null,null,"a) 3700mm high, refer to DRG R029197/01","No.",1,null,0]
[]
[null,null,"b) 1300mm high, refer to DRG R029197/01","No.",2,null,0]
[]
["9.2.1.2","PSHA  8.3.7","Supply and install Grab Rails as detailed on Rand Water Detail (as per DRG. No. A9858)"]
[]
[null,null,"Pretorius Rand Meter Connection Chamber (Refer to DRG No. R029197/01)","No.",1,null,0]
[]
[]
[]
[]
["Section Carried Forward to Summary",{"$nulls":5},0]

{"sheet":"Summary","index":8,"n_rows":27,"n_cols":4,"rows_kept":27,"merged":[[0,0,0,3],[0,9,0,11],[1,9,1,11],[2,9,2,11],[5,0,5,3],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[20,5,20,7],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2]],"flags":["formulas_cached_only"]}
["RAND WATER"]
["Project Name      ",":","Installation of a 300 mm meter connection in Pretoriusrand"]
["Document Name ",":"]
["Date ",":","2023-05-22"]
[]
["SUMMARY"]
["SECTION","DESCRIPTION",null,"TOTAL AMOUNT"]
[]
[1,"PRELIMINARY AND GENERAL : FIXED CHARGES",null,0]
[]
[2,"PRELIMINARY AND GENERAL : TIME RELATED",null,0]
[]
[3,"OCCUPATIONAL HEALTH AND SAFETY",null,0]
[]
[4,"ENVIRONMENT",null,0]
[]
[5,"DAYWORKS",null,0]
[]
[6,"SITE CLEARANCE",null,0]
[]
[7,"EARTHWORKS AND BEDDING",null,0]
[]
[9,"CONNECTION CHAMBERS - CONCRETE AND STEELWORK",null,0]
[]
["TOTAL (Excl. VAT)",null,null,0]
["(VAT@ 15%)",null,null,0]
["TOTAL (Incl. VAT)",null,null,0]