{"text_format":"3","workbook":"xlsx","n_sheets":8,"sheets":["Sect 1","Sect 2","Sect 3","Sect 4","Sect 5","Sect 6","Sect 7-12","Final Summary"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sect 1","index":0,"n_rows":223,"n_cols":5,"rows_kept":223}
["Description","Uom","Quantity","Rate","Amount"]
["MEANING OF TERMS 'TENDER / TENDERER'",""]
["Any reference to the words 'Tender' or 'Tenderer' herein and/or in any other documentation shall be construed to have the same meaning as the words 'Bid' or 'Bidder'.",""]
["PRELIMINARIES",""]
["The JBCC Preliminaries Code 2103, May 2005 edition for use with the JBCC Principal Building Agreement Edition 4.1 Code 2101, March 2005 is taken to be incorporated herein. The tenderer is deemed to have referred to these documents for the full intent and ",""]
["PRICING OF PRELIMINARIES",""]
["Should Option A, as set out in clause B10.3.1 hereinafter be used for the adjustment of preliminaries then each item priced is to be allocated to one or more of the three categories Fixed, Value Related or Time Related and the respective amounts entered i",""]
["Items not priced in these Preliminaries shall be deemed to be included elsewhere in these Bills of Quantities.",""]
["SECTION A: JBCC PRINCIPAL BUILDING AGREEMENT",""]
["A1.0 DEFINITIONS AND INTERPRETATION",""]
["Clause 1.1 Definition of 'Commencement Date' is added: 'COMMENCEMENT DATE' means the date that the agreement, made in terms of the Form of Offer and Acceptance, comes into effect         \n \nClause 1.1 Definition of 'Construction Guarantee' is amended by r","Item",{"v":1,"d":"1.00"}]
["OBJECTIVE AND PREPARATION",""]
["A2.0 OFFER, ACCEPTANCE AND PERFORMANCE",""]
["Clause 2.0","Item",{"v":1,"d":"1.00"}]
["A3.0 DOCUMENTS",""]
["Clause 3.0   \nClause 3.2.1 is amended by replacing '14.1' with '14.0'   \nClause 3.5 is deleted                          \nClause 3.7 is amended by the addition of the following: The contractor shall keep a copy of all drawings, schedules, priced bills of q","Item",{"v":1,"d":"1.00"}]
["A4.0 DESIGN RESPONSIBILITY",""]
["Clause 4.0   \nClause 4.1 The contractor shall be responsible for the design of the works, including for any temporary works. The contractor shall be responsible for the primary coordination of design elements. All designs must be submitted to the Principa","Item",{"v":1,"d":"1.00"}]
["A5.0 EMPLOYER'S AGENTS",""]
["Clause 5.0 Clause 5.1.2 is amended to include clauses 32.6.3, 34.3, 34.4 and 38.5.8","Item",{"v":1,"d":"1.00"}]
["A6.0 SITE REPRESENTATIVE",""]
["Clause 6.0","Item",{"v":1,"d":"1.00"}]
["A7.0 COMPLIANCE WITH REGULATIONS",""]
["Clause 7. Note: A separate clause has been included in Section C : Specific Preliminaries of the bills of quantities / lump sum document for the contractor to have the opportunity to price for all the requirements of the Occupational Health and Safety Act","Item",{"v":1,"d":"1.00"}]
["A8.0 WORKS RISK",""]
["Clause 8.0","Item",{"v":1,"d":"1.00"}]
["A9.0 INDEMNITIES",""]
["Clause 9","Item",{"v":1,"d":"1.00"}]
["A10.0 WORKS INSURANCES",""]
["Clause 10.0      \n \nClause 10.0 is amended by the addition of the following clauses:            \n \n10.5  Damage to the Works  \n(a) Without in any way limiting the contractor’s obligations in terms of the contract, the contractor shall bear the full risk o","Item",{"v":1,"d":"1.00"}]
["Clause 11.0","Item",{"v":1,"d":"1.00"}]
["A12.0 EFFECTING INSURANCES",""]
["Clause 12.0","Item",{"v":1,"d":"1.00"}]
["A13.0 No clause",""]
["A14.0 SECURITY",""]
["Retain sub-clause 14.1 but amend to read: “The employer shall have the right to choose the security to be provided in terms of 14.3 or 14.4 as stated in the schedule. The contractor shall provide the security required or chosen by the employer in the sche",""]
["F.......... V.........T..........","Item",{"v":1,"d":"1.00"}]
["EXECUTION",""]
["A15.0 PREPARATION FOR AND EXECUTION OF THE WORKS",""]
["Clause 15.0   \n \nIn sub-clause 15.1 replace “principal agent” with “employer”\n           \n15.1.4 An acceptable health and safety plan, required in terms of the Occupational Health and Safety Act, 1993 (Act 85 of 1993), within twenty-one (21) calendar days","Item",{"v":1,"d":"1.00"}]
["A16.0 ACCESS TO THE WORKS",""]
["Clause 16.0","Item",{"v":1,"d":"1.00"}]
["A17.0 CONTRACT INSTRUCTIONS",""]
["Clause 17.0      Clause 17.1.11 is amended by deleting the words 'and the appointment of nominated and selected subcontractors'","Item",{"v":1,"d":"1.00"}]
["A18.0 SETTING OUT OF THE WORKS",""]
["Clause 18.0","Item",{"v":1,"d":"1.00"}]
["A19.0 ASSIGNMENT",""]
["Clause 19.0","Item",{"v":1,"d":"1.00"}]
["Delete Clause 19.0 in its entirety and replace it with the following:\n \n19.1 The contractor does not cede, delegate or assign any of its rights or obligations to any person.\n19.2 Notwithstanding the above, the employer may, on written notice to the contra","Item",{"v":1,"d":"1.00"}]
["A20.0 NOMINATED SUBCONTRACTORS",""]
["Clause 20.0      \n \nClause 20.1.3 is amended by replacing it with the following: No clause  \n \nNote: See item B9.1 hereinafter for adjustment of attendance on nominated subcontractors executing work allowed for under provisional sums","Item",{"v":1,"d":"1.00"}]
["A21.0 SELECTED SUBCONTRACTORS",""]
["Clause 21.0      Clause 21 is amended by replacing it with:    No clause\n \nReplace sub-clause 21.1.2 to 21.1.4 and 21.2 to 21.6 with the following:\n“The contractor and principal agent shall appoint a selected subcontractor in accordance with the provision","Item",{"v":1,"d":"1.00"}]
["A22.0 EMPLOYER’S DIRECT CONTRACTORS",""]
["Clause 22.0","Item",{"v":1,"d":"1.00"}]
["A23.0 CONTRACTOR’S DOMESTIC SUBCONTRACTORS",""]
["Clause 23.0\n \nAdd sub-clause 23.3\n“The contractor may not subcontract the whole of the work without the written instruction or approval of the employer. In such event the employer may require the contractor to cede the contract to the subcontractor.”\nAdd ","Item",{"v":1,"d":"1.00"}]
["COMPLETION",""]
["A24.0 PRACTICAL COMPLETION",""]
["Clause 24.0","Item",{"v":1,"d":"1.00"}]
["A25.0 WORKS COMPLETION",""]
["Clause 25.0","Item",{"v":1,"d":"1.00"}]
["A26.0 FINAL COMPLETION",""]
["Clause 26.0      Clause 26.1.2 is amended by inserting '#' next to 26.1.2","Item",{"v":1,"d":"1.00"}]
["A27.0 LATENT DEFECTS LIABILITY PERIOD",""]
["Clause 27.0","Item",{"v":1,"d":"1.00"}]
["A28.0 SECTIONAL COMPLETION",""]
["Clause 28.0","Item",{"v":1,"d":"1.00"}]
["A29.0 REVISION OF DATE FOR PRACTICAL COMPLETION",""]
["Clause 29.0    \n \n29.1.1 The contractor shall allow Twelve (12) working days during the contract period per 12 months for the adverse effect of weather conditions and shall not be entitled to a revision of the date for Practical Completion for delays suff","Item",{"v":1,"d":"1.00"}]
["A30.0 PENALTY FOR NON-COMPLETION",""]
["Clause 30.0\n \nClause 30.1 Replace reference to “36.3” at end of sentence with “36.0”","Item",{"v":1,"d":"1.00"}]
["PAYMENT",""]
["A31.0 INTERIM PAYMENT TO THE CONTRACTOR",""]
["Clause 31.0  \n31.3 The issue of an interim payment certificates shall be done no later than the 20th of each month    \nSub-clause 31.9 is hereby amended by the substitution of the words \"seven (7) calendar days\" in the first line by the words \"thirty (30)","Item",{"v":1,"d":"1.00"}]
["A32.0 ADJUSTMENT TO THE CONTRACT VALUE",""]
["Clause 32.0      Clauses 32.5.1, 32.5.4 and 32.5.7 are amended by the addition of the following at the end of the sentence: 'due to no fault of the contractor'\n \nClause 32.13 is amended by adding the following:\nCPAP shall only be applicable to works that ","Item"]
["A33.0 RECOVERY OF EXPENSE AND LOSS",""]
["Clause 33.0","Item",{"v":1,"d":"1.00"}]
["A34.0 FINAL ACCOUNT AND FINAL PAYMENT",""]
["Delete the words in sub-clause 34.13 “subject to the employer giving the contractor a tax invoice for the amount due”","Item",{"v":1,"d":"1.00"}]
["A35.0 PAYMENT TO OTHER PARTIES",""]
["Clause 35.0","Item",{"v":1,"d":"1.00"}]
["CANCELLATION",""]
["A36.0 CANCELLATION BY EMPLOYER - CONTRACTOR’S DEFAULT",""]
["Clause 36.0      \nClause 36.1 is amended by the addition of the following clauses:      \n \n36.1.3 refuses or neglects to comply strictly with any of the conditions of contract     \n \n36.1.4 estate being sequestrated, liquidated or surrendered in terms of ","Item",{"v":1,"d":"1.00"}]
["A37.0 CANCELLATION BY EMPLOYER - LOSS AND DAMAGE",""]
["Clause 37.0      \nClause 37.0 is amended by the addition of the following clause: \n \nClause 37.3.5 is amended by replacing 'ninety (90)' with 'one-hundred and twenty (120)'         \n \n37.5 Notwithstanding any clause to the contrary, on cancellation of thi","Item",{"v":1,"d":"1.00"}]
["A38.0 CANCELLATION BY CONTRACTOR - EMPLOYER’S DEFAULT",""]
["Clause 38.0      \n \nClause 38.5.4 is amended by replacing 'ninety (90)' with 'one-hundred and twenty (120)'         \n \nClause 38.0 is amended by the addition of the following clause:       \n \n38.7 Notwithstanding any clause to the contrary, on cancellatio","Item",{"v":1,"d":"1.00"}]
["A39.0 CANCELLATION - CESSATION OF THE WORKS",""]
["Clause 39.0      \n \nClause 39.3.5 is amended by the addition of the following at the end of the sentence: 'within one hundred and twenty (120) working days of completion of such a report'","Item",{"v":1,"d":"1.00"}]
["DISPUTE",""]
["A40.0 DISPUTE SETTLEMENT",""]
["Clause 40.0  \nRetention of clause 40 in respect of dispute settlement in its original form not applying the state clause amendments.  \n \nDispute resolution shall be by adjudication. If a dispute is unresolved by adjudication the dispute shall be finally s","Item",{"v":1,"d":"1.00"}]
["SUBSTITUTE PROVISIONS",""]
["A41.0 STATE CLAUSES",""]
["Clause 41.0\n \n  \nClause 41 State Substitutions is amended as set out below with reference to sub-clause 41.1 or the original clause number stated therein.\n  \nIn sub-clause 41.1.3 the definition for CONSTRUCTION PERIOD is amended to read:\nCONSTRUCTION PERI","Item",{"v":1,"d":"1.00"}]
["CONTRACT VARIABLES",""]
["A42.0 THE SCHEDULE (DPW-04EC)",""]
["Clause 42.0      \n \nTenderers are referred to the Contract Data DBSA Volume 3 of 3 The Contract for variables pertaining to this contract (Refer to Part One - Data provided by the Employer on Item 42.1.1 to 42.5.4)","Item",{"v":1,"d":"1.00"}]
["SECTION B: JBCC PRELIMINARIES",""]
["B1.0 DEFINITIONS AND INTERPRETATION",""]
["B2.0 DOCUMENTS",""]
["B2.1 Checking of documents","Item",{"v":1,"d":"1.00"}]
["B2.2 Provisional bills of quantities","Item",{"v":1,"d":"1.00"}]
["B2.3 Availability of construction documentation","Item",{"v":1,"d":"1.00"}]
["B2.4 Interests of agents","Item",{"v":1,"d":"1.00"}]
["B2.5 Priced documents","Item",{"v":1,"d":"1.00"}]
["B2.6 Tender submission         Clause 2.6 is amended by replacing  'JBCC Form of Tender' with 'Form of Offer and Acceptance DPW-07(EC)'","Item",{"v":1,"d":"1.00"}]
["B3.0 THE SITE",""]
["B3.1 Defined works area","Item",{"v":1,"d":"1.00"}]
["B3.2 Geotechnical investigation","Item",{"v":1,"d":"1.00"}]
["B3.3 Inspection of the site","Item",{"v":1,"d":"1.00"}]
["B3.4 Existing premises occupied","Item",{"v":1,"d":"1.00"}]
["B3.6 Previous work - defects","Item",{"v":1,"d":"1.00"}]
["B3.7 Services - known","Item",{"v":1,"d":"1.00"}]
["B3.8 Services - unknown","Item",{"v":1,"d":"1.00"}]
["B3.9 Protection of trees","Item",{"v":1,"d":"1.00"}]
["B3.10 Articles of value","Item",{"v":1,"d":"1.00"}]
["B3.11 Inspection of adjoining properties","Item",{"v":1,"d":"1.00"}]
["B4.0 MANAGEMENT OF CONTRACT",""]
["B4.1 Management of works","Item",{"v":1,"d":"1.00"}]
["B4.2 Programme for the works","Item",{"v":1,"d":"1.00"}]
["B4.3 Progress meetings","Item",{"v":1,"d":"1.00"}]
["B4.4 Technical meetings","Item",{"v":1,"d":"1.00"}]
["B4.5 Labour and plant records","Item",{"v":1,"d":"1.00"}]
["B5.0 SAMPLES, SHOP DRAWINGS AND MANUFACTURERS’ INSTRUCTIONS",""]
["B5.1 Samples of materials","Item",{"v":1,"d":"1.00"}]
["B5.2 Workmanship samples","Item",{"v":1,"d":"1.00"}]
["B5.3 Shop drawings","Item",{"v":1,"d":"1.00"}]
["B5.4 Compliance with manufacturers’ instructions","Item",{"v":1,"d":"1.00"}]
["B6.0 TEMPORARY WORKS AND PLANT",""]
["B6.1 Deposits and fees","Item",{"v":1,"d":"1.00"}]
["B6.2 Encloser of the works","Item",{"v":1,"d":"1.00"}]
["B6.3 Advertising","Item",{"v":1,"d":"1.00"}]
["B6.4 Plant, equipment,sheds and offices","Item",{"v":1,"d":"1.00"}]
["B6.5 Main notice board","Item",{"v":1,"d":"1.00"}]
["B6.6 Subcontractors' notice board","Item",{"v":1,"d":"1.00"}]
["B7.0 TEMPORARY SERVICES",""]
["B7.1 Location","Item",{"v":1,"d":"1.00"}]
["B7.2 Water","Item",{"v":1,"d":"1.00"}]
["B7.3 Electricity","Item",{"v":1,"d":"1.00"}]
["B7.4 Telecommunication facilities","Item",{"v":1,"d":"1.00"}]
["B7.5 Ablution facilities","Item",{"v":1,"d":"1.00"}]
["B8.0 PRIME COST AMOUNTS",""]
["B8.1 Responsibility for prime cost amounts","Item",{"v":1,"d":"1.00"}]
["B9.0 ATTENDANCE ON N/S SUBCONTRACTORS",""]
["B9.1 General Attendance","Item",{"v":1,"d":"1.00"}]
["B9.2 Special Attendance","Item",{"v":1,"d":"1.00"}]
["B9.3 Commissioning - fuel, water and electricity","Item",{"v":1,"d":"1.00"}]
["B10.0 FINANCIAL ASPECTS",""]
["B10.1 Statutory taxes, duties and levies","Item",{"v":1,"d":"1.00"}]
["B10.3 Adjustment of preliminaries     \n \nClauses B10.3.1 and B10.3.2 are amended by replacing 'within fifteen (15) working days of taking possession of the site' with 'when submitting his priced bills of quantities / lump sum document'","Item",{"v":1,"d":"1.00"}]
["B10.4 Payment certificate cash flow","Item",{"v":1,"d":"1.00"}]
["B11.0 GENERAL",""]
["B11.1 Protection of the works","Item",{"v":1,"d":"1.00"}]
["B11.2 Protection/isolation of existing/sectionally occupied works","Item",{"v":1,"d":"1.00"}]
["B11.3 Security of the works","Item",{"v":1,"d":"1.00"}]
["B11.4 Notice before covering work","Item",{"v":1,"d":"1.00"}]
["B11.5 Disturbance","Item",{"v":1,"d":"1.00"}]
["B11.6 Environmental disturbance","Item",{"v":1,"d":"1.00"}]
["B11.7 Works cleaning and clearing","Item",{"v":1,"d":"1.00"}]
["B11.8 Vermin","Item",{"v":1,"d":"1.00"}]
["B11.9 Overhand work","Item",{"v":1,"d":"1.00"}]
["B11.11 As built information","Item",{"v":1,"d":"1.00"}]
["B11.12 Tenant installations","Item",{"v":1,"d":"1.00"}]
["B12.0 SCHEDULE OF VARIABLES",""]
["Schedule of variables:",""]
["This schedule contains all variables referred to in this document and is divided into pre-tender and post-tender categories. The pre-tender categorymust be completed in full and included in the tender documents. Both the pre-tender and post-tender categor","Item",{"v":1,"d":"1.00"}]
["12.1 PRE-TENDER INFORMATION",""]
["12.1.1 Provisional bills of quantities       No",""]
["The quantities are provisional: No",""]
["12.1.2 Availability of construction documentation        \n \n[2.3] Construction documentation complete: Yes",""]
["12.1.3 Interests of agents       \n \n[2.4] Details: None",""]
["12.1.4 Defined works area      \n \n[3.1] Details: As per architect's indication",""]
["12.1.5 Geotechnical investigation      \n \n[3.2] Details: None conducted.",""]
["12.1.6 Existing premises occupied      \n \n[3.4] Specific requirements: Yes.",""]
["12.1.7 Previous work - dimensional accuracy      \n \n[3.5] Details:",""]
["12.1.8 Previous work - defects      \n \n[3.6] Details:",""]
["12.1.9 Services - known     \n \n[3.7] Details:",""]
["12.1.10 Protection of trees         \n \n[3.9] Specific requirements: The contractor is to preserve all trees on site and is to request instruction from the Principal Agent where trees are constricting the work areas or progress of work.",""]
["12.1.11 Inspection of adjoining properties          \n \n[3.11] Specific requirements: The contractor is to ensure that no harm comes to adjoining buildings or property during the progress of the works.",""]
["12.1.12 Enclosure of the works          \n \n[6.2] Specific requirements: The contractor is to enclose the works in the manner necessary to prevent members of the public, the client's workers or any other persons from being hurt due to coming into areas whe",""]
["12.1.13 Offices         \n \n[6.4.3] Specific requirements: The contractor shall provide, maintain and remove on completion of the works an office for the exclusive use of the principal agent, minimum size 4 x 3 x 3m high internally, suitably insulated and ",""]
["Defined works area",""]
["12.1.14 Main notice board          \n \n[6.5] Specific requirements: The contractor shall provide, erect where directed, maintain and remove on completion of the works a notice board size 3 x 3m as type Drawing GEN 063, constructed of suitable boarding with",""]
["12.1.15 Subcontractors' notice board         \n \n[6.6] A Notice Board is required: No              \n \nNo Specific requirements: Not Applicable",""]
["12.1.16 Water      \n \n[7.2]  Option A - by Contractor (Yes)         \n \nOption B - by employer (free of charge)                 \n \nOption C - by employer (metered)",""]
["12.1.17 Electricity          \n \nOption A - by Contractor (Yes)                 \n \nOption B - by employer (free of charge)                 \n \nOption C - by employer (metered)",""]
["12.1.18 Telecommunications          \n \n[7.4] Telephone: Yes                \n \nFacsimile: Not necessary",""]
["12.1.19 Ablution facilities          \n \n[7.5] Option A (by contractor) (Yes)              \n \nOption B (by employer) (No)",""]
["12.1.20 Protection of existing/sectionally occupied works         \n \n[11.2] Protection is required (Yes/No) Yes",""]
["12.1.21 Special attendance          \n \n[9.2] Subcontractor (1) details: Not applicable",""]
["12.1.22 Protection of the works          \n \n[11.1] Specific requirements: All precautions are to be taken to prevent damage or harm to the works. The client is to be indemnified against any and all eventualities. The existing buildings are to be insured a",""]
["12.1.23 Disturbance          \n \n[11.5] Specific requirements:The contractor shall keep the site, structures, etc. well watered during operations to prevent dust and shall provide and erect and remove on completion of the works all necessary temporary dust",""]
["12.1.24 Environmental disturbance          \n \n[11.6] Specific requirements: The contractor is to ensure that no environmental damage occurs on or over the site during the execution of the works and whilst he is in possession of the site. All precautions a",""]
["12.2 POST-TENDER INFORMATION",""]
["12.2.1 Payment of preliminaries         \n \n[10.2] Option A (prorated) (Yes/No):                                                        \n \nOption B (calculated) (Yes/No): ",""]
["12.2.2 Adjustment of preliminaries        \n \n[10.3] Option A (three categories) (Yes/No):\n                                                           \nOption B (detailed breakdown) (Yes/No): ",""]
["12.2.3 Additional agreed preliminaries items      Details:",""]
["SECTION C: SPECIFIC PRELIMINARIES",""]
["Section C contains specific preliminary items which apply to this contract except where N/A (Not Applicable) appears against an item.  Tenderers are advised to familiarise themselves as much as possible with these items as no later financial costs will be",""]
["GENERAL \n \nThe contractor's attention is drawn to the Contract Participation Goals and CIDB Build Programme. All requirements of the aforesaid are detailed in the Provisional Sums (Section No. 11, Bill No.2) of these Bills of Quantities document including","",{"v":1,"d":"1.00"}]
["C1: CONTRACT DRAWINGS  \n \nThe drawings issued with the tender documents do not comprise the complete set but serve as a guide only for tendering purposes and for indicating the scope of the work to enable the tenderer to acquaint himself with the nature a","Item",{"v":1,"d":"1.00"}]
["C2: GENERAL PREAMBLES       \n \nThe document 'Specification of Materials and Methods to be used (PW371-A)' is obtainable on the Department's website (http://www.publicworks.gov.za/ under 'Consultants Guidelines') and shall be read in conjunction with the P","Item",{"v":1,"d":"1.00"}]
["C3: TRADE NAMES  \n \nWherever a trade name for any product has been described in the  bills of quantities / lump sum document , the tenderer' s attention is drawn to the fact that any other product of equal quality may be used subject to the written approv","Item",{"v":1,"d":"1.00"}]
["C4: IMPORTED MATERIALS AND EQUIPMENT   \n \nWhere imported items are listed in the tender documents, the tenderer shall provide all the information called for, failing which the price of any such item, materials or equipment shall be excluded from currency ","Item",{"v":1,"d":"1.00"}]
["C5: VIEWING THE SITE    \n \nThe site is located within the municipal boundaries of Hankey, Eastern Cape, just south east of the town, on either side of the R330, and falls under the jurisdiction of the Kouga Local Municipality (see locality map included)  ","Item",{"v":1,"d":"1.00"}]
["C6: COMMENCEMENT OF WORKS IN SENSITIVE AREAS  \n \nThe site is classified as a National Heritage site and the vegetation on and surrounding the site are classified as environmentally sensitive zones, therefore the following procedures are compulsory and sho","Item",{"v":1,"d":"1.00"}]
["C7: SECURITY CHECK OF PERSONNEL  \n \nThe Principal Agent may require the contractor to have his personnel and workmen, or a certain number of them, security classified.  In the event of the principal agent requesting removal of a person or persons from the","Item",{"v":1,"d":"1.00"}]
["C8: PROHIBITION ON TAKING OF PHOTOGRAPHS  \n \nThe scope of the works involves minor works to a school adjacent to the site. Any photographs taken of the school or its grounds is prohibited to eliminate exposure of the children at the school.   ","Item",{"v":1,"d":"1.00"}]
["C9: HIV/AIDS AWARENESS  \n \nIt is required of the contractor to thoroughly study the HIV/AIDS Specification (PW1544) of the Department that must be read together with and is deemed to be incorporated under this Section of the bills of quantities (C3.4). Pr",""]
["C9.1: AWARENESS CHAMPION   \n \nSelection, appointment, briefing and making available of an Awareness Champion including provision of all relevant services, all in accordance with the HIV/AIDS Specification.  ","Item",{"v":1,"d":"1.00"}]
["C9.2: AWARENESS WORKSHOP  \n \nSelection and appointment of a competent Service Provider approved by the  principal agent , provision of a Service Provider Workshop Plan and a suitable venue, conducting of awareness workshops by means of traditional and/or ","Item",{"v":1,"d":"1.00"}]
["C9.3: POSTERS, BOOKLETS, VIDEOS, ETC.  \n \nProvision, displaying, maintaining and replacing when necessary of four plastic laminated posters, booklets and educational videos, etc. for the duration of the  construction period, all in accordance with the HIV","Item",{"v":1,"d":"1.00"}]
["C9.4: ACCESS TO CONDOMS   \n \nProvision and maintenance of condom dispensers fixed in position, including male and female condoms, replenishing male and female condoms on a daily basis as required for the duration of the  construction period, all in accord","Item",{"v":1,"d":"1.00"}]
["C9.5: MONITORING  \n \nMonitoring HIV/AIDS awareness of workers, providing the  principal agent with access to information including making available all reports (HIV/AIDS Awareness, Record of HIV/AIDS awareness activities, Monthly Summary of both these) as","Item",{"v":1,"d":"1.00"}]
["C10: COPYRIGHT, ETC  \n \nThe contractor may be required to obtain copyright permission to use certain material from original artist. All the requirements are of this item are to be priced hereunder. No additional items or extras to the contract in this reg","Item",{"v":1,"d":"1.00"}]
["C11: OCCUPATIONAL HEALTH AND SAFETY ACT  \n \nThe contractor shall comply with all the requirements set out in the Construction Regulations, 2014 issued under the Occupational Health and Safety Act, 1993 (Act No.85 of 1993). It is required of the contractor","Item",{"v":1,"d":"1.00"}]
["C12: COVID-19 REGULATIONS  \n \nThe contractor shall comply with all the requirements set out in the Code of Practice: Managing exposure to SARS-CoV-2 in the workplace. It is up to the contractor to use this as the basis for pricing this item, which in itse","Item",{"v":1,"d":"1.00"}]
["C13: CERTIFIED ROOF INSPECTOR\n \nThe contractor shall make available a suitably qualified individual to inspect all timber roof trusses.\n \nThe individual to be registered with the Engineering Council of South Afrrica (ECSA) and be a certified ITC roof trus","Item",{"v":1,"d":"1.00"}]
["C14: REPORTING BY CONTRACTOR  \n \nThe contractor is required to complete the Contractors Monthly Report (to be agreed)which is to be submitted together with the contractors payment claim. Payment of the contractor is conditional on this information being a","Item",{"v":1,"d":"1.00"}]

{"sheet":"Sect 2","index":1,"n_rows":582,"n_cols":5,"rows_kept":582}
["Description","Uom","Quantity","Rate","Amount"]
["SUPPLEMENTARY PREAMBLES",""]
["TEMPORARY BARRICADES, SCREENS, ETC",""]
["Temporary barricades, screens, roofs, etc including removal",""]
["Take down and remove temporary timber hoarding boards","m²",{"v":10,"d":"10.00"}]
["Take out and remove temporary timber hoarding frames not exceeding 300mm width and repair holes by patching in plaster and finish of wall neatly","m",{"v":13,"d":"13.00"}]
["Take out and remove gumpoles including hacking up and removing, prepare surface for new screed  and lay- in new screed.","No",{"v":30,"d":"30.00"}]
["REMOVAL OF EXISTING WORK",""]
["Breaking up and removing exposed aggregate",""]
["Paving","m²",{"v":34,"d":"34.00"}]
["Breaking up and removing unreinforced concrete, etc",""]
["450 x 100mm In-situ copings","m",{"v":156,"d":"156.00"}]
["500 x 100mm In-situ copings","m",{"v":75,"d":"75.00"}]
["550 x 100mm In-situ copings","m",{"v":245,"d":"245.00"}]
["Internal sill to W01 & W03 window approximately 120mm x 30mm thick","m",{"v":38,"d":"38.00"}]
["Breaking up and removing reinforced concrete, including cutting off and removing reinforcement.",""]
["125 mm Thick surface beds.","m³",{"v":28,"d":"28.00"}]
["170mm Thick slabs","m³",{"v":23,"d":"23.00"}]
["Retaining wall","m³",{"v":88,"d":"88.00"}]
["Retaining wall including digging up and removing foundations","m³",{"v":4,"d":"4.00"}]
["Columns","m³",{"v":3,"d":"3.00"}]
["170mm Thick rib and block.","m²",{"v":50,"d":"50.00"}]
["Taking down and removing roofs, floors, panelling, ceilings, partitions, etc",""]
["Shutter board from soffit of ceiling","m²",{"v":2,"d":"2.00"}]
["Shutter pieces on reception curved rafter stub Columns","m",{"v":22,"d":"22.00"}]
["Carefully remove, set aside internal toilet partition for alteration work and place back to same postion when work completed.","m",{"v":65,"d":"65.00"}]
["Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc",""]
["Skimming off skimmed concrete ceilings, prepare surface and re-skim to match exisiting.","m²",{"v":108,"d":"108.00"}]
["Internal plaster from walls and columns, prepare surface and replaster to match exisitng.","m²",{"v":6,"d":"6.00"}]
["Plaster from brick walls","m²",{"v":169,"d":"169.00"}]
["75mm Wide stone cladding from concrete walls","m²",{"v":19,"d":"19.00"}]
["Hacking up/off and removing ceramic tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc",""]
["Tiles to walls including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc","m²",{"v":14,"d":"14.00"}]
["Hacking up/off and removing mosiac tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc",""]
["Tiles to walls including removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new tile finish, etc ","m²",{"v":176,"d":"176.00"}]
["Taking out and removing sanitary fittings, tanks, geysers, etc, including disconnecting from pipes, traps, etc and making good floor and wall finishes (making good tiling and paintwork elsewhere)",""]
["Stainless steel wash hand basin","No",{"v":1,"d":"1.00"}]
["Porcelain wash hand basin ","No",{"v":1,"d":"1.00"}]
["Chromium plated shower trap","No",{"v":1,"d":"1.00"}]
["REMEDIAL WORKS TO CONCRETE, FORMWORK AND REINFORCEMENT",""]
["Bases",""]
["Fill up bases below structural base plates as per engineers specification with suitable concrete material as directed and make neat and square with 20mm 45 degree chamfered corners","No",{"v":6,"d":"6.00"}]
["Cement Screed",""]
["Prepare by cleaning, removing laitance, airborne dust, where applicable chip to expose main aggregate, cut out all suspect material, free surface of all debris and apply ABE Epidermix 314 structural repair mortar to damaged screeds according to manufactur","m²",{"v":2146,"d":"2146.00"}]
["Liquid bituminous waterproofing to floor drain channel","m²",{"v":5,"d":"5.00"}]
["Repair saw cut joint by reaming 10 x 20mm deep, apply 10mm backing cord sealed with 10 x 10mm Sikaflex 11FC polyurethane joint sealant.","m",{"v":372,"d":"372.00"}]
["Repair wall isolation joint by reaming 10 x 20mm deep, apply 10mm backing cord sealed with 10 x 10mm Sikaflex 11FC polyurethane joint sealant.","m",{"v":77,"d":"77.00"}]
["Repair crack to surface bed by reaming 10 x 20mm deep, apply 10mm backing cord sealed with 10 x 10mm Sikaflex 11FC polyurethane joint sealant.","m",{"v":4,"d":"4.00"}]
["Off-shutter concrete ceilings",""]
["Repair by chiselling off unsuitable build-up product and apply one even coat of ABE Durarep FR polymer-modified, fibre reinforced, cement-based non-shrink mortar according to manufacturer's instructions to match existing.","m²",{"v":332,"d":"332.00"}]
["Skimming to concrete ceilings to achieve uniform colour and finish through out (removal of skimming elsewhere measured)","m²",{"v":130,"d":"130.00"}]
["Redirect fall on canopy slab to fall towards spouts","m²",{"v":116,"d":"116.00"}]
["Repair skimming on concrete coping on top of parapet wall","m²",{"v":8,"d":"8.00"}]
["Repair chipped and damaged concrete thresholds","m²",{"v":9,"d":"9.00"}]
["Remove nails in concrete ceiling fill holes ","No",{"v":9,"d":"9.00"}]
["Beams",""]
["Removal of shutter material and nails on concrete beam (BM33 on REC/5007), complete rough brick support interface and ensure slipjoint on top of brickwork is completed as per engineers specification.\n \n ","m²",{"v":14,"d":"14.00"}]
["Removal of shutter material and nails on concrete soffit, repairs around light fittings to be done as per architect and engineers specification including skim repair of internal slab and rough edges and provision of brickwall slip joint as per engineer's ","m²",{"v":58,"d":"58.00"}]
["Repair to top 100mm of upstand concrete beam as per drawing REC/1007 and architect and engineers specification","m",{"v":102,"d":"102.00"}]
["Cut new drip recess on underside of concrete as per specification","m",{"v":171,"d":"171.00"}]
["Remove ferrule cones and grout holes with an approved non-shrink grout to beams.","m",{"v":13,"d":"13.00"}]
["Pile caps",""]
["Repairs to exposed pile cap not flushed with wall and floor edge including removing and repairs to excess concrete","No",{"v":3,"d":"3.00"}]
["Concrete Walls",""]
["Repair defective pigmented concrete walls","m²",{"v":474,"d":"474.00"}]
["Repair defective pigmented concrete wall in patches","m²",{"v":78,"d":"78.00"}]
["Repair skew pigmented concrete buttress wall at rear planter box (Wall size 250mm wide x 680mm deep x 2000mm High)","m³",{"v":1,"d":"1.00"}]
["Fill aperture in concrete wall with ABE Dura rep FR matching adjacent surface. ","m²",{"v":3,"d":"3.00"}]
["One coat clear matt sealant paint on concrete grey walls","m²",{"v":74,"d":"74.00"}]
["REMEDIAL WORKS TO EXISTING CONCRETE SURFACES",""]
["SUPPLEMENTARY PREAMBLES",""]
["OPTION 1: ABRASIVE (SAND) BLAST CLEANING OF EXISTING CONCRETE SURFACES",""]
["Preparation - removal of currently applied skimming product",""]
["* Contractor to prepare concrete surface by removing all skimming compound varying in depth between 0.5 ad 5mm on currently constructed concrete surfaces. To be done using various procedures including but not limited to grinding, grit blasting or manual m",""]
["* Mechanical breakers will not be permitted in the removal of currently applied skimming product. Contractor to ensure that no damage occurs to the existing concrete substrate located beneath the existing skim product.",""]
["* It is to be assumed that prior to blasting all walls will be repaired as elsewhere specified.",""]
["Equipment",""]
["*Equipment shall be adequate to be able to provide the blast profile specified.",""]
["*The required finish to the concrete surface will have a profile from the current raw surface (NOT CURRENT SKIMMED SURFACE) as outlined below:\n \nPercentage of concrete surface vs the maximum profile depth excluding 19mm stone aggregate \n \n95% of all surfa",""]
["Workmanship & OHS requirements",""]
["*The method of abrasive blasting finishes to be carried out by generally accepted methods of the trade and by qualified tradesman and equipment.\n*The abrasive blast cleaner is to ensure that they are suitably protected as required by current health and sa",""]
["Cleaning of area on Completion of Works ",""]
["Upon completion of Works:\n*All blasted surfaces to be washed down to remove residue material.\n*All equipment protection, masking materials and residue to be removed.\n*All blast material to be removed from site and disposed of as required by current legisl",""]
["OPTION 2: BUSH HAMMER EXISTING CONCRETE SURFACES",""]
["Preparation -removal of currently applied skimming product",""]
["*Contractor to prepare concrete surface by removing all skimming compound varying in depth between 0.5 ad 5mm on currently constructed concrete surfaces. To be done using various procedures including but not limited to grinding, grit blasting or manual me",""]
["*Mechanical breakers will not be permitted in the removal of currently applied skimming product. Contractor to ensure that no damage occurs to the existing concrete substrate located beneath the existing skim product.",""]
["*Alternative to the above, the existing skim coat may be removed in one action by means of a bush hammer tool, when bush hammer effect is applied, but care must be taken not to penetrate the wall deeper than described above",""]
["*It is to be assumed that prior to blasting all walls will be repaired as elsewhere specified.",""]
["Equipment",""]
["*Equipment shall be adequate to be able to provide the bush hammer profile specified.\n*Breakers should not exceed 7kg in size",""]
["Required finish to the concrete surface\n*Remove the minimum matrix, including all laitance, using bush hammering to expose the coarse aggregate without recessing the matrix deeper than the aggregate, to give a uniform texture with insignificant random too",""]
["Workmanship\n \n*The method of brush hammering finishes to be carried out by generally accepted methods of the trade and by qualified tradesmen and equipment.\n ",""]
["AESTHETIC REMEDIAL WORK TO GENERAL SURFACE FINISHES OF EXTERNAL CONCRETE RETAINING WALLS",""]
["Abrasive blasting finish concrete, as described above (penetrating sealer measured elsewhere) including preparatory work as previously decsribed\n \n ","m²",{"v":4630,"d":"4630.00"}]
["Bush hammer finish complete, as described above (penetrating sealer measured elsewhere) including preparatory work as previously described ","m²",{"v":1984,"d":"1984.00"}]
["Prepare and apply two coats TFC Topseal or equally approved clear matt sealant on",""]
["Abrasive blasted concrete surfaces","m²",{"v":4630,"d":"4630.00"}]
["Bush hammered concrete surfaces ","m²",{"v":1984,"d":"1984.00"}]
["MARMORAN ",""]
["SURFACE PREPARATION",""]
["Apply Marmoran Marmocide to areas where algea growth is present. High pressure wash using a hydroblaster with a combination of flat & rotating nozzels. Mechanically remove contaminents and loose materials",""]
["Prepare and apply Marmoran Mormocide including high pressure wash with combination hydroblaster to mechanically remove all contaminents and loose materials",""]
["On concrete walls","m²",{"v":1,"d":"1.00"}]
["Using a block brush, slush apply Marmoran Easykey/Riversand/Cement compound as a slurry to create a key",""]
["On concrete walls","m²",{"v":1,"d":"1.00"}]
["MARMORAN EASYPLAST",""]
["Mechanically batch Marmoran Easyplast add mix with sand/cement and trowel apply on the treated surfaces in layers to achieve an even surface",""]
["On concrete walls","m²",{"v":1,"d":"1.00"}]
["On concrete benches","m²",{"v":1,"d":"1.00"}]
["On tops of concrete walls n.e. 300mm wide","m",{"v":1,"d":"1.00"}]
["Polyurethane sealing compound including backing cord, bond breaker, primer, etc.",""]
["10 x 10mm In expansion joints in walls, etc. including raking out expansion joint filler as necessary","m",{"v":1,"d":"1.00"}]
["Three of coats Marmoran GP Waterproofing",""]
["On tops of concrete walls n.e 300mm wide","m",{"v":1,"d":"1.00"}]
["MARMORAN PERMAPLAST (10 YEAR GUARANTEE)",""]
["Roller apply Marmoran pigmented Rbp Masony textured solvent primer to suitably prepared surface & allow to dry. Trowel apply Marmoran Permacrete Warm Embrace resin bonded plaster to achieve a minimum wft of 1.0mm & using a plastic trowel, pattern to the d",""]
["To wall areas","m²",{"v":1,"d":"1.00"}]
["MARMORAN CONCRETEX (10 YEAR GUARANTEE)",""]
["Roller apply Marmoran pigmented Rbp Masony textured solvent primer to suitably prepared surface & allow to dry. Trowel apply Marmoran Concretex resin bonded plaster using a steel trowel and polish with same. Allow to dry then roller apply two coats of Mar",""]
["To wall areas (rate only)","m²",{"v":1,"d":"1.00"}]
["SCAFFOLDING ACCESS",""]
["Supply sufficient safe scaffold in uninterrupted section","Item",{"v":1,"d":"1.00"}]
["TRANSPORT, ACCOMMODATION, PRELIMINARY & GENERAL COSTS, HEALTH & SAFETY",""]
["P&G costs transport management etc. 15%","Item",{"v":1,"d":"1.00"}]
["STRUCTURAL REMEDIAL WORK TO GENERAL SURFACES OF EXTERNAL CONCRETE RETAINING WALLS",""]
["Shallow repair to walls in patches (Maximum 70mm repair depth- see specification S9615/SPEC/002)",""]
["a)Grind (square cut) minimum 10mm deep around area to be repaired- no feathering of repair product permitted.\nb)Remove rejected concrete/repair product as applicable.\nc)Ensure that entire repair area is chipped back minimum 10mm deep and that adhesion sur",""]
["To grey concrete walls","m²",{"v":180,"d":"180.00"}]
["To pigmented concrete walls, including pigment additive to match adjacent colour","m²",{"v":50,"d":"50.00"}]
["Extra over for bulking Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume","m²",{"v":90,"d":"90.00"}]
["Deep repair to walls in patches (Minimum 50mm repair depth – see specification S9615/SPEC/002)",""]
["a)Grind (square cut) minimum 10mm deep around area to be repaired- no feathering of repair product permitted.\nb)Demolish rejected concrete or repair product.\nc)Ensure that entire repair area is chipped back minimum 50mm deep and that adhesion surface is f",""]
["To grey concrete walls","m²",{"v":48,"d":"48.00"}]
["To pigmented concrete walls, including pigment additive to match adjacent colour","m²",{"v":57,"d":"57.00"}]
["Finishing off and cleaning pigmented walls, corners, edges and marked areas including one coat clear matt sealant.","m²",{"v":144,"d":"144.00"}]
["Extra over for bulking Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume","m²",{"v":48,"d":"48.00"}]
["Top of pigmented wall (see specification S9615/spec/002)",""]
["a)Remove existing repair product (where present)\nb)Grind 30deep (square cut) on each side of the wall to form a straight level line along the entire wall length. Demolish the upper concrete portion.\nc) Grind top surface to remove laitance.\nd) Remove rejec",""]
["Repairs to top of pigmented concrete retaining walls not exceeding 300mm wide including pigment addictive to match adjacent colour","m",{"v":240,"d":"240.00"}]
["Extra over for bulking for Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume","m",{"v":45,"d":"45.00"}]
["Top of grey concrete wall (See specification S9615/SPEC/002)",""]
["a)Remove existing repair product (where present)\nb)Grind 30 deep (square cut) on each side of the wall to form a straight level line along the entire wall length. Demolish the upper concrete portion.                              c) Grind top surface to re",""]
["Repairs to top of grey concrete retaining walls not exceeding 300mm wide ","m",{"v":203,"d":"203.00"}]
["Ditto, box channel walls ","m",{"v":222,"d":"222.00"}]
["Extra over for bulking Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume ","m",{"v":52,"d":"52.00"}]
["REMEDIAL WORK TO EXPANSION JOINTS ",""]
["Repair to out of plumb wall expansion/construction joints ( See specification S9615/SPEC/002)",""]
["a) Grind reinforced concrete 30mm deep x 100mm offset on either side of the joint.\nb) Demolish 30mm deep x 200mm wide concrete strip across joint.\nc) Remove foreign matter, dust, loose aggregate by means of a high-pressure cleaning.\nd) Place a vertical sh",""]
["12mm Wide joint","m",{"v":204,"d":"204.00"}]
["20mm Wide joint","m",{"v":145,"d":"145.00"}]
["Repair to plumb wall expansion/construction joints (See specification S9615/SPEC/002)",""]
["a) Rub down joint to produce neat straight smoth joint\nb) For 20mm wide joint: Rake out 20mm joint material. For 10mm/12mm wide joint: Rake out 20mm joint former material\nc) Place 20mm/12mm/10mm backing cord (as per joint width)\nd) For 20mm wide joint: Se",""]
["12mm Wide joint","m",{"v":109,"d":"109.00"}]
["20mm Wide joint","m",{"v":77,"d":"77.00"}]
["'Sikaflex 11FC+' polyurethane sealing compound including backing cord, bond breaker, primer, etc.",""]
["12 x 10mm in expansion joints in walls including raking out expansion joint filler as necessary","m",{"v":302,"d":"302.00"}]
["20x20mm In expansion joints in walls incuding raking out expansion joint filler as necessary","m",{"v":156,"d":"156.00"}]
["Repair edge of expansion joint as per engineer detail and fill with polysulfide(brown)","m",{"v":15,"d":"15.00"}]
["'ABE Epidermix 344' two-component, solvent-free, polysulphide modified epoxy adhesive substrate",""]
["On concrete walls","m²",{"v":102,"d":"102.00"}]
["'ABE Durarep FR' single component, polymer modified fibre-reinforced, cement based, chloride free, non-shrink mortar",""]
["30mm Thick on concrete walls","m",{"v":102,"d":"102.00"}]
["Sand down plastered sill and work off to have a minor fall, apply ABE Durarep FR and sand smooth,clean out drip joint and repair chips to sills","m²",{"v":21,"d":"21.00"}]
["REPAIR PAINTING TO PREVIOUSLY PAINTED WALLS",""]
["Cutting in corners - mask corner or ther material (such as window frame, pigment etc) securely and in a straight line, and then apply 2 coats of paint, colour to match wall.\n \nAll paint specification to adhere to original paint specfication.",""]
["Minor preparatory work to painted plastered walls as directed by architect","m²",{"v":56,"d":"56.00"}]
["Fill holes and chips with crack filler, sand down smooth, and clean from dust and dirt. Inspect wall to identify patches where second final coat is not applied, then paint entire wall surface with final coat. In case of a chipped and patched area then pat","m²",{"v":5579,"d":"5579.00"}]
["Approved water proofing sealant on treated 220mm brickwalls","m²",{"v":14,"d":"14.00"}]
["Skim rough product finish and repair damaged edges","m²",{"v":120,"d":"120.00"}]
["REPAIR WORK TO WALLS WHERE TERYLENE PLASTER PREVIOUSLY APPLIED",""]
["Remove terylene plaster using metal paint scraper, taking care not to damage plaster surface.","m²",{"v":5189,"d":"5189.00"}]
["Demolish existing plaster copings. Clean top of wall from all loose mortar until raw brick surface is visible and take care not to damage plaster below or any other building element. Apply one layer of cementitious waterproofing to top of raw wall such as","m",{"v":172,"d":"172.00"}]
["Demolish cement plastered concrete copings and reconstruct with approved joints and seal concrete wall after construction as per engineers specifications and drawings","m",{"v":51,"d":"51.00"}]
["Cut neatly all corners to form neat corner between wall and floors","m",{"v":216,"d":"216.00"}]
["Cut neatly all corners to form neat corner between wall and concrete ceilings","m",{"v":26,"d":"26.00"}]
["REMEDIAL WORKS TO ROOF COVERING",""]
["Metal roofs and flashings:",""]
["Warped sidewall flashing removed, straightened and repainted with similar paint and replaced in similar position","m",{"v":5,"d":"5.00"}]
["Remove and replace a portion of bent flashing in the same position ensuring same matching colour paint.","m",{"v":4,"d":"4.00"}]
["Cut neatly all protruding insulation from underside of metal roof and ensure that it is straight and flush with purlin including cutting off bolts","m",{"v":49,"d":"49.00"}]
["REMEDIAL WORKS TO CARPENTRY AND JOINERY, IRONMONGERY, ETC",""]
["Doors",""]
["Prepare for painting timber door and frame size 900 x 2100mm high and apply one coat of piant for timber door as per specification on all sides including leaf and frame","m²",{"v":16,"d":"16.00"}]
["Final preparation and paint work to door and frame of cupboard, cupboard sized 1520 x 2032 high","m²",{"v":12,"d":"12.00"}]
[" Paint to incomplete D04 at Kitchen entrance","m²",{"v":6,"d":"6.00"}]
["Remove damaged timber door leaf  for D01 as per door schedule and set aside ironmongery for re-installation, replace with new similar door and fix ironmongery into position","No",{"v":1,"d":"1.00"}]
["Remove timber door in the disabled bathroom, make good to walls and replace door in new position to accommodate new position of door handle. (D06)","No",{"v":1,"d":"1.00"}]
["Remove damaged door leaf at W02 shopfront ","No",{"v":1,"d":"1.00"}]
["Repair broken apron patch sized approximately 50 x 100mm wide with wood filler and paint with enamel paint","No",{"v":1,"d":"1.00"}]
["Supply and instal glazing and Ironmongergy to D03 door as per door schedule","No",{"v":1,"d":"1.00"}]
["Install 300mm diameter circular glazing to door leafs (Door 04)","No",{"v":2,"d":"2.00"}]
["Skirting",""]
["Make good and touch up exisiting skirting","m",{"v":45,"d":"45.00"}]
["Joinery",""]
["Final preparation and paintwork to Workshop joinery","m²",{"v":37,"d":"37.00"}]
["Ironmongery",""]
["Replace ironmongery for right leaf only on door D01 as per door schedule ","No",{"v":1,"d":"1.00"}]
["Install glazing and Ironmongergy to D23 door as per door schedule","No",{"v":1,"d":"1.00"}]
["Make good to loose door handles","No",{"v":3,"d":"3.00"}]
["Make good to broken door catch(D22)","No",{"v":1,"d":"1.00"}]
["Replace broken striker plate(D22)","No",{"v":1,"d":"1.00"}]
["Repairs to door frames and catch plates where necessary (as per Architects specification)","No",{"v":15,"d":"15.00"}]
["Supply and install pop rivets to fire signage, 4 pop rivets per sign","No",{"v":4,"d":"4.00"}]
["Repair locker door","No",{"v":1,"d":"1.00"}]
["Repair with wood filler, sanded smooth, cleaned and repainted. Paint as per original specification, undercoat for wood plus 2 coats of matt enamel solvent base paint.","No",{"v":15,"d":"15.00"}]
["Inspect, prepare, resolve water leakage and test for water tightness",""]
["Inside Classroom 4","Item",{"v":1,"d":"1.00"}]
["Inside Reading Room","Item",{"v":1,"d":"1.00"}]
["Walkway above FHR","Item",{"v":1,"d":"1.00"}]
["REMEDIAL WORKS TO CEILINGS, PARTITIONS AND ACCESS FLOORING",""]
["Thermal Insulation",""]
["Make tidy ensuring all areas are covered, tie in or cut off all loose ends, clean all and remove all paint and cement, skimming or concrete marks on the foil aluminium insulation.","m²",{"v":220,"d":"220.00"}]
["Suspended Ceilings",""]
["Sand down minor defects, fill and sand smooth if required and clean dirt marks and touch up entire surface with second coat of paint. Note: all visible hangers must be 100% vertical.\n \nIncase panel outstanding or damaged, replace to match existing.","m²",{"v":481,"d":"481.00"}]
["Sand down smooth, fill, clean dirt marks and apply one coat PVA as per Architect's specification to ceilings.","m²",{"v":476,"d":"476.00"}]
["Sand down smooth, fill, clean dirt marks and apply one coat PVA as per Architect's specification to ceilings in patches","m²",{"v":4,"d":"4.00"}]
["Apply one coat of acoustic plaster and one undercoat and two coats of paint (as per original specification).","m²",{"v":236,"d":"236.00"}]
["Making good to gypsum plaster and finish with 3mm to 6mm thick lightwieght plaster","m²",{"v":11,"d":"11.00"}]
["Carefully remove all paint from metal shadow line cornices with turpentine cloth. If needed use small  cutter blade/knife to loosen paint. Take care not to scratch powder coat surface. The white powder coat surface must be the visible surface.","m",{"v":191,"d":"191.00"}]
["Repair large hole sized approximately 250mm x 320mm wide to ceiling and match to existing finish","No",{"v":1,"d":"1.00"}]
["REMEDIAL WORKS TO STRUCTURAL STEELWORK",""]
["Carefully take out/off and set aside for later use, take from store, fix to steel rafter with electro galvanised  M6 CSK bolts and nuts (elsewhere measured) ",""]
["Flat metal plate canopy cladding.","m²",{"v":157,"d":"157.00"}]
["Carefully take out/off  and remove all rejected structural steelwork",""]
["Structural steel various members","Tonnes",{"v":7,"d":"7.00"}]
["Carefully take out/off bolted structural steel members, inspect, remove off site to hot dip galvanise on an approved galvaniser within the 100km radius, return the galvanised structural member to site fix into same postion and bolted with new M12 and M16 ",""]
["Structural steel various members.","Tonnes",{"v":9,"d":"9.00"}]
["Carefully clean all loose and flaking rust, dust and dirt with soft sponge and seal with \"Everbite\" clear matt metal sealant applied strictly as per manufacturer's specifications",""]
["On flat metal plate canopy cladding.","m²",{"v":314,"d":"314.00"}]
["On gate, screens, etc.","m²",{"v":16,"d":"16.00"}]
["Prepare and apply one prime coat of zinc phosphate to DFT of 45 microns, apply coat of micaceous iron oxide to DFT of 40 microns and apply coat of enamel to DFT of 35 microns",""]
["On galvanised structural steelwork","m²",{"v":434,"d":"434.00"}]
["Bolts, washers, nuts, etc",""]
["M16 Grade 8.8 electro galvanised bolts and nuts","Tonnes",{"v":1,"d":"1.00"}]
["M12 Grade 8.8 electro galvanised bolts and nuts","Tonnes",{"v":1,"d":"1.00"}]
["M6 electro galvanised bolts and nuts","Tonnes",{"v":1,"d":"1.00"}]
["Test",""]
["Test thickness of exisiting galvanising  with electromagnetic gauge.","No",{"v":300,"d":"300.00"}]
["REMEDIAL WORKS TO METALWORK",""]
["Galvanized steel cupboards",""]
["Make good to galvanized steel cupboards by removing doors, galvanizing, making good to welded joints, remove welding flakm sand down smooth all doors and frames, finish with undercoat for metal and two coats of semi gloss enamel paint. New escutcheon plat","No",{"v":6,"d":"6.00"}]
["Make good to galvanized steel cupboards by removing doors, galvanizing, making good to welded joints, remove welding flake sand down smooth all doors and frames, finish with undercoat for metal and 2 coats of semi glass enamel paint. New escutcheon plates","No",{"v":3,"d":"3.00"}]
["Doors, windows, shopfronts, etc",""]
["Remove and replace broken glass windows ","m²",{"v":3,"d":"3.00"}]
["Touch up and paint in patches (Shopfront W02)","m²",{"v":2,"d":"2.00"}]
["Paint to internal steel door frames frames not exceeding 300mm wide","m²",{"v":15,"d":"15.00"}]
["Remove and repair silicone around window frame (Shopfront W02)","m",{"v":1,"d":"1.00"}]
["Take out and remove, inspect for damage, repair and place back into position shopfront W02 due to powder coated finish on frame","No",{"v":1,"d":"1.00"}]
["New aluminium door to shopfront W02 replacing damaged door","No",{"v":3,"d":"3.00"}]
["Align door for consistant gap at frame( Classroom 4, Shopfront W02)","No",{"v":1,"d":"1.00"}]
["Replace corroded or damaged window stay","No",{"v":11,"d":"11.00"}]
["Replace broken pane of glass","No",{"v":2,"d":"2.00"}]
["Align Doors(Classroom 3, Shopfront W01)","No",{"v":1,"d":"1.00"}]
["Re-do Threshold  to appropiate height and include expansion joints (Threshold approximately 1000mm wide).","No",{"v":2,"d":"2.00"}]
["Fill holes in shopfronts with steel epoxy for metal, finish smooth and finish with matching colour spray paint","No",{"v":1,"d":"1.00"}]
["Repair door frame with steel epoxy for metal, finish smooth and finish with matching colour spray paint","No",{"v":1,"d":"1.00"}]
["Fasten loose window handle","No",{"v":2,"d":"2.00"}]
["Fasten nuts and touch up paint to nut at shopfront W02","No",{"v":24,"d":"24.00"}]
["Repair with metal epoxy, sand smooth and paint horizontal structural I beams at shop front D08 beams, size 805 x 4060mm long.","No",{"v":3,"d":"3.00"}]
["Service all window stays","No",{"v":84,"d":"84.00"}]
["Replacement of window stays","No",{"v":27,"d":"27.00"}]
["Repair of opening section of Windows","No",{"v":3,"d":"3.00"}]
["Servicing of all window stays and replace where necessary","No",{"v":33,"d":"33.00"}]
["Remove metal plate at top W03 window","No",{"v":1,"d":"1.00"}]
["Replace missing window handle (W10 as per window schedule)","No",{"v":2,"d":"2.00"}]
["Clean joint between gas gate and plaster and fill with polysulpfide filler.","m",{"v":6,"d":"6.00"}]
["Fill gaps around windows, doors and shopfronts inside and outside with dove grey ABE Dowsil 813C silicone, one-part UV resistant oea when meeting grey concrete or plaster and painted walls, Use brown colour (as alreadu used on site) when meeting pigmented","m",{"v":1830,"d":"1830.00"}]
["REMEDIAL WORKS TO TILING",""]
["Removing grouting and sealing in areas condemned by architect to prepare for remedial work and carry out remedial work as follows:",""]
["Grouting all tile wall joints","m²",{"v":54,"d":"54.00"}]
["Grouting all tile floor joints","m²",{"v":235,"d":"235.00"}]
["Minor grouting repair to showers","m²",{"v":3,"d":"3.00"}]
["Grouting to tile and other finish junction","m",{"v":86,"d":"86.00"}]
["Grouting to floor tile and wall junction","m",{"v":9,"d":"9.00"}]
["Reduce excess tiling grout between edge trim and tile","m",{"v":1,"d":"1.00"}]
["Create small V-Joint at wall junction 5mm wide","m",{"v":17,"d":"17.00"}]
["Cut new vertical 5mm wide expansion joint between pigmented concrete wall and window cill","m",{"v":1,"d":"1.00"}]
["Colour tile grout to recess at metal edge of concrete vanity slab recessed y 5mm","m",{"v":9,"d":"9.00"}]
["Colour tile grout to gap between metal edge trim and concrete vanity slab not exceeeding 300mm wide","m",{"v":9,"d":"9.00"}]
["Fill gap between metal and concrete at vanity with concrete not exceeding 300mm wide","m",{"v":9,"d":"9.00"}]
["Remove and entirely replace with new continuous new strip similar to what is installed.","m",{"v":69,"d":"69.00"}]
["Recess wall by 2mm from metal dividing strip and skim with pigmented colour skimming product and seal with clear matt sealant","m²",{"v":30,"d":"30.00"}]
["Seal junction between wall tiles and floor tiles","m",{"v":18,"d":"18.00"}]
["REMEDIAL WORKS TO PLUMBING AND DRAINAGE",""]
["20mm Diameter Blue PVC spouts(not exceeding 300mm in length) incorrectly positioned in planter boxers and concrete slabs for drainage spouts and make good to concrete (making good elsewhere measured)","m",{"v":37,"d":"37.00"}]
["115mm diameter uPVC pipes embedded in external concrete screed, 2 lengths in screed","m",{"v":2,"d":"2.00"}]
["200mm diameter pipe embedded in screed and make good to area.","m",{"v":125,"d":"125.00"}]
["Supply and install porcelain wash hand basin as per specification to disabled toilet","No",{"v":1,"d":"1.00"}]
["Supply and install shower trap as per architects specification","No",{"v":1,"d":"1.00"}]
["Supply and install flush push buttons to urinals","No",{"v":6,"d":"6.00"}]
["Supply and install shower rose as per architects specification","No",{"v":1,"d":"1.00"}]
["Supply and install toilet roll holder","No",{"v":1,"d":"1.00"}]
["Supply and install mirrors in bathrooms as per architect specification","No",{"v":2,"d":"2.00"}]
["Repair leakage at underside of urinal","No",{"v":1,"d":"1.00"}]
["Complete plumbing connections for water supply including taps and connections for sink, plumbing drainage pipes etc as dircted by architect drawings and specification","No",{"v":2,"d":"2.00"}]
["Testing of all water fittings and reticulation","Item",{"v":1,"d":"1.00"}]
["HOLE, ETC",""]
["Core drilling hole not exceeding 50mm diameter",""]
["256mm Thick reinforced slab, beam, wall, etc","No",{"v":11,"d":"11.00"}]
["REMEDIAL WORKS TO  ELECTRICAL  WORKS, MECHANICAL WORKS, ETC",""]
["Electrical works",""]
["Remove redundant pvc conduits and make good to surface","m",{"v":57,"d":"57.00"}]
["Temporary removal of all lightening protection, storage thereof and re-installation after terylene plaster is installed.","m",{"v":16,"d":"16.00"}]
["Seal with white silicone around electrical trunking going through white wall tile","m",{"v":3,"d":"3.00"}]
["Remove mesh cable tray to access to untiled wall section behind at top of west facing wall including reinstatement (tiling eslewhere measured)","m",{"v":6,"d":"6.00"}]
["Remove reticulation piping and insulation to access to untiled wall section behind at top of west facing wall including reinstatement (tiling eslewhere measured)","m",{"v":12,"d":"12.00"}]
["Remove light fittings and sensors on concrete ceiling and reinstate after repair work to concrete ceiling(repair work elsewhere measured)","No",{"v":29,"d":"29.00"}]
["Remove and reinstallation lightnening protection for repair of concrete skimming","m",{"v":20,"d":"20.00"}]
["Sand down corroded fire hydrant connection and paint as per Architect and Mechanical engineer specification.","No",{"v":1,"d":"1.00"}]
["Remove all exterior light fittings and re-installation after wall finish is complete.","No",{"v":43,"d":"43.00"}]
["Coldroom",""]
["Breakdown and remove 110mm Brick wall encasing  front façade of coldroom taking care not to damage wall & floor tiles beyond that area","m²",{"v":5,"d":"5.00"}]
["Seal around coldroom doors at tile and coldroom junction.","m",{"v":15,"d":"15.00"}]
["Disconnect connections to the coldroom and move to give access to floor and walls for tiling (tiling elsewhere measure) and return to position and reinstate connections ","Item",{"v":1,"d":"1.00"}]
["RMEDIAL WORKS TO EXTERNAL WORKS",""]
["Walkways & Ramps",""]
["Scarify Concrete walkway and ramps to a suitable height of 30mm for wheelchair access as directed by engineer/architect drawings and add suitable adhesive and concrete topping to ensure suitable height of 30mm is achieved.","m²",{"v":93,"d":"93.00"}]
["Replace cracked exposed aggregate panel paving","m²",{"v":21,"d":"21.00"}]
["Cut new 5mm wide expansion joint on exposed aggregate paving as per landscape architect report","m",{"v":3,"d":"3.00"}]
["Replace missing precast type D7 concrete stormwater channel panel","m",{"v":1,"d":"1.00"}]
["Rake out cracked mortar joint between precast storm water channels, channels 550mm wide","Item",{"v":1,"d":"1.00"}]
["Timber screens",""]
["Remove all poles, sand bottom, top and edge where saw cut to remove rough edges with 100 grit sandpaper. Remove all splinteres visible, and lose remainders of bark. Rub matt clear silicone into top surface of pole to prevent water ingress(NB not to be vis","No",{"v":177,"d":"177.00"}]
["Install outstanding pole into brackets, clean brackets prior. Poles 150mm diameter X 2860mm long","No",{"v":24,"d":"24.00"}]
["MAKING GOOD OF FINISHES ETC",""]
["Make good to concrete copings, benches, in-situ edges, stormwater channels; etc",""]
["Make good to in-situ cast concrete slab as per specification","m²",{"v":21,"d":"21.00"}]
["Make good to concrete slab ceiling after removing shutterboard (work required to be determined once shutterboard is removed)","m²",{"v":203,"d":"203.00"}]
["Make good concrete soffit roof slab at bench","m²",{"v":19,"d":"19.00"}]
["Make good to concrete benches including repairing chip marks, cleaning and sealing concete bench with applicable sealant .","m²",{"v":154,"d":"154.00"}]
["Make good to concrete surface beds including repairing chip marks, cleaning and sealing concete surface bed with applicable sealant (As per Architects and engineers specification see drawing REC/1005 to 1006)","m²",{"v":132,"d":"132.00"}]
["Make good to skimmed concrete wall below vanity slab behind apron","m²",{"v":3,"d":"3.00"}]
["Make good to concrete wall and floor connections.","m",{"v":20,"d":"20.00"}]
["Make good to skimmed concrete wall ","m²",{"v":56,"d":"56.00"}]
["Make good concrete soffit roof slab at planter box","m²",{"v":18,"d":"18.00"}]
["Make good soffit of copings at parapet wall ne 300mm wide","m",{"v":11,"d":"11.00"}]
["Make good 5mm expansion joint where concrete wall meets new wall","m",{"v":13,"d":"13.00"}]
["Make good to storm water channels","m",{"v":21,"d":"21.00"}]
["CLEANING TO EXISTING COMPLETED WORK",""]
["Cleaning to floors",""]
["Clean floor of excess cement, paint and seal concrete screed","m²",{"v":67,"d":"67.00"}]
["Remove and clean all building residue on screeded floors as per the architect's specification","m²",{"v":104,"d":"104.00"}]
["Clean and apply sealant to screeded floors","m²",{"v":24,"d":"24.00"}]
["Clean all tiled floors including metal edge strips","m²",{"v":383,"d":"383.00"}]
["Clean office carpet tiles not yet installed","m²",{"v":55,"d":"55.00"}]
["Clean and seal screeded floors including corners where screed meets wall.","m²",{"v":247,"d":"247.00"}]
["Remove plaster and paint and clean all concrete floors","m²",{"v":7,"d":"7.00"}]
["Clean all tiled walls includihng tile edge strips","m²",{"v":526,"d":"526.00"}]
["Clean tile grouting","m",{"v":16,"d":"16.00"}]
["Cleaning to walls",""]
["Clean grout on wall tiles including minor grout jointed not worked off","m²",{"v":36,"d":"36.00"}]
["Clean all internal skimmed concrete walls especially in corners, door frame and where walls meet floor and allow for minor repair works as directed by architect and prepare to receive one coat of clear matt sealant","m²",{"v":36,"d":"36.00"}]
["Clean out cement between concrete seat and stone wall cladding ","m",{"v":126,"d":"126.00"}]
["Clean out drip on under side of cills and external walls and seal cills with UV Resitant light grey silicone sealant around all aluminium frames between walls and window frames and Cills and window frames","m",{"v":111,"d":"111.00"}]
["Clean cement and paint off wall tiles","m²",{"v":13,"d":"13.00"}]
["Clean partitions from dust and marks","m²",{"v":72,"d":"72.00"}]
["Remove tape and clean from partition legs 150mm long","No",{"v":8,"d":"8.00"}]
["Cleaning to ceilings",""]
["Clean metal roof sheet flashing at IBR roof sheeting","m²",{"v":8,"d":"8.00"}]
["Clean all metal roof including metal flashings by removing plaster and paint marks and testing for water tightness.","m²",{"v":192,"d":"192.00"}]
["Remove terylene plaster and paint on metal roof","m²",{"v":18,"d":"18.00"}]
["Remove cement, paint and plaster from roof insulation","m²",{"v":14,"d":"14.00"}]
["Clean corner of ceilings including sanding down and touch ups","m",{"v":30,"d":"30.00"}]
["Clean concrete ceilings including corners","m²",{"v":7,"d":"7.00"}]
["Clean marks on concrete slab ceiling","m²",{"v":61,"d":"61.00"}]
["Carefully clean and remove all paint from metal shadow line cornices with turpentine. ","m",{"v":867,"d":"867.00"}]
["Cleaning to metalwork",""]
["Cleaning of glass and frames inside and outside, including inside reveals of frames, and opening sections, and tracks in case of stack doors . Blow out dust dirt from inside of frames with electric blower, and clean glass and aluminium thoroughly with non","m²",{"v":1592,"d":"1592.00"}]
["Clean aluminium frames to doors, windows and shop fronts n e 300mm wide","m",{"v":640,"d":"640.00"}]
["Clean all loose and flaking rust, dust and dirt from structural steel panels top and bottom with sponge without making scratches","m²",{"v":572,"d":"572.00"}]
["Clean aluminium window, remove plastic around window frame including cement joint and replace with expandable polysulphide joint filler including covering the entire strip with a luminium flat continiuos section (min 20x3mm) powder coated the same as wind","m",{"v":28,"d":"28.00"}]
["Clean all aluminium Windows","m²",{"v":83,"d":"83.00"}]
["Clean aluminium frames to doors, windows and shop fronts exceeding 300mm wide including glazing","m²",{"v":562,"d":"562.00"}]
["Scrape off Terylene skimming off window sills","m²",{"v":4,"d":"4.00"}]
["Clean window sill from paint","m²",{"v":2,"d":"2.00"}]
["Clean window sill sized 230x380mm wide","No",{"v":1,"d":"1.00"}]
["Clean all cement on floor channel gril and support frame","m²",{"v":4,"d":"4.00"}]
["Clean and make good steel signage at front 250mm wide x 5000mm high","m",{"v":1,"d":"1.00"}]
["Clean excess grout off reticulation and mesh tray on west facing walling kitchen","m",{"v":5,"d":"5.00"}]
["Clean markings on walls, floors and ceilings of cold rooms","m²",{"v":28,"d":"28.00"}]
["Clean steel support brackets to vanity slab and finish with clear matt sealant to prevent corrosion not exceeding 300mm wide","m",{"v":11,"d":"11.00"}]
["Clean metal dividing strip from dirt, paint and cement","m",{"v":15,"d":"15.00"}]
["Clean metal edge around 4 x 40mm mild steel flat bar bend forming diving strip sawn joints.","m",{"v":154,"d":"154.00"}]
["Clean metal edge strip on tiled floors","m",{"v":61,"d":"61.00"}]
["Aluminium carpet edge strip in anodized aluminium between carpet and stainless steel plate","m",{"v":82,"d":"82.00"}]
["4mm thick solid rubber packing cut sheet to fit width 75mm width applied to cement screed using contact adhesive","m",{"v":82,"d":"82.00"}]
["Clean metal edge of vanity slab and apply matt sealant not exceeding 300mm wide","m",{"v":9,"d":"9.00"}]
["Clean tiling aluminium edge trim of paint and grout ","m",{"v":27,"d":"27.00"}]
["Clean sheet metal flashing 400mm wide","m",{"v":18,"d":"18.00"}]
["Steel cabin hook from external wall, clean and store to be fixed in same position on wall","No",{"v":15,"d":"15.00"}]
["Clean all cabin hooks","No",{"v":45,"d":"45.00"}]
["Remove all paint on hinges, remove hinges and sand down the end of hinge and reinstall hinges in same position","No",{"v":30,"d":"30.00"}]
["Clean all steel bed frames","No",{"v":15,"d":"15.00"}]
["Clean all metal steel louvres","No",{"v":6,"d":"6.00"}]
["Markings on all joinery fittings (see joinery drawings)","No",{"v":2,"d":"2.00"}]
["Cleaning to plumbing",""]
["Clean 20mm diameter copper pipes","m",{"v":11,"d":"11.00"}]
["Carefully remove incorrect shower trap and install shower trap as per architects specification","No",{"v":1,"d":"1.00"}]
["Clean 100mm diameter PVC pipes","m",{"v":5,"d":"5.00"}]
["Clean 50mm diameter PVC pipes","m",{"v":8,"d":"8.00"}]
["Clean 110mm Diameter PVC waste pipes at duct","m",{"v":2,"d":"2.00"}]
["Clean 30mm Diameter copper pipe at FHR","m",{"v":2,"d":"2.00"}]
["Clean 50mm Diameter PVC waste pipes at duct","m",{"v":4,"d":"4.00"}]
["Clean all external concrete walls and apply matt sealant","m²",{"v":105,"d":"105.00"}]
["Clean all external service pipes (PVC, Copper Water suply etc)","No",{"v":2,"d":"2.00"}]
["Powder coated aluminium weather bar to gap at W06 window(Slab window frame Junction).","m",{"v":4,"d":"4.00"}]
["Remove skimming off storm water channels","m²",{"v":21,"d":"21.00"}]
["Aluminium edge trim around tiling at coldroom entrance","m",{"v":22,"d":"22.00"}]
["Clean and make neat along type D7 concrete stormwater channel panel","m",{"v":16,"d":"16.00"}]
["Aluminium cover strip to close gap between coldroom and wall (approximately 30 to 60mm wide)","m",{"v":6,"d":"6.00"}]
["Remove stickers from water closets","No",{"v":4,"d":"4.00"}]
["Aluminium drip 80mm from edge of concrete","m",{"v":86,"d":"86.00"}]
["Clean concrete vanity slab and apply matt sealant","m²",{"v":11,"d":"11.00"}]
["Clean, sand and remove all foreign materials (nails, malthoid visible, shutter pieces etc)  from underside of concrete slab","m²",{"v":66,"d":"66.00"}]
["Powder coated aluminium U-Plate fixed to wooden packing screwed underneath to metal cover size 205mmx 20mm","m",{"v":31,"d":"31.00"}]
["PLUMBING AND DRAINAGE",""]
["Clean concrete bench, allow for minimum 5 chip marks to be repaired and apply matt sealant","No",{"v":1,"d":"1.00"}]
["HOLES,ETC",""]
["Remove plaster and paint and clean on all toilet fittings","No",{"v":2,"d":"2.00"}]
["Remove plaster and paint and clean all concrete shelves","m²",{"v":14,"d":"14.00"}]
["Core drilling hole not exceeding 50mm diameter",""]
["100mm Thick concrete slabs, walls, etc.","No",{"v":38,"d":"38.00"}]
[" 220mm Thick concrete slab for galvanised spouts ","No",{"v":8,"d":"8.00"}]
[" 410mm Thick concrete slab, wall, etc","No",{"v":3,"d":"3.00"}]
["Clean galvanised steel electrical ducting ne 300mm wide","m",{"v":10,"d":"10.00"}]
["Clean galvanised steel electrical ducting n e 300mm wide","m",{"v":5,"d":"5.00"}]
["Clean surface mounted electrical conduits","m",{"v":14,"d":"14.00"}]
["Clean all external light fittings including removing of plaster and paint","No",{"v":2,"d":"2.00"}]
["Core drilling hole exceeding 50mm not exceeding 100mm diameter",""]
["Remove all pebbles and clean out soil in stormwater channel sized 150mm wide x 310mm deep x 39 000mm long","Item",{"v":2,"d":"2.00"}]
["100mm Thick concrete slab, wall, etc ","No",{"v":12,"d":"12.00"}]
["270mm Think concrete slab for galvanised spouts as per detail","No",{"v":6,"d":"6.00"}]
["Cleaning of 40mm Pebble trench","m²",{"v":14,"d":"14.00"}]
["TESTING OF EXISTING WORKS",""]
["Testing of existing works",""]
["Allow for testing of aluminium window stays and where replacement necessary elsewhere measured.","No",{"v":72,"d":"72.00"}]
["Flat concrete roofs ",""]
["Carefully lift up chipped stone and malthoid, set aside to be later placed on the same area,  clean and inspect (inspection elsewhere measured) and place back the chipped stone and malthoid as per manufacturer's instruction to roof slabs.","m²",{"v":2450,"d":"2450.00"}]
["Allow for inspection of minimum 6 sqm of waterproofing, falls and water disposal at outlets on toilet block sod roof, waterproofing to be removed and falls to be rectified on sod roof if water disposal test is failed.","m²",{"v":6,"d":"6.00"}]
["Allow for inspection of area sized 3000mm long x 360mm wide x 900mm deep for presence of screed with fall and waterproofing","Item",{"v":1,"d":"1.00"}]
["Allow for inspection of roof for leakage and repair","Item",{"v":1,"d":"1.00"}]
["Allow for inspection of minimum 2 sqm of waterproofing, falls and water disposal to each isolated roof sections, waterproofing to be removed and falls to be rectified on sod roof if water disposal test is failed","m²",{"v":2,"d":"2.00"}]
["Removal of works for inspection",""]
["Allow for removal of minimum 2 sqm of chipped stone, surface to be cleaned, for inspection (inspection elsewhere measured) at each isolated roof section.","m²",{"v":2,"d":"2.00"}]
["Allow for removal of minimum 6 sqm of soil, surface to be cleaned, for inspection(inspection elsewhere measured) at outlets on toilet block sod roof.","m²",{"v":6,"d":"6.00"}]
["Allow for removal of waterproofing and rectificaton of falls on entire sod roof if water disposal test failed including clearing of entire toilet block sod roof of soil, carting away, storage and reinstatement after completion of works","Item",{"v":1,"d":"1.00"}]
["Allow for clearing of entire toilet block sod roof of chipped stone, carting away, storage and reinstatement after completion of rectification works to waterproofing and falls on sod roof if water disposal test failed","Item",{"v":1,"d":"1.00"}]
["Remove soil volume sized 3000mm long x 360mm wide x 900mm deep to inspect presence of screed with fall and waterproofing(inspection elsewhere measured)","Item",{"v":1,"d":"1.00"}]
["BUILDING UP OPENINGS",""]
["Brickwork in stock bricks in building up openings",""]
["Half brick wall partially incasing front of coldroom store","m²",{"v":2,"d":"2.00"}]
["Half brick wall building up fire hose reel","m²",{"v":2,"d":"2.00"}]
["NEW WORK CHIEFLY INSIDE EXISTING BUILDING(S)",""]
["User note\n\nNew work chiefly inside existing building(s) shall be given in accordance with the principles laid down in the relevant trades",""]
["EARTHWORKS",""]
["EXCAVATIONS, ETC",""]
["Excavation in earth",""]
[" \nExcavation in earth not exceeding 2m deep to expose foundations (Provisional) \n \n ","m³",{"v":95,"d":"95.00"}]
[" \nExcavation in earth not exceeding 2m deep (Provisional) \n \n ","m³",{"v":9,"d":"9.00"}]
["Sand blinding layer to bottoms of trenches","m³",{"v":1,"d":"1.00"}]
["25MPa/19mm stone reinforced concrete to planter walls","m³",{"v":5,"d":"5.00"}]
["Smooth formwork to sides of concrete walls not exceeding 1.5m high","m²",{"v":48,"d":"48.00"}]
["Form 20mm chamfer edges too corners of walls","m",{"v":34,"d":"34.00"}]
["10mm expansion joint to receive 10mm backing cord and sealing with 10x10mm deep Sikaflex 11FC+ polyutherane joint sealant","m",{"v":13,"d":"13.00"}]
["PRECAST CONCRETE",""]
["PRECAST CONCRETE COPINGS, ETC",""]
["Precast concrete finished smooth on exposed surfaces including bedding, jointing and pointing",""]
["Modcon Type 14 precast concrete coping.","m",{"v":393,"d":"393.00"}]
["Ditto, but on radius not exceeding 5m.","m",{"v":57,"d":"57.00"}]
["Modcon Type 20 precast concrete coping.","m",{"v":250,"d":"250.00"}]
["Ditto, but on radius not exceeding 5m","m",{"v":104,"d":"104.00"}]
["MASONRY",""]
["NATURAL STONEWORK",""]
["Natural stone walls of uncoursed random local stone to the principal agents approval",""]
["Stone cladding and remove excess cement, fill small apertures where no stones including removal of galvanised hoop irons.","m²",{"v":36,"d":"36.00"}]
["WATERPROOFING",""]
["WATERPROOFING ON BASEMENT",""]
["One layer 4mm special polyester fully bonded waterproof membrane comprising a matrix modified with polypropylene dual reinforced with non-woven polyester cloth and glass fibre tissue, laid with 75mm side and 100mm end laps",""]
["Top end of waterproofing to form a straight horizontal line on inside of planter box","m",{"v":55,"d":"55.00"}]
["WATERPROOFING ON ROOFS",""]
["Take out and remove malthoid protection layer including primer and waterproof membrane  ",""]
["On concrete flat roofs","m²",{"v":2416,"d":"2416.00"}]
["In turn ups and turn downs","m²",{"v":438,"d":"438.00"}]
["Ditto but circular on plan","m²",{"v":48,"d":"48.00"}]
["On turn ups and turn downs not exceeding 300mm girth","m",{"v":1128,"d":"1128.00"}]
["Take out and remove any other waterproofing membrane ",""]
["On concrete flat roofs","m²",{"v":2464,"d":"2464.00"}]
["Take out and remove 10-15mm diameter chipped aggregate in light coloured shades of brown stone dressing evenly spread with larger stones around outlets",""]
["50mm thick on waterproofing to flat roofs","m²",{"v":2464,"d":"2464.00"}]
["Prepare and apply two coats of TFC or equally approved clear matt cement sealant to Architect's acceptance",""]
["On parapet walls.","m²",{"v":366,"d":"366.00"}]
["On top and sides of precast concrete coping","m²",{"v":149,"d":"149.00"}]
["Three coats a.b.e laykold or equally approved rubberised bitumen emulsion",""]
["On lining not exceeding 300mm","m",{"v":1,"d":"1.00"}]
["Provide guaranteed on roofs upon completion of the waterproofing","Item",{"v":1,"d":"1.00"}]
["CEILING, PARTITION AND ACCESS FLOORING",""]
["SUSPENDED CEILINGS",""]
["9mm Gypsum plasterboard on screw-up tee suspension grid including hangers etc, with tape fixed over joints and the whole finished with gypsum plaster trowelled to a smooth polished surface",""]
["9mm Thick plasterboard fixed to existing galvanised suspended ceiling grid syestem plastered with 3mm thick gypsum plaster as manufacturer's specification and PVA applied as per manufacturer's specifications.","m²",{"v":517,"d":"517.00"}]
["132mm Bulkhead of  9mm thick plasterboard fixed to existing galvanised suspended ceiling grid system plastered with 3mm thick gypsum plaster as manufacturer's specification and one coat PVA applied as per manufacturer's specifications.","m",{"v":128,"d":"128.00"}]
["150mm Bulkhead of  9mm thick plasterboard fixed to existing galvanised suspended ceiling grid system plastered with 3mm thick gypsum plaster as manufacturer's specification and one coat PVA applied as per manufacturer's specifications.","m",{"v":132,"d":"132.00"}]
["425mm Bulkhead of  9mm thick plasterboard fixed to existing galvanised suspended ceiling grid system plastered with 3mm thick gypsum plaster as manufacturer's specification and one coat PVA applied as per manufacturer's specifications.","m",{"v":11,"d":"11.00"}]
["1090mm Bulkhead of  9mm thick plasterboard fixed to existing galvanised suspended ceiling grid system plastered with 3mm thick gypsum plaster as manufacturer's specification and one coat PVA applied as per manufacturer's specifications.","m",{"v":12,"d":"12.00"}]
["IRONMONGERY",""]
["HINGES, BOLTS, ETC",""]
["Thumb turn to door with indicator bolt as per specification","No",{"v":5,"d":"5.00"}]
["Indicator bolts on partition doors in toilets as per architects specification.","No",{"v":3,"d":"3.00"}]
["CATCHES, CABIN HOOKS, ETC",""]
["Cabin hook to wall","No",{"v":15,"d":"15.00"}]
["LOCKS",""]
["Latches fitted to D01 as per door schedule","No",{"v":7,"d":"7.00"}]
["Remove incorrect latches fitted to D01 as per door schedule","No",{"v":7,"d":"7.00"}]
["Door lock for Male Toilets","No",{"v":3,"d":"3.00"}]
["Sliding lock with catchplates on all doors where necessary (Architects specification)","No",{"v":15,"d":"15.00"}]
["Sliding hatch on all doors ( as per Architects specification)","No",{"v":15,"d":"15.00"}]
["HANDLES",""]
["Anodised aluminium handle","No",{"v":3,"d":"3.00"}]
["Handle and latch on all top lights ","No",{"v":15,"d":"15.00"}]
["Remove corroded steel door handle to aluminum door at male staff toilets","No",{"v":3,"d":"3.00"}]
["STRUCTURAL STEELWORK",""]
["GALVANISED COLUMNS, BEAMS, PURLINS, GIRTHS, ETC",""]
["Welded and bolted  trusses, beams, columns. Purlins, giths, etc :",""]
["Structural steelwork various members ","Tonnes",{"v":13,"d":"13.00"}]
["Beams",""]
["Galvanized I-Beams in roofing structure","Tonnes",{"v":10,"d":"10.00"}]
["GALVANISED MILD STEEL PLATE",""]
["2mm Mild steel plate with Corten steel finish with 60mm return flange to stiffen the plate and protected with a one coat of Everbrite clear protection coat as per manufacturer's instructions","Kg",{"v":31,"d":"31.00"}]
["GALVANISED MILD STEEL PIPE",""]
["Steel tube 150mm long, cut away  in front to form spout with a 4 x 90mm diameter steel flange two times holed and epoxy fixed into wall with  6mm solid round pin (No. 2) ",""]
["2.5 x 38mm (Spigot No.3)","No",{"v":3,"d":"3.00"}]
["PAINT TO STRUCTURAL STEELWORK",""]
["Prepare and apply one prime coat of zinc phosphate to DFT of 45 microns, apply coat of micaceous iron oxide to DFT of 40 microns and apply coat of enamel to DFT of 35 microns:",""]
["METALWORK",""]
["Allow for inspection of stackaway doors for ease of opening and undertake repairs to these doors where required","Prov Sum",{"v":1,"d":"1.00"}]
["Allow for foam filling and aluminium coper strips to align windows where gaps exist between windows or doors and walls ","Prov Sum",{"v":1,"d":"1.00"}]
["ALUMINIUM LOUVRE UNITS ",""]
["Install aluminium fixed louvre size 585 x 350 mm high with 20mm framed door grille complete with telescopic back frame manufactured of extruded type 50 S anodising grade aluminium with fixed horizontal chevron louvres with blade spacing 19mm, as per detai","No",{"v":4,"d":"4.00"}]
["PLASTERING",""]
["EXTERNAL PLASTERING",""]
["Terylene plaster of an intermediate texture according to SANS 2001-construction works part EM1, including bonding liquid mixed in and plaster applied with Terylene machine. Cement mixture of one part cement and half parts of course sand with water for a s",""]
["Sample on walls for fine texture","m²",{"v":20,"d":"20.00"}]
["Sample on walls for medium texture","m²",{"v":20,"d":"20.00"}]
["Sample on walls for course texture","m²",{"v":20,"d":"20.00"}]
["On walls.","m²",{"v":5189,"d":"5189.00"}]
["Apply Marmoran perma plast light grey to previously terylene plastered walls after walls have been thoroughly cleaned","m²",{"v":5189,"d":"5189.00"}]
["TILING",""]
["WALL TILING",""]
["200 x 200 x 5mm White matt ceramic tiles on brickwork including cement plaster backing",""]
["On walls","m²",{"v":49,"d":"49.00"}]
["Mosaic tiles to match existing on brickwork including cement plaster backing",""]
["On walls","m²",{"v":176,"d":"176.00"}]
["FLOOR TILING",""]
["Porcelain floor tiles fixed with adhesive to screed (screed elsewhere) and flush pointed with tinted  grout",""]
["On floors ","m²",{"v":10,"d":"10.00"}]
["Aluminium edge strip from mosaic tile work to be replaced by a deeper size strip","m",{"v":156,"d":"156.00"}]
["SUNDRIES",""]
["Aluminium corner protectors, stair nosings, expansion joint strips, etc",""]
["Powder coated aluminium weather bar to gap at bottom of door on inside and outside(to stop 6mm above finished floor level)","m",{"v":4,"d":"4.00"}]
["ALLOWANCE FOR UNQUANTIFIED REMEDIAL WORK TO AREAS TO BE LATER DETERMINED",""]
["The following work to existing tyrelene finish walls",""]
["Hack off and remove terylene plaster from plastered walls, rinse off surfaces with low pressure wash off and prepare surfaces for new finish","m²",{"v":10,"d":"10.00"}]
["Cut open crack to wall, patch and fill with latex modified repair modified to be approved by architect","m²",{"v":10,"d":"10.00"}]
["Apply terylene plaster of an intermediate nature accoring to SANS 2001 - onstruction works part EM1 including bonding liquid to be approved by architect mixed in plaster applied with terylene machine to bare areas","m²",{"v":10,"d":"10.00"}]
["Apply high performance all seasons paint to cover areas using airless spray or equally approved ","m²",{"v":10,"d":"10.00"}]
["Wash, and apply one coat AR sealer , two coats Fibreseal to tops and two coats of Neuklad or equally approved paint to capping","m²",{"v":10,"d":"10.00"}]
["Prime and seal with Sikaflex construction including backing cord where necessary ","m",{"v":1,"d":"1.00"}]
["The following work to existing concrete walls",""]
["High pressure wash to tops of concrete walls, removing any residue","m²",{"v":10,"d":"10.00"}]
["Skimming of walls using ABE skim coat to a maximum of two layers","m²",{"v":10,"d":"10.00"}]
["Cut open damaged areas and prepare to join wth repaired area to wall, patch and fill with latex modified repair modified to be approved by architect","m²",{"v":10,"d":"10.00"}]
["Clean out around existing reveals to a gap of maximum 10mm, prime and seal with Sikaflex construction or equally approved including backing chord where necessary","m",{"v":1,"d":"1.00"}]
["Apply one coat AR sealer , two coats Fibreseal to tops and two coats of Neuklad or equally approved paint to capping","m²",{"v":10,"d":"10.00"}]
["Prime and seal with Sikaflex construction including backing cord where necessary","m",{"v":1,"d":"1.00"}]
["The following work to existing galvanised steel",""]
["High pressure wash to galvanised steel, removing any residue, apply degrease and rust remover. Wash down after 1-3 hours with water. Allow to dry completely before applying any finish","m²",{"v":2,"d":"2.00"}]
["Apply one coat Intergard 269 Red, two coats Intergard 201 Surf Grey and three coats Interthane 990 grey paint all in accordance with manufacturer's instructions","m²",{"v":2,"d":"2.00"}]
["The following work to mild steel",""]
["High pressure wash to mild steel, removing any residue, apply degrease spot blast SA 2 or mechaical prep ST2 with feather edges. Clean and allow to dry completely ","m²",{"v":2,"d":"2.00"}]
["Apply one coat Intergard 269 Red, two coats Intergard 201 Surf Grey and three coats Interthane 990 grey paint all in accordance with manufacturer's instructions","m²",{"v":2,"d":"2.00"}]
["ALLOWANCE FOR MISCELLANEOUS UNQUANTIFIABLE REMEDIAL WORK ",""]
["Allow the sum of  R 2 000 000.00 (Two Million Rand) for sundry repairs and renovations, addition discovery work and further deterioration of existing work to be measured and valued in terms of these Bills of Quantities","Item",{"v":1,"d":"1.00"}]

{"sheet":"Sect 3","index":2,"n_rows":1567,"n_cols":5,"rows_kept":1567}
["Description","Uom","Quantity","Rate","Amount"]
["SUPPLEMENTARY PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["NOTE: Contractor to refer to the TOPSOIL (ECO-1) Item C17 Of the preliminaries section for the protection and preservation of the ecological integrity of the topsoil.  Contractor to seek advice from Landscape Architect in terms of topsoil management. Salv",""]
["All earthworks to be in accordance with SANS 1200 D",""]
["Density tests:",""]
["Density tests measured below are those specifically instructed by the engineer to be taken on filling material. All control tests to ensure layerworks are compacted to the required density are to be allowed for by the contractor in scheduled rates",""]
["BULK EXCAVATION",""]
["Open face excavation in earth over sloping site:",""]
["Reduce levels under floors, steps, pavings, etc. (Labour Intensive Construction)","m³",{"v":5,"d":"5.00"}]
["EXCAVATION, FILLING, ETC OTHER THAN BULK",""]
["Excavation in earth not exceeding 2000mm deep",""]
["Holes","m³",0.22]
["CARTING AWAY",""]
["Extra over all excavations for loading, carting and dumping surplus excavated material (no allowance made for increase in bulk):",""]
["In spoil heaps where directed on site (Labour Intensive Construction)","m³",{"v":7,"d":"7.00"}]
["Off site to a dumping site to be found by the Contractor (Labour Intensive Construction)","m³",{"v":4,"d":"4.00"}]
["COMPACTION",""]
["Compaction of Surfaces:",""]
["Trim and level off surface of G5 filled surfaces to receive concrete surface beds, including ripping and scarifying as necessary and compacting the whole area for a depth of 200mm to a density of at least 95% Mod. AASHTO maximum density (Labour Intensive ","m²",{"v":53,"d":"53.00"}]
["PROTECTIVE DRAINAGE SYSTEM",""]
["Protective drainage system :",""]
["100mm Crushed stone laid on and including geotextile non-woven needle punched polypropylene fabric on compacted fill","m²",{"v":33,"d":"33.00"}]
["50mm River pebble laid on and including geotextile non-woven needle punched polypropylene fabric on concrete surface","m²",{"v":1,"d":"1.00"}]
["100mm River pebble laid on and including geotextile non-woven needle punched polypropylene fabric on concrete surface","m²",{"v":1,"d":"1.00"}]
["DECORATIVE STONE FLOORING",""]
["River Pebbles :",""]
["100mm Thick river pebbles in recess formed in concrete surface","m²",{"v":6,"d":"6.00"}]
["100mm Thick river pebbles in recess formed in concrete surface laid circular on plan","m²",{"v":2,"d":"2.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["NOTE: Contractor to refer to the TOPSOIL (ECO-1) Item C17 Of the preliminaries section for the protection and preservation of the ecological integrity of the topsoil.  Contractor to seek advice from Landscape Architect in terms of topsoil management. Salv",""]
["Formwork",""]
["Formwork to sides of bases, pile caps, ground beams, etc. will only be measured where it is prescribed by the engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shal",""]
["Descriptions of formwork shall be deemed to include use and waste only (except where described as 'left in' or 'permanent'), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy r",""]
["LIABILITY",""]
["(a) The contractor shall indemnify the employer against all claims arising from allegations of nuisance caused to other persons and damage caused to other structures\n(b) Notwithstanding any other period named in the contract as the period of maintenance, ",""]
["GUARANTEE",""]
["Guarantee:",""]
["Notwithstanding any other indemnity or insurance that the contractor is required to provide in terms of the contract, and unless otherwise specified, the contractor shall provide a written guarantee, underwritten by an approved insurance company, to bear ",""]
["Provision of the specified piling guarantee and insurance","Item",{"v":1,"d":"1.00"}]
["TESTING",""]
["Transport and establishment of plant for testing:",""]
["Transporting and establishment on site of necessary plant for the testing of piles and removal of thereof on completion","Item",{"v":1,"d":"1.00"}]
["Concrete testing of piles:",""]
["Exposing 500mm diameter pile for inspection including excavation 2m deep in pickable material and backfilling","No",{"v":4,"d":"4.00"}]
["Allow for testing 500mm diameter pile to a max load of 700kN","No",{"v":4,"d":"4.00"}]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["PREAMBLES",""]
["SUPPLEMENTARY PREAMBLES",""]
["Concrete:",""]
["Concrete, formwork and reinforcement to be in accordance with SANS 1200 G",""]
["All cement to comply with the requirements of SANS 50197-1. Use CEM1 42.5",""]
["The costs of making, storing and testing of concrete test cubes as required under clause 7 'Tests' of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the p",""]
["For exposed concrete, and concrete on or below ground, the total alkali content (i.e., the product of the Na20-equivalent of the cement and the cement content of the concrete) must be limited to a maximum of 2.1kg/m3 of concrete, if such concrete is made ",""]
["NOTE: Pigment off-shutter concrete walls  \na) Pigment material must be suitable to colour concrete and not affect the strength and durability of the concrete.\nb) The colouring agent used shall be a single component, pigmented admixture of approximately 2-",""]
["*Pigmented off shutter concrete wall placed in layers not less than 400mm thick.  *Allow for a minimum 4 pigment colours, and pigment material must not affect the strength or durability concrete",""]
["Sample Panels: \n*The contractor shall prepare sample panels and shall get the approval of the architect prior to proceeding with colour concrete works.\n*Samples shall be prepared in batches of not less than one-half cubic metre per sample to ensure accura",""]
["Formwork:",""]
["Descriptions of formwork shall be deemed to include use and waste only (except where described as left in or permanent), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy relea",""]
["Descriptions of smooth formwork shall be deemed to include rubbing off all projections at seams, etc. after removal of formwork, making good any defects with 2:1 cement mortar and leaving a smooth surface with all arises slightly rounded",""]
["The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself",""]
["Formwork to soffits of solid slabs etc. shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described",""]
["Formwork to sides of bases, pile caps, ground beams, etc., will only be measured where it is prescribed by the Engineer for design reasons.  Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof sha",""]
["UNREINFORCED CONCRETE ",""]
["20Mpa/19mm concrete",""]
["Bases","m³",0.13]
["REINFORCED CONCRETE",""]
["30MPa/19mm concrete:",""]
["Rectangular plinth on roof slab","m³",{"v":4,"d":"4.00"}]
["Slabs including beams and inverted beams","m³",{"v":45,"d":"45.00"}]
["Slabs dowelled into pigmented concrete wall","m³",{"v":3,"d":"3.00"}]
["Cantilever slabs in benches","m³",{"v":2,"d":"2.00"}]
["Cast in-situ concrete bench","m³",{"v":5,"d":"5.00"}]
["Cast in-situ leaf shaped concrete bench as per architects detail marked \"Detail A\" Drawing 25379-GP-4200.02","m³",{"v":4,"d":"4.00"}]
["Retaining walls","m³",{"v":8,"d":"8.00"}]
["75mm Thick concrete worktop size 968 x 5804mm","No",{"v":1,"d":"1.00"}]
["30MPa/19mm concrete with waterproofing admixture:",""]
["Purpose made cast insitu reinforced concrete wash basin, size 2630 x 710 x 150mm thick overall with void with sloping sides formed in top including smooth formwork to sides and soffit and with top surface steel trowelled to a smooth finish all as per deta","No",{"v":2,"d":"2.00"}]
["TESTING",""]
["Test blocks",""]
["Making and testing set of three 150 x 150 x 150mm concrete strength test cubes","Sets",{"v":15,"d":"15.00"}]
["INSULATION TO CONCRETE",""]
["Insulation to concrete slab:",""]
["30mm High density rigid extruded polystyrene insulation boarding as per SANS 1506","m²",{"v":257,"d":"257.00"}]
["CONCRETE SUNDRIES",""]
["Finishing top surfaces of concrete smooth with a steel trowel",""]
["Concrete surface beds, slabs, etc. (Labour Intensive Construction)","m²",{"v":193,"d":"193.00"}]
["Finishing top surfaces of reinforced concrete vanity tops to a smooth steel troweled finish (labour Intensive Construction)","m²",{"v":10,"d":"10.00"}]
["Finishing top surfaces of reinforced concrete server tops to a smooth steel trowelled finish (Labour Intensive Construction)","m²",{"v":6,"d":"6.00"}]
["SMOOTH FORMWORK (DEGREE OF ACCURACY I)",""]
["Work bench slabs and similar","m²",{"v":21,"d":"21.00"}]
["Smooth formwork to sides and soffits of slabs:",""]
["Slabs propped up exceeding 3,5m not exceeding 5m high","m²",{"v":202,"d":"202.00"}]
["Slabs propped up exceeding 5m not exceeding 6,5m high","m²",{"v":195,"d":"195.00"}]
["Smooth formwork to sides:",""]
["Rectangular plinth on concrete roof slab","m²",{"v":17,"d":"17.00"}]
["Rectangular stub columns on roof slab","m²",{"v":28,"d":"28.00"}]
["Walls exceeding 1,5 and not exceeding 3.5m high","m²",{"v":943,"d":"943.00"}]
["Walls exceeding 3.5m and not exceeding 5m high","m²",{"v":135,"d":"135.00"}]
["Retaining walls circular not exceeding 1m radius","m²",{"v":15,"d":"15.00"}]
["Retaining walls circular exceeding 1m radius","m²",{"v":23,"d":"23.00"}]
["Edge not exceeding 300mm high in built in shelving","m",{"v":5,"d":"5.00"}]
["Edge not exceeding 300mm high in built in benches","m",{"v":23,"d":"23.00"}]
["Edge not exceeding 300mm high in built in shelving curved on elevation to radius not exceeding 1m.","m",{"v":5,"d":"5.00"}]
["Smooth Formwork to soffits:",""]
["Boxing in smooth formwork to form:",""]
["100 x 200mm Chamfer along top or bottom edge","m",{"v":22,"d":"22.00"}]
["10 x 10mm Rainwater drip at edge of slab","m",{"v":70,"d":"70.00"}]
["SUNDRIES",""]
["Labour only in building in: (Labour Intensive Construction)",""]
["Building in 4 x 40mm mild steel flat bar with welded lugs fixed to top of concrete surface bed ","m",{"v":19,"d":"19.00"}]
["Building in 4 x 40mm mild steel flat bar with welded lugs fixed to top of concrete surface bed bend to radius ","m",{"v":33,"d":"33.00"}]
["Building in 4 x 40 x 40mm mild steel angle with welded lugs fixed to top of concrete surface bed","m",{"v":12,"d":"12.00"}]
["Building in 4 x 40mm polished stainless steel flat bar with lugs into top of concrete surface bed","m",{"v":78,"d":"78.00"}]
["CONCRETE COPINGS, ETC. ",""]
["In-situ conrete copings finished smooth on exposed surfaes to be cast on retaining walls, with expansion jionts at maximum 1,5m centres, including all concrete, formwork, and finishes",""]
["550 x 100mm Thick overall copings, with and including 50 x 30mm recess and separate deep groove in bottom along one edge.","m",{"v":245,"d":"245.00"}]
["550 x 100mm Thick overall copings circular to not exceeding 1m radius, with and including 50 x 30mm recess and separate deep groove in bottom along one edge.","m",{"v":3,"d":"3.00"}]
["550 x 100mm Thick overall copings circular to exceeding 1m radius, with and including 50 x 30mm recess and separate deep groove in bottom along one edge.","m",{"v":3,"d":"3.00"}]
["550 x 100mm Thick overall copings with sloping tops; the copings circular on plan and elevation to not exceeding 1m radius","m",{"v":3,"d":"3.00"}]
["550 x 100mm Thick overall copings with sloping tops; the copings circular on plan and elevation to exceeding 1m radius","m",{"v":3,"d":"3.00"}]
["500 x 100mm Thick overall copings with and including 50 x 30mm recess and separate drip groove in bottowm alone one edge.","m",{"v":75,"d":"75.00"}]
["500 x 100mm Thick overall copings, circular to not exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge. ","m",{"v":2,"d":"2.00"}]
["500 x 100mm Thick overall copings, circular to exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge. ","m",{"v":2,"d":"2.00"}]
["500 x 100mm Thick overall copings, with sloping tops; the copings on plan and elevation to not exceeding 1m radius. ","m",{"v":2,"d":"2.00"}]
["500 x 100mm Thick overall copings, with sloping tops; the copings on plan and elevation to exceeding 1m radius. ","m",{"v":2,"d":"2.00"}]
["Precast conrete finished smooth on exposed surfaces including beddinig on ABE Epidermix epoxy mortar, jointing and pointing with ABE Dura cement grout with TAL keycoat water repellent additive in max. 5mm gaps between units",""]
["440 x 100mm Thick overall Modcon, or similar approved, mono pitch coping weathered on top, with concave mortar joints between units (coping type 021)","m",{"v":210,"d":"210.00"}]
["Ditto, but to radius not exceeding 4m","m",{"v":6,"d":"6.00"}]
["Extra over for fair returned stopped end.","No",{"v":2,"d":"2.00"}]
["Extra over for mitred angle intersection","No",{"v":1,"d":"1.00"}]
["WATERPROOFING",""]
["Prepare and APPLY ABE Duraflex cementitious flexible slurry waterproofing with ecofelt membrane.",""]
["To tops of parapet walls","m²",{"v":34,"d":"34.00"}]
["Prepare and apply TFC or similar approved, cement sealant. ",""]
["To general surfaces of precast conrete copings","m²",{"v":165,"d":"165.00"}]
["Two coats bitumen emulsion waterproofing coating on",""]
["Concrete walls and columns in foundations","m²",{"v":39,"d":"39.00"}]
["Concrete walls, columns and beams ","m²",{"v":126,"d":"126.00"}]
["SEALING STRIPS, JOINT SEALANTS, ETC",""]
["\"Sikaflex 11FC\" polyurethane sealing compound including backing cord, bond breaker, primer, etc ",""]
["5 x 5mm Pointing to expansion joints between precast concrete coping units. ","m",{"v":128,"d":"128.00"}]
["10 x 10mm In expansion joints in floors, etc including raking out expansion joint filler as necessary","m",{"v":10,"d":"10.00"}]
["PLASTERING ",""]
["Cement plaster wood floated, on brickwork",""]
["On walls","m²",{"v":169,"d":"169.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["PRECAST CONCRETE PAVING",""]
["Paving of 450 x 450 x 50mm precast concrete paving slabs with smooth finish:",""]
["Exposed Granite aggregate paving slabs laid on waterproofing to walkway and including 20 mm sand layer with pointed joints","m²",{"v":14,"d":"14.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Contractor to comply with the following:\n1. All masonry walls to be laid to standards and tolerances in compliance with SANS 10164 and SANS 10145\n2. Masonry cement to comply with requirements of SANS 50413-1 type MC5\n3. Mortar to be Class II to SANS 10164",""]
["BRICKWORK IN SUPERSTRUCTURE",""]
["Brickwork of NFP bricks in class II mortar:",""]
["Half brick wall linings to concrete","m²",{"v":118,"d":"118.00"}]
["One brick wall with 500 x 510mm high opening with precast lintel over ","m²",{"v":7,"d":"7.00"}]
["PREAMBLES",""]
["SUPPLEMENTARY PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["Guarantee:",""]
["The manufacturer of waterproofing materials shall comply with ISO9002 Quality Management System.  Sheeting shall be laid in strict accordance with the manufacturer's specifications by an approved contractor. A written and approved five year guarantee of s",""]
["Waterproofing of roofs:",""]
["All rainwater outlets are to be cast in position before waterproofing commences to ensure that outlets are set lower than the surrounding areas to prevent ponding",""]
["DAMPPROOFING OF WALLS AND FLOORS",""]
["One layer 375 micron green polyethylene waterproof covering (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape",""]
["To cavity walls in parapet walls","m²",{"v":9,"d":"9.00"}]
["To 270mm cavity walls","m²",{"v":3,"d":"3.00"}]
["To 290 mm cavity walls","m²",{"v":5,"d":"5.00"}]
["To brick copings","m²",{"v":4,"d":"4.00"}]
["Fibre-reinforced waterproofing",""]
["Acrylic based flexible fibre reinforced waterproofing compound to with G1 non-woven polyester reinforcing membrane.","m²",{"v":126,"d":"126.00"}]
["Prime with one coat bitumen primer and one layer 4mm fully bonded waterproof membrane comprising two bitumen layers reinforced with woven spun bonded polyester fabric and coated with polyethylene film for heat bonding, laid with 100mm side and 150mm end l",""]
["On walls","m²",{"v":31,"d":"31.00"}]
["Two coats bitumen emulsion waterproof  coating ",""]
["On walls","m²",{"v":549,"d":"549.00"}]
["WATERPROOFING TO ROOFS, BASEMENTS, ETC",""]
["Cementitious waterproofing system (suitable for tiling) comprising primer coat plasticised modified acrylic (PMA) (consisting of 51 PMA, 5 litres water and 16,5kg cement (32,5N), one layer pre-cut polypropylene fabric fully saturated in PMA slurry and two",""]
["On walls","m²",{"v":372,"d":"372.00"}]
["Apply one coat of flexible slurry based synthetics resin dispersion waterproofing compound and saturate strips of 200mm polypropylene membrane and apply to all angles, sharp edges and verges etc.  and apply second coat of flexible slurry based synthetic r",""]
["On walls","m²",{"v":171,"d":"171.00"}]
["Apply one coat water-based tile and cement sealer for unglazed porous substrates to be applied with a paint brush strictly as per manufacture's specification:",""]
["On floors","m²",{"v":2448,"d":"2448.00"}]
["Prime concrete surface with one coat bitumen primer and one layer 4mm fully bonded waterproof membrane comprising two bitumen layers reinforced with woven spun bonded polyester fabric and coated with polyethylene film for heat bonding, laid with 100mm sid",""]
["On concrete flat roofs","m²",{"v":3789,"d":"3789.00"}]
["On concrete retaining walls","m²",{"v":91,"d":"91.00"}]
["In turn ups and turn downs","m²",{"v":440,"d":"440.00"}]
["Ditto but circular on plan","m²",{"v":13,"d":"13.00"}]
["On turn-ups and turn-downs not exceeding 300mm girth","m",{"v":1344,"d":"1344.00"}]
["Sealing edges to brickwork or concrete including trowelled mastic bead","m",{"v":162,"d":"162.00"}]
["Additional membrane and sealing into 80 mm diameter outlet","No",{"v":31,"d":"31.00"}]
["Additional membrane and sealing into 150 mm diameter outlet","No",{"v":32,"d":"32.00"}]
["Thinly applied cold dressing waterproofing compound fixed over opening of 50mm diameter rainwater outlet to hold gravel back","No",{"v":2,"d":"2.00"}]
["Apply one coat bituminous solution and one layer 3mm waterproofing membrane by means of torch on fusion with 75mm side laps and 100mm end laps:",""]
["On concrete flat roofs","m²",{"v":93,"d":"93.00"}]
["On box gutters","m²",{"v":1,"d":"1.00"}]
["ABE 5ply malthoid protection layer",""]
["On concrete flat roofs","m²",{"v":1908,"d":"1908.00"}]
["Anti root membrane for soil roofs",""]
["On concrete flat roofs","m²",{"v":317,"d":"317.00"}]
["Dimpled HDPE ABE Drain protection membrane ",""]
["On concrete flat roofs","m²",{"v":291,"d":"291.00"}]
["SEALING STRIPS, JOINT SEALANTS, ETC",""]
["Prepare and apply one coat of TFC or equally approved clear matt cement sealant:",""]
["On walls","m²",{"v":43,"d":"43.00"}]
["Silicone sealant:",""]
["On sills","m²",{"v":57,"d":"57.00"}]
["6 x 6mm Triangular sealant around windows, doors, etc.","m",{"v":810,"d":"810.00"}]
["6 x 6mm Triangular sealant at junction of steel drain and concrete wash hand basin","m",{"v":4,"d":"4.00"}]
["Two-part non-sag polysulphide sealing compound including backing cord, bond breaker, primer, etc. according to SANS 1077 of type two gun application:",""]
["8  x 10mm In joints in face of brick wall including raking out existing expansion joint filler","m",{"v":135,"d":"135.00"}]
["10 x 10mm In expansion joints in floors including raking out expansion joint filler as necessary","m",{"v":386,"d":"386.00"}]
["20 x 10mm Sealing of façade joints","m",{"v":298,"d":"298.00"}]
["One component non-sag polyurethane elastomeric flexible joint sealant to SABS 1077:",""]
["3 x 10mm In soft joints between new plaster and existing floors","m",{"v":247,"d":"247.00"}]
["6 x 10mm In saw cut joints in floors","m",{"v":479,"d":"479.00"}]
["12 x 10mm In Isolation joints in floors","m",{"v":60,"d":"60.00"}]
["6 x 10mm In construction joints in floors","m",{"v":100,"d":"100.00"}]
["Rake out 12 x 10mm deep foam Jointex in junctions of concrete surface beds and walls, prime and caulk with Sikaflex 11 FC sealant","m",{"v":1455,"d":"1455.00"}]
["FLASHINGS, ETC",""]
["Flashings shall be manufactured from ZINCALUME® AZ150 0.8mm coated steel with a custom formulated polyster pant with inorganic pigments finish (architect to advise) and fixed by way of S10 brackets all in strict accordance with manufacturer’s specificatio",""]
["Headwall Flashing 375mm with counter flashing 185mm girth 2 times bent and notched on site to suit roof profile","m",{"v":59,"d":"59.00"}]
["Sidewall Flash 408mm with counter flashing 185mm girth 2 times bent.","m",{"v":79.7,"d":"79.70"}]
["Acrylic based flexible fibre-reinforced waterproofing  compound including G1 non-woven polyester reinforcing membrane:",""]
["Parapet walls","m²",{"v":501,"d":"501.00"}]
["Parapet walls circular on plan","m²",{"v":20,"d":"20.00"}]
["On turn-ups and turn-downs exceeding 300mm girth","m²",{"v":13,"d":"13.00"}]
["Bandage flashing 120mm wide","m",{"v":134,"d":"134.00"}]
["Bandage flashing 250mm wide","m",{"v":142,"d":"142.00"}]
["PROTECTIVE STONE DRESSING",""]
["10-15mm Diameter chipped aggregate in light coloured shades of brown stone dressing evenly spread with larger stones around outlets:",""]
["50mm Thick on waterproofing to flat roofs","m²",{"v":1921,"d":"1921.00"}]
["Under stone dressing to flat roofs","m²",{"v":705,"d":"705.00"}]
["PROTECTIVE ROOFING PAINT",""]
["Prapare and apply one coat acrylic based paint finish on exposed waterproofing :",""]
["On bituminous waterproofing to roofs","m²",{"v":2506,"d":"2506.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Fixing:",""]
["Items described as 'nailed' shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete",""]
["Items described as 'plugged' shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as 'bolted', the bolts have been given elsewhere",""]
["Joinery:",""]
["All screws used to be suitable for wood according to SAN 1170.  Hardwood for fittings to be selected by Architect.  Hardwood to be sourced from locally situated timber supplier that complies to The Forest Stewardship Council (FSC) standards",""]
["Descriptions of frames shall be deemed to include frames, transomes, rails, etc.",""]
["Descriptions of hardwood joinery shall be deemed to include sinking and pelleting heads and nuts of bolts",""]
["Doors:",""]
["Doors to be manufactured in accordance with SANS 545:2009",""]
["ROOF CONSTRUCTION",""]
["ROOFS ETC",""]
["Provisional sum for remedial work to timber roof trusses","Prov Sum",{"v":1,"d":"1.00"}]
["SOLID DOORS",""]
["Wrought hardwood doors hung to timber frames:",""]
["44mm Purpose made heavy duty Class 1 extra length double action swing door, size 895 x 2425mm high with 300mm diameter circular framed porthole marked as D24 at LIVING HERITAGE","No",{"v":1,"d":"1.00"}]
["FRAMED FRAMES ETC",""]
["Wrought hardwood:",""]
["Hardwood door frame size 1420x 2032 high with 90x55mm rebated moulded grooved frame without sill as per detail marked D22 at LIVING HERITAGE","No",{"v":1,"d":"1.00"}]
["Hardwood door frame size 1500x 2085 high with 90x55mm rebated moulded grooved frame without sill as per detail marked D22 on drawing no EDUC 3200.04","No",{"v":1,"d":"1.00"}]
["Hardwood door frame size 1694x 2125 high with 90x55mm rebated moulded grooved frame without sill as per detail marked D21 on drawing no EDUC 3200.04","No",{"v":1,"d":"1.00"}]
["Hardwood door frame size 1694x 2425 high with 90x55mm rebated moulded grooved frame without sill as per detail marked D03 and D04  on at MUSEUM","No",{"v":2,"d":"2.00"}]
["Hardwood door frame size 2039x 2095 high with 90x55mm rebated moulded grooved frame without sill as per detail marked and D04  at RECEPTION","No",{"v":1,"d":"1.00"}]
["Hardwood door frame size 2384x 2425 high with 90x55mm rebated moulded grooved frame without sill as per detail marked and D08  at MUSEUM","No",{"v":1,"d":"1.00"}]
["WINDOWS",""]
["Timber Windows:",""]
["Hardwood timber window surround, size 3800x1035mm high, as per detail marked W27 on drawing EDUC 3100.06","No",{"v":1,"d":"1.00"}]
["BEADS, ARCHITRAVES, ETC",""]
["Wrought Meranti:",""]
["12mm Quadrant beads pinned","m",{"v":35,"d":"35.00"}]
["22 x 75mm Skirting","m",{"v":274,"d":"274.00"}]
["TIMBER WALL PANELLING",""]
["Decorative timber wall panelling:",""]
["Slatted landscape wall formed of 38 x 38mm hard wood slats with cut out profile on 6mm thick hardwood veneer plywood board mounted securely to 38 x 38mm SA pine brandering","m²",{"v":10,"d":"10.00"}]
["HARDWOOD PARQUET FLOORING",""]
["8mm Hardwood parquet basket weave flooring laid according to SAN978 comprising hardwood timber suitable for high traffic class and fixed to cement screed with modified vinyl emulsion water-based adhesive:",""]
["Hardwood parquet basket weave flooring","m²",{"v":289,"d":"289.00"}]
["JOINERY FITTINGS",""]
["Shelving and framed shelving units:",""]
["16 x 580mm wide shelving comprising of melamine-impregnated decorative paper, fused under heat and pressure to both sides of a smooth surface particle board substrate mounting bracket to be plastic white 44 x 50 x 47 with brackets to be fixed to wall with","m",{"v":50,"d":"50.00"}]
["Built-in shelves size 2443 x 590 x 3030mm high overall formed of particle board with hardwood veneer to match 75 x 22mm hardwood edge strip on a 40 x 40mm  substructure  and 30 x 30 x 2mm mild steel support securely fixed  into concrete wall with epoxy an","No",{"v":1,"d":"1.00"}]
["Solid hardwood storage shelves type 3550 x 350 x 2240mm high with internal shelving to be 16mm thick single layer of veneer bonded to particle board with 22 x 50mm solid hardwood front edge strip fixed with 20mm diameter countersunk stainless steel screws","No",{"v":1,"d":"1.00"}]
["Shelving unit size 4218 x 3455mm high overall comprising 16mm thick single layer of veneer bonded to particle board against brickwork with sub-frame fixed to brick wall with anchor bolts as per Detail of Retail Shop shelving 02 Drawing 25379-LHW&R-7000.04","No",{"v":1,"d":"1.00"}]
["Shelving unit size 5930 x 3455mm high overall comprising 16mm thick single layer of veneer bonded to particle board against brickwork with sub-frame fixed to brick wall with anchor bolts all as per Detail of Retail Shop shelving 01 Drawing 25379-LHW&R-700","No",{"v":1,"d":"1.00"}]
["Counters:",""]
["Cashier counter complete with cabinets and doors below and pay station size 2100 x 654mm as per Dwg 25379-LHW&R -7000.05 complete with graphic\nNote: This is a 'Unconquerable spirit George Stow's History paintings of the San by Pippa Skotnes, Page 190' - a","No",{"v":1,"d":"1.00"}]
["Tables:",""]
["A sample of each table type to be manufactured for final approval by Architects to confirm ideal height and quality. Sample to be approved before commencing with the manufacture of all.",""]
["800 x 800 x 775mm high restaurant Table2 type tables complete with 220 x 69 SA pine slats screwed securely on corners, and fixed to 38 x 38mm SA Pine surround below table top with 50mm min length metal screws for wood with 30mm recess filled flush with ma","No",{"v":25,"d":"25.00"}]
["3000 x 900 x 775mm high restaurant Table1 type tables complete with 220 x 69 SA pine screwed securely on corners, and fixed to frame with 50mm min length metal screws for wood with 30mm recess filled flush with matching standard wood filler including, cro","No",{"v":4,"d":"4.00"}]
["3800 x 900mm Workshop benches complete with 220 x 69 SA pine including 50 x 50 x 4mm mild steel angle iron surround , mitred and welded securely on corners, and fixed to frame with 30mm min length metal screws for wood at 30mm spacing max including 25 x 2","No",{"v":4,"d":"4.00"}]
["Kitchen Cupboards:",""]
["Sink cupboard size 1800 x 600 x 900mm high with 32mm thick worktop with Delta 90 degree profile and formed of 16mm thick single layer of melamine-impregnated decorative paper with sides, bottom, division, shelf, back and single hinged doors dividing frame","No",{"v":1,"d":"1.00"}]
["Wall cupboard size 1820 x 350 x 510mm high from approved 19mm compressed board, spray painted with  sides, bottom, division, shelf, back and single hinged doors dividing frame complete with all handles to be 20mm diameter 25mm anodised aluminium circular ","No",{"v":1,"d":"1.00"}]
["Floor cupboard size 2676 x 600 x 900mm high with 32mm thick worktop with Delta 90 degree profile and formed of 16mm thick single layer of melamine-impregnated decorative paper with sides, bottom, division, shelf, back and single hinged doors dividing fram","No",{"v":1,"d":"1.00"}]
["Wall cupboard size 3320 x 350 x 1000 high formed of 16mm thick single layer of melamine-impregnated decorative paper, with sides, bottom, division, shelf, back and single and double hinged doors, dividing frame complete with all handles to be 20mm diamete","No",{"v":1,"d":"1.00"}]
["Sink cupboard overall size 3741 x 600 x 900mm high with 30mm thick light grey granite worktop, 19mm thick spray painted MDF board on all visible parts, 19mm thick particle board for carcass covered with  single layer of melamine-impregnated decorative pap","No",{"v":1,"d":"1.00"}]
["Cupboard and shelf unit size 4190 x 600 x 1000mm high formed of 16mm thick carcass of single layer melamine-impregnated decorative paper, fused under heat and pressure to both sides of a smooth surface Particleboard substrate laminated on both sides, with","No",{"v":1,"d":"1.00"}]
["Cupboard and drawer cabinet size 4190 x 600 x 900mm high formed of 32mm thick worktop with Delta 90 degree consisting of a high pressure laminate bonded to a moisture resistant particle board substrate with laminated on one side backer with a carcass made","No",{"v":1,"d":"1.00"}]
["Cupboards:",""]
["Solid hardwood cupboards with internal shelving of 16mm thick single layer of veneer bonded to particle board with 22 x 50mm solid hardwood front edge strip including three drawers each size 550 x 350 x 218mm high fixed with 20mm diameter countersunk stai","No",{"v":1,"d":"1.00"}]
["Laundry store cupboard overall size 1520 x 600 x 2126 mm high, 16mm thick single layer of melamine-impregnated decorative paper, with side, bottom, division, shelf, back and single and double hinged doors, dividing frame complete with all ironmongery, han","No",{"v":1,"d":"1.00"}]
["Solid hardwood cupboards type 1950 x 900 x 785mm high with internal shelving to be 16mm thick single layer of veneer bonded to particle board with 22 x 50mm solid hardwood front edge strip fixed with 20mm diameter countersunk stainless steel screws as per","No",{"v":1,"d":"1.00"}]
["Built in cupboard size 2390 x 600 x 2350mm high formed carcass 16mm thick single layer of melamine-impregnated decorative paper, fused under heat and pressure to both sides of a smooth surface particleboard substrate laminated on both sides with 16mm thic","No",{"v":1,"d":"1.00"}]
["Desks and work stations:",""]
["Solid hardwood work desk with computer cable inlets size 2650 x 700 x 785mm high with internal shelving to be 16mm thick single layer of veneer bonded to particle board with 22 x 50mm solid hardwood front edge strip fixed with 20mm diameter countersunk st","No",{"v":1,"d":"1.00"}]
["Purpose made control room desk size 4000 x 650mm wide supported on 710 x 60mm work top leg fixed to the underside of a 40 x 40mm SA Pine sub frame behind with brass self tapping wood screws as  per architects drawing 25379-EDUC-7000.02","No",{"v":1,"d":"1.00"}]
["Reception desk size  5804 x 968mm comprising 19x19mm hardwood slates, fixed securely to 3mm hardwood veneered plywood, on 19mm supawood or equally approved back board fixed with 25mm min length counter sunk timber screws fixed at minimum 300centres with b","No",{"v":1,"d":"1.00"}]
["Purpose made timber curved work station size 7759 x 710mm wide formed of  60mm top with 3mm hardwood veneer and 75 x 22mm hardwood edge strip on a substructure of 44 x 44mm and 76 x 38mm SA Pine members with adjustable footing in matt black (No.3)  as per","No",{"v":1,"d":"1.00"}]
["The following in slatted timber bench seats:",""]
["22 x 76 x 76mm Hardwood spacers","No",{"v":192,"d":"192.00"}]
["44 x 76mm Hardwood slats","m",{"v":162,"d":"162.00"}]
["Solid timber bench seats:",""]
["Solid Eucalyptus bench size 3150 x 450 x 325mm high with all edges finished to a rough saw cut surface fitted with 32mm diameter matt stainless steel off the shelf adjustable footings (No.10) placed at  centres of 685mm and 735mm respectively.","No",{"v":3,"d":"3.00"}]
["Benches formed of timber with steel supports:",""]
["900 x 450mm Ablution benches complete with 30 x 30mm mild steel hollow square tubing frame in three equally spaced supports and where adjacent to wall, securely fixed with M10 anchors including a 12mm thick mild steel flat welded to frame supports complet","No",{"v":1,"d":"1.00"}]
["1180 x 450mm Ablution benches complete with 30 x 30mm mild steel hollow square tubing frame in three equally spaced supports and where adjacent to wall, securely fixed with M10 anchors including a 12mm thick mild steel flat welded to frame supports comple","No",{"v":3,"d":"3.00"}]
["1180 x 450mm Ablution benches complete with 30 x 30mm mild steel hollow square tubing frame in three equally spaced supports and where adjacent to wall, securely fixed with M10 anchors including a 12mm thick mild steel flat welded to frame supports comple","No",{"v":1,"d":"1.00"}]
["2050 x 450mm Ablution benches complete with 30 x 30mm mild steel hollow square tubing frame in three equally spaced supports and where adjacent to wall, securely fixed with M10 anchors including a 12mm thick mild steel flat welded to frame supports comple","No",{"v":1,"d":"1.00"}]
["Seat formed of 32mm thick  laminated solid hardwood fixed securely to concrete bench with standard 45mm minimum length Fischer plugs or equal approved brassed metal expansion screws:",""]
["Timber seat size 4984 x 1370mm high as per detail on Drawing no 25379-REC-7000.02","No",{"v":1,"d":"1.00"}]
["Timber seat size 7574 x 1370 high as per detail on Drawing no 25379-REC-7000.02","No",{"v":1,"d":"1.00"}]
["RESIN FITTINGS",""]
["Quartz polyester resin fittings:",""]
["Mobile server table, size 2000 x 800 x 868mm high Quartz polyester resin 30mm Thick table top with all exposed edges small bevel edged fixed to supports using clear silicone adhesive at 200 to 300mm centres along all supports with all joints filled with m","No",{"v":2,"d":"2.00"}]
["WALL PANELS",""]
["Wall panel formed of 6mm thick hardwood veneer plywood board mounted securely to 38 x 38mm SA pine brandering with 200mm length timber screws with brandering mounted to wall horizontally with recessed approved brassed expansion metal screws at 300mm centr",""]
["Panel size 10412 x 2500mm high overall  as per architect drawing 25379-REC-7000.02","No",{"v":1,"d":"1.00"}]
["ACOUSTIC WALL PANELS",""]
["Auditorium acoustic wall panel Type A protruding 150mm from wall comprising of 16mm thick middle density fibre, Acoustic Solutions linear perforated acoustic panel with perforations 5.8mm and groove 2.2mm fixed in tongue and groove system to 38 x 38 SA Pi",""]
["Panel Type A, size 1001 x 490mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type A, size 1000 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type A, size 1937 x 980mm high all as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type A, size 1974 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type A, size 1937 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type A1 protruding 150mm from wall comprising of 16mm thick middle density fibre, Acoustic Solutions linear perforated acoustic panel with perforations 5.8mm and groove 2.2mm fixed in tongue and groove system to 38 x 38 SA Pine battens at 600mm cent",""]
["Panel Type A1, size 2004 x 735mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":1,"d":"1.00"}]
["Panel Type B protruding 100mm from wall comprising of 16mm thick middle density fibre Acoustic Solutions linear perforated acoustic panel with perforations 5.8mm and groove 2.2mm fixed in tongue and groove system to 38 x 38 SA Pine battens at 600mm centre",""]
["Panel Type B, size 774 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills.","No",{"v":2,"d":"2.00"}]
["Panel Type B, size 1000 x 1230mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type B, size 1000 x 1470mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type B, size 1200 x 1180mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type B, size 2001 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type C protruding 58mm from wall comprising of 16mm thick middle density fibre, Acoustic solutions linear perforated acoustic panel with perforations 5.8mm and groove 2.2mm fixed in tongue and groove system to 38 x 38 SA Pine battens at 600mm centre",""]
["Panel type C, size 774 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type C, size 1000 x 1390mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type C, size 1000 x 1860mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type C, size 1000 x 2450mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Panel Type C, size 1200 x 980mm high as per drawing 25379-EDUC-7000.01 attached to the back of these bills","No",{"v":2,"d":"2.00"}]
["Rear wall acoustic panel to be mounted onto a concealed wedge slider 1200mm above floor level and to step 100mm short of ceiling:",""]
["Green Acoustics Tunesober 1800 x 900 x 58mm thick","No",{"v":16,"d":"16.00"}]
["ACOUSTIC INSULATION",""]
["Green Acoustics Fibran Geolan 40mm 50kg/m3 Stonewool or equally approved product to be installed in the cavity of the middle density fibre and the wall:",""]
["On acoustic panel walls","m²",{"v":183,"d":"183.00"}]
["TRENCH COVERS, ETC",""]
["220 x 22mm Thick hardwood trench cover with 30mm diameter cut out hole in either end of the cover with 32 x 10mm SA Pine lateral support at 300mm centres  under floor board fixed from below with brass wood screws including 32 x 10mm SA pine packer piece w",""]
["Trench cover 679mm long","No",{"v":2,"d":"2.00"}]
["Trench cover 711mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 755mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 762mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 794mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 844mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 900mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 919mm long","No",{"v":2,"d":"2.00"}]
["Trench cover 949mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 969mm long","No",{"v":2,"d":"2.00"}]
["Trench cover 1010mm long","No",{"v":1,"d":"1.00"}]
["Trench cover 1145mm long","No",{"v":2,"d":"2.00"}]
["Trench cover 1200mm long","No",{"v":76,"d":"76.00"}]
["SCREENS:",""]
["Screens formed of 150mm maximum diameter CCA treated free standing eucalyptus poles at 200mm centres 2437mm high with galvanised mild steel cap fixed to top of each pole, with cap comprising 10 x 150mm diameter galvanised mild steel disk welded to 20 x 10",""]
["Free standing pole screen, size 3985 x 2437mm high overall as per architects detail marked Detail b/3700.02 on Drawing No 25379-DORM-3700.02","No",{"v":1,"d":"1.00"}]
["Screens formed of 150mm maximum diameter CCA treated eucalyptus pole at 280mm centres  with galvanised mild steel shoe fixed to top and bottom of each pole, with shoe comprising 10 x 100mm diameter galvanised mild steel disk welded to 20 x 90mm pin with o",""]
["Pole screen, size 1200 x 2590mm high overall as per architects detail marked \"Screen Detail D\" on Drawing 25379-GP-3700.04","No",{"v":1,"d":"1.00"}]
["Pole screen, size 3900 x 3560mm high overall as per architects detail marked \"Screen Detail D\" on Drawing 25379-EDUC-3700.03","No",{"v":1,"d":"1.00"}]
["Pole screen, size 4050 x 3060mm high overall as per architects detail marked \"Screen Detail B\" on Drawing 25379-EDUC-3700.02","No",{"v":4,"d":"4.00"}]
["Pole screen, size 4490 x 2840mm high overall as per architect detail marked \"Screen Detail A\" on Drawing 25379-DORM 3700.01","No",{"v":4,"d":"4.00"}]
["Pole screen, size 4500 x 3060mm high overall as per architects detail marked \"Screen Detail A\" on Drawing 25379-EDUC-3700.03","No",{"v":5,"d":"5.00"}]
["Pole screen, size 6933 x 3230mm high overall as per architects detail on Drawing 25379-REC-3300.01","No",{"v":1,"d":"1.00"}]
["Pole screen, size 7500 x 3060mm high overall as per architects detail marked \"Screen Detail C\" on Drawing 25379-EDUC-3700.02","No",{"v":1,"d":"1.00"}]
["WATTLE SCREENS",""]
["Screens formed of interwoven eucalyptus laths with all bark removed and treated with CCA according to SANS 10005:",""]
["20mm Diameter Wattle laths in 2200mm lengths laid directly abutting each other and fixed to stainless steel cables at 500mm centres (elsewhere measured) to form screen circular on plan","m²",{"v":7,"d":"7.00"}]
["20mm Diameter Wattle laths in 2700mm lengths laid directly abutting each other and fixed to stainless steel cables at 500mm centres (elsewhere measured) to form screen circular on plan","m²",{"v":21,"d":"21.00"}]
["20mm Diameter Wattle laths in lengths not exceeding 3300mm laid directly abutting each other on and over steel frame (elsewhere measured) to form woven screen","m²",{"v":1160,"d":"1160.00"}]
["20mm Diameter Wattle laths in lengths not exceeding 3300mm laid directly abutting each other on and over steel frame (elsewhere measured) to form woven screen circular on elevation","m²",{"v":387,"d":"387.00"}]
["JOINERY SUNDRIES",""]
["Hardwood",""]
["Slatted shelving, seats, etc of 76 x 44mm wide slats at 66mm centres, screwed to steel framing including holes","m²",11.39]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Fixing:",""]
["Unless otherwise described ceilings shall be deemed to be horizontal",""]
["Prices for openings for light fittings, ventilation grilles, air conditioning diffusers, etc. are to include for any necessary additional support, trimming around, etc.",""]
["Where electrical light fittings, diffusers, panels etc. are lay-in units of the same dimensions as the suspension grid described allowance must be made in the rates accordingly for their support inclusive of any flexibility in setting out that may be requ",""]
["Items described as 'nailed' shall be deemed to be fixed with hardened steel nails or pins, or to be shot-pinned, to brickwork or concrete",""]
["Items described as 'plugged' shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 500mm centres, and where described as 'bolted', the bolts have been given elsewhere",""]
["Hangers, suspension grids, lay-in panels, etc. are to be in accordance with the manufacturers' recommendations",""]
["INSULATION",""]
["Green Acoustic Fibran Geolan 40mm 50kg/m3 Stonewool or equally approved product:",""]
["Stonewool flush ceiling insulation","m²",{"v":685,"d":"685.00"}]
["Composite thermal insulation 50mm thick polyester thermal insulation with aluminium foil to one face  with a density 10kg/m3 laid with foil facing down between steel rafters on straining wires at 300mm centres, with insulation to have no chemical additive",""]
["Insulation on hand woven reed matt ceiling fixed to underside of purlins","m²",{"v":274,"d":"274.00"}]
["SUSPENDED CEILINGS",""]
["Gypsum plaster grid ceiling system with 9mm thick plasterboard, fixed at right angles to 35mm concealed face suspended ceiling grid system with 24 x 35mm high galvanised steel knurled capped main tees at 1200mm centres and cross tees at 400mm centres usin",""]
["Plasterboard ceilings","m²",{"v":623,"d":"623.00"}]
["Horizontal margins 360mm wide","m",{"v":28,"d":"28.00"}]
["9mm Thick vertical bulkhead 682mm high and skimmed","m",{"v":80,"d":"80.00"}]
["Vertical bulkhead 250mm girth comprising 9mm thick plaster board fixed to a galvanised suspended celling grid system","m",{"v":241,"d":"241.00"}]
["Bulkhead 250mm girth comprising of 132mm upstand with no rebate and 90 degree angle and skimmed","m",{"v":234,"d":"234.00"}]
["Acoustic ceiling system plasterboard, size 600 x 600mm fixed at right angles to 35mm concealed face suspended ceiling grid system with 24 x 35mm high galvanised steel knurled capped main tees at 1200mm centres and cross tees at 400mm centres using 25mm dr",""]
["Acoustic ceiling","m²",{"v":62,"d":"62.00"}]
["Acoustic plaster ceiling installed as a suspended ceiling construction clad on one side with VoglToptec acoustic plaster system panels with acoustic fleece on the reverse fixed to a rigid ceiling framework made of zinc-plated metal profiles suspended hori",""]
["Flush acoustic plastered ceilings","m²",{"v":565,"d":"565.00"}]
["Extra over ceilings for bulk heads 500mm high","m",{"v":100,"d":"100.00"}]
["Rockfon Tropic smooth acoustic ceiling finish tile inlay or other approved comprising Tropic E15 15mm thick 600 x 600mm boards with class A1 fire rating on system SY15 (T15) suspension grid including hangers, fixings, channels etc.:",""]
["Rockfon Tropic smooth acoustic ceiling","m²",{"v":164,"d":"164.00"}]
["Hand woven reed matt fixed with the underside of the 9mm plywood frame with synthetic rubber-based universal adhesive paste and average 16mm panel pins:",""]
["Reed mat ceiling","m²",{"v":274,"d":"274.00"}]
["MODULAR PANEL CEILING",""]
["The following in modular panel ceiling comprising galvanised mild steel support channels and angle section frames (elsewhere measured) with plywood panels with timber stiffeners with hand woven wattle reed mat fixed beneath all as per architects Drawings ",""]
["12mm Thick U/F SA Pine plywood as backs","m²",{"v":158,"d":"158.00"}]
["44 x 68mm Wrought SA Pine stiffeners screwed to timber with brass screws at 300mm centres","m",{"v":306,"d":"306.00"}]
["Hand woven reed mat fixed to plywood backing with panel pins and adhesive","m²",{"v":158,"d":"158.00"}]
["The following in modular panel ceiling comprising hot dipped galvanised mild steel hollow section frames and flat section supports (elsewhere measured) with slatted hardwood feature ceiling with stiffening braces all as per architects Drawings no 25379-MU",""]
["38 x 38mm Hardwood ceiling bracing screwed","m",{"v":35,"d":"35.00"}]
["69 x 114mm Hardwood ceiling slats screwed","m",{"v":173,"d":"173.00"}]
["Labour in cutting 38 x 38mm notch in 69mm thick hardwood (Labour Intensive Construction)","No",{"v":216,"d":"216.00"}]
["Labour in cutting 50 x 50mm notch in 69mm thick hardwood (Labour Intensive Construction)","No",{"v":216,"d":"216.00"}]
["SPECIALIST CEILINGS",""]
["Specialist insulated ceiling for cold rooms:",""]
["Specialist insulated ceiling for cold rooms","m²",{"v":11,"d":"11.00"}]
["CORNICES",""]
["Shadow line wall angles with all joints taped and plastered:",""]
["25mm Epoxy coated aluminium shadow line plaster trim on flush plastered ceilings","m",{"v":1002,"d":"1002.00"}]
["Edge E Shadow Moulding System SY15 (T15) cornice","m",{"v":190,"d":"190.00"}]
["34 x 40 mm Powder coated pressed metal recessed shadow line wall angle","m",{"v":659,"d":"659.00"}]
["PARTITIONING, ETC",""]
["Gypsum fixed partitions drywall partitioning system with an overall thickness of 112mm comprising internal framing formed of 64mm galvanised steel studs fixed at 600mm centres to galvanised steel track positioned at floor, head and wall plastered with 3mm",""]
["Partitioning 2600mm high","m",{"v":17,"d":"17.00"}]
["Extra over partition 2600mm high for vertical abutment","m",{"v":3,"d":"3.00"}]
["Extra over partition 2600mm high for corner","m",{"v":4,"d":"4.00"}]
["Extra over partition 2600mm high for T-intersection","m",{"v":8,"d":"8.00"}]
["Extra over partition 2600mm for forming opening to suit door size 740 x 1780mm including all studding, trimming, etc.","No",{"v":1,"d":"1.00"}]
["Partition doors size 740 x 1780mm high including standard ironmongery, comprising indicator bolts, hat and coat hooks with buffers","No",{"v":18,"d":"18.00"}]
["18mm Solid core colour finished melamine faced particle board edged all round 2050mm high, manufactured in accordance with SANS 1763:1998 with partitions supported by stainless steel hanging clamp, 48mm diameter x 170mm high grade 316 stainless steel supp",""]
["Partitioning 2050mm high","m",{"v":56,"d":"56.00"}]
["Extra over partition 2600mm high for vertical abutment","m",{"v":4,"d":"4.00"}]
["Extra over partition 2600mm high for corner","m",{"v":2,"d":"2.00"}]
["Extra over partition 2600mm high for T-intersection","m",{"v":3,"d":"3.00"}]
["Moveable partitions Aluglass Bautech Veriflex VX110 mobile acoustic (operable wall) partition, size 900 x 3570mm high to suit structural opening size 6000 x 4000mm high comprising 105 thick tongued and grooved acoustically decoupled 51dB STC rated panels ",""]
["Moveable partitions","m",{"v":66,"d":"66.00"}]
["Extra for forming opening to suit door size 740 x 1780mm including all framing","No",{"v":4,"d":"4.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Fixing",""]
["Floor coverings, wall linings, etc. shall, where applicable, be fixed with adhesive as recommended by the manufacturers of the flooring, linings, etc.",""]
["High quality polyurethane-coated non directional homogenous vinyl floor coverings in sheeting form suitable for heavy traffic areas. Colour to be a homogenous grey, samples to be provided to be approved by the Architect. Sub-floors must be smooth, hard, c",""]
["Carpet tile Adhesive",""]
["The maximum TVOC content limit may not exceed 50g/l for carpet tile adhesive products. The contractor  is required to obtain approval of the design team or client before substituting the finishes listed in the adhesive products schedule. At the end of con",""]
["CARPET TILING",""]
["Carpet tile size 500 x 500 x 7mm thick plain back carpet tile for Heavy commercial use (SABS use class U5), with SABS Class 2 fire rating. Manufactured in accordance with SANS 1415:2005, all installed by approved installer in accordance with SANS 10186:20",""]
["Carpet tiling to screeded floors","m²",{"v":516,"d":"516.00"}]
["VINYL FLOORING COVERINGS",""]
["Flexible vinyl flooring:",""]
["Vinyl floor sheeting obtained at a PC Sum of R275.00 per m2 and laid to floors with an approved adhesive",""]
["2.0mm thick x 2m wide fully flexible single layered vinyl floor sheeting manufactured to specification EN 649 laid in acrylic adhesive spread with a A24F at a rate of between 5m2 and 6.5m2 per litre, depending on sub-floor porosity. It is essential that t",""]
["On floors","m²",{"v":1045,"d":"1045.00"}]
["POLISH, SEALERS, ETC",""]
["Sealing and polishing :",""]
["Strip, seal and polish vinyl flooring","m²",1044.59]
["SKIRTINGS, NOSINGS, ETC",""]
["Snap-on Stringer access floor system with 600 x 600mm Type 3 steel clad cementitious core panels with factory bonded conductive and anti-static vinyl finish with bevelled trim edge, supported by and including all necessary under structure components as pe",""]
["On access floors","m²",{"v":12,"d":"12.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["All ironmongery is to be approved by the architect in writing after submission of samples by the contractor",""]
["All ironmongery to be confirmed by specialist for confirmation prior to ordering",""]
["Unless otherwise described all steel signage to be grade 316 stainless steel plate, plasma cut as per Architect's design. Stainless steel to be sandblasted to create a matt finish. Sample to be prepared for Architects approval.",""]
["HINGES, BOLTS, ETC",""]
["Architect approved:",""]
["Allow an amount of R60 000.00 for all outstanding ironmongery to be specified and approved by the architect","No",{"v":1,"d":"1.00"}]
["Savignac or equally approved :",""]
["Gearbox:",""]
["150mm Restrictor stay (Code: RESTAY 150)","Pairs",{"v":172,"d":"172.00"}]
["Manual reduction gearbox installation for crank operation. Gearbox to be sized according to the door size, to be confirmed by manufacturer","No",{"v":3,"d":"3.00"}]
["Key box:",""]
["Break glass key box wall plugged","No",{"v":4,"d":"4.00"}]
["MATS",""]
["Closed construction primary barrier mat comprising 25mm wide Gadwall nylon wiper inserts in black moulded rubber base with 25mm wide PVC strips laid in mat surround:",""]
["3000 x 1600 x 12mm Thick overall size barrier mat","No",{"v":14,"d":"14.00"}]
["PINNING BOARDS, WHITE BOARDS ETC",""]
["Non-magnetic white boards fixed to walls",""]
["1200 x 3000mm High white board","No",{"v":4,"d":"4.00"}]
["Notice board formed of colour grey or charcoal 9mm thick needlepunch 2.50m wide broadloom carpet with SABS Class 3 fine rating, fibre weight 335g/m2 and total weight 2435g/m2 fixed with adhesive to back board with 20 x 20mm timber surround:",""]
["1854 x 1790mm High notice board","No",{"v":1,"d":"1.00"}]
["CURTAINS:",""]
["Stage curtain:",""]
["Provide the sum of R35 000,00 (Thirty Five Thousand Rand) for stage curtain to fit size 12000 x 4200mm high opening, to be made in fabric and colour to be approved by architect, including medium duty track and hanging over the stage area in the auditorium","Item",{"v":1,"d":"1.00"}]
["Add for profit.","Item",{"v":1,"d":"1.00"}]
["Add for attendance and making good in all trades.","Item",{"v":1,"d":"1.00"}]
["Bead curtain:",""]
["Provide the sum of R120 000,00 (One Hundred and Twenty Thousand Rand) for beaded curtain made by artist and track to suit window W16 (LHW&R)","Item",{"v":1,"d":"1.00"}]
["Add for profit","Item",{"v":1,"d":"1.00"}]
["Add for attendance and making good in all trades","Item",{"v":1,"d":"1.00"}]
["VENETIAN BLINDS",""]
["25mm Wide plain aluminium Venetian blinds as supplied by an approved blind manufacturer fixed to underside of window heads:",""]
["Blind for window type W26 size 2053 x 750mm high","No",{"v":3,"d":"3.00"}]
["Blind for window type W25 size 2552 x 750mm high","No",{"v":12,"d":"12.00"}]
["Blind for window type W06 size 4000 x 4560mm high","No",{"v":1,"d":"1.00"}]
["ROLLER BLINDS",""]
["Sheerweave 4500 roller blinds as supplied by an approved blind manufacturer in colour to be approved by architect, fixed to underside of window head:",""]
["Manually operated blind to fit window size 1340 x 2350mm high","No",{"v":15,"d":"15.00"}]
["Manually operated blind to fit window size 1970 x 753mm high","No",{"v":2,"d":"2.00"}]
["Manually operated blind to fit window size 3750 x 755mm high","No",{"v":1,"d":"1.00"}]
["Manually operated blind split in two parts to fit window size 7213 x 3060mm high, incl. easy lift spring","No",{"v":1,"d":"1.00"}]
["Automated blind to fit window size 2053 x 750mm high, including suitable motor, kit, etc ","No",{"v":3,"d":"3.00"}]
["Automated blind to fit window size 2552 x 750mm high, including suitable motor, kit, etc ","No",{"v":12,"d":"12.00"}]
["Automated blind to fit window size 2830 x 800mm high, including suitable motor, kit, etc ","No",{"v":2,"d":"2.00"}]
["Automated blind to fit window size 3045 x 754mm high, including suitable motor, kit, etc ","No",{"v":5,"d":"5.00"}]
["Automated blind to fit window size 3677 x 800mm high, including suitable motor, kit, etc ","No",{"v":4,"d":"4.00"}]
["Automated blind to fit window size 3963 x 800mm high, including suitable motor, kit, etc ","No",{"v":4,"d":"4.00"}]
["SEATING",""]
["Auditorium seating:",""]
["'Rodlin Design' Wave or other approved 540mm wide high-backed seats, individually floor mounted with automatic fold down mechanism, fully upholstered seat and back with a common polyurethane armrest and an individual fold-away writing tablet including all","No",{"v":250,"d":"250.00"}]
["CATCHES, CABIN HOOKS, ETC",""]
["Manufactured by Halstead",""]
["Pole Hook Brass For Window #131 Halstead fixed with screws on a 4m long hardwood timber pole securely mounted to wall with brass clips","No",{"v":6,"d":"6.00"}]
["LETTERS, NAMEPLATES, SIGNAGE, ETC",""]
["Samples of signs are to be provided to the architects for written approval of all fonts and sized before work commences",""]
["Aluminium Nameplates:",""]
["60 x 100 x 3mm Thick anodised aluminium plate with one 40mm high engraved and painted letter or numeral","No",{"v":1,"d":"1.00"}]
["60 x 450 x 3mm Thick anodised aluminium plate with not exceeding ten 40mm high engraved and painted letters or numerals","No",{"v":1,"d":"1.00"}]
["60 x 500 x 3mm Thick anodised aluminium plate with not exceeding twenty 40mm high engraved and painted letters or numerals","No",{"v":1,"d":"1.00"}]
["Aluminium pictograms:",""]
["150 x 150 x 3mm Thick anodised aluminium plate with male or female symbol","No",{"v":6,"d":"6.00"}]
["150 x 150 x 3mm Thick anodised aluminium plate with paraplegic symbol","No",{"v":1,"d":"1.00"}]
["150 x 150 x 3mm Thick anodised aluminium plate with fire exit symbol","No",{"v":1,"d":"1.00"}]
["Stainless steel pictograms:",""]
["Stainless steel signs to be grade 316 stainless steel plate plasma cut as per Architect's design with stainless steel to be sandblasted to create a matt finish and with samples to be prepared for the architects approval",""]
["152 x 152mm SS5066E-06SS/E01 electrical engraved stainless steel door sign","No",{"v":1,"d":"1.00"}]
["152 x 152mm SSS5066-06SS/E05 fire hose reel stainless steel pictogram","No",{"v":1,"d":"1.00"}]
["152 x 152mm SSS5066-06SS/E06 fire extinguisher stainless steel pictogram","No",{"v":1,"d":"1.00"}]
["Wall mounted single sided photoluminescent signs in SABS 1186 certified ABS plastic plugged with non corrosive screws:",""]
["Type A size 450 x 150mm Fire hose reel, fire extinguisher and arrow sign fixed to and including 6 x 510 x 210mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 71","No",{"v":1,"d":"1.00"}]
["Type B size 300 x 150mm Running man and arrow sign fixed to and including 6 x 360 x 210mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.02 Detail A","No",{"v":1,"d":"1.00"}]
["Type C size 300 x 150mm Fire exit sign fixed to and including 16mm Supawood backing fixed with synthetic rubber based adhesive with Supawood edges painted black, the sign suspended on two 4 x 900mm long stainless steel nautical cables with high grade alum","No",{"v":1,"d":"1.00"}]
["Type D size 450 x 150mm Left arrow, running man and right arrow sign fixed to and including 6 x 510 x 210mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.0","No",{"v":1,"d":"1.00"}]
["Type E size 300 x 150mm Left arrow, running man and right arrow sign fixed to and including 6 x 360 x 210mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.0","No",{"v":1,"d":"1.00"}]
["Type F size 300 x 300mm Environmental control sign fixed to and including 6 x 360 x 360mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.02 Detail C ","No",{"v":1,"d":"1.00"}]
["Type G size 300 x 470mm Environmental control sign fixed to and including 6 x 530 x 360mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.02 Detail D  ","No",{"v":1,"d":"1.00"}]
["Type H size 300 x 150mm Environmental control sign fixed to and including 6 x 360 x 210mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.02 Detail A","No",{"v":1,"d":"1.00"}]
["Type J size 300 x 150mm Environmental control sign fixed to and including 6 x 360 x 210mm perspex cell cast acrylic sheet with four 13 x 15mm long mm diameter through hole stainless steel panel support feet all as per Dwg No 25379 7100.02 Detail A","No",{"v":1,"d":"1.00"}]
["GENERAL FACADE SIGNAGE",""]
["Samples of signs are to be provided to the architects for written approval of all fonts and sized before work commences",""]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 85MM HIGH fixed to wall with 10mm round pins with minimum six pins per sign with pins to be fixed into wall at a minimum depth of 50mm with two component hybrid",""]
["\"toilets\" Sign with 8 x 50mm flat section stainless steel bottom member with arrow, size 1310 x 327mm  high","No",{"v":1,"d":"1.00"}]
["\"reception\" Sign with 8 x 50mm flat section stainless steel bottom member with arrow, size 1342 x 327mm high","No",{"v":1,"d":"1.00"}]
["\"guard house\" Sign with 8 x 50mm flat section stainless steel bottom member with arrow, size 1342 x 327mm high","No",{"v":1,"d":"1.00"}]
["\"administration\" Sign with 8 x 50mm flat section stainless steel bottom member with arrow, size 1342 x 327mm high","No",{"v":1,"d":"1.00"}]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 132MM HIGH  fixed to wall with 8 x 70mm long round pins at 300mm centres with pins to be fixed into wall at a minimum depth of 50mm with two component hybrid mo",""]
["8 x 50mm Flat section stainless steel stiffener fixed to wall at 300mm centres","m",{"v":4,"d":"4.00"}]
["Extra on 8 x 50mm Flat section stainless steel for bend","No",{"v":2,"d":"2.00"}]
["\"gents\" Sign 132mm high","No",{"v":1,"d":"1.00"}]
["\"ladies\" Sign 132mm high","No",{"v":1,"d":"1.00"}]
["\"toilets\" Sign 132mm high","No",{"v":1,"d":"1.00"}]
["\"great place of celebration\" Sign with 8 x 50mm flat section stainless steel bottom member, size 4055 x 132mm high","No",{"v":1,"d":"1.00"}]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 150MM HIGH fixed to wall with 8 x 70mm long round pins at 300mm centres with pins to be fixed into wall at a minimum depth of 50mm with two component hybrid mor",""]
["\"museum\" Sign 150mm  high","No",{"v":1,"d":"1.00"}]
["\"centre of remembrance\" Sign with 8 x 50mm flat section stainless steel bottom member, size 3200 x 150mm  high","No",{"v":1,"d":"1.00"}]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 225mm high fixed to wall with 6mm round pins with minimum three pins per sign with pins to be fixed into wall at a minimum depth of 50mm with two component hybr",""]
["\"yard\" Sign size approximately 731mm long","No",{"v":1,"d":"1.00"}]
["\"kiosk\" Sign size approximately 906mm long","No",{"v":1,"d":"1.00"}]
["\"toilets\" Sign size approximately 1075mm long","No",{"v":2,"d":"2.00"}]
["\"the kraal\" Sign size approximately 1500mm long","No",{"v":1,"d":"1.00"}]
["\"restaurant\" Sign size 1770mm long","No",{"v":1,"d":"1.00"}]
["\"workshops\" Sign size approximately1856mm long","No",{"v":1,"d":"1.00"}]
["\"maintenance\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"classrooms\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"reading room\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"Hao-ai-!khaes\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"Ga-omi\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"U! na-oms\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"Uitsama, Kiosk\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"ii om!na - oms\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"Ama-dib\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"service yard\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"language lab\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["\"multi purpose hall\" Sign 225mm high","No",{"v":1,"d":"1.00"}]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 327MM HIGH fixed to wall with 6mm round pins with minimum three pins per sign with pins to be fixed into wall at a minimum depth of 50mm with two component hybr",""]
["\"reception\" Sign with 8 x 50mm flat section stainless steel bottom member, size 4363 x 327mm  high","No",{"v":1,"d":"1.00"}]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 350MM HIGH fixed to wall with 8 x 70mm long round pins at 300mm centres with pins to be fixed into wall at a minimum depth of 50mm with two component hybrid mor",""]
["\"auditorium\" Sign with 8 x 50mm flat section stainless steel bottom member, size 3585 x 350mm  high","No",{"v":1,"d":"1.00"}]
["8mm Thick sandblasted stainless steel with text plasma cut out with lowercase font Arial Black 400mm HIGH fixed to wall with 8 x 70mm long round pins at 300mm centres with pins to be fixed into wall at a minimum depth of 50mm with two component hybrid mor",""]
["\"Sarah Bartmann Centre of Remembrance\" Sign with 8 x 50mm flat section stainless steel bottom member, size 4760 x 400mm  high","No",{"v":2,"d":"2.00"}]
["15 x 6mm Stainless steel irregularly shaped flat section fixed to wall between plaster finishes as feature with 20 x 20 x 3mm lugs welded on and fixed to brickwork at 300mm centres with expanding bolts:",""]
["Kudu head shaped feature 3350mm high overall all as per detail marked \"Detail B/7100.01: Elevation - male toilets signage\" on Drawing 25379-GP-7100.01","No",{"v":1,"d":"1.00"}]
["Kudu head shaped feature 3350mm high overall all as per detail marked \"Detail C/7100.01: Elevation - female toilets signage\" on Drawing 25379-GP-7100.01","No",{"v":1,"d":"1.00"}]
["Sign backing or feature plates:",""]
["6mm Thick Cor-Ten galvanised mild steel sheeting with epoxy coating finish one side and grey undercoat other side attached to self-compacting concrete walls with 20mm diameter pins at 500mm centres:","m²",{"v":15,"d":"15.00"}]
["10mm Thick corten steel plate size 3165 x 1950mm high with stencil text font type plasma-cut through metal with purpose made 5mm thick metal flat plate channel surround to hold sign plate in place with and including 6mm diameter bolts, nuts and washers as","No",{"v":1,"d":"1.00"}]
["Vinyl decals:",""]
["Provide the sum of R85 000,00 (Eighty Five Thousand Rand) for printable paper backed vinyl decals to be fitted to glass","Item",{"v":1,"d":"1.00"}]
["Add for profit","Item",{"v":1,"d":"1.00"}]
["Add for attendance","Item",{"v":1,"d":"1.00"}]
["Additional signage:",""]
["Allow the sum of R200 000,00 (Two Hundred Thousand Rand) for additional signage to be specified by the architect and to be remeasured on completion at scheduled rates","Item",{"v":1,"d":"1.00"}]
["Add for profit","Item",{"v":1,"d":"1.00"}]
["Add for attendance.","Item",{"v":1,"d":"1.00"}]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["PREAMBLES",""]
["SUPPLEMENTARY PREAMBLES",""]
["Steel type:",""]
["All structural steel to be grade 350W according to SANA 1431. All visible welds to be continuous and ground smooth with all cut edges and holes dressed to remove dross, burrs and irregularities",""]
["Bolts and holding down bolts:",""]
["Unless otherwise described all bolts to be Grade 8,8 chromate passivated electro-galvanised.",""]
["Descriptions of bolts shall be deemed to include nuts and washers.",""]
["Descriptions of L-shaped and U-shaped anchor bolts shall be deemed to include bending, threading, nuts and washers and embedding in concrete.",""]
["Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete.",""]
["Galvanising:",""]
["All exposed structural steelwork,  lipped channels and mild steel gutters are to be hot dip galvanised to SANS  ISO 1461:1999",""]
["GALVANISED STEEL COLUMNS,  BEAMS, ETC",""]
["Welded and bolted lattice trusses comprising angle section chords and internal members:",""]
["Angle section lattice trusses","Tonnes",{"v":6,"d":"6.00"}]
["Welded columns in single lengths with specialist connections:",""]
["Shaped columns built up from 8 x 130mm flat section flanges and 6mm flat plate webs","Tonnes",{"v":4,"d":"4.00"}]
["180 x 91 x 19 kg/m IPE column","Tonnes",1.18]
["152 x 152 x 23 kg/m Universal I-section stub column","Tonnes",1.08]
["200 x 100 x 22 kg/m IPE stub column","Tonnes",2.04]
["200 x 100 x 22 kg/m IPE window posts","Tonnes",1.19]
["203 x 133 x 25 kg/m Universal beam section stub column","Tonnes",1.94]
["305 x 165 x 54 kg/m Universal beam section prop","Tonnes",{"v":1,"d":"1.00"}]
["Welded beams and rafters in single lengths with flat section bearer and connection plates bolted on:",""]
["6 x 75 x 100mm Angle section wall rafter","Tonnes",0.86]
["6 x 75 x 100mm Angle section wall rafter circular on plan","Tonnes",0.28]
["200 x 100 x 22kg/m IPE rafter","Tonnes",{"v":4,"d":"4.00"}]
["200 x 100 x 22kg/m IPE window beams","Tonnes",{"v":2,"d":"2.00"}]
["203 x 133 x 25 kg/m Universal support beam","Tonnes",12.03]
["203 x 133 x 25 kg/m Universal beam with shaped ends as rafter","Tonnes",{"v":2,"d":"2.00"}]
["Round hollow section beams:",""]
["3 x 76mm Diameter round hollow section struts","Tonnes",{"v":1,"d":"1.00"}]
["4 x 127mm Diameter round hollow section  beam","Tonnes",1.45]
["Curved rafters with connectors:",""]
["180 x 91 x 19 kg/m IPE rafter circular on elevation","Tonnes",{"v":3,"d":"3.00"}]
["200 x 100  x 22 kg/m IPE rafter circular on elevation","Tonnes",{"v":7,"d":"7.00"}]
["Pivot joints:",""]
["Pivoting joint between column and beam comprising welded shaped gussets formed of 10mm flat plate sections with one end welded to top of column and other end bolted to roof members with 20mm Grade 8,8 bolt at pivot","Tonnes",1.48]
["GALVANISED PURLINS, GIRTS AND BRACING",""]
["Purlins and girts welded and bolted with angle section cleats:",""]
["25 x 25 x 5mm Angle section flashing angle section welded","Tonnes",{"v":1,"d":"1.00"}]
["50 x 50 x 3mm Angle section false rafter","Tonnes",{"v":1,"d":"1.00"}]
["100 x 50 x 2,5mm Rectangular hollow section purlins","Tonnes",{"v":11,"d":"11.00"}]
["100 x 50 x 2,5mm Rectangular hollow section girts","Tonnes",{"v":1,"d":"1.00"}]
["150 x 75 x 20 x 2.5mm Cold rolled lipped channel section purlins","Tonnes",{"v":6,"d":"6.00"}]
["150 x 75 x 20 x 2.5mm Cold rolled lipped channel section purlins circular on plan","Tonnes",{"v":1,"d":"1.00"}]
["Bracing welded and bolted with angle section cleats:",""]
["2,5 x 76mm Diameter round hollow section bracing","Tonnes",{"v":3,"d":"3.00"}]
["3 x 50 x 50mm Angle section knee bracing","Tonnes",0.18]
["5 x 60 x 60mm Angle section knee bracing","Tonnes",2.28]
["Angle section knee bracing with gussets","Tonnes",{"v":2,"d":"2.00"}]
["WATTLE SCREEN FRAMES",""]
["Galvanised mild steel part circular on elevation wattle screen frames:",""]
["Provide fabricated mock up of wattle frame screen system for the approval of the architect and structural engineer","No",{"v":1,"d":"1.00"}]
["6 x 100mm Mild steel flat bar clamp member circular on elevation","Tonnes",{"v":13,"d":"13.00"}]
["12 x 40mm Mild steel flat bar clamp member circular on elevation","Tonnes",{"v":4,"d":"4.00"}]
["17 x 40 x 100mm Solid mild steel spacer","Tonnes",1.55]
["20mm Diameter mild steel rod welded to posts as stiffener part circular on plan to approximately 2m radius","Tonnes",0.63]
["38 x 76mm Channel section closure member","Tonnes",{"v":4,"d":"4.00"}]
["4 x 50mm Diameter mild steel round hollow section post 2900mm long with one end closed off flush with welded 4mm plate and other end coated for a length of 900mm with bituminous paint and cast into concrete","No",{"v":12,"d":"12.00"}]
["75 x 75 x 5mm Mild steel channel section post 2900mm long with one end closed off flush with welded 4mm plate and other end coated for a length of 900mm with bituminous paint and cast into concrete","No",{"v":14,"d":"14.00"}]
["GALVANISED MILD STEEL GUTTERS AND RAINWATER PIPES",""]
["Laser cut and welded plate, welded at underside of the downpipe with a hole to suit M12 rawl bolt at one end",""]
["6 x 97mm Wide plate laser cut and welded ","Kg",{"v":2,"d":"2.00"}]
["6mm Laser cut and welded plate 308mm girth once bent with a hole to suit M12 rawl bolt at both ends with one end to bolted to the fin (elsewhere measured) and another end bolted into concrete floor",""]
["97mm Wide welded plate","Kg",5.64]
["Welded plate gutters fixed into wall with rawl bolts (elsewhere measured)",""]
["Box gutters 4 x  450mm girth, two times bent along length ","Tonnes",0.02]
["Welded plate rainwater pipes, including holderbats, brackets, etc",""]
["Purpose made 2 x 110mm Diameter pipes fitted with a 90 degree PVC bend (elsewhere measured)","Tonnes",0.04]
["Welded plate formed into U-shaped cover welded to 4 x 30mm mild steel bracket bent twice and epoxy fixed into concrete with 6mm rods",""]
["110mm PVC 90 degree bend\n ","No",{"v":2,"d":"2.00"}]
["2 x 300mm High U-shaped mild steel.","Kg",1.11]
["Extra over 2mm welded plate rainwater pipes for fitting",""]
["BOLTS",""]
["Rawl bolts:",""]
["M12 x 90mm Long.","No",{"v":8,"d":"8.00"}]
["Grade 8,8 chromate passivated electro-galvanised bolts:",""]
["Bolts with nuts and washers","Tonnes",{"v":1,"d":"1.00"}]
["M12 Bolts with nuts and washers","No",{"v":2,"d":"2.00"}]
["Chemical anchors:",""]
["12 x 150mm Long chemical anchor","No",{"v":111,"d":"111.00"}]
["16 x 150mm Long chemical anchor","No",{"v":154,"d":"154.00"}]
["Holding-down bolts:",""]
["16mm U-shaped holding down bolt of 460mm girth including two nuts and four washers","No",{"v":130,"d":"130.00"}]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["PREAMBLES",""]
["Note: Tenderers are specifically referred to Clauses 13.12.4 and 13.12.5 of 'The Specification of Materials and Methods to be used - PW 371' for the material to be used and manufacturing of windows and the written approval of materials and sample window.",""]
["Descriptions of bolts shall be deemed to include nuts and washers.",""]
["Descriptions of expansion anchors and bolts and chemical anchors and bolts shall be deemed to include nuts, washers and mortices in brickwork or concrete.",""]
["Metalwork described as holed for bolts shall be deemed to exclude the bolts unless otherwise described.",""]
["HOT DIP-GALVANISED AFTER MANUFACTURE MILD STEEL SCREENS AND GATES",""]
["Purpose made welded galvanised mild steel screen:",""]
["Duct screen size 500 x 3060mm high overall formed of 20 x 50 x 2mm mild steel hollow section fixed with galvanised self tapping screws on a 50 x 50 x 3mm mild steel angle securely fixed into brickwork with M10 anchor bolt with 30 x 30 x 2mm mild steel ang","No",{"v":1,"d":"1.00"}]
["Duct screen size 580 x 3060mm high overall formed of 20 x 50 x 2mm mild steel hollow section fixed with galvanised self tapping screws on a 50 x 50 x 3mm mild steel angle securely fixed into brickwork with M10 anchor bolt with 30 x 30 x 2mm mild steel ang","No",{"v":1,"d":"1.00"}]
["Duct screen size 820 x 3060mm high overall formed of 20 x 50 x 2mm mild steel hollow section fixed with galvanised self tapping screws on a 50 x 50 x 3mm mild steel angle securely fixed into brickwork with M10 anchor bolt with 30 x 30 x 2mm mild steel ang","No",{"v":1,"d":"1.00"}]
["Screen size 6008 x 2475mm high overall formed of 75x50x3mm welded mild steel hollow sections with an opening section size 1470 x 2470mm high with a frame  of 25 x 50 x 3mm mild steel fixed securely to wall on either side  with brassed M8 expansion bolts i","No",{"v":1,"d":"1.00"}]
["Purpose made welded galvanised mild steel gates:",""]
["Gate size 803 x 3215mm high overall formed of 75x50x3mm welded mild steel hollow sections with a galvanised welded industrial mesh size 50 x 25mm with 2mm thick wire with a frame  of 25 x 50 x 3mm mild steel fixed securely to wall on either side  with bra","No",{"v":1,"d":"1.00"}]
["Gate size 1000 x 1800mm high formed of 75 x 50 x 3mm mild steel rectangular hollow profile welded together to form gate main frame with 10 x 10mm solid square mild steel profile to form beading around mesh on either side and spot welded into position as p","No",{"v":2,"d":"2.00"}]
["Gate size 1200mm x 2790mm with 25 x 50 x 3mm mild steel frame fixed to wall all as G01 at GREAT PLACE","No",{"v":1,"d":"1.00"}]
["Gate size 1470 x 2475mm high formed of 75 x 50 x 3mm mild steel rectangular hollow profile welded together to form gate main frame with 10 x 10mm solid square mild steel profile and spot welded into position at LIVING HERITAGE","No",{"v":1,"d":"1.00"}]
["Gates size 1710 x 2292mm high, with frame size 50 x 75 x 2mm rectangular hollow section gate frame, with galvanised welded industrial mesh size 50 x 25mm with 2mm thick wire size 680 x 589 high ( 6 NO) and including hinges, and 20mm diameter solid round t","No",{"v":1,"d":"1.00"}]
["Gate size 1664 x 2125 mm in two leaves with 25 x 75 x 2mm mild steel frame fixed to wall all marked as G02 at GREAT PLACE","No",{"v":1,"d":"1.00"}]
["Gate size 2900 x 1915mm high formed of 2mm mild steel rectangular flat metal sheet with plasma cut aperture with 10mm diameter solid round pins securely welded to gate surround and to handle formed of 20mm diameter mild steel complete with 50 x 25 x 2mm r","No",{"v":1,"d":"1.00"}]
["Gate size 2900 x 3122mm high formed of 2mm mild steel rectangular flat metal sheet with plasma cut aperture with 10mm diameter solid round pins securely welded to gate surround and to handle formed of 20mm diameter mild steel complete with 50 x 25 x 2mm r","No",{"v":1,"d":"1.00"}]
["Sliding gate size 3000 x 2115mm with 200 x 75mm open channel attached to concrete and gate with a 110 x 10mm flat plate; gate comprising 50 x 100mm surround; 10 x 25mm horizontal flat bars welded on at 110mm centres and 10mm diameter vertical rods threade","No",{"v":1,"d":"1.00"}]
["Sliding gate size 3000 x 2115mm with 200 x 75mm open channel attached to concrete and gate with a 110 x 10mm flat plate; gate comprising 50 x 100mm surround; 10 x 25mm horizontal flat bars welded on at 110mm centres and 10mm diameter vertical rods threade","No",{"v":1,"d":"1.00"}]
["Gate size 3465 x 2945mm high formed of 2mm mild steel rectangular flat metal sheet with plasma cut aperture with 10mm diameter solid round pins securely welded to gate surround and to handle formed of 20mm diameter mild steel complete with 50 x 100 x 2mm ","No",{"v":1,"d":"1.00"}]
["Top hung sliding gate size 3465 x 2945  with overhead track enclosed by 100 x 6mm flat plate attached to top of I beam; gate comprising 120 x 60mm surround; front and back 4mm steel flat plates pop riveted to frame with plasma cut out text; 40 x 10mm hori","No",{"v":1,"d":"1.00"}]
["Gate size 4400 x 2410mm high formed of 50 x 100mm mild steel rectangular hollow section surround with 10mm diameter rods with flat bars securely welded with a seamless weld at connections as per marked detail G01 on Drawing no 25379-EDUC-3300.01","No",{"v":1,"d":"1.00"}]
["Gate size 5400 x 2410mm high formed of 50 x 100mm mild steel rectangular hollow section surround with 10mm diameter rods with flat bars securely welded with a seamless weld at connections as per marked detail G02 on Drawing 25379-EDUC-3300.01","No",{"v":1,"d":"1.00"}]
["HOT DIP-GALVANIZED STEEL TRANSFORMER ROOM DOORS AND FRAMES",""]
["MV Type transformer doors:",""]
["Approved MV Type steel transformer room door and frame unit including vent with one shop coat red oxide, with door size 1524 x 2125mm high D24 at AUDITORIUM","No",{"v":2,"d":"2.00"}]
["Approved MV type steel transformer room unit including vent with door size 1524 x2085mm high, complete with frame, with no glazing as per detail marked D07 on the drawing DORM 3200.02","No",{"v":1,"d":"1.00"}]
["Durowin MV or other approved galvanised mild steel transformer room double door and frame unit with vent in both leaves, size 1524 x 2495high to suit wall 230mm thick  as per detail marked D11 at LIVING HERITAGE","No",{"v":1,"d":"1.00"}]
["Durowin M.V type steel transformer room unit including vent with door size 2480 x 2125mm high complete with frame, with NO glazing, as per detail marked D25 on the drawing EDUC 3200.05","No",{"v":1,"d":"1.00"}]
["Hot dipped galvanised substation transformer room door size 2500 x 2550 in two equal leaves and two fixed side panels(with ventilation panel comprising 2.5 mm louvred strips and vermin proof backing with 1.2 mm solid steel slats, cabin hooks, earth strap,","No",{"v":1,"d":"1.00"}]
["Substation transformer room door size 5500 x 2510mm high comprising one panel  size 1770 x 2085mm door and 1815 x 2085mm fixed louvre panels in two equal leaves with ventilation panel made comprising 2,5mm louvred strips and vermin proof backing, with 1,2","No",{"v":1,"d":"1.00"}]
["Substation transformer room door in two equal leaves and two fixed side louvre panels, size 5500 x 2085mm high, with ventilation panel comprising 2.5mm louvred strips and vermin proof backing, with 1.2mm solid steel slats, cabin hooks, earth strap, shooti","No",{"v":1,"d":"1.00"}]
["Hot dipped galvanised substation transformer room door size 6023 x 2510 in two equal leaves and two fixed side panels (with ventilation panel comprising 2.5mm louvred strips and vermin proof backing with 1.2mm solid steel slats, cabin hooks, earth strap, ","No",{"v":1,"d":"1.00"}]
["STEEL HANDRAILS, BALUSTRADES, ETC",""]
["GALVANISED STEEL HANDRAILS",""]
["Galvanised mild steel handrails",""]
["20 x 50 x 2mm Hollow section rectangular tubing with 14mm solid mild steel pin of 291mm girth at equal centres bent to form 90 degree angle with one end welded to the hollow section and another end fixed into wall with cement based epoxy as per Architect ","m",1.97]
["GALVANISED  MILD STEEL  BALUSTRADES",""]
["Galvanised mild steel welded balustrades:",""]
["Balustrade size 1866 x 1000mm high formed of 50 x 12mm mild steel flat bar to form handrail securely welded to  50 x 8mm uprights with a neat seamless weld complete with a 12 x 50mm mild steel flat bar securely welded to baluster uprights fixed into concr","No",{"v":2,"d":"2.00"}]
["Balustrade size 2347 x 1000mm high overall formed of 20 x 50 x 2mm mild steel hollow section rectangular tubing to form handrail and bottom rail securely welded to  20 x 50 x 2mm uprights at 1143mm centres with the bottom of the upright a neatly seamless ","No",{"v":1,"d":"1.00"}]
["Balustrade size 2400 x 1000mm high overall formed of 20 x 50 x 2mm mild steel hollow section rectangular tubing to form handrail securely welded to  20 x 50 x 2mm uprights at 1170mm centres with a neat seamless weld to 8mm mild steel baseplate fixed to co","No",{"v":4,"d":"4.00"}]
["Balustrade size 2500 x 1005mm high formed of 50 x 12mm mild steel flat bar to form handrail securely welded to  50 x 8mm uprights with a neat seamless weld complete with a 12 x 50mm mild steel flat bar securely welded to baluster uprights fixed into concr","No",{"v":5,"d":"5.00"}]
["Balustrade size 2834 x 1000mm high formed of various sizes of mild steel flat bar welded back to front along 8 x 20mm horizontal mild steel flat bars to form panels securely welded to  50 x 8mm uprights with a neat seamless weld complete with a 12 x 50mm ","No",{"v":1,"d":"1.00"}]
["Balustrade size 3703 x 1000mm high formed of various sizes of mild steel flat bar welded back to front along 8 x 20mm horizontal mild steel flat bars to form panels securely welded to  50 x 8mm uprights with a neat seamless weld complete with a 12 x 50mm ","No",{"v":1,"d":"1.00"}]
["Balustrade size 4490 x 1000mm high overall formed of 20 x 50 x 2mm mild steel hollow section rectangular tubing to form handrail and bottom rail securely welded to  20 x 50 x 2mm uprights at 1098mm centres with the bottom of the upright a neatly seamless ","No",{"v":1,"d":"1.00"}]
["Balustrade size 6690 x 1000mm high overall formed of 25 x 50 x 3mm mild steel rectangular section top rail with 50 x 25 x 3mm mild steel rectangular section upright welded to the toprail by cutting a V- joint into the top of the upright laser weld into re","No",{"v":1,"d":"1.00"}]
["Balustrade size 6925 x 1000mm high formed of various sizes of mild steel flat bar welded back to front along 8 x 20mm horizontal mild steel flat bars to form panels securely welded to  50 x 8mm uprights with a neat seamless weld complete with a 12 x 50mm ","No",{"v":1,"d":"1.00"}]
["GALVANISED MILD STEEL GLAZED SKYLIGHTS",""]
["Mild steel safety glazed skylight to be constructed in accordance with AAAMSA performance criteria class designation A2 and architects drawings",""]
["Galvanised mild steel safety glazed skylight to be constructed from clear (PVB) single glazed 6,38mm thick laminated glass with steel frame to be polyester powder coated (50-100 microns thick) including flashing and counter flashing, condensation outlets ",""]
["Double glazed skylight size 900 x 3500mm with glass slope to follow style of lean-to","No",{"v":1,"d":"1.00"}]
["HOT DIP-GALVANISED AFTER MANUFACTURE MILD STEEL BALUSTRADES",""]
["Welded balustrades to ramps",""]
["50 x 12mm Flat section continuous middle and bottom rails","Kg",{"v":2300,"d":"2300.00"}]
["Extra over for mitred L-intersection","No",{"v":15,"d":"15.00"}]
["Extra over for ramp or knee","No",{"v":24,"d":"24.00"}]
["50 x 8mm Flat section balusters","Kg",{"v":1980,"d":"1980.00"}]
["Extra over for T-intersection","No",{"v":32,"d":"32.00"}]
["20 x 18mm Flat section balusters","Kg",{"v":566,"d":"566.00"}]
["Extra over for T-intersection.","No",{"v":24,"d":"24.00"}]
["Extra over for irregular T-intersection","No",{"v":4,"d":"4.00"}]
["125 x 75 x 10mm Fixing plate twice holed for bolt(s) and welded on","No",{"v":13,"d":"13.00"}]
["60 mm External diameter x 2,8 mm thick continuous pipe handrails","m",{"v":13,"d":"13.00"}]
["Extra over for rounded closed end","No",{"v":4,"d":"4.00"}]
["10 mm Expansion bolt","No",{"v":52,"d":"52.00"}]
["MODULAR CEILING FRAMES",""]
["The following in modular panel ceiling comprising galvanised hot dipped mild steel support channels and angle section frames for plywood panels with timber stiffeners with hand woven wattle reed mat fixed beneath (timberwork measured elsewhere) all as per",""]
["25 x 25 x 2mm Angle section trim screwed with self tapping screws at 300mm centres to structural steelwork","Kg",{"v":52,"d":"52.00"}]
["50 x 75 x 4mm Angle section surround bolted to structural steelwork","Kg",{"v":258,"d":"258.00"}]
["50 x 3mm Flat section purlin lug welded on","Kg",{"v":34,"d":"34.00"}]
["50 x 50 x 3mm Angle section surround screwed with self tapping screws at 300mm centres to structural steelwork","Kg",{"v":1020,"d":"1020.00"}]
["150 x 75 x20 x 2,5mm Lipped channel section ceiling supports","Kg",{"v":416,"d":"416.00"}]
["220 x 6mm Thick flat plate as closure","Kg",{"v":75,"d":"75.00"}]
["12mm Diameter Grade 8.8 bolts","Kg",{"v":120,"d":"120.00"}]
["The following in modular panel ceiling comprising hot dipped galvanised mild steel hollow section frames and flat section supports for slatted timber panels (timberwork measured elsewhere) all as per architects Drawings no 25379-MUS-4500.01 and 4500.03:",""]
["120 x 60 x 2mm Hollow section framing with welded lugs","Kg",{"v":1015,"d":"1015.00"}]
["120 x 60 x 2mm Hollow section framing with welded lugs circular on plan","Kg",{"v":25,"d":"25.00"}]
["50 x 6mm Flat section plate welded on as support","Kg",{"v":68,"d":"68.00"}]
["30 x 50 x 6mm Flat section lugs welded on","Kg",{"v":4,"d":"4.00"}]
["60 x 50 x 12mm Flat section lugs welded on","Kg",{"v":4,"d":"4.00"}]
["10mm Thick stainless steel nautical cables","m",{"v":27,"d":"27.00"}]
["Stainless steel loop clamp to suit 10mm thick cable","No",{"v":30,"d":"30.00"}]
["20 x 200mm Open eye chemical anchor bolt including forming 150mm deep mortice in concrete","No",{"v":15,"d":"15.00"}]
["HOT DIP-GALVANISED SCREENS",""]
["Latticework screens:",""]
["10 x 10mm Square section mild steel bars","Kg",{"v":120,"d":"120.00"}]
["20mm Diameter round bars woven to form lattice work","Kg",{"v":280,"d":"280.00"}]
["50 x 50 x 3mm Angle section framing","Kg",{"v":523,"d":"523.00"}]
["180 x 91 IPE curved rafters","Kg",{"v":633,"d":"633.00"}]
["SCREENS",""]
["The following in galvanised mild steel modular ceiling panels with steel to be grade 350W according to SANS 1431:",""]
["Reed mat ceiling frame","m²",{"v":164,"d":"164.00"}]
["The following in support to wattle lath as roof covering feature to Guard House:",""]
["4mm Stainless steel cable","m",{"v":15,"d":"15.00"}]
["12 x 120mm Galvanised mild steel hook anchor expanding bolt with one end fixed to concrete","m",{"v":10,"d":"10.00"}]
["WIND MOBILE",""]
["The following in wind mobile formed of Corten steel all as per architects details marked 25379-GP-3700.02 and 3700.03:",""]
["Beam formed of two 203 x 103 x 25 Kg/m Corten steel I-beams with end plates, cross plates and 15mm solid round bars welded on including holing","Kg",{"v":420,"d":"420.00"}]
["10 x 322mm Girth top hook threaded for and including 50mm threaded coupling and heavy weight stainless steel karabiner self closing clip","No",{"v":5,"d":"5.00"}]
["12 x 150mm Expansion bolts","No",{"v":19,"d":"19.00"}]
["100 x 3 x 1572mm Long round hollow section pipe with 10mm diameter holes randomly spaced","No",{"v":5,"d":"5.00"}]
["100 x 3 x 1572mm Long round hollow section pipe with engraving","No",{"v":10,"d":"10.00"}]
["Set of hanging members of mobile size 6000 x 1875mm high overall comprising pipes, flatbars, rods, etc. with engraving, holes, etc. including 10 x 322mm Girth top hooks threaded for and including 50mm threaded coupling and heavy weight stainless steel kar","No",{"v":1,"d":"1.00"}]
["COVER AND SEALING STRIPS",""]
["Welded polished stainless steel:",""]
["4x40mm polished stainless steel flat bar bend to edge indicated on floor plan, welded 40x40x4mm lugs at 300mm centers and fixed to concrete surface stair with brass self-expanding screws","m",{"v":155,"d":"155.00"}]
["6x130mm polished stainless steel plate with plasma cut vents, circular on plan with 6x30mm stainless steel flat section with  lugs welded along two edges on the underside of the plate, all as per detail k / 4000.03 plan on drawing 25379-EDUC 4000.03","m",{"v":78,"d":"78.00"}]
["Welded mild steel dividing strip:",""]
["3 x 50mm Flat bar dividing strip fixed into top of concrete surface beds and screed with adhesive","m",{"v":32,"d":"32.00"}]
["4 x 40mm Flat bar with 40 x 40 x 4mm lugs at 300mm centers welded to flat bar along length of the strip","m",{"v":62,"d":"62.00"}]
["4 x 40mm Flat bar circular on plan, with welded 40 x 40 x 4mm lugs at 300mm centers along length of the strip","m",{"v":447,"d":"447.00"}]
["4 x 40 x 40mm Angle fixed into top of concrete surface with 4 x 50 x 50mm lugs at 300 centres welded to flat bar and with 4mm rubber packing fixed to steel","m",{"v":626,"d":"626.00"}]
["Natural anodised aluminium dividing strip:",""]
["3 x 40mm High aluminium flat bar dividing strip  fixed in position with adhesive","m",{"v":47,"d":"47.00"}]
["3 x 50mm High aluminium flat bar dividing strip  fixed in position with adhesive","m",{"v":6,"d":"6.00"}]
["GALVANISED STEEL GATES, SCREENS, ETC",""]
["Powder coated matt umber grey welded burglar bars of 8 x 8mm square solid horizontal bars welded at 100mm centres onto two vertical 25 x 3mm flat bars on each side and to be screwed/ rivited onto aluminium frame through holes (No.4) on the flat bars.",""]
["Note: Contractor to check the sizes of windows before ordering or making burglar bars",""]
["Size 400 x 579mm high","No",{"v":4,"d":"4.00"}]
["Size 600 x 565mm high","No",{"v":2,"d":"2.00"}]
["Size 600 x 1060mm high","No",{"v":2,"d":"2.00"}]
["Size 600 x 1303mm high","No",{"v":4,"d":"4.00"}]
["Size 600 x 1345mm high","No",{"v":8,"d":"8.00"}]
["Size 688 x 1414mm high","No",{"v":11,"d":"11.00"}]
["Size 713 x 1414mm high","No",{"v":2,"d":"2.00"}]
["Size 725 x 1466mm high","No",{"v":1,"d":"1.00"}]
["Size 744 x 854mm high","No",{"v":1,"d":"1.00"}]
["Size 750 x 1128mm high","No",{"v":1,"d":"1.00"}]
["Size 750 x 1151mm high","No",{"v":1,"d":"1.00"}]
["Size 763 x 1414mm high","No",{"v":1,"d":"1.00"}]
["Size 775 x 1644mm high","No",{"v":1,"d":"1.00"}]
["Size 775 x 1669mm high","No",{"v":2,"d":"2.00"}]
["Size 775 x 1869mm high","No",{"v":2,"d":"2.00"}]
["Size 775 x 1894mm high","No",{"v":2,"d":"2.00"}]
["Size 806 x 1414mm high","No",{"v":4,"d":"4.00"}]
["Size 811 x 1466mm high","No",{"v":2,"d":"2.00"}]
["Size 818 x 770mm high","No",{"v":1,"d":"1.00"}]
["Size 818 x 1490mm high","No",{"v":1,"d":"1.00"}]
["Size 820 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 820 x 1414mm high","No",{"v":2,"d":"2.00"}]
["Size 820 x 1417mm high","No",{"v":1,"d":"1.00"}]
["Size 822 x 707mm high","No",{"v":18,"d":"18.00"}]
["Size 825 x 707mm high","No",{"v":18,"d":"18.00"}]
["Size 827 x 733mm high","No",{"v":4,"d":"4.00"}]
["Size 836 x 707mm high","No",{"v":16,"d":"16.00"}]
["Size 845 x 1414mm high","No",{"v":8,"d":"8.00"}]
["Size 852 x 770mm high","No",{"v":1,"d":"1.00"}]
["Size 852 x 1750mm high","No",{"v":1,"d":"1.00"}]
["Size 853 x 707mm high","No",{"v":1,"d":"1.00"}]
["Size 900 x 712mm high","No",{"v":4,"d":"4.00"}]
["Size 916 x 835mm high","No",{"v":1,"d":"1.00"}]
["Size 925 x 619mm high","No",{"v":1,"d":"1.00"}]
["Size 935 x 1065mm high","No",{"v":2,"d":"2.00"}]
["Size 940 x 835mm high","No",{"v":2,"d":"2.00"}]
["Size 949 x 1608mm high","No",{"v":2,"d":"2.00"}]
["Size 957 x 1296mm high","No",{"v":2,"d":"2.00"}]
["Size 966 x 1085mm high","No",{"v":1,"d":"1.00"}]
["Size 973 x 707mm high","No",{"v":2,"d":"2.00"}]
["Size 974 x 708mm high","No",{"v":4,"d":"4.00"}]
["Size 974 x 709mm high","No",{"v":4,"d":"4.00"}]
["Size 974 x 880mm high","No",{"v":4,"d":"4.00"}]
["Size 975 x 707mm high","No",{"v":8,"d":"8.00"}]
["Size 976 x 707mm high","No",{"v":4,"d":"4.00"}]
["Size 999 x 708mm high","No",{"v":1,"d":"1.00"}]
["Size 999 x 709mm high","No",{"v":10,"d":"10.00"}]
["Size 999 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 1000 x 680mm high","No",{"v":2,"d":"2.00"}]
["Size 1000 x 687mm high","No",{"v":3,"d":"3.00"}]
["Size 1000 x 707mm high","No",{"v":6,"d":"6.00"}]
["Size 1000 x 712mm high","No",{"v":3,"d":"3.00"}]
["Size 1000 x 733mm high","No",{"v":2,"d":"2.00"}]
["Size 1000 x 770mm high","No",{"v":2,"d":"2.00"}]
["Size 1000 x 795mm high","No",{"v":1,"d":"1.00"}]
["Size 1000 x 820mm high","No",{"v":1,"d":"1.00"}]
["Size 1000 x 835mm high","No",{"v":3,"d":"3.00"}]
["Size 1000 x 1303mm high","No",{"v":2,"d":"2.00"}]
["Size 1025 x 707mm high","No",{"v":1,"d":"1.00"}]
["Size 1065 x 1222mm high","No",{"v":1,"d":"1.00"}]
["Size 1065 x 1247mm high","No",{"v":1,"d":"1.00"}]
["Size 1103 x 707mm high","No",{"v":4,"d":"4.00"}]
["Size 1125 x 565mm high","No",{"v":2,"d":"2.00"}]
["Size 1164 x 600mm high","No",{"v":2,"d":"2.00"}]
["Size 1200 x 565mm high","No",{"v":1,"d":"1.00"}]
["Size 1200 x 737mm high","No",{"v":2,"d":"2.00"}]
["Size 1200 x 795mm high","No",{"v":1,"d":"1.00"}]
["Size 1200 x 820mm high","No",{"v":1,"d":"1.00"}]
["Size 1200 x 1135mm high","No",{"v":1,"d":"1.00"}]
["Size 1200 x 1160mm high","No",{"v":1,"d":"1.00"}]
["Size 1233 x 775mm high","No",{"v":1,"d":"1.00"}]
["Size 1250 x 600mm high","No",{"v":4,"d":"4.00"}]
["Size 1258 x 775mm high","No",{"v":2,"d":"2.00"}]
["Size 1280 x 600mm high","No",{"v":4,"d":"4.00"}]
["Size 1333 x 565mm high","No",{"v":3,"d":"3.00"}]
["Size 1340 x 707mm high","No",{"v":30,"d":"30.00"}]
["Size 1340 x 733mm high","No",{"v":15,"d":"15.00"}]
["Size 1366 x 565mm high","No",{"v":3,"d":"3.00"}]
["Size 1366 x 619mm high","No",{"v":1,"d":"1.00"}]
["Size 1371 x 695mm high","No",{"v":2,"d":"2.00"}]
["Size 1375 x 880mm high","No",{"v":2,"d":"2.00"}]
["Size 1375 x 1417mm high","No",{"v":2,"d":"2.00"}]
["Size 1395 x 854mm high","No",{"v":1,"d":"1.00"}]
["Size 1471 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 1506 x 957mm high","No",{"v":3,"d":"3.00"}]
["Size 1506 x 1065mm high","No",{"v":2,"d":"2.00"}]
["Size 1506 x 2022mm high","No",{"v":2,"d":"2.00"}]
["Size 1520 x 600mm high","No",{"v":1,"d":"1.00"}]
["Size 1565 x 600mm high","No",{"v":2,"d":"2.00"}]
["Size 1647 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 1647 x 1417mm high","No",{"v":1,"d":"1.00"}]
["Size 1670 x 600mm high","No",{"v":2,"d":"2.00"}]
["Size 1870 x 957mm high","No",{"v":1,"d":"1.00"}]
["Size 1871 x 957mm high","No",{"v":1,"d":"1.00"}]
["Size 1875 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 1900 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 1926 x 880mm high","No",{"v":4,"d":"4.00"}]
["Size 1946 x 880mm high","No",{"v":1,"d":"1.00"}]
["Size 1970 x 733mm high","No",{"v":2,"d":"2.00"}]
["Size 2471 x 1417mm high","No",{"v":1,"d":"1.00"}]
["Size 4064 x 2180mm high","No",{"v":1,"d":"1.00"}]
["Size 4519 x 830mm high","No",{"v":1,"d":"1.00"}]
["Size 5000 x 600mm high","No",{"v":1,"d":"1.00"}]
["Size 5199 x 830mm high","No",{"v":3,"d":"3.00"}]
["Size 5872 x 830mm high","No",{"v":2,"d":"2.00"}]
["Size 6095 x 854mm high","No",{"v":2,"d":"2.00"}]
["Powder coated Type 2 matt umber grey Filligree screens made with 50 x 50mm square tubing frame modules with 50 x 50 x 2mm aluminium frame membersfixed vertically to aluminim window frame.",""]
["Size 1981 x 400mm high","No",{"v":8,"d":"8.00"}]
["Size 8526 x 1166mm high","No",{"v":5,"d":"5.00"}]
["GALVANISED MILD STEEL MINOR WORK",""]
["30mm Wide link galvanised chain","m",107.46]
["50 x 50 x 3mm thick mild steel angle with 100 x 50 x 3mm lugs fixed into concrete","m",81.18]
["Galvanised chain with a link width of 30mm secured at the top on mountaineering clip on M6 bolt and nut (elsewhere measured) and secured at the bottom with eye expansion bolt  (elsewhere measured) with mountaineering clip.",""]
["Mid link or equally approved zinc-plated general purpose utility chain 37mm wide with inside link length of 40mm and chain wall of 10mm secure at the top on a mountaineering clip on M6 bolt and nut (elsewhere measured) and hooked at the bottom on a hook a",""]
["10mm Zinc-plated chain","m",{"v":50.4,"d":"50.40"}]
["Welded hollow pipe 350mm long, cut away  in front to form spout with a 4 x 50 x 30mm plate welded to underside of pipe to form connection bracket and drip with a 4 x 200mm diameter backplate four times holed and epoxy fixed into wall with  6mm solid round",""]
["2.5 x 127mm Spigot (Type 02)","No",{"v":34,"d":"34.00"}]
["Welded hollow pipe 450mm long, cut away  in front to form spout with a 2.5 X 75mm diameter pipe seam welded to the underside of  the larger pipe with two holes to suit M6 bolt pin and nut  for a mountaineering clip to secure galvanised  chain with a link ",""]
["2.5 x 127mm Spigot (Type 01)","No",{"v":33,"d":"33.00"}]
["Bolts",""]
["M5 x 55mm Long eye expansion bolt","No",{"v":93,"d":"93.00"}]
["M12 x 90mm Long eye expansion bolt","No",{"v":26,"d":"26.00"}]
["M6 x 90mm Long bolt and nut with washer","No",{"v":26,"d":"26.00"}]
["ALUMINIUM MINOR WORK",""]
["Aluminium brushweld to door ","m",11.48]
["STAINLESS STEEL MINOR WORK",""]
["Plates",""]
["4mm thick stainless steel plate Type 01 290mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 02 1375mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["4mm thick stainless steel plate Type 03 415mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 04 1460mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["4mm thick stainless steel plate Type 05 645mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 06 1545mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["4mm thick stainless steel plate Type 07 885mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 08 1635mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["4mm thick stainless steel plate Type 09 1125mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 10 1720mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["4mm thick stainless steel plate Type 11 1355mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 12 1810mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["4mm thick stainless steel plate Type 13 1635mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":2,"d":"2.00"}]
["4mm thick stainless steel plate Type 14 1915mm as per drawing 25379-NC-EDUC 4000.03_Rev01 bent to form unequal angles fixed to screed with 8mm fischer plugs at 300mm centres with apertures in plate for ventilation","No",{"v":6,"d":"6.00"}]
["CHROMADEK ROLLER DOORS ETC",""]
["'Starck Chromadek Deluxe' manually operated roller doors including ironmongery, centre lift lock, guide rails, springs, rubber weather strip to bottom, etc. and 'Chromadek' finish",""]
["Steel roll-up garage door with Chromadek finish, size 2440 x 2085mm high, to suit daylight opening, including locks, handles, Roll-A-Guides, hinges, fixing bolts, tracks etc., fixed to brickwork or concrete with a minimum of 100mm sideroom and 350mm headr","No",{"v":1,"d":"1.00"}]
["KITCHEN FITTINGS",""]
["Stainless steel catering fittings:",""]
["Free standing table 1,2mm Grade 304 18/10 stainless steel table, size 1650 x 700 x 4050mm high with 50 x 10mm turndown with stainless steel slatted undershelf size 1650 x 420mm wide, supported on detachable Grade 304 (18/10) stainless steel round legs.","No",{"v":3,"d":"3.00"}]
["MILD STEEL SUNDRIES:",""]
["Stormwater trench covers",""]
["6mm mild steel plate with slots plasma cut welded to 30 x 30 x 2mm mild steel tubing, including 40 x 40 x 2mm mild steel angle fixed to both sides",""]
["2400 x 310mm fixed to concrete","No",{"v":6,"d":"6.00"}]
["2400 x 400mm fixed to concrete","No",{"v":20,"d":"20.00"}]
["Galvanised vanity top supports:",""]
["8 x 100mm Flat mild steel shaped to form front edge restraint of vanity top with 25 x 4 x 150mm long lugs welded on at 400mm centres","Kg",{"v":27,"d":"27.00"}]
["8 x 100mm Flat mild steel to form front edge restraint of vanity top circular on plan with 25 x 4 x 150mm long lugs welded on at 400mm centres","Kg",{"v":3,"d":"3.00"}]
["Mild steel worktop frame and permanent shutter for concrete worktop size 76 x 968 x 5804mm long formed from 6 x 75 x 75mm galvanised mild steel frame with 2mm thick mild steel sheet metal plate at bottom as per detail on drawing no 25379-REC 7000.01","No",{"v":1,"d":"1.00"}]
["Expanded metal mesh sheet to cover Vitex W81RZ or similar approved (40SWM x 115LWM, 4.5 x 4.5 strand) fixed with M10 bolts, nuts and washers at 300mm centres","m²",{"v":21,"d":"21.00"}]
["Galvanised bench supports:",""]
["Flat section surrounds and rails welded at intersections","Kg",{"v":610,"d":"610.00"}]
["10mm Threaded bar with nuts and washers","Kg",{"v":9,"d":"9.00"}]
["Powder coated galvanised I-beams with angle cleats:",""]
["100 x 200mm I-beam with both ends built approximately 500mm deep into brickwork.","Kg",{"v":1049,"d":"1049.00"}]
["Powder coated galvanised angle sections as shopfront stiffeners:",""]
["90 x 90 x 6mm Angle section cleats.","Kg",{"v":7,"d":"7.00"}]
["100 x 100 x 5mm Angle section.","Kg",{"v":27,"d":"27.00"}]
["M16 x 60mm long Grade 8,8 bolt including nut and two washers.","No",{"v":4,"d":"4.00"}]
["M16 x 100mm long chemical anchor bolt including nut and two washers.","No",{"v":4,"d":"4.00"}]
["Gas external fire:",""]
["Take from store and fit gas eternal fire complete formed of 15mm thick solid circular Corten steel rod welded to 50 x 6mm flat bar legs and supported with 4 additional 10mm diameter solid circular pins with and including 6mm thick removable lid with downs","No",{"v":1,"d":"1.00"}]
["ALUMINIUM WINDOWS",""]
["Purpose made 80 micron powder coated (for architectural applications, applied by a certified mark holder of SANS 1578, SANS 1796 and SANS 1651) aluminium windows constructed to withstand wind pressures of 1500Pa (in accordance with SANS 613, related SABS ",""]
["Aluminium window, size 600 x 1345mm high with side hung opening sections and stainless steel concealed friction stays, as per detail marked W10 at Living Heritage as per drawing number 25379 - LHW & R 3100.02","No",{"v":8,"d":"8.00"}]
["Aluminium window, size 981 x 3686mm high suitable for acoustic glazing, glazed with 6mm LAMINATED glass with 100mm cavity between the two sheets of glazing, as per detail marked W27 on drawing EDUCATION 3100.06","No",{"v":1,"d":"1.00"}]
["Aluminium window, size 1000 x 565mm high with top hung opening sections and stainless steel concealed friction stays, marked W12 at AUDITORIUM","No",{"v":1,"d":"1.00"}]
["Aluminium window, size 1398 x 3535mm high with top hung opening sections and stainless steel concealed friction stays, as per detail marked W09 at MUSEUM","No",{"v":1,"d":"1.00"}]
["Aluminium window, size 1398 x 3535mm high with top hung opening sections and stainless steel concealed friction stays, as per detail marked W10 at MUSEUM","No",{"v":1,"d":"1.00"}]
["Aluminium window, size 2053 x 750mm high, with NO opening sections, glazed with 6.76mm SOUNDPRUFE glazing, as per detail marked W26 on drawing EDUC 3100.06.","No",{"v":3,"d":"3.00"}]
["Aluminium window, size 3280 x 854mm high with opening sections and stainless steel concealed friction stays, as per detail marked W21 as per drawing no 25379 - LHW & R 3100.05","No",{"v":2,"d":"2.00"}]
["Aluminium window, size 3677 x 800mm high with centre pivot opening sections and stainless steel concealed friction stays, as per detail marked W18 at MUSEUM","No",{"v":4,"d":"4.00"}]
["Aluminium window, size 3686 x 921mm high with centre pivot opening sections and stainless steel concealed friction stays, as per detail marked W27 at EDUCATION","No",{"v":1,"d":"1.00"}]
["Aluminium window, size 3980 x 3020mm high, with top hung opening sections and concealed friction stays, glazed with 6mm OBSCURE glazing, as per detail marked W10 on drawing EDUC 3100.03.","No",{"v":1,"d":"1.00"}]
["Aluminium window size 3980 x 3060mm with side hung and top hung opening sections and steel concealed friction stays, as per architects drawing 25379-EDUC-3100.03 marked W10","No",{"v":1,"d":"1.00"}]
["Aluminium window, size 5280 x 565mm high with horizontal pivot opening section, marked W11 at AUDITORIUM","No",{"v":1,"d":"1.00"}]
["Aluminium window size 5484 x 3060mm with side hung and top hung opening sections and steel concealed friction stays, as per architects drawing 25379-EDUC 3100.02 marked W05","No",{"v":1,"d":"1.00"}]
["GLAZED ALUMINIUM DOORS",""]
["Aluminium doors, etc., are to be constructed and installed in accordance with the guidelines of The Association of Architectural Aluminium Manufactures of South Africa (AAAMSA). Unless otherwise stated ironmongery is to be the manufacturer's standard corr",""]
["AAAMSA test certificates:",""]
["Each door is to be marked with the mark and number of test certificate issued by AAAMSA.",""]
["Opening sizes:",""]
["The manufacturer of the doors is responsible to confirm the opening size into which the frame and door are fitted.",""]
["Shop drawings:",""]
["All profile types to be used are to be confirmed with the architect by means of complete shop drawings or physical samples prior to manufacture.",""]
["Laminated glass:",""]
["All laminated glass is to be marked by etching, engraving or sandblasting with glazier's name and relevant glass code.",""]
["Purpose made 80 micron powder coated (for architectural applications, applied by a certified markholder of SANS 1578 and SANS 1796) aluminium doors constructed to withstand wind pressures of 1500Pa (in accordance with SANS 613, related SABS standards and ",""]
["Aluminium and glass hinged double door and frame size 1000 x 2275mm made up of standard aluminium profiles as per detail marked D02 at HALL","No",{"v":5,"d":"5.00"}]
["Aluminium and glass hinged single door and frame size 1470 x 2475mm made up of standard aluminium profiles at Living Heritage (Window 16)","No",{"v":2,"d":"2.00"}]
["Aluminium and glass hinged double door and frame, size 1500 x 2125mm, glazed with OBSCURE safety glass, as per detail marked D13 at MUSEUM","No",{"v":1,"d":"1.00"}]
["Aluminium and glass pivot hinged single door and frame, size 1616 x 3135mm, as per detail marked D12 at MUSEUM","No",{"v":1,"d":"1.00"}]
["Aluminium and glass hinged double door and frame, size 1694 x 2125mm high  with aluminium louvre size 600 x 350mm complete with telescopic back frame including 19mm blade spacing as per detail marked D18 at AUDITORIUM","No",{"v":1,"d":"1.00"}]
["Purpose made 80 micron powder coated (for architectural applications, applied by a certified markholder of SANS 1578 and SANS 1796, with colour to SABS 1274) aluminium doors constructed to withstand wind pressures of 1500Pa (in accordance with SANS 613, r",""]
["Aluminium door, size 8907 x 4411mm high, with side hung and top opening sections and concealed friction stays, frame to accommodate single door, glazed with 6.76mm SOUNDPRUFE glazing, as per detail marked D01 at RECEPTION","No",{"v":1,"d":"1.00"}]
["ALUMINIUM SHOPFRONTS",""]
["Purpose made aluminium glazed shopfronts:",""]
["Purpose made mild steel shopfront size 8987 x 3740mm with double glazing and 60mm air void including purpose made side light aluminium window complete with door frame  made up of standard aluminium profiles with top hung opening sections and stainless ste","No",{"v":1,"d":"1.00"}]
["ALUMINIUM ROLLER SHUTTER DOORS",""]
["Aluminium roller shutter doors:",""]
["Solid aluminium roller shutter door, size 4140 x 2660mm with a double wall cavity and no safety glazing, as per detail marked D14 at MUSEUM","No",{"v":1,"d":"1.00"}]
["SHOWER DOORS",""]
["Shower Doors:",""]
["Anodised aluminium shower door and frame size 700 x 1900mm high, glazed in 6mm toughened safety glass sandblasted in full negative frosting, including pull knob.","No",{"v":9,"d":"9.00"}]
["Powder coated to match colour aluminium brushweld fixed to bottom of door",""]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["NOTE: Walls to receive plaster according to SANS 2001 Construction Works Part EM1: Cement Plaster, comprising Base coat of 1 part cement ( SABS specification 471 or SABS specification 831) and 5 parts sand( SABS specifications 1090, unless specialist advi",""]
["Cement topping :- Cement topping according SANS 50197-1. Finished to be hard and steel trowelled until smooth and even. Sealed with a water-based tile and cement sealer for unglazed porous substrates, sealant to be  applied with a paint brush strictly as ",""]
["Plaster to internal walls to be according to SANS 2001 construction works Part EMI: Render coat:-1 Part cement and 4 parts  sands (SABS Specification 471 or SABS specification 831) and (SABS specification 1090, unless specialist advice is obtained) Settin",""]
["Plaster to External Walls to be according SANS 2001 Construction Works Part EM1 : Base Coat :- 1 part cement and 5 parts sand (SABS specification 471 or SABS specification 831) and (SABS specification 1090, unless specialist advice is obtained). Finish to",""]
["Plaster to compose of 1 part cement and 4 parts sand for internal work. The material shall be mixed dry until dry and uniform in colour and the water is added and the mixture is turned over until the ingredients are thoroughly incorporated:",""]
["SCREEDS",""]
["Screeds on concrete slab",""]
["30mm Thick on floors and landings","m²",{"v":1673,"d":"1673.00"}]
["On narrow widths","m²",{"v":2,"d":"2.00"}]
["Average 48mm thick on roof slabs to falls","m²",{"v":2372,"d":"2372.00"}]
["Coved skirtings 75mm high","m",{"v":34,"d":"34.00"}]
["CEMENT TOPPING",""]
["40mm Cement topping finished to a hard, smooth and even surface with steel trowel including sealing surface with a water based tile and cement sealer for unglazed porous substrate:",""]
["On floors and landings","m²",{"v":1609,"d":"1609.00"}]
["On ramps","m²",{"v":49,"d":"49.00"}]
["40mm brushed cement topping on concrete:",""]
["On floors","m²",{"v":65,"d":"65.00"}]
["20mm Thick 1:1 cement non-shrink grout tightly rammed in small quantities:",""]
["Grout beneath base plates","m²",{"v":12,"d":"12.00"}]
["GRANOLITHIC",""]
["Untinted granolithic, on concrete",""]
["30mm Thick on floors and landings","m²",{"v":173,"d":"173.00"}]
["30mm Thick on ramps","m²",{"v":60,"d":"60.00"}]
["30mm Thick on treads and risers of stairs including reedings","m²",{"v":12,"d":"12.00"}]
["INTERNAL PLASTER",""]
["Two coats cement plaster according to SANS 2001 Construction Works Part EM1: Cement Plaster, with surface to be dry, sound and clean and cured for a minimum of 14 days, with a moisture content measured with a Doser Hygrometer (or equivalent), of BD 2 scal",""]
["On walls","m²",{"v":383,"d":"383.00"}]
["On narrow widths","m²",{"v":910,"d":"910.00"}]
["15mm thick on walls to receive mosaic tiles","m²",{"v":1,"d":"1.00"}]
["On walls circular on plan","m²",{"v":71,"d":"71.00"}]
["Underside of concrete slab","m²",{"v":169,"d":"169.00"}]
["On internal cills 110mm wide","m",{"v":27,"d":"27.00"}]
["Form 20mm Shadowline recess in plaster at junction of slab and wall (Labour Intensive Construction)","m",{"v":72,"d":"72.00"}]
["30mm Thick Two coat cement plaster including chicken mesh reinforcement fixed with expanding bolts at 300mm centres in both directions according to SANS 2001 Construction Works Part EM1: Cement Plaster with surface to be dry, sound and clean and cured for",""]
["30mm Thick plaster in irregular pattern on feature walls","m²",{"v":11,"d":"11.00"}]
["Terylene plaster of an intermediate texture according to SANS 2001-construction works part EM1, including bonding liquid mixed in and plaster applied with Terylene machine. Cement mixture of one part cement and half parts of course sand with water for a s",""]
["On concrete plinths","m²",{"v":5,"d":"5.00"}]
["On walls","m²",{"v":11,"d":"11.00"}]
["EXTERNAL PLASTER",""]
["25mm Thick cement plaster steel floated, on brickwork with 3mm diameter fischer plugs No. 268 staggered along entire length.",""]
["On walls.","m²",{"v":50,"d":"50.00"}]
["Two coats cement plaster according to SANS 2001 Construction Works Part EM1: Cement Plaster, with surface to be dry, sound and clean and cured for a minimum of 14 days, with a moisture content measured with a Doser Hygrometer (or equivalent), of BD 2 scal",""]
["On walls","m²",{"v":430,"d":"430.00"}]
["On narrow widths","m²",{"v":684,"d":"684.00"}]
["Terylene plaster of an intermediate texture according to SANS 2001-construction works part EM1, including bonding liquid mixed in and plaster applied with Terylene machine. Cement mixture of one part cement and half parts of course sand with water for a s",""]
["Sample panel of Terylene plaster","m²",{"v":10,"d":"10.00"}]
["On walls","m²",{"v":411,"d":"411.00"}]
["On narrow widths","m²",{"v":36,"d":"36.00"}]
["On sloping edge of coping 230mm girth","m",{"v":44,"d":"44.00"}]
["On sloping edge of coping 230mm girth circular on plan","m",{"v":7,"d":"7.00"}]
["On sloping cill 380mm girth including forming rainwater drip along bottom edge","m",{"v":27,"d":"27.00"}]
["On sloping edge projecting soffits of coping 750mm girth","m",{"v":57,"d":"57.00"}]
["On sloping edge projecting soffits of coping 1305mm girth","m",{"v":72,"d":"72.00"}]
["On 330mm brick on edge projection 30mm over brickwork on both sides on coping.","m",{"v":315,"d":"315.00"}]
["Labour forming 10 x 10mm chamfer:",""]
["On coping including wood float finish (Labour Intensive Construction)","m",{"v":11,"d":"11.00"}]
["3mm to 6mm thick lightweight plaster polyurethane screed consisting of BASF Primer SC (solvent-free, three part primer) and BASF Ucrete UD200 or equal approved heavy duty temperature and chemical resistant four part polyurethane screed laid strictly in ac",""]
["Ceilings","m²",{"v":354,"d":"354.00"}]
["PEBBLE INLAY",""]
["Pebble inlay in 40mm of 25 diameter river pebbles on concrete surface beds sourced locally in shades of brown:",""]
["Pebble inlay on floors","m²",{"v":295,"d":"295.00"}]
["MOVEMENT JOINTS",""]
["Provide facade joints in plaster at 3000mm interval unless otherwise indicated on the Architects drawings. Seal all joints with a polyurethane sealant according to SANS 1077, type two gun applications and non-sag. Colour to match the final wall finish.",""]
["Labour forming joint in plaster to façade","m",{"v":586,"d":"586.00"}]
["Sawn construction joints","m",{"v":380,"d":"380.00"}]
["5mm Expansion joint","m",{"v":419,"d":"419.00"}]
["Sealing of joints:",""]
["Seal joints with 5 x 10mm polyurethane sealant according to SANS 1077, type two gun applications and non-sag.","m",{"v":519,"d":"519.00"}]
["SUNDRIES",""]
["Building in only of metal dividing strips to screed and concrete floors:",""]
["Build in 4 x 40mm galvanised mild steel flat bar circular on plan with 4 x 40 x 40mm lugs at 300mm centers","m",{"v":514,"d":"514.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Fixing:",""]
["Unless described as 'fixed with adhesive to plaster (plaster elsewhere)' descriptions of tiling on brick or concrete walls, columns, etc. shall be deemed to include 1:4 cement plaster backing and descriptions of tiling on concrete floors etc. shall be dee",""]
["WALL TILING",""]
["Mesh backed porcelain tiles, size 50 x 250mm tiles, sheet size 250 x 250mm fixed mesh side down to internal plastered wall with super white powder adhesive for fixing ceramic mosaics onto walls mixed with bonding liquid in lieu of water laid with joints c",""]
["On walls","m²",{"v":181,"d":"181.00"}]
["On splash backs","m²",{"v":6,"d":"6.00"}]
["On narrow widths","m²",{"v":52,"d":"52.00"}]
["Porcelain tiles size 100 x 100 x 8mm thick to wood floated 1:4 cement and sand screed with tile adhesive on concrete surface bed:",""]
["On sloping floors and landings","m²",{"v":23,"d":"23.00"}]
["Broken tile mosaics fixed to internal plastered wall with super white powder adhesive for fixing ceramic mosaics onto walls mixed with bonding liquid in lieu of water laid, tile grout applied with flexible spatula:",""]
["On walls","m²",{"v":110,"d":"110.00"}]
["On narrow widths","m²",{"v":37,"d":"37.00"}]
["FLOOR TILING",""]
["PORCELAIN TILES:",""]
["400 x 400 x 8mm thick Porcelain tiles fixed to wood floated screed with adhesive mixed with bonding liquid in lieu of water on concrete surface bed, with 3mm joints continuous in both directions, grouted with tile grout with minimum 5mm expansion and cons",""]
["On floors and landings","m²",{"v":44,"d":"44.00"}]
["On narrow widths","m²",{"v":12,"d":"12.00"}]
["Skirting 125mm high Code 902-4030","m",{"v":26,"d":"26.00"}]
["Extra for internal corner tile Code 902-4034","No",{"v":15,"d":"15.00"}]
["100 x 100 x 8mm Thick Porcelain floor tiles fixed to wood floated screed with tile adhesive mixed with bonding liquid in lieu of water on concrete surface bed, with 3mm joints continuous in both directions, grouted with tile grout with minimum 5mm joints ",""]
["On shower floors","m²",{"v":3,"d":"3.00"}]
["MOSAIC TILING",""]
["Mosaic tiling:",""]
["5mm Thick glazed mosaic tile pattern as per artist design to concrete in worktops","m²",{"v":6,"d":"6.00"}]
["Provide the sum of R25 000,00 (Twenty Five Thousand Rand) for obtaining artist designs for tiling work","Item",{"v":1,"d":"1.00"}]
["Add for profit","Item",{"v":1,"d":"1.00"}]
["Add for attendance","Item",{"v":1,"d":"1.00"}]
["NOSING, JOINT COVERS, PROTECTORS, ETC.",""]
["Edge trims",""]
["6mm Aluminium straight edge trim in matt silver suitable for selected glazed tile thickness at corners, changes in wall finish and mirror surrounds with strip to be securely bedded in cement-based adhesive:",""]
["6mm Natural anodised aluminium tiling edge trim","m",{"v":298,"d":"298.00"}]
["9mm Natural anodised aluminium tiling edge trim","m",{"v":530,"d":"530.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Flush pans:",""]
["Flush Pans shall have straight or side outlets and 'P' or 'S' traps as necessary.",""]
["RAINWATER DISPOSAL",""]
["Water spouts:",""]
["50mm Diameter PVC overflow sleeve pipe 250mm long built into brickwork","No",{"v":32,"d":"32.00"}]
["50mm Diameter PVC overflow sleeve pipe 335mm long built into brickwork","No",{"v":28,"d":"28.00"}]
["50mm Diameter PVC bend","No",{"v":28,"d":"28.00"}]
["50mm Diameter hot dipped galvanised pipe 250mm long with one end angle cut to form spout and other end epoxy fixed 140mm deep into PVC sleeve pipe with all edges ground smooth to remove all burrs and irregularities","No",{"v":90,"d":"90.00"}]
["Aluminium gutters and rainwater pipes:",""]
["140 x 127 x 83mm VHV roof gutters fixed with concealed brackets with verandah bolts at 1165mm centres","m",{"v":192,"d":"192.00"}]
["125 x 100mm Zincalume rectangular roof gutters fixed with concealed brackets with verandah bolts at 1165mm centres","m",{"v":98,"d":"98.00"}]
["125 x 100mm Zincalume rectangular roof gutters fixed with concealed brackets with verandah bolts at 1165mm centres circular on plan","m",{"v":33,"d":"33.00"}]
["Extra over gutter for stopped end","No",{"v":18,"d":"18.00"}]
["Extra over gutter for outlet for 100 x 75mm pipe","No",{"v":33,"d":"33.00"}]
["85mm Rainwater pipes","m",{"v":166,"d":"166.00"}]
["Extra over rainwater pipe for bend","No",{"v":53,"d":"53.00"}]
["Extra over rainwater pipe for swan-neck","No",{"v":27,"d":"27.00"}]
["Spreader 300mm long for 85mm diameter pipe with half closed ends and 20mm holes at 50mm centres","No",{"v":4,"d":"4.00"}]
["uPVC pipes:",""]
["110mm Pipes cast into concrete","m",{"v":375,"d":"375.00"}]
["Extra over uPVC pipes for fittings:",""]
["110mm Bend","No",{"v":216,"d":"216.00"}]
["110mm Shoe","No",{"v":90,"d":"90.00"}]
["Galvanised mild steel:",""]
["Extra over galvanised iron piping for fittings:",""]
["Cast iron:",""]
["80mm 90 Degree centre bolt vertical roof fullbore outlet with dome grate including adaptor to 110mm PVC pipe","No",{"v":98,"d":"98.00"}]
["SANITARY FITTINGS:",""]
["WC Pans, etc.:",""]
["Vitreous china Charisma close coupled suite colour White (Code: 77526WH) or equally approved, comprising 90 degree outlet rim washdown pan fixed on and including floor bracket (Code: 8082Z0) with matching 6 litre cistern top dual flush cistern including f","No",{"v":8,"d":"8.00"}]
["Urinals:",""]
["Vitreous china Charisma or equally approved white wall mounted back inlet urinal (Code: 705127) size 565 x 275 310mm including 38mm chromium plated domical grating (Code: 8787Z2), flush valve, flush pipe and fittings","No",{"v":2,"d":"2.00"}]
["Stainless Steel:",""]
["1,2mm Grade 304 18/10 stainless steel Oval A or equally approved wall mounted wash hand basin (code: 357456), size 420 x 340 x 185mm deep with a one piece pressed bowl, 50mm splashback and 100mm radiused apron and 40mm waste outlet, fixed to wall with 4x6","No",{"v":3,"d":"3.00"}]
["Sinks:",""]
["0,9mm Grade 304 18/10 stainless steel LDS or equally approved drip sink (code:350960), size 600 x 500 x 258mm deep with pressed drip sink bowl, 40mm waste outlet connected to chromium plated bottle trap (code: 345/40), hinged bucket grid fitted over drip ","No",{"v":1,"d":"1.00"}]
["0,9mm Grade 304 18/10 stainless steel LDS or equally approved drip sink (code:350960), size 1500 x 500mm two 410x343 x 153mm deep bowls fitted onto cupboard including 90mm waste fitting and PVC traps  with 40mm waste outlet connected to chromium plated bo","No",{"v":1,"d":"1.00"}]
["Wash troughs:",""]
["0.8mm Grade 430 17/0 stainless steel ET102 or equally approved fabricated single wash trough (Code 320200), size 1030 x 430 x 300mm deep with two bowls, wash ridges and 40mm waste outlet fixed to wall with fixing lugs and anchor bolts","No",{"v":1,"d":"1.00"}]
["Prep bowl:",""]
["Rondo RDX610-45 Grade 304 18/10 or equally approved polished stainless single prep bowl (code: 820058), overall size 450mm diameter with  one 450mm x 161mm deep bowl, including 90mm waste fitting without overflow and PVC trap","No",{"v":1,"d":"1.00"}]
["Mop wash:",""]
["0,9mm Grade 304 18/10 stainless steel LDS or equally approved drip sink (code: 350960), size 600 x 500 x 258mm deep with pressed drip sink bowl, 40mm waste outlet connected to Cobra chromium plated bottle trap (code: 345/40), hinged bucket grid fitted ove","No",{"v":3,"d":"3.00"}]
["SANITARY PLUMBING",""]
["Waste unions:",""]
["La Gio Bella or equally approved solid brass 80mm slotted click waste (Code BW202S) in chrome plated finish","No",{"v":49,"d":"49.00"}]
["Traps, drains and channels:",""]
["50mm shower trap with chromium plated grid","No",{"v":26,"d":"26.00"}]
["Chromium plated high-gloss 32mm bottle trap for wash hand basin","No",{"v":52,"d":"52.00"}]
["Geberit chromium plated high-gloss 32mm bottle trap for washbasin (Code 151.034.21.1)","No",{"v":37,"d":"37.00"}]
["100 x 50mm Deep purpose made wash hand basin drain channel 2090mm long formed of 1mm thick stainless steel with closed ends  including cutting three 32mm diameter outlet holes with the channel and fixed to underside of concrete wash hand basin","No",{"v":2,"d":"2.00"}]
["Grade AISI 304 stainless steel RO 200 NW 100 square floor drain with perforated circular grating pattern suitable for tiled floor covering, size 240 x 210mm deep, with 104mm  diameter  horizontal waste outlet with mitred  bend connected to waste pipe.","No",{"v":2,"d":"2.00"}]
["Taps, valves, etc.:",""]
["15mm Carina or equally approved chromium square pattern pillar tap with aerator outlet and flanged backnut (Code:114CA-15), manufactured in accordance with SANS 226:2004 Type 1 (BS 5412)","No",{"v":14,"d":"14.00"}]
["15mm Strata or equally approved single lever chromium plated single taphole basin mixer with 110mm body extension and 3/8 C x 400mm long flexible inlets (Code: SA-851R), manufactured in accordance with SAN 1480:2005 (BS EN 1286)","No",{"v":59,"d":"59.00"}]
["uPVC pipes:",""]
["40mm Pipes built into brickwork","m",{"v":140,"d":"140.00"}]
["50mm Pipes built into brickwork","m",{"v":372,"d":"372.00"}]
["110mm Pipes fixed to walls with brackets","m",{"v":225,"d":"225.00"}]
["110mm Pipes laid in trenches not exceeding 1m deep","m",{"v":580,"d":"580.00"}]
["Extra over uPVC pipes for fittings:",""]
["40mm Bend","No",{"v":73,"d":"73.00"}]
["50mm Bend","No",{"v":190,"d":"190.00"}]
["110mm Bend","No",{"v":111,"d":"111.00"}]
["50mm Junction","No",{"v":31,"d":"31.00"}]
["110mm Junction","No",{"v":80,"d":"80.00"}]
["110mm Reducing junction","No",{"v":20,"d":"20.00"}]
["110mm Double junction","No",{"v":6,"d":"6.00"}]
["110mm Pan connector","No",{"v":1,"d":"1.00"}]
["110mm Access bent pan connector","No",{"v":15,"d":"15.00"}]
["110mm Access bend","No",{"v":127,"d":"127.00"}]
["110mm Access junction","No",{"v":21,"d":"21.00"}]
["110mm Access double junction","No",{"v":4,"d":"4.00"}]
["50mm 'GI Two-way' vent valve","No",{"v":3,"d":"3.00"}]
["110mm 'GI Two-way' vent valve","No",{"v":30,"d":"30.00"}]
["SOIL DRAINAGE (CPAP Work Group No 146)",""]
["Cast iron pipes:",""]
["110mm Supercast pipes laid in and including trenches not exceeding 1m deep beneath surface beds","m",{"v":80,"d":"80.00"}]
["uPVC:",""]
["110mm Pipes vertically or ramped to cleaning eyes etc. (no excavation)","m",{"v":37,"d":"37.00"}]
["110mm Pipes laid in and including trenches not exceeding 1m deep","m",{"v":554,"d":"554.00"}]
["110mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",{"v":129,"d":"129.00"}]
["Extra over uPVC pipes for fittings:",""]
["110mm Bend","No",{"v":79,"d":"79.00"}]
["110mm Junction","No",{"v":26,"d":"26.00"}]
["110mm Access pipe","No",{"v":15,"d":"15.00"}]
["Vitrified clay gulleys:",""]
["110mm Gulley not exceeding 1m deep","No",{"v":14,"d":"14.00"}]
["Precast concrete:",""]
["Precast concrete gulley surround","No",{"v":18,"d":"18.00"}]
["Inspection chambers including covers",""]
["Inspection chamber 450 x 600mm and not exceeding 1m deep internally comprising one brick walls and concrete base and slab","No",{"v":10,"d":"10.00"}]
["Inspection chamber 450 x 600mm and exceeding 1m and not exceeding 2m deep internally comprising one brick walls and concrete base and slab","No",{"v":6,"d":"6.00"}]
["Precast concrete circular inspection chambers (covers elsewhere):",""]
["Inspection chamber 1130mm diameter and exceeding 1m and not exceeding 2m deep internally","No",{"v":6,"d":"6.00"}]
["Sundries:",""]
["Extra over excavation in earth for pipe trenches, chambers, etc. for excavation in soft rock","m³",{"v":100,"d":"100.00"}]
["Extra over excavation in earth for pipe trenches, chambers, etc. for excavation in hard rock","m³",{"v":60,"d":"60.00"}]
["Extra over excavation for pipe trenches, chambers, etc. for carting away surplus material to a dumping site to be located by the Contractor","m³",{"v":185,"d":"185.00"}]
["Extra over backfilling to drain trenches, chambers, etc. for earth backfilling supplied by the Contractor","m³",{"v":135,"d":"135.00"}]
["Unreinforced concrete encasing to110mm diameter horizontal pipe","m³",{"v":33,"d":"33.00"}]
["Unreinforced concrete encasing to 110mm diameter vertical pipe","m",{"v":37,"d":"37.00"}]
["300 x 300 x 50mm Precast concrete inspection eye marker slab set in ground","No",{"v":19,"d":"19.00"}]
["100mm Cast iron 'ABC' cleaning eye","No",{"v":8,"d":"8.00"}]
["TESTING",""]
["Testing drainage pipe system","Item",{"v":1,"d":"1.00"}]
["WATER SUPPLIES",""]
["Water supplies by Mechanical Engineer:",""]
["NOTE: The bulk of hot and cold water supply piping and fittings are taken in the Mechanical Engineering schedules of quantities",""]
["Class 2 copper pipes:",""]
["15mm Pipes chased into brick walls","m",{"v":260,"d":"260.00"}]
["22mm Pipes chased into brick walls","m",{"v":214,"d":"214.00"}]
["28mm Pipes chased into brick walls","m",{"v":236,"d":"236.00"}]
["35mm Pipes chased into brick walls","m",{"v":170,"d":"170.00"}]
["50mm Pipes chased into brick walls","m",{"v":106,"d":"106.00"}]
["50mm Pipes laid in and including trenches","m",{"v":92,"d":"92.00"}]
["Extra over class 2 copper pipes for capillary fittings:",""]
["15mm Fittings","No",{"v":318,"d":"318.00"}]
["22mm Fittings","No",{"v":220,"d":"220.00"}]
["28mm Fittings","No",{"v":191,"d":"191.00"}]
["Extra over class 2 copper pipes for brass compression fittings:",""]
["15mm Fittings","No",{"v":275,"d":"275.00"}]
["22mm Fittings","No",{"v":233,"d":"233.00"}]
["28mm Fittings","No",{"v":220,"d":"220.00"}]
["35mm Elbow","No",{"v":38,"d":"38.00"}]
["50mm Elbow","No",{"v":24,"d":"24.00"}]
["35mm Tee","No",{"v":27,"d":"27.00"}]
["50mm Tee","No",{"v":11,"d":"11.00"}]
["35mm Reducing elbow","No",{"v":11,"d":"11.00"}]
["50mm Reducing elbow","No",{"v":10,"d":"10.00"}]
["35mm Reducing tee","No",{"v":8,"d":"8.00"}]
["50mm Reducing tee","No",{"v":5,"d":"5.00"}]
["50mm Multi-step reducer","No",{"v":4,"d":"4.00"}]
["50mm Adaptor coupling","No",{"v":8,"d":"8.00"}]
["Copper service and overflow pipes:",""]
["15mm Flexible service pipe 300mm girth","No",{"v":227,"d":"227.00"}]
["22mm Overflow pipe 500mm girth twice bent","No",{"v":71,"d":"71.00"}]
["Sundries:",""]
["300 x 450mm Cast iron stopcock box including brick chamber below not exceeding 1m deep internally","No",{"v":3,"d":"3.00"}]
["450 x 600mm Meter or valve box including brick chamber below not exceeding 1m deep internally","No",{"v":3,"d":"3.00"}]
["ELECTRIC WATER HEATERS",""]
["Hot water cylinders complying with SABS 151:1992:",""]
["50 Litre Under counter electric water heater","No",{"v":1,"d":"1.00"}]
["100 Litre Horizontally mounted 2kW 'Kompakt' electric water heater (code WE100)","No",{"v":3,"d":"3.00"}]
["200 Litre Horizontally mounted 3kW 'Kompakt' electric water heater (code WE200)","No",{"v":6,"d":"6.00"}]
["200 Litre Horizontally mounted Solar Geyser","No",{"v":1,"d":"1.00"}]
["Black polyethylene geyser trays (SABS 1848:2000):",""]
["Geyser tray to suit 100 litre capacity horizontal geyser (elsewhere measured), with and including 50mm diameter PVC overflow connector (code GT200)","No",{"v":1,"d":"1.00"}]
["Geyser tray to suit 200 litre capacity horizontal geyser (elsewhere measured), with and including 50mm diameter PVC overflow connector (code GT200)","No",{"v":2,"d":"2.00"}]
["TESTING",""]
["Testing water pipe system","Item",{"v":1,"d":"1.00"}]
["FIRE APPLIANCES ETC.",""]
["Approved:",""]
["'Everyway' hose reel complete with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket","No",{"v":11,"d":"11.00"}]
["4,5kg Carbon dioxide fire extinguisher","No",{"v":30,"d":"30.00"}]
["9kg Dry chemical fire extinguisher","No",{"v":3,"d":"3.00"}]
["WATER SUPPLIES TO FIRE APPLIANCES",""]
["Galvanised steel pipes:",""]
["28mm Pipes fixed to walls with brackets","m",{"v":27,"d":"27.00"}]
["35mm Pipes fixed to walls with brackets","m",{"v":50,"d":"50.00"}]
["50mm Pipes laid in trench not exceeding 1m deep","m",{"v":411,"d":"411.00"}]
["Extra over galvanised steel pipes for steel fittings:",""]
["28mm Fittings","No",{"v":28,"d":"28.00"}]
["35mm Elbow","No",{"v":30,"d":"30.00"}]
["35mm Union","No",{"v":11,"d":"11.00"}]
["50mm Bend","No",{"v":33,"d":"33.00"}]
["50mm Tee","No",{"v":4,"d":"4.00"}]
["50mm Adaptor coupling","No",{"v":8,"d":"8.00"}]
["Sundries:",""]
["Unreinforced concrete in thrust blocks at bends, tees, etc. including necessary extra excavation, formwork, etc.","m³",{"v":11,"d":"11.00"}]
["TESTING",""]
["Testing of fire supply:",""]
["Testing fire water pipe system","Item",{"v":1,"d":"1.00"}]
["PIPE PROTECTION",""]
["'Densyl Tape':",""]
["Wrapping around 22mm pipe including couplings","m",{"v":101,"d":"101.00"}]
["Extra for wrapping around fittings","No",{"v":4,"d":"4.00"}]
["Extra for wrapping around 50mm bend","No",{"v":9,"d":"9.00"}]
["Extra for wrapping around 50mm tee","No",{"v":2,"d":"2.00"}]
["LAGGING",""]
["'Thermaflex' pipe insulation:",""]
["Insulation to 15mm pipe and couplings","m",{"v":1,"d":"1.00"}]
["Insulation to 22mm pipe and couplings","m",{"v":1,"d":"1.00"}]
["Insulation to 28mm pipe and couplings","m",{"v":1,"d":"1.00"}]
["Extra for wrapping around fittings","No",{"v":39,"d":"39.00"}]
["SLEEVES",""]
["Sleeves through concrete or brickwork:",""]
["PVC sleeve not exceeding 100mm diameter and exceeding 250 and not exceeding 500mm long cast into concrete slab","No",{"v":5,"d":"5.00"}]
["PVC sleeve exceeding 100 and not exceeding 200mm diameter and exceeding 250 and not exceeding 500mm long cast into concrete slab","No",{"v":85,"d":"85.00"}]
["PVC sleeve exceeding 200 and not exceeding 300mm diameter and exceeding 250 and not exceeding 500mm long cast into concrete slab","No",{"v":10,"d":"10.00"}]
["DUCTS FOR ELECTRICAL AND TELEPHONE CABLES ETC (CPAP Work Group No 146)",""]
["110mm Pipes laid in trench not exceeding 1m deep","m",{"v":24,"d":"24.00"}]
["110mm Pipes laid in trench exceeding 1m and not exceeding 2m deep","m",{"v":16,"d":"16.00"}]
["Set of two 110mm pipes laid in trench not exceeding 1m deep","m",{"v":12,"d":"12.00"}]
["Set of two 110mm pipes laid in trench exceeding 1m and not exceeding 2m deep","m",{"v":8,"d":"8.00"}]
["Set of three 110mm pipes laid in trench not exceeding 1m deep","m",{"v":6,"d":"6.00"}]
["Extra over backfilling to pipe trenches, chambers, etc. for compaction to 95% Mod AASHTO density","m³",{"v":20,"d":"20.00"}]
["'Everite' class T fibre-cement pipes:",""]
["110mm Pipes laid in and including trenches not exceeding 1m deep","m",{"v":20,"d":"20.00"}]
["110mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep.","m",{"v":10,"d":"10.00"}]
["Extra over class T fibre-cement pipes for fittings:",""]
["110mm Bend","No",{"v":4,"d":"4.00"}]
["110mm Access junction","No",{"v":2,"d":"2.00"}]
["110mm Access double junction","No",{"v":2,"d":"2.00"}]
["Inspection chambers (covers elsewhere):",""]
["Junction box 600 x 900mm and exceeding 1mm and not exceeding 2mm deep internally","No",{"v":2,"d":"2.00"}]
["Gratings, covers, etc.:",""]
["450 x 600mm x 68kg Type 9D cast iron single seal manhole cover and frame","No",{"v":2,"d":"2.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Laminated glass",""]
["Laminated glass to have polyvinyl butyral (PVB) interlayers",""]
["GLAZING TO TIMBER WITH BEADS",""]
["6mm Normal strength (NS) clear laminated safety glass:",""]
["Panes exceeding 0,1m2 and not exceeding 0,5m2","m²",{"v":22,"d":"22.00"}]
["Panes exceeding 0,5m2 and not exceeding 2m2","m²",{"v":38,"d":"38.00"}]
["Circular panes of 300mm diameter","No",{"v":3,"d":"3.00"}]
["6mm Normal strength (NS) white obscure laminated safety glass:",""]
["Panes exceeding 0,1m2 and not exceeding 0,5m2","m²",{"v":9,"d":"9.00"}]
["MIRRORS, ETC",""]
["5mm silver float glass copper backed mirror with polished edges, to comply with SABS 1236 - Class A, fixed with vertical strips of double sided adhesive tape:.",""]
["Mirror size 350 x 950mm high","No",{"v":4,"d":"4.00"}]
["Mirror size 350 x 1000mm high","No",{"v":1,"d":"1.00"}]
["Mirror size 400 x 905mm high","No",{"v":4,"d":"4.00"}]
["Mirror size 600 x 900mm high","No",{"v":16,"d":"16.00"}]
["Mirror size 2250 x 850mm high","No",{"v":2,"d":"2.00"}]
["6mm Silvered float glass copper backed mirrors with polished edges, fixed with construction silicone",""]
["Mirror size 250 x 250mm high","No",{"v":1,"d":"1.00"}]
["FRAMELESS GLASS",""]
["Frameless Glass:",""]
["8mm Clear float glass window with brushed stainless steel glazing brackets, size 200 x 4147mm high as per detail marked W11 at Museum","No",{"v":1,"d":"1.00"}]
["8mm Clear float glass window with brushed stainless steel glazing brackets, size 400 x 4135mm high as per detail marked W13 at Museum","No",{"v":1,"d":"1.00"}]
["12mm Clear safety frameless glass window, size 220 x 3020 high as per detail marked W17 on drawing EDUC 3100.04","No",{"v":1,"d":"1.00"}]
["12mm Clear safety frameless glass window, size 340 x 3020mm high, as per detail marked W18 on drawing EDUC 3100.04","No",{"v":1,"d":"1.00"}]
["12mm Clear float glass window with brushed stainless steel glazing brackets, size 4405 x 3535mm high as per detail marked W08 at Museum","No",{"v":1,"d":"1.00"}]
["SKYLIGHTS",""]
["Acrylic skylights sealed with and including aluminium flashing all around, glazing tape and structural silicone sealant:",""]
["Circular domed acrylic skylight of radius 680mm fixed to concrete all as per detail marked \"Skylight 4/4600.01 on Drawing 25379-MUS-4600.01 and details on Drawing 25379-MUS-4600.02","No",{"v":2,"d":"2.00"}]
["Galvanised mild steel glazed skylights with 3 x 30 x 50mm rectangular galvanised mild steel framing fixed to top of concrete with 12mm mild steel anchor bolts at 500mm centres and glazed with 6mm Armourplate toughened safety glass complying with SANS 1263",""]
["Set of eight skylights of various sizes comprising 1853 x 710mm; 1853 x 710mm; 3906 x 710mm; 4506 x 710mm; 5106 x 710mm and 5106 x 710mm wide all as per detail marked \"Skylight 8/4600.01\" on Drawing 25379-MUS-4600.01  and section f-f on Drawing 25379-MUS-","No",{"v":1,"d":"1.00"}]
["Skylight size 6890 x 870mm wide overall including 3 x 30 x 50mm galvanised mild steel mullion as per detail marked \"Skylight 2/4600.01\" on Drawing 25379-MUS-4600.01 and section a-a on Drawing 25379-MUS-4600.02  and section b-b on Drawing 25379-MUS-4600.02","No",{"v":1,"d":"1.00"}]
["Set of two skylights each size 9623 x 970mm wide overall as per detail marked \"Skylight 6/4600.01\" on Drawing 25379-MUS-4600.01  and section e-e on Drawing 25379-MUS-4600.02","No",{"v":1,"d":"1.00"}]
["Skylight size 9829 x 970mm wide overall including two 3 x 30 x 50mm galvanised mild steel mullion as per detail marked \"Skylight 5/4600.01\" on Drawing 25379-MUS-4600.01 and section d-d on Drawing 25379-MUS-4600.02","No",{"v":1,"d":"1.00"}]
["Skylight size 11966 x 710mm wide overall including three 3 x 30 x 50mm galvanised mild steel mullion as per detail marked \"Skylight 7/4600.01\" on Drawing 25379-MUS-4600.01 and section h-h on Drawing 25379-MUS-4600.02","No",{"v":1,"d":"1.00"}]
["Skylight size 13422 x 710mm wide overall including three 3 x 30 x 50mm galvanised mild steel mullion as per detail marked \"Skylight 1/4600.01\" on Drawing 25379-MUS-4600.01 and section a-a on Drawing 25379-MUS-4600.02","No",{"v":1,"d":"1.00"}]
["Skylight size 16496 x 940mm wide overall including four 3 x 30 x 50mm galvanised mild steel mullion as per detail marked \"Skylight 3/4600.01\" on Drawing 25379-MUS-4600.01 and section c-c on Drawing 25379-MUS-4600.02","No",{"v":1,"d":"1.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["Environmental factors:",""]
["All preparation and application of paintwork is to be for Environmental Factor: C5 - Coastal Marine",""]
["PAINTWORK ETC TO NEW WORK",""]
["ON INTERNAL FLOATED PLASTER SURFACES",""]
["Prepare and apply one coat alkali resistant plaster primer and two coats of low odour premium quality highly washable and stain resistant acrylic emulsion paint",""]
["On walls","m²",{"v":4388,"d":"4388.00"}]
["On underside of concrete slab","m²",{"v":166,"d":"166.00"}]
["Prepare and apply one coat tinted coarse aggregate primer and two coats of environmentally friendly textured acrylic coating that has subtle graded nuances with matt, robust look applied with a roller including laying off with a block brush using vertical",""]
["On walls","m²",{"v":594,"d":"594.00"}]
["On background of shelving","m²",{"v":35,"d":"35.00"}]
["On shelving","m²",{"v":46,"d":"46.00"}]
["ON EXTERNAL FLOATED PLASTER OR CONCRETE SURFACES",""]
["Prepare and apply one coat penetrating matt cement sealant on:",""]
["Precast concrete cills","m²",{"v":131,"d":"131.00"}]
["ON PLASTERBOARD",""]
["Prepare and apply one coat plaster primer and two coats of low odour premium quality highly washable and stain resistant acrylic emulsion paint for interior use:",""]
["On walls","m²",{"v":176,"d":"176.00"}]
["On flush ceilings","m²",{"v":797,"d":"797.00"}]
["ON METAL SURFACES",""]
["Prepare by brushing mild steel flat bar with steel wool and seal with polyurethane floor sealer with matt finish by brush strictly as per manufacturers specification according to SANS 12944:",""]
["On galvanised mild steel flat bar dividing strips not exceeding 300mm girth","m",{"v":512,"d":"512.00"}]
["On galvanised mild steel flat bar vanity edge restraints not exceeding 300mm girth","m",{"v":36,"d":"36.00"}]
["Prepare and apply one coat professional high build zinc phosphate primer and two coats pure acrylic emulsion sheen paint for interior and exterior use:",""]
["On steel doors","m²",{"v":36,"d":"36.00"}]
["On steel bench supports","m²",{"v":22,"d":"22.00"}]
["Prepare and apply one coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint:",""]
["On grille gates","m²",{"v":33,"d":"33.00"}]
["Prepare and chemically clean steelwork with a galvanised iron cleaner, apply one coat epoxy primer compatible with zinc to a DFT of 50-60 microns and two finishing coats of polyurethane gloss enamel paint to a DFT of 60-90 microns:",""]
["On galvanised structural steelwork","m²",{"v":4921,"d":"4921.00"}]
["ON WOOD SURFACES",""]
["Two coats oil wood primer:",""]
["Backs of frames, linings, etc. not exceeding 300mm wide","m",{"v":65,"d":"65.00"}]
["Prepare and apply one coat alkali resistant primer and two coats acrylic emulsion paint suitable for interior and exterior use:",""]
["On timber doors","m²",{"v":151,"d":"151.00"}]
["Prepare and apply one coat primer, one coat alkyd based universal undercoat and two coats superior quality universal enamel paint:",""]
["On doors","m²",{"v":44,"d":"44.00"}]
["On door frames, etc.","m²",{"v":10,"d":"10.00"}]
["Prepare and apply one coat professional high build zinc phosphate wood  primer and two coats pure acrylic emulsion sheen paint for interior and exterior use:",""]
["On doors","m²",{"v":4,"d":"4.00"}]
["Prepare and apply two coats premium quality nano-particle water based wood varnish for interior use on wood:",""]
["On door frames, etc.","m²",{"v":70,"d":"70.00"}]
["On doors","m²",{"v":136,"d":"136.00"}]
["On timber ceiling members","m²",{"v":65,"d":"65.00"}]
["On slatted timber bench seats","m²",{"v":39,"d":"39.00"}]
["Prepare and apply one coat penetrating primer for exterior wood and two coats durable, washable, pure acrylic emulsion sheen paint:",""]
["On doors","m²",{"v":24,"d":"24.00"}]
["On door frames etc.","m²",{"v":4,"d":"4.00"}]
["Prepare and apply three coats clear matt polyurethane floor sealer applied by brush strictly as per manufacturers specifications:",""]
["On hardwood parquet flooring","m²",{"v":289,"d":"289.00"}]
["On vanity hardwood slats","m²",{"v":2,"d":"2.00"}]
["Prepare and apply one coat penetrating oil based coating and finish with two coats penetrating oil based coating applied by brush strictly as per manufacturers specifications. Note: allow an overcoating time of minimum 24 hours in-between coats",""]
["On hardwood meranti slats","m²",{"v":5,"d":"5.00"}]
["On meranti skirting.","m²",{"v":25,"d":"25.00"}]
["Prepare and apply two coats water-based tile and cement sealer for unglazed porous substrates by brush strictly in accordance with the manufacturers specifications:",""]
["On cement topping","m²",{"v":2380,"d":"2380.00"}]
["On concrete vanity tops","m²",{"v":18,"d":"18.00"}]
["PREAMBLES",""]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["SUPPLEMENTARY PREAMBLES",""]
["NOTE: Contractor to refer to the TOPSOIL (ECO-1) Item C17 Of the preliminaries section for the protection and preservation of the ecological integrity of the topsoil.  Contractor to seek advice from Landscape Architect in terms of topsoil management. Salv",""]
["NOTE: Pigment off-shutter concrete walls:   \na) Pigment material must be suitable to colour concrete and not affect the strength and durability of the concrete.\nb) The colouring agent used shall be a single component, pigmented admixture of approximately ",""]
["Sample Panels: The contractor shall prepare sample panels and shall get the approval of the architect in writing prior to proceeding with colour concrete works. Samples shall be prepared in batches of not less than one-half cubic metre per sample to ensur",""]
["Density tests:",""]
["Density tests measured below are those specifically instructed by the engineer to be taken on filling material. All control tests to ensure layerworks are compacted to the required density are to be allowed for by the contractor in scheduled rates",""]
["EXCAVATIONS ETC  (CPAP Work Group No 104)",""]
["Excavate in earth not exceeding 2m deep:",""]
["Trenches (Labour Intensive Construction)","m³",{"v":26,"d":"26.00"}]
["Holes (Labour Intensive Construction)","m³",{"v":1,"d":"1.00"}]
["Extra over trench and hole excavations in earth for excavation in:",""]
["Soft rock","m³",{"v":7,"d":"7.00"}]
["Hard  rock","m³",{"v":1,"d":"1.00"}]
["Allow for risk of collapse of excavations:",""]
["Sides of trench and hole excavations not exceeding 1.5m deep","m²",{"v":38,"d":"38.00"}]
["Sides of holes and trenches excavations exceeding 1.5m deep","m²",{"v":8,"d":"8.00"}]
["Keeping excavations free of water:",""]
["Allow for keeping excavations free of water","Item",{"v":1,"d":"1.00"}]
["FILLING (CPAP Work Group No 104)",""]
["Earth filling selected from the excavated material, deposited in layers not exceeding 150mm thick, watered and consolidated to 95% modified AASHTO dry density as backfilling:",""]
["Backfilling to trenches, holes, etc. (Labour Intensive Construction)","m³",{"v":32,"d":"32.00"}]
["Earth filling supplied by the Contractor, deposited in layers not exceeding 150mm thick, watered and consolidated to 95% modified AASHTO dry density as filling in foundation:",""]
["Filling to trenches, holes, etc. (Labour Intensive Construction)","m³",{"v":26,"d":"26.00"}]
["Prescribed density tests on filling required by the engineer:",""]
["Modified AASHTO Density test","No",{"v":4,"d":"4.00"}]
["CARTING AWAY",""]
["Extra over all excavations for loading, carting and dumping surplus excavated material (no allowance made for increase in bulk):",""]
["Surplus material from excavations to a dumping site to be located by the contractor (Labour Intensive Construction)","m³",{"v":26,"d":"26.00"}]
["CONCRETE (CPAP Work Group No 110)",""]
["UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES",""]
["20Mpa/19mm Unreinforced concrete cast against excavated surfaces:",""]
["Surface blinding under footings and bases","m³",{"v":30,"d":"30.00"}]
["Filling of cavity walls in foundations","m³",{"v":22,"d":"22.00"}]
["REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES",""]
["30Mpa/19mm Reinforced concrete:",""]
["Footings","m³",{"v":7,"d":"7.00"}]
["Ground beams","m³",{"v":8,"d":"8.00"}]
["Concrete wall in foundations","m³",{"v":6,"d":"6.00"}]
["ROUGH FORMWORK (CPAP Work Group No 110)",""]
["Rough formwork to sides:",""]
["Of concrete walls in foundations","m²",{"v":17,"d":"17.00"}]
["Of ground beams","m²",{"v":1,"d":"1.00"}]
["REINFORCEMENT (CPAP Work Group No 114)",""]
["Mild steel reinforcement to structural concrete work:",""]
["12mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["10mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["High tensile steel reinforcement to structural concrete work:",""]
["32mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["20mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["16mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["8mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["BRICKWORK IN FOUNDATIONS (CPAP Work Group No 116)",""]
["Brickwork of NFX bricks (14Mpa nominal compressive strength) in class I mortar:",""]
["220mm brick walls (Labour Intensive Construction)","m²",{"v":31,"d":"31.00"}]
["270mm Cavity walls in two skins with wire ties (Labour Intensive Construction)","m²",{"v":12,"d":"12.00"}]
["340mm Cavity walls in two skins with wire ties (Labour Intensive Construction)","m²",{"v":18,"d":"18.00"}]
["Brickwork reinforcement:",""]
["75mm Wide reinforcement built in horizontally","m",{"v":92,"d":"92.00"}]
["150mm Wide reinforcement built in horizontally","m",{"v":32,"d":"32.00"}]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["FILLING, ETC",""]
["Filling with approved material supplied and carted onto site by the Contractor compacted to a density 95% Mod. AASHTO maximum density:",""]
["Behind retaining walls","m³",{"v":59,"d":"59.00"}]
["Retaining walls","m²",{"v":84,"d":"84.00"}]
["Coarse river sand filling compacted to 95% Mod. AASHTO maximum density:",""]
["KEEPING EXCAVATIONS FREE OF WATER",""]
["Keeping excavations free of water:",""]
["Keeping excavations free of all water other than subterranean water","Item",{"v":1,"d":"1.00"}]
["TESTS",""]
["Prescribed density tests on filling:",""]
["Modified AASHTO density test","No",{"v":10,"d":"10.00"}]
["Gamtoos River Valley sand filling lightly compacted:",""]
["Sand laid over site","m³",{"v":68,"d":"68.00"}]
["Geotextile composite mesh for weed growth prevention:",""]
["Geotextile composite mesh for weed growth prevention","m²",{"v":345,"d":"345.00"}]
["REINFORCED CONCRETE (CPAP Work Group No 110)",""]
["30 MPa/19mm Concrete:",""]
["Footings","m³",{"v":22,"d":"22.00"}]
["Bases","m³",{"v":13,"d":"13.00"}]
["Walls","m³",{"v":23,"d":"23.00"}]
["TEST BLOCKS",""]
["Test blocks:",""]
["Making and testing set of three 150 x 150 x 150mm concrete strength test cubes","Sets",{"v":5,"d":"5.00"}]
["REINFORCEMENT (CPAP Work Group No 114)",""]
["Mild steel reinforcement to structural concrete work:",""]
["12mm Diameter bars","Tonnes",{"v":2,"d":"2.00"}]
["10mm Diameter bars","Tonnes",{"v":1,"d":"1.00"}]
["Tenderers are advised to study the \"Specification of Materials and Methods to be used (PW371-A read in conjunction with PW371-B)\" before pricing this bill. PW371-A is available on the website at: http://www.publicworks.gov.za/PDFs/consultants_docs whilst ",""]
["PREAMBLES",""]
["SUPPLEMENTARY PREAMBLES",""]
["Roof sheeting guarantee:",""]
["The roof sheeting manufacturer shall comply with ISO9002 Quality Management System. Sheeting shall be laid in strict accordance with the manufacturer’s specifications by an approved contractor. A written and approved five year guarantee of site-workmanshi",""]
["PROFILED METAL SHEETING AND ACCESSORIES",""]
["0.6mm G550 AZ150 Zincalume roof sheeting shall be double-interlocking concealed-fix profile roll-formed in continuous lengths and cut to length by a pneumatic cut-off process from certified Z275 galvanized steel complying with ASTM 446 Grade \"E\" 3T (A653)",""]
["Roof covering with pitches not exceeding 25 degrees","m²",{"v":219,"d":"219.00"}]
["Raking cutting to steel roof sheeting","m",{"v":42,"d":"42.00"}]
["0,8mm Thick Zincalume steel purpose rolled flashings finished on one side with a custom formulated polyester paint with inorganic pigments fixed to sheeting with concealed clips:",""]
["Counter flashing 192mm girth three times bent","m",{"v":33,"d":"33.00"}]
["Headwall flashing 367mm girth twice bent","m",{"v":11,"d":"11.00"}]
["Head wall flashing 425mm girth three times bent","m",{"v":8,"d":"8.00"}]
["Side wall flashing 425mm girth three times bent","m",{"v":21,"d":"21.00"}]
["Parapet flashing 510mm girth four times bent","m",{"v":38,"d":"38.00"}]
["Apex and side wall barge flashing 540mm girth six times bent","m",{"v":31,"d":"31.00"}]
["Barge flashing 600mm girth six times bent","m",{"v":23,"d":"23.00"}]
["INSULATION",""]
["Insulation laid on concrete slabs:",""]
["30mm High density rigid extruded polystyrene insulation boarding laid on concrete slab","m²",{"v":349,"d":"349.00"}]
["50mm thick Composite polyester thermal insulation with aluminium foil to one face (density 10 kg/m³) laid with foil facing down between steel rafters on straining wires at 300mm centres including thermal breaks (on top of the rafter) as per architects det",""]
["Insulation fixed to steel purlins beneath roof sheeting","m²",{"v":218,"d":"218.00"}]
["Insulation fixed to steel purlins beneath roof sheeting in void closures","m²",{"v":11,"d":"11.00"}]
["Green Acoustics Fibran Geolan 40mm 50kg/m3 Stonewool or equally approved insulation:",""]
["Stonewool insulation to roofs","m²",{"v":60,"d":"60.00"}]

{"sheet":"Sect 4","index":3,"n_rows":397,"n_cols":5,"rows_kept":397}
["Description","Uom","Quantity","Rate","Amount"]
["FIRE DETECTION",""]
["SUPPLEMENTARY PREAMBLES",""]
["Specifications, drawings, etc",""]
["Tenderers are referred to the Mechanical Installation specification (see separately bound Volume 3 part 3) and drawings numbered ? to ? prepared by CA du Toit Consulting Engineers, accompanying these bills of quantities for the mechanical work, for the fu",""]
["Major equipment",""]
["Descriptions of major equipment such as chillers, air handling units and the like shall be deemed to include connections to water, air and electrical supply and/or discharge points, supports, bearers, vibration insulation mountings, filters, insulation, i",""]
["Piping",""]
["Pipe diameters are nominal internal unless otherwise stated  Where fittings have reducing ends or branches they are described as 'reducing'. In the case of pipes with diameters not exceeding 60mm only the largest end or branch diameter is given.  Should t",""]
["Fixing of pipes",""]
["Unless otherwise stated, descriptions of pipes shall be deemed to include fixing to walls etc, casting in, building in or suspending not exceeding 1m below suspension level",""]
["Insulation",""]
["Descriptions of insulation shall be deemed to include priming the pipes with zinc chromate primer before the insulation is applied, painting the insulation when completed and applying vapour barrier where specified",""]
["FIRE DETECTION",""]
["FIRE CONTROL PANEL",""]
["Supply, Install and Commission complete with battery backup and charger",""]
["Main Fire Alarm and Control Panel","No",{"v":3,"d":"3.00"}]
["Supply, Install and Commission complete with battery backup charger etc, as specified",""]
["Fire Control and Alarm Repeater Panel","No",{"v":3,"d":"3.00"}]
["DETECTORS",""]
["Supply, Install and Commission complete with bases",""]
["Smoke Detector",""]
["Supply","No",{"v":46,"d":"46.00"}]
["Fit and Commission\n ","No",{"v":46,"d":"46.00"}]
["Heat Detector",""]
["Supply","No",{"v":9,"d":"9.00"}]
["Fit and Commission\n ","No",{"v":9,"d":"9.00"}]
["Tamper-proof Smoke Detector",""]
["Supply","No",{"v":12,"d":"12.00"}]
["Fit and Commission\n ","No",{"v":12,"d":"12.00"}]
["BREAKGLASS UNITS & SIRENS",""]
["Supply. Install and Commission Standard Breakglass unit",""]
["Type 1",""]
["Supply","No",{"v":5,"d":"5.00"}]
["Fit and Commission\n ","No",{"v":5,"d":"5.00"}]
["Sirens complete with bases",""]
["Supply\n ","No",{"v":14,"d":"14.00"}]
["Fit and Commission\n \n ","No",{"v":14,"d":"14.00"}]
["CABLING",""]
["Supply, Install and Commission complete with all accessories to complete installation",""]
["Fire retardant cable PH30",""]
["Supply\n ","No",{"v":103,"d":"103.00"}]
["Fit and Commission\n \n \n ","No",{"v":103,"d":"103.00"}]
["AUTOMATED CO2 FIRE PROTECTION SYSTEM",""]
["Supply, Install and Commission complete with all accessories to complete installation",""]
["Portable Automated carbon Dioxide fire protection system incorporated in fire detection and alarm system",""]
["Supply\n ","No",{"v":1,"d":"1.00"}]
["Fit and Commission\n \n \n ","No",{"v":1,"d":"1.00"}]
["MISCELLANEOUS",""]
["Remote LED indication for Optical Smoke Sensor located in Ceiling Void complete with base",""]
["Supply\n ","No",{"v":4,"d":"4.00"}]
["Install and Commission\n \n \n ","No",{"v":4,"d":"4.00"}]
["Input/Output Module to interface Fire Alarm Panel to the Access Control System",""]
["Supply\n ","No",{"v":4,"d":"4.00"}]
["Install and Commission1\n \n \n ","No",{"v":4,"d":"4.00"}]
["Input/Output Module to interface Fire Alarm Panel to the HVAC equipment",""]
["Supply\n ","No",{"v":2,"d":"2.00"}]
["Install and Commission\n \n \n ","No",{"v":2,"d":"2.00"}]
["Compilation of 3 sets of operation and maintenance manuals including training of staff on system","No",{"v":18,"d":"18.00"}]
["Install LPG detection system in trench","No",{"v":2,"d":"2.00"}]
["Commisioning of fire detection system","No",{"v":6,"d":"6.00"}]
["Issue CoC for complete fire detection system per building","No",{"v":6,"d":"6.00"}]
["Network Card",""]
["Supply\n ","No",{"v":6,"d":"6.00"}]
["Install and Commission\n \n \n ","No",{"v":6,"d":"6.00"}]
["Remote LED",""]
["Supply\n ","No",{"v":3,"d":"3.00"}]
["Install and Commission\n \n \n ","No",{"v":3,"d":"3.00"}]
["GENERAL",""]
["Provide full 12-months guarantee on all First Aid fire fighting equipment and signage after practical completionof the entire project","Item",{"v":1,"d":"1.00"}]
["Issue CoC for complete entire fire detection system for the project","No",{"v":1,"d":"1.00"}]
["Issue a set of operation and maintenance manuals and soft copy on USB flash drive","No",{"v":6,"d":"6.00"}]
["Sundry Items ","Item",{"v":1,"d":"1.00"}]
["Issue Health & Safety File for the Fire Detection Installation","Item",{"v":1,"d":"1.00"}]
["Travelling for the entire project from base to site","Item",{"v":1,"d":"1.00"}]
["Training for the relevant skills as required by client on the Fire Detection system","Item",{"v":1,"d":"1.00"}]
["FIRE PROTECTION",""]
["SUPPLEMENTARY PREAMBLES",""]
["Specifications, drawings, etc",""]
["Tenderers are referred to the Mechanical Installation specification (see separately bound Volume 3 part 3) and drawings numbered ? to ? prepared by Ballended & Robb Consulting Engineers, accompanying these bills of quantities for the mechanical work, for ",""]
["Major equipment",""]
["Descriptions of major equipment such as chillers, air handling units and the like shall be deemed to include connections to water, air and electrical supply and/or discharge points, supports, bearers, vibration insulation mountings, filters, insulation, i",""]
["Piping",""]
["Pipe diameters are nominal internal unless otherwise stated  Where fittings have reducing ends or branches they are described as 'reducing'. In the case of pipes with diameters not exceeding 60mm only the largest end or branch diameter is given.  Should t",""]
["Fixing of pipes",""]
["Unless otherwise stated, descriptions of pipes shall be deemed to include fixing to walls etc, casting in, building in or suspending not exceeding 1m below suspension level \n \n ",""]
["Insulation",""]
["Descriptions of insulation shall be deemed to include priming the pipes with zinc chromate primer before the insulation is applied, painting the insulation when completed and applying vapour barrier where specified \n \n ",""]
["Fire Protection",""]
["Supply and install 30m fire hose reel complete with connection, valves, fittings and piping with full 12-months guarantee","No",{"v":4,"d":"4.00"}]
["Commissioning of and pressure flow test complete with results as per qualified SAQCC Fire Certified person","No",{"v":5,"d":"5.00"}]
["Allow for pressure testing of existing piping","No",{"v":5,"d":"5.00"}]
["Supply and install 4.5kg DCP fire extinguisher complete with timbeer backing board painted with pink wood primer and final coat","No",{"v":33,"d":"33.00"}]
["Certification of 4.5Kg DCP fire extinguishers as per qualified SAQCC fire certified person","No",{"v":3,"d":"3.00"}]
["Supply and install 5kg CO2 fire extinguisher complete with timber backing board painted with pink wood primer and final coat","No",{"v":9,"d":"9.00"}]
["Certification of 5Kg CO2 fire extinguishers as per qualified SAQCC fire certified person","No",{"v":5,"d":"5.00"}]
["0.81m2 - 0.9 x 0.9 fire blanket complete as indicated on drawing","No",{"v":4,"d":"4.00"}]
["Photoluminescent signs with aluminium frame to SANS 1186-1 & SANS 1186-5, complete as per the drawing and specification","No",{"v":263,"d":"263.00"}]
["Provide for a full 12-months guarantee on all First Aid Fire fighting equipment and signage after practical completion of the entire projct","Lump Sum",{"v":1,"d":"1.00"}]
["Commissioning of all fire protection equipment","Lump Sum",{"v":1,"d":"1.00"}]
["MISCELLANEOUS",""]
["Issue CoC for complete entire fire detection system for the project","No",{"v":1,"d":"1.00"}]
["Issue a set of operation and maintenance manuals and soft copy on USB flash drive","Item",{"v":1,"d":"1.00"}]
["Sundry Items ","Item",{"v":1,"d":"1.00"}]
["Issue Health & Safety File","Item",{"v":2,"d":"2.00"}]
["Travelling","Item",{"v":1,"d":"1.00"}]
["Training","Item",{"v":1,"d":"1.00"}]
["Ventilation",""]
["Work to existing HVAC installation",""]
["Inspection of existing installation and reporting on findings","No",{"v":1,"d":"1.00"}]
["Cleaning and servicing of all existing installed equipment","No",{"v":41,"d":"41.00"}]
["Kitchen canopy inspection and cleaning","No",{"v":1,"d":"1.00"}]
["Treatment of units to extend warranties","No",{"v":5,"d":"5.00"}]
["Extended warranties on all equipment for 12months after completion of complete project","No",{"v":6,"d":"6.00"}]
["CoC of complete installation","No",{"v":6,"d":"6.00"}]
["Additional Ventilation to Auditorium",""]
["Supply and install intake ducting","No",{"v":1,"d":"1.00"}]
["Supply and install FA 2 - Forced Air Fan - 4375l/s @250Pa","No",{"v":1,"d":"1.00"}]
["Supply and install sound attenuators 2D to fit above fan","No",{"v":2,"d":"2.00"}]
["Supply and install ducting as per the drawings","No",{"v":1,"d":"1.00"}]
["Supply and install control panel with VSD","No",{"v":1,"d":"1.00"}]
["Supply and install temperature sensor","No",{"v":4,"d":"4.00"}]
["Supply and install CO2 sensor","No",{"v":4,"d":"4.00"}]
["Supply and install wiring for field sensor","m",{"v":200,"d":"200.00"}]
["Supply and install RH sensor","No",{"v":4,"d":"4.00"}]
["Supply and install occupancy sensor","No",{"v":4,"d":"4.00"}]
["Verification of sensors","No",{"v":8,"d":"8.00"}]
["Supply of boulders","m³",{"v":2,"d":"2.00"}]
["Washing of boulders","m³",{"v":2,"d":"2.00"}]
["Sanitising of boulders","m³",{"v":2,"d":"2.00"}]
["Packing of boulders","m³",{"v":2,"d":"2.00"}]
["Supply of cobbles","m³",{"v":2,"d":"2.00"}]
["Washing of cobbles","m³",{"v":2,"d":"2.00"}]
["Sanitising of cobbles","m³",{"v":2,"d":"2.00"}]
["Packing of cobbles","m³",{"v":2,"d":"2.00"}]
["Core drilling 200mm diameter hole","No",{"v":5,"d":"5.00"}]
["Additional Ventilation to Reception Area",""]
["Supply and install 300 diameter whirly birds","No",{"v":1,"d":"1.00"}]
["Supply and install midwall split type air conditioning unit cooling only complete with condensing unit, piping and wall brackets. 18000 BTU/hr with condensate drain pump, auto restart and abient control.","No",{"v":2,"d":"2.00"}]
["Take from store and fix into position 350mm diameter whirly birds","No",{"v":3,"d":"3.00"}]
["Supply and install 500 diameter whirly birds","No",{"v":1,"d":"1.00"}]
["Supply and install 350mm diameter whirly birds","No",{"v":1,"d":"1.00"}]
["Supply and install 300 diameter alu-flex","m",{"v":1,"d":"1.00"}]
["Supply and install 350 diameter alu-flex","m",{"v":1,"d":"1.00"}]
["Supply and install 500 diameter alu-flex","m",{"v":1,"d":"1.00"}]
["Supply and install 300 diameter exhaust air disc valve","No",{"v":1,"d":"1.00"}]
["Supply and install 350 diameter exhaust air disc valve","No",{"v":1,"d":"1.00"}]
["Supply and install 500 diameter exhaust air disc valve","No",{"v":1,"d":"1.00"}]
["CoC of complete installation to reception area","No",{"v":1,"d":"1.00"}]
["Additional General Ventilation ",""]
["Take from store and fit 1000 x 1100 weather louvre","No",{"v":2,"d":"2.00"}]
["Take from store and fit 975 x 1000 weather louvre","No",{"v":4,"d":"4.00"}]
["Take from store and fit 975 x 1000 square ducting piece","No",{"v":4,"d":"4.00"}]
["Supply and install 1200 x 1100 weather louvre","No",{"v":1,"d":"1.00"}]
["Supply and install 1400 x 1100 weather louvre","No",{"v":1,"d":"1.00"}]
["Supply and install 1500 x 1100 weather louvre","No",{"v":1,"d":"1.00"}]
["Supply and install 1000 x 1100 weather louvre AWK Hinged and filter","No",{"v":1,"d":"1.00"}]
["Supply and install 1000 x 1100 motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 900 x 570H motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 800 x 480H motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 720 x 500 motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 900 x 570 motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 1200 x 1100 motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 1400 x 1100 motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 1500 x 1100 motorised 220V damper","No",{"v":1,"d":"1.00"}]
["Supply and install 400 x 250 neck: colour ANP357 dark umber grey matt","No",{"v":1,"d":"1.00"}]
["Supply and install 300 x 200 door grilles powder coated to architect's detail","No",{"v":6,"d":"6.00"}]
["Supply and install 400 x 200 door grilles powder coated to architect's detail","No",{"v":1,"d":"1.00"}]
["Supply and install Advantage Air SL5450 grilles","No",{"v":1,"d":"1.00"}]
["Supply and install UV resistant sealant","Litres",{"v":4500,"d":"4500.00"}]
["General",""]
["Commissioning of all HVAC equipment","Item",{"v":1,"d":"1.00"}]
["Full 12-months guarantee on all First Aid Fire fighting equipment and signage after practical completion of the entire project","Lump Sum",{"v":1,"d":"1.00"}]
["Provide CoC for the complete installation of the entire project","Item",{"v":1,"d":"1.00"}]
["Provide set of operation and maintenance manuals and soft copy on USB flash drive","No",{"v":4,"d":"4.00"}]
["Sundry items","Lump Sum",{"v":1,"d":"1.00"}]
["Health and Safety file","Lump Sum",{"v":1,"d":"1.00"}]
["Travelling","Lump Sum",{"v":1,"d":"1.00"}]
["Training","Lump Sum",{"v":1,"d":"1.00"}]
["KITCHEN INSTALLATION",""]
["Refrigeration, freezers etc.",""]
["Take from store, and put into position and install, test and commission chiller u/bar rc-1800c 1800x700mm deep with solid doors 201806192 201806193","No",{"v":2,"d":"2.00"}]
["Install, test and commission Defy chest freezer 420 litre","No",{"v":2,"d":"2.00"}]
["Take from store and Install, test and commission underbar polar top fridge 1180 x 750 915mm high","No",{"v":1,"d":"1.00"}]
["Take from store and Install, test and commission chiller u/bar rc-1800c 1800x700mm deep with solid doors 201806192","No",{"v":4,"d":"4.00"}]
["Hot surfaces, stoves, etc",""]
["Take from store, inspect for suitability and fit into position 4 burner gas stove","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability and fit into position bain marie h/cupboad: bmhc 180 Oe 5 div (1800mm) stainless steel ext 6.5kW 072/51/1815","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability and fit into position 1050 x 750 x 900mm high fl/model 155/12/0950 rgb-8 gas radiant broiler","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability, install into position, test and commission Griddle frytop (ftg10) with right hand 1/2 ribbed top-elec 090/25/4860a","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability, install into position, test and commission Fryer 2/20 litre double pan electric c/w oil receiver -30kw 400v 3ph 095/77/4526","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability, install into position, test and commission 175 x 280 x 130mm deep expanded metal tin plated fryer basket","No",{"v":4,"d":"4.00"}]
["Take from store, inspect for suitabilty, install into position, test and commission 50/pack filter paper conical code 5549 (for holder 2715404) ","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitabilty, install into position, test and commission Conical filter holder dwg 8/5452/a for vulcan fryer","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability, install into position, test and commission range r-g4: 4xopen burner lpg/oven 1000x850x910mm 118000kj/h 148/45/1966","No",{"v":2,"d":"2.00"}]
["Take from store and Install, test and commission Lainox saev101r direct steam combi steamer oven c/wcore probe & cleaning liquid la020147578","No",{"v":2,"d":"2.00"}]
["Take from store and Install, test and commission stand for naboo/sapiens 7 & 10 pan combi oven with storage under","No",{"v":2,"d":"2.00"}]
["Wash-up area, sinks etc.",""]
["Take from store and Install, test and commission dish wash table 1650x620mm inlet cw scrapehole","No",{"v":2,"d":"2.00"}]
["LAUNDRY INSTALLATION",""]
["Washers",""]
["Take from store, install, test and commission Speed Queen 6.5 kg timer operated washer extractor","No",{"v":2,"d":"2.00"}]
["Take from store, Install, test and commission Custom fire place as per architects design","No",{"v":2,"d":"2.00"}]
["Take from store, Install, test and commission comenda pc07 dishwasher hood tipe 40 racks(ph) 624x740x1460 multipower 230v~50hz 2.2kw y10095550919","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Speed Queen 6.5 kg timer operated washer extractor","No",{"v":2,"d":"2.00"}]
["Ironing",""]
["Take from store, inspect for suitability, install, test and commission Tullis 1000 x 250mm diameter electric heated flatwork ironer","No",{"v":1,"d":"1.00"}]
["Take from store, inspect for suitability, install, test and commission Bluitalia 2.2 litre steam generator with steam iron 220/50/1","No",{"v":2,"d":"2.00"}]
["Take from store, inspect for suitability, install, test and commission Bluitalia heavy duty traditional collapsable ironing board + sleeve arm ","No",{"v":2,"d":"2.00"}]
["Tables",""]
["Take from store, inspect for suitability and place in position stainless steel tables 1650mm x 750mm x 910mm laundry folding tables complete with 12-month guarantee.","No",{"v":2,"d":"2.00"}]
["Wash-up area, sinks, etc",""]
["Take from store, install, test and commission Table swb: 1050x650x910mm high 150mm s/back- stainless steel top and legs","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Table: 1850x650x915mm high 1.0mm 150mm s/back- stainless steel top and legs","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Table: 1050x650x915mm high 1.0mm 150mm s/back- stainless steel top and legs","No",{"v":2,"d":"2.00"}]
["Take from store, Install, test and commission overhead spray/pre-rinse unit: c/w 150 support brkt-w/o h&c taps","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Table swb: 1400x650x900mm high 1.0mm 430mm ss with rear splash back","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission Table shelf 1400mm solid galvanized","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission Cambro element add on shelving 910x460x1830mm (ea184272) vente","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Cambro element add on shelving 1070x460x1830mm (ea184272) vente","No",{"v":9,"d":"9.00"}]
["Take from store, install, test and commission bin dolly ibp0001-only(refuse) ingredients bins ibp0085/1085","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Vco wash hand basin 40x31cm h & c tap holes- 0759.40311.31","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission double pot bowl sink 1850x650x900mm","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission sink 1850x650x915mm vps-r304 stainless steel","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission bridging pre-rinse sink 900x620 stainless steel","No",{"v":1,"d":"1.00"}]
["Mobile units, etc",""]
["Take from store, install, test and commission refuse bin 85 litre (black) with lid code ibp1085","No",{"v":2,"d":"2.00"}]
["Take from store, install, test and commission Pot rack: mobile model mpr - 1200 x 600 x 1450mm high","No",{"v":1,"d":"1.00"}]
["Take from store, install ,test and commission 300 Piece capacity mobile crockery rack 1140x610x1010mm high 3 tier","No",{"v":1,"d":"1.00"}]
["Shelving",""]
["1.2mm thick 430 type stainless wall-mounted 2-tier shelving size 3200 x 300mm wide","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission dump table 1400x620mm c/w waste disposal & flat shelf","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission wall mounted shelving 2 tier 3000 x 300 x 1.2mm type 430","No",{"v":1,"d":"1.00"}]
["Tables, Counters, etc",""]
["Take from store, install, test and commission unheated stainless steel counter size 1300 x 750mm","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission outlet table 1650x620mm c/w basket shelf","No",{"v":1,"d":"1.00"}]
["Take from store, install, test and commission cambro element add on shelving 1220x460x1830mm (ea184872) vente","No",{"v":4,"d":"4.00"}]
["Gas Installation",""]
["Supply and Install 22mm Class copper pipe","m",{"v":78,"d":"78.00"}]
["Supply and Install 22mm Capillary 90 degree elbow","No",{"v":18,"d":"18.00"}]
["Supply and Install 22mm Capillary Equal Tee","No",{"v":5,"d":"5.00"}]
["Supply and Install 1/2\" Isolation Valve","No",{"v":5,"d":"5.00"}]
["Supply and Install 3/4\" Isolation Valve","No",{"v":5,"d":"5.00"}]
["Supply and Install Manual change-over device","No",{"v":3,"d":"3.00"}]
["Supply and Install 1/4\" Pigtail 500mm","No",{"v":10,"d":"10.00"}]
["Supply and Install High Pressure Regulator","No",{"v":9,"d":"9.00"}]
["Supply and Install Low Pressure Regulator","No",{"v":10,"d":"10.00"}]
["Supply and Install LPG 8mm Flexible Hose","No",{"v":16,"d":"16.00"}]
["Supply and Install 22mm Pipe Clamps and fixings","No",{"v":42,"d":"42.00"}]
["Supply and Install Flared Brass Fittings","No",{"v":18,"d":"18.00"}]
["Supply and Install 40mm x 40mm x 3mm Stainless Steel Angle Pedestal","No",{"v":3,"d":"3.00"}]
["Paint and label all pipeline","No",{"v":3,"d":"3.00"}]
["Supply and Install Cylinder safety chains and fixings","No",{"v":6,"d":"6.00"}]
["Supply and Install Safety signage","No",{"v":18,"d":"18.00"}]
["Supply and Install 15 - 17mm O Clips","No",{"v":30,"d":"30.00"}]
["Supply and Install 48kg LPG Cylinders and deposit","No",{"v":10,"d":"10.00"}]
["Sundries","No",{"v":3,"d":"3.00"}]
["Safety File","No",{"v":3,"d":"3.00"}]
["GENERAL",""]
["Refrigeration, freezers, etc",""]
["Existing freezer and cold rooms - inspect and service","No",{"v":1,"d":"1.00"}]
["Guarantees and Certificates of Compliance",""]
["Full 12 months guarntee on all kitchen and laundry equipment after practical completion of the entire project","No",{"v":1,"d":"1.00"}]
["Commissioning of All laundry and kitchen equipment","No",{"v":1,"d":"1.00"}]
["COC of complete installation","No",{"v":1,"d":"1.00"}]
["Sundry Items",""]
["Set of operation and maintenance manuals and soft copy on USB flash drive","No",{"v":4,"d":"4.00"}]
["Sundry items","No",{"v":1,"d":"1.00"}]
["Health and safety file","No",{"v":1,"d":"1.00"}]
["Travelling","No",{"v":1,"d":"1.00"}]
["Training","N/A",{"v":1,"d":"1.00"}]
["Supply, install and commission SABS 460 Class I copper piping ",""]
["15mm diameter ","m",{"v":85,"d":"85.00"}]
["22mm diameter ","m",{"v":85,"d":"85.00"}]
["28mm diameter ","m",{"v":80,"d":"80.00"}]
["35mm diameter ","m",{"v":71,"d":"71.00"}]
["42mm diameter ","m",{"v":14,"d":"14.00"}]
["54mm diameter ","m",{"v":14,"d":"14.00"}]
["The following in Class I copper-to-copper elbows to SANS 1067 to fit SABS 460/1 piping",""]
["15mm diameter ","No",{"v":53,"d":"53.00"}]
["22mm diameter ","No",{"v":53,"d":"53.00"}]
["28mm diameter ","No",{"v":49,"d":"49.00"}]
["35mm diameter ","No",{"v":42,"d":"42.00"}]
["42mm diameter ","No",{"v":14,"d":"14.00"}]
["54mm diameter ","No",{"v":14,"d":"14.00"}]
["The following in Class I copper pipe saddles",""]
["15mm diameter ","No",{"v":60,"d":"60.00"}]
["22mm diameter ","No",{"v":60,"d":"60.00"}]
["28mm diameter ","No",{"v":60,"d":"60.00"}]
["35mm diameter ","No",{"v":50,"d":"50.00"}]
["42mm diameter ","No",{"v":20,"d":"20.00"}]
["54mm diameter ","No",{"v":20,"d":"20.00"}]
["The following in copper-to-copper tee pieces to SANS 1067 to fit SABS 460 Class 1 piping",""]
["15mm diameter ","No",{"v":53,"d":"53.00"}]
["22mm diameter ","No",{"v":53,"d":"53.00"}]
["28mm diameter ","No",{"v":49,"d":"49.00"}]
["35mm diameter ","No",{"v":40,"d":"40.00"}]
["42mm diameter ","No",{"v":12,"d":"12.00"}]
["54mm diameter ","No",{"v":12,"d":"12.00"}]
["The following in capillary straight couplings to SANS 1067 to fit SABS 460 Class 1 piping",""]
["15mm diameter ","No",{"v":45,"d":"45.00"}]
["22mm diameter ","No",{"v":45,"d":"45.00"}]
["28mm diameter ","No",{"v":45,"d":"45.00"}]
["35mm diameter ","No",{"v":38,"d":"38.00"}]
["42mm diameter ","No",{"v":14,"d":"14.00"}]
["54mm diameter ","No",{"v":14,"d":"14.00"}]
["The following in Class I copper reducers",""]
["22mm to 15mm","No",{"v":53,"d":"53.00"}]
["28mm to 22mm","No",{"v":53,"d":"53.00"}]
["28mm to 15mm","No",{"v":53,"d":"53.00"}]
["35mm to 28mm","No",{"v":38,"d":"38.00"}]
["35mm to 22mm","No",{"v":33,"d":"33.00"}]
["Valves, DZR Brass SABS Approved etc",""]
["15mm isolating Valve","No",{"v":26,"d":"26.00"}]
["22mm Gate Valve","No",{"v":26,"d":"26.00"}]
["28mm Gate Valve","No",{"v":24,"d":"24.00"}]
["35mm Gate Valve","No",{"v":22,"d":"22.00"}]
["28mm 3-Way Manually Operated Valve","No",{"v":4,"d":"4.00"}]
["35mm 3-Way Manually Operated Valve","No",{"v":5,"d":"5.00"}]
["42mm 3-Way Manually Operated Valve","No",{"v":3,"d":"3.00"}]
["Valves, taps etc",""]
["Air/vacuum control valve capable of passing 100l/min at a pressure drop of 7kPa","No",{"v":6,"d":"6.00"}]
["Hose bib tap complete with wall plate elbow 90degrees","No",{"v":5,"d":"5.00"}]
["Supply and install",""]
["10 litre under counter compact geyser","No",{"v":1,"d":"1.00"}]
["15 litre under counter compact geyser","No",{"v":4,"d":"4.00"}]
["270 litre integrated Heat pump combination complete with 3.6kW pump unit","No",{"v":2,"d":"2.00"}]
["Solar PV water heating complete with panels (3x 470W), DC fuses/ circuit breakers","No",{"v":10,"d":"10.00"}]
["Hot water pipe insulation for pipes",""]
["15mm diameter","m",{"v":64,"d":"64.00"}]
["22mm diameter","m",{"v":52,"d":"52.00"}]
["28mm diameter","m",{"v":22,"d":"22.00"}]
["35mm diameter","m",{"v":22,"d":"22.00"}]
["Compilation of 3 sets of operation and maintenance manuals including training of staff on system","No",{"v":1,"d":"1.00"}]
["Miscellaneous",""]
["Inspection and installation on findings","No",{"v":168,"d":"168.00"}]
["Cleaning and servicing of all fittings connected to existing installation","No",{"v":168,"d":"168.00"}]
["Provide extended warranties on all equipment for 12months after completion of complete project","No",{"v":6,"d":"6.00"}]
["Issue CoC for complete of plumbing installation","No",{"v":6,"d":"6.00"}]
["SAQCC Fire certification installation","Lump Sum",{"v":1,"d":"1.00"}]
["Testing",""]
["Pressure testing of existing piping","No",{"v":6,"d":"6.00"}]
["Commissioning and pressure/flow test results as per qualified SAQCC fire certified person","No",{"v":4,"d":"4.00"}]
["Supply, install and commission SABS 460 Class I copper piping",""]
["15mm diameter ","m",{"v":60,"d":"60.00"}]
["22mm diameter ","m",{"v":63,"d":"63.00"}]
["28mm diameter ","m",{"v":53,"d":"53.00"}]
["35mm diameter ","m",{"v":38,"d":"38.00"}]
["42mm diameter ","m",{"v":10,"d":"10.00"}]
["54mm diameter ","m",{"v":5,"d":"5.00"}]
["The following in capillary elbows to SANS 1067 to fit SABS 460 Class 1 piping",""]
["15mm diameter ","No",{"v":48,"d":"48.00"}]
["22mm diameter ","No",{"v":48,"d":"48.00"}]
["28mm diameter ","No",{"v":48,"d":"48.00"}]
["35mm diameter ","No",{"v":28,"d":"28.00"}]
["42mm diameter ","No",{"v":2,"d":"2.00"}]
["54mm diameter ","No",{"v":1,"d":"1.00"}]
["The following in Class I copper pipe saddles",""]
["15mm diameter ","No",{"v":70,"d":"70.00"}]
["22mm diameter ","No",{"v":70,"d":"70.00"}]
["28mm diameter ","No",{"v":70,"d":"70.00"}]
["35mm diameter ","No",{"v":58,"d":"58.00"}]
["42mm diameter ","No",{"v":10,"d":"10.00"}]
["54mm diameter ","No",{"v":6,"d":"6.00"}]
["The following in capillary tees to SANS 1067 to fit SABS 460 Class 1 piping",""]
["15mm diameter","No",{"v":46,"d":"46.00"}]
["22m diameter","No",{"v":46,"d":"46.00"}]
["28mm diameter","No",{"v":46,"d":"46.00"}]
["35mm diameter","No",{"v":28,"d":"28.00"}]
["42mm diameter","No",{"v":2,"d":"2.00"}]
["54mm diameter","No",{"v":2,"d":"2.00"}]
["The following in Class I copper reducers",""]
["22mm to 15mm","No",{"v":33,"d":"33.00"}]
["28mm to 22mm","No",{"v":33,"d":"33.00"}]
["28mm to 15mm","No",{"v":33,"d":"33.00"}]
["35mm to 28mm","No",{"v":28,"d":"28.00"}]
["35mm to 22mm","No",{"v":28,"d":"28.00"}]
["Valves, etc",""]
["15mm isolating Valve","No",{"v":1,"d":"1.00"}]
["22mm Gate Valve","No",{"v":1,"d":"1.00"}]
["28mm Gate Valve","No",{"v":1,"d":"1.00"}]
["35mm Gate Valve","No",{"v":1,"d":"1.00"}]
["42mm 3-Way Manually Operated Valve","No",{"v":1,"d":"1.00"}]
["35mm 3-Way Manually Operated Valve","No",{"v":1,"d":"1.00"}]
["28mm 3-Way Manually Operated Valve","No",{"v":1,"d":"1.00"}]
["Air / Vacuum Control Valve - Capable of passing 100l/min @ at a pressure drop of 7kPa ","No",{"v":6,"d":"6.00"}]
["Hose Bib Tap complete with wall plate elbow 90deg","No",{"v":1,"d":"1.00"}]
["Miscellaneous",""]
["Inspection of installation and reporting on findings","Item",{"v":1,"d":"1.00"}]
["Cleaning and servicing of all fittings connected to existing installation","No",{"v":103,"d":"103.00"}]
["Provide extended warranties on all equipment for 12monts after completion of completion project","No",{"v":1,"d":"1.00"}]
["Pressure test of all existing piping","No",{"v":1,"d":"1.00"}]
["Issue CoC for comlete plumbing installation","No",{"v":1,"d":"1.00"}]
["Issue set of operation manual and soft copy on USB flash drive","No",{"v":1,"d":"1.00"}]
["Health and safety file","No",{"v":1,"d":"1.00"}]
["Traveling","Item",{"v":1,"d":"1.00"}]
["Training, where required ","Item",{"v":1,"d":"1.00"}]

{"sheet":"Sect 5","index":4,"n_rows":589,"n_cols":5,"rows_kept":589}
["Description","Uom","Quantity","Rate ","Amount"]
["SUPERVISION",""]
["The contractor to price for the following items:",""]
["Liaison with Main Contractor and for attendance for the checking of Builder's and Subcontractors work pertaining to the Electrical Installation.","Item",{"v":1,"d":"1.00"}]
["Site supervision and reporting according to the Health and Safety Specification as per this document.","Item",{"v":1,"d":"1.00"}]
["Liaison with the various ICT services with their installation and making sure all their power requirements and wireways are installed correctly, namely, CCTV, Telephone System, Data, Access Control, AV & Sound Systems, etc.","Item",{"v":1,"d":"1.00"}]
["Allowance for the connection and supply of cable and equipment for the site temporary electrical conncetions required for construction in the various areas.","Item",{"v":1,"d":"1.00"}]
["Insurance and Guarantee, pertaining to the Electrical sub-contractor","Item",{"v":1,"d":"1.00"}]
["Liaison with Eskom and relevant application for timeous connections supply.","Item",{"v":1,"d":"1.00"}]
["Nett price to comply with all the requirements of the Health & Safety specifications of the main contractor.","Item",{"v":1,"d":"1.00"}]
["Nett price for provision of 'As Built' drawings and O & M Manuals, as per specification.","Item",{"v":1,"d":"1.00"}]
["Scanned copy on CD of all items of item above.","Item",{"v":1,"d":"1.00"}]
["CABLE TRENCHES",""]
["Excavation, smoothing out of bottom of the trench, installing sand bedding and backfilling and making good as specified:",""]
["In earth","m³",{"v":120,"d":"120.00"}]
["Extra over excavation, smoothing out of bottom of the trench, installing sand bedding and backfilling and making good as specified:",""]
["In hard rock","m³",{"v":12,"d":"12.00"}]
["In soft rock","m³",{"v":36,"d":"36.00"}]
["Excavating by hand 1-100m lengths in soft material to expose existing services.","m",{"v":20,"d":"20.00"}]
["Warning tape","m",{"v":120,"d":"120.00"}]
["Class 1 PVC cable sleeves",""]
["100mm diameter","m",{"v":10,"d":"10.00"}]
["75mm diameter","m",{"v":40,"d":"40.00"}]
["50mm diameter","m",{"v":10,"d":"10.00"}]
["45 degrees slow bends for Class 1 PVC cable sleeves ",""]
["100mm diameter","No",{"v":2,"d":"2.00"}]
["75mm diameter","No",{"v":4,"d":"4.00"}]
["50mm diameter","No",{"v":2,"d":"2.00"}]
["Seal off all sleeves against the ingress of moisture, dust and vermin after all cables have been installed. (including spare leaves)","Item",{"v":1,"d":"1.00"}]
["Pyramid type cable and sleeve markers",""]
["Supply and install","No",{"v":155,"d":"155.00"}]
["GENERAL",""]
["General items, pertaining specifically to the CCTV and Access control installations.",""]
["Check existing MV installation to check for safety and faults","Item",{"v":1,"d":"1.00"}]
["MV installation safety report","Item",{"v":1,"d":"1.00"}]
["Certificate of completion for the two mini-substations","Item",{"v":1,"d":"1.00"}]
["GENERAL",""]
["General items, pertaining specifically to the CCTV and Access control installations.",""]
["Nett price for site establishment and compliance with the conditions of contract, including storage, traveling and other overheads","Lump Sum",{"v":1,"d":"1.00"}]
["Insurance and guarantee","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price to comply with all the requirements of the Health and Safety Specifications","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price for the provision of 'As Built' drawings as per specification.","Lump Sum",{"v":1,"d":"1.00"}]
["Scanned copy on CD of all items of item above.","Item",{"v":1,"d":"1.00"}]
["CCTV CAMERAS",""]
["Reference to any particular trade name, name, patent, design,type, specific origin or producer is purely to establish a standard for requirements. Products or articles of an equivalent standard may be substituted and written proof that it is equal,is to b",""]
["Supply, installation, commissioning and testing for the complete CCTV cameras as per the specification.   ",""]
["Type CM1: PTZ IP Speed dome, 35 X High Res, IP67, bracket.","No",{"v":6,"d":"6.00"}]
["Type CM2: Bullet camera, IP66 with intergrated sunshield and cable management bracket with P/T swivel","No",{"v":18,"d":"18.00"}]
["Type CM3: Fixed Indoor Mini-dome with Smoked bubble. 3.3-12mm Standard Lens","No",{"v":15,"d":"15.00"}]
["ADDITIONAL EQUIPMENT",""]
["Supply, installation, commissioning and testing additional equipment for the CCTV installationas and per the specification",""]
["Pole, 6m MH, for outdoor cameras, complete with concrete base, mounting brackets,etc","No",{"v":5,"d":"5.00"}]
["Video Edge NVR 4.0 bundled R710 with 16 camera licences 1TB boot drive +3TB video storage.","No",{"v":1,"d":"1.00"}]
["One (1) Additional Camera Licence for Video Edge NVR v4.0 and later.","No",{"v":20,"d":"20.00"}]
["Victor Site Manager, Base software including licences for two (2) concurrent user interface connections.","No",{"v":1,"d":"1.00"}]
["Controller, Touch Tracker, SensorNet, controls up to 16 cameras/domes","No",{"v":1,"d":"1.00"}]
["Mecer 3000VA 4U/2U ON-LINE SINE WAVE Rack mountable UPS,with Monitoring Software","No",{"v":1,"d":"1.00"}]
["34U CP server/ networking cabinet 4x uprights 4x feets Incl.Glands + Screws","No",{"v":2,"d":"2.00"}]
["Power rail 10 way 16A 19' rack mount ZA plug","No",{"v":1,"d":"1.00"}]
["4X FAN DROP-IN UNIVERSAL FOR CP Ver","No",{"v":1,"d":"1.00"}]
["24 Port POE Switch, Layer 3","No",{"v":3,"d":"3.00"}]
["8 Port POE Switch","No",{"v":1,"d":"1.00"}]
["Fast Ethernet Fibre Optic Data TCVR Module,10/100/Base- TX, 1300nm, (1) RJ 45 coppper port & (1) single fibre TX/RX port,SC, MM,2KM Distance","No",{"v":6,"d":"6.00"}]
["Rack for MXR units including Power Supply","No",{"v":1,"d":"1.00"}]
["Power Supply for MXRC-1 Subrack","No",{"v":1,"d":"1.00"}]
["Work Station complete, for CCTV Monitoring system to be connected to the data system","No",{"v":1,"d":"1.00"}]
["Wireless transmitter for CCTV cameras mounted on pole in remote areas","No",{"v":1,"d":"1.00"}]
["Receiver for CCTV cameras","No",{"v":4,"d":"4.00"}]
["Operational/General spares. Includes fixed cameras, power supplies etc","Lump Sum",{"v":1,"d":"1.00"}]
["GENERAL ITEMS PERTAINING TO THE CCTV INSTALLATION",""]
["Commissioning spares- Rotakin Test Target","Lump Sum",{"v":1,"d":"1.00"}]
["Work Perfomance Certificate  certificate- Handover and as built documentation, includes drawings of CCTV poles.","Lump Sum",{"v":1,"d":"1.00"}]
["Training of plant operating and technical (maintenance) staff including course materials and manuals.","Lump Sum",{"v":1,"d":"1.00"}]
["System support and maintenance post handover for a period of 3 years. Warranty on materials & workmanship 12 months.","Lump Sum",{"v":1,"d":"1.00"}]
["ACCESS CONTROL SYSTEM",""]
["Supply,installation ,commissioning and testing for the complete Access control system as per the specification.    \n \nReference to any particular trade name, name, patent, design,type, specific origin or producer is purely to establish a standard for requ",""]
["Finger print reader for entry from attack side","No",{"v":8,"d":"8.00"}]
["Egress button to exit","No",{"v":8,"d":"8.00"}]
["Glass break","No",{"v":8,"d":"8.00"}]
["Electronic lock","No",{"v":8,"d":"8.00"}]
["I/Net SCU pack. Access control","No",{"v":1,"d":"1.00"}]
["Door controller","No",{"v":8,"d":"8.00"}]
["Site controller","No",{"v":1,"d":"1.00"}]
["NPR communication controller to link database","No",{"v":2,"d":"2.00"}]
["Intercom from guard station to reception","No",{"v":1,"d":"1.00"}]
["Access Control Server with Windows 2003","No",{"v":1,"d":"1.00"}]
["24 Port Switch","No",{"v":2,"d":"2.00"}]
["Sundries- cabling, trunking","Lump Sum",{"v":1,"d":"1.00"}]
["Installation, commissioning and configuration","Lump Sum",{"v":1,"d":"1.00"}]
["Training of plant operating and technical (maintenance) staff including course materials and manuals.","Lump Sum",{"v":1,"d":"1.00"}]
["System support and maintenance post handover for a period of 3 years. Warranty on materials & workmanship 12 months.","Lump Sum",{"v":1,"d":"1.00"}]
["CABLE TRAYS",""]
["Galvanised heavy duty return flange cable trays, including short lengths, cross arms complete with hangers, brackets covers and threaded rods, couplers etc and fixed to walls",""]
["300mm wide cable tray","m",{"v":50,"d":"50.00"}]
["Extra over for",""]
["90 degrees Horizontal Elbow, internal or external.","No",{"v":2,"d":"2.00"}]
["90 degrees, internal or external riser.","No",{"v":2,"d":"2.00"}]
["Tee Piece","No",{"v":1,"d":"1.00"}]
["4-way Piece","No",{"v":1,"d":"1.00"}]
["CABLE TRAY,MEDIUM DUTY",""]
["Take from store and fix into positiion the galvanised medium duty return flange cable trays, including short lengths, cross arms complete with hangers, brackets covers and threaded rods, couplers etc and fixed to walls",""]
["300mm wide cable tray (Museum)","m",{"v":6,"d":"6.00"}]
["Galvanised medium duty return flange cable trays, including short lengths, cross arms complete with hangers, brackets covers and threaded rods, couplers etc and fixed to walls",""]
["300mm wide cable tray","m",{"v":50,"d":"50.00"}]
["Extra over for",""]
["90 degrees Horizontal Elbow, internal or external.","No",{"v":2,"d":"2.00"}]
["90 degrees, internal or external riser.","No",{"v":2,"d":"2.00"}]
["Tee Piece","No",{"v":1,"d":"1.00"}]
["4-way Piece","No",{"v":1,"d":"1.00"}]
["Trunking",""]
["P9000 Trunking complete with hangers brackets, covers and threaded rods, as indicated on the plan.",""]
["P9000 trunking, complete with splices and pvc covers.","m",{"v":50,"d":"50.00"}]
["Extra over P9000 trunking for ",""]
["End cap ","No",{"v":4,"d":"4.00"}]
["Elbow ","No",{"v":4,"d":"4.00"}]
["Tee ","No",{"v":1,"d":"1.00"}]
["4-way Junction ","No",{"v":1,"d":"1.00"}]
["Riser ","No",{"v":1,"d":"1.00"}]
["Distribution outlet ","No",{"v":2,"d":"2.00"}]
["Hanger, complete with threaded rod and all other items required to install the trunking","No",{"v":20,"d":"20.00"}]
["P8000 Trunking complete with hangers brackets, covers and threaded rods, as indicated on the plan.",""]
["P8000 white powder-coated trunking, complete with splices and galvanised covers, hangers, etc","m",{"v":50,"d":"50.00"}]
["Extra over P8000 white powder-coated trunking for",""]
["End cap ","No",{"v":4,"d":"4.00"}]
["Elbow/Risers ","No",{"v":4,"d":"4.00"}]
["Tee ","No",{"v":1,"d":"1.00"}]
["4-way Junction ","No",{"v":1,"d":"1.00"}]
["Distribution outlet ","No",{"v":1,"d":"1.00"}]
["WELDED WIRE MESH HEAVY DUTY",""]
["Take from store and fix into position 300mm wide welded wire mesh galvanised heavy duty cable tray complete with brackets, cross arms, hangers, covers and threaded rods, couplers etc.",""]
["Welded Wire Mesh HD ","m",{"v":31,"d":"31.00"}]
["Welded Wire Mesh HD 4-way piece","m",{"v":1,"d":"1.00"}]
["Tee piece","m",{"v":9,"d":"9.00"}]
["300mm wide welded wire mesh galvanised heavy duty cable tray complete with brackets, cross arms, hangers, covers and threaded rods, couplers etc.",""]
["Welded Wire Mesh HD ","m",{"v":10,"d":"10.00"}]
["Extra over 300mm wide welded wire mesh galvanised heavy duty cable for:",""]
["90 degrees Horizontal Elbow, internal or external.","No",{"v":1,"d":"1.00"}]
["Tee Piece.","No",{"v":1,"d":"1.00"}]
["4-way Piece.","No",{"v":1,"d":"1.00"}]
["90 degrees internal or external riser.","No",{"v":1,"d":"1.00"}]
["150mm wide welded wire mesh heavy duty","m",{"v":50,"d":"50.00"}]
["Extra over 150mm wide welded wire mesh heavy duty cable for:",""]
["90 degrees Horizontal Elbow, internal or external.","No",{"v":2,"d":"2.00"}]
["Tee Piece.","No",{"v":2,"d":"2.00"}]
["4-way Piece.","No",{"v":2,"d":"2.00"}]
["90 degrees internal or external riser.","No",{"v":1,"d":"1.00"}]
["GALVANISED STEEL CONDUIT",""]
["Galvanised Steel, \"Bosal\" type conduit including couplings, cutting, reaming, bending, fixing, etc. As per specification.",""]
["20mm diameter","m",{"v":205,"d":"205.00"}]
["25mm diameter","m",{"v":50,"d":"50.00"}]
["32mm diameter","m",{"v":345,"d":"345.00"}]
["20mm galvanised steel, plastic sheethed flexible tubing","m",{"v":20,"d":"20.00"}]
["CONDUIT BOXES FOR GALV. STEEL CONDUIT",""]
["65mm diameter round outlet boxes, 25mm deep, complete with covers and screws, with conduit ends",""]
["1-way for 20mm galvanised conduit","No",{"v":20,"d":"20.00"}]
["2-way for 20mm galvanised conduit","No",{"v":8,"d":"8.00"}]
["3-way for 20mm galvanised conduit","No",{"v":4,"d":"4.00"}]
["4-way for 20mm galvanised conduit","No",{"v":4,"d":"4.00"}]
["1-way for 25mm galvanised conduit","No",{"v":4,"d":"4.00"}]
["2-way for 25mm galvanised conduit","No",{"v":2,"d":"2.00"}]
["3-way for 25mm galvanised conduit","No",{"v":1,"d":"1.00"}]
["4-way for 25mm galvanised conduit","No",{"v":2,"d":"2.00"}]
["100 x 50 x 50 Recessed box - Galvanised","No",{"v":20,"d":"20.00"}]
["100 x 100 x 50 Recessed box - Galvanised","No",{"v":30,"d":"30.00"}]
["100 x 50 x 50 Surface box - Galvanised/powder coated white","No",{"v":5,"d":"5.00"}]
["100 x 100 x 50 Surface box - Galvanised/powder coated white","No",{"v":5,"d":"5.00"}]
["Connector for coupling flexible tubing, galvanised steel, plastic sheethed, 20mm, as per the specification.","No",{"v":4,"d":"4.00"}]
["CONDUCTORS",""]
["PVC insulated 600/1000V House wire copper conductors",""]
["1.5mm2 - (House Wire)","m",{"v":500,"d":"500.00"}]
["2.5mm2 - (House Wire)","m",{"v":100,"d":"100.00"}]
["4mm2 - (House Wire)","m",{"v":1000,"d":"1000.00"}]
["6mm2 - (House Wire)","m",{"v":100,"d":"100.00"}]
["10mm2 - (House Wire)","m",{"v":50,"d":"50.00"}]
["PVC insulated 600/1000V Copper conductors, for earth conductor, drawn into conduit with power wires",""]
["1.5mm2 - (House Wire)","m",{"v":250,"d":"250.00"}]
["2.5mm2 - (House Wire)","m",{"v":1200,"d":"1200.00"}]
["4mm2 - (House Wire)","m",{"v":100,"d":"100.00"}]
["6mm2 - (House Wire)","m",{"v":10,"d":"10.00"}]
["ISOLATORS",""]
["32A double pole isolator complete, flush","No",{"v":4,"d":"4.00"}]
["Weather Proof, Surface 32A double pole isolator complete","No",{"v":2,"d":"2.00"}]
["63A triple pole isolator complete.","No",{"v":6,"d":"6.00"}]
["Weather Proof, Surface 63A triple pole isolator complete.","No",{"v":2,"d":"2.00"}]
["GALVANISED DRAW WIRE",""]
["Galvanised draw wite to be drawn into conduit for Data, Telephone, Access Control, etc, installations.",""]
["Supply","m",{"v":600,"d":"600.00"}]
["SWITCHED SOCKET OUTLETS",""]
["Recessed 16A, switched socket outlet (shuttered type) complete with cover plate ",""]
["100 x 100 Single Switched Socket Outlet ","No",{"v":20,"d":"20.00"}]
["100 x 50 Single Switched Socket Outlet ","No",{"v":10,"d":"10.00"}]
["Double Switched Socket Outlet","No",{"v":40,"d":"40.00"}]
["Double Switched Socket Outlet - 1xSTD SSO & 1x2Pin Euro & SW","No",{"v":5,"d":"5.00"}]
["Double Switched Socket Outlet, dedicated,shaved earth, red.","No",{"v":10,"d":"10.00"}]
["Single SSO - Weather proof -S15","No",{"v":8,"d":"8.00"}]
["Cluster plug, Type A, consisting of 3 x 100 x 100 outlets, 1xDUO SSO&Euro, 1, Duo DED SSO and 1x with 2 RJ45 outlets, with one single cradle and galvanised recessed purpose box.","No",{"v":1,"d":"1.00"}]
["100x50, box complete with RJ45 for CCVT, Access control and Projectors","No",{"v":10,"d":"10.00"}]
["FLOOR BOX",""]
["Complete floor box with all necessary fittings, cradles covers, screws, etc.",""]
["Floor plug, complete pop-up pedestal with standard SSO. Exact position to be determined during construction.","No",{"v":5,"d":"5.00"}]
["Floor box,type B, 200x300 complete with 2xStd SSO, 2xEuro 2Pin&SW, 2xDED SSO & 2xRJ45, recessed box and all craddles and components.","No",{"v":4,"d":"4.00"}]
["Floor box,type E, 300x300 complete with 2xStd SSO, 2xEuro 2Pin&SW, 2xRJ45, recessed box and all craddles and components.","No",{"v":5,"d":"5.00"}]
["Floor box,type F, 200x300 complete with 4xStd SSO, 2xEuro 2Pin&saw, recessed box and all craddles and components.","No",{"v":8,"d":"8.00"}]
["Take from store and fix into position",""]
["Floor box lids","No",{"v":22,"d":"22.00"}]
["POWER SKIRTING",""]
["Power skirting, SABS approved, 2 tier, galvanised and powder coated, complete with covers, end caps and all accessories",""]
["Power Skirting, complete with covers, splices etc.","m",{"v":30,"d":"30.00"}]
["Extra over power skirting for:",""]
["16A switch socket skirting type complete with covers and cradles (Normal)","No",{"v":45,"d":"45.00"}]
["Euro 2- Pin, switch socket skirting type complete with switch, covers and cradles (Normal)","No",{"v":16,"d":"16.00"}]
["16A, switch socket skirting type complete with covers and cradles (Dedicated, Red, Top shaved)","No",{"v":23,"d":"23.00"}]
["Data/Telephone outlets, RJ45, skirting type complete with covers and cradles.","No",{"v":5,"d":"5.00"}]
["Internal Corners ","No",{"v":2,"d":"2.00"}]
["T Joint for risers ","No",{"v":1,"d":"1.00"}]
["End caps ","No",{"v":10,"d":"10.00"}]
["UTILITY POWER POLE",""]
["Utility Power Pole, installed at workstations to areas as indicated on the drawings, complete with covers and all accessories required for installation.",""]
["Power Pole, 4.5m, complete with covers.","No",{"v":4,"d":"4.00"}]
["Outlets box for SSO's and standard SSO","No",{"v":24,"d":"24.00"}]
["Outlets box for Data/Telephone complete with 2xRJ45 sockets.","No",{"v":16,"d":"16.00"}]
["LIGHT SWITCHES",""]
["Take from store and fix into position 16A light switches complete with cover plates and screws as per the specification.",""]
["16A, 1-lever, 1-way, 100x50","No",{"v":2,"d":"2.00"}]
["16A, 1-lever, 2-way, 100x50","No",{"v":11,"d":"11.00"}]
["16A, 2-lever, 1-way, 100x50","No",{"v":2,"d":"2.00"}]
["16A, 2-lever, 2-way, 100x50","No",{"v":5,"d":"5.00"}]
["16A, 3-lever, 1-way, 100x50","No",{"v":1,"d":"1.00"}]
["16A, 4-lever, 1-way, 100x50","No",{"v":1,"d":"1.00"}]
["16A, 4-lever, 2-way, 100x50","No",{"v":2,"d":"2.00"}]
["16A light switches complete with cover plates and screws as per the specification.",""]
["16A, 1-lever, 1-way, 100x50","No",{"v":18,"d":"18.00"}]
["16A, 1-lever, 2 way, 100x50","No",{"v":2,"d":"2.00"}]
["16A, 2-lever, 1-way, 100x50","No",{"v":4,"d":"4.00"}]
["16A, 2-lever, 2 way, 100x50","No",{"v":1,"d":"1.00"}]
["16A, 3-lever, 1 way, 100x50","No",{"v":8,"d":"8.00"}]
["16A, 4-lever, 1 way, 100x100","No",{"v":1,"d":"1.00"}]
["16A, 1-lever, \"dim press\" rocker  switch","No",{"v":2,"d":"2.00"}]
["16A, 100x50, Key switch, two way latched.","No",{"v":2,"d":"2.00"}]
["16A, weather proof switch, IP65, rocker type complete with housing, surface mount over round conduit box.","No",{"v":10,"d":"10.00"}]
["Photocell Sensor as per specification","No",{"v":5,"d":"5.00"}]
["Motion/Presence sensor Type M1, as per specification","No",{"v":9,"d":"9.00"}]
["Motion/Presence sensor Type M2, as per specification","No",{"v":4,"d":"4.00"}]
["Motion/Presence sensor Type M3, as per specification","No",{"v":3,"d":"3.00"}]
["Motion/Presence sensor Type M4, as per specification","No",{"v":1,"d":"1.00"}]
["PLUG SOCKETS FOR LUMINAIRES",""]
["5A 3pin socket outlet, unswitched, for power connection to luminaire, 60mm diameter.","No",{"v":20,"d":"20.00"}]
["LUMINAIRES",""]
["Luminaires:  Note: See the project electrical specification for the full description of acceptable luminaires.",""]
["Take from store and fix into position the following lights. (Contractor to check on the quantities of the lights in store before ordering new lights)",""]
["Light fitting Type A1 300 x 1200","No",{"v":5,"d":"5.00"}]
["Custom made nest lights","No",{"v":4,"d":"4.00"}]
["Light fitting Type A3 600 x 600","No",{"v":1,"d":"1.00"}]
["Type B1/B2","No",{"v":22,"d":"22.00"}]
["Type B3 Grey","No",{"v":10,"d":"10.00"}]
["Type D1","No",{"v":18,"d":"18.00"}]
["Type D2","No",{"v":7,"d":"7.00"}]
["Type D3","No",{"v":39,"d":"39.00"}]
["Type D7 Dimmable","No",{"v":14,"d":"14.00"}]
["Light fitting Type F1 300 x 1200","No",{"v":3,"d":"3.00"}]
["Light fitting Type F1 600 x 1200","No",{"v":9,"d":"9.00"}]
["Type F3","No",{"v":2,"d":"2.00"}]
["Type F4","No",{"v":1,"d":"1.00"}]
["Type F6","No",{"v":3,"d":"3.00"}]
["Type F8","No",{"v":18,"d":"18.00"}]
["Type G2","No",{"v":1,"d":"1.00"}]
["Type J2","No",{"v":5,"d":"5.00"}]
["Type J3","No",{"v":11,"d":"11.00"}]
["Type J4","No",{"v":2,"d":"2.00"}]
["Type L1","No",{"v":24,"d":"24.00"}]
["Type S1","No",{"v":13,"d":"13.00"}]
["Type S6","No",{"v":19,"d":"19.00"}]
["Type S7","No",{"v":12,"d":"12.00"}]
["Led driver 200W","No",{"v":4,"d":"4.00"}]
["Led driver 150W","No",{"v":6,"d":"6.00"}]
["Supply and Install:",""]
["Type A1","No",{"v":4,"d":"4.00"}]
["Type B3","No",{"v":3,"d":"3.00"}]
["Type D1","No",{"v":46,"d":"46.00"}]
["Type D2","No",{"v":17,"d":"17.00"}]
["Type D3","No",{"v":9,"d":"9.00"}]
["Type D5","No",{"v":7,"d":"7.00"}]
["Type D7","No",{"v":12,"d":"12.00"}]
["Type E1","No",{"v":3,"d":"3.00"}]
["Type E3","No",{"v":8,"d":"8.00"}]
["Type F2","No",{"v":11,"d":"11.00"}]
["Type F3","No",{"v":3,"d":"3.00"}]
["Type F4","No",{"v":1,"d":"1.00"}]
["Type F6","No",{"v":3,"d":"3.00"}]
["Type F8","No",{"v":5,"d":"5.00"}]
["Type F9","No",{"v":3,"d":"3.00"}]
["Type F10","No",{"v":4,"d":"4.00"}]
["Type G4","No",{"v":7,"d":"7.00"}]
["Type J2","No",{"v":6,"d":"6.00"}]
["Type J3","No",{"v":13,"d":"13.00"}]
["Type J4","No",{"v":2,"d":"2.00"}]
["Type K1","No",{"v":1,"d":"1.00"}]
["Type S1","No",{"v":4,"d":"4.00"}]
["Type S3","No",{"v":10,"d":"10.00"}]
["Type S4","No",{"v":13,"d":"13.00"}]
["Type S6","No",{"v":5,"d":"5.00"}]
["Type S7","No",{"v":2,"d":"2.00"}]
["Type T2","No",{"v":128,"d":"128.00"}]
["Type T3","No",{"v":56,"d":"56.00"}]
["Type T4","No",{"v":63,"d":"63.00"}]
["Type T6","No",{"v":32,"d":"32.00"}]
["LED STRIP LIGHT",""]
["LED Strip light complete with controller(s), termination, end caps, couplers and aluminium 20x20 angles and mounting screws as per the specification.",""]
["Take from store and fix in position",""]
["LED strip driver box 6 (13.7m +10m)","No",{"v":1,"d":"1.00"}]
["LED strip driver box 5 (15m)","No",{"v":2,"d":"2.00"}]
["LED strip driver box 7 (15m +13.5m)","No",{"v":1,"d":"1.00"}]
["LED strip driver box  (14.7m)","No",{"v":1,"d":"1.00"}]
["LED strip drop off  (21.8m)","No",{"v":1,"d":"1.00"}]
["LED strip PVC driver box","No",{"v":6,"d":"6.00"}]
["Supply and install:",""]
["Type C1 LED strip, 18m, completre with 1 controller and all neccessary components.","No",{"v":2,"d":"2.00"}]
["Type C2 LED strip, 10m, completre with 1 controller and all neccessary components.","No",{"v":5,"d":"5.00"}]
["Type C2 LED strip, 18m, completre with 1 controller and all neccessary components.","No",{"v":4,"d":"4.00"}]
["SPOT LIGHTS, LED TYPE T1 COMPLETE AS PER THE SPECIFICATION",""]
["Supply and install:",""]
["LED Spot light, ± 24W, 50Deg beam angle, COB, Tilt and rotation Action, Protecive Glass, 4000K, L90B10, complete with base, control gear, cabtyre and 5Aplug,","No",{"v":110,"d":"110.00"}]
["LED Spot light, ±24W, 30Deg beam angle, COB, Tilt and rotation Action, Protecive Glass, 4000K, L90B10, complete with base, control gear, cabtyre and 5Aplug,","No",{"v":62,"d":"62.00"}]
["LED Spot light, ±35W, 50Deg beam angle, COB, Tilt and rotation Action, Protecive Glass, 4000K, L90B10, complete with base, control gear, cabtyre and 5Aplug,","No",{"v":25,"d":"25.00"}]
["LED Spot light, ±17W, 24Deg beam angle, COB, Tilt and rotation Action, Protecive Glass, 4000K, L90B10, complete with base, control gear, cabtyre and 5Aplug,","No",{"v":25,"d":"25.00"}]
["LED Spot light, ±17W, 10Deg beam angle, COB, Tilt and rotation Action, Protecive Glass, 4000K, L90B10, complete with base, control gear, cabtyre and 5Aplug,","No",{"v":25,"d":"25.00"}]
["WEATHERPROOF,IP65, BOXES FOR THE LED STRIP LIGHTS COMPLETE AS PER THE SPECIFICATION",""]
["Supply","No",{"v":35,"d":"35.00"}]
["LABOUR RATE FOR ADDITIONAL ITEMS/DAY WORKS",""]
["Supervisor/ Foreman","Hrs"]
["Electrician","Hrs"]
["Labour staff","Hrs"]
["GENERAL ITEMS",""]
["General items, pertaining specifically to the Data and Telephone Installation:",""]
["Nett price for site establishment and compliance withthe conditions of contract, including storage, travelling and other overheads.","Lump Sum",{"v":1,"d":"1.00"}]
["Insurance and Guarantee.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price to comply with all the requirements of the Health & Safety specification.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price for provision of 'As Built' drawings as per specifications.","Lump Sum",{"v":1,"d":"1.00"}]
["Scanned copy on CD of all items of item above.","Lump Sum",{"v":1,"d":"1.00"}]
["FIBRE OPTIC CABLE INSTALLATION",""]
["4 Core HDD Fibre optic cable -50/125:",""]
["Supply and install","m",{"v":1500,"d":"1500.00"}]
["24 Port Duplex ST Fibre Panel",""]
["Supply and install","No",{"v":2,"d":"2.00"}]
["12 Port Duplex ST Fibre Panel",""]
["Supply and Install","m",{"v":10,"d":"10.00"}]
["Splice and terminate in splice tray by core at both ends:",""]
["Splice and terminate (core) cores","No",{"v":64,"d":"64.00"}]
["SC-SC Fibre Patch cord - 1m","No",{"v":10,"d":"10.00"}]
["ST-SC Fibre Patch cord - 1m","No",{"v":24,"d":"24.00"}]
["Test and label fibre cores at both ends","No",{"v":64,"d":"64.00"}]
["UTP INSTALLATION - CAT 6",""]
["UTP  single data outlet data outlet sockets of the RJ45 standard and mounted on power skirting, or in 100x50 box, drawbox cover plates, etc:",""]
["Supply and Install","No",{"v":128,"d":"128.00"}]
["UTP cable installed on cable tray, in cable trunking, sleeves, etc.:",""]
["Supply and Install","m",{"v":2500,"d":"2500.00"}]
["Marking of UTP data outlet sockets as specified:",""]
["Supply and Install","No",{"v":128,"d":"128.00"}]
["Marking of UTP data cable installation at patch panels in distribution cabinets:",""]
["Supply and Install","No",{"v":128,"d":"128.00"}]
["Patch leads for patching of UTP connections at patch panels:",""]
["Supply and Install","No",{"v":128,"d":"128.00"}]
["Marking of patch leads at both ends as specified (allow for markings per lead):",""]
["Supply and Install","No",{"v":128,"d":"128.00"}]
["Testing, recording of test results and reporting for each UTP cable connection as specified:",""]
["Connections tested (UTP)","No",{"v":128,"d":"128.00"}]
["Documentation",""]
["DISTRIBUTION CABINETS",""]
["Distribution cabinets with basic equipment, i.e cooling fans, power sockets, cable tray for cable mounting, support structure for mounting of the cabling:",""]
["47U 600mm x 1000mm deep with plinth:",""]
["Supply and Install","No",{"v":1,"d":"1.00"}]
["9U x 600 Swing Wall Mounted:",""]
["Supply and Install","No",{"v":8,"d":"8.00"}]
["Brush panels for mounting between patch panels.",""]
["Supply and Install","No",{"v":36,"d":"36.00"}]
["Patch panels as specified:",""]
["Supply- 24 Port","No",{"v":24,"d":"24.00"}]
["Spare shelves and blank face plates (Supply and install):",""]
["Shelves","No",{"v":11,"d":"11.00"}]
["Blank face plates 1 U","No",{"v":13,"d":"13.00"}]
["Blank face plates 2  U","No",{"v":17,"d":"17.00"}]
["Fly leads of 3m length with RJ11  male connectors to connect telephones in the RJ45 telephone outlets:",""]
["Supply and Install","No",{"v":128,"d":"128.00"}]
["ACTIVE NETWORK COMPONENTS",""]
["Supply, installation, commisssioning, testing, and training for the complete data system as per the specification.  Reference to any particular tradename, name, patent, design, type specific origin or producer is purelyto establish a standard for requirem",""]
["Cisco Catlyst 3560 48 10/100/1000T Port Switch with 4 SPF ports as per specification.",""]
["Supply","No",{"v":6,"d":"6.00"}]
["Cisco Catalyst 3560 48 10/100/1000T Port Switch with 4 SPF ports as specified:",""]
["Supply and Install","No",{"v":1,"d":"1.00"}]
["Cisco Catalyst 2960 48 10/100 ports and 2 fixed Ethernet 10/100/1000T uplink ports switch as specified:",""]
["Supply and Install","No",{"v":8,"d":"8.00"}]
["UPS",""]
["UPS, Rack mountable, 3000 VA 4uU / ON-LINE SINE WAVE, with Monitoring Software","No",{"v":2,"d":"2.00"}]
["TELEPHONE",""]
["Telephone system:",""]
["PABX unit, wall mounted to connect to the Telkom incoming line, as specified.","No",{"v":1,"d":"1.00"}]
["Fibre Router - 1Gbps","No",{"v":1,"d":"1.00"}]
["All cables and wiring required to connect to data network and patch panels.","Item",{"v":1,"d":"1.00"}]
["Telephones IP units as to communicate with the PABX:",""]
["Receptionist console","No",{"v":2,"d":"2.00"}]
["Fixed IP Phone with display","No",{"v":11,"d":"11.00"}]
["Fixed IP Phone - no display","No",{"v":13,"d":"13.00"}]
["Portable handset with base","No",{"v":8,"d":"8.00"}]
["Fax line point","No",{"v":7,"d":"7.00"}]
["Additional equipment required to complete the installation in accordance with the specified requirements:","Lump Sum",{"v":1,"d":"1.00"}]
["EARTH CONDUCTORS",""]
["CABLES",""]
["Supply, install, terminate and commissioning the following 600/1000 V PVC/PVC/SWA/ECC/PVC copper cable as specified.",""]
["150 mm², 4-core","m",{"v":10,"d":"10.00"}]
["35 mm², 4-core","m",{"v":10,"d":"10.00"}]
["16 mm², 4-core","m",{"v":50,"d":"50.00"}]
["6 mm², 4-core","m",{"v":50,"d":"50.00"}]
["2.5 mm², 3-core","m",{"v":100,"d":"100.00"}]
["2.5 mm², 3-core, HN5 submersible cable","m",{"v":150,"d":"150.00"}]
["CABLE TERMINATION",""]
["For PVC/PVC/SWA/ECC/PVC cables, including armour glands, shrouds, lugs, connections, insulation tape, cadmium plated bolts, nuts, spring- washers, etc.",""]
["150 mm², 4-core","No",{"v":2,"d":"2.00"}]
["35 mm², 4-core","No",{"v":2,"d":"2.00"}]
["16 mm², 4-core","No",{"v":4,"d":"4.00"}]
["6 mm², 4-core","No",{"v":4,"d":"4.00"}]
["2.5 mm², 3-core","No",{"v":10,"d":"10.00"}]
["2.5 mm², 3-core, HN5 submersible cable","No",{"v":10,"d":"10.00"}]
["BARE EARTH COPPER CONDUCTORS INSTALLED WITH SUPPLY CABLES",""]
["Bare copper earth conductors laid with cable in trenches or sleeve pipes and bonded to cables with plastic strapping at 2m centres",""]
["70mm²","m"]
["25mm²","m"]
["16mm²","m"]
["10mm²","m"]
["Bare Earth Copper Conductor Terminations (inlcuding lugs and other necessary equipment)",""]
["70mm²","No"]
["25mm²","No"]
["16mm²","No"]
["10mm²","No"]
["EARTHING INSTALLATION",""]
["Supply and install the project main earthing installation complete with all necessary equipment e.g electrodes, copper conductors, draw boxes, terminations on main earth bar etc. To comply with Supply Authority requirements and the Specification.","Lump Sum",{"v":1,"d":"1.00"}]
["Bonding of taps and hand wash basins.","Lump Sum",{"v":1,"d":"1.00"}]
["Bonding of gutters and down pipes","Lump Sum",{"v":1,"d":"1.00"}]
["Earthing continuity tests","Lump Sum",{"v":1,"d":"1.00"}]
["Testing and Commissioning of project main earthing installation to the satisfaction of the Supply Authority. (including earth resistance tests)","Lump Sum",{"v":1,"d":"1.00"}]
["Supply and Install the earthing to the mini-substation. The contractor is to obtain the services of Messrs. Lightning Protection and Earthing Systems to complete this installation and provide the relevant certificates for both LV and MV earthing as per th","Lump Sum",{"v":1,"d":"1.00"}]
["Distribution Boards",""]
["Supply and Install in position the following distribution board, complete with trays, labels, conduit and trunking terminations as required and all other necessary items as per the specification. \n \n ",""]
["DB-SUMP 2","No",{"v":1,"d":"1.00"}]
["DB-E-STG","No",{"v":1,"d":"1.00"}]
["DB-SUMP3","No",{"v":1,"d":"1.00"}]
["Test the following distribution board, complete with trays, labels, conduit and trunking terminations as required and all other necessary items as per the specification.",""]
["DB-LV1","No",{"v":1,"d":"1.00"}]
["DB-M1","No",{"v":1,"d":"1.00"}]
["DB-M2","No",{"v":1,"d":"1.00"}]
["DB-M3","No",{"v":1,"d":"1.00"}]
["SUMP 1","No",{"v":1,"d":"1.00"}]
["DB-GP","No",{"v":1,"d":"1.00"}]
["DB-LV 2","No",{"v":1,"d":"1.00"}]
["DB-E1","No",{"v":1,"d":"1.00"}]
["DB-E2","No",{"v":1,"d":"1.00"}]
["DB-E3","No",{"v":1,"d":"1.00"}]
["DB-R","No",{"v":1,"d":"1.00"}]
["DB-L","No",{"v":1,"d":"1.00"}]
["DB-D","No",{"v":1,"d":"1.00"}]
["DB-GH","No",{"v":1,"d":"1.00"}]
["DISTRIBUTION KIOSK",""]
["Test the following distribution kiosks, complete with trays, labels, conduit and trunking terminations and concrete base, as required and all other necessary items as per the specification.",""]
["KS-B","No",{"v":1,"d":"1.00"}]
["KS-SRG","No",{"v":1,"d":"1.00"}]
["KS-SD","No",{"v":1,"d":"1.00"}]
["UPS",""]
["Nett price for the Supply, Install and Commission of a 20kVA UPS complete with 5 year batteries to run for 30min, as per the specification.","No",{"v":2,"d":"2.00"}]
["Nett price for the Supply, Install and Commission of a 10kVA UPS complete with 5 year batteries to run for 30min, as per the specification.","No",{"v":1,"d":"1.00"}]
["GENERAL",""]
["Prelimiminary and General items, pertaining specifically to the Audio Visual Installation:",""]
["Nett price for site establishment and compliance with the conditions of contract, including storage, travelling and other overheads.","Lump Sum",{"v":1,"d":"1.00"}]
["Insurance and Guarantee.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price to comply with all the requirements of the Health & Safety specification.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price for provision of 'As Built' drawings as per specifications.","Lump Sum",{"v":1,"d":"1.00"}]
["Scanned copy on CD of all items of item above.","Lump Sum",{"v":1,"d":"1.00"}]
["AUDITORIUM LIGHTING AND AUDIO SYSTEM",""]
["Supply,installation,commissioning and testing additional equipment for the Audio Visual installation and as per the specification.",""]
["Martin MAC Aura RGBW LED Wash Moving Light.","No",{"v":2,"d":"2.00"}]
["Martin MAC 350 Entour LED Profile Moving Light.","No",{"v":2,"d":"2.00"}]
["Martin M2Go controler","No",{"v":1,"d":"1.00"}]
["ELO 22' Touch screen for M-Series","No",{"v":1,"d":"1.00"}]
["Movinlight Roof Mount Bracket","No",{"v":4,"d":"4.00"}]
["Versa Light LED High Bright 1M Strip RGB","No",{"v":6,"d":"6.00"}]
["Versa Light LED Amber/White High/Power","No",{"v":2,"d":"2.00"}]
["Denon DN-4500 Dual CD/Mp 3 Player","No",{"v":1,"d":"1.00"}]
["Sennheser EW-500/845 Wireless Hand Held System","No",{"v":2,"d":"2.00"}]
["Sennheiser EW-66 Riffle Microphone wiyh K6 Power Module.","No",{"v":2,"d":"2.00"}]
["Martin Audio W 8- 4X8'Differential Dispersion System.","No",{"v":1,"d":"1.00"}]
["Martin Audio DD-6 Ultra-compact Differential Dispersion System","No",{"v":2,"d":"2.00"}]
["MC Squared E- 100 Power Amplifier four channel.","No",{"v":1,"d":"1.00"}]
["DC 10484 In, 8 Out Matrix/MIXER WITH FULL dsp, CORE","No",{"v":1,"d":"1.00"}]
["Presonus 24:4:2 S tudio Live Digital Mixer","No",{"v":1,"d":"1.00"}]
["Sommer 8 pair Audio Multi-core","m",{"v":180,"d":"180.00"}]
["8 way stage box with 3 pin Xlr 6 input 2 output","No",{"v":3,"d":"3.00"}]
["Equipment Rack 16U","No",{"v":1,"d":"1.00"}]
["Cabling","Lump Sum",{"v":1,"d":"1.00"}]
["Installation Items, Plugs, connectors, trunking etc","Lump Sum",{"v":1,"d":"1.00"}]
["Installation & Testing","Lump Sum",{"v":1,"d":"1.00"}]
["AUDIO VISUAL EQUIPMENT FOR THE CLASSROMS,BOARDROOM, FILMROOM,AND PRESENTATION AREAS.",""]
["Supply,installation,commissioning and testing additional equipment for the CCTV installation and as per the specification.  Reference to any particular tradename, name, patent, design,type, specific origin or producer is purely to establish a standard for",""]
["Christie LX-400 LCD XGA Projector (inc standard 1.5-1.8:1 zoom lens) Black","No",{"v":11,"d":"11.00"}]
["Projection Screen Electric 16:9 Ratio 3620mm x 2080mm","No",{"v":11,"d":"11.00"}]
["Quad Industrial C 8 Ceiling Speaker - Set of 4","No",{"v":11,"d":"11.00"}]
["Dsppa MP-300 60 watt mixer amplifier","No",{"v":11,"d":"11.00"}]
["Dsan Laptop Sound Port (Custom) Built into wall Box 50x100","No",{"v":11,"d":"11.00"}]
["In Ceiling Wall mount rack 4 U","No",{"v":11,"d":"11.00"}]
["VGA","No",{"v":11,"d":"11.00"}]
["VGA Patch Point","No",{"v":11,"d":"11.00"}]
["5m VGA & Audio Fly lead","No",{"v":11,"d":"11.00"}]
["Cabling","Lump Sum",{"v":1,"d":"1.00"}]
["Installation items, Plugs, connectors, trunking etc","Lump Sum",{"v":1,"d":"1.00"}]
["Installation  & Testing","Lump Sum",{"v":1,"d":"1.00"}]
["GENERAL",""]
["General items, pertaining specifically to the Lightning Protection and Earthing System.",""]
["Nett price for site establishment and compliance with the conditions of contract, including storage, travelling and other overheads.","Lump Sum",{"v":1,"d":"1.00"}]
["Insurance and Guarantee.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price to comply with all the requirements of the Health & Safety specification.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price for provision of 'As Built' drawings as per specifications.","Lump Sum",{"v":1,"d":"1.00"}]
["Scanned copy on CD of all items of item above.","Lump Sum",{"v":1,"d":"1.00"}]
["LIGHTNING PROTECTION",""]
["Reception building:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["Educational, Auditorium and Maintenance buildings:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["Living heritage workshops and restaurant:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["Dormitories buiding:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["Museum building:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["Great place of celebration:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["Guard house building:",""]
["Risk and existing installation analysis by specialist.","Lump Sum",{"v":1,"d":"1.00"}]
["Details of new design of Lighting protection system to suit site conditions","Lump Sum",{"v":1,"d":"1.00"}]
["Air termination system to be checked on compliance and adjusted where required","Lump Sum",{"v":1,"d":"1.00"}]
["Down conductor to be moved to more concealed and not on main face of building","Lump Sum",{"v":1,"d":"1.00"}]
["Earth termination system connections to be checked and verified ","Lump Sum",{"v":1,"d":"1.00"}]
["Downconductor bonding to earth termination system","Lump Sum",{"v":1,"d":"1.00"}]
["All labour, testing and issuing of the appropriate COC's.","Lump Sum",{"v":1,"d":"1.00"}]
["GENERAL",""]
["General items, pertaining specifically to the Building Management System:",""]
["Nett price for site establishment and compliance with the conditions of contract, including storage, travelling and other overheads.","Lump Sum",{"v":1,"d":"1.00"}]
["Insurance and Guarantee.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price to comply with all the requirements of the Health & Safety specification.","Lump Sum",{"v":1,"d":"1.00"}]
["Nett price for provision of 'As Built' drawings as per specifications.","Lump Sum",{"v":1,"d":"1.00"}]
["Scanned copy on CD of all items of item above.","Lump Sum",{"v":1,"d":"1.00"}]
["BMS SYSTEM",""]
["PC, complete with screen, keyboard, mouse, box, etc. as per specification for the building management system.","Lump Sum",{"v":1,"d":"1.00"}]
["40 inch flat LED screen, to be mounted in the reception to indicate certain criteria relevant to the centre.","No",{"v":1,"d":"1.00"}]
["SCADA, as specified, incorporated with the Data network system","Lump Sum",{"v":1,"d":"1.00"}]
["Training of plant operating and technical (maintenance) staff including course materials and manuals.","Lump Sum",{"v":1,"d":"1.00"}]
["System support and maintenance post handover for a period of 3 years. Warranty on materials & workmanship 12 months.","Lump Sum",{"v":1,"d":"1.00"}]

{"sheet":"Sect 6","index":5,"n_rows":258,"n_cols":5,"rows_kept":258}
["Description","Uom","Quantity","Rate","Amount"]
["CREDIT FOR MATERIALS ON SITE - RELATING TO BUILDING WORKS (PROVISIONAL)",""]
["Note: The Note : The following materials have been left on site by the previous contractor and are intended for the works. Tenderers\nare expected to utilize these materials and therefore provide credit by pricing a negative price against each item \nThere ",""]
["GENERAL MATERIALS",""]
["Brown roof stone","Tonnes",{"v":21,"d":"21.00"}]
["White roof stone\n ","Tonnes",{"v":4,"d":"4.00"}]
["Stonecor Prostruct (per 20L)","No",{"v":7,"d":"7.00"}]
["Epidermix 344 (per 1L)","No",{"v":4,"d":"4.00"}]
["Epidermix 395 (per 2L)","No",{"v":5,"d":"5.00"}]
["Super Power Clean (per 5L)","No",{"v":8,"d":"8.00"}]
["Plywood shutter board (size to be confirmed)","No",{"v":10,"d":"10.00"}]
["PRECAST CONCRETE MATERIALS",""]
["1200mm long lintels","No",{"v":11,"d":"11.00"}]
["1500mm long lintels","No",{"v":10,"d":"10.00"}]
["2100mm long lintels","No",{"v":11,"d":"11.00"}]
["1000mm long window cills","No",{"v":29,"d":"29.00"}]
["2000mm long window cills","No",{"v":34,"d":"34.00"}]
["Full set of rib rite precast auditorium beams ","Item",{"v":1,"d":"1.00"}]
["WATERPROOFING MATERIALS",""]
["Dividing angles (6m lengths)","No",{"v":186,"d":"186.00"}]
["Service screen ducts 420 x 1000mm high","No",{"v":2,"d":"2.00"}]
["Service screen ducts 370 x 1000mm high","No",{"v":3,"d":"3.00"}]
["Roof wire rolls","No",{"v":9,"d":"9.00"}]
["Gabion boxes size 2000 x 500 x 500mm","No",{"v":25,"d":"25.00"}]
["Malthoid rolls (20m roll)","No",{"v":11,"d":"11.00"}]
["ABE membrane (10m)","No",{"v":9,"d":"9.00"}]
["Unigum rolls (10m)","No",{"v":17,"d":"17.00"}]
["Dimple sheet ABE drain (10m roll)","No",{"v":1,"d":"1.00"}]
["Chryso Deco Lav (25L)","No",{"v":10,"d":"10.00"}]
["Acrylic primer ABE (20L)","No",{"v":11,"d":"11.00"}]
["Cemflex waterproofing (20L)","No",{"v":5,"d":"5.00"}]
["Bitugrip (25L)","No",{"v":4,"d":"4.00"}]
["ABE Brixeal (20L)","No",{"v":5,"d":"5.00"}]
["Damp Proof Course (Rolls)","No",{"v":60,"d":"60.00"}]
["CARPENTRY SUNDRIES",""]
["Sand Paper","No",{"v":213,"d":"213.00"}]
["TIMBER MATERIALS",""]
["Timber double door frame 1500 x 2120mm","No",{"v":1,"d":"1.00"}]
["Timber double door frame 1720 x 2130mm","No",{"v":1,"d":"1.00"}]
["Timber double door frame 1720 x 2430mm","No",{"v":1,"d":"1.00"}]
["Timber double door frame 1600 x 2200mm","No",{"v":1,"d":"1.00"}]
["Single timber doors","No",{"v":2,"d":"2.00"}]
["Timber doors 900 x 2100mm","No",{"v":1,"d":"1.00"}]
["Timber doors 930 x 2465mm","No",{"v":1,"d":"1.00"}]
["Quadrant bead (3m length)","No",{"v":15,"d":"15.00"}]
["CEILINGS & PARTITIONS MATERIALS",""]
["Armstrong ceiling tiles (Box)","No",{"v":1,"d":"1.00"}]
["Ceiling sheets","No",{"v":72,"d":"72.00"}]
["Shadowline wall angle","No",{"v":20,"d":"20.00"}]
["Rock fibre (10/Box)","No",{"v":16,"d":"16.00"}]
["Reed mat (Rolls)","No",{"v":11,"d":"11.00"}]
["White boards","No",{"v":8,"d":"8.00"}]
["FURNITURE AND RELATED ITEMS",""]
["76C Help desk","No",{"v":1,"d":"1.00"}]
["80A Cupboards","No",{"v":1,"d":"1.00"}]
["80B Cupboards","No",{"v":1,"d":"1.00"}]
["80C Help desk","No",{"v":1,"d":"1.00"}]
["81A Help desk","No",{"v":1,"d":"1.00"}]
["81C Cupboards","No",{"v":1,"d":"1.00"}]
["81E Help desk","No",{"v":1,"d":"1.00"}]
["81F Desk","No",{"v":1,"d":"1.00"}]
["82F Bench","No",{"v":1,"d":"1.00"}]
["83A Bench","No",{"v":1,"d":"1.00"}]
["83B Bench","No",{"v":1,"d":"1.00"}]
["84I Trollies","No",{"v":2,"d":"2.00"}]
["Filing cabinet (Furniture)","No",{"v":4,"d":"4.00"}]
["STEEL (STRUCTURAL AND STAINLESS) MATERIALS",""]
["Gum poles","No",{"v":45,"d":"45.00"}]
["Gum pole steel brackets","No",{"v":14,"d":"14.00"}]
["Stainless steel plate 800 x 150mm","No",{"v":2,"d":"2.00"}]
["Stainless steel plate 800 x 200mm","No",{"v":6,"d":"6.00"}]
["Stainless steel plate 800 x 300mm","No",{"v":4,"d":"4.00"}]
["IPE200 Columns with base plates(not glavanized)","Tonnes",1.12]
["IPE200 Rafters(not glavanized)","Tonnes",{"v":1,"d":"1.00"}]
["200 Section Curved portion (Not glavanized)","Tonnes",{"v":1,"d":"1.00"}]
["90x6mm Flat bars (Not galvanized)","Tonnes",{"v":2,"d":"2.00"}]
["Reception structure","Tonnes",{"v":1,"d":"1.00"}]
["METALWORK MATERIALS",""]
["Mesh sheet (3000 x 2000mm Type45)","No",{"v":9.5,"d":"9.50"}]
["Brickforce (rolls)","No",{"v":150,"d":"150.00"}]
["Hoop iron (rolls)","No",{"v":9,"d":"9.00"}]
["Wire tie bundle","No",{"v":9,"d":"9.00"}]
["Roofing brackets (per box)","No",{"v":7,"d":"7.00"}]
["Gate 2 - Education","No",{"v":1,"d":"1.00"}]
["Gate 1 - Education","No",{"v":1,"d":"1.00"}]
["Gate 1 - Dormotories","No",{"v":1,"d":"1.00"}]
["External Fire","No",{"v":1,"d":"1.00"}]
["Reception SS Sign","No",{"v":1,"d":"1.00"}]
["PLASTERING MATERIALS",""]
["Terelyne flicking machine","No",{"v":7,"d":"7.00"}]
["Sika grout (bags)","No",{"v":30,"d":"30.00"}]
["Crete Stone Skimming plaster (Bags)","No",{"v":9,"d":"9.00"}]
["Backing Chords 10mm ","m",{"v":90,"d":"90.00"}]
["Sikaflex expansion joint sealant","No",{"v":89,"d":"89.00"}]
["SikaTop (5 Litre)","No",{"v":6,"d":"6.00"}]
["SikaTop (1.75 Litre)","No",{"v":2,"d":"2.00"}]
["SikaTop Seal (Bags)","No",{"v":6,"d":"6.00"}]
["Duraflex","No",{"v":129,"d":"129.00"}]
["Flexothane 27 Sika 11FC Sealant (Tube)","No",{"v":6,"d":"6.00"}]
["Plaster primer (20 Litre)","No",{"v":1,"d":"1.00"}]
["Coverland waterproof vapour","No",{"v":30,"d":"30.00"}]
["TILING MATERIALS",""]
["Dorma sealing compound","No",{"v":6,"d":"6.00"}]
["White Tiles 200 x 200mm (1.52m2/box)","No",4.56]
["John Deco black tile (1.8m2/box)","No",{"v":1,"d":"1.00"}]
["Grout (20kg Bags)","No",{"v":23,"d":"23.00"}]
["Tile magic flexi grip (20kg Bags)","No",{"v":32,"d":"32.00"}]
["300 x 200mm Slate tiles","m²",{"v":35.4,"d":"35.40"}]
["PLUMBING MATERIALS",""]
["Shower rose and arm","No",{"v":2,"d":"2.00"}]
["Spouts for dorm","No",{"v":10,"d":"10.00"}]
["Paraplegic mixer","No",{"v":3,"d":"3.00"}]
["Gauges","No",{"v":3,"d":"3.00"}]
["Flexi Hose","No",{"v":1,"d":"1.00"}]
["15mm extension piece","No",{"v":1,"d":"1.00"}]
["Ring for manhole","No",{"v":1,"d":"1.00"}]
["32mm HDPE female elbow","No",{"v":2,"d":"2.00"}]
["22mm Ball-O-Stop","No",{"v":2,"d":"2.00"}]
["15mm Ball-O-Stop","No",{"v":1,"d":"1.00"}]
["22mm Connc brass fitting","No",{"v":7,"d":"7.00"}]
["28mm Connc brass fitting","No",{"v":8,"d":"8.00"}]
["S/S nozzel to healing pond","No",{"v":12,"d":"12.00"}]
["350mm core fitting hose","No",{"v":4,"d":"4.00"}]
["Basin mixer(long shaft) raise karoo","No",{"v":1,"d":"1.00"}]
["Weaver basin","No",{"v":1,"d":"1.00"}]
["Basin waste pop up","No",{"v":25,"d":"25.00"}]
["Sink waste","No",{"v":4,"d":"4.00"}]
["15mm Demand tap","No",{"v":1,"d":"1.00"}]
["15mm Angle valve","No",{"v":12,"d":"12.00"}]
["28mm Master bat","No",{"v":15,"d":"15.00"}]
["75mm Grey pvc 45 degree bend","No",{"v":2,"d":"2.00"}]
["50mm Grey pvc 90 degree bend","No",{"v":5,"d":"5.00"}]
["50mm diameter pvc female STR connect","No",{"v":6,"d":"6.00"}]
["Toilet seat","No",{"v":6,"d":"6.00"}]
["Chrome bottle trap FBT18","No",{"v":33,"d":"33.00"}]
["Underwall stop taps","No",{"v":44,"d":"44.00"}]
["Tubes of silicone sealant","No",{"v":16,"d":"16.00"}]
["Basin bracket","No",{"v":1,"d":"1.00"}]
["Pump control float switch","No",{"v":1,"d":"1.00"}]
["S/S tee 80mm diameter","No",{"v":2,"d":"2.00"}]
["Black basin (Lecico Nile)","No",{"v":15,"d":"15.00"}]
["15mm Niplo fitting","No",{"v":6,"d":"6.00"}]
["22mm Niplo fitting","No",{"v":2,"d":"2.00"}]
["22mm GMS fitting","No",{"v":1,"d":"1.00"}]
["15mm conncx fitting","No",{"v":30,"d":"30.00"}]
["28mm conncx brass fitting","No",{"v":1,"d":"1.00"}]
["Double bowl trap for sinks SP2","No",{"v":3,"d":"3.00"}]
["Double bowl sink","No",{"v":1,"d":"1.00"}]
["15mm Pillar tap","No",{"v":6,"d":"6.00"}]
["80mm Diameter GMS puddle pipe 500mm long flanged","No",{"v":5,"d":"5.00"}]
["80 x 50mm flanged reducer piece","No",{"v":4,"d":"4.00"}]
["110mm R.I rodding eye","No",{"v":5,"d":"5.00"}]
["160mm R.I rodding eye","No",{"v":1,"d":"1.00"}]
["15mm BIB tap","No",{"v":19,"d":"19.00"}]
["28mm Diameter brass gate valve","No",{"v":1,"d":"1.00"}]
["28mm HDPE male STR connector","No",{"v":4,"d":"4.00"}]
["110mm Diameter pan connector","No",{"v":3,"d":"3.00"}]
["110mm Diameter kimberly socket","No",{"v":5,"d":"5.00"}]
["28mm diameter HDPE Saddle","No",{"v":3,"d":"3.00"}]
["22mm Brass gate valve","No",{"v":2,"d":"2.00"}]
["22mm GMS nipple","No",{"v":2,"d":"2.00"}]
["50mm Diameter HDPE STR connector","No",{"v":11,"d":"11.00"}]
["75mm Diameter HDPE elbow\n ","No",{"v":1,"d":"1.00"}]
["28mm Diameter brass gate valve ","No",{"v":4,"d":"4.00"}]
["50mm Diameter flanged gate valve blue with key","No",{"v":1,"d":"1.00"}]
["160mm Diameter gully and cap","No",{"v":4,"d":"4.00"}]
["110mm Diameter gully and cap","No",{"v":4,"d":"4.00"}]
["110mm Diameter saddle","No",{"v":4,"d":"4.00"}]
["50mm HDPE reducing tee","No",{"v":1,"d":"1.00"}]
["32mm HDPE male straight connector","N/A",{"v":3,"d":"3.00"}]
["50mm HDPE female straight connector","No",{"v":3,"d":"3.00"}]
["75mm HDPE bend","No",{"v":12,"d":"12.00"}]
["75mm HDPE straight connector","No",{"v":5,"d":"5.00"}]
["75mm HDPE Tee","No",{"v":2,"d":"2.00"}]
["160mm diameter PVC bend","No",{"v":1,"d":"1.00"}]
["110mm diameter PVC bend","No",{"v":1,"d":"1.00"}]
["Precast gully","No",{"v":1,"d":"1.00"}]
["Fire cement channel (Manhole)","No",{"v":6,"d":"6.00"}]
["Spoilt bottom trap","No",{"v":3,"d":"3.00"}]
["Paraplegic shower seat","No",{"v":1,"d":"1.00"}]
["50mm Diameter HDPE end cap","No",{"v":4,"d":"4.00"}]
["32mm Diameter HDPE end cap","No",{"v":3,"d":"3.00"}]
["110mm Diameter PVC water bems (build pressure)","No",{"v":4,"d":"4.00"}]
["Fire hose reel","No",{"v":1,"d":"1.00"}]
["160mm Diameter PVC watch bend (ditto)","No",{"v":2,"d":"2.00"}]
["Bag bolts and nuts","No",{"v":1,"d":"1.00"}]
["28mm Diameter copper pipe 6m long","No",{"v":1,"d":"1.00"}]
["GLAZING MATERIALS",""]
["Round Mirror","No",{"v":38,"d":"38.00"}]
["Mirror (Sample)","No",{"v":1,"d":"1.00"}]
["Oval Mirror","No",{"v":6,"d":"6.00"}]
["PAINTING MATERIALS",""]
["Paint (20 Litre)","No",{"v":8,"d":"8.00"}]
["Primer (20 Litre)","No",{"v":2,"d":"2.00"}]
["Pink Wood Primer (5 Litre)","No",{"v":2,"d":"2.00"}]
["Velvaglo plascon (5 Litre)","No",{"v":8,"d":"8.00"}]
["Professional wall coat (20 Litre)","No",{"v":13,"d":"13.00"}]
["ELECTRICAL INSTALLATION MATERIALS",""]
["Nest Lights (LHW & R))","No",{"v":4,"d":"4.00"}]
["Light fitting Type B3 grey","No",{"v":10,"d":"10.00"}]
["Light fitting Type G2","No",{"v":1,"d":"1.00"}]
["Light fitting Type B1/B2","No",{"v":22,"d":"22.00"}]
["Light fitting Type J2","No",{"v":5,"d":"5.00"}]
["Light fitting Type S1","No",{"v":13,"d":"13.00"}]
["Light fitting Type F8","No",{"v":18,"d":"18.00"}]
["Light fitting Type S7","No",{"v":12,"d":"12.00"}]
["Light fitting Type S6","No",{"v":19,"d":"19.00"}]
["LED driver 200w","No",{"v":4,"d":"4.00"}]
["LED driver 150w","No",{"v":6,"d":"6.00"}]
["White metal powerskirt for LHWS","m",{"v":2,"d":"2.00"}]
["Galv Cable tray (Museum)","m",{"v":6,"d":"6.00"}]
["300 x 1200 Surface metal box white","No",{"v":8,"d":"8.00"}]
["Light fitting Type F1 600 x 1200","No",{"v":9,"d":"9.00"}]
["Light fitting Type A1 300 x 1200","No",{"v":5,"d":"5.00"}]
["Light fitting Type F1 300 x 1200","No",{"v":3,"d":"3.00"}]
["Light fitting Type D3","No",{"v":39,"d":"39.00"}]
["Light fitting Type D1","No",{"v":18,"d":"18.00"}]
["Light fitting Type D2","No",{"v":7,"d":"7.00"}]
["Light fitting Type D7 Dimmable","No",{"v":14,"d":"14.00"}]
["Light fitting Type F6","No",{"v":3,"d":"3.00"}]
["Light fitting Type F3","No",{"v":2,"d":"2.00"}]
["Light fitting Type F4","No",{"v":1,"d":"1.00"}]
["DB - Sump 1","No",{"v":1,"d":"1.00"}]
["DB - Sump 2","No",{"v":1,"d":"1.00"}]
["LED driver box metal","No",{"v":1,"d":"1.00"}]
["LED driver box PVC","No",{"v":6,"d":"6.00"}]
["Floor box lids","No",{"v":22,"d":"22.00"}]
["Light fitting type A3 600x600","No",{"v":1,"d":"1.00"}]
["Light fitting type L1","No",{"v":24,"d":"24.00"}]
["Light fitting type J4","No",{"v":2,"d":"2.00"}]
["Light fitting type J3","N/A",{"v":11,"d":"11.00"}]
["Lesco Single Ded","No",{"v":4,"d":"4.00"}]
["Lesco Single + Euro","No",{"v":29,"d":"29.00"}]
["Lesco 1 Lever 2 Way","No",{"v":11,"d":"11.00"}]
["Lesco 1 Lever Bell Press","No",{"v":3,"d":"3.00"}]
["Lesco 2 Lever 2 Way","No",{"v":5,"d":"5.00"}]
["Lesco 4 Lever 1 Way","No",{"v":1,"d":"1.00"}]
["Lesco 4 Lever 2 Way","No",{"v":2,"d":"2.00"}]
["Lesco 3 Lever 1 Way x 2 Way x2 x1","No",{"v":1,"d":"1.00"}]
["Lesco 2 Lever 1 Way","No",{"v":2,"d":"2.00"}]
["Lesco 1 Lever 1 Way","No",{"v":2,"d":"2.00"}]
["LED Strip Museum drop off 21.8m","No",{"v":1,"d":"1.00"}]
["LED Strip driver box 6 (13.7m + 10m)","No",{"v":1,"d":"1.00"}]
["LED Strip driver box 5 (15m x 2)","No",{"v":1,"d":"1.00"}]
["LED Strip reading room (14.7m)","No",{"v":1,"d":"1.00"}]
["LED Strip driver box 7 (15m + 13.5m)","No",{"v":1,"d":"1.00"}]
["White 300mm wire mesh","No",{"v":31,"d":"31.00"}]
["White 300mm wire mesh 4 way","No",{"v":1,"d":"1.00"}]
["White 300mm wire mesh Tee","No",{"v":9,"d":"9.00"}]
["White PVC 4x2 Box (Wall)","No",{"v":119,"d":"119.00"}]
["White PVC 4x4 Box (Wall)","No",{"v":136,"d":"136.00"}]
["150mm Diameter PVC disc valves","No",{"v":8,"d":"8.00"}]
["MECHANICAL INSTALLATION MATERIALS",""]
["350mm Diameter Whirly Birds","No",{"v":3,"d":"3.00"}]
["975 x 1000mm over flange weather louvre","No",{"v":4,"d":"4.00"}]
["1000 x 1000mm over flange weather louvre","No",{"v":2,"d":"2.00"}]
["975 x 1000mm Square ducting piece","No",{"v":4,"d":"4.00"}]
["NOTE : THIS BILL SHOULD HAVE A NEGATIVE TOTAL, WHICH SHOULD BE CARRIED TO THE SECTION SUMMARY AS A NEGATIVE (MINUS) VALUE",""]

{"sheet":"Sect 7-12","index":6,"n_rows":3136,"n_cols":17,"rows_kept":3136}
[null,null,"1102C","03/10/2023","03:08:41",".","3.3.6.4"]
[null,null,"SARAH BARTMANN COMPLETION CONTRACT"]
["COUNTER","ISC","SECTION","BILL","PAGE NO","ITEM NO","DOC REF","PAY REF","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT","LABOUR INTENSIVE","WORDING","EDIT DATE"]
[1,9446,7,1,"7/1","","7/1","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:49:02",""]
[2,6085,7,1,"7/1","","7/1","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:52:40",""]
[3,9447,7,1,"7/1","","7/1","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 08:54:28",""]
[4,77,7,1,"7/1","","7/1","","SITE CLEARANCE AND BULK EARTHWORKS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:53:15",""]
[5,79,7,1,"7/1","","7/1","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","04/05/2012 03:55:13",""]
[6,80,7,1,"7/1","","7/1","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","29/06/2023 08:28:49",""]
[7,81,7,1,"7/1","","7/1","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","04/05/2012 03:55:13",""]
[8,5619,7,1,"7/1","","7/1","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 05:59:23",""]
[9,5620,7,1,"7/1","","7/1","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:03:43",""]
[10,4063,7,1,"7/1","","7/1","","Materials arising from the demolitions and alterations","H4",{"v":0,"d":"0.0"},"","","","","22/08/2012 05:43:50",""]
[11,4064,7,1,"7/1","","7/1","","Materials arising from the demolitions and alterations will become the property of the contractor. An item is provided in the Calculation of Tender / Bid Sum at the end of the bills of quantities for \" Credit for old materials arising from the demolitions and alterations which become the property of the contractor\".","",{"v":0,"d":"0.0"},"","","","","15/11/2021 01:35:32",""]
[12,82,7,1,"7/1","","7/1","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","01/10/2012 09:23:00",""]
[13,83,7,1,"7/2","","7/2","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","04/05/2012 03:55:13",""]
[14,84,7,1,"7/2","","7/2","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","17/11/2012 05:30:34",""]
[15,3868,7,1,"7/2","","7/2","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","19/08/2012 05:55:09",""]
[16,3869,7,1,"7/2","","7/2","","Demolishing and removing","H4",{"v":0,"d":"0.0"},"","","","","15/11/2021 01:33:15",""]
[17,9256,7,1,"7/2"," A","7/2. A","","Single storey covered parking building with ASBESTOS roof sheeting on timber support structure approximately 75m2 on plan and approximately 3 500mm high at eaves, comprising concrete surface bed, corrugated fibre cement side cladding on timber rails and timber pole supports, concrete apron, etc. complete","No",1,"","","","","06/12/2021 10:08:16",""]
[18,9423,7,1,"7/2"," B","7/2. B","","Single storey store-room building with ASBESTOS roof to low pitch approximately 36m2 on plan and approximately 2 500mm high overall comprising concrete surface bed, apron, and precast concrete panel walls, etc. complete","No",1,"","","","","06/12/2021 10:08:46",""]
[19,11203,7,1,"7/2"," C","7/2. C","","Single storey rectangular shaped temporary ablution building with double pitched timber roof structure and fibre cement covering approximately 30m2 and approximately 3 000mm high overall comprising concrete surface bed, plastered brick walls, etc. complete","No",1,"","","","","08/12/2021 08:27:40",""]
[21,9448,7,2,"7/4","","7/4","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:18:08",""]
[22,6086,7,2,"7/4","","7/4","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:53:35",""]
[23,9449,7,2,"7/4","","7/4","","BILL NO. 2","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 08:55:28",""]
[24,172,7,2,"7/4","","7/4","","EXTERNAL WATER SUPPLIES","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:53:42",""]
[25,173,7,2,"7/4","","7/4","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:56:22",""]
[26,174,7,2,"7/4","","7/4","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:07",""]
[27,175,7,2,"7/4","","7/4","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:56:22",""]
[28,5621,7,2,"7/4","","7/4","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 05:59:33",""]
[29,5622,7,2,"7/4","","7/4","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:03:52",""]
[30,185,7,2,"7/4","","7/4","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:58:20",""]
[31,176,7,2,"7/4","","7/4","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:56:22",""]
[32,177,7,2,"7/4","","7/4","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:56:22",""]
[33,180,7,2,"7/4","","7/4","","Disinfection of water pipework","H4",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:58:20",""]
[34,181,7,2,"7/4","","7/4","","Water pipework is to be disinfected at completion in accordance with SANS 1200L","",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:58:20",""]
[35,536,7,2,"7/5","","7/5","","WATER SUPPLIES","H2",{"v":0,"d":"0.0"},"","","","","15/05/2012 01:35:47",""]
[36,537,7,2,"7/5"," A","7/5. A","","Excavation in earth not exceeding 2m deep for pipe trenches (Labour Intensive)","m3",10,"","","","","26/06/2023 11:03:39",""]
[37,5792,7,2,"7/5"," B","7/5. B","","Excavation in earth exceeding 2m and not exceeding 4m deep for pipe trenches","m3",2,"","","","","26/06/2023 11:03:45",""]
[38,539,7,2,"7/5"," C","7/5. C","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 90% Mod AASHTO density","m3",7,"","","","","26/06/2023 11:04:28",""]
[39,540,7,2,"7/5"," D","7/5. D","","Imported backfilling to pipe trenches, compacted to 90% Mod AASHTO density","m3",2,"","","","","26/06/2023 11:04:13",""]
[40,690,7,2,"7/5"," E","7/5. E","","Imported G5 backfilling to pipe trenches, compacted to 95% Mod AASHTO density","m3",2,"","","","","26/06/2023 11:04:01",""]
[41,7754,7,2,"7/5"," F","7/5. F","","Bedding material supplied by the contractor, compacted to 93% Mod AASHTO density","m3",3,"","","","","06/12/2021 10:11:22",""]
[42,576,7,2,"7/5"," G","7/5. G","","Extra over trench excavations in earth for excavation in soft rock","m3",1,"","","","","24/01/2014 03:15:39",""]
[43,577,7,2,"7/5"," H","7/5. H","","Extra over trench excavations in earth for excavation in hard rock","m3",1,"","","","","24/01/2014 03:15:42",""]
[44,1186,7,2,"7/5"," I","7/5. I","","Extra over all excavations for carting away surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",3,"","","","","27/01/2014 02:44:46",""]
[45,556,7,2,"7/5","","7/5","","Class 9 PVC pressure pipes with solvent welded joints","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 11:06:05",""]
[46,603,7,2,"7/5"," J","7/5. J","","110mm Pipes laid in trenches (Trenches elsewhere)","m",9,"","","","","21/05/2012 12:37:51",""]
[47,558,7,2,"7/5","","7/5","","Extra over Class 9 PVC pressure pipes for fittings with solvent welded joints","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 11:06:11",""]
[48,1284,7,2,"7/5"," K","7/5. K","","110mm Bend","No",1,"","","","","06/12/2021 10:11:42",""]
[49,564,7,2,"7/5","","7/5","","Class 10 HDPe type PE100 pipes","H4",{"v":0,"d":"0.0"},"","","","","06/10/2012 09:47:57",""]
[50,565,7,2,"7/5"," L","7/5. L","","75mm Pipes laid in trenches (Trenches elsewhere)","m",5,"","","","","07/12/2021 03:48:21",""]
[51,566,7,2,"7/5","","7/5","","Extra over Class 10 HDPe type PE100 pipes for screw-type compression fittings","H4",{"v":0,"d":"0.0"},"","","","","06/10/2012 09:48:12",""]
[52,1097,7,2,"7/5"," M","7/5. M","","50mm Saddle with female threaded connection","No",4,"","","","","05/06/2012 11:26:34",""]
[53,747,7,2,"7/6"," A","7/6. A","","75mm Tee","No",1,"","","","","06/12/2021 10:12:42",""]
[54,7611,7,2,"7/6","","7/6","","Grade 316 stainless steel pipes","H4",{"v":0,"d":"0.0"},"","","","","17/11/2012 03:27:06",""]
[55,7613,7,2,"7/6"," B","7/6. B","","15mm Standpipe 1 300 mm long, and three times fixed to gumpole (elsewhere measured) with and including pipe clamps","No",2,"","","","","09/12/2021 04:51:40",""]
[56,7612,7,2,"7/6","","7/6","","Extra over stainless steel pipes for welded fittings","H4",{"v":0,"d":"0.0"},"","","","","17/11/2012 03:26:41",""]
[57,7614,7,2,"7/6"," C","7/6. C","","15mm Fittings","No",4,"","","","","06/12/2021 10:14:00",""]
[58,1076,7,2,"7/6","","7/6","","Galvanised steel pipes with screwed and socketed joints","H4",{"v":0,"d":"0.0"},"","","","","17/11/2012 03:28:06",""]
[59,1090,7,2,"7/6"," D","7/6. D","","15mm Standpipe 1 300 mm long threaded both ends, and three times fixed to and including 2 000mm gumpole with 400 x 400 x 250mm unreinforced concrete base with and including pipe clamps","No",3,"","","","","06/12/2021 10:14:14",""]
[60,1079,7,2,"7/6","","7/6","","Extra over galvanised steel pipes with screwed and socketed joints for steel fittings","H4",{"v":0,"d":"0.0"},"","","","","17/11/2012 03:28:14",""]
[61,1080,7,2,"7/6"," E","7/6. E","","15mm Fittings","No",4,"","","","","14/11/2013 01:15:26",""]
[62,13691,7,2,"7/6","","7/6","","Sundries","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:26:42",""]
[63,1094,7,2,"7/6"," F","7/6. F","","75mm Nominal diameter x 1 525mm long creosote treated gumpole for water standpipe, with the bottom 700mm embedded in the ground","No",4,"","","","","30/08/2013 04:10:51",""]
[64,594,7,2,"7/6","","7/6","","Valves, etc","H3",{"v":0,"d":"0.0"},"","","","","01/10/2012 09:50:57",""]
[65,758,7,2,"7/6","","7/6","","Note : references in brackets after descriptions refer to notes on drawings C5593-SITE-WAT-34, 35 and 43","",{"v":0,"d":"0.0"},"","","","","29/08/2013 09:43:39",""]
[66,1088,7,2,"7/6"," G","7/6. G","","15mm Brass bibcock with threaded hose union","No",4,"","","","","05/06/2012 11:27:11",""]
[67,1089,7,2,"7/6"," H","7/6. H","","15mm Brass wallplate elbow, and fixing to gumpole with and including brass bolts","No",4,"","","","","05/06/2012 11:27:17",""]
[68,683,7,2,"7/6"," I","7/6. I","","Epoxy resin-coated ductile iron non-return/check valve in accordance with SANS1551/DN80/PN16, flanged and drilled to ISO7005-2, and connecting to 50mm diameter HDPe pipe","No",1,"","","","","06/06/2012 09:58:53",""]
[69,681,7,2,"7/6"," J","7/6. J","","Epoxy resin-coated ductile iron non-return/check valve in accordance with SANS1551/DN80/PN16, flanged and drilled to ISO7005-2, and connecting to 75mm diameter HDPe pipe","No",7,"","","","","06/06/2012 09:58:49",""]
[70,685,7,2,"7/6"," K","7/6. K","","20mm Volumetric water meter connected to HDPe pipe","No",2,"","","","","23/10/2012 04:20:52",""]
[71,1209,7,2,"7/7"," A","7/7. A","","40mm Electromagnetic flowmeter connected to CI pipe (reservoir control valve chamber fitting list item E)","No",1,"","","","","06/06/2012 12:00:37",""]
[72,1069,7,2,"7/7"," B","7/7. B","","40mm Volumetric water meter connected to HDPe or steel pipe","No",2,"","","","","06/08/2012 02:32:58",""]
[73,542,7,2,"7/7","","7/7","","VALVE BOX CHAMBERS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:13:48",""]
[74,545,7,2,"7/7"," C","7/7. C","","Type 3A Thermoplastic valve and hydrant box, including 330mm diameter x 500mm long fibre cement extension sleeve and 480 x 480mm concrete collar finish","No",4,"","","","","30/10/2021 07:48:13",""]
[75,1086,7,2,"7/7"," D","7/7. D","","900 x 900mm Isolating valve chamber not exceeding 1 000mm deep internally, as per detail on drawing C5593-SITE-WAT-34 & 43 (Cover and frame elsewhere)","No",2,"","","","","10/04/2013 09:32:25",""]
[76,9651,7,2,"7/7","","7/7","","Completion of brick chamber concrete cover slabs (covers and frames elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 03:38:08",""]
[77,9653,7,2,"7/7"," E","7/7. E","","900 x 900mm Isolating valve chamber as per detail on drawing C5593-SITE-WAT-34 & 43","No",8,"","","","","10/12/2021 03:25:13",""]
[78,13721,7,2,"7/7","","7/7","","Completion of brick inspection chambers by raising or breaking down of brickwork to final levels","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:25:54",""]
[79,13722,7,2,"7/7"," F","7/7. F","","Breaking down and removing one brick walls in inspection chambers to final levels","m2",10,"","","","","26/06/2023 10:58:15",""]
[80,13723,7,2,"7/7"," G","7/7. G","","One brick walls of NFPE bricks (14 MPa nominal compressive strength) in class II (1:3) cement mortar in draw chambers, catchpits, manholes, etc.","m2",10,"","","","","19/05/2022 12:34:44",""]
[81,13724,7,2,"7/7"," H","7/7. H","","150mm Wide brick reinforcement built in horizontally","m",58,"","","","","19/05/2022 12:35:43",""]
[82,13725,7,2,"7/7"," I","7/7. I","","One coat 1:5 cement plaster, on brickwork in draw chambers, catchpits, manholes, etc.","m2",10,"","","","","19/05/2022 12:36:33",""]
[83,11179,7,2,"7/7","","7/7","","COVERS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:13:44",""]
[84,1075,7,2,"7/7"," J","7/7. J","","600 x 600mm x 38kg Type 9B Polymer lockable manhole cover and frame","No",10,"","","","","02/10/2012 04:26:33",""]
[85,514,7,2,"7/7","","7/7","","FIRE APPLIANCES, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:13:41",""]
[86,518,7,2,"7/7"," K","7/7. K","","80 x 65mm Brass right-angle shielded spindle hydrant valve with cap and chain, in accordance with SANS 1128-2","No",1,"","","","","15/05/2012 01:33:04",""]
[87,517,7,2,"7/7"," L","7/7. L","","80 x 65mm Brass straight-through shielded spindle hydrant valve with cap and chain, in accordance with SANS 1128-2","No",1,"","","","","15/05/2012 01:33:07",""]
[88,515,7,2,"7/8","","7/8","","Fire hydrant pedestals","H4",{"v":0,"d":"0.0"},"","","","","15/05/2012 01:16:39",""]
[89,516,7,2,"7/8"," A","7/8. A","","Unreinforced concrete hydrant pedestal 900mm high, cast around vertical pipe with bottom 300mm below ground, 305 x 305mm square at base and tapering to 200 x 200mm overall octagonal shaped top, including excavation, formwork and two coats of paint to exposed surfaces","No",1,"","","","","15/05/2012 01:32:36",""]
[90,519,7,2,"7/8","","7/8","","WATER SUPPLIES TO FIRE APPLIANCES","H2",{"v":0,"d":"0.0"},"","","","","15/05/2012 01:23:02",""]
[91,520,7,2,"7/8","","7/8","","Grade 316 stainless steel pipes","H4",{"v":0,"d":"0.0"},"","","","","17/11/2012 03:28:42",""]
[92,521,7,2,"7/8"," B","7/8. B","","80mm Pipes","m",1,"","","","","06/12/2021 10:32:28",""]
[93,12956,7,2,"7/8"," C","7/8. C","","100mm Pipes","m",1,"","","","","06/12/2021 10:32:43",""]
[94,523,7,2,"7/8","","7/8","","Extra over stainless steel pipes for welded fittings","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 10:08:31",""]
[95,527,7,2,"7/8"," D","7/8. D","","80mm Bend","No",1,"","","","","06/12/2021 10:32:54",""]
[96,528,7,2,"7/8"," E","7/8. E","","80mm Tee","No",1,"","","","","06/12/2021 10:33:05",""]
[97,674,7,2,"7/8"," F","7/8. F","","100mm Diameter long radius bend","No",1,"","","","","06/12/2021 10:33:13",""]
[98,534,7,2,"7/8","","7/8","","Sundries","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 10:09:20",""]
[99,12970,7,2,"7/8"," G","7/8. G","","Prepare surface and apply two coats enamel paint to concrete pedestal","m2",2,"","","","","08/12/2021 05:11:12",""]
[100,607,7,2,"7/8"," H","7/8. H","","285 x 140mm Triangular-shaped x 1 000mm long precast concrete valve and hydrant marker, with either \"V\" or \"FH\" inscribed on the side, the whole painted with two coats road paint.","No",1,"","","","","17/05/2012 07:50:51",""]
[101,547,7,2,"7/8"," I","7/8. I","","Hot-dip galvanised fire hydrant key formed of 300 x 16mm diameter handle with attached key, as per detail on drawing C5593-SITE-WAT-34","No",3,"","","","","10/12/2021 08:33:48",""]
[102,6991,7,2,"7/8","","7/8","","Disinfecting","H4",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:11:18",""]
[103,6992,7,2,"7/8"," J","7/8. J","","Disinfecting water pipe and tank system","Item",{"v":1,"d":"1.00"},"","","","","06/10/2012 10:11:32",""]
[104,764,7,2,"7/8","","7/8","","Municipal connection","H4",{"v":0,"d":"0.0"},"","","","","23/05/2012 08:29:57",""]
[105,765,7,2,"7/8"," K","7/8. K","","Provide the sum of R50 000.00 (Fifty Thousand) Rand for municipal water connection","Item",{"v":1,"d":"1.00"},{"v":50000,"d":"50000.00"},{"v":50000,"d":"50000.00"},"","","09/12/2021 04:54:29",""]
[106,766,7,2,"7/8"," L","7/8. L","","Allow for profit on the above","Item",{"v":1,"d":"1.00"},"","","","","06/12/2021 10:35:50",""]
[107,2790,7,2,"7/9","","7/9","","GABIONS AND INTERLOCKING BLOCK RETAINING STRUCTURES","H2",{"v":0,"d":"0.0"},"","","","","06/08/2012 12:07:59",""]
[108,2791,7,2,"7/9","","7/9","","Gabions","H4",{"v":0,"d":"0.0"},"","","","","06/08/2012 12:07:59",""]
[109,2792,7,2,"7/9","","7/9","","Gabions are to be of double twisted hexagonal wire mesh (nominal 80 x 100mm mesh of 2,7mm galvanised wire, with 3,5mm galvanised wire framing and with partitions at 1m centres).  All wire to be hot-dip galvanised to SANS 675","",{"v":0,"d":"0.0"},"","","","","06/08/2012 12:07:59",""]
[110,2793,7,2,"7/9","","7/9","","Gabions of galvanised wire boxes laced together and filled with broken stone","H4",{"v":0,"d":"0.0"},"","","","","06/08/2012 12:07:59",""]
[111,2794,7,2,"7/9"," A","7/9. A","","300mm Thick embankment protection of 2 x 1 x 0,3m mattress with diaphragm divisions at 1m centres, butt jointed","No",1,"","","","","09/08/2012 03:37:34",""]
[112,6993,7,2,"7/9","","7/9","","AS-BUILT DRAWINGS","H2",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:11:54",""]
[113,6994,7,2,"7/9"," B","7/9. B","","Provision of as-built drawings of the complete water reticulation installation","Item",{"v":1,"d":"1.00"},"","","","","10/12/2021 08:27:08",""]
[115,9450,7,3,"7/11","","7/11","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:18:12",""]
[116,6087,7,3,"7/11","","7/11","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:17:36",""]
[117,9451,7,3,"7/11","","7/11","","BILL NO. 3","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 08:58:04",""]
[118,1125,7,3,"7/11","","7/11","","RESERVOIRS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:17:41",""]
[119,1126,7,3,"7/11","","7/11","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","05/06/2012 12:44:49",""]
[120,1127,7,3,"7/11","","7/11","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:17",""]
[121,1128,7,3,"7/11","","7/11","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","05/06/2012 12:44:49",""]
[122,5623,7,3,"7/11","","7/11","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 05:59:41",""]
[123,5624,7,3,"7/11","","7/11","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:01",""]
[124,1129,7,3,"7/11","","7/11","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","05/06/2012 12:44:49",""]
[125,1130,7,3,"7/11","","7/11","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","05/06/2012 12:44:50",""]
[126,775,7,3,"7/11","","7/11","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","28/05/2012 09:37:14",""]
[127,791,7,3,"7/11","","7/11","","FILLING, ETC","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 02:09:03",""]
[128,9528,7,3,"7/11","","7/11","","Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 90% Mod AASHTO density in maximum 300mm layers","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:40:28",""]
[129,9527,7,3,"7/11"," A","7/11. A","","Backfilling to hole excavations (Labour Intensive)","m3",300,"","","","","26/06/2023 10:06:51",""]
[130,9526,7,3,"7/12","","7/12","","G5 Earth filling supplied by the contractor deposited in layers not exceeding 150mm thick and compacted to 95% modified AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","09/09/2021 12:55:57",""]
[131,9525,7,3,"7/12"," A","7/12. A","","Forming storm water berm 600mm wide at top and 1 800mm at base x average 300mm high above adjacent surfaces, including finishing to slopes, etc.","m",90,"","","","","09/09/2021 12:56:14",""]
[132,812,7,3,"7/12","","7/12","","PROTECTIVE STONE DRESSING","H2",{"v":0,"d":"0.0"},"","","","","28/05/2012 09:37:21",""]
[133,813,7,3,"7/12","","7/12","","Clean 19mm crushed stone evenly spread with larger stones around outlets","H4",{"v":0,"d":"0.0"},"","","","","28/05/2012 09:37:22",""]
[134,6155,7,3,"7/12"," B","7/12. B","","On flat roofs","m3",13,"","","","","01/10/2012 12:41:39",""]
[135,1159,7,3,"7/12","","7/12","","METALWORK","H2",{"v":0,"d":"0.0"},"","","","","05/06/2012 04:17:12",""]
[136,1160,7,3,"7/12","","7/12","","Double hot-dip galvanised after manufacture ladders formed of 40mm ID heavy black steel tubing (refer to detail on drawing C5593-SITE-WAT-43)","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:00:53",""]
[137,1161,7,3,"7/12"," C","7/12. C","","Ladder 4 586mm overall girth with 9 rungs, bending, flanges, and fixing to concrete structure","No",1,"","","","","06/12/2021 03:01:17",""]
[138,1162,7,3,"7/12"," D","7/12. D","","Ladder 6 086mm overall girth with 14 rungs, bending, flanges, and fixing to concrete structure","No",1,"","","","","06/12/2021 03:01:24",""]
[139,853,7,3,"7/12","","7/12","","Covers, etc.","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:07:48",""]
[140,854,7,3,"7/12"," E","7/12. E","","600mm Diameter x 63kg type 2A concrete-filled light-duty polymer lockable cover and frame","No",2,"","","","","07/12/2021 12:09:16",""]
[141,1143,7,3,"7/12","","7/12","","Valves, etc.","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:07:45",""]
[142,1144,7,3,"7/12"," F","7/12. F","","250mm Diameter x 410mm long purpose-made hot-dip galvanised mild steel air vent, including painting and caulking into and forming opening through 200mm chamber cover slab; all as per detail on drawing C5593-SITE-WAT-43","No",1,"","","","","09/12/2021 04:57:43",""]
[143,2818,7,3,"7/12","","7/12","","PAINTING","H2",{"v":0,"d":"0.0"},"","","","","06/08/2012 04:27:40",""]
[144,2819,7,3,"7/12","","7/12","","Prepare, prime and apply two coats enamel paint on:","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:07:38",""]
[145,2820,7,3,"7/12"," G","7/12. G","","Galvanised steel pipes","m2",5,"","","","","30/08/2013 04:12:52",""]
[146,7001,7,3,"7/12","","7/12","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:16:30",""]
[147,7000,7,3,"7/12"," H","7/12. H","","Disinfecting water pipe and tank system","Item",{"v":1,"d":"1.00"},"","","","","06/10/2012 10:16:43",""]
[149,9452,7,4,"7/14","","7/14","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:18:16",""]
[150,6088,7,4,"7/14","","7/14","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:17:53",""]
[151,9453,7,4,"7/14","","7/14","","BILL NO. 4","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 08:58:27",""]
[152,3247,7,4,"7/14","","7/14","","PUMP STATION AND SUMP","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:17:49",""]
[153,3248,7,4,"7/14","","7/14","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","08/08/2012 02:53:29",""]
[154,3249,7,4,"7/14","","7/14","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:22",""]
[155,3250,7,4,"7/14","","7/14","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","08/08/2012 02:53:29",""]
[156,5625,7,4,"7/14","","7/14","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 05:59:49",""]
[157,5626,7,4,"7/14","","7/14","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:11",""]
[158,3251,7,4,"7/14","","7/14","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","08/08/2012 02:53:29",""]
[159,3252,7,4,"7/14","","7/14","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","08/08/2012 02:53:29",""]
[160,3288,7,4,"7/14","","7/14","","PLUMBING AND DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","08/08/2012 03:35:13",""]
[161,3304,7,4,"7/14","","7/14","","RAINWATER DISPOSAL","H3",{"v":0,"d":"0.0"},"","","","","08/08/2012 04:11:24",""]
[162,3305,7,4,"7/14","","7/14","","0,8mm Thick aluminium gutters and rainwater downpipes","H4",{"v":0,"d":"0.0"},"","","","","02/10/2012 03:31:16",""]
[163,3306,7,4,"7/14"," A","7/14. A","","110mm Diameter rainwater pipes with factory applied epoxy powder-coated finish fixed to brick walls with and including pre-painted downpipe cleats","m",2,"","","","","06/12/2021 10:44:27",""]
[164,3309,7,4,"7/15"," A","7/15. A","","Extra over rainwater pipe for bend","No",1,"","","","","06/12/2021 10:44:36",""]
[165,1862,7,4,"7/15","","7/15","","Galvanised steel pipes with screwed and socketed joints","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 10:50:13",""]
[166,1863,7,4,"7/15"," B","7/15. B","","50mm Pipes","m",1,"","","","","09/08/2012 02:32:43",""]
[167,1867,7,4,"7/15"," C","7/15. C","","80mm Pipes","m",4,"","","","","09/08/2012 02:32:47",""]
[168,1864,7,4,"7/15","","7/15","","Extra over galvanised steel pipes with screwed and socketed joints for steel fittings","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 10:50:36",""]
[169,1865,7,4,"7/15"," D","7/15. D","","50mm Bend","No",2,"","","","","09/08/2012 02:32:51",""]
[170,1868,7,4,"7/15"," E","7/15. E","","80mm Bend","No",1,"","","","","09/08/2012 02:32:56",""]
[171,3289,7,4,"7/15","","7/15","","SUMP","H2",{"v":0,"d":"0.0"},"","","","","08/08/2012 03:35:49",""]
[172,1843,7,4,"7/15"," F","7/15. F","","Hot-dip galvanised waterpipe bracket suitable for 50mm diameter pipe, including neoprene gasket, bolts, fixing to brick or concrete walls, complete as per detail on drawing C5593-SITE-WAT-35","No",1,"","","","","27/02/2014 08:00:52",""]
[173,1841,7,4,"7/15"," G","7/15. G","","Hot-dip galvanised waterpipe bracket suitable for 80mm diameter pipe, including neoprene gasket, bolts, fixing to brick or concrete walls, complete as per detail on drawing C5593-SITE-WAT-35","No",1,"","","","","27/02/2014 08:01:01",""]
[175,9454,7,5,"7/17","","7/17","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:18",""]
[176,6089,7,5,"7/17","","7/17","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:17:57",""]
[177,9455,7,5,"7/17","","7/17","","BILL NO. 5","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 08:59:01",""]
[178,151,7,5,"7/17","","7/17","","EXTERNAL SEWER DRAINAGE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:22",""]
[179,152,7,5,"7/17","","7/17","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:52:06",""]
[180,153,7,5,"7/17","","7/17","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:27",""]
[181,154,7,5,"7/17","","7/17","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:52:07",""]
[182,5627,7,5,"7/17","","7/17","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 05:59:56",""]
[183,5628,7,5,"7/17","","7/17","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:18",""]
[184,155,7,5,"7/17","","7/17","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:52:07",""]
[185,156,7,5,"7/17","","7/17","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:52:07",""]
[186,159,7,5,"7/17","","7/17","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:53:35",""]
[187,130,7,5,"7/17","","7/17","","SOIL DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:46:07",""]
[188,1272,7,5,"7/17"," A","7/17. A","","Excavation in earth not exceeding 2m deep for pipe trenches (Labour Intensive)","m3",285,"","","","","26/06/2023 01:29:33",""]
[189,5213,7,5,"7/18"," A","7/18. A","","Excavation in earth not exceeding 2m deep for holes (Labour Intensive)","m3",2,"","","","","26/06/2023 10:15:00",""]
[190,1290,7,5,"7/18"," B","7/18. B","","Excavation in earth exceeding 2m deep and not exceeding 4m deep for pipe trenches","m3",5,"","","","","26/06/2023 10:48:27",""]
[191,1611,7,5,"7/18"," C","7/18. C","","Excavation in earth exceeding 4m deep and not exceeding 6m deep for pipe trenches","m3",5,"","","","","28/10/2021 10:27:31",""]
[192,1273,7,5,"7/18"," D","7/18. D","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",228,"","","","","26/06/2023 10:15:12",""]
[193,1274,7,5,"7/18"," E","7/18. E","","Imported G7 backfilling to pipe trenches, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 10:15:16",""]
[194,1275,7,5,"7/18"," F","7/18. F","","Imported G5 backfilling to pipe trenches, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 10:15:21",""]
[195,1276,7,5,"7/18"," G","7/18. G","","Selected granular filling from stock piles on site in bedding under and filling around pipes compacted to 95% Modified AASHTO density (Labour Intensive)","m3",58,"","","","","26/06/2023 10:15:27",""]
[196,1277,7,5,"7/18"," H","7/18. H","","Extra over trench and hole excavations in earth for excavation in soft rock","m3",51,"","","","","10/04/2013 09:42:40",""]
[197,1278,7,5,"7/18"," I","7/18. I","","Extra over trench and hole excavations in earth for excavation in hard rock","m3",35,"","","","","01/10/2012 11:03:25",""]
[198,1279,7,5,"7/18"," J","7/18. J","","Extra over all excavations for carting away surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",60,"","","","","08/06/2012 09:34:17",""]
[199,131,7,5,"7/18","","7/18","","Heavy duty (Class 34) uPVC sewer and drain pipes","H4",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:46:08",""]
[200,132,7,5,"7/18"," K","7/18. K","","110mm Pipes vertically or ramped to cleaning eyes, etc. (no excavation)","m",2,"","","","","26/06/2023 10:15:38",""]
[201,146,7,5,"7/18"," L","7/18. L","","160mm Pipes vertically or ramped to cleaning eyes, etc. (no excavation)","m",14,"","","","","26/06/2023 10:15:42",""]
[202,134,7,5,"7/18"," M","7/18. M","","110mm Pipes laid in trenches (Trenches elsewhere)","m",85,"","","","","24/04/2023 09:40:54",""]
[203,13750,7,5,"7/18"," N","7/18. N","","160mm Pipes laid in trenches (Trenches elsewhere)","m",140,"","","","","24/04/2023 09:40:42",""]
[204,1287,7,5,"7/18","","7/18","","Extra over heavy duty (Class 34) uPVC sewer and drain pipes for uPVC fittings","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 02:43:31",""]
[205,13806,7,5,"7/18"," O","7/18. O","","110mm Bend","No",8,"","","","","26/06/2023 08:13:25",""]
[206,6638,7,5,"7/19"," A","7/19. A","","160mm Bend","No",11,"","","","","06/12/2021 10:47:31",""]
[207,9720,7,5,"7/19"," B","7/19. B","","ABC cast iron straight or bent rodding/cleaning eye with removable cover jointed to 160mm uPVC pipe and set in and including mass concrete class C surround size 500 x 500 x 150mm thick, including necessary shallow excavations, form work, backfilling, etc.","No",2,"","","","","06/12/2021 10:47:50",""]
[208,8810,7,5,"7/19","","7/19","","Galvanised mild steel pipes","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:50:08",""]
[209,8811,7,5,"7/19"," C","7/19. C","","100mm Pipes","m",2,"","","","","28/10/2021 10:24:55",""]
[210,9765,7,5,"7/19"," D","7/19. D","","100mm Pipes laid in trenches (Trenches elsewhere)","m",12,"","","","","28/10/2021 10:25:00",""]
[211,8806,7,5,"7/19","","7/19","","Extra over galvanised mild steel pipes for galvanised steel fittings","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:50:19",""]
[212,8818,7,5,"7/19"," E","7/19. E","","100mm 90 Degree double flanged bend","No",3,"","","","","06/12/2021 10:49:43",""]
[213,9768,7,5,"7/19"," F","7/19. F","","100mm 22,5 Degree double flanged bend","No",2,"","","","","06/12/2021 10:49:56",""]
[214,9764,7,5,"7/19"," G","7/19. G","","100mm Puddle flange","No",1,"","","","","30/10/2021 07:51:55",""]
[215,8808,7,5,"7/19"," H","7/19. H","","100mm Perrot coupling","No",2,"","","","","30/10/2021 07:51:58",""]
[216,9769,7,5,"7/19"," I","7/19. I","","Bracket suitable for 100mm diameter pipe, including neoprene gasket, bolts, fixing to brick or concrete walls, complete as per detail on drawing C5593-SITE-SEW-13","No",1,"","","","","15/11/2021 03:24:06",""]
[217,144,7,5,"7/19","","7/19","","uPVC gulleys","H4",{"v":0,"d":"0.0"},"","","","","10/05/2012 12:46:27",""]
[218,160,7,5,"7/19"," J","7/19. J","","PVC gulley comprising 110mm diameter S-trap with 140mm x 1,8kg cast iron grating set into screed in precast concrete surround, finished smooth on exposed surfaces in cement mortar with rounded angles including excavation, formwork, etc","No",1,"","","","","10/05/2012 12:54:11",""]
[219,1265,7,5,"7/19","","7/19","","Precast concrete circular inspection chambers including precast concrete cover slabs (cast iron covers elsewhere) and channels in benching, in accordance with SANS 1200LD","H4",{"v":0,"d":"0.0"},"","","","","08/06/2012 08:06:48",""]
[220,13752,7,5,"7/19"," K","7/19. K","","1 200mm Diameter inspection chamber not exceeding 1 000mm deep internally, including all excavations, backfilling, etc.","No",1,"","","","","24/04/2023 09:28:36",""]
[221,932,7,5,"7/19"," L","7/19. L","","1 200mm Diameter inspection chamber exceeding 1 000mm and not exceeding 1 500mm deep internally, including all excavations, backfilling, etc.","No",4,"","","","","10/02/2022 12:41:32",""]
[222,13751,7,5,"7/20"," A","7/20. A","","1 200mm Diameter inspection chamber exceeding 1 500mm and not exceeding 2 000mm deep internally, including all excavations, backfilling, etc.","No",2,"","","","","24/04/2023 09:28:24",""]
[223,9544,7,5,"7/20","","7/20","","Completion of partially built precast concrete manholes, inspection chambers, etc. including concrete kerbs or precast concrete cover slabs (covers and frames elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 03:02:18",""]
[224,13689,7,5,"7/20"," B","7/20. B","","Precast or in-situ reinforced concrete cover slab to 1 010mm internal diameter manhole (cover and frame elsewhere)","No",1,"","","","","09/12/2021 03:59:22",""]
[225,10009,7,5,"7/20"," C","7/20. C","","Break out and remove full single manhole ring","No",2,"","","","","10/12/2021 03:39:18",""]
[226,10010,7,5,"7/20"," D","7/20. D","","Supply and build in new 1 080mm diameter manhole ring","No",2,"","","","","10/12/2021 03:39:11",""]
[227,10011,7,5,"7/20"," E","7/20. E","","Trim manhole ring to final levels","No",2,"","","","","10/12/2021 03:39:07",""]
[228,8820,7,5,"7/20","","7/20","","Suction head chamber","H4",{"v":0,"d":"0.0"},"","","","","06/10/2021 09:07:24",""]
[229,8819,7,5,"7/20"," F","7/20. F","","660 x 660mm Brick chamber not exceeding 1 000mm deep internally complete, including all excavations, backfilling, etc., as per detail on drawing C5593-SITE-SEW-14 (cover and pipe installations measured elsewhere)","No",2,"","","","","06/12/2021 10:52:19",""]
[230,936,7,5,"7/20","","7/20","","Gratings, covers, etc.","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:16:03",""]
[231,5210,7,5,"7/20"," G","7/20. G","","600 x 600mm x 82kg Type 9B medium duty cast iron manhole cover and frame","No",2,"","","","","27/02/2014 08:02:23",""]
[232,12495,7,5,"7/20"," H","7/20. H","","650mm Diameter x 89,6kg type 1A concrete-filled polymer heavy duty lockable manhole cover","No",1,"","","","","07/12/2021 12:07:48",""]
[233,937,7,5,"7/20"," I","7/20. I","","650mm Diameter x 151kg type 1A concrete-filled polymer heavy duty lockable manhole cover and frame (2230)","No",7,"","","","","07/12/2021 12:07:41",""]
[234,938,7,5,"7/20","","7/20","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","28/05/2012 09:42:59",""]
[235,164,7,5,"7/20"," J","7/20. J","","Coarse river sand with particles larger than 2mm supplied by contractor compacted to 90% Modified AASHTO Density","m3",0.3,"","","","","06/12/2021 10:53:12",""]
[236,165,7,5,"7/20"," K","7/20. K","","19mm Crushed stone filling in holes","m3",2,"","","","","06/12/2021 10:53:24",""]
[237,5218,7,5,"7/20"," L","7/20. L","","U24 Geotextile fabric with 150mm laps","m2",9,"","","","","27/02/2014 08:02:38",""]
[238,5219,7,5,"7/20"," M","7/20. M","","110mm Diameter slotted drain pipe","m",3,"","","","","28/10/2021 10:24:40",""]
[239,167,7,5,"7/21"," A","7/21. A","","Cutting into side of existing manhole approximately 1 500mm deep for and connecting 160mm pipe including inserting 160mm channel bend and making good concrete benching and screed (160mm pipe elsewhere) (Labour Intensive)","No",1,"","","","","09/12/2021 05:02:22",""]
[240,929,7,5,"7/21"," B","7/21. B","","150 x 150 x 200mm High precast concrete inspection/rodding eye marker slab set in ground","No",32,"","","","","02/10/2012 03:24:27",""]
[241,169,7,5,"7/21"," C","7/21. C","","Testing soil drainage pipe system","Item",{"v":1,"d":"1.00"},"","","","","14/05/2013 11:00:01",""]
[242,13754,7,5,"7/21"," D","7/21. D","","Provisional Sum of R100 000.00 (One Hundred Thousand) nett for alterations to the existing sewer manhole and conservancy tank to disconnect the two from each other, to be measured and valued in terms of these bills of quantities.","Item",{"v":1,"d":"1.00"},"","","","","20/06/2023 09:26:17",""]
[243,13803,7,5,"7/21","","7/21","","Municipal sewer connection","H4",{"v":0,"d":"0.0"},"","","","","20/06/2023 09:19:24",""]
[244,13804,7,5,"7/21"," E","7/21. E","","Provide the sum of R60 000.00 (Sixty Thousand) for municipal sewer connection","Item",{"v":1,"d":"1.00"},{"v":60000,"d":"60000.00"},{"v":60000,"d":"60000.00"},"","","20/06/2023 09:19:35",""]
[245,13805,7,5,"7/21"," F","7/21. F","","Allow for profit on the above","Item",{"v":1,"d":"1.00"},"","","","","31/05/2023 08:53:27",""]
[246,2807,7,5,"7/21","","7/21","","PAINTING","H2",{"v":0,"d":"0.0"},"","","","","06/08/2012 03:08:51",""]
[247,2809,7,5,"7/21","","7/21","","Prepare, prime and two coats enamel paint on:","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:16:13",""]
[248,2810,7,5,"7/21"," G","7/21. G","","Galvanised steel pipes","m2",10,"","","","","11/08/2012 04:35:01",""]
[249,6995,7,5,"7/21","","7/21","","AS-BUILT DRAWINGS","H2",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:12:10",""]
[250,6996,7,5,"7/21"," H","7/21. H","","Provision of as-built drawings of the complete external sewer drainage installation","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 10:57:19",""]
[251,1165,7,5,"7/21","","7/21","","SEWER CONSERVANCY TANK","H2",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:34:47",""]
[252,925,7,5,"7/21","","7/21","","SOIL DRAINAGE","H3",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:34:53",""]
[253,1190,7,5,"7/21","","7/21","","Galvanised steel","H4",{"v":0,"d":"0.0"},"","","","","23/11/2012 10:07:18",""]
[254,1201,7,5,"7/21"," I","7/21. I","","160mm Pipes","m",1,"","","","","30/10/2021 07:53:44",""]
[255,1202,7,5,"7/21"," J","7/21. J","","200mm Pipes","m",2,"","","","","30/10/2021 07:53:48",""]
[256,1203,7,5,"7/21"," K","7/21. K","","Extra for welded intersection between 160 and 200mm pipe","No",1,"","","","","30/10/2021 07:53:55",""]
[257,1191,7,5,"7/21","","7/21","","Extra over galvanised steel pipes for steel fittings","H4",{"v":0,"d":"0.0"},"","","","","23/11/2012 10:07:37",""]
[258,1211,7,5,"7/21"," L","7/21. L","","75mm Flanged adaptor to 75mm HDPe pipe","No",1,"","","","","30/10/2021 07:54:07",""]
[259,1205,7,5,"7/22"," A","7/22. A","","160mm Straight coupling to 160mm uPVC pipe","No",1,"","","","","30/10/2021 07:54:17",""]
[260,1196,7,5,"7/22","","7/22","","PAINTING","H3",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:34:58",""]
[261,1197,7,5,"7/22","","7/22","","Two coats coal tar epoxy paint on:","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:16:22",""]
[262,1204,7,5,"7/22"," B","7/22. B","","General surfaces of galvanised pipes","m2",2,"","","","","11/11/2021 11:18:00",""]
[264,9458,7,6,"7/24","","7/24","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:25",""]
[265,6091,7,6,"7/24","","7/24","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:01",""]
[266,9459,7,6,"7/24","","7/24","","BILL NO. 6","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:55:45",""]
[267,188,7,6,"7/24","","7/24","","STORMWATER DRAINAGE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:26",""]
[268,189,7,6,"7/24","","7/24","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:29:42",""]
[269,190,7,6,"7/24","","7/24","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:31",""]
[270,191,7,6,"7/24","","7/24","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:29:42",""]
[271,5631,7,6,"7/24","","7/24","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:00:11",""]
[272,5632,7,6,"7/24","","7/24","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:32",""]
[273,192,7,6,"7/24","","7/24","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:29:42",""]
[274,193,7,6,"7/24","","7/24","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:29:42",""]
[275,857,7,6,"7/24","","7/24","","STORMWATER DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","28/05/2012 09:37:51",""]
[276,1628,7,6,"7/24","","7/24","","SUB-SOIL DRAINAGE","H3",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:45:57",""]
[277,1807,7,6,"7/24","","7/24","","Earthworks","H4",{"v":0,"d":"0.0"},"","","","","31/07/2012 03:43:20",""]
[278,1629,7,6,"7/24"," A","7/24. A","","Excavation in earth not exceeding 2m deep for pipe trenches (Labour Intensive)","m3",53,"","","","","26/06/2023 10:16:32",""]
[279,1631,7,6,"7/25"," A","7/25. A","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",41,"","","","","26/06/2023 10:17:19",""]
[280,1666,7,6,"7/25"," B","7/25. B","","Imported G5 backfilling to pipe trenches, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 10:17:24",""]
[281,7660,7,6,"7/25"," C","7/25. C","","Bedding material supplied by the contractor, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",12,"","","","","26/06/2023 10:17:28",""]
[282,1667,7,6,"7/25"," D","7/25. D","","Extra over trench excavations in earth for excavation in soft rock","m3",2,"","","","","30/10/2021 07:54:58",""]
[283,1668,7,6,"7/25"," E","7/25. E","","Extra over trench excavations in earth for excavation in hard rock","m3",1,"","","","","30/10/2021 07:55:01",""]
[284,1669,7,6,"7/25"," F","7/25. F","","Extra over all excavations for carting away surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",19,"","","","","30/10/2021 07:55:04",""]
[285,862,7,6,"7/25","","7/25","","Class 100D concrete pipes to SANS677","H4",{"v":0,"d":"0.0"},"","","","","28/05/2012 09:37:52",""]
[286,1650,7,6,"7/25"," G","7/25. G","","450mm Pipes laid in trenches (Trenches elsewhere)","m",16,"","","","","26/06/2023 10:18:06",""]
[287,1665,7,6,"7/25"," H","7/25. H","","525mm Pipes laid in trenches (Trenches elsewhere)","m",14,"","","","","26/06/2023 10:18:14",""]
[288,1643,7,6,"7/25","","7/25","","Sumps, catchpits, inspection chambers etc., including concrete kerbs or precast concrete cover slabs (as per details on drawings C5593-SITE-SW-54 & 55) (gratings and covers elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:55:20",""]
[289,1679,7,6,"7/25"," I","7/25. I","","1 160 x 930mm Single inlet roadside stormwater catchpit exceeding 1 000mm and not exceeding 2 000mm deep internally, complete including kerbing, reinforced covers, etc. (as per detail on drawing C5593-SITE-SW-54)","No",1,"","","","","30/10/2021 07:55:37",""]
[290,1647,7,6,"7/25"," J","7/25. J","","1 160 x 930mm Catchpit exceeding 1 000mm and not exceeding 2 000mm deep internally","No",1,"","","","","06/12/2021 10:55:46",""]
[291,1644,7,6,"7/25"," K","7/25. K","","930 x 930mm Inspection chamber not exceeding 1 000mm deep internally","No",2,"","","","","06/12/2021 10:56:18",""]
[292,1645,7,6,"7/25"," L","7/25. L","","930 x 930mm Inspection chamber exceeding 1 000mm and not exceeding 2 000mm deep internally","No",3,"","","","","06/12/2021 10:56:45",""]
[293,1880,7,6,"7/25"," M","7/25. M","","930 x 930mm Inspection chamber exceeding 2 000mm and not exceeding 3 000mm deep internally","No",1,"","","","","06/12/2021 10:57:04",""]
[294,13694,7,6,"7/26","","7/26","","Completion of brick inspection concrete cover slabs (gratings and covers elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 03:34:54",""]
[295,9980,7,6,"7/26"," A","7/26. A","","1 160 x 930mm Single inlet roadside stormwater catchpit","No",7,"","","","","27/06/2023 03:40:14",""]
[296,9895,7,6,"7/26"," B","7/26. B","","1 160 x 930mm Brick catchpit","No",8,"","","","","27/06/2023 03:40:18",""]
[297,9953,7,6,"7/26"," C","7/26. C","","930 x 930mm Brick inspection chamber","No",6,"","","","","27/06/2023 03:40:23",""]
[298,13719,7,6,"7/26","","7/26","","Completion of brick inspection chambers by raising or breaking down of brickwork to final levels","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:20:38",""]
[299,13720,7,6,"7/26"," D","7/26. D","","Breaking down and removing one brick walls in inspection chambers to reach final levels","m2",10,"","","","","27/06/2023 03:17:03",""]
[300,13682,7,6,"7/26"," E","7/26. E","","One brick walls of NFPE bricks (14 MPa nominal compressive strength) in class II (1:3) cement mortar in draw chambers, catchpits, manholes, etc.","m2",10,"","","","","09/12/2021 03:56:37",""]
[301,13683,7,6,"7/26"," F","7/26. F","","150mm Wide brick reinforcement built in horizontally","m",17,"","","","","09/12/2021 03:56:38",""]
[302,1648,7,6,"7/26","","7/26","","Gratings, covers, etc.","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:18:29",""]
[303,9909,7,6,"7/26"," G","7/26. G","","610 x 610mm Pre-cast concrete cover (as per drawing no. C5593-SITE-SW-55)","No",11,"","","","","30/10/2021 07:56:42",""]
[304,1707,7,6,"7/26"," H","7/26. H","","640 x 640mm Pre-cast concrete cover and steel frame (as per drawing no. C5593-SITE-SW-55)","No",20,"","","","","30/10/2021 07:56:46",""]
[305,1649,7,6,"7/26"," I","7/26. I","","Galvanised steel catchpit grating and frame size 640 x 640mm (as per details of grids and frames on drawing C5593-SITE-SW-55)","No",9,"","","","","30/10/2021 07:57:01",""]
[306,7157,7,6,"7/26"," J","7/26. J","","Galvanised steel double catchpit grating and frame size 1 250 x 640mm (as per details of grids and frames on drawing C5593-SITE-SW-55)","No",1,"","","","","10/10/2012 05:01:40",""]
[307,3898,7,6,"7/26","","7/26","","SURFACE DRAINAGE","H3",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:46:12",""]
[308,3899,7,6,"7/26","","7/26","","Precast or in-situ concrete (25MPa/19mm stone) open stormwater channels with dished waterway formed in top, finished smooth on all exposed surfaces and with angles rounded, cast in suitable lengths, and reinforced as necessary for handling if precast, including all formwork, moulds, shallow excavation, filling and ramming, damp proofing, laying to falls, bedding and pointing in (3:1) cement mortar","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:07:18",""]
[309,12293,7,6,"7/26"," K","7/26. K","","Channel size 300 x 100mm thick overall","m",252,"","","","","06/11/2021 12:16:20",""]
[310,12294,7,6,"7/27"," A","7/27. A","","Ditto, but circular to not exceeding 4m radius","m",3,"","","","","06/11/2021 12:16:23",""]
[311,12295,7,6,"7/27"," B","7/27. B","","Ditto, but circular to exceeding 4m radius ","m",89,"","","","","06/11/2021 12:16:26",""]
[312,12296,7,6,"7/27"," C","7/27. C","","Extra for angle intersection","No",9,"","","","","06/11/2021 12:16:30",""]
[313,12297,7,6,"7/27"," D","7/27. D","","Extra for stop end","No",5,"","","","","06/11/2021 12:16:33",""]
[314,12298,7,6,"7/27"," E","7/27. E","","Channel size 370 x 200mm thick overall","m",41,"","","","","06/11/2021 12:16:50",""]
[315,12299,7,6,"7/27"," F","7/27. F","","Extra for stop end","No",3,"","","","","06/11/2021 12:16:54",""]
[316,8205,7,6,"7/27"," G","7/27. G","","Channel size 500 x 140mm thick overall","m",96,"","","","","06/11/2021 12:17:13",""]
[317,8206,7,6,"7/27"," H","7/27. H","","Ditto, but circular to not exceeding 4m radius","m",17,"","","","","06/11/2021 12:17:24",""]
[318,8207,7,6,"7/27"," I","7/27. I","","Ditto, but circular to exceeding 4m radius","m",15,"","","","","06/11/2021 12:17:30",""]
[319,8208,7,6,"7/27"," J","7/27. J","","Extra for angle intersection","No",5,"","","","","06/11/2021 12:17:35",""]
[320,8209,7,6,"7/27"," K","7/27. K","","Extra for stop end","No",5,"","","","","06/11/2021 12:17:40",""]
[321,6136,7,6,"7/27","","7/27","","BOX CHANNELS","H3",{"v":0,"d":"0.0"},"","","","","01/10/2012 10:00:05",""]
[322,12305,7,6,"7/27","","7/27","","20MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:55:25",""]
[323,12306,7,6,"7/27"," L","7/27. L","","Benching to bottoms of box channels","m3",13,"","","","","18/11/2021 07:50:00",""]
[324,6226,7,6,"7/27","","7/27","","Finishing surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 04:35:17",""]
[325,6227,7,6,"7/27"," M","7/27. M","","Sloping bottoms of box channels","m2",89,"","","","","04/10/2012 03:58:10",""]
[326,12896,7,6,"7/27","","7/27","","Prepare and apply two coats bitumen paint on:","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:57:55",""]
[327,12897,7,6,"7/27"," N","7/27. N","","Concrete surfaces of stormwater channels","m2",145,"","","","","06/12/2021 10:58:57",""]
[328,12857,7,6,"7/27","","7/27","","METALWORK","H2",{"v":0,"d":"0.0"},"","","","","16/11/2021 12:15:15",""]
[329,12858,7,6,"7/27","","7/27","","GALVANISED STEEL DUCT COVERS","H3",{"v":0,"d":"0.0"},"","","","","28/06/2023 10:43:29",""]
[330,12859,7,6,"7/27","","7/27","","Hot-dip galvanised after manufacture stormwater channel covers","H4",{"v":0,"d":"0.0"},"","","","","16/11/2021 12:15:15",""]
[331,13864,7,6,"7/27"," O","7/27. O","","5mm Curved plate duct covers in approximately 500mm widths and approximately 1 400mm lengths (fixing bolts elsewhere)","kg",69,"","","","","28/06/2023 10:44:30",""]
[332,12860,7,6,"7/28"," A","7/28. A","","6mm Plate duct covers in approximately 500mm widths and approximately 1 300mm lengths (taper edge and fixing bolts elsewhere)","kg",528,"","","","","16/11/2021 12:15:23",""]
[333,12861,7,6,"7/28"," B","7/28. B","","20 x 4mm Flat section bearers welded to plate covers","kg",37,"","","","","16/11/2021 12:15:27",""]
[334,13865,7,6,"7/28"," C","7/28. C","","50 x 50 x 3mm Angle section bearers cast into concrete with and including fishtail lugs at 450mm centres","kg",31,"","","","","26/06/2023 08:50:05",""]
[335,12862,7,6,"7/28"," D","7/28. D","","Extra over 6mm plate for 50mm wide tapered edge to perimeter ","m",45,"","","","","06/12/2021 09:06:28",""]
[336,12863,7,6,"7/28"," E","7/28. E","","Hole through 6mm steel for small bolt","No",68,"","","","","16/11/2021 12:15:36",""]
[337,12864,7,6,"7/28"," F","7/28. F","","8 x 40mm Fischer plug and screw including mortice in concrete","No",68,"","","","","07/12/2021 04:57:09",""]
[338,13477,7,6,"7/28"," G","7/28. G","","25 x 4mm Rubber packing between plate and concrete below","m",49,"","","","","07/12/2021 04:58:00",""]
[339,12865,7,6,"7/28","","7/28","","PAINTWORK","H2",{"v":0,"d":"0.0"},"","","","","16/11/2021 12:15:16",""]
[340,12866,7,6,"7/28","","7/28","","Stoncor Stonshield non-slip textured epoxy urethane coating on galvanised surfaces","H4",{"v":0,"d":"0.0"},"","","","","16/11/2021 12:15:16",""]
[341,12867,7,6,"7/28"," H","7/28. H","","Stormwater channel cover plates","m2",25,"","","","","23/06/2023 11:01:27",""]
[342,1809,7,6,"7/28","","7/28","","GABIONS AND INTERLOCKING BLOCK RETAINING STRUCTURES","H2",{"v":0,"d":"0.0"},"","","","","31/07/2012 03:46:52",""]
[343,1811,7,6,"7/28","","7/28","","Gabions are to be of double twisted hexagonal wire mesh (nominal 80 x 100mm mesh of 2,7mm galvanised wire, with 3,5mm galvanised wire framing and with partitions at 1m centres).  All wire to be hot-dip galvanised to SANS 675","",{"v":0,"d":"0.0"},"","","","","31/07/2012 03:46:52",""]
[344,1812,7,6,"7/29","","7/29","","Gabions of galvanised wire boxes with diaphragm divisions @ 1m c/c, butt-jointed, laced together and filled with broken stone","H4",{"v":0,"d":"0.0"},"","","","","29/10/2021 11:23:00",""]
[345,5126,7,6,"7/29"," A","7/29. A","","2 x 0,5 x 0,5m Box properly bonded","No",10,"","","","","19/11/2021 10:02:52",""]
[346,1817,7,6,"7/29"," B","7/29. B","","2 x 1 x 0,3m Mattress","No",7,"","","","","19/11/2021 10:03:00",""]
[347,5147,7,6,"7/29"," C","7/29. C","","2 x 2 x 0,3m Mattress","No",2,"","","","","19/11/2021 10:03:07",""]
[348,5228,7,6,"7/29","","7/29","","Type U24 filter fabric blanket with 200mm laps","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 11:30:02",""]
[349,5230,7,6,"7/29"," D","7/29. D","","Under stone filled gabion mattresses including preparing ground surface under","m2",12,"","","","","27/02/2014 08:04:53",""]
[350,5231,7,6,"7/29"," E","7/29. E","","Vertically behind stone filled gabion retaining walls","m2",8,"","","","","27/02/2014 08:04:58",""]
[351,1651,7,6,"7/29","","7/29","","HEADWALLS","H2",{"v":0,"d":"0.0"},"","","","","27/07/2012 12:53:13",""]
[352,1652,7,6,"7/29","","7/29","","Earthworks","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 08:17:54",""]
[353,1653,7,6,"7/29"," F","7/29. F","","Excavate in earth for foundation trenches not exceeding 2m deep and deposit excavated material on site for use as filling or backfilling (Labour Intensive)","m3",4,"","","","","26/06/2023 10:19:24",""]
[354,1654,7,6,"7/29"," G","7/29. G","","Earth filling arising from the excavations compacted to 90% Modified AASHTO density in backfilling to foundation excavations (Labour Intensive)","m3",3,"","","","","26/06/2023 10:19:27",""]
[355,1236,7,6,"7/29"," H","7/29. H","","Risk of collapse of sides of excavations not exceeding 1,5m deep","m2",2,"","","","","06/12/2021 10:37:02",""]
[356,1252,7,6,"7/29"," I","7/29. I","","Compaction of ground surface under floors, etc. including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 90% Mod AASHTO density","m2",1,"","","","","06/12/2021 10:37:40",""]
[357,1655,7,6,"7/29","","7/29","","Concrete","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 08:18:18",""]
[358,1656,7,6,"7/29"," J","7/29. J","","20Mpa Unreinforced concrete in foundations cast against excavated surfaces","m3",1,"","","","","06/12/2021 11:18:31",""]
[359,1657,7,6,"7/29"," K","7/29. K","","20Mpa Unreinforced concrete in pavings cast against excavated surfaces","m3",3,"","","","","06/12/2021 11:19:01",""]
[360,5145,7,6,"7/29"," L","7/29. L","","20Mpa Unreinforced concrete in walls cast in/on formwork","m3",3,"","","","","06/12/2021 11:19:33",""]
[361,1658,7,6,"7/30"," A","7/30. A","","Extra for floating off smooth tops of surface beds laid in panels with a wood float including slightly rounded edges to panels.","m2",11,"","","","","09/08/2012 02:58:41",""]
[362,1659,7,6,"7/30","","7/30","","Formwork","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 08:18:28",""]
[363,5146,7,6,"7/30"," B","7/30. B","","Rough formwork to walls","m2",24,"","","","","21/09/2012 11:35:45",""]
[364,1260,7,6,"7/30"," C","7/30. C","","Rough formwork to edges exceeding 300mm high","m2",0.5,"","","","","07/06/2012 03:52:55",""]
[365,1660,7,6,"7/30"," D","7/30. D","","Rough formwork to edges, risers, ends and reveals not exceeding 300mm high","m",29,"","","","","06/12/2021 11:19:59",""]
[366,12997,7,6,"7/30","","7/30","","Mild steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","02/12/2021 10:15:37",""]
[367,12998,7,6,"7/30"," E","7/30. E","","Various diameter bars","t",0.05,"","","","","02/12/2021 10:15:37",""]
[368,12999,7,6,"7/30","","7/30","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","02/12/2021 10:15:37",""]
[369,13000,7,6,"7/30"," F","7/30. F","","Various diameter bars","t",0.11,"","","","","02/12/2021 10:15:37",""]
[370,1245,7,6,"7/30","","7/30","","BRICKWORK","H3",{"v":0,"d":"0.0"},"","","","","07/06/2012 08:54:38",""]
[371,1246,7,6,"7/30"," G","7/30. G","","One brick wall in extra hard burnt engineering bricks","m2",0.4,"","","","","06/12/2021 10:39:23",""]
[372,1251,7,6,"7/30"," H","7/30. H","","Extra over brickwork for brick-on-edge header course","m",2,"","","","","06/12/2021 10:39:42",""]
[373,1262,7,6,"7/30","","7/30","","SUNDRIES","H3",{"v":0,"d":"0.0"},"","","","","15/11/2021 01:39:19",""]
[374,1263,7,6,"7/30"," I","7/30. I","","300 x 300mm Hot-dipped galvanised expanded metal mesh grid with and including 40 x 3mm flat frame, bolted to concrete wall with and including four M10 rawlbolts","No",1,"","","","","04/10/2012 12:48:53",""]
[375,7006,7,6,"7/30","","7/30","","TESTING","H2",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:23:46",""]
[376,7007,7,6,"7/30"," J","7/30. J","","Testing stormwater pipe system","Item",{"v":1,"d":"1.00"},"","","","","10/04/2013 09:55:27",""]
[377,6997,7,6,"7/30","","7/30","","AS-BUILT DRAWINGS","H2",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:12:44",""]
[378,6998,7,6,"7/30"," K","7/30. K","","Provision of as-built drawings","Item",{"v":1,"d":"1.00"},"","","","","11/11/2021 11:18:27",""]
[380,9460,7,7,"7/32","","7/32","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:29",""]
[381,6092,7,7,"7/32","","7/32","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:05",""]
[382,9461,7,7,"7/32","","7/32","","BILL NO. 7","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:55:49",""]
[383,1721,7,7,"7/32","","7/32","","STORMWATER HARVESTING TANK AND OIL INTERCEPTOR","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:32",""]
[384,1722,7,7,"7/32","","7/32","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:20",""]
[385,1723,7,7,"7/32","","7/32","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:35",""]
[386,1724,7,7,"7/32","","7/32","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:20",""]
[387,5633,7,7,"7/32","","7/32","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:00:20",""]
[388,5634,7,7,"7/32","","7/32","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:39",""]
[389,1725,7,7,"7/32","","7/32","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:20",""]
[390,1726,7,7,"7/32","","7/32","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:21",""]
[391,1731,7,7,"7/32","","7/32","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:21",""]
[392,1747,7,7,"7/32","","7/32","","FILLING, ETC","H3",{"v":0,"d":"0.0"},"","","","","24/10/2012 12:51:05",""]
[393,1748,7,7,"7/32","","7/32","","Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 93% Modified AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 12:53:15",""]
[394,1749,7,7,"7/32"," A","7/32. A","","Backfilling to hole excavations (Labour Intensive)","m3",200,"","","","","26/06/2023 10:19:56",""]
[395,1758,7,7,"7/33","","7/33","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:25",""]
[396,1759,7,7,"7/33","","7/33","","40MPa/19mm Concrete with an approved waterproofing admixture (C500NF at a ratio of 1.5% by weight of total cementitious material, including blast furnace slag) added at the batching plant","H4",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:16:17",""]
[397,1760,7,7,"7/33"," A","7/33. A","","Surface beds","m3",0.4,"","","","","06/12/2021 11:21:35",""]
[398,1761,7,7,"7/33"," B","7/33. B","","Slabs including beams and inverted beams","m3",7,"","","","","06/12/2021 11:21:55",""]
[399,1762,7,7,"7/33"," C","7/33. C","","Walls","m3",3,"","","","","06/12/2021 11:22:10",""]
[400,1764,7,7,"7/33","","7/33","","TEST CUBES","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:26",""]
[401,1765,7,7,"7/33"," D","7/33. D","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",6,"","","","","06/12/2021 11:22:20",""]
[402,1766,7,7,"7/33","","7/33","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:26",""]
[403,1767,7,7,"7/33","","7/33","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:26",""]
[404,1768,7,7,"7/33"," E","7/33. E","","Surface beds, slabs, etc. to falls (Labour Intensive)","m2",30,"","","","","26/06/2023 10:29:17",""]
[405,1769,7,7,"7/33","","7/33","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:27",""]
[406,1770,7,7,"7/33","","7/33","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:27",""]
[407,1771,7,7,"7/33"," F","7/33. F","","Walls with total height not exceeding 3,5m above bearing level","m2",34,"","","","","06/12/2021 11:22:30",""]
[408,1773,7,7,"7/33"," G","7/33. G","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",23,"","","","","06/12/2021 11:22:43",""]
[409,1777,7,7,"7/33","","7/33","","Rough formwork to soffits","H4",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:28",""]
[410,1795,7,7,"7/33"," H","7/33. H","","Slabs propped up not exceeding 1,5m high","m2",1,"","","","","06/12/2021 11:22:58",""]
[411,1828,7,7,"7/33"," I","7/33. I","","Slabs propped up exceeding 1.5m and not exceeding 3.5m high, including removal through 600 x 600mm opening","m2",26,"","","","","06/12/2021 11:23:08",""]
[412,1778,7,7,"7/33"," J","7/33. J","","Slabs propped up exceeding 1.5m and not exceeding 3.5m high, including removal through 900 x 900mm opening","m2",1,"","","","","06/12/2021 11:23:28",""]
[413,1779,7,7,"7/34","","7/34","","Rough formwork to form","H4",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:28",""]
[414,1780,7,7,"7/34"," A","7/34. A","","600mm Diameter opening through not exceeding 300mm thick slab","No",2,"","","","","06/12/2021 11:23:38",""]
[415,1834,7,7,"7/34"," B","7/34. B","","Opening exceeding 2m and not exceeding 3m girth through not exceeding 300mm slab","No",4,"","","","","06/12/2021 11:23:48",""]
[416,1804,7,7,"7/34"," C","7/34. C","","Opening exceeding 3m and not exceeding 4m girth through not exceeding 300mm wall or beam","No",1,"","","","","06/12/2021 11:24:01",""]
[417,1782,7,7,"7/34","","7/34","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:29",""]
[418,1785,7,7,"7/34","","7/34","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","30/07/2012 09:07:29",""]
[419,13491,7,7,"7/34"," D","7/34. D","","Various diameter bars","t",{"v":0.5,"d":"0.50"},"","","","","08/12/2021 05:10:12",""]
[420,1806,7,7,"7/34","","7/34","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","31/07/2012 12:31:51",""]
[421,1800,7,7,"7/34"," E","7/34. E","","600mm Diameter x 63kg type 2A concrete-filled light-duty polymer lockable cover and frame","No",2,"","","","","07/12/2021 12:08:28",""]
[422,1832,7,7,"7/34"," F","7/34. F","","600 x 600mm x 38kg Type 9B Polymer lockable manhole cover and frame","No",4,"","","","","02/10/2012 04:39:00",""]
[423,10244,7,7,"7/34"," G","7/34. G","","560mm Heavy duty HDPe (class 10) puddle flange including setting up and fix into position and grouted as per engineers specifications","No",1,"","","","","08/12/2021 05:10:49",""]
[424,1896,7,7,"7/34","","7/34","","SOIL DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","03/08/2012 05:24:58",""]
[425,1897,7,7,"7/34","","7/34","","Galvanised steel pipes with screwed and socketed joints","H4",{"v":0,"d":"0.0"},"","","","","02/10/2012 04:02:55",""]
[426,1898,7,7,"7/34"," H","7/34. H","","75mm Pipes in concrete floors","m",1,"","","","","06/12/2021 11:24:19",""]
[427,6337,7,7,"7/34","","7/34","","Grade 316 stainless steel pipes","H4",{"v":0,"d":"0.0"},"","","","","02/10/2012 04:01:43",""]
[428,1909,7,7,"7/34"," I","7/34. I","","75mm Pipes","m",1,"","","","","06/12/2021 11:24:28",""]
[429,1899,7,7,"7/34","","7/34","","Extra over stainless steel pipes for stainless steel fittings ","H4",{"v":0,"d":"0.0"},"","","","","02/10/2012 04:07:16",""]
[430,1903,7,7,"7/34"," J","7/34. J","","75mm Bend","No",1,"","","","","06/12/2021 11:24:42",""]
[431,1908,7,7,"7/34"," K","7/34. K","","75mm Flanged adaptor to 75mm HDPe pipe","No",2,"","","","","06/12/2021 11:24:53",""]
[432,1910,7,7,"7/34"," L","7/34. L","","75mm Puddle flange","No",2,"","","","","06/12/2021 11:25:05",""]
[433,1905,7,7,"7/35"," A","7/35. A","","75mm x 850mm Long pipe flanged at one end","No",1,"","","","","06/12/2021 11:25:20",""]
[434,1911,7,7,"7/35"," B","7/35. B","","75mm Diameter x 300mm long flanged both ends puddle pipe","No",1,"","","","","06/12/2021 11:25:28",""]
[436,9462,7,8,"7/37","","7/37","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:32",""]
[437,6094,7,8,"7/37","","7/37","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:09",""]
[438,9463,7,8,"7/37","","7/37","","BILL NO. 8","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:55:52",""]
[439,212,7,8,"7/37","","7/37","","WATER PONDS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:37",""]
[440,213,7,8,"7/37","","7/37","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:13",""]
[441,214,7,8,"7/37","","7/37","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:41",""]
[442,215,7,8,"7/37","","7/37","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:13",""]
[443,5637,7,8,"7/37","","7/37","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:00:36",""]
[444,5638,7,8,"7/37","","7/37","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:48",""]
[445,216,7,8,"7/37","","7/37","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:13",""]
[446,217,7,8,"7/37","","7/37","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:13",""]
[447,6169,7,8,"7/37","","7/37","","EXCAVATIONS, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","24/10/2012 12:58:17",""]
[448,6525,7,8,"7/37","","7/37","","EXCAVATIONS, ETC","H3",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:16:34",""]
[449,6626,7,8,"7/37","","7/37","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","27/08/2013 05:37:52",""]
[450,7105,7,8,"7/37"," A","7/37. A","","Reduced levels under floors (Labour Intensive)","m3",15,"","","","","26/06/2023 10:56:44",""]
[451,7081,7,8,"7/37"," B","7/37. B","","Holes (Labour Intensive)","m3",4,"","","","","26/06/2023 10:56:49",""]
[452,6531,7,8,"7/38","","7/38","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:17:07",""]
[453,6532,7,8,"7/38"," A","7/38. A","","Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",18,"","","","","30/10/2021 07:59:14",""]
[454,6533,7,8,"7/38","","7/38","","Risk of collapse of excavations","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:17:08",""]
[455,6534,7,8,"7/38"," B","7/38. B","","Sides of excavations not exceeding 1,5m deep","m2",31,"","","","","04/11/2021 01:29:21",""]
[456,6524,7,8,"7/38","","7/38","","FILLING, ETC","H3",{"v":0,"d":"0.0"},"","","","","24/10/2012 01:00:29",""]
[457,6633,7,8,"7/38","","7/38","","Selected earth filling obtained from stock piles on site","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 02:36:46",""]
[458,6628,7,8,"7/38"," C","7/38. C","","Filling under floors, well watered and consolidated in layers not exceeding 150 mm thick to obtain 93% modified AASHTO dry density (Labour Intensive)","m3",50,"","","","","26/06/2023 10:20:30",""]
[459,6631,7,8,"7/38","","7/38","","Earth filling supplied by the contractor","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 02:28:11",""]
[460,6632,7,8,"7/38"," D","7/38. D","","Imported G5 filling under floors, well watered and consolidated in layers not exceeding 150 mm thick to obtain 95% modified AASHTO dry density (Labour Intensive)","m3",24,"","","","","26/06/2023 10:56:32",""]
[461,3499,7,8,"7/38"," E","7/38. E","","Clean, washed river sand filling (Labour Intensive)","m3",2,"","","","","26/06/2023 10:20:42",""]
[462,7109,7,8,"7/38","","7/38","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","09/10/2012 01:14:00",""]
[463,7111,7,8,"7/38"," F","7/38. F","","Scarify surface of in-situ material for a depth of 150mm and compact to 93% modified AASHTO density (Labour Intensive)","m2",21,"","","","","26/06/2023 10:29:00",""]
[464,6608,7,8,"7/38","","7/38","","Pebble covering obtained from the Gamtoos river area","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 09:58:56",""]
[465,6617,7,8,"7/38"," G","7/38. G","","Covering of river stone pebbles varying in size from 20mm to 40mm diameter in stormwater channel (Labour Intensive)","m3",2,"","","","","26/06/2023 10:20:49",""]
[466,6539,7,8,"7/38","","7/38","","REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:17:37",""]
[467,6540,7,8,"7/38","","7/38","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:17:37",""]
[468,7090,7,8,"7/38"," H","7/38. H","","Surface beds","m3",29,"","","","","24/01/2014 03:27:58",""]
[469,6542,7,8,"7/38","","7/38","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:17:55",""]
[470,6543,7,8,"7/38","","7/38","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:17:55",""]
[471,7091,7,8,"7/38"," I","7/38. I","","Surface beds","m3",19,"","","","","09/10/2012 12:49:44",""]
[472,6545,7,8,"7/39","","7/39","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:18:58",""]
[473,6546,7,8,"7/39","","7/39","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:18:58",""]
[474,7084,7,8,"7/39"," A","7/39. A","","Inner face of planter box walls (other face against excavated or existing surfaces)","m2",27,"","","","","04/09/2013 08:58:35",""]
[475,7083,7,8,"7/39"," B","7/39. B","","Ditto, but circular to exceeding 1m radius","m2",45,"","","","","18/10/2012 08:21:04",""]
[476,6548,7,8,"7/39"," C","7/39. C","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",13,"","","","","06/12/2021 11:27:20",""]
[477,7082,7,8,"7/39"," D","7/39. D","","Ditto, but circular to exceeding 1m radius","m",10,"","","","","06/12/2021 05:37:57",""]
[478,6553,7,8,"7/39","","7/39","","Rough formwork to form","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:19:46",""]
[479,6554,7,8,"7/39"," E","7/39. E","","50mm Diameter opening through 200mm slab","No",10,"","","","","04/10/2012 03:49:24",""]
[480,6555,7,8,"7/39"," F","7/39. F","","50mm Diameter opening through 250mm slab","No",18,"","","","","04/10/2012 03:53:33",""]
[481,7089,7,8,"7/39"," G","7/39. G","","50mm Diameter opening through 260mm slab","No",3,"","","","","08/10/2012 02:59:16",""]
[482,6598,7,8,"7/39"," H","7/39. H","","50mm Diameter opening through 200mm wall or beam","No",4,"","","","","24/10/2012 01:06:24",""]
[483,6836,7,8,"7/39"," I","7/39. I","","600 x 600mm Opening through 150mm slab","No",8,"","","","","05/10/2012 10:46:17",""]
[484,6557,7,8,"7/39","","7/39","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:20:02",""]
[485,6558,7,8,"7/39","","7/39","","Mild steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:20:02",""]
[486,6559,7,8,"7/39"," J","7/39. J","","Various diameter bars","t",{"v":0.5,"d":"0.50"},"","","","","17/11/2021 12:00:26",""]
[487,6561,7,8,"7/39","","7/39","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:20:03",""]
[488,6563,7,8,"7/39"," K","7/39. K","","Various diameter bars","t",{"v":1,"d":"1.00"},"","","","","17/11/2021 12:00:45",""]
[489,6568,7,8,"7/39","","7/39","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:20:04",""]
[490,6569,7,8,"7/39"," L","7/39. L","","Type S500 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",222,"","","","","26/06/2023 10:21:09",""]
[491,6611,7,8,"7/39","","7/39","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:36:04",""]
[492,6612,7,8,"7/40","","7/40","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 01:09:40",""]
[493,7113,7,8,"7/40"," A","7/40. A","","Surface beds, slabs, etc.","m2",111,"","","","","26/06/2023 10:21:14",""]
[494,3417,7,8,"7/40","","7/40","","GRANITE WALL LININGS, ETC","H2",{"v":0,"d":"0.0"},"","","","","24/10/2012 01:09:58",""]
[495,3418,7,8,"7/40","","7/40","","Flamed Rustenburg granite with polished finish, fixed with silicone adhesive (plaster by others)","H4",{"v":0,"d":"0.0"},"","","","","09/08/2012 05:04:18",""]
[496,3419,7,8,"7/40"," B","7/40. B","","20mm Thick composite horisontal slab size approximately 3,87m2 total area; comprising 5 separately cut odd-shaped panels as detailed on drawings no. 25379-NC-HP-4200-02 & 4200.04 (Artwork and engraving measured elsewhere)","No",1,"","","","","27/06/2023 02:15:20",""]
[497,3420,7,8,"7/40"," C","7/40. C","","Extra over for cutting 150mm diameter hole through 30mm granite top","No",1,"","","","","17/11/2021 11:51:52",""]
[498,13833,7,8,"7/40"," D","7/40. D","","Provisional Sum of R10 000.00 (Ten Thousand) for the engravings on granite slab, to be done by a specialist sub-contractor","Item",{"v":1,"d":"1.00"},{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"","","22/06/2023 08:53:33",""]
[499,6570,7,8,"7/40","","7/40","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 11:20:46",""]
[500,3476,7,8,"7/40","","7/40","","Flexible waterproofing slurry compound of a two component polymer modified cementitious coating applied in accordance with the manufacturers recommendations. The coating shall conform to the equirements of EMPA test 235.528, EMPA test 162.475/2. The compound shall have a resistance to positive pressure of 20 bars and negative pressure of 4 bars. Waterproofiing to be reinforced at all corners/direction change with membrane felt as per waterproofing specialist","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 01:12:16",""]
[501,3470,7,8,"7/40"," E","7/40. E","","To bottoms and sides of ponds, pump rooms, etc.","m2",251,"","","","","26/06/2023 10:21:24",""]
[502,7085,7,8,"7/40","","7/40","","Expanding hydrophilic rubber waterstops fixed to concrete","H4",{"v":0,"d":"0.0"},"","","","","08/10/2012 02:28:17",""]
[503,7086,7,8,"7/40"," F","7/40. F","","23mm Diameter waterstops fixed with concrete nails at 300mm centres or 6mm thick adhesive","m",84,"","","","","08/10/2012 02:28:22",""]
[504,7210,7,8,"7/40","","7/40","","PLASTERING","H2",{"v":0,"d":"0.0"},"","","","","17/10/2012 10:29:29",""]
[505,7215,7,8,"7/40","","7/40","","Screeds wood floated, on concrete","H4",{"v":0,"d":"0.0"},"","","","","17/10/2012 11:12:44",""]
[506,3471,7,8,"7/40"," G","7/40. G","","To floors (Labour Intensive)","m2",116,"","","","","26/06/2023 10:21:37",""]
[507,12099,7,8,"7/41"," A","7/41. A","","40mm Thick on floors laid to falls (Labour Intensive)","m2",5,"","","","","26/06/2023 10:21:41",""]
[508,7213,7,8,"7/41","","7/41","","One coat 1:5 cement plaster, on concrete","H4",{"v":0,"d":"0.0"},"","","","","17/10/2012 10:36:19",""]
[509,3475,7,8,"7/41"," B","7/41. B","","On narrow widths circular on plan (Labour Intensive)","m2",47,"","","","","30/10/2021 08:10:32",""]
[510,3494,7,8,"7/41"," C","7/41. C","","On horisontal surfaces in narrow widths (Labour Intensive)","m2",38,"","","","","30/10/2021 08:10:48",""]
[511,3491,7,8,"7/41"," D","7/41. D","","Walls circular on plan (Labour Intensive)","m2",88,"","","","","30/10/2021 08:10:58",""]
[512,7211,7,8,"7/41","","7/41","","METALWORK","H2",{"v":0,"d":"0.0"},"","","","","17/10/2012 10:30:46",""]
[513,3496,7,8,"7/41"," E","7/41. E","","Perimeter edging formed of 6 x 100mm Grade 316 Stainless steel plate fixed to concrete pond surround (elsewhere) with neutral curing, low modulus construction and concrete silicone sealant","m",8,"","","","","09/12/2021 05:16:01",""]
[514,3424,7,8,"7/41","","7/41","","STEPPING STONES","H2",{"v":0,"d":"0.0"},"","","","","17/10/2012 11:03:45",""]
[515,3425,7,8,"7/41","","7/41","","THE FOLLOWING IN PURPOSE-MADE GENOCIDE POND LEAF-SHAPED STEPPING STONES & PLANTERS, INCLUDING ALL FINISHES (ARTISTIC IN-LAYS MEASURED ELSEWHERE) (ALL AS PER DETAILS ON DRAWING 25116-MUS-102)","",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:30:56",""]
[516,7102,7,8,"7/41"," F","7/41. F","","25Mpa/19mm Reinforced concrete infill to stepping stone","m3",4,"","","","","06/12/2021 11:31:43",""]
[517,3464,7,8,"7/41"," G","7/41. G","","Grade 316 stainless steel planter box framework size 805 x 1 880mm overall (Type 5)","No",3,"","","","","30/10/2021 08:11:57",""]
[518,3427,7,8,"7/41"," H","7/41. H","","Ditto, size 1 047 x 2 579mm overall (Type 3)","No",2,"","","","","04/11/2021 02:34:25",""]
[519,3426,7,8,"7/41"," I","7/41. I","","Ditto, size 1 385 x 3 350mm overall (Type 1)","No",1,"","","","","04/11/2021 02:34:35",""]
[520,3463,7,8,"7/41"," J","7/41. J","","Grade 316 stainless steel stepping stone framework size 630 x 1 555mm overall (Type 6)","No",2,"","","","","30/10/2021 08:12:21",""]
[521,3429,7,8,"7/41"," K","7/41. K","","Ditto, size 915 x 2 280mm overall (Type 4)","No",9,"","","","","04/11/2021 02:34:46",""]
[522,3428,7,8,"7/41"," L","7/41. L","","Ditto, size 1 385 x 3 350mm overall (Type 2)","No",5,"","","","","04/11/2021 02:34:59",""]
[523,3432,7,8,"7/41","","7/41","","END OF THE FOLLOWING IN PURPOSE-MADE GENOCIDE POND LEAF STEPPING STONES","",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:32:21",""]
[524,7214,7,8,"7/41","","7/41","","SUNDRIES","H3",{"v":0,"d":"0.0"},"","","","","17/10/2012 10:48:32",""]
[525,3480,7,8,"7/41"," M","7/41. M","","19mm Crushed stone in filling in planter boxes (Labour Intensive)","m3",14,"","","","","30/10/2021 08:13:13",""]
[526,12888,7,8,"7/42"," A","7/42. A","","Approximately 20 to 40mm diameter round and smooth river pebbles from Gamtoos River area set in concrete, colour charcoal grey to brown - group sample to be provided for final approval by architect and landscape architect","m3",4,"","","","","07/12/2021 01:43:32",""]
[527,3483,7,8,"7/42"," B","7/42. B","","Approximately 20 to 40mm diameter round and smooth river pebbles from Gamtoos River area, colour charcoal grey to brown - group sample to be provided for final approval by architect and landscape architect (Labour Intensive)","m3",4,"","","","","09/12/2021 05:17:31",""]
[528,12122,7,8,"7/42"," C","7/42. C","","Approximately 100 to 150mm diameter round and smooth river pebbles from Gamtoos River area, colour charcoal grey to brown - group sample to be provided for final approval by architect and landscape architect (Labour Intensive)","m3",10,"","","","","09/12/2021 05:17:38",""]
[529,3481,7,8,"7/42"," D","7/42. D","","30mm Deep, continuous glass fibre strand grating with mesh size 20 x 20 and gritted top surface, cut to irregular shapes (S21)","m2",28,"","","","","30/10/2021 08:13:37",""]
[530,3482,7,8,"7/42"," E","7/42. E","","A1 grade general-purpose drainage geotextile membrane, with through flow of 300l/s/m². All in accordance with to SANS 10221-88 (S22)","m2",28,"","","","","30/10/2021 08:13:48",""]
[531,3486,7,8,"7/42"," F","7/42. F","","220 x 110 x 75mm Hard-burnt engineering brick bedded in Class II mortar on edge as support to grating over","No",18,"","","","","06/12/2021 11:33:54",""]
[532,7571,7,8,"7/42","","7/42","","Pond installation","H3",{"v":0,"d":"0.0"},"","","","","03/11/2012 07:06:19",""]
[533,7572,7,8,"7/42"," G","7/42. G","","507-552 x 211 x 340mm, 0,43Kw 230V, Self priming pool pump with 190l/min maximum flow (S11)","No",3,"","","","","17/11/2021 11:40:12",""]
[534,12242,7,8,"7/42"," H","7/42. H","","50mm Diameter grade 326 stainless steel water skimmer outlet connected to stainless steel skimmer pipe","No",2,"","","","","10/12/2021 10:37:14",""]
[535,12243,7,8,"7/42"," I","7/42. I","","50mm Diameter grade 316 stainless steel pipe cast in concrete","m",4,"","","","","06/11/2021 12:18:49",""]
[536,13650,7,8,"7/42"," J","7/42. J","","Extra over 50mm diameter stainless steel pipe for bend","No",2,"","","","","10/12/2021 10:38:10",""]
[537,7575,7,8,"7/42"," K","7/42. K","","350 x 284 x 163mm Energy Efficient, electric pool pump with seasonal flow control, flow optimized impeller and hydraulic pump. 170 Watt, 220 – 240v/50Hz Voltage and max flow at 16000l/H (S14)","No",2,"","","","","09/12/2021 05:18:28",""]
[538,7573,7,8,"7/42"," L","7/42. L","","260l/m flow, 950h x 635Ø Bobbin wound Fibreglass and polyester sand filter filled with sand and fitted with side mount valve. Filter to have clamp lock lid, oil filled stainless steel pressure gauge and drainage plug (S12)","No",3,"","","","","09/12/2021 05:18:36",""]
[539,7574,7,8,"7/43"," A","7/43. A","","90mmØ Pvc Dome top overflow/drain with black pvc pipe and 50mm x 1 1/2” male adaptor, all screwed to flanged wall conduit with an o ring to connect to drain point (S13)","No",20,"","","","","17/11/2021 02:37:29",""]
[540,12244,7,8,"7/43"," B","7/43. B","","450 x 450 x 200mm, 2mm Thick grade 3CR12 stainless steel valve box with flush lockable door","No",2,"","","","","09/12/2021 08:19:11",""]
[541,12119,7,8,"7/43"," C","7/43. C","","Custom made stainless steel drain outlet (Prime cost R2 500.00) as per drawing 25379-NC-HP-4200.03","No",1,"","","","","27/06/2023 02:22:39",""]
[542,12077,7,8,"7/43"," D","7/43. D","","150mm Diameter Expanda drain with 110mm outlet as per detail on drawing 25379-HP-4200.03","No",1,"","","","","08/12/2021 05:09:41",""]
[543,12076,7,8,"7/43"," E","7/43. E","","50 x 50 x 75mm, 4mm Thick stainless steel cup nozzle with 50mm thread for PVC adaptor (Prime cost R5 000.00)","No",12,"","","","","10/12/2021 10:37:21",""]
[544,12120,7,8,"7/43"," F","7/43. F","","80 x 80 x 3mm Grade 316 stainless steel square cover plate with and including two M4 countersunk hex bolts fixed into cup nozzle, water outlet hole to be 20 x 20mm","No",12,"","","","","09/12/2021 08:56:43",""]
[545,7576,7,8,"7/43"," G","7/43. G","","Flush fit single jet nozzle (Prime cost R2 500.00) with flow regulator, ball and socket joint to incline water jet from the vertical (S17)","No",6,"","","","","17/11/2021 02:38:25",""]
[546,12239,7,8,"7/43"," H","7/43. H","","40mm Class 16 uPVC pipe cast in concrete","m",1,"","","","","09/12/2021 09:12:42",""]
[547,12245,7,8,"7/43"," I","7/43. I","","40mm Class 16 uPVC pipe laid in and including trenches not exceeding 1m deep","m",6,"","","","","09/12/2021 09:12:53",""]
[548,7577,7,8,"7/43"," J","7/43. J","","50mm Class 16 uPVC pipe laid in and including trenches not exceeding 1m deep","m",54,"","","","","09/12/2021 09:12:30",""]
[549,7578,7,8,"7/43"," K","7/43. K","","Extra over 50mm piping for bend","No",5,"","","","","03/11/2012 05:14:52",""]
[550,7579,7,8,"7/43"," L","7/43. L","","Extra over 50mm piping for tee","No",8,"","","","","04/11/2021 02:37:03",""]
[551,12116,7,8,"7/43"," M","7/43. M","","Extra over 50mm piping for female threaded pipe adaptor","No",12,"","","","","04/11/2021 02:37:07",""]
[552,12110,7,8,"7/43"," N","7/43. N","","50mm HDPe pipe (no excavations)","m",1,"","","","","10/12/2021 02:43:51",""]
[553,13651,7,8,"7/43"," O","7/43. O","","75mm Class 16 uPVC pipe","m",4,"","","","","10/12/2021 10:37:27",""]
[554,13652,7,8,"7/43"," P","7/43. P","","Extra over 75mm pipe for bend","No",4,"","","","","10/12/2021 10:37:31",""]
[555,13653,7,8,"7/43"," Q","7/43. Q","","Extra over 75mm pipe for flanged outlet adaptor","No",2,"","","","","10/12/2021 10:38:03",""]
[556,12117,7,8,"7/43"," R","7/43. R","","22mm Gate valve","No",1,"","","","","07/12/2021 01:51:55",""]
[557,12118,7,8,"7/44"," A","7/44. A","","22mm Ball valve","No",1,"","","","","07/12/2021 01:51:51",""]
[558,12268,7,8,"7/44"," B","7/44. B","","50mm Ball valve","No",2,"","","","","08/12/2021 05:10:02",""]
[560,9464,7,9,"7/46","","7/46","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:36",""]
[561,6095,7,9,"7/46","","7/46","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:13",""]
[562,9465,7,9,"7/46","","7/46","","BILL NO. 9","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:55:56",""]
[563,5821,7,9,"7/46","","7/46","","SYMBOLIC AND PRODUCTIVE GARDEN","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:43",""]
[564,5822,7,9,"7/46","","7/46","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","26/09/2012 01:11:34",""]
[565,5823,7,9,"7/46","","7/46","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:47",""]
[566,5824,7,9,"7/46","","7/46","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","26/09/2012 01:11:34",""]
[567,5825,7,9,"7/46","","7/46","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","26/09/2012 01:11:34",""]
[568,5826,7,9,"7/46","","7/46","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:04:55",""]
[569,5827,7,9,"7/46","","7/46","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","26/09/2012 01:11:35",""]
[570,5828,7,9,"7/46","","7/46","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","26/09/2012 01:11:35",""]
[571,13210,7,9,"7/46","","7/46","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:35:56",""]
[572,13211,7,9,"7/46","","7/46","","FILLING, ETC","H3",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:35:56",""]
[573,13212,7,9,"7/46","","7/46","","Pebble/Stone coverings","H4",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:24:02",""]
[574,13213,7,9,"7/46"," A","7/46. A","","Covering stones obtained from the Gamtoos river area varying in size from 20mm to 40mm diameter","m3",3,"","","","","10/02/2022 12:24:30",""]
[575,13732,7,9,"7/46"," B","7/46. B","","Covering stones obtained from the site of maximum 14mm diameter","m3",3,"","","","","19/05/2022 12:33:58",""]
[576,13214,7,9,"7/47","","7/47","","UNREINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:36:59",""]
[577,13215,7,9,"7/47","","7/47","","30MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:36:59",""]
[578,13216,7,9,"7/47"," A","7/47. A","","Surface beds","m3",1,"","","","","06/12/2021 12:23:37",""]
[579,13245,7,9,"7/47","","7/47","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:47:15",""]
[580,13246,7,9,"7/47","","7/47","","Finishing top surfaces of concrete smooth with a steel trowel","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:47:15",""]
[581,13247,7,9,"7/47"," B","7/47. B","","Surface beds, slabs, etc","m2",7,"","","","","06/12/2021 12:23:53",""]
[582,13217,7,9,"7/47","","7/47","","MOVEMENT JOINTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:57:34",""]
[583,13218,7,9,"7/47"," C","7/47. C","","6mm Thick x 100mm wide galvanised mild steel flat plate in permanent construction joint formwork, with lugs welded on at 350mm centres ","kg",28,"","","","","06/12/2021 11:04:05",""]
[584,13237,7,9,"7/47"," D","7/47. D","","Hole through 6mm plate for small bolt","No",20,"","","","","06/12/2021 11:04:32",""]
[585,13236,7,9,"7/47"," E","7/47. E","","M10 x 80mm Anchor including mortice in concrete","No",20,"","","","","06/12/2021 11:01:05",""]
[586,13238,7,9,"7/47"," F","7/47. F","","Shutter release oils applied to general surfaces of steel formwork","m2",5,"","","","","06/12/2021 11:06:28",""]
[587,13248,7,9,"7/47","","7/47","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:47:49",""]
[588,13249,7,9,"7/47","","7/47","","Fabric reinforcement","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:47:49",""]
[589,13250,7,9,"7/47"," G","7/47. G","","Type 617 fabric reinforcement in concrete surface beds, etc.","m2",7,"","","","","27/06/2023 09:11:38",""]
[590,13252,7,9,"7/47","","7/47","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 12:30:43",""]
[591,13265,7,9,"7/47","","7/47","","Sika grout 212, or similar approved, non-shrink grout","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 01:10:07",""]
[592,13266,7,9,"7/47"," H","7/47. H","","In 50mm diameter x 100mm deep holes","No",5,"","","","","08/12/2021 05:08:20",""]
[593,13253,7,9,"7/47","","7/47","","Type A2 filter fabric blanket with 200mm laps","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 12:32:05",""]
[594,13254,7,9,"7/47"," I","7/47. I","","Under pebble stone covering including preparing ground surface under","m2",29,"","","","","06/12/2021 01:00:18",""]
[595,13262,7,9,"7/47","","7/47","","Core drilling hole not exceeding 50mm diameter","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 01:00:29",""]
[596,13263,7,9,"7/47"," J","7/47. J","","100mm Thick reinforced concrete slab, beam, wall, etc.","No",5,"","","","","08/12/2021 05:08:31",""]
[597,6188,7,9,"7/48","","7/48","","ARTWORK","H2",{"v":0,"d":"0.0"},"","","","","01/10/2012 01:27:50",""]
[598,6299,7,9,"7/48"," A","7/48. A","","Granite boulder of not exceeding 750kg, and placing in position on fill where indicated on site (Allow the prime cost amount of R3 000.00 per boulder for supply to site and artwork by a specialist)","No",9,"","","","","30/10/2021 08:21:10",""]
[600,9466,7,10,"7/50","","7/50","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:40",""]
[601,6096,7,10,"7/50","","7/50","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:17",""]
[602,9467,7,10,"7/50","","7/50","","BILL NO. 10","H1",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:50:51",""]
[603,4854,7,10,"7/50","","7/50","","STORY TELLING PIT","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:48",""]
[604,4855,7,10,"7/50","","7/50","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/09/2012 09:13:58",""]
[605,4856,7,10,"7/50","","7/50","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:51",""]
[606,4857,7,10,"7/50","","7/50","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/09/2012 09:13:58",""]
[607,5641,7,10,"7/50","","7/50","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:00:52",""]
[608,5642,7,10,"7/50","","7/50","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:05:03",""]
[609,4858,7,10,"7/50","","7/50","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","14/09/2012 09:13:58",""]
[610,4859,7,10,"7/50","","7/50","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","14/09/2012 09:13:58",""]
[611,8823,7,10,"7/50","","7/50","","METALWORK","H2",{"v":0,"d":"0.0"},"","","","","23/07/2020 03:49:33",""]
[612,8824,7,10,"7/50"," A","7/50. A","","\"PermaEdge\" 125mm high galvanised spiked garden edging in 1 000mm lengths, bent to shape, and fitted together with integral male and female interlocking ends","m",27,"","","","","27/06/2023 12:10:12",""]
[614,9468,7,11,"7/51","","7/51","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:47",""]
[615,6097,7,11,"7/51","","7/51","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:21",""]
[616,9469,7,11,"7/51","","7/51","","BILL NO. 11","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:56:04",""]
[617,220,7,11,"7/51","","7/51","","WALKWAYS, RAMPS & STEPS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:52",""]
[618,221,7,11,"7/51","","7/51","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:20",""]
[619,222,7,11,"7/51","","7/51","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:37:56",""]
[620,223,7,11,"7/51","","7/51","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:20",""]
[621,5639,7,11,"7/51","","7/51","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:00:46",""]
[622,5640,7,11,"7/51","","7/51","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:05:10",""]
[623,3002,7,11,"7/51","","7/51","","Earthworks are to be executed in accordance with SANS 1200 DM, SANS 1200 D or SANS 1200 DA 1979 \"Earthworks (Small Works)\" as applicable.  Consolidations are to be done at optimum moisture content.  Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","07/08/2012 12:39:47",""]
[624,224,7,11,"7/51","","7/51","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:20",""]
[625,225,7,11,"7/51","","7/51","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/08/2012 12:39:57",""]
[626,13867,7,11,"7/51","","7/51","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 08:58:32",""]
[627,13868,7,11,"7/52","","7/52","","Taking out and set aside for re-use, or handing to the client (Re-use measured elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 08:58:32",""]
[628,13869,7,11,"7/52"," A","7/52. A","","Inter-locking precast concrete pavers (Labour Intensive)","m2",11,"","","","","26/06/2023 10:23:43",""]
[629,4325,7,11,"7/52","","7/52","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","29/08/2012 11:07:48",""]
[630,4326,7,11,"7/52","","7/52","","EXCAVATIONS","H3",{"v":0,"d":"0.0"},"","","","","01/10/2012 12:01:31",""]
[631,4294,7,11,"7/52","","7/52","","Open face excavation in earth over sloping site","H4",{"v":0,"d":"0.0"},"","","","","03/10/2012 11:11:06",""]
[632,4295,7,11,"7/52"," B","7/52. B","","Open face excavation to reduce levels (Labour Intensive)","m3",86,"","","","","26/06/2023 10:52:56",""]
[633,4485,7,11,"7/52","","7/52","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","31/08/2012 01:20:43",""]
[634,4373,7,11,"7/52"," C","7/52. C","","Trenches (Labour Intensive)","m3",7,"","","","","03/11/2021 06:28:47",""]
[635,13870,7,11,"7/52"," D","7/52. D","","Reduced levels under paving (Labour Intensive)","m3",7,"","","","","26/06/2023 10:24:11",""]
[636,4327,7,11,"7/52","","7/52","","Extra over excavations in earth for excavation in","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:36:38",""]
[637,4302,7,11,"7/52"," E","7/52. E","","Soft rock","m3",2,"","","","","28/01/2014 08:09:27",""]
[638,4303,7,11,"7/52"," F","7/52. F","","Hard rock ","m3",1,"","","","","28/01/2014 08:09:31",""]
[639,4305,7,11,"7/52","","7/52","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:20:03",""]
[640,4306,7,11,"7/52"," G","7/52. G","","Surplus material from stock piles on site to a dumping site to be located by the contractor","m3",30,"","","","","26/06/2023 10:53:06",""]
[641,4328,7,11,"7/52","","7/52","","Risk of collapse of excavations","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:20:06",""]
[642,4304,7,11,"7/52"," H","7/52. H","","Allow for risk of collapse to sides of excavations to trenches, etc. to not exceeding 1,5 m deep","m2",12,"","","","","26/06/2023 10:24:24",""]
[643,4331,7,11,"7/52","","7/52","","FILLING, ETC","H3",{"v":0,"d":"0.0"},"","","","","24/10/2012 01:39:00",""]
[644,5268,7,11,"7/52","","7/52","","Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:20:37",""]
[645,4357,7,11,"7/52"," I","7/52. I","","Over site to make up levels (Labour Intensive)","m3",25,"","","","","26/06/2023 10:53:20",""]
[646,4332,7,11,"7/52","","7/52","","Earth filling supplied by the contractor","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:20:09",""]
[647,4565,7,11,"7/52"," J","7/52. J","","Imported G7 selected material under walkways compacted to 93% Mod AASHTO density (Labour Intensive)","m3",3,"","","","","26/06/2023 10:24:30",""]
[648,4340,7,11,"7/53"," A","7/53. A","","Imported G5 subbase selected material under walkways compacted to 95% Mod AASHTO density (Labour Intensive)","m3",140,"","","","","26/06/2023 10:24:34",""]
[649,12645,7,11,"7/53"," B","7/53. B","","Imported G5 subbase selected material under walkways compacted to 98% Mod AASHTO density (Labour Intensive)","m3",13,"","","","","26/06/2023 10:24:38",""]
[650,4566,7,11,"7/53"," C","7/53. C","","Imported G1 base course selected material under walkways compacted to 98% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 10:24:42",""]
[651,12874,7,11,"7/53","","7/53","","Filling of coarse river sand supplied by the contractor, consolidated","H4",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:04:25",""]
[652,12871,7,11,"7/53"," D","7/53. D","","Under precast concrete pavers (Labour Intensive)","m3",10,"","","","","26/06/2023 10:24:49",""]
[653,11149,7,11,"7/53","","7/53","","Selected earth filling obtained from stock piles on site","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 03:55:05",""]
[654,11150,7,11,"7/53"," E","7/53. E","","Filling under floors, well watered and consolidated in layers not exceeding 150 mm thick to obtain 93% modified AASHTO dry density (Labour Intensive)","m3",98,"","","","","26/06/2023 10:24:54",""]
[655,4313,7,11,"7/53","","7/53","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:20:12",""]
[656,10472,7,11,"7/53"," F","7/53. F","","Compaction of ground surface under pavings, etc. including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density (Labour Intensive)","m2",1119,"","","","","26/06/2023 10:25:00",""]
[657,12872,7,11,"7/53","","7/53","","UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:02:07",""]
[658,12873,7,11,"7/53","","7/53","","15MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:03:24",""]
[659,12614,7,11,"7/53"," G","7/53. G","","Blinding (Labour Intensive)","m3",0.4,"","","","","26/06/2023 10:25:08",""]
[660,6419,7,11,"7/53","","7/53","","REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","10/12/2021 09:45:03",""]
[661,6420,7,11,"7/53","","7/53","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:02:01",""]
[662,6444,7,11,"7/53"," H","7/53. H","","Strip footings (Labour Intensive)","m3",2,"","","","","30/10/2021 08:27:31",""]
[663,6846,7,11,"7/53","","7/53","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","10/12/2021 09:44:05",""]
[664,11151,7,11,"7/53","","7/53","","25MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:02:23",""]
[665,11152,7,11,"7/53"," I","7/53. I","","Stairs including landings, beams and inverted beams (Labour Intensive)","m3",5,"","","","","26/06/2023 10:47:25",""]
[666,13871,7,11,"7/54"," A","7/54. A","","Edge restraints (Labour Intensive)","m3",1,"","","","","26/06/2023 09:02:50",""]
[667,6446,7,11,"7/54","","7/54","","30MPa/19mm Pigmented concrete","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 11:46:27",""]
[668,6451,7,11,"7/54","","7/54","","Material:- Allow for a minimum of 1 pigment colour;- Pigment material must be suitable for use to colour concrete and must not affect the strength or durability of the concrete; - The colouring agent shall be a single-component, pigmented admixture of approximately 2%-4% of the cement volume.- Only pigment materials approved by SANS shall be allowed to be used.","",{"v":0,"d":"0.0"},"","","","","08/12/2021 03:30:14",""]
[669,6447,7,11,"7/54"," B","7/54. B","","Walls","m3",7,"","","","","27/02/2014 08:13:14",""]
[670,6448,7,11,"7/54","","7/54","","Smooth formwork to sides (Degree of accuracy II)","H4",{"v":0,"d":"0.0"},"","","","","03/10/2012 12:48:53",""]
[671,6449,7,11,"7/54"," C","7/54. C","","Walls in foundations","m2",8,"","","","","30/10/2021 08:28:12",""]
[672,6450,7,11,"7/54"," D","7/54. D","","Walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level","m2",34,"","","","","30/10/2021 08:28:40",""]
[673,8719,7,11,"7/54"," E","7/54. E","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",102,"","","","","06/12/2021 11:38:37",""]
[674,12612,7,11,"7/54","","7/54","","Boxing in smooth formwork to form","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 11:41:45",""]
[675,12613,7,11,"7/54"," F","7/54. F","","20 x 20mm Chamfers along top or bottom edges","m",11,"","","","","19/11/2021 08:58:34",""]
[676,6425,7,11,"7/54","","7/54","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","03/10/2012 11:29:13",""]
[677,6426,7,11,"7/54"," G","7/54. G","","Surface beds, slabs, etc. (Labour Intensive)","m2",31,"","","","","26/06/2023 10:25:33",""]
[678,12383,7,11,"7/54","","7/54","","SPECIAL CONCRETE","H2",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:01:38",""]
[679,12384,7,11,"7/54","","7/54","","In-situ decorative exposed aggregate 30MPa concrete (19mm screened locally sourced aggregate - colour to match existing walkways), mixed and applied in accordance with the manufacturers specifications (Refer to B10 : Landscape specification)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 11:43:26",""]
[680,12385,7,11,"7/54"," H","7/54. H","","Paving to walkways","m3",65,"","","","","28/06/2023 09:29:09",""]
[681,11117,7,11,"7/54"," I","7/54. I","","Stair treads and risers (Formwork elsewhere)","m3",4.9,"","","","","06/11/2021 02:53:04",""]
[682,12386,7,11,"7/55","","7/55","","Test cubes","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:43:21",""]
[683,12387,7,11,"7/55"," A","7/55. A","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",15,"","","","","06/11/2021 02:43:30",""]
[684,12388,7,11,"7/55","","7/55","","Wire brushing of concrete surfaces to expose aggregate (1-2mm), including surface application of retarding agent","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:43:21",""]
[685,12389,7,11,"7/55"," B","7/55. B","","Top surfaces of paving","m2",188,"","","","","06/11/2021 02:43:33",""]
[686,10448,7,11,"7/55","","7/55","","Saw-cut joints","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 06:29:15",""]
[687,10449,7,11,"7/55"," C","7/55. C","","3 x 50mm Saw-cut joints in top of concrete","m",99,"","","","","30/10/2021 08:29:29",""]
[688,10450,7,11,"7/55"," D","7/55. D","","Ream previously cut/formed expansion joint by increasing the top 25mm to 6mm wide","m",99,"","","","","30/10/2021 08:29:32",""]
[689,8659,7,11,"7/55","","7/55","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","19/01/2020 02:11:20",""]
[690,8701,7,11,"7/55","","7/55","","Mild steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","12/02/2020 03:58:21",""]
[691,8702,7,11,"7/55"," E","7/55. E","","Various diameter bars","t",0.03,"","","","","29/11/2021 03:15:55",""]
[692,8703,7,11,"7/55","","7/55","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","12/02/2020 03:58:45",""]
[693,8704,7,11,"7/55"," F","7/55. F","","Various diameter bars","t",0.59,"","","","","29/11/2021 03:15:42",""]
[694,8660,7,11,"7/55","","7/55","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","19/01/2020 02:11:30",""]
[695,11153,7,11,"7/55"," G","7/55. G","","Type 395 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",672,"","","","","06/12/2021 11:39:29",""]
[696,3003,7,11,"7/55","","7/55","","PRECAST CONCRETE PAVING","H2",{"v":0,"d":"0.0"},"","","","","07/08/2012 12:40:04",""]
[697,5592,7,11,"7/55","","7/55","","Note : Paving is to be laid in accordance with SANS 1200 MJ, SANS 1058 and the Concrete Masonry Association's specifications","",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:40:08",""]
[698,5593,7,11,"7/55","","7/55","","Paving is to be laid on 50mm (thickness after final compaction) clean river sand Class II dry mortar mix (preparation of ground or filling elsewhere)","",{"v":0,"d":"0.0"},"","","","","21/09/2012 04:05:22",""]
[699,5594,7,11,"7/55","","7/55","","Clean sand is to be swept into joints","",{"v":0,"d":"0.0"},"","","","","21/09/2012 04:07:23",""]
[700,5595,7,11,"7/56","","7/56","","The contractor will be required to provide a certificate from a registered pest control company certifying that a weed killer has been applied in accordance with the manufacturer's instructions. (PW371 clause 19.6)","",{"v":0,"d":"0.0"},"","","","","25/09/2012 10:12:18",""]
[701,8646,7,11,"7/56","","7/56","","C.E.L. 200 x 100 x 50mm precast concrete pavers with 9mm exposed aggregate finish suitable for foot traffic including bedding, jointing and pointing (colour : 02 - granite)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:58:41",""]
[702,8647,7,11,"7/56"," A","7/56. A","","On walkways","m2",335,"","","","","06/12/2021 11:39:50",""]
[703,8680,7,11,"7/56"," B","7/56. B","","Circular cutting","m",35,"","","","","03/11/2021 06:26:30",""]
[704,13872,7,11,"7/56","","7/56","","Take from store previously set aside for re-use and re-instate","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 09:06:49",""]
[705,13873,7,11,"7/56"," C","7/56. C","","Inter-locking precast concrete pavers (Labour Intensive)","m2",11,"","","","","26/06/2023 10:26:35",""]
[706,13874,7,11,"7/56"," D","7/56. D","","Fair circular cutting (Labour Intensive)","m",14,"","","","","26/06/2023 10:26:39",""]
[707,4457,7,11,"7/56","","7/56","","Galvanised mild steel corner protectors, stair nosings, expansion joint strips, etc","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:19:49",""]
[708,4458,7,11,"7/56"," E","7/56. E","","55 x 75 x 3mm Thick purpose-made stair nosing, with one leg of angle bedded in mortar under tread paving, and other leg flush against vertical edge of paving","m",10,"","","","","05/10/2012 11:57:26",""]
[709,6013,7,11,"7/56","","7/56","","EDGE RESTRAINTS","H2",{"v":0,"d":"0.0"},"","","","","26/09/2012 02:19:03",""]
[710,8706,7,11,"7/56","","7/56","","Precast concrete finished smooth on exposed surfaces, including bedding, jointing and pointing","H4",{"v":0,"d":"0.0"},"","","","","14/02/2020 08:17:15",""]
[711,11116,7,11,"7/56"," F","7/56. F","","75 x 150mm High kerbs (SANS 927 fig 12) with 200 x 270mm unreinforced 20MPa/19mm concrete haunching continuous at back of, including shallow excavation, backfilling, etc.","m",282,"","","","","10/12/2021 09:48:07",""]
[712,11154,7,11,"7/56"," G","7/56. G","","Ditto, but to radius not exceeding 4m","m",39,"","","","","30/10/2021 08:32:28",""]
[713,11174,7,11,"7/56"," H","7/56. H","","100 x 250mm High kerbs (SANS 927 fig 10) raking adjacent to stairs with 200 x 270mm unreinforced 20MPa/19mm concrete haunching continuous at back of, including shallow excavation, backfilling, etc.","m",25,"","","","","09/12/2021 05:28:34",""]
[714,8707,7,11,"7/56"," I","7/56. I","","150 x 250mm High kerbs (SANS 927 fig 4) with 150 x 150 x 300mm unreinforced 20MPa/19mm concrete haunching continuous at back of, including excavation, backfilling, etc.","m",8,"","","","","06/12/2021 11:40:33",""]
[715,12049,7,11,"7/56"," J","7/56. J","","Fig. 4 kerb 150 x 250mm high","m",235,"","","","","01/11/2021 02:32:46",""]
[716,12050,7,11,"7/57"," A","7/57. A","","Ditto, but to radius not exceeding 4m","m",1,"","","","","01/11/2021 02:32:46",""]
[717,12051,7,11,"7/57"," B","7/57. B","","Ditto, but to radius exceeding 4m","m",54,"","","","","01/11/2021 02:32:46",""]
[718,10441,7,11,"7/57","","7/57","","MOVEMENT JOINTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:26:02",""]
[719,10442,7,11,"7/57","","7/57","","Expansion joints with 12mm closed cell expanded polyethylene between vertical concrete surfaces","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 06:25:41",""]
[720,10443,7,11,"7/57"," C","7/57. C","","Not exceeding 300mm high to edges of surface beds","m",93,"","","","","30/10/2021 08:31:48",""]
[721,10444,7,11,"7/57","","7/57","","SEALING STRIPS, JOINT SEALANTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:26:07",""]
[722,10445,7,11,"7/57","","7/57","","Sikaflex 11 FC, or similar approved, single component sealant with backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:45:21",""]
[723,10447,7,11,"7/57"," D","7/57. D","","6 x 10mm Pointing to expansion joints in floors including raking out joint filler","m",161,"","","","","30/10/2021 08:31:52",""]
[724,10446,7,11,"7/57"," E","7/57. E","","10 x 12mm Pointing to expansion joints in floors including raking out joint filler","m",31,"","","","","30/10/2021 08:31:55",""]
[725,11111,7,11,"7/57","","7/57","","GALVANISED STEEL MINOR WORK","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 12:33:07",""]
[726,11114,7,11,"7/57","","7/57","","Corner and edge protectors hot-dip galvanised after drilling and cutting to required lengths","H4",{"v":0,"d":"0.0"},"","","","","19/06/2023 09:11:26",""]
[727,11115,7,11,"7/57"," F","7/57. F","","100 X 65 X 8mm Angle section tread edge protector in varying lengths with holes for small bolts at approximately 350mm centres (Bolts measured elsewhere)","kg",2260,"","","","","10/02/2022 02:55:17",""]
[728,11112,7,11,"7/57","","7/57","","Hilti HIT-HY170, or similar approved, adhesive anchors with loose nuts including mortices in concrete","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 02:17:10",""]
[729,11113,7,11,"7/57"," G","7/57. G","","M10 x 130mm anchor","No",582,"","","","","30/10/2021 08:32:10",""]
[730,11119,7,11,"7/57","","7/57","","Non-shrink grout","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 02:35:42",""]
[731,11120,7,11,"7/57"," H","7/57. H","","Thin layer of non-shrink grout below angle iron tread nosing and concrete below","m2",18,"","","","","30/10/2021 08:32:16",""]
[733,9470,7,12,"7/59","","7/59","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:51",""]
[734,6098,7,12,"7/59","","7/59","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:27",""]
[735,9471,7,12,"7/59","","7/59","","BILL NO. 12","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:56:08",""]
[736,228,7,12,"7/59","","7/59","","PARKING, PAVING AND ROADS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:57",""]
[737,229,7,12,"7/59","","7/59","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:29",""]
[738,230,7,12,"7/59","","7/59","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:01",""]
[739,231,7,12,"7/59","","7/59","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:29",""]
[740,5643,7,12,"7/59","","7/59","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:01:00",""]
[741,5644,7,12,"7/59","","7/59","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:05:20",""]
[742,1108,7,12,"7/59","","7/59","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","06/10/2012 10:37:20",""]
[743,3680,7,12,"7/59","","7/59","","Testing of material and filling","H4",{"v":0,"d":"0.0"},"","","","","12/08/2012 04:09:47",""]
[744,3681,7,12,"7/59","","7/59","","Descriptions of earth filling, compaction, etc. shall be deemed to include for all necessary testing required in accordance with the SANS 1200 series","",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:30:30",""]
[745,232,7,12,"7/59","","7/59","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:29",""]
[746,233,7,12,"7/59","","7/59","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:29",""]
[747,13838,7,12,"7/60","","7/60","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:14:32",""]
[748,13839,7,12,"7/60","","7/60","","Taking out and set aside for re-use, or handing to the client (Re-use measured elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:14:33",""]
[749,13840,7,12,"7/60"," A","7/60. A","","Bevel-edged full inter-locking precast concrete pavers (Labour Intensive)","m2",32,"","","","","26/06/2023 10:26:46",""]
[750,3598,7,12,"7/60","","7/60","","PARKING, PAVING AND ROADS (On site)","H2",{"v":0,"d":"0.0"},"","","","","30/10/2021 08:33:13",""]
[751,5520,7,12,"7/60","","7/60","","EARTHWORKS","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:34:13",""]
[752,13851,7,12,"7/60","","7/60","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:37:15",""]
[753,13852,7,12,"7/60"," B","7/60. B","","Reduced levels under paving (Labour Intensive)","m3",2,"","","","","26/06/2023 10:26:51",""]
[754,5352,7,12,"7/60","","7/60","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","20/09/2012 11:32:10",""]
[755,5354,7,12,"7/60"," C","7/60. C","","Compaction of ground surfaces under pavings etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density (Labour Intensive)","m2",258,"","","","","26/06/2023 10:26:55",""]
[756,5795,7,12,"7/60","","7/60","","Prescribed density tests on filling","H4",{"v":0,"d":"0.0"},"","","","","25/09/2012 09:58:02",""]
[757,3637,7,12,"7/60"," D","7/60. D","","\"Modified AASHTO Density\" test","No",30,"","","","","01/10/2012 03:39:20",""]
[758,13848,7,12,"7/60","","7/60","","FILLING, ETC.","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:36:12",""]
[759,13849,7,12,"7/60","","7/60","","Filling of natural gravel material G5 supplied by the contractor, compacted to 95% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:36:42",""]
[760,13850,7,12,"7/60"," E","7/60. E","","Under floors, steps, pavings, etc. (Labour Intensive)","m3",2,"","","","","26/06/2023 10:27:01",""]
[761,13853,7,12,"7/60","","7/60","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:38:12",""]
[762,13854,7,12,"7/60","","7/60","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:38:28",""]
[763,13855,7,12,"7/60"," F","7/60. F","","Ramps","m3",4,"","","","","26/06/2023 11:01:14",""]
[764,13856,7,12,"7/60","","7/60","","CONCRETE SUNDRIES","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:39:34",""]
[765,13857,7,12,"7/60","","7/60","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:40:05",""]
[766,13858,7,12,"7/60"," G","7/60. G","","Surface beds, slabs, etc. to falls (Labour Intensive)","m2",12,"","","","","26/06/2023 10:27:11",""]
[767,13859,7,12,"7/61","","7/61","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:40:52",""]
[768,13860,7,12,"7/61","","7/61","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:40:57",""]
[769,13861,7,12,"7/61"," A","7/61. A","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",17,"","","","","26/06/2023 09:22:01",""]
[770,5412,7,12,"7/61","","7/61","","PAVING","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:34:18",""]
[771,5579,7,12,"7/61","","7/61","","Note : Paving is to be laid in accordance with SANS 1200 MJ, SANS 1058 and the Concrete Masonry Association's specifications","",{"v":0,"d":"0.0"},"","","","","21/09/2012 03:40:08",""]
[772,5580,7,12,"7/61","","7/61","","Paving is to be laid on 20mm (thickness after final compaction) clean river sand (preparation of ground or filling elsewhere)","",{"v":0,"d":"0.0"},"","","","","21/09/2012 03:40:09",""]
[773,5581,7,12,"7/61","","7/61","","Clean sand is to be swept into joints between roadstones","",{"v":0,"d":"0.0"},"","","","","21/09/2012 03:40:09",""]
[774,5582,7,12,"7/61","","7/61","","The contractor will be required to provide a certificate from a registered pest control company certifying that a weed killer has been applied in accordance with the manufacturer's instructions. (PW371 clause 19.6)","",{"v":0,"d":"0.0"},"","","","","17/10/2012 09:57:04",""]
[775,8211,7,12,"7/61","","7/61","","Bosun 105 x 210 x 70mm 35Mpa bevel-edged full inter-locking precast concrete pavers with 9mm exposed granite aggregate finish, suitable for foot traffic, cars, vans and small pick-up trucks, including bedding, jointing and pointing (colour : Kalahari)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 02:00:53",""]
[776,8212,7,12,"7/61"," B","7/61. B","","On roadway and parking area (Labour Intensive)","m2",214,"","","","","26/06/2023 10:27:22",""]
[777,9159,7,12,"7/61"," C","7/61. C","","Fair circular cutting (Labour Intensive)","m",30,"","","","","26/06/2023 10:27:26",""]
[778,5770,7,12,"7/61"," D","7/61. D","","200mm Wide border to paving on and including 35mm mortar bed (Labour Intensive)","m",70,"","","","","02/11/2021 08:13:16",""]
[779,13841,7,12,"7/61","","7/61","","Take from store previously set aside for re-use and re-instate","H4",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:15:29",""]
[780,13842,7,12,"7/61"," E","7/61. E","","Bevel-edged full inter-locking precast concrete pavers laid to falls on and including sand bed (Labour Intensive)","m2",1,"","","","","26/06/2023 10:27:37",""]
[781,13843,7,12,"7/61"," F","7/61. F","","Fair circular cutting (Labour Intensive)","m",2,"","","","","26/06/2023 10:27:41",""]
[782,12390,7,12,"7/61","","7/61","","SPECIAL CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:34:35",""]
[783,12391,7,12,"7/62","","7/62","","In-situ decorative exposed aggregate 30MPa concrete (19mm screened locally sourced aggregate - colour to match existing walkways), mixed and applied in accordance with the manufacturers specifications (Refer to B10 : Landscape specification)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 11:43:35",""]
[784,12392,7,12,"7/62"," A","7/62. A","","Paving to walkways, cast against excavated surfaces","m3",101,"","","","","07/12/2021 02:01:09",""]
[785,12393,7,12,"7/62","","7/62","","Test cubes","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:48:27",""]
[786,12394,7,12,"7/62"," B","7/62. B","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",51,"","","","","06/11/2021 02:49:08",""]
[787,12395,7,12,"7/62","","7/62","","Wire brushing of concrete surfaces to expose aggregate (1-2mm), including surface application of retarding agent","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:48:27",""]
[788,12396,7,12,"7/62"," C","7/62. C","","Top surfaces of paving","m2",1015,"","","","","26/06/2023 11:01:40",""]
[789,12415,7,12,"7/62","","7/62","","Saw-cut joints","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 03:17:04",""]
[790,12416,7,12,"7/62"," D","7/62. D","","3 x 50mm Saw-cut joints in top of concrete","m",300,"","","","","06/11/2021 03:17:10",""]
[791,12414,7,12,"7/62","","7/62","","REINFORCEMENT","H3",{"v":0,"d":"0.0"},"","","","","23/06/2023 10:34:38",""]
[792,9185,7,12,"7/62","","7/62","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","07/09/2020 04:07:05",""]
[793,12021,7,12,"7/62"," E","7/62. E","","Type 395 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",1039,"","","","","03/11/2021 06:19:19",""]
[794,5514,7,12,"7/62","","7/62","","CHANNELING, KERBING, EDGING, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:27:55",""]
[795,5536,7,12,"7/62","","7/62","","Kerbing","H3",{"v":0,"d":"0.0"},"","","","","21/09/2012 10:36:56",""]
[796,10777,7,12,"7/62","","7/62","","Precast concrete kerbs (SANS 927) finished smooth on exposed surfaces, including bedding, continuous 150 x 200mm high 20MPa/19mm stone rough-shuttered backing concrete and pointing to all joints, including shallow excavations, backfilling, carting away, etc.","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 11:52:57",""]
[797,10776,7,12,"7/62"," F","7/62. F","","Fig. 4 kerb 150 x 250mm high","m",8,"","","","","26/06/2023 11:02:11",""]
[798,13844,7,12,"7/62"," G","7/62. G","","Ditto, but to radius not exceeding 4m","m",2,"","","","","26/06/2023 11:02:19",""]
[799,1107,7,12,"7/62","","7/62","","ROAD TO RESERVOIRS (Off site)","H2",{"v":0,"d":"0.0"},"","","","","30/10/2021 08:35:29",""]
[800,1110,7,12,"7/63","","7/63","","Site Clearance","H4",{"v":0,"d":"0.0"},"","","","","12/08/2012 05:04:51",""]
[801,1111,7,12,"7/63"," A","7/63. A","","Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc. and trees not exceeding 200mm girth (previously cleared area)","m2",1083,"","","","","08/12/2021 03:43:13",""]
[802,1112,7,12,"7/63","","7/63","","Excavations, filling, base courses, etc.","H4",{"v":0,"d":"0.0"},"","","","","12/08/2012 05:04:56",""]
[803,1113,7,12,"7/63"," B","7/63. B","","Open face excavation to roadbed, etc and deposit excavated material in spoil heaps on site","m3",162,"","","","","30/10/2021 08:35:34",""]
[804,1114,7,12,"7/63","","7/63","","Road bed preparation","H4",{"v":0,"d":"0.0"},"","","","","12/08/2012 05:05:00",""]
[805,1115,7,12,"7/63"," C","7/63. C","","Scarify in-situ road bed surface to a depth of 150 mm and compact to 95% Mod AASTO density at optimum moisture content","m2",1083,"","","","","30/10/2021 08:36:01",""]
[806,1116,7,12,"7/63","","7/63","","Filling","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:33:09",""]
[807,1117,7,12,"7/63"," D","7/63. D","","Over site of G5 material in accordance with SANS 1200 ME,  and compacted to 90% Mod AASHTO density","m3",162,"","","","","06/12/2021 11:41:25",""]
[808,1118,7,12,"7/63","","7/63","","Sundries","H4",{"v":0,"d":"0.0"},"","","","","12/08/2012 05:05:11",""]
[809,1119,7,12,"7/63"," E","7/63. E","","Cart away surplus excavated material to a dumping site to be located by the contractor","m3",162,"","","","","27/02/2014 08:15:31",""]
[811,9472,7,13,"7/65","","7/65","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:55",""]
[812,6100,7,13,"7/65","","7/65","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:31",""]
[813,9473,7,13,"7/65","","7/65","","BILL NO. 13","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:56:12",""]
[814,244,7,13,"7/65","","7/65","","RETAINING WALLS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:03",""]
[815,245,7,13,"7/65","","7/65","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:44",""]
[816,246,7,13,"7/65","","7/65","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:05",""]
[817,247,7,13,"7/65","","7/65","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:44",""]
[818,5647,7,13,"7/65","","7/65","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:01:15",""]
[819,5648,7,13,"7/65","","7/65","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:05:37",""]
[820,249,7,13,"7/65","","7/65","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:44",""]
[821,3756,7,13,"7/65","","7/65","","EXCAVATION, FILLING, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:02:34",""]
[822,248,7,13,"7/65","","7/65","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:44",""]
[823,3757,7,13,"7/65","","7/65","","EXCAVATIONS, ETC.","H3",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:02:42",""]
[824,11025,7,13,"7/65","","7/65","","Excavate in pickable material not exceeding 2m deep below natural or reduced ground level","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:34:13",""]
[825,11026,7,13,"7/65"," A","7/65. A","","Reduce levels under floors, ramps, etc. (Labour Intensive)","m3",11,"","","","","26/06/2023 10:30:41",""]
[826,3758,7,13,"7/66","","7/66","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:42:48",""]
[827,3759,7,13,"7/66"," A","7/66. A","","Trenches (Labour Intensive)","m3",238,"","","","","26/06/2023 10:30:46",""]
[828,3937,7,13,"7/66","","7/66","","Excavation in earth exceeding 2m and not exceeding 4m deep","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:42:51",""]
[829,3938,7,13,"7/66"," B","7/66. B","","Trenches","m3",12,"","","","","27/06/2023 03:27:13",""]
[830,4982,7,13,"7/66","","7/66","","Excavation in earth exceeding 4m and not exceeding 6m deep","H4",{"v":0,"d":"0.0"},"","","","","15/09/2012 06:56:42",""]
[831,4983,7,13,"7/66"," C","7/66. C","","Trenches","m3",5,"","","","","27/06/2023 03:27:44",""]
[832,3760,7,13,"7/66","","7/66","","Extra over trench and hole excavations in earth for excavation in","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:42:48",""]
[833,3761,7,13,"7/66"," D","7/66. D","","Soft rock","m3",29,"","","","","31/10/2021 05:33:04",""]
[834,3762,7,13,"7/66"," E","7/66. E","","Hard rock","m3",23,"","","","","31/10/2021 05:33:10",""]
[835,3763,7,13,"7/66","","7/66","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:42:48",""]
[836,3764,7,13,"7/66"," F","7/66. F","","Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m3",69,"","","","","19/08/2012 06:00:54",""]
[837,3766,7,13,"7/66","","7/66","","Risk of collapse of excavations","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:42:49",""]
[838,3767,7,13,"7/66"," G","7/66. G","","Sides of trench and hole excavations not exceeding 1,5m deep","m2",432,"","","","","31/10/2021 05:33:21",""]
[839,3768,7,13,"7/66"," H","7/66. H","","Sides of trench and hole excavations exceeding 1,5m deep","m2",6,"","","","","27/06/2023 03:28:08",""]
[840,3769,7,13,"7/66","","7/66","","FILLING, ETC.","H3",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:02:56",""]
[841,3875,7,13,"7/66","","7/66","","Approved G6 earth filling supplied by the contractor, compacted to 95% Mod AASHTO density in 150mm layers","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 03:39:22",""]
[842,8198,7,13,"7/66"," I","7/66. I","","Backfilling behind retaining walls","m3",11,"","","","","06/12/2021 11:43:21",""]
[843,8791,7,13,"7/66","","7/66","","Earth filling supplied by the contractor, compacted to 95% Mod AASHTO density in 150mm layers","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:03:51",""]
[844,8792,7,13,"7/66"," J","7/66. J","","Base course of G7 material in accordance with SABS 1200 ME, stabilised to attain UCS>1,0 MPa after seven days","m3",10,"","","","","06/12/2021 11:43:45",""]
[845,3887,7,13,"7/67","","7/67","","Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 98% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 04:23:29",""]
[846,3888,7,13,"7/67"," A","7/67. A","","Backfilling behind retaining walls","m3",106,"","","","","20/08/2012 09:58:40",""]
[847,3889,7,13,"7/67"," B","7/67. B","","Backfilling to trenches, holes, etc.","m3",150,"","","","","24/10/2012 03:53:01",""]
[848,3890,7,13,"7/67","","7/67","","\"Free draining\" coarse filling material obtained from excavations as per engineers specifications","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 03:47:15",""]
[849,3891,7,13,"7/67"," C","7/67. C","","Behind retaining walls","m3",77,"","","","","14/11/2021 03:39:42",""]
[850,3777,7,13,"7/67","","7/67","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:51:46",""]
[851,3778,7,13,"7/67"," D","7/67. D","","Scarify surface of in-situ material for a depth of 150mm and compact to 93% Mod AASHTO density (Labour Intensive)","m2",269,"","","","","26/06/2023 10:31:19",""]
[852,3892,7,13,"7/67","","7/67","","UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","07/04/2021 03:03:05",""]
[853,3893,7,13,"7/67","","7/67","","15MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 03:55:09",""]
[854,3894,7,13,"7/67"," E","7/67. E","","Surface blinding under footings and bases","m3",11,"","","","","31/10/2021 05:34:28",""]
[855,8641,7,13,"7/67","","7/67","","20MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","03/08/2020 09:49:18",""]
[856,8642,7,13,"7/67"," F","7/67. F","","In filling to cavity of hollow wall","m3",4,"","","","","31/10/2021 05:34:39",""]
[857,3782,7,13,"7/67","","7/67","","REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","07/04/2021 03:02:57",""]
[858,9195,7,13,"7/67","","7/67","","20MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","20/11/2020 08:17:04",""]
[859,9196,7,13,"7/67"," G","7/67. G","","Retaining wall footings","m3",27,"","","","","31/10/2021 05:34:48",""]
[860,3783,7,13,"7/67","","7/67","","30MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 03:55:31",""]
[861,7200,7,13,"7/67"," H","7/67. H","","Ground beams","m3",1,"","","","","31/10/2021 05:34:56",""]
[862,7160,7,13,"7/67"," I","7/67. I","","Strip footings","m3",1,"","","","","31/10/2021 05:35:00",""]
[863,4091,7,13,"7/67"," J","7/67. J","","Retaining wall footings","m3",38,"","","","","31/10/2021 05:35:04",""]
[864,4090,7,13,"7/67","","7/67","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","07/04/2021 03:02:48",""]
[865,4092,7,13,"7/68","","7/68","","30MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 03:56:05",""]
[866,3784,7,13,"7/68"," A","7/68. A","","Retaining wall footings","m3",1,"","","","","27/06/2023 03:28:32",""]
[867,3785,7,13,"7/68"," B","7/68. B","","Retaining walls in foundations","m3",9,"","","","","31/10/2021 05:35:21",""]
[868,3786,7,13,"7/68"," C","7/68. C","","Retaining walls","m3",22,"","","","","28/01/2014 08:14:40",""]
[869,6039,7,13,"7/68"," D","7/68. D","","Benches","m3",1,"","","","","27/06/2023 03:28:52",""]
[870,6224,7,13,"7/68"," E","7/68. E","","Steps","m3",5,"","","","","28/01/2014 08:14:49",""]
[871,11027,7,13,"7/68"," F","7/68. F","","Surface beds","m3",8,"","","","","06/12/2021 11:44:09",""]
[872,6847,7,13,"7/68","","7/68","","PIGMENTED CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","05/10/2012 11:48:22",""]
[873,6708,7,13,"7/68","","7/68","","SUPPLEMENTARY PREAMBLES","H3",{"v":0,"d":"0.0"},"","","","","05/10/2012 08:21:02",""]
[874,6484,7,13,"7/68","","7/68","","Material:- Allow for 1 pigment colour;- Pigment material must be suitable for use to colour concrete and must not affect the strength or durability of the concrete; - The colouring agent shall be a single-component, pigmented admixture of approximately 2%-4% of the cement volume.-Only pigment materials approved by SANS shall be allowed to be used.","",{"v":0,"d":"0.0"},"","","","","06/12/2021 08:59:56",""]
[875,6217,7,13,"7/68","","7/68","","30MPa/19mm Pigmented concrete","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 11:49:11",""]
[876,12747,7,13,"7/68"," G","7/68. G","","Retaining walls in foundations","m3",2,"","","","","14/11/2021 05:04:27",""]
[877,6218,7,13,"7/68"," H","7/68. H","","Retaining walls","m3",11,"","","","","27/02/2014 08:16:27",""]
[878,5016,7,13,"7/68","","7/68","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","16/09/2012 07:32:01",""]
[879,5017,7,13,"7/68","","7/68","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","16/09/2012 07:32:01",""]
[880,5266,7,13,"7/68"," I","7/68. I","","Surface beds, slabs, etc.","m2",54,"","","","","09/12/2021 05:35:33",""]
[881,5030,7,13,"7/68"," J","7/68. J","","Tops of beams, walls, etc.","m2",18,"","","","","09/12/2021 05:35:39",""]
[882,3787,7,13,"7/68","","7/68","","TEST CUBES","H2",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:55:16",""]
[883,3788,7,13,"7/68"," K","7/68. K","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",70,"","","","","01/10/2012 02:34:11",""]
[884,3789,7,13,"7/69","","7/69","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:57:00",""]
[885,3791,7,13,"7/69","","7/69","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:57:10",""]
[886,4093,7,13,"7/69"," A","7/69. A","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",31,"","","","","23/08/2012 06:14:27",""]
[887,3790,7,13,"7/69","","7/69","","SMOOTH FORMWORK (DEGREE OF ACCURACY I)","H2",{"v":0,"d":"0.0"},"","","","","07/04/2021 03:02:30",""]
[888,3793,7,13,"7/69","","7/69","","Smooth formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 03:57:23",""]
[889,6228,7,13,"7/69"," B","7/69. B","","Retaining walls with total height not exceeding 3,5m above bearing level","m2",279,"","","","","14/11/2021 03:44:17",""]
[890,6229,7,13,"7/69"," C","7/69. C","","Retaining walls with total height not exceeding 3,5m above bearing level circular to not exceeding 1m radius","m2",5,"","","","","14/11/2021 03:44:34",""]
[891,6230,7,13,"7/69"," D","7/69. D","","Retaining walls with total height not exceeding 3,5m above bearing level circular to exceeding 1m radius","m2",5,"","","","","06/12/2021 05:35:06",""]
[892,6231,7,13,"7/69"," E","7/69. E","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level","m2",75,"","","","","14/11/2021 03:44:52",""]
[893,6232,7,13,"7/69"," F","7/69. F","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level circular to not exceeding 1m radius","m2",5,"","","","","14/11/2021 03:45:06",""]
[894,12748,7,13,"7/69"," G","7/69. G","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level circular to exceeding 1m radius","m2",5,"","","","","08/12/2021 03:44:19",""]
[895,5022,7,13,"7/69","","7/69","","MOVEMENT JOINTS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:04:25",""]
[896,8802,7,13,"7/69","","7/69","","Expansion joints with 12mm closed cell expanded polyethylene between vertical concrete surfaces","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 03:46:14",""]
[897,8803,7,13,"7/69"," H","7/69. H","","Not exceeding 300mm high to edges of surface beds","m",14,"","","","","14/11/2021 03:46:20",""]
[898,5023,7,13,"7/69","","7/69","","Expansion joints with 25mm bitumen impregnated softboard between vertical concrete surfaces, including necessary formwork through","H4",{"v":0,"d":"0.0"},"","","","","15/10/2012 08:57:24",""]
[899,5024,7,13,"7/69"," I","7/69. I","","Walls not exceeding 300mm thick","m",15,"","","","","03/10/2012 04:26:41",""]
[900,13036,7,13,"7/70","","7/70","","Expansion joints with 10mm closed cell expanded polyethylene between vertical concrete surfaces, including necessary formwork","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 07:29:04",""]
[901,13037,7,13,"7/70"," A","7/70. A","","Not exceeding 300mm wide through retaining walls","m",0.2,"","","","","06/12/2021 05:35:25",""]
[902,3803,7,13,"7/70","","7/70","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","13/08/2012 04:06:11",""]
[903,3804,7,13,"7/70","","7/70","","Mild steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 04:06:11",""]
[904,3805,7,13,"7/70"," B","7/70. B","","Various diameter bars","t",2.41,"","","","","14/11/2021 03:47:02",""]
[905,3806,7,13,"7/70","","7/70","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 04:06:11",""]
[906,3807,7,13,"7/70"," C","7/70. C","","Various diameter bars","t",8.89,"","","","","14/11/2021 03:46:48",""]
[907,7177,7,13,"7/70","","7/70","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","12/10/2012 08:23:52",""]
[908,7178,7,13,"7/70"," D","7/70. D","","Type 311 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",71,"","","","","06/12/2021 01:03:27",""]
[909,11039,7,13,"7/70","","7/70","","CONCRETE COPINGS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:04:42",""]
[910,12889,7,13,"7/71","","7/71","","20mm Thick x 300 x 100mm Smooth cement tile to match existing fixed to concrete retaining walls at junction of coping and stone cladding fixed with Tal Goldflex, or similar approved, grey flexible rapid setting high-strength shrinkage-compensated cement-based adhesive, and flush pointed in dove grey grout","H4",{"v":0,"d":"0.0"},"","","","","23/11/2021 03:34:12",""]
[911,12890,7,13,"7/71"," A","7/71. A","","100mm Wide horizontal 'cill' tile bedded on top of stone cladding (cladding measured elsewhere) ","m",192,"","","","","06/12/2021 09:50:10",""]
[912,12971,7,13,"7/71"," B","7/71. B","","100mm High tile to concrete walls","m",2,"","","","","23/11/2021 03:34:40",""]
[913,12972,7,13,"7/71","","7/71","","In-situ concrete copings finished smooth on exposed surfaces, with expansion joints at maximum 1,5m centres, including all concrete, formwork, and finishes","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 02:52:35",""]
[914,12973,7,13,"7/71"," C","7/71. C","","550 x 100mm Thick overall coping, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",44,"","","","","21/06/2023 11:25:31",""]
[915,12976,7,13,"7/71"," D","7/71. D","","550 x 100mm Thick overall coping, circular to not exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",2,"","","","","21/06/2023 11:25:38",""]
[916,12977,7,13,"7/71"," E","7/71. E","","550 x 100mm Thick overall coping, circular to exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",7,"","","","","21/06/2023 11:25:46",""]
[917,12974,7,13,"7/71"," F","7/71. F","","550 x 100mm Thick overall coping, with sloping tops; the coping circular on plan and elevation to not exceeding 1m radius","m",2,"","","","","21/06/2023 11:25:54",""]
[918,12975,7,13,"7/72"," A","7/72. A","","550 x 100mm Thick overall coping, with sloping tops; the coping circular on plan and elevation to exceeding 1m radius","m",2,"","","","","21/06/2023 11:26:03",""]
[919,12978,7,13,"7/72"," B","7/72. B","","500 x 100mm Thick overall coping, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",10,"","","","","21/06/2023 11:26:08",""]
[920,12981,7,13,"7/72"," C","7/72. C","","500 x 100mm Thick overall coping, circular to not exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",2,"","","","","21/06/2023 11:26:14",""]
[921,12982,7,13,"7/72"," D","7/72. D","","500 x 100mm Thick overall coping, circular to exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",2,"","","","","21/06/2023 11:26:21",""]
[922,12979,7,13,"7/72"," E","7/72. E","","500 x 100mm Thick overall coping, with sloping tops; the coping circular on plan and elevation to not exceeding 1m radius","m",2,"","","","","21/06/2023 11:26:29",""]
[923,12980,7,13,"7/72"," F","7/72. F","","500 x 100mm Thick overall coping, with sloping tops; the coping circular on plan and elevation to exceeding 1m radius","m",2,"","","","","21/06/2023 11:26:47",""]
[924,11040,7,13,"7/72","","7/72","","Precast concrete finished smooth on exposed surfaces including bedding on ABE Epidermix epoxy mortar, jointing and pointing with ABE Dura cement grout with TAL keycoat water repellent additive in max. 5mm gaps between units","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 05:06:05",""]
[925,12518,7,13,"7/72"," G","7/72. G","","440 x 100mm Thick overall Modcon, or similar approved, mono pitch coping weathered on top, with concave mortar  joints between units (coping type 021)","m",82,"","","","","20/06/2023 11:41:37",""]
[926,12519,7,13,"7/72"," H","7/72. H","","Ditto, but to radius not exceeding 4m","m",17,"","","","","20/06/2023 11:41:43",""]
[927,12522,7,13,"7/72"," I","7/72. I","","Ditto, but to radius exceeding 4m","m",15,"","","","","20/06/2023 11:41:49",""]
[928,12520,7,13,"7/72"," J","7/72. J","","Extra over for fair returned stopped end","No",4,"","","","","20/06/2023 11:41:56",""]
[929,12521,7,13,"7/72"," K","7/72. K","","Extra over for mitred angle intersection","No",2,"","","","","20/06/2023 11:42:27",""]
[930,11041,7,13,"7/72"," L","7/72. L","","520 x 100mm Thick overall Deranco, or similar approved, mono pitch coping weathered on top, with concave mortar  joints between units","m",18,"","","","","20/06/2023 11:42:14",""]
[931,11042,7,13,"7/72"," M","7/72. M","","Extra over for fair returned stopped end","No",2,"","","","","20/06/2023 11:42:20",""]
[932,11043,7,13,"7/72"," N","7/72. N","","Extra over for mitred angle intersection","No",4,"","","","","20/06/2023 11:42:34",""]
[933,7152,7,13,"7/73","","7/73","","MASONRY","H2",{"v":0,"d":"0.0"},"","","","","10/10/2012 02:17:07",""]
[934,11031,7,13,"7/73","","7/73","","Brickwork of NFP bricks (7 MPa nominal compressive strength) in class II (1:3) cement mortar","H4",{"v":0,"d":"0.0"},"","","","","25/10/2021 04:28:02",""]
[935,11032,7,13,"7/73"," A","7/73. A","","330mm Cavity walls","m2",34,"","","","","06/12/2021 01:04:06",""]
[936,7176,7,13,"7/73","","7/73","","Brickwork of NFX bricks (14 MPa nominal compressive strength) in class 1 mortar","H4",{"v":0,"d":"0.0"},"","","","","12/10/2012 03:16:27",""]
[937,8825,7,13,"7/73"," B","7/73. B","","One brick walls","m2",167,"","","","","30/10/2021 08:37:45",""]
[938,9207,7,13,"7/73"," C","7/73. C","","One brick walls circular on plan","m2",26,"","","","","30/10/2021 08:37:52",""]
[939,7171,7,13,"7/73","","7/73","","Brickwork reinforcement","H4",{"v":0,"d":"0.0"},"","","","","12/10/2012 08:08:24",""]
[940,7172,7,13,"7/73"," D","7/73. D","","75mm Wide reinforcement built in horizontally","m",199,"","","","","06/12/2021 11:45:54",""]
[941,8827,7,13,"7/73"," E","7/73. E","","150mm Wide reinforcement built in horizontally","m",2260,"","","","","06/12/2021 11:46:03",""]
[942,11035,7,13,"7/73","","7/73","","BRICKWORK SUNDRIES","H3",{"v":0,"d":"0.0"},"","","","","25/10/2021 04:33:31",""]
[943,11036,7,13,"7/73"," F","7/73. F","","Closing 110mm cavities of hollow walls vertically with brickwork half brick wide","m",4,"","","","","06/12/2021 05:38:51",""]
[944,5025,7,13,"7/73","","7/73","","SEALING STRIPS, JOINT SEALANTS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:04:59",""]
[945,8804,7,13,"7/73","","7/73","","Polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","08/05/2020 10:15:25",""]
[946,8805,7,13,"7/73"," G","7/73. G","","12 x 10mm Pointing to expansion joints in floors including raking out joint filler","m",14,"","","","","31/10/2021 05:53:03",""]
[947,8634,7,13,"7/73","","7/73","","\"Sikaflex\" polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 07:29:44",""]
[948,8635,7,13,"7/73"," H","7/73. H","","10mm In expansion joints in walls including raking out expansion joint filler as necessary","m",47,"","","","","03/12/2021 07:29:34",""]
[949,4033,7,13,"7/73","","7/73","","STONE CLADDING TO WALLS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:05:21",""]
[950,8213,7,13,"7/73","","7/73","","\"Potgieter gabion\" stone cladding, secured to wall with adhesive and short galvanised hoop iron strips shot pinned to walls","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 12:10:24",""]
[951,8617,7,13,"7/73"," I","7/73. I","","75mm Lining to sides of brick walls","m2",468,"","","","","31/10/2021 05:52:29",""]
[952,3903,7,13,"7/74","","7/74","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 03:14:55",""]
[953,3905,7,13,"7/74","","7/74","","Two coats bitumen emulsion waterproof coating on","H4",{"v":0,"d":"0.0"},"","","","","11/06/2013 08:56:52",""]
[954,3906,7,13,"7/74"," A","7/74. A","","Concrete walls and columns in foundations","m2",44,"","","","","11/06/2013 08:57:40",""]
[955,3904,7,13,"7/74"," B","7/74. B","","Concrete walls, columns and beams","m2",83,"","","","","11/06/2013 08:57:57",""]
[956,8830,7,13,"7/74","","7/74","","PLASTERING","H2",{"v":0,"d":"0.0"},"","","","","03/08/2020 11:40:22",""]
[957,8831,7,13,"7/74","","7/74","","EXTERNAL PLASTER","H3",{"v":0,"d":"0.0"},"","","","","03/08/2020 11:40:31",""]
[958,8832,7,13,"7/74","","7/74","","1:5 Cement plaster 15mm thick on brickwork","H4",{"v":0,"d":"0.0"},"","","","","03/08/2020 11:40:42",""]
[959,8833,7,13,"7/74"," C","7/74. C","","On walls","m2",468,"","","","","31/10/2021 05:47:06",""]
[960,8834,7,13,"7/74"," D","7/74. D","","On narrow widths","m2",1,"","","","","31/10/2021 05:47:00",""]
[961,6238,7,13,"7/74","","7/74","","SUBSOIL DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","02/10/2012 09:38:43",""]
[962,6240,7,13,"7/74"," E","7/74. E","","19mm Crushed stone encasing to pipes","m3",24,"","","","","27/02/2014 08:11:03",""]
[963,6241,7,13,"7/74"," F","7/74. F","","Geofabric filter blanket (PSDK 3.1.3) wrapped around 300 x 300mm stone encasing(elsewhere measured) with 100mm side and end laps, including stitching","m2",291,"","","","","31/10/2021 05:46:40",""]
[964,3897,7,13,"7/74"," G","7/74. G","","Geofabric filter blanket (PSDK 3.1.3) with 100mm side and end laps, including stitching","m2",317,"","","","","31/10/2021 05:46:31",""]
[965,6242,7,13,"7/74"," H","7/74. H","","Fin drain drainage core of HDPe type with a mass 500g/m2, tensile strength of 3kN, and discharge capacity under 50kPa of 0.4l/s/m to walls (PSLE 3.5.1)","m2",120,"","","","","10/12/2021 02:44:16",""]
[966,6243,7,13,"7/74"," I","7/74. I","","100mm  HDPe perforated pipes laid in stone encasing (encasing elsewhere) (PSLE 3.5.2)","m",298,"","","","","10/12/2021 02:44:04",""]
[967,6244,7,13,"7/74","","7/74","","Extra over for","H4",{"v":0,"d":"0.0"},"","","","","02/10/2012 09:38:45",""]
[968,6245,7,13,"7/74"," J","7/74. J","","110mm End cap","No",12,"","","","","02/10/2012 09:38:45",""]
[969,7845,7,13,"7/74","","7/74","","RETAINING STRUCTURES","H2",{"v":0,"d":"0.0"},"","","","","24/07/2020 12:38:55",""]
[970,7846,7,13,"7/74","","7/74","","INTERLOCKING PLANTER BLOCKS","H3",{"v":0,"d":"0.0"},"","","","","24/07/2020 12:39:05",""]
[971,7847,7,13,"7/75","","7/75","","Precast concrete grey interlocking planter blocks finished smooth on exposed surfaces","H4",{"v":0,"d":"0.0"},"","","","","24/07/2020 12:39:14",""]
[972,7848,7,13,"7/75"," A","7/75. A","","Retaining structures with stepped face and curves as required to suit slopes, of 335 x 295 x 200mm high interlocking planter blocks laid with horizontal bed joints to 60 degree slope, including average 300mm thick compacted earth filling behind the blocks and filling blocks with garden soil lightly tamped as the work proceeds (to match existing)","m2",26,"","","","","29/11/2021 02:41:11",""]
[973,13023,7,13,"7/75","","7/75","","GALVANISED METALWORK","H2",{"v":0,"d":"0.0"},"","","","","02/12/2021 03:12:05",""]
[974,13024,7,13,"7/75","","7/75","","Bolted to concrete","H4",{"v":0,"d":"0.0"},"","","","","02/12/2021 03:13:48",""]
[975,13025,7,13,"7/75"," B","7/75. B","","40 x 40 x 3mm Angle section","kg",37,"","","","","06/12/2021 01:22:25",""]
[976,13033,7,13,"7/75"," C","7/75. C","","40 x 40 x 3mm Angle section with 100 x 30 x 3mm fishtail lugs embedded in concrete","kg",39,"","","","","06/12/2021 01:22:30",""]
[977,13028,7,13,"7/75"," D","7/75. D","","70 x 70 x 6mm Angle section","kg",319,"","","","","06/12/2021 01:22:34",""]
[978,13026,7,13,"7/75","","7/75","","BOLTS, FASTENERS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:06:41",""]
[979,13027,7,13,"7/75"," E","7/75. E","","M8 Expansion bolt 80mm long","No",167,"","","","","06/12/2021 01:22:57",""]
[981,9474,7,14,"7/77","","7/77","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:19:59",""]
[982,6103,7,14,"7/77","","7/77","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:35",""]
[983,9475,7,14,"7/77","","7/77","","BILL NO. 14","H1",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:50:47",""]
[984,252,7,14,"7/77","","7/77","","BOUNDARY WALLING AND SECURITY FENCING","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:11",""]
[985,253,7,14,"7/77","","7/77","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:54",""]
[986,254,7,14,"7/77","","7/77","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:10",""]
[987,255,7,14,"7/77","","7/77","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:54",""]
[988,5651,7,14,"7/77","","7/77","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:01:31",""]
[989,5652,7,14,"7/77","","7/77","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:05:59",""]
[990,256,7,14,"7/77","","7/77","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:54",""]
[991,257,7,14,"7/77","","7/77","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:30:54",""]
[992,7610,7,14,"7/77","","7/77","","FENCING","H2",{"v":0,"d":"0.0"},"","","","","15/11/2012 05:11:46",""]
[993,3043,7,14,"7/77","","7/77","","Note : Fencing to be erected to conform to all Occupational Health & Safety Act requirements, including appropriate signage.","",{"v":0,"d":"0.0"},"","","","","07/08/2012 12:41:37",""]
[994,3056,7,14,"7/78","","7/78","","Site clearance and demolitions","H4",{"v":0,"d":"0.0"},"","","","","15/11/2012 05:08:20",""]
[995,7609,7,14,"7/78"," A","7/78. A","","Allow for clearing site for the width of 1000mm where fencing runs are to be erected including removing trees, shrubs etc. not exceeding 200 mm girth, grubbing up roots and roughly levelling (Labour Intensive) ","m",337,"","","","","09/12/2021 05:39:42",""]
[996,3059,7,14,"7/78"," B","7/78. B","","Excavate in earth and fill adjacent portion to make up levels under fence line","m3",36,"","","","","28/01/2014 08:18:13",""]
[997,3042,7,14,"7/78","","7/78","","TEMPORARY FENCING","H2",{"v":0,"d":"0.0"},"","","","","07/08/2012 12:41:37",""]
[998,7596,7,14,"7/78","","7/78","","300 x 300mm Temporary PVC signs fixed to metal fencing, with vinyl lettering as described, and later remove","H4",{"v":0,"d":"0.0"},"","","","","15/11/2012 03:25:44",""]
[999,7597,7,14,"7/78"," C","7/78. C","","\"No unauthorised entry\"","No",50,"","","","","15/11/2012 03:24:25",""]
[1000,7598,7,14,"7/78"," D","7/78. D","","\"All visitors to report to site office\"","No",5,"","","","","15/11/2012 03:24:50",""]
[1001,7599,7,14,"7/78"," E","7/78. E","","\"Caution : Deep excavations\"","No",18,"","","","","15/11/2012 03:25:12",""]
[1002,3060,7,14,"7/78","","7/78","","PROPRIETARY METAL FENCING","H2",{"v":0,"d":"0.0"},"","","","","26/10/2012 12:36:46",""]
[1003,3061,7,14,"7/78","","7/78","","\"Clearvue\" Reinforced high density anti-climbing and anti-cut pressed mesh panel fencing, formed of 3mm diameter horizontal and 4mm diameter vertical high tensile wires galvanised with marine fusion bond coating (colour medium grey) with aperture size 76,2 x 12,7mm and reinforcing v-section ribs, all bolted with vandal resistant bolts and clamping plates to 85 - 45mm taper locking post 3,0m high including locking recess mechanism at centres as indicated with sealed end caps and 30 x 3 x 250mm long angle section base anchors with posts bedded in 15mpa concrete bases size 400 x 400 x 600mm deep","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:40:23",""]
[1004,3062,7,14,"7/78","","7/78","","Note : The fence to have a 10 year manufacturer-issued guarantee, issued after completion of the work","",{"v":0,"d":"0.0"},"","","","","26/10/2012 12:37:13",""]
[1005,3063,7,14,"7/78"," F","7/78. F","","Security fencing 2 400mm high, in 3 300mm long panels, including all intermediate posts, bases, fixing mechanisms, etc.","m",95,"","","","","09/12/2021 05:41:12",""]
[1006,3859,7,14,"7/78"," G","7/78. G","","600mm High bitumen-coated under-dig, of fencing material as specified, to above fencing, including all fixations, trenches, backfilling, etc.","m",95,"","","","","31/10/2021 05:54:54",""]
[1007,3412,7,14,"7/79"," A","7/79. A","","100mm High marine fusion-bonded coated shark-tooth security spikes fixed to top of fencing at 150mm centres with anti-vandal bolts (as per manufacturers specification)","m",119,"","","","","31/10/2021 05:55:01",""]
[1008,3064,7,14,"7/79"," B","7/79. B","","Extra over fencing as described above for approximately 80 degree internal intersection","No",2,"","","","","31/10/2021 05:55:09",""]
[1009,3065,7,14,"7/79"," C","7/79. C","","Extra over fencing as described above for end post (Labour Intensive)","No",4,"","","","","28/10/2021 11:09:38",""]
[1010,3826,7,14,"7/79"," D","7/79. D","","Security fencing 2 400mm high in 1 223mm panels, and fixing to brick piers (piers elsewhere) (Labour Intensive)","No",1,"","","","","28/10/2021 11:11:01",""]
[1011,3830,7,14,"7/79"," E","7/79. E","","Security fencing 2 400mm high in 1 356mm panels, and fixing to brick piers (piers elsewhere) (Labour Intensive)","No",1,"","","","","28/10/2021 11:11:09",""]
[1012,3831,7,14,"7/79"," F","7/79. F","","Security fencing 2 400mm high in 1 483mm panels, and fixing to brick piers (piers elsewhere) (Labour Intensive)","No",1,"","","","","28/10/2021 11:11:15",""]
[1013,3832,7,14,"7/79"," G","7/79. G","","Security fencing 2 400mm high in 1 561mm panels, and fixing to brick piers (piers elsewhere) (Labour Intensive)","No",1,"","","","","28/10/2021 11:11:21",""]
[1014,3829,7,14,"7/79"," H","7/79. H","","Security fencing 2 400mm high in 1 737mm panels, and fixing to brick piers (piers elsewhere) (Labour Intensive)","No",1,"","","","","28/10/2021 11:11:27",""]
[1015,3833,7,14,"7/79"," I","7/79. I","","Security fencing 2 400mm high in 3 297mm panels, and fixing to brick piers (piers elsewhere) (Labour Intensive)","No",5,"","","","","28/10/2021 11:11:34",""]
[1016,13862,7,14,"7/79"," J","7/79. J","","50mm Insurance graded brass padlock","No",3,"","","","","23/06/2023 10:45:48",""]
[1017,3413,7,14,"7/79","","7/79","","Gates","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 09:57:51",""]
[1018,3415,7,14,"7/79"," K","7/79. K","","Extra over fencing as described above for single pedestrian gate size 1 052 x 2 400mm high overall, complete including gateposts, bases, mesh covering, locking mechanisms, all in accordance with details on drawing 25116-GEN-101a (Gate Type B)","No",5,"","","","","28/10/2021 11:11:45",""]
[1019,3414,7,14,"7/79"," L","7/79. L","","Extra over fencing as described above for double vehicular gate size 3 330 x 2 400mm high overall, complete including gateposts, bases, mesh covering, locking mechanisms, all in accordance with details on drawing 25116-GEN-101a (Gate Type A)","No",2,"","","","","28/10/2021 11:11:50",""]
[1020,13863,7,14,"7/79"," M","7/79. M","","Double vehicular gate size 4 295 x 2 400mm high overall (Prime cost R18 000.00), complete including gateposts, bases, mesh covering and locking mechanisms","No",2,"","","","","26/06/2023 08:18:49",""]
[1021,3416,7,14,"7/80"," A","7/80. A","","Extra over fencing as described above for single sliding gate size 2 150 x 2 476mm high overall, complete including gateposts, bases, mesh covering, locking mechanisms, sliding tracks, stops, all in accordance with details on drawing 25116-GEN-101a (Gate Type C) (Motor elsewhere measured)","No",1,"","","","","28/10/2021 11:12:05",""]
[1022,1098,7,14,"7/80","","7/80","","PRECAST CONCRETE FENCING","H2",{"v":0,"d":"0.0"},"","","","","05/06/2012 11:37:07",""]
[1023,1099,7,14,"7/80","","7/80","","Precast concrete security fence with standards, posts, stays, gates, etc including galvanised steel bolts, straining eye bolts, etc, site clearance and preparation of ground (refer to detail on drawing C5593-SITE-WAT-40)","H4",{"v":0,"d":"0.0"},"","","","","28/10/2021 11:39:48",""]
[1024,1100,7,14,"7/80"," B","7/80. B","","Security fence 2,4m high vertically of 100 x 100mm precast concrete posts (CKS 451) embedded in and including 400 x 400 x 900mm deep 15MPa/19mm stone concrete base at maximum 3m centres; the posts with 450mm long overhang to one side, and fitted with 3 strands of single strand HT 2,6 x 2,0mm fully galvanised barbed wire (SANS 675), and 5 strands of 4mm PVC covered straining wire tied to standards, posts and eye bolts and the vertical height (2,4m) covered with 50 x 25 x 2,5mm Class A Carbon hardened welded mesh tied at 300mm centres to each straining wire, with the bottom of the mesh fixed to the ground with and including 10mm diameter x 300mm long galvanised mild steel pins at 900mm centres (Labour Intensive)","m",154,"","","","","28/10/2021 11:40:24",""]
[1025,1101,7,14,"7/80"," C","7/80. C","","Extra over for 150 x 150mm straining or corner post with 450mm long overhang, including 650 x 650 x 940mm 15Mpa/19mm stone concrete base (Labour Intensive)","No",7,"","","","","28/10/2021 10:22:47",""]
[1026,1102,7,14,"7/80"," D","7/80. D","","50mm Diameter x 2,8mm wall thickness galvanised inclined stay 3 185mm long with top end flattened and bolted to posts with and including 12mm diameter galvanised bolts and other end fitted with 150 x 150 x 6mm mild steel baseplate welded on and embedded in 700 x 700 x 450mm deep 15MPa/19mm stone concrete base (Labour Intensive)","No",14,"","","","","28/10/2021 10:24:13",""]
[1027,1122,7,14,"7/80"," E","7/80. E","","50mm Diameter x 2,8mm wall thickness galvanised inclined stay 3 800mm long with top end flattened and bolted to posts with and including 12mm diameter galvanised bolts and other end fitted with 150 x 150 x 6mm mild steel baseplate welded on and embedded in 700 x 700 x 450mm deep 15MPa/19mm stone concrete base (Labour Intensive)","No",2,"","","","","28/10/2021 10:24:26",""]
[1028,1106,7,14,"7/80"," F","7/80. F","","Gate post formed of 40kg/m x 3 500mm long rail (wire brushed and coated with two coats Colgalv paint), embedded in and including 650 x 650 x 900mm deep 15MPa/19mm stone concrete base; the post eight times holed for fixing wires (Labour Intensive)","No",2,"","","","","28/10/2021 11:40:55",""]
[1029,1103,7,14,"7/81"," A","7/81. A","","12mm Galvanised straining eye bolt 230mm girth bolted through posts with eye of bolt welded closed","No",384,"","","","","27/02/2014 08:20:26",""]
[1030,1105,7,14,"7/81"," B","7/81. B","","Double vehicle gate size 4 000 x 2 700mm high formed in two equal leaves, each leaf formed of 50mm diameter x 2,2mm wall thickness tubular section framing and one raking brace scribed and welded at all intersections and covered with 50 x 25 x 2,5mm galvanised Class A carbon hardened welded mesh 2 400mm high fixed with binding wire to two 4mm galvanised straining wires and the top fitted with three strands of barbed wire; the gate fitted with four M24 eyebolt hinges, stops and one locking mechanism","No",1,"","","","","28/10/2021 10:25:04",""]
[1031,1104,7,14,"7/81"," C","7/81. C","","50mm Insurance graded brass weatherproof padlock","No",1,"","","","","06/12/2021 11:47:23",""]
[1032,3690,7,14,"7/81","","7/81","","BOUNDARY WALL (FENCE TYPE B)","H2",{"v":0,"d":"0.0"},"","","","","13/08/2012 11:05:56",""]
[1033,3696,7,14,"7/81","","7/81","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 12:11:10",""]
[1034,3697,7,14,"7/81"," D","7/81. D","","Surface trenches (Labour Intensive)","m3",24,"","","","","28/10/2021 11:39:18",""]
[1035,3699,7,14,"7/81"," E","7/81. E","","Holes (Labour Intensive)","m3",15,"","","","","06/12/2021 11:47:40",""]
[1036,3702,7,14,"7/81"," F","7/81. F","","Extra over all excavations for carting away surplus material from the excavations and/or stock piles on site to an approved dumping site to be located by the contractor","m3",18,"","","","","28/01/2014 08:19:37",""]
[1037,3703,7,14,"7/81"," G","7/81. G","","Risk of collapse of sides of trench and hole excavations not exceeding 1,5m deep","m2",130,"","","","","06/12/2021 11:48:46",""]
[1038,5511,7,14,"7/81","","7/81","","Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 93% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 09:56:12",""]
[1039,5512,7,14,"7/81"," H","7/81. H","","Backfilling to trenches (Labour Intensive)","m3",15,"","","","","06/12/2021 11:49:00",""]
[1040,3710,7,14,"7/81","","7/81","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 12:11:11",""]
[1041,3711,7,14,"7/81"," I","7/81. I","","Compaction of ground surface under floors etc including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density (Labour Intensive)","m2",12,"","","","","28/10/2021 11:38:46",""]
[1042,3719,7,14,"7/81","","7/81","","CONCRETE, FORMWORK AND REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 09:56:38",""]
[1043,9191,7,14,"7/81","","7/81","","UNREINFORCED CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","10/09/2020 09:41:26",""]
[1044,9192,7,14,"7/82","","7/82","","15MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","10/09/2020 09:41:06",""]
[1045,9193,7,14,"7/82"," A","7/82. A","","Surface blinding under footings and bases","m3",1,"","","","","06/12/2021 11:49:30",""]
[1046,3720,7,14,"7/82","","7/82","","REINFORCED CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","13/08/2012 12:41:29",""]
[1047,3721,7,14,"7/82","","7/82","","25MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 11:55:51",""]
[1048,3722,7,14,"7/82"," B","7/82. B","","In foundations cast against excavated surfaces","m3",7,"","","","","06/12/2021 11:49:39",""]
[1049,3746,7,14,"7/82"," C","7/82. C","","In Bases","m3",3,"","","","","06/12/2021 11:49:47",""]
[1050,3725,7,14,"7/82"," D","7/82. D","","In filling to hollow brick piers","m3",2,"","","","","06/12/2021 11:49:56",""]
[1051,3727,7,14,"7/82","","7/82","","REINFORCEMENT","H3",{"v":0,"d":"0.0"},"","","","","13/08/2012 12:48:14",""]
[1052,3728,7,14,"7/82","","7/82","","Mild steel reinforcement","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 12:48:14",""]
[1053,3882,7,14,"7/82"," E","7/82. E","","Various diameter bars","t",0.14,"","","","","30/10/2021 08:39:07",""]
[1054,3730,7,14,"7/82","","7/82","","High tensile steel reinforcement","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 12:48:15",""]
[1055,3880,7,14,"7/82"," F","7/82. F","","Various diameter bars","t",0.43,"","","","","30/10/2021 08:39:15",""]
[1056,3734,7,14,"7/82","","7/82","","MASONRY","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 09:56:49",""]
[1057,3736,7,14,"7/82","","7/82","","Brickwork of NFPE bricks (7 MPa nominal compressive strength) in class II (1:3) cement mortar","H4",{"v":0,"d":"0.0"},"","","","","02/10/2012 10:10:49",""]
[1058,3739,7,14,"7/82"," G","7/82. G","","Half brick wall in forming hollow piers (Concrete filling elsewhere measured) (Labour Intensive)","m2",43,"","","","","06/12/2021 11:50:15",""]
[1059,3740,7,14,"7/82"," H","7/82. H","","One brick walls (Labour Intensive)","m2",38,"","","","","06/12/2021 11:50:41",""]
[1060,3747,7,14,"7/82","","7/82","","Brickwork sundries","H4",{"v":0,"d":"0.0"},"","","","","01/10/2012 04:30:23",""]
[1061,3773,7,14,"7/82"," I","7/82. I","","Rake out mortar to every fourth perpend to form weephole to one brick wall (Labour Intensive)","m",40,"","","","","28/10/2021 11:34:02",""]
[1062,3808,7,14,"7/82","","7/82","","In-situ concrete coping with smooth wood float finish including bedding and pointing","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 09:56:55",""]
[1063,5542,7,14,"7/82"," J","7/82. J","","330mm Wide x 54/60mm thick coping top on brick wall (Labour Intensive)","m",57,"","","","","06/12/2021 11:53:02",""]
[1064,3809,7,14,"7/82"," K","7/82. K","","550 x 550 x 100/110mm Thick coping top on brick column (Labour Intensive)","No",8,"","","","","26/06/2023 08:21:20",""]
[1065,3748,7,14,"7/83","","7/83","","Brickwork reinforcement","H4",{"v":0,"d":"0.0"},"","","","","13/08/2012 02:44:44",""]
[1066,3750,7,14,"7/83"," A","7/83. A","","150mm Wide reinforcement built in horizontally (Labour Intensive)","m",671,"","","","","26/06/2023 08:21:30",""]
[1067,8851,7,14,"7/83","","7/83","","PLASTERING","H2",{"v":0,"d":"0.0"},"","","","","05/08/2020 11:15:06",""]
[1068,8853,7,14,"7/83","","7/83","","One coat 1:5 cement plaster, on brickwork","H4",{"v":0,"d":"0.0"},"","","","","05/08/2020 11:15:26",""]
[1069,8854,7,14,"7/83"," B","7/83. B","","Walls","m2",60,"","","","","30/10/2021 08:39:36",""]
[1070,5566,7,14,"7/83","","7/83","","SPECIALISED PLASTER TYPE WALL COATINGS","H2",{"v":0,"d":"0.0"},"","","","","21/09/2012 12:20:53",""]
[1071,5567,7,14,"7/83","","7/83","","All specialised plaster type wall coatings are to be executed in strict accordance with the manufacturer's instructions and by registered applicators","",{"v":0,"d":"0.0"},"","","","","02/10/2012 11:29:58",""]
[1072,7542,7,14,"7/83","","7/83","","Intermediate texture rough-cast plaster (1 part cement/1,5 parts coarse sand), with bonding liquid additive (10% of water volume), applied with a Terylene application machine","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:43:13",""]
[1073,3755,7,14,"7/83"," C","7/83. C","","On walls","m2",41,"","","","","06/12/2021 11:53:52",""]
[1074,3837,7,14,"7/83"," D","7/83. D","","On narrow widths not exceeding 300mm wide","m2",9,"","","","","06/12/2021 11:54:06",""]
[1075,3752,7,14,"7/83"," E","7/83. E","","On projecting and isolated piers","m2",39,"","","","","06/12/2021 11:55:02",""]
[1077,9476,7,15,"7/85","","7/85","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:02",""]
[1078,6104,7,15,"7/85","","7/85","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:40",""]
[1079,9477,7,15,"7/85","","7/85","","BILL NO. 15","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:56:20",""]
[1080,11044,7,15,"7/85","","7/85","","LITTER BINS, BOLLARDS, BENCHES, ETC","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:20",""]
[1081,5655,7,15,"7/85","","7/85","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:02:21",""]
[1082,5656,7,15,"7/85","","7/85","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:15",""]
[1083,13919,7,15,"7/85","","7/85","","LITTER BINS, BOLLARDS, BENCHES, ETC","H2",{"v":0,"d":"0.0"},"","","","","28/06/2023 12:28:44",""]
[1084,3437,7,15,"7/85"," A","7/85. A","","Bollard formed of 219mm diameter x 6mm wall thickness x 1 300mm long galvanised mild steel tube approximately 150 times perforated with 10mm diameter holes(for aesthetic purposes); the tube bedded in and including 550mm diameter x 400mm thick 25Mpa unreinforced concrete base, including all excavations, backfilling, etc. (Refer to drawing GEN-104)","No",27,"","","","","28/10/2021 09:53:12",""]
[1085,7567,7,15,"7/85"," B","7/85. B","","130 x 130 x 800mm \"Corolla Bollard\" with aluminium pole and body, glass diffuser, aluminium reflector, silicone gasket and stainless steel screws (Refer to drawing GEN-100) (Concrete base elsewhere)","No",10,"","","","","28/10/2021 09:54:23",""]
[1086,7568,7,15,"7/85"," C","7/85. C","","330 x 330 x 245mm High 25Mpa unreinforced concrete bollard base finished smooth off the mould with chamfered top edges, including short sleeves, excavations, formwork, backfilling, etc. (Refer to drawing GEN-100)","No",10,"","","","","28/10/2021 09:55:19",""]
[1087,7569,7,15,"7/85"," D","7/85. D","","180 x 180 x 5mm Thick galvanised mild steel four times holed bollard gusset plate, fixed to concrete base with and including 4No. 10mm diameter x 100mm long stainless steel masonry expansion bolts","No",10,"","","","","28/10/2021 09:55:45",""]
[1088,12303,7,15,"7/85"," E","7/85. E","","Purpose-made galvanised mild steel litter bin size 530mm triangular on plan x 1 174mm high overall with integral basket, support framework and support posts to match Rizel Engineering Services bins on site (concrete bases elsewhere), (Refer to drawing GEN-103)","No",96,"","","","","08/12/2021 03:51:44",""]
[1089,11204,7,15,"7/86"," A","7/86. A","","Remove minor surface rust, prepare and apply three coats spray-on Everbrite clear matt sealant on general surfaces of litter bins (in-and outside)","m2",332,"","","","","28/06/2023 03:02:10",""]
[1090,11046,7,15,"7/86"," B","7/86. B","","1 000 x 400 x 400mm High 25Mpa unreinforced concrete waste bin base finished smooth off the mould with chamfered top edges, including all excavations, formwork, backfilling, etc. (Refer to drawing GEN-103)","No",96,"","","","","08/12/2021 04:07:37",""]
[1091,11055,7,15,"7/86"," C","7/86. C","","Purpose-made \"FLAT\" \"metal lightbox sign\" size 900 x 1 618mm high overall, complete including supports, cladding and finishes; as per detail on drawing GEN-102 (Electrical supply, light fittings, concrete base, and laser-cutting of artwork into plate measured elsewhere)","No",38,"","","","","28/10/2021 09:57:49",""]
[1092,11047,7,15,"7/86"," D","7/86. D","","2 000 x 2 000 x 425mm Thick 25Mpa unreinforced concrete signage base finished smooth off the mould with chamfered top edges, on and including 200mm thick G5 filling compacted to 95% Mod AASHTO, including all shallow excavations, formwork, backfilling, etc. (Refer to drawing GEN-102)","No",38,"","","","","08/12/2021 03:58:00",""]
[1093,11062,7,15,"7/86"," E","7/86. E","","Purpose-made \"L-SHAPED\" \"metal lightbox sign\" size 1 212 x 1 000 x 2 243mm high overall, complete including supports, cladding and finishes; as per detail on drawing GEN-102 (Electrical supply, light fittings, concrete base, and laser-cutting of artwork into plate measured elsewhere)","No",2,"","","","","27/10/2021 05:50:13",""]
[1094,11048,7,15,"7/86"," F","7/86. F","","2 000 x 2 000 x 425mm Thick 25Mpa unreinforced concrete signage base finished smooth off the mould with chamfered top edges, on and including 200mm thick G5 filling compacted to 95% Mod AASHTO, including all shallow excavations, formwork, backfilling, etc.","No",2,"","","","","15/11/2021 03:52:43",""]
[1095,4197,7,15,"7/86"," G","7/86. G","","Exposed aggregate precast tower drinking fountain Prime Cost R8 000.00 (Eight Thousand Rand) delivered to site, installed according to manufacturer's specifications (tap, pipes and fitting measured elsewhere)","No",7,"","","","","05/11/2021 11:52:07",""]
[1096,7158,7,15,"7/86"," H","7/86. H","","15mm BSP Brass drinking fountain pillar cock with adjustable nozzle flow control (code : 109) Prime Cost R500.00 (Five Hundred Rand)","No",7,"","","","","09/12/2021 05:45:10",""]
[1097,12023,7,15,"7/86"," I","7/86. I","","Garantia 600L Eco King green, or similar approved,  composter, fully assembled and placed in position","No",9,"","","","","29/10/2021 08:21:44",""]
[1098,3443,7,15,"7/86","","7/86","","THE FOLLOWING IN CANTILEVER PRECAST CONCRETE BENCHES","",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:57:11",""]
[1099,5676,7,15,"7/87","","7/87","","Note : All moulds to be min. 5mm thick steel, and concrete to be wet-cast in one pour. Exposed edges to be 45-degree 20mm wide chamfered","",{"v":0,"d":"0.0"},"","","","","28/10/2021 10:01:15",""]
[1100,11051,7,15,"7/87","","7/87","","30MPa Precast concrete (85kg/m3 reinforcement, Class 1 formwork with 7mm stone and fine grit) left smooth from the mould including metal leaf imprints at the rate of 3 per 1 500mm (see drawing MUS-103), bedding, jointing and pointing, all in accordance with details on drawing GEN-100","H4",{"v":0,"d":"0.0"},"","","","","15/11/2021 12:48:15",""]
[1101,6031,7,15,"7/87"," A","7/87. A","","75mm Thick L-shaped on elevation bench, 600mm wide x 2 285mm length on plan, including all off-the-mould finishes, and reinforcement as necessary (concrete base, and fixations to supports measured elsewhere)","No",16,"","","","","28/10/2021 10:02:34",""]
[1102,3867,7,15,"7/87"," B","7/87. B","","100mm Thick L-shaped on elevation bench, 600mm wide x 5 860mm length on plan, including all off-the-mould finishes, and reinforcement as necessary (concrete base, and fixations to supports measured elsewhere)","No",2,"","","","","28/10/2021 10:02:45",""]
[1103,13279,7,15,"7/87","","7/87","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:11:06",""]
[1104,13280,7,15,"7/87"," C","7/87. C","","Bases (Labour Intensive)","m3",10,"","","","","26/06/2023 10:55:13",""]
[1105,13281,7,15,"7/87","","7/87","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:11:06",""]
[1106,13282,7,15,"7/87"," D","7/87. D","","Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor (Labour Intensive)","m3",10,"","","","","26/06/2023 10:55:18",""]
[1107,5678,7,15,"7/87","","7/87","","Bases","H4",{"v":0,"d":"0.0"},"","","","","22/09/2012 11:12:12",""]
[1108,5679,7,15,"7/87"," E","7/87. E","","25Mpa unreinforced concrete in bases cast against excavated surfaces (Labour Intensive)","m3",10,"","","","","26/06/2023 10:55:23",""]
[1109,5677,7,15,"7/87","","7/87","","Supports, including mortices in concrete or stone","H4",{"v":0,"d":"0.0"},"","","","","28/10/2021 10:03:11",""]
[1110,11053,7,15,"7/87"," F","7/87. F","","50 x 50 x 3mm Galvanised mild steel angle section bench supports fixed to underside of bench with and including 6mm diameter x 40mm long dowels construction silicone-fixed","kg",358,"","","","","28/10/2021 10:03:37",""]
[1111,3445,7,15,"7/87"," G","7/87. G","","10mm Diameter x 150mm long galvanised mild steel support rod with one end epoxy grouted into bottom of bench and other end into top of supporting rock below","No",36,"","","","","28/10/2021 10:04:00",""]
[1112,3446,7,15,"7/87"," H","7/87. H","","10mm Diameter x 200mm long galvanised mild steel support rod with one end epoxy grouted into bottom of bench and other end into top of supporting rock below","No",36,"","","","","28/10/2021 10:04:21",""]
[1113,3447,7,15,"7/88"," A","7/88. A","","10mm Diameter x 300mm long galvanised mild steel support rod with one end epoxy grouted into bottom of bench and other end into top of supporting rock below","No",36,"","","","","28/10/2021 10:04:37",""]
[1114,5674,7,15,"7/88","","7/88","","Natural stone from the area","H4",{"v":0,"d":"0.0"},"","","","","22/09/2012 10:54:47",""]
[1115,13737,7,15,"7/88"," B","7/88. B","","Allow the sum of R25 000.00 (Twenty Five Thousand) excl VAT for the location and placement of natural stones from the area, to be measured and valued in terms of these bills of quantities","Item",{"v":1,"d":"1.00"},{"v":25000,"d":"25000.00"},{"v":25000,"d":"25000.00"},"","","15/03/2023 08:53:39",""]
[1116,3444,7,15,"7/88","","7/88","","END OF THE FOLLOWING IN CANTILEVER PRECAST  CONCRETE BENCHES","",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:58:09",""]
[1117,3449,7,15,"7/88","","7/88","","THE FOLLOWING IN GENOCIDE POND PRECAST CONCRETE BENCHES","",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:58:27",""]
[1118,3452,7,15,"7/88","","7/88","","PRECAST CONCRETE SLABS, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:06:57",""]
[1119,3453,7,15,"7/88","","7/88","","Precast concrete, (Class 1 with 7mm stone and fine grit), left smooth from the mould including metal leaf imprints at the rate of 3 per 1 500mm, bedding, jointing and pointing, all in accordance with details on drawing MUS-103","H4",{"v":0,"d":"0.0"},"","","","","28/10/2021 10:06:33",""]
[1120,3454,7,15,"7/88"," C","7/88. C","","510  x 100mm Thick seat slabs in 2 417mm lengths with closely butted rebated ends including bedding edges at ends (supports and reinforcement elsewhere) (Genocide pond bench type 3)","m",15,"","","","","28/10/2021 10:06:47",""]
[1121,3457,7,15,"7/88"," D","7/88. D","","510 x 3 000 x 100mm Thick seat slab including bedding ends (supports and reinforcement elsewhere) (Genocide pond bench type 2)","No",1,"","","","","28/10/2021 10:06:54",""]
[1122,3461,7,15,"7/88"," E","7/88. E","","450 x 4 887 x 100mm Thick curved on plan seat slab including bedding on supports (supports and reinforcement elsewhere) (Genocide pond bench type 1)","No",1,"","","","","28/10/2021 10:07:10",""]
[1123,3462,7,15,"7/88"," F","7/88. F","","200 x 200 x 380mm High support with 200 x 200 x 220mm high void and recess for light fitting (light fitting elsewhere) to bench slab including mass concrete foundations complete as per drawing S9615/GP/9004","No",12,"","","","","28/08/2013 09:58:02",""]
[1124,3450,7,15,"7/88","","7/88","","END OF THE FOLLOWING IN GENOCIDE POND PRECAST CONCRETE BENCHES","",{"v":0,"d":"0.0"},"","","","","06/12/2021 11:59:30",""]
[1125,12264,7,15,"7/88","","7/88","","BICYCLE RACKS","H2",{"v":0,"d":"0.0"},"","","","","05/11/2021 08:40:45",""]
[1126,12265,7,15,"7/89","","7/89","","Brushed stainless steel grade 316 bicycle rack","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 01:56:12",""]
[1127,12266,7,15,"7/89"," A","7/89. A","","5-Bicycle rack 3 350 x 885mm high overall formed of 50mm dia. x 2mm thickness continuous hollow pipe section eleven times curved to 125mm radius (total pipe length per rack = 12 282mm) (concrete bases measured elsewhere) ","No",3,"","","","","06/12/2021 09:53:25",""]
[1128,12267,7,15,"7/89"," B","7/89. B","","20MPa Unreinforced concrete bicycle rack base size 300 x 300 x 350mm deep including excavations, carting away, backfilling, etc.","No",3,"","","","","06/11/2021 11:56:29",""]
[1130,9478,7,16,"7/91","","7/91","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:09",""]
[1131,6105,7,16,"7/91","","7/91","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:44",""]
[1132,9479,7,16,"7/91","","7/91","","BILL NO. 16","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:56:24",""]
[1133,4191,7,16,"7/91","","7/91","","WORK TO BURIAL SITE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:25",""]
[1134,4192,7,16,"7/91","","7/91","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","27/08/2012 04:27:45",""]
[1135,4193,7,16,"7/91","","7/91","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:20",""]
[1136,4194,7,16,"7/91","","7/91","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","27/08/2012 04:27:45",""]
[1137,5653,7,16,"7/91","","7/91","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","21/09/2012 06:01:47",""]
[1138,5654,7,16,"7/91","","7/91","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.","",{"v":0,"d":"0.0"},"","","","","31/10/2021 06:05:10",""]
[1139,12026,7,16,"7/91","","7/91","","Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","31/10/2021 06:05:21",""]
[1140,7224,7,16,"7/91","","7/91","","Materials arising from the demolitions and alterations","H4",{"v":0,"d":"0.0"},"","","","","18/10/2012 08:18:15",""]
[1141,7225,7,16,"7/91","","7/91","","Materials arising from the demolitions and alterations will become the property of the contractor. An item is provided in the Calculation of Tender / Bid Sum at the end of the bills of quantities for \" Credit for old materials arising from the demolitions and alterations which become the property of the contractor\"","",{"v":0,"d":"0.0"},"","","","","18/10/2012 08:18:15",""]
[1142,7226,7,16,"7/91","","7/91","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","18/10/2012 08:18:15",""]
[1143,4195,7,16,"7/92","","7/92","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","27/08/2012 04:27:45",""]
[1144,4196,7,16,"7/92","","7/92","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","27/08/2012 04:27:45",""]
[1145,6986,7,16,"7/92","","7/92","","Work in sensitive area","H4",{"v":0,"d":"0.0"},"","","","","06/10/2012 09:14:11",""]
[1146,6987,7,16,"7/92","","7/92","","The Burial site is an area with historical significance and classified as a National Heritage Site (Management Authority - Greater Baviaanskloof Concervancy, contact - Kouga Municipality). The site is subject to the NHRA (National Heritage Resources Act). All work on and around the Burial site shall therefore be executed with extra care not to cause any potential damage to the actual Burial Site or surrounding vegetation and must be strictly within the guidelines as stipulated in the landscape architect’s specification as well as the EMP and NHRA. This includes the protection of all indigenous species on and around Vergaderingskop.","",{"v":0,"d":"0.0"},"","","","","09/12/2021 05:47:47",""]
[1147,4198,7,16,"7/92","","7/92","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","28/08/2012 10:08:44",""]
[1148,4199,7,16,"7/92","","7/92","","EXCAVATIONS, ETC","H3",{"v":0,"d":"0.0"},"","","","","28/08/2012 10:08:44",""]
[1149,4200,7,16,"7/92","","7/92","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","28/08/2012 10:08:44",""]
[1150,4201,7,16,"7/92"," A","7/92. A","","Trenches (Labour Intensive)","m3",4,"","","","","26/06/2023 10:55:50",""]
[1151,4219,7,16,"7/92","","7/92","","UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","28/08/2012 10:08:46",""]
[1152,4220,7,16,"7/92","","7/92","","20MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","24/10/2012 04:18:14",""]
[1153,4289,7,16,"7/92"," B","7/92. B","","Edge strips","m3",4,"","","","","31/10/2021 06:09:54",""]
[1154,4282,7,16,"7/92","","7/92","","GRANITE SLABS","H2",{"v":0,"d":"0.0"},"","","","","28/08/2012 04:17:11",""]
[1155,4283,7,16,"7/92","","7/92","","Zimbabwe granite with polished surface and edges, fixed to concrete slab (elsewhere) with suitable adhesive","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 12:17:54",""]
[1156,4284,7,16,"7/92"," C","7/92. C","","Slab size 30 x 1 175 x 2 980mm","No",1,"","","","","27/06/2023 02:18:29",""]
[1157,13738,7,16,"7/92"," D","7/92. D","","Provisional Sum of R10 000.00 (Ten Thousand) for engraving to the above slab, to be done by a specialist sub-contractor","Item",{"v":1,"d":"1.00"},{"v":10000,"d":"10000.00"},{"v":10000,"d":"10000.00"},"","","27/06/2023 02:17:21",""]
[1158,4287,7,16,"7/93","","7/93","","METALWORK","H2",{"v":0,"d":"0.0"},"","","","","28/08/2012 04:23:43",""]
[1159,13896,7,16,"7/93"," A","7/93. A","","\"PermaEdge\" 75mm high galvanised spiked garden edging in 1 000mm lengths, bent to shape, and fitted together with integral male and female interlocking ends","m",16,"","","","","27/06/2023 01:42:44",""]
[1160,4288,7,16,"7/93"," B","7/93. B","","\"PermaEdge\" 125mm high galvanised spiked garden edging in 1 000mm lengths, bent to shape, and fitted together with integral male and female interlocking ends","m",63,"","","","","27/06/2023 12:09:05",""]
[1162,10969,7,17,"7/95","","7/95","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:54:22",""]
[1163,10970,7,17,"7/95","","7/95","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:52",""]
[1164,10971,7,17,"7/95","","7/95","","BILL NO. 17","H1",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:50:35",""]
[1165,10972,7,17,"7/95","","7/95","","BALUSTRADING AND HANDRAILS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:37",""]
[1166,10973,7,17,"7/95","","7/95","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","22/10/2021 01:02:05",""]
[1167,10974,7,17,"7/95","","7/95","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:31",""]
[1168,12072,7,17,"7/95","","7/95","","MILD STEEL BALUSTRADING","H2",{"v":0,"d":"0.0"},"","","","","03/11/2021 09:21:52",""]
[1169,12073,7,17,"7/95","","7/95","","Welded balustrading to walkways and stairs, including all mitres, seamless laser welds, plates, etc. (paint finishes measured separately)","H4",{"v":0,"d":"0.0"},"","","","","03/11/2021 09:21:59",""]
[1170,12074,7,17,"7/95"," A","7/95. A","","Raking balustrading to staircases formed of 20 x 50 x 2mm RHS continuous top and bottom rails, and 20 x 50 x 2mm RHS posts at approximately 880mm centres each with 200 x 50 x 8mm flat section base plate bolted to concrete (bolts elsewhere)","kg",498,"","","","","03/11/2021 09:22:32",""]
[1171,10975,7,17,"7/95","","7/95","","GALVANISED STEEL HANDRAILS","H2",{"v":0,"d":"0.0"},"","","","","05/11/2021 07:16:32",""]
[1172,10989,7,17,"7/95","","7/95","","Galvanised steel welded handrails","H4",{"v":0,"d":"0.0"},"","","","","28/10/2021 02:42:07",""]
[1173,10990,7,17,"7/95"," B","7/95. B","","50 x 20 x 2mm RHS continuous handrails fixed to walls at not exceeding 900mm centres, with and including  14mm diameter x 285mm long once bent solid intermediate fixing pins epoxy-grouted 100mm deep into concrete or brick walls, including mortices in walls; the pins fitted with 50mm dia. x 2mm thick cover plates over openings in walls","m",8,"","","","","05/11/2021 07:17:21",""]
[1174,10991,7,17,"7/95"," C","7/95. C","","Extra over for closed end","No",4,"","","","","28/10/2021 02:40:22",""]
[1175,11021,7,17,"7/95"," D","7/95. D","","Extra over 90 degree bend","No",4,"","","","","28/10/2021 02:40:25",""]
[1176,13914,7,17,"7/95","","7/95","","PROPRIETARY METAL FENCING","H2",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:35:53",""]
[1177,13915,7,17,"7/96","","7/96","","\"Clearvue\" Reinforced high density anti-climbing and anti-cut pressed mesh panel fencing, formed of 3mm diameter horizontal and 4mm diameter vertical high tensile wires galvanised with marine fusion bond coating (colour medium grey) with aperture size 76,2 x 12,7mm and reinforcing v-section ribs, all bolted with vandal resistant bolts and clamping plates to 85 - 45mm taper locking post 1 000mm high including locking recess mechanism at centres as indicated with sealed end caps on and including 200 x 200 x 10mm thick mild steel marine fusion bond coated base plates epoxy anchored into concrete with 4No. M12 x 80mm long mild steel bolts","H4",{"v":0,"d":"0.0"},"","","","","28/06/2023 12:11:04",""]
[1178,13916,7,17,"7/96"," A","7/96. A","","Security fencing 1 000mm high, in 3 300mm long panels, including all intermediate posts, fixing mechanisms, etc.","m",60,"","","","","28/06/2023 12:01:54",""]
[1179,13917,7,17,"7/96"," B","7/96. B","","Extra over fencing as described above for end post","No",4,"","","","","28/06/2023 11:45:26",""]
[1180,10980,7,17,"7/96","","7/96","","GALVANISED STEEL BALUSTRADING","H2",{"v":0,"d":"0.0"},"","","","","27/10/2021 09:12:34",""]
[1181,13907,7,17,"7/96","","7/96","","\"Mentis Africa\" Ball and tube interlinked patent balustrading","H4",{"v":0,"d":"0.0"},"","","","","28/06/2023 09:52:49",""]
[1182,13908,7,17,"7/96"," C","7/96. C","","Horizontal balustrade 1 000mm high of 34,1mm diameter continuous pipe top and bottom rails and 42,9mm diameter stanchions at average 1 000mm centres bolted to concrete (bolts elsewhere)","m",30,"","","","","28/06/2023 10:58:40",""]
[1183,13909,7,17,"7/96"," D","7/96. D","","Raking balustrade 1 000mm high of 34,1mm diameter continuous pipe top and bottom rails and 42,9mm diameter stanchions at average 1 000mm centres bolted to concrete (bolts elsewhere)","m",10,"","","","","28/06/2023 10:58:49",""]
[1184,13910,7,17,"7/96"," E","7/96. E","","Extra over for end closure to horizontal balustrade","No",6,"","","","","28/06/2023 09:58:47",""]
[1185,13911,7,17,"7/96"," F","7/96. F","","Extra over for end closure to raking balustrade","No",4,"","","","","28/06/2023 09:58:52",""]
[1186,10992,7,17,"7/96","","7/96","","Welded balustrading to walkways and stairs, including all mitres, seamless laser welds, plates, etc. (paint finishes measured separately)","H4",{"v":0,"d":"0.0"},"","","","","27/10/2021 09:12:24",""]
[1187,11001,7,17,"7/96"," G","7/96. G","","Raking balustrading to staircases formed of 20 x 50 x 2mm RHS continuous top and bottom rails, and 20 x 50 x 2mm RHS posts at approximately 880mm centres each with 200 x 50 x 8mm flat section base plate bolted to concrete (bolts elsewhere)","kg",451,"","","","","28/10/2021 02:39:16",""]
[1188,12289,7,17,"7/97"," A","7/97. A","","Horizontal balustrading circular on plan to not exceeding  3 000mm radius to walkways of 38mm external diameter x 2mm thick continuous pipe handrail on and including 10mm dia. solid pins and base plates bolted to 20 x 50 x 2mm RHS continuous top rail at approximately 835mm centres, and 20 x 50 x 2mm RHS posts at approximately 800mm centres each with 200 x 50 x 8mm flat section base plate bolted to concrete (bolts elsewhere) and 34mm dia. x 2mm thick intermediate rail between posts (Drawing No 25116-GEN-106)","kg",227,"","","","","16/11/2021 11:41:27",""]
[1189,13836,7,17,"7/97"," B","7/97. B","","Horizontal balustrading circular on plan to not exceeding  3 000mm radius to walkways of 32mm external diameter x 2mm thick continuous pipe handrail on and including 32 x 150 x 8mm thick fixing plate on and including 50 x 12 x 544mm long flat section posts at approximately 735mm centres each with 200 x 50 x 4mm flat section base plate bolted to concrete (bolts elsewhere) and 32 x 8mm thick flat section intermediate rail between posts (Drawing No 25379-NC-GEN-3400.03)","kg",71,"","","","","22/06/2023 10:49:39",""]
[1190,12290,7,17,"7/97"," C","7/97. C","","Raking balustrading to staircases of 38mm external diameter x 2mm thick continuous pipe handrail on and including 10mm dia. solid pins and base plates bolted to 20 x 50 x 2mm RHS continuous top rail at approximately 835mm centres, and 20 x 50 x 2mm RHS posts at approximately 800mm centres each with 200 x 50 x 8mm flat section base plate bolted to concrete (bolts elsewhere) and 34mm dia. x 2mm thick intermediate rail between posts (Drawing No 25116-GEN-106)","kg",2897,"","","","","16/11/2021 11:41:37",""]
[1191,12856,7,17,"7/97"," D","7/97. D","","Horizontal balustrading to walkways of 20 x 50 x 2mm RHS top and bottom rails, and 20 x 50 x 2mm RHS posts at approximately 1 190mm centres each with 200 x 50 x 8mm flat section base plate bolted to concrete (bolts elsewhere) and 12mm solid round rods as intermediate rails (Drawing No 25379-NC-MUS-3400.01)","kg",88,"","","","","19/11/2021 08:57:23",""]
[1192,12075,7,17,"7/97","","7/97","","Galvanised bolts","H3",{"v":0,"d":"0.0"},"","","","","28/06/2023 10:59:00",""]
[1193,11003,7,17,"7/97"," E","7/97. E","","M8 x 80 Expansion anchor with loose bolt, including mortice in concrete","No",1072,"","","","","03/11/2021 09:23:40",""]
[1194,13837,7,17,"7/97"," F","7/97. F","","M12 x 80 Expansion anchor with loose bolt, including mortice in concrete","No",64,"","","","","28/06/2023 11:47:53",""]
[1195,11004,7,17,"7/97","","7/97","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","22/10/2021 02:11:36",""]
[1196,10985,7,17,"7/97"," G","7/97. G","","5mm Thick Sikaflex 11FC, or equally approved  polyurethane sealant 124mm girth x 40mm high around balustrade upright where protruding through floor screed","No",536,"","","","","10/12/2021 08:11:25",""]
[1197,11005,7,17,"7/97","","7/97","","PAINTWORK","H2",{"v":0,"d":"0.0"},"","","","","22/10/2021 02:12:14",""]
[1198,10987,7,17,"7/98","","7/98","","Prepare by sandblasting and apply two coats SigmaCover 380 epoxy primer (DFT 125) and one finishing coat SigmaDur 520 (DFT65) polyurethane paint (combined total DFT of 190) (colour : Plascon Rhine castle GR-Y10) on:","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 10:49:43",""]
[1199,10988,7,17,"7/98"," A","7/98. A","","General surfaces of balustrading not exceeding 300mm girth","m",1807,"","","","","06/12/2021 12:07:19",""]
[1201,9480,7,18,"7/100","","7/100","","SECTION NO. 7","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:13",""]
[1202,6106,7,18,"7/100","","7/100","","EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:18:48",""]
[1203,9481,7,18,"7/100","","7/100","","BILL NO. 18","H1",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:50:42",""]
[1204,5084,7,18,"7/100","","7/100","","BUILDERS WORK IN CONNECTION WITH SPECIALIST INSTALLATIONS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:30",""]
[1205,5085,7,18,"7/100","","7/100","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1206,5086,7,18,"7/100","","7/100","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:26",""]
[1207,5087,7,18,"7/100","","7/100","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1208,5088,7,18,"7/100","","7/100","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1209,5089,7,18,"7/100","","7/100","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1210,5090,7,18,"7/100","","7/100","","Laying, backfilling, bedding, etc of pipes","H4",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1211,5091,7,18,"7/100","","7/100","","All sleeve pipes are to be laid in accordance with SANS 1200 LC","",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1212,5092,7,18,"7/100","","7/100","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:14",""]
[1213,5093,7,18,"7/100","","7/100","","SLEEVES FOR ELECTRICAL, TELEPHONE CABLES, IRRIGATION PIPES, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:08:29",""]
[1214,5094,7,18,"7/100","","7/100","","EARTHWORKS","H3",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:02:18",""]
[1215,5095,7,18,"7/101","","7/101","","Excavate in earth and set excavated material aside for re-use as filling for:","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:01:49",""]
[1216,5096,7,18,"7/101"," A","7/101. A","","Excavation in earth not exceeding 2m deep for pipe trenches (Labour Intensive)","m3",35,"","","","","26/06/2023 01:24:48",""]
[1217,5098,7,18,"7/101"," B","7/101. B","","Extra over trench excavations in earth for excavation in soft rock","m3",10,"","","","","28/01/2014 08:25:21",""]
[1218,5099,7,18,"7/101"," C","7/101. C","","Extra over trench excavations in earth for excavation in hard rock","m3",5,"","","","","28/01/2014 08:25:25",""]
[1219,5100,7,18,"7/101"," D","7/101. D","","Selected and approved material from the excavations, in backfilling in trenches, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",21,"","","","","26/06/2023 10:56:17",""]
[1220,5101,7,18,"7/101"," E","7/101. E","","Bedding material supplied by the contractor, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",9,"","","","","26/06/2023 10:56:20",""]
[1221,5102,7,18,"7/101"," F","7/101. F","","Bedding material supplied by the contractor, stabilised with 5% OPC, and compacted to 93% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 10:56:25",""]
[1222,5103,7,18,"7/101"," G","7/101. G","","Cart away surplus excavated material from the excavations to a dumping site to be located by the contractor","m3",14,"","","","","26/06/2023 10:56:30",""]
[1223,5104,7,18,"7/101","","7/101","","uPVC class 51 sleeve piping including short lengths and jointing, laid in trench (trenches and backfilling measured elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 12:01:52",""]
[1224,5105,7,18,"7/101"," H","7/101. H","","50mm Diameter pipe","m",10,"","","","","27/02/2014 08:30:32",""]
[1225,5106,7,18,"7/101"," I","7/101. I","","110mm Diameter pipe","m",50,"","","","","27/02/2014 08:30:36",""]
[1226,5107,7,18,"7/101"," J","7/101. J","","160mm Diameter pipe","m",180,"","","","","27/02/2014 08:30:43",""]
[1227,5108,7,18,"7/101","","7/101","","Extra over uPVC piping for:","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 05:08:22",""]
[1228,5109,7,18,"7/101"," K","7/101. K","","50mm Diameter long radius bend","No",5,"","","","","01/10/2012 03:09:19",""]
[1229,5110,7,18,"7/101"," L","7/101. L","","110mm Diameter long radius bend","No",5,"","","","","27/02/2014 08:31:18",""]
[1230,5111,7,18,"7/101"," M","7/101. M","","160mm Diameter long radius bend","No",5,"","","","","27/02/2014 08:31:24",""]
[1231,5112,7,18,"7/101","","7/101","","Draw wires","H4",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:17",""]
[1232,5113,7,18,"7/101"," N","7/101. N","","3mm Galvanised steel draw wires in pipes","m",230,"","","","","06/10/2012 11:11:52",""]
[1233,5114,7,18,"7/102","","7/102","","Brick draw chambers, including precast or in-situ reinforced concrete cover slab (cover and frame elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 04:04:05",""]
[1234,5117,7,18,"7/102"," A","7/102. A","","1 000 x 1 000mm Chamber not exceeding 1 000mm deep internally","No",9,"","","","","06/12/2021 12:03:48",""]
[1235,5118,7,18,"7/102"," B","7/102. B","","1 000 x 1 000mm Chamber exceeding 1 000mm and not exceeding 1 500mm deep internally","No",4,"","","","","06/12/2021 12:05:13",""]
[1236,5119,7,18,"7/102"," C","7/102. C","","1 000 x 1 000mm Chamber exceeding 1 500mm and not exceeding 2 000mm deep internally","No",1,"","","","","27/06/2023 02:56:17",""]
[1237,13700,7,18,"7/102","","7/102","","Construct concrete cover slabs to suite brick draw chamber (covers and frames elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 03:20:32",""]
[1238,12803,7,18,"7/102"," D","7/102. D","","1 000 x 1 000mm Chamber","No",46,"","","","","27/06/2023 03:21:03",""]
[1239,13726,7,18,"7/102","","7/102","","Completion of brick draw chambers by raising or breaking down of brickwork to final levels","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:29:05",""]
[1240,13727,7,18,"7/102"," E","7/102. E","","Breaking down and removing one brick walls in inspection chambers to final levels","m2",10,"","","","","26/06/2023 10:59:02",""]
[1241,13728,7,18,"7/102"," F","7/102. F","","One brick walls of NFPE bricks (14 MPa nominal compressive strength) in class II (1:3) cement mortar in draw chambers, catchpits, manholes, etc.","m2",10,"","","","","19/05/2022 12:43:03",""]
[1242,13729,7,18,"7/102"," G","7/102. G","","150mm Wide brick reinforcement built in horizontally","m",15,"","","","","19/05/2022 12:43:06",""]
[1243,12796,7,18,"7/102","","7/102","","Covers","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:10:08",""]
[1244,5120,7,18,"7/102"," H","7/102. H","","450 x 450mm Type 4 Cast iron single seal manhole cover and frame","No",1,"","","","","27/06/2023 03:09:21",""]
[1245,5121,7,18,"7/102"," I","7/102. I","","650mm Diameter Type 1A concrete-filled polymer heavy duty lockable manhole cover and frame (code : 2230)","No",34,"","","","","14/11/2021 08:07:29",""]
[1246,5122,7,18,"7/102"," J","7/102. J","","650mm Diameter Type 1A concrete-filled (exposed aggregate, to match adjacent paving) cast iron heavy duty manhole cover and frame (code : 2230)","No",17,"","","","","31/10/2021 06:22:40",""]
[1247,5123,7,18,"7/102","","7/102","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","18/09/2012 08:07:18",""]
[1248,5124,7,18,"7/102"," K","7/102. K","","20MPa/13mm Stone unreinforced concrete encasing to horizontal pipes, cast against excavated surfaces","m3",1,"","","","","14/11/2021 08:04:33",""]
[1249,10101,7,18,"7/103","","7/103","","PLINTHS, BALUSTRADES, POSTS, ETC. FOR ARTWORK","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 01:07:45",""]
[1250,12569,7,18,"7/103","","7/103","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:39:29",""]
[1251,12570,7,18,"7/103"," A","7/103. A","","Bases (Labour Intensive)","m3",19,"","","","","26/06/2023 01:26:02",""]
[1252,12571,7,18,"7/103","","7/103","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:39:29",""]
[1253,12572,7,18,"7/103"," B","7/103. B","","Surplus material from the excavations and/or stock piles on site to an approved dumping site to be located by the contractor","m3",18,"","","","","06/12/2021 12:06:07",""]
[1254,12573,7,18,"7/103","","7/103","","Risk of collapse of excavations","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:39:29",""]
[1255,12574,7,18,"7/103"," C","7/103. C","","Sides of trench and hole excavations not exceeding 1,5m deep","m2",72,"","","","","06/12/2021 12:06:19",""]
[1256,12575,7,18,"7/103","","7/103","","Earth filling from excavations or stockpiles on site compacted to 93% modified AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:40:26",""]
[1257,12576,7,18,"7/103"," D","7/103. D","","Backfilling to bases (Labour Intensive)","m3",7,"","","","","26/06/2023 10:59:26",""]
[1258,12809,7,18,"7/103","","7/103","","Earth filling G5 supplied by the contractor, compacted to 95% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","15/11/2021 12:38:35",""]
[1259,12808,7,18,"7/103"," E","7/103. E","","Backfilling to bases (Labour Intensive)","m3",2,"","","","","26/06/2023 10:59:31",""]
[1260,12577,7,18,"7/103","","7/103","","REINFORCED CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:39:29",""]
[1261,12578,7,18,"7/103","","7/103","","25MPa/19mm Reinforced concrete cast against excavated surfaces","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:41:14",""]
[1262,12579,7,18,"7/103"," F","7/103. F","","Bases","m3",10,"","","","","11/11/2021 12:41:21",""]
[1263,12580,7,18,"7/103","","7/103","","Fabric reinforcement","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 12:39:29",""]
[1264,12581,7,18,"7/103"," G","7/103. G","","Type 193 fabric reinforcement in surface beds","m2",29,"","","","","06/12/2021 12:06:44",""]
[1266,60,7,19,"7/0","1","7/0.1","","Site clearance and bulk earthworks","Page","7/3",0,"","","","04/05/2012 03:50:23",""]
[1267,61,7,19,"7/0","2","7/0.2","","External water supplies","Page","7/10",0,"","","","04/05/2012 03:51:40",""]
[1268,770,7,19,"7/0","3","7/0.3","","Reservoirs","Page","7/13",0,"","","","28/05/2012 09:36:36",""]
[1269,3244,7,19,"7/0","4","7/0.4","","Pump station and sump","Page","7/16",0,"","","","08/08/2012 02:52:13",""]
[1270,62,7,19,"7/0","5","7/0.5","","External sewer drainage","Page","7/23",0,"","","","04/05/2012 03:52:06",""]
[1271,63,7,19,"7/0","6","7/0.6","","Stormwater drainage","Page","7/31",0,"","","","04/05/2012 03:52:17",""]
[1272,1718,7,19,"7/0","7","7/0.7","","Stormwater harvesting tank & Oil interceptor","Page","7/36",0,"","","","30/07/2012 09:05:18",""]
[1273,66,7,19,"7/0","8","7/0.8","","Water ponds","Page","7/45",0,"","","","04/05/2012 03:52:47",""]
[1274,5818,7,19,"7/0","9","7/0.9","","Symbolic and productive garden","Page","7/49",0,"","","","26/09/2012 01:11:14",""]
[1275,4851,7,19,"7/0","10","7/0.10","","Story telling pit","Page","7/50",0,"","","","14/09/2012 09:12:14",""]
[1276,67,7,19,"7/0","11","7/0.11","","Walkways, ramps & steps","Page","7/58",0,"","","","04/05/2012 03:52:58",""]
[1277,68,7,19,"7/0","12","7/0.12","","Parking, paving and roads","Page","7/64",0,"","","","04/05/2012 03:53:18",""]
[1278,70,7,19,"7/0","13","7/0.13","","Retaining walls","Page","7/76",0,"","","","04/05/2012 03:53:33",""]
[1279,71,7,19,"7/0","14","7/0.14","","Boundary walling and Security fencing","Page","7/84",0,"","","","04/05/2012 03:53:48",""]
[1280,3860,7,19,"7/0","15","7/0.15","","Litter bins, bollards, benches, etc","Page","7/90",0,"","","","19/08/2012 03:33:08",""]
[1281,4188,7,19,"7/0","16","7/0.16","","Work to burial site","Page","7/94",0,"","","","27/08/2012 04:26:34",""]
[1282,10968,7,19,"7/0","17","7/0.17","","Balustrading and handrails","Page","7/99",0,"","","","22/10/2021 01:01:31",""]
[1283,74,7,19,"7/0","18","7/0.18","","BWICW","Page","7/104",0,"","","","04/05/2012 03:54:16",""]
[1284,9482,8,1,"8/1","","8/1","","SECTION NO. 8","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:22",""]
[1285,6669,8,1,"8/1","","8/1","","R331 ROAD UPGRADE (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:54:00",""]
[1286,9483,8,1,"8/1","","8/1","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:05:24",""]
[1287,6671,8,1,"8/1","","8/1","","R331 ROAD","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:54:09",""]
[1288,6672,8,1,"8/1","","8/1","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:32:44",""]
[1289,6673,8,1,"8/1","","8/1","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:35",""]
[1290,6674,8,1,"8/1","","8/1","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:32:44",""]
[1291,6675,8,1,"8/1","","8/1","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:32:44",""]
[1292,6676,8,1,"8/1","","8/1","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","05/10/2012 05:03:31",""]
[1293,7220,8,1,"8/1","","8/1","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","17/10/2012 04:04:02",""]
[1294,6678,8,1,"8/1","","8/1","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:32:45",""]
[1295,6679,8,1,"8/1","","8/1","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","04/10/2012 03:32:45",""]
[1296,6851,8,1,"8/1","","8/1","","Testing of material and filling","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 12:40:46",""]
[1297,6852,8,1,"8/1","","8/1","","Descriptions of earth filling, compaction, etc. shall be deemed to include for all necessary testing required in accordance with the SANS 1200 series","",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:12:59",""]
[1298,7217,8,1,"8/2","","8/2","","SAFEGUARDING AND ACCOMMODATION OF TRAFFIC","H2",{"v":0,"d":"0.0"},"","","","","17/10/2012 04:02:54",""]
[1299,7017,8,1,"8/2"," A","8/2. A","","Provide all necessary temporary works, signage, and traffic control measures during construction, on a 24-hour basis (Refer to PSA 5.10, SANS 1200 A5.2, and SANS 1200 D5 1.6)","Item",{"v":1,"d":"1.00"},"","","","","10/12/2021 08:13:28",""]
[1300,9988,8,1,"8/2","","8/2","SANS 1200MM 8.2 ","ROADSIDE PROTECTION GUARD RAILS","H2",{"v":0,"d":"0.0"},"","","","","13/10/2021 12:03:25",""]
[1301,9989,8,1,"8/2","","8/2","8.2.1 ","Hot-dip galvanised single-sided guard rails on and including timber posts, including all spacer blocks, bolts, reinforcing plates, excavations, backfilling, etc., complying with SANS 1350, and in accordance with DWP drawings WCS/54/1/C3, C4, C5, & C6","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 02:06:02",""]
[1302,9990,8,1,"8/2"," B","8/2. B","8.2.1a ","Guard rail (bullnoses and end wings elsewhere)","m",103,"","","","","30/10/2021 08:46:09",""]
[1303,9991,8,1,"8/2"," C","8/2. C","8.2.2 ","Extra-over for horizontally curved guardrails factory-bent to a radius of less than 150m","m",40,"","","","","08/12/2021 03:27:23",""]
[1304,9992,8,1,"8/2"," D","8/2. D","8.2.4 ","Additional guardrail post, including all spacer blocks, excavations, backfilling, etc.","No",10,"","","","","30/10/2021 08:46:20",""]
[1305,9993,8,1,"8/2"," E","8/2. E","8.2.3 ","Bullnose end wing, including additional spacer blocks, bolts, etc.","No",1,"","","","","30/10/2021 08:46:25",""]
[1306,9994,8,1,"8/2"," F","8/2. F","8.2.5 ","V-shaped reflector plate","No",28,"","","","","30/10/2021 08:46:29",""]
[1307,6855,8,1,"8/2","","8/2","","ROADWORK","H2",{"v":0,"d":"0.0"},"","","","","05/10/2012 12:41:40",""]
[1308,6853,8,1,"8/2","","8/2","","Site clearance","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 12:41:07",""]
[1309,10103,8,1,"8/2"," G","8/2. G","","Cutting down and removing thorn tree exceeding 200mm and not exceeding 500mm girth","No",1,"","","","","28/10/2021 10:31:43",""]
[1310,6872,8,1,"8/2","","8/2","","Additional tests required by the engineer","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 12:44:47",""]
[1311,6873,8,1,"8/2"," H","8/2. H","","In-situ dry density test in accordance with method A10(b) of TMH1","No",10,"","","","","06/10/2012 01:20:33",""]
[1312,7040,8,1,"8/2"," I","8/2. I","","\"Modified AASHTO Density\" test","No",10,"","","","","06/10/2012 01:20:16",""]
[1313,6927,8,1,"8/2","","8/2","","FILLING ETC","H3",{"v":0,"d":"0.0"},"","","","","05/10/2012 12:42:31",""]
[1314,6928,8,1,"8/2","","8/2","","Earth filling supplied by the contractor","H4",{"v":0,"d":"0.0"},"","","","","05/10/2012 12:42:31",""]
[1315,10104,8,1,"8/2"," J","8/2. J","","Imported G7 selected material in forming road side drains, compacted to 93% Mod AASHTO density","m3",480,"","","","","30/10/2021 08:40:19",""]
[1316,10105,8,1,"8/3","","8/3","","Note : unless indicated otherwise all rates for signs are to include poles, bases, etc. ","",{"v":0,"d":"0.0"},"","","","","14/10/2021 03:16:26",""]
[1317,7128,8,1,"8/3","","8/3","","Traffic signs (as per drawings C5593-SITE-RDS-74 & 96)","H4",{"v":0,"d":"0.0"},"","","","","17/10/2012 11:52:53",""]
[1318,7130,8,1,"8/3"," A","8/3. A","","60km/h Speed limit & No overtaking sign (Codes : R201 & R214)","No",1,"","","","","11/10/2012 08:54:16",""]
[1319,7149,8,1,"8/3"," B","8/3. B","","60km/h Speed limit & Sharp curve right sign (Codes : R201 & W204)","No",1,"","","","","11/10/2012 08:54:21",""]
[1320,10106,8,1,"8/3"," C","8/3. C","","Sharp curve right sign (Code : W204) to existing pole","No",1,"","","","","30/10/2021 08:40:28",""]
[1321,7131,8,1,"8/3"," D","8/3. D","","No overtaking sign (Code : R214)","No",1,"","","","","11/10/2012 08:54:54",""]
[1322,7132,8,1,"8/3"," E","8/3. E","","Additional lane sign (Code : GS202)","No",1,"","","","","11/10/2012 08:54:57",""]
[1323,7146,8,1,"8/3"," F","8/3. F","","Additional lane sign (Code : GS203)","No",1,"","","","","11/10/2012 08:55:00",""]
[1324,7134,8,1,"8/3"," G","8/3. G","","Staggered junction (L-R) sign (Code : W110)","No",1,"","","","","11/10/2012 08:55:05",""]
[1325,7137,8,1,"8/3"," H","8/3. H","","Fingerboard sign (Code : GD4)","No",4,"","","","","11/10/2012 08:55:19",""]
[1326,7138,8,1,"8/3"," I","8/3. I","","Sharp curve chevron sign (Code : W405)","No",8,"","","","","11/10/2012 08:55:35",""]
[1327,10109,8,1,"8/3"," J","8/3. J","","Sharp curve chevron sign (W405), and fixing to existing pole","No",6,"","","","","30/10/2021 08:40:34",""]
[1328,10110,8,1,"8/3"," K","8/3. K","","Adjust alignment of sharp curve chevron sign (W405) (pole to remain as-is) ","No",1,"","","","","30/10/2021 08:40:48",""]
[1329,10111,8,1,"8/3"," L","8/3. L","","Take down and remove stack-type direction & T-junction chevron sign (GD2 & W409) - poles to remain","No",2,"","","","","30/10/2021 08:40:57",""]
[1330,10112,8,1,"8/3"," M","8/3. M","","Stack-type direction & T-junction chevron sign (GD2 & W409), and fixing to existing poles","No",2,"","","","","30/10/2021 08:41:04",""]
[1331,6909,8,1,"8/3","","8/3","","PAINTWORK","H3",{"v":0,"d":"0.0"},"","","","","22/06/2023 11:59:30",""]
[1332,8602,8,1,"8/3","","8/3","","Prepare and apply two coats white reflective road marking paint on bituminous road surfacing, precast concrete paving blocks, etc.","H4",{"v":0,"d":"0.0"},"","","","","21/06/2019 11:15:33",""]
[1333,6944,8,1,"8/3"," N","8/3. N","","Traffic arrow 5 500 x 1 400mm wide extreme (Labour Intensive)","No",1,"","","","","26/06/2023 11:00:09",""]
[1334,12928,8,1,"8/4","","8/4","","STORMWATER DRAINAGE","H3",{"v":0,"d":"0.0"},"","","","","18/11/2021 07:40:50",""]
[1335,12953,8,1,"8/4"," A","8/4. A","","Excavation in earth not exceeding 2m deep to reduce levels (Labour Intensive)","m3",8,"","","","","26/06/2023 11:00:15",""]
[1336,7039,8,1,"8/4"," B","8/4. B","","Forming v-shaped cut-off surface drain average 4 000mm wide x 300mm deep with average 2 000mm wide x 500mm high triangular berm to one side, all compacted to 95% Modified AASHTO density, including finishing to slopes, etc.","m",265,"","","","","19/11/2021 10:16:26",""]
[1337,12937,8,1,"8/4","","8/4","","GABIONS AND INTERLOCKING BLOCK RETAINING STRUCTURES","H2",{"v":0,"d":"0.0"},"","","","","19/11/2021 10:15:52",""]
[1338,12938,8,1,"8/4","","8/4","","Bedding material supplied by the contractor, stabilised with 3% OPC, and compacted to 98% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 10:15:52",""]
[1339,12939,8,1,"8/4"," C","8/4. C","","Under stone filled gabion mattresses","m3",21,"","","","","06/12/2021 05:32:55",""]
[1340,12940,8,1,"8/4","","8/4","","Note : Gabions are to be of double twisted hexagonal wire mesh (nominal 80 x 100mm mesh of 2,7mm galvanised wire, with 3,5mm galvanised wire framing and with partitions at 1m centres).  All wire to be hot-dip galvanised to SANS 675","",{"v":0,"d":"0.0"},"","","","","06/12/2021 05:32:44",""]
[1341,12941,8,1,"8/4","","8/4","","Gabions of galvanised wire boxes with diaphragm divisions @ 1m c/c, butt-jointed, laced together and filled with broken stone","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 10:15:52",""]
[1342,12943,8,1,"8/4"," D","8/4. D","","2 x 1 x 0,5m Box properly bonded","No",28,"","","","","10/12/2021 03:23:35",""]
[1343,12946,8,1,"8/4"," E","8/4. E","","3 x 1 x 0,3m Mattress","No",28,"","","","","10/12/2021 03:23:29",""]
[1344,12948,8,1,"8/4","","8/4","","Type U24 filter fabric blanket with 200mm laps","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 10:15:53",""]
[1345,12949,8,1,"8/4"," F","8/4. F","","Under stone filled gabion mattresses including preparing ground surface under","m2",155,"","","","","23/11/2021 08:47:20",""]
[1346,12934,8,1,"8/4","","8/4","","PRECAST CONCRETE KERBS","H2",{"v":0,"d":"0.0"},"","","","","19/11/2021 10:15:34",""]
[1347,12935,8,1,"8/4","","8/4","","Precast concrete finished smooth on exposed surfaces, including bedding, jointing and pointing","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 10:15:34",""]
[1348,12936,8,1,"8/4"," G","8/4. G","","150 x 250mm High kerbs (SANS 927 fig 4) laid on and including 450 x 250mm thick concrete base, including shallow excavation, bedding, backfilling, etc.","m",39,"","","","","10/12/2021 08:16:11",""]
[1350,9486,9,1,"9/1","","9/1","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:48:51",""]
[1351,6212,9,1,"9/1","","9/1","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:54:25",""]
[1352,9487,9,1,"9/1","","9/1","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:06:24",""]
[1353,3915,9,1,"9/1","","9/1","","GENERAL LANDSCAPING","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:54:32",""]
[1354,264,9,1,"9/1","","9/1","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:31:48",""]
[1355,265,9,1,"9/1","","9/1","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:40",""]
[1356,266,9,1,"9/1","","9/1","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:31:48",""]
[1357,267,9,1,"9/1","","9/1","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","11/05/2012 07:31:48",""]
[1358,268,9,1,"9/1","","9/1","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:31:14",""]
[1359,943,9,1,"9/1","","9/1","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 08:07:47",""]
[1360,944,9,1,"9/1","","9/1","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\"","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:51:41",""]
[1361,1450,9,1,"9/1","","9/1","","Plants need to be installed as per plans All plants needed can be either grown and maintained at the contractors own nursery or sourced from any other nursery, but must adhere to the sizes and quality as specified in the tender document at the time of installation.","",{"v":0,"d":"0.0"},"","","","","11/08/2012 11:37:29",""]
[1362,3536,9,1,"9/1","","9/1","","All plants to be free from any damage, parasites, fungus or any other plant diseases or insects. No container bound plants will be acceptable.All leaves to be dust free.All plants are to be viewed and approved by the Landscape Architect before planting.","",{"v":0,"d":"0.0"},"","","","","11/08/2012 11:37:50",""]
[1363,3537,9,1,"9/2","","9/2","","All plants must be transported to the site in trucks with closed canopies. Plants in transit may not be exposed to wind or any other harmful elements. Plants need to be watered regularly as for the specific needs of each species. No pot bound roots will be accepted.","",{"v":0,"d":"0.0"},"","","","","11/08/2012 11:38:09",""]
[1364,3538,9,1,"9/2","","9/2","","Plants must be well rooted and well established. The nursery must be clean and presentable, with suiatble growing conditions established for growing of the plants. All plants to be planted in a grid/diamond pattern in perfectly straight lines. All existing trees encountered to be neatly pruned.","",{"v":0,"d":"0.0"},"","","","","11/08/2012 11:38:18",""]
[1365,13794,9,1,"9/2","","9/2","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:07:31",""]
[1366,13897,9,1,"9/2","","9/2","","LANDSCAPING","H3",{"v":0,"d":"0.0"},"","","","","28/06/2023 08:26:22",""]
[1367,1055,9,1,"9/2","","9/2","","Earthworks","H3",{"v":0,"d":"0.0"},"","","","","04/06/2012 11:21:43",""]
[1368,1066,9,1,"9/2","","9/2","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting planting areas in maximum 300mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","10/08/2012 08:40:38",""]
[1369,946,9,1,"9/2"," A","9/2. A","","General shaping of landscaped areas","m3",129,"","","","","04/06/2012 12:26:18",""]
[1370,1067,9,1,"9/2","","9/2","","Precision shaping of landscape areas and earth mounds","H4",{"v":0,"d":"0.0"},"","","","","10/08/2012 08:25:33",""]
[1371,1068,9,1,"9/2"," B","9/2. B","","Precision shaping of landscape areas and earth mounds by means of accurate levels taken with a dumpy level, and adjustment of levels to ensure a level appearance","m2",1118,"","","","","10/08/2012 08:26:18",""]
[1372,7431,9,1,"9/3","","9/3","","Open face excavation in earth over sloping site","H4",{"v":0,"d":"0.0"},"","","","","20/10/2012 12:02:06",""]
[1373,7432,9,1,"9/3"," A","9/3. A","","Open face excavation in planters, flower beds, etc.","m3",100,"","","","","20/10/2012 12:03:00",""]
[1374,7433,9,1,"9/3","","9/3","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","20/10/2012 12:02:06",""]
[1375,7434,9,1,"9/3"," B","9/3. B","","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",97,"","","","","20/10/2012 12:02:06",""]
[1376,1410,9,1,"9/3","","9/3","","Earthworks and composting","H3",{"v":0,"d":"0.0"},"","","","","20/07/2012 09:25:04",""]
[1377,1411,9,1,"9/3","","9/3","","All planted areas at the front at the road side shall be ripped and rotivated using machinery by breaking up the earth to a depth of 300mm at 300mm centres in both directions, unless otherwise described.","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:56:41",""]
[1378,3535,9,1,"9/3","","9/3","","Ground preparation","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 10:44:09",""]
[1379,3534,9,1,"9/3","","9/3","","Cultivation, including ripping and machine rotivating by breaking up earth to a depth of 300mm at 300mm centres in both directions, and preparation of areas to be planted","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 10:47:14",""]
[1380,1412,9,1,"9/3"," C","9/3. C","","Shrubs and groundcover areas","m2",50,"","","","","11/08/2012 10:47:29",""]
[1381,1413,9,1,"9/3"," D","9/3. D","","Lawn areas","m2",2584,"","","","","11/08/2012 10:47:41",""]
[1382,1414,9,1,"9/3","","9/3","","Fine grading","H3",{"v":0,"d":"0.0"},"","","","","20/07/2012 09:28:34",""]
[1383,1415,9,1,"9/3","","9/3","","Ensure that all areas to be planted are compacted sufficiently to avoid any subsidence later on, and that surface to be planted does not exceed a tolerance of 30mm in height when measured from the basic topographical line","H4",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:26:57",""]
[1384,1416,9,1,"9/3"," E","9/3. E","","Shrubs and groundcover areas","m2",10,"","","","","19/07/2023 08:26:35",""]
[1385,1417,9,1,"9/3"," F","9/3. F","","Lawn areas","m2",2584,"","","","","19/07/2023 08:26:39",""]
[1386,1418,9,1,"9/3","","9/3","","Topsoil","H3",{"v":0,"d":"0.0"},"","","","","10/08/2012 08:53:24",""]
[1387,1420,9,1,"9/4","","9/4","","Topsoil varying between sandy loamy soil and sandy clayey soil with a ideal ratio of 15% to 25% clay, 10% Silt/Sludge and 65% to 75% sand, with a minimum ratio of organic material of 2% of volume. All material to be free of harmful deposits such as salts, weed seeds and waste of any kind","H4",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:26:48",""]
[1388,1421,9,1,"9/4"," A","9/4. A","","Imported topsoil supplied by the contractor and spreading and levelling on site, filling plant and tree holes, etc.","m3",250,"","","","","20/08/2012 06:31:43",""]
[1389,1422,9,1,"9/4"," B","9/4. B","","Topsoil from stock piles on site and spreading and levelling on site, filling plant and tree holes, etc.","m3",10,"","","","","20/08/2012 06:31:57",""]
[1390,1423,9,1,"9/4","","9/4","","Permeable planter topsoil mix","H3",{"v":0,"d":"0.0"},"","","","","20/07/2012 09:38:47",""]
[1391,1424,9,1,"9/4","","9/4","","Imported topsoil mix consisting 50% clean sifted topsoil (see specification above), 30% clean washed river sand and 20% vermiculite","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:58:29",""]
[1392,1425,9,1,"9/4"," C","9/4. C","","To planter areas, including spreading, levelling and lightly compacting","m3",107,"","","","","08/12/2021 03:07:10",""]
[1393,1426,9,1,"9/4","","9/4","","Compost","H3",{"v":0,"d":"0.0"},"","","","","11/08/2012 09:18:24",""]
[1394,1427,9,1,"9/4","","9/4","","Properly decayed organic material, free from harmful deposits, salts, seeds and other waste material, with a pH of more than 4 and less than 7","H4",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:27:23",""]
[1395,7384,9,1,"9/4"," D","9/4. D","","In tree holes, shrub and groundcover areas","m3",172,"","","","","19/10/2012 02:31:25",""]
[1396,1437,9,1,"9/4","","9/4","","Organic Fertilizers","H3",{"v":0,"d":"0.0"},"","","","","20/07/2012 11:24:36",""]
[1397,1438,9,1,"9/4","","9/4","","Fertilizers shall be of the type specified, mixed thoroughly into the soil as prescribed. No fertilizer shall be added more than two weeks prior to planting.All fertilizers to areas to be grassed shall be strewn on the final layer before the final finishing is commenced and worked mechanically into the top 150 mm soil","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:32:45",""]
[1398,1439,9,1,"9/4"," E","9/4. E","","2:3:2 in tree holes","kg",4,"","","","","31/10/2021 06:24:09",""]
[1399,1440,9,1,"9/4"," F","9/4. F","","2:3:2 in shrubs and groundcover areas","kg",226,"","","","","31/10/2021 06:24:16",""]
[1400,1441,9,1,"9/4"," G","9/4. G","","2:3:2 in lawn areas","kg",145,"","","","","31/10/2021 06:24:26",""]
[1401,965,9,1,"9/5","","9/5","","Trees and aloes","H3",{"v":0,"d":"0.0"},"","","","","10/08/2012 08:55:03",""]
[1402,1462,9,1,"9/5","","9/5","","Note : Trees (Tree stakes included, 2 per 50l,100l trees and 4 per 200 and 400l trees) The height of the trees shall be measured from the top of the root ball to the top of the tree. Where trees are pruned, such prune wounds shall not be more than 25mm in diameter and be sealed with an approved sealing compound","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:27:39",""]
[1403,3942,9,1,"9/5","","9/5","","400l trees : min. 5 000mm tall, with a stem diameter of 450mm and a crown width of 3 diameters. 200l trees : min. 3 800mm stem height; 2 200mm crown spread after planting, with a stem diameter of 200mm measured 300mm above soil level. 100l trees : min. 2 800mm stem height; 1 800mm crown spread after planting, with a stem diameter of 40mm measured 300mm above soil level. 50l trees : min. 2 400mm stem height; 1 400mm crown spread after planting, with a stem diameter of 30mm measured 300mm above soil level","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:27:46",""]
[1404,966,9,1,"9/5"," A","9/5. A","","Podocarpus fulcatus(400l)","No",15,"","","","","06/12/2021 12:08:55",""]
[1405,1064,9,1,"9/5"," B","9/5. B","","Podocarpus latifolius(100l)","No",15,"","","","","06/12/2021 12:09:09",""]
[1406,1292,9,1,"9/5"," C","9/5. C","","Acacia karroo(50l)","No",44,"","","","","10/12/2021 03:01:04",""]
[1407,1293,9,1,"9/5"," D","9/5. D","","Ziziphus mucronata(100l)","No",17,"","","","","06/12/2021 12:09:32",""]
[1408,1294,9,1,"9/5"," E","9/5. E","","Schotia brachypetala(50l)","No",24,"","","","","06/12/2021 12:09:45",""]
[1409,1295,9,1,"9/5"," F","9/5. F","","Harpephyllum caffrum(200l)","No",62,"","","","","06/12/2021 12:10:04",""]
[1410,1296,9,1,"9/5"," G","9/5. G","","Boscia albitrunca(100l)","No",21,"","","","","06/12/2021 12:10:16",""]
[1411,1297,9,1,"9/5"," H","9/5. H","","Pappea capensis(100l)","No",33,"","","","","06/12/2021 12:10:28",""]
[1412,1298,9,1,"9/5"," I","9/5. I","","Curtisia dentate(100l)","No",6,"","","","","06/12/2021 12:10:41",""]
[1413,1299,9,1,"9/5"," J","9/5. J","","Olea africana(200l)","No",39,"","","","","06/12/2021 12:10:55",""]
[1414,1300,9,1,"9/5"," K","9/5. K","","Ocotea bullata(100l)","No",7,"","","","","06/12/2021 12:11:06",""]
[1415,1301,9,1,"9/5"," L","9/5. L","","Erythrina caffra(400l)","No",48,"","","","","06/12/2021 12:11:20",""]
[1416,1302,9,1,"9/5"," M","9/5. M","","Sideroxylon inerme(100l)","No",24,"","","","","06/12/2021 12:11:31",""]
[1417,1303,9,1,"9/5"," N","9/5. N","","Protorhus longifolia(100l)","No",11,"","","","","06/12/2021 12:11:42",""]
[1418,1304,9,1,"9/6"," A","9/6. A","","Calodendron capense(100l)","No",32,"","","","","06/12/2021 12:11:54",""]
[1419,1305,9,1,"9/6"," B","9/6. B","","Milletia grandis(100l)","No",11,"","","","","06/12/2021 12:12:04",""]
[1420,1306,9,1,"9/6"," C","9/6. C","","Salix mucronata(100l)","No",24,"","","","","06/12/2021 12:16:06",""]
[1421,1307,9,1,"9/6"," D","9/6. D","","Pterocelastrus tricuspidata(100l)","No",12,"","","","","06/12/2021 12:16:20",""]
[1422,1308,9,1,"9/6"," E","9/6. E","","Ehretia rigida(100l)","No",5,"","","","","06/12/2021 12:16:30",""]
[1423,1309,9,1,"9/6"," F","9/6. F","","Schotia afra(100l)","No",1,"","","","","06/12/2021 12:16:41",""]
[1424,1310,9,1,"9/6"," G","9/6. G","","Schrebera alata(100l)","No",24,"","","","","06/12/2021 12:16:52",""]
[1425,1311,9,1,"9/6"," H","9/6. H","","Hippobromus pauciflorus(100l)","No",2,"","","","","06/12/2021 12:17:01",""]
[1426,1312,9,1,"9/6"," I","9/6. I","","Pterocelastrus rostratus(100l)","No",12,"","","","","06/12/2021 12:17:10",""]
[1427,1313,9,1,"9/6"," J","9/6. J","","Ficus sur(400l)","No",4,"","","","","06/12/2021 12:17:19",""]
[1428,1314,9,1,"9/6"," K","9/6. K","","Colpoon compressum(100l)","No",10,"","","","","06/12/2021 12:17:33",""]
[1429,1315,9,1,"9/6"," L","9/6. L","","Xymalos monospora(100l)","No",10,"","","","","06/12/2021 12:17:47",""]
[1430,1316,9,1,"9/6"," M","9/6. M","","Dovyalis caffra(50l)","No",30,"","","","","06/12/2021 12:17:56",""]
[1431,13912,9,1,"9/6"," N","9/6. N","","Dovyalis caffra(100l)","No",5,"","","","","28/06/2023 09:38:45",""]
[1432,1317,9,1,"9/6"," O","9/6. O","","Noltea africana(100l)","No",3,"","","","","06/12/2021 12:18:05",""]
[1433,1318,9,1,"9/6"," P","9/6. P","","Cussonia spicata(100l)","No",19,"","","","","06/12/2021 12:18:16",""]
[1434,1319,9,1,"9/6"," Q","9/6. Q","","Ptaeroxylon obliquum(100l)","No",62,"","","","","06/12/2021 12:18:26",""]
[1435,1320,9,1,"9/6"," R","9/6. R","","Vepris ianceolata(100l)","No",19,"","","","","06/12/2021 12:18:35",""]
[1436,1321,9,1,"9/6"," S","9/6. S","","Apodytes dimidiate(100l)","No",26,"","","","","06/12/2021 12:18:45",""]
[1437,1040,9,1,"9/6","","9/6","","Shrubs and ground covers","H3",{"v":0,"d":"0.0"},"","","","","04/06/2012 10:38:27",""]
[1438,1041,9,1,"9/6","","9/6","","Note :Shrubs and groundcovers shall meet the requirements for height and spread as specified below and in specifications. Thin or sparsely-branched plants will not be accepted. Plants shall be well rooted (especially plugs), well-spread with ample young branches and the plant as a whole shall be well grown.  Only vigorous full growing plants will be accepted","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:28:09",""]
[1439,1042,9,1,"9/7","","9/7","","Cuttings = to be well rooted and well established 2kg/lt = 250mm stem lengths and well established 4kg/lt = 350mm stem lengths and well established Plugs = to be well rooted and well established","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:29:50",""]
[1440,961,9,1,"9/7","","9/7","","Shrubs","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 10:35:26",""]
[1441,1039,9,1,"9/7"," A","9/7. A","","Carissa bispinosa(2l)","No",6854,"","","","","06/12/2021 12:19:16",""]
[1442,1043,9,1,"9/7"," B","9/7. B","","Portulacaria affra(2l)","No",3341,"","","","","06/12/2021 12:19:27",""]
[1443,1323,9,1,"9/7"," C","9/7. C","","Cussonia thyrsifolia(2l)","No",6854,"","","","","06/12/2021 12:19:41",""]
[1444,1324,9,1,"9/7"," D","9/7. D","","Maytenus procumbens(4l)","No",2522,"","","","","06/12/2021 12:19:53",""]
[1445,1325,9,1,"9/7"," E","9/7. E","","Rhus glauca(4l)","No",1309,"","","","","06/12/2021 12:20:02",""]
[1446,1326,9,1,"9/7"," F","9/7. F","","Rhus crenata(4l)","No",1442,"","","","","06/12/2021 12:20:12",""]
[1447,1327,9,1,"9/7"," G","9/7. G","","Rhus pallens(2l)","No",694,"","","","","06/12/2021 12:20:28",""]
[1448,1328,9,1,"9/7"," H","9/7. H","","Euclea undulate(4l)","No",5110,"","","","","06/12/2021 12:20:39",""]
[1449,1329,9,1,"9/7"," I","9/7. I","","Euclea racemosa(4l)","No",3120,"","","","","06/12/2021 12:20:49",""]
[1450,1330,9,1,"9/7"," J","9/7. J","","Maytenus heterophylla(4l)","No",1870,"","","","","06/12/2021 12:21:05",""]
[1451,1332,9,1,"9/7"," K","9/7. K","","Grewia occidentalis(2l)","No",1652,"","","","","06/12/2021 12:21:24",""]
[1452,1333,9,1,"9/7"," L","9/7. L","","Chrysanthemoides monilifera(4l)","No",3154,"","","","","06/12/2021 12:21:38",""]
[1453,1334,9,1,"9/7"," M","9/7. M","","Pavetta revolute(4l)","No",347,"","","","","06/12/2021 12:21:47",""]
[1454,1335,9,1,"9/7"," N","9/7. N","","Salvia africana lutea(4l)","No",1309,"","","","","06/12/2021 12:21:58",""]
[1455,1336,9,1,"9/7"," O","9/7. O","","Capparis seperiara(4l)","No",3427,"","","","","06/12/2021 12:22:08",""]
[1456,1337,9,1,"9/7"," P","9/7. P","","Putterlickia pyrecantha H(4l)","No",6682,"","","","","06/12/2021 12:22:19",""]
[1457,1338,9,1,"9/7"," Q","9/7. Q","","Putterlickia verrucosa(2l)","No",10220,"","","","","06/12/2021 12:22:31",""]
[1458,13892,9,1,"9/7"," R","9/7. R","","Jasminum multipartitum(4l)","No",32,"","","","","27/06/2023 10:18:27",""]
[1459,1034,9,1,"9/7","","9/7","","Succulents","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 09:35:35",""]
[1460,1036,9,1,"9/7"," S","9/7. S","","Euphorbia triagularis(Plugs)","No",1389,"","","","","06/12/2021 12:22:58",""]
[1461,1037,9,1,"9/8"," A","9/8. A","","Euphorbia caerulucens(2l)","No",10088,"","","","","06/12/2021 12:23:08",""]
[1462,1339,9,1,"9/8"," B","9/8. B","","Crassula ovate(2l)","No",3740,"","","","","06/12/2021 12:23:20",""]
[1463,1340,9,1,"9/8"," C","9/8. C","","Cotyledon orbiculata(4l)","No",1309,"","","","","06/12/2021 12:23:33",""]
[1464,1341,9,1,"9/8"," D","9/8. D","","Cotyledon campanulata(2l)","No",3740,"","","","","06/12/2021 12:23:47",""]
[1465,1342,9,1,"9/8"," E","9/8. E","","Crassula muscosa(4l)","No",2885,"","","","","06/12/2021 12:23:56",""]
[1466,1343,9,1,"9/8"," F","9/8. F","","Crassula perfoliata(2l)","No",10220,"","","","","06/12/2021 12:24:05",""]
[1467,1344,9,1,"9/8"," G","9/8. G","","Crassula perforate(2l)","No",1652,"","","","","06/12/2021 12:24:15",""]
[1468,1345,9,1,"9/8"," H","9/8. H","","Aloe ferox(2l)","No",146,"","","","","06/12/2021 12:24:24",""]
[1469,1346,9,1,"9/8"," I","9/8. I","","Aloe pluridens(2l)","No",130,"","","","","06/12/2021 12:24:33",""]
[1470,1347,9,1,"9/8"," J","9/8. J","","Aloe Africana(2l)","No",125,"","","","","06/12/2021 12:24:42",""]
[1471,1348,9,1,"9/8"," K","9/8. K","","Aloe speciosa(4l)","No",170,"","","","","06/12/2021 12:24:52",""]
[1472,1349,9,1,"9/8"," L","9/8. L","","Aloe striata(4l)","No",210,"","","","","06/12/2021 12:25:02",""]
[1473,13913,9,1,"9/8"," M","9/8. M","","Aloe arborescenes (2l)","No",80,"","","","","28/06/2023 10:22:27",""]
[1474,1350,9,1,"9/8"," N","9/8. N","","Delosperma sp(2l)","No",6239,"","","","","06/12/2021 12:25:12",""]
[1475,1351,9,1,"9/8"," O","9/8. O","","Delosprema ecklonis(2l)","No",6854,"","","","","06/12/2021 12:25:21",""]
[1476,1352,9,1,"9/8"," P","9/8. P","","Delosperma littoralis(2l)","No",6308,"","","","","06/12/2021 12:25:31",""]
[1477,1353,9,1,"9/8"," Q","9/8. Q","","Gasteria pulchra(plugs)","No",13363,"","","","","06/12/2021 12:25:41",""]
[1478,1354,9,1,"9/8"," R","9/8. R","","Sanseviera hyacinthoides(4l)","No",5110,"","","","","06/12/2021 12:25:50",""]
[1479,1044,9,1,"9/8","","9/8","","Ground covers","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 10:38:20",""]
[1480,1038,9,1,"9/8"," S","9/8. S","","Gazania krebsiana(4l)","No",347,"","","","","06/12/2021 12:26:19",""]
[1481,1355,9,1,"9/8"," T","9/8. T","","Carbobrotus edulis(4l)","No",2522,"","","","","06/12/2021 12:26:31",""]
[1482,1357,9,1,"9/8"," U","9/8. U","","Bulbine latifolia(10l)","No",935,"","","","","06/12/2021 12:26:41",""]
[1483,1358,9,1,"9/8"," V","9/8. V","","Bulbine frutescens(2l)","No",2617,"","","","","06/12/2021 12:26:50",""]
[1484,1359,9,1,"9/9"," A","9/9. A","","Plecthranthus grandidentatus(10l)","No",413,"","","","","06/12/2021 12:27:00",""]
[1485,1360,9,1,"9/9"," B","9/9. B","","Crassula expansa(4l)","No",3154,"","","","","06/12/2021 12:27:11",""]
[1486,1045,9,1,"9/9","","9/9","","Shade plants","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 10:38:38",""]
[1487,1361,9,1,"9/9"," C","9/9. C","","Clivia miniata(4l)","No",1442,"","","","","06/12/2021 12:27:20",""]
[1488,1362,9,1,"9/9"," D","9/9. D","","Crinum moorei(4l)","No",1442,"","","","","06/12/2021 12:27:30",""]
[1489,1363,9,1,"9/9"," E","9/9. E","","Haemanthus albiflos(4l)","No",826,"","","","","06/12/2021 12:27:59",""]
[1490,1364,9,1,"9/9"," F","9/9. F","","Plechthranthus dentatus(plugs)","No",12478,"","","","","06/12/2021 12:28:20",""]
[1491,1046,9,1,"9/9","","9/9","","Feature plants","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 10:38:52",""]
[1492,1365,9,1,"9/9"," G","9/9. G","","Strelitzia nicolai(4l)","No",3427,"","","","","06/12/2021 12:28:30",""]
[1493,1366,9,1,"9/9"," H","9/9. H","","Strelitzia reginae(4l)","No",3154,"","","","","06/12/2021 12:28:48",""]
[1494,1367,9,1,"9/9"," I","9/9. I","","Strelitzia juncea(4l)","No",3341,"","","","","06/12/2021 12:28:57",""]
[1495,1368,9,1,"9/9"," J","9/9. J","","Euphorbia species(plugs)","No",2440,"","","","","06/12/2021 12:29:08",""]
[1496,1378,9,1,"9/9","","9/9","","Planting in islands","H4",{"v":0,"d":"0.0"},"","","","","16/07/2012 03:15:58",""]
[1497,1379,9,1,"9/9"," K","9/9. K","","Euphorbia ingens - 3 meters","No",5,"","","","","06/12/2021 12:29:32",""]
[1498,1380,9,1,"9/9"," L","9/9. L","","Euphorbia ingens - 2 meters","No",12,"","","","","06/12/2021 12:29:47",""]
[1499,1381,9,1,"9/9"," M","9/9. M","","Euphorbia ingens - 1 meter","No",10,"","","","","06/12/2021 12:29:57",""]
[1500,1382,9,1,"9/9"," N","9/9. N","","Euphorbia tirucallii - 4kg","No",12,"","","","","06/12/2021 12:30:08",""]
[1501,1383,9,1,"9/9"," O","9/9. O","","Euphorbia tirucallii - 2kg","No",25,"","","","","06/12/2021 12:30:16",""]
[1502,1384,9,1,"9/9"," P","9/9. P","","Euphorbia millii - 2kg","No",35,"","","","","06/12/2021 12:30:26",""]
[1503,1385,9,1,"9/9"," Q","9/9. Q","","Aloe chabaudi - large","No",8,"","","","","06/12/2021 12:30:35",""]
[1504,1386,9,1,"9/9"," R","9/9. R","","Aloe chabaudi - medium","No",16,"","","","","06/12/2021 12:30:44",""]
[1505,1387,9,1,"9/9"," S","9/9. S","","Aloe vanbalenii - large","No",24,"","","","","06/12/2021 12:30:52",""]
[1506,1388,9,1,"9/9"," T","9/9. T","","Aloe vanbalenii - medium","No",25,"","","","","06/12/2021 12:31:02",""]
[1507,1389,9,1,"9/9"," U","9/9. U","","Euphorbia cooperii - 3 meters","No",8,"","","","","06/12/2021 12:31:10",""]
[1508,1390,9,1,"9/10"," A","9/10. A","","Euphorbia cooperii - 2 meters","No",24,"","","","","06/12/2021 12:31:19",""]
[1509,1391,9,1,"9/10"," B","9/10. B","","Euphorbia cooperii - 1 meter","No",35,"","","","","06/12/2021 12:31:31",""]
[1510,1393,9,1,"9/10"," C","9/10. C","","Pachypodium spp - 1 meter","No",14,"","","","","06/12/2021 12:31:40",""]
[1511,968,9,1,"9/10","","9/10","","Grassing","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 11:54:50",""]
[1512,1058,9,1,"9/10","","9/10","","Note : All sods to be free of weeds, and laid side to side and gaps filled in with topsoil.  Top of lawn levels to be 35mm below adjacent kerb or paving level.  Top-dress lawn area where instructed by the landscape architects (top-dressing material to be approved by the landscape architects).  Maintain until maintenance period commences","",{"v":0,"d":"0.0"},"","","","","19/07/2023 08:31:03",""]
[1513,1059,9,1,"9/10"," D","9/10. D","","\"Cynodon dactylon\" instant lawn","m2",3066,"","","","","06/12/2021 12:32:05",""]
[1514,1061,9,1,"9/10","","9/10","","Veld grass/meadow mixture","H3",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:55:45",""]
[1515,1062,9,1,"9/10","","9/10","","Specification :Seed to be of a approved quality.Apply Gromor (or similar) organic supplement @ 2.00 kg/ha to area to be grassed.Supply all materials to be hydraulically seeded with the specific grass mixture or alternatively supply and plant grass tufts to all areas to be grassed.Payment on 80% generation per m².  All grass to be a minimum of 300mm high.","",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:06:00",""]
[1516,3503,9,1,"9/10","","9/10","","Seed mixture: Veld grass mixture: 100% - Erogrostis tef 10% - Erogrostis curvula 10% - Cynodon dactylon 40% - Digitaria eriantha 10% - Chloris gayana 10% - Themeda triandra 10% - Heteropogon contortus 5% - Local grass mixture 5% Meadow mixture to be mixed into veldgrass mixture at a 100% rate. - Meadow mixture 100%","",{"v":0,"d":"0.0"},"","","","","11/08/2012 07:38:19",""]
[1517,1063,9,1,"9/10"," E","9/10. E","","Veld grass/meadow mix hydroseeding as described above","m2",23818,"","","","","27/01/2014 10:24:39",""]
[1518,13695,9,1,"9/10","","9/10","","\"Kaytech Enviromat\" biodegradable erosion control blanket","H3",{"v":0,"d":"0.0"},"","","","","10/12/2021 11:19:12",""]
[1519,8447,9,1,"9/10"," F","9/10. F","","To embankments","m2",4014,"","","","","10/12/2021 11:16:17",""]
[1520,1394,9,1,"9/11","","9/11","","Gravel and rocks","H3",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:55:37",""]
[1521,3506,9,1,"9/11","","9/11","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 07:59:53",""]
[1522,3507,9,1,"9/11"," A","9/11. A","","Over site between buildings, retaining walls etc., to reduce levels under gravel and rock filling, and dispose in prescribed stock piles on site","m3",110,"","","","","06/12/2021 12:33:42",""]
[1523,3508,9,1,"9/11","","9/11","","Extra over all excavations for carting away","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 07:59:54",""]
[1524,3509,9,1,"9/11"," B","9/11. B","","Surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",130,"","","","","11/08/2012 08:14:35",""]
[1525,3510,9,1,"9/11","","9/11","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 08:00:16",""]
[1526,3511,9,1,"9/11"," C","9/11. C","","Compaction of ground surfaces under pavings etc., including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",2738,"","","","","06/12/2021 12:34:11",""]
[1527,3518,9,1,"9/11","","9/11","","U22 non-woven continuous filament needle punch polyester filter fabric blanket","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 08:07:51",""]
[1528,3519,9,1,"9/11"," D","9/11. D","","Over stone percolation beds in flower boxes, etc.","m2",2838,"","","","","20/08/2012 07:19:45",""]
[1529,3512,9,1,"9/11","","9/11","","Stone filling","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 08:13:26",""]
[1530,3952,9,1,"9/11"," E","9/11. E","","11mm Diameter dark charcoal gravel layer 75mm thick, lightly compacted with a plate compactor","m3",105,"","","","","20/08/2012 07:13:14",""]
[1531,3953,9,1,"9/11"," F","9/11. F","","32mm Diameter dark charcoal gravel layer 75mm thick, lightly compacted with a plate compactor","m3",120,"","","","","20/08/2012 07:13:04",""]
[1532,3954,9,1,"9/11"," G","9/11. G","","100-150mm Diameter dark charcoal packed rock layer 150mm thick, lightly compacted with a plate compactor","m3",1,"","","","","20/08/2012 07:12:54",""]
[1533,6520,9,1,"9/11","","9/11","","Pebble covering obtained form the Gamtoos river area","H4",{"v":0,"d":"0.0"},"","","","","04/10/2012 10:58:48",""]
[1534,7115,9,1,"9/11"," H","9/11. H","","Covering of river stone pebbles varying in size from 20mm to 50mm diameter between stepping stones","m3",60,"","","","","27/06/2023 02:44:24",""]
[1535,6502,9,1,"9/11"," I","9/11. I","","Stepping stones laid on filling (elsewhere) in planted areas","No",70,"","","","","27/06/2023 02:44:37",""]
[1536,7229,9,1,"9/11","","9/11","","GARDEN AND EMBANKMENT EDGING","H3",{"v":0,"d":"0.0"},"","","","","28/06/2023 08:25:38",""]
[1537,13893,9,1,"9/12","","9/12","","\"PermaEdge\" 75mm high galvanised spiked garden edging in 1 000mm lengths, bent to shape, and fitted together with integral male and female interlocking ends","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 10:31:02",""]
[1538,13894,9,1,"9/12"," A","9/12. A","","To edges of flower beds","m",56,"","","","","27/06/2023 10:31:32",""]
[1539,11050,9,1,"9/12","","9/12","","\"PermaEdge\" 125mm high galvanised spiked garden edging in 1 000mm lengths, bent to shape, and fitted together with integral male and female interlocking ends","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 10:29:01",""]
[1540,7231,9,1,"9/12"," B","9/12. B","","To edges of flower beds","m",1297,"","","","","26/06/2023 01:17:47",""]
[1541,13900,9,1,"9/12","","9/12","","Timber bollards to hiking trail entrance","H4",{"v":0,"d":"0.0"},"","","","","28/06/2023 08:42:41",""]
[1542,13899,9,1,"9/12"," C","9/12. C","","2 100mm Overall length x 150mm nominal diameter CCA treated gumpole with the bottom 600mm set in and including 450mm diameter x 600mm deep 25MPa concrete base, including all excavations, sand blinding layer at bottom of base, carting away, etc.","No",19,"","","","","28/06/2023 01:12:11",""]
[1543,13903,9,1,"9/12","","9/12","","Timber post edging to sloped planters","H4",{"v":0,"d":"0.0"},"","","","","28/06/2023 08:43:31",""]
[1544,13904,9,1,"9/12"," D","9/12. D","","300mm High garden edging formed of 35mm nominal diameter black wattle or eucalyptus droppers tightly strung together with and including 3No 2mm dia. galvanised binding wire through drilled holes; the edging kept upright and in position by means of 450mm long spiked integral stakes driven into the ground at 500mm centres (replacing 300mm droppers)","m",770,"","","","","28/06/2023 09:01:33",""]
[1545,13898,9,1,"9/12","","9/12","","PLANT SUPPORTS","H3",{"v":0,"d":"0.0"},"","","","","28/06/2023 08:26:47",""]
[1546,13888,9,1,"9/12","","9/12","","GARDELI, or similar approved climbing aid set consisting of 4 x Stainless steel combined bracket and fixing screw, 4 x all purpose dowels, stainless steel Ø3mm x 5m wire rope, and 8 x PVC end caps, all installed as per manufacturer’s instructions (S37)","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 09:42:19",""]
[1547,13889,9,1,"9/12"," E","9/12. E","","Climbing aid set fixed to concrete or brickwork","No",25,"","","","","27/06/2023 09:59:44",""]
[1548,13890,9,1,"9/12"," F","9/12. F","","Climbing aid set fixed to flange of steel column","No",7,"","","","","27/06/2023 09:59:55",""]
[1549,13733,9,1,"9/12","","9/12","","SUNDRIES","H3",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:29:35",""]
[1550,13735,9,1,"9/12"," G","9/12. G","","Tree ring formed of 1 000mm diameter x 250mm high \"Rocla\", or similar approved precast concrete manhole rings and set in ground not exceeding 1 000mm deep, including all excavations, backfilling, etc.","No",12,"","","","","26/06/2023 12:32:20",""]
[1552,9488,9,2,"9/14","","9/14","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:31",""]
[1553,6213,9,2,"9/14","","9/14","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:06",""]
[1554,9489,9,2,"9/14","","9/14","","BILL NO. 2","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:06:44",""]
[1555,3923,9,2,"9/14","","9/14","","RE-INSTATEMENT OF DISTURBED ON-SITE AREAS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:48",""]
[1556,3932,9,2,"9/14","","9/14","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:47",""]
[1557,3933,9,2,"9/14","","9/14","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:45",""]
[1558,3934,9,2,"9/14","","9/14","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:47",""]
[1559,3935,9,2,"9/14","","9/14","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:48",""]
[1560,3936,9,2,"9/14","","9/14","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:48",""]
[1561,3955,9,2,"9/14","","9/14","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 07:34:01",""]
[1562,3956,9,2,"9/14","","9/14","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\"","",{"v":0,"d":"0.0"},"","","","","01/10/2012 03:34:54",""]
[1563,3957,9,2,"9/14","","9/14","","Plants need to be installed as per plans All plants needed can be either grown and maintained at the contractors own nursery or sourced from any other nursery, but must adhere to the sizes and quality as specified in the tender document at the time of installation.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 07:34:02",""]
[1564,3958,9,2,"9/14","","9/14","","All plants to be free from any damage, parasites, fungus or any other plant diseases or insects. No container bound plants will be acceptable.All leaves to be dust free.All plants are to be viewed and approved by the Landscape Architect before planting.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 07:34:02",""]
[1565,3959,9,2,"9/15","","9/15","","All plants must be transported to the site in trucks with closed canopies. Plants in transit may not be exposed to wind or any other harmful elements. Plants need to be watered regularly as for the specific needs of each species. No pot bound roots will be accepted.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 07:34:02",""]
[1566,3960,9,2,"9/15","","9/15","","Plants must be well rooted and well established. The nursery must be clean and presentable, with suiatble growing conditions established for growing of the plants. All plants to be planted in a grid/diamond pattern in perfectly straight lines. All existing trees encountered to be neatly pruned.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 07:34:03",""]
[1567,13795,9,2,"9/15","","9/15","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:03:43",""]
[1568,7265,9,2,"9/15","","9/15","","Note : This section is intended for work to be carried out in areas where vegetation has been discturbed by the installation of electrical and water services, and mainly occurs adjacent to the demarcated site","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:38:42",""]
[1569,7270,9,2,"9/15","","9/15","","Earthworks","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:45:15",""]
[1570,7267,9,2,"9/15","","9/15","","Precision shaping of landscape areas and earth mounds","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:44:30",""]
[1571,7269,9,2,"9/15"," A","9/15. A","","Precision shaping of landscape areas and earth mounds by means of accurate levels taken with a dumpy level, and adjustment of levels to ensure a level appearance","m2",4777,"","","","","19/10/2012 10:44:31",""]
[1572,7273,9,2,"9/15","","9/15","","Ground preparation","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:30",""]
[1573,7274,9,2,"9/16","","9/16","","Cultivation, including ripping and machine rotivating by breaking up earth to a depth of 300mm at 300mm centres in both directions, and preparation of areas to be planted","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:31",""]
[1574,7275,9,2,"9/16"," A","9/16. A","","Shrubs and groundcover areas","m2",1800,"","","","","28/06/2023 03:48:55",""]
[1575,7276,9,2,"9/16"," B","9/16. B","","Veld areas","m2",5541,"","","","","28/06/2023 03:48:58",""]
[1576,7277,9,2,"9/16","","9/16","","Fine grading","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:31",""]
[1577,7278,9,2,"9/16","","9/16","","Ensure that all areas to be planted are compacted sufficiently to avoid any subsidence later on, and that surface to be planted does not exceed a tolerance of 30mm in height when measured from the basic topographical line","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:26:51",""]
[1578,7279,9,2,"9/16"," C","9/16. C","","Shrubs and groundcover areas.","m2",1800,"","","","","28/06/2023 03:49:08",""]
[1579,7280,9,2,"9/16"," D","9/16. D","","Veld areas","m2",5541,"","","","","19/07/2023 08:26:16",""]
[1580,7281,9,2,"9/16","","9/16","","Topsoil","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:31",""]
[1581,7282,9,2,"9/16","","9/16","","Topsoil shall vary between sandy loamy soil and sandy clayey soil with a ideal ratio of 15% to 25% clay, 10% Silt/Sludge and 65% to 75% sand, with a minimum ratio of organic material of 2% of volume. All material shall be free of harmful deposits such as salts, weed seeds and waste of any kind","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:26:58",""]
[1582,7283,9,2,"9/16"," E","9/16. E","","Imported topsoil supplied by the contractor and spreading and levelling on site, filling plant and tree holes, etc.","m3",761,"","","","","19/10/2012 10:55:32",""]
[1583,7284,9,2,"9/16"," F","9/16. F","","Topsoil from stock piles on site and spreading and levelling on site, filling plant and tree holes, etc.","m3",290,"","","","","06/12/2021 12:34:58",""]
[1584,7288,9,2,"9/16","","9/16","","Compost","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:32",""]
[1585,7289,9,2,"9/16","","9/16","","Properly decayed organic material, free from harmful deposits, salts, seeds and other waste material, with a pH of more than 4 and less than 7","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:27:05",""]
[1586,7383,9,2,"9/16"," G","9/16. G","","In tree holes, shrub and groundcover areas","m3",59,"","","","","06/12/2021 12:35:24",""]
[1587,7291,9,2,"9/16","","9/16","","Organic Fertilizers","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:33",""]
[1588,7292,9,2,"9/17","","9/17","","Fertilizers shall be of the type specified, mixed thoroughly into the soil as prescribed. No fertilizer shall be added more than two weeks prior to planting.All fertilizers to areas to be grassed shall be strewn on the final layer before the final finishing is commenced and worked mechanically into the top 150 mm soil","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:33",""]
[1589,7293,9,2,"9/17"," A","9/17. A","","2:3:2 In tree holes","kg",4,"","","","","10/12/2021 03:01:47",""]
[1590,7294,9,2,"9/17"," B","9/17. B","","2:3:2 In shrubs and groundcover areas","kg",90,"","","","","10/12/2021 03:01:58",""]
[1591,7295,9,2,"9/17"," C","9/17. C","","2:3:2 In lawn areas","kg",150,"","","","","10/12/2021 03:02:18",""]
[1592,7296,9,2,"9/17","","9/17","","Trees and aloes","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:33",""]
[1593,7297,9,2,"9/17","","9/17","","Note : Trees (Tree stakes included, 2 per 50l,100l trees and 4 per 200 and 400l trees) The height of the trees shall be measured from the top of the root ball to the top of the tree. Where trees are pruned, such prune wounds shall not be more than 25mm in diameter and be sealed with an approved sealing compound.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:33",""]
[1594,7298,9,2,"9/17","","9/17","","400l trees : min. 5 000mm tall, with a stem diameter of 450mm and a crown width of 3 diameters. 200l trees : min. 3 800mm stem height; 2 200mm crown spread after planting, with a stem diameter of 200mm measured 300mm above soil level. 100l trees : min. 2 800mm stem height; 1 800mm crown spread after planting, with a stem diameter of 40mm measured 300mm above soil level. 50l trees : min. 2 400mm stem height; 1 400mm crown spread after planting, with a stem diameter of 30mm measured 300mm above soil level.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:33",""]
[1595,7299,9,2,"9/17"," D","9/17. D","","Olea africana(200l)","No",5,"","","","","28/06/2023 03:50:32",""]
[1596,7300,9,2,"9/17"," E","9/17. E","","Ocotea bullata(100l)","No",6,"","","","","28/06/2023 03:50:24",""]
[1597,7301,9,2,"9/17"," F","9/17. F","","Erythrina caffra(400l)","No",4,"","","","","28/06/2023 03:50:39",""]
[1598,7302,9,2,"9/17"," G","9/17. G","","Sideroxylon inerme(100l)","No",7,"","","","","28/06/2023 03:49:54",""]
[1599,7303,9,2,"9/17"," H","9/17. H","","Protorhus longifolia(100l)","No",9,"","","","","28/06/2023 03:50:17",""]
[1600,7304,9,2,"9/17"," I","9/17. I","","Calodendron capense(100l)","No",3,"","","","","28/06/2023 03:50:03",""]
[1601,7305,9,2,"9/17"," J","9/17. J","","Milletia grandis(100l)","No",2,"","","","","28/06/2023 03:50:12",""]
[1602,7306,9,2,"9/18","","9/18","","Shrubs and ground covers","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:34",""]
[1603,7307,9,2,"9/18","","9/18","","Note :Shrubs and groundcovers shall meet the requirements for height and spread as specified below and in specifications. Thin or sparsely-branched plants will not be accepted. Plants shall be well rooted (especially plugs), well-spread with ample young branches and the plant as a whole shall be well grown. Only vigorous full growing plants will be accepted.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:34",""]
[1604,7308,9,2,"9/18","","9/18","","Cuttings = to be well rooted and well established. 2kg/lt = 250mm stem lengths and well established. 4kg/lt = 350mm stem lengths and well established. Plugs = to be well rooted and well established.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:34",""]
[1605,7309,9,2,"9/18","","9/18","","Shrubs","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:35",""]
[1606,7310,9,2,"9/18"," A","9/18. A","","Carissa bispinosa(2l)","No",504,"","","","","06/12/2021 12:36:25",""]
[1607,7311,9,2,"9/18"," B","9/18. B","","Portulacaria affra(2l)","No",378,"","","","","06/12/2021 12:36:33",""]
[1608,7312,9,2,"9/18"," C","9/18. C","","Cussonia thyrsifolia(2l)","No",630,"","","","","06/12/2021 12:36:41",""]
[1609,7313,9,2,"9/18"," D","9/18. D","","Maytenus procumbens(4l)","No",216,"","","","","06/12/2021 12:36:50",""]
[1610,7314,9,2,"9/18"," E","9/18. E","","Rhus glauca(4l)","No",144,"","","","","06/12/2021 12:36:58",""]
[1611,7315,9,2,"9/18"," F","9/18. F","","Rhus crenata(4l)","No",216,"","","","","06/12/2021 12:37:08",""]
[1612,7316,9,2,"9/18"," G","9/18. G","","Rhus pallens(2l)","No",756,"","","","","06/12/2021 12:37:18",""]
[1613,7317,9,2,"9/18","","9/18","","Succulents","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:36",""]
[1614,7318,9,2,"9/18"," H","9/18. H","","Euphorbia triagularis(Plugs)","No",1080,"","","","","06/12/2021 12:38:05",""]
[1615,7319,9,2,"9/18"," I","9/18. I","","Euphorbia caerulucens(2l)","No",1008,"","","","","06/12/2021 12:38:13",""]
[1616,7320,9,2,"9/18"," J","9/18. J","","Crassula ovate(2l)","No",378,"","","","","06/12/2021 12:38:21",""]
[1617,7321,9,2,"9/18"," K","9/18. K","","Cotyledon orbiculata(4l)","No",144,"","","","","06/12/2021 12:38:29",""]
[1618,7322,9,2,"9/18"," L","9/18. L","","Cotyledon campanulata(2l)","No",756,"","","","","06/12/2021 12:38:38",""]
[1619,7323,9,2,"9/18"," M","9/18. M","","Crassula muscosa(4l)","No",144,"","","","","06/12/2021 12:38:48",""]
[1620,7324,9,2,"9/18"," N","9/18. N","","Crassula perfoliata(2l)","No",126,"","","","","06/12/2021 12:38:57",""]
[1621,7325,9,2,"9/19"," A","9/19. A","","Crassula perforate(2l)","No",504,"","","","","06/12/2021 12:39:06",""]
[1622,7326,9,2,"9/19"," B","9/19. B","","Aloe ferox(2l)","No",630,"","","","","06/12/2021 12:39:14",""]
[1623,7327,9,2,"9/19"," C","9/19. C","","Aloe pluridens(2l)","No",504,"","","","","06/12/2021 12:39:23",""]
[1624,7328,9,2,"9/19"," D","9/19. D","","Aloe Africana(2l)","No",378,"","","","","06/12/2021 12:39:38",""]
[1625,7329,9,2,"9/19"," E","9/19. E","","Aloe speciosa(4l)","No",144,"","","","","06/12/2021 12:39:47",""]
[1626,7330,9,2,"9/19"," F","9/19. F","","Aloe striata(4l)","No",72,"","","","","06/12/2021 12:39:55",""]
[1627,7331,9,2,"9/19","","9/19","","Ground covers","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:55:37",""]
[1628,7332,9,2,"9/19"," G","9/19. G","","Gazania krebsiana(4l)","No",72,"","","","","06/12/2021 12:40:06",""]
[1629,7333,9,2,"9/19"," H","9/19. H","","Carbobrotus edulis(4l)","No",360,"","","","","06/12/2021 12:40:18",""]
[1630,7334,9,2,"9/19"," I","9/19. I","","Carbobrotus deliciosus(4l)","No",288,"","","","","06/12/2021 12:40:26",""]
[1631,7335,9,2,"9/19"," J","9/19. J","","Bulbine latifolia(10l)","No",216,"","","","","06/12/2021 12:40:45",""]
[1632,7336,9,2,"9/19"," K","9/19. K","","Bulbine frutescens(2l)","No",756,"","","","","06/12/2021 12:40:54",""]
[1633,7337,9,2,"9/19"," L","9/19. L","","Plecthranthus grandidentatus(10l)","No",108,"","","","","06/12/2021 12:41:03",""]
[1634,7338,9,2,"9/19"," M","9/19. M","","Crassula expansa(4l)","No",216,"","","","","06/12/2021 12:41:12",""]
[1635,7339,9,2,"9/19","","9/19","","Veld grass/meadow mixture","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:56:07",""]
[1636,7340,9,2,"9/19","","9/19","","Specification :Seed to be of a approved quality.Apply Gromor (or similar) organic supplement @ 2.00 kg/ha to area to be grassed.Supply all materials to be hydraulically seeded with the specific grass mixture or alternatively supply and plant grass tufts to all areas to be grassed.Payment on 80% generation per m².  All grass to be a minimum of 300mm high.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:56:07",""]
[1637,7341,9,2,"9/20","","9/20","","Seed mixture: Veld grass mixture: 100% - Erogrostis tef 10% - Erogrostis curvula 10% - Cynodon dactylon 40% - Digitaria eriantha 10% - Chloris gayana 10% - Themeda triandra 10% - Heteropogon contortus 5% - Local grass mixture 5% Meadow mixture to be mixed into veldgrass mixture at a 100% rate. - Meadow mixture 100%","",{"v":0,"d":"0.0"},"","","","","19/10/2012 11:15:13",""]
[1638,7342,9,2,"9/20"," A","9/20. A","","Veld grass/meadow mix hydroseeding as described above","m2",5541,"","","","","27/02/2014 08:50:07",""]
[1640,9490,9,3,"9/22","","9/22","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:35",""]
[1641,7441,9,3,"9/22","","9/22","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:10",""]
[1642,9491,9,3,"9/22","","9/22","","BILL NO. 3","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:07:05",""]
[1643,7443,9,3,"9/22","","9/22","","RE-INSTATEMENT OF DISTURBED BYPASS ROAD AREAS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:53",""]
[1644,7444,9,3,"9/22","","9/22","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:24",""]
[1645,7445,9,3,"9/22","","9/22","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:50",""]
[1646,7446,9,3,"9/22","","9/22","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1647,7447,9,3,"9/22","","9/22","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1648,7448,9,3,"9/22","","9/22","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1649,7449,9,3,"9/22","","9/22","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1650,7450,9,3,"9/22","","9/22","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\"","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1651,7451,9,3,"9/22","","9/22","","Plants need to be installed as per plans All plants needed can be either grown and maintained at the contractors own nursery or sourced from any other nursery, but must adhere to the sizes and quality as specified in the tender document at the time of installation.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1652,7452,9,3,"9/22","","9/22","","All plants to be free from any damage, parasites, fungus or any other plant diseases or insects. No container bound plants will be acceptable.All leaves to be dust free.All plants are to be viewed and approved by the Landscape Architect before planting.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1653,7453,9,3,"9/23","","9/23","","All plants must be transported to the site in trucks with closed canopies. Plants in transit may not be exposed to wind or any other harmful elements. Plants need to be watered regularly as for the specific needs of each species. No pot bound roots will be accepted.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:25",""]
[1654,7454,9,3,"9/23","","9/23","","Plants must be well rooted and well established. The nursery must be clean and presentable, with suitable growing conditions established for growing of the plants. All plants to be planted in a grid/diamond pattern in perfectly straight lines. All existing trees encountered to be neatly pruned.","",{"v":0,"d":"0.0"},"","","","","10/06/2013 04:09:19",""]
[1655,13796,9,3,"9/23","","9/23","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:03:50",""]
[1656,7455,9,3,"9/23","","9/23","","Note : This section is intended for work to be carried out in areas where vegetation has been disturbed by the installation of electrical and water services, and mainly occurs adjacent to the demarcated site","",{"v":0,"d":"0.0"},"","","","","10/06/2013 04:10:21",""]
[1657,7464,9,3,"9/23","","9/23","","Earthworks","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:26",""]
[1658,7470,9,3,"9/23","","9/23","","Ground preparation","H4",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:26",""]
[1659,7471,9,3,"9/23","","9/23","","Cultivation, including ripping and machine rotivating by breaking up earth to a depth of 300mm at 300mm centres in both directions, and preparation of areas to be planted","H4",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:26",""]
[1660,7472,9,3,"9/23"," A","9/23. A","","Shrubs and groundcover areas","m2",418,"","","","","25/10/2012 07:19:26",""]
[1661,7473,9,3,"9/23"," B","9/23. B","","Veld areas","m2",1139,"","","","","25/10/2012 07:19:26",""]
[1662,7474,9,3,"9/24","","9/24","","Fine grading","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:26",""]
[1663,7475,9,3,"9/24","","9/24","","Ensure that all areas to be planted are compacted sufficiently to avoid any subsidence later on, and that surface to be planted does not exceed a tolerance of 30mm in height when measured from the basic topographical line","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:29:16",""]
[1664,7476,9,3,"9/24"," A","9/24. A","","Shrubs and groundcover areas","m2",418,"","","","","10/12/2021 08:29:48",""]
[1665,7477,9,3,"9/24"," B","9/24. B","","Veld areas","m2",1139,"","","","","10/12/2021 08:29:55",""]
[1666,7478,9,3,"9/24","","9/24","","Topsoil","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:27",""]
[1667,7479,9,3,"9/24","","9/24","","Topsoil shall vary between sandy loamy soil and sandy clayey soil with a ideal ratio of 15% to 25% clay, 10% silt/sludge and 65% to 75% sand, with a minimum ratio of organic material of 2% of volume. All material shall be free of harmful deposits such as salts, weed seeds and waste of any kind.","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:03:30",""]
[1668,7480,9,3,"9/24"," C","9/24. C","","Imported topsoil supplied by the contractor and spreading and levelling on site, filling plant and tree holes, etc.","m3",103,"","","","","25/10/2012 07:19:27",""]
[1669,7481,9,3,"9/24"," D","9/24. D","","Topsoil from stock piles on site and spreading and levelling on site, filling plant and tree holes, etc.","m3",91,"","","","","06/12/2021 12:41:46",""]
[1670,7485,9,3,"9/24","","9/24","","Organic Fertilizers","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:27",""]
[1671,7486,9,3,"9/24","","9/24","","Fertilizers shall be of the type specified, mixed thoroughly into the soil as prescribed. No fertilizer shall be added more than two weeks prior to planting.All fertilizers to areas to be grassed shall be strewn on the final layer before the final finishing is commenced and worked mechanically into the top 150 mm soil","H4",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:27",""]
[1672,7487,9,3,"9/24"," E","9/24. E","","2:3:2 In tree holes","kg",1,"","","","","10/12/2021 03:02:56",""]
[1673,7489,9,3,"9/24"," F","9/24. F","","2:3:2 In lawn areas","kg",71,"","","","","10/12/2021 03:03:05",""]
[1674,7490,9,3,"9/24","","9/24","","Trees and aloes","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:27",""]
[1675,7491,9,3,"9/24","","9/24","","Note : Trees (Tree stakes included, 2 per 50l,100l trees and 4 per 200 and 400l trees) The height of the trees shall be measured from the top of the root ball to the top of the tree. Where trees are pruned, such prune wounds shall not be more than 25mm in diameter and be sealed with an approved sealing compound.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:27",""]
[1676,7492,9,3,"9/25","","9/25","","400l trees : min. 5 000mm tall, with a stem diameter of 450mm and a crown width of 3 diameters. 200l trees : min. 3 800mm stem height; 2 200mm crown spread after planting, with a stem diameter of 200mm measured 300mm above soil level. 100l trees : min. 2 800mm stem height; 1 800mm crown spread after planting, with a stem diameter of 40mm measured 300mm above soil level. 50l trees : min. 2 400mm stem height; 1 400mm crown spread after planting, with a stem diameter of 30mm measured 300mm above soil level.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:27",""]
[1677,7496,9,3,"9/25"," A","9/25. A","","Sideroxylon inerme(100l)","No",1,"","","","","06/12/2021 12:43:24",""]
[1678,7498,9,3,"9/25"," B","9/25. B","","Calodendron capense(100l)","No",3,"","","","","06/12/2021 12:43:33",""]
[1679,7499,9,3,"9/25"," C","9/25. C","","Milletia grandis(100l)","No",1,"","","","","06/12/2021 12:43:44",""]
[1680,7500,9,3,"9/25","","9/25","","Shrubs and ground covers","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:28",""]
[1681,7501,9,3,"9/25","","9/25","","Note :Shrubs and groundcovers shall meet the requirements for height and spread as specified below and in specifications. Thin or sparsely-branched plants will not be accepted. Plants shall be well rooted (especially plugs), well-spread with ample young branches and the plant as a whole shall be well grown. Only vigorous full growing plants will be accepted.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:28",""]
[1682,7502,9,3,"9/25","","9/25","","Cuttings = to be well rooted and well established. 2kg/lt = 250mm stem lengths and well established. 4kg/lt = 350mm stem lengths and well established. Plugs = to be well rooted and well established.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:28",""]
[1683,7503,9,3,"9/25","","9/25","","Shrubs","H4",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:28",""]
[1684,7504,9,3,"9/25"," D","9/25. D","","Carissa bispinosa(2l)","No",1800,"","","","","28/06/2023 03:52:42",""]
[1685,7505,9,3,"9/25"," E","9/25. E","","Portulacaria affra(2l)","No",5000,"","","","","06/12/2021 12:44:07",""]
[1686,7533,9,3,"9/26","","9/26","","Veld grass/meadow mixture","H3",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:30",""]
[1687,7534,9,3,"9/26","","9/26","","Specification :Seed to be of a approved quality.Apply Gromor (or similar) organic supplement @ 2.00 kg/ha to area to be grassed.Supply all materials to be hydraulically seeded with the specific grass mixture or alternatively supply and plant grass tufts to all areas to be grassed.Payment on 80% generation per m².  All grass to be a minimum of 300mm high.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:30",""]
[1688,7535,9,3,"9/26","","9/26","","Seed mixture: Veld grass mixture: 100% - Erogrostis tef 10% - Erogrostis curvula 10% - Cynodon dactylon 40% - Digitaria eriantha 10% - Chloris gayana 10% - Themeda triandra 10% - Heteropogon contortus 5% - Local grass mixture 5% Meadow mixture to be mixed into veldgrass mixture at a 100% rate. - Meadow mixture 100%","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:19:30",""]
[1689,7536,9,3,"9/26"," A","9/26. A","","Veld grass/meadow mix hydroseeding as described above","m2",1353,"","","","","27/02/2014 08:51:23",""]
[1691,9492,9,4,"9/28","","9/28","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:39",""]
[1692,7234,9,4,"9/28","","9/28","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:14",""]
[1693,9493,9,4,"9/28","","9/28","","BILL NO. 4","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:07:25",""]
[1694,7236,9,4,"9/28","","9/28","","VEGETATION REHABILITATION, SEARCH AND RESCUE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:22:59",""]
[1695,7237,9,4,"9/28","","9/28","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:44",""]
[1696,7238,9,4,"9/28","","9/28","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:38:55",""]
[1697,7239,9,4,"9/28","","9/28","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:44",""]
[1698,7240,9,4,"9/28","","9/28","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:44",""]
[1699,7241,9,4,"9/28","","9/28","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1700,7242,9,4,"9/28","","9/28","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1701,7243,9,4,"9/28","","9/28","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\"","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1702,7244,9,4,"9/28","","9/28","","Plants need to be installed as per plans All plants needed can be either grown and maintained at the contractors own nursery or sourced from any other nursery, but must adhere to the sizes and quality as specified in the tender document at the time of installation.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1703,7245,9,4,"9/28","","9/28","","All plants to be free from any damage, parasites, fungus or any other plant diseases or insects. No container bound plants will be acceptable.All leaves to be dust free.All plants are to be viewed and approved by the Landscape Architect before planting.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1704,7246,9,4,"9/29","","9/29","","All plants must be transported to the site in trucks with closed canopies. Plants in transit may not be exposed to wind or any other harmful elements. Plants need to be watered regularly as for the specific needs of each species. No pot bound roots will be accepted.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1705,7247,9,4,"9/29","","9/29","","Plants must be well rooted and well established. The nursery must be clean and presentable, with suiatble growing conditions established for growing of the plants. All plants to be planted in a grid/diamond pattern in perfectly straight lines. All existing trees encountered to be neatly pruned.","",{"v":0,"d":"0.0"},"","","","","19/10/2012 10:20:45",""]
[1706,13797,9,4,"9/29","","9/29","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:03:57",""]
[1707,7351,9,4,"9/29","","9/29","","TEMPORARY STORAGE","H2",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:17:45",""]
[1708,7352,9,4,"9/29","","9/29","","Holding nursery (Open ground)","H4",{"v":0,"d":"0.0"},"","","","","01/11/2021 12:52:17",""]
[1709,7353,9,4,"9/29"," A","9/29. A","","Supply and maintain nursery as per specification, for the duration of the contract","Item",{"v":1,"d":"1.00"},"","","","","19/10/2012 02:20:14",""]
[1710,7354,9,4,"9/29","","9/29","","Holding facility (Protected cover)","H4",{"v":0,"d":"0.0"},"","","","","01/11/2021 12:52:24",""]
[1711,7355,9,4,"9/29"," B","9/29. B","","Supply and maintain holding facility as per specification, for the duration of the contract","Item",{"v":1,"d":"1.00"},"","","","","01/11/2021 02:49:12",""]
[1712,12047,9,4,"9/29","","9/29","","SITE CLEARANCE, ETC.","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 04:10:42",""]
[1713,12048,9,4,"9/29"," C","9/29. C","","Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc. and trees not exceeding 200mm girth. Note - the removal, and protection, of sensitive vegetation has been allowed for in the Landscaping section","m2",3509,"","","","","07/12/2021 02:11:23",""]
[1714,7356,9,4,"9/30","","9/30","","EARTHWORKS","H2",{"v":0,"d":"0.0"},"","","","","01/11/2021 12:55:33",""]
[1715,7357,9,4,"9/30","","9/30","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting planting areas in maximum 300mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:22:08",""]
[1716,7358,9,4,"9/30"," A","9/30. A","","General shaping of landscaped areas","m3",401,"","","","","19/10/2012 02:22:09",""]
[1717,7359,9,4,"9/30","","9/30","","Precision shaping of landscape areas and earth mounds","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:22:09",""]
[1718,7360,9,4,"9/30"," B","9/30. B","","Allow for the use of a dumpy level throughout","SUM",1,"","","","","22/10/2012 08:59:47",""]
[1719,7362,9,4,"9/30","","9/30","","EARTHWORKS AND COMPOSTING","H2",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:36:48",""]
[1720,7375,9,4,"9/30","","9/30","","Compost","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:24:56",""]
[1721,7376,9,4,"9/30","","9/30","","Properly decayed organic material, free from harmful deposits, salts, seeds and other waste material, with a pH of more than 4 and less than 7","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 08:35:51",""]
[1722,7382,9,4,"9/30"," C","9/30. C","","In tree holes, shrub and groundcover areas","m3",201,"","","","","19/10/2012 02:29:36",""]
[1723,7378,9,4,"9/30","","9/30","","Organic Fertilizers","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:24:57",""]
[1724,7379,9,4,"9/30","","9/30","","Fertilizers shall be of the type specified, mixed thoroughly into the soil as prescribed. No fertilizer shall be added more than two weeks prior to planting.All fertilizers to areas to be grassed shall be strewn on the final layer before the final finishing is commenced and worked mechanically into the top 150 mm soil","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:24:57",""]
[1725,7380,9,4,"9/30"," D","9/30. D","","2:3:2 In tree holes","kg",64,"","","","","26/06/2023 12:33:32",""]
[1726,7385,9,4,"9/30","","9/30","","Mulch","H3",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:32:49",""]
[1727,13895,9,4,"9/30"," E","9/30. E","","Mulch, as per specification","m3",217,"","","","","27/06/2023 11:56:56",""]
[1728,7387,9,4,"9/31","","9/31","","PLANTING","H2",{"v":0,"d":"0.0"},"","","","","19/10/2012 02:37:09",""]
[1729,7404,9,4,"9/31","","9/31","","When transplanting rootball still to be intact. Prune 40% of leaves back. Plant still to retain natural character. Contractor to ensure that plant will not get ring barked.  Plant to be properly bagged with hessian bag and wire basket.  Plants to be replanted in newly indicated spots when appropriate.  Contractor to guarantee all plants.  Contractor to repair areas where plants are transplanted from in order to have the same appearance as the surroundings. Payment upon landscape architects approval.","",{"v":0,"d":"0.0"},"","","","","25/10/2012 07:42:00",""]
[1730,7395,9,4,"9/31","","9/31","","Plants to be transplanted from an on-site location to a different location on site. (The complete plant)","H4",{"v":0,"d":"0.0"},"","","","","22/10/2012 09:08:40",""]
[1731,7388,9,4,"9/31"," A","9/31. A","","Plant height: 0mm - 100mm","No",526,"","","","","01/11/2021 02:34:52",""]
[1732,7389,9,4,"9/31"," B","9/31. B","","Plant height: 100mm - 500mm","No",421,"","","","","01/11/2021 02:34:56",""]
[1733,7390,9,4,"9/31"," C","9/31. C","","Plant height: 500mm - 1,000mm","No",351,"","","","","01/11/2021 02:35:01",""]
[1734,7391,9,4,"9/31"," D","9/31. D","","Plant height: 1 000mm - 1 500mm","No",281,"","","","","01/11/2021 02:35:17",""]
[1735,7392,9,4,"9/31"," E","9/31. E","","Plant height: 1 500mm - 2 500mm","No",211,"","","","","01/11/2021 02:35:34",""]
[1736,7394,9,4,"9/31"," F","9/31. F","","Plant height: 2 500mm - 4 000mm","No",140,"","","","","01/11/2021 02:35:52",""]
[1737,7393,9,4,"9/31"," G","9/31. G","","Plant height: 4 000mm and higher","No",35,"","","","","01/11/2021 02:36:12",""]
[1738,7396,9,4,"9/31","","9/31","","Plants to be transplanted from an onsite location to an on-site nursery and replanted when appropriate (The complete plant)","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:05:18",""]
[1739,7397,9,4,"9/31"," H","9/31. H","","Plant height: 0mm - 100mm","No",526,"","","","","01/11/2021 02:37:38",""]
[1740,7398,9,4,"9/31"," I","9/31. I","","Plant height: 100mm - 500mm","No",421,"","","","","01/11/2021 02:37:28",""]
[1741,7399,9,4,"9/31"," J","9/31. J","","Plant height: 500mm - 1,000mm","No",351,"","","","","01/11/2021 02:37:16",""]
[1742,7400,9,4,"9/31"," K","9/31. K","","Plant height: 1 000mm - 1 500mm","No",281,"","","","","01/11/2021 02:37:06",""]
[1743,7401,9,4,"9/31"," L","9/31. L","","Plant height: 1 500mm - 2 500mm","No",211,"","","","","01/11/2021 02:36:52",""]
[1744,7402,9,4,"9/31"," M","9/31. M","","Plant height: 2 500mm - 4 000mm","No",140,"","","","","01/11/2021 02:36:41",""]
[1745,7403,9,4,"9/32"," A","9/32. A","","Plant height: 4 000mm and higher","No",35,"","","","","01/11/2021 02:36:25",""]
[1746,7405,9,4,"9/32","","9/32","","Cuttings of plants to be rescued to a on site nursery and replanted when appropriate","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:05:25",""]
[1747,7406,9,4,"9/32"," B","9/32. B","","Plant height: 0mm - 100mm","No",500,"","","","","01/11/2021 02:38:00",""]
[1748,7407,9,4,"9/32"," C","9/32. C","","Plant height: 100mm - 500mm","No",300,"","","","","01/11/2021 02:38:19",""]
[1749,7408,9,4,"9/32"," D","9/32. D","","Plant height: 500mm - and higher","No",200,"","","","","01/11/2021 02:38:35",""]
[1750,7409,9,4,"9/32","","9/32","","Seed harvesting of plants to be mixed in the hydroseeding mixture","H4",{"v":0,"d":"0.0"},"","","","","19/10/2012 03:10:15",""]
[1751,7410,9,4,"9/32"," E","9/32. E","","Harvesting as per specification","kg",5,"","","","","19/10/2012 03:11:08",""]
[1752,12599,9,4,"9/32","","9/32","","PERMITS","H2",{"v":0,"d":"0.0"},"","","","","12/11/2021 08:30:05",""]
[1753,12600,9,4,"9/32"," F","9/32. F","","Allow for permits for all landscaping requirements as per Landscape Architects specifications","Item",{"v":1,"d":"1.00"},"","","","","10/12/2021 03:05:45",""]
[1755,9494,9,5,"9/34","","9/34","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:43",""]
[1756,6214,9,5,"9/34","","9/34","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:18",""]
[1757,9495,9,5,"9/34","","9/34","","BILL NO. 5","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:07:46",""]
[1758,3946,9,5,"9/34","","9/34","","IRRIGATION SYSTEM","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:04",""]
[1759,3947,9,5,"9/34","","9/34","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:57:21",""]
[1760,3948,9,5,"9/34","","9/34","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:00",""]
[1761,3949,9,5,"9/34","","9/34","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:57:21",""]
[1762,3950,9,5,"9/34","","9/34","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:57:21",""]
[1763,3951,9,5,"9/34","","9/34","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:57:21",""]
[1764,4098,9,5,"9/34","","9/34","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","24/08/2012 09:23:51",""]
[1765,4099,9,5,"9/34","","9/34","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\"","",{"v":0,"d":"0.0"},"","","","","01/10/2012 03:40:42",""]
[1766,13798,9,5,"9/35","","9/35","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:04:07",""]
[1767,986,9,5,"9/35","","9/35","","IRRIGATION SYSTEM","H2",{"v":0,"d":"0.0"},"","","","","04/06/2012 08:07:52",""]
[1768,1484,9,5,"9/35","","9/35","","Water connection point installation","H3",{"v":0,"d":"0.0"},"","","","","11/08/2012 02:30:46",""]
[1769,4052,9,5,"9/35"," A","9/35. A","","65mm Galvanised barrel nipple","No",1,"","","","","26/06/2023 02:48:15",""]
[1770,1487,9,5,"9/35"," B","9/35. B","","80mm \"Nelson 800\", or equal approved, series pressure reducing valve","No",1,"","","","","26/06/2023 02:51:43",""]
[1771,4054,9,5,"9/35"," C","9/35. C","","Grundfos, or equal approved, Hydro Multi-E 2 CRE 15-7 7,5kW pump set (Prime Cost R420 000.00 excl. VAT supply only), complete including all switchgear (electrical supply measured elsewhere)","No",1,"","","","","28/06/2023 03:14:27",""]
[1772,4056,9,5,"9/35"," D","9/35. D","","Manifold for above pump set","No",1,"","","","","27/02/2014 08:53:44",""]
[1773,4055,9,5,"9/35"," E","9/35. E","","Grundfos, or equal approved, 450l pressure tank","No",1,"","","","","29/06/2023 08:35:18",""]
[1774,4053,9,5,"9/35"," F","9/35. F","","SPIN-KLIN JASPER PP 2 130 micron filter bank","No",1,"","","","","27/06/2023 08:58:41",""]
[1775,3543,9,5,"9/35","","9/35","","Mainline and Sprayline","H3",{"v":0,"d":"0.0"},"","","","","26/06/2023 03:37:30",""]
[1776,1049,9,5,"9/35","","9/35","","High density polyethylene class 6 PE80 piping complying with SANS 4427, with compression couplings","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 11:11:51",""]
[1777,1498,9,5,"9/35"," G","9/35. G","","32mm Pipes laid in and including trences not exceeding 1m deep","m",46,"","","","","20/08/2012 08:56:29",""]
[1778,1050,9,5,"9/35"," H","9/35. H","","50mm Pipes, ditto","m",1232,"","","","","26/06/2023 03:34:46",""]
[1779,1051,9,5,"9/36"," A","9/36. A","","63mm Pipes, ditto","m",968,"","","","","06/12/2021 02:38:31",""]
[1780,988,9,5,"9/36"," B","9/36. B","","75mm Pipes, ditto","m",37,"","","","","06/12/2021 02:38:54",""]
[1781,3963,9,5,"9/36","","9/36","","Extra over HDPe piping for  compression fittings","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:44:04",""]
[1782,1501,9,5,"9/36"," C","9/36. C","","32mm x 1\" SAB Male elbow","No",2,"","","","","20/08/2012 08:37:31",""]
[1783,1496,9,5,"9/36"," D","9/36. D","","32mm x 1\" SAB Male adaptor","No",2,"","","","","20/08/2012 08:37:19",""]
[1784,1494,9,5,"9/36"," E","9/36. E","","50mm x 1\" SAB Male adaptor","No",2,"","","","","26/06/2023 02:46:54",""]
[1785,1493,9,5,"9/36"," F","9/36. F","","50mm x 1\" SAB Saddle with steel ring","No",2,"","","","","26/06/2023 02:47:00",""]
[1786,1492,9,5,"9/36"," G","9/36. G","","63mm x 1\" SAB Saddle with steel ring","No",2,"","","","","26/06/2023 02:47:04",""]
[1787,1491,9,5,"9/36"," H","9/36. H","","75mm x 1\" SAB Saddle with steel ring","No",2,"","","","","26/06/2023 02:47:19",""]
[1788,1052,9,5,"9/36","","9/36","","Low density polyethylene class 4 piping","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 11:13:56",""]
[1789,1053,9,5,"9/36"," I","9/36. I","","15mm Pipes","m",470,"","","","","26/06/2023 02:38:09",""]
[1790,1054,9,5,"9/36"," J","9/36. J","","25mm Pipes","m",1029,"","","","","26/06/2023 02:38:13",""]
[1791,1145,9,5,"9/36"," K","9/36. K","","15mm Pipes laid in and including trenches not exceeding 1m deep","m",544,"","","","","27/01/2014 10:20:56",""]
[1792,1146,9,5,"9/36"," L","9/36. L","","25mm Pipes laid in and including trenches not exceeding 1m deep","m",3999,"","","","","27/01/2014 10:21:02",""]
[1793,991,9,5,"9/36","","9/36","","Extra over low density polyethylene piping for full-flow fittings","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:12:13",""]
[1794,992,9,5,"9/36"," M","9/36. M","","15mm Fittings","No",50,"","","","","20/08/2012 09:05:43",""]
[1795,3962,9,5,"9/36"," N","9/36. N","","25mm Fittings","No",11,"","","","","26/06/2023 02:38:27",""]
[1796,3994,9,5,"9/36","","9/36","","Sundry fittings","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 09:05:14",""]
[1797,1502,9,5,"9/36"," O","9/36. O","","25mm BSP compact ball valve","No",2,"","","","","11/08/2012 02:27:09",""]
[1798,1506,9,5,"9/36"," P","9/36. P","","250mm Diameter valve box with lid","No",2,"","","","","26/06/2023 03:39:42",""]
[1799,8562,9,5,"9/36"," Q","9/36. Q","","15mm x 1/2\" FF male comb elbow","No",393,"","","","","07/12/2021 02:37:23",""]
[1800,8564,9,5,"9/36"," R","9/36. R","","15mm FF Elbow","No",86,"","","","","07/12/2021 02:38:14",""]
[1801,8567,9,5,"9/37"," A","9/37. A","","15mm x 3/4\" Male elbow","No",50,"","","","","07/12/2021 02:39:10",""]
[1802,8565,9,5,"9/37"," B","9/37. B","","15mm FF Male adaptor","No",86,"","","","","07/12/2021 02:40:45",""]
[1803,8561,9,5,"9/37"," C","9/37. C","","25 x 15mm FF Reducing tee","No",30,"","","","","07/12/2021 02:43:59",""]
[1804,8563,9,5,"9/37"," D","9/37. D","","25 x 15mm FF Reducer","No",25,"","","","","07/12/2021 02:44:08",""]
[1805,8559,9,5,"9/37"," E","9/37. E","","25mm Male/Female BSP elbow","No",5,"","","","","07/12/2021 02:44:16",""]
[1806,8560,9,5,"9/37"," F","9/37. F","","25mm Female tee","No",5,"","","","","07/12/2021 02:44:21",""]
[1807,3995,9,5,"9/37"," G","9/37. G","","Signature MP1000 rotator","No",222,"","","","","20/08/2012 09:18:54",""]
[1808,1515,9,5,"9/37"," H","9/37. H","","Signature MP2000 rotator","No",5,"","","","","11/08/2012 03:05:20",""]
[1809,1516,9,5,"9/37"," I","9/37. I","","Signature MP3000 rotator","No",5,"","","","","11/08/2012 03:05:25",""]
[1810,1521,9,5,"9/37"," J","9/37. J","","3/4\" BSP socket","No",5,"","","","","11/08/2012 03:06:57",""]
[1811,1508,9,5,"9/37"," K","9/37. K","","Rainbird, or equal approved, 12\" hi pop body pop-up body","No",906,"","","","","19/08/2012 04:01:31",""]
[1812,1518,9,5,"9/37"," L","9/37. L","","Rainbird, or equal approved, 5012PC 12\" pop-up","No",50,"","","","","19/08/2012 04:02:36",""]
[1813,8568,9,5,"9/37","","9/37","","Dripline installation","H3",{"v":0,"d":"0.0"},"","","","","10/05/2019 02:43:55",""]
[1814,11006,9,5,"9/37"," M","9/37. M","","16mm Netafim pressure comp dripper line 0,4m spacing x 1,6L/H","m",608,"","","","","08/12/2021 05:07:01",""]
[1815,11012,9,5,"9/37"," N","9/37. N","","XFS dripline 17mm x 2,3L/H x 0,3m x 152m coil","No",6,"","","","","08/12/2021 04:12:51",""]
[1816,8570,9,5,"9/37"," O","9/37. O","","Techline 17mm x 3/4\" female tee","No",40,"","","","","07/12/2021 02:46:27",""]
[1817,8571,9,5,"9/37"," P","9/37. P","","15mm class 4 L.D.P.E","m",40,"","","","","07/12/2021 02:46:46",""]
[1818,8573,9,5,"9/37"," Q","9/37. Q",""," 25 x 15mm FF reducing coupling","No",1,"","","","","07/12/2021 02:47:48",""]
[1819,8574,9,5,"9/37"," R","9/37. R",""," 15mm x 3/4\" FF male adaptor","No",12,"","","","","07/12/2021 02:48:15",""]
[1820,8576,9,5,"9/37"," S","9/37. S","","17mm Drip coupling","No",9,"","","","","07/12/2021 02:48:27",""]
[1821,8584,9,5,"9/37"," T","9/37. T","","17mm Drip elbow","No",110,"","","","","07/12/2021 02:48:38",""]
[1822,8577,9,5,"9/37"," U","9/37. U","","17mm Drip tee","No",160,"","","","","07/12/2021 02:48:45",""]
[1823,8578,9,5,"9/37"," V","9/37. V","","17mm Drip end cap","No",5,"","","","","07/12/2021 02:48:55",""]
[1824,8579,9,5,"9/38"," A","9/38. A",""," 17mm Techline cross","No",10,"","","","","07/12/2021 02:49:18",""]
[1825,8580,9,5,"9/38"," B","9/38. B","","Vacuum breaker","No",2,"","","","","07/12/2021 02:49:28",""]
[1826,8581,9,5,"9/38"," C","9/38. C","","Line flush valve","No",1,"","","","","07/12/2021 02:49:48",""]
[1827,8582,9,5,"9/38"," D","9/38. D","","25mm Disc filter","No",2,"","","","","07/12/2021 02:49:58",""]
[1828,8583,9,5,"9/38"," E","9/38. E","","250mm Diameter valve box with lid","No",1,"","","","","07/12/2021 02:50:05",""]
[1829,3545,9,5,"9/38","","9/38","","Turf valve line installation","H3",{"v":0,"d":"0.0"},"","","","","20/08/2012 09:12:19",""]
[1830,3546,9,5,"9/38","","9/38","","Extra over polyethylene pipes for compression fittings","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 01:49:50",""]
[1831,8221,9,5,"9/38"," F","9/38. F","","1\" x 3/4\" BSP Reducing bush","No",9,"","","","","26/06/2023 03:22:35",""]
[1832,1541,9,5,"9/38"," G","9/38. G","","AQUA 20 plastic turf valve","No",37,"","","","","20/08/2012 09:26:17",""]
[1833,3547,9,5,"9/38"," H","9/38. H","","20mm Diameter standard duty dragline hose","m",4,"","","","","20/08/2012 09:13:14",""]
[1834,1551,9,5,"9/38"," I","9/38. I","","20 x 600mm Galvanised mild steel dragline hose stand","No",2,"","","","","20/08/2012 09:27:36",""]
[1835,3548,9,5,"9/38"," J","9/38. J","","Aqua 20mm brass P/C sprinkler","No",4,"","","","","26/06/2023 03:24:42",""]
[1836,1554,9,5,"9/38","","9/38","","Automatic irrigation system","H3",{"v":0,"d":"0.0"},"","","","","11/08/2012 12:49:33",""]
[1837,8587,9,5,"9/38"," K","9/38. K","","Satelite cable","m",500,"","","","","26/06/2023 03:12:33",""]
[1838,4018,9,5,"9/38"," L","9/38. L","","90mm x 2\" SAB Male adaptor","No",6,"","","","","26/06/2023 03:12:41",""]
[1839,1555,9,5,"9/38"," M","9/38. M","","Rainbird, or equal approved, 25mm PGA solenoid valve","No",56,"","","","","26/06/2023 03:11:43",""]
[1840,1561,9,5,"9/38"," N","9/38. N","","Rainbird, or equal approved, rain trip wired rain sensor ","No",1,"","","","","26/06/2023 03:13:02",""]
[1841,4020,9,5,"9/38"," O","9/38. O","","Rainbird, or equal approved, FD-101 field decoder","No",49,"","","","","26/06/2023 03:13:35",""]
[1842,4021,9,5,"9/38"," P","9/38. P","","Rainbird, or equal approved,LSP-1 decoder surge arrestor","No",20,"","","","","26/06/2023 03:13:53",""]
[1843,4016,9,5,"9/38"," Q","9/38. Q","","Rainbird, or equal approved, PD210 pump decoder","No",7,"","","","","26/06/2023 03:16:39",""]
[1844,4017,9,5,"9/38"," R","9/38. R","","Rainbird, or equal approved, CST Flow meter","No",3,"","","","","26/06/2023 03:18:19",""]
[1845,1563,9,5,"9/38"," S","9/38. S","","Rainbird, or equal approved, 50-station LX decoder controller","No",1,"","","","","08/12/2021 05:17:55",""]
[1846,13649,9,5,"9/38"," T","9/38. T","","Rainbird irrigation controller (Prime Cost R10 000.00 excl. VAT supply only)","No",2,"","","","","26/06/2023 02:27:13",""]
[1847,1003,9,5,"9/39","","9/39","","Testing","H4",{"v":0,"d":"0.0"},"","","","","04/06/2012 08:07:54",""]
[1848,1004,9,5,"9/39"," A","9/39. A","","Testing irrigation system to the satisfaction of the landscape architect","Item",{"v":1,"d":"1.00"},"","","","","06/12/2021 02:41:56",""]
[1849,7436,9,5,"9/39","","9/39","","AS-BUILT DRAWINGS","H2",{"v":0,"d":"0.0"},"","","","","22/10/2012 09:21:25",""]
[1850,7437,9,5,"9/39"," B","9/39. B","","Provision of as-built drawings","Item",{"v":1,"d":"1.00"},"","","","","22/10/2012 09:21:25",""]
[1852,9496,9,6,"9/41","","9/41","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:46",""]
[1853,7421,9,6,"9/41","","9/41","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:22",""]
[1854,9497,9,6,"9/41","","9/41","","BILL NO. 6","H1",{"v":0,"d":"0.0"},"","","","","09/09/2021 09:08:08",""]
[1855,7423,9,6,"9/41","","9/41","","SUB-SOIL DRAINAGE IN LANDSCAPED AREAS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:09",""]
[1856,7424,9,6,"9/41","","9/41","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:28:04",""]
[1857,7425,9,6,"9/41","","9/41","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:05",""]
[1858,7426,9,6,"9/41","","9/41","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:28:04",""]
[1859,7427,9,6,"9/41","","9/41","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:28:04",""]
[1860,7428,9,6,"9/41","","9/41","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:28:04",""]
[1861,7429,9,6,"9/41","","9/41","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:28:04",""]
[1862,7430,9,6,"9/41","","9/41","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\"","",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:28:04",""]
[1863,13799,9,6,"9/42","","9/42","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:04:14",""]
[1864,1404,9,6,"9/42","","9/42","","Sub-soil drainage","H3",{"v":0,"d":"0.0"},"","","","","20/10/2012 11:30:27",""]
[1865,3527,9,6,"9/42"," A","9/42. A","","Excavation in earth not exceeding 2m deep for pipe trenches","m3",212,"","","","","26/06/2023 11:00:38",""]
[1866,3528,9,6,"9/42"," B","9/42. B","","Extra over all excavations for carting away surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",212,"","","","","26/06/2023 11:00:44",""]
[1867,3529,9,6,"9/42"," C","9/42. C","","19mm Crushed stone encasing to pipes","m3",212,"","","","","26/06/2023 11:00:29",""]
[1868,3530,9,6,"9/42"," D","9/42. D","","U22 geofabric filter blanket wrapped around stone encasing with 300mm side and end laps, including stitching","m2",653,"","","","","06/12/2021 05:24:38",""]
[1869,3539,9,6,"9/42"," E","9/42. E","","A2 geofabric filter blanket wrapped around stone encasing with 300mm side and end laps, including stitching","m2",1146,"","","","","06/12/2021 05:24:42",""]
[1870,3532,9,6,"9/42"," F","9/42. F","","110mm Slotted uPVC pipes laid in stone encasing (encasing elsewhere)","m",740,"","","","","07/12/2021 03:51:50",""]
[1871,3540,9,6,"9/42"," G","9/42. G","","Extra for end cap to 110mm perforated pipe","No",1,"","","","","06/12/2021 05:27:09",""]
[1872,3542,9,6,"9/42"," H","9/42. H","","Extra for Junction to 110mm perforated pipe","No",1,"","","","","06/12/2021 05:27:13",""]
[1873,11107,9,6,"9/42","","9/42","","Exploratory excavations","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 12:00:36",""]
[1874,11108,9,6,"9/42"," I","9/42. I","","Excavation in earth not exceeding 2m deep, in isolated holes, to locate sub-soil installations","m3",26,"","","","","06/12/2021 05:27:20",""]
[1875,11109,9,6,"9/42"," J","9/42. J","","Backfilling to isolated holes with material from the excavations or stockpiles on site, compacted to 93% Mod AASHTO density","m3",26,"","","","","06/12/2021 05:27:23",""]
[1877,9498,9,7,"9/44","","9/44","","SECTION NO. 9","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:50",""]
[1878,6215,9,7,"9/44","","9/44","","LANDSCAPING (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:25",""]
[1879,9499,9,7,"9/44","","9/44","","BILL NO. 7","H1",{"v":0,"d":"0.0"},"","","","","06/11/2021 12:15:31",""]
[1880,3926,9,7,"9/44","","9/44","","MAINTENANCE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:14",""]
[1881,3927,9,7,"9/44","","9/44","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:40",""]
[1882,3928,9,7,"9/44","","9/44","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:10",""]
[1883,3929,9,7,"9/44","","9/44","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:41",""]
[1884,4100,9,7,"9/44","","9/44","","Landscaping specification","H4",{"v":0,"d":"0.0"},"","","","","24/08/2012 09:24:02",""]
[1885,4101,9,7,"9/44","","9/44","","Refer to the landscape architect's specification annexed to these bills of quantities which is supplementary to and shall take precedence over the \"Specification of Materials and Methods to be used (PW371)\" ","",{"v":0,"d":"0.0"},"","","","","17/11/2015 09:06:15",""]
[1886,13800,9,7,"9/44","","9/44","","Registrations:  1.\tThe Landscaping sub-contractor must be registered with the CIDB as a minimum level 6 in the SH - Landscaping, irrigation and horticulture works category.  2.\tThe Landscaping sub-contractor must price for shop drawings for the irrigation system as well as the irrigation pump.  The design of the irrigation system and pump must be done by a registered member of LIA (Landscape irrigation Association of South Africa). Shop drawings to be produced for the Healing pond and Genocide pond pumps and circulation systems as well.  3.\tThe Landscaping sub-contractor to be appointed as a Selected Sub-Contractor in terms of the JBCC PBA and N/S Sub-Contract Agreement.","",{"v":0,"d":"0.0"},"","","","","22/05/2023 10:04:21",""]
[1887,3930,9,7,"9/45","","9/45","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:41",""]
[1888,3931,9,7,"9/45","","9/45","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","20/08/2012 04:39:41",""]
[1889,1571,9,7,"9/45","","9/45","","Maintenance","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 09:05:47",""]
[1890,1569,9,7,"9/45","","9/45","","Note : Full maintenance and establishment of all bulk irrigation services, landscape and water course areas inclusive but not restricted to the maintenance of the irrigation, sewer, features, electrical, water features, buildings, paved areas and water system, application of pesticides, fertilizers and replacement of plants etc. All in accordance with the routine maintenance specifications. Maintenance to commence upon date of practical completion.","",{"v":0,"d":"0.0"},"","","","","17/11/2012 06:31:57",""]
[1891,3941,9,7,"9/45","","9/45","","All equipment to be supplied, including comissioning and training of two persons employed by the client for maintenance and operation","",{"v":0,"d":"0.0"},"","","","","20/08/2012 06:35:47",""]
[1892,1570,9,7,"9/45"," A","9/45. A","","Provision of maintenance as described above (per month)","Mth",{"v":12,"d":"12.00"},"","","","","06/11/2021 12:15:57",""]
[1894,3910,9,8,"9/110","1","9/110.1","","General landscaping","Page","9/13",0,"","","","20/08/2012 04:37:20",""]
[1895,3911,9,8,"9/110","2","9/110.2","","Re-instatement of disturbed on-site areas","Page","9/21",0,"","","","20/08/2012 04:37:30",""]
[1896,7439,9,8,"9/110","3","9/110.3","","Re-instatement of disturbed bypass road areas","Page","9/27",0,"","","","25/10/2012 07:19:24",""]
[1897,7232,9,8,"9/110","4","9/110.4","","Vegetation rehabilitation, search and rescue","Page","9/33",0,"","","","19/10/2012 10:19:49",""]
[1898,3943,9,8,"9/110","5","9/110.5","","Irrigation system","Page","9/40",0,"","","","20/08/2012 06:56:59",""]
[1899,7419,9,8,"9/110","6","9/110.6","","Sub-soil drainage in landscaped areas","Page","9/43",0,"","","","20/10/2012 11:27:24",""]
[1900,3912,9,8,"9/110","7","9/110.7","","Maintenance","Page","9/46",0,"","","","20/08/2012 04:37:37",""]
[1901,9240,10,1,"10/1","","10/1","","SECTION NO. 10","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:20:57",""]
[1902,9241,10,1,"10/1","","10/1","","MATERIALS ON SITE - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:55:04",""]
[1903,9242,10,1,"10/1","","10/1","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"","","","","27/10/2021 05:30:58",""]
[1904,10219,10,1,"10/1","","10/1","","CREDIT FOR MATERIALS ON SITE - RELATING TO EXTERNAL WORKS AND LANDSCAPING ONLY","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:54:56",""]
[1905,9629,10,1,"10/1","","10/1","","Note : The following materials have been left on site by the previous contractor and are intended for the works. Tenderers are expected to utilize these materials and therefore provide credit by pricing a negative price against each item","",{"v":0,"d":"0.0"},"","","","","15/09/2021 04:35:02",""]
[1906,9628,10,1,"10/1","","10/1","","There are 4 separate Materials On Site storage areas - see area allocation in brackets at the end of descriptions","",{"v":0,"d":"0.0"},"","","","","08/12/2021 04:18:10",""]
[1907,9255,10,1,"10/1","","10/1","","GENERAL LANDSCAPING MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","09/09/2021 10:31:24",""]
[1908,9257,10,1,"10/1"," A","10/1. A","","\"Kaytech Enviromat\" biodegradable erosion control blanket roll (50 x 2,5m wide x 26 rolls)","m2",3250,"","","","","18/10/2021 10:26:42",""]
[1909,9258,10,1,"10/1"," B","10/1. B","","Imported topsoil supplied by the contractor (Various areas on site)","m3",20,"","","","","18/10/2021 02:10:34",""]
[1910,9259,10,1,"10/1"," C","10/1. C","","Fine grit (1,6tons per m3)","t",{"v":10,"d":"10.00"},"","","","","10/12/2021 03:14:26",""]
[1911,9287,10,1,"10/1"," D","10/1. D","","Hot-dip galvanised after manufacture mild steel edging size 75 x 2,5mm thick, with and including 95mm long wedge-shaped spikes welded on at 200mm centres, end locking mechanisms (Perma edge 100mm)","No",500,"","","","","19/10/2021 11:42:34",""]
[1912,9260,10,1,"10/1"," E","10/1. E","","Aloes speciosa (4l)","No",151,"","","","","10/12/2021 10:06:56",""]
[1913,9261,10,1,"10/1"," F","10/1. F","","Bulbine frutescens (2l)","No",151,"","","","","10/11/2021 08:46:51",""]
[1914,9262,10,1,"10/1"," G","10/1. G","","Cotyledon (2l)","No",1426,"","","","","10/11/2021 08:45:49",""]
[1915,9263,10,1,"10/1"," H","10/1. H","","Cotyledon orbiculata (4l)","No",500,"","","","","10/11/2021 08:45:33",""]
[1916,9264,10,1,"10/1"," I","10/1. I","","Crassula mucosa (4l)","No",191,"","","","","10/11/2021 08:43:54",""]
[1917,9265,10,1,"10/1"," J","10/1. J","","Crassula perforate (2l)","No",480,"","","","","10/11/2021 08:44:03",""]
[1918,9266,10,1,"10/2"," A","10/2. A","","Delosperma (2l)","No",210,"","","","","10/11/2021 08:47:24",""]
[1919,9267,10,1,"10/2"," B","10/2. B","","Euphorbia species (plugs)","No",785,"","","","","10/11/2021 08:48:05",""]
[1920,9268,10,1,"10/2"," C","10/2. C","","Euphorbia spp","No",314,"","","","","13/09/2021 12:47:46",""]
[1921,9270,10,1,"10/2"," D","10/2. D","","Portulacaria affra (2l)","No",1489,"","","","","09/09/2021 10:17:12",""]
[1922,9509,10,1,"10/2","","10/2","","IRRIGATION SYSTEM MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","09/09/2021 10:31:50",""]
[1923,9309,10,1,"10/2"," E","10/2. E","","15mm Class 3 LDPE pipe","m",100,"","","","","10/12/2021 03:15:34",""]
[1924,9302,10,1,"10/2"," F","10/2. F","","25mm Class 3 LDPE pipe","m",550,"","","","","10/12/2021 03:15:25",""]
[1925,9303,10,1,"10/2"," G","10/2. G","","50mm Class 8 PE100 HDPE pipe","m",550,"","","","","10/12/2021 03:14:58",""]
[1926,9304,10,1,"10/2"," H","10/2. H","","2,5mm Rainbird cable","m",510,"","","","","10/11/2021 08:53:27",""]
[1927,9305,10,1,"10/2"," I","10/2. I","","1 Poly nipple BSP","No",6,"","","","","09/09/2021 10:18:01",""]
[1928,9307,10,1,"10/2"," J","10/2. J","","3/4\" BSP Reducing bush","No",17,"","","","","10/11/2021 08:56:38",""]
[1929,9308,10,1,"10/2"," K","10/2. K","","15mm x 1/2\" FF male comb elbow","No",393,"","","","","10/11/2021 08:57:55",""]
[1930,9310,10,1,"10/2"," L","10/2. L","","15mm FF elbow","No",86,"","","","","09/09/2021 09:51:31",""]
[1931,9311,10,1,"10/2"," M","10/2. M","","15mm FF male adaptor","No",86,"","","","","09/09/2021 09:51:40",""]
[1932,9312,10,1,"10/2"," N","10/2. N","","15 x 750mm Green PVC riser with attachment fittings","No",180,"","","","","10/11/2021 09:00:15",""]
[1933,9313,10,1,"10/2"," O","10/2. O","","2\" BSP poly nipple","No",8,"","","","","10/11/2021 09:00:26",""]
[1934,9314,10,1,"10/2"," P","10/2. P","","20mm Medium duty dragline hose (30m line)","No",3,"","","","","10/11/2021 09:02:23",""]
[1935,9315,10,1,"10/2"," Q","10/2. Q","","20 x 600mm Galvanised mild steel dragline hose stand","No",1,"","","","","10/11/2021 09:03:08",""]
[1936,9316,10,1,"10/2"," R","10/2. R","","20mm x 3/4\" \"EMJAY\" long male elbow","No",17,"","","","","10/12/2021 03:17:27",""]
[1937,9317,10,1,"10/2"," S","10/2. S","","3/4\" BSP Socket","No",9,"","","","","10/11/2021 09:08:32",""]
[1938,9318,10,1,"10/2"," T","10/2. T","","450 Litre vertical pressure tank","No",1,"","","","","09/09/2021 09:53:30",""]
[1939,9320,10,1,"10/2"," U","10/2. U","","50 x 300mm Galvanised riser pipe","No",2,"","","","","10/11/2021 09:09:18",""]
[1940,9321,10,1,"10/2"," V","10/2. V","","65mm Galvanised barrel nipple","No",1,"","","","","06/09/2021 09:59:33",""]
[1941,9322,10,1,"10/3"," A","10/3. A","","20mm Aqua brass P/C sprinkler","No",2,"","","","","10/11/2021 09:10:26",""]
[1942,9323,10,1,"10/3"," B","10/3. B","","25 Aqua plastic turf valve","No",8,"","","","","10/11/2021 09:12:45",""]
[1943,9325,10,1,"10/3"," C","10/3. C","","50mm Galvanised female elbow","No",2,"","","","","09/09/2021 09:58:35",""]
[1944,9327,10,1,"10/3"," D","10/3. D","","65mm Galvanised barrel nipple","No",2,"","","","","10/11/2021 09:13:17",""]
[1945,9328,10,1,"10/3"," E","10/3. E","","63mm x 2\" PERLA compression female tee","No",1,"","","","","10/11/2021 09:14:20",""]
[1946,9329,10,1,"10/3"," F","10/3. F","","80mm \"Nelson 800\" series pressure reducing valve","No",1,"","","","","10/11/2021 09:15:19",""]
[1947,9330,10,1,"10/3"," G","10/3. G","","PTFE seal & bond tape","No",12,"","","","","10/11/2021 09:17:01",""]
[1948,9331,10,1,"10/3"," H","10/3. H","","PVC compact ball valve BSP THR 1","No",11,"","","","","09/09/2021 10:04:29",""]
[1949,9332,10,1,"10/3"," I","10/3. I","","PVC compact ball valve BSP THR 2","No",30,"","","","","09/09/2021 10:11:39",""]
[1950,9333,10,1,"10/3"," J","10/3. J","","PVC compact ball valve BSP THR 2,1/2","No",2,"","","","","10/11/2021 09:17:45",""]
[1951,9334,10,1,"10/3"," K","10/3. K","","1812 Rainbird SAM spray head","No",11,"","","","","09/09/2021 10:23:01",""]
[1952,9335,10,1,"10/3"," L","10/3. L","","25mm Rainbird PGA solenoid valve","No",18,"","","","","10/11/2021 09:21:17",""]
[1953,9336,10,1,"10/3"," M","10/3. M","","250mm Rainbird economy valve box with lid","No",32,"","","","","10/11/2021 09:24:10",""]
[1954,9337,10,1,"10/3"," N","10/3. N","","Rainbird 5012PC 12\" pop-up","No",50,"","","","","10/11/2021 09:25:05",""]
[1955,9340,10,1,"10/3"," O","10/3. O","","Rainbird rain trip wired rain sensor","No",1,"","","","","10/11/2021 09:26:55",""]
[1956,9341,10,1,"10/3"," P","10/3. P","","Rainbird soil moisture sensor kit","No",4,"","","","","10/11/2021 09:27:11",""]
[1957,9339,10,1,"10/3"," Q","10/3. Q","","Rainbird FD-101 field decoder","No",49,"","","","","10/11/2021 09:26:35",""]
[1958,9342,10,1,"10/3"," R","10/3. R","","Rainbird LSP-1 decoder surge arrestor","No",7,"","","","","10/11/2021 09:27:36",""]
[1959,9324,10,1,"10/3"," S","10/3. S","","Rainbird CST Flow meter","No",8,"","","","","10/11/2021 09:11:21",""]
[1960,9338,10,1,"10/3"," T","10/3. T","","Rainbird 50-station LX decoder controller","No",1,"","","","","10/11/2021 09:26:13",""]
[1961,9343,10,1,"10/3"," U","10/3. U","","50mm SAB compression coupling","No",7,"","","","","09/09/2021 10:20:40",""]
[1962,9344,10,1,"10/3"," V","10/3. V","","50mm SAB compression elbow","No",5,"","","","","09/09/2021 10:20:52",""]
[1963,9345,10,1,"10/3"," W","10/3. W","","50mm SAB compression end plug","No",2,"","","","","09/09/2021 10:21:01",""]
[1964,9346,10,1,"10/4"," A","10/4. A","","50mm SAB compression tee","No",20,"","","","","09/09/2021 10:21:10",""]
[1965,9347,10,1,"10/4"," B","10/4. B","","50mm x 1\" SAB Saddle with steel ring","No",18,"","","","","10/11/2021 09:30:01",""]
[1966,9348,10,1,"10/4"," C","10/4. C","","63mm x 1\" SAB Saddle with steel ring","No",15,"","","","","10/11/2021 09:30:13",""]
[1967,9349,10,1,"10/4"," D","10/4. D","","90mm x 2\" SAB compression female adaptor","No",4,"","","","","10/11/2021 09:31:44",""]
[1968,9350,10,1,"10/4"," E","10/4. E","","SPIN-KLIN JASPER PP 2 filter bank 130 MIC","No",1,"","","","","10/11/2021 09:35:35",""]
[1969,9351,10,1,"10/4"," F","10/4. F","","20-32mm Hose clamp 10mm perforated (20/25mm)","No",2,"","","","","10/12/2021 10:14:28",""]
[1970,9352,10,1,"10/4"," G","10/4. G","","20-32mm Hose clamp non-perforated","No",2,"","","","","10/12/2021 10:14:39",""]
[1971,9353,10,1,"10/4"," H","10/4. H","","50mm Brass gate valve","No",1,"","","","","09/09/2021 11:42:38",""]
[1972,9506,10,1,"10/4","","10/4","","PARKING, PAVING, AND ROADWORK MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","17/10/2021 06:03:24",""]
[1973,9271,10,1,"10/4"," I","10/4. I","","150 x 300mm High kerbs in 1 000mm lengths (SANS 927 fig 3) (Area 2)","m",42,"","","","","10/12/2021 03:18:06",""]
[1974,9273,10,1,"10/4"," J","10/4. J","","150 x 250mm High kerbs in 1 000mm lengths (SANS 927 fig 4) (Area 2)","m",50,"","","","","10/12/2021 03:18:12",""]
[1975,9272,10,1,"10/4"," K","10/4. K","","200 x 100 x 50mm \"CEL\" exposed granite aggregate finish paver (Area 3 & museum) (10,5 pallets)","No",11,"","","","","10/12/2021 03:18:21",""]
[1976,10775,10,1,"10/4"," L","10/4. L","","105 x 210 x 70mm 35Mpa bevel-edged full inter-locking precast concrete pavers with 9mm exposed granite aggregate finish (Area 1, 2 & 3 and 1 pallet at museum, 29 pallets)","No",29,"","","","","10/12/2021 03:18:30",""]
[1977,9277,10,1,"10/4"," M","10/4. M","","450 x 450mm Charcoal paving slabs \"stepping stones\" (Area 3) (8 pallets)","No",8,"","","","","10/12/2021 03:18:36",""]
[1978,9278,10,1,"10/4"," N","10/4. N","","300 x 300mm \"Smartile\" coping tiles (Area 3) (3,5 pallets)","No",700,"","","","","10/12/2021 03:18:47",""]
[1979,9279,10,1,"10/4"," O","10/4. O","","\"Algoa brick\" stock bricks (Sundial Area 3 & grave site) (21 pallets)","No",21,"","","","","10/12/2021 03:18:53",""]
[1980,9280,10,1,"10/4"," P","10/4. P","","\"Potgieter gabion\" stones for cladding to walls (Area 3)","t",{"v":5,"d":"5.00"},"","","","","18/10/2021 02:38:41",""]
[1981,12525,10,1,"10/4"," Q","10/4. Q","","MP300 Precast concrete major fencing post (Cavcon manufacturing) (Area 1)","No",7,"","","","","10/12/2021 03:19:02",""]
[1982,12524,10,1,"10/4"," R","10/4. R","","IP300 Precast concrete fencing post (Cavcon manufacturing) (Area 1)","No",49,"","","","","10/12/2021 03:19:11",""]
[1983,12526,10,1,"10/5"," A","10/5. A","","MOC overhang (Cavcon manufacturing) (Area 1)","No",4,"","","","","10/12/2021 03:19:17",""]
[1984,12527,10,1,"10/5"," B","10/5. B","","MO overhang (Cavcon manufacturing) (Area 1)","No",3,"","","","","10/12/2021 03:19:23",""]
[1985,12528,10,1,"10/5"," C","10/5. C","","PO overhang (Cavcon manufacturing) (Area 1)","No",38,"","","","","10/12/2021 03:19:28",""]
[1986,12529,10,1,"10/5"," D","10/5. D","","Gate bracket complete (Cavcon manufacturing) (Area 1)","No",2,"","","","","10/12/2021 03:19:35",""]
[1987,12530,10,1,"10/5"," E","10/5. E","","Stay bracket complete (Cavcon manufacturing) (Area 1)","No",11,"","","","","10/12/2021 03:19:40",""]
[1988,9505,10,1,"10/5","","10/5","","FENCING MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","09/09/2021 10:24:01",""]
[1989,9630,10,1,"10/5","","10/5","","Note : all fencing materials are marine fusion bonded","",{"v":0,"d":"0.0"},"","","","","08/12/2021 04:18:37",""]
[1990,9626,10,1,"10/5","","10/5","","\"Cochrane Clearvu\"","H4",{"v":0,"d":"0.0"},"","","","","19/10/2021 10:12:09",""]
[1991,9282,10,1,"10/5"," F","10/5. F","","Black fence panel size 3 305 x 2 400mm high (Area 1)","No",12,"","","","","19/10/2021 10:11:57",""]
[1992,9283,10,1,"10/5"," G","10/5. G","","Taper locking post 3 000mm long (Area 1)","No",39,"","","","","15/09/2021 04:43:53",""]
[1993,9284,10,1,"10/5"," H","10/5. H","","Single sliding gate size 1 640 x 2 400mm high (Area 1)","No",1,"","","","","19/10/2021 10:11:21",""]
[1994,9285,10,1,"10/5"," I","10/5. I","","Saw tooth 1 500mm long (Area 1)","No",26,"","","","","19/10/2021 10:14:51",""]
[1995,9286,10,1,"10/5"," J","10/5. J","","Under dig (anti-burrow) panel size 3 305 x 600mm (Area 1)","No",42,"","","","","10/12/2021 03:20:06",""]
[1996,9627,10,1,"10/5","","10/5","","\"Betafence\"","H4",{"v":0,"d":"0.0"},"","","","","19/10/2021 10:12:16",""]
[1997,9299,10,1,"10/5"," K","10/5. K","","Fencing panels size 2 515 x 2 400mm (covers approximately 200m) (Area 1)","No",10,"","","","","08/12/2021 04:19:28",""]
[1998,9300,10,1,"10/5"," L","10/5. L","","Betafix post (Area 1) ","No",18,"","","","","06/12/2021 02:50:05",""]
[1999,9301,10,1,"10/5"," M","10/5. M","","Tooth spike 3 050mm long (Area 1)","No",106,"","","","","10/11/2021 09:52:36",""]
[2000,9504,10,1,"10/5","","10/5","","STORMWATER MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","09/09/2021 10:23:44",""]
[2001,9276,10,1,"10/5"," N","10/5. N","","\"Deranco blocks\" 500 x 140mm Precast concrete rain water channels, 1 000mm long (Area 2 & 3)","m",156,"","","","","08/12/2021 12:19:09",""]
[2002,9289,10,1,"10/5"," O","10/5. O","","450mm Class 100D concrete storm water pipes, 2 500mm long (Area 2)","No",14,"","","","","08/12/2021 12:17:13",""]
[2003,9290,10,1,"10/5"," P","10/5. P","","\"Enviro precast solutions\" C-beams, 1 355mm long (205kg) (Area 2)","No",10,"","","","","08/12/2021 12:15:18",""]
[2004,9291,10,1,"10/6"," A","10/6. A","","Type 1A Polymer manhole covers & frames (black & grey types) (Area 2 & 3)","No",11,"","","","","10/12/2021 03:20:30",""]
[2005,9292,10,1,"10/6"," B","10/6. B","","1 250 x 640mm Galvanised steel double catchpit grating and frame (Area 2)","No",1,"","","","","19/10/2021 11:56:04",""]
[2006,9294,10,1,"10/6"," C","10/6. C","","640 x 640mm Galvanised steel catchpit grating and frame (Area 2)","No",13,"","","","","19/10/2021 11:58:39",""]
[2007,9295,10,1,"10/6"," D","10/6. D","","600 x 600mm x 82kg Type 9B medium duty cast iron manhole cover and frame (Area 2)","No",14,"","","","","28/10/2021 11:19:33",""]
[2008,9297,10,1,"10/6"," E","10/6. E","","640 x 640mm Steel frames as per details on dwg. C5593-SITE-SW-55 (for pre-cast concrete cover and steel frame to storm water inspection chambers - concrete still to be done)","No",49,"","","","","08/12/2021 04:32:31",""]
[2009,9514,10,1,"10/6","","10/6","","PLUMBING MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","09/09/2021 12:11:14",""]
[2010,9516,10,1,"10/6"," F","10/6. F","","110mm uPVC pipes, 6 000mm long","No",13,"","","","","19/10/2021 02:49:29",""]
[2011,9515,10,1,"10/6"," G","10/6. G","","110mm x 90 Degree uPVC bend  ","No",6,"","","","","19/10/2021 02:48:52",""]
[2012,9517,10,1,"10/6"," H","10/6. H","","110mm HDPe compression bend","No",3,"","","","","10/11/2021 10:28:51",""]
[2013,9518,10,1,"10/6"," I","10/6. I","","110mm HDPe straight connector  ","No",3,"","","","","10/11/2021 10:28:57",""]
[2014,9298,10,1,"10/6"," J","10/6. J","","160mm \"CL4 Duraflo\" uPVC pipes, 6 000mm long (Underpass approach storage)","No",8,"","","","","10/11/2021 10:31:19",""]
[2015,9519,10,1,"10/6"," K","10/6. K","","160mm PVC bend","No",2,"","","","","08/12/2021 12:16:47",""]
[2016,9520,10,1,"10/6"," L","10/6. L","","160mm \"Plasduct\" PVC pipes, 6 000mm long","No",5,"","","","","10/11/2021 10:30:33",""]
[2017,9521,10,1,"10/6"," M","10/6. M","","160mm x 90 degree \"Plasduct\" slow bend","No",4,"","","","","19/10/2021 02:38:09",""]
[2018,9522,10,1,"10/6"," N","10/6. N","","75mm Diameter HDPe pipe (50m Roll)","No",1,"","","","","10/11/2021 10:32:10",""]
[2019,9524,10,1,"10/6"," O","10/6. O","","\"Badger modMAG model M5000\" flow meter with DN50 flanged PN16 hard rubber liner and 4D cell battery including grounding rings","No",1,"","","","","19/10/2021 02:27:44",""]
[2020,9507,10,1,"10/6","","10/6","","LITTER BINS, BOLLARDS, BENCHES MATERIALS","H3",{"v":0,"d":"0.0"},"","","","","09/09/2021 10:27:44",""]
[2021,9288,10,1,"10/6"," P","10/6. P","","Steel leaf benches (to match Rizel Engineering Services benches on site)","No",5,"","","","","08/12/2021 04:45:16",""]
[2022,9244,10,1,"10/6","","10/6","","NOTE : THIS BILL SHOULD HAVE A NEGATIVE TOTAL, WHICH SHOULD BE CARRIED TO THE SECTION SUMMARY AS A NEGATIVE (MINUS) VALUE","",{"v":0,"d":"0.0"},"","","","","03/09/2021 07:27:34",""]
[2024,9356,11,1,"11/1","","11/1","","SECTION NO. 11","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:21:02",""]
[2025,9357,11,1,"11/1","","11/1","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"","","","","10/11/2021 01:43:48",""]
[2026,9358,11,1,"11/1","","11/1","","PROVISIONAL SUMS : SUB-CONTRACTORS","H1",{"v":0,"d":"0.0"},"","","","","11/07/2023 08:48:09",""]
[2027,9359,11,1,"11/1","","11/1","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:14",""]
[2028,9360,11,1,"11/1","","11/1","","General","H4",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:14",""]
[2029,9361,11,1,"11/1","","11/1","","Work for which budgetary allowances are provided will be measured and valued in accordance with clause 32 of the Principal Building Agreement and deducted in whole or in part if not required without any compensation for loss or profit on the said allowances.","",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:04:29",""]
[2030,9362,11,1,"11/1","","11/1","","Prime cost amounts and provisional sums are net and include for delivery to site of all articles concerned.  Provisional sums are for material and equipment supplied and installed complete by firms of specialists.","",{"v":0,"d":"0.0"},"","","","","07/09/2021 08:23:31",""]
[2031,9365,11,1,"11/1","","11/1","","General attendance","H4",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:04:22",""]
[2032,9366,11,1,"11/1","","11/1","","The item \"Attendance\" which follows each provisional sum for nominated/selected subcontractors' work, shall be deemed to cover all the contractor's costs incurred in providing free of charge to the nominated/selected subcontractors, the following:","",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:04:47",""]
[2033,9367,11,1,"11/1","","11/1","","1. The services as set out in clause B9.1 of the Preliminaries.  2. Making good in all trades, cleaning and removal of rubbish on completion.","",{"v":0,"d":"0.0"},"","","","","06/11/2021 11:59:27",""]
[2034,9368,11,1,"11/1","","11/1","","Builder's work","H4",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:14",""]
[2035,9369,11,1,"11/1","","11/1","","Builder's work in connection with specialist services is given elsewhere in these bills of quantities","",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:14",""]
[2036,9370,11,1,"11/1","","11/1","","BUDGETARY ALLOWANCES","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:14",""]
[2037,9376,11,1,"11/1"," A","11/1. A","","Provisional Sum of R80 000.00 (Eighty Thousand) for the services of a Community Liaison Officer  Note: This allowance is for salary, UIF, main contractor mark-up and ancillary costs","Item",{"v":1,"d":"1.00"},{"v":80000,"d":"80000.00"},{"v":80000,"d":"80000.00"},"","","26/06/2023 01:04:33",""]
[2038,9379,11,1,"11/2","","11/2","","PROVISIONAL SUMS FOR NOMINATED/SELECTED SUBCONTRACT WORKS","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:15",""]
[2039,9407,11,1,"11/2","","11/2","","ARTWORK","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:16",""]
[2040,12089,11,1,"11/2","","11/2","","Note : Previously appointed artists who have partially completed their work, and will be required to complete off-site studio work as well on-site installation","",{"v":0,"d":"0.0"},"","","","","03/11/2021 01:17:18",""]
[2041,9408,11,1,"11/2"," A","11/2. A","","Provisional Sum of R3 300 000.00 (Three Million Three Hundred Thousand) for major Artwork to be done by sub-contractors  1. Skylore : David Jones 2. Genodice Pond : Graham Jones 3. Genocide Wall : Graham Jones 4. Migration Map : Kim Lieberman 5. Songsmith : Jenna Burchell","Item",{"v":1,"d":"1.00"},{"v":3300000,"d":"3300000.00"},{"v":3300000,"d":"3300000.00"},"","","22/06/2023 08:38:50",""]
[2042,9411,11,1,"11/2"," B","11/2. B","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","21/06/2023 02:38:28",""]
[2043,9413,11,1,"11/2"," C","11/2. C","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","21/06/2023 02:38:31",""]
[2044,12380,11,1,"11/2"," D","11/2. D","","Provisional Sum of R200 000.00 (Two Hundred Thousand) for minor Artwork eg, graphic mosaic inlays, to be done by sub-contractors","Item",{"v":1,"d":"1.00"},{"v":200000,"d":"200000.00"},{"v":200000,"d":"200000.00"},"","","26/06/2023 09:49:37",""]
[2045,12382,11,1,"11/2"," E","11/2. E","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 09:49:47",""]
[2046,12381,11,1,"11/2"," F","11/2. F","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 09:49:51",""]
[2047,10314,11,1,"11/2"," G","11/2. G","","Provisional Sum of R80 000.00 (Eighty Thousand) for Poems to be done by a sub-contractor  Khoi-San Poems : Prof. D Ferrus","Item",{"v":1,"d":"1.00"},{"v":80000,"d":"80000.00"},{"v":80000,"d":"80000.00"},"","","20/06/2023 11:36:17",""]
[2048,10316,11,1,"11/2"," H","11/2. H","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","03/11/2021 01:18:37",""]
[2049,10317,11,1,"11/2"," I","11/2. I","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","03/11/2021 01:18:40",""]
[2050,9416,11,1,"11/3","","11/3","","ARTWORK CO-ORDINATOR","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:17",""]
[2051,9417,11,1,"11/3"," A","11/3. A","","Provisional Sum of R220 000.00 (Two Hundred and Twenty Thousand) for Artwork co-ordination to be done by a sub-contractor  Previously appointed person familiar with the works and who will be required to see the project through to completion : Theresa Hardman","Item",{"v":1,"d":"1.00"},"","","","","20/06/2023 11:36:30",""]
[2052,9418,11,1,"11/3"," B","11/3. B","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","12/11/2021 10:48:04",""]
[2053,9419,11,1,"11/3"," C","11/3. C","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","12/11/2021 10:48:09",""]
[2054,13819,11,1,"11/3","","11/3","","BACKUP POWER (GENERATORS)","H2",{"v":0,"d":"0.0"},"","","","","20/06/2023 11:49:55",""]
[2055,13820,11,1,"11/3"," D","11/3. D","","Provisional Sum of R1 000 000.00 (One Million) for the supply, installation and commissioning of generator backup equipment consisting of:  1 x 200kVA Generator (North side) 1 x 100kVA Generator (South side)","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:05:54",""]
[2056,13821,11,1,"11/3"," E","11/3. E","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:06:01",""]
[2057,13822,11,1,"11/3"," F","11/3. F","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:06:06",""]
[2058,13823,11,1,"11/3","","11/3","","BACKUP POWER (SOLAR)","H2",{"v":0,"d":"0.0"},"","","","","20/06/2023 11:50:04",""]
[2059,13824,11,1,"11/3"," G","11/3. G","","Provisional Sum of R950 000.00 (Nine Hundred and Fifty Thousand) for the supply, installation and commissioning of a 30kVA/3PH inverter system consisting of:  - 30kVA/3PH inverter and batteries - 30KW Grid tied PV system - All changes to associated DB boards, wiring, connections, etc. and relevant trenching required","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:06:24",""]
[2060,13825,11,1,"11/3"," H","11/3. H","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:06:32",""]
[2061,13826,11,1,"11/3"," I","11/3. I","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:06:37",""]
[2062,12093,11,1,"11/3","","11/3","","PUMP INSTALLATIONS","H2",{"v":0,"d":"0.0"},"","","","","03/11/2021 01:21:29",""]
[2063,12090,11,1,"11/3"," J","11/3. J","","Provisional Sum of R85 000.00 (Eighty Five Thousand) for the finalisation of water pump installations to be done by a specialist sub-contractor","Item",{"v":1,"d":"1.00"},{"v":85000,"d":"85000.00"},{"v":85000,"d":"85000.00"},"","","20/06/2023 11:36:48",""]
[2064,12091,11,1,"11/3"," K","11/3. K","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","03/11/2021 01:23:04",""]
[2065,12092,11,1,"11/4"," A","11/4. A","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","03/11/2021 01:23:10",""]
[2066,13810,11,1,"11/4","","11/4","","BOREHOLE INTEGRATION","H2",{"v":0,"d":"0.0"},"","","","","14/06/2023 03:17:41",""]
[2067,13811,11,1,"11/4"," B","11/4. B","","Provisional Sum of R350 000.00 (Three Hundred and Fifty Thousand) for the borehole integration installation to be done by a specialist sub-contractor","Item",{"v":1,"d":"1.00"},{"v":350000,"d":"350000.00"},{"v":350000,"d":"350000.00"},"","","20/06/2023 11:37:01",""]
[2068,13812,11,1,"11/4"," C","11/4. C","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","14/06/2023 03:20:28",""]
[2069,13813,11,1,"11/4"," D","11/4. D","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","14/06/2023 03:20:31",""]
[2070,9380,11,1,"11/4","","11/4","","SIGNAGE","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:15",""]
[2071,9382,11,1,"11/4"," E","11/4. E","","Provisional Sum of R450 000.00 (Four Hundred and Fifty Thousand) for external signage to be supplied and fitted by a selected sub-contractor","Item",{"v":1,"d":"1.00"},{"v":450000,"d":"450000.00"},{"v":450000,"d":"450000.00"},"","","20/06/2023 12:44:23",""]
[2072,9383,11,1,"11/4"," F","11/4. F","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","11/11/2021 09:25:38",""]
[2073,9384,11,1,"11/4"," G","11/4. G","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","11/11/2021 09:25:43",""]
[2074,9385,11,1,"11/4","","11/4","","LOOSE FURNITURE AND FITTINGS","H2",{"v":0,"d":"0.0"},"","","","","07/09/2021 07:03:15",""]
[2075,9386,11,1,"11/4"," H","11/4. H","","Provisional Sum of R400 000.00 (Four Hundred Thousand) for furniture and fittings","Item",{"v":1,"d":"1.00"},{"v":400000,"d":"400000.00"},{"v":400000,"d":"400000.00"},"","","20/06/2023 11:38:32",""]
[2076,9388,11,1,"11/4"," I","11/4. I","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","06/11/2021 12:08:48",""]
[2077,9390,11,1,"11/4"," J","11/4. J","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","06/11/2021 12:08:54",""]
[2078,12555,11,1,"11/4","","11/4","","APPLIANCES","H2",{"v":0,"d":"0.0"},"","","","","11/11/2021 09:26:59",""]
[2079,12556,11,1,"11/4"," K","11/4. K","","Provisional Sum of R100 000.00 (One Hundred Thousand) for appliances","Item",{"v":1,"d":"1.00"},{"v":100000,"d":"100000.00"},{"v":100000,"d":"100000.00"},"","","20/06/2023 11:41:10",""]
[2080,12557,11,1,"11/4"," L","11/4. L","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","15/11/2021 12:51:53",""]
[2081,12558,11,1,"11/4"," M","11/4. M","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","15/11/2021 12:51:57",""]
[2082,9392,11,1,"11/4","","11/4","","MATTRESSES, BEDDING, ETC.","H2",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:21:01",""]
[2083,9393,11,1,"11/4"," N","11/4. N","","Provisional Sum of R250 000.00 (Two Hundred and Fifty Thousand) for mattresses, bedding, etc.","Item",{"v":1,"d":"1.00"},{"v":250000,"d":"250000.00"},{"v":250000,"d":"250000.00"},"","","20/06/2023 11:41:22",""]
[2084,9394,11,1,"11/4"," O","11/4. O","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","07/09/2021 07:03:16",""]
[2085,9395,11,1,"11/5"," A","11/5. A","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","07/09/2021 07:03:16",""]
[2086,12085,11,1,"11/5","","11/5","","PRECISION PLASMA-CUT SIGNAGE","H2",{"v":0,"d":"0.0"},"","","","","03/11/2021 01:14:54",""]
[2087,12086,11,1,"11/5"," B","11/5. B","","Provisional Sum of R100 000.00 (One Hundred Thousand) for plasma-cut metal signage","Item",{"v":1,"d":"1.00"},{"v":100000,"d":"100000.00"},{"v":100000,"d":"100000.00"},"","","20/06/2023 12:44:01",""]
[2088,12087,11,1,"11/5"," C","11/5. C","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","03/11/2021 01:16:06",""]
[2089,12088,11,1,"11/5"," D","11/5. D","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","03/11/2021 01:16:11",""]
[2091,13921,11,2,"11/7","","11/7","","SECTION NO. 11","H1",{"v":0,"d":"0.0"},"","","","","11/07/2023 08:52:28",""]
[2092,13922,11,2,"11/7","","11/7","","BILL NO. 2","H1",{"v":0,"d":"0.0"},"","","","","11/07/2023 08:52:24",""]
[2093,13923,11,2,"11/7","","11/7","","PROVISIONAL SUMS : CONTRACT PARTICIPATION GOALS & CIDB BUILD PROGRAMME","H1",{"v":0,"d":"0.0"},"","","","","11/07/2023 01:39:05",""]
[2094,13949,11,2,"11/7","","11/7","","Note to tenderers: CPGs may not provide any bidder with a competitive advantage and therefore provisional amounts and fixed percentages for profit and attendance have been provided for tender purposes. Provisional amounts and profit and attendance will be adjusted once the awarded tender amount and/or the beneficiaries have been appointed, and the final values have been ascertained. Percentages will remain unchanged.","",{"v":0,"d":"0.0"},"","","","","11/07/2023 09:13:03",""]
[2095,13924,11,2,"11/7","","11/7","","MINIMUM TARGETED LOCAL BUILDING MATERIAL SUPPLIERS ","H3",{"v":0,"d":"0.0"},"","","","","11/07/2023 08:54:01",""]
[2096,13925,11,2,"11/7","","11/7","","Provision is made for the Minimum Targeted Local Building Material Suppliers CPG in the execution of this project as described in SCOPE OF WORKS. Material to the value of R2 130 000.00 should be purchased from local suppliers as defined in the CPG specifications in terms of locality (25km radius).","",{"v":0,"d":"0.0"},"","","","","24/07/2023 02:32:23",""]
[2097,13953,11,2,"11/7"," A","11/7. A","","Allowance for monitoring and monthly reporting on material purchased from Local Building Material Suppliers by the main contractor and subcontractors (Fixed at 3% of material value).","Item",{"v":1,"d":"1.00"},{"v":63900,"d":"63900.00"},{"v":63900,"d":"63900.00"},"","","24/07/2023 02:33:12",""]
[2098,13954,11,2,"11/7"," B","11/7. B","","Allowance for profit, all inclusive of associated costs to the contractor for implementation (Fixed at 5% of monitoring and reporting value).","Item",{"v":1,"d":"1.00"},{"v":3195,"d":"3195.00"},{"v":3195,"d":"3195.00"},"","","24/07/2023 02:33:17",""]
[2099,13955,11,2,"11/7"," C","11/7. C","","Allowance for attendance, all inclusive of associated costs to the contractor for implementation (Fixed at 5% of monitoring and reporting value).","Item",{"v":1,"d":"1.00"},{"v":3195,"d":"3195.00"},{"v":3195,"d":"3195.00"},"","","24/07/2023 02:33:22",""]
[2100,13934,11,2,"11/7","","11/7","","MINIMUM TARGETED ENTERPRISE DEVELOPMENT","H3",{"v":0,"d":"0.0"},"","","","","11/07/2023 08:54:01",""]
[2101,13935,11,2,"11/7"," D","11/7. D","","Provision is made for 5% compulsory subcontracting to SMMEs in the execution of this project as described in the SCOPE OF WORKS. The percentage is the contractor's allowance for Preliminaries for the SMME's. The PQS is to define the actual Preliminaries items applicable to the SMME's e.g. scaffolding , PPE, etc (Fixed at 7,5% of sub-contracting value).","Item",{"v":1,"d":"1.00"},{"v":342058,"d":"342058.00"},{"v":342058,"d":"342058.00"},"","","24/07/2023 04:12:53",""]
[2102,13936,11,2,"11/8"," A","11/8. A","","A provisional amount has been allowed for in the execution of this project as described in the  SCOPE OF WORKS. The provisional amount allowed is for the appointment of  training coordinator, mentor, training service providers and training of the beneficiary enterprises including monitoring and monthly reporting.","Item",{"v":1,"d":"1.00"},{"v":400000,"d":"400000.00"},{"v":400000,"d":"400000.00"},"","","24/07/2023 02:34:25",""]
[2103,13937,11,2,"11/8"," B","11/8. B","","Allowance for monitoring and monthly reporting on SMME subcontracting by main contractor and subcontractors including training provided (Fixed at 5% of Preliminaries and training values above).","Item",{"v":1,"d":"1.00"},{"v":37103,"d":"37103.00"},{"v":37103,"d":"37103.00"},"","","24/07/2023 04:13:00",""]
[2104,13938,11,2,"11/8"," C","11/8. C","","Allowance for profit, all inclusive of associated costs to the contractor for implementation (Fixed at 5% of Preliminaries and training values above).","Item",{"v":1,"d":"1.00"},{"v":37103,"d":"37103.00"},{"v":37103,"d":"37103.00"},"","","24/07/2023 04:13:06",""]
[2105,13939,11,2,"11/8"," D","11/8. D","","Allowance for attendance, all inclusive of associated costs to the contractor for implementation (Fixed at 5% of Preliminaries and training values above).","Item",{"v":1,"d":"1.00"},{"v":37103,"d":"37103.00"},{"v":37103,"d":"37103.00"},"","","24/07/2023 04:13:13",""]
[2106,13945,11,2,"11/8","","11/8","","LABOUR INTENSIVE PARTICIPATION GOAL","H3",{"v":0,"d":"0.0"},"","","","","11/07/2023 08:54:02",""]
[2107,13946,11,2,"11/8","","11/8","","Labour Intensive Participation Goal - Works to the value of approximately R1 738 000.00 to be executed by labour intensive means. Allowance for monthly reporting of labour intensive works by main contractor based on determination by PQS taking into account specific project variables.","",{"v":0,"d":"0.0"},"","","","","24/07/2023 02:35:49",""]
[2108,13947,11,2,"11/8"," E","11/8. E","","Allowance for monitoring and monthly reporting on Works executed by means of Labour Intensive methods by main contractor and subcontractors (Fixed at 2% of work value).","Item",{"v":1,"d":"1.00"},{"v":34760,"d":"34760.00"},{"v":34760,"d":"34760.00"},"","","24/07/2023 02:37:20",""]
[2109,13948,11,2,"11/8"," F","11/8. F","","Allowance for profit, all inclusive of associated costs to the contractor for implementation (Fixed at 10% of monitoring and reporting value).","Item",{"v":1,"d":"1.00"},{"v":3476,"d":"3476.00"},{"v":3476,"d":"3476.00"},"","","24/07/2023 02:36:16",""]
[2111,9355,11,3,"11/164","1","11/164.1","","Prov sums : sub-contractors","Page","11/6",0,"","","","02/11/2021 02:21:33",""]
[2112,13920,11,3,"11/164","2","11/164.2","","Prov sums : CPG & CIDB BUILD","Page","11/9",0,"","","","11/07/2023 08:34:56",""]
[2113,11058,12,1,"12/1","","12/1","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:48:41",""]
[2114,11059,12,1,"12/1","","12/1","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:55:23",""]
[2115,11060,12,1,"12/1","","12/1","","BILL NO. 1","H1",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:55:31",""]
[2116,11061,12,1,"12/1","","12/1","","WORK TO ADJACENT SCHOOL (ALL TRADES)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 10:55:30",""]
[2117,11063,12,1,"12/1","","12/1","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:56:11",""]
[2118,11064,12,1,"12/1","","12/1","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:20",""]
[2119,11065,12,1,"12/1","","12/1","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:56:19",""]
[2120,13319,12,1,"12/1","","12/1","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:25:43",""]
[2121,13320,12,1,"12/1","","12/1","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:25:43",""]
[2122,11066,12,1,"12/1","","12/1","","Materials arising from the demolitions and alterations","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:56:19",""]
[2123,11067,12,1,"12/1","","12/1","","Materials arising from the demolitions and alterations will become the property of the contractor.","",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:56:19",""]
[2124,11072,12,1,"12/1","","12/1","","ALTERATIONS","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:59:53",""]
[2125,11073,12,1,"12/1","","12/1","","Breaking up and removing unreinforced concrete","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:00:10",""]
[2126,11074,12,1,"12/1"," A","12/1. A","","100mm Thick surface bed","m2",0.2,"","","","","26/06/2023 11:00:57",""]
[2127,11075,12,1,"12/2","","12/2","","Taking down and removing roofs, floors, panelling, ceilings, partitions, etc.","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:00:46",""]
[2128,11076,12,1,"12/2"," A","12/2. A","","Gypsum plasterboard ceilings including cornices and timber ceiling brandering","m2",88,"","","","","12/11/2021 10:50:10",""]
[2129,11083,12,1,"12/2","","12/2","","Cutting through","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:02:40",""]
[2130,11084,12,1,"12/2"," B","12/2. B","","Saw cut through 100mm thick concrete floors","m",2,"","","","","27/10/2021 05:14:14",""]
[2131,11078,12,1,"12/2","","12/2","","Making good cement screeds","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:01:33",""]
[2132,11079,12,1,"12/2"," C","12/2. C","","Floors in patches","m2",0.2,"","","","","12/11/2021 10:50:15",""]
[2133,11080,12,1,"12/2","","12/2","","Repairs to joints and cracks in walls","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:02:05",""]
[2134,11189,12,1,"12/2"," D","12/2. D","","Repair cracks to plastered walls by exposing the full extent of the crack where directed, notifying the Principal Agent of the same, thoroughly clean and fill with Polycell Mendall 90 crack filler or equal approved, in strict accordance with the manufacturers instructions","m",18,"","","","","28/10/2021 10:33:42",""]
[2135,11129,12,1,"12/2","","12/2","","Taking out doors, windows, etc., including thresholds, sills, etc., setting aside for re-use and later refixing in similar new position","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:21:53",""]
[2136,11130,12,1,"12/2"," E","12/2. E","","Timber single door 813 x 2 032mm high overall, from steel frame","No",1,"","","","","28/10/2021 11:24:51",""]
[2137,11133,12,1,"12/2"," F","12/2. F","","Take from storage and re-fit previously set aside timber door to steel frame","No",1,"","","","","28/10/2021 11:24:47",""]
[2138,11099,12,1,"12/2","","12/2","","CONCRETE, FORMWORK AND REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:11:08",""]
[2139,11100,12,1,"12/2","","12/2","","UNREINFORCED CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:11:08",""]
[2140,11101,12,1,"12/2","","12/2","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:11:09",""]
[2141,11102,12,1,"12/2"," G","12/2. G","","In surface beds","m3",0.02,"","","","","26/06/2023 10:58:41",""]
[2142,11103,12,1,"12/2","","12/2","","MOVEMENT JOINTS, ETC","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:11:09",""]
[2143,11104,12,1,"12/2","","12/2","","Expansion joints with 12mm closed cell expanded polyethylene between vertical concrete surfaces","H4",{"v":0,"d":"0.0"},"","","","","28/10/2021 09:24:46",""]
[2144,11105,12,1,"12/2"," H","12/2. H","","Not exceeding 300mm high to edges of surface beds","m",2,"","","","","27/10/2021 05:15:42",""]
[2145,11068,12,1,"12/3","","12/3","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:57:02",""]
[2146,11124,12,1,"12/3","","12/3","","DAMPPROOFING OF WALLS AND FLOORS","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 02:46:56",""]
[2147,11125,12,1,"12/3","","12/3","","One layer 250 micron green polyethylene waterproof sheeting (SANS 952-1985 type C) sealed at laps with PVC self-adhesive tape","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 02:46:46",""]
[2148,11126,12,1,"12/3"," A","12/3. A","","Under surface beds","m2",0.2,"","","","","27/10/2021 05:15:35",""]
[2149,11069,12,1,"12/3","","12/3","","JOINT SEALANTS, ETC","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:57:02",""]
[2150,11070,12,1,"12/3","","12/3","","Polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 10:57:02",""]
[2151,11071,12,1,"12/3"," B","12/3. B","","12 x 10mm Pointing to expansion joints in floors including raking out joint filler","m",2,"","","","","15/11/2021 01:21:47",""]
[2152,12591,12,1,"12/3","","12/3","","CEILINGS, PARTITIONS AND ACCESS FLOORING","H2",{"v":0,"d":"0.0"},"","","","","11/11/2021 03:20:58",""]
[2153,12592,12,1,"12/3","","12/3","","NAILED-UP CEILINGS","H3",{"v":0,"d":"0.0"},"","","","","11/11/2021 03:20:48",""]
[2154,12593,12,1,"12/3","","12/3","","6,4mm Gypsum plasterboard with H-profile PVC jointing strips","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 08:51:52",""]
[2155,12594,12,1,"12/3"," C","12/3. C","","Ceilings including 38 x 38mm sawn softwood brandering at 45mm centres","m2",88,"","","","","15/11/2021 01:21:42",""]
[2156,12595,12,1,"12/3","","12/3","","Gypsum plasterboard cornices","H4",{"v":0,"d":"0.0"},"","","","","11/11/2021 03:22:59",""]
[2157,12596,12,1,"12/3"," D","12/3. D","","75mm Coved cornices","m",55,"","","","","12/11/2021 10:51:52",""]
[2158,11085,12,1,"12/3","","12/3","","PAINTWORK, ETC. TO PREVIOUSLY PAINTED WORK","H2",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:26:44",""]
[2159,11086,12,1,"12/3","","12/3","","Previously painted plastered surfaces","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:03:23",""]
[2160,11087,12,1,"12/3","","12/3","","Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied.  Blistered or peeling paint shall be completely removed and cracks opened, filled with a suitable filler and finished smooth  Provision is made elsewhere for hacking off loose and crumbling plaster and re-plastering such areas before painting is undertaken","",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:03:23",""]
[2161,11088,12,1,"12/3","","12/3","","ON FLOATED PLASTER OR PLASTERBOARD","H3",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:04:59",""]
[2162,11091,12,1,"12/4","","12/4","","Prepare surface by washing down with a solution of sugar soap (500g Polycell Sugar Soap Powder dissolved in 5 litres of hot/cold water (501703)) or (Polycell Sugar Soap Liquid (5018010)), rinse with tap water to remove all traces of sugar soap after area has been cleaned and allow to dry, remove all friable material, sand down to sound substrate, prime bare and repaired areas, and two coats low sheen paint (Colour to match existing school building) on:","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 02:59:09",""]
[2163,11092,12,1,"12/4"," A","12/4. A","","Walls","m2",131,"","","","","27/10/2021 05:15:20",""]
[2164,11093,12,1,"12/4","","12/4","","Prepare and apply one coat plaster primer and two coats low sheen acrylic paint (Colour to match existing school building) on:","H4",{"v":0,"d":"0.0"},"","","","","26/10/2021 11:05:10",""]
[2165,11094,12,1,"12/4"," B","12/4. B","","Walls","m2",45,"","","","","27/10/2021 05:15:23",""]
[2166,12587,12,1,"12/4","","12/4","","PAINTWORK, ETC. TO NEW WORK","H2",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:22:30",""]
[2167,12588,12,1,"12/4","","12/4","","ON INTERNAL GYPSUM PLASTER SURFACES","H3",{"v":0,"d":"0.0"},"","","","","11/11/2021 03:18:24",""]
[2168,12589,12,1,"12/4","","12/4","","One coat primer and two coats PVA on:","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 08:53:08",""]
[2169,12590,12,1,"12/4"," C","12/4. C","","Ceilings","m2",88,"","","","","12/11/2021 10:52:01",""]
[2171,8233,12,2,"12/6","","12/6","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:21:10",""]
[2172,8234,12,2,"12/6","","12/6","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:47",""]
[2173,8235,12,2,"12/6","","12/6","","BILL NO. 2","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:56:59",""]
[2174,10406,12,2,"12/6","","12/6","","SITE CLEARANCE AND BULK EARTHWORKS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:33",""]
[2175,13875,12,2,"12/6","","12/6","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:41",""]
[2176,13876,12,2,"12/6","","12/6","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:41",""]
[2177,13877,12,2,"12/6","","12/6","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2178,13878,12,2,"12/6","","12/6","","Civil Engineer's specifications","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2179,13879,12,2,"12/6","","12/6","","Tenderers are advised to study the \"Civil engineer's Specification\" before pricing this bill.  Where there are contradictions between this specification and the PW371 specification the Engineer shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2180,13880,12,2,"12/6","","12/6","","Materials arising from the demolitions and alterations","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2181,13881,12,2,"12/6","","12/6","","Materials arising from the demolitions and alterations will become the property of the contractor. An item is provided in the Calculation of Tender / Bid Sum at the end of the bills of quantities for \" Credit for old materials arising from the demolitions and alterations which become the property of the contractor\".","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2182,13882,12,2,"12/6","","12/6","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2183,13883,12,2,"12/7","","12/7","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2184,13884,12,2,"12/7","","12/7","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:39:55",""]
[2185,3549,12,2,"12/7","","12/7","","SITE CLEARANCE, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:08:12",""]
[2186,3550,12,2,"12/7","","12/7","","Site clearance","H4",{"v":0,"d":"0.0"},"","","","","11/08/2012 04:21:27",""]
[2187,3551,12,2,"12/7"," A","12/7. A","","Digging up and removing rubbish, debris, vegetation, hedges, shrubs, bush, etc. and trees not exceeding 200mm girth (previously cleared area of the site measured, excluding surfaced roads, pathways and buildings)","m2",9243,"","","","","07/12/2021 02:15:43",""]
[2188,7435,12,2,"12/7"," B","12/7. B","","Stripping average 200mm thick layer of top soil and depositing material in prescribed stock piles on site.","m2",10,"","","","","24/01/2014 03:11:59",""]
[2189,9631,12,2,"12/7","","12/7","","ALLOWANCE FOR MISCELLANEOUS UN-QUANTIFIABLE REMEDIAL WORK","H2",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:23:27",""]
[2190,9632,12,2,"12/7"," C","12/7. C","","Allow the sum of R4 000 000.00 (Four Million Rand) for sundry repairs and renovations, additional discovery work, and further deterioration of existing work to be measured and valued in terms of these Bills of Quantities","Item",{"v":1,"d":"1.00"},{"v":4000000,"d":"4000000.00"},{"v":4000000,"d":"4000000.00"},"","","28/06/2023 10:47:24",""]
[2192,10325,12,3,"12/9","","12/9","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:59",""]
[2193,10326,12,3,"12/9","","12/9","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:19:54",""]
[2194,10327,12,3,"12/9","","12/9","","BILL NO. 3","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:03",""]
[2195,10328,12,3,"12/9","","12/9","","EXTERNAL WATER SUPPLIES","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:38",""]
[2196,10329,12,3,"12/9","","12/9","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:59",""]
[2197,10330,12,3,"12/9","","12/9","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:02",""]
[2198,10331,12,3,"12/9","","12/9","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:59",""]
[2199,13321,12,3,"12/9","","12/9","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:26:58",""]
[2200,13322,12,3,"12/9","","12/9","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:26:58",""]
[2201,10334,12,3,"12/9","","12/9","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:59",""]
[2202,10335,12,3,"12/9","","12/9","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:59",""]
[2203,10336,12,3,"12/9","","12/9","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:59",""]
[2204,10337,12,3,"12/10","","12/10","","Note : The lifting, setting aside and later re-fitting of covers to allow for inspection, cleaning and/or repairs to catch pits, manholes, and draw chambers is not measured separately and is deemed to be included in the rates below.","",{"v":0,"d":"0.0"},"","","","","08/12/2021 10:35:19",""]
[2205,12425,12,3,"12/10","","12/10","","Replacement of pipelines","H3",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:01:08",""]
[2206,12475,12,3,"12/10"," A","12/10. A","","Excavation in earth not exceeding 2m deep for pipe trenches (Labour Intensive)","m3",115,"","","","","29/06/2023 08:28:23",""]
[2207,12476,12,3,"12/10"," B","12/10. B","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 90% Mod AASHTO density (Labour Intensive)","m3",88,"","","","","26/06/2023 11:01:41",""]
[2208,12477,12,3,"12/10"," C","12/10. C","","Imported G5 backfilling to pipe trenches, compacted to 95% Mod AASHTO density (Labour Intensive)","m3",10,"","","","","26/06/2023 11:01:46",""]
[2209,12478,12,3,"12/10"," D","12/10. D","","Bedding material supplied by the contractor, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",29,"","","","","26/06/2023 11:01:50",""]
[2210,12479,12,3,"12/10"," E","12/10. E","","Extra over all excavations for carting away surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",29,"","","","","12/11/2021 10:52:58",""]
[2211,12513,12,3,"12/10"," F","12/10. F","","Taking out HDPe water pipe exceeding 50mm and not exceeding 100mm external diameter and later re-laying in similar position (excavations, bedding and backfill elsewhere)","m",50,"","","","","08/12/2021 10:46:29",""]
[2212,12430,12,3,"12/10","","12/10","","Class 9 PVC pressure pipes with solvent welded joints in trenches (trenches elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 01:55:57",""]
[2213,12432,12,3,"12/10"," G","12/10. G","","110mm Pipes","m",15,"","","","","26/06/2023 10:59:18",""]
[2214,12435,12,3,"12/10"," H","12/10. H","","160mm Pipes","m",10,"","","","","26/06/2023 10:59:22",""]
[2215,12436,12,3,"12/10"," I","12/10. I","","200mm Pipes","m",20,"","","","","26/06/2023 10:59:26",""]
[2216,12437,12,3,"12/10","","12/10","","Class 10 HDPe type PE100 pipes in trenches (trenches elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 02:53:15",""]
[2217,12439,12,3,"12/10"," J","12/10. J","","32mm Pipes","m",91,"","","","","06/12/2021 02:54:02",""]
[2218,12442,12,3,"12/10"," K","12/10. K","","75mm Pipes","m",87,"","","","","06/12/2021 02:54:33",""]
[2219,12443,12,3,"12/10"," L","12/10. L","","110mm Pipes","m",50,"","","","","13/03/2023 02:37:21",""]
[2220,12426,12,3,"12/10","","12/10","","Repairs to inspections chambers, water meter chambers, etc.","H3",{"v":0,"d":"0.0"},"","","","","07/11/2021 09:51:37",""]
[2221,12427,12,3,"12/11","","12/11","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting around manhole covers in maximum 300mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","07/11/2021 11:30:41",""]
[2222,12428,12,3,"12/11"," A","12/11. A","","General shaping of areas around sumps, catch pits, inspection chambers, etc.","m3",19,"","","","","26/06/2023 11:05:20",""]
[2223,12429,12,3,"12/11","","12/11","","Cleaning of sumps, inspection chambers, etc.","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 10:35:31",""]
[2224,9654,12,3,"12/11"," B","12/11. B","","Clean out and remove silt, vegetation, rubble, etc. from  inside of square, rectangular or round catchpit, manhole or valve chamber (Labour Intensive)","No",13,"","","","","26/06/2023 11:02:08",""]
[2225,12472,12,3,"12/11","","12/11","","DEMOLITIONS","H2",{"v":0,"d":"0.0"},"","","","","08/11/2021 11:53:14",""]
[2226,12473,12,3,"12/11","","12/11","","Taking up/out water piping (excavations elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 08:54:21",""]
[2227,12474,12,3,"12/11"," C","12/11. C","","Piping exceeding 50mm and not exceeding 100mm external diameter","m",145,"","","","","08/12/2021 08:53:45",""]
[2228,13705,12,3,"12/11"," D","12/11. D","","Piping exceeding 100mm and not exceeding 150mm external diameter","m",15,"","","","","13/03/2023 02:36:07",""]
[2229,13704,12,3,"12/11"," E","12/11. E","","Piping exceeding 150mm and not exceeding 200mm external diameter","m",30,"","","","","13/03/2023 02:36:10",""]
[2230,12954,12,3,"12/11","","12/11","","Taking out and removing fire appliances and piping, including cutting off as necessary","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 10:13:25",""]
[2231,12955,12,3,"12/11"," F","12/11. F","","900mm High unreinforced concrete fire hydrant pedestal including hydrant valve and piping","No",1,"","","","","08/12/2021 10:43:32",""]
[2232,12468,12,3,"12/11","","12/11","","FIRE APPLIANCES, ETC","H2",{"v":0,"d":"0.0"},"","","","","07/11/2021 10:02:48",""]
[2233,12957,12,3,"12/11"," G","12/11. G","","80 x 65mm Brass right-angle shielded spindle hydrant valve with cap and chain, in accordance with SANS 1128-2","No",1,"","","","","19/11/2021 01:46:44",""]
[2234,12469,12,3,"12/11","","12/11","","Fire hydrant pedestals","H4",{"v":0,"d":"0.0"},"","","","","07/11/2021 10:02:48",""]
[2235,12470,12,3,"12/11"," H","12/11. H","","Unreinforced concrete hydrant pedestal 900mm high, cast around vertical pipe with bottom 300mm below ground, 305 x 305mm square at base and tapering to 200 x 200mm overall octagonal shaped top, including excavation, formwork and two coats of paint to exposed surfaces","No",1,"","","","","06/12/2021 02:55:30",""]
[2236,12959,12,3,"12/11","","12/11","","WATER SUPPLIES TO FIRE APPLIANCES","H2",{"v":0,"d":"0.0"},"","","","","19/11/2021 01:47:11",""]
[2237,12960,12,3,"12/12","","12/12","","Grade 316 stainless steel pipes","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 01:47:11",""]
[2238,12962,12,3,"12/12"," A","12/12. A","","100mm Pipes","m",1,"","","","","06/12/2021 02:55:53",""]
[2239,12963,12,3,"12/12","","12/12","","Extra over stainless steel pipes for welded fittings","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 01:47:11",""]
[2240,12966,12,3,"12/12"," B","12/12. B","","100mm Diameter long radius bend","No",1,"","","","","06/12/2021 02:56:20",""]
[2241,12967,12,3,"12/12","","12/12","","Sundries","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 01:47:11",""]
[2242,12968,12,3,"12/12"," C","12/12. C","","15Mpa Unreinforced concrete in thrust blocks in trenches at bends, tees, etc., including extra excavation, formwork, etc.","m3",1,"","","","","10/12/2021 03:24:43",""]
[2243,12461,12,3,"12/12","","12/12","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","07/11/2021 12:27:41",""]
[2244,12462,12,3,"12/12","","12/12","","Cleaning and disinfecting of water pipelines as per engineers specification (PSL 5.1.3)","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:24:55",""]
[2245,12463,12,3,"12/12"," D","12/12. D","","Pipeline not exceeding 200mm diameter","m",3997,"","","","","15/11/2021 01:19:53",""]
[2246,12464,12,3,"12/12"," E","12/12. E","","Site establishment of water pipe cleaning equipment","Item",{"v":1,"d":"1.00"},"","","","","08/12/2021 11:02:19",""]
[2247,12465,12,3,"12/12"," F","12/12. F","","Site de-establishment of water pipe cleaning equipment","Item",{"v":1,"d":"1.00"},"","","","","08/12/2021 11:02:25",""]
[2248,12459,12,3,"12/12","","12/12","","TESTING","H2",{"v":0,"d":"0.0"},"","","","","07/11/2021 12:20:19",""]
[2249,12460,12,3,"12/12"," G","12/12. G","","Pressure testing of pipeline not exceeding 200mm diameter as per engineers specification (PSL 7.3)","m",3810,"","","","","10/12/2021 03:25:10",""]
[2251,10396,12,4,"12/14","","12/14","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:28:12",""]
[2252,10397,12,4,"12/14","","12/14","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:02",""]
[2253,10398,12,4,"12/14","","12/14","","BILL NO. 4","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:07",""]
[2254,10395,12,4,"12/14","","12/14","","RESERVOIRS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:42",""]
[2255,10399,12,4,"12/14","","12/14","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:28:29",""]
[2256,10400,12,4,"12/14","","12/14","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:07",""]
[2257,10401,12,4,"12/14","","12/14","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:28:29",""]
[2258,13323,12,4,"12/14","","12/14","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:27:10",""]
[2259,13324,12,4,"12/14","","12/14","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:27:10",""]
[2260,12993,12,4,"12/14","","12/14","","Repairs to reservoirs","H3",{"v":0,"d":"0.0"},"","","","","30/11/2021 01:44:17",""]
[2261,13692,12,4,"12/14"," A","12/14. A","","Provisional sums allowance for water tightness testing and sealing of the water and fire reservoirs","Item",{"v":1,"d":"1.00"},"","","","","13/03/2023 02:46:34",""]
[2262,12531,12,4,"12/14","","12/14","","VALVES, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:08:31",""]
[2263,12532,12,4,"12/14","","12/14","","Note : references in brackets after descriptions refer to notes on drawings C5593-SITE-WAT-34, 35 and 43","",{"v":0,"d":"0.0"},"","","","","10/11/2021 12:57:20",""]
[2264,12533,12,4,"12/14"," B","12/14. B","","50mm Double flanged gate valve (reservoir control valve chamber fitting list item G)","No",2,"","","","","12/11/2021 11:00:30",""]
[2265,12534,12,4,"12/15"," A","12/15. A","","100mm Non-rising spindle RSV gate valve (reservoir control valve chamber fitting list item O)","No",3,"","","","","12/11/2021 11:00:40",""]
[2266,12535,12,4,"12/15"," B","12/15. B","","100mm Diameter Swing check valve (reservoir control valve chamber fitting list item P)","No",1,"","","","","12/11/2021 11:00:51",""]
[2267,12536,12,4,"12/15"," C","12/15. C","","150mm Non-rising spindle RSV gate valve (reservoir control valve chamber fitting list item Z)","No",2,"","","","","12/11/2021 11:00:59",""]
[2269,9574,12,5,"12/17","","12/17","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","14/09/2021 10:30:16",""]
[2270,9575,12,5,"12/17","","12/17","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:07",""]
[2271,9576,12,5,"12/17","","12/17","","BILL NO. 5","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:11",""]
[2272,9577,12,5,"12/17","","12/17","","PUMP STATION AND SUMP","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:48",""]
[2273,9578,12,5,"12/17","","12/17","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/09/2021 10:29:47",""]
[2274,9579,12,5,"12/17","","12/17","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:13",""]
[2275,9580,12,5,"12/17","","12/17","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/09/2021 10:29:47",""]
[2276,9581,12,5,"12/17","","12/17","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","14/09/2021 10:36:13",""]
[2277,9583,12,5,"12/17","","12/17","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:23:58",""]
[2278,10214,12,5,"12/17","","12/17","","Breaking up and removing plastered brick copings, including preparing walls below to receive new copings","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:12:33",""]
[2279,12319,12,5,"12/17"," A","12/17. A","","370 x 110mm Copings","m",17,"","","","","07/12/2021 09:13:19",""]
[2280,12448,12,5,"12/17","","12/17","","Repairs to sump, inspection chamber, etc.","H3",{"v":0,"d":"0.0"},"","","","","07/11/2021 11:49:36",""]
[2281,12450,12,5,"12/17","","12/17","","Cleaning of sumps, inspection chambers, etc.","H4",{"v":0,"d":"0.0"},"","","","","07/11/2021 12:01:35",""]
[2282,12449,12,5,"12/17"," B","12/17. B","","Clean out and remove silt, vegetation, rubble, etc., from  inside of square, rectangular or round catchpit, manhole or valve chamber","No",1,"","","","","26/06/2023 01:34:01",""]
[2283,12457,12,5,"12/18","","12/18","","Breaking up and removing of concrete roof slab of completed sumps, inspection chambers, etc., and construct new cover slab as per detail drawings (covers, frames and piping elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:23:32",""]
[2284,12458,12,5,"12/18"," A","12/18. A","","Cover slab to 1 800mm internal diameter sump chamber as per detail on drawing C5593-SITE-WAT-35","No",1,"","","","","26/06/2023 01:33:54",""]
[2285,12451,12,5,"12/18","","12/18","","Completion of partially built sumps, inspection chambers, etc. including precast concrete cover slabs (covers, frames and piping elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 10:05:28",""]
[2286,12452,12,5,"12/18"," B","12/18. B","","1 600 x 1 640mm Overall brick chamber including building up brickwork not exceeding 500mm to required level as per detail on drawing C5593-SITE-WAT-35","No",1,"","","","","27/06/2023 10:06:49",""]
[2287,13886,12,5,"12/18"," C","12/18. C","","One coat 1:5 cement plaster, on brickwork in draw chambers, catchpits, manholes, etc.","m2",4,"","","","","27/06/2023 10:06:55",""]
[2288,12453,12,5,"12/18","","12/18","","COVERS, ETC","H2",{"v":0,"d":"0.0"},"","","","","07/11/2021 11:55:30",""]
[2289,12454,12,5,"12/18"," D","12/18. D","","600 x 600mm x 38kg Type 9B Polymer lockable manhole cover and frame","No",2,"","","","","12/11/2021 11:01:46",""]
[2290,12361,12,5,"12/18","","12/18","","PRECAST CONCRETE COPINGS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:06:29",""]
[2291,12362,12,5,"12/18","","12/18","","Precast concrete finished smooth on exposed surfaces including bedding on ABE Epidermix epoxy mortar, jointing and pointing with ABE Dura cement grout with TAL keycoat water repellent additive in max. 5mm gaps between units","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:03:03",""]
[2292,12366,12,5,"12/18"," E","12/18. E","","440 x 100mm Thick overall Modcon, or similar approved, mono pitch coping weathered on top, with concave mortar  joints between units (coping type 021)","m",17,"","","","","12/11/2021 11:01:56",""]
[2293,12368,12,5,"12/18"," F","12/18. F","","Extra over for mitred angle intersection","No",4,"","","","","12/11/2021 11:02:01",""]
[2294,12369,12,5,"12/18","","12/18","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","05/11/2021 02:24:35",""]
[2295,12370,12,5,"12/18","","12/18","","Prepare and apply ABE Duraflex cementitous flexible slurry waterproofing with ecofelt membrane","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 02:24:35",""]
[2296,12371,12,5,"12/18"," G","12/18. G","","To tops of parapet walls","m2",4,"","","","","26/06/2023 01:03:47",""]
[2297,12372,12,5,"12/19","","12/19","","Prepare and apply TFC, or similar approved, cement sealant","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 02:24:35",""]
[2298,12373,12,5,"12/19"," A","12/19. A","","To general surfaces of precast concrete copings","m2",11,"","","","","12/11/2021 11:02:19",""]
[2299,12374,12,5,"12/19","","12/19","","SEALING STRIPS, JOINT SEALANTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:06:23",""]
[2300,12375,12,5,"12/19","","12/19","","Sikaflex 11FC polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 02:24:35",""]
[2301,12376,12,5,"12/19"," B","12/19. B","","5 x 5mm Pointing to expansion joints between precast concrete coping units","m",7,"","","","","12/11/2021 11:02:28",""]
[2302,9565,12,5,"12/19","","12/19","","STONE CLADDING TO WALLS, ETC","H3",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:06:37",""]
[2303,9566,12,5,"12/19","","12/19","","\"Potgieter gabion\" stone cladding, secured to wall with adhesive and short galvanised hoop iron strips shot pinned to walls","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 07:38:54",""]
[2304,9568,12,5,"12/19"," C","12/19. C","","75mm Lining to brick walls","m2",8,"","","","","08/12/2021 05:04:48",""]
[2305,9559,12,5,"12/19","","12/19","","Remove individual stones in wall cladding, prepare void for new stone and fix new suitably sized stones in position","H3",{"v":0,"d":"0.0"},"","","","","14/09/2021 10:22:18",""]
[2306,9560,12,5,"12/19","","12/19","","Stones from stockpiles on site (all sizes nominal diameter)","H4",{"v":0,"d":"0.0"},"","","","","14/09/2021 10:26:35",""]
[2307,9562,12,5,"12/19"," D","12/19. D","","Stone not exceeding 50mm","No",10,"","","","","08/12/2021 05:05:11",""]
[2308,9563,12,5,"12/19"," E","12/19. E","","Stone exceeding 50 and not exceeding 100mm","No",10,"","","","","08/12/2021 05:05:14",""]
[2309,9564,12,5,"12/19"," F","12/19. F","","Stone exceeding 100 and not exceeding 150mm","No",10,"","","","","08/12/2021 05:05:18",""]
[2310,9572,12,5,"12/19"," G","12/19. G","","Stone exceeding 150 and not exceeding 200mm","No",10,"","","","","08/12/2021 05:05:21",""]
[2311,13411,12,5,"12/19"," H","12/19. H","","Stone exceeding 200 and not exceeding 250mm","No",10,"","","","","08/12/2021 05:05:25",""]
[2312,9584,12,5,"12/19","","12/19","","Sundries","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 11:06:10",""]
[2313,9587,12,5,"12/19"," I","12/19. I","","Cut back protruding 30mm wide x 1,2mm thick galvanised mild steel cladding tie and coat cut with cold-galvanizing, in confined spaces in between stones (removal of cladding stones around metal tie elsewhere measured)","No",16,"","","","","13/03/2023 02:48:16",""]
[2314,9585,12,5,"12/20","","12/20","","Remove mortar splatter from stone surfaces","H4",{"v":0,"d":"0.0"},"","","","","14/09/2021 11:36:16",""]
[2315,9586,12,5,"12/20"," A","12/20. A","","General surfaces of stone cladding (measured over the flat surface on elevation)","m2",57,"","","","","13/03/2023 02:49:32",""]
[2316,12496,12,5,"12/20","","12/20","","SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","09/11/2021 08:26:35",""]
[2317,12497,12,5,"12/20"," B","12/20. B","","Provisional sums allowance for installation and commissioning of pumps (domestic water, raw water, sewer, irrigation including tanks, manifolds, etc.) in pump station and providing shop drawings for complete installations, by specialist contractors","Item",{"v":1,"d":"1.00"},{"v":30000,"d":"30000.00"},{"v":30000,"d":"30000.00"},"","","08/12/2021 11:11:16",""]
[2318,12498,12,5,"12/20"," C","12/20. C","","Allow for profit","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:04:09",""]
[2319,12499,12,5,"12/20"," D","12/20. D","","Allow for general attendance","Item",{"v":1,"d":"1.00"},"","","","","26/06/2023 01:04:13",""]
[2321,9781,12,6,"12/22","","12/22","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","06/10/2021 12:12:02",""]
[2322,9782,12,6,"12/22","","12/22","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:12",""]
[2323,9783,12,6,"12/22","","12/22","","BILL NO. 6","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:15",""]
[2324,9784,12,6,"12/22","","12/22","","EXTERNAL SEWER DRAINAGE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:53",""]
[2325,9999,12,6,"12/22","","12/22","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","13/10/2021 12:12:40",""]
[2326,10000,12,6,"12/22","","12/22","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:18",""]
[2327,10001,12,6,"12/22","","12/22","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","13/10/2021 12:12:40",""]
[2328,13325,12,6,"12/22","","12/22","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:27:33",""]
[2329,13326,12,6,"12/22","","12/22","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:27:33",""]
[2330,10004,12,6,"12/22","","12/22","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","13/10/2021 12:12:41",""]
[2331,10005,12,6,"12/22","","12/22","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","13/10/2021 12:12:41",""]
[2332,10006,12,6,"12/22","","12/22","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","13/10/2021 12:12:41",""]
[2333,9668,12,6,"12/23","","12/23","","Note : The lifting, setting aside and later re-fitting of covers to allow for inspection, cleaning and/or repairs to catch pits, manholes, and draw chambers is not measured separately and is deemed to be included in the rates below.","",{"v":0,"d":"0.0"},"","","","","08/12/2021 10:35:08",""]
[2334,9685,12,6,"12/23","","12/23","","Replacement of pipelines","H3",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:00:32",""]
[2335,13718,12,6,"12/23"," A","12/23. A","","Take up/out of sewer pipes not exceeding 160mm diameter (excavations elsewhere) (Labour Intensive)","m",20,"","","","","26/06/2023 11:04:18",""]
[2336,13476,12,6,"12/23"," B","12/23. B","","Excavation in earth not exceeding 2m deep to expose pipe lines (Labour Intensive)","m3",10,"","","","","26/06/2023 11:04:25",""]
[2337,13703,12,6,"12/23"," C","12/23. C","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",10,"","","","","26/06/2023 11:04:31",""]
[2338,13706,12,6,"12/23","","12/23","","Class 9 PVC pressure pipes with spigot and socket joints in trenches (Trenches elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:05:46",""]
[2339,13707,12,6,"12/23"," D","12/23. D","","110mm Pipes","m",5,"","","","","26/06/2023 11:52:22",""]
[2340,13708,12,6,"12/23","","12/23","","Heavy duty (Class 34) uPVC sewer and drain pipes in trenches (Trenches elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:06:12",""]
[2341,13709,12,6,"12/23"," E","12/23. E","","110mm Pipes","m",5,"","","","","13/03/2023 03:09:31",""]
[2342,13710,12,6,"12/23"," F","12/23. F","","160mm Pipes","m",10,"","","","","13/03/2023 03:09:45",""]
[2343,9686,12,6,"12/23","","12/23","","Cleaning of pipelines by rodding and introducing sufficient water to ensure motility of solids, rubbish and silt","H4",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:11",""]
[2344,9687,12,6,"12/23"," G","12/23. G","","110mm Pipeline","m",69,"","","","","31/10/2021 06:51:44",""]
[2345,9688,12,6,"12/23"," H","12/23. H","","160mm Pipeline","m",548,"","","","","31/10/2021 06:51:48",""]
[2346,9669,12,6,"12/23","","12/23","","Repairs to manholes","H3",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:10",""]
[2347,9670,12,6,"12/23","","12/23","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting around manhole covers in maximum 300mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","06/10/2021 11:14:29",""]
[2348,9671,12,6,"12/23"," I","12/23. I","","General shaping of areas around manholes","m3",5,"","","","","31/10/2021 06:49:17",""]
[2349,9678,12,6,"12/24","","12/24","","Cleaning of manholes","H4",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:10",""]
[2350,9712,12,6,"12/24"," A","12/24. A","","Clean out and remove silt, vegetation, rubble, etc. from  inside of square, rectangular or round catchpit, manhole or valve chamber","No",19,"","","","","08/12/2021 01:26:28",""]
[2351,9704,12,6,"12/24"," B","12/24. B","","Precast concrete sewer pump station and adjacent brick chamber as per detail on drawing C5593-SITE-SEW-13","No",1,"","","","","31/10/2021 06:54:34",""]
[2352,9672,12,6,"12/24","","12/24","","Seal pipe protrusions through precast concrete manhole rings with grout as per engineers specifications","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 10:42:25",""]
[2353,9673,12,6,"12/24"," C","12/24. C","","110mm Pipe","No",1,"","","","","31/10/2021 06:55:24",""]
[2354,9674,12,6,"12/24"," D","12/24. D","","160mm Pipe","No",3,"","","","","31/10/2021 06:55:27",""]
[2355,9675,12,6,"12/24","","12/24","","Seal internal joints of precast concrete manhole rings with an approved polyurethane cement or bitumastic filler as per detail B on dwg. C5593-SITE-SEW-14","H4",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:10",""]
[2356,9677,12,6,"12/24"," E","12/24. E","","Manhole 1 080mm internal dia. exceeding 1 000mm and not exceeding 1 500mm deep","No",2,"","","","","07/12/2021 03:31:38",""]
[2357,9717,12,6,"12/24"," F","12/24. F","","Ditto, exceeding 1 500mm and not exceeding 2 000mm deep","No",3,"","","","","06/12/2021 02:57:58",""]
[2358,9756,12,6,"12/24"," G","12/24. G","","Ditto, exceeding 2 000mm and not exceeding 2 500mm deep","No",1,"","","","","06/12/2021 02:58:09",""]
[2359,9708,12,6,"12/24"," H","12/24. H","","Ditto, exceeding 2 500mm and not exceeding 3 000mm deep","No",1,"","","","","06/12/2021 02:58:21",""]
[2360,9743,12,6,"12/24","","12/24","","Seal external joints of precast concrete manhole rings with self adhesive tape including cleaning and priming of external surface and internal joints with an approved polyurethane cement or bitumastic filler as per detail B on dwg. C5593-SITE-SEW-14","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:22:28",""]
[2361,9744,12,6,"12/24"," I","12/24. I","","Manhole 1 080mm internal dia. exceeding 1 000mm and not exceeding 1 500mm deep","No",1,"","","","","31/10/2021 06:54:48",""]
[2362,12493,12,6,"12/24","","12/24","","Take out/off existing manhole covers","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 03:36:16",""]
[2363,12494,12,6,"12/24"," J","12/24. J","","Take up polymer cover (cover only) and replace with new lockable cover (no frame) (lockable cover elsewhere)","No",1,"","","","","07/12/2021 03:47:35",""]
[2364,9680,12,6,"12/24","","12/24","","Breaking up and removing benching to bottoms of completed manholes ","H4",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:10",""]
[2365,9728,12,6,"12/24"," K","12/24. K","","1 080mm Internal dia. exceeding 2 000mm and not exceeding 2 500mm deep","No",1,"","","","","08/12/2021 04:33:25",""]
[2366,9706,12,6,"12/25"," A","12/25. A","","Ditto, exceeding 2 500mm and not exceeding 3 000mm deep","No",1,"","","","","08/12/2021 01:27:16",""]
[2367,9683,12,6,"12/25","","12/25","","Construct benching to bottoms of completed manholes, in accordance with dwg. C5593-SITE-SEW-14","H4",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:11",""]
[2368,9707,12,6,"12/25"," B","12/25. B","","1 080mm Internal dia. exceeding 2 500mm deep and not exceeding 3 000mm deep","No",1,"","","","","08/12/2021 04:33:33",""]
[2369,9689,12,6,"12/25","","12/25","","Repairs to rodding eyes","H3",{"v":0,"d":"0.0"},"","","","","04/10/2021 11:41:11",""]
[2370,9690,12,6,"12/25","","12/25","","Heavy duty (Class 34) uPVC sewer and drain pipes","H4",{"v":0,"d":"0.0"},"","","","","06/10/2021 11:14:49",""]
[2371,9691,12,6,"12/25"," C","12/25. C","","110mm Pipes vertically or ramped to cleaning eyes, etc. (no excavation)","m",1,"","","","","10/12/2021 03:27:43",""]
[2372,9692,12,6,"12/25"," D","12/25. D","","160mm Pipes vertically or ramped to cleaning eyes, etc. (no excavation)","m",1,"","","","","10/12/2021 03:27:55",""]
[2373,9693,12,6,"12/25"," E","12/25. E","","Cut back and remove short length of 110mm pipe","No",1,"","","","","31/10/2021 06:52:14",""]
[2374,9694,12,6,"12/25"," F","12/25. F","","Cut back and remove short length of 160mm pipe","No",1,"","","","","31/10/2021 06:52:18",""]
[2375,9737,12,6,"12/25"," G","12/25. G","","Take out installed rodding eye, set aside and later reinstall in similar position (concrete surround elsewhere)","No",1,"","","","","08/12/2021 12:01:41",""]
[2376,9695,12,6,"12/25"," H","12/25. H","","Break up and remove unreinforced concrete rodding eye surround approximately 300 x 300 x 150mm thick","No",1,"","","","","10/12/2021 03:28:09",""]
[2377,9696,12,6,"12/25"," I","12/25. I","","Cast unreinforced concrete rodding eye cover surround size 500 x 500 x 150mm thick, including necessary shallow excavations, form work, backfilling, etc.","No",2,"","","","","08/12/2021 11:59:42",""]
[2378,9780,12,6,"12/25","","12/25","","TESTING","H2",{"v":0,"d":"0.0"},"","","","","06/10/2021 12:09:01",""]
[2379,9703,12,6,"12/25"," J","12/25. J","","CCTV inspection including video recording and marking-up suspected internal pipeline defects on drawings (drawings by others) of pipeline not exceeding 160mm diameter (PSLD 7.2.8)","m",616,"","","","","10/12/2021 03:28:22",""]
[2380,9715,12,6,"12/25"," K","12/25. K","","Pressure testing of pipeline not exceeding 160mm diameter as per engineers specifications","m",616,"","","","","10/12/2021 10:49:16",""]
[2381,9701,12,6,"12/25"," L","12/25. L","","Water tightness testing of manhole - per manhole (PSLD 7.2.6)","No",19,"","","","","08/12/2021 05:04:35",""]
[2382,9702,12,6,"12/25"," M","12/25. M","","Torch and mirror test - per manhole (PSLD 7.2.7)","No",28,"","","","","31/10/2021 06:50:39",""]
[2383,10386,12,6,"12/25","","12/25","","SEWER CONSERVANCY TANK","H2",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:32:58",""]
[2384,11009,12,6,"12/26","","12/26","","Repairs to conservancy tank","H3",{"v":0,"d":"0.0"},"","","","","25/10/2021 12:46:03",""]
[2385,11010,12,6,"12/26","","12/26","","Cleaning of insides of tanks","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 11:06:19",""]
[2386,11011,12,6,"12/26"," A","12/26. A","","170KL sewer conservancy tank","No",1,"","","","","08/12/2021 11:06:34",""]
[2388,9835,12,7,"12/28","","12/28","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:22:20",""]
[2389,9836,12,7,"12/28","","12/28","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:16",""]
[2390,9837,12,7,"12/28","","12/28","","BILL NO. 7","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:19",""]
[2391,9838,12,7,"12/28","","12/28","","STORMWATER DRAINAGE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:23:58",""]
[2392,13329,12,7,"12/28","","12/28","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:28:54",""]
[2393,13330,12,7,"12/28","","12/28","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:22",""]
[2394,13331,12,7,"12/28","","12/28","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:28:54",""]
[2395,13336,12,7,"12/28","","12/28","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:29:09",""]
[2396,13337,12,7,"12/28","","12/28","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:29:09",""]
[2397,9839,12,7,"12/28","","12/28","","Note : The lifting, setting aside and later re-fitting of covers/gratings, etc. to allow for inspection, cleaning and/or repairs to sumps, catch pits, inspection chambers, and draw chambers are not measured separately and is deemed to be included in the rates below.","",{"v":0,"d":"0.0"},"","","","","06/10/2021 04:29:30",""]
[2398,13334,12,7,"12/28","","12/28","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:28:54",""]
[2399,13335,12,7,"12/28","","12/28","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:28:54",""]
[2400,13711,12,7,"12/29","","12/29","","Replacement of pipelines","H3",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:20:07",""]
[2401,13717,12,7,"12/29"," A","12/29. A","","Take up/out and remove concrete stormwater pipes not exceeding 525mm diameter (excavations elsewhere)","m",25,"","","","","13/03/2023 03:26:08",""]
[2402,13712,12,7,"12/29"," B","12/29. B","","Excavation in earth not exceeding 2m deep to expose pipes (Labour Intensive)","m3",25,"","","","","26/06/2023 11:07:36",""]
[2403,13713,12,7,"12/29"," C","12/29. C","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",25,"","","","","26/06/2023 11:07:46",""]
[2404,13714,12,7,"12/29","","12/29","","Class 100D concrete pipes to SANS677","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:20:45",""]
[2405,13715,12,7,"12/29"," D","12/29. D","","450mm Pipes laid in trenches (Trenches elsewhere)","m",15,"","","","","26/06/2023 11:07:55",""]
[2406,13716,12,7,"12/29"," E","12/29. E","","525mm Pipes laid in trenches (Trenches elsewhere)","m",10,"","","","","26/06/2023 11:08:02",""]
[2407,9834,12,7,"12/29","","12/29","","Repairs to inspections chambers","H3",{"v":0,"d":"0.0"},"","","","","06/10/2021 04:28:01",""]
[2408,9903,12,7,"12/29","","12/29","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting around manhole covers in maximum 300mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","08/10/2021 12:08:54",""]
[2409,9904,12,7,"12/29"," F","12/29. F","","General shaping of areas around sumps, catch pits, inspection chambers, etc.","m3",5,"","","","","31/10/2021 06:43:03",""]
[2410,9846,12,7,"12/29","","12/29","","Seal pipe protrusions through brick inspection chambers with grout as per engineers specifications","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 12:59:14",""]
[2411,10024,12,7,"12/29"," G","12/29. G","","110mm Pipe","No",2,"","","","","31/10/2021 06:43:16",""]
[2412,10025,12,7,"12/29"," H","12/29. H","","160mm Pipe","No",2,"","","","","31/10/2021 06:43:19",""]
[2413,9847,12,7,"12/29"," I","12/29. I","","450mm Pipe","No",6,"","","","","31/10/2021 06:57:11",""]
[2414,9815,12,7,"12/29","","12/29","","Cleaning of sumps, catchpits, inspection chambers, etc., including cutting and removing protruding rebars","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:28:51",""]
[2415,13693,12,7,"12/29"," J","12/29. J","","Clean out and remove silt, vegetation, rubble, etc. from  inside of square, rectangular or round catchpit, manhole or valve chamber (Labour Intensive)","No",47,"","","","","26/06/2023 11:08:47",""]
[2416,9941,12,7,"12/30","","12/30","","Construct benching to bottoms of completed sumps, catchpits, inspection chambers, etc. in accordance with dwg. C5593-SITE-SW-54 & 55","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:05:28",""]
[2417,9942,12,7,"12/30"," A","12/30. A","","930 x 930mm Brick inspection chamber exceeding 1 000mm and not exceeding 2 000mm deep internally","No",1,"","","","","08/12/2021 01:07:08",""]
[2418,9910,12,7,"12/30","","12/30","","Take out/off covers, frames, etc. and set aside for re-use and later refixing in similar new position","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:06:37",""]
[2419,9911,12,7,"12/30"," B","12/30. B","","Single steel inlet grid from frame size 610 x 610mm overall","No",11,"","","","","08/12/2021 01:06:52",""]
[2420,9905,12,7,"12/30","","12/30","","Repairs to headwalls","H3",{"v":0,"d":"0.0"},"","","","","08/10/2021 12:09:44",""]
[2421,9906,12,7,"12/30","","12/30","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting in maximum 300mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","08/10/2021 12:10:11",""]
[2422,9907,12,7,"12/30"," C","12/30. C","","General shaping of areas around sumps, catch pits, inspection chambers, headwalls, etc","m3",16,"","","","","31/10/2021 06:46:00",""]
[2423,9959,12,7,"12/30","","12/30","","Cutting back of concrete pipe protrusions from headwalls (pipes to be flush with headwall)","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:07:31",""]
[2424,9960,12,7,"12/30"," D","12/30. D","","450mm Pipes","No",1,"","","","","31/10/2021 06:46:30",""]
[2425,11187,12,7,"12/30","","12/30","","Filling of gravel-soil material G7 supplied by the contractor, compacted to 93% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:09:00",""]
[2426,11188,12,7,"12/30"," E","12/30. E","","Backfilling around headwalls and excavations, etc.","m3",10,"","","","","08/12/2021 01:07:52",""]
[2427,10295,12,7,"12/30","","12/30","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 02:43:15",""]
[2428,10296,12,7,"12/30","","12/30","","Breaking up and removing unreinforced concrete","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 02:43:15",""]
[2429,12127,12,7,"12/30"," F","12/30. F","","Surface beds, slabs, aprons, etc.","m3",21,"","","","","04/11/2021 01:14:01",""]
[2430,10297,12,7,"12/30"," G","12/30. G","","Manhole cover slabs, bases, surrounds, etc.","m3",5,"","","","","04/11/2021 01:15:14",""]
[2431,10298,12,7,"12/30","","12/30","","Breaking up and removing reinforced concrete, including cutting off and removing reinforcement","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 02:43:15",""]
[2432,12128,12,7,"12/30"," H","12/30. H","","Surface beds, slabs, aprons, etc.","m3",16,"","","","","04/11/2021 01:14:52",""]
[2433,10299,12,7,"12/30"," I","12/30. I","","Manhole cover slabs, bases, surrounds, etc.","m3",4,"","","","","04/11/2021 01:15:18",""]
[2434,10300,12,7,"12/31","","12/31","","Breaking down and removing brickwork, etc.","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 04:51:08",""]
[2435,10301,12,7,"12/31"," A","12/31. A","","Mass brickwork","m3",4,"","","","","07/12/2021 04:28:10",""]
[2436,10302,12,7,"12/31"," B","12/31. B","","One brick walls","m2",8,"","","","","07/12/2021 04:28:14",""]
[2437,12307,12,7,"12/31","","12/31","","Taking up and removing piping","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 12:47:55",""]
[2438,12308,12,7,"12/31"," C","12/31. C","","160mm uPVC pipes (Trenches elsewhere)","m",7,"","","","","26/06/2023 11:09:18",""]
[2439,9791,12,7,"12/31","","12/31","","SUB-SOIL DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","06/10/2021 04:24:03",""]
[2440,9792,12,7,"12/31","","12/31","","Earthworks","H4",{"v":0,"d":"0.0"},"","","","","06/10/2021 04:24:03",""]
[2441,9793,12,7,"12/31"," D","12/31. D","","Excavation in earth not exceeding 2m deep for pipe trenches","m3",5,"","","","","12/11/2021 11:03:59",""]
[2442,9796,12,7,"12/31"," E","12/31. E","","Backfilling to pipe trenches with material from the excavations or stockpiles on site, compacted to 93% Mod AASHTO density","m3",3,"","","","","12/11/2021 11:04:05",""]
[2443,9797,12,7,"12/31"," F","12/31. F","","Imported G5 backfilling to pipe trenches, compacted to 93% Mod AASHTO density","m3",1,"","","","","08/12/2021 05:03:45",""]
[2444,9798,12,7,"12/31"," G","12/31. G","","Selected granular filling from stock piles on site in bedding under and filling around pipes compacted to 95% Modified AASHTO density","m3",1,"","","","","08/12/2021 05:03:49",""]
[2445,9799,12,7,"12/31"," H","12/31. H","","Bedding material supplied by the contractor, compacted to 93% Mod AASHTO density","m3",2,"","","","","10/12/2021 03:30:00",""]
[2446,9800,12,7,"12/31"," I","12/31. I","","Extra over all excavations for carting away surplus material from excavations and/or stock piles on site to a dumping site to be located by the contractor","m3",2,"","","","","12/11/2021 11:04:17",""]
[2447,12309,12,7,"12/31","","12/31","","Heavy duty (Class 34) uPVC stormwater pipes","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 12:50:49",""]
[2448,12310,12,7,"12/31"," J","12/31. J","","160mm Pipes laid in trenches (Trenches elsewhere)","m",7,"","","","","12/11/2021 11:04:25",""]
[2449,10460,12,7,"12/31","","12/31","","CLEANING OF SURFACE CHANNELS","H2",{"v":0,"d":"0.0"},"","","","","17/10/2021 05:18:08",""]
[2450,10461,12,7,"12/31"," K","12/31. K","","Clean surface channel not exceeding 1m wide, by removing all silt, sand, rubbish and vegetation (Labour Intensive)","m",1800,"","","","","26/06/2023 11:10:02",""]
[2451,9853,12,7,"12/31","","12/31","","CLEANING OF PIPES","H2",{"v":0,"d":"0.0"},"","","","","07/10/2021 11:21:04",""]
[2452,9840,12,7,"12/31","","12/31","","Pressure hydro-jetting of existing pipe lines","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 12:55:08",""]
[2453,9841,12,7,"12/31"," L","12/31. L","","Pressure hydro-jetting of pipeline not exceeding 525mm diameter","m",901,"","","","","31/10/2021 06:47:10",""]
[2454,9842,12,7,"12/32"," A","12/32. A","","Site establishment of pressure-jetting equipment","Item",{"v":1,"d":"1.00"},"","","","","31/10/2021 06:47:01",""]
[2455,9843,12,7,"12/32"," B","12/32. B","","Site de-establishment of pressure-jetting equipment","Item",{"v":1,"d":"1.00"},"","","","","31/10/2021 06:47:05",""]
[2456,9785,12,7,"12/32","","12/32","","TESTING","H2",{"v":0,"d":"0.0"},"","","","","06/10/2021 04:17:01",""]
[2457,9786,12,7,"12/32"," C","12/32. C","","CCTV inspection including video recording and marking-up suspected internal pipeline defects on drawings (drawings by others) of pipeline not exceeding 525mm diameter (PSLE 7.2.1)","m",901,"","","","","10/12/2021 03:30:15",""]
[2458,9789,12,7,"12/32"," D","12/32. D","","Torch and mirror test - per catchpit/inspection chamber (PSLE 7.2.2)","No",86,"","","","","31/10/2021 06:47:34",""]
[2460,9858,12,8,"12/34","","12/34","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","07/10/2021 12:13:37",""]
[2461,9859,12,8,"12/34","","12/34","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:21",""]
[2462,9860,12,8,"12/34","","12/34","","BILL NO. 8","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:24",""]
[2463,10383,12,8,"12/34","","12/34","","STORMWATER HARVESTING TANK AND OIL INTERCEPTOR","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:03",""]
[2464,13338,12,8,"12/34","","12/34","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:29:53",""]
[2465,13339,12,8,"12/34","","12/34","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:27",""]
[2466,13340,12,8,"12/34","","12/34","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:29:54",""]
[2467,13345,12,8,"12/34","","12/34","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:09",""]
[2468,13346,12,8,"12/34","","12/34","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:09",""]
[2469,13343,12,8,"12/34","","12/34","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:29:54",""]
[2470,13344,12,8,"12/34","","12/34","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:29:54",""]
[2471,9869,12,8,"12/34","","12/34","","Repairs to harvesting tank","H3",{"v":0,"d":"0.0"},"","","","","07/10/2021 01:33:06",""]
[2472,9870,12,8,"12/35","","12/35","","Cutting back end of protruding rebar, including chipping surrounding concrete sufficiently to provide 50mm concrete cover, and repair holes with suitable waterproof industrial epoxy grouting","H4",{"v":0,"d":"0.0"},"","","","","27/06/2023 02:38:48",""]
[2473,9871,12,8,"12/35"," A","12/35. A","","Rebar from concrete walls, etc.","No",10,"","","","","27/06/2023 02:38:10",""]
[2474,9874,12,8,"12/35","","12/35","","Cleaning of insides of tanks","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 11:07:03",""]
[2475,9877,12,8,"12/35"," B","12/35. B","","260kl Stormwater harvesting tank as per engineers specifications","No",1,"","","","","27/06/2023 10:04:27",""]
[2476,9891,12,8,"12/35","","12/35","","DEMOLITIONS","H2",{"v":0,"d":"0.0"},"","","","","08/12/2021 01:40:36",""]
[2477,9892,12,8,"12/35"," C","12/35. C","","Reinforced concrete oil interceptor tank structure (without roof slab), 3 x 4,3m on plan and 2,9m high overall, comprising of reinforced concrete surface bed, reinforced concrete perimeter and internal walls","No",1,"","","","","10/12/2021 03:30:42",""]
[2478,11013,12,8,"12/35","","12/35","","PREPARATORY WORK TO EXISTING SURFACES","H2",{"v":0,"d":"0.0"},"","","","","25/10/2021 02:15:28",""]
[2479,11016,12,8,"12/35","","12/35","","Prepare concrete surface by wire brushing or bush-hammering to expose aggregate and apply wet to dry epoxy mix","H4",{"v":0,"d":"0.0"},"","","","","31/10/2021 06:32:02",""]
[2480,11014,12,8,"12/35"," D","12/35. D","","Top of slabs","m2",1,"","","","","31/10/2021 06:32:07",""]
[2481,11017,12,8,"12/35"," E","12/35. E","","Sides of walls","m2",1,"","","","","31/10/2021 06:32:11",""]
[2482,9862,12,8,"12/35","","12/35","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:31:28",""]
[2483,10247,12,8,"12/35","","12/35","","EXCAVATIONS, ETC","H3",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:31:32",""]
[2484,9864,12,8,"12/35","","12/35","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","07/10/2021 12:15:05",""]
[2485,9865,12,8,"12/35"," F","12/35. F","","Holes, partially underneath existing structure (no supports required) (Labour Intensive)","m3",2,"","","","","26/06/2023 11:10:40",""]
[2486,10251,12,8,"12/35","","12/35","","UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:30",""]
[2487,10252,12,8,"12/35","","12/35","","15MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:30",""]
[2488,10253,12,8,"12/35"," G","12/35. G","","Surface blinding under surface beds","m3",1,"","","","","27/06/2023 02:38:43",""]
[2489,10254,12,8,"12/36","","12/36","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:30",""]
[2490,10255,12,8,"12/36","","12/36","","40MPa/19mm Concrete with an approved waterproofing admixture(C500NF at a ratio of 1.5% by weight of total cementitious material, including blastfurnace slag) added at the batching plant","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:30",""]
[2491,10256,12,8,"12/36"," A","12/36. A","","Surface beds","m3",4,"","","","","07/12/2021 04:47:37",""]
[2492,10257,12,8,"12/36"," B","12/36. B","","Walls","m3",10,"","","","","07/12/2021 04:47:43",""]
[2493,10259,12,8,"12/36","","12/36","","TEST CUBES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:31",""]
[2494,10260,12,8,"12/36"," C","12/36. C","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",7,"","","","","30/10/2021 08:42:01",""]
[2495,10261,12,8,"12/36","","12/36","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:31",""]
[2496,10262,12,8,"12/36","","12/36","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:31",""]
[2497,10263,12,8,"12/36"," D","12/36. D","","Surface beds, slabs, etc. to falls","m2",16,"","","","","26/06/2023 11:11:05",""]
[2498,10264,12,8,"12/36","","12/36","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:31",""]
[2499,10265,12,8,"12/36","","12/36","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:41:31",""]
[2500,10266,12,8,"12/36"," E","12/36. E","","Walls with total height not exceeding 3,5m above bearing level","m2",104,"","","","","07/12/2021 04:47:56",""]
[2501,10269,12,8,"12/36","","12/36","","Rough formwork to form","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:42:01",""]
[2502,10270,12,8,"12/36"," F","12/36. F","","75mm Diameter opening through not exceeding 300mm thick wall or beam","No",1,"","","","","30/10/2021 08:42:18",""]
[2503,10271,12,8,"12/36"," G","12/36. G","","450mm Diameter opening through not exceeding 300mm thick wall or beam","No",1,"","","","","30/10/2021 08:42:22",""]
[2504,10272,12,8,"12/36"," H","12/36. H","","525mm Diameter opening through not exceeding 300mm thick wall or beam","No",1,"","","","","30/10/2021 08:42:26",""]
[2505,10273,12,8,"12/36"," I","12/36. I","","560mm Diameter opening through not exceeding 300mm thick wall or beam","No",1,"","","","","30/10/2021 08:42:29",""]
[2506,10279,12,8,"12/36","","12/36","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:42:01",""]
[2507,13001,12,8,"12/37","","12/37","","Mesh reinforcement with 300mm side and end laps in surface beds, walls, slabs, etc.","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 10:31:28",""]
[2508,13004,12,8,"12/37"," A","12/37. A","","Type 311 Mesh reinforcement","m2",17,"","","","","08/12/2021 05:03:24",""]
[2509,13003,12,8,"12/37"," B","12/37. B","","Type 500 Mesh reinforcement","m2",75,"","","","","08/12/2021 05:03:27",""]
[2510,13002,12,8,"12/37"," C","12/37. C","","Type 617 Mesh reinforcement","m2",30,"","","","","08/12/2021 05:03:32",""]
[2511,10280,12,8,"12/37","","12/37","","Mild steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:42:01",""]
[2512,10281,12,8,"12/37"," D","12/37. D","","Various diameter bars","t",{"v":0.1,"d":"0.10"},"","","","","08/12/2021 04:53:52",""]
[2513,10282,12,8,"12/37","","12/37","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 09:42:01",""]
[2514,10283,12,8,"12/37"," E","12/37. E","","Various diameter bars","t",0.56,"","","","","08/12/2021 04:54:01",""]
[2516,10338,12,9,"12/39","","12/39","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:23:54",""]
[2517,10339,12,9,"12/39","","12/39","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:25",""]
[2518,10340,12,9,"12/39","","12/39","","BILL NO. 9","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:31",""]
[2519,10375,12,9,"12/39","","12/39","","WATER PONDS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:08",""]
[2520,10376,12,9,"12/39","","12/39","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:49",""]
[2521,10377,12,9,"12/39","","12/39","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:31",""]
[2522,10378,12,9,"12/39","","12/39","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:49",""]
[2523,13347,12,9,"12/39","","12/39","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:19",""]
[2524,13348,12,9,"12/39","","12/39","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:19",""]
[2525,10381,12,9,"12/39","","12/39","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:50",""]
[2526,10382,12,9,"12/39","","12/39","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:50",""]
[2527,12079,12,9,"12/39","","12/39","","DEMOLITIONS","H2",{"v":0,"d":"0.0"},"","","","","03/11/2021 11:51:48",""]
[2528,12081,12,9,"12/39","","12/39","","Breaking up and removing","H4",{"v":0,"d":"0.0"},"","","","","03/11/2021 11:56:19",""]
[2529,12082,12,9,"12/39"," A","12/39. A","","250mm Thick reinforced concrete surface beds, paving, etc.","m2",16,"","","","","10/12/2021 03:31:21",""]
[2530,12083,12,9,"12/39"," B","12/39. B","","350mm Thick reinforced concrete surface beds, paving, etc.","m2",7,"","","","","10/12/2021 03:31:27",""]
[2531,12100,12,9,"12/40","","12/40","","Taking up and removing piping (no excavations)","H4",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:19:53",""]
[2532,12101,12,9,"12/40"," A","12/40. A","","50mm PVC pipe, including fittings","m",45,"","","","","04/11/2021 01:17:04",""]
[2533,12104,12,9,"12/40"," B","12/40. B","","90mm HDPe pipe, including fittings","m",8,"","","","","10/12/2021 02:44:04",""]
[2534,12159,12,9,"12/40","","12/40","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:33:14",""]
[2535,12160,12,9,"12/40","","12/40","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:33:14",""]
[2536,12161,12,9,"12/40"," C","12/40. C","","Surface beds","m3",3,"","","","","12/11/2021 11:04:46",""]
[2537,12162,12,9,"12/40","","12/40","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:34:33",""]
[2538,12163,12,9,"12/40","","12/40","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:34:33",""]
[2539,12169,12,9,"12/40"," D","12/40. D","","Edges, risers, ends and reveals not exceeding 300mm high or wide, circular to exceeding 1m radius","m",41,"","","","","12/11/2021 11:05:15",""]
[2540,12182,12,9,"12/40","","12/40","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:34:41",""]
[2541,12183,12,9,"12/40","","12/40","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:34:41",""]
[2542,12184,12,9,"12/40"," E","12/40. E","","Type S500 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",47,"","","","","10/12/2021 03:31:38",""]
[2543,12186,12,9,"12/40","","12/40","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","08/12/2021 04:55:33",""]
[2544,12190,12,9,"12/40","","12/40","","Finishing top surfaces of concrete smooth with a steel trowel","H4",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:34:53",""]
[2545,12191,12,9,"12/40"," F","12/40. F","","Surface beds, slabs, etc.","m2",2,"","","","","06/12/2021 03:08:59",""]
[2546,12195,12,9,"12/40","","12/40","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:35:32",""]
[2547,12196,12,9,"12/41","","12/41","","Flexible waterproofing slurry compound of a two component polymer modified cementitious coating applied in accordance with the manufacturers recommendations. The coating shall conform to the requirements of EMPA test 235.528, EMPA test 162.475/2. The compound shall have a resistance to positive pressure of 20 bars and negative pressure of 4 bars. Waterproofing to be reinforced at all corners/direction change with membrane felt as per waterproofing specialist","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 03:04:23",""]
[2548,12197,12,9,"12/41"," A","12/41. A","","To bottoms and sides of ponds, pump rooms, etc.","m2",2,"","","","","10/12/2021 03:31:45",""]
[2549,12200,12,9,"12/41","","12/41","","PLASTERING","H2",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:35:45",""]
[2550,12204,12,9,"12/41","","12/41","","One coat 1:5 cement plaster, on concrete","H4",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:35:45",""]
[2551,12205,12,9,"12/41"," B","12/41. B","","On narrow widths circular on plan","m2",2,"","","","","06/12/2021 03:10:13",""]
[2552,12238,12,9,"12/41","","12/41","","PLUMBING AND DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","28/06/2023 11:22:01",""]
[2553,12212,12,9,"12/41","","12/41","","Pond installation","H3",{"v":0,"d":"0.0"},"","","","","04/11/2021 01:43:46",""]
[2554,12225,12,9,"12/41"," C","12/41. C","","50mm Class 12 uPVC pipe cast in concrete (concrete elsewhere measured)","m",6,"","","","","28/06/2023 11:46:20",""]
[2555,12229,12,9,"12/41"," D","12/41. D","","90mm Class 12 uPVC pipes cast in concrete (concrete elsewhere measured)","m",17,"","","","","28/06/2023 11:46:26",""]
[2556,12230,12,9,"12/41"," E","12/41. E","","Extra over 90mm piping for bend","No",3,"","","","","15/11/2021 01:15:40",""]
[2557,12231,12,9,"12/41"," F","12/41. F","","Extra over 90mm piping for reducing tee","No",12,"","","","","15/11/2021 01:15:44",""]
[2558,12232,12,9,"12/41"," G","12/41. G","","90mm Class 12 uPVC pipes laid in and including trenches not exceeding 1m deep","m",8,"","","","","28/06/2023 11:47:12",""]
[2559,12233,12,9,"12/41"," H","12/41. H","","110mm Class 12 uPVC pipe laid in and including trenches not exceeding 1m deep","m",7,"","","","","28/06/2023 11:47:18",""]
[2560,12234,12,9,"12/41"," I","12/41. I","","Extra over 110mm piping for bend","No",2,"","","","","27/06/2023 10:08:06",""]
[2562,10341,12,10,"12/43","","12/43","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:00",""]
[2563,10342,12,10,"12/43","","12/43","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:30",""]
[2564,10343,12,10,"12/43","","12/43","","BILL NO. 10","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:35",""]
[2565,10367,12,10,"12/43","","12/43","","SYMBOLIC AND PRODUCTIVE GARDEN","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:15",""]
[2566,10368,12,10,"12/43","","12/43","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:36",""]
[2567,10369,12,10,"12/43","","12/43","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:37",""]
[2568,10370,12,10,"12/43","","12/43","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:37",""]
[2569,13349,12,10,"12/43","","12/43","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:27",""]
[2570,13350,12,10,"12/43","","12/43","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:27",""]
[2571,10373,12,10,"12/43","","12/43","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:37",""]
[2572,10374,12,10,"12/43","","12/43","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:37",""]
[2573,13092,12,10,"12/43","","12/43","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:09:14",""]
[2574,13093,12,10,"12/43","","12/43","","Breaking up and removing reinforced concrete","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 08:05:53",""]
[2575,13094,12,10,"12/43"," A","12/43. A","","210 x 100mm In-situ copings","m",47,"","","","","08/12/2021 05:01:37",""]
[2576,13267,12,10,"12/43"," B","12/43. B","","350 x 65mm In-situ copings","m",57,"","","","","08/12/2021 05:01:42",""]
[2577,13287,12,10,"12/44"," A","12/44. A","","500 x 100mm In-situ copings","m",39,"","","","","08/12/2021 05:01:47",""]
[2578,13284,12,10,"12/44","","12/44","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:27:36",""]
[2579,13286,12,10,"12/44","","12/44","","Taking out pebble covering and setting aside for re-use and later placing in similar new position","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:30:54",""]
[2580,13285,12,10,"12/44"," B","12/44. B","","Covering stones varying in size from 20mm to 40mm diameter in windpipe boxes","m3",5,"","","","","08/12/2021 05:02:33",""]
[2581,13276,12,10,"12/44","","12/44","","MOVEMENT JOINTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:09:20",""]
[2582,13277,12,10,"12/44","","12/44","","Two layers of 250 micron dampproof course in slip joints between horizontal concrete surfaces including thin cement mortar levelling bed under","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 05:10:10",""]
[2583,13278,12,10,"12/44"," C","12/44. C","","Not exceeding 300mm wide","m",286,"","","","","07/12/2021 05:10:25",""]
[2584,13095,12,10,"12/44","","12/44","","CONCRETE COPINGS, ETC","H2",{"v":0,"d":"0.0"},"","","","","03/12/2021 01:54:35",""]
[2585,13096,12,10,"12/44","","12/44","","In-situ concrete copings finished smooth on exposed surfaces to be cast on retaining walls, with expansion joints at maximum 1,5m centres, including all concrete, formwork, and finishes","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 02:52:14",""]
[2586,13097,12,10,"12/44"," D","12/44. D","","210 x 100mm Thick overall copings","m",47,"","","","","07/12/2021 05:10:36",""]
[2587,13283,12,10,"12/44"," E","12/44. E","","350 x 100mm Thick overall copings","m",57,"","","","","02/08/2022 08:22:08",""]
[2588,13288,12,10,"12/44"," F","12/44. F","","500 x 100mm Thick overall copings","m",39,"","","","","07/12/2021 05:10:47",""]
[2589,13103,12,10,"12/44","","12/44","","SEALING STRIPS, JOINT SEALANTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","03/12/2021 01:54:50",""]
[2590,13104,12,10,"12/44","","12/44","","Sikaflex 11FC polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 01:54:50",""]
[2591,13105,12,10,"12/44"," G","12/44. G","","5 x 5mm Pointing to expansion joints between precast concrete coping units","m",53,"","","","","08/12/2021 05:03:00",""]
[2593,10344,12,11,"12/46","","12/46","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:06",""]
[2594,10345,12,11,"12/46","","12/46","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:34",""]
[2595,10346,12,11,"12/46","","12/46","","BILL NO. 11","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:42",""]
[2596,10359,12,11,"12/46","","12/46","","STORY TELLING PIT","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:21",""]
[2597,10360,12,11,"12/46","","12/46","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:18",""]
[2598,10361,12,11,"12/46","","12/46","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:42",""]
[2599,10362,12,11,"12/46","","12/46","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:18",""]
[2600,13351,12,11,"12/46","","12/46","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:38",""]
[2601,13352,12,11,"12/46","","12/46","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:38",""]
[2602,10365,12,11,"12/46","","12/46","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:18",""]
[2603,10366,12,11,"12/46","","12/46","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:25:18",""]
[2604,12241,12,11,"12/46","","12/46","","DEMOLITIONS","H2",{"v":0,"d":"0.0"},"","","","","04/11/2021 03:40:21",""]
[2605,12240,12,11,"12/46"," A","12/46. A","","Take out and remove metal railings approximately 700mm high","m",6,"","","","","08/12/2021 03:43:38",""]
[2607,10347,12,12,"12/47","","12/47","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:17",""]
[2608,10348,12,12,"12/47","","12/47","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:38",""]
[2609,10349,12,12,"12/47","","12/47","","BILL NO. 12","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:46",""]
[2610,10350,12,12,"12/47","","12/47","","WALKWAYS, RAMPS & STEPS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:28",""]
[2611,10351,12,12,"12/47","","12/47","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:57",""]
[2612,10352,12,12,"12/47","","12/47","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:46",""]
[2613,10353,12,12,"12/47","","12/47","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:57",""]
[2614,13353,12,12,"12/47","","12/47","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:48",""]
[2615,13354,12,12,"12/47","","12/47","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:30:48",""]
[2616,10357,12,12,"12/47","","12/47","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:57",""]
[2617,10358,12,12,"12/47","","12/47","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:24:57",""]
[2618,10309,12,12,"12/47","","12/47","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:09:31",""]
[2619,9538,12,12,"12/47","","12/47","","Breaking up and removing concrete","H4",{"v":0,"d":"0.0"},"","","","","10/09/2021 03:58:28",""]
[2620,10115,12,12,"12/47"," A","12/47. A","","Average 100mm thick reinforced concrete surface beds, paving, etc.","m2",574,"","","","","07/12/2021 04:49:00",""]
[2621,10310,12,12,"12/47"," B","12/47. B","","Precast concrete kerb","m",112,"","","","","30/10/2021 08:42:53",""]
[2622,13311,12,12,"12/48","","12/48","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:58:25",""]
[2623,13290,12,12,"12/48","","12/48","","Taking up precast concrete pavers and setting aside for re-use and later relaying in similar position","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 04:00:27",""]
[2624,13291,12,12,"12/48"," A","12/48. A","","9mm Exposed aggregate C.E.L pavers","m2",5,"","","","","06/12/2021 06:51:16",""]
[2625,10466,12,12,"12/48","","12/48","","SITE CLEARANCE, ETC","H2",{"v":0,"d":"0.0"},"","","","","17/10/2021 06:14:41",""]
[2626,10467,12,12,"12/48","","12/48","","Site clearance","H4",{"v":0,"d":"0.0"},"","","","","17/10/2021 06:14:41",""]
[2627,10469,12,12,"12/48"," B","12/48. B","","Clean surface of in-situ exposed aggregate concrete paving by removing and disposing of weeds, silt, rubble, rubbish, etc.","m2",493,"","","","","06/12/2021 06:50:36",""]
[2628,12098,12,12,"12/48"," C","12/48. C","","Clean precast concrete paving and channels by removing and disposing of weeds, silt, rubble, rubbish, etc.","m2",6184,"","","","","06/12/2021 06:50:58",""]
[2629,10463,12,12,"12/48","","12/48","","EARTHWORKS","H2",{"v":0,"d":"0.0"},"","","","","17/10/2021 05:23:32",""]
[2630,10117,12,12,"12/48","","12/48","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 08:01:25",""]
[2631,10118,12,12,"12/48"," D","12/48. D","","Reduced levels under floors (Labour Intensive)","m3",15,"","","","","26/06/2023 11:12:48",""]
[2632,10120,12,12,"12/48","","12/48","","Earth filling supplied by the contractor","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 08:01:25",""]
[2633,10121,12,12,"12/48"," E","12/48. E","","Imported G7 selected material under walkways compacted to 93% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 11:12:52",""]
[2634,10122,12,12,"12/48"," F","12/48. F","","Imported G5 subbase selected material under walkways compacted to 95% Mod AASHTO density (Labour Intensive)","m3",5,"","","","","26/06/2023 11:12:56",""]
[2635,10451,12,12,"12/48"," G","12/48. G","","Imported G1 base course selected material under walkways compacted to 98% Mod AASHTO density (Labour Intensive)","m3",4,"","","","","26/06/2023 11:13:00",""]
[2636,10124,12,12,"12/48","","12/48","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 08:01:25",""]
[2637,10125,12,12,"12/48"," H","12/48. H","","Compaction of ground surface under pavings, etc. including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",558,"","","","","17/10/2021 06:26:42",""]
[2638,12397,12,12,"12/48","","12/48","","SPECIAL CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:49:32",""]
[2639,12398,12,12,"12/49","","12/49","","In-situ decorative exposed aggregate 30MPa concrete (19mm screened locally sourced aggregate - colour to match existing walkways), mixed and applied in accordance with the manufacturers specifications (Refer to B10 : Landscape specification)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 10:46:19",""]
[2640,12399,12,12,"12/49"," A","12/49. A","","Paving to walkways, cast against excavated surfaces","m3",58,"","","","","08/12/2021 03:44:11",""]
[2641,12400,12,12,"12/49","","12/49","","Test cubes","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:49:32",""]
[2642,12401,12,12,"12/49"," B","12/49. B","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",29,"","","","","06/11/2021 02:49:40",""]
[2643,12402,12,12,"12/49","","12/49","","Wire brushing of concrete surfaces to expose aggregate (1-2mm), including surface application of retarding agent","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:49:32",""]
[2644,12403,12,12,"12/49"," C","12/49. C","","Top surfaces of paving","m2",580,"","","","","06/11/2021 02:49:42",""]
[2645,12064,12,12,"12/49","","12/49","","Saw-cut joints","H4",{"v":0,"d":"0.0"},"","","","","03/11/2021 06:22:34",""]
[2646,12065,12,12,"12/49"," D","12/49. D","","3 x 50mm Saw-cut joints in top of concrete","m",273,"","","","","03/11/2021 06:22:48",""]
[2647,12066,12,12,"12/49"," E","12/49. E","","Ream previously cut/formed expansion joint by increasing the top 25mm to 6mm wide","m",273,"","","","","03/11/2021 06:22:59",""]
[2648,10303,12,12,"12/49","","12/49","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","15/10/2021 02:15:22",""]
[2649,10304,12,12,"12/49","","12/49","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 02:15:22",""]
[2650,10462,12,12,"12/49"," F","12/49. F","","Type 395 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",581,"","","","","07/12/2021 04:18:17",""]
[2651,10321,12,12,"12/49","","12/49","","CHANNELING, KERBING, EDGING, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:09:41",""]
[2652,10322,12,12,"12/49","","12/49","","Grouting of joints","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:20:45",""]
[2653,10323,12,12,"12/49"," G","12/49. G","","Rake out mortar in precast concrete kerb butt joints and re-grout with cement mortar","No",170,"","","","","03/11/2021 06:29:28",""]
[2654,10413,12,12,"12/49","","12/49","","Cleaning of kerbs","H4",{"v":0,"d":"0.0"},"","","","","16/10/2021 03:55:00",""]
[2655,10414,12,12,"12/49"," H","12/49. H","","Remove paint spills from kerbs","m",125,"","","","","31/10/2021 06:33:40",""]
[2656,10417,12,12,"12/49"," I","12/49. I","","Remove mortar splashes from kerbs","m",70,"","","","","31/10/2021 06:33:44",""]
[2657,10415,12,12,"12/50","","12/50","","Sikaflex 11 FC, or similar approved, single component sealant with backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","03/11/2021 06:23:38",""]
[2658,10416,12,12,"12/50"," A","12/50. A","","6 x 10mm In joints in exposed aggregate panels","m",6,"","","","","27/06/2023 10:08:28",""]
[2660,10131,12,13,"12/52","","12/52","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","14/10/2021 10:31:28",""]
[2661,10132,12,13,"12/52","","12/52","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:43",""]
[2662,10133,12,13,"12/52","","12/52","","BILL NO. 13","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:55",""]
[2663,10134,12,13,"12/52","","12/52","","PARKING, PAVING & ROADS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:33",""]
[2664,13355,12,13,"12/52","","12/52","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:15",""]
[2665,13356,12,13,"12/52","","12/52","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:52",""]
[2666,13357,12,13,"12/52","","12/52","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:15",""]
[2667,13365,12,13,"12/52","","12/52","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:31",""]
[2668,13366,12,13,"12/52","","12/52","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:32",""]
[2669,13361,12,13,"12/52","","12/52","","Testing of material and filling","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:15",""]
[2670,13362,12,13,"12/52","","12/52","","Descriptions of earth filling, compaction, etc shall be deemed to include for all necessary testing required in accordance with the SANS 1200 series","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:15",""]
[2671,13363,12,13,"12/52","","12/52","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:15",""]
[2672,13364,12,13,"12/52","","12/52","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:31:15",""]
[2673,10135,12,13,"12/52","","12/52","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","15/10/2021 05:34:09",""]
[2674,9541,12,13,"12/53","","12/53","","Breaking up and removing concrete","H4",{"v":0,"d":"0.0"},"","","","","10/09/2021 03:58:40",""]
[2675,9542,12,13,"12/53"," A","12/53. A","","Average 100mm thick concrete surface beds, paving, etc.","m2",110,"","","","","08/12/2021 04:59:40",""]
[2676,10136,12,13,"12/53"," B","12/53. B","","Precast concrete kerb","m",36,"","","","","30/10/2021 08:43:41",""]
[2677,9540,12,13,"12/53","","12/53","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","10/09/2021 03:58:40",""]
[2678,10137,12,13,"12/53","","12/53","","Taking out and set aside for re-use, or handing to the client (Re-use measured elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 05:03:34",""]
[2679,10138,12,13,"12/53"," C","12/53. C","","Bevel-edged full inter-locking precast concrete pavers","m2",282,"","","","","26/06/2023 11:13:41",""]
[2680,10139,12,13,"12/53","","12/53","","SITE CLEARANCE, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:09:49",""]
[2681,10143,12,13,"12/53"," D","12/53. D","","Clean precast concrete paving and channels by removing and disposing of weeds, silt, rubble, rubbish, etc.","m2",5052,"","","","","03/11/2021 02:48:11",""]
[2682,10144,12,13,"12/53","","12/53","","EARTHWORKS","H2",{"v":0,"d":"0.0"},"","","","","15/10/2021 05:35:20",""]
[2683,11746,12,13,"12/53","","12/53","","Earth filling supplied by the contractor under parking areas, roadways, etc.","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:16:55",""]
[2684,10147,12,13,"12/53"," E","12/53. E","","Imported filling under pavers to make up levels in sagged areas","m3",2,"","","","","31/10/2021 06:34:15",""]
[2685,11745,12,13,"12/53"," F","12/53. F","","Base course of G5 material in accordance with SABS 1200 ME, stabilised to attain UCS>1,0 MPa after seven days and compacted to 95% Mod AASHTO density","m3",101,"","","","","13/03/2023 03:33:41",""]
[2686,11747,12,13,"12/53","","12/53","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","29/10/2021 02:23:25",""]
[2687,11748,12,13,"12/53"," G","12/53. G","","Compaction of ground surfaces under pavings etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m2",1124,"","","","","30/10/2021 08:43:37",""]
[2688,10148,12,13,"12/53","","12/53","","PAVING","H2",{"v":0,"d":"0.0"},"","","","","15/10/2021 04:56:33",""]
[2689,10149,12,13,"12/53","","12/53","","Note : Paving is to be laid in accordance with SANS 1200 MJ, SANS 1058 and the Concrete Masonry Association's specifications","",{"v":0,"d":"0.0"},"","","","","15/10/2021 04:56:33",""]
[2690,10150,12,13,"12/53","","12/53","","Paving is to be laid on 20mm (thickness after final compaction) clean river sand (preparation of ground or filling elsewhere)","",{"v":0,"d":"0.0"},"","","","","15/10/2021 04:56:34",""]
[2691,10151,12,13,"12/53","","12/53","","Clean sand is to be swept into joints between roadstones","",{"v":0,"d":"0.0"},"","","","","15/10/2021 04:56:34",""]
[2692,10152,12,13,"12/54","","12/54","","The contractor will be required to provide a certificate from a registered pest control company certifying that a weed killer has been applied in accordance with the manufacturer's instructions. (PW371 clause 19.6)","",{"v":0,"d":"0.0"},"","","","","15/10/2021 04:56:53",""]
[2693,10154,12,13,"12/54","","12/54","","Bosun 105 x 210 x 70mm 35Mpa bevel-edged full inter-locking precast concrete pavers with 9mm exposed granite aggregate finish, suitable for foot traffic, cars, vans and small pick-up trucks, including bedding, jointing and pointing (colour : Kalahari)","H4",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:14:10",""]
[2694,10155,12,13,"12/54"," A","12/54. A","","On roadway and parking area ","m2",17,"","","","","06/12/2021 03:11:37",""]
[2695,10157,12,13,"12/54"," B","12/54. B","","200mm Wide full-paver border to paving","m",40,"","","","","08/12/2021 05:00:41",""]
[2696,10158,12,13,"12/54","","12/54","","Take from store previously set aside for re-use and re-instate","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 05:02:59",""]
[2697,10159,12,13,"12/54"," C","12/54. C","","105 x 210 x 70mm 35Mpa Bevel-edged full inter-locking precast concrete pavers laid to falls on and including sand bed","m2",263,"","","","","30/10/2021 08:44:21",""]
[2698,10160,12,13,"12/54"," D","12/54. D","","Fair circular cutting","m",40,"","","","","30/10/2021 08:44:25",""]
[2699,10161,12,13,"12/54"," E","12/54. E","","200mm Wide full-paver border to paving","m",16,"","","","","08/12/2021 05:00:58",""]
[2700,10162,12,13,"12/54","","12/54","","Grouting","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 07:30:32",""]
[2701,10163,12,13,"12/54"," F","12/54. F","","Rake out mortar, debris, etc. and re-sand pavers","m2",50,"","","","","30/10/2021 08:44:37",""]
[2702,10164,12,13,"12/54"," G","12/54. G","","Rake out mortar, debris, etc. and re-sand (stabilised) joint between edge pavers and adjacent concrete ","m",100,"","","","","30/10/2021 08:44:42",""]
[2703,10165,12,13,"12/54","","12/54","","CHANNELING, KERBING, EDGING, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:09:57",""]
[2704,10166,12,13,"12/54","","12/54","","KERBING","H3",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:14:28",""]
[2705,10167,12,13,"12/54","","12/54","","Precast concrete finished smooth on exposed surfaces, including bedding, jointing and pointing","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 05:47:44",""]
[2706,10168,12,13,"12/54"," H","12/54. H","","150 x 250mm High kerbs (SANS 927 fig 3) with 20MPa/19mm concrete continuous haunching, including excavation, backfilling, etc","m",18,"","","","","30/10/2021 08:44:48",""]
[2707,10169,12,13,"12/54"," I","12/54. I","","Ditto, but to radius not exceeding 4m","m",2,"","","","","30/10/2021 08:44:52",""]
[2708,10170,12,13,"12/54"," J","12/54. J","","Ditto, but to radius exceeding 4m","m",16,"","","","","30/10/2021 08:44:56",""]
[2709,10171,12,13,"12/55","","12/55","","Grouting of joints","H4",{"v":0,"d":"0.0"},"","","","","15/10/2021 05:48:04",""]
[2710,10172,12,13,"12/55"," A","12/55. A","","Rake out loose mortar in precast concrete kerb butt joints and re-grout with cement mortar","No",126,"","","","","09/11/2021 11:57:44",""]
[2711,10173,12,13,"12/55"," B","12/55. B","","Cut and rake out mortar joint between kerbs and fit sealant with backing cord, primer, bond breaker, etc. as per SANS 1200 MK","No",8,"","","","","12/11/2021 08:41:03",""]
[2712,10440,12,13,"12/55"," C","12/55. C","","Remove mortar splashes from kerbs","m",85,"","","","","03/11/2021 06:32:53",""]
[2713,13420,12,13,"12/55","","12/55","","REINFORCED CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","07/12/2021 10:59:02",""]
[2714,13421,12,13,"12/55","","12/55","","30MPa/19mm concrete","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 10:59:43",""]
[2715,13422,12,13,"12/55"," D","12/55. D","","Paving to walkways, cast against excavated surfaces","m3",2,"","","","","08/12/2021 04:59:48",""]
[2716,13424,12,13,"12/55","","12/55","","Pebble covering set in top of concrete","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 09:21:03",""]
[2717,13423,12,13,"12/55"," E","12/55. E","","Covering of river stone pebbles varying in size from 20mm to 40mm diameter in paving","m3",1,"","","","","08/12/2021 04:59:54",""]
[2718,12404,12,13,"12/55","","12/55","","SPECIAL CONCRETE","H3",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:50:01",""]
[2719,12405,12,13,"12/55","","12/55","","In-situ decorative exposed aggregate 30MPa concrete (19mm screened locally sourced aggregate - colour to match existing walkways), mixed and applied in accordance with the manufacturers specifications (Refer to B10 : Landscape specification)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 10:46:02",""]
[2720,12406,12,13,"12/55"," F","12/55. F","","Paving to walkways, cast against excavated surfaces","m3",9,"","","","","08/12/2021 03:45:23",""]
[2721,12407,12,13,"12/55","","12/55","","Test cubes","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:50:01",""]
[2722,12408,12,13,"12/55"," G","12/55. G","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",1,"","","","","06/11/2021 02:50:36",""]
[2723,12409,12,13,"12/55","","12/55","","Wire brushing of concrete surfaces to expose aggregate (1-2mm), including surface application of retarding agent","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:50:01",""]
[2724,12410,12,13,"12/55"," H","12/55. H","","Top surfaces of paving","m2",92,"","","","","06/11/2021 02:50:38",""]
[2725,13313,12,13,"12/55","","12/55","","Saw-cut joints","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 04:53:26",""]
[2726,13314,12,13,"12/55"," I","12/55. I","","3 x 50mm Saw-cut joints in top of concrete","m",250,"","","","","06/12/2021 04:53:26",""]
[2727,12411,12,13,"12/55","","12/55","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:50:23",""]
[2728,12412,12,13,"12/56","","12/56","","Mesh reinforcement","H4",{"v":0,"d":"0.0"},"","","","","06/11/2021 02:50:23",""]
[2729,12413,12,13,"12/56"," A","12/56. A","","Type 395 Mesh reinforcement with 300mm side and end laps in surface beds, ramps, etc.","m2",110,"","","","","26/06/2023 04:53:19",""]
[2731,10175,12,14,"12/58","","12/58","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:37:02",""]
[2732,10176,12,14,"12/58","","12/58","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:47",""]
[2733,10177,12,14,"12/58","","12/58","","BILL NO. 14","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:57:58",""]
[2734,10178,12,14,"12/58","","12/58","","RETAINING WALLS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:39",""]
[2735,13367,12,14,"12/58","","12/58","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:32:44",""]
[2736,13368,12,14,"12/58","","12/58","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:40:57",""]
[2737,13369,12,14,"12/58","","12/58","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:32:44",""]
[2738,13374,12,14,"12/58","","12/58","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:33:05",""]
[2739,13375,12,14,"12/58","","12/58","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:33:05",""]
[2740,13372,12,14,"12/58","","12/58","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:32:44",""]
[2741,13373,12,14,"12/58","","12/58","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:32:44",""]
[2742,12813,12,14,"12/59","","12/59","","REMEDIAL WORK TO CONCRETE SURFACES","H2",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:57:40",""]
[2743,13155,12,14,"12/59","","12/59","","OPTION 1 : ABRASIVE (SAND) BLAST CLEANING OF EXISTING CONCRETE SURFACES","H3",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:22:34",""]
[2744,13156,12,14,"12/59","","12/59","","Preparation - removal of previously applied skimming product Contractor to prepare concrete surface by removing all skimming compound varying in depth between 0,5 and 5mm on currently constructed concrete surfaces. To be done using various procedures including but not limited to grinding, grit blasting or manual means. Mechanical breakers will not be permitted in the removal of currently applied skimming product. Contractor to ensure that no damage occurs to the existing concrete substrate located beneath the existing skim product. It is to be assumed that prior to blasting all walls will be repaired as elsewhere specified.","",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:36:58",""]
[2745,13157,12,14,"12/59","","12/59","","Equipment Equipment shall be adequate to be able to provide the blast profile specified.","",{"v":0,"d":"0.0"},"","","","","06/12/2021 09:57:50",""]
[2746,13158,12,14,"12/59","","12/59","","Required finish to the concrete surface The required finish to the concrete surface will have a profile from the current raw concrete surface (NOT CURRENT SKIMMED SURFACE) as outlined below: Percentage of concrete surface\tMaximum profile depth excluding 19mm stone aggregate\tMinimum profile depth excluding 19mm stone aggregate 95% of all concrete surfaces\t5mm\t3mm Remaining 5% of surfaces\t8mm\t3mm ","",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:39:17",""]
[2747,13159,12,14,"12/59","","12/59","","Workmanship & OHS requirements The method of abrasive blasting finishes to be carried out by generally accepted methods of the trade and by qualified tradesman and equipment. The abrasive blast cleaner is to ensure that they are suitably protected as required by current health and safety regulations. All areas adjacent to where blasting is to be carried out need to be suitably protected to ensure that no damage to adjacent surfaces occurs. Dust control to be implemented to reduce air pollution","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:11:09",""]
[2748,13160,12,14,"12/60","","12/60","","Cleaning of area on completion of Works Upon completion of works: All blasted surfaces to be washed down to remove residue material. All equipment protection, masking materials and residue to be removed. All blast material to be removed from site and disposed of as required by current legislation.","",{"v":0,"d":"0.0"},"","","","","06/12/2021 09:57:51",""]
[2749,13161,12,14,"12/60","","12/60","","OPTION 2 : BUSH HAMMER EXISTING CONCRETE SURFACES","H3",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:22:44",""]
[2750,13162,12,14,"12/60","","12/60","","Preparation - removal of previously applied skimming product Contractor to prepare concrete surface by removing all skimming compound varying in depth between 0,5mm and 5mm on currently constructed concrete surfaces. To be done using various procedures including but not limited to grinding, grit blasting or manual means. Mechanical breakers will not be permitted in the removal of currently applied skimming product. Contractor to ensure that no damage occurs to the existing concrete substrate located beneath the existing skim product. Alternative to the above, the existing skim coat may be removed in one action by means of a bush hammer tool, when bush hammer effect is applied, but care must be taken not to penetrate the wall deeper than described above. It is to be assumed that prior to bush hammering all walls will be repaired as elsewhere specified.","",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:38:20",""]
[2751,13163,12,14,"12/60","","12/60","","Equipment Equipment shall be adequate to be able to provide the bush hammer profile specified.Breakers should not exceed 7kg in size","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:12:29",""]
[2752,13164,12,14,"12/61","","12/61","","Required finish to the concrete surface Remove the minimum matrix, including all laitance, using bush hammering to expose the coarse aggregate without recessing the matrix deeper than the aggregate, to give a uniform texture with insignificant random tool marks.  The required finish to the concrete surface will have a profile from the current raw concrete surface (NOT CURRENT SKIMMED SURFACE) as outlined below: Percentage of concrete surface\tMaximum profile depth excluding 19mm stone aggregate\tMinimum profile depth excluding 19mm stone aggregate 95% of all concrete surfaces\t5mm\t3mm Remaining 5% of surfaces\t8mm\t3mm ","",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:39:29",""]
[2753,13165,12,14,"12/61","","12/61","","Workmanship The method of bush hammering finishes to be carried out by generally accepted methods of the trade and by qualified tradesmen and equipment.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 12:21:25",""]
[2754,13169,12,14,"12/61","","12/61","","OPTION 3 : GRINDING OF EXISTING CONCRETE SURFACES","H3",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:22:51",""]
[2755,13170,12,14,"12/61","","12/61","","Grind concrete, providing a smooth finish through a seven stage grind of surface Concrete surface to be ground smooth providing an exposed slight exposed aggregate finish. Concrete to receive 7 stages of grinding ie. to be ground 7 times with a combination of the following profiles : #100 #200 #800 #1 500","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:14:54",""]
[2756,13439,12,14,"12/61","","12/61","","Thereafter to receive a further three stages of grinding to provide a smooth profile. Tops of walls to be grinded to have a slight fall (1 degree) towards roof or always away from public face of respective wall to divert water away from public face. Concrete to be sealed with appropriate sealant consisting of 2 x coats abe.SEAL Finisol penetrating sealer, or equal approved, to the ‘prepared surface’ working on 4hrs between each coat. During grinding process all corners to receive a 3mm diameter pencil round edge","",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:13:31",""]
[2757,13166,12,14,"12/62","","12/62","","OPTION 4 : SKIMMING OF EXISTING CONCRETE SURFACES WITH DURA.REP FC AND SEALING OF SURFACES","H3",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:22:57",""]
[2758,13167,12,14,"12/62","","12/62","","Preparation - removal of previously applied skimming product Contractor to prepare concrete surface by removing all skimming compound varying in depth between 0,5 and 5mm on currently constructed concrete surfaces. To be done using various procedures including but not limited to grinding, grit blasting or manual means. Mechanical breakers will not be permitted in the removal of currently applied skimming product. Contractor to ensure that no damage occurs to the existing concrete substrate located beneath the existing skim product. It is to be assumed that prior to skimming all walls will be repaired as elsewhere specified.","",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:39:42",""]
[2759,13168,12,14,"12/62","","12/62","","Application of dura.rep FC and sealing of surfacesdura.rep FC to be applied to walls strictly in accordance with manufactures instructions.Pre-saturate the ‘prepared substrate’ with water (SSD)Prime the ‘prepared substrate’ with dura.bond GP and while tacky;Apply the dura.rep FC skimming compound between 1-3mm thick with a (1:1) mix ratio, dura.latex to water (see TDS for mixing instructions) For Terracotta pigmented concrete walls add between 2-5% of Chryso Terracotta Oxide by volume of dura.rep FC. In order to determine the correct percentage mix of oxide to be added, it is critical that dried out samples be prepared to match the existing colour of adjacent walls exactly.When the dura.rep FC can no longer be marred, apply dura.bond GP as a curing compound.Apply 2 x coats abe.seal Finisol  penetrating sealer to the ‘prepared surface’ working on 4hrs between each coat.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:09:36",""]
[2760,13433,12,14,"12/62","","12/62","","OPTION 5 : CLEAN & GRIND SURFACES","H3",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:23:02",""]
[2761,13434,12,14,"12/62","","12/62","","Concrete surfaces to be ground smooth to get rid of ridges formed by concrete leaks through shuttering and other concrete droppings. Concrete to receive 1 stage of grinding, profile #100. Clean surface thoroughly after grinding.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 12:43:26",""]
[2762,12831,12,14,"12/62","","12/62","",".....................................................................","",{"v":0,"d":"0.0"},"","","","","15/11/2021 03:56:06",""]
[2763,12832,12,14,"12/63","","12/63","","AESTHETIC REMEDIAL WORK TO GENERAL SURFACE FINISHES OF EXTERNAL CONCRETE RETAINING WALLS","H2",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:57:46",""]
[2764,12833,12,14,"12/63"," A","12/63. A","","Abrasive blasting finish complete (Option 1), as described above (penetrating sealer measured elsewhere)","m2",2651,"","","","","10/12/2021 02:18:17",""]
[2765,12834,12,14,"12/63"," B","12/63. B","","Bush hammer finish complete (Option 2), as described above (penetrating sealer measured elsewhere)","m2",1,"","","","Rate only","14/06/2023 11:44:07",""]
[2766,13435,12,14,"12/63"," C","12/63. C","","Grinding finish complete (Option 3), as described above (penetrating sealer measured elsewhere)","m2",1,"","","","Rate only","14/06/2023 11:47:49",""]
[2767,13448,12,14,"12/63"," D","12/63. D","","Extra over grinding finish (Option 3) for 3mm rounded edges","m",1,"","","","Rate only","14/06/2023 11:48:06",""]
[2768,12835,12,14,"12/63"," E","12/63. E","","Skimming finish to vertical surfaces complete (Option 4), as described above (penetrating sealer measured elsewhere)","m2",1,"","","","Rate only","14/06/2023 11:47:04",""]
[2769,12837,12,14,"12/63"," F","12/63. F","","Skimming finish to horizontal surfaces complete (Option 4), as described above (penetrating sealer measured elsewhere)","m2",1,"","","","Rate only","14/06/2023 11:47:25",""]
[2770,13442,12,14,"12/63"," G","12/63. G","","Grinding finish to vertical surfaces complete (Option 5), as described above","m2",1,"","","","Rate only","14/06/2023 11:50:58",""]
[2771,12838,12,14,"12/63"," H","12/63. H","","Grinding finish to horizontal surfaces complete (Option 5), as described above","m2",250,"","","","","19/06/2023 08:42:32",""]
[2772,13427,12,14,"12/63","","12/63","","Prepare and apply two coats abe.seal Finisol penetrating sealer on","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:17:46",""]
[2773,13428,12,14,"12/63"," I","12/63. I","","Abrasive blasted concrete surfaces (Option 1)","m2",1181,"","","","","10/12/2021 02:09:45",""]
[2774,13429,12,14,"12/63"," J","12/63. J","","Bush hammered concrete surfaces (Option 2)","m2",1,"","","","Rate only","14/06/2023 11:52:36",""]
[2775,13436,12,14,"12/63"," K","12/63. K","","Grinded concrete surfaces (Option 3)","m2",250,"","","","","19/06/2023 08:56:40",""]
[2776,13430,12,14,"12/63"," L","12/63. L","","Skimmed concrete surfaces (Option 4)","m2",1,"","","","Rate only","14/06/2023 11:52:46",""]
[2777,13827,12,14,"12/63","","12/63","","SPECIALISED PLASTER TYPE WALL COATINGS","H2",{"v":0,"d":"0.0"},"","","","","21/06/2023 10:23:05",""]
[2778,13828,12,14,"12/63","","12/63","","All specialised plaster type wall coatings are to be executed in strict accordance with the manufacturer's instructions","",{"v":0,"d":"0.0"},"","","","","21/06/2023 10:23:05",""]
[2779,13756,12,14,"12/63","","12/63","","SURFACE PREPARATION","H3",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:57:52",""]
[2780,13757,12,14,"12/64","","12/64","","Prepare surface by applying a spray coat of Marmoran Marmocide antifungal disinfectan, pressure wash with high pressure washer using a combination of flat and rotating nozzles, and mechanically remove contaminants and loose materials","H4",{"v":0,"d":"0.0"},"","","","","22/06/2023 09:08:48",""]
[2781,13758,12,14,"12/64"," A","12/64. A","","On concrete walls","m2",1,"","","","Rate only","21/06/2023 10:16:44",""]
[2782,13759,12,14,"12/64","","12/64","","Prepare and apply Marmoran Easykey with cement and sand compound slurry mixture with a block brush to create a key","H4",{"v":0,"d":"0.0"},"","","","","22/06/2023 09:09:14",""]
[2783,13760,12,14,"12/64"," B","12/64. B","","On concrete walls","m2",1,"","","","Rate only","21/06/2023 10:19:31",""]
[2784,13793,12,14,"12/64","","12/64","","MARMORAN EASYPLAST","H3",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:57:56",""]
[2785,13814,12,14,"12/64","","12/64","","Prepare and apply Marmoran Easyplast trowel to surfaces in layers to achieve an even surface","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 10:27:20",""]
[2786,13815,12,14,"12/64"," C","12/64. C","","On off shutter concrete walls","m2",1,"","","","Rate only","21/06/2023 10:29:28",""]
[2787,13761,12,14,"12/64","","12/64","","Prepare and apply Marmoran Easyplast with sand and cement compound mixture trowelled on in layers to achieve an even surface","H4",{"v":0,"d":"0.0"},"","","","","22/06/2023 09:08:40",""]
[2788,13762,12,14,"12/64"," D","12/64. D","","On off-shutter concrete walls","m2",1,"","","","Rate only","21/06/2023 10:21:56",""]
[2789,13764,12,14,"12/64"," E","12/64. E","","On concrete benches","m2",1,"","","","Rate only","21/06/2023 10:22:09",""]
[2790,13829,12,14,"12/64"," F","12/64. F","","On tops of concrete walls n.e. 300mm wide","m2",1,"","","","Rate only","21/06/2023 10:23:40",""]
[2791,13767,12,14,"12/64","","12/64","","Prepare and apply three of coats Marmoran GP Waterproofing","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 10:27:03",""]
[2792,13830,12,14,"12/64"," G","12/64. G","","On tops of concrete walls n.e. 300mm wide","m2",1,"","","","Rate only","21/06/2023 10:28:23",""]
[2793,13769,12,14,"12/64","","12/64","","MARMORAN PERMAPLAST (10 YEAR GUARANTEE)","H3",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:58:02",""]
[2794,13770,12,14,"12/64","","12/64","","Prepare and apply Marmoran pigmented RBP masony textured solvent primer and trowel apply Marmoran Permacrete Warm Embrace resin bonded plaster to a minimum thickness of 1mm and roller apply two coats Marmoran universal glaze satin","H4",{"v":0,"d":"0.0"},"","","","","22/06/2023 09:10:02",""]
[2795,13771,12,14,"12/64"," H","12/64. H","","To wall areas","m2",1,"","","","Rate only","21/06/2023 10:32:45",""]
[2796,13772,12,14,"12/64","","12/64","","MARMORAN CONCRETEX (10 YEAR GUARANTEE)","H3",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:58:05",""]
[2797,13773,12,14,"12/65","","12/65","","Prepare and apply Marmoran pigmented RBP masony textured solvent primer and trowel apply Marmoran Concretex and two coats Marmoran universal glaze satin","H4",{"v":0,"d":"0.0"},"","","","","22/06/2023 09:10:21",""]
[2798,13774,12,14,"12/65"," A","12/65. A","","To wall areas","m2",1,"","","","Rate only","21/06/2023 10:32:52",""]
[2799,13831,12,14,"12/65","","12/65","","WATERPROOFING","H3",{"v":0,"d":"0.0"},"","","","","21/06/2023 10:26:00",""]
[2800,13765,12,14,"12/65","","12/65","","Polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","17/05/2023 09:31:04",""]
[2801,13766,12,14,"12/65"," B","12/65. B","","10 x 10mm In expansion joints in walls, etc. including raking out expansion joint filler as necessary","m",1,"","","","Rate only","19/06/2023 01:46:18",""]
[2802,13467,12,14,"12/66","","12/66","","STRUCTURAL REMEDIAL WORK TO GENERAL SURFACES OF EXTERNAL CONCRETE RETAINING WALLS","H2",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:58:14",""]
[2803,13468,12,14,"12/66","","12/66","","Shallow repairs to walls in patches (Maximum 70mm repair depth - see specification S9615/SPEC/002)","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:30:03",""]
[2804,13469,12,14,"12/66","","12/66","","a) Grind (square cut) minimum 10mm deep around area to be repaired - no feathering of repair product permitted.b) Remove rejected concrete/repair product as applicable.c) Ensure that entire repair area is chipped back minimum 10mm deep and that adhesion surface is free of laitance. Scabble the surface to remove laitance and loose concrete. d) Any exposed rebar to be grit blast or wire brushed to remove corrosion.e) Exposed rebar to be treated with ABE Dura.rep ZR Primer (brush application) and allowed to dry.f) Apply ABE Epidermix 344 Primer to the prepared concrete substrate (brush application).g) While the bonding primer is tacky, repair using ABE Durarep FR structural fibre-reinforced repair mortar (trowel application).h) Once the final finish has been achieved and the surface can no longer be stained, apply ABE Dura.bond GP curing compound.i) Ensure repair is applied to accuracy 1 tolerance.j) Final finish of pigmented concrete to Architect’s details.","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:54:57",""]
[2805,13474,12,14,"12/66"," A","12/66. A","","To grey concrete walls","m2",120,"","","","","21/06/2023 11:17:50",""]
[2806,13472,12,14,"12/66"," B","12/66. B","","To pigmented concrete walls, including pigment additive to match adjacent colour","m2",30,"","","","","21/06/2023 11:17:56",""]
[2807,13696,12,14,"12/66"," C","12/66. C","","Extra over for bulking Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume","m2",75,"","","","","10/12/2021 11:59:31",""]
[2808,13470,12,14,"12/67","","12/67","","Deep repairs to walls in patches (Minimum 50mm repair depth - see specification S9615/SPEC/002)","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:29:56",""]
[2809,13471,12,14,"12/67","","12/67","","a) Grind (square cut) minimum 10mm deep around area to be repaired - no feathering of repair product permitted. b) Demolish rejected concrete or repair product.c) Ensure that entire repair area is chipped back minimum 50mm deep and that adhesion surface is free of laitance. Scabble the surface to remove laitance if required. Where repaired area is less than 50mm deep, repair as per shallow repair methodology.d) Any exposed rebar to be grit blast or wire brushed to remove corrosion.e) Exposed rebar to be treated with ABE Dura rep ZR Primer (brush application) and allowed to dry.f) Apply ABE Epidermix 345 Primer to the prepared concrete substrate (brush application).g) Place shutters, sealed to prevent grout loss. Allow a letter-box opening as required ensuring the repair concrete will completely fill the repair void.h) Pour ABE Dura.rep FMC into shuttered repair area.i) Apply ABE Dura.bond GP curing compound.j) Grind surface down to accuracy 1 tolerance, final finish to Architect’s details.","",{"v":0,"d":"0.0"},"","","","","08/12/2021 08:22:48",""]
[2810,13475,12,14,"12/67"," A","12/67. A","","To grey concrete walls","m2",25,"","","","","21/06/2023 11:48:54",""]
[2811,13473,12,14,"12/67"," B","12/67. B","","To pigmented concrete walls, including pigment additive to match adjacent colour","m2",25,"","","","","21/06/2023 11:48:58",""]
[2812,13045,12,14,"12/68","","12/68","","Repairs to tops of pigmented walls (See specification S9615/SPEC/002)","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:18:28",""]
[2813,13046,12,14,"12/68","","12/68","","a) Remove existing repair product (where present) b) Grind 30 deep (square cut) on each side of the wall to form a straight level line along the entire wall length. Demolish the upper concrete portion. c) Grind top surface to remove laitance. d) Any exposed rebar to be grit blast or wire brushed to remove corrosion. e) Exposed rebar to be treated with ABE Dura.rep ZR Primer (brush application) and allowed to dry. f) Apply ABE Epidermix 344 Primer to the prepared concrete substrate (brush application). g) While the bonding primer is tacky, repair using ABE Durarep FR structural fibre-reinforced repair mortar (trowel application). h) Note: Top of walls to be level along length of the wall with a cross fall as indicated by the Architect. Top of walls to have 20mm chamfers as indicated by the Architect. i) Once the final finish has been achieved and the surface can no longer be blemished, apply  ABE Durabond GP curing compound. k) Ensure repair is applied to accuracy 1 tolerance. l) Final finish of pigmented concrete to Architect’s details.","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:56:13",""]
[2814,13047,12,14,"12/68"," A","12/68. A","","Tops of pigmented concrete retaining walls not exceeding 300mm wide including pigment additive to match adjacent colour","m",112,"","","","","21/06/2023 11:49:27",""]
[2815,13698,12,14,"12/68"," B","12/68. B","","Extra over for bulking Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume","m",17,"","","","","21/06/2023 10:42:06",""]
[2816,13042,12,14,"12/69","","12/69","","Repairs to tops of grey concrete walls (See specification S9615/SPEC/002)","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:19:13",""]
[2817,13041,12,14,"12/69","","12/69","","a) Remove existing repair product (where present) b) Grind 30 deep (square cut) on each side of the wall to form a straight level line along the  entire wall length. Demolish the upper concrete portion. c) Grind top surface to remove laitance. d) Any exposed rebar to be grit blast or wire brushed to remove corrosion. e) Exposed rebar to be treated with ABE Dura.rep ZR Primer (brush application) and allowed to  dry. f) Apply ABE Epidermix 344 Primer to the prepared concrete substrate (brush application). g) While the bonding primer is tacky, repair using ABE Durarep FR structural fibre-reinforced  repair mortar (trowel application). h) Note: Top of walls to be level along length of the wall with a cross fall as indicated by the Architect. Top of walls to have 20mm chamfers as indicated by the Architect. i) Once the final finish has been achieved and the surface can no longer be blemished, apply  ABE Durabond GP curing compound. i) Ensure repair is applied to accuracy 1 tolerance.","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:56:26",""]
[2818,13044,12,14,"12/69"," A","12/69. A","","Tops of grey concrete retaining walls not exceeding 300mm wide","m",254,"","","","","21/06/2023 11:50:37",""]
[2819,13136,12,14,"12/69"," B","12/69. B","","Tops of grey concrete box channels not exceeding 300mm wide","m",199,"","","","","23/06/2023 11:49:41",""]
[2820,13699,12,14,"12/69"," C","12/69. C","","Extra over for bulking Durarep FR structural fibre-reinforced repair mortar with 6mm stone 25% by volume","m",38,"","","","","21/06/2023 10:42:10",""]
[2821,13020,12,14,"12/69","","12/69","","REMEDIAL WORK TO EXPANSION JOINTS","H2",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:58:20",""]
[2822,13035,12,14,"12/70","","12/70","","Repairs to out of plumb wall expansion/construction joints (See specification S9615/SPEC/002)","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:29:45",""]
[2823,13486,12,14,"12/70","","12/70","","a) Grind reinforced concrete 30mm deep x 100mm offset on either side of the joint. b) Demolish 30mm deep x 200mm wide concrete strip across joint. c) Remove foreign matter, dust, loose aggregate by means of a high-pressure cleaning. d) Place a vertical shutter at the joint to form a new straight/plumb joint. e) Prime one side of the repair by applying ABE Epidermix 344 primer to the prepared concrete substrate (brush application). f) While the bonding primer is tacky, repair using ABE Durarep FR structural fibre-reinforced repair mortar (trowel application) applied to one side of the shutter. g) Remove the shutter and place joint former (jointex or similar approved) to the thickness of the existing joint (10mm, 12mm or 20mm thick as applicable). Jointex to be glued to the repaired concrete. h) Repeat the procedure above to repair the second portion on the other side of the joint. i) Rake out the joint former, place backing cord (10/12/20mm wide as per joint width) and seal the joint as per the joint sealant detailing using Sikaflex 11FC+.","",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:56:50",""]
[2824,13012,12,14,"12/70"," A","12/70. A","","12mm Wide joint","m",108,"","","","","08/12/2021 03:57:15",""]
[2825,13013,12,14,"12/70"," B","12/70. B","","20mm Wide joint","m",61,"","","","","08/12/2021 03:57:19",""]
[2826,13009,12,14,"12/70","","12/70","","Repairs to plumb wall expansion/construction joints (See specification S9615/SPEC/002)","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:29:36",""]
[2827,13481,12,14,"12/70","","12/70","","a) Rub down joint to produce neat straight smooth joint. b) For 20mm wide joint: Rake out 40mm joint former material. For 10mm/12mm wide joint: Rake out 20mm joint former material. c) Place 20mm/12mm/10mm backing cord (as per joint width). d) For 20mm wide joint: Seal joint 20x20mm deep with Sikaflex 11FC+. For 12mm wide joint: Seal joint 12x10mm deep with Sikaflex 11FC+.  For 10mm wide joint: Seal joint 10mm deep with Sikaflex 11FC+.","",{"v":0,"d":"0.0"},"","","","","26/06/2023 09:53:27",""]
[2828,13005,12,14,"12/70"," C","12/70. C","","12mm Wide joint","m",83,"","","","","27/06/2023 10:09:57",""]
[2829,13010,12,14,"12/70"," D","12/70. D","","20mm Wide joint","m",40,"","","","","27/06/2023 10:10:01",""]
[2830,13007,12,14,"12/71","","12/71","","\"Sikaflex 11FC+\" polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 08:40:39",""]
[2831,13008,12,14,"12/71"," A","12/71. A","","12 x 10mm In expansion joints in walls including raking out expansion joint filler as necessary","m",192,"","","","","21/06/2023 11:21:26",""]
[2832,13480,12,14,"12/71"," B","12/71. B","","20 x 20mm In expansion joints in walls including raking out expansion joint filler as necessary","m",101,"","","","","21/06/2023 11:21:30",""]
[2833,13014,12,14,"12/71","","12/71","","\"ABE Epidermix 344\" two-component, solvent-free, polysulphide modified epoxy adhesive substrate","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 03:55:08",""]
[2834,13017,12,14,"12/71"," C","12/71. C","","On concrete walls","m2",34,"","","","","08/12/2021 03:55:20",""]
[2835,13015,12,14,"12/71","","12/71","","\"ABE Durarep FR\" single component, polymer modified fibre-reinforced, cement based, chloride free, non-shrink mortar","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:57:02",""]
[2836,13016,12,14,"12/71"," D","12/71. D","","30mm Thick on concrete walls","m2",34,"","","","","08/12/2021 03:54:29",""]
[2837,12611,12,14,"12/71","","12/71","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:10:37",""]
[2838,12646,12,14,"12/71","","12/71","","Breaking up and removing reinforced concrete","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 10:32:19",""]
[2839,12343,12,14,"12/71"," E","12/71. E","","450 x 100mm In-situ copings","m",156,"","","","","10/12/2021 01:47:45",""]
[2840,13431,12,14,"12/71"," F","12/71. F","","500 x 100mm In-situ copings","m",75,"","","","","10/12/2021 01:47:49",""]
[2841,13432,12,14,"12/71"," G","12/71. G","","550 x 100mm In-situ copings","m",245,"","","","","10/12/2021 01:47:53",""]
[2842,12647,12,14,"12/71","","12/71","","Demolishing and removing","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:17:13",""]
[2843,12648,12,14,"12/71"," H","12/71. H","","Portions of reinforced concrete retaining walls built in panels including foundations (excavations to expose foundations measured elsewhere)","m3",88,"","","","","20/06/2023 10:42:53",""]
[2844,12644,12,14,"12/71","","12/71","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","12/11/2021 12:06:18",""]
[2845,12502,12,14,"12/71","","12/71","","Hacking up/off and removing granolithic, screeds, plaster, etc. from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc.","H4",{"v":0,"d":"0.0"},"","","","","22/06/2023 09:11:04",""]
[2846,12503,12,14,"12/71"," I","12/71. I","","Plaster from brick walls","m2",169,"","","","","08/12/2021 05:34:44",""]
[2847,12987,12,14,"12/71"," J","12/71. J","","75mm Wide stone cladding from concrete walls","m2",19,"","","","","08/12/2021 10:33:15",""]
[2848,12651,12,14,"12/71","","12/71","","EXCAVATION, FILLING, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:10:43",""]
[2849,13816,12,14,"12/72","","12/72","","EXCAVATIONS","H3",{"v":0,"d":"0.0"},"","","","","20/06/2023 12:15:48",""]
[2850,13817,12,14,"12/72","","12/72","","Excavation in earth not exceeding 2m deep","H4",{"v":0,"d":"0.0"},"","","","","20/06/2023 09:55:10",""]
[2851,12649,12,14,"12/72"," A","12/72. A","","To expose foundations (Labour Intensive)","m3",95,"","","","","26/06/2023 11:15:16",""]
[2852,12660,12,14,"12/72","","12/72","","FILLING, ETC","H3",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:10:55",""]
[2853,12661,12,14,"12/72","","12/72","","Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 98% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","01/12/2021 03:16:25",""]
[2854,12662,12,14,"12/72"," B","12/72. B","","Backfilling behind retaining walls","m3",63,"","","","","07/12/2021 04:20:29",""]
[2855,12663,12,14,"12/72"," C","12/72. C","","Backfilling to trenches, holes, etc.","m3",49,"","","","","07/12/2021 04:20:41",""]
[2856,12664,12,14,"12/72","","12/72","","G7 Earth filling supplied by the contractor, compacted to 98% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:45:45",""]
[2857,12665,12,14,"12/72"," D","12/72. D","","Backfilling behind retaining walls","m3",5,"","","","","08/12/2021 03:49:15",""]
[2858,12666,12,14,"12/72"," E","12/72. E","","Backfilling to trenches, holes, etc.","m3",7,"","","","","08/12/2021 03:49:20",""]
[2859,12667,12,14,"12/72","","12/72","","\"Free draining\" coarse filling material obtained from excavations as per engineers specifications","H4",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:49:10",""]
[2860,12668,12,14,"12/72"," F","12/72. F","","Behind retaining walls","m3",27,"","","","","20/06/2023 10:49:17",""]
[2861,12669,12,14,"12/72","","12/72","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:24:28",""]
[2862,12670,12,14,"12/72"," G","12/72. G","","Scarify surface of in-situ material for a depth of 150mm and compact to 93% Mod AASHTO density","m2",90,"","","","","15/11/2021 01:03:04",""]
[2863,12671,12,14,"12/72","","12/72","","UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:24:28",""]
[2864,12672,12,14,"12/72","","12/72","","15MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:24:28",""]
[2865,12673,12,14,"12/72"," H","12/72. H","","Surface blinding under footings and bases","m3",5,"","","","","15/11/2021 01:03:08",""]
[2866,12674,12,14,"12/72","","12/72","","REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:24:44",""]
[2867,12675,12,14,"12/72","","12/72","","30MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:24:44",""]
[2868,12676,12,14,"12/72"," I","12/72. I","","Retaining wall footings","m3",27,"","","","","07/12/2021 04:49:28",""]
[2869,12678,12,14,"12/73","","12/73","","REINFORCED CONCRETE CAST ON/IN FORMWORK","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:03",""]
[2870,12679,12,14,"12/73","","12/73","","30MPa/19mm Concrete","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:03",""]
[2871,12680,12,14,"12/73"," A","12/73. A","","Retaining wall footings","m3",1,"","","","","02/12/2021 03:50:39",""]
[2872,12681,12,14,"12/73"," B","12/73. B","","Retaining walls in foundations","m3",5,"","","","","02/12/2021 03:50:42",""]
[2873,12682,12,14,"12/73"," C","12/73. C","","Retaining walls","m3",23,"","","","","02/12/2021 03:50:45",""]
[2874,12683,12,14,"12/73","","12/73","","PIGMENTED CONCRETE","H2",{"v":0,"d":"0.0"},"","","","","14/06/2023 11:58:31",""]
[2875,12684,12,14,"12/73","","12/73","","SUPPLEMENTARY PREAMBLES","H3",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:12",""]
[2876,12685,12,14,"12/73","","12/73","","Material:- Allow for 1 pigment colour;- Pigment material must be suitable for use to colour concrete and must not affect the strength or durability of the concrete; - The colouring agent shall be a single-component, pigmented admixture of approximately 2%-4% of the cement volume.-Only pigment materials approved by SANS shall be allowed to be used.","",{"v":0,"d":"0.0"},"","","","","06/12/2021 08:56:44",""]
[2877,12688,12,14,"12/73","","12/73","","30MPa/19mm Pigmented concrete","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:12",""]
[2878,12741,12,14,"12/73"," D","12/73. D","","Retaining walls in foundations","m3",5,"","","","","21/06/2023 11:34:51",""]
[2879,12689,12,14,"12/73"," E","12/73. E","","Retaining walls","m3",23,"","","","","21/06/2023 11:34:56",""]
[2880,12690,12,14,"12/73","","12/73","","CONCRETE SUNDRIES","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:26",""]
[2881,12691,12,14,"12/73","","12/73","","Finishing top surfaces of concrete smooth with a wood float","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:26",""]
[2882,12693,12,14,"12/73"," F","12/73. F","","Tops of beams, walls, etc.","m2",15,"","","","","21/06/2023 11:35:02",""]
[2883,12694,12,14,"12/73","","12/73","","TEST CUBES","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:25:26",""]
[2884,12695,12,14,"12/73"," G","12/73. G","","Making and testing 150 x 150 x 150mm concrete strength test cube","No",41,"","","","","15/11/2021 01:03:41",""]
[2885,12696,12,14,"12/73","","12/73","","ROUGH FORMWORK (DEGREE OF ACCURACY II)","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:26:37",""]
[2886,12697,12,14,"12/74","","12/74","","Rough formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:26:37",""]
[2887,12698,12,14,"12/74"," A","12/74. A","","Retaining walls with total height not exceeding 3,5m above bearing level","m2",1,"","","","Rate only","06/12/2021 03:12:45",""]
[2888,12699,12,14,"12/74"," B","12/74. B","","Retaining walls with total height not exceeding 3,5m above bearing level circular to not exceeding 1m radius","m2",1,"","","","Rate only","06/12/2021 03:12:54",""]
[2889,12745,12,14,"12/74"," C","12/74. C","","Retaining walls with total height not exceeding 3,5m above bearing level circular to exceeding 1m radius","m2",1,"","","","Rate only","06/12/2021 03:13:37",""]
[2890,12701,12,14,"12/74"," D","12/74. D","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level","m2",1,"","","","Rate only","08/12/2021 03:49:41",""]
[2891,12700,12,14,"12/74"," E","12/74. E","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level circular to not exceeding 1m radius","m2",1,"","","","Rate only","07/12/2021 04:21:56",""]
[2892,12746,12,14,"12/74"," F","12/74. F","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level circular to exceeding 1m radius","m2",1,"","","","Rate only","07/12/2021 04:22:09",""]
[2893,12702,12,14,"12/74"," G","12/74. G","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",1,"","","","Rate only","07/12/2021 04:22:28",""]
[2894,12703,12,14,"12/74"," H","12/74. H","","Edges, risers, ends and reveals not exceeding 300mm high or wide circular to exceeding 1m radius","m",1,"","","","Rate only","07/12/2021 04:22:43",""]
[2895,12704,12,14,"12/74","","12/74","","SMOOTH FORMWORK (DEGREE OF ACCURACY I)","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:26:50",""]
[2896,12705,12,14,"12/74","","12/74","","Smooth formwork to sides","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:26:50",""]
[2897,12706,12,14,"12/74"," I","12/74. I","","Retaining walls with total height not exceeding 3,5m above bearing level","m2",210,"","","","","21/06/2023 11:35:23",""]
[2898,12707,12,14,"12/74"," J","12/74. J","","Retaining walls with total height not exceeding 3,5m above bearing level circular to not exceeding 1m radius","m2",1,"","","","Rate only","21/06/2023 11:35:48",""]
[2899,12708,12,14,"12/74"," K","12/74. K","","Retaining walls with total height not exceeding 3,5m above bearing level circular to exceeding 1m radius","m2",1,"","","","Rate only","21/06/2023 11:35:52",""]
[2900,12709,12,14,"12/74"," L","12/74. L","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level","m2",240,"","","","","21/06/2023 11:36:03",""]
[2901,12739,12,14,"12/74"," M","12/74. M","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level circular to not exceeding 1m radius","m2",1,"","","","Rate only","15/11/2021 01:04:44",""]
[2902,12740,12,14,"12/75"," A","12/75. A","","Retaining walls with total height exceeding 3,5m and not exceeding 5,0m above bearing level circular to exceeding 1m radius","m2",1,"","","","Rate only","07/12/2021 04:23:06",""]
[2903,12710,12,14,"12/75"," B","12/75. B","","Edges, risers, ends and reveals not exceeding 300mm high or wide","m",1,"","","","Rate only","15/11/2021 01:04:53",""]
[2904,12711,12,14,"12/75"," C","12/75. C","","Edges, risers, ends and reveals not exceeding 300mm high or wide circular to not exceeding 1m radius","m",1,"","","","Rate only","15/11/2021 01:04:57",""]
[2905,12712,12,14,"12/75","","12/75","","MOVEMENT JOINTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:11:08",""]
[2906,12713,12,14,"12/75","","12/75","","Expansion joints with 12mm closed cell expanded polyethylene between vertical concrete surfaces","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 03:25:28",""]
[2907,12714,12,14,"12/75"," D","12/75. D","","Not exceeding 300mm high to edges of surface beds","m",10,"","","","","08/12/2021 05:35:18",""]
[2908,12715,12,14,"12/75","","12/75","","Expansion joints with 25mm bitumen impregnated softboard between vertical concrete surfaces, including necessary formwork through","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:27:21",""]
[2909,12716,12,14,"12/75"," E","12/75. E","","Walls not exceeding 300mm thick","m",24,"","","","","15/11/2021 01:01:32",""]
[2910,12717,12,14,"12/75","","12/75","","REINFORCEMENT","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:27:33",""]
[2911,13240,12,14,"12/75","","12/75","","Mild steel dowel bars","H4",{"v":0,"d":"0.0"},"","","","","02/08/2022 08:23:11",""]
[2912,13241,12,14,"12/75"," F","12/75. F","","25mm Diameter dowel bar 500mm long with one end embedded in side of concrete at expansion joint and other end greased and wrapped in polythene sheeting, including hole through formwork","No",16,"","","","","02/08/2022 08:23:01",""]
[2913,12718,12,14,"12/75","","12/75","","Mild steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:27:33",""]
[2914,12719,12,14,"12/75"," G","12/75. G","","Various diameter bars","t",3.33,"","","","","15/11/2021 01:01:26",""]
[2915,12720,12,14,"12/75","","12/75","","High tensile steel reinforcement to structural concrete work","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:27:34",""]
[2916,12721,12,14,"12/75"," H","12/75. H","","Various diameter bars","t",8.33,"","","","","15/11/2021 01:01:22",""]
[2917,12514,12,14,"12/75","","12/75","","STONE CLADDING TO WALLS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:11:15",""]
[2918,12515,12,14,"12/75","","12/75","","\"Potgieter gabion\" stone cladding, secured to wall with adhesive and short galvanised hoop iron strips shot pinned to walls","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 12:09:58",""]
[2919,12744,12,14,"12/75"," I","12/75. I","","75mm Lining to sides of concrete walls","m2",50,"","","","","15/11/2021 01:01:13",""]
[2920,12517,12,14,"12/76"," A","12/76. A","","75mm Lining to sides of brick walls","m2",10,"","","","","15/11/2021 01:01:17",""]
[2921,13453,12,14,"12/76","","12/76","","Remove individual stones in wall cladding, prepare void for new stone and fix new suitably sized stones in position","H3",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:57:42",""]
[2922,13455,12,14,"12/76","","12/76","","Stones from stockpiles on site (all sizes nominal diameter)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:57:42",""]
[2923,13456,12,14,"12/76"," B","12/76. B","","Stone not exceeding 50mm","No",779,"","","","","08/12/2021 03:51:02",""]
[2924,13457,12,14,"12/76"," C","12/76. C","","Stone exceeding 50 and not exceeding 100mm","No",779,"","","","","08/12/2021 03:51:09",""]
[2925,13458,12,14,"12/76"," D","12/76. D","","Stone exceeding 100 and not exceeding 150mm","No",779,"","","","","08/12/2021 03:51:14",""]
[2926,13459,12,14,"12/76"," E","12/76. E","","Stone exceeding 150 and not exceeding 200mm","No",779,"","","","","08/12/2021 03:51:18",""]
[2927,13460,12,14,"12/76"," F","12/76. F","","Stone exceeding 200 and not exceeding 250mm","No",779,"","","","","08/12/2021 03:51:23",""]
[2928,13461,12,14,"12/76","","12/76","","Stones supplied by the contractor (all sizes nominal diameter)","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:57:42",""]
[2929,13462,12,14,"12/76"," G","12/76. G","","Stone not exceeding 50mm","No",15,"","","","","08/12/2021 03:51:43",""]
[2930,13463,12,14,"12/76"," H","12/76. H","","Stone exceeding 50 and not exceeding 100mm","No",15,"","","","","08/12/2021 03:51:49",""]
[2931,13464,12,14,"12/76"," I","12/76. I","","Stone exceeding 100 and not exceeding 150mm","No",15,"","","","","08/12/2021 03:51:52",""]
[2932,13465,12,14,"12/76"," J","12/76. J","","Stone exceeding 150 and not exceeding 200mm","No",15,"","","","","08/12/2021 03:51:56",""]
[2933,13466,12,14,"12/76"," K","12/76. K","","Stone exceeding 200 and not exceeding 250mm","No",15,"","","","","08/12/2021 03:52:00",""]
[2934,13449,12,14,"12/76","","12/76","","Sundries","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 11:05:37",""]
[2935,13450,12,14,"12/76"," L","12/76. L","","Cut back protruding 30mm wide x 1,2mm thick galvanised mild steel cladding tie and coat cut with cold-galvanizing, in confined spaces in between stones (removal of cladding stones around metal tie elsewhere measured)","No",1299,"","","","","08/12/2021 03:50:25",""]
[2936,13451,12,14,"12/76","","12/76","","Remove mortar splatter from stone surfaces","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:57:30",""]
[2937,13452,12,14,"12/76"," M","12/76. M","","General surfaces of stone cladding (measured over the flat surface on elevation)","m2",1382,"","","","","08/12/2021 05:36:58",""]
[2938,12342,12,14,"12/76","","12/76","","CONCRETE COPINGS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:11:29",""]
[2939,12917,12,14,"12/77","","12/77","","In-situ concrete copings finished smooth on exposed surfaces, cast on retaining walls, with expansion joints at maximum 1,5m centres, including all concrete, formwork, and finishes","H4",{"v":0,"d":"0.0"},"","","","","20/06/2023 10:51:21",""]
[2940,12918,12,14,"12/77"," A","12/77. A","","550 x 100mm Thick overall coping, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",245,"","","","","21/06/2023 11:27:10",""]
[2941,12921,12,14,"12/77"," B","12/77. B","","550 x 100mm Thick overall coping, circular to not exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",3,"","","","","21/06/2023 11:27:14",""]
[2942,12922,12,14,"12/77"," C","12/77. C","","550 x 100mm Thick overall coping, circular to exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",3,"","","","","21/06/2023 11:27:17",""]
[2943,12919,12,14,"12/77"," D","12/77. D","","550 x 100mm Thick overall coping, with sloping top; the coping circular on plan and elevation to not exceeding 1m radius","m",3,"","","","","21/06/2023 11:27:20",""]
[2944,12920,12,14,"12/77"," E","12/77. E","","550 x 100mm Thick overall coping, with sloping top; the coping circular on plan and elevation to exceeding 1m radius","m",3,"","","","","21/06/2023 11:27:23",""]
[2945,12923,12,14,"12/77"," F","12/77. F","","500 x 100mm Thick overall coping, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",75,"","","","","21/06/2023 11:27:26",""]
[2946,12926,12,14,"12/77"," G","12/77. G","","500 x 100mm Thick overall coping, circular to not exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",2,"","","","","21/06/2023 11:27:29",""]
[2947,12927,12,14,"12/77"," H","12/77. H","","500 x 100mm Thick overall coping, circular to exceeding 1m radius, with and including 50 x 30mm recess and separate drip groove in bottom along one edge","m",2,"","","","","21/06/2023 11:27:32",""]
[2948,12924,12,14,"12/77"," I","12/77. I","","500 x 100mm Thick overall coping, with sloping top; the coping circular on plan and elevation to not exceeding 1m radius","m",2,"","","","","21/06/2023 11:27:35",""]
[2949,12925,12,14,"12/77"," J","12/77. J","","500 x 100mm Thick overall coping, with sloping top; the coping circular on plan and elevation to exceeding 1m radius","m",2,"","","","","21/06/2023 11:27:37",""]
[2950,12344,12,14,"12/77","","12/77","","Precast concrete finished smooth on exposed surfaces including bedding on ABE Epidermix epoxy mortar, jointing and pointing with ABE Dura cement grout with TAL keycoat water repellent additive in max. 5mm gaps between units","H4",{"v":0,"d":"0.0"},"","","","","05/11/2021 02:23:06",""]
[2951,12348,12,14,"12/77"," K","12/77. K","","440 x 100mm Thick overall Modcon, or similar approved, mono pitch coping weathered on top, with concave mortar  joints between units (coping type 021)","m",210,"","","","","12/11/2021 11:08:56",""]
[2952,12510,12,14,"12/78"," A","12/78. A","","Ditto, but to radius not exceeding 4m","m",6,"","","","","12/11/2021 11:08:59",""]
[2953,12349,12,14,"12/78"," B","12/78. B","","Extra over for fair returned stopped end","No",2,"","","","","12/11/2021 11:09:02",""]
[2954,12350,12,14,"12/78"," C","12/78. C","","Extra over for mitred angle intersection","No",1,"","","","","12/11/2021 11:09:06",""]
[2955,12351,12,14,"12/78","","12/78","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","05/11/2021 02:23:06",""]
[2956,12352,12,14,"12/78","","12/78","","Prepare and apply ABE Duraflex cementitious flexible slurry waterproofing with ecofelt membrane on","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:31:45",""]
[2957,12353,12,14,"12/78"," D","12/78. D","","Tops of parapet walls","m2",34,"","","","","21/06/2023 11:31:53",""]
[2958,12354,12,14,"12/78","","12/78","","Prepare and apply TFC, or similar approved, cement sealant on","H4",{"v":0,"d":"0.0"},"","","","","21/06/2023 11:32:01",""]
[2959,12355,12,14,"12/78"," E","12/78. E","","General surfaces of precast concrete copings","m2",165,"","","","","21/06/2023 11:32:08",""]
[2960,12731,12,14,"12/78","","12/78","","Two coats bitumen emulsion waterproof coating on","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:29:07",""]
[2961,12732,12,14,"12/78"," F","12/78. F","","Concrete walls and columns in foundations","m2",39,"","","","","15/11/2021 01:00:18",""]
[2962,12733,12,14,"12/78"," G","12/78. G","","Concrete walls, columns and beams","m2",126,"","","","","15/11/2021 01:00:20",""]
[2963,12356,12,14,"12/78","","12/78","","SEALING STRIPS, JOINT SEALANTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:11:39",""]
[2964,12357,12,14,"12/78","","12/78","","\"Sikaflex 11FC\" polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 08:40:02",""]
[2965,12358,12,14,"12/78"," H","12/78. H","","5 x 5mm Pointing to expansion joints between precast concrete coping units","m",128,"","","","","12/11/2021 11:09:21",""]
[2966,13244,12,14,"12/78"," I","12/78. I","","10 x 10mm In expansion joints in floors, etc, including raking out expansion joint filler as necessary","m",10,"","","","","08/12/2021 05:37:10",""]
[2967,12504,12,14,"12/78","","12/78","","PLASTERING","H2",{"v":0,"d":"0.0"},"","","","","09/11/2021 09:59:27",""]
[2968,12505,12,14,"12/78","","12/78","","Cement plaster wood floated, on brickwork","H4",{"v":0,"d":"0.0"},"","","","","20/06/2023 11:15:16",""]
[2969,12506,12,14,"12/78"," J","12/78. J","","On walls","m2",169,"","","","","12/11/2021 11:09:31",""]
[2970,12724,12,14,"12/78","","12/78","","SUBSOIL DRAINAGE","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 09:28:31",""]
[2971,12726,12,14,"12/78"," K","12/78. K","","19mm Crushed stone encasing to pipes","m3",5,"","","","","07/12/2021 04:24:30",""]
[2972,12727,12,14,"12/79"," A","12/79. A","","Geofabric filter blanket (PSDK 3.1.3) wrapped around 300 x 300mm stone encasing (measured elsewhere) with 100mm side and end laps, including stitching","m2",72,"","","","","21/06/2023 11:33:19",""]
[2973,12728,12,14,"12/79"," B","12/79. B","","Geofabric filter blanket (PSDK 3.1.3) with 100mm side and end laps, including stitching","m2",350,"","","","","10/12/2021 03:19:40",""]
[2974,12729,12,14,"12/79"," C","12/79. C","","Fin drain drainage core of HDPe type with a mass 500g/m2, tensile strength of 3kN, and discharge capacity under 50kPa of 0.4l/s/m to walls (PSLE 3.5.1)","m2",165,"","","","","10/12/2021 03:19:48",""]
[2975,12730,12,14,"12/79"," D","12/79. D","","100mm HDPe perforated pipes laid in stone encasing (encasing elsewhere) (PSLE 3.5.2)","m",60,"","","","","21/06/2023 11:33:26",""]
[2977,9590,12,15,"12/82","","12/82","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:21:28",""]
[2978,9591,12,15,"12/82","","12/82","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:52",""]
[2979,9592,12,15,"12/82","","12/82","","BILL NO. 15","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:58:02",""]
[2980,9593,12,15,"12/82","","12/82","","BOUNDARY WALLING AND SECURITY FENCING","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:45",""]
[2981,9594,12,15,"12/82","","12/82","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","15/09/2021 06:43:01",""]
[2982,9595,12,15,"12/82","","12/82","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:41:02",""]
[2983,9596,12,15,"12/82","","12/82","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","15/09/2021 06:43:01",""]
[2984,9600,12,15,"12/82","","12/82","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","15/09/2021 06:45:08",""]
[2985,9601,12,15,"12/82","","12/82","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:33:59",""]
[2986,13381,12,15,"12/82","","12/82","","Note : Fencing to be erected to conform to all Occupational Health & Safety Act requirements, including appropriate signage.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:34:46",""]
[2987,13378,12,15,"12/82","","12/82","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:34:35",""]
[2988,13379,12,15,"12/82","","12/82","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:34:35",""]
[2989,12623,12,15,"12/82","","12/82","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:11:50",""]
[2990,12624,12,15,"12/82"," A","12/82. A","","Break down and remove 300 x 64/60mm thick in-situ concrete copings","m",114,"","","","","19/11/2021 08:51:08",""]
[2991,12615,12,15,"12/83","","12/83","","REMOVAL OF EXISTING WORK","H2",{"v":0,"d":"0.0"},"","","","","12/11/2021 12:02:58",""]
[2992,7602,12,15,"12/83"," A","12/83. A","","Take down and remove 2 400mm high temporary fencing complete at completion of project, including removing posts, concrete bases, filling up holes, and leaving surfaces level and tidy","m",135,"","","","","07/12/2021 12:16:10",""]
[2993,12616,12,15,"12/83","","12/83","","Taking out 2 400mm high Betafence/Clearvue security fencing panels and set aside for re-use including later re-fixing in same position to brick piers (piers elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 03:12:49",""]
[2994,12617,12,15,"12/83"," B","12/83. B","","1 223mm Panel","No",1,"","","","","09/12/2021 03:12:00",""]
[2995,12618,12,15,"12/83"," C","12/83. C","","1 356mm Panel","No",1,"","","","","09/12/2021 03:12:08",""]
[2996,12619,12,15,"12/83"," D","12/83. D","","1 483mm Panel","No",1,"","","","","09/12/2021 03:12:11",""]
[2997,12620,12,15,"12/83"," E","12/83. E","","1 561mm Panel","No",1,"","","","","09/12/2021 03:12:15",""]
[2998,12621,12,15,"12/83"," F","12/83. F","","1 737mm Panel","No",1,"","","","","09/12/2021 03:12:18",""]
[2999,12622,12,15,"12/83"," G","12/83. G","","3 297mm Panel","No",35,"","","","","09/12/2021 03:12:04",""]
[3000,12642,12,15,"12/83","","12/83","","Hacking up/off and removing granolithic, screeds, plaster, etc. from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc.","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:20:45",""]
[3001,12643,12,15,"12/83"," H","12/83. H","","Plaster from brick walls","m2",25,"","","","","19/11/2021 08:51:21",""]
[3002,12625,12,15,"12/83","","12/83","","PRECAST CONCRETE COPINGS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:11:57",""]
[3003,12626,12,15,"12/83","","12/83","","Precast concrete finished smooth on exposed surfaces including bedding on ABE Epidermix epoxy mortar, jointing and pointing with ABE Dura cement grout with TAL keycoat water repellent additive in max. 5mm gaps between units","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 12:04:55",""]
[3004,12627,12,15,"12/83"," I","12/83. I","","370 x 100mm Thick overall Modcon, or similar approved, mono pitch coping weathered on top, with concave mortar  joints between units (coping type 014)","m",114,"","","","","19/11/2021 08:51:30",""]
[3005,12628,12,15,"12/83"," J","12/83. J","","Extra over for fair returned stopped end","No",5,"","","","","26/06/2023 12:06:57",""]
[3006,12629,12,15,"12/83"," K","12/83. K","","Extra over for mitred angle intersection","No",2,"","","","","26/06/2023 12:06:53",""]
[3007,12634,12,15,"12/83","","12/83","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","12/11/2021 12:05:05",""]
[3008,12635,12,15,"12/84","","12/84","","Prepare and apply ABE Duraflex cementitious flexible slurry waterproofing with ecofelt membrane","H4",{"v":0,"d":"0.0"},"","","","","13/04/2023 09:28:15",""]
[3009,12636,12,15,"12/84"," A","12/84. A","","To tops of parapet walls","m2",50,"","","","","27/06/2023 10:02:51",""]
[3010,12637,12,15,"12/84","","12/84","","Prepare and apply TFC, or similar approved, cement sealant","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 12:05:05",""]
[3011,12638,12,15,"12/84"," B","12/84. B","","To general surfaces of precast concrete copings","m2",107,"","","","","19/11/2021 08:51:39",""]
[3012,12639,12,15,"12/84","","12/84","","SEALING STRIPS, JOINT SEALANTS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:12:04",""]
[3013,12640,12,15,"12/84","","12/84","","Sikaflex 11FC polyurethane sealing compound including backing cord, bond breaker, primer, etc.","H4",{"v":0,"d":"0.0"},"","","","","12/11/2021 12:05:05",""]
[3014,12641,12,15,"12/84"," C","12/84. C","","5 x 5mm Pointing to expansion joints between precast concrete coping units","m",42,"","","","","19/11/2021 08:51:50",""]
[3015,11202,12,15,"12/84","","12/84","","PROPRIETARY METAL FENCING","H2",{"v":0,"d":"0.0"},"","","","","28/10/2021 03:33:25",""]
[3016,9611,12,15,"12/84","","12/84","","Repairs to damaged panels, posts etc.","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 11:08:15",""]
[3017,13654,12,15,"12/84"," D","12/84. D","","Take out and remove 2 500 x 2 400mm high fence panel (adjacent posts to remain)","No",25,"","","","","09/12/2021 12:09:32",""]
[3018,13663,12,15,"12/84"," E","12/84. E","","Take out and remove maximum 2 500mm long x 1 600-1 900mm high panels (adjacent posts to remain)","No",20,"","","","","09/12/2021 12:11:51",""]
[3019,13668,12,15,"12/84"," F","12/84. F","","Take out and remove incorrectly sized posts, including removing sheer bolts from adjacent panels","No",20,"","","","","09/12/2021 12:10:22",""]
[3020,13671,12,15,"12/84"," G","12/84. G","","Take out and remove damaged posts, including removing sheer bolts from adjacent panels","No",25,"","","","","09/12/2021 01:42:01",""]
[3021,13655,12,15,"12/84"," H","12/84. H","","Take off saw-tooth spike strip from 2 500mm long panel and set aside for re-use (re-use elsewhere)","No",45,"","","","","09/12/2021 02:30:46",""]
[3022,13673,12,15,"12/84"," I","12/84. I","","Take off saw-tooth spike from 2 500mm long panel and remove","No",20,"","","","","09/12/2021 02:29:46",""]
[3023,13656,12,15,"12/84"," J","12/84. J","","Take off underdig from 2 500mm long panel and set aside for re-use (re-use elsewhere)","No",45,"","","","","09/12/2021 12:13:53",""]
[3024,13658,12,15,"12/84"," K","12/84. K","","Take off and remove underdig from 2 500mm long panel","No",25,"","","","","09/12/2021 12:13:44",""]
[3025,13660,12,15,"12/84"," L","12/84. L","","Take out and remove defective fence clamps","No",80,"","","","","09/12/2021 12:14:21",""]
[3026,13669,12,15,"12/84"," M","12/84. M","","Take out and remove damaged sheer bolts","No",200,"","","","","09/12/2021 12:14:17",""]
[3027,13670,12,15,"12/85"," A","12/85. A","","New sheer bolt with head, nut & washers - as per manufacturer's installation instructions","No",300,"","","","","09/12/2021 12:15:09",""]
[3028,13661,12,15,"12/85"," B","12/85. B","","New set of fence clamps including fixing bolt with shear nut","No",280,"","","","","09/12/2021 01:41:29",""]
[3029,13666,12,15,"12/85"," C","12/85. C","","Re-fit underdig to 2 500mm long fence panel, including fitting new sheer bolts","No",45,"","","","","09/12/2021 01:41:45",""]
[3030,13667,12,15,"12/85"," D","12/85. D","","Re-fit saw-tooth spike strip to 2 500mm long fence panel, including fitting new sheer bolts","No",45,"","","","","09/12/2021 02:30:34",""]
[3031,13675,12,15,"12/85"," E","12/85. E","","New saw-tooth spike strip to 2 500mm long fence panel, including fixing mechanisms","No",20,"","","","","09/12/2021 02:54:19",""]
[3032,13659,12,15,"12/85"," F","12/85. F","","New underdig to 2 500mm long panel including fixing mechanisms","No",25,"","","","","09/12/2021 01:40:42",""]
[3033,13657,12,15,"12/85"," G","12/85. G","","New 2 500 x 2 400mm high fence panel including fixing mechanisms on either side","No",25,"","","","","09/12/2021 01:40:22",""]
[3034,13665,12,15,"12/85"," H","12/85. H","","New 2 400mm high post including base and fixing mechanisms, and attaching adjacent panels to post","No",45,"","","","","09/12/2021 01:39:50",""]
[3035,13672,12,15,"12/85"," I","12/85. I","","Provide the sum of R30 000.00 (Thirty Thousand) for fence panel and post coating repairs to be done by an approved specialist","Item",{"v":1,"d":"1.00"},{"v":30000,"d":"30000.00"},{"v":30000,"d":"30000.00"},"","","09/12/2021 02:25:21",""]
[3036,9608,12,15,"12/85","","12/85","","General cleaning of fence by removing all dirt, grime, mortar splatter, etc., (without damaging the fence material) and leave in a clean and sound state","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:21:09",""]
[3037,13676,12,15,"12/85"," J","12/85. J","","Fence 2 400mm high","m",1434,"","","","","09/12/2021 02:55:18",""]
[3038,9609,12,15,"12/85","","12/85","","Inspect, align and tighten fence bolts and ensure that heads snap off (replacement of missing bolts measured elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","09/12/2021 02:34:30",""]
[3039,9638,12,15,"12/85"," K","12/85. K","","Fence 2 400mm high","m",1434,"","","","","09/12/2021 02:55:27",""]
[3040,12930,12,15,"12/85","","12/85","","PLASTERING","H2",{"v":0,"d":"0.0"},"","","","","19/11/2021 08:12:52",""]
[3041,12931,12,15,"12/85","","12/85","","One coat 1:5 cement plaster, on brickwork","H4",{"v":0,"d":"0.0"},"","","","","19/11/2021 08:12:52",""]
[3042,12932,12,15,"12/85"," L","12/85. L","","Walls","m2",25,"","","","","19/11/2021 08:52:19",""]
[3043,12875,12,15,"12/86","","12/86","","SPECIALISED PLASTER TYPE WALL COATINGS","H2",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:09:52",""]
[3044,12876,12,15,"12/86","","12/86","","All specialised plaster type wall coatings are to be executed in strict accordance with the manufacturer's instructions and by registered applicators","",{"v":0,"d":"0.0"},"","","","","17/11/2021 11:09:52",""]
[3045,12877,12,15,"12/86","","12/86","","Intermediate texture rough-cast plaster (1 part cement/1.5 parts coarse sand), with bonding liquid additive (10% of water volume), applied with a Terylene application machine","H4",{"v":0,"d":"0.0"},"","","","","18/11/2021 07:47:10",""]
[3046,12878,12,15,"12/86"," A","12/86. A","","On walls","m2",25,"","","","","18/11/2021 07:46:59",""]
[3047,12879,12,15,"12/86"," B","12/86. B","","On narrow widths not exceeding 300mm wide","m2",30,"","","","","08/12/2021 04:59:09",""]
[3048,12880,12,15,"12/86"," C","12/86. C","","On projecting and isolated piers","m2",20,"","","","","08/12/2021 04:59:13",""]
[3050,10179,12,16,"12/88","","12/88","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","10/02/2022 12:21:31",""]
[3051,10180,12,16,"12/88","","12/88","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:20:58",""]
[3052,10181,12,16,"12/88","","12/88","","BILL NO. 16","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:58:06",""]
[3053,10182,12,16,"12/88","","12/88","","WORK TO BURIAL SITE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:50",""]
[3054,13382,12,16,"12/88","","12/88","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:09",""]
[3055,13383,12,16,"12/88","","12/88","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:41:06",""]
[3056,13384,12,16,"12/88","","12/88","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:10",""]
[3057,13391,12,16,"12/88","","12/88","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:43",""]
[3058,13392,12,16,"12/88","","12/88","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:43",""]
[3059,13387,12,16,"12/88","","12/88","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:10",""]
[3060,13388,12,16,"12/88","","12/88","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:10",""]
[3061,13389,12,16,"12/89","","12/89","","Work in sensitive area","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:10",""]
[3062,13390,12,16,"12/89","","12/89","","The Burial site is an area with historical significance and classified as a National Heritage Site (Management Authority - Greater Baviaanskloof Concervancy, contact - Kouga Municipality). The site is subject to the NHRA (National Heritage Resources Act) . All work on and around the Burial site shall therefore be executed with extra care not to cause any potential damage to the actual Burial Site or surrounding vegetation and must be strictly within the guidelines as stipulated in the landscape architect’s specification as well as the EMP and NHRA. This includes the protection of all indigenous species on and around Vergaderingskop.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:36:10",""]
[3063,13048,12,16,"12/89","","12/89","","DEMOLITIONS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:12:20",""]
[3064,13049,12,16,"12/89","","12/89","","Breaking up and removing","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 12:42:03",""]
[3065,13050,12,16,"12/89"," A","12/89. A","","650 x 100mm In-situ copings","m",130,"","","","","06/12/2021 08:47:53",""]
[3066,13051,12,16,"12/89","","12/89","","CONCRETE COPINGS, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:12:24",""]
[3067,13054,12,16,"12/89","","12/89","","In-situ concrete copings finished smooth on exposed surfaces to be cast on retaining walls, with expansion joints at maximum 1,5m centres, including all concrete, formwork, and finishes","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 08:49:46",""]
[3068,13055,12,16,"12/89"," B","12/89. B","","650 x 175mm Thick overall copings, with and including 50 x 50mm recess and drip groove in bottom along one edge","m",130,"","","","","08/12/2021 04:58:29",""]
[3069,13056,12,16,"12/89"," C","12/89. C","","Extra over for fair returned stopped end","No",2,"","","","","08/12/2021 04:58:35",""]
[3070,13057,12,16,"12/89"," D","12/89. D","","Extra over for mitred angle intersection","No",10,"","","","","08/12/2021 04:58:39",""]
[3071,13058,12,16,"12/89","","12/89","","WATERPROOFING","H2",{"v":0,"d":"0.0"},"","","","","03/12/2021 12:50:02",""]
[3072,13059,12,16,"12/89","","12/89","","Prepare and apply TFC, or similar approved, cement sealant","H4",{"v":0,"d":"0.0"},"","","","","03/12/2021 12:50:02",""]
[3073,13060,12,16,"12/89"," E","12/89. E","","To general surfaces of precast concrete copings","m2",175,"","","","","03/12/2021 12:50:02",""]
[3074,13090,12,16,"12/89","","12/89","","3-Ply malthoid","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 08:51:59",""]
[3075,13091,12,16,"12/89"," F","12/89. F","","Two layers to tops of retaining walls, including thin mortar bed below","m2",39,"","","","","08/12/2021 04:58:47",""]
[3077,10183,12,17,"12/91","","12/91","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","14/10/2021 10:33:31",""]
[3078,10184,12,17,"12/91","","12/91","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:02",""]
[3079,10185,12,17,"12/91","","12/91","","BILL NO. 17","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:58:10",""]
[3080,10186,12,17,"12/91","","12/91","","BUILDERS WORK IN CONNECTION WITH SPECIALIST INSTALLATIONS","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:24:55",""]
[3081,12760,12,17,"12/91","","12/91","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3082,12761,12,17,"12/91","","12/91","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:41:11",""]
[3083,12762,12,17,"12/91","","12/91","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3084,13393,12,17,"12/91","","12/91","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:20",""]
[3085,13394,12,17,"12/91","","12/91","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:20",""]
[3086,12763,12,17,"12/91","","12/91","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3087,12764,12,17,"12/91","","12/91","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3088,12765,12,17,"12/91","","12/91","","Laying, backfilling, bedding, etc. of pipes","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 03:21:58",""]
[3089,12766,12,17,"12/91","","12/91","","All sleeves are to be laid in accordance with SANS 1200 LC","",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:15:53",""]
[3090,12767,12,17,"12/92","","12/92","","Tenderers are hereby informed that where SANS specifications are referred to in these Bills of Quantities and specifications, then ONLY the Specification of work clauses will apply. The method of measurement and payment clauses will NOT apply to this contract.","",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3091,12768,12,17,"12/92","","12/92","","SLEEVES FOR ELECTRICAL, TELEPHONE CABLES, IRRIGATION PIPES, ETC","H2",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:12:34",""]
[3092,12769,12,17,"12/92","","12/92","","EARTHWORKS","H3",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3093,12770,12,17,"12/92","","12/92","","Excavate in earth and set excavated material aside for re-use as filling","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 12:30:10",""]
[3094,12771,12,17,"12/92"," A","12/92. A","","Excavation in earth not exceeding 2m deep for pipe trenches (Labour Intensive)","m3",170,"","","","","26/06/2023 11:16:18",""]
[3095,12774,12,17,"12/92"," B","12/92. B","","Selected and approved material from the excavations, in backfilling in trenches, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",170,"","","","","26/06/2023 11:16:22",""]
[3096,12775,12,17,"12/92"," C","12/92. C","","Bedding material supplied by the contractor, compacted to 93% Mod AASHTO density (Labour Intensive)","m3",30,"","","","","26/06/2023 11:16:26",""]
[3097,12776,12,17,"12/92"," D","12/92. D","","Bedding material supplied by the contractor, stabilised with 5% OPC, and compacted to 93% Mod AASHTO density (Labour Intensive)","m3",15,"","","","","26/06/2023 11:16:42",""]
[3098,12777,12,17,"12/92"," E","12/92. E","","Cart away surplus excavated material from the excavations to a dumping site to be located by the contractor","m3",5,"","","","","26/06/2023 11:16:36",""]
[3099,12798,12,17,"12/92","","12/92","","Repairs to sleeves","H3",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:11:14",""]
[3100,12778,12,17,"12/92","","12/92","","uPVC class 51 sleeve piping including short lengths and jointing, laid in trenches (trenches and backfilling measured elsewhere)","H4",{"v":0,"d":"0.0"},"","","","","10/12/2021 02:55:46",""]
[3101,12779,12,17,"12/92"," F","12/92. F","","50mm Diameter pipe","m",5,"","","","","14/11/2021 08:09:19",""]
[3102,12780,12,17,"12/92"," G","12/92. G","","110mm Diameter pipe","m",200,"","","","","14/11/2021 08:09:19",""]
[3103,12781,12,17,"12/92"," H","12/92. H","","160mm Diameter pipe","m",200,"","","","","14/11/2021 08:09:19",""]
[3104,12782,12,17,"12/92","","12/92","","Extra over uPVC piping for:","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 05:17:38",""]
[3105,12783,12,17,"12/92"," I","12/92. I","","50mm Diameter long radius bend","No",1,"","","","","14/11/2021 08:09:19",""]
[3106,12784,12,17,"12/92"," J","12/92. J","","110mm Diameter long radius bend","No",1,"","","","","06/12/2021 05:18:41",""]
[3107,12785,12,17,"12/93"," A","12/93. A","","160mm Diameter long radius bend","No",1,"","","","","06/12/2021 05:18:44",""]
[3108,12786,12,17,"12/93","","12/93","","Draw wires","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:09:19",""]
[3109,12787,12,17,"12/93"," B","12/93. B","","3mm Galvanised steel draw wires in pipes","m",400,"","","","","14/11/2021 08:09:20",""]
[3110,12799,12,17,"12/93","","12/93","","Repairs to draw chambers","H3",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:11:35",""]
[3111,13437,12,17,"12/93"," C","12/93. C","","Take up broken lockable polymer draw chamber cover (cover only)","No",1,"","","","","10/12/2021 02:42:33",""]
[3112,12795,12,17,"12/93"," D","12/93. D","","Take up and remove broken lockable cast iron draw chamber cover (cover only)","No",1,"","","","","10/12/2021 02:42:16",""]
[3113,12800,12,17,"12/93","","12/93","","Excavate in earth and dispose on site, in cut-to-fill operation including lightly compacting around draw chamber covers in maximum 150mm thick layers to 90% Mod AASHTO density","H4",{"v":0,"d":"0.0"},"","","","","06/12/2021 03:18:33",""]
[3114,12801,12,17,"12/93"," E","12/93. E","","General filling and shaping of areas around draw chambers, etc.","m3",15,"","","","","09/12/2021 04:05:02",""]
[3115,12788,12,17,"12/93","","12/93","","Cleaning of brick draw chambers, etc.","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 01:08:37",""]
[3116,12789,12,17,"12/93"," F","12/93. F","","Clean out and remove silt, vegetation, rubble, etc. from  inside of square, rectangular or round catchpit, manhole or valve chamber","No",46,"","","","","10/12/2021 01:57:36",""]
[3117,12797,12,17,"12/93","","12/93","","Covers","H4",{"v":0,"d":"0.0"},"","","","","14/11/2021 08:10:21",""]
[3118,12807,12,17,"12/93"," G","12/93. G","","450 x 450mm Type 4 Cast iron single seal manhole cover (no frame)","No",1,"","","","","15/11/2021 01:07:46",""]
[3119,12792,12,17,"12/93"," H","12/93. H","","450 x 450mm Type 4 Cast iron single seal manhole cover and frame","No",1,"","","","","09/12/2021 03:32:18",""]
[3120,12793,12,17,"12/93"," I","12/93. I","","650mm Diameter Type 1A concrete-filled polymer heavy duty lockable manhole cover and frame (code : 2230)","No",2,"","","","","14/11/2021 08:09:43",""]
[3121,12794,12,17,"12/93"," J","12/93. J","","650mm Diameter Type 1A concrete-filled (exposed aggregate, to match adjacent paving) cast iron heavy duty manhole cover and frame (code : 2230)","No",2,"","","","","14/11/2021 08:09:43",""]
[3123,10187,12,18,"12/95","","12/95","","SECTION NO. 12","H1",{"v":0,"d":"0.0"},"","","","","14/10/2021 10:13:09",""]
[3124,10188,12,18,"12/95","","12/95","","R331 UPGRADE - REMEDIAL WORK (Provisional)","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:21:07",""]
[3125,10189,12,18,"12/95","","12/95","","BILL NO. 18","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 02:58:14",""]
[3126,10190,12,18,"12/95","","12/95","","R331 UPGRADE","H1",{"v":0,"d":"0.0"},"","","","","26/06/2023 11:25:01",""]
[3127,13395,12,18,"12/95","","12/95","","PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:44",""]
[3128,13396,12,18,"12/95","","12/95","","For Preambles refer to \"Department : Public Works : Construction works : specifications - PW 371-A & B\"  PW 371-A(Generic) is available at : www.publicworks.gov.za/consultantsdocs.html  PW 371-B(Project-specific) is bound elsewhere in the tender documents","",{"v":0,"d":"0.0"},"","","","","26/06/2023 12:41:15",""]
[3129,13397,12,18,"12/95","","12/95","","SUPPLEMENTARY PREAMBLES","H2",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:44",""]
[3130,13406,12,18,"12/95","","12/95","","Additional project-specific specifications","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:38:29",""]
[3131,13407,12,18,"12/95","","12/95","","Tenderers are advised to study the relevant project-specific specifications and reports accompanying the tender documents before pricing this bill.  Where there are contradictions between the above mentioned specifications and/or reports and the PW371 specification the relevant consultant shall be requested to advise which specification shall apply, failing which the PW371 specification shall apply.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:38:30",""]
[3132,13400,12,18,"12/95","","12/95","","Nature of ground","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:44",""]
[3133,13401,12,18,"12/95","","12/95","","A geotechnical investigation has been carried out on the site and the report is annexed to these documents.","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:44",""]
[3134,13402,12,18,"12/95","","12/95","","Testing of material and filling","H4",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:44",""]
[3135,13403,12,18,"12/95","","12/95","","Descriptions of earth filling, compaction, etc shall be deemed to include for all necessary testing required in accordance with the SANS 1200 series","",{"v":0,"d":"0.0"},"","","","","07/12/2021 09:37:44",""]
[3136,12481,12,18,"12/96","","12/96","","SAFEGUARDING AND ACCOMMODATION OF TRAFFIC","H2",{"v":0,"d":"0.0"},"","","","","08/11/2021 03:33:56",""]
[3137,12482,12,18,"12/96"," A","12/96. A","","Provide all necessary temporary works, signage, and traffic control measures during construction, on a 24-hour basis (Refer to PSA 5.10, SANS 1200 A5.2, and SANS 1200 D5 1.6)","Item",{"v":1,"d":"1.00"},"","","","","21/06/2023 11:28:23",""]
[3138,10324,12,18,"12/96","","12/96","","ALTERATIONS/REPAIRS","H2",{"v":0,"d":"0.0"},"","","","","09/12/2021 03:29:14",""]
[3139,12483,12,18,"12/96"," B","12/96. B","","Saw cut existing tarmac surface","m",29,"","","","","09/11/2021 11:50:46",""]
[3140,12484,12,18,"12/96","","12/96","","Compaction of surfaces","H4",{"v":0,"d":"0.0"},"","","","","08/11/2021 03:34:19",""]
[3141,12485,12,18,"12/96"," C","12/96. C","","Compaction of ground surfaces under pavings etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 95% Mod AASHTO density (Labour Intensive)","m2",10,"","","","","26/06/2023 11:17:08",""]
[3142,12486,12,18,"12/96","","12/96","","Bituminous premix road surfacing in repairs to damaged road surface where rumble strips removed","H3",{"v":0,"d":"0.0"},"","","","","15/11/2021 03:18:58",""]
[3143,12489,12,18,"12/96","","12/96","","Asphalt surface treatment","H4",{"v":0,"d":"0.0"},"","","","","08/11/2021 03:34:19",""]
[3144,12490,12,18,"12/96"," D","12/96. D","","30mm Surface treatment to roadways, etc, including bitumen spray prime coat to base course (PSMH)","m2",10,"","","","","08/11/2021 03:34:19",""]
[3145,12491,12,18,"12/96","","12/96","","Hot-pour asphalt sealant","H4",{"v":0,"d":"0.0"},"","","","","15/11/2021 01:13:52",""]
[3146,12492,12,18,"12/96"," E","12/96. E","","In joint between new and old asphalt surfaces","m",29,"","","","","08/11/2021 03:34:19",""]
[3147,10191,12,18,"12/96","","12/96","","TRAFFIC SIGNS","H2",{"v":0,"d":"0.0"},"","","","","14/10/2021 10:10:57",""]
[3148,10192,12,18,"12/96","","12/96","","Traffic signs (as per dwgs C5593-SITE-RDS-74 & 96)","H4",{"v":0,"d":"0.0"},"","","","","08/12/2021 02:16:07",""]
[3149,10194,12,18,"12/96"," F","12/96. F","","Take down and remove speed limit sign on and including timber pole","No",2,"","","","","30/10/2021 08:46:41",""]
[3150,10204,12,18,"12/96","","12/96","","Paintwork","H3",{"v":0,"d":"0.0"},"","","","","26/06/2023 01:13:27",""]
[3151,10205,12,18,"12/96","","12/96","","Prepare and apply two coats white reflective road marking paint on bituminous road surfacing, precast concrete paving blocks, etc.","H4",{"v":0,"d":"0.0"},"","","","","14/10/2021 03:56:18",""]
[3152,10206,12,18,"12/96"," G","12/96. G","","Traffic arrow 5 500 x 900mm wide extreme","No",1,"","","","","14/10/2021 03:56:18",""]
[3153,10207,12,18,"12/96"," H","12/96. H","","Traffic arrow 6 300 x 750mm wide extreme","No",1,"","","","","14/10/2021 03:56:18",""]
[3154,10208,12,18,"12/96"," I","12/96. I","","Traffic arrow 5 500 x 1 400mm wide extreme","No",1,"","","","","14/10/2021 03:56:18",""]
[3156,11057,12,19,"12/174","1","12/174.1","","Work to adjacent school","Page","12/5",0,"","","","26/10/2021 10:54:52",""]
[3157,9219,12,19,"12/174","2","12/174.2","","Site clearance and bulk earthworks","Page","12/8",0,"","","","26/08/2021 11:20:07",""]
[3158,9220,12,19,"12/174","3","12/174.3","","External water supplies","Page","12/13",0,"","","","26/08/2021 11:22:00",""]
[3159,9221,12,19,"12/174","4","12/174.4","","Reservoirs","Page","12/16",0,"","","","26/08/2021 11:22:26",""]
[3160,9237,12,19,"12/174","5","12/174.5","","Pump station and sump","Page","12/21",0,"","","","26/08/2021 11:24:51",""]
[3161,9222,12,19,"12/174","6","12/174.6","","External sewer drainage","Page","12/27",0,"","","","26/08/2021 11:22:34",""]
[3162,9238,12,19,"12/174","7","12/174.7","","Stormwater drainage","Page","12/33",0,"","","","26/08/2021 11:25:12",""]
[3163,9224,12,19,"12/174","8","12/174.8","","Stormwater harvesting tank & Oil interceptor","Page","12/38",0,"","","","26/08/2021 11:22:49",""]
[3164,9225,12,19,"12/174","9","12/174.9","","Water ponds","Page","12/42",0,"","","","26/08/2021 11:22:56",""]
[3165,9226,12,19,"12/174","10","12/174.10","","Symbolic and productive garden","Page","12/45",0,"","","","26/08/2021 11:23:04",""]
[3166,9227,12,19,"12/174","11","12/174.11","","Story telling pit","Page","12/46",0,"","","","26/08/2021 11:23:08",""]
[3167,9228,12,19,"12/174","12","12/174.12","","Walkways, ramps & steps","Page","12/51",0,"","","","26/08/2021 11:23:12",""]
[3168,9229,12,19,"12/174","13","12/174.13","","Parking, paving and roads","Page","12/57",0,"","","","26/08/2021 11:23:18",""]
[3169,9230,12,19,"12/174","14","12/174.14","","Retaining walls","Page","12/81",0,"","","","26/08/2021 11:23:24",""]
[3170,9231,12,19,"12/174","15","12/174.15","","Boundary walling and Security fencing","Page","12/87",0,"","","","26/08/2021 11:23:39",""]
[3171,9233,12,19,"12/174","16","12/174.16","","Work to burial site","Page","12/90",0,"","","","26/08/2021 11:23:55",""]
[3172,9234,12,19,"12/174","17","12/174.17","","BWICW","Page","12/94",0,"","","","26/08/2021 11:24:00",""]
[3173,9235,12,19,"12/174","18","12/174.18","","R331 Road upgrade","Page","12/97",0,"","","","26/08/2021 11:24:16",""]
[3174,2,13,1,"13/272","7","13/272.7","","EXTERNAL WORKS (Provisional)","Page","7/105",0,"","","","04/05/2012 03:45:35",""]
[3175,6696,13,1,"13/272","8","13/272.8","","R331 ROAD UPGRADE (Provisional)","Page","8/5",0,"","","","04/10/2012 04:33:47",""]
[3176,3909,13,1,"13/272","9","13/272.9","","LANDSCAPING (Provisional)","Page","9/47",0,"","","","20/08/2012 04:37:05",""]
[3177,9556,13,1,"13/272","10","13/272.10","","MATERIALS ON SITE - EXTERNAL WORKS (Provisional)","Page","10/7",0,"","","","13/09/2021 02:53:43",""]
[3178,1,13,1,"13/272","11","13/272.11","","PROVISIONAL SUMS","Page","11/10",0,"","","","04/05/2012 03:45:27",""]
[3179,9218,13,1,"13/272","12","13/272.12","","REMEDIAL WORK - EXTERNAL WORKS (Provisional)","Page","12/98",0,"","","","26/08/2021 11:19:32",""]
[3180,4066,13,1,"13/272","","13/272","","SUB-TOTAL","ST",{"v":0,"d":"0.00"},"","Sub Total","","","22/08/2012 05:44:46",""]

{"sheet":"Final Summary","index":7,"n_rows":47,"n_cols":9,"rows_kept":47,"merged":[[0,5,0,8],[6,1,6,5],[7,1,7,5],[10,1,10,5],[11,1,11,5],[12,1,12,5],[13,1,13,5],[14,1,14,5],[15,1,15,5],[18,1,18,5],[19,1,19,5],[20,1,20,5],[21,1,21,5],[22,1,22,5],[23,1,23,5],[24,1,24,5],[25,1,25,5],[26,1,26,5],[27,1,27,5],[28,1,28,5],[29,1,29,5],[30,1,30,5],[31,1,31,5],[32,1,32,5],[33,1,33,5],[34,1,34,5],[37,1,37,5],[38,1,38,5],[39,1,39,5],[40,1,40,5],[41,1,41,5],[42,1,42,5],[43,1,43,5],[44,1,44,5],[45,1,45,5]]}
[{"$nulls":5},"Sarah Bartmann: Centre of Remembrance ( Completion Contract)"]
[{"$nulls":8},"WCS 047427"]
[]
["Section ","FINAL SUMMMARY "]
["No.",{"$nulls":5},"Page ",null,"Amount"]
[]
[1,"PRELIMINARIES"]
[]
[2,"REMEDIAL WORK TO EXISTING BUILDINGS (Provisional)"]
[]
[3,"BUILDING WORKS - COMPLETION "]
[]
[4,"MECHANICAL INSTALLATION"]
[]
[5,"ELECTRICAL INSTALLATION"]
[]
[6,"MATERIALS ON SITE - BUILDING WORKS (Provisional)"]
[]
[7,"EXTERNAL WORKS (Provisional)"]
[]
[8,"R331 ROAD UPGRADE (Provisional)"]
[]
[9,"LANDSCAPING (Provisional)"]
[]
[10,"MATERIALS ON SITE - EXTERNAL WORKS (Provisional)"]
[]
[11,"PROVISIONAL SUMS"]
[]
[12,"REMEDIAL WORK - EXTERNAL WORKS (Provisional)"]
[]
[13,"SUB-TOTAL"]
[]
[null,"ADD VAT @15%"]
[]
[null,"SUB-TOTAL"]
[]
[null,"Less: Credit for old materials from the Demolition/ Alterations"]
[]
[]
[null,"Carried to Form of Offer and Acceptance",{"$nulls":4},"R",null,{"v":0,"d":"R 0.00"}]
[]
[]
[]
[]
[]
[]
[{"$nulls":4},"FS"]