{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["General","Equipment List","Technical Data","Safety Equipment"],"read":"whole","date_system":"1900"}

{"sheet":"General","index":0,"n_rows":29,"n_cols":2,"rows_kept":29,"merged":[[1,0,1,1]]}
["HELICOPTER SPECIFICATION SHEET"]
["Provide detailed description of item for each individual helicopter (number of helicopters will depend on helicopter capability as determined by the operator)"]
["Note: Fields provided with an asterisk * must be accompanied by the relevant documents or certificates"]
["Helicopter Detail, History and Documents","Helicopter 1"]
["Manufacturer "]
["Type "]
["Variant "]
["Date of Manufacture"]
["Serial Number"]
["Registration "]
["Ownership and Nationality "]
["Airframe Hours "]
["Hours until next major MPI "]
["Next MPI (Specify type)"]
["Engine Model"]
["Engine Hours "]
["Category (A or B) Certification "]
["Type Certificate (Number)* "]
["Aircraft CoR*"]
["Release to Service* "]
["Aircraft CoA* "]
["Lease agreements* "]
["Major modifications"]
["Approved Rotorcraft Flight Manual (State approval) "]
["Approved company specific SOPs and checklists for normal, abnormal and emergency procedures with human factor integration (State approval) "]
["STC Approvals "]
["Approved Minimum Equipment List (State authority) "]
["Available Date "]
["Current location of helicopter "]

{"sheet":"Equipment List","index":1,"n_rows":55,"n_cols":3,"rows_kept":55}
[]
["Radio Navigation, Communication and other Equipment (specify as applicable amount fitted, description and make and model)","Required                     Recommended","Helicopter 1"]
["DME (minimum 1)"]
["ADF (minimum 1)"]
["VOR / ILS (minimum 2)"]
["Weather radar with colour screen (min. scale 2.5nm)\n\n"]
["- with SART beacon detection"]
["GPS "]
["Fixed ELT"]
["Removeable ELT"]
["ADELT"]
["Cospas-Sarsat 406 MHz ELT"]
["Portable locator beacon for crew"]
["Search and rescue transponder (SART) beacon"]
["Underwater locator beacon"]
["Upper torso restraints, all seats (State number of attach points)"]
["Public Address System"]
["Push out windows (location)"]
["Emergency flotation gear"]
["Slinging equipment "]
["Rescue Hoist System (state lifting capacity, min 272 kg)"]
["Automatic flotation deployment system (AFDS)"]
["Helicopter Emergency Exit Lighting (HEEL)"]
["VHF Transceiver (2)"]
["HF Transceiver"]
["Marine FM VHF"]
["Mode C or S transponder (or equivalent)"]
["Instantaneous Vertical Speed Indicator"]
["EGPWS or TAWS"]
["TCAS"]
["Radio Altimeter"]
["Audio Alarm on Rad Alt"]
["Altitude Voice Alert Device (AVAD) "]
["Flight Hour Meter"]
["Flight Data Recorder (SACAA CARS has reference)"]
["Cockpit Voice Recorder (SACAA CARS has reference)"]
["Health Usage Monitoring System (HUMS), if approved by the regulatory authority for the helicopter type"]
["Other monitoring system (if not full HUMS)"]
["Vibration Health Monitoring (VHM) equipment, if approved by the regulatory authority for the helicopter type."]
["Helicopter Operations Monitoring Programme (HOMP) or equivalent"]
["Autopliot or AFCS (four axis recommended)"]
["Flight Director"]
["Flight Management System"]
["Emergency Exit Indicating System"]
["Satelite tracking system (with normal refresh rate 30 seconds or less)"]
[]
["Aircraft and Operator Requirements - General"]
["Two engines"]
["IFR Certified"]
["Two flight crew (on all contract flights) and hoist / sling operator in case of hoisting or slinging operations"]
["Wheeled / skid undercarriage"]
["Minumum passenger to be carried = 12"]
["Endurance 440 nms"]
[]
["Additional equipment: (Provide details)"]

{"sheet":"Technical Data","index":2,"n_rows":42,"n_cols":2,"rows_kept":42}
[]
["Technical Data","Helicopter 1"]
["Approved passenger seating capacity (offshore)"]
["Helicopter dimensions (Rotors turning)"]
["Helicopter D-Value and t-value"]
["Helicopter empty weight (offshore equipped)"]
["Approved type of operations"]
["Restrictions and prohibited manoeuvres"]
["Crew composition"]
["Approved MAUW"]
["Baggage compartment location"]
["Internal loads and floor loading limitations. Provide weight limitations and dimensions of baggage bay area"]
["Speed limitations"]
["Maximum taxi speed"]
["Maximum Vne (power on) "]
["Recommended cruise power / speeds"]
["Altitude limitations"]
["Class 2 Take-off and landing"]
["Enroute"]
["Wind limitations"]
["Max for start up and shutdown"]
["Max In-flight "]
["Take-off and landing"]
["Rear wind (landing and take-off)"]
["Side wind (landing and take-off)"]
["Performance (Where applicable assume helideck elevation 200 ft)"]
["Class 2 helideck MTOM (ISA and ISA +15°C)"]
["HIGE and HOGE OEI MCP Performance @ 25 OAT"]
["Maximum range at MTOM ISA +15°C, cruise @ ZP 3000 ft"]
["Maximum payload at maximum range, ISA +15°C, cruise @ ZP 3000 ft)"]
["HOGE performance, ISA +15°C"]
["Maximum TOM with external load"]
["Maximum undeslung load capacity"]
["Performance limitation with external load"]
["Fuel"]
["Total usable capacity"]
["Average fuel consumption (MTOW, ISA, cruise, ZP 3000 ft)"]
["Average fuel consumption (MTOW, ISA +15°C, cruise, ZP 3000 ft)"]
["Medical configuration and maximum number of stretchers"]
["Any Limitations with Rescue Hoist fitted"]
["Time taken to fit rescue hoist"]
["Time taken to change configuration from passenger to medical (stretchers)"]

{"sheet":"Safety Equipment","index":3,"n_rows":15,"n_cols":3,"rows_kept":15}
[]
["Safety Equipment","Required                     Recommended","Helicopter 1"]
[]
["First Aid Kits (Indicate number)"]
["Life Rafts (Indicate type, number, deployment system, capacity and onboard equipment)"]
["Fireman's axe (Indicate number and location)"]
["Hand Fire-Extinguishers (Indicate type and number)"]
["Crew Life Jackets (Include portable survival equipment included with jacket)"]
["Torches (Number)"]
["Helicopter Emergency Rapid Deployment System (HERDS) One kit required for contract"]
["Company specific and type specific passenger briefing cards (location)"]
["Safety briefing videos specific to the type on- and offshore"]
[]
[]
["Other (Specify):"]