{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["1757-BQ"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1757-BQ","index":0,"n_rows":2211,"n_cols":9,"rows_kept":2211,"merged":[[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8]],"flags":["formulas_cached_only"]}
["CDSIA TERMINAL CAPACITY EXPANSION"]
[]
["SECTION","BILL","PAGE NO","ITEM NO","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[]
[1,1,1,null,"SECTION NO. 1",null,0]
[]
[1,1,1,null,"PRELIMINARIES",null,0]
[]
[1,1,1,null,"BILL NO. 1",null,0]
[]
[1,1,1,null,"PRELIMINARIES",null,0]
[]
[1,1,1,null,"SECTION A : PREAMBLES FOR TRADES",null,0]
[]
[1,1,1,null,"The Model Preambles for Trades (2017 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claims arising from brevity of description of items fully described in the said Model Preambles will be entertained",null,0]
[]
[1,1,1,null,"SECTION B : NEC3 ENGINEERING AND CONSTRUCTION CONTRACT",null,0]
[]
[1,1,1,null,"The NEC3 Engineering and Construction Contract Option B, April 2013 in conjuction with the Contract Data shall be the applicable building agreement  The tenderer is deemed to have taken cognisance of the above mentioned  documents for the full intent and meaning of each clause.",null,0]
[]
[1,1,1,null,"NEC3 ENGINEERING AND CONSTRUCTION CONTRACT",null,0]
[]
[1,1,1,null,"GENERAL",null,0]
[]
[1,1,1," A","Clause 10  -  Action  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,1," B","Clause 11  -  Identified and defined terms  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," A","Clause 12  -  Interpretation and the law  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," B","Clause 13  -  Communication  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," C","Clause 14 - The Project Manager and the Supervisor  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," D","Clause 15 - Adding to the working areas  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," E","Clause 16 - Early warning  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," F","Clause 17 - Ambiguities and inconsistencies  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," G","Clause 18 - Illegal and impossible requirements  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2," H","Clause 19 - Prevention F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,2,null,"THE CONTRACTORS MAIN RESPONSIBILITIES",null,0]
[]
[1,1,2," I","Clause 20  -  Providing the works  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," A","Clause 21 - The Contractor's design  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," B","Clause 22 - Using the Contractor's design  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," C","Clause 23 - Design of equipment  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," D","Clause 24 - People  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," E","Clause 25 - Working with the Employer and others  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," F","Clause 26 - Subcontracting F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," G","Clause 27 - Other responsibilities  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3,null,"TIME",null,0]
[]
[1,1,3," H","Clause 30  -  Starting completion and key dates  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," I","Clause 31 - The programme  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,3," J","Clause 32 - Revising the programme  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," A","Clause 33 - Access to and use of the Site  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," B","Clause 34 - Instructions to stop or not to start work  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," C","Clause 35 - Take over  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," D","Clause 36 - Acceleration F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4,null,"TESTING AND DEFECTS",null,0]
[]
[1,1,4," E","Clause 40 - Tests and inspections  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," F","Clause 41 - Testing and inspection before delivery  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," G","Clause 42 - Searching for and notifying defects  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," H","Clause 43 - Correcting defects  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," I","Clause 44 - Accepting defects  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,4," J","Clause 45 - Uncorrected defects  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5,null,"PAYMENT",null,0]
[]
[1,1,5," A","Clause 50 - Assessing the amount due  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," B","Clause 51 - Payment  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," C","Clause 52 - Defined cost  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5,null,"COMPENSATION EVENTS",null,0]
[]
[1,1,5," D","Clause 60 - Compensation events  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," E","Clause 61 - Notifying compensation events  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," F","Clause 62 - Quotations for compensation events  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," G","Clause 63 - Assessing compensation events  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," H","Clause 64 - The Project Manager's assessments  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,5," I","Clause 65 - Implementing compensation events  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6,null,"TITLE",null,0]
[]
[1,1,6," A","Clause 70 - The Employer's title to plant and materials  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," B","Clause 71 - Marking equipment, plant and materials outside the working areas  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," C","Clause 72 - Removing equipment  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," D","Clause 73 - Objects and materials within the Site  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6,null,"RISKS AND INSURANCES",null,0]
[]
[1,1,6," E","Clause 80 - Employer's risks  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," F","Clause 81 - The Contractor's risks  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," G","Clause 82 - Repairs  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," H","Clause 83 - Indemnity  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,6," I","Clause 84 - Insurance cover  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7," A","Clause 85 - Insurance policies  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7," B","Clause 86 - If the Contractor does not insure  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7," C","Clause 87 - Insurance by the Employer  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7,null,"TERMINATION",null,0]
[]
[1,1,7," D","Clause 90 - Termination  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7," E","Clause 91 - Reasons for termination  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7," F","Clause 92 - Procedures on termination  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7," G","Clause 93 - Payment on termination  F:.....................  V:..................... T:......................","Item",1]
[]
[1,1,7,null,"CONTRACT DATA",null,0]
[]
[1,1,7,null,"Tenderers are referred to Part C1.2: Contract Data for variables pertaining to this contract  F:.....................  V:..................... T:......................",null,0]
[]
[1,1,7,null,"Community liason officer",null,0]
[]
[1,1,7," H","Budgetary allowance of R50 000.00 (Fifty Thousand Rand) for the utilisation of a community liaison officer as directed by the Project Manager","Item",1,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
[1,1,8,null,"Access permits",null,0]
[]
[1,1,8," A","Budgetary allowance of R100 000.00 (One Hundred Thousand Rand) for access permits as directed by the Project Manager","Item",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[2,1,9,null,"SECTION NO. 2",null,0]
[]
[2,1,9,null,"AREA A - EXISTING ABLUTIONS TO SECURITY CHECK-IN",null,0]
[]
[2,1,9,null,"BILL NO. 1",null,0]
[]
[2,1,9,null,"ALTERATIONS AND DEMOLITIONS",null,0]
[]
[2,1,9,null,"TEMPORARY SCREENS AND HOARDINGS",null,0]
[]
[2,1,9,null,"Take out from store and re-fix temporary hoarding sourced from areas C, D and E",null,0]
[]
[2,1,9," A","Re-install temporary hoarding (Take down and set aside to re-use elsewhere measured) 2400mm high with 22mm five-ply shutterboard including support framework and remove on completion and make good to any surfaces disturbed","m",71]
[]
[2,1,9,null,"Temporary hoardings",null,0]
[]
[2,1,9," B","Provide, erect and maintain temporary hoarding 2400mm high with 22mm five-ply shutterboard including support framework and remove on completion and make good to any surfaces disturbed","m",20]
[]
[2,1,9,null,"Dust proof hoarding",null,0]
[]
[2,1,9," C","Provide, erect and maintain temporary dust proof hoarding 5000mm high to underside of slab with 250 micron plastic sheeting taped to bottom and sides of slab, walls, floor and joints taped double sided with and including staining wires to both sides of sheeting at 300mm centres","m",91]
[]
[2,1,10,null,"Painting to public side of hoarding",null,0]
[]
[2,1,10," A","Clean down existing surfaces, prepare and two coats Dulux Pearlglo Water Based paint internally to one side of timber hoarding","m²",218]
[]
[2,1,10,null,"DEMOLITIONS",null,0]
[]
[2,1,10,null,"Demolish, break up or take out and remove",null,0]
[]
[2,1,10," B","Demolish existing wimpy kiosk overall size approximately 2,8 x 8m on plan x average 4m high, formed of drywall paritions, stiffener columns, ceiling support structure, etc. including disconnecting and stopping off all services, breaking up and removing all ceilings, windows, doors, joinery fittings, etc. and make good area to receive new finishes","No",1]
[]
[2,1,10,null,"Brickwork",null,0]
[]
[2,1,10," C","110mm Wall including finishes","m²",314]
[]
[2,1,10," D","230mm Wall including finishes","m²",277]
[]
[2,1,10,null,"Wall finishes",null,0]
[]
[2,1,10," E","Ceramic tiles to plastered walls","m²",43]
[]
[2,1,10," F","Ceramic tiles to columns","m²",83]
[]
[2,1,10," G","50mm Timber dado","m",56]
[]
[2,1,10,null,"Floor finishes",null,0]
[]
[2,1,10," H","Floor tiles to screeded floors and prepare to receive new floor finish","m²",325]
[]
[2,1,11,null,"Ceilings",null,0]
[]
[2,1,11," A","Suspended ceiling and bulkheads with and including suspension grid, hangers, etc","m²",112]
[]
[2,1,11," B","Rhinoboard flush ceiling with cornices Including suspension grid, hangers, etc","m²",121]
[]
[2,1,11,null,"Doors",null,0]
[]
[2,1,11," C","Timber door size 900 x 2100mm high complete with frame, ironmongery, etc","No",18]
[]
[2,1,11," D","Glazed aluminium door size 900 x 2100mm high complete with frame, ironmongery, etc","No",1]
[]
[2,1,11,null,"Windows",null,0]
[]
[2,1,11," E","Glazed steel window size 7500 x 900mm high","No",2]
[]
[2,1,11,null,"Joinery fittings",null,0]
[]
[2,1,11," F","Granite vanity counter top 600mm wide","m",6]
[]
[2,1,11,null,"Sundries",null,0]
[]
[2,1,11," G","Toilet roll holder plugged to wall","No",14]
[]
[2,1,11," H","Paraplegic grab rails","No",4]
[]
[2,1,11," I","Mirror size 3000 x 800mm high","No",2]
[]
[2,1,11,null,"Take out and remove piping, sanitary fittings, etc. including disconnecting  piping  from fittings  and  making good floor and wall finishes (making good tiling and paintwork elsewhere)",null,0]
[]
[2,1,11," J","WC suite complete with flush valves including disconnecting and stopping off water supply and waste pipes","No",14]
[]
[2,1,12," A","Wash hand basin complete with mixer, waste, etc. including disconnecting and stopping off water supply and waste pipes","No",10]
[]
[2,1,12," B","Urinal complete with flush valve including disconnecting and stopping off water supply and waste pipes","No",6]
[]
[2,1,12," C","15mm Copper piping including fittings and brackets.","m",120]
[]
[2,1,12," D","22mm Copper piping including fittings and brackets.","m",90]
[]
[2,1,12," E","28mm Copper piping including fittings and brackets.","m",60]
[]
[2,1,12," F","40mm PVC piping including fittings and brackets.","m",32]
[]
[2,1,12," G","50mm PVC piping including fittings and brackets.","m",64]
[]
[2,1,12," H","110mm PVC piping including fittings and brackets.","m",94]
[]
[2,1,12,null,"Take off and set aside for re-use or hand over to Employer",null,0]
[]
[2,1,12," I","Bumper rails 200mm high fixed to top of concrete surface bed","m",9]
[]
[2,1,12," J","Handrails 900mm high fixed to top of concrete surface bed","m",35]
[]
[2,1,12," K","Glazed aluminium double door size 1700 x 2100mm high complete with frame, ironmongery, etc","No",1]
[]
[2,1,12,null,"Take out from store and re-fix",null,0]
[]
[2,1,12," L","Glazed aluminium double door size 1700 x 2100mm high complete with frame, ironmongery, etc","No",1]
[]
[2,1,13,null,"Build up, alter or break new openings in existing walls",null,0]
[]
[2,1,13," A","Break through existing 270mm hollow wall for and form new door opening size 1700 x 2100mm, form new lintol over, built cavity solid to reveals and make good smooth plaster to walls and reveals on both sides and screed to threshold","No",1]
[]
[2,1,13,null,"Making good to existing surfaces",null,0]
[]
[2,1,13," B","Smooth plaster to walls where 110mm wall removed","m",15]
[]
[2,1,13," C","Smooth plaster to walls where 230mm wall removed","m",35]
[]
[2,1,13," D","Screed to floor where 110mm wall removed","m",63]
[]
[2,1,13," E","Screed to floor where 230mm wall removed","m",56]
[]
[2,2,14,null,"BILL NO. 2",null,0]
[]
[2,2,14,null,"REINFORCED CONCRETE STRUCTURE",null,0]
[]
[2,2,14,null,"CONCRETE",null,0]
[]
[2,2,14,null,"Test Cubes",null,0]
[]
[2,2,14," A","Set of three concrete strength cubes each size 150 x 150 x 150mm, send to an independent laboratory for test crushing including all charges ","Sets",1]
[]
[2,2,14,null,"Reinforced concrete 25MPa/19mm stone",null,0]
[]
[2,2,14," B","Topping, ribs and solid margins to composite rib and hollow block slabs including striking off and curing","m³",3]
[]
[2,2,14," C","Plinths","m³",3]
[]
[2,2,14,null,"Sundries",null,0]
[]
[2,2,14," D","Finish top of concrete plinth to a steel trowel finish in one operation, including any additional mortar required","m²",15]
[]
[2,2,14," E","16mm Diameter dowel rods 300mm long including drilling 150mm deep into existing concrete surface bed and fixed with Hilti HIT - RE500 epoxy grout","No",40]
[]
[2,2,14," F","150 x 150 x 10mm Thick galvanised steel angle fixed to concrete slab with M16 Hilti HIT-V rods 150mm long with HIT-RE 500 epoxy adhesive at 1000mm centres","m",33]
[]
[2,2,15,null,"COMPOSITE SUSPENDED RIB AND HOLLOW BLOCK SLAB CONSTRUCTION",null,0]
[]
[2,2,15," A","250 x 50mm Light rib precast concrete plank in varying lengths and hoist and place in position average 3,5m high above floor level with ends bearing on steel support angle (main reinforcement to planks elsewhere measured)","m",35]
[]
[2,2,15," B","Lightrib precast concrete hollow block type FT90 size 500 x 200 x 90mm overall and place in position between precast concrete planks","No",120]
[]
[2,2,15," C","76 x 152mm Timber runner to soffit of precast concrete planks and horsing up not exceeding 3,5m high including propping at not exceeding 1500mm centres","m",10]
[]
[2,2,15," D","12mm Diameter high tensile steel reinforcement to precast concrete planks","t",0.17]
[]
[2,2,15,null,"ROUGH FORMWORK (DEGREE OF ACCURACY II)",null,0]
[]
[2,2,15,null,"Rough formwork to sides, edges, risers, etc.",null,0]
[]
[2,2,15," E","Plinths","m²",4]
[]
[2,2,15,null,"Extra on rough formwork for blocking in, boxing in or out, etc. including angles, stop ends, etc. to form",null,0]
[]
[2,2,15," F","25 x 25mm Chamfer to edge of concrete","m",26]
[]
[2,2,15,null,"REINFORCEMENT",null,0]
[]
[2,2,15,null,"Mesh reinforcement",null,0]
[]
[2,2,15," G","Reference 245 standard square fabric reinforcement in concrete slab","m²",21]
[]
[2,2,16,null,"High tensile steel reinforcement",null,0]
[]
[2,2,16," A","12mm Diameter","t",0.3]
[]
[2,3,17,null,"BILL NO. 3",null,0]
[]
[2,3,17,null,"BRICK STRUCTURE",null,0]
[]
[2,3,17,null,"BRICKWORK",null,0]
[]
[2,3,17,null,"Brickwork in burnt clay NFP bricks in Class II mortar",null,0]
[]
[2,3,17," A","230mm Wall","m²",19]
[]
[2,3,17," B","270mm Hollow wall formed of two 110mm skins with cavity between including wire ties","m²",25]
[]
[2,3,17," C","270mm Hollow wall circular on plan formed of two 110mm skins with cavity between including wire ties","m²",18]
[]
[2,3,17,null,"Sundries",null,0]
[]
[2,3,17," D","75mm Wide galvanised brick reinforcement","m",344]
[]
[2,3,17," E","150mm Wide galvanised brick reinforcement","m",76]
[]
[2,3,17," F","70 x 102mm Prestressed concrete lintol not exceeding 3m long cut to lengths with both ends built into brickwork including propping ","m",3]
[]
[2,3,17," G","70 x 152mm Prestressed concrete lintol not exceeding 3m long cut to lengths with both ends built into brickwork including propping ","m",3]
[]
[2,3,17," H","1,6mm Galvanised hoop iron tie 32mm wide and 450mm girth, one end gun nailed to existing brick wall and other end built into new brickwork to bond new brickwork to existing","No",160]
[]
[2,3,18,null,"Movement joints, etc.",null,0]
[]
[2,3,18," A","10mm Expanded polyethylene expansion joint filler fixed vertically between concrete and brick surfaces not exceeding 300mm wide","m",30]
[]
[2,3,18,null,"WATERPROOFING",null,0]
[]
[2,3,18," B","375 Micron polyethylene sheeting complying with SANS 952 Type C as dampproof course on walls, reveals, etc.","m²",3]
[]
[2,3,18,null,"Pointing",null,0]
[]
[2,3,18," C","Rake out 10mm expanded polyethylene joint filler for a depth of 10mm, prime and point with polysulphide sealant","m",59]
[]
[2,4,19,null,"BILL NO. 4",null,0]
[]
[2,4,19,null,"ROOF COVERINGS",null,0]
[]
[2,4,19,null,"WATERPROOFING",null,0]
[]
[2,4,19,null,"Note:  The Contractor will be required to provide a ten year written guarantee in respect of this waterproofing",null,0]
[]
[2,4,19,null,"Derbigum waterproofing comprising priming surface of sub strata and 4mm thick Derbigum SP waterproofing laid with 75mm wide side laps and 100mm wide end laps with waterproofing sealed to screed and at laps by torch-on fusion",null,0]
[]
[2,4,19," A","Horizontal surfaces of screed to falls including dressing to turn-ups and turn-downs not exceeding 300mm girth","m²",48]
[]
[2,4,19," B","Two coats bituminous based aluminium paint on derbigum waterproofing ","m²",48]
[]
[2,4,19," C","150mm Wide glass fibre/polyester membrane flashing at junction of waterproofing and wall surface","m",54]
[]
[2,4,19," D","Dress waterproofing into rainwater outlet and seal","No",1]
[]
[2,4,19,null,"IN SITU FINISHES",null,0]
[]
[2,4,19,null,"1:3 Cement mortar screed finished smooth with a steel trowel on concrete",null,0]
[]
[2,4,19," E","Average 60mm thick to concrete slab to falls and cross falls","m²",34]
[]
[2,4,19," F","75 x 75mm Triangular fillet at junction of vertical and horizontal surfaces","m",54]
[]
[2,4,20,null,"PLUMBING",null,0]
[]
[2,4,20,null,"Hot dip galvanised rainwater goods and fittings",null,0]
[]
[2,4,20," A","1,6mm Thick VHV box gutter size 200 x 200 x 200mm with beaded edges and all joints soldered and double rivetted fixed to falls on and including gutter brackets fixed to edge of concrete slab","m",2]
[]
[2,4,20," B","Extra for stop end","No",2]
[]
[2,4,20," C","Extra for outlet with nozzle for 110mm rainwater pipe","No",1]
[]
[2,4,20,null,"uPVC Class 9 pressure pipes complying with SANS 966 as rainwater pipes",null,0]
[]
[2,4,20," D","110mm Pipe fixed to wall with aluminium alloy downpipe clips spaced at not exceeding 1,5m centres and plugged to wall","m",6]
[]
[2,4,20," E","Extra for bend","No",2]
[]
[2,4,20," F","Extra for shoe","No",1]
[]
[2,4,20,null,"Rainwater outlets",null,0]
[]
[2,4,20," G","100mm Saint Gobain fulbore centre bolt two way roof outlet code: 03540 and joint to uPVC pipe including adaptor and cast into concrete","No",1]
[]
[2,4,20,null,"BUILDERS WORK INCLUDING MAKING GOOD",null,0]
[]
[2,4,20,null,"Core drilling of hole for pipe not exceeding 200mm diameter",null,0]
[]
[2,4,20," H","600mm Reinforced concrete slab, beam, wall, etc","No",2]
[]
[2,5,21,null,"BILL NO. 5",null,0]
[]
[2,5,21,null,"INTERNAL WALL FINISHES",null,0]
[]
[2,5,21,null,"IN SITU FINISHES",null,0]
[]
[2,5,21,null,"One coat internal 1:5 cement plaster finished smooth with a steel trowel",null,0]
[]
[2,5,21,null,"On brickwork (small part on flush concrete)",null,0]
[]
[2,5,21," A","Walls","m²",128]
[]
[2,5,21," B","Existing walls","m²",43]
[]
[2,5,21," C","Walls and reveals in narrow widths not exceeding 300mm wide","m²",2]
[]
[2,5,21,null,"On concrete",null,0]
[]
[2,5,21," D","Existing columns","m²",83]
[]
[2,5,21,null,"TIMBER WALL CLADDING",null,0]
[]
[2,5,21,null,"The following in OWA Idealux FL wall cladding",null,0]
[]
[2,5,21," E","Acoustic timber wall cladding formed of Idealux FL solid wood panels size 600 x 2400mm high complete with polyester fibre backing and fixed to wall with fixing adhesive and screws all in accordance with manufacturers recommendations","m²",44]
[]
[2,5,21," F","Acoustic timber wall cladding circular on plan formed of Idealux FL solid wood panels size 600 x 2400mm high complete with polyester fibre backing and fixed to wall with fixing adhesive and screws all in accordance with manufacturers recommendations","m²",15]
[]
[2,5,22," A","Extra for trimming for and forming door opening size 900 x 2100mm (door and frame elsewhere measured)","No",1]
[]
[2,5,22," B","Extra for trimming for and forming door opening size 1700 x 2100mm (door and frame elsewhere measured)","No",1]
[]
[2,5,22,null,"METAL WORK",null,0]
[]
[2,5,22,null,"Sundries",null,0]
[]
[2,5,22," C","50 x 50mm Kirk stainless steel corner protector Code SCP500 fixed to corners of columns","m",60]
[]
[2,6,23,null,"BILL NO. 6",null,0]
[]
[2,6,23,null,"FLOOR FINISHES",null,0]
[]
[2,6,23,null,"IN SITU FINISHES",null,0]
[]
[2,6,23,null,"Screed leveller finished smooth with a steel trowel to receive floor tiles",null,0]
[]
[2,6,23," A","Pavelite screed leveller on existing screeded surfaces to receive new floor coverings","m²",325]
[]
[2,6,23,null,"TILING",null,0]
[]
[2,6,23,null,"Supply only porcelain floor tiles PC R400.00 (Four Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[2,6,23," B","Floors","m²",6]
[]
[2,6,23," C","100mm High skirting","m",11]
[]
[2,6,23,null,"Take delivery, store until required and fix 600 x 600mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[2,6,23," D","Floors","m²",6]
[]
[2,6,23," E","100mm High skirting","m",11]
[]
[2,6,23,null,"Supply only porcelain floor tiles PC R500.00 (Five Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[2,6,23," F","Floors","m²",319]
[]
[2,6,23," G","100mm High skirting","m",60]
[]
[2,6,24,null,"Take delivery, store until required and fix 600 x 1200mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[2,6,24," A","Floors","m²",319]
[]
[2,6,24," B","100mm High skirting","m",60]
[]
[2,6,24,null,"Sundries",null,0]
[]
[2,6,24," C","Kirk aluminium 10mm straight edge trim Code ASE100 to top of skirtings","m",71]
[]
[2,6,24," D","Kirk stainless steel 15mm straight edge trim Code SSE150 between tile floor finishes","m",56]
[]
[2,6,24," E","Kirk aluminium 15mm movement joint Code AMJ150 between tile floor finishes","m",181]
[]
[2,7,25,null,"BILL NO. 7",null,0]
[]
[2,7,25,null,"CEILINGS",null,0]
[]
[2,7,25,null,"SUSPENDED NON-METAL CEILINGS",null,0]
[]
[2,7,25,null,"Rhinoboard flush plastered ceilings",null,0]
[]
[2,7,25," A","Gyproc plasterboard screw up flush suspended ceiling formed of concealed suspension system with galvanised steel angle section hangers and 9.5mm Rhinoboard flush ceiling complying with SANS 266 with joints between boards covered for 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m²",232]
[]
[2,7,25," B","Trim for and form trap door size 600 x 600mm in clear formed of 38 x 50mm Sawn SA pine frame covered on one side with 9.5mm gypsum plasterboard and set on and including 19 x 32mm Wrot SA pine bearer all round opening","No",4]
[]
[2,7,25," C","Cut and fit ceiling around 150mm diameter downlighter","No",20]
[]
[2,7,25," D","Cut and fit ceiling around 100mm diameter smoke detector","No",10]
[]
[2,7,25,null,"Rhinoboard bulkheads, etc. ",null,0]
[]
[2,7,25," E","Vertical bulkhead 200mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m",58]
[]
[2,7,26," A","Ditto but circular on plan","m",8]
[]
[2,7,26," B","Vertical bulkhead 240mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m",50]
[]
[2,7,26," C","Recessed rectangular shaped boxed bulkhead 1660mm girth, overall size 600mm wide x 300mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead detail 01 on drawing no. A-(54)200)","m",56]
[]
[2,7,26," D","Ditto but circular on plan","m",8]
[]
[2,7,26,null,"Suspended ceilings ",null,0]
[]
[2,7,26," E","Suspended ceiling formed of Donn exposed tee system with 25mm wide tees with aluminium pre-painted low sheen satin exposed tees, built in with and including 12,5mm Gyprex gypsum vinyl faced ceiling tiles size 1200 x 600mm complete with holding down clips and suspended not exceeding 1000mm below soffit of slab including any necessary supplementary support system","m²",6]
[]
[2,7,26," F","Extra for trimming around recessed light fittings size 600 x 600mm","No",2]
[]
[2,7,27,null,"Cornices",null,0]
[]
[2,7,27," A","Sigma 50 x 50mm white epoxy coated plaster trim plugged to wall (Trim type 3)","m",79]
[]
[2,7,27," B","Capco Trim-Tex (code: 4010) corner bead to exposed corners of bulkheads","m",303]
[]
[2,7,27,null,"REPAIRS TO EXISTING CEILING",null,0]
[]
[2,7,27," C","Budgetary allowance of R10 000.00 (Ten Thousand Rand) for repairs to existing ceiling as directed by the Project Manager","Item",1,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[2,8,28,null,"BILL NO. 8",null,0]
[]
[2,8,28,null,"DOORS",null,0]
[]
[2,8,28,null,"JOINERY",null,0]
[]
[2,8,28,null,"Semi-solid flush doors complying with SANS 545 with two hardwood concealed edges",null,0]
[]
[2,8,28," A","40 x 813 x 2032mm Horizontal grooved single door","No",1]
[]
[2,8,28," B","Cut opening size 500 x 560mm in semi-solid flush door for ventilator grille (elsewhere measured) ","No",1]
[]
[2,8,28,null,"Solid core flush doors complying with SANS 545 with two hardwood concealed edges",null,0]
[]
[2,8,28," C","40 x 813 x 2032mm Door with hardboard facing on both sides","No",1]
[]
[2,8,28,null,"IRONMONGERY",null,0]
[]
[2,8,28,null,"Hinges, etc",null,0]
[]
[2,8,28," D","DORMAKABA DBB-SS-009 102 x 75 x 3mm two ball bearing butt hinge ","Pairs",1.5]
[]
[2,8,28," E","DORMAKABA 1040 100mm aluminium sinkless hinges","Pairs",1.5]
[]
[2,8,28,null,"Locks, etc",null,0]
[]
[2,8,28," F","DORMAKABA D036S SS cylinder sash lock","No",2]
[]
[2,8,28," G","DORMAKABA DCE-002 SS round cylinder escutcheon","Pairs",2]
[]
[2,8,28," H","DORMAKABA DKC056501 KD 65mm five pin euro-profile knob cylinder","No",2]
[]
[2,8,29,null,"Door furniture, etc.",null,0]
[]
[2,8,29," A","DORMAKABA TH126 LATCH SS lever handle set with latch","Sets",2]
[]
[2,8,29,null,"Door closer, etc.",null,0]
[]
[2,8,29," B","DORMAKABA TS68-SL EN 2/3/4 rack and pinion door closer with non hold open scissor arm","Sets",2]
[]
[2,8,29,null,"ALUMINIUM WORK",null,0]
[]
[2,8,29,null,"Donn 89mm natural anodised aluminium door frame with full height timber insert including setting up and building in",null,0]
[]
[2,8,29," C","Aluminium door frame for timber door (door elsewhere measured) size 813 x 2032mm high","No",2]
[]
[2,8,29,null,"Aluminium louvre units",null,0]
[]
[2,8,29," D","Natural anodised aluminium louvre grille size 500 x 560mm formed of outer frame and horizontal fixed louvre blades and fix in opening (opening elsewhere measured) in door","No",1]
[]
[2,9,30,null,"BILL NO. 9",null,0]
[]
[2,9,30,null,"SUNDRIES",null,0]
[]
[2,9,30,null,"BALUSTRADING AND HANDRAILS",null,0]
[]
[2,9,30,null,"Stainless Steel grade 316 balustrades to passenger queuing area",null,0]
[]
[2,9,30," A","Stainless steel balustrade 900mm high formed of 50mm diameter x 2.5mm thick circular hollow section handrail with 50mm diameter x 2.5mm thick circular hollow section posts 800mm high at 900mm centres, the posts connected to the handrails with 10mm diameter x 50mm long solid pins welded to underside of handrails and top of closer piece of post including 75mm diameter x mm thick base plates, the base plates each two times drilled and bolted to concrete floor with and including 22mm Diameter x 170mm long threaded rod chemically fixed with Fischer FIS V Plus injection mortar including mortice in concrete; the balustrade filled in with one 16mm diameter solid bar horizontal rods fitted through holes drilled in posts and welded to same all in accordance with drawing no. A-(12)2001 rev1","m",100]
[]
[2,9,30," B","Extra for 90° bend","No",4]
[]
[2,9,30," C","Extra for plugged and welded end","No",22]
[]
[2,9,30," D","Extra for pedestrian access gate size 1000 x 900mm high formed of 50mm diameter x 2.5mm thick circular hollow section frame fixed to 50mm diameter x 2.5mm thick circular hollow section posts 900mm high with and including hinges all in accordance with drawing no. A-(12)2001 rev1","No",4]
[]
[2,9,31,null,"BUMPER RAILS",null,0]
[]
[2,9,31,null,"Stainless Steel grade 316 bump rail",null,0]
[]
[2,9,31," A","Stainless steel bump rail 125mm high formed of 48mm diameter x 5,3mm thick circular hollow section bump rail with 43mm diameter x 4mm thick circular hollow section floor posts 100mm high at max 2000mm centres, the posts welded to the underside of the bump rail including 90mm diameter x 6mm thick base plates welded to bottom of posts with base plates each two times drilled and fixed to concrete floor with and including M10 chemical anchors including mortices in concrete all in accordance with drawing no. A-(12)2001 rev1","No",12]
[]
[2,9,31," B","Ditto but circular on plan","No",4]
[]
[2,9,31," C","Extra for 90° bend","No",2]
[]
[2,9,31," D","Extra for end supports","No",6]
[]
[2,9,31,null,"SIGNAGE",null,0]
[]
[2,9,31,null,"Corporate signage",null,0]
[]
[2,9,31," E","Subcontract allowance of R30 000.00 (Thirty Thousand Rand) net for corporate signage by a Subcontractor approved by the Project Manager","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"}]
[]
[2,9,31," F","Profit","%IT"]
[]
[2,9,31," G","Attendance","%IT"]
[]
[2,9,32,null,"Fire signage",null,0]
[]
[2,9,32," A","Subcontract allowance of R10 000.00 (Ten Thousand Rand) net for fire signage by a Subcontractor approved by the Project Manager","Item",1,{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[2,9,32," B","Profit","%IT"]
[]
[2,9,32," C","Attendance","%IT"]
[]
[2,10,33,null,"BILL NO. 10",null,0]
[]
[2,10,33,null,"PLUMBING AND DRAINAGE",null,0]
[]
[2,10,33,null,"WATER SUPPLIES",null,0]
[]
[2,10,33,null,"uPVC Class 12 pressure water supply piping with integral rubber ring joints in accordance with SANS 966",null,0]
[]
[2,10,33," A","42mm Pipe and fixing to walls, chases, roofs etc. including labour bends","m",28]
[]
[2,10,33,null,"Extra over uPVC water supply piping for the following uPVC fittings with integral rubber ring joints",null,0]
[]
[2,10,33," B","42mm Bend","No",10]
[]
[2,10,33," C","42mm Tee","No",2]
[]
[2,10,33,null,"Copper water supply pipes complying with SANS 460 Class II with brass compression couplings",null,0]
[]
[2,10,33," D","15mm Pipe and fixing to walls, chases, roofs etc. including labour bends","m",45]
[]
[2,10,33," E","22mm Ditto","m",60]
[]
[2,10,33," F","28mm Ditto","m",21]
[]
[2,10,33," G","35mm Ditto","m",16]
[]
[2,10,33,null,"Extra over copper pipes for the following brass compression fittings",null,0]
[]
[2,10,33," H","15mm Elbow, tee, connector, etc.","No",60]
[]
[2,10,33," I","22mm Elbow, tee, connector, etc.","No",60]
[]
[2,10,33," J","28mm Elbow, tee, connector, etc.","No",30]
[]
[2,10,34," A","35mm Bend","No",15]
[]
[2,10,34," B","35mm Tee or reducing tee","No",15]
[]
[2,10,34,null,"Valves, etc. complying with SANS 226 and connections to copper and multi layer pipes including connectors",null,0]
[]
[2,10,34," C","22mm Cobra lever type ball-o-stop including adaptors to copper pipe","No",2]
[]
[2,10,34," D","28mm Cobra lever type ball-o-stop including adaptors to copper pipe","No",2]
[]
[2,10,34," E","35mm Cobra lever type ball-o-stop including adaptors to copper pipe","No",2]
[]
[2,10,34,null,"Pump to water tank",null,0]
[]
[2,10,34," F","DAB Jetcom 132M 1KW self-priming centrifugal pump complete with pressure control switch fixed in position","No",1]
[]
[2,10,34,null,"SANITARY PLUMBING",null,0]
[]
[2,10,34,null,"Rigid PVC waste, soil and vent pipes complying with SANS 967",null,0]
[]
[2,10,34," G","40mm Pipe and fixing to walls, chases, roofs etc.","m",39]
[]
[2,10,34," H","50mm Pipe and fixing to walls, chases, roofs, etc.","m",47]
[]
[2,10,34," I","110mm Pipe and fixing to walls, chases, roofs, etc.","m",62]
[]
[2,10,34,null,"Extra over PVC pipes for",null,0]
[]
[2,10,34," J","110mm Vent cowl","No",2]
[]
[2,10,34," K","110mm End cap","No",2]
[]
[2,10,34," L","50 x 40mm Reducer","No",4]
[]
[2,10,35," A","40mm Bend","No",8]
[]
[2,10,35," B","50mm Bend","No",8]
[]
[2,10,35," C","110mm Bend","No",2]
[]
[2,10,35," D","40mm Inspection eye bend","No",16]
[]
[2,10,35," E","50mm Inspection eye bend","No",16]
[]
[2,10,35," F","110mm Inspection eye bend","No",14]
[]
[2,10,35," G","40mm Junction","No",8]
[]
[2,10,35," H","50mm Junction","No",8]
[]
[2,10,35," I","40mm Inspection eye junction","No",16]
[]
[2,10,35," J","50mm Inspection eye junction","No",16]
[]
[2,10,35," K","110mm Inspection eye junction","No",14]
[]
[2,10,35," L","110mm Inspection eye reducing junction","No",8]
[]
[2,10,35," M","110mm Inspection eye double junction","No",4]
[]
[2,10,35," N","110mm Inspection eye double reducing junction","No",4]
[]
[2,10,35,null,"Inspection chambers",null,0]
[]
[2,10,35," O","Budgetary allowance of R20 000.00 (Twenty Thousand Rand) for altering existing manhole as directed by the Project Manager","Item",1,{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[2,10,35,null,"TESTING",null,0]
[]
[2,10,35," P","Test the plumbing and drainage installation","Item",1]
[]
[2,11,36,null,"BILL NO. 11",null,0]
[]
[2,11,36,null,"PAINTING",null,0]
[]
[2,11,36,null,"ON PLASTER ETC.",null,0]
[]
[2,11,36,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[2,11,36," A","Plastered walls (\"Pastel\" colour group)","m²",213]
[]
[2,11,36,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[2,11,36," B","Plastered rhinoboard ceiling (\"White\" colour group)","m²",232]
[]
[2,11,36," C","Plastered bulkheads (\"White\" colour group)","m²",131]
[]
[2,11,36,null,"ON WOOD",null,0]
[]
[2,11,36,null,"Prepare, one coat Dulux Primer for Wood (Code: D33), one coat Dulux Universal Undercoat (Code: D34) and two coats Dulux Pearlglo Water Based (Code:  D40) paint internally",null,0]
[]
[2,11,36," D","Flush doors (\"Deep\" colour group)","m²",7]
[]
[2,11,37,null,"REDECORATION",null,0]
[]
[2,11,37,null,"The term \"clean down\" shall mean that existing painted surfaces shall be treated in the following manner prior to applying the paint required:  Existing PVA finished plaster surfaces shall be rubbed down ready to receive new PVA but where the PVA is in a poor condition, or otherwise unsuitable to receive further coats, or where the plaster is to receive a finish other than PVA, the old PVA shall be completely removed by wetting and scraping, and the surfaces filled where necessary and rubbed down ready to receive the new finishings",null,0]
[]
[2,11,37,null,"Existing painted plaster surfaces shall be washed down, filled where necessary, spot primed and rubbed down ready to receive new paint.  Existing painted metal surfaces shall be thoroughly rubbed and cleaned down before repainting, but where paint film has blistered or broken down, the paint must be completely removed down to the bare metal.",null,0]
[]
[2,11,37,null,"After cleaning off rust on metalwork, those portions so affected shall be treated with an approved rust inhibitor.  Existing woodwork previously painted shall be washed and rubbed down before repainting, but where the old paint must be completely removed back to the bare surface by the use of a blow lamp or paint removed, and the woodwork knotted, primed, stopped and rubbed down ready to receive new paint.",null,0]
[]
[2,11,38,null,"Care must be taken in burning off old paint not to char or otherwise damage the woodwork, and paint removers used must be free from soda or other caustic substances.  Existing oiled or varnished wood shall be scraped as may be necessary, stopped with tinted stopping and rubbed down and existing woodwork shall be cleaned and similarly stopped and rubbed down.",null,0]
[]
[2,11,38,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[2,11,38," A","Plastered walls (\"Pastel\" colour group)","m²",241]
[]
[{"$nulls":4},"SECTIONAL SUMMARY",null,0]
[]
[null,null,39,1,"ALTERATIONS AND DEMOLITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,2,"REINFORCED CONCRETE STRUCTURE",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,3,"BRICK STRUCTURE",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,4,"ROOFS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,5,"INTERNAL FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,6,"FLOOR FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,7,"CEILINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,8,"DOORS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,9,"SUNDRIES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,10,"PLUMBING AND DRAINAGE",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,39,11,"PAINTING",null,null,{"v":0,"d":"0.00"}]
[]
[3,1,40,null,"SECTION NO. 3",null,0]
[]
[3,1,40,null,"AREA B - INCREASE PASSENGER CIRCULATION",null,0]
[]
[3,1,40,null,"BILL NO. 1",null,0]
[]
[3,1,40,null,"ALTERATIONS AND DEMOLITIONS",null,0]
[]
[3,1,40,null,"TEMPORARY SCREENS AND HOARDINGS",null,0]
[]
[3,1,40,null,"Take out from store and re-fix temporary hoarding sourced from areas C, D and E",null,0]
[]
[3,1,40," A","Re-install temporary hoarding (Take down and set aside to re-use elsewhere measured) 2400mm high with 22mm five-ply shutterboard including support framework and remove on completion and make good to any surfaces disturbed","m",48]
[]
[3,1,40,null,"Dust proof hoarding",null,0]
[]
[3,1,40," B","Provide, erect and maintain temporary dust proof hoarding 5000mm high to underside of slab with 250 micron plastic sheeting taped to bottom and sides of slab, walls, floor and joints taped double sided with and including staining wires to both sides of sheeting at 300mm centres","m",48]
[]
[3,1,40,null,"Painting to public side of hoarding",null,0]
[]
[3,1,40," C","Clean down existing surfaces, prepare and two coats Dulux Pearlglo Water Based paint internally to one side of timber hoarding","m²",115]
[]
[3,1,41,null,"DEMOLITIONS",null,0]
[]
[3,1,41,null,"Demolish, break up or take out and remove",null,0]
[]
[3,1,41,null,"Brickwork",null,0]
[]
[3,1,41," A","110mm Wall including finishes","m²",10]
[]
[3,1,41," B","230mm Wall including finishes","m²",50]
[]
[3,1,41,null,"Drywall partitions",null,0]
[]
[3,1,41," C","Drywall partition 4000mm high including finishes","m",51]
[]
[3,1,41,null,"Wall finishes",null,0]
[]
[3,1,41," D","Ceramic tiles to plastered walls","m²",2]
[]
[3,1,41,null,"Floor finishes",null,0]
[]
[3,1,41," E","Floor tiles to screeded floors and prepare to receive new floor finish","m²",9]
[]
[3,1,41," F","Carpet tiles to screeded floors and prepare to receive new floor finish","m²",91]
[]
[3,1,41," G","Timber skirting","m",57]
[]
[3,1,41,null,"Ceilings",null,0]
[]
[3,1,41," H","Suspended ceiling and bulkheads with and including suspension grid, hangers, etc","m²",127]
[]
[3,1,41,null,"Doors",null,0]
[]
[3,1,41," I","Glazed aluminium door size 900 x 2100mm high complete with frame, ironmongery, etc","No",6]
[]
[3,1,41," J","Glazed aluminium window size 3250 x 1500mm high","No",1]
[]
[3,1,42,null,"Take  out and remove piping, sanitary fittings, etc. including disconnecting  piping  from fittings  and  making good floor and wall finishes (making good tiling and paintwork elsewhere)",null,0]
[]
[3,1,42," A","22mm Lever valve including disconnecting and stopping off water supply","No",2]
[]
[3,1,42," B","22mm Copper piping including fittings and brackets.","m",4]
[]
[3,1,42,null,"Making good to existing surfaces",null,0]
[]
[3,1,42," C","Smooth plaster to walls where 110mm wall removed","m",40]
[]
[3,1,42," D","Smooth plaster to walls where 230mm wall removed","m",10]
[]
[3,1,42," E","Screed to floor where 110mm wall removed","m",51]
[]
[3,1,42," F","Screed to floor where 230mm wall removed","m",10]
[]
[3,1,42,null,"REPAIRS TO ROOF AND WATER DAMAGED WALLS",null,0]
[]
[3,1,42," G","Budgetary allowance of R100 000.00 (One Hundred Thousand Rand) for repairs to roof and water damaged walls as directed by the Project Manager","Item",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[3,2,43,null,"BILL NO. 2",null,0]
[]
[3,2,43,null,"INTERNAL PARTITIONS",null,0]
[]
[3,2,43,null,"GYPROC Gypwall Soundbloc Drywall Partitions",null,0]
[]
[3,2,43," A","Drywall partition 4000mm high formed of 102mm drywall steel stud frame, with bottom track fixed to concrete floor and upper track to soffit of bulkhead with and including support angels, drywall studs spaced at 600mm centres, with 102mm \"cavitybat\" insulation inserted into the cavity of the partition and both sides covered with including two layers of 15mm Rhinoboard Soundbloc drywall panels, the joints between boards covered with drywall jointing tape and finished with Rhinoglide drywall joint filler; with natural anodised aluminium head channel","m",4]
[]
[3,2,43," B","Extra for end junction with wall including natural anodised aluminium channel","No",2]
[]
[3,2,43," C","264mm Wide drywall partition 4000mm high formed of double layer of 102mm drywall steel stud frame, with bottom track fixed to concrete floor and upper track to soffit of bulkhead with and including support angels, drywall studs spaced at 600mm centres, with 102mm \"cavitybat\" insulation inserted into the cavity of the partition and both outer sides covered with including two layers of 15mm Rhinoboard Soundbloc drywall panels, the joints between boards covered with drywall jointing tape and finished with Rhinoglide drywall joint filler; with natural anodised aluminium head channel","m",7]
[]
[3,2,43," D","Extra for trimming for and forming door opening to suit door size 900 x 2100mm and fitting with and including natural anodised aluminium frame (door and ironmongery elsewhere measured)","No",2]
[]
[3,2,44,null,"Sundries",null,0]
[]
[3,2,44," A","10 x 10mm Sondor strip acoustic barrier between aluminium framing and abutting vertical and horizontal surfaces ","m",29]
[]
[3,3,45,null,"BILL NO. 3",null,0]
[]
[3,3,45,null,"INTERNAL FINISHES",null,0]
[]
[3,3,45,null,"IN SITU FINISHES",null,0]
[]
[3,3,45,null,"One coat Gypsum skim plaster to receive wall paper",null,0]
[]
[3,3,45," A","Existing walls","m²",20]
[]
[3,3,45,null,"WALL PAPER",null,0]
[]
[3,3,45,null,"Paper backed vinyl wallpaper PC R700.00 (Seven Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of wall paper)",null,0]
[]
[3,3,45," B","On existing walls including narrow widths","m²",20]
[]
[3,3,45,null,"Take delivery, store until required and fix paper backed vinyl wall paper (supply of wall paper elsewhere measured) on previously painted surfaces, including one coat preparatory emulsion paint",null,0]
[]
[3,3,45," C","On existing walls including narrow widths","m²",20]
[]
[3,4,46,null,"BILL NO. 4",null,0]
[]
[3,4,46,null,"FLOOR FINISHES",null,0]
[]
[3,4,46,null,"IN SITU FINISHES",null,0]
[]
[3,4,46,null,"Screed leveller finished smooth with a steel trowel to receive floor tiles",null,0]
[]
[3,4,46," A","Pavelite screed leveller on existing screeded surfaces to receive new floor coverings","m²",100]
[]
[3,4,46,null,"TILING",null,0]
[]
[3,4,46,null,"Supply only porcelain floor tiles PC R400.00 (Four Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[3,4,46," B","Floors","m²",100]
[]
[3,4,46," C","100mm High skirting","m",48]
[]
[3,4,46,null,"Take delivery, store until required and fix 600 x 600mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[3,4,46," D","Floors","m²",100]
[]
[3,4,46," E","100mm High skirting","m",48]
[]
[3,4,47,null,"Sundries",null,0]
[]
[3,4,47," A","Kirk aluminium 10mm straight edge trim Code ASE100 to top of skirtings","m",48]
[]
[3,4,47," B","Kirk stainless steel 15mm straight edge trim Code SSE150 between tile floor finishes","m",30]
[]
[3,4,47," C","Kirk aluminium 15mm movement joint Code AMJ150 between tile floor finishes","m",46]
[]
[3,5,48,null,"BILL NO. 5",null,0]
[]
[3,5,48,null,"CEILINGS",null,0]
[]
[3,5,48,null,"SUSPENDED NON-METAL CEILINGS",null,0]
[]
[3,5,48,null,"Rhinoboard flush plastered ceilings",null,0]
[]
[3,5,48," A","Gyproc plasterboard screw up flush suspended ceiling formed of concealed suspension system with galvanised steel angle section hangers and 9.5mm Rhinoboard flush ceiling complying with SANS 266 with joints between boards covered for 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m²",41]
[]
[3,5,48," B","Trim for and form trap door size 700 x 700mm in clear formed of 38 x 50mm Sawn SA pine frame covered on one side with 9.5mm gypsum plasterboard and set on and including 19 x 32mm Wrot SA pine bearer all round opening","No",1]
[]
[3,5,48," C","Cut and fit ceiling around 150mm diameter downlighter","No",5]
[]
[3,5,48," D","Cut and fit ceiling around 100mm diameter smoke detector","No",5]
[]
[3,5,48,null,"Rhinoboard bulkheads, etc. ",null,0]
[]
[3,5,48," E","Vertical bulkhead 200mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m",24]
[]
[3,5,49," A","Recessed L shaped bulkhead 725mm girth, overall size 350mm wide x 275mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead detail 02 on drawing no. A-(54)200)","m",27]
[]
[3,5,49," B","Recessed rectangular shaped boxed bulkhead 1660mm girth, overall size 600mm wide x 300mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead detail 01 on drawing no. A-(54)200)","m",27]
[]
[3,5,49,null,"Acoustic suspended ceilings",null,0]
[]
[3,5,49," C","Suspended ceiling formed of fire rated S3a exposed demountable T24 suspension system comprising galvanised main tees and cross tees, built in with and including 15mm OWAcoustic Cosmo/N Premium biologically absorbable mineral wool ceiling tiles size 600 x 600mm complete with holding down clips and suspended not exceeding 1000mm below tie beam or average 2000mm from top chord of timber roof trusses including any necessary supplementary support system","m²",48]
[]
[3,5,49," D","Extra for trimming around recessed light fittings size 600 x 600mm","No",8]
[]
[3,5,49,null,"Cornices",null,0]
[]
[3,5,49," E","OWAconstruct Shadowline W-trim, plugged and screwed at centres not exceeding 200mm","m",29]
[]
[3,5,50," A","Sigma 50 x 50mm white epoxy coated plaster trim plugged to wall (Trim type 3)","m",28]
[]
[3,5,50," B","Capco Trim-Tex (code: 4010) corner bead to exposed corners of bulkheads","m",162]
[]
[3,6,51,null,"BILL NO. 6",null,0]
[]
[3,6,51,null,"PAINTING",null,0]
[]
[3,6,51,null,"ON PLASTER ETC.",null,0]
[]
[3,6,51,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[3,6,51," A","Plastered dry wall partition (\"Pastel\" colour group)","m²",88]
[]
[3,6,51,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[3,6,51," B","Plastered rhinoboard ceiling (\"White\" colour group)","m²",30]
[]
[3,6,51," C","Plastered bulkheads (\"White\" colour group)","m²",69]
[]
[3,6,51,null,"REDECORATION",null,0]
[]
[3,6,51,null,"The term \"clean down\" shall mean that existing painted surfaces shall be treated in the following manner prior to applying the paint required:  Existing PVA finished plaster surfaces shall be rubbed down ready to receive new PVA but where the PVA is in a poor condition, or otherwise unsuitable to receive further coats, or where the plaster is to receive a finish other than PVA, the old PVA shall be completely removed by wetting and scraping, and the surfaces filled where necessary and rubbed down ready to receive the new finishings",null,0]
[]
[3,6,52,null,"Existing painted plaster surfaces shall be washed down, filled where necessary, spot primed and rubbed down ready to receive new paint.  Existing painted metal surfaces shall be thoroughly rubbed and cleaned down before repainting, but where paint film has blistered or broken down, the paint must be completely removed down to the bare metal.",null,0]
[]
[3,6,52,null,"After cleaning off rust on metalwork, those portions so affected shall be treated with an approved rust inhibitor.  Existing woodwork previously painted shall be washed and rubbed down before repainting, but where the old paint must be completely removed back to the bare surface by the use of a blow lamp or paint removed, and the woodwork knotted, primed, stopped and rubbed down ready to receive new paint.",null,0]
[]
[3,6,52,null,"Care must be taken in burning off old paint not to char or otherwise damage the woodwork, and paint removers used must be free from soda or other caustic substances.  Existing oiled or varnished wood shall be scraped as may be necessary, stopped with tinted stopping and rubbed down and existing woodwork shall be cleaned and similarly stopped and rubbed down.",null,0]
[]
[3,6,52,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[3,6,52," A","Plastered walls (\"Pastel\" colour group)","m²",226]
[]
[{"$nulls":4},"SECTIONAL SUMMARY",null,0]
[]
[null,null,53,1,"ALTERATIONS AND DEMOLITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,53,2,"INTERNAL PARTITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,53,3,"INTERNAL FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,53,4,"FLOOR FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,53,5,"CEILINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,53,6,"PAINTING",null,null,{"v":0,"d":"0.00"}]
[]
[4,1,54,null,"SECTION NO. 4",null,0]
[]
[4,1,54,null,"AREA C - EXISTING OFFICES TO ONLINE CHECK-IN AREA",null,0]
[]
[4,1,54,null,"BILL NO. 1",null,0]
[]
[4,1,54,null,"ALTERATIONS AND DEMOLITIONS",null,0]
[]
[4,1,54,null,"TEMPORARY SCREENS AND HOARDINGS",null,0]
[]
[4,1,54,null,"Temporary hoardings",null,0]
[]
[4,1,54," A","Provide, erect and maintain temporary hoarding 2400mm high with 22mm five-ply shutterboard including support framework","m",31]
[]
[4,1,54,null,"Dust proof hoarding",null,0]
[]
[4,1,54," B","Provide, erect and maintain temporary dust proof hoarding 5000mm high to underside of slab with 250 micron plastic sheeting taped to bottom and sides of slab, walls, floor and joints taped double sided with and including staining wires to both sides of sheeting at 300mm centres","m",31]
[]
[4,1,54,null,"Painting to public side of hoarding",null,0]
[]
[4,1,54," C","Prepare, one coat Dulux Primer for Wood and two coats Dulux Pearlglo Water Based paint internally to one side of timber hoarding","m²",74]
[]
[4,1,54,null,"Take Down and set aside for re-use temporary hoardings upon completion of this section of works",null,0]
[]
[4,1,54," D","Temporary hoarding 2400mm high (take out from store and re-fixing elsewhere measured) complete with 22mm five-ply shutterboard including support framework and make good to any surfaces disturbed","m",31]
[]
[4,1,55,null,"DEMOLITIONS",null,0]
[]
[4,1,55,null,"Demolish, break up or take out and remove",null,0]
[]
[4,1,55," A","Demolish existing ticket offices overall size approximately 14,2 x 3,6m on plan x average 2,8m high, formed of drywall paritions, stiffener columns, ceiling support structure, etc. including disconnecting and stopping off all services, breaking up and removing all ceilings, windows, doors, joinery fittings, etc. and make good area to receive new finishes","No",1]
[]
[4,1,55,null,"Floor finishes",null,0]
[]
[4,1,55," B","Floor tiles to screeded floors and prepare to receive new floor finish","m²",53]
[]
[4,1,55,null,"Take off and set aside for re-use or hand over to Employer",null,0]
[]
[4,1,55," C","Bumper rails 200mm high fixed to top of concrete surface bed","m",21]
[]
[4,2,56,null,"BILL NO. 2",null,0]
[]
[4,2,56,null,"FLOOR FINISHES",null,0]
[]
[4,2,56,null,"IN SITU FINISHES",null,0]
[]
[4,2,56,null,"Screed leveller finished smooth with a steel trowel to receive floor tiles",null,0]
[]
[4,2,56," A","Pavelite screed leveller on existing screeded surfaces to receive new floor coverings","m²",52]
[]
[4,2,56,null,"TILING",null,0]
[]
[4,2,56,null,"Supply only porcelain floor tiles PC R500.00 (Five Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[4,2,56," B","Floors","m²",52]
[]
[4,2,56," C","100mm High skirting","m",15]
[]
[4,2,56,null,"Take delivery, store until required and fix 600 x 1200mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[4,2,56," D","Floors","m²",52]
[]
[4,2,56," E","100mm High skirting","m",15]
[]
[4,2,57,null,"Sundries",null,0]
[]
[4,2,57," A","Kirk aluminium 10mm straight edge trim Code ASE100 to top of skirtings","m",15]
[]
[4,2,57," B","Kirk stainless steel 15mm straight edge trim Code SSE150 between tile floor finishes","m",22]
[]
[4,2,57," C","Kirk aluminium 15mm movement joint Code AMJ150 between tile floor finishes","m",32]
[]
[4,3,58,null,"BILL NO. 3",null,0]
[]
[4,3,58,null,"CEILINGS",null,0]
[]
[4,3,58,null,"SUSPENDED NON-METAL CEILINGS",null,0]
[]
[4,3,58,null,"Rhinoboard flush plastered ceilings",null,0]
[]
[4,3,58," A","Gyproc plasterboard screw up flush suspended ceiling formed of concealed suspension system with galvanised steel angle section hangers and 9.5mm Rhinoboard flush ceiling complying with SANS 266 with joints between boards covered for 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 2500mm below soffit of slab","m²",20]
[]
[4,3,58," B","Trim for and form trap door size 600 x 600mm in clear formed of 38 x 50mm Sawn SA pine frame covered on one side with 9.5mm gypsum plasterboard and set on and including 19 x 32mm Wrot SA pine bearer all round opening","No",1]
[]
[4,3,58," C","Cut and fit ceiling around 150mm diameter downlighter","No",6]
[]
[4,3,58," D","Cut and fit ceiling around 100mm diameter smoke detector","No",4]
[]
[4,3,58,null,"Rhinoboard bulkheads, etc. ",null,0]
[]
[4,3,58," E","Vertical bulkhead 200mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 2000mm below existing ceiling","m",21]
[]
[4,3,59," A","Recessed rectangular shaped boxed bulkhead 1260mm girth, overall size 400mm wide x 300mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead detail 03 on drawing no. A-(54)200)","m",22]
[]
[4,3,59,null,"Cornices",null,0]
[]
[4,3,59," B","Sigma 50 x 50mm white epoxy coated plaster trim plugged to wall (Trim type 3)","m",24]
[]
[4,3,59," C","Capco Trim-Tex (code: 4010) corner bead to exposed corners of bulkheads","m",90]
[]
[4,4,60,null,"BILL NO. 4",null,0]
[]
[4,4,60,null,"SUNDRIES",null,0]
[]
[4,4,60,null,"BUMPER RAILS",null,0]
[]
[4,4,60,null,"Stainless Steel grade 316 bump rail",null,0]
[]
[4,4,60," A","Stainless steel bump rail 125mm high formed of 48mm diameter x 5,3mm thick circular hollow section bump rail with 43mm diameter x 4mm thick circular hollow section floor posts 100mm high at max 2000mm centres, the posts welded to the underside of the bump rail including 90mm diameter x 6mm thick base plates welded to bottom of posts with base plates each two times drilled and fixed to concrete floor with and including M10 chemical anchors including mortices in concrete all in accordance with drawing no. A-(12)2001 rev1","No",17]
[]
[4,4,60," B","Extra for end supports","No",2]
[]
[4,4,60,null,"RELOCATE EXISTING SEATING",null,0]
[]
[4,4,60," C","Budgetary allowance of R25 000.00 (Twenty Five Thousand Rand) for the relocation of existing seating as directed by the Project Manager","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[4,5,61,null,"BILL NO. 5",null,0]
[]
[4,5,61,null,"PAINTING",null,0]
[]
[4,5,61,null,"ON PLASTER ETC.",null,0]
[]
[4,5,61,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[4,5,61," A","Plastered rhinoboard ceiling (\"White\" colour group)","m²",20]
[]
[4,5,61," B","Plastered bulkheads (\"White\" colour group)","m²",32]
[]
[4,5,61,null,"REDECORATION",null,0]
[]
[4,5,61,null,"The term \"clean down\" shall mean that existing painted surfaces shall be treated in the following manner prior to applying the paint required:  Existing PVA finished plaster surfaces shall be rubbed down ready to receive new PVA but where the PVA is in a poor condition, or otherwise unsuitable to receive further coats, or where the plaster is to receive a finish other than PVA, the old PVA shall be completely removed by wetting and scraping, and the surfaces filled where necessary and rubbed down ready to receive the new finishings",null,0]
[]
[4,5,61,null,"Existing painted plaster surfaces shall be washed down, filled where necessary, spot primed and rubbed down ready to receive new paint.  Existing painted metal surfaces shall be thoroughly rubbed and cleaned down before repainting, but where paint film has blistered or broken down, the paint must be completely removed down to the bare metal.",null,0]
[]
[4,5,62,null,"After cleaning off rust on metalwork, those portions so affected shall be treated with an approved rust inhibitor.  Existing woodwork previously painted shall be washed and rubbed down before repainting, but where the old paint must be completely removed back to the bare surface by the use of a blow lamp or paint removed, and the woodwork knotted, primed, stopped and rubbed down ready to receive new paint.",null,0]
[]
[4,5,62,null,"Care must be taken in burning off old paint not to char or otherwise damage the woodwork, and paint removers used must be free from soda or other caustic substances.  Existing oiled or varnished wood shall be scraped as may be necessary, stopped with tinted stopping and rubbed down and existing woodwork shall be cleaned and similarly stopped and rubbed down.",null,0]
[]
[4,5,62,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[4,5,62," A","Plastered walls (\"Pastel\" colour group)","m²",84]
[]
[{"$nulls":4},"SECTIONAL SUMMARY",null,0]
[]
[null,null,63,1,"ALTERATIONS AND DEMOLITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,63,2,"FLOOR FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,63,3,"CEILINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,63,4,"SUNDRIES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,63,5,"PAINTING",null,null,{"v":0,"d":"0.00"}]
[]
[5,1,64,null,"SECTION NO. 5",null,0]
[]
[5,1,64,null,"AREA D - ADDITIONAL CHECK-IN COUNTERS",null,0]
[]
[5,1,64,null,"BILL NO. 1",null,0]
[]
[5,1,64,null,"ALTERATIONS AND DEMOLITIONS",null,0]
[]
[5,1,64,null,"TEMPORARY SCREENS AND HOARDINGS",null,0]
[]
[5,1,64,null,"Temporary hoardings",null,0]
[]
[5,1,64," A","Provide, erect and maintain temporary hoarding 2400mm high with 22mm five-ply shutterboard including support framework","m",37]
[]
[5,1,64,null,"Dust proof hoarding",null,0]
[]
[5,1,64," B","Provide, erect and maintain temporary dust proof hoarding 5000mm high to underside of slab with 250 micron plastic sheeting taped to bottom and sides of slab, walls, floor and joints taped double sided with and including staining wires to both sides of sheeting at 300mm centres","m",37]
[]
[5,1,64,null,"Painting to public side of hoarding",null,0]
[]
[5,1,64," C","Prepare, one coat Dulux Primer for Wood and two coats Dulux Pearlglo Water Based paint internally to one side of timber hoarding","m²",89]
[]
[5,1,64,null,"Take down and set aside for re-use temporary hoardings upon completion of this section of works",null,0]
[]
[5,1,64," D","Temporary hoarding 2400mm high (take out from store and re-fixing elsewhere measured) complete with 22mm five-ply shutterboard including support framework and make good to any surfaces disturbed","m",37]
[]
[5,1,65,null,"DEMOLITIONS",null,0]
[]
[5,1,65,null,"Demolish, break up or take out and remove",null,0]
[]
[5,1,65,null,"Drywall partitions",null,0]
[]
[5,1,65," A","Drywall partition 3000mm high including finishes","m",20]
[]
[5,1,65," B","Drywall partition 4000mm high including finishes","m",13]
[]
[5,1,65,null,"Floor finishes",null,0]
[]
[5,1,65," C","Floor tiles to screeded floors and prepare to receive new floor finish","m²",51]
[]
[5,1,65,null,"Ceilings",null,0]
[]
[5,1,65," D","Rhinoboard flush ceiling with cornices Including suspension grid, hangers, etc","m²",51]
[]
[5,1,65," E","Rhinoboard bulkhead 400mm wide x 500mm high","m",8]
[]
[5,1,65," F","200mm Wide timber capping to top and soffit of bulkhead","m",35]
[]
[5,1,65,null,"Doors",null,0]
[]
[5,1,65," G","Timber door size 900 x 2100mm high complete with frame, ironmongery, etc","No",3]
[]
[5,1,65," H","Glazed aluminium door size 900 x 2100mm high complete with frame, ironmongery, etc","No",3]
[]
[5,1,65," I","Roller shutter door size 1800 x 2400mm high complete with steel frame, etc","No",3]
[]
[5,1,65," J"," Glazed aluminium shopfront size 1500 x 2400mm high","No",1]
[]
[5,1,65," K"," Glazed aluminium shopfront size 2800 x 2400mm high","No",1]
[]
[5,1,66,null,"Windows",null,0]
[]
[5,1,66," A","Aluminium window size 1000 x 1000mm high","No",1]
[]
[5,1,66," B","Aluminium window size 1500 x 1200mm high","No",2]
[]
[5,1,66,null,"Build up, alter or break new openings in existing walls",null,0]
[]
[5,1,66,null,"Build up existing openings",null,0]
[]
[5,1,66," C","Build up existing door opening size 900 x 2100mm in 90mm drywall partition and make good on both sides","No",3]
[]
[5,1,66,null,"Break new openings",null,0]
[]
[5,1,66," D","Break through existing 90mm drywall partition for and form new door opening size 900 x 2100mm high, including making good both sides","No",1]
[]
[5,1,66,null,"Alter existing openings",null,0]
[]
[5,1,66," E","Alter existing window opening size 1500 x 1200mm high in 90mm drywall partition to form new door opening size 900 x 2100mm high by building up partition as necessary, including making good to both sides","No",1]
[]
[5,1,66,null,"Take off and set aside for re-use or hand over to Employer",null,0]
[]
[5,1,66," F","Bumper rails 200mm high fixed to top of concrete surface bed","m",16]
[]
[5,2,67,null,"BILL NO. 2",null,0]
[]
[5,2,67,null,"BRICK STRUCTURE",null,0]
[]
[5,2,67,null,"BRICKWORK",null,0]
[]
[5,2,67,null,"Brickwork in burnt clay NFP bricks in Class II mortar",null,0]
[]
[5,2,67," A","230mm Wall","m²",5]
[]
[5,2,67,null,"Sundries",null,0]
[]
[5,2,67," B","150mm Wide galvanised brick reinforcement","m",14]
[]
[5,3,68,null,"BILL NO. 3",null,0]
[]
[5,3,68,null,"INTERNAL PARTITIONS",null,0]
[]
[5,3,68,null,"GYPROC Gypwall Drywall Partitions",null,0]
[]
[5,3,68," A","Drywall partition 2400mm high overall formed of 63mm drywall steel tracks with bottom track fixed to concrete floor, upper track fixed to soffit of bulkhead and drywall studs spaced at 600mm centres, with 63mm \"cavitybat\" insulation inserted into the cavity of the partition and both sides covered with including 12.5mm gypsum plasterboard drywall panels, the joints between boards covered with drywall jointing tape and finished with Rhinoglide drywall joint filler","m",11]
[]
[5,3,68," B","Extra for end junction with wall including natural anodised aluminium channel","No",5]
[]
[5,3,68," C","Extra for trimming for and forming door opening to suit door size 900 x 2100mm and fitting with and including natural anodised aluminium frame (door and ironmongery elsewhere measured)","No",2]
[]
[5,3,68," D","Extra for trimming for and forming window opening to suit window size 1800 x 1500mm (window elsewhere measured)","No",2]
[]
[5,3,68," E","Extra for trimming for and forming window opening to suit window size 1500 x 1500mm (window elsewhere measured)","No",1]
[]
[5,4,69,null,"BILL NO. 4",null,0]
[]
[5,4,69,null,"INTERNAL WALL FINISHES",null,0]
[]
[5,4,69,null,"IN SITU FINISHES",null,0]
[]
[5,4,69,null,"One coat internal 1:5 cement plaster finished smooth with a steel trowel",null,0]
[]
[5,4,69," A","On walls","m²",9]
[]
[5,4,69," B","On narrow widths not exceeding 300mm wide","m²",1]
[]
[5,5,70,null,"BILL NO. 5",null,0]
[]
[5,5,70,null,"FLOOR FINISHES",null,0]
[]
[5,5,70,null,"CARPENTRY",null,0]
[]
[5,5,70,null,"Skirtings",null,0]
[]
[5,5,70," A","19 x 69mm Wrot Meranti angle rounded skirting plugged to wall","m",32]
[]
[5,5,70,null,"RESILIENT FLOOR COVERINGS, ETC.",null,0]
[]
[5,5,70,null,"Carpeting",null,0]
[]
[5,5,70," B","500 x 500mm Belgotex Fringe Beaded medium commercial PP Tuffed Loop pile with miracle fibre and stainproof miracle fibre blend carpet tiles to screeded floors","m²",19]
[]
[5,5,70,null,"IN SITU FINISHES",null,0]
[]
[5,5,70,null,"Screed leveller finished smooth with a steel trowel to receive floor tiles",null,0]
[]
[5,5,70," C","Pavelite screed leveller on existing screeded surfaces to receive new floor coverings","m²",36]
[]
[5,5,70,null,"TILING",null,0]
[]
[5,5,70,null,"Supply only porcelain floor tiles PC R500.00 (Five Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[5,5,70," D","Floors","m²",17]
[]
[5,5,70," E","100mm High skirting","m",11]
[]
[5,5,71,null,"Take delivery, store until required and fix 600 x 1200mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[5,5,71," A","Floors","m²",17]
[]
[5,5,71," B","100mm High skirting","m",11]
[]
[5,5,71,null,"Supply only porcelain floor tiles PC R400.00 (Five Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[5,5,71," C","Floors","m²",13]
[]
[5,5,71,null,"Take delivery, store until required and fix 300 x 300mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[5,5,71," D","Floors","m²",13]
[]
[5,5,71,null,"Sundries",null,0]
[]
[5,5,71," E","Kirk aluminium 10mm straight edge trim Code ASE100 to top of skirtings","m",11]
[]
[5,5,71," F","Kirk stainless steel 15mm straight edge trim Code SSE150 between tile floor finishes","m",10]
[]
[5,5,71," G","Kirk aluminium 15mm movement joint Code AMJ150 between tile floor finishes","m",11]
[]
[5,6,72,null,"BILL NO. 6",null,0]
[]
[5,6,72,null,"CEILINGS",null,0]
[]
[5,6,72,null,"SUSPENDED NON-METAL CEILINGS",null,0]
[]
[5,6,72,null,"Rhinoboard bulkheads, etc. ",null,0]
[]
[5,6,72," A","L shaped bulkhead 615mm girth, overall size 435mm wide x 180mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead and ceiling detail 01 on drawing no. A-(54)200)","m",14]
[]
[5,6,72," B","L shaped bulkhead 660mm girth, overall size 480mm wide x 180mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead and ceiling detail 01 on drawing no. A-(54)200)","m",19]
[]
[5,6,72," C","L shaped bulkhead 690mm girth, overall size 510mm wide x 180mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead and ceiling detail 01 on drawing no. A-(54)200)","m",5]
[]
[5,6,73," A","L shaped bulkhead 815mm girth, overall size 635mm wide x 180mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead and ceiling detail 01 on drawing no. A-(54)200)","m",5]
[]
[5,6,73,null,"Acoustic suspended ceilings",null,0]
[]
[5,6,73," B","Suspended ceiling formed of fire rated S3a exposed demountable T24 suspension system comprising galvanised main tees and cross tees, built in with and including 15mm OWAcoustic Cosmo/N Premium biologically absorbable mineral wool ceiling tiles size 600 x 600mm complete with holding down clips and suspended not exceeding 1000mm below soffit of slab","m²",38]
[]
[5,6,73," C","Extra for trimming around recessed light fittings size 600 x 600mm","No",8]
[]
[5,6,73," D","Cut and fit ceiling around 150mm diameter downlighter","No",10]
[]
[5,6,73,null,"Cornices",null,0]
[]
[5,6,73," E","OWAconstruct Shadowline W-trim, plugged and screwed at centres not exceeding 200mm","m",29]
[]
[5,6,73," F","Sigma 50 x 50mm white epoxy coated plaster trim plugged to wall (Trim type 3)","m",43]
[]
[5,6,73," G","Capco Trim-Tex (code: 4010) corner bead to exposed corners of bulkheads","m",29]
[]
[5,7,74,null,"BILL NO. 7",null,0]
[]
[5,7,74,null,"ALUMINIUM WINDOWS AND DOORS",null,0]
[]
[5,7,74,null,"GENERAL SPECIFICATION",null,0]
[]
[5,7,74,null,"Scope",null,0]
[]
[5,7,74,null,"This general specification specifies materials, construction, finishes, fastenings, installation and performance standards for aluminium alloy shopfronts, doors and windows.",null,0]
[]
[5,7,74,null,"Materials",null,0]
[]
[5,7,74,null,"Extruded aluminium members shall be fabricated from alloy of designation 6063 or 6061 in temper T5 or T6 complying with BS EN 755",null,0]
[]
[5,7,74,null,"Ancillary members such as cills, flashings, infill panels and the like which may be formed from flat sheet material having an appropriate alloy selected from alloy designations - 1200 or 3004 or 5251, of a temper suitable for the method of forming and a composition suitable for anodising or painting as required.  Alloys shall comply with BS EN 573",null,0]
[]
[5,7,74,null,"Anodising",null,0]
[]
[5,7,74,null,"All architectural anodising shall be in strict accordance with SANS 1407 and SANS 999",null,0]
[]
[5,7,74,null,"Powder coating",null,0]
[]
[5,7,74,null,"All architectural powder coating shall be in accordance with SANS 1796 and SANS 1578",null,0]
[]
[5,7,74,null,"Air Infiltration",null,0]
[]
[5,7,74,null,"All fenestration air infiltration shall be in accordance with SANS 613 as per part XA of SANS 10400",null,0]
[]
[5,7,75,null,"Construction",null,0]
[]
[5,7,75,null,"Construction shall comply with the minimum performance requirements contained in the relevant \"Selection Guides\" as published by AAAMSA from time to time.",null,0]
[]
[5,7,75,null,"Designs not covered by AAAMSA shall comply with SANS 0160 specification in particular and current National Building Regulations.",null,0]
[]
[5,7,75,null,"Note:",null,0]
[]
[5,7,75,null,"Notwithstanding the foregoing, the sub-contractor must ensure the strength and stiffness of the aluminium section/s to be used i.e. after any surface finishing has been applied, is adequate for the purpose. The manufacturer shall at all times ensure that contact between incompatible materials shall be prevented.",null,0]
[]
[5,7,75,null,"Manufacture",null,0]
[]
[5,7,75,null,"Joints in frames and sashes shall be made by mechanical means (cleating, screwing, etc.) or by welding. Joints may have flush, stepped or lapped surfaces. Mitred joints shall only have flush surfaces.  The windows and door shall be free from all sharp edges, burrs and the like.  Welded joints shall be cleaned off smooth on surfaces abutting closing faces, i.e. glazing rebates, etc.  Hardware and fittings shall be removable without removing the aluminium frames from the structure.  Sliding members shall be constructed so that no metal to metal sliding contact occurs.",null,0]
[]
[5,7,76,null,"Fittings",null,0]
[]
[5,7,76,null,"Weather sealing shall be of materials that are compatible with aluminium and shall be such that any degradation, shrinking, warping or adherence to closing surfaces does not impair the performance of the installation.",null,0]
[]
[5,7,76,null,"Glazing beads, gaskets and glazing compounds shall be of materials that are compatible with the aluminium, finishes, the glass or any other glazing materials.",null,0]
[]
[5,7,76,null,"Hardware, bearing devices and fittings in general must be made from non corrosive material, and shall be of a design so as to be accessible for adjustment, repair and replacement after the windows and door have been installed.  Fastenings shall be of materials which is compatible with aluminium and aluminium finishes.  Sub-frames shall be to manufacturer's specification and design and be compatible with aluminium and aluminium finishes.",null,0]
[]
[5,7,76,null,"Installation",null,0]
[]
[5,7,76,null,"Installation shall be such that the installed products are undamaged, securely anchored, sealed and meet with the above construction requirements in an installed position.  Exposed surfaces are to be protected by means of low tack adhesive tape",null,0]
[]
[5,7,77,null,"Glazing",null,0]
[]
[5,7,77,null,"Glazing shall be carried out in accordance with current National Building Regulations Part B (structure), N (glazing), T (fire) and read in conjunction with SANS Code of Practice 10137 - including other SANS Standards referred to in this specification particularly the appropriate parts of SANS 10400 & 1263 and AAAMSA selection guide for safety glazing materials.  All Safety Glazing materials (individual panes) shall be permanently marked. Such marking to be visible after glazing.  In the case of structural glazing written proof is to be provided that all stages of fabrication and installation have been executed with disciplined quality assurance in accordance with the relevant parts of SANS ISO 9000.",null,0]
[]
[5,7,77,null,"Written confirmation of compatibility of structural sealant with extrusion surface, glazing tape and glass is to be supplied by the structural sealant manufacturer together with the regular test reports regarding the adhesion of the sealant to the aluminium frame in accordance with ASTM/C 794-80 (Standard test of adhesion-in-peel of elastometric joint sealants)",null,0]
[]
[5,7,78,null,"Performance Test Certificates, Warranties, etc.",null,0]
[]
[5,7,78,null,"All curtain walls, windows, doors and shopfronts are to meet the performance requirements for air leakage, water penetration and uniform loading of the Association of Architectural Aluminium Manufacturers of South Africa. The Contractor will be required to provide the following:Tender Stage - Returnable Documentation with Tender1.\tAn AAAMSA Performance Test Certificate, \tas issued by the Manufacture/specialist \tContractor supplying/installing the glazed \tarchitectural products, for each framing \tsystem, testifying that their products meet \tthe requirements of the specified \tPerformance \tClass \tDesignation.  \tFAILURE TO SUBMIT THESE \tCERTIFICATES AT TENDER STAGE \tWILL RESULT IN THE TENDER BEING \tNON COMPLIANTPrior to Commencement of any site workA full set of detailed manufacturing drawings/manuals relevant to the installed products.Upon Completion of all site work at Practical Completion1.\tAn AAAMSA Performance Test Certificate2.\tAn AAAMSA Surface Finishing Certificate \tof conformance in respect of product \tfinishes such as anodising and powder \tcoating.3.\tA guarantee on powder coating of not less \tthan 15 years against peeling and \tdiscolouration.4.\tA warranty in laminated glass against \tdelamination and colour degradation for a \tperiod of not less than 5 years.5.\tAn AAAMSA Glass and Glazing Certificate \tof conformance in respect of all glazed \tsections, glazed in accordance with \tBuilding Regulations",null,0]
[]
[5,7,79,null,"Testing of windows for watertightness",null,0]
[]
[5,7,79,null,"All windows, doors and shopfronts shall be tested for watertightness with water sprayed on using adequate pressure. If in the opinion of the Principal Agent, the pressure proves to be in adequate, then the pressure shall be boosted by means of compressed air or other approved means",null,0]
[]
[5,7,79,null,"Reference to drawings",null,0]
[]
[5,7,79,null,"All descriptions are for reference purposes only and must be read in conjunction with the attached drawings to ascertain the full scope and extent of the works.",null,0]
[]
[5,7,79,null,"Contractor to provide shop details",null,0]
[]
[5,7,79,null,"Shop details are required. The contractor shall submit shop drawings to the Architect two weeks prior to fabrication, written approval of shop drawings must be given by the Architect prior to ordering of materials and fabrication. The Contractor shall, prior to submitting his shop drawings to the Architect, carefully check all dimensions of existing structures to ascertain the correctness of \"As Built\" dimensions and information as provided by the Architect. The Contractor's shop details shall make provision for any deviation from this information. No shop details will be provided by the Architect.",null,0]
[]
[5,7,79,null,"Sealing",null,0]
[]
[5,7,79,null,"All joints between aluminium sections and wall finishes to be polyurethane sealed both sides (internal and external) and to be included in the pricing of the windows and shopfronts",null,0]
[]
[5,7,80,null,"ALUMINIUM WINDOWS AND DOORS",null,0]
[]
[5,7,80,null,"Crealco Swift 38 natural anodised aluminium window system including setting up and building in and glazing with thickness and type of glass to comply with current National Building Regulations Part  B, N, T and SANS 10137, SANS 10400, SANS 1263 & AAAMSA SELECTION GUIDE for SAFETY GLAZING MATERIALS",null,0]
[]
[5,7,80," A","Window Type W01 size 1800 x 1500mm glazed with and including Clear Laminated safety glass all in accordance with drawing A-(35)5001","No",2]
[]
[5,7,80," B","Window Type SF02 size 1500 x 1500mm glazed with and including Clear Laminated safety glass all in accordance with drawing A-(32)5002","No",1]
[]
[5,7,80,null,"Crealco Clip 44 natural anodised aluminium shopfront and door system including setting up and building in and glazing with thickness and type of glass to comply with current National Building Regulations Part  B, N, T and SANS 10137, SANS 10400, SANS 1263 & AAAMSA SELECTION GUIDE for SAFETY GLAZING MATERIALS",null,0]
[]
[5,7,80," C","Door Type D04 size 900 x 2100mm high glazed with and including Clear Laminated safety glass all in accordance with drawing A-(31)5004","No",3]
[]
[5,7,80," D","Stacking door Type D03 size 1500 x 2400mm high glazed with and including Clear Laminated safety glass all in accordance with drawing A-(31)5003","No",1]
[]
[5,7,80," E","Shopfront Type SF01 size 4530 x 2400mm high with double stacking door size 1500 x 2400mm high glazed with and including Clear Laminated glass all in accordance with drawing A-(32)5001","No",1]
[]
[5,7,81,null,"IRONMONGERY",null,0]
[]
[5,7,81,null,"Hinges, etc",null,0]
[]
[5,7,81," A","DORMAKABA 1040 100mm aluminium sinkless hinges","Pairs",10.5]
[]
[5,7,81,null,"Locks, etc",null,0]
[]
[5,7,81," B","DORMAKABA D036S SS cylinder sash lock","No",3]
[]
[5,7,81," C","DORMAKABA DCE-002 SS round cylinder escutcheon","Pairs",3]
[]
[5,7,81," D","DORMAKABA DCE-105 SS narrow stile cylinder escutcheon","Pairs",2]
[]
[5,7,81," E","DORMAKABA DKC056501 KD 65mm five pin euro-profile knob cylinder","No",5]
[]
[5,7,81," F","DORMAKABA D02935 SS Narrow stile hook lock operating with European Profile cylidner","No",2]
[]
[5,7,81,null,"Door furniture, etc.",null,0]
[]
[5,7,81," G","DORMAKABA TH126 LATCH SS lever handle set with latch","Sets",3]
[]
[5,7,81," H","DORMAKABA DFP-SS-024 120 x 40mm Oval flush pull handle","No",4]
[]
[5,7,81,null,"Door closer, etc.",null,0]
[]
[5,7,81," I","DORMAKABA TS68-SL EN 2/3/4 rack and pinion door closer with non hold open scissor arm","Sets",3]
[]
[5,8,82,null,"BILL NO. 8",null,0]
[]
[5,8,82,null,"JOINERY FITTINGS",null,0]
[]
[5,8,82,null,"GENERAL SPECIFICATION",null,0]
[]
[5,8,82,null,"Drawings, descriptions, etc.",null,0]
[]
[5,8,82,null,"The fittings are to be constructed, installed and finished complete in accordance with the drawings issued with these bills of quantities and referred to in the descriptions of the fittings.  The abbreviated descriptions of fittings are sufficient only to identify the respective fittings or group of fittings and their locations.  The sizes of fittings are given either as length/girth x width x height or as length/girth x width or as length/girth x height as applicable.  The dimensions given are the overall \"squared off\" dimensions measured to the major external surfaces of the fitting regardless of notchings, cut-backs, etc., and to the extremeties of splayed ends.  The exact size, shape and position of fittings must be ascertained by reference to the detail drawings and all dimensions are to be checked on site.",null,0]
[]
[5,8,82,null,"In certain instances the fittings in a particular location form an integral whole;  but to facilitate measuring, scheduling, pricing and adjustment in the event of variations, the various component fittings comprising an integrated arrangement have been scheduled as individual items, each of which is to be priced separately, and the prices for the individual items are to include for all work at the junctions of adjacent component fittings to form the integral arrangement as detailed.",null,0]
[]
[5,8,83,null,"General",null,0]
[]
[5,8,83,null,"The fittings are to be constructed with materials and in the manner shown on the drawings, complete with all framing, bearers, rails, cleats, beads, fixing and assembly accessories, etc., as detailed or as necessary for rigid, best quality construction and finish.",null,0]
[]
[5,8,83,null,"Wherever possible all melamine finished chipboard worktops, etc., and plastic laminate finishes on worktops are to be in one piece without joints.",null,0]
[]
[5,8,83,null,"Where joints are unavoidable they are to be symmetrically spaced about the centre of the fitting or at the angle of L-shaped worktops, etc.  Joints in processed board worktops are to occur over the supporting framing, divisions, brackets, etc.  All abutments of worktops with walls or stainless steel sinks, etc., are to be pointed with silicone sealant, and the voids between the floor and the bottom of all fittings on wood bearers are to be sealed off by pointing with silicone sealant along the skirtings and bottoms at junctions with floor and walls.",null,0]
[]
[5,8,83,null,"Manufacture and Installation",null,0]
[]
[5,8,83,null,"All fittings, wherever possible, are to be completely manufactured in the joinery factory and must arrive on site with doors fitted.",null,0]
[]
[5,8,84,null,"Finishes, etc.",null,0]
[]
[5,8,84,null,"Carcass, shelving, drawers, etc. to be 16mm Melawood Peen melamine faced boards  Where fittings are required to be painted they are to be finished as per the specification  as indicated on the detailed drawings.  PC allowance for handles R100.00 each excluding Value Added Tax.",null,0]
[]
[5,8,84,null,"Prices of fittings",null,0]
[]
[5,8,84,null,"The joinery fittings are measured in number and are to be priced as complete units including all joinery work, ironmongery, metalwork, glazing, etc., and installation complete with all wall plugs, grounds, screws, bolts, expanding bolts, metal brackets, spacers and distance pieces, pointing with silicone sealant, painting, priming backs, etc., and all of the general provisions of this preamble.",null,0]
[]
[5,8,84,null,"Prices are also to include for any additional pointing with silicone sealant and/or trimming with beads as may be directed by the Principal Agent to make good any imperfect abutments of fittings with walls, etc.  Prices of joinery fittings are to exclude brick walls, under counter fittings, electrical installation to counters and sinks, all of which are elsewhere measured.",null,0]
[]
[5,8,85,null,"CHECK-IN COUNTERS",null,0]
[]
[5,8,85,null,"The following in check-in counters to area D",null,0]
[]
[5,8,85," A","Check in counter overall size 1185mm long x 1190mm wide x 1140mm high complete with 35mm Staron Salvocorp solid surfacing to tops, sides, bottom and front of unit including ironmongery, stainless steel lockable door, support framework, etc. and fix in position all in accordance with drawing no. A-(74)1000 ","No",2]
[]
[5,9,86,null,"BILL NO. 9",null,0]
[]
[5,9,86,null,"SUNDRIES",null,0]
[]
[5,9,86,null,"BUMPER RAILS",null,0]
[]
[5,9,86,null,"Stainless Steel grade 316 bump rail",null,0]
[]
[5,9,86," A","Stainless steel bump rail 125mm high formed of 48mm diameter x 5,3mm thick circular hollow section bump rail with 43mm diameter x 4mm thick circular hollow section floor posts 100mm high at max 2000mm centres, the posts welded to the underside of the bump rail including 90mm diameter x 6mm thick base plates welded to bottom of posts with base plates each two times drilled and fixed to concrete floor with and including M10 chemical anchors including mortices in concrete all in accordance with drawing no. A-(12)2001 rev1","No",14]
[]
[5,9,86," B","Extra for 90° bend","No",1]
[]
[5,9,86," C","Extra for end supports","No",6]
[]
[5,9,86,null,"SIGNAGE",null,0]
[]
[5,9,86," D","Subcontract allowance of R25 000.00 (Twenty Five Thousand Rand) net for signage by a Subcontractor approved by the Project Manager","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"}]
[]
[5,9,86," E","Profit","%IT"]
[]
[5,9,86," F","Attendance","%IT"]
[]
[5,9,86,null,"TICKET SALES AND RETAIL STORE FITOUT",null,0]
[]
[5,9,86," G","Budgetary allowance of R120 000.00 (One Hundred and Twenty Thousand Rand) for ticket sales and retail store fitout as directed by the Project Manager","Item",1,{"v":120000,"d":"120,000.00"},{"v":120000,"d":"120,000.00"}]
[]
[5,10,87,null,"BILL NO. 10",null,0]
[]
[5,10,87,null,"PAINTING",null,0]
[]
[5,10,87,null,"ON PLASTER ETC.",null,0]
[]
[5,10,87,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[5,10,87," A","Plastered walls (\"Pastel\" colour group)","m²",10]
[]
[5,10,87,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[5,10,87," B","Plastered dry wall partition (\"Pastel\" colour group)","m²",53]
[]
[5,10,87,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[5,10,87," C","Plastered bulkheads (\"White\" colour group)","m²",29]
[]
[5,10,87,null,"REDECORATION",null,0]
[]
[5,10,87,null,"The term \"clean down\" shall mean that existing painted surfaces shall be treated in the following manner prior to applying the paint required:  Existing PVA finished plaster surfaces shall be rubbed down ready to receive new PVA but where the PVA is in a poor condition, or otherwise unsuitable to receive further coats, or where the plaster is to receive a finish other than PVA, the old PVA shall be completely removed by wetting and scraping, and the surfaces filled where necessary and rubbed down ready to receive the new finishings",null,0]
[]
[5,10,88,null,"Existing painted plaster surfaces shall be washed down, filled where necessary, spot primed and rubbed down ready to receive new paint.  Existing painted metal surfaces shall be thoroughly rubbed and cleaned down before repainting, but where paint film has blistered or broken down, the paint must be completely removed down to the bare metal.",null,0]
[]
[5,10,88,null,"After cleaning off rust on metalwork, those portions so affected shall be treated with an approved rust inhibitor.  Existing woodwork previously painted shall be washed and rubbed down before repainting, but where the old paint must be completely removed back to the bare surface by the use of a blow lamp or paint removed, and the woodwork knotted, primed, stopped and rubbed down ready to receive new paint.",null,0]
[]
[5,10,88,null,"Care must be taken in burning off old paint not to char or otherwise damage the woodwork, and paint removers used must be free from soda or other caustic substances.  Existing oiled or varnished wood shall be scraped as may be necessary, stopped with tinted stopping and rubbed down and existing woodwork shall be cleaned and similarly stopped and rubbed down.",null,0]
[]
[5,10,88,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[5,10,88," A","Plastered dry wall partition (\"Pastel\" colour group)","m²",68]
[]
[5,10,88," B","Plastered walls (\"Pastel\" colour group)","m²",63]
[]
[5,10,89,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[5,10,89," A","Plastered bulkheads (\"White\" colour group)","m²",21]
[]
[{"$nulls":4},"SECTIONAL SUMMARY",null,0]
[]
[null,null,90,1,"ALTERATIONS AND DEMOLITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,2,"BRICK STRUCTURE",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,3,"INTERNAL PARTITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,4,"INTERNAL FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,5,"FLOOR FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,6,"CEILINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,7,"ALUMINIUM WINDOWS AND DOORS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,8,"JOINERY FITTINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,9,"SUNDRIES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,90,10,"PAINTING",null,null,{"v":0,"d":"0.00"}]
[]
[6,1,91,null,"SECTION NO. 6",null,0]
[]
[6,1,91,null,"AREA E - BUSINESS CLASS SECURITY CHECK-IN",null,0]
[]
[6,1,91,null,"BILL NO. 1",null,0]
[]
[6,1,91,null,"ALTERATIONS AND DEMOLITIONS",null,0]
[]
[6,1,91,null,"TEMPORARY SCREENS AND HOARDINGS",null,0]
[]
[6,1,91,null,"Temporary hoardings",null,0]
[]
[6,1,91," A","Provide, erect and maintain temporary hoarding 2400mm high with 22mm five-ply shutterboard including support framework","m",51]
[]
[6,1,91,null,"Dust proof hoarding",null,0]
[]
[6,1,91," B","Provide, erect and maintain temporary dust proof hoarding 5000mm high to underside of slab with 250 micron plastic sheeting taped to bottom and sides of slab, walls, floor and joints taped double sided with and including staining wires to both sides of sheeting at 300mm centres","m",51]
[]
[6,1,91,null,"Painting to public side of hoarding",null,0]
[]
[6,1,91," C","Prepare, one coat Dulux Primer for Wood and two coats Dulux Pearlglo Water Based paint internally to one side of timber hoarding","m²",122]
[]
[6,1,91,null,"Take down and set aside for re-use temporary hoardings upon completion of this section of works",null,0]
[]
[6,1,91," D","Temporary hoarding 2400mm high (take out from store and re-fixing elsewhere measured) complete with 22mm five-ply shutterboard including support framework and make good to any surfaces disturbed","m",51]
[]
[6,1,92,null,"DEMOLITIONS",null,0]
[]
[6,1,92,null,"Demolish, break up or take out and remove",null,0]
[]
[6,1,92,null,"Drywall partitions",null,0]
[]
[6,1,92," A","Drywall partition 4000mm high including finishes","m",24]
[]
[6,1,92,null,"Floor finishes",null,0]
[]
[6,1,92," B","150mm Thick screed to floors (removal of floor tiles elsewhere measured)","m²",84]
[]
[6,1,92," C","Floor tiles to screeded floors and prepare to receive new floor finish","m²",152]
[]
[6,1,92," D","Timber skirting","m",41]
[]
[6,1,92,null,"Ceilings",null,0]
[]
[6,1,92," E","Suspended ceiling and bulkheads with and including suspension grid, hangers, etc","m²",280]
[]
[6,1,92,null,"Doors",null,0]
[]
[6,1,92," F","Glazed aluminium door size 900 x 2100mm high complete with frame, ironmongery, etc","No",2]
[]
[6,1,92," G","Glazed aluminium door size 1600 x 2100mm high complete with frame, ironmongery, etc","No",1]
[]
[6,1,92," H"," Glazed aluminium shopfront size 5000 x 2100mm high","No",1]
[]
[6,1,92,null,"Making good to existing surfaces",null,0]
[]
[6,1,92," I","Smooth plaster to walls where 110mm wall removed","m",24]
[]
[6,1,92," J","Screed to floor where 110mm wall removed","m",24]
[]
[6,1,93,null,"Build up, alter or break new openings in existing walls",null,0]
[]
[6,1,93,null,"Build up existing openings",null,0]
[]
[6,1,93," A","Build up existing door opening size 900 x 2100mm in 110mm wall and make good smooth plaster on both sides","No",1]
[]
[6,1,93,null,"Break new openings",null,0]
[]
[6,1,93," B","Break through existing 110mm wall for and form new door opening size 900 x 2100mm, form new lintol over and make good smooth plaster to walls and reveals on both sides and screed to threshold","No",1]
[]
[6,2,94,null,"BILL NO. 2",null,0]
[]
[6,2,94,null,"INTERNAL PARTITIONS",null,0]
[]
[6,2,94,null,"GYPROC Gypwall Drywall Partitions",null,0]
[]
[6,2,94," A","Drywall partition 2100mm high overall formed of 63mm drywall steel tracks with bottom track fixed to concrete floor and drywall studs spaced at 600mm centres, with 63mm \"cavitybat\" insulation inserted into the cavity of the partition and both sides covered with including 12.5mm gypsum plasterboard drywall panels, the joints between boards covered with drywall jointing tape and finished with Rhinoglide drywall joint filler","m",5]
[]
[6,2,94," B","Extra for end junction with wall including natural anodised aluminium channel","No",1]
[]
[6,2,94," C","Extra for angle intersection","No",1]
[]
[6,2,94," D","Extra for fair exposed end to partition including natural anodised aluminium channel","No",1]
[]
[6,2,94," E","Drywall partition 4000mm high overall formed of 63mm drywall steel tracks with bottom track fixed to concrete floor, upper track fixed to soffit of bulkhead and drywall studs spaced at 600mm centres, with 63mm \"cavitybat\" insulation inserted into the cavity of the partition and both sides covered with including 12.5mm gypsum plasterboard drywall panels, the joints between boards covered with drywall jointing tape and finished with Rhinoglide drywall joint filler","m",2]
[]
[6,2,94," F","Extra for end junction with wall including natural anodised aluminium channel","No",2]
[]
[6,3,95,null,"BILL NO. 3",null,0]
[]
[6,3,95,null,"INTERNAL WALL FINISHES",null,0]
[]
[6,3,95,null,"IN SITU FINISHES",null,0]
[]
[6,3,95,null,"One coat Gypsum skim plaster to receive wall paper",null,0]
[]
[6,3,95," A","Existing walls","m²",54]
[]
[6,3,95,null,"TIMBER WALL CLADDING",null,0]
[]
[6,3,95,null,"The following in OWA Idealux FL wall cladding",null,0]
[]
[6,3,95," B","Acoustic timber wall cladding formed of Idealux FL solid wood panels size 600 x 2400mm high complete with polyester fibre backing and fixed to wall with fixing adhesive and screws all in accordance with manufacturers recommendations","m²",88]
[]
[6,3,95," C","Extra for trimming for and forming door opening size 900 x 2100mm (door and frame elsewhere measured)","No",1]
[]
[6,3,95," D","Extra for trimming for and forming door opening size 1600 x 2100mm (door and frame elsewhere measured)","No",1]
[]
[6,3,95,null,"WALL PAPER",null,0]
[]
[6,3,95,null,"Paper backed vinyl wallpaper PC R700.00 (Seven Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of wall paper)",null,0]
[]
[6,3,95," E","On existing walls including narrow widths","m²",54]
[]
[6,3,96,null,"Take delivery, store until required and fix paper backed vinyl wall paper (supply of wall paper elsewhere measured) on previously painted surfaces, including one coat preparatory emulsion paint",null,0]
[]
[6,3,96," A","On existing walls including narrow widths","m²",54]
[]
[6,4,97,null,"BILL NO. 4",null,0]
[]
[6,4,97,null,"FLOOR FINISHES",null,0]
[]
[6,4,97,null,"IN SITU FINISHES",null,0]
[]
[6,4,97,null,"Screed leveller finished smooth with a steel trowel to receive floor tiles",null,0]
[]
[6,4,97," A","Pavelite screed leveller on existing screeded surfaces to receive new floor coverings","m²",152]
[]
[6,4,97,null,"TILING",null,0]
[]
[6,4,97,null,"Supply only porcelain floor tiles PC R500.00 (Five Hundred Rand) per square metre net including all necessary waste (rate to include for waste) (area measured is nett area of tiling)",null,0]
[]
[6,4,97," B","Floors","m²",152]
[]
[6,4,97," C","100mm High skirting","m",48]
[]
[6,4,97,null,"Take delivery, store until required and fix 600 x 1200mm porcelain tiles (supply of tiles elsewhere measured) to screeded surface unless otherwise described with TAL Gold Star 6 adhesive and flush point in tinted TAL High Traffic tile grout mixed with TAl Bond",null,0]
[]
[6,4,97," D","Floors","m²",152]
[]
[6,4,97," E","100mm High skirting","m",48]
[]
[6,4,98,null,"Sundries",null,0]
[]
[6,4,98," A","Kirk aluminium 10mm straight edge trim Code ASE100 to top of skirtings","m",48]
[]
[6,4,98," B","Kirk stainless steel 15mm straight edge trim Code SSE150 between tile floor finishes","m",23]
[]
[6,4,98," C","Kirk aluminium 15mm movement joint Code AMJ150 between tile floor finishes","m",128]
[]
[6,5,99,null,"BILL NO. 5",null,0]
[]
[6,5,99,null,"CEILINGS",null,0]
[]
[6,5,99,null,"SUSPENDED NON-METAL CEILINGS",null,0]
[]
[6,5,99,null,"Rhinoboard flush plastered ceilings",null,0]
[]
[6,5,99," A","Gyproc plasterboard screw up flush suspended ceiling formed of concealed suspension system with galvanised steel angle section hangers and 9.5mm Rhinoboard flush ceiling complying with SANS 266 with joints between boards covered for 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m²",237]
[]
[6,5,99," B","Trim for and form trap door size 600 x 600mm in clear formed of 38 x 50mm Sawn SA pine frame covered on one side with 9.5mm gypsum plasterboard and set on and including 19 x 32mm Wrot SA pine bearer all round opening","No",1]
[]
[6,5,99," C","Cut and fit ceiling around 150mm diameter downlighter","No",50]
[]
[6,5,99," D","Cut and fit ceiling around 100mm diameter smoke detector","No",8]
[]
[6,5,99,null,"Rhinoboard bulkheads, etc. ",null,0]
[]
[6,5,99," E","Vertical bulkhead 180mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m",52]
[]
[6,5,100," A","Vertical bulkhead 200mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab","m",91]
[]
[6,5,100," B","Recessed rectangular shaped boxed bulkhead 1660mm girth, overall size 600mm wide x 300mm high formed of concealed suspension system with galvanised steel angle section hangers and 9,5mm Rhinoboard with joints between boards covered with 63mm wide wire mesh strips and the whole finished with one coat cretestone plaster steel trowelled to a smooth surface and suspended not exceeding 1000mm below soffit of slab (bulkhead detail 01 on drawing no. A-(54)200)","m",91]
[]
[6,5,100,null,"Acoustic suspended ceilings",null,0]
[]
[6,5,100," C","Suspended ceiling formed of fire rated S3a exposed demountable T24 suspension system comprising galvanised main tees and cross tees, built in with and including 15mm OWAcoustic Cosmo/N Premium biologically absorbable mineral wool ceiling tiles size 600 x 600mm complete with holding down clips and suspended not exceeding 1000mm below tie beam or average 2000mm from top chord of timber roof trusses including any necessary supplementary support system","m²",103]
[]
[6,5,100," D","Extra for trimming around recessed light fittings size 600 x 600mm","No",15]
[]
[6,5,100,null,"Cornices",null,0]
[]
[6,5,100," E","OWAconstruct Shadowline W-trim, plugged and screwed at centres not exceeding 200mm","m",52]
[]
[6,5,101," A","Sigma 50 x 50mm white epoxy coated plaster trim plugged to wall (Trim type 3)","m",77]
[]
[6,5,101," B","Capco Trim-Tex (code: 4010) corner bead to exposed corners of bulkheads","m",52]
[]
[6,6,102,null,"BILL NO. 6",null,0]
[]
[6,6,102,null,"ALUMINIUM WINDOWS AND DOORS",null,0]
[]
[6,6,102,null,"GENERAL SPECIFICATION",null,0]
[]
[6,6,102,null,"Scope",null,0]
[]
[6,6,102,null,"This general specification specifies materials, construction, finishes, fastenings, installation and performance standards for aluminium alloy shopfronts, doors and windows.",null,0]
[]
[6,6,102,null,"Materials",null,0]
[]
[6,6,102,null,"Extruded aluminium members shall be fabricated from alloy of designation 6063 or 6061 in temper T5 or T6 complying with BS EN 755",null,0]
[]
[6,6,102,null,"Ancillary members such as cills, flashings, infill panels and the like which may be formed from flat sheet material having an appropriate alloy selected from alloy designations - 1200 or 3004 or 5251, of a temper suitable for the method of forming and a composition suitable for anodising or painting as required.  Alloys shall comply with BS EN 573",null,0]
[]
[6,6,102,null,"Anodising",null,0]
[]
[6,6,102,null,"All architectural anodising shall be in strict accordance with SANS 1407 and SANS 999",null,0]
[]
[6,6,102,null,"Powder coating",null,0]
[]
[6,6,102,null,"All architectural powder coating shall be in accordance with SANS 1796 and SANS 1578",null,0]
[]
[6,6,102,null,"Air Infiltration",null,0]
[]
[6,6,102,null,"All fenestration air infiltration shall be in accordance with SANS 613 as per part XA of SANS 10400",null,0]
[]
[6,6,103,null,"Construction",null,0]
[]
[6,6,103,null,"Construction shall comply with the minimum performance requirements contained in the relevant \"Selection Guides\" as published by AAAMSA from time to time.",null,0]
[]
[6,6,103,null,"Designs not covered by AAAMSA shall comply with SANS 0160 specification in particular and current National Building Regulations.",null,0]
[]
[6,6,103,null,"Note:",null,0]
[]
[6,6,103,null,"Notwithstanding the foregoing, the sub-contractor must ensure the strength and stiffness of the aluminium section/s to be used i.e. after any surface finishing has been applied, is adequate for the purpose. The manufacturer shall at all times ensure that contact between incompatible materials shall be prevented.",null,0]
[]
[6,6,103,null,"Manufacture",null,0]
[]
[6,6,103,null,"Joints in frames and sashes shall be made by mechanical means (cleating, screwing, etc.) or by welding. Joints may have flush, stepped or lapped surfaces. Mitred joints shall only have flush surfaces.  The windows and door shall be free from all sharp edges, burrs and the like.  Welded joints shall be cleaned off smooth on surfaces abutting closing faces, i.e. glazing rebates, etc.  Hardware and fittings shall be removable without removing the aluminium frames from the structure.  Sliding members shall be constructed so that no metal to metal sliding contact occurs.",null,0]
[]
[6,6,104,null,"Fittings",null,0]
[]
[6,6,104,null,"Weather sealing shall be of materials that are compatible with aluminium and shall be such that any degradation, shrinking, warping or adherence to closing surfaces does not impair the performance of the installation.",null,0]
[]
[6,6,104,null,"Glazing beads, gaskets and glazing compounds shall be of materials that are compatible with the aluminium, finishes, the glass or any other glazing materials.",null,0]
[]
[6,6,104,null,"Hardware, bearing devices and fittings in general must be made from non corrosive material, and shall be of a design so as to be accessible for adjustment, repair and replacement after the windows and door have been installed.  Fastenings shall be of materials which is compatible with aluminium and aluminium finishes.  Sub-frames shall be to manufacturer's specification and design and be compatible with aluminium and aluminium finishes.",null,0]
[]
[6,6,104,null,"Installation",null,0]
[]
[6,6,104,null,"Installation shall be such that the installed products are undamaged, securely anchored, sealed and meet with the above construction requirements in an installed position.  Exposed surfaces are to be protected by means of low tack adhesive tape",null,0]
[]
[6,6,105,null,"Glazing",null,0]
[]
[6,6,105,null,"Glazing shall be carried out in accordance with current National Building Regulations Part B (structure), N (glazing), T (fire) and read in conjunction with SANS Code of Practice 10137 - including other SANS Standards referred to in this specification particularly the appropriate parts of SANS 10400 & 1263 and AAAMSA selection guide for safety glazing materials.  All Safety Glazing materials (individual panes) shall be permanently marked. Such marking to be visible after glazing.  In the case of structural glazing written proof is to be provided that all stages of fabrication and installation have been executed with disciplined quality assurance in accordance with the relevant parts of SANS ISO 9000.",null,0]
[]
[6,6,105,null,"Written confirmation of compatibility of structural sealant with extrusion surface, glazing tape and glass is to be supplied by the structural sealant manufacturer together with the regular test reports regarding the adhesion of the sealant to the aluminium frame in accordance with ASTM/C 794-80 (Standard test of adhesion-in-peel of elastometric joint sealants)",null,0]
[]
[6,6,106,null,"Performance Test Certificates, Warranties, etc.",null,0]
[]
[6,6,106,null,"All curtain walls, windows, doors and shopfronts are to meet the performance requirements for air leakage, water penetration and uniform loading of the Association of Architectural Aluminium Manufacturers of South Africa. The Contractor will be required to provide the following:Tender Stage - Returnable Documentation with Tender1.\tAn AAAMSA Performance Test Certificate, \tas issued by the Manufacture/specialist \tContractor supplying/installing the glazed \tarchitectural products, for each framing \tsystem, testifying that their products meet \tthe requirements of the specified \tPerformance \tClass \tDesignation.  \tFAILURE TO SUBMIT THESE \tCERTIFICATES AT TENDER STAGE \tWILL RESULT IN THE TENDER BEING \tNON COMPLIANTPrior to Commencement of any site workA full set of detailed manufacturing drawings/manuals relevant to the installed products.Upon Completion of all site work at Practical Completion1.\tAn AAAMSA Performance Test Certificate2.\tAn AAAMSA Surface Finishing Certificate \tof conformance in respect of product \tfinishes such as anodising and powder \tcoating.3.\tA guarantee on powder coating of not less \tthan 15 years against peeling and \tdiscolouration.4.\tA warranty in laminated glass against \tdelamination and colour degradation for a \tperiod of not less than 5 years.5.\tAn AAAMSA Glass and Glazing Certificate \tof conformance in respect of all glazed \tsections, glazed in accordance with \tBuilding Regulations",null,0]
[]
[6,6,107,null,"Testing of windows for watertightness",null,0]
[]
[6,6,107,null,"All windows, doors and shopfronts shall be tested for watertightness with water sprayed on using adequate pressure. If in the opinion of the Principal Agent, the pressure proves to be in adequate, then the pressure shall be boosted by means of compressed air or other approved means",null,0]
[]
[6,6,107,null,"Reference to drawings",null,0]
[]
[6,6,107,null,"All descriptions are for reference purposes only and must be read in conjunction with the attached drawings to ascertain the full scope and extent of the works.",null,0]
[]
[6,6,107,null,"Contractor to provide shop details",null,0]
[]
[6,6,107,null,"Shop details are required. The contractor shall submit shop drawings to the Architect two weeks prior to fabrication, written approval of shop drawings must be given by the Architect prior to ordering of materials and fabrication. The Contractor shall, prior to submitting his shop drawings to the Architect, carefully check all dimensions of existing structures to ascertain the correctness of \"As Built\" dimensions and information as provided by the Architect. The Contractor's shop details shall make provision for any deviation from this information. No shop details will be provided by the Architect.",null,0]
[]
[6,6,107,null,"Sealing",null,0]
[]
[6,6,107,null,"All joints between aluminium sections and wall finishes to be polyurethane sealed both sides (internal and external) and to be included in the pricing of the windows and shopfronts",null,0]
[]
[6,6,108,null,"ALUMINIUM WINDOWS AND DOORS",null,0]
[]
[6,6,108,null,"Crealco Clip 44 natural anodised aluminium shopfront and door system including setting up and building in and glazing with thickness and type of glass to comply with current National Building Regulations Part  B, N, T and SANS 10137, SANS 10400, SANS 1263 & AAAMSA SELECTION GUIDE for SAFETY GLAZING MATERIALS",null,0]
[]
[6,6,108," A","Door Type D04 size 900 x 2100mm high glazed with and including Clear Laminated safety glass all in accordance with drawing A-(31)5004","No",1]
[]
[6,6,108," B","Shopfront Type SF03 size 5300 x 3100mm high glazed with and including Frosted Laminated glass all in accordance with drawing A-(32)5003","No",1]
[]
[6,6,108,null,"IRONMONGERY",null,0]
[]
[6,6,108,null,"Hinges, etc",null,0]
[]
[6,6,108," C","DORMAKABA 1040 100mm aluminium sinkless hinges","Pairs",1.5]
[]
[6,6,108,null,"Locks, etc",null,0]
[]
[6,6,108," D","DORMAKABA D036S SS cylinder sash lock","No",1]
[]
[6,6,108," E","DORMAKABA DCE-002 SS round cylinder escutcheon","Pairs",1]
[]
[6,6,108," F","DORMAKABA DKC056501 KD 65mm five pin euro-profile knob cylinder","No",1]
[]
[6,6,108,null,"Door furniture, etc.",null,0]
[]
[6,6,108," G","DORMAKABA TH126 LATCH SS lever handle set with latch","Sets",1]
[]
[6,6,109,null,"Door closer, etc.",null,0]
[]
[6,6,109," A","DORMAKABA TS68-SL EN 2/3/4 rack and pinion door closer with non hold open scissor arm","Sets",1]
[]
[6,7,110,null,"BILL NO. 7",null,0]
[]
[6,7,110,null,"JOINERY FITTINGS",null,0]
[]
[6,7,110,null,"COFFEE STATION",null,0]
[]
[6,7,110," A","Subcontract allowance of R150 000.00 (One Hundred and Fifty Thousand Rand) net for coffee station by a Subcontractor approved by the Project Manager","Item",1,{"v":150000,"d":"150,000.00"},{"v":150000,"d":"150,000.00"}]
[]
[6,7,110," B","Profit","%IT"]
[]
[6,7,110," C","Attendance","%IT"]
[]
[6,8,111,null,"BILL NO. 8",null,0]
[]
[6,8,111,null,"SUNDRIES",null,0]
[]
[6,8,111,null,"BALUSTRADING AND HANDRAILS",null,0]
[]
[6,8,111," A","Budgetary allowance of R30 000.00 (Thirty Thousand Rand) for balustrading and handrails as directed by the Project Manager","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"}]
[]
[6,8,111,null,"SIGNAGE",null,0]
[]
[6,8,111," B","Subcontract allowance of R20 000.00 (Twenty Thousand Rand) net for signage by a Subcontractor approved by the Project Manager","Item",1,{"v":20000,"d":"20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[6,8,111," C","Profit","%IT"]
[]
[6,8,111," D","Attendance","%IT"]
[]
[6,9,112,null,"BILL NO. 9",null,0]
[]
[6,9,112,null,"PLUMBING AND DRAINAGE",null,0]
[]
[6,9,112,null,"WATER SUPPLIES",null,0]
[]
[6,9,112,null,"Copper water supply pipes complying with SANS 460 Class II with brass compression couplings",null,0]
[]
[6,9,112," A","15mm Pipe and fixing to walls, chases, roofs etc. including labour bends","m",12]
[]
[6,9,112," B","22mm Ditto","m",46]
[]
[6,9,112,null,"Extra over copper pipes for the following brass compression fittings",null,0]
[]
[6,9,112," C","15mm Elbow, tee, connector, etc.","No",10]
[]
[6,9,112," D","22mm Elbow, tee, connector, etc.","No",15]
[]
[6,9,112,null,"Valves, etc. complying with SANS 226 and connections to copper and multi layer pipes including connectors",null,0]
[]
[6,9,112," E","22mm Cobra lever type ball-o-stop including adaptors to copper pipe","No",2]
[]
[6,9,112,null,"SANITARY PLUMBING",null,0]
[]
[6,9,112,null,"Rigid PVC waste, soil and vent pipes complying with SANS 967",null,0]
[]
[6,9,112," F","40mm Pipe and fixing to walls, chases, roofs etc.","m",16]
[]
[6,9,112," G","50mm Pipe and fixing to walls, chases, roofs, etc.","m",46]
[]
[6,9,112," H","110mm Pipe and fixing to walls, chases, roofs, etc.","m",6]
[]
[6,9,112,null,"Extra over PVC pipes for",null,0]
[]
[6,9,112," I","110mm End cap","No",1]
[]
[6,9,113," A","50 x 40mm Reducer","No",2]
[]
[6,9,113," B","40mm Bend","No",2]
[]
[6,9,113," C","50mm Bend","No",4]
[]
[6,9,113," D","40mm Inspection eye bend","No",2]
[]
[6,9,113," E","50mm Inspection eye bend","No",4]
[]
[6,9,113," F","110mm Inspection eye bend","No",2]
[]
[6,9,113," G","40mm Inspection eye junction","No",2]
[]
[6,9,113," H","50mm Inspection eye junction","No",4]
[]
[6,9,113," I","110mm Inspection eye junction","No",1]
[]
[6,9,113," J","110mm Inspection eye reducing junction","No",1]
[]
[6,9,113,null,"TESTING",null,0]
[]
[6,9,113," K","Test the plumbing and drainage installation","Item",1]
[]
[6,10,114,null,"BILL NO. 10",null,0]
[]
[6,10,114,null,"PAINTING",null,0]
[]
[6,10,114,null,"ON PLASTER ETC.",null,0]
[]
[6,10,114,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[6,10,114," A","Plastered dry wall partition (\"Pastel\" colour group)","m²",37]
[]
[6,10,114,null,"Prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[6,10,114," B","Plastered rhinoboard ceiling (\"White\" colour group)","m²",237]
[]
[6,10,114," C","Plastered bulkheads (\"White\" colour group)","m²",179]
[]
[6,10,114,null,"REDECORATION",null,0]
[]
[6,10,114,null,"The term \"clean down\" shall mean that existing painted surfaces shall be treated in the following manner prior to applying the paint required:  Existing PVA finished plaster surfaces shall be rubbed down ready to receive new PVA but where the PVA is in a poor condition, or otherwise unsuitable to receive further coats, or where the plaster is to receive a finish other than PVA, the old PVA shall be completely removed by wetting and scraping, and the surfaces filled where necessary and rubbed down ready to receive the new finishings",null,0]
[]
[6,10,115,null,"Existing painted plaster surfaces shall be washed down, filled where necessary, spot primed and rubbed down ready to receive new paint.  Existing painted metal surfaces shall be thoroughly rubbed and cleaned down before repainting, but where paint film has blistered or broken down, the paint must be completely removed down to the bare metal.",null,0]
[]
[6,10,115,null,"After cleaning off rust on metalwork, those portions so affected shall be treated with an approved rust inhibitor.  Existing woodwork previously painted shall be washed and rubbed down before repainting, but where the old paint must be completely removed back to the bare surface by the use of a blow lamp or paint removed, and the woodwork knotted, primed, stopped and rubbed down ready to receive new paint.",null,0]
[]
[6,10,115,null,"Care must be taken in burning off old paint not to char or otherwise damage the woodwork, and paint removers used must be free from soda or other caustic substances.  Existing oiled or varnished wood shall be scraped as may be necessary, stopped with tinted stopping and rubbed down and existing woodwork shall be cleaned and similarly stopped and rubbed down.",null,0]
[]
[6,10,115,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 100 Lowsheen (Code:  T2001) paint internally",null,0]
[]
[6,10,115," A","Plastered dry wall partition (\"Pastel\" colour group)","m²",617]
[]
[6,10,116,null,"Clean down existing surfaces, prepare, one coat Dulux Trade Alkali Resistant Primer (Code: T1004) and two coats Dulux Trade 65 Matt PVA (Code:  T2003) paint internally",null,0]
[]
[6,10,116," A","Plastered bulkheads (\"White\" colour group)","m²",50]
[]
[6,10,116,null,"Clean down existing, prepare, one coat Dulux Primer for Wood (Code: D33), one coat Dulux Universal Undercoat (Code: D34) and two coats Dulux Pearlglo Water Based (Code:  D40) paint internally",null,0]
[]
[6,10,116," B","Skirting, cill, etc. not exceeding 300 mm girth","m",85]
[]
[{"$nulls":4},"SECTIONAL SUMMARY",null,0]
[]
[null,null,117,1,"ALTERATIONS AND DEMOLITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,2,"INTERNAL PARTITIONS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,3,"INTERNAL FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,4,"FLOOR FINISHES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,5,"CEILINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,6,"ALUMINIUM WINDOWS AND DOORS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,7,"JOINERY FITTINGS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,8,"SUNDRIES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,9,"PLUMBING AND DRAINAGE",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,117,10,"PAINTING",null,null,{"v":0,"d":"0.00"}]
[]
[7,1,118,null,"SECTION NO. 7",null,0]
[]
[7,1,118,null,"MECHANICAL AND ELECTRICAL  INSTALLATIONS",null,0]
[]
[7,1,118,null,"BILL NO. 1",null,0]
[]
[7,1,118,null,"MECHANICAL AND ELECTRICAL INSTALLATIONS",null,0]
[]
[7,1,118,null,"ELECTRICAL INSTALLATION",null,0]
[]
[7,1,118,null,"For details of this section of the Bills of Quantities please refer to \"C2.2.1 - Electrical Bill of Quantities\" and \"P8081 - Electrical Specifcation\"",null,0]
[]
[7,1,118," A","Electrical subcontract sub-total brought forward from Electrical installation Bill of Quantities - Part C2.2.1 (Value Added Tax excluded)","Item",1]
[]
[7,1,118," B","Profit","%IT"]
[]
[7,1,118," C","Attendance","%IT"]
[]
[7,1,118,null,"HVAC INSTALLATION",null,0]
[]
[7,1,118,null,"For details of this section of the Bills of Quantities please refer to \"C2.2.2 - HVAC Bill of Quantities\" and \"P8081 - HVAC Specifcation\"",null,0]
[]
[7,1,118," D","HVAC subcontract sub-total brought forward from HVAC installation Bill of Quantities - Part C2.2.2 (Value Added Tax excluded)","Item",1]
[]
[7,1,118," E","Profit","%IT"]
[]
[7,1,118," F","Attendance","%IT"]
[]
[7,1,119,null,"SECURITY EQUIPMENT INSTALLATION",null,0]
[]
[7,1,119," A","Subcontract allowance of R3 000 000.00 (Three Million Rand) net for security equipment installation by a Subcontractor approved by the Project Manager","Item",1,{"v":3000000,"d":"3,000,000.00"},{"v":3000000,"d":"3,000,000.00"}]
[]
[7,1,119," B","Profit","%IT"]
[]
[7,1,119," C","Attendance","%IT"]
[]
[7,1,119,null,"CHECK-IN COUNTER EQUIPMENT INSTALLATION",null,0]
[]
[7,1,119," D","Subcontract allowance of R350 000.00 (Three Hundred and Fifty Thousand Rand) net for check-in counter equipment installation by a Subcontractor approved by the Project Manager","Item",1,{"v":350000,"d":"350,000.00"},{"v":350000,"d":"350,000.00"}]
[]
[7,1,119," E","Profit","%IT"]
[]
[7,1,119," F","Attendance","%IT"]
[]
[7,1,119,null,"SMOKE DETECTION INSTALLATION",null,0]
[]
[7,1,119," G","Subcontract allowance of R30 000.00 (Thirty Thousand Rand) net for smoke detection installation by a Subcontractor approved by the Project Manager","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"}]
[]
[7,1,119," H","Profit","%IT"]
[]
[7,1,119," I","Attendance","%IT"]
[]
[7,1,119,null,"CCTV INSTALLATION",null,0]
[]
[7,1,119," J","Subcontract allowance of R220 000.00 (Two Hundred and Twenty Thousand Rand) net for CCTV installation by a Subcontractor approved by the Project Manager","Item",1,{"v":220000,"d":"220,000.00"},{"v":220000,"d":"220,000.00"}]
[]
[7,1,120," A","Profit","%IT"]
[]
[7,1,120," B","Attendance","%IT"]
[]
[7,1,120,null,"DATA NETWORKS INSTALLATION",null,0]
[]
[7,1,120," C","Subcontract allowance of R200 000.00 (Two Hundred Thousand Rand) net for date networks installation by a Subcontractor approved by the Project Manager","Item",1,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"}]
[]
[7,1,120," D","Profit","%IT"]
[]
[7,1,120," E","Attendance","%IT"]
[]
[7,1,120,null,"BUILDERS WORK",null,0]
[]
[7,1,120," F","Budgetary allowance of R100 000.00 (One Hundred Thousand Rand) for builders work as directed by the Project Manager","Item",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"}]
[]
[{"$nulls":4},"FINAL SUMMARY",null,0]
[]
[null,null,121,1,"PRELIMINARIES",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,121,2,"AREA A - EXISTING ABLUTIONS TO SECURITY CHECK-IN",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,121,3,"AREA B - INCREASE PASSENGER CIRCULATION",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,121,4,"AREA C - EXISTING OFFICES TO ONLINE CHECK-IN AREA",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,121,5,"AREA D - ADDITIONAL CHECK-IN COUNTERS",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,121,6,"AREA E - BUSINESS CLASS SECURITY CHECK-IN",null,null,{"v":0,"d":"0.00"}]
[]
[null,null,121,7,"MECHANICAL AND ELECTRICAL INSTALLATIONS",null,null,{"v":0,"d":"0.00"}]
[]
[]
[null,null,121,null,"SUB TOTAL"]
[]
[null,null,121,null,"BUDGETARY ALLOWANCE of R1 350 000.00 (One Million Three Hundred and Fifty Thousand Rand) net for variations and site instructions to be used as directed by the Project Manager or omitted in whole or in part if not required","Item",1,{"v":1350000,"d":"1,350,000.00"},{"v":1350000,"d":"1,350,000.00"}]
[]
[]
[null,null,121,null,"SUB TOTAL"]
[]
[null,null,121,null,"ADD:  15% VALUE ADDED TAX","TAX",{"v":0.15,"d":"15%"}]
[]
[]
[{"$nulls":4},"TOTAL INCLUDING VALUE ADDED TAX"]