{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Abnormal Spec","Scope"],"not_rendered":{"images":2},"read":"whole","date_system":"1900"}

{"sheet":"Abnormal Spec","index":0,"n_rows":72,"n_cols":5,"rows_kept":72,"merged":[[3,1,3,4],[4,2,4,3],[65,0,65,4]]}
[]
[]
[]
["Vehicle Job Description:","ABNORMAL Truck Tractor To handle a Trailer of >110 000Kg <135 000Kg (Mobile Substation)"]
["T10\n ","Annexure A3","Tendering Service Provider to complete",null,"Eskom technical team to complete"]
["Vehicle Type Required:","Abnormal Truck Tractor 6x4  GCM  130 000Kgs","Comply","Provide reason for Comply or non-compliance","Eskom technical evaluation comments"]
["AIR CONDITIONER (Factory Warranty)","To be Standard Factory Fitted"]
["RADIO/CD/BLUETOOTH PRICE FITTED (IF NOT STD)","To be Standard Factory Fitted"]
["SEAT  BELTS: SABS APPROVED","To be Standard Factory Fitted"]
["DRIVER AND PASSENGER SEATBELT REMINDER INDICATOR/ALARM","To be Standard Factory Fitted"]
["EBS BRAKES","To be Standard Factory Fitted"]
["POWER STEERING","To be Standard Factory Fitted"]
["DAY TIME RUNNING LIGHTS INSTALLED","To be Standard Factory Fitted"]
["TWO EMMERGENCY TRIANGLES","To be Standard Factory Fitted"]
["IMMOBILISER (Factory Warranty)","To be Standard Factory Fitted"]
["ALARM (Factory Warranty)","To be Standard Factory Fitted"]
["ENGINE PROTECTION DEVICE( Water level, water temperature,oil pressure etc) ","To be Standard Factory Fitted"]
["TRAILER BRAKE CONTROL","To be Standard Factory Fitted"]
["AIR CHARGE LINE TO THE FRONT","To be Standard Factory Fitted"]
["REVERSE ALARM/BEEPER","To be Standard Factory Fitted"]
["FITTED TOWING/RECOVERY FACILITY ON FRONT","To be Standard Factory Fitted"]
["VEHICLE CONFIGURATION :","Truck tractor"]
["TRACTION: ","6x4"]
["PBS Ready","YES"]
["LED Working lights - 2 fitted facing rear of vehicle","YES"]
["Amber Light (Bar Type)","YES"]
["Brackets To Mount ABNORMAL Sign Board with dual flags, left & right, front of truck tractor","YES"]
["Double bunk sleeper cab","YES"]
["Cooler / fridge","YES"]
["Adjustable double oscillating 5th Wheel To Accommodate a 90mm King Pin","YES"]
["PTO","YES"]
["Walkway on Fuel Tank & rear of cab to access air lines","YES"]
["Adjustable Hydraulic / air bag suspension - Lower & raise vehicle","YES"]
["Liftable Drive Axle","YES"]
["Diesel Powered (Normally aspirated or Turbo)","YES"]
["Fuel Tank Capacity","600l + 200l"]
["Power Rating - Kw","520 to 650"]
["Torque Rating - NM","Manufacturer to specify"]
["Permissible Front axle rating “ Max.”","7700 kg"]
["Permissible Rear axle rating “ Max.”","18000 kg"]
["OEM Front axle rating","OEM to Specify"]
["OEM Rear axle rating","OEM to Specify"]
["D/T Rating “Min.”","130000Kg"]
["Wheel base (Center front axle to center of rear axle unit) (Max)","3890mm"]
["Transmission","Heavy Duty"]
["Crawler Gears","YES"]
["Retarder","YES"]
["Roll Back Brake Assist","YES"]
["Diff Lock","YES"]
["Hub Reduction","YES"]
["Vehicle to be able to pull a trailer of 110000 Kgs to 135000 Kgs","YES"]
["Tyre Size Front ","385/65 R 22.5"]
["Tyre Size Rear ","315/80 R 22.5"]
["Spare wheel should be one of each size (2)","YES"]
["Jost Tow Hitch at rear to accommodate a- frame trailer","YES"]
["All Air Couplings to be fitted with isolating valves","YES"]
["Mud-flaps: Factory fitted","YES"]
["Maintenance Plan (60 Months)","YES, OEM to specify details of plan"]
["Operator training","YES"]
["WARRANTY PERIOD: MONTHS/DISTANCE","OEM to specify"]
["CARBON DIOXIDE (CO2) EMISSION:  g/km","OEM to specify"]
["Acceptance / Acceptance"]
["Name of Evaluator 1: ",null,"Signature :"]
["Name of Evaluator 2: ",null,"Signature :"]
["Name of Verifier  :",null,"Signature :"]
["Any proposed deviations from this specification shall be listed below with reasons for the deviation(s).  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective than that specified by Eskom."]
[]
["Tendering supplier to score 90 in order to be Technically Acceptable"]
["Fully completed questionnaire in Annexure A3 confirming the compliance and non-compliance to the technical specification as well as prove (brochures) for verification of compliance.",50]
["Original Equipment manufacturer (OEM) or Registered dealer, to provide a confirmation letter from Original Equipment manufacturer (OEM)",20]
["Proof of 12 (twelve) month warranty certificate from the Original Equipment manufacturer (OEM)",20]
["Proof of after sales service and repairs (OEM Service Level Agreement) ",10]

{"sheet":"Scope","index":1,"n_rows":1,"n_cols":1,"rows_kept":1}
["The Supply and Delivery of One (1) 6x4 Abnormal Truck Tractor to haul a mobile substation with a GVM of 75 tons. The unit will also be used to transport a Transformer with mass of 90 Tons complete with all accessories as per Eskom’s specifications for Eskom PPM Department, 1 Portland Road, Mkondeni, KZN Operating Unit in the CentralEast Cluster as per the Eskom Technical Specifications."]