{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["LT CB_33_132kV Items List "],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"LT CB_33_132kV Items List ","index":0,"n_rows":66,"n_cols":7,"rows_kept":66,"merged":[[2,4,2,5]],"flags":["formulas_cached_only"]}
[{"$nulls":3},"HV AIS outdoor Live Tank Circuit Breakers for Eskom Transmission"]
[]
[{"$nulls":3},"Live Tank Circuit Breakers - 22 kV to 33 kV COMBO design; 33kV up to 132kV - non-SF6 gas CB's and SF6 CB' including 132 kV 50 kA CB's; Live-tank 132 kV DCB's; Electronic controllers and Online Condition Monitoring","Please indicated with \"X\""]
[null,"Item","Material SAP Number","        Description","Offered (X)","Not Offered (X)","Unit Price"]
[null,1,null,"BKR:CMB;22 KV;2500 A;31.5 KA;3;110 VDC"]
[null,2,null,"BKR:CMB;22 KV;2500 A;31.5 KA;3;220 VDC"]
[null,3,null,"BKR:CMB;33 KV;2500 A;31.5 KA;3;110 VDC"]
[null,4,null,"BKR:CMB;33 KV;2500 A;31.5 KA;3;220 VDC"]
[]
[null,5,null,"33 kV 2500 A 31.5 kA 3P 31 mm/kV 110 VDC non-SF6"]
[null,6,null,"33 kV 2500 A 31.5 kA 3P 31 mm/kV 220 VDC non-SF6"]
[{"$nulls":3},"Deviation Schedule - 33 kV Live-tank SF6-free circuit-breaker 3P offered"]
[{"$nulls":3},"Tools, Spares, Drawings and Summary of Type Test reports/ certificates Schedule for 33 kV Live-tank SF6-free circuit-breaker 3P offered"]
[{"$nulls":3},"33 kV 1600 A 31.5 kA 3P 31 mm/kV 110 VDC"]
[{"$nulls":3},"33 kV 1600 A 31.5 kA 3P 31 mm/kV 220 VDC"]
[null,7,null,"33 kV 2500 A 31.5 kA 3P 31 mm/kV 110 VDC"]
[null,8,null,"33 kV 2500 A 31.5 kA 3P 31 mm/kV 220 VDC"]
[]
[null,9,null,"66 kV 2500 A 31.5 kA 3P 31 mm/kV 110 VDC non-SF6"]
[null,10,null,"66 kV 2500 A 31.5 kA 3P 31 mm/kV 220 VDC non-SF6"]
[null,11,null,"66 kV 3150 A 31.5 kA 3P 31 mm/kV 110 VDC non-SF6"]
[null,12,null,"66 kV 3150 A 31.5 kA 3P 31 mm/kV 220 VDC non-SF6"]
[]
[null,13,null,"66 kV 2500 A 31.5 kA 3P 31 mm/kV 110 VDC"]
[null,14,null,"66 kV 2500 A 31.5 kA 3P 31 mm/kV 220 VDC"]
[null,15,null,"66 kV 3150 A 31.5 kA 3P 31 mm/kV 110 VDC"]
[null,16,null,"66 kV 3150 A 31.5 kA 3P 31 mm/kV 220 VDC"]
[]
[null,17,null,"132 kV 3150 A 40 kA 3P 31 mm/kV 110 VDC non-SF6"]
[null,18,null,"132 kV 3150 A 40 kA 3P 31 mm/kV 220 VDC non-SF6"]
[]
[null,19,null,"132 kV 3150 A 40 kA 3P 31 mm/kV 110 VDC"]
[null,20,null,"132 kV 3150 A 40 kA 3P 31 mm/kV 220 VDC"]
[]
[null,21,null,"132 kV 3150 A 40 kA 1P 31 mm/kV 110 VDC non-SF6"]
[null,22,null,"132 kV 3150 A 40 kA 1P 31 mm/kV 220 VDC non-SF6"]
[null,23,null,"132kV Point on Wave Relay for Controlled Switching Device 110 VDC/ 220 VDC"]
[]
[null,24,null,"132kV 3150A 40kA 1P 31mm/kV 110VDC"]
[null,25,null,"132kV 3150A 40kA 1P 31mm/kV 220VDC"]
[null,26,null,"132kV 3150A 40kA 1P 31mm/kV 110VDC with Controlled Switching Device"]
[null,27,null,"132kV 3150A 40kA 1P 31mm/kV 220VDC with Controlled Switching Device"]
[null,28,null,"132kV Point on Wave Relay for Controlled Switching Device 110 VDC/ 220 VDC"]
[]
[null,29,null,"132kV 3150A 50kA 3P 31mm/kV 110VDC (puffer)"]
[null,30,null,"132kV 3150A 50kA 3P 31mm/kV 220VDC (puffer)"]
[]
[null,31,null,"132 kV 3150 A 50 kA 1P 31 mm/kV 110 VDC"]
[null,32,null,"132 kV 3150 A 50 kA 1P 31 mm/kV 220 VDC"]
[]
[null,33,null,"DCB 132 kV 3150A 40 kA 3P 31 mm/kV 110VDC"]
[null,34,null,"DCB 132 kV 3150A 40 kA 3P 31 mm/kV 220VDC"]
[]
[null,35,null,"DCB 132 kV 3150 A 40 kA 1P 31 mm/kV 110 VDC"]
[null,36,null,"DCB 132 kV 3150 A 40 kA 1P 31 mm/kV 220 VDC"]
[null,37,null,"132kV Point on Wave Relay for Controlled Switching Device 110 VDC/ 220 VDC"]
[]
[null,38,null,"132kV Surge Capacitor used for mitigation of switching overstress on 132 kV CB of the MTS feeders"]
[null,39,null,"Electronic Online Condition Monitoring and/or Integrated Diagnostic Devices"]
[null,40,null,"GAS:340415; SF6;99.9 PCT;CYL 9 KG"]
[null,41,null,"Gas, SF6, 9KG"]
[null,42,null,"GAS: TYPE: SF6; PURITY: 99.993 PCT; CONTAINER: CYL; 20KG."]
[null,43,null,"GAS:SF6;99.9 PCT;CYL 50 KG"]
[null,44,null,"GAS:SF6;99.9 PCT;CYL 63 KG"]
[]
[{"$nulls":3},"Total "]