{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Bills Of Quantities"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Bills Of Quantities","index":0,"n_rows":1326,"n_cols":34,"rows_kept":1326,"flags":["formulas_cached_only"]}
["Item","Description","Uom","Quantity","Rate","Amount","Total","x","Formatted Qty","x","Abstract RecID","x","Lcode","x","x","x","x","x","x","x","x","x","x","x","x","Package","Section","Bill","Trade","Type","ABUm","PayRef"]
[]
[null,"SECTION NO. 1 : PRELIMINARIES",{"$nulls":23},1,1,1,-2,"H"]
[{"$nulls":33},"NOTE:  the column headings a - z must be present for the importer."]
[]
[]
[null,"SECTION NO. 2 : BUILDINGS",{"$nulls":23},1,2,1,3,"H"]
[]
[]
[null,"BILL NO.1 : ALTERATIONS",{"$nulls":23},1,2,1,3,"H"]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":8},1922,null,340,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"View site",{"$nulls":8},1923,null,370,{"$nulls":12},1,2,1,3,"S","0"]
[]
[null,"Before submitting his tender the tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials salvageable from the alterations.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained",{"$nulls":8},1924,null,380,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"General",{"$nulls":8},1925,null,410,{"$nulls":12},1,2,1,3,"S","0"]
[]
[null,"Note to tenderers: The removal, storage ,disposal, etc  of asbestos sheeting, etc to be executed in strict accordance to the bye laws (OHS) regarding same by a specialist asbestos sub-contractor. Prices to include for this.",{"$nulls":8},2498,null,410,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to tenants in the building and to adjoining premises and their tenants. He shall provide proper protection and provide , erect and remove when directed , any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent",{"$nulls":8},1926,null,420,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to remain the property of the employer shall be carefully taken out, temporarily stored",{"$nulls":8},1927,null,430,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to be re-used shall be thoroughly overhauled before refixing including taking off, easing and rehanging, cramping up, re-wedging as required and making good cramps, dowels, etc, and oiling, adjusting and repairing ironmongery  as  necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described . Re-painting or re-varnishing is given separately",{"$nulls":8},1928,null,440,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)",{"$nulls":8},1930,null,490,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"REMOVAL OF EXISTING WORK",{"$nulls":8},1879,null,570,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement",{"$nulls":8},2501,null,610,{"$nulls":12},1,2,1,3,"S","0"]
[]
["1","Stairs and landings","m³",3,null,0,null,null,3,null,2533,null,610,{"$nulls":12},1,2,1,3,"I","3"]
[]
[null,"Taking out and removing doors, windows, etc, including thresholds, sills, etc",{"$nulls":8},1887,null,860,{"$nulls":12},1,2,1,3,"S","0"]
[]
["2","Timber single door and frame, size 813 x 2032mm high","No",4,null,0,null,null,4,null,1888,null,870,{"$nulls":12},1,2,1,3,"I","N"]
[]
["3","Cubicle doors, size 813 x 1900mm high","No",28,null,0,null,null,28,null,2638,null,870,{"$nulls":12},1,2,1,3,"I","N"]
[]
["4","Glazing from steel window 1090 x 430mm high","m²",2,null,0,null,null,2,null,2639,null,910,{"$nulls":12},1,2,1,3,"I","2"]
[]
["5","Single security gate, 925 x 2032mm high","No",4,null,0,null,null,4,null,2149,null,910,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc",{"$nulls":8},1890,null,1080,{"$nulls":12},1,2,1,3,"S","0"]
[]
["6","Corrugated sheet steel roof covering and timber purlins","m²",431,null,0,null,null,431,null,1892,null,1090,{"$nulls":12},1,2,1,3,"I","2"]
[]
["7","Roof insulation","m²",288,null,0,null,null,288,null,2096,null,1090,{"$nulls":12},1,2,1,3,"I","2"]
[]
["8","Fibre cement fascias and bargeboards","m",81,null,0,null,null,81,null,2073,null,1090,{"$nulls":12},1,2,1,3,"I","1"]
[]
["9","Gutters and rainwater pipes","m",333,null,0,null,null,333,null,2072,null,1100,{"$nulls":12},1,2,1,3,"I","1"]
[]
["10","Gypsum plasterboard ceilings, including timber brandering, cornices, etc","m²","  1 026",null,0,null,null,1026,null,1891,null,1140,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Taking out and removing sundry joinery work, fittings, etc",{"$nulls":8},1893,null,1180,{"$nulls":12},1,2,1,3,"S","0"]
[]
["11","Timber skirtings","m",427,null,0,null,null,427,null,2094,null,1200,{"$nulls":12},1,2,1,3,"I","1"]
[]
["12","Timber shelves  2500  x  750  x  750 mm high","No",4,null,0,null,null,4,null,2636,null,1250,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Taking up and removing wood block floor coverings, vinyl floor coverings, carpets, etc and preparing screeds for new floor coverings",{"$nulls":8},1895,null,1340,{"$nulls":12},1,2,1,3,"S","0"]
[]
["13","Vinyl tile floor covering","m²",718,null,0,null,null,718,null,1896,null,1360,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc",{"$nulls":8},1903,null,1500,{"$nulls":12},1,2,1,3,"S","0"]
[]
["14","30mm Screed from floor","m²",49,null,0,null,null,49,null,2531,null,1560,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Taking out and removing sanitary fittings, tanks, geysers, etc, including disconnecting from pipes, traps, etc and making good floor and wall finishes (making good tiling and paintwork elsewhere)",{"$nulls":8},1911,null,1680,{"$nulls":12},1,2,1,3,"S","0"]
[]
["15","Vitreous china wash hand basin","No",2,null,0,null,null,2,null,1912,null,1710,{"$nulls":12},1,2,1,3,"I","N"]
[]
["16","Vitreous china WC pan with cistern and flush pipe","No",23,null,0,null,null,23,null,1913,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
["17","CP star pillar taps","No",1,null,0,null,null,1,null,2137,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Servicing of existing work",{"$nulls":8},2527,null,1720,{"$nulls":12},1,2,1,3,"S","0"]
[]
["18","Investigate and isolate tap leak and repair","No",1,null,0,null,null,1,null,2528,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"PREPARATORY WORK TO EXISTING SURFACES",{"$nulls":8},1914,null,2020,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"MAKING GOOD OF FINISHES ETC",{"$nulls":8},1918,null,2080,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"Making good cement screeds",{"$nulls":8},2662,null,2220,{"$nulls":12},1,2,1,3,"S","0"]
[]
["19","30mm Thick on floors in patches","m²",49,null,0,null,null,49,null,2663,null,2230,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Pavelite steel trowelled on existing screed",{"$nulls":8},1920,null,2230,{"$nulls":12},1,2,1,3,"S"]
[]
["20","Average 4mm thick on floors and landings","m²",718,null,0,null,null,718,null,2074,null,2230,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Wire brush along length of crack and ream open cracks 20mm width x 20mm deep and scratch out any debris that may block the crack in the sides of the hole. Epoxy R8 bars in grooves at 250mm centres over the crack length. Fill the \"V\" grooves and plaster with structural mortar and mesh ref 100.",{"$nulls":8},1934,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["21","On cracks on plastered walls","m",14,null,0,null,null,14,null,1935,null,2230,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Chip open the crack to form a \"V\" shape 20mm wide x 10mm deep and scratch out the debris that may block the crack in the sides of the hole. Grinding in the floor approximately 200mm to 300mm apart from the rebar to be placed into an epoxy repair mortar 'SIKA TOP-ARMATEC 100'. Fill the crack with structural epoxy repair mortar 'SIKA MONO TOP 615HB'",{"$nulls":8},1936,null,2230,{"$nulls":12},1,2,1,3,"S"]
[]
["22","On cracks on concrete floors, walkways, etc","m",35,null,0,null,null,35,null,1937,null,2230,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Resealing of joints",{"$nulls":8},2530,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["23","Ream out joint and install UV resistant polysulphide sealant","m",149,null,0,null,null,149,null,2529,null,2230,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Pressure cleaning existing buildings",{"$nulls":8},1932,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["24","External facebrick","m²",959,null,0,null,null,959,null,1933,null,2230,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"BUDGETARY ALLOWANCE",{"$nulls":8},1921,null,2470,{"$nulls":12},1,2,1,3,"H","0"]
[]
["25","Allow a budgetary amount of R200 000.00 for Remedial Works","Item",null,{"v":200000,"d":"200,000.00"},{"v":200000,"d":"200,000.00"},null,null,1,null,1931,null,2470,{"$nulls":12},1,2,1,3,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},{"v":200000,"d":"200,000.00"}]
[]
[]
[]
[null,"BILL NO.2 : EARTHWORKS",{"$nulls":23},1,2,2,6,"H"]
[]
[null,"EARTHWORKS (PROVISIONAL)",{"$nulls":8},2443,null,2500,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"EXCAVATION, FILLING, ETC OTHER THAN BULK",{"$nulls":8},2444,null,6450,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Excavation in earth not exceeding 2m deep",{"$nulls":8},2445,null,8560,{"$nulls":12},1,2,2,6,"S","0"]
[]
["1","Reduced levels under floors","m³","  1 149",null,0,null,null,1149,null,2505,null,8900,{"$nulls":12},1,2,2,6,"I","3"]
[]
["2","Trenches","m³",503,null,0,null,null,503,null,2564,null,8910,{"$nulls":12},1,2,2,6,"I","3"]
[]
["3","Holes","m³",3,null,0,null,null,3,null,2584,null,8910,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Extra over bulk excavations in earth for excavation in",{"$nulls":8},2447,null,9360,{"$nulls":12},1,2,2,6,"S","0"]
[]
["4","Soft rock","m³",57,null,0,null,null,57,null,2448,null,9370,{"$nulls":12},1,2,2,6,"I","3"]
[]
["5","Intermediate rock.","m³",57,null,0,null,null,57,null,2449,null,9380,{"$nulls":12},1,2,2,6,"I","3"]
[]
["6","Hard rock","m³",28,null,0,null,null,28,null,2614,null,9370,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Back excavation of vertical sides of excavations in earth for working space including backfilling compacted to ?% Mod AASHTO density",{"$nulls":8},2450,null,9430,{"$nulls":12},1,2,2,6,"S","0"]
[]
["7","Not exceeding 500mm deep for placing and removing formwork to walls etc, ?mm away from excavated face","m²",719,null,0,null,null,719,null,2451,null,9440,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"Extra over all excavations for carting away",{"$nulls":8},2452,null,9620,{"$nulls":12},1,2,2,6,"S","0"]
[]
["8","Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m³",746,null,0,null,null,746,null,2453,null,9630,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Risk of collapse of excavations",{"$nulls":8},2455,null,7380,{"$nulls":12},1,2,2,6,"S","0"]
[]
["9","Sides of excavations not exceeding 1,5m deep","m²","  1 438",null,0,null,null,1438,null,2456,null,7390,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"Keeping excavations free of water",{"$nulls":8},2462,null,9700,{"$nulls":12},1,2,2,6,"S","0"]
[]
["10","Keeping excavations free of all water other than subterranean water","Item",1,null,0,null,null,1,null,2463,null,9710,{"$nulls":12},1,2,2,6,"I","I"]
[]
[null,"FILLING, ETC",{"$nulls":8},2507,null,7480,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 95% Mod AASHTO density",{"$nulls":8},2508,null,7570,{"$nulls":12},1,2,2,6,"S","0"]
[]
["11","Under floors, steps, pavings, etc","m³",243,null,0,null,null,243,null,2509,null,9770,{"$nulls":12},1,2,2,6,"I","3"]
[]
["12","Backfilling to trenches, holes, etc.","m³",68,null,0,null,null,68,null,2560,null,9770,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Filling of G7 supplied by the contractor, compacted to 95% Mod AASHTO density",{"$nulls":8},2567,null,7610,{"$nulls":12},1,2,2,6,"S","0"]
[]
["13","Backfilling to trenches, holes, etc","m³",169,null,0,null,null,169,null,2568,null,7610,{"$nulls":12},1,2,2,6,"I","3"]
[]
["14","Under floors, steps, paving, etc.","m³",243,null,0,null,null,243,null,2583,null,7610,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Filling of coarse river sand supplied by the contractor, consolidated",{"$nulls":8},2580,null,7830,{"$nulls":12},1,2,2,6,"S","0"]
[]
["15","Under floors etc","m³",51,null,0,null,null,51,null,2581,null,7840,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Compaction of ground surfaces",{"$nulls":8},2514,null,7940,{"$nulls":12},1,2,2,6,"S","0"]
[]
["16","Compaction of natural or excavated ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to ?% Mod AASHTO density","m²","  1 799",null,0,null,null,1799,null,2515,null,7960,{"$nulls":12},1,2,2,6,"I","2"]
[]
["17","Bottoms of trenches, holes, etc","m²",503,null,0,null,null,503,null,2570,null,7960,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"WEED KILLERS, INSECTICIDES, ETC",{"$nulls":8},2516,null,8390,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Soil insecticide in accordance with SANS 5859",{"$nulls":8},2517,null,8440,{"$nulls":12},1,2,2,6,"S","0"]
[]
["18","Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m²","  1 799",null,0,null,null,1799,null,2518,null,8450,{"$nulls":12},1,2,2,6,"I","2"]
[]
["19","To bottoms and sides of trenches etc","m²","  1 941",null,0,null,null,1941,null,2569,null,8460,{"$nulls":12},1,2,2,6,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.3 : CONCRETE, FORMWORK AND REINFORCEMENT",{"$nulls":23},1,2,3,15,"H"]
[]
[null,"UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES",{"$nulls":8},2474,null,16890,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"15Mpa/19mm concrete",{"$nulls":8},2475,null,81590,{"$nulls":12},1,2,3,15,"S","0"]
[]
["1","Surface blinding under footings","m³",25,null,0,null,null,25,null,2476,null,81630,{"$nulls":12},1,2,3,15,"I","3"]
[]
[null,"REINFORCED CONCRETE",{"$nulls":8},1685,null,2660,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"25 Mpa/19mm Concrete:",{"$nulls":8},1811,null,2660,{"$nulls":12},1,2,3,15,"S","0"]
[]
["2","Strip footings","m³",126,null,0,null,null,126,null,2565,null,2671,{"$nulls":12},1,2,3,15,"I","3"]
[]
["3","Surface beds on waterproofing","m³",276,null,0,null,null,276,null,2579,null,2671,{"$nulls":12},1,2,3,15,"I","3"]
[]
["4","Thickenings, size 600 x 400mm","m",185,null,0,null,null,185,null,1710,null,2671,{"$nulls":12},1,2,3,15,"I","1"]
[]
["5","Stairs, including landings, beams, etc","m³",2,null,0,null,null,2,null,2664,null,2671,{"$nulls":12},1,2,3,15,"I","3"]
[]
[null,"TEST BLOCKS",{"$nulls":8},2606,null,2671,{"$nulls":12},1,2,3,15,"H","0"]
[]
["6","Making and testing set of three 150 x 150 x 150mm concrete strength test cubes.","Sets",28,null,0,null,null,28,null,90,null,2926,{"$nulls":12},1,2,3,15,"I","S"]
[]
[null,"CONCRETE SUNDRIES",{"$nulls":8},2519,null,17960,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Finishing top surfaces of concrete smooth with a wood float",{"$nulls":8},2520,null,18110,{"$nulls":12},1,2,3,15,"S","0"]
[]
["7","Surface beds, slabs, etc","m²",298,null,0,null,null,298,null,2521,null,18120,{"$nulls":12},1,2,3,15,"I","2"]
[]
[null,"ROUGH FORMWORK (DEGREE OF ACCURACY II)",{"$nulls":8},91,null,3857,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Rough Formwork to Sides:",{"$nulls":8},92,null,3861,{"$nulls":12},1,2,3,15,"S","0"]
[]
["8","Footings","m","  1 438",null,0,null,null,1438,null,93,null,3928,{"$nulls":12},1,2,3,15,"I","1"]
[]
["9","Edges, risers, ends and reveals not exceeding 300mm high or wide.","m",104,null,0,null,null,104,null,2665,null,3928,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"MOVEMENT JOINTS ETC",{"$nulls":8},105,null,9632,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Slip joints with three layers of damp proof sheeting between horizontal concrete and brick surfaces including cement mortar bed:",{"$nulls":8},106,null,9634,{"$nulls":12},1,2,3,15,"S","0"]
[]
["10","Not exceeding 300mm wide.","m",34,null,0,null,null,34,null,107,null,9636,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"Expansion joints with bitumen emulsion paint between horizontal concrete and brick surfaces:",{"$nulls":8},110,null,9641,{"$nulls":12},1,2,3,15,"S","0"]
[]
["11","Joints not exceeding 300mm high.","m",722,null,0,null,null,722,null,111,null,9643,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"Saw cut joints:",{"$nulls":8},112,null,9645,{"$nulls":12},1,2,3,15,"S","0"]
[]
["12","3 x 25mm Saw cut joints in two operations in top of concrete.","m",220,null,0,null,null,220,null,113,null,9646,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"REINFORCEMENT",{"$nulls":8},116,null,9660,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Mild steel reinforcement to structural concrete work:",{"$nulls":8},117,null,9662,{"$nulls":12},1,2,3,15,"S","0"]
[]
["13","Bars of varying diameters.","Tonnes",12,null,0,null,null,12,null,2615,null,9663,{"$nulls":12},1,2,3,15,"I","T"]
[]
[null,"High tensile steel reinforcement to structural concrete work:",{"$nulls":8},2667,null,9663,{"$nulls":12},1,2,3,15,"S"]
[]
["14","Bars of varying diameters.","Tonnes",5,null,0,null,null,5,null,2666,null,9663,{"$nulls":12},1,2,3,15,"I","T"]
[]
[null,"Fabric reinforcement:",{"$nulls":8},121,null,9703,{"$nulls":12},1,2,3,15,"S","0"]
[]
["15","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m²","  1 799",null,0,null,null,1799,null,123,null,9704,{"$nulls":12},1,2,3,15,"I","2"]
[]
[null,"Test blocks:",{"$nulls":8},89,null,2925,{"$nulls":12},1,2,3,15,"S","0"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.4 : MASONRY",{"$nulls":23},1,2,4,21,"H"]
[]
[null,"BRICKWORK IN FOUNDATIONS (PROVISIONAL)",{"$nulls":8},2571,null,28790,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive strength) in class II mortar",{"$nulls":8},2572,null,94630,{"$nulls":12},1,2,4,21,"S","0"]
[]
["1","One brick walls","m²",597,null,0,null,null,597,null,2573,null,94880,{"$nulls":12},1,2,4,21,"I","2"]
[]
[null,"Fair face to brickwork of selected building bricks in horizontal stretcher bond pointed with flush horizontal and vertical joints",{"$nulls":8},2574,null,29690,{"$nulls":12},1,2,4,21,"S","0"]
[]
["2","Extra over for fair face","m²",206,null,0,null,null,206,null,2575,null,84870,{"$nulls":12},1,2,4,21,"I","2"]
[]
[null,"2,5mm Brickwork reinforcement",{"$nulls":8},2576,null,29890,{"$nulls":12},1,2,4,21,"S","0"]
[]
["3","150mm Wide reinforcement built in horizontally","m","  2 388",null,0,null,null,2388,null,2577,null,84900,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"BRICKWORK IN SUPERSTRUCTURE",{"$nulls":8},124,null,10216,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Brickwork in NFP bricks in  Class II mortar:",{"$nulls":8},125,null,46684,{"$nulls":12},1,2,4,21,"S","0"]
[]
["4","Piers.","m³",{"v":0.5,"d":"1"},null,0,null,null,0.5,null,126,null,51267,{"$nulls":12},1,2,4,21,"I","3"]
[]
["5","Half brick walls.","m²",204,null,0,null,null,204,null,127,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["6","Half brick walls in beamfilling.","m²",108,null,0,null,null,108,null,130,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["7","Half brick walls in hollow column.","m²",10,null,0,null,null,10,null,2619,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["8","One brick walls","m²",579,null,0,null,null,579,null,2592,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["9","One brick walls (firewalls)","m²",147,null,0,null,null,147,null,2650,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["10","One brick walls of two half brick skins bagged and sealed.","m²","  1 037",null,0,null,null,1037,null,133,null,51287,{"$nulls":12},1,2,4,21,"I","2"]
[]
["11","One brick walls of two half brick skins bagged and sealed (gable walls).","m²",47,null,0,null,null,47,null,134,null,51287,{"$nulls":12},1,2,4,21,"I","2"]
[]
["12","One and half brick walls","m²",11,null,0,null,null,11,null,2617,null,51287,{"$nulls":12},1,2,4,21,"I","2"]
[]
[null,"BRICKWORK SUNDRIES",{"$nulls":8},144,null,10546,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Brickwork reinforcement:",{"$nulls":8},148,null,10596,{"$nulls":12},1,2,4,21,"S","0"]
[]
["13","75mm Wide reinforcement built in horizontally.","m",902,null,0,null,null,902,null,149,null,10597,{"$nulls":12},1,2,4,21,"I","1"]
[]
["14","150mm Wide reinforcement built in horizontally.","m","  7 412",null,0,null,null,7412,null,150,null,10598,{"$nulls":12},1,2,4,21,"I","1"]
[]
["15","225mm Wide reinforcement built in horizontally.","m",40,null,0,null,null,40,null,2618,null,10598,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Prestressed concrete fabricated lintels:",{"$nulls":8},151,null,10602,{"$nulls":12},1,2,4,21,"S","0"]
[]
["16","90 x 114mm Lintels laid side by side in lengths not exceeding 3m.","m",324,null,0,null,null,324,null,152,null,10603,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Turning pieces:",{"$nulls":8},154,null,10609,{"$nulls":12},1,2,4,21,"S","0"]
[]
["17","110mm Wide turning piece to lintels etc.","m",167,null,0,null,null,167,null,155,null,10610,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Galvanised hoop iron cramps, ties, etc:",{"$nulls":8},156,null,10614,{"$nulls":12},1,2,4,21,"S","0"]
[]
["18","30 x 1,6mm Roof tie 1,5m long with one end fixed to timber and other end built into brickwork.","No",260,null,0,null,null,260,null,157,null,10619,{"$nulls":12},1,2,4,21,"I","N"]
[]
[null,"Air bricks etc:",{"$nulls":8},158,null,10622,{"$nulls":12},1,2,4,21,"S","0"]
[]
["19","Set of two Terra-cotta 229 x 152mm clay vermin proof air bricks.","No",16,null,0,null,null,16,null,159,null,10625,{"$nulls":12},1,2,4,21,"I","N"]
[]
[null,"FACE BRICKWORK",{"$nulls":8},160,null,10629,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Corobrik Ruby Light Satin FBS or Equivalent/similar approved face bricks pointed with recessed horizontal and vertical joints:",{"$nulls":8},161,null,51530,{"$nulls":12},1,2,4,21,"S","0"]
[]
["20","Extra over brickwork for face brickwork externally.","m²","  1 072",null,0,null,null,1072,null,162,null,51531,{"$nulls":12},1,2,4,21,"I","2"]
[]
["21","Extra over brickwork for face brickwork internally (dado) 0.94m high.","m²",350,null,0,null,null,350,null,2620,null,51531,{"$nulls":12},1,2,4,21,"I","2"]
[]
["22","Extra over brickwork for face brickwork externally in gabbles.","m²",47,null,0,null,null,47,null,165,null,51531,{"$nulls":12},1,2,4,21,"I","2"]
[]
["23","Extra over brickwork for face brickwork in beamfilling.","m²",108,null,0,null,null,108,null,166,null,51531,{"$nulls":12},1,2,4,21,"I","2"]
[]
["24","Extra over brickwork for brick-on-edge header course lintel pointed on one face and 220mm soffit.","m",228,null,0,null,null,228,null,169,null,51546,{"$nulls":12},1,2,4,21,"I","1"]
[]
["25","Fair raking cutting.","m",81,null,0,null,null,81,null,171,null,51546,{"$nulls":12},1,2,4,21,"I","1"]
[]
["26","Fair splay cutting.","m",137,null,0,null,null,137,null,172,null,51546,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Brick-on-edge header course copings, sills, etc of Corobrik Ruby Light Satin SBS face bricks, pointed with flush joints on all exposed faces",{"$nulls":8},2598,null,30580,{"$nulls":12},1,2,4,21,"S","0"]
[]
["27","170 mm Wide sills set sloping and slightly projecting","m",177,null,0,null,null,177,null,2599,null,30660,{"$nulls":12},1,2,4,21,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.5 : WATERPROOFING",{"$nulls":23},1,2,5,24,"H"]
[]
[null,"DAMPPROOFING OF WALLS AND FLOORS",{"$nulls":8},178,null,11302,{"$nulls":12},1,2,5,24,"H","0"]
[]
[null,"Brikgrip SABS approved DPC embossed damp proof course:",{"$nulls":8},179,null,11306,{"$nulls":12},1,2,5,24,"S","0"]
[]
["1","In walls","m²",216,null,0,null,null,216,null,2578,null,11307,{"$nulls":12},1,2,5,24,"I","2"]
[]
["2","In walls under cills.","m²",206,null,0,null,null,206,null,181,null,11307,{"$nulls":12},1,2,5,24,"I","2"]
[]
[null,"One layer of 250 micron Consol Plastics Gunplas USB Green waterproof sheeting sealed at laps with Gunplas Pressure Sensitive Tape:",{"$nulls":8},2478,null,11307,{"$nulls":12},1,2,5,24,"S","0"]
[]
["3","Under surface beds.","m²","  1 799",null,0,null,null,1799,null,2479,null,11307,{"$nulls":12},1,2,5,24,"I","2"]
[]
[null,"FLASHINGS ETC.",{"$nulls":8},1391,null,40213,{"$nulls":12},1,2,5,24,"H","0"]
[]
[null,"One coat primer and three coats SABS approved acrylic emulsion.",{"$nulls":8},1392,null,85961,{"$nulls":12},1,2,5,24,"S","0"]
[]
["4","Bandage flashing 300mm wide.","m",132,null,0,null,null,132,null,1393,null,85967,{"$nulls":12},1,2,5,24,"I","1"]
[]
[null,"JOINT SEALANTS ETC",{"$nulls":8},188,null,11582,{"$nulls":12},1,2,5,24,"H","0"]
[]
[null,"Approved clear silicone sealant:",{"$nulls":8},189,null,37239,{"$nulls":12},1,2,5,24,"S","0"]
[]
["5","In joints between steel frames and walls","m",887,null,0,null,null,887,null,190,null,37240,{"$nulls":12},1,2,5,24,"I","1"]
[]
[null,"Two - part polysulphide sealing compound including backing cord, bond breaker, primer, etc",{"$nulls":8},191,null,37254,{"$nulls":12},1,2,5,24,"S","0"]
[]
["6","3 x 25 mm In saw cut joints in floors.","m",286,null,0,null,null,286,null,192,null,37255,{"$nulls":12},1,2,5,24,"I","1"]
[]
["7","10 x 10mm In expansion / seperation joints in floors including raking out expansion joint filler as necessary.","m",722,null,0,null,null,722,null,2477,null,37255,{"$nulls":12},1,2,5,24,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.6 : ROOF COVERINGS",{"$nulls":23},1,2,6,27,"H"]
[]
[null,"RIBBED METAL SHEETING AND ACCESSORIES",{"$nulls":8},195,null,12196,{"$nulls":12},1,2,6,27,"H","0"]
[]
[null,"Safintra Saflok 700 AZ 200 0.55mm thick concealed",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[null,"fixing roof sheeting with Colorplus pre-painted white",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[null,"finish fixed to steel purlins at about 1600mm centres",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[null,"in accordance with manufacturers instruction",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[]
["1","Roof covering with pitch not exceeding 25 degrees, in transportable lengths not exceeding 20m.","m²","  1 943",null,0,null,null,1943,null,197,null,41889,{"$nulls":12},1,2,6,27,"I","2"]
[]
[null,"Flashings:",{"$nulls":8},198,null,41725,{"$nulls":12},1,2,6,27,"S","0"]
[]
["2","Ridge capping 462mm girth, three times bent along girth and notched on site to suit roof profile.","m",225,null,0,null,null,225,null,199,null,41728,{"$nulls":12},1,2,6,27,"I","1"]
[]
["3","Polyclosers to suite profile of sheeting.","m",900,null,0,null,null,900,null,202,null,41739,{"$nulls":12},1,2,6,27,"I","1"]
[]
["4","Ridge end cap","No",12,null,0,null,null,12,null,203,null,41739,{"$nulls":12},1,2,6,27,"I","N"]
[]
[null,"ROOF AND WALL LINING AND INSULATION",{"$nulls":8},204,null,12278,{"$nulls":12},1,2,6,27,"H","0"]
[]
[null,"Super Sisalation® Heavy Industrial Grade 430 - Double sided reflective foil laminate incorporating layers of kraft paper and reinforcing scrim, laminated together with low density polyethylene (293gsm).",{"$nulls":8},205,null,59216,{"$nulls":12},1,2,6,27,"S","0"]
[]
["5","Insulation laid taut over timber rafters (at approximately 1200mm centres) and fixed concurrent with tiling battens, purlins, etc.","m²","  1 741",null,0,null,null,1741,null,206,null,59217,{"$nulls":12},1,2,6,27,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.7 : CARPENTRY AND JOINERY",{"$nulls":23},1,2,7,30,"H"]
[]
[null,"PREFABRICATED ROOF TRUSSES, ETC.",{"$nulls":8},2544,null,12364,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Prefabricated plate nailed timber roof truss construction:",{"$nulls":8},2543,null,12364,{"$nulls":12},1,2,7,30,"S","0"]
[]
["1","Double pitch roof truss with a clear span of 7400mm rising 1400mm to apex with a 750mm eaves overhang on both sides.","No",25,null,0,null,null,25,null,2545,null,12364,{"$nulls":12},1,2,7,30,"I","N"]
[]
["2","Double pitch roof truss with a clear span of 7920mm rising 1400mm to apex with a 750mm eaves overhang on both sides.","No",158,null,0,null,null,158,null,2607,null,12364,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"ROOF CONSTRUCTION",{"$nulls":8},215,null,12364,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Sawn softwood :",{"$nulls":8},216,null,12366,{"$nulls":12},1,2,7,30,"S","0"]
[]
["3","38 x 114mm Wall plates","m",355,null,0,null,null,355,null,2493,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["4","38 x 114mm Bracings.","m",355,null,0,null,null,355,null,2546,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["5","38 x 114mm Sprockets.","m",16,null,0,null,null,16,null,2547,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["6","50 x 76mm Purlins.","m","  1 423",null,0,null,null,1423,null,223,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["7","50 x 76mm Trimmer batten.","m",276,null,0,null,null,276,null,2551,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["8","50 x 76mm Gable trim.","m",99,null,0,null,null,99,null,2552,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"Wrought softwood:",{"$nulls":8},226,null,12402,{"$nulls":12},1,2,7,30,"S","0"]
[]
["9","70 x 56mm wrought splayed purlins.","m",355,null,0,null,null,355,null,229,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"LAMINATED TIMBER",{"$nulls":8},2608,null,12372,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Wrought softwood Grade 5:",{"$nulls":8},2609,null,12372,{"$nulls":12},1,2,7,30,"S","0"]
[]
["10","50 x 220mm Beams bolted.","m",290,null,0,null,null,290,null,2610,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"ROOF SUNDRIES",{"$nulls":8},233,null,12452,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Sundries:",{"$nulls":8},234,null,12454,{"$nulls":12},1,2,7,30,"S","0"]
[]
["11","Two coats creosote on sawn timbers.","m²",275,null,0,null,null,275,null,236,null,12456,{"$nulls":12},1,2,7,30,"I","2"]
[]
["12","300mm Long wrought end to 50 x 75mm sawn timber.","No",80,null,0,null,null,80,null,2611,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["13","600mm Long wrought end to 50 X 75mm sawn timber.","No",105,null,0,null,null,105,null,237,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["14","840mm Long wrought end to 50 X 75mm sawn timber.","No",50,null,0,null,null,50,null,2621,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["15","2500mm Long wrought and splay cut end to 38 x 114mm sawn timber.","No",105,null,0,null,null,105,null,2612,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["16","Teco rafter / beam connector.","No",478,null,0,null,null,478,null,2613,null,12459,{"$nulls":12},1,2,7,30,"I","N"]
[]
["17","2,5mm Diameter galvanised wire tie 400mm girth wrapped around rafter and purlin with ends tied together.","No","  1 040",null,0,null,null,1040,null,242,null,12461,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"EAVES, VERGES, ETC",{"$nulls":8},243,null,12463,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Pressed fibre-cement:",{"$nulls":8},244,null,12507,{"$nulls":12},1,2,7,30,"S","0"]
[]
["18","12 x 225mm  Medium density fascia boards including galvanised steel H-profile jointing strips.","m",479,null,0,null,null,479,null,245,null,12513,{"$nulls":12},1,2,7,30,"I","1"]
[]
["19","12 x 80 x 200mm Medium density angle section bargeboards including galvanised steel H-profile jointing strips.","m",140,null,0,null,null,140,null,246,null,12513,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"NUTEC-CEMENT/FIBRE-CEMENT WINDOW SILLS",{"$nulls":8},247,null,61610,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Natural grey sills in single lengths bedded in class II",{"$nulls":8},248,null,63446,{"$nulls":12},1,2,7,30,"S","0"]
[null,"mortar including metal fixing lugs etc",{"$nulls":8},248,null,63446,{"$nulls":12},1,2,7,30,"S","0"]
[]
["20","Everite Nutec window external sills 15 x 150mm wide set",{"$nulls":8},249,null,63448,{"$nulls":12},1,2,7,30,"I","1"]
[null,"flat and slightly projecting","m",152,null,0,null,null,152,null,249,null,63448,{"$nulls":12},1,2,7,30,"I","1"]
[]
["21","Everite Nutec window internal sills 15 x 150mm wide set",{"$nulls":8},2635,null,63448,{"$nulls":12},1,2,7,30,"I","1"]
[null,"flat and slightly projecting","m",26,null,0,null,null,26,null,2635,null,63448,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"SKIRTINGS",{"$nulls":8},250,null,12538,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Wrought meranti:",{"$nulls":8},251,null,12550,{"$nulls":12},1,2,7,30,"S","0"]
[]
["22","19 x 70mm Skirting including 19mm quadrant bead.","m","  1 468",null,0,null,null,1468,null,252,null,12558,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"FRAMED DOORS, ETC",{"$nulls":8},2600,null,12558,{"$nulls":12},1,2,7,30,"H"]
[]
[null,"Blaco wrought saligna doors hung to steel frames:",{"$nulls":8},2601,null,12558,{"$nulls":12},1,2,7,30,"S","0"]
[]
["23","40mm Framed ledged and braced batten door 813 x 2032mm","No",49,null,0,null,null,49,null,2602,null,12558,{"$nulls":12},1,2,7,30,"I","N"]
[]
["24","40mm Framed ledged and braced batten door 813 x 2032mm (cut 100mm high)","No",33,null,0,null,null,33,null,2642,null,12558,{"$nulls":12},1,2,7,30,"I","N"]
[]
["25","40mm Framed ledged and braced batten door 900x 2032mm (Paraplegic).","No",1,null,0,null,null,1,null,2603,null,12558,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"SEMI SOLID CORE FLUSH DOORS",{"$nulls":8},257,null,45924,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Flush doors with hardboard covering on both sides with hardwood finger-jointed stiles hung to steel frames:",{"$nulls":8},258,null,46432,{"$nulls":12},1,2,7,30,"S","0"]
[]
["26","40mm Door 1500 x 2032mm high (BIC).","No",2,null,0,null,null,2,null,260,null,46434,{"$nulls":12},1,2,7,30,"I","N"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.8 : CEILINGS PARTITIONS AND ACCESS FLOORING",{"$nulls":23},1,2,8,33,"H"]
[]
[null,"NAILED UP AND SCREW UP CEILINGS",{"$nulls":8},263,null,13420,{"$nulls":12},1,2,8,33,"H","0"]
[]
[null,"6,4mm 'Rhinoboard' M-Strip ceiling fixed print side up to brandering with 32mm galvanized clout nails or 32mm grabber screws at 150mm centers with 'M-Strip' cover strips over joints with all nail or screw heads stopped and sanded level, all in strict accordance with the manufacturer's instructions:",{"$nulls":8},264,null,49613,{"$nulls":12},1,2,8,33,"S","0"]
[]
["1","Ceilings including 50 x 50 mm sawn softwood brandering at 400mm centres in one direction only to trusses (elsewhere) at 1,5mm centres.","m²","  2 270",null,0,null,null,2270,null,265,null,49615,{"$nulls":12},1,2,8,33,"I","2"]
[]
["2","Extra over ceiling for 600 x 600mm trap door.","No",18,null,0,null,null,18,null,266,null,49629,{"$nulls":12},1,2,8,33,"I","N"]
[]
[null,"Wrot softwood cornices",{"$nulls":8},267,null,49319,{"$nulls":12},1,2,8,33,"S","0"]
[]
["3","19 x 44mm Cornice nailed","m","  1 685",null,0,null,null,1685,null,268,null,49320,{"$nulls":12},1,2,8,33,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.9 : FLOOR COVERINGS",{"$nulls":23},1,2,9,36,"H"]
[]
[null,"VINYL FLOOR COVERINGS, WALL LININGS, ETC.",{"$nulls":8},270,null,41329,{"$nulls":12},1,2,9,36,"H","0"]
[]
[null,"All vinyl flooring materials require a smooth, hard, clean, true and level surface, not only for appearance but also for achieving a satisfactory adhesive bond and long term durability",{"$nulls":8},1702,null,41329,{"$nulls":12},1,2,9,36,"C","0"]
[]
[null,"The main contractor shall ensure that the sub-floor is acceptable to receive the vinyl flooring specified in respect of levelness, smoothness, soundness and cleanness",{"$nulls":8},1703,null,41329,{"$nulls":12},1,2,9,36,"C","0"]
[]
[null,"300 x 300 x  2,5mm Thick hard wearing  semi-flexible vinyl floor tiles fixed with 'Marley No.60 Acrylic Adhesive':",{"$nulls":8},271,null,41336,{"$nulls":12},1,2,9,36,"S","0"]
[]
["1","On floors.","m²","  2 019",null,0,null,null,2019,null,272,null,41337,{"$nulls":12},1,2,9,36,"I","2"]
[]
[null,"POLISH, SEALERS, ETC",{"$nulls":8},273,null,14681,{"$nulls":12},1,2,9,36,"H","0"]
[]
[null,"Polish, sealers, etc:",{"$nulls":8},274,null,14683,{"$nulls":12},1,2,9,36,"S","0"]
[]
["2","Two coats wax polish on vinyl flooring.","m²","  2 019",null,0,null,null,2019,null,275,null,14684,{"$nulls":12},1,2,9,36,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.10 : IRONMONGERY",{"$nulls":23},1,2,10,39,"H"]
[]
[null,"IRONMONGERY",{"$nulls":8},2138,null,46520,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"LOCKS",{"$nulls":8},2480,null,46950,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by Union",{"$nulls":8},2605,null,46950,{"$nulls":12},1,2,10,39,"S","0"]
[]
["1","40mm Padlock (gate)","No",22,null,0,null,null,22,null,2604,null,47011,{"$nulls":12},1,2,10,39,"I","N"]
[]
["2","65mm Padlock (trap door)","No",8,null,0,null,null,8,null,2482,null,47011,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Manufactured by Geze",{"$nulls":8},2481,null,47010,{"$nulls":12},1,2,10,39,"S","0"]
[]
["3","Ref 730/68 - 76 mm Profile arch sashlock S/S","No",49,null,0,null,null,49,null,2483,null,47169,{"$nulls":12},1,2,10,39,"I","N"]
[]
["4","Ref  880-66/78 - 5 Pin NP Double cylinder 66mm 3K N.PL","No",49,null,0,null,null,49,null,2484,null,47173,{"$nulls":12},1,2,10,39,"I","N"]
[]
["5","Ref AZ2001SR TS2000VP DCL with P/ARM BRACKET SR","No",33,null,0,null,null,33,null,2668,null,47173,{"$nulls":12},1,2,10,39,"I","N"]
[]
["6","Master key","No",4,null,0,null,null,4,null,2486,null,47183,{"$nulls":12},1,2,10,39,"I","N"]
[]
["7","Grand master key","No",4,null,0,null,null,4,null,2487,null,47184,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"HANDLES",{"$nulls":8},2111,null,47490,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by Geze",{"$nulls":8},2112,null,47500,{"$nulls":12},1,2,10,39,"S","0"]
[]
["8","Ref EDE/101C-Daytona19mm/165X165X1.5/PL.CYL","No",49,null,0,null,null,49,null,2485,null,47501,{"$nulls":12},1,2,10,39,"I","N"]
[]
["9","Ref 295/01 - Helping hand L/H OR R/H","No",3,null,0,null,null,3,null,2488,null,47501,{"$nulls":12},1,2,10,39,"I","N"]
[]
["10","Ref JD213/305 - B/T S.S P/hand 330X305X25mm","No",4,null,0,null,null,4,null,2489,null,47501,{"$nulls":12},1,2,10,39,"I","N"]
[]
["11","Ref 075/160/B - 075/160 -BT P/H 111X19 ON 160X160 BPL SS","No",33,null,0,null,null,33,null,2669,null,47501,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"PUSH PLATES AND KICK PLATES",{"$nulls":8},2114,null,47590,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by 'Geze'",{"$nulls":8},2115,null,47650,{"$nulls":12},1,2,10,39,"S","0"]
[]
["12","160 x 160mm stainless steel push  plate","No",3,null,0,null,null,3,null,2116,null,47651,{"$nulls":12},1,2,10,39,"I","N"]
[]
["13","813 x 20mm stainless steel kick plate","No",3,null,0,null,null,3,null,2117,null,47652,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"DOOR CLOSERS",{"$nulls":8},290,null,14985,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Dorma:",{"$nulls":8},291,null,15002,{"$nulls":12},1,2,10,39,"S","0"]
[]
["14","TS91' Overhead door closer with bracket fixed to metal","No",2,null,0,null,null,2,null,292,null,15003,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"LETTERS, NAMEPLATES, ETC.",{"$nulls":8},293,null,15017,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by 'Geze'",{"$nulls":8},294,null,15019,{"$nulls":12},1,2,10,39,"S","0"]
[]
["15","90 x 32 x 3mm Thick perspex plate with 25mm high engraved and painted letters or numerals.","No",2,null,0,null,null,2,null,295,null,15022,{"$nulls":12},1,2,10,39,"I","N"]
[]
["16","Ref 079/160E-S/ST P/PL 160 x 160 x 1.2mm annodised aluminium plate with male or female symbol.","No",2,null,0,null,null,2,null,296,null,15024,{"$nulls":12},1,2,10,39,"I","N"]
[]
["17","Ref 079/160E-S/ST P/PL 160 x 160 x 1.2mm anodised aluminium plate with paraplegic symbol.","No",1,null,0,null,null,1,null,297,null,15024,{"$nulls":12},1,2,10,39,"I","N"]
[]
["18","200 x 200 x 3mm Thick perspex plate  with fire exit, fire extinguisher, fire hose reel or fire hydrant symbol.","No",21,null,0,null,null,21,null,298,null,15026,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"BATHROOM FITTINGS",{"$nulls":8},299,null,15061,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Kimberley-Clark:",{"$nulls":8},300,null,15085,{"$nulls":12},1,2,10,39,"S","0"]
[]
["19","Approved lockable two roll toilet roll holder, size 144 x 138 x 301mm, plugged.","No",5,null,0,null,null,5,null,301,null,15093,{"$nulls":12},1,2,10,39,"I","N"]
[]
["20","Approved liquid soap dispenser, size 200 x 85 x 140mm, grade 304 stainless steel unit, plugged.","No",3,null,0,null,null,3,null,302,null,15094,{"$nulls":12},1,2,10,39,"I","N"]
[]
["21","19mm Diameter chromium plated towel rail 600mm long including end brackets.","No",3,null,0,null,null,3,null,303,null,15094,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"SUNDRIES",{"$nulls":8},304,null,15114,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Geze:",{"$nulls":8},305,null,15116,{"$nulls":12},1,2,10,39,"S","0"]
[]
["22","Ref 140/83 - Door stop floor mounted","No",51,null,0,null,null,51,null,308,null,15125,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Chairman Industries:",{"$nulls":8},309,null,15116,{"$nulls":12},1,2,10,39,"S","0"]
[]
["23","32mm Stainless steel side grab rail plugged.","No",1,null,0,null,null,1,null,310,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
["24","32mm Stainless steel rear grab rail plugged.","No",1,null,0,null,null,1,null,311,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Lecico:",{"$nulls":8},2168,null,15120,{"$nulls":12},1,2,10,39,"S","0"]
[]
["25","Toilet seat cover to match existing toilet","No",5,null,0,null,null,5,null,2169,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC",{"$nulls":8},312,null,15209,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Parrot:",{"$nulls":8},313,null,15211,{"$nulls":12},1,2,10,39,"S","0"]
[]
["26","Educational board side panel green writing board 1220 x 920mm high (ED2068) with aluminium chalk rail plugged (AL0120A).","No",30,null,0,null,null,30,null,315,null,15213,{"$nulls":12},1,2,10,39,"I","N"]
[]
["27","Edu BD Centre Panel magnetic white board 1820 x 1220mm high (ED7068) with aluminium chalk rail plugged (AL0120B).","No",16,null,0,null,null,16,null,2422,null,15213,{"$nulls":12},1,2,10,39,"I","N"]
[]
["28","Pinning board 3000 x 1200mm high plugged","No",18,null,0,null,null,18,null,317,null,15213,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Monetary Allowance",{"$nulls":8},2670,null,15213,{"$nulls":12},1,2,10,39,"S","0"]
[]
["29","Allow a monetary allowance of R30 000.00 for Ironmongery","Item",null,null,0,null,null,1,null,2671,null,15213,{"$nulls":12},1,2,10,39,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.11 : METALWORK",{"$nulls":23},1,2,11,45,"H"]
[]
[null,"SUNDRY GALVANISED STEELWORK",{"$nulls":8},2585,null,15717,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Welded columns to walkways (unpainted):",{"$nulls":8},2586,null,15717,{"$nulls":12},1,2,11,45,"S","0"]
[]
["1","76 x 76 x 4mm Hollow section column 3000mm high.","No",61,null,0,null,null,61,null,2587,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["2","150 x 150 x 8mm Base or cap plate welded on and four times drilled for bolts.","No",61,null,0,null,null,61,null,2588,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["3","U-shaped bracket formed of 125 x 3mm flat section 380mm girth welded on and twice drilled for bolts.","No",61,null,0,null,null,61,null,2589,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["4","12mm Diameter x 90mm long fixing bolt.","No",122,null,0,null,null,122,null,2590,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["5","10mm Expansion bolt.","No",244,null,0,null,null,244,null,2591,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED STEEL BALUSTRADING",{"$nulls":8},1411,null,15717,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Framed and welded balustrading to access balconies (unpainted):",{"$nulls":8},1412,null,15719,{"$nulls":12},1,2,11,45,"S","0"]
[]
["6","1100mm High balustrading comprising 25 x 50 x 2,5mm hollow section top and bottom rails, filled with 12 x 12mm solid section balusters at 100mm cenres, 40 x 40 x 3mm hollow section baluster with 100 x 150 x 8mm base plate welded on and twice bolted at 1500mm centres (As per drawing).","m",31,null,0,null,null,31,null,1415,null,15732,{"$nulls":12},1,2,11,45,"I","1"]
[]
[null,"WELDED GALVANISED SCREENS, GATES, ETC.",{"$nulls":8},321,null,15717,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Screens and gates",{"$nulls":8},322,null,15719,{"$nulls":12},1,2,11,45,"S","0"]
[]
["7","Gate 925 x 2032mm high, 10 x 10mm mild steel bars placed at 100mm centres at a 45egress angle with outer frame and inner frame including a pair of suitable hinges welded to frame and lockable sliding bolt with keep in frame (G1)","No",24,null,0,null,null,24,null,2151,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
["8","Double gate with two fixed panels 3554 x 2115mm high overall with double gate 1600 x 2000mm of outer frame and inner frame with a pair of suitable hinges welded to frame and lockable sliding bolt with keep in frame (G2)","No",2,null,0,null,null,2,null,2622,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED STEEL CUPBOARDS",{"$nulls":8},2557,null,15732,{"$nulls":12},1,2,11,45,"H","0"]
[]
["9","Lockable steel cupboard, size 1050 x 500 x 2100mm high","No",2,null,0,null,null,2,null,2558,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED PRESSED STEEL DOOR FRAMES",{"$nulls":8},1725,null,15732,{"$nulls":12},1,2,11,45,"H"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls",{"$nulls":8},1726,null,15732,{"$nulls":12},1,2,11,45,"S"]
[]
["10","Frame for door 813 x 2032mm high","No",16,null,0,null,null,16,null,1783,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
["11","Frame for door 900 x 2032mm high","No",1,null,0,null,null,1,null,1727,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
["12","Frame for door 1515 x 2032mm high","No",2,null,0,null,null,2,null,2625,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"1,2mm Double rebated frames suitable for One brick walls",{"$nulls":8},2623,null,15732,{"$nulls":12},1,2,11,45,"S","0"]
[]
["13","Frame for door 813 x 2032mm high","No",45,null,0,null,null,45,null,2624,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED STEEL WINDOWS, DOORS, ETC.",{"$nulls":8},336,null,15911,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"All windows shall be fitted with standard brass fittings recommended by the manufacturer.",{"$nulls":8},337,null,15923,{"$nulls":12},1,2,11,45,"C","0"]
[]
[null,"Burglar bars shall be standard pattern 5 x 20mm flat section bars corresponding horizontally and vertically with glazing bars.",{"$nulls":8},338,null,15923,{"$nulls":12},1,2,11,45,"C","0"]
[]
[null,"Burglar bars to be fitted to all opening sections only unless otherwise described.",{"$nulls":8},339,null,15923,{"$nulls":12},1,2,11,45,"C","0"]
[]
[null,"Standard residential windows:",{"$nulls":8},2628,null,15923,{"$nulls":12},1,2,11,45,"S","0"]
[]
["14","Composite window, 533 x 654mm high (W4)","No",7,null,0,null,null,7,null,2629,null,15923,{"$nulls":12},1,2,11,45,"I","N"]
[]
["15","Composite window, 1022 x 654mm high (W2)","No",7,null,0,null,null,7,null,2630,null,15923,{"$nulls":12},1,2,11,45,"I","N"]
[]
["16","Composite window, 1022 x 1245mm high (W5)","No",14,null,0,null,null,14,null,2631,null,15923,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"Standard school windows:",{"$nulls":8},348,null,15923,{"$nulls":12},1,2,11,45,"S","0"]
[]
["17","Composite window, 889 x 457mm high (W5)","No",150,null,0,null,null,150,null,2626,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["18","Composite window, 889 x 1248mm high (W7)","No",20,null,0,null,null,20,null,2627,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"Standard galvanised steel cottage pane french door",{"$nulls":8},2647,null,15924,{"$nulls":12},1,2,11,45,"S","0"]
[]
["19","Double door size 1600 x 2135mm high (D3). 3 pairs bush  bearing hinges)","No",2,null,0,null,null,2,null,2648,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"STEEL RECORDROOM AND STRONGROOM DOORS, VENTILATORS, ETC",{"$nulls":8},2643,null,53640,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Strong room doors etc suitable for 230mm walls fixed to brickwork or concrete",{"$nulls":8},2644,null,53650,{"$nulls":12},1,2,11,45,"S","0"]
[]
["20","Record room door and frame 830 x 1935mm high overall with a mass of 180kg","No",1,null,0,null,null,1,null,2646,null,53670,{"$nulls":12},1,2,11,45,"I","N"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.12 : PLASTERING",{"$nulls":23},1,2,12,48,"H"]
[]
[null,"SCREEDS",{"$nulls":8},373,null,16166,{"$nulls":12},1,2,12,48,"H","0"]
[]
[null,"All vinyl flooring materials require a smooth, hard, clean, true and level surface, not only for appearance but also for achieving satisfactory adhesive bond and long term durability",{"$nulls":8},1686,null,16168,{"$nulls":12},1,2,12,48,"C","0"]
[]
[null,"The main contractor should ensure the sub-floor is acceptable to receive vinyl flooring specified in respect of levelness. Smoothness, soundness and cleanness",{"$nulls":8},1687,null,16168,{"$nulls":12},1,2,12,48,"C","0"]
[]
[null,"Screeds on concrete:",{"$nulls":8},374,null,16168,{"$nulls":12},1,2,12,48,"S","0"]
[]
["1","20mm Thick on floors and landings to falls to receive glazed tiles.","m²",107,null,0,null,null,107,null,375,null,16173,{"$nulls":12},1,2,12,48,"I","2"]
[]
["2","23mm Thick on floors and landings to receive vinyl tiles.","m²","  1 300",null,0,null,null,1300,null,376,null,16173,{"$nulls":12},1,2,12,48,"I","2"]
[]
[null,"INTERNAL PLASTER",{"$nulls":8},385,null,16378,{"$nulls":12},1,2,12,48,"H","0"]
[]
[null,"Cement plaster on brickwork:",{"$nulls":8},386,null,16414,{"$nulls":12},1,2,12,48,"S","0"]
[]
["3","On walls.","m²","  2 451",null,0,null,null,2451,null,387,null,16623,{"$nulls":12},1,2,12,48,"I","2"]
[]
["4","On walls to receive tiles.","m²",92,null,0,null,null,92,null,388,null,16623,{"$nulls":12},1,2,12,48,"I","2"]
[]
["5","On narrow widths.","m²",82,null,0,null,null,82,null,389,null,16423,{"$nulls":12},1,2,12,48,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.13 : TILING",{"$nulls":23},1,2,13,51,"H"]
[]
[null,"WALL TILING",{"$nulls":8},399,null,16855,{"$nulls":12},1,2,13,51,"H","0"]
[]
[null,"200 x 200 x 4mm White glazed wall tiles  fixed with adhesive to plaster (elsewhere) and flush pointed with tinted jointing compound:",{"$nulls":8},400,null,16987,{"$nulls":12},1,2,13,51,"S","0"]
[]
["1","On walls","m²",92,null,0,null,null,92,null,401,null,16988,{"$nulls":12},1,2,13,51,"I","2"]
[]
["2","Fair exposed cutting and fitting around pipe not exceeding 50mm diameter.","No",1,null,0,null,null,1,null,405,null,17043,{"$nulls":12},1,2,13,51,"I","N"]
[]
["3","Ditto but exceeding 50mm and not exceeding 100mm diameter.","No",6,null,0,null,null,6,null,406,null,17043,{"$nulls":12},1,2,13,51,"I","N"]
[]
[null,"FLOOR TILING",{"$nulls":8},407,null,17000,{"$nulls":12},1,2,13,51,"H","0"]
[]
[null,"300 x 300 x 8mm Colour glazed floor tiles ( PC. Of R100.00m2 net supply only excluding VAT) fixed with adhesive to screeded (elsewhere)  concrete floors and flush pointed with tinted waterproof jointing compound including approved expansion joints:",{"$nulls":8},408,null,17042,{"$nulls":12},1,2,13,51,"S","0"]
[]
["4","On floors and landings.","m²",107,null,0,null,null,107,null,409,null,17043,{"$nulls":12},1,2,13,51,"I","2"]
[]
["5","Skirting 100mm high of cut tiles.","m",90,null,0,null,null,90,null,410,null,17043,{"$nulls":12},1,2,13,51,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.14 : PLUMBING AND DRAINAGE",{"$nulls":23},1,2,14,54,"H"]
[]
[null,"RAINWATER DISPOSAL",{"$nulls":8},411,null,17852,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Ogee  aluminium:",{"$nulls":8},412,null,17896,{"$nulls":12},1,2,14,54,"S","0"]
[]
["1","125mm Ogee eaves gutters.","m",618,null,0,null,null,618,null,413,null,17899,{"$nulls":12},1,2,14,54,"I","1"]
[]
["2","Extra over Ogee  eaves gutter for stopped end.","No",64,null,0,null,null,64,null,414,null,17903,{"$nulls":12},1,2,14,54,"I","N"]
[]
["3","Extra over Ogee eaves gutter for outlet for 100 x 75mm pipe.","No",52,null,0,null,null,52,null,415,null,17906,{"$nulls":12},1,2,14,54,"I","N"]
[]
["4","100 x 75mm Rainwater pipes.","m",167,null,0,null,null,167,null,416,null,17908,{"$nulls":12},1,2,14,54,"I","1"]
[]
["5","Extra over 100 x 75mm  rainwater pipe for bend.","No",104,null,0,null,null,104,null,417,null,17909,{"$nulls":12},1,2,14,54,"I","N"]
[]
["6","Extra over 100 x 75mm  rainwater pipe for shoe.","No",52,null,0,null,null,52,null,418,null,17910,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"SANITARY FITTINGS",{"$nulls":8},419,null,18028,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Prices are to include for sealing all round with approved silicone waterproofing sealant at junction/gaps with tiled walls, timber fittings, vanity tops, etc.",{"$nulls":8},420,null,75842,{"$nulls":12},1,2,14,54,"C","0"]
[]
[null,"Lecico Sanitaryware' vitreous china wash hand basins and pedestals:",{"$nulls":8},421,null,75801,{"$nulls":12},1,2,14,54,"S","0"]
[]
["7","410 x 500mm 'Atlas' white vitreous china lavatory basin (product code ATLDUOBAS0500BE) with one taphole including integrated overflow and chainstay hole, fixed with stainless steel screws and washers to plugs in wall  (tap and waste fitting elsewhere).","No",4,null,0,null,null,4,null,423,null,75802,{"$nulls":12},1,2,14,54,"I","N"]
[]
["8","Ditto but to paraplegic","No",1,null,0,null,null,1,null,2632,null,75802,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Lecico Sanitaryware' vitreous china WC suites:",{"$nulls":8},425,null,75856,{"$nulls":12},1,2,14,54,"S","0"]
[]
["9","Madison' white vitreous china close couple suite  (product code MADBOXDFL0SCSBE) with 100mm outlet  and matching 6 litre cistern including lid, fitments, flushpipe, etc., bedded in 4:1 cement mortar on concrete floors.","No",28,null,0,null,null,28,null,426,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
["10","Ditto but to paraplegic","No",1,null,0,null,null,1,null,2633,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Plumline' vitreous china urinals:",{"$nulls":8},2540,null,75858,{"$nulls":12},1,2,14,54,"S"]
[]
["11","Amaro' urinal  (code 031129) size 300 x 245 x 400mm high or equal approved with top inlet spreader and waste outlet including wall mounting brackets and connected to water supply, sealed with silicone sealant where urinal meets wall","No",2,null,0,null,null,2,null,2541,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Franke' grade 304 (18/10) stainless steel domestic drop on sinks",{"$nulls":8},2672,null,75858,{"$nulls":12},1,2,14,54,"S","0"]
[]
["12","Franke' standard drop on sink and drainer size 1000 x 500mm with single end bowl, set on cupboard fitting (elsewhere), including cutting one taphole (tap and wastefitting elsewhere)","No",1,null,0,null,null,1,null,2673,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"WASTE UNIONS ETC",{"$nulls":8},437,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Cobra Watertech':",{"$nulls":8},438,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
["13","32 mm CP basin waste union.","No",5,null,0,null,null,5,null,439,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["14","40 mm CP waste union.","No",1,null,0,null,null,1,null,440,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"TRAPS ETC",{"$nulls":8},441,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Priced are to include for jointing to uPVC pipe with and including the necessary adaptors unless otherwise described.",{"$nulls":8},442,null,18034,{"$nulls":12},1,2,14,54,"C","0"]
[]
[null,"Butyl rubber:",{"$nulls":8},443,null,18034,{"$nulls":12},1,2,14,54,"S","0"]
[]
["15","32 mm deep seal \"P\" or \"S\" trap.","No",5,null,0,null,null,5,null,444,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Cobra Watertech':",{"$nulls":8},1382,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
["16","40mm CP bottle trap.","No",2,null,0,null,null,2,null,447,null,18110,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"TAPS,VALVES, ETC",{"$nulls":8},449,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Priced are to include  for jointing to copper pipe with and including the necessary fittings unless otherwise described.",{"$nulls":8},450,null,18034,{"$nulls":12},1,2,14,54,"C","0"]
[]
[null,"Brass.",{"$nulls":8},451,null,18034,{"$nulls":12},1,2,14,54,"S","0"]
[]
["17","15 mm Fulway gate valve.","No",33,null,0,null,null,33,null,452,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["18","22 mm Fulway gate valve.","No",16,null,0,null,null,16,null,453,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["19","28 mm Fulway gate valve.","No",12,null,0,null,null,12,null,1206,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Plumline",{"$nulls":8},455,null,18034,{"$nulls":12},1,2,14,54,"S","0"]
[]
["20","15 mm CP Ballostop.","No",5,null,0,null,null,5,null,456,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["21","22 mm CP Ballostop.","No",2,null,0,null,null,2,null,457,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["22","15 mm CP Star pillartaps.","No",24,null,0,null,null,24,null,459,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["23","15 mm CP 'Moderna' pillartap with swivel outlet (Code: 038735).","No",1,null,0,null,null,1,null,460,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"SANITARY PLUMBING",{"$nulls":8},467,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"uPVC pipes:",{"$nulls":8},468,null,18200,{"$nulls":12},1,2,14,54,"S","0"]
[]
["24","50mm Pipes.","m",15,null,0,null,null,15,null,469,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["25","110mm Pipes.","m",10,null,0,null,null,10,null,470,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["26","50mm Pipes under surface beds.","m",12,null,0,null,null,12,null,471,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["27","110mm Pipes under surface beds.","m",12,null,0,null,null,12,null,472,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["28","110mm Pipes laid in and including trenches not exceeding 1m deep.","m",5,null,0,null,null,5,null,473,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["29","50mm Pipes chased into brick walls.","m",0,null,0,null,null,0,null,474,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
[null,"Extra over uPVC pipes for fittings:",{"$nulls":8},475,null,18321,{"$nulls":12},1,2,14,54,"S","0"]
[]
["30","110mm Reducer.","No",6,null,0,null,null,6,null,477,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["31","50mm Bend.","No",10,null,0,null,null,10,null,478,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["32","110mm Bend.","No",2,null,0,null,null,2,null,479,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["33","50mm Junction.","No",2,null,0,null,null,2,null,480,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["34","110mm Junction.","No",1,null,0,null,null,1,null,481,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["35","110mm Pan connector.","No",1,null,0,null,null,1,null,482,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["36","110mm Acess bent pan connector.","No",1,null,0,null,null,1,null,483,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["37","50mm Acess bend.","No",2,null,0,null,null,2,null,485,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["38","110mm Acess bend.","No",2,null,0,null,null,2,null,486,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["39","50mm Acess junction.","No",2,null,0,null,null,2,null,487,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["40","110mm Acess junction.","No",1,null,0,null,null,1,null,488,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["41","110mm Acess reducing junction.","No",2,null,0,null,null,2,null,489,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["42","110mm Acess double junction.","No",2,null,0,null,null,2,null,490,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"WATER SUPPLIES",{"$nulls":8},493,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Class 1 copper pipes:",{"$nulls":8},494,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["43","15mm Pipes.","m",5,null,0,null,null,5,null,495,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["44","22mm Pipes.","m",9,null,0,null,null,9,null,496,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["45","28mm Pipes.","m",7,null,0,null,null,7,null,497,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["46","15mm Pipes chased into brick walls.","m",12,null,0,null,null,12,null,500,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["47","22mm Pipes chased into brick walls.","m",13,null,0,null,null,13,null,501,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
[null,"Extra over copper pipe for capillary fitting:",{"$nulls":8},502,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["48","15mm Fittings.","No",22,null,0,null,null,22,null,503,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["49","22mm Fittings.","No",15,null,0,null,null,15,null,504,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["50","28mm Fittings.","No",11,null,0,null,null,11,null,505,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Extra over copper pipe for brass compression fitting:",{"$nulls":8},506,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["51","15mm Fittings.","No",12,null,0,null,null,12,null,507,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["52","22mm Fittings.","No",7,null,0,null,null,7,null,508,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["53","28mm Fittings.","No",4,null,0,null,null,4,null,509,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Copper overflow and service pipes:",{"$nulls":8},510,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["54","15mm Bent service pipe average 450mm girth and joint to copper pipe and fittings.","No",2,null,0,null,null,2,null,511,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["55","22mm Bent overflow pipe average 450mm girth and joint to fittings.","No",2,null,0,null,null,2,null,512,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"FIRE APPLIANCES ETC.",{"$nulls":8},528,null,18635,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Chubb':",{"$nulls":8},529,null,18637,{"$nulls":12},1,2,14,54,"S","0"]
[]
["56","Everyway' hose reel complete with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket.","No",4,null,0,null,null,4,null,530,null,18639,{"$nulls":12},1,2,14,54,"I","N"]
[]
["57","4,5kg DPC fire extinguisher complete with backboard and wall bracket plugged to wall.","No",7,null,0,null,null,7,null,531,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["58","Ditto but 9kg.","No",11,null,0,null,null,11,null,532,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["59","Watertight high impact, UV- stablised clear acrylic fire hose reel cupboard with numbered twist-action closer seal fixed to brick wall.","No",4,null,0,null,null,4,null,533,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"WATER SUPPLIES TO FIRE APPLIANCES",{"$nulls":8},534,null,18656,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Class 1 copper pipes:",{"$nulls":8},535,null,18710,{"$nulls":12},1,2,14,54,"S","0"]
[]
["60","28mm Pipes.","m",9,null,0,null,null,9,null,536,null,18715,{"$nulls":12},1,2,14,54,"I","1"]
[]
["61","28mm Pipes under surface bed.","m",4,null,0,null,null,4,null,537,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
[null,"Extra over class 1 copper pipes for capillary fittings:",{"$nulls":8},538,null,18732,{"$nulls":12},1,2,14,54,"S","0"]
[]
["62","28mm Fittings.","No",4,null,0,null,null,4,null,539,null,18733,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"TESTING",{"$nulls":8},540,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
["63","Testing all pipe systems.","Item",1,null,0,null,null,1,null,541,null,18351,{"$nulls":12},1,2,14,54,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.15 : GLAZING",{"$nulls":23},1,2,15,63,"H"]
[]
[null,"GLAZING TO STEEL WITH PUTTY",{"$nulls":8},545,null,20715,{"$nulls":12},1,2,15,63,"H","0"]
[]
[null,"4mm clear toughned class.",{"$nulls":8},2653,null,20729,{"$nulls":12},1,2,15,63,"S","0"]
[]
["1","Panes exceeding 0,1m2 and not exceeding 0.5m2.","m²",7,null,0,null,null,7,null,552,null,20729,{"$nulls":12},1,2,15,63,"I","2"]
[]
["2","Panes exceeding 0,5m2 and not exceeding 2.5m2.","m²",167,null,0,null,null,167,null,2538,null,20729,{"$nulls":12},1,2,15,63,"I","2"]
[]
[null,"TOPS, SHELVES, DOORS, MIRRORS, ETC.",{"$nulls":8},553,null,21649,{"$nulls":12},1,2,15,63,"H","0"]
[]
[null,"3mm Silvered float glass copper backed mirrors with polished edges fixed with double sided adhesive tape:",{"$nulls":8},554,null,21663,{"$nulls":12},1,2,15,63,"S","0"]
[]
["3","Frameless mirror 700 x 450 mm high.","No",5,null,0,null,null,5,null,555,null,21664,{"$nulls":12},1,2,15,63,"I","N"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.16 : PAINTWORK",{"$nulls":23},1,2,16,66,"H"]
[]
[null,"PAINTWORK ETC. TO NEW SURFACES",{"$nulls":8},557,null,21780,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"ON FLOATED PLASTER",{"$nulls":8},1709,null,21780,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coat Alkali Resistant Plaster Primer  and two coats superior quality acrylic emulsion paint:",{"$nulls":8},558,null,43774,{"$nulls":12},1,2,16,66,"S","0"]
[]
["1","On interior walls.","m²","  2 531",null,0,null,null,2531,null,559,null,43775,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON PLASTER BOARD",{"$nulls":8},568,null,25056,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coatAlkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:",{"$nulls":8},569,null,44054,{"$nulls":12},1,2,16,66,"S","0"]
[]
["2","On internal ceilings and cornices.","m²","  2 514",null,0,null,null,2514,null,570,null,44055,{"$nulls":12},1,2,16,66,"I","2"]
[]
["3","On external ceilings and cornices.","m²",231,null,0,null,null,231,null,2561,null,44055,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON FIBRE-CEMENT, ETC.",{"$nulls":8},571,null,25602,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coat Alkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:",{"$nulls":8},572,null,44071,{"$nulls":12},1,2,16,66,"S","0"]
[]
["4","On exterior fascias and barge boards.","m²",143,null,0,null,null,143,null,574,null,44073,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON METAL",{"$nulls":8},575,null,26148,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, dust, grease, salts and contamination with one coat ater based primer, one coat alkyd based universal  undercoat  and two coats superior quality universal enamel paint on: galvanised steel or aluminium:",{"$nulls":8},581,null,44120,{"$nulls":12},1,2,16,66,"S","0"]
[]
["5","On door frames.","m²",257,null,0,null,null,257,null,582,null,44123,{"$nulls":12},1,2,16,66,"I","2"]
[]
["6","On window frames with burglar bars (bsm).","m²",393,null,0,null,null,393,null,584,null,44123,{"$nulls":12},1,2,16,66,"I","2"]
[]
["7","On security gates","m²",92,null,0,null,null,92,null,2150,null,44123,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON WOOD, WOOD BOARD",{"$nulls":8},585,null,26286,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Stop, fill, sand down and prepare wood surfaces and apply three coats superior quality clear gloss varnish",{"$nulls":8},588,null,44266,{"$nulls":12},1,2,16,66,"S","0"]
[]
["8","On interior / exterior doors.","m²",103,null,0,null,null,103,null,589,null,44270,{"$nulls":12},1,2,16,66,"I","2"]
[]
["9","On interior / exterior skirtings, rails, etc not exceeding 300mm girth.","m",416,null,0,null,null,416,null,590,null,44277,{"$nulls":12},1,2,16,66,"I","1"]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":8},2076,null,70730,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"PREPARATORY WORK TO EXISTING WORK",{"$nulls":8},2077,null,70740,{"$nulls":12},1,2,16,66,"S","0"]
[]
[null,"Previously painted plastered surfaces",{"$nulls":8},2078,null,70760,{"$nulls":12},1,2,16,66,"C","0"]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth",{"$nulls":8},2078,null,70760,{"$nulls":12},1,2,16,66,"C","0"]
[]
[null,"Previously painted metal surfaces",{"$nulls":8},2079,null,70780,{"$nulls":12},1,2,16,66,"C","0"]
[null,"Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal",{"$nulls":8},2079,null,70780,{"$nulls":12},1,2,16,66,"C","0"]
[]
[null,"Previously painted wood surfaces",{"$nulls":8},2080,null,70800,{"$nulls":12},1,2,16,66,"C","0"]
[null,"Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth",{"$nulls":8},2080,null,70800,{"$nulls":12},1,2,16,66,"C","0"]
[]
[null,"ON PREVIOUSLY PAINTED SURFACES",{"$nulls":8},1704,null,586000,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"ON EXISTING INTERNAL FLOATED PLASTER SURFACES",{"$nulls":8},2085,null,72190,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Two coats superior quality acrylic emulsion paint for interior and exterior use",{"$nulls":8},2086,null,72200,{"$nulls":12},1,2,16,66,"S","0"]
[]
["10","On exterior wall","m²",502,null,0,null,null,502,null,2087,null,72201,{"$nulls":12},1,2,16,66,"I","2"]
[]
["11","On interior wall","m²","  1 567",null,0,null,null,1567,null,2634,null,72201,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON EXISTING METAL SURFACES",{"$nulls":8},2082,null,72410,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint",{"$nulls":8},2083,null,72420,{"$nulls":12},1,2,16,66,"S","0"]
[]
["12","Door frames","m²",42,null,0,null,null,42,null,2084,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
["13","Security gates","m²",23,null,0,null,null,23,null,2147,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
["14","On window frames with burglar bars (bsm).","m²",8,null,0,null,null,8,null,2109,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON EXISTING WOOD SURFACES",{"$nulls":8},2091,null,72510,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint",{"$nulls":8},2092,null,72520,{"$nulls":12},1,2,16,66,"S","0"]
[]
["15","Doors","m²",12,null,0,null,null,12,null,2093,null,72521,{"$nulls":12},1,2,16,66,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[null,"Section Total ",{"$nulls":4},{"v":200000,"d":"200,000.00"}]
[]
[]
[null,"SECTION NO. 3 : EXTERNAL WORKS",{"$nulls":23},1,3,1,6,"H"]
[]
[]
[null,"BILL NO.1 : EXTERNAL WORKS (PROVISIONAL)",{"$nulls":23},1,3,1,6,"H"]
[]
[null,"REMOVAL OF EXISTING WORK",{"$nulls":8},1739,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Note to tenderers: The removal, storage ,disposal, etc  of asbestos sheeting, etc to be executed in strict accordance to the bye laws (OHS) regarding same by a specialist asbestos sub-contractor. Prices to include for this.",{"$nulls":8},2494,null,1650,{"$nulls":12},1,3,1,6,"C","0"]
[]
[null,"All work to be demolished, etc is to be removed off site, unless otherwise stated, prices to include for this.",{"$nulls":8},2495,null,1650,{"$nulls":12},1,3,1,6,"C","0"]
[]
[null,"Demolition of existing work",{"$nulls":8},1740,null,1650,{"$nulls":12},1,3,1,6,"S"]
[]
["1","Blocks A1 - Single storey building with pitched roof, approximately 52 859mm x 6 700mm on plan, comprising reinforced concrete surface bed, brick walls, and roof sheeting on timber trusses, including grubbing up all foundations, removal and disposal thereof complete","No",1,null,0,null,null,1,null,2490,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
["2","Blocks A2 - Single storey building with pitched roof, approximately 40 305mm x 6 700mm and 6 840mm x 6 470mm on plan, comprising reinforced concrete surface bed, brick walls, and roof sheeting on timber trusses, including grubbing up all foundations, removal and disposal thereof complete","No",1,null,0,null,null,1,null,2651,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
["3","Blocks A3 - Single storey building with pitched roof, approximately 47 363mm x 7 160mm on plan, comprising reinforced concrete surface bed, brick walls, and roof sheeting on timber trusses, including grubbing up all foundations, removal and disposal thereof complete","No",1,null,0,null,null,1,null,2652,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
[null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement including removing all layerworks in existing ramp",{"$nulls":8},2160,null,1650,{"$nulls":12},1,3,1,6,"S"]
[]
["4","Concrete V-drains 900mm wide","m",52,null,0,null,null,52,null,2674,null,1650,{"$nulls":12},1,3,1,6,"I","1"]
[]
["5","Take up and remove 60mm thick corobrik block paving including 200mm thick layer works, and set aside paving including later relaying in new position","m²",180,null,0,null,null,180,null,2677,null,1650,{"$nulls":12},1,3,1,6,"I","2"]
[]
[null,"ALTERATIONS",{"$nulls":8},2426,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"JOINT SEALANTS",{"$nulls":8},2427,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Chip open the crack to form a \"V\" shape 20mm wide x 10mm deep and scratch out the debris that may block the crack in the sides of the hole. Grinding in the floor approximately 200mm to 300mm apart from the rebar to be placed into an",{"$nulls":8},2431,null,1650,{"$nulls":12},1,3,1,6,"S","0"]
[null,"epoxy repair mortar 'SIKA TOP-ARMATEC 100'. Fill the crack with structural epoxy repair mortar SIKA MONO TOP 615HB'",{"$nulls":8},2431,null,1650,{"$nulls":12},1,3,1,6,"S","0"]
[]
["6","Concrete V-drains, walkways, etc.","m",52,null,0,null,null,52,null,2430,null,1650,{"$nulls":12},1,3,1,6,"I","1"]
[]
[null,"TEMPORARY WORKS",{"$nulls":8},596,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
["7","1,5m High 'Bonnox' wire mesh temporary fencing with shade cloth.","m",290,null,0,null,null,290,null,597,null,1650,{"$nulls":12},1,3,1,6,"I","1"]
[]
["8","Single gate 900 x 1,5m high.","No",1,null,0,null,null,1,null,598,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
["9","Double gate 1,5 x 1,5m high.","No",1,null,0,null,null,1,null,2675,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
[null,"GENERAL SITE CLEARANCE, ETC.",{"$nulls":8},599,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Site clearance, etc.:",{"$nulls":8},600,null,1652,{"$nulls":12},1,3,1,6,"S","0"]
[]
["10","Allow for clearing of the site all grass, weeds, shrubs, debris, etc and cartwawy all vegetation and stockpile","m²",280,null,0,null,null,280,null,602,null,1654,{"$nulls":12},1,3,1,6,"I","2"]
[]
["11","Strip average 100mm thick layer of topsoil and stockpile on site","m²",100,null,0,null,null,100,null,1731,null,1654,{"$nulls":12},1,3,1,6,"I","2"]
[]
["12","Spread and level imported topsoil oversite as directed","m²",100,null,0,null,null,100,null,1732,null,1654,{"$nulls":12},1,3,1,6,"I","2"]
[]
[null,"KEEPING EXCAVATIONS FREE OF WATER",{"$nulls":8},607,null,1812,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Keeping excavations free of water:",{"$nulls":8},608,null,1814,{"$nulls":12},1,3,1,6,"S","0"]
[]
["13","Keeping excavations free of all water other than subterranean water through out this bill .","Item",1,null,0,null,null,1,null,609,null,1815,{"$nulls":12},1,3,1,6,"I","I"]
[]
[null,"APRONS, PAVING, RAMPS, PATHS AND STEPS",{"$nulls":8},684,null,1816,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Earthworks:",{"$nulls":8},685,null,1816,{"$nulls":12},1,3,1,6,"S","0"]
[]
["14","Excavate in soft excavations in earth for thickenings under ramps, pavings, aprons, including trimming to splayed sides.","m³",80,null,0,null,null,80,null,686,null,1816,{"$nulls":12},1,3,1,6,"I","3"]
[]
["15","Extra over excavations for excavating in soft rock.","m³",8,null,0,null,null,8,null,689,null,1816,{"$nulls":12},1,3,1,6,"I","3"]
[]
["16","Extra over excavations for carting away surplus material off site.","m³",56,null,0,null,null,56,null,690,null,1816,{"$nulls":12},1,3,1,6,"I","3"]
[]
["17","Approved filling supplied by the Contractor under pavings and paths compacted to a density of 93% Mod AASHTO.","m³",27,null,0,null,null,27,null,691,null,1816,{"$nulls":12},1,3,1,6,"I","3"]
[]
["18","Over site of G5 material as sub -base layer in",{"$nulls":8},692,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[null,"accordance with SABS 1200DM 125mm layer",{"$nulls":8},692,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[null,"compacted to 95% Mod AASHTO density and trim to",{"$nulls":8},692,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[null,"grades","m²",180,null,0,null,null,180,null,692,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[]
["19","Over site of G2 material as base layer in according with SABS 1200DM 125mm layer compacted to 98% Mod AASHTO density and trim to grades.","m²",180,null,0,null,null,180,null,2678,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[]
["20","Trim, level, excavate and scarify for a depth of 150mm ground surface to receive concrete paving and compact to 93% Mod AASHTO density.","m²",180,null,0,null,null,180,null,693,null,1765,{"$nulls":12},1,3,1,6,"I","2"]
[]
["21","Approved weed killer to surface of earth under pavings, aprons, etc.","m²",180,null,0,null,null,180,null,694,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[]
[null,"Take from where set aside and relay paving",{"$nulls":8},695,null,1816,{"$nulls":12},1,3,1,6,"S","0"]
[]
["22","Relay corobrik block paving","m²",180,null,0,null,null,180,null,696,null,1816,{"$nulls":12},1,3,1,6,"I","2"]
[]
[null,"Monetary Allowance",{"$nulls":8},1765,null,1668,{"$nulls":12},1,3,1,6,"S"]
[]
["23","Allow a provisional allowance of R 150 000.00 (One Hundred and Fifty Thousand Rands) for external works to be ascertained on site","Item",null,null,0,null,null,1,null,1806,null,1668,{"$nulls":12},1,3,1,6,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.2 : PLUMBING AND DRAINAGE (PROVISIONAL)",{"$nulls":23},1,3,2,54,"H"]
[]
[null,"STORM WATER CHANNELS.",{"$nulls":8},992,null,1761,{"$nulls":12},1,3,2,54,"H","0"]
[]
[null,"Smooth finished in-situ reinforced concrete 25Mpa/13mm channels:",{"$nulls":8},993,null,1763,{"$nulls":12},1,3,2,54,"S","0"]
[]
["1","900 x 130mm Smooth  finished open V shaped  channel to detail, cast in alternative panels and to falls, including excavations, shaping and grading ground as required, formwork, mesh Ref 193.","m",86,null,0,null,null,86,null,999,null,17287,{"$nulls":12},1,3,2,54,"I","1"]
[]
["2","Extra for angles, intersections, ends, dressing into sides of catchpits, etc.","No",4,null,0,null,null,4,null,995,null,17289,{"$nulls":12},1,3,2,54,"I","N"]
[]
["3","12mm Thick bitumen impregnated softboard between vertical concrete surfaces of channels.","m",32,null,0,null,null,32,null,1000,null,17287,{"$nulls":12},1,3,2,54,"I","1"]
[]
["4","Approved polysulphide sealing compound to joints of channels.","m",32,null,0,null,null,32,null,1001,null,17287,{"$nulls":12},1,3,2,54,"I","1"]
[]
[null,"Monetary Allowance",{"$nulls":8},1808,null,1816,{"$nulls":12},1,3,2,54,"S"]
[]
["5","Allow a monetary allowance fo R50 000.00 for proving and cleaning pipework","Item",null,null,0,null,null,1,null,1809,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
["6","Allow a monetary allowance of R30 000.00 for cleaning of all sewer and stormwater manholes","Item",null,null,0,null,null,1,null,1810,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
[null,"TESTING",{"$nulls":8},1187,null,1816,{"$nulls":12},1,3,2,54,"H","0"]
[]
["7","Testing all plumbing systems.","Item",1,null,0,null,null,1,null,1188,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[null,"Section Total ",{"$nulls":4},0]
[]
[]
[null,"SECTION NO. 4 : PROVISIONAL SUMS",{"$nulls":23},1,4,1,99,"H"]
[]
[]
[null,"BILL NO.1 : PROVISIONAL SUMS",{"$nulls":23},1,4,1,99,"H"]
[]
[null,"The following Provisional Amounts are all Net amounts Exclusive of commision for the Contractor. These amounts are for the work to be executed complete by the Nominated/Selected Sub-Contractors:",{"$nulls":8},1272,null,27973,{"$nulls":12},1,4,1,99,"S","0"]
[]
[null,"LANDSCAPING",{"$nulls":8},1317,null,28007,{"$nulls":12},1,4,1,99,"H","0"]
[]
["1","Provide the amount of R 50,000.00 (Fifty Thousand Rands) for Landscaping, etc.","Item",1,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"},null,null,1,null,1349,null,28010,{"$nulls":12},1,4,1,99,"I","I"]
[]
["2","Profit on above item.","Item",1,null,0,null,null,1,null,1319,null,28011,{"$nulls":12},1,4,1,99,"I","I"]
[]
["3","Attendance on ditto.","Item",1,null,0,null,null,1,null,1320,null,28012,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"SIGNAGE",{"$nulls":8},1321,null,28007,{"$nulls":12},1,4,1,99,"H","0"]
[]
["4","Provide the amount of R 30,000.00 (Thirty Thousand Rands) for Signage.","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"},null,null,1,null,1350,null,28010,{"$nulls":12},1,4,1,99,"I","I"]
[]
["5","Profit on above item.","Item",1,null,0,null,null,1,null,1323,null,28011,{"$nulls":12},1,4,1,99,"I","I"]
[]
["6","Attendance on ditto.","Item",1,null,0,null,null,1,null,1324,null,28012,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":8},1325,null,36185,{"$nulls":12},1,4,1,99,"H","0"]
[]
["7","Provide the amount of R 400 000.00 (Four Hundred Thousand Rands) for Plumbing and Drainage.","Item",1,{"v":400000,"d":"400,000.00"},{"v":400000,"d":"400,000.00"},null,null,1,null,1351,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["8","Profit on above item.","Item",1,null,0,null,null,1,null,1327,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["9","Attendance on ditto.","Item",1,null,0,null,null,1,null,1328,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"TEMPORARY ACCOMMODATION & ABLUTIONS",{"$nulls":8},2658,null,36195,{"$nulls":12},1,4,1,99,"H","0"]
[]
["10","Provide the amount of R 4 100 000.00 (Four Million and One Hundred Thousand Rands) for the purchase, transportation, ground preparation works and the erection of mobile classrooms and ablution facilities for the duration of construction. The units are made good upon project completion and relocated to another site determined by the Principal Agent and/or client, less than or equal to 200km from the siote as per Architectural / Engineering specifications, to be performed by specialist where required","Item",1,{"v":4100000,"d":"4,100,000.00"},{"v":4100000,"d":"4,100,000.00"},null,null,1,null,2659,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["11","Profit on above item.","Item",1,null,0,null,null,1,null,2660,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["12","Attendance on ditto.","Item",1,null,0,null,null,1,null,2661,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"CARPENTRY & JOINERY",{"$nulls":8},2439,null,36195,{"$nulls":12},1,4,1,99,"H","I"]
[]
["13","Provide the amount of R 500,000.00 (Five Hundred Thousand Rands) for Carpentry & Joinery to Classrooms.","Item",1,{"v":500000,"d":"500,000.00"},{"v":500000,"d":"500,000.00"},null,null,1,null,2440,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["14","Profit on above item.","Item",1,null,0,null,null,1,null,2441,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["15","Attendance on ditto.","Item",1,null,0,null,null,1,null,2442,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"GEOTECH & SURVEY",{"$nulls":8},2686,null,36195,{"$nulls":12},1,4,1,99,"H"]
[]
["16","Provide the amount of R 150,000.00 (One Hundred Thousand Rands) for Geotech & Survey","Item",1,{"v":150000,"d":"150,000.00"},{"v":150000,"d":"150,000.00"},null,null,1,null,2687,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["17","Profit on above item.","Item",1,null,0,null,null,1,null,2688,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["18","Attendance on ditto.","Item",1,null,0,null,null,1,null,2689,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"The following Electrical Works are to be undertaken by direct contractors, selected at the client's discretion",{"$nulls":8},2436,null,36195,{"$nulls":12},1,4,1,99,"S","I"]
[]
[null,"ELECTRICAL INSTALLATION",{"$nulls":8},1754,null,36195,{"$nulls":12},1,4,1,99,"H"]
[]
["19","Provide the amount of R 800 000.00 (Eight Hundred Thousand Rands) for Electrical Installation","Item",1,{"v":800000,"d":"800,000.00"},{"v":800000,"d":"800,000.00"},null,null,1,null,1755,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["20","Profit on above item.","Item",1,null,0,null,null,1,null,1756,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["21","Attendance on ditto.","Item",1,null,0,null,null,1,null,1757,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"BUDGETARY ALLOWANCES",{"$nulls":8},1677,null,36195,{"$nulls":12},1,4,1,99,"H","0"]
[]
["22","Allow a budgetary amount of R 150 000.00 (One Hundred and Fifty Thousand Rands) for Community Liaison Officer (CLO)","Item",1,{"v":150000,"d":"150,000.00"},{"v":150000,"d":"150,000.00"},null,null,1,null,1683,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["23","Allow a budgetary amount of R 6 500.00 / month for Project Steering Committee","Item",1,{"v":78000,"d":"78,000.00"},{"v":78000,"d":"78,000.00"},null,null,1,null,2435,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
["24","Allow a budgetary amount of R 5 330.00 / month for CIDB Build / Skills Development","Item",1,{"v":63960,"d":"63,960.00"},{"v":63960,"d":"63,960.00"},null,null,1,null,2438,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"BUILDER'S WORK IN CONNECTION WITH PROVISIONAL SUMS",{"$nulls":8},2437,null,36195,{"$nulls":12},1,4,1,99,"H","0"]
[]
["25","Provide the amount of R 25 000.00 (Twenty Five Thousand Rands) for Builder's Work in connection with Provisional Sums.","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"},null,null,1,null,2438,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},{"v":6346960,"d":"6,346,960.00"}]
[]
[]
[null,"Section Total ",{"$nulls":4},{"v":6346960,"d":"6,346,960.00"}]