{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":202,"n_cols":6,"rows_kept":202,"merged":[[0,4,0,5],[2,4,2,5],[4,0,4,5],[201,0,201,4]],"flags":["formulas_cached_only"]}
["PLASGAS BUNDS CIVIL WORKS"]
[]
["Bill of Quantities",null,null,"REV 2.0","2026-02-02"]
["Item","Bill description","Unit","Bill quantity","Rate","Amount"]
["CIVIL & STRUCTURAL WORKS "]
[]
["Reference Drawings:","NNDD-V-H2-C-BUNDE-0001","rev 2.0"]
[null,"NNDD-V-H2-C-BUNDE-0002","rev 2.0"]
[null,"NNDD-V-H2-C-BUNDE-0003","rev 2.0"]
[null,"NNDD-V-H2-C-BUNDE-0004","rev 2.0"]
[null,"NNDD-V-H2-C-BUNDE-0005","rev 2.0"]
["CONCRETE (STRUCTURAL)"]
[]
[1,"EXCAVATION"]
[]
[null,"COOLING WATER SYSTEM SLAB"]
[]
["1.1.1","Break out existing asphalt surface","m3",{"v":10,"d":"10.00"}]
[null,"Excavate in-situ layerworks soils up to 0.5m deep"]
[null,"Remove excavated material; from site"]
[]
["1.1.2","Bottom of excavation, In-situ soil compacted","m2",{"v":33,"d":"33.00"}]
[null,"to 93% Mod Aahsto"]
[]
[null,"METHANE, LPG, ARGON SLAB"]
[]
["1.1.3","Excavate in-situ layerworks soils up to 0.5m deep","m3",{"v":5,"d":"5.00"}]
[null,"Remove excavated material; from site"]
[]
["1.1.4","Bottom of excavation, In-situ soil compacted","m2",{"v":16,"d":"16.00"}]
[null,"to 93% Mod Aahsto"]
[]
[null,"LIQUID OXYGEN-MAXI SLAB"]
[]
["1.1.3","Excavate in-situ layerworks soils up to 0.5m deep","m3",{"v":3,"d":"3.00"}]
[null,"Remove excavated material; from site"]
[]
["1.1.4","Bottom of excavation, In-situ soil compacted","m2",{"v":9,"d":"9.00"}]
[null,"to 93% Mod Aahsto"]
[]
[]
["2.1","FORMWORK"]
[]
[null,"COOLING WATER SYSTEM SLAB"]
[]
["2.1.1","Vertical formwork for slab perimeter edge","m2",{"v":7,"d":"7.00"}]
[null,"with 25x25 corner chamfers"]
[]
[null,"METHANE, LPG, ARGON SLAB"]
[]
["2.1.2","Vertical formwork for slab perimeter edge","m2",{"v":5,"d":"5.00"}]
[null,"with 25x25 corner chamfers"]
[]
[null,"LIQUID OXYGEN-MAXI SLAB"]
[]
["2.1.3","Vertical formwork for slab perimeter edge","m2",{"v":2,"d":"2.00"}]
[null,"with 25x25 corner chamfers"]
[]
[]
[]
["3.1","REINFORCEMENT"]
[]
["3.1.1","High Tensile Steel (Rate to include ordering from schedule, supply, delivered to site, fixed in position)"]
[]
["3.1.1.1","Y12, Y10 diameter bars - Cooling water","kg",714]
[]
["3.1.1.2","Y12, Y10 diameter bars - Methane, LPG, Argon","kg",387]
[]
["3.1.1.3","Y12, Y10 diameter bars - Liquid Oxygen","kg",182]
[]
["3.1.1.4","Mesh Ref 193 - Methane, LPG, Argon Ramp","kg",28]
[]
["4.1","CONCRETE"]
[]
[]
[4.1,"Reinforced Concrete"]
[]
["4.1.1","Concrete 25 MPa/19mm"]
[]
["4.1.1.1","Foundation slab - Cooling water","m3",{"v":10,"d":"10.00"}]
[]
["4.1.1.2","Foundation slab and ramp - Methane, LPG, Argon","m3",{"v":5,"d":"5.00"}]
[]
["4.1.1.3","Foundation slab - Liquid Oxygen","m3",{"v":2.5,"d":"2.50"}]
[]
[]
[]
[5.1,"STEELWORK"]
[]
[5.1,"COOLING WATER SYSTEM CANOPY"]
[]
["5.1.1","Steelwork canopy over slab"]
[null,"(Price to include workshop detailing and drawings,"]
[null,"all bolts Gr8.8, Painted to Necsa specs)"]
[null,"All hot rolled steelwork Grade S355JR"]
[null,"Hollow Sections Min Grade 300WA"]
[null,"Cold formed Sections min yield 240 MPa"]
[]
[null,"(a) 160 IPE columns","kg",{"v":400,"d":"400.00"}]
[]
[null,"(b) 160 IPE Rafters","kg",{"v":255,"d":"255.00"}]
[]
[null,"(c) 100x50x20x2.5 Cold formed lipped channels","kg",{"v":170,"d":"170.00"}]
[]
[null,"(d) 60x60x4 Angles","kg",{"v":66,"d":"66.00"}]
[]
[null,"(e) 60x60x3.0 Square Hollow Sections","kg",{"v":434,"d":"434.00"}]
[]
[null,"(f) 10mm Base plates","kg",{"v":40,"d":"40.00"}]
[]
[null,"(g) Cleats, plates, etc.","kg",{"v":60,"d":"60.00"}]
[]
[]
["5.1.2","M20 chemical anchors","No",{"v":16,"d":"16.00"}]
[]
["5.1.3","Sheeting, 0.58mm Galv. IBR 686 sheeting","m2",{"v":42,"d":"42.00"}]
[]
["5.1.4","1.8mm x 75 Galv. Daimond mesh fencing","m2",{"v":76,"d":"76.00"}]
[]
["5.1.5","Double lockable swing gates","No",{"v":2,"d":"2.00"}]
[]
["5.1.6","100x100x2.0  Galvanized gutter","m",{"v":7.8,"d":"7.80"}]
[]
["5.1.7","75mm diameter downpipes with bends","No",{"v":2,"d":"2.00"}]
[]
[]
[5.2,"METHANE, LPG, ARGON SLAB"]
[]
["5.2.1","Steelwork canopy over slab"]
[null,"(Price to include workshop detailing and drawings,"]
[null,"all bolts Gr8.8, Painted to Necsa specs)"]
[null,"All hot rolled steelwork Grade S355JR"]
[null,"Hollow Sections Min Grade 300WA"]
[null,"Cold formed Sections min yield 240 MPa"]
[]
[null,"(a) 100x100x4.0 SHS columns","kg",{"v":175,"d":"175.00"}]
[]
[null,"(b) 160 IPE Rafters","kg",{"v":130,"d":"130.00"}]
[]
[null,"(c) 100x50x20x2.5 Cold formed lipped channels","kg",{"v":110,"d":"110.00"}]
[]
[null,"(d) 60x60x4 Angles","kg",{"v":60,"d":"60.00"}]
[]
[null,"(e) 10mm Base plates","kg",{"v":20,"d":"20.00"}]
[]
[null,"(f) Cleats, plates, etc.","kg",{"v":40,"d":"40.00"}]
[]
["5.2.2","M16 chemical anchors","No",{"v":24,"d":"24.00"}]
[]
["5.2.3","Sheeting, 0.58mm Galv. IBR 686 sheeting","m2",{"v":12,"d":"12.00"}]
[]
["5.2.4","Single lockable swing gates","No",{"v":3,"d":"3.00"}]
[null,"with diamond mesh and frame"]
[]
[]
[5.3,"LIQUID OXYGEN-MAXI SLAB"]
[]
["5.3.1","Steelwork canopy over slab"]
[null,"(Price to include workshop detailing and drawings,"]
[null,"all bolts Gr8.8, Painted to Necsa specs)"]
[null,"All hot rolled steelwork Grade S355JR"]
[null,"Hollow Sections Min Grade 300WA"]
[null,"Cold formed Sections min yield 240 MPa"]
[]
[null,"(a) 160 IPE columns","kg",{"v":270,"d":"270.00"}]
[]
[null,"(b) 160 IPE Rafters","kg",{"v":110,"d":"110.00"}]
[]
[null,"(c) 100x50x20x2.5 Cold formed lipped channels","kg",{"v":60,"d":"60.00"}]
[]
[null,"(d) 60x60x4 Angles","kg",{"v":40,"d":"40.00"}]
[]
[null,"(e) 10mm Base plates","kg",{"v":28,"d":"28.00"}]
[]
[null,"(f) Cleats, plates, etc.","kg",{"v":30,"d":"30.00"}]
[]
[]
["5.3.2","M20 chemical anchors","No",{"v":8,"d":"8.00"}]
[]
["5.3.3","Sheeting, 0.58mm Galv. IBR 686 sheeting","m2",{"v":12,"d":"12.00"}]
[]
["5.3.4","1.8m high Galv, palisade fencing","m",{"v":11,"d":"11.00"}]
[]
["5.3.5","Single lockable Palisade swing gates","No",{"v":1,"d":"1.00"}]
[null,"with posts, galvanized"]
[]
[]
[5.2,"MISCELANEOUS WORKS"]
[]
["5.2.1","Slabs Floor area ","m2",{"v":58,"d":"58.00"}]
[null,"acid resistant epoxy flooring paint"]
[null,"Includes floor cleaning, surface "]
[null,"preparation as per supplier details"]
[]
["5.2.2","220mm Face brick walls, 1.8m high","m2",{"v":1,"d":"1.00"}]
[null,"Brickforce every 3rd layer"]
[]
[]
[]
[]
[]
["TOTAL"]