{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Template Identifier","Column Descriptions","Unit 24 VDC Board A","Unit 24 VDC Board B"],"not_rendered":{"images":3,"external_links":2,"defined_names":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Template Identifier","index":0,"n_rows":15,"n_cols":4,"rows_kept":15,"merged":[[1,0,5,0],[1,1,5,1],[5,2,5,3],[8,0,8,2],[10,0,10,3]],"flags":["formulas_cached_only"]}
[]
[null,"24 VDC Load Schedule Consumer Per Battery Charger Template","Template Identifier","240-72345357 (Rev 3)"]
[null,null,"Document Identifier","<xxx-xxx>"]
[null,null,"Doc Revision","<x.x>"]
[null,null,"Effective Date","2019-02-01"]
[null,null,"Control & Instrumentation Plant CoE"]
[]
["Notes:"]
["The purpose of this template is to capture all 24VDC C&I loads to enable the Electrical CoE to size the Charger and associated power supply equipment."]
[]
["REVISION HISTORY"]
["Date","Remarks","Compiler","Rev."]
["N/A","First Published Version","Andre van den Berg",{"v":1,"d":"1.0"}]
["2018-02-22","Template revised","Andre van den Berg",{"v":2,"d":"2.0"}]
["2019-01-01","Template revised to include columns D9 to D13.\nDesign phase columns added to \"Column Description\" tab.","Christoph Kohlmeyer",{"v":3,"d":"3.0"}]

{"sheet":"Column Descriptions","index":1,"n_rows":20,"n_cols":5,"rows_kept":20,"merged":[[0,0,0,4],[1,0,2,3],[1,4,2,4],[3,1,3,2],[4,1,4,2],[5,1,6,2],[7,1,15,1],[17,1,18,1],[19,1,19,2]],"flags":["formulas_cached_only"]}
["Column Descriptions"]
["Columns",{"$nulls":3},"Descriptions"]
[]
["D1","Number of items",null,null,"How many of these identical cubicles are there in the design?"]
["D2","Description ",null,null,"Text description as shown on documentation."]
["D3","Tag Name",null,"KKS/ AKZ Identification Tag of cabinet","KKS/AKZ Equipment Identification Tag as shown on C&I documentation."]
["D4",null,null,"KKS/ AKZ Identification Tag of feeding circuit (CCT)","KKS/AKZ Equipment Identification Tag as shown on Electrical documentation."]
["D5","Circuit Specifications","Rated Power","(W)","Electrical Power rating of the cabinet. If the feed is dual, this is the rating for each feed."]
["D6",null,"Rated Voltage","(V)","Voltage rating for the cabinet."]
["D7",null,"Nominal Current","(A)","Total Current of the cabinet for feeder calculations."]
["D8",null,"Thermal Power Dissipation","(W)","Calculated Thermal Power dissipation of the cabinet."]
["D9",null,"Standby Time","(min)","Standby Time for the equipment"]
["D10",null,"Single / Dual Supply","(Single /Dual)","Does the load require a single or dual power supply feed."]
["D11",null,"Load Location","Room / Area of Load","Area or Room description of the load (e.g. Unit 1 Equipment room, WTP Control Room, Imcline Coal Conveyer 10B Drive end, ect) "]
["D12",null,"Sub-DB allocation","KKS/ AKZ Description of Sub-DB","Description of Sub-DB feeding the load. This is a Sub-DB fed by the main Charger DB."]
["D13",null,"Sub-DB KKS","KKS/ AKZ Identification Tag of Sub-DB","KKS/AKZ of Sub-DB feeding the load. This is a Sub-DB fed by the main Charger DB."]
["D14",null,"Sub-DB Location","Room / Area of sub-DB","Area or Room description of the sub-DB feeding the load"]
["D15","Physical Properties","Dimensions","(mm)","Width, Height, Depth of the cabinet."]
["D16",null,"Weight","(Kg)","Weight of cabinets to be used by civil department for floor baring calculations"]
["D17","Remarks",null,null,"Enter remarks here to eliminate ambiguity in the requirements."]

{"sheet":"Unit 24 VDC Board A","index":2,"n_rows":33,"n_cols":19,"rows_kept":33,"merged":[[1,1,5,2],[1,3,5,7],[1,14,1,16],[1,17,1,18],[2,14,2,16],[3,14,3,16],[4,14,4,16],[5,14,5,18]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"24 VDC LOAD SCHEDULE CONSUMER TEMPLATE",{"$nulls":10},"Template Identifier",null,null,"240-72345357 (Rev 3)"]
[{"$nulls":14},"Document Identifier",null,null,"<xxx-xxx>"]
[{"$nulls":14},"Revision",null,null,"<x.x>"]
[{"$nulls":14},"Effective Date",null,null,"2019-02-01"]
[{"$nulls":14},"Group Technology"]
[null,"D1","D2","D3","D4","D5","D6","D7",null,"D8","D9","D10","D11","D12","D13","D14","D15","D16","D17"]
[null,"Number of items","Description","KKS code of cabinet","KKS code of feeding CCT","Rated power \n","Rated voltage","Current for feeder calc.","Nominal Current","Thermal power dissipation","Single / Dual Supply","Standby Time","Load Location","Sub-DB Description","Sub-DB KKS","Sub-DB Location","Dimensions of load","Appr. weight of load","Remark"]
[null,"[...]","[...]","[...]","[...]","[W]","[V]","[A]","[A]","[W]","[Single / Dual]","[min]","[…]","[…]","[...]","[...]","[WxHxD in mm]","[kg]"]
[{"$nulls":6}," Total:",null,48.8,{"v":0,"d":"0.0"},{"$nulls":6}," Total:",0]
[null,null,"380/220 VAC Power Distribution Cabinet","0*JD01",19,null,"0+24 V",60,{"v":6,"d":"6.0"},null,"Dual",240,"Unit Equipment room",{"$nulls":5},"This is the 220 V AC essential supply to loads. Fed from 380VAC switchgear.\nRefer to 44744 sheets 1 to 25 for internal wiring diagram of JD01."]
[null,null,"Sampling Control Panel","0*JW01P001",32,null,"0+24 V",16,3.2,null,"Dual",240,"Units 4-6 CPP",{"$nulls":5},"Units 4-6 only. This is a LCS for the CPP"]
[null,null,"Siemens Cubicle","0*JY61",34,null,"0+24 V",16,3.2,null,"Dual",240]
[null,null,"380V Unit Diesel Gen Board","0*CG102",35,null,"0±24V",32,6.4,null,"Dual",240,"Unit LV Room",{"$nulls":5},"Spare on Units 2,3,6."]
[null,null,"3.3KV Station Diesel Gen Board","50FC003",41,null,"0±24V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Station Switchgear Room, Aux bay 11m lvl",{"$nulls":5},"Unit 1 only"]
[null,null,"Rectifier Cubicle","HI003",42,null,"0+24 V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Turbine floor, 11m lvl"]
[null,null,"Excitation Panel","HI002",42,null,"0+24 V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Turbine floor, 11m lvl"]
[null,null,"Automatic Voltage Regulator","HI001",44,null,"0+24 V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Unit Equipment room"]
[null,null,"Siemens 220V DC Power Distribution Cubicle","DU01",48,null,"0+24 V",60,{"v":6,"d":"6.0"},null,"Dual",240,"Unit Equipment room"]
[null,null,"Group 5 Cubicle","0*DY002",70,null,"0+24 V",80,{"v":16,"d":"16.0"},null,"Dual",240,"Behind the SSC NDE",{"$nulls":5},"Loads to be investigated"]
[]
[]
[]
[]
[]
[]
[null,"Index of revisions:",{"$nulls":5},"Date"]
["e.g.","Rev. 0","Preliminary - Status of tender",{"$nulls":4},"2013-11-20"]
[null,"Rev. 1"]
[null,"Rev. 2"]
[null,"Rev. 3"]
[null,"Rev. 4"]
[null,"Rev. 5"]

{"sheet":"Unit 24 VDC Board B","index":3,"n_rows":34,"n_cols":19,"rows_kept":34,"merged":[[1,1,5,2],[1,3,5,7],[1,14,1,16],[1,17,1,18],[2,14,2,16],[3,14,3,16],[4,14,4,16],[5,14,5,18]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"24 VDC LOAD SCHEDULE CONSUMER TEMPLATE",{"$nulls":10},"Template Identifier",null,null,"240-72345357 (Rev 3)"]
[{"$nulls":14},"Document Identifier",null,null,"<xxx-xxx>"]
[{"$nulls":14},"Revision",null,null,"<x.x>"]
[{"$nulls":14},"Effective Date",null,null,"2019-02-01"]
[{"$nulls":14},"Group Technology"]
[null,"D1","D2","D3","D4","D5","D6","D7",null,"D8","D9","D10","D11","D12","D13","D14","D15","D16","D17"]
[null,"Number of items","Description","KKS code of cabinet","KKS code of feeding CCT","Rated power\n(* denotes breaker rating where rated power is not avaialble)","Rated voltage","Current for feeder calc.","Nominal Current","Thermal power dissipation","Single / Dual Supply","Standby Time","Load Location","Sub-DB Description","Sub-DB KKS","Sub-DB Location","Dimensions of load","Appr. weight of load","Remark"]
[null,"[...]","[...]","[...]","[...]","[W]","[V]","[A]","[A]","[W]","[Single / Dual]","[min]","[…]","[…]","[...]","[...]","[WxHxD in mm]","[kg]"]
[{"$nulls":6}," Total:",null,52.8,0,{"$nulls":6}," Total:",0]
[null,null,"380/220 VAC Power Distribution Cabinet","0*JD01",19,null,"0+24 V",60,{"v":6,"d":"6.0"},null,"Dual",240,"Unit Equipment room",{"$nulls":5},"This is the 220 V AC essential supply to loads. Fed from 380VAC switchgear.\nRefer to 44744 sheets 1 to 25 for internal wiring diagram of JD01."]
[null,null,"Sampling Control Panel","0*JW01P001",32,null,"0+24 V",16,3.2,null,"Dual",240,"Units 4-6 CPP",{"$nulls":5},"Units 4-6 only. This is a LCS for the CPP"]
[null,null,"Siemens Cubicle","0*JY61",34,null,"0+24 V",16,3.2,null,"Dual",240]
[null,null,"380V Unit Diesel Gen Board","0*CG102",42,null,"0±24V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Unit LV Room",{"$nulls":5},"Spare on Units 2,3,6."]
[null,null,"3.3KV Station Diesel Gen Board","50FC003",40,null,"0±24V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Station Switchgear Room, Aux bay 11m lvl",{"$nulls":5},"Unit 1 only"]
[null,null,"C&I Workshop PLC Test Bench","04JJ00B001",40,null,"0±24V",10,{"v":2,"d":"2.0"},null,"Single",240,"Unit 4 Aux bay, 22m lvl",{"$nulls":5},"Unit 4 only"]
[null,null,"Rectifier Cubicle","HI003",35,null,"0+24 V",32,6.4,null,"Dual",240,"Turbine floor, 11m lvl"]
[null,null,"Excitation Panel","HI002",43,null,"0+24 V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Turbine floor, 11m lvl"]
[null,null,"Automatic Voltage Regulator","HI001",44,null,"0+24 V",10,{"v":2,"d":"2.0"},null,"Dual",240,"Unit Equipment room"]
[null,null,"Siemens 220V DC Power Distribution Cubicle","DU01",48,null,"0+24 V",60,{"v":12,"d":"12.0"},null,"Dual",240,"Unit Equipment room"]
[null,null,"Group 5 Cubicle","0*DY002",60,null,"0+24 V",60,{"v":12,"d":"12.0"},null,"Dual",240,"Behind the SSC NDE",{"$nulls":5},"Loads to be investigated"]
[]
[]
[]
[]
[]
[]
[null,"Index of revisions:",{"$nulls":5},"Date"]
["e.g.","Rev. 0","Preliminary - Status of tender",{"$nulls":4},"2013-11-20"]
[null,"Rev. 1"]
[null,"Rev. 2"]
[null,"Rev. 3"]
[null,"Rev. 4"]
[null,"Rev. 5"]