{"text_format":"3","workbook":"xls","n_sheets":21,"sheets":["Alterations","Earthworks","Concrete, Formwork & Reinf","Masonry","Waterproofing","Roof Covering","Carpentry and Joinery","Ceilings, Partitions etc.","Floor covering, etc.","Ironmongery","Metalwork","Plastering","Tiling","Glazing","Painting","Ext. Works","Mechanical Works","Provisional Sums","Inspection and Report","Miscellaneous Chargers","SUMMARY"],"not_rendered":{"external_links":1,"defined_names":41},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Alterations","index":0,"n_rows":1137,"n_cols":7,"rows_kept":1137,"flags":["formulas_cached_only"]}
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[null,"SCHEDULE No. 1"]
[]
[null,"ALTERATIONS"]
[]
[null,"NOTES"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"Site inspection"]
[]
[null,"Contractors are required to inspect the site and acquaint themselves with all aspects of the works to be executed under this contract prior to the submission of their tender. No claim whatsoever will be entertained in the event of any unforeseen difficulties arising during the execution of the contract that could have been foreseen by a thorough investigation of the site, drawings and specifications."]
[]
[null,"General"]
[]
[null,"The contractor shall carry out the whole of the The Works with as little mess and noise as possible and with a minimum of disturbance to adjoining premises and their tenants/occupants. He/She shall provide proper protection and provide, erect and maintain in position proper temporary tarpaulins that may be necessary to protect existing fixtures, fittings and furniture during the progress of the works and remove on completion or when directed, all to the satisfaction of the Project Manager/Principal Agent  "]
[null,"Water supply pipes and other piping that may be encountered and found necessary to disconnect or cut, shall be effectually stopped off or grubbed up and removed, and any new connections that may be necessary shall be made with proper fittings, to the satisfaction of the Project Manager/Principal Agent "]
[null,"Doors, fanlights, fittings, frames, linings, etc which are to be re-used shall be thoroughly overhauled before re-fixing, including taking off, easing and re-hanging, cramping up, re-wedging as required and making good cramps, dowels, etc, and easing, oiling, adjusting and repairing ironmongery as necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described. Re-painting or re-vanishing is given separately"]
[null,"Prices for taking out doors, windows, etc. shall include for removal of all beads, architraves, ironmongery, etc"]
[null,"Prices for taking out and removing doors and frames shall include for removing door stops, cabin hooks, etc. and making good floor and wall finishes to match existing"]
[null,"With regards to building up of openings in existing walls, cement screeds and paving, granolithic, tops of walls, etc. shall be levelled and prepared for raising of bricwork"]
[null,"Making good finishes shall include making good of the brick and concrete surfaces onto which the new finishes are applied, where necessary"]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (Doors, windows, fittings, etc)"]
[]
[null,"TEMPORARY BARRIERS, SCREENS ETC"]
[]
[1.1,"Temporary barriers, screens, etc including removal"]
[]
["1.1.1","Half brick barrier wall 3000mm high including cement plaster and two coats interior quality PVA emulsion paint on one side.","m",1,{"v":932.3273248000002,"d":"932.33"},null,0]
[{"$nulls":4},0]
["1.1.2","Dust screen 3000mm high between concrete floor and ceiling formed of suitable timber framing with 250 micron polyethylene sheeting stapled on including corners, ends, etc.","m",1,{"v":185.23871848000005,"d":"185.24"},null,0]
[{"$nulls":4},0]
["1.1.3","Dust screen 3600mm high between concrete floor and ceiling formed of suitable timber framing with 250 micron polyethylene sheeting stapled on including corners, ends, etc.","m",1,{"v":223.26785936000005,"d":"223.27"},null,0]
[{"$nulls":4},0]
["1.1.4","Drywall barrier 3000mm high formed of galvanised steel channel section rails and studs covered on one side with 12,7mm gypsum board panels and finished with two coats interior quality PVA emulsion paint on one side including corners, ends, etc.","m",1,{"v":502.9660568000001,"d":"502.97"},null,0]
[{"$nulls":4},0]
["1.1.5","Drywall barrier 3600mm high formed of galvanised steel channel section rails and studs covered on one side with 12,7mm gypsum board panels and finished with two coats interior quality PVA emulsion paint on one side including corners, ends, etc.","m",1,{"v":603.5592681600001,"d":"603.56"},null,0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"REMOVAL OF EXISTING WORK",null,null,0]
[{"$nulls":4},0]
[1.2,"Break up and removing mass concrete",null,null,0]
[{"$nulls":4},0]
["1.2.1","Steps","m³",1,{"v":197.50618328000002,"d":"197.51"},null,0]
[{"$nulls":4},0]
["1.2.2","85mm thick surface bed","m²",1,{"v":17.17445072,"d":"17.17"},null,0]
[{"$nulls":4},0]
["1.2.3","150mm thick surface bed","m²",1,{"v":29.441915520000006,"d":"29.44"},null,0]
[{"$nulls":4},0]
[1.3,"Break up and removing reinforced concrete including cutting off and removing reinforcement",null,null,0]
[{"$nulls":4},0]
["1.3.1","Steps and landings","m³",1,{"v":206.09340864000004,"d":"206.09"},null,0]
[{"$nulls":4},0]
["1.3.2","Beams","m³",1,{"v":355.7564792000001,"d":"355.76"}]
[{"$nulls":4},0]
["1.3.3","Columns","m³",1,{"v":355.7564792000001,"d":"355.76"}]
[{"$nulls":4},0]
["1.3.4","250mm thick slabs","m²",1,{"v":65.01756344,"d":"65.02"}]
[{"$nulls":4},0]
["1.3.5","Opening through 250mm thick slab not exceeding 2,5m²","no",1,{"v":163.15728184000005,"d":"163.16"}]
[{"$nulls":4},0]
[1.4,"Breaking down and removing brickwork etc.",null,null,0]
[{"$nulls":4},0]
["1.4.1","Mass brickwork","m³",1,{"v":177.87823960000006,"d":"177.88"}]
[{"$nulls":4},0]
["1.4.2","Half brick wall","m²",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.4.3","One brick wall","m²",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["1.4.4","One and a half brick wall","m²",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["1.4.5","280mm Hollow walls of two half brick skins","m²",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
[1.5,"Taking out and removing doors, windows, etc. from brickwork to be demolished",null,null,0]
[{"$nulls":4},0]
["1.5.1","Timber single door and frame not exceeding 2,5m²","no",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["1.5.2","Timber double door and frame exceeding 2,5m² and not exceeding 5,0m²","no",1,{"v":182.78522552,"d":"182.79"}]
[{"$nulls":4},0]
["1.5.3","Timber single door and steel frame not exceeding 2,5m²","no",1,{"v":109.18043672000002,"d":"109.18"}]
[{"$nulls":4},0]
["1.5.4","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m²","no",1,{"v":218.36087344000003,"d":"218.36"}]
[{"$nulls":4},0]
["1.5.5","Timber single door not exceeding 2,5m²","no",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["1.5.6","Timber double door exceeding 2,5m² and not exceeding 5,0m²","no",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["1.5.7","Steel single door and steel frame not exceeding 2,5m2","no",1,{"v":109.18043672000002,"d":"109.18"}]
[{"$nulls":4},0]
["1.5.8","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m²","no",1,{"v":218.36087344000003,"d":"218.36"}]
[{"$nulls":4},0]
["1.5.9","Glazed timber window not exceeding 2,5m²","no",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["1.5.10","Glazed timber window exceeding 2,5m² and not exceeding 5.0m²","no",1,{"v":182.78522552,"d":"182.79"}]
[{"$nulls":4},0]
["1.5.11","Glazed steel window not exceeding 2,5m²","no",1,{"v":109.18043672000002,"d":"109.18"}]
[{"$nulls":4},0]
["1.5.12","Glazed steel window exceeding 2,5m² and not exceeding 5.0m²","no",1,{"v":218.36087344000003,"d":"218.36"}]
[{"$nulls":4},0]
["1.5.13","Glazed aluminium window not exceeding 2,5m²","no",1,{"v":109.18043672000002,"d":"109.18"}]
[{"$nulls":4},0]
["1.5.14","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m²","no",1,{"v":218.36087344000003,"d":"218.36"}]
[{"$nulls":4},0]
[1.6,"Taking out and removing doors, windows, etc. including thresholds, sills, etc. (building up openings elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.6.1","Timber single door and frame not exceeding 2,5m² from half or one brick wall","no",1,{"v":182.78522552,"d":"182.79"}]
[{"$nulls":4},0]
["1.6.2","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from half or one brick wall","no",1,{"v":242.89580304000003,"d":"242.90"}]
[{"$nulls":4},0]
["1.6.3","Timber double door and frame not exceeding 2,5m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.6.4","Timber double door and frame exceeding 2,5m² and not exceeding 5,0m² from half or one brick wall","no",1,{"v":291.9656622400001,"d":"291.97"}]
[{"$nulls":4},0]
["1.6.5","Timber single door and steel frame not exceeding 2,5m² from half brick wall","no",1,{"v":199.95967624000002,"d":"199.96"}]
[{"$nulls":4},0]
["1.6.6","Timber single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":218.36087344000003,"d":"218.36"}]
[{"$nulls":4},0]
["1.6.7","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.6.8","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":291.9656622400001,"d":"291.97"}]
[{"$nulls":4},0]
["1.6.9","Steel single door and frame not exceeding 2,5m² from half or one brick wall","no",1,{"v":199.95967624000002,"d":"199.96"}]
[{"$nulls":4},0]
["1.6.10","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":291.9656622400001,"d":"291.97"}]
[{"$nulls":4},0]
["1.6.11","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":291.9656622400001,"d":"291.97"}]
[{"$nulls":4},0]
["1.6.12","Glazed timber window not exceeding 2,5m² from half or one brick wall","no",1,{"v":182.78522552,"d":"182.79"}]
[{"$nulls":4},0]
["1.6.13","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":242.89580304000003,"d":"242.90"}]
[{"$nulls":4},0]
["1.6.14","Glazed steel window not exceeding 2,5m² from half or one brick  wall","no",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["1.6.15","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.6.16","Glazed aluminium window not exceeding 2,5m² from half or one brick  wall","no",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["1.6.17","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
[1.7,"Taking out doors, windows, etc. including thresholds, sills, etc. and setting aside for re-use (refixing and building up openings elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.7.1","Timber single door and frame not exceeding 2,5m² from half or one brick wall","no",1,{"v":199.95967624000002,"d":"199.96"}]
[{"$nulls":4},0]
["1.7.2","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.7.3","Timber single door and steel frame not exceeding 2,5m² from half brick wall","no",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
["1.7.4","Timber single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["1.7.5","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.7.6","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":320.18083128000006,"d":"320.18"}]
[{"$nulls":4},0]
["1.7.7","Steel single door and steel frame not exceeding 2,5m² from half or one brick wall","no",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["1.7.9","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.7.10","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":320.18083128000006,"d":"320.18"}]
[{"$nulls":4},0]
["1.7.11","Aluminium single door and frame not exceeding 2,5m² from half or one brick wall","no",1,{"v":199.95967624000002,"d":"199.96"}]
[{"$nulls":4},0]
["1.7.12","Aluminium single door and frame exceeding 2,5m² and not exceeding 5,0m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.7.13","Aluminium double door and frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.7.14","Aluminum double door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":320.18083128000006,"d":"320.18"}]
[{"$nulls":4},0]
["1.7.15","Glazed timber window not exceeding 2,5m² from half or one brick wall","no",1,{"v":199.95967624000002,"d":"199.96"}]
[{"$nulls":4},0]
["1.7.16","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.7.17","Glazed steel window not exceeding 2,5m² from half or one brick  wall","no",1,{"v":211.00039456000007,"d":"211.00"}]
[{"$nulls":4},0]
["1.7.18","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.7.19","Glazed aluminium window not exceeding 2,5m² from half or one brick  wall","no",1,{"v":211.00039456000007,"d":"211.00"}]
[{"$nulls":4},0]
["1.7.20","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.7.21","Steel roller shutter door not exceeding 2,5m²  from half or one brick wall","no",1,{"v":190.14570440000003,"d":"190.15"}]
[{"$nulls":4},0]
["1.7.22","Steel roller shutter door exceeding 2,5m² and not exceeding 5.0m² from half or one brick wall","no",1,{"v":267.43073264000003,"d":"267.43"}]
[{"$nulls":4},0]
["1.7.23","Steel roller shutter door exceeding 5.0m² from half or one brick wall","no",1,{"v":398.69260600000007,"d":"398.69"}]
[{"$nulls":4},0]
[1.8,"Taking out and removing doors, windows, etc. including thresholds, sills, etc. and building up openings in brick walls including making good cement plaster on both sides (making good paintwork elsewhere).",null,null,0]
[{"$nulls":4},0]
["1.8.1","Timber single door and frame not exceeding 2,5m² from half brick wall","no",1,{"v":917.6063670400001,"d":"917.61"}]
[{"$nulls":4},0]
["1.8.2","Timber single door and frame not exceeding 2,5m² from one brick wall","no",1,{"v":1603.35764936,"d":"1,603.36"}]
[{"$nulls":4},0]
["1.8.3","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":1718.6718184800004,"d":"1,718.67"}]
[{"$nulls":4},0]
["1.8.4","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3033.7440450400004,"d":"3,033.74"}]
[{"$nulls":4},0]
["1.8.5","Timber single door and steel frame not exceeding 2,5m² from half brick wall","no",1,{"v":936.0075642400002,"d":"936.01"}]
[{"$nulls":4},0]
["1.8.6","Timber single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":1631.5728184000006,"d":"1,631.57"}]
[{"$nulls":4},0]
["1.8.7","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":1750.5672269600002,"d":"1,750.57"}]
[{"$nulls":4},0]
["1.8.8","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.9","Steel single door and steel frame not exceeding 2,5m² from half brick wall","no",1,{"v":936.0075642400002,"d":"936.01"}]
[{"$nulls":4},0]
["1.8.10","Steel single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":1631.5728184000006,"d":"1,631.57"}]
[{"$nulls":4},0]
["1.8.11","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":1750.5672269600002,"d":"1,750.57"}]
[{"$nulls":4},0]
["1.8.12","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.13","Aluminium single door and frame not exceeding 2,5m² from half brick wall","no",1,{"v":936.0075642400002,"d":"936.01"}]
[{"$nulls":4},0]
["1.8.14","Aluminium single door and frame not exceeding 2,5m² from one brick wall","no",1,{"v":1631.5728184000006,"d":"1,631.57"}]
[{"$nulls":4},0]
["1.8.15","Aluminium double door and frame exceeding 2,5m² and not exceeding 5,0m² from half brick wall","no",1,{"v":1750.5672269600002,"d":"1,750.57"}]
[{"$nulls":4},0]
["1.8.16","Aluminium double door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.17","Glazed timber window not exceeding 2,5m² from half brick wall","no",1,{"v":917.6063670400001,"d":"917.61"}]
[{"$nulls":4},0]
["1.8.18","Glazed timber window not exceeding 2,5m² from one brick wall","no",1,{"v":1603.35764936,"d":"1,603.36"}]
[{"$nulls":4},0]
["1.8.19","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from half brick wall","no",1,{"v":1718.6718184800004,"d":"1,718.67"}]
[{"$nulls":4},0]
["1.8.20","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.21","Glazed steel window not exceeding 2,5m² from half brick  wall","no",1,{"v":936.0075642400002,"d":"936.01"}]
[{"$nulls":4},0]
["1.8.22","Glazed steel window not exceeding 2,5m² from one brick  wall","no",1,{"v":1631.5728184000006,"d":"1,631.57"}]
[{"$nulls":4},0]
["1.8.23","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from half brick wall","no",1,{"v":1750.5672269600002,"d":"1,750.57"}]
[{"$nulls":4},0]
["1.8.24","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.25","Glazed aluminium window not exceeding 2,5m² from half brick  wall","no",1,{"v":936.0075642400002,"d":"936.01"}]
[{"$nulls":4},0]
["1.8.26","Glazed aluminium window not exceeding 2,5m² from one brick  wall","no",1,{"v":1631.5728184000006,"d":"1,631.57"}]
[{"$nulls":4},0]
["1.8.27","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m² from half brick wall","no",1,{"v":1750.5672269600002,"d":"1,750.57"}]
[{"$nulls":4},0]
["1.8.28","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.29","Timber shopfront exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3082.8139042400003,"d":"3,082.81"}]
[{"$nulls":4},0]
["1.8.30","Timber shopfront exceeding 5,0m² from one brick wall","no",1,{"v":4624.220856360001,"d":"4,624.22"}]
[{"$nulls":4},0]
[1.9,"Taking out and removing doors, windows, etc. including thresholds, sills, etc. and building up openings in brick walls including making good face brickwork on one side and cement plaster on other side (making good paintwork elsewhere).",null,null,0]
[{"$nulls":4},0]
["1.9.1","Timber single door and frame not exceeding 2,5m² from one brick wall","no",1,{"v":1899.0035510400003,"d":"1,899.00"}]
[{"$nulls":4},0]
["1.9.2","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3626.262594880001,"d":"3,626.26"}]
[{"$nulls":4},0]
["1.9.3","Timber single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":1927.2187200800004,"d":"1,927.22"}]
[{"$nulls":4},0]
["1.9.4","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3674.1057076000006,"d":"3,674.11"}]
[{"$nulls":4},0]
["1.9.5","Steel single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":1927.2187200800004,"d":"1,927.22"}]
[{"$nulls":4},0]
["1.9.6","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3674.1057076000006,"d":"3,674.11"}]
[{"$nulls":4},0]
["1.9.7","Glazed timber window not exceeding 2,5m² from one brick wall","no",1,{"v":1899.0035510400003,"d":"1,899.00"}]
[{"$nulls":4},0]
["1.9.8","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":3626.262594880001,"d":"3,626.26"}]
[{"$nulls":4},0]
["1.9.9","Glazed steel window not exceeding 2,5m² from one brick  wall","no",1,{"v":1927.2187200800004,"d":"1,927.22"}]
[{"$nulls":4},0]
["1.9.10","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":3674.1057076000006,"d":"3,674.11"}]
[{"$nulls":4},0]
["1.9.11","Glazed aluminium window not exceeding 2,5m² from one brick  wall","no",1,{"v":1927.2187200800004,"d":"1,927.22"}]
[{"$nulls":4},0]
["1.9.12","Glazed aluminium window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":3674.1057076000006,"d":"3,674.11"}]
[{"$nulls":4},0]
[{"v":1.1,"d":"1.10"},"Taking out and removing doors, windows, etc. including thresholds, sills, etc. and building up openings in brick walls including making good face brickwork on both side.",null,null,0]
[{"$nulls":4},0]
["1.10.1","Timber single door and frame not exceeding 2,5m² from one brick wall","no",1,{"v":2232.6785936,"d":"2,232.68"}]
[{"$nulls":4},0]
["1.10.2","Timber single door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":4291.159187040001,"d":"4,291.16"}]
[{"$nulls":4},0]
["1.10.3","Timber single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":2259.6670161600005,"d":"2,259.67"}]
[{"$nulls":4},0]
["1.10.4","Timber single door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":2643.638664400001,"d":"2,643.64"}]
[{"$nulls":4},0]
["1.10.5","Timber double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":4340.2290462400015,"d":"4,340.23"}]
[{"$nulls":4},0]
["1.10.6","Steel single door and steel frame not exceeding 2,5m² from one brick wall","no",1,{"v":2643.638664400001,"d":"2,643.64"}]
[{"$nulls":4},0]
["1.10.7","Steel single door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":3092.6278760800005,"d":"3,092.63"}]
[{"$nulls":4},0]
["1.10.8","Steel double door and steel frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":4340.2290462400015,"d":"4,340.23"}]
[{"$nulls":4},0]
["1.10.9","Aluminium single door and frame not exceeding 2,5m² from one brick wall","no",1,{"v":2259.6670161600005,"d":"2,259.67"}]
[{"$nulls":4},0]
["1.10.10","Aluminium single door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":2643.638664400001,"d":"2,643.64"}]
[{"$nulls":4},0]
["1.10.11","Aluminium double door and frame exceeding 2,5m² and not exceeding 5,0m² from one brick wall","no",1,{"v":4340.2290462400015,"d":"4,340.23"}]
[{"$nulls":4},0]
["1.10.12","Glazed timber window not exceeding 2,5m² from one brick wall","no",1,{"v":2232.6785936,"d":"2,232.68"}]
[{"$nulls":4},0]
["1.10.13","Glazed timber window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":4291.159187040001,"d":"4,291.16"}]
[{"$nulls":4},0]
["1.10.14","Glazed steel window not exceeding 2,5m² from one brick  wall","no",1,{"v":2259.6670161600005,"d":"2,259.67"}]
[{"$nulls":4},0]
["1.10.15","Glazed steel window exceeding 2,5m² and not exceeding 5.0m² from one brick wall","no",1,{"v":4340.2290462400015,"d":"4,340.23"}]
[{"$nulls":4},0]
[1.11,"Refixing of existing doors, windows, etc. (removal and setting aside elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.11.1","Setting up and building in timber door frame 813x2032mm high in brickwork, rehanging single door on new 100mm brass hinges and replacing lock with four lever mortice lock","no",1,{"v":855.0422965600002,"d":"855.04"}]
[{"$nulls":4},0]
["1.11.2","Setting up and building in steel door frame 813x2032mm high in brickwork, re-hanging single door and replacing lock with four lever mortice lock","no",1,{"v":855.0422965600002,"d":"855.04"}]
[{"$nulls":4},0]
["1.11.3","Setting up and building in steel door frame 813x2032mm high, including fanlight 813x305mm high in brickwork, rehanging single door and replacing lock with four lever mortice lock","no",1,{"v":855.0422965600002,"d":"855.04"}]
[{"$nulls":4},0]
["1.11.4","Setting up and building in timber double door frame 1600x2032mm high in brickwork, rehanging double door on new 100mm brass hinges and replacing lock with four lever mortice lock including rebated conversion set","no",1,{"v":1283.1768180800002,"d":"1,283.18"}]
[{"$nulls":4},0]
["1.11.5","Setting up and building in steel double door frame 1600x2032mm high, including fanlight 1600x305mm high in brickwork, rehanging double door and replacing lock with four lever mortice lock including rebated conversion set","no",1,{"v":1283.1768180800002,"d":"1,283.18"}]
[{"$nulls":4},0]
["1.11.6","Setting up steel window not exceeding 1,0m² in brickwork and replacing any broken glass panes with 4mm clear float glass","no",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["1.11.7","Setting up wooden window not exceeding 1,0m² in brickwork and replacing any broken glass panes with 4mm clear float glass","no",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["1.11.8","Setting up steel window not exceeding 1,0m² in brickwork and replacing any broken glass panes with 4mm patterned glass","no",1,{"v":390.10538064000013,"d":"390.11"}]
[{"$nulls":4},0]
["1.11.9","Setting up wooden window not exceeding 1,0m² in brickwork and replacing any broken glass panes with 4mm patterned glass","no",1,{"v":390.10538064000013,"d":"390.11"}]
[{"$nulls":4},0]
["1.11.12","Setting up steel window exceeding 1,0m² and not exceeding 2,0m² in brickwork and replacing any broken glass panes with 4mm clear float glass","no",1,{"v":547.1289300800001,"d":"547.13"}]
[{"$nulls":4},0]
["1.11.13","Setting up wooden window exceeding 1,0m² and not exceeding 2,0m² in brickwork and replacing any broken glass panes with 4mm clear float glass","no",1,{"v":547.1289300800001,"d":"547.13"}]
[{"$nulls":4},0]
["1.11.14","Setting up steel window exceeding 1,0m² and not exceeding 2,0m² in brickwork and replacing any broken glass panes with 4mm patterned glass","no",1,{"v":656.3093668000001,"d":"656.31"}]
[{"$nulls":4},0]
["1.11.15","Setting up wooden window exceeding 1,0m² and not exceeding 2,0m² in brickwork and replacing any broken glass panes with 4mm patterned glass","no",1,{"v":656.3093668000001,"d":"656.31"}]
[{"$nulls":4},0]
["1.11.16","Setting up steel window exceeding 2,0m² and not exceeding 3,0m² in brickwork and replacing any broken glass panes with 4mm clear float glass","no",1,{"v":956.8622544000002,"d":"956.86"}]
[{"$nulls":4},0]
["1.11.17","Setting up wooden window exceeding 2,0m² and not exceeding 3,0m² in brickwork and replacing any broken glass panes with 4mm clear float glass","no",1,{"v":956.8622544000002,"d":"956.86"}]
[{"$nulls":4},0]
["1.11.18","Setting up steel window exceeding 2,0m² and not exceeding 3,0m² in brickwork and replacing any broken glass panes with 4mm patterned glass","no",1,{"v":1148.2347052800003,"d":"1,148.23"}]
[{"$nulls":4},0]
["1.11.19","Setting up wooden window exceeding 2,0m² and not exceeding 3,0m² in brickwork and replacing any broken glass panes with 4mm patterned glass","no",1,{"v":1148.2347052800003,"d":"1,148.23"}]
[{"$nulls":4},0]
[null,"Removing, cutting and refixing of door to specified heights as per site condition, eg: tile and floor covering",null,null,0]
[{"$nulls":4},0]
["1.11.20","Single wooden door 813 x2032mm high","no",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["1.11.21","Double wooden door 1600x2032mm high","no",1,{"v":241.66905656000006,"d":"241.67"}]
[{"$nulls":4},0]
["1.11.22","Single alluminium glass door 813 x2032mm high","no",1,{"v":380.29140880000006,"d":"380.29"}]
[{"$nulls":4},0]
["1.11.23","Double alluminium door 1600x2032mm high","no",1,{"v":552.035916,"d":"552.04"}]
[{"$nulls":4},0]
[1.12,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc.",null,null,0]
[{"$nulls":4},0]
["1.12.1","Corrugate sheet iron roof covering, valley linings, ridge flashings and timber purlins","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["1.12.2","Concrete, Harveytile sheet iron tile, slate, thatch, etc. roof covering, valley linings, ridge, hip cappings, flashings and timber brandering,purlins, etc.","m²",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["1.12.3","Pitched corrugated iron roof 10000 x 10000  by not exceeding 2000mm high overall including roof covering, timber trusses, ceilings and cornices, eaves soffit covering, fascias, barge boards, gutters and rainwater pipes ","no",1,{"v":2431.41152336,"d":"2,431.41"}]
[{"$nulls":4},0]
["1.12.4","Timber rafters, beams, etc","m",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["1.12.5","Tongued and grooved timber suspended floor including skirting, joists, bearers, etc","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["1.12.6","Gypsum plasterboard ceilings including cornices, timber brandering, etc","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["1.12.7","Flush plastered gypsum plasterboard suspended ceilings, including cornices, suspension grid, hangers, etc.","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.12.8","Flush plastered gypsum plasterboard bulkheads, including cornices, suspension grid, hangers, etc.","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.12.9","Wood panel bulkheads, including cornices, suspension grid, hangers, etc.","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.12.10","Acoustic tiles suspended ceiling including suspension grid, hangers, etc","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["1.12.11","Acoustic tiles suspended ceiling only","m²",1,{"v":7.973852120000002,"d":"7.97"}]
[{"$nulls":4},0]
["1.12.12","Drywall partitioning 3000mm high including doors, ironmongery, glazed borrowed lights, etc","m",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["1.12.13","Carefully cut out rusted or damaged roof sheeting","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.12.13","Taking down and removing rainwater goods",null,null,0]
[{"$nulls":4},0]
["1.12.13a","100 x 125mm Box gutters including downpipes","m",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
[1.13,"Taking out and removing sundry joinery work",null,null,0]
[{"$nulls":4},0]
["1.13.1","Timber cornices from brickwork","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["1.13.2","Timber skirting from brickwork","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["1.13.3","Timber or asbestos cement sills from brickwork","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["1.13.4","Timber or asbestos cement fascias and barge boards","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
[1.14,"Taking out and removing joinery fittings etc",null,null,0]
[{"$nulls":4},0]
["1.14.1","Timber wall cupboard 600 x 300 x 900mm high","no",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["1.14.2","Timber wall cupboard 900 x 300 x 900mm high","no",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["1.14.3","Timber wall cupboard 1200 x 300 x 900mm high","no",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["1.14.4","Timber floor cupboard 600 x 600 x 900mm high","no",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["1.14.5","Timber floor cupboard 900 x 600 x 900mm high","no",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["1.14.6","Timber floor cupboard 1200 x 600 x 900mm high","no",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["1.14.7","Timber sink cupboard 900 x 600 x 900mm high including disconnecting waste pipe and taps","no",1,{"v":61.33732400000001,"d":"61.34"}]
[{"$nulls":4},0]
["1.14.8","Timber sink cupboard 1200 x 600 x 900mm high including disconnecting waste pipe (new trap and connecting to new waste pipe elsewhere)","no",1,{"v":76.05828176,"d":"76.06"}]
[{"$nulls":4},0]
["1.14.9","Timber sink cupboard 1800 x 600 x 900mm high including disconnecting waste pipe (new trap and connecting to new waste pipe elsewhere)","no",1,{"v":114.08742264000001,"d":"114.09"}]
[{"$nulls":4},0]
["1.14.10","Timber counter 1200 x 600 x 900mm high","no",1,{"v":62.56407048000001,"d":"62.56"}]
[{"$nulls":4},0]
["1.14.11","Timber counter 1600 x 600 x 900mm high","no",1,{"v":62.56407048000001,"d":"62.56"}]
[{"$nulls":4},0]
["1.14.12","Timber counter 1800 x 600 x 900mm high","no",1,{"v":62.56407048000001,"d":"62.56"}]
[{"$nulls":4},0]
["1.14.13","Timber counter 2400 x 600 x 900mm high","no",1,{"v":62.56407048000001,"d":"62.56"}]
[{"$nulls":4},0]
[1.15,"Taking out and removing joinery fittings etc, setting aside for re-use and later refixing in new position",null,null,0]
[{"$nulls":4},0]
["1.15.1","Timber wall cupboard 600 x 300 x 900mm high","no",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["1.15.2","Timber wall cupboard 900 x 300 x 900mm high","no",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["1.15.3","Timber wall cupboard 1200 x 300 x 900mm high","no",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["1.15.4","Timber floor cupboard 600 x 600 x 900mm high","no",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["1.15.5","Timber floor cupboard 900 x 600 x 900mm high","no",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["1.15.6","Timber floor cupboard 1200 x 600 x 900mm high","no",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["1.15.7","Timber sink cupboard 900 x 600 x 900mm high including disconnecting waste pipe and taps","no",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["1.15.8","Timber sink cupboard 1200 x 600 x 900mm high including disconnecting waste pipe (new trap and connecting to new waste pipe elsewhere)","no",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["1.15.9","Timber sink cupboard 1800 x 600 x 900mm high including disconnecting waste pipe (new trap and connecting to new waste pipe elsewhere)","no",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
["1.15.10","Timber counter 1200 x 600 x 900mm high","no",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["1.15.11","Timber counter 1600 x 600 x 900mm high","no",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["1.15.12","Timber counter 1800 x 600 x 900mm high","no",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["1.15.13","Timber counter 2400 x 600 x 900mm high","no",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
[1.16,"Take up and remove wooden wall panneling, vinyl wall covering, wall carpeting, waterproofing, etc.",null,null,0]
[{"$nulls":4},0]
["1.16.1","Wood panels including preparing walls for new finishes.","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["1.16.2","Vinyl wall covering including preparing walls for new finishes.","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.16.3","Carpet wall covering including preparing walls for new finishes.","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.16.4","Derbigum waterproofing from vertical roof sheeting, walls, etc.","m²",1,{"v":30.668662000000005,"d":"30.67"}]
[{"$nulls":4},0]
[1.17,"Take up and remove wood block floor covering, vinyl floor covering, carpeting, waterproofing, etc.",null,null,0]
[{"$nulls":4},0]
["1.17.1","Wood block floor covering including preparing screed for new floor covering.","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["1.17.2","Vinyl tile floor covering including preparing screed for new floor covering.","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.17.3","Vinyl sheet floor covering with welded joints including preparing screed for new floor covering.","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.17.4","Carpet tile floor covering including preparing screed for floor covering","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.17.5","Carpet sheet floor covering including preparing screed for floor covering","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.17.6","Derbigum waterproofing from roof sheeting, wood flooring, etc.","m²",1,{"v":30.668662000000005,"d":"30.67"}]
[{"$nulls":4},0]
[1.18,"Taking out and removing ironmongery",null,null,0]
[{"$nulls":4},0]
["1.18.1","Mortice lock and striking plate from timber door and steel frame","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.2","Mortice lock and striking plate from timber door and wooden frame","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.3","Mortice lock and rebate conversion set from timber doors","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.4","Mortice lock and rebate conversion set from steel doors","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.5","Metal striking plate from steel door frame","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.6","Metal striking plate from timber door frame","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.7","Overhead door closer","no",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.18.8","150mm Metal cabin hook and eye including chamfered hardwood block","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.9","Chromium plated towel rail not exceeding 1000mm long","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.10","Chromium plated toilet roll holder","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.11","Chromium plated hat and coat hook","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.18.12","Side hung window catch","no",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.18.13","Side or top hung window stay","no",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
[1.19,"Taking out/off and removing sundry metalwork",null,null,0]
[{"$nulls":4},0]
["1.19.1","Steel pipe handrail from walls including making good plaster finish","m",1,{"v":30.668662000000005,"d":"30.67"}]
[{"$nulls":4},0]
["1.19.2","Steel balustrade 900mm high from concrete stairs including making good granolithic finish to kerb","m",1,{"v":61.33732400000001,"d":"61.34"}]
[{"$nulls":4},0]
["1.19.3","Steel staircase comprising two flights and one landing, 3.5x2.00m overall on plan and rising 3.20m, including supporting columns, balustrades, etc","no",1,{"v":447.7624652000001,"d":"447.76"}]
[{"$nulls":4},0]
["1.19.4","Steel wire mesh burglar proofing not exceeding 1,0m² bolted to brickwork and making good face brickwork","no",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["1.19.5","Steel wire mesh burglar proofing exceeding 1,0m² and not exceeding 2,0m² bolted to brickwork and making good face brickwork","no",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["1.19.6","Steel wire mesh burglar proofing exceeding 2,0m² and not exceeding 3,0m² bolted to brickwork and making good face brickwork","no",1,{"v":130.03512688,"d":"130.04"}]
[{"$nulls":4},0]
["1.19.7","Steel single leaf security gate not exceeding 2,5m² ","no",1,{"v":107.95369024000001,"d":"107.95"}]
[{"$nulls":4},0]
["1.19.8","Steel double leaf security gate exceeding 2,5m² and not exceeding 5,0m²","no",1,{"v":215.90738048000003,"d":"215.91"}]
[{"$nulls":4},0]
["1.19.9","Sheet metal eaves gutters and rainwater down pipes","m",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
[{"v":1.2,"d":"1.20"},"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screeds, plaster, etc",null,null,0]
[{"$nulls":4},0]
["1.20.1","30mm Granolithic from floors","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.20.2","30mm Granolithic from treads and risers of stairs","m²",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.20.3","Granolithic skirting 100mm high","m",1,{"v":13.494211280000002,"d":"13.49"}]
[{"$nulls":4},0]
["1.20.4","30mm Screed from floors","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.20.5","Internal plaster from walls and columns","m²",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.20.6","Internal plaster from ceilings and beams","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["1.20.7","External plaster from walls, columns and beams","m²",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
[1.21,"Hacking up/off and removing ceramic tile floor and wall finishers including removing mortar bed or backing and  preparing concrete or brick surfaces for new screed, plaster or tile finishers",null,null,0]
[{"$nulls":4},0]
["1.21.1","Tiles to floors","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.21.2","Tiles to treads and risers of stairs","m²",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.21.3","Tiles to walls","m²",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.21.4","Tile skirting 100mm high","m",1,{"v":13.494211280000002,"d":"13.49"}]
[{"$nulls":4},0]
[null,"Sandblasting to finished surfaces",null,null,0]
[{"$nulls":4},0]
["1.21.5","Wall plaster","m²",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["1.21.6","Floor screeds","m²",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
[null,"Taking out and cleaning",null,null,0]
[{"$nulls":4},0]
["1.21.7","Expansion joints not exceeding 300mm deep and prepare to receive new","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
[null,"Scraping off paint in bad conditions and prepare for new paint",null,null,0]
[{"$nulls":4},0]
["1.21.8","On plaster","m2",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.21.9","On gamma zenith","m2",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["1.21.10","On  Ceilings","m2",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["1.21.11","On Metal roofs, doors, frames, etc","m2",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["1.21.12","On Wood","m2",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
[null,"IN HERITAGE BUILDINGS - Scraping off paint in bad conditions and prepare for new paint",null,null,0]
[{"$nulls":4},0]
["1.21.12","On plaster","m2",1,{"v":31.282035240000006,"d":"31.28"}]
[{"$nulls":4},0]
["1.21.13","On gamma zenith","m2",1,{"v":31.282035240000006,"d":"31.28"}]
[{"$nulls":4},0]
["1.21.14","On  Ceilings","m2",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["1.21.15","On Metal roofs, doors, frames, etc","m2",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["1.21.16","On Wood","m2",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
[1.22,"Taking out and removing piping, sanitary fittings, etc including disconnecting piping from fittings and making good floor and wall finishes (making good tiling and paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.22.1","110mm PVC piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.2","75mm PVC piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.3","75mm Galvanised steel piping including fittings and brackets","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["1.22.4","25mm Galvanised steel piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.5","40mm Galvanised steel piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.6","100mm Cast iron piping including fittings and brackets","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["1.22.7","15mm Copper piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.8","22mm Copper piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.9","32mm Copper piping including fittings and brackets","m",1,{"v":3.6802394400000007,"d":"3.68"}]
[{"$nulls":4},0]
["1.22.10","Stainless steel wash hand basin","no",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["1.22.11","Stainless steel sink and drainer on timber cupboard 900 x 600 x 900mm high","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.12","Stainless steel sink and drainer on timber cupboard 1200 x 600 x 900mm high","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.13","Stainless steel sink and drainer on timber cupboard 1800 x 600 x 900mm high","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.22.14","Stainless steel wash trough 1200 x 600 x 900mm high","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.15","Precast concrete wash trough 1200 x 600 x 900mm high","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.16","Vitreous china high level urinal cistern","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.17","Vitreous china wash hand basin","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.18","Vitreous china WC pan and cistern","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.22.19","Vitreous china WC pan and high level cistern","no",1,{"v":61.33732400000001,"d":"61.34"}]
[{"$nulls":4},0]
["1.22.20","Vitreous china WC pan with flush valve","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.22.21","Vitreous china wall hung urinal with flush valve","no",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.22.22","Vitreous china urinal 1200 x 1500mm high including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":381.5181552800001,"d":"381.52"}]
[{"$nulls":4},0]
["1.22.23","Vitreous china urinal 1200 x 1500mm high and high level cistern including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":386.42514120000004,"d":"386.43"}]
[{"$nulls":4},0]
["1.22.24","Stainless steel urinal 900 x 1500mm high including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":255.16326784000006,"d":"255.16"}]
[{"$nulls":4},0]
["1.22.25","Stainless steel high level urinal cistern","no",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["1.22.26","Stainless steel urinal 900 x 1500mm high and high level cistern including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.22.27","Stainless steel urinal 1200 x 1500mm high including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":381.5181552800001,"d":"381.52"}]
[{"$nulls":4},0]
["1.22.28","Stainless steel urinal 1200 x 1500mm high and high level cistern including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["1.22.29","Stainless steel urinal 1800 x 1500mm high including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":509.0997892000001,"d":"509.10"}]
[{"$nulls":4},0]
["1.22.30","Stainless steel urinal 1800 x 1500mm high and high level cistern including breaking up and removing 400mm wide concrete urinal step","no",1,{"v":548.3556765600002,"d":"548.36"}]
[{"$nulls":4},0]
[1.23,"Taking out and removing glass and mirrors",null,null,0]
[{"$nulls":4},0]
["1.23.1","Glass from steel windows including cleaning out rebates and preparing for new glass","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.23.2","Glass from timber windows with beads including cleaning out rebates and preparing for new glass","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["1.23.3","Mirror from wall","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["1.23.4","Mirror from wall, including making good tiling","m²",1,{"v":190.14570440000003,"d":"190.15"}]
[{"$nulls":4},0]
["1.23.5","Stainless steel sheet mirror","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
[1.24,"CUTTING THROUGH FLOORS AND CEILINGS",null,null,0]
[{"$nulls":4},0]
["1.24.1","Cutting through 100mm thick concrete surface bed for 460mm wide concrete wall footing including making good concrete on both sides of new half brick wall.","m",1,{"v":78.51177472000002,"d":"78.51"}]
[{"$nulls":4},0]
["1.24.2","Cutting through 100mm thick concrete surface bed for 700mm wide concrete wall footing including making good concrete on both sides of new one brick wall.","m",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["1.24.3","Cutting through gypsum ceiling and brandering for half brick wall including making good on both sides of wall (new cornices elsewhere)","m",1,{"v":12.2674648,"d":"12.27"}]
[{"$nulls":4},0]
["1.24.4","Cutting through gypsum ceiling and brandering for one brick wall including making good on both sides of wall (new cornices elsewhere)","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["1.24.5","Cutting through \"Nutec\" fibre-cement ceiling and brandering for half brick wall including making good on both sides of wall (new cornices elsewhere)","m",1,{"v":12.2674648,"d":"12.27"}]
[{"$nulls":4},0]
["1.24.6","Cutting through \"Nutec\" fibre-cement ceiling and brandering for one brick wall including making good on both sides of wall (new cornices elsewhere)","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
[null,"BUILDING UP OPENINGS",null,null,0]
[{"$nulls":4},0]
[1.25,"Brickwork in NFP bricks in class II mortar in building up openings",null,null,0]
[{"$nulls":4},0]
["1.25.1","Half brick walls","m²",1,{"v":271.11097208000007,"d":"271.11"}]
[{"$nulls":4},0]
["1.25.2","One brick walls","m²",1,{"v":539.7684512000001,"d":"539.77"}]
[{"$nulls":4},0]
["1.25.3","280mm Cavity wall of two half brick skins","m²",1,{"v":547.1289300800001,"d":"547.13"}]
[{"$nulls":4},0]
["1.25.4","One and half brick walls","m²",1,{"v":810.8794232800002,"d":"810.88"}]
[{"$nulls":4},0]
[1.26,"Sundries",null,null,0]
[{"$nulls":4},0]
["1.26.1","Cutting toothing and bonding new brickwork to existing","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
[1.27,"Face brick pointed with flush or recessed horizontal and vertical joints",null,null,0]
[{"$nulls":4},0]
["1.27.1","Extra over brickwork for face brickwork in patches (PC R3,000.00 for Face brick)","m²",1,{"v":344.7157608800001,"d":"344.72"}]
[{"$nulls":4},0]
["1.27.2","230mm wide brick-on-edge header course lintel","m",1,0]
[{"$nulls":4},0]
["1.27.3","230mm wide brick-on-edge header course sill set sloping and slightly projecting","m",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["1.27.4","Cutting toothing and bonding new face brickwork to existing","m",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
[null,"PREPARATORY WORK TO EXISTING SURFACES",null,null,0]
[{"$nulls":4},0]
[1.28,"Preparatory work to existing surfaces",null,null,0]
[{"$nulls":4},0]
["1.28.1","Cutting out joints of existing brickwork to receive plaster.","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["1.28.2","Hacking face of existing concrete columns, beams, etc to receive plaster","m²",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["1.28.3","Hacking face of existing face brickwork to receive plaster","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["1.28.4","Making good defects in existing screeded floors with \"Pavelite\"","m²",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["1.28.5","Chasing existing brick / concrete walls ","m",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
[null,"MAKING GOOD OF FINISHES ETC.",null,null,0]
[{"$nulls":4},0]
[1.29,"Making good of finishes etc.",null,null,0]
[{"$nulls":4},0]
["1.29.1","Making good brickwork at ends of half brick wall","m",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["1.29.2","Making good brickwork at ends of one brick wall","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.29.3","Making good brickwork at ends of one and half brick wall","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.29.4","Making good brickwork to face of wall where half brick cross wall removed","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.29.5","Making good brickwork to face of wall where one brick cross wall removed","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.29.6","Making good brickwork to face of wall where one and half brick cross wall removed","m",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["1.29.7","Making good face brickwork at ends of half brick wall","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["1.29.8","Making good face brickwork at ends of one brick wall","m",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["1.29.9","Making good face brickwork at ends of one and half brick wall","m",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["1.29.10","Making good face brickwork to face of wall where half brick cross wall removed","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["1.29.11","Making good face brickwork to face of wall where one brick cross wall removed","m",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["1.29.12","Making good face brickwork to face of wall where one and half brick cross wall removed","m",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
[{"v":1.3,"d":"1.30"},"Making good \"Rhino\" gypsum board ceiling and brandering.",null,null,0]
[{"$nulls":4},0]
["1.30.1","Ceilings in patches","m²",1,{"v":127.58163392000003,"d":"127.58"}]
[{"$nulls":4},0]
["1.30.2","Ceilings where half brick walls removed","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["1.30.3","Ceilings where one brick walls removed","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["1.30.4","Ceilings where one and half brick walls removed","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
[1.31,"Making good \"Nutec\" fibre-cement board ceiling and brandering.",null,null,0]
[{"$nulls":4},0]
["1.31.1","Ceilings in patches","m²",1,{"v":132.48861984,"d":"132.49"}]
[{"$nulls":4},0]
["1.31.2","Ceilings where half brick walls removed","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["1.31.3","Ceilings where one brick walls removed","m",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["1.31.4","Ceilings where one and half brick walls removed","m",1,{"v":160.70378888000002,"d":"160.70"}]
[{"$nulls":4},0]
[1.32,"Making good 300x300x2,0mm Vinyl floor tiles",null,null,0]
[{"$nulls":4},0]
["1.32.1","Floors in patches","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["1.32.2","Floors where partitions removed","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.32.3","Floors where half brick walls removed","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.32.4","Floors where one brick walls removed","m",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["1.32.5","Floors where one and half brick walls removed","m",1,{"v":131.26187336000004,"d":"131.26"}]
[{"$nulls":4},0]
[1.33,"Making good 2,0mm \"Superflex\" fully flexible vinyl sheeting ",null,null,0]
[{"$nulls":4},0]
["1.33.1","Floors in patches","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["1.33.2","Floors where partitions removed","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.33.3","Floors where half brick walls removed","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["1.33.4","Floors where one brick walls removed","m",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["1.33.5","Floors where one and half brick walls removed","m",1,{"v":131.26187336000004,"d":"131.26"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[1.34,"Making good 2,5mm \"Superflex\" fully flexible vinyl sheeting ",null,null,0]
[{"$nulls":4},0]
["1.34.1","Floors in patches","m²",1,{"v":206.09340864000004,"d":"206.09"}]
[{"$nulls":4},0]
["1.34.2","Floors where partitions removed","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["1.34.3","Floors where half brick walls removed","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["1.34.4","Floors where one brick walls removed","m",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["1.34.5","Floors where one and half brick walls removed","m",1,{"v":157.02354944000004,"d":"157.02"}]
[{"$nulls":4},0]
[1.35,"Making good 3,5mm \"Industrial floor\" flexible vinyl sheeting ",null,null,0]
[{"$nulls":4},0]
["1.35.1","Floors in patches","m²",1,{"v":266.20398616,"d":"266.20"}]
[{"$nulls":4},0]
["1.35.2","Floors where partitions removed","m",1,{"v":76.05828176,"d":"76.06"}]
[{"$nulls":4},0]
["1.35.3","Floors where half brick walls removed","m",1,{"v":76.05828176,"d":"76.06"}]
[{"$nulls":4},0]
["1.35.4","Floors where one brick walls removed","m",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
["1.35.5","Floors where one and half brick walls removed","m",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
[1.36,"Making good untinted granolithic",null,null,0]
[{"$nulls":4},0]
["1.36.1","Floors in patches","m²",1,{"v":94.45947896000001,"d":"94.46"}]
[{"$nulls":4},0]
["1.36.2","Floors where partitions removed","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["1.36.3","Floors where half brick walls removed","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["1.36.4","Floors where one brick walls removed","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["1.36.5","Floors where one and half brick walls removed","m",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["1.36.6","Floor structural cracks not exceeding 300mm wide and 300mm deep with \"Duraquatz\" sealant including hacking, saw-cutting, structural anchoring and support.","m",1,{"v":962.1986015880002,"d":"962.20"}]
[{"$nulls":4},0]
[1.37,"Making good screed and 300x300x2,0mm Vinyl floor tiles",null,null,0]
[{"$nulls":4},0]
["1.37.1","Floors in patches","m²",1,{"v":193.82594384000006,"d":"193.83"}]
[{"$nulls":4},0]
["1.37.2","Floors where partitions removed","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.37.3","Floors where half brick walls removed","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.37.4","Floors where one brick walls removed","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["1.37.5","Floors where one and half brick walls removed","m",1,{"v":133.71536632000002,"d":"133.72"}]
[{"$nulls":4},0]
[1.38,"Making good screed and 2,0mm \"Superflex\" fully flexible vinyl sheeting ",null,null,0]
[{"$nulls":4},0]
["1.38.1","Floors in patches","m²",1,{"v":193.82594384000006,"d":"193.83"}]
[{"$nulls":4},0]
["1.38.2","Floors where partitions removed","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.38.3","Floors where half brick walls removed","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.38.4","Floors where one brick walls removed","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["1.38.5","Floors where one and half brick walls removed","m",1,{"v":133.71536632000002,"d":"133.72"}]
[{"$nulls":4},0]
[1.39,"Making good screed and 2,5mm \"Superflex\" fully flexible vinyl sheeting ",null,null,0]
[{"$nulls":4},0]
["1.39.1","Floors in patches","m²",1,{"v":228.17484528000003,"d":"228.17"}]
[{"$nulls":4},0]
["1.39.2","Floors where partitions removed","m",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["1.39.3","Floors where half brick walls removed","m",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["1.39.4","Floors where one brick walls removed","m",1,{"v":105.50019728000004,"d":"105.50"}]
[{"$nulls":4},0]
["1.39.5","Floors where one and half brick walls removed","m",1,{"v":182.78522552,"d":"182.79"}]
[{"$nulls":4},0]
[{"v":1.4,"d":"1.40"},"Making good screed and 3,5mm \"Industrial floor\" flexible vinyl sheeting ",null,null,0]
[{"$nulls":4},0]
["1.40.1","Floors in patches","m²",1,{"v":288.28542280000005,"d":"288.29"}]
[{"$nulls":4},0]
["1.40.2","Floors where partitions removed","m",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["1.40.3","Floors where half brick walls removed","m",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["1.40.4","Floors where one brick walls removed","m",1,{"v":132.48861984,"d":"132.49"}]
[{"$nulls":4},0]
["1.40.5","Floors where one and half brick walls removed","m",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
[1.41,"Making good internal cement plaster.",null,null,0]
[{"$nulls":4},0]
["1.41.1","Walls in patches","m²",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["1.41.2","Walls where half brick walls removed.","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["1.41.3","Walls where one brick walls removed.","m",1,{"v":52.75009864000002,"d":"52.75"}]
[{"$nulls":4},0]
["1.41.4","Walls where one and half brick walls removed.","m",1,{"v":71.15129584000002,"d":"71.15"}]
[{"$nulls":4},0]
["1.41.5","Concrete ceilings in patches","m²",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["1.41.6","Concrete ceilings where half brick walls removed","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["1.41.7","Concrete ceilings where one brick walls removed","m",1,{"v":52.75009864000002,"d":"52.75"}]
[{"$nulls":4},0]
["1.41.8","Concrete ceilings where one and half brick walls removed","m",1,{"v":71.15129584000002,"d":"71.15"}]
[{"$nulls":4},0]
["1.41.9","Making good of chased walls","m",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
[1.42,"Making good internal cement plaster including chicken mesh spiked to (bases) walls.",null,null,0]
[{"$nulls":4},0]
["1.43.1","Walls in patches","m²",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["1.43.2","Walls where half brick walls removed.","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.43.3","Walls where one brick walls removed.","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.43.4","Walls where one and half brick walls removed.","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["1.43.5","Concrete ceilings in patches","m²",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["1.43.6","Concrete ceilings where half brick walls removed","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.43.7","Concrete ceilings where one brick walls removed","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.43.8","Concrete ceilings where one and half brick walls removed","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["1.43.9","In scum channels not exceeding 300mm wide","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
[1.44,"Making good internal two coat plaster with gypsum finish",null,null,0]
[{"$nulls":4},0]
["1.44.1","Walls in patches","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["1.44.2","Walls where half brick walls removed.","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.44.3","Walls where one brick walls removed.","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["1.44.4","Walls where one and half brick walls removed.","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["1.44.5","Concrete ceilings in patches","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["1.44.6","Concrete ceilings where half brick walls removed","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.44.7","Concrete ceilings where one brick walls removed","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["1.44.8","Concrete ceilings where one and half brick walls removed","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
[1.45,"Making good external cement plaster.",null,null,0]
[{"$nulls":4},0]
["1.45.1","Walls in patches","m²",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["1.45.2","Walls where half brick walls removed.","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["1.45.3","Walls where one brick walls removed.","m",1,{"v":52.75009864000002,"d":"52.75"}]
[{"$nulls":4},0]
["1.45.4","Walls where one and half brick walls removed.","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
[1.46,"Making good external cement plaster including chicken mesh spiked to (bases) walls.",null,null,0]
[{"$nulls":4},0]
["1.46.1","Walls in patches","m²",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["1.46.2","Walls where half brick walls removed.","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["1.46.3","Walls where one brick walls removed.","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["1.46.4","Walls where one and half brick walls removed.","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
[1.47,"Making good 200x200x4mm white glazed ceramic tiles",null,null,0]
[{"$nulls":4},0]
["1.47.1","Walls in patches","m²",1,{"v":198.73292976000002,"d":"198.73"}]
[{"$nulls":4},0]
["1.47.2","Walls where half brick walls removed.","m",1,{"v":47.843112720000015,"d":"47.84"}]
[{"$nulls":4},0]
["1.47.3","Walls where one brick walls removed.","m",1,{"v":78.51177472000002,"d":"78.51"}]
[{"$nulls":4},0]
["1.47.4","Walls where one and half brick walls removed.","m",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
[null,"OPENINGS THROUGH EXISTING WALLS, ETC.",null,null,0]
[{"$nulls":4},0]
[1.48,"Altering openings",null,null,0]
[{"$nulls":4},0]
["1.48.1","Altering opening in half brick wall where 813 x 2032mm high steel combination door and steel frame removed to form opening for new single door and frame 813 x 2337mm high overall by breaking out brickwork including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":675.9373104800001,"d":"675.94"}]
[{"$nulls":4},0]
["1.48.2","Altering opening in half brick wall where 813 x 2032mm high timber  door and steel frame removed to form opening for new single door and frame 813 x 2337mm high overall by breaking out brickwork including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":675.9373104800001,"d":"675.94"}]
[{"$nulls":4},0]
["1.48.3","Altering opening in one brick wall where 813 x 2032mm high steel combination door and frame removed to form opening for new single door and frame 813 x 2337mm high overall by breaking out brickwork on both sides including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":922.51335296,"d":"922.51"}]
[{"$nulls":4},0]
["1.48.4","Altering opening in one brick wall where 813 x 2032mm high timber door and steel frame removed to form opening for new single door and frame 813 x 2337mm high overall by breaking out brickwork on both sides including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":922.51335296,"d":"922.51"}]
[{"$nulls":4},0]
["1.48.4a","Altering opening in one brick wall where 813 x 2032mm high timber door and steel frame removed to form opening for new single door and frame 945 x 2065mm high overall by breaking out brickwork on both sides including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":988.7576628800002,"d":"988.76"}]
[{"$nulls":4},0]
["1.48.5","Altering opening in one brick wall where 813 x 2032mm high timber door and steel frame removed to form opening for new single door and frame 965 x 2065mm high overall by breaking out brickwork on both sides including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":1069.7229305600001,"d":"1,069.72"}]
[{"$nulls":4},0]
["1.48.6","Altering opening in half brick wall where 813 x 2032mm high steel combination door and steel frame removed to form opening for new single door and frame 965 x 2065mm high overall by breaking out brickwork including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)","no",1,{"v":1069.7229305600001,"d":"1,069.72"}]
[{"$nulls":4},0]
["1.48.7","Altering opening in half brick wall where 813 x 2032mm high timber door and steel frame removed to form opening for new single door and frame 965 x 2337mm high overall by breaking out brickwork including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete with quarry tile finish to threshold (new door and frame and making good paintwork elsewhere)","no",1,{"v":764.2630570400001,"d":"764.26"}]
[{"$nulls":4},0]
["1.48.8","Altering opening in half brick wall where 813 x 2032mm high steel combination door and frame removed to form opening for new single door and frame 965 x 2337mm high overall by breaking out brickwork including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete with quarry tile finish to threshold (new door and frame and making good paintwork elsewhere)","no",1,{"v":764.2630570400001,"d":"764.26"}]
[{"$nulls":4},0]
["1.48.9","Altering opening in one brick wall where 813 x 2032mm high timber door and steel frame removed to form opening for new single door and frame 1613 x 2337mm high overall by breaking out brickwork on both sides including necessary precast concrete lintel and making good plaster on both sides and into reveals with concrete with quarry tile finish to threshold (new door and frame and making good paintwork elsewhere)","no",1,{"v":1484.3632408000003,"d":"1,484.36"}]
[{"$nulls":4},0]
["1.48.10","Altering opening in one brick wall where window not exceeding 2,5m² removed to form opening for new single leaf timber door and steel frame 965 x 2065mm high overall by breaking out brickwork on both sides and bottom including necessary precast concrete lintel and making good plaster on both sides (new door and frame and making good paintwork elsewhere)","no",1,{"v":988.7576628800002,"d":"988.76"}]
[{"$nulls":4},0]
["1.48.11","Altering opening in one brick wall where window not exceeding 2,5m² removed to form opening for new double leaf timber door and steel frame 1575 x 2065mm high overall by breaking out brickwork on both sides and bottom including necessary precast concrete lintel and making good plaster on both sides (new door and frame and making good paintwork elsewhere)","no",1,{"v":1153.1416912000002,"d":"1,153.14"}]
[{"$nulls":4},0]
["1.48.12","Altering opening in one brick wall where window not exceeding 2,5m² removed to form opening for new single leaf timber door and steel frame 1575 x 2065mm high overall by breaking out brickwork on both sides and bottom including necessary precast concrete lintel and making good plaster on one side and into reveals and face brickwork on other side and into reveals (new door and frame and making good paintwork elsewhere)","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
[1.49,"Breaking out for and forming plain openings through brick walls including necessary precast concrete lintels and making good plaster on both sides and into reveals and with concrete thresholds with steel trowelled finish (making good paintwork elsewhere",null,null,0]
[{"$nulls":4},0]
["1.49.1","Opening 900 x 2100mm high through half brick wall","no",1,{"v":691.8850147200001,"d":"691.89"}]
[{"$nulls":4},0]
["1.49.2","Opening 1200 x 2100mm high through half brick wall","no",1,{"v":760.5828176000001,"d":"760.58"}]
[{"$nulls":4},0]
["1.49.3","Opening 1500 x 2100mm high through half brick wall","no",1,{"v":830.50736696,"d":"830.51"}]
[{"$nulls":4},0]
["1.49.4","Opening 900 x 2100mm high through one brick wall","no",1,{"v":1037.82752208,"d":"1,037.83"}]
[{"$nulls":4},0]
["1.49.5","Opening 1200 x 2100mm high through one brick wall","no",1,{"v":1107.7520714400002,"d":"1,107.75"}]
[{"$nulls":4},0]
["1.49.6","Opening 1500 x 2100mm high through one brick wall","no",1,{"v":1176.4498743200002,"d":"1,176.45"}]
[{"$nulls":4},0]
["1.49.7","Opening 900 x 2100mm high through one and half brick wall","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
["1.49.8","Opening 1200 x 2100mm high through one and half brick wall","no",1,{"v":1454.9213252800002,"d":"1,454.92"}]
[{"$nulls":4},0]
["1.49.9","Opening 1500 x 2100mm high through one and half brick wall","no",1,{"v":1522.3923816800002,"d":"1,522.39"}]
[{"$nulls":4},0]
["1.49.10.","Breaking out for and forming plain openings through brick walls including necessary precast concrete lintels and making good plaster on side and face brick on the other and into reveals and with concrete thresholds with steel trowelled finish (making good paintwork elsewhere",null,null,0]
[{"$nulls":4},0]
["1.49.10a","Opening 900 x 2100mm high through half brick wall","no",1,{"v":726.4792654560002,"d":"726.48"}]
[{"$nulls":4},0]
["1.49.10b","Opening 1200 x 2100mm high through half brick wall","no",1,{"v":798.6119584800001,"d":"798.61"}]
[{"$nulls":4},0]
["1.49.10c","Opening 1500 x 2100mm high through half brick wall","no",1,{"v":872.0327353080003,"d":"872.03"}]
[{"$nulls":4},0]
["1.49.10d","Opening 900 x 2100mm high through one brick wall","no",1,{"v":1089.718898184,"d":"1,089.72"}]
[{"$nulls":4},0]
["1.49.10e","Opening 1200 x 2100mm high through one brick wall","no",1,{"v":1163.1396750120002,"d":"1,163.14"}]
[{"$nulls":4},0]
["1.49.10f","Opening 1500 x 2100mm high through one brick wall","no",1,{"v":1235.2723680360002,"d":"1,235.27"}]
[{"$nulls":4},0]
["1.49.10g","Opening 900 x 2100mm high through one and half brick wall","no",1,{"v":1452.9585309120005,"d":"1,452.96"}]
[{"$nulls":4},0]
["1.49.10h","Opening 1200 x 2100mm high through one and half brick wall","no",1,{"v":1527.6673915440003,"d":"1,527.67"}]
[{"$nulls":4},0]
["1.49.10i","Opening 1500 x 2100mm high through one and half brick wall","no",1,{"v":1598.512000764,"d":"1,598.51"}]
[{"$nulls":4},0]
["1.49.11.","Breaking out for and forming plain openings through brick walls including necessary precast concrete lintels and making good plaster on side and face brick on the other and into reveals and with concrete thresholds with steel trowelled finish (making good paintwork elsewhere",null,null,0]
[{"$nulls":4},0]
["1.49.11a","Opening 900 x 2100mm high through half brick wall","no",1,{"v":762.8032287288001,"d":"762.80"}]
[{"$nulls":4},0]
["1.49.11b","Opening 1200 x 2100mm high through half brick wall","no",1,{"v":838.5425564040002,"d":"838.54"}]
[{"$nulls":4},0]
["1.49.11c","Opening 1500 x 2100mm high through half brick wall","no",1,{"v":915.6343720734002,"d":"915.63"}]
[{"$nulls":4},0]
["1.49.11d","Opening 900 x 2100mm high through one brick wall","no",1,{"v":1144.2048430932005,"d":"1,144.20"}]
[{"$nulls":4},0]
["1.49.11e","Opening 1200 x 2100mm high through one brick wall","no",1,{"v":1221.2966587626004,"d":"1,221.30"}]
[{"$nulls":4},0]
["1.49.11f","Opening 1500 x 2100mm high through one brick wall","no",1,{"v":1297.0359864378004,"d":"1,297.04"}]
[{"$nulls":4},0]
["1.49.11g","Opening 900 x 2100mm high through one and half brick wall","no",1,{"v":1525.6064574576003,"d":"1,525.61"}]
[{"$nulls":4},0]
["1.49.11h","Opening 1200 x 2100mm high through one and half brick wall","no",1,{"v":1604.0507611212001,"d":"1,604.05"}]
[{"$nulls":4},0]
["1.49.11i","Opening 1500 x 2100mm high through one and half brick wall","no",1,{"v":1678.4376008022004,"d":"1,678.44"}]
[{"$nulls":4},0]
[{"v":1.5,"d":"1.50"},"Breaking out for and forming plain openings through brick walls for new doors and frames including necessary precast concrete lintels and making good plaster on both side and into reveals and with concrete threshold with steel trowelled finish (new door and frame and making good paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.50.1","Opening for door with steel frame 880 x 2065mm high overall through half brick wall","no",1,{"v":691.8850147200001,"d":"691.89"}]
[{"$nulls":4},0]
["1.50.2","Opening for door with steel frame 964 x 2065mm high overall through half brick wall","no",1,{"v":691.8850147200001,"d":"691.89"}]
[{"$nulls":4},0]
["1.50.3","Opening for door with steel frame 1575 x 2065mm high overall through half brick wall","no",1,{"v":830.50736696,"d":"830.51"}]
[{"$nulls":4},0]
["1.50.4","Opening for door with steel frame 880 x 2065mm high overall through one brick wall","no",1,{"v":1037.82752208,"d":"1,037.83"}]
[{"$nulls":4},0]
["1.50.5","Opening for door with steel frame 964 x 2065mm high overall through one brick wall","no",1,{"v":1037.82752208,"d":"1,037.83"}]
[{"$nulls":4},0]
["1.50.6","Opening for door with steel frame 1575 x 2065mm high overall through one brick wall","no",1,{"v":1176.4498743200002,"d":"1,176.45"}]
[{"$nulls":4},0]
["1.50.7","Opening for door with steel frame 880 x 2065mm high overall through one and half brick wall","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
["1.50.8","Opening for door with steel frame 964 x 2065mm high overall through one and half brick wall","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
["1.50.9","Opening for door with steel frame 1575 x 2065mm high overall through one and half brick wall","no",1,{"v":1522.3923816800002,"d":"1,522.39"}]
[{"$nulls":4},0]
["1.50.10","Opening for door with timber frame 880 x 2065mm high overall through half brick wall","no",1,{"v":691.8850147200001,"d":"691.89"}]
[{"$nulls":4},0]
["1.50.11","Opening for door with timber frame 964 x 2065mm high overall through half brick wall","no",1,{"v":691.8850147200001,"d":"691.89"}]
[{"$nulls":4},0]
["1.50.12","Opening for door with timber frame 1575 x 2065mm high overall through half brick wall","no",1,{"v":830.50736696,"d":"830.51"}]
[{"$nulls":4},0]
["1.50.13","Opening for door with timber frame 880 x 2065mm high overall through one brick wall","no",1,{"v":1037.82752208,"d":"1,037.83"}]
[{"$nulls":4},0]
["1.50.14","Opening for door with timber frame 964 x 2065mm high overall through one brick wall","no",1,{"v":1037.82752208,"d":"1,037.83"}]
[{"$nulls":4},0]
["1.50.15","Opening for door with timber frame 1575 x 2065mm high overall through one brick wall","no",1,{"v":1176.4498743200002,"d":"1,176.45"}]
[{"$nulls":4},0]
["1.50.16","Opening for door with timber frame 880 x 2065mm high overall through one and half brick wall","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
["1.50.17","Opening for door with timber frame 964 x 2065mm high overall through one and half brick wall","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
["1.50.18","Opening for door with timber frame 1575 x 2065mm high overall through one and half brick wall","no",1,{"v":1522.3923816800002,"d":"1,522.39"}]
[{"$nulls":4},0]
[1.51,"Breaking out for and forming openings through brick walls for new windows including necessary precast concrete lintels and making good plaster on both sides and into reveals (new windows, sills and making good paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.51.1","Opening for window not exceeding 2,5m² through half brick wall","no",1,{"v":836.6410993600001,"d":"836.64"}]
[{"$nulls":4},0]
["1.51.2","Opening for window exceeding 2,5m² and not exceeding 5.0m²  through half brick wall","no",1,{"v":978.9436910400001,"d":"978.94"}]
[{"$nulls":4},0]
["1.51.3","Opening for window not exceeding 2,5m² through one brick wall","no",1,{"v":1153.1416912000002,"d":"1,153.14"}]
[{"$nulls":4},0]
["1.51.4","Opening for window exceeding 2,5m² and not exceeding 5.0m²  through one brick wall","no",1,{"v":1383.7700294400001,"d":"1,383.77"}]
[{"$nulls":4},0]
["1.51.5","Opening for window not exceeding 2,5m² through one and half brick wall","no",1,{"v":1469.6422830400006,"d":"1,469.64"}]
[{"$nulls":4},0]
["1.51.6","Opening for window exceeding 2,5m² and not exceeding 5.0m²  through one and half brick wall","no",1,{"v":1788.59636784,"d":"1,788.60"}]
[{"$nulls":4},0]
[1.52,"Breaking out for and forming openings through brick walls for new windows including necessary precast concrete lintels and making good plaster on one side and into reveals and face brickwork on other side and into reveals (new windows, sills and making good paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.52.1","Opening for window not exceeding 2,5m² through half brick wall","no",1,{"v":878.3504796800001,"d":"878.35"}]
[{"$nulls":4},0]
["1.52.2","Opening for window exceeding 2,5m² and not exceeding 5.0m²  through half brick wall","no",1,{"v":1028.0135502400003,"d":"1,028.01"}]
[{"$nulls":4},0]
["1.52.3","Opening for window not exceeding 2,5m² through one brick wall","no",1,{"v":1210.7987757600001,"d":"1,210.80"}]
[{"$nulls":4},0]
["1.52.4","Opening for window exceeding 2,5m² and not exceeding 5.0m²  through one brick wall","no",1,{"v":1453.6945788000003,"d":"1,453.69"}]
[{"$nulls":4},0]
["1.52.5","Opening for window not exceeding 2,5m² through one and half brick wall","no",1,{"v":1543.2470718400002,"d":"1,543.25"}]
[{"$nulls":4},0]
["1.52.6","Opening for window exceeding 2,5m² and not exceeding 5.0m²  through one and half brick wall","no",1,{"v":1879.37560736,"d":"1,879.38"}]
[{"$nulls":4},0]
[1.53,"Breaking out one course brickwork and istall 110 x 75mm precast concrete lintel and making good plaster on one side (making good paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["1.53.1","In half brickwall","m",1,{"v":314.0470988800001,"d":"314.05"}]
[{"$nulls":4},0]
["1.53.2","In one brickwall","m",1,{"v":628.0941977600002,"d":"628.09"}]
{"$rows_empty":18}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Earthworks","index":1,"n_rows":359,"n_cols":7,"rows_kept":359,"flags":["formulas_cached_only"]}
[]
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 2"]
[]
[null,"EARTHWORKS (PROVISIONAL)"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Nature of ground"]
[]
[null,"No soil investigation is available."]
[]
[null,"Carting away of excavated material"]
[]
[null,"Descriptions of carting away of excavated material shall be deemed to include loading excavated material onto trucks directly from the excavations or, alternatively, from stock piles situated on the building site."]
[]
[null,"Subterranean water"]
[]
[null,"No information regarding subterranean water is available.  The contractor must acquaint himself of the presence and depth of subterranean water and allow therefore in his rates."]
[]
[null,"Prices"]
[]
[null,"Prices for all filling and carting away of surplus materials must make allowance for bulking."]
[]
[null,"Carting away of excavated material"]
[]
[null,"Descriptions of carting away of excavated material shall be deemed to include loading excavated material onto trucks directly from the excavations or, alternatively, from stock piles situated on the building site"]
[]
[null,"DEMOLITIONS ETC"]
[]
[2.1,"Breaking up and removing"]
[]
["2.1.1","85mm thick concrete surface beds, paving, etc","m²",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["2.1.2","100mm thick concrete surface beds, paving, etc","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["2.1.3","150mm thick concrete surface beds, paving, etc","m²",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["2.1.4","85mm thick mesh reinforced concrete surface beds, paving, etc","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["2.1.5","100mm thick mesh reinforced concrete surface beds, paving, etc","m²",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
["2.1.6","150mm thick mesh reinforced concrete surface beds, paving, etc","m²",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["2.1.7","60mm thick brick paving with mortar joints","m²",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["2.1.8","80mm thick brick paving with mortar joints","m²",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["2.1.9","300 x 300 x 30mm thick paving","m²",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["2.1.10","230 x 75mm concrete kerb","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["2.1.11","300 x 150mm half-battered concrete kerb","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["2.1.12","280 x 180 x 140mm mountable concrete kerb","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["2.1.13","300 x 200 x 100mm mountable concrete kerb","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["2.1.14","230 x 110mm brick kerb with mortar joints","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
[2.2,"Take down and removing",null,null,0]
[{"$nulls":4},0]
["2.2.5","Steel palisade, round bar, square tube, etc. gate size 813 x 2032mm high ","no",1,{"v":128.80838040000003,"d":"128.81"}]
[{"$nulls":4},0]
["2.2.6","Steel palisade, round bar, square tube, etc. gate size 1200 x 2032mm high ","no",1,{"v":128.80838040000003,"d":"128.81"}]
[{"$nulls":4},0]
["2.2.7","Steel sliding palisade, round bar, square tube, etc. gate size 6000 x 1800mm high ","no",1,{"v":300.5528876,"d":"300.55"}]
[{"$nulls":4},0]
["2.2.8","Steel two leaf palisade, round bar, square tube, etc. gate size 6000 x 1800mm high ","no",1,{"v":300.5528876,"d":"300.55"}]
[{"$nulls":4},0]
["2.2.9","Steel burglar gates, screens, etc. size 813 x 2032mm high ","no",1,{"v":128.80838040000003,"d":"128.81"}]
[{"$nulls":4},0]
["2.2.10","Steel burglar gates, screens, etc. size 1626 x 2032mm high ","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["2.2.11","Steel two leaf palisade, round bar, square tube, etc. fence panel size3000 x 1800mm high ","no",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
["2.2.12","Diamond mesh fence 2,1m high with flat wrap razor wire fixed to top and bottom and 750mm high overall with steel post and droppers","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["2.2.12a","Diamond mesh fence 1.2 m high formed of 50mm mesh chain link netting 2.5 mm diameter galvanised mild steel wire stained and secured to top and bottom rails and posts","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["2.2.13","Half brick, precast, etc. boundary or yard wall 1,8m high","m",1,{"v":159.47704240000004,"d":"159.48"}]
[{"$nulls":4},0]
["2.2.14","One brick boundary or yard wall 1,8m high","m",1,{"v":291.9656622400001,"d":"291.97"}]
[{"$nulls":4},0]
["2.2.15","Steel Palisade fencing not exceeding 2400mm high","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["2.2.16","Concrete Palisade fencing not exceeding 2400mm high","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["2.2.17","Wooden picket fence 1500mm high","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
[null,"SITE CLEARANCE, ETC.",null,null,0]
[{"$nulls":4},0]
[null,"User Note",null,null,0]
[{"$nulls":4},0]
[null,"Where the value is of significance, the removal of hedges, etc. shall be given separately in meters or in number",null,null,0]
[{"$nulls":4},0]
[2.3,"Site clearance",null,null,0]
[{"$nulls":4},0]
["2.3.1","Dig up and remove rubbish, debris, vegetation, hedges, shrubs and trees not exceeding 200mm girth, bush etc.","m²",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["2.3.1a","Dig up and remove contaminated rubbish, debris","m3",1,{"v":138.87696000000003,"d":"138.88"}]
[{"$nulls":4},0]
["2.3.2","Strip average 150mm. thick layer top soil and stockpile on site where directed","m²",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["2.3.3","Rip, scarify and compact ground 150mm average","m²",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["2.3.4","Carting away rubble up to 5km radius (to dumping area, return distance not covered)","m3",1,{"v":75.22502000000001,"d":"75.23"}]
[{"$nulls":4},0]
["2.3.5","Overhaul exceeding 5km limited overhaul to dumping area, return distance not covered","m³-km",1,{"v":15.334331000000002,"d":"15.33"}]
[{"$nulls":4},0]
[null,"REMOVAL OF TREES, ETC.",null,null,0]
[{"$nulls":4},0]
[2.4,"Taking out and removing, grubbing up roots and filling in holes",null,null,0]
[{"$nulls":4},0]
["2.4.1","Tree stump exceeding 200mm. and not exceeding 500mm. girth","no",1,{"v":1594.7704240000003,"d":"1,594.77"}]
[{"$nulls":4},0]
["2.4.2","Tree stump exceeding 500mm. and not exceeding 1000mm. girth","no",1,{"v":2330.8183120000003,"d":"2,330.82"}]
[{"$nulls":4},0]
["2.4.3","Tree stump exceeding 1000mm. and not exceeding 2000mm. girth","no",1,{"v":3373.552820000001,"d":"3,373.55"}]
[{"$nulls":4},0]
["2.4.4","Tree stump exceeding 2000mm. and not exceeding 3000mm. girth","no",1,{"v":4416.287328,"d":"4,416.29"}]
[{"$nulls":4},0]
[2.5,"Cutting down and removing, grubbing up roots and filling in holes including importing filling where required",null,null,0]
[{"$nulls":4},0]
["2.5.1","Hedge not exceeding 1500mm high","m",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["2.5.2","Hedge exceeding 1500mm high and not exceeding 2500mm high","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["2.5.3","Tree exceeding 200mm. and not exceeding 500mm. girth","no",1,{"v":1833.9859876,"d":"1,833.99"}]
[{"$nulls":4},0]
["2.5.4","Tree exceeding 500mm. and not exceeding 1000mm. girth","no",1,{"v":2680.4410588000005,"d":"2,680.44"}]
[{"$nulls":4},0]
["2.5.5","Tree exceeding 1000mm. and not exceeding 2000mm. girth","no",1,{"v":5078.7304272,"d":"5,078.73"}]
[{"$nulls":4},0]
["2.5.6","Tree exceeding 2000mm. and not exceeding 3000mm. girth","no",1,{"v":13324.613579140001,"d":"13,324.61"}]
[{"$nulls":4},0]
[null,"Cutting of tree excluding tree stump and carting away off site",null,null,0]
["2.5.7","Tree exceeding 200mm. and not exceeding 500mm. girth","no",1,{"v":1328.9753533333337,"d":"1,328.98"}]
[{"$nulls":4},0]
["2.5.8","Tree exceeding 500mm. and not exceeding 1000mm. girth","no",1,{"v":1942.3485933333338,"d":"1,942.35"}]
[{"$nulls":4},0]
["2.5.9","Tree exceeding 1000mm. and not exceeding 2000mm. girth","no",1,{"v":2811.294016666667,"d":"2,811.29"}]
[{"$nulls":4},0]
["2.5.10","Tree exceeding 2000mm. and not exceeding 3000mm. girth","no",1,{"v":3680.2394400000007,"d":"3,680.24"}]
[{"$nulls":4},0]
[null,"BULK EXCAVATION, FILLING, ETC.",null,null,0]
[{"$nulls":4},0]
[null,"User Note",null,null,0]
[{"$nulls":4},0]
[null,"This section is given as an alternative option and in the event of it being utilised, the excavation, filling, etc other than bulk is to be given in the later section under the appropriate heading",null,null,0]
[null,"If this alternative is not utilised, then all excavations, etc (bulk and otherwise) is to be given in the later section under the appropriated heading",null,null,0]
[{"$nulls":4},0]
[null,"EXCAVATION, FILLING, ETC.",null,null,0]
[{"$nulls":4},0]
[2.6,"Open face excavations in earth over sloping site",null,null,0]
[{"$nulls":4},0]
["2.6.1","Open face excavations","m³",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
[2.7,"Excavation in earth not exceeding 2m. deep",null,null,0]
[{"$nulls":4},0]
["2.7.1","Reducing levels under floors","m³",1,{"v":78.51177472000002,"d":"78.51"}]
[{"$nulls":4},0]
["2.7.2","Trenches.","m³",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["2.7.3","Holes","m³",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["2.7.4","Trenches and holes for thickening under surface beds etc.","m³",1,{"v":78.51177472000002,"d":"78.51"}]
[{"$nulls":4},0]
[null,"Hand excavation to expose existing services where ordered by the Engineer / QS ",null,null,0]
[{"$nulls":4},0]
["2.7.5","In Soft material","m³",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["2.7.6","In Intermediate material","m³",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["2.7.7","In Hard material",null,null,0]
[null,null,"m³",1,{"v":466.1636624000001,"d":"466.16"}]
[2.8,"Extra over Blasting of trench and hole excavations in earth for excavation in",null,null,0]
[{"$nulls":4},0]
["2.8.1","Soft rock.","m³",1,{"v":525.0474934400002,"d":"525.05"}]
[{"$nulls":4},0]
["2.8.2","Hard rock.","m³",1,{"v":1221.8394940800001,"d":"1,221.84"}]
[{"$nulls":4},0]
["2.8.3","Back excavation in earth for working space for excavation in soft rock","m2",1,{"v":134.94211280000002,"d":"134.94"}]
[{"$nulls":4},0]
[2.9,"Extra over excavations in earth for breaking up and removing",null,null,0]
[{"$nulls":4},0]
["2.9.1","Brickwork","m³",1,{"v":333.67504256,"d":"333.68"}]
[{"$nulls":4},0]
["2.9.2","Unreinforced concrete","m³",1,{"v":333.67504256,"d":"333.68"}]
[{"$nulls":4},0]
["2.9.3","Reinforced concrete","m³",1,{"v":668.5768316000001,"d":"668.58"}]
[{"$nulls":4},0]
[{"v":2.1,"d":"2.10"},"Extra over all excavations for carting away",null,null,0]
[{"$nulls":4},0]
["2.10.1","Surplus material from excavations and /or stock pile on site to a dumping site to be located by the contractor (up to a radius of 5km - return distance not covered)","m³",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["2.10.2","Overhaul exceeding 5km limited overhaul to dumping area, return distance not covered","m³-km",1,{"v":15.334331000000002,"d":"15.33"}]
[{"$nulls":4},0]
[2.11,"Risk of collapse of excavations",null,null,0]
[{"$nulls":4},0]
["2.11.1","Sides of trench and hole excavations not exceeding 1,5m deep including keeping excavations free from water","m²",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
["2.11.2","Sides of trench and hole excavations exceeding 1,5m deep including keeping excavations free from water.","m²",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
["2.11.3","Sides of bulk excavations not exceeding 1,5m deep including keeping excavations free from water","m²",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
["2.11.4","Sides of bulk excavations exceeding 1,5m deep including keeping excavations free from water.","m²",1,{"v":12.2674648,"d":"12.27"}]
[{"$nulls":4},0]
[2.12,"Keeping excavations free of water",null,null,0]
[{"$nulls":4},0]
["2.12.1","Keeping excavations free of water other than subterranean water","Item",1,{"v":736.0478880000001,"d":"736.05"}]
[{"$nulls":4},0]
[2.13,"Earth filling obtained from excavations and/or prescribed stock piles on site (not compacted) ",null,null,0]
[{"$nulls":4},0]
["2.13.1","Over site","m³",1,{"v":89.55249304000002,"d":"89.55"}]
[{"$nulls":4},0]
["2.13.2","Landscape mounds, berms, etc","m³",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
[2.14,"Earth filling obtained from excavations and/or prescribed stock piles on site compacted to 95% Mod AASHTO density ",null,null,0]
[{"$nulls":4},0]
["2.14.1","Under floors, steps, pavings, etc.","m³",1,{"v":88.32574656000003,"d":"88.33"}]
[{"$nulls":4},0]
["2.14.2","Backfill behind retaining walls","m³",1,{"v":93.23273248000002,"d":"93.23"}]
[{"$nulls":4},0]
["2.14.3","Backfill to trenches, holes, etc.","m³",1,{"v":93.23273248000002,"d":"93.23"}]
[{"$nulls":4},0]
["2.14.4","Over site to make up levels","m³",1,{"v":93.23273248000002,"d":"93.23"}]
[{"$nulls":4},0]
["2.14.5","Bedding","m³",1,{"v":93.23273248000002,"d":"93.23"}]
[{"$nulls":4},0]
[2.15,"Earth filling supplied by the contractor compacted to 95% Mod AASHTO density.",null,null,0]
[{"$nulls":4},0]
["2.15.1","Under floors, steps, pavings, etc.","m³",1,{"v":356.9832256800001,"d":"356.98"}]
[{"$nulls":4},0]
["2.15.2","Backfill behind retaining walls","m³",1,{"v":361.89021160000004,"d":"361.89"}]
[{"$nulls":4},0]
["2.15.3","Backfill to trenches, holes, etc.","m³",1,{"v":361.89021160000004,"d":"361.89"}]
[{"$nulls":4},0]
[2.16,"Garden top soil filling obtained from the excavations and/or prescribed stock piles on site",null,null,0]
[{"$nulls":4},0]
["2.16.1","In flower boxes","m³",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["2.16.2","Over site","m³",1,{"v":78.51177472000002,"d":"78.51"}]
[{"$nulls":4},0]
["2.16.3","Landscape mounds, berms, etc","m³",1,{"v":88.32574656000003,"d":"88.33"}]
[{"$nulls":4},0]
[2.17,"Garden top soil filling supplied by the contractor",null,null,0]
[{"$nulls":4},0]
["2.17.1","In flower boxes","m³",1,{"v":564.3033808000001,"d":"564.30"}]
[{"$nulls":4},0]
["2.17.2","Over site","m³",1,{"v":564.3033808000001,"d":"564.30"}]
[{"$nulls":4},0]
["2.17.3","Landscape mounds, berms, etc","m³",1,{"v":576.5708456000001,"d":"576.57"}]
[{"$nulls":4},0]
[2.18,"Coarse river sand filling supplied by the contractor",null,null,0]
[{"$nulls":4},0]
["2.18.1","Under floors etc","m³",1,{"v":425.6810285600001,"d":"425.68"}]
[{"$nulls":4},0]
["2.18.2","Behind retaining walls","m³",1,{"v":431.81476096000006,"d":"431.81"}]
[{"$nulls":4},0]
["2.18.3","In floor ducts","m³",1,{"v":431.81476096000006,"d":"431.81"}]
[{"$nulls":4},0]
[2.19,"Hardcore filling",null,null,0]
[{"$nulls":4},0]
["2.19.1","Under floors etc","m³",1,{"v":306.68662,"d":"306.69"}]
[{"$nulls":4},0]
[{"v":2.2,"d":"2.20"},"Crusher filling of 19mm stone",null,null,0]
[{"$nulls":4},0]
["2.20.1","Under floors etc","m³",1,{"v":581.47783152,"d":"581.48"}]
[{"$nulls":4},0]
["2.20.2","Behind retaining walls","m³",1,{"v":581.47783152,"d":"581.48"}]
[{"$nulls":4},0]
["2.20.3","In flower boxes","m³",1,{"v":579.0243385600002,"d":"579.02"}]
[{"$nulls":4},0]
[2.21,"Compaction of surfaces",null,null,0]
[{"$nulls":4},0]
["2.21.1","Compaction of ground surface under floors, etc. including scarifying for a depth of 100mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m²",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
[null,"TESTS",null,null,0]
[{"$nulls":4},0]
[2.22,"Prescribed density test on filling.",null,null,0]
[{"$nulls":4},0]
["2.22.1","\"Modified AASHTO density\" test ","no.",1,{"v":354.5297327200001,"d":"354.53"}]
[{"$nulls":4},0]
["2.22.2","\"Natural California Bearing Ratio\" test","no",1,{"v":488.24509904000007,"d":"488.25"}]
[{"$nulls":4},0]
["2.22.3","\"Field Density\" test including \"Optimum Moisture Content\" (four readings per test)","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
["2.22.4","Maximum dry density and optimum moisture content test in accordance with Method A7 of TMH1 (Technical Method of Highways","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
["2.22.5","In situ dry density (sand replacement) test in accprdance with metho A7 of TMH1 (Technican Method of Highwats)","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
[null,"STONE PITCHING",null,null,0]
[{"$nulls":4},0]
[2.23,"Stone pitching of approximately 250mm diameter river stones tightly packed including preparation of ground surface under",null,null,0]
[{"$nulls":4},0]
["2.23.1","250mm thick against sloping banks","m²",1,{"v":381.5181552800001,"d":"381.52"}]
[{"$nulls":4},0]
["2.23.2","250mm thick against sloping banks bedded and jointed in 1:8 cement mortar and pointed with hollow recessed joints","m²",1,{"v":464.9369159200001,"d":"464.94"}]
[{"$nulls":4},0]
[null,"GABIONS",null,null,0]
[{"$nulls":4},0]
[2.24,"Gabions of Mesh Type 80 with 3mm Class A galvanised wire boxes laced and braced together and filled with broken stone as per Maccaferri SA (Pty) Ltd specifications",null,null,0]
[{"$nulls":4},0]
["2.24.1","1000mm thick retaining wall of 1000 x 1000 x 1000mm boxes properly bonded","m³",1,{"v":966.6762262400002,"d":"966.68"}]
[{"$nulls":4},0]
["2.24.2","1000mm thick retaining wall of 2000 x 1000 x 1000mm boxes properly bonded","m³",1,{"v":931.1005783200002,"d":"931.10"}]
[{"$nulls":4},0]
[2.25,"Reno Mattresses of Mesh Type 60 with 2,7mm Class A galvanised wire boxes laced and braced together and filled with broken stone as per Maccaferri SA (Pty) Ltd specifications",null,null,0]
[{"$nulls":4},0]
["2.25.1","300mm thick embankment protection of 2000 x 1000 x 300mm mattresses with diaphragm divisions at 1000mm centres butt jointed","m³",1,{"v":1171.5428884000003,"d":"1,171.54"}]
[{"$nulls":4},0]
["2.25.2","300mm thick embankment protection of 3000 x 1000 x 300mm mattresses with diaphragm divisions at 1000mm centres butt jointed","m³",1,{"v":1527.2993676000003,"d":"1,527.30"}]
[{"$nulls":4},0]
[null,"FILTER FABRIC",null,null,0]
[{"$nulls":4},0]
[2.26,"AG 300 Geotextile continuous polyester filament double needle-punched filter fabric with 300 mm laps as per Maccaferri SA (Pty) Ltd specifications",null,null,0]
[{"$nulls":4},0]
["2.26.1","Under stone filled gabions including preparing ground surface under","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["2.26.2","Vertically behind stone filled gabion retaining walls","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["2.26.3","Over stone percolation beds in flower boxes","m²",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["2.26.4","Around stone filling in sub-soil drain trenches","m²",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
[null,"SOIL POISONING",null,null,0]
[{"$nulls":4},0]
[2.27,"Weedkillers, Insecticides, etc. Environmentaly friendly and SABS approved.",null,null,0]
[{"$nulls":4},0]
["2.27.1","Under paving, etc","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["2.27.2","Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming.","m²",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["2.27.3","Bottoms and sides of trenches etc.","m²",1,{"v":19.627943680000005,"d":"19.63"}]
{"$rows_empty":19}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Concrete, Formwork & Reinf","index":2,"n_rows":663,"n_cols":7,"rows_kept":663,"merged":[[0,4,0,6]],"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 3"]
[]
[]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Cost of tests"]
[]
[null,"The costs of making, storing and testing of concrete test cubes as required under clause 7 \"Tests\" of SABS 1200 G shall include the cost of providing cube moulds necessary for the purpose, for testing costs and for submitting reports on the tests to the Principal Agent/Project Manager. The testing shall be undertaken by an independent firm or institution nominated by the contractor to the approval of the Principal Agen/Project Manager.  (Test cubes are measured separately)"]
[]
[null,"Formwork"]
[]
[null,"Descriptions of formwork shall be deemed to include use and waste only (except where described as \"left in\" or \"permanent\"), for fitting together in the required forms, wedging, plumbing and fixing to true angles and surfaces as necessary to ensure easy release during stripping and for reconditioning as necessary before re-use"]
[]
[null,"The vertical strutting shall be carried down to such construction as is sufficiently strong to afford the required support without damage and shall remain in position until the newly constructed work is able to support itself."]
[]
[null,"Formwork to soffits of (solid) slabs etc. shall be deemed to be to slabs not exceeding 250mm thick unless otherwise described."]
[]
[null,"Formwork to sides of bases, pile caps, ground beams, etc. will only be measured where it is prescribed by the engineer for design reasons. Formwork necessitated by irregularity or collapse of excavated faces will not be measured and the cost thereof shall be deemed to be included in the allowance for taking the risk of collapse of the sides of the excavations, provision for which is made in \"Earthworks\""]
[]
[null,"RAPID HARDENING CONCRETE"]
[]
[3.1,"Backfill trenches in high trafficked road surfaces"]
[]
["3.1.1","25 Mpa concrete","m3",1,{"v":1878.2015015400002,"d":"1,878.20"}]
[{"$nulls":4},0]
["3.1.2","30 Mpa concrete","m3",1,{"v":1938.0163475400002,"d":"1,938.02"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"CELLULAR LIGHT RAPID HARDENING CONCRETE",null,null,0]
[{"$nulls":4},0]
[3.2,"Cellular light Breeze concrete - Backfill trenches in high trafficked road surfaces",null,null,0]
[{"$nulls":4},0]
["3.2.1","Grading to slabs","m3",1,{"v":1418.1427512000002,"d":"1,418.14"}]
[{"$nulls":4},0]
["3.2.2","Finishing smooth top surfaces of grading to falls for waterproofing including 1:8 monolithic cement plaster screed as necessary","m2",1,{"v":15.006801600000003,"d":"15.01"}]
[{"$nulls":4},0]
["3.2.3","Finishing smooth top surfaces of grading to falls and currents for waterproofing including 1:8 monolithic cement plaster screed as necessary","m2",1,{"v":15.006801600000003,"d":"15.01"}]
[{"$nulls":4},0]
["3.2.4","70 x 70mm 1:8 Cement plaster triangular fillets against walls, etc.","m",1,{"v":15.507028320000005,"d":"15.51"}]
[{"$nulls":4},0]
[null,"UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES",null,null,0]
[{"$nulls":4},0]
[3.3,"15MPa/20mm. concrete",null,null,0]
[{"$nulls":4},0]
["3.3.1","Surface blinding under surface beds","m³",1,{"v":1581.9670020000003,"d":"1,581.97"}]
[{"$nulls":4},0]
["3.3.2","Surface blinding under footings and bases","m³",1,{"v":1581.9670020000003,"d":"1,581.97"}]
[{"$nulls":4},0]
[3.4,"20MPa/20mm. concrete",null,null,0]
[{"$nulls":4},0]
["3.4.1","Strip footings","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.2","Surface bed","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.3","Surface bed on waterproofing ","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.4","Surface bed cast in panels","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.5","Surface bed cast in panels on waterproofing ","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.6","Pavings","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.7","Pavings cast in panels","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.8","Ramps","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.9","Bottoms and sides of floor ducts","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.10","Machine bases","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.4.11","Steps, urinal steps, cupboard platforms, etc.","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
[3.5,"25MPa/20mm. concrete",null,null,0]
[{"$nulls":4},0]
["3.5.1","Strip footings","m³",1,{"v":1616.9828724000001,"d":"1,616.98"}]
[{"$nulls":4},0]
["3.5.2","Surface bed","m³",1,{"v":1616.9828724000001,"d":"1,616.98"}]
[{"$nulls":4},0]
["3.5.3","Surface bed on waterproofing ","m³",1,{"v":1616.9828724000001,"d":"1,616.98"}]
[{"$nulls":4},0]
["3.5.4","Surface bed cast in panels","m³",1,{"v":1616.9828724000001,"d":"1,616.98"}]
[{"$nulls":4},0]
["3.5.5","Surface bed cast in panels on waterproofing ","m³",1,{"v":1616.9828724000001,"d":"1,616.98"}]
[{"$nulls":4},0]
["3.5.6","Pavings","m³",1,{"v":1629.4885404000004,"d":"1,629.49"}]
[{"$nulls":4},0]
["3.5.7","Pavings cast in panels","m³",1,{"v":1629.4885404000004,"d":"1,629.49"}]
[{"$nulls":4},0]
["3.5.8","Ramps","m³",1,{"v":1629.4885404000004,"d":"1,629.49"}]
[{"$nulls":4},0]
["3.5.9","Bottoms and sides of floor ducts","m³",1,{"v":1640.7436416000003,"d":"1,640.74"}]
[{"$nulls":4},0]
["3.5.10","Machine bases","m³",1,{"v":1640.7436416000003,"d":"1,640.74"}]
[{"$nulls":4},0]
["3.5.11","Steps","m³",1,{"v":1640.7436416000003,"d":"1,640.74"}]
[{"$nulls":4},0]
[null,"REINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES",null,null,0]
[{"$nulls":4},0]
[3.6,"20MPa/20mm. concrete",null,null,0]
[{"$nulls":4},0]
["3.6.1","Strip footings","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.2","Bases","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.3","Foundation beams","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.4","Surface bed","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.5","Surface bed on waterproofing ","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.6","Surface bed cast in panels","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.7","Surface bed cast in panels on waterproofing ","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.8","Pavings","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.9","Pavings cast in panels","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.10","Ramps","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.11","Bottoms and sides of floor ducts","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.12","Machine bases","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.13","Steps","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
["3.6.14","In cavity walls","m³",1,{"v":1606.9783380000003,"d":"1,606.98"}]
[{"$nulls":4},0]
[3.7,"25MPa/20mm. concrete",null,null,0]
[{"$nulls":4},0]
["3.7.1","Strip footings","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.2","Bases","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.3","Foundation beams","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.4","Surface bed","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.5","Surface bed on waterproofing ","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.6","Surface bed cast in panels","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.7","Surface bed cast in panels on waterproofing ","m³",1,{"v":1650.7481760000003,"d":"1,650.75"}]
[{"$nulls":4},0]
["3.7.8","Pavings","m³",1,{"v":1663.2538440000005,"d":"1,663.25"}]
[{"$nulls":4},0]
["3.7.9","Pavings cast in panels","m³",1,{"v":1663.2538440000005,"d":"1,663.25"}]
[{"$nulls":4},0]
["3.7.10","Ramps","m³",1,{"v":1663.2538440000005,"d":"1,663.25"}]
[{"$nulls":4},0]
["3.7.11","Bottoms and sides of floor ducts","m³",1,{"v":1663.2538440000005,"d":"1,663.25"}]
[{"$nulls":4},0]
["3.7.12","Machine bases","m³",1,{"v":1663.2538440000005,"d":"1,663.25"}]
[{"$nulls":4},0]
["3.7.13","Steps","m³",1,{"v":1663.2538440000005,"d":"1,663.25"}]
[{"$nulls":4},0]
[null,"REINFORCED CONCRETE",null,null,0]
[{"$nulls":4},0]
[3.8,"30MPa/20mm. concrete",null,null,0]
[{"$nulls":4},0]
["3.8.1","Slabs including beams and inverted beams","m³",1,{"v":1713.2765160000004,"d":"1,713.28"}]
[{"$nulls":4},0]
["3.8.2","Stepped slabs including beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.3","Raking slabs, ramps, etc. including beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.4","Coffered slabs including beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.5","Troughed slabs including beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.6","Composite hollow block slabs including beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.7","Composite prefabricated beam and trough slabs including beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.8","Hood slabs","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.9","Vanity slabs, cupboard slabs, cover slabs, etc","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.10","Isolated beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.11","Bottoms and sides of isolated gutter beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.7.12","Lintels","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.13","Stairs including landings, beams and inverted beams","m³",1,{"v":1725.7821840000004,"d":"1,725.78"}]
[{"$nulls":4},0]
["3.8.14","Retaining walls in foundations (Provisional)","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
["3.8.15","Retaining walls","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
["3.8.16","Walls in foundations (Provisional)","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
["3.8.17","Walls","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
["3.8.18","Balustrade walls","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
["3.8.19","Columns in foundations (Provisional)","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
["3.8.20","Columns","m³",1,{"v":1744.5406860000005,"d":"1,744.54"}]
[{"$nulls":4},0]
[null,"TEST BLOCKS",null,null,0]
[{"$nulls":4},0]
["3.8.21","Making and testing a set of three 150 x 150 x 150mm. concrete strength test cubes (Provisional)","no",1,{"v":497.7255864,"d":"497.73"}]
[{"$nulls":4},0]
[null,"CONCRETE SUNDRIES",null,null,0]
[{"$nulls":4},0]
[null,"Curing surfaces of concrete with \"Masterseal\" curing compound applied at arate of 1 litre/10m2",null,null,0]
[{"$nulls":4},0]
["3.8.22","Horizontal top surfaces",null,null,0]
[{"$nulls":4},0]
["3.8.23","Vertical surfaces",null,null,0]
[{"$nulls":4},0]
[null,"Colouring surfaces of concrete with \"Oxide\" including curing compound applied at a rate of 1 litre/10m2",null,null,0]
[{"$nulls":4},0]
["3.8.24","Horizontal top surfaces","m²",1,{"v":36.89172060000001,"d":"36.89"}]
[{"$nulls":4},0]
["3.8.25","Vertical surfaces","m²",1,{"v":36.89172060000001,"d":"36.89"}]
[{"$nulls":4},0]
[3.9,"Finishing top surface of concrete smooth with wood float or steel trowel",null,null,0]
[{"$nulls":4},0]
["3.9.1","Surface bed, slabs, etc","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.9.2","Surface bed, slabs, etc to falls and currents","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.9.3","Paving to falls","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.9.4","Paving to falls and currents","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.9.5","Tops of beams, walls, etc","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
["3.9.6","Sloping and splayed tops of beams, walls, etc","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
[{"v":3.1,"d":"3.10"},"Finishing top surfaces of concrete smooth with a steel float",null,null,0]
[{"$nulls":4},0]
["3.10.1","Surface bed, slabs, etc.","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.10.2","Surface bed, slabs, etc to falls and currents","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.10.3","Paving to falls","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.10.4","Paving to falls and currents","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.10.5","Tops of beams, walls, etc","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
["3.10.6","Sloping and splayed tops of beams, walls, etc","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
[3.11,"Finishing top surfaces of concrete smooth with a power float",null,null,0]
[{"$nulls":4},0]
["3.11.1","Surface bed, slabs, etc.","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
["3.11.2","Surface bed, slabs, etc to falls and currents","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
["3.11.3","Paving to falls","m²",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
[3.12,"Finishing top surfaces of concrete to an evenly ribbed non-slip surface",null,null,0]
[{"$nulls":4},0]
["3.12.1","Surface bed, slabs, etc","m²",1,{"v":10.004534400000002,"d":"10.00"}]
[{"$nulls":4},0]
["3.12.2","Surface bed, slabs, etc to falls","m²",1,{"v":10.004534400000002,"d":"10.00"}]
[{"$nulls":4},0]
["3.12.3","Surface bed, slabs, etc to falls and currents","m²",1,{"v":10.004534400000002,"d":"10.00"}]
[{"$nulls":4},0]
["3.12.4","Paving to falls","m²",1,{"v":10.004534400000002,"d":"10.00"}]
[{"$nulls":4},0]
["3.12.5","Paving to falls and currents","m²",1,{"v":10.004534400000002,"d":"10.00"}]
[{"$nulls":4},0]
[3.13,"Finishing top surfaces of concrete smooth with a power float with \"Masterplate\" hardener added (5kg/m²) and curing with \"Masterseal\" curing compound at a rate of 1 litre/10m²",null,null,0]
[{"$nulls":4},0]
["3.13.1","Surface bed, slabs, etc.","m²",1,{"v":30.013603200000006,"d":"30.01"}]
[{"$nulls":4},0]
[3.14,"Wire brushing of concrete surfaces to expose aggregate",null,null,0]
[{"$nulls":4},0]
["3.14.1","Sides of walls","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.14.2","Sides of columns","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.14.3","Soffits of slab","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
["3.14.4","Sides and soffits of beams","m²",1,{"v":25.01133600000001,"d":"25.01"}]
[{"$nulls":4},0]
[3.15,"Sandblasting of concrete surfaces to expose aggregate",null,null,0]
[{"$nulls":4},0]
["3.15.1","Sides of walls","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
["3.15.2","Sides of columns","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
["3.15.3","Soffits of slab","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
["3.15.4","Sides and soffits of beams","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
[3.16,"Bush-hammering of concrete surfaces to expose aggregate",null,null,0]
[{"$nulls":4},0]
["3.16.1","Sides of walls","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
["3.16.2","Sides of columns","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
["3.16.3","Soffits of slab","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
["3.16.4","Sides and soffits of beams","m²",1,{"v":52.52380560000001,"d":"52.52"}]
[{"$nulls":4},0]
[3.17,"Grooves, channels, mortices, sinkings, etc in concrete",null,null,0]
[{"$nulls":4},0]
["3.17.1","20x20mm Grooves in top","m",1,{"v":22.510202400000004,"d":"22.51"}]
[{"$nulls":4},0]
["3.17.2","35x35mm Channels in top","m",1,{"v":22.510202400000004,"d":"22.51"}]
[{"$nulls":4},0]
["3.17.3","20mmx 20mm segmental channels in top","m",1,{"v":22.510202400000004,"d":"22.51"}]
[{"$nulls":4},0]
["3.17.4","Mortice in top, side, etc not exceeding 150mm deep","m",1,{"v":22.510202400000004,"d":"22.51"}]
[{"$nulls":4},0]
["3.17.5","20x20mm Sinking in top","m",1,{"v":22.510202400000004,"d":"22.51"}]
[{"$nulls":4},0]
[3.18,"Cement work of 1:3 liquid cement and sand mixture applied with a brush",null,null,0]
[{"$nulls":4},0]
["3.18.1","On concrete walls","m2",1,{"v":43.76983800000001,"d":"43.77"}]
[{"$nulls":4},0]
["3.18.2","On soffits of slabs, landings, stairs, etc","m2",1,{"v":43.76983800000001,"d":"43.77"}]
[{"$nulls":4},0]
["3.18.3","On soffits of coffered slabs","m2",1,{"v":43.76983800000001,"d":"43.77"}]
[{"$nulls":4},0]
[3.19,"Bedding under base plates etc.",null,null,0]
[{"$nulls":4},0]
["3.19.1","25mm thick non-shrink grout under steel base plate size 500 x 350mm. including chamfered edge all round","no",1,{"v":77.5351416,"d":"77.54"}]
[{"$nulls":4},0]
[null,"HOLLOW BLOCKS ETC",null,null,0]
[{"$nulls":4},0]
[{"v":3.2,"d":"3.20"},"\"SuperSlab\" hollow blocks in composite slabs",null,null,0]
[{"$nulls":4},0]
["3.20.1","440 x 220 x 120mm block type S120 laid end to end in rows","no",1,{"v":35.015870400000004,"d":"35.02"}]
[{"$nulls":4},0]
["3.20.2","440 x 220 x 205mm block type S205 laid end to end in rows","no",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
["3.20.3","440 x 220 x 290mm block type S290 laid end to end in rows","no",1,{"v":50.02267200000002,"d":"50.02"}]
[{"$nulls":4},0]
[null,"PREFABRICATED CONCRETE BEAMS",null,null,0]
[{"$nulls":4},0]
[3.21,"\"SuperSlab\" prefabricated prestressed concrete beams in composite slabs",null,null,0]
[{"$nulls":4},0]
["3.21.1","150 x 58mm beam with Three 4mm reinforcing wires, in lengths not exceeding 5,0m","m",1,{"v":140.06348160000002,"d":"140.06"}]
[{"$nulls":4},0]
["3.21.2","150 x 58mm beam with Five 4mm reinforcing wires, in lengths exceeding 5,0m and not exceeding 7,5m","m",1,{"v":145.06574880000002,"d":"145.07"}]
[{"$nulls":4},0]
["3.21.3","150 x 58mm beam with Seven 4mm reinforcing wires, in lengths exceeding 7,5m and not exceeding 10,0m","m",1,{"v":150.068016,"d":"150.07"}]
[{"$nulls":4},0]
[3.22,"Supporting bearers to prefabricated beams",null,null,0]
[{"$nulls":4},0]
["3.22.1","Beares","m",1,{"v":411.4364772,"d":"411.44"}]
[{"$nulls":4},0]
["3.22.2","Beares propped up exceeding 3,5m and not exceeding 5,0m high","m",1,{"v":581.5135620000002,"d":"581.51"}]
[{"$nulls":4},0]
[3.23,"Rough formwork to composite hollow block slabs",null,null,0]
[{"$nulls":4},0]
["3.23.1","Soffit of composite slabs","m²",1,{"v":277.6258296000001,"d":"277.63"}]
[{"$nulls":4},0]
["3.23.2","Soffit of composite slabs propped up exceeding 3,5m and not exceeding 5,0m high","m²",1,{"v":350.15870400000006,"d":"350.16"}]
[{"$nulls":4},0]
[3.24,"\"Echo Floors\" prefabricated prestressed concrete slabs",null,null,0]
[{"$nulls":4},0]
["3.24.1","Slabs","m²",1,{"v":687.8117400000001,"d":"687.81"}]
[{"$nulls":4},0]
["3.24.2","Beares propped up exceeding 3,5m and not exceeding 5,0m high","m",1,{"v":719.07591,"d":"719.08"}]
[{"$nulls":4},0]
[null,"ROUGH FORMWORK (DEGREE OF ACCURACY II)",null,null,0]
[{"$nulls":4},0]
[3.25,"Rough formwork to sides",null,null,0]
[{"$nulls":4},0]
["3.25.1","Strip footings (Provisional)","m²",1,{"v":372.6689064000001,"d":"372.67"}]
[{"$nulls":4},0]
["3.25.2","Bases (Provisional)","m²",1,{"v":372.6689064000001,"d":"372.67"}]
[{"$nulls":4},0]
["3.25.3","Foundation beams (Provisional)","m²",1,{"v":372.6689064000001,"d":"372.67"}]
[{"$nulls":4},0]
["3.25.4","Foundation beams circular exceeding 1m radius (Provisional)","m²",1,{"v":380.1723072000001,"d":"380.17"}]
[{"$nulls":4},0]
["3.25.5","Retaining walls (Provisional)","m²",1,{"v":346.40700360000005,"d":"346.41"}]
[{"$nulls":4},0]
["3.25.6","Retaining walls circular exceeding 1m radius (Provisional)","m²",1,{"v":352.6598376000001,"d":"352.66"}]
[{"$nulls":4},0]
["3.25.7","Walls (Provisional)","m²",1,{"v":351.4092708000001,"d":"351.41"}]
[{"$nulls":4},0]
["3.25.8","Walls circular exceeding 1m radius (Provisional)","m²",1,{"v":358.91267160000007,"d":"358.91"}]
[{"$nulls":4},0]
["3.25.9","Stub columns in foundations (Provisional)","m²",1,{"v":255.11562720000003,"d":"255.12"}]
[{"$nulls":4},0]
[null,"SMOOTH FORMWORK (DEGREE OF ACCURACY II)",null,null,0]
[{"$nulls":4},0]
[3.26,"Smooth formwork to sides",null,null,0]
[{"$nulls":4},0]
["3.26.1","Steps","m²",1,{"v":357.66210480000007,"d":"357.66"}]
[{"$nulls":4},0]
["3.26.2","Retaining walls","m²",1,{"v":357.66210480000007,"d":"357.66"}]
[{"$nulls":4},0]
["3.26.3","Retaining walls circular exceeding 1m radius","m²",1,{"v":365.1655056000001,"d":"365.17"}]
[{"$nulls":4},0]
["3.26.4","One face of retaining walls (other face against excavated or existing surfaces)","m²",1,{"v":330.1496352000001,"d":"330.15"}]
[{"$nulls":4},0]
["3.26.5","One face of retaining walls (other face against excavated or existing surfaces) circular exceeding 1m radius","m²",1,{"v":336.4024692,"d":"336.40"}]
[{"$nulls":4},0]
["3.26.6","Walls","m²",1,{"v":357.66210480000007,"d":"357.66"}]
[{"$nulls":4},0]
["3.26.7","Walls circular exceeding 1m radius","m²",1,{"v":365.1655056000001,"d":"365.17"}]
[{"$nulls":4},0]
["3.26.8","Inner face of balustrade walls","m²",1,{"v":330.1496352000001,"d":"330.15"}]
[{"$nulls":4},0]
["3.26.9","Inner face of balustrade walls circular exceeding 1m radius","m²",1,{"v":336.4024692,"d":"336.40"}]
[{"$nulls":4},0]
["3.26.10","Outer face of balustrade walls","m²",1,{"v":330.1496352000001,"d":"330.15"}]
[{"$nulls":4},0]
["3.26.11","Outer face of balustrade walls circular exceeding 1m radius","m²",1,{"v":336.4024692,"d":"336.40"}]
[{"$nulls":4},0]
["3.26.12","Columns","m²",1,{"v":330.1496352000001,"d":"330.15"}]
[{"$nulls":4},0]
["3.26.13","Beams","m²",1,{"v":346.40700360000005,"d":"346.41"}]
[{"$nulls":4},0]
["3.26.14","Beams circular exceeding 1m radius","m²",1,{"v":353.9104044000001,"d":"353.91"}]
[{"$nulls":4},0]
["3.26.15","Inverted beams","m²",1,{"v":346.40700360000005,"d":"346.41"}]
[{"$nulls":4},0]
["3.26.16","Inverted beams circular exceeding 1m radius","m²",1,{"v":353.9104044000001,"d":"353.91"}]
[{"$nulls":4},0]
["3.26.17","Isolated beams","m²",1,{"v":346.40700360000005,"d":"346.41"}]
[{"$nulls":4},0]
["3.26.18","Isolated beams circular exceeding 1m radius","m²",1,{"v":353.9104044000001,"d":"353.91"}]
[{"$nulls":4},0]
["3.26.19","Edges, risers, ends and reveals not exceeding 300mm. high or wide","m",1,{"v":113.80157880000003,"d":"113.80"}]
[{"$nulls":4},0]
["3.26.20","Edges, risers, ends and reveals not exceeding 300mm. high or wide circular exceeding 1m radius","m",1,{"v":121.30497960000002,"d":"121.30"}]
[{"$nulls":4},0]
[3.27,"Smooth formwork to soffits",null,null,0]
[{"$nulls":4},0]
["3.27.1","Slabs","m²",1,{"v":301.3865988,"d":"301.39"}]
[{"$nulls":4},0]
["3.27.2","Slabs propped up exceeding 3,5m and not exceeding 5,0m high","m²",1,{"v":373.9194732,"d":"373.92"}]
[{"$nulls":4},0]
["3.27.3","Slabs exceeding 250mm and not exceeding 500mm thick","m²",1,{"v":301.3865988,"d":"301.39"}]
[{"$nulls":4},0]
["3.27.4","Slabs exceeding 250mm and not exceeding 500mm thick propped up exceed 3,5m and not exceeding 5,0m high","m²",1,{"v":373.9194732,"d":"373.92"}]
[{"$nulls":4},0]
["3.27.5","Slabs with sloping soffits","m²",1,{"v":305.13829920000006,"d":"305.14"}]
[{"$nulls":4},0]
["3.27.6","Cantilever slabs","m²",1,{"v":301.3865988,"d":"301.39"}]
[{"$nulls":4},0]
["3.27.7","Cantilever slabs propped up exceed 3,5m and not exceeding 5,0m high","m²",1,{"v":373.9194732,"d":"373.92"}]
[{"$nulls":4},0]
["3.27.8","Vanity slabs, cupboard slabs, cover slabs, etc","m²",1,{"v":321.3956676000001,"d":"321.40"}]
[{"$nulls":4},0]
["3.27.9","Landings","m²",1,{"v":321.3956676000001,"d":"321.40"}]
[{"$nulls":4},0]
["3.27.10","Landings exceeding 250mm and not exceeding 500mm thick","m²",1,{"v":321.3956676000001,"d":"321.40"}]
[{"$nulls":4},0]
["3.27.11","Stairs and sloping soffits","m²",1,{"v":492.7233192000001,"d":"492.72"}]
[{"$nulls":4},0]
["3.27.12","Beams","m²",1,{"v":337.653036,"d":"337.65"}]
[{"$nulls":4},0]
["3.27.13","Beams circular exceeding 1m radius","m²",1,{"v":343.90587000000005,"d":"343.91"}]
[{"$nulls":4},0]
["3.27.14","Beams propped up exceeding 3,5m and not exceeding 5,0m high","m²",1,{"v":410.18591040000007,"d":"410.19"}]
[{"$nulls":4},0]
["3.27.15","Beams with sloping soffits","m²",1,{"v":343.90587000000005,"d":"343.91"}]
[{"$nulls":4},0]
["3.27.16","Beams with sloping soffits propped up exceeding 3,5m and not exceeding 5,0m high","m²",1,{"v":417.6893112000001,"d":"417.69"}]
[{"$nulls":4},0]
["3.27.17","Isolated beams","m²",1,{"v":337.653036,"d":"337.65"}]
[{"$nulls":4},0]
["3.27.18","Isolated beams circular exceeding 1m radius","m²",1,{"v":343.90587000000005,"d":"343.91"}]
[{"$nulls":4},0]
["3.27.19","Isolated beams propped up exceeding 3,5m and not exceeding 5,0m high","m²",1,{"v":410.18591040000007,"d":"410.19"}]
[{"$nulls":4},0]
[3.28,"Smooth formwork to circular columns",null,null,0]
[{"$nulls":4},0]
["3.28.1","250mm diameter column not exceeding 3,5m high","no",1,{"v":737.834412,"d":"737.83"}]
[{"$nulls":4},0]
["3.28.2","250mm diameter column exceeding 3,5m high not exceeding 5,0m high","no",1,{"v":1054.2278124000002,"d":"1,054.23"}]
[{"$nulls":4},0]
["3.28.3","350mm diameter column not exceeding 3,5m high","no",1,{"v":861.6405252000002,"d":"861.64"}]
[{"$nulls":4},0]
["3.28.4","350mm diameter column exceeding 3,5m high not exceeding 5,0m high","no",1,{"v":1391.8808484,"d":"1,391.88"}]
[{"$nulls":4},0]
["3.28.5","450mm diameter column not exceeding 3,5m high","no",1,{"v":986.6972052000001,"d":"986.70"}]
[{"$nulls":4},0]
["3.28.6","450mm diameter column exceeding 3,5m high not exceeding 5,0m high","no",1,{"v":2008.4102808000005,"d":"2,008.41"}]
[{"$nulls":4},0]
[3.29,"Boxing in smooth formwork to form",null,null,0]
[{"$nulls":4},0]
["3.29.1","25 x 25mm chamfer along top or bottom edge","m",1,{"v":17.507935200000002,"d":"17.51"}]
[{"$nulls":4},0]
["3.29.2","25 x 25mm chamfer along top or bottom edge circular not exceeding 1m radius","m",1,{"v":22.510202400000004,"d":"22.51"}]
[{"$nulls":4},0]
["3.29.3","25 x 25mm vertical chamfer at corner","m",1,{"v":17.507935200000002,"d":"17.51"}]
[{"$nulls":4},0]
["3.29.4","40 x 25mm horizontal chase or groove in side","m",1,{"v":30.013603200000006,"d":"30.01"}]
[{"$nulls":4},0]
["3.29.5","40 x 25mm horizontal chase or groove in side circular not exceeding 1m radius","m",1,{"v":35.015870400000004,"d":"35.02"}]
[{"$nulls":4},0]
["3.29.6","40 x 25mm raking or vertical chase or groove in side","m",1,{"v":30.013603200000006,"d":"30.01"}]
[{"$nulls":4},0]
[{"v":3.3,"d":"3.30"},"Smooth formwork to form",null,null,0]
[{"$nulls":4},0]
["3.30.1","Opening not exceeding 1m girth through not exceeding 300mm  slab","no",1,{"v":213.84692280000007,"d":"213.85"}]
[{"$nulls":4},0]
["3.30.2","100mm diameter opening through not exceeding 300mm slab","no",1,{"v":21.259635600000003,"d":"21.26"}]
[{"$nulls":4},0]
["3.30.3","150mm diameter opening through not exceeding 300mm slab","no",1,{"v":23.760769200000006,"d":"23.76"}]
[{"$nulls":4},0]
["3.30.4","100mm diameter opening through 340mm slab","no",1,{"v":23.760769200000006,"d":"23.76"}]
[{"$nulls":4},0]
["3.30.5","150mm diameter opening through 340mm slab","no",1,{"v":27.512469600000003,"d":"27.51"}]
[{"$nulls":4},0]
["3.30.6","Opening not exceeding 1m girth through not exceeding 300mm wall or beam","no",1,{"v":233.85599160000004,"d":"233.86"}]
[{"$nulls":4},0]
["3.30.7","Opening not exceeding 1m girth through 350mm wall or beam","no",1,{"v":275.1246960000001,"d":"275.12"}]
[{"$nulls":4},0]
[null,"MOVEMENT JOINTS, ETC.",null,null,0]
[{"$nulls":4},0]
[3.31,"Expansion joints with bitumen impregnated softboard between vertical concrete surfaces",null,null,0]
[{"$nulls":4},0]
["3.31.1","10mm. joint exceeding 300mm. high","m2",1,{"v":91.29137640000002,"d":"91.29"}]
[{"$nulls":4},0]
["3.31.2","10mm. joint not exceeding 300mm. high","m",1,{"v":27.512469600000003,"d":"27.51"}]
[{"$nulls":4},0]
[3.32,"Expansion joints with bitumen impregnated softboard between vertical concrete and brick surfaces",null,null,0]
[{"$nulls":4},0]
["3.32.1","10mm. joint exceeding 300mm. high","m2",1,{"v":91.29137640000002,"d":"91.29"}]
[{"$nulls":4},0]
["3.32.2","10mm. joint not exceeding 300mm. high","m",1,{"v":27.512469600000003,"d":"27.51"}]
[{"$nulls":4},0]
[3.33,"Saw cut joints",null,null,0]
[{"$nulls":4},0]
["3.33.1","5 x 35mm. saw cut jointson top of concrete","m",1,{"v":50.02267200000002,"d":"50.02"}]
[{"$nulls":4},0]
[3.34,"Vertical toggle construction joint through concrete including thick cement slurry to one face",null,null,0]
[{"$nulls":4},0]
["3.34.1","Surface bed not exceeding 300mm thick","m",1,{"v":35.015870400000004,"d":"35.02"}]
[{"$nulls":4},0]
["3.34.2","Slabs not exceeding 300mm thick","m",1,{"v":35.015870400000004,"d":"35.02"}]
[{"$nulls":4},0]
["3.34.3","Slabs 350mm thick","m",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
["3.34.4","Walls not exceeding 300mm thick","m",1,{"v":35.015870400000004,"d":"35.02"}]
[{"$nulls":4},0]
["3.34.5","Walls 350mm thick","m",1,{"v":41.26870440000001,"d":"41.27"}]
[{"$nulls":4},0]
[null,"REINFORCEMENT",null,null,0]
[{"$nulls":4},0]
[3.35,"Mild steel reinforcement to structural concrete work",null,null,0]
[{"$nulls":4},0]
["3.35.1","8mm. diameter bar","t",1,{"v":36640.35667320001,"d":"36,640.36"}]
[{"$nulls":4},0]
["3.35.2","10mm. diameter bar","t",1,{"v":34809.52687800001,"d":"34,809.53"}]
[{"$nulls":4},0]
["3.35.3","12mm. diameter bar","t",1,{"v":33068.73789240001,"d":"33,068.74"}]
[{"$nulls":4},0]
["3.35.4","16mm. diameter bar","t",1,{"v":32149.571294400004,"d":"32,149.57"}]
[{"$nulls":4},0]
[3.36,"High tensile steel reinforcement to structural concrete work",null,null,0]
[{"$nulls":4},0]
["3.36.1","10mm. diameter bar","t",1,{"v":34808.2763112,"d":"34,808.28"}]
[{"$nulls":4},0]
["3.36.2","12mm. diameter bar","t",1,{"v":33067.4873256,"d":"33,067.49"}]
[{"$nulls":4},0]
["3.36.3","16mm. diameter bar","t",1,{"v":32149.571294400004,"d":"32,149.57"}]
[{"$nulls":4},0]
["3.36.4","20mm. diameter bar","t",1,{"v":31978.24364280001,"d":"31,978.24"}]
[{"$nulls":4},0]
["3.36.5","25mm. diameter bar","t",1,{"v":32262.122306400004,"d":"32,262.12"}]
[{"$nulls":4},0]
["3.36.6","32mm. diameter bar","t",1,{"v":32398.434087600006,"d":"32,398.43"}]
[{"$nulls":4},0]
[3.37,"High tensile steel dowel bars",null,null,0]
[{"$nulls":4},0]
["3.37.1","16mm diameter dowel bar 700mm long with one end embedded 350mm deep in side of concrete at expansion joint and other end greased and wrapped in polythene sheeting including hole through formwork","no",1,{"v":36.266437200000006,"d":"36.27"}]
[{"$nulls":4},0]
[3.38,"Fabric reinforcement",null,null,0]
[{"$nulls":4},0]
["3.38.1","Type Ref. 100 in concrete surface beds, slabs, etc.","m²",1,{"v":60.02720640000001,"d":"60.03"}]
[{"$nulls":4},0]
["3.38.2","Type Ref. 193 in concrete surface beds, slabs, etc.","m²",1,{"v":66.2800404,"d":"66.28"}]
[{"$nulls":4},0]
["3.38.3","Type Ref. 245 in concrete surface beds, slabs, etc.","m²",1,{"v":73.78344120000003,"d":"73.78"}]
[{"$nulls":4},0]
["3.38.4","Type Ref. 311 in concrete surface beds, slabs, etc.","m²",1,{"v":80.03627520000002,"d":"80.04"}]
[{"$nulls":4},0]
["3.38.5","Type Ref. 395 in concrete surface beds, slabs, etc.","m²",1,{"v":86.2891092,"d":"86.29"}]
[{"$nulls":4},0]
[null,"CONCRETE FLOOR POLISHING",null,null,0]
[{"$nulls":4},0]
[3.39,"Grinding and polishing of existing concrete floor",null,null,0]
[{"$nulls":4},0]
["3.39.1","Areas not exceeding 500m2","m²",1,{"v":650.2947360000002,"d":"650.29"}]
[{"$nulls":4},0]
["3.39.2","Areas exceeding 500m2 and not exceeding 1000m2","m²",1,{"v":471.4636836,"d":"471.46"}]
[{"$nulls":4},0]
["3.39.3","Areas exceeding 1000m2 and not exceeding 2000m2","m²",1,{"v":455.2063152000001,"d":"455.21"}]
[{"$nulls":4},0]
["3.39.4","Areas exceeding 2000m2 and not exceeding 5000m2","m²",1,{"v":438.9489468000001,"d":"438.95"}]
[{"$nulls":4},0]
["3.39.5","Areas exceeding 5000m2 and not exceeding 10000m2","m²",1,{"v":422.6915784000001,"d":"422.69"}]
[{"$nulls":4},0]
["3.39.6","Areas exceeding 1000m2 and not exceeding 20000m2","m²",1,{"v":406.43421000000006,"d":"406.43"}]
[{"$nulls":4},0]
[{"v":3.4,"d":"3.40"},"Grinding and polishing of existing concrete floor in confined areas",null,null,0]
[{"$nulls":4},0]
["3.40.1","Areas not exceeding 500m2","m²",1,{"v":700.3174080000001,"d":"700.32"}]
[{"$nulls":4},0]
["3.40.2","Areas exceeding 500m2 and not exceeding 1000m2","m²",1,{"v":521.4863556,"d":"521.49"}]
[{"$nulls":4},0]
["3.40.3","Areas exceeding 1000m2 and not exceeding 2000m2","m²",1,{"v":505.2289872000001,"d":"505.23"}]
[{"$nulls":4},0]
["3.40.4","Areas exceeding 2000m2 and not exceeding 5000m2","m²",1,{"v":488.9716188000001,"d":"488.97"}]
[{"$nulls":4},0]
["3.40.5","Areas exceeding 5000m2 and not exceeding 10000m2","m²",1,{"v":472.7142504,"d":"472.71"}]
[{"$nulls":4},0]
["3.40.6","Areas exceeding 1000m2 and not exceeding 20000m2","m²",1,{"v":456.4568820000001,"d":"456.46"}]
[{"$nulls":4},0]
[null,"POLISH, SEALERS, ETC.",null,null,0]
[{"$nulls":4},0]
[3.41,"Stain resistance sealing",null,null,0]
[{"$nulls":4},0]
["3.41.1","Single coat seal to flooring","m²",1,{"v":56.275506000000014,"d":"56.28"}]
[{"$nulls":4},0]
[3.42,"Deep Clean Restoration",null,null,0]
[{"$nulls":4},0]
["3.42.1","To linoleum, vinyl, etc","m²",1,{"v":211.34578920000004,"d":"211.35"}]
[{"$nulls":4},0]
["3.42.2","To powerfloated concrete floors","m²",1,{"v":243.86052600000005,"d":"243.86"}]
[{"$nulls":4},0]
["3.42.3","To granite","m²",1,{"v":243.86052600000005,"d":"243.86"}]
[{"$nulls":4},0]
["3.42.4","To marble","m²",1,{"v":243.86052600000005,"d":"243.86"}]
[{"$nulls":4},0]
["3.42.5","To terrazzo","m²",1,{"v":243.86052600000005,"d":"243.86"}]
[{"$nulls":4},0]
[3.43,"Cementations overlay",null,null,0]
[{"$nulls":4},0]
["3.43.1","Supply and placement","m²",1,{"v":1454.4091884000002,"d":"1,454.41"}]
[{"$nulls":4},0]
[3.44,"Sundries",null,null,0]
[{"$nulls":4},0]
["3.44.1","Raising of doors","m²",1,{"v":276.3752628000001,"d":"276.38"}]
{"$rows_empty":17}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Masonry","index":3,"n_rows":546,"n_cols":7,"rows_kept":546,"merged":[[0,4,0,6]],"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 4"]
[]
[null,"MASONRY"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"BRICKWORK"]
[]
[null,"Size and descriptions"]
[]
[null,"Where sizes in descriptions are given in brick units, \"One brick\" shall represent length and \"Half brick\" the width of a brick"]
[]
[null,"Hollow walls, etc"]
[]
[null,"Description of hollow walls shall be deemed to include leaving every fifth perpend of the bottom course of the external skin open as a weep hole"]
[]
[null,"User Note"]
[]
[null,"The following preamble generally applies for works in hot and humid coastal areas"]
[]
[null,"Bagged and sealed walls"]
[]
[null,"Walls in two skins described as \"bagged and sealed\" shall be deemed to include having the outer face of the inner skin bagged with 1:6 cement and sand mixture and sealed with two coats bitumen emulsion waterproofing coating "]
[]
[null,"Face bricks"]
[]
[null,"Bricks shall be ordered timeously to obtain uniformity in size and colour"]
[]
[null,"Pointing"]
[]
[null,"Descriptions of recessed pointing to fair face brickwork and face brickwork shall be deemed to include square recessed, hollow recessed, weathered pointing, etc."]
[]
[null,"BLOCKWORK"]
[]
[null,"Concrete masonry units"]
[]
[null,"Blocks are to be either solid or hollow modular dense concrete masonry units having a compressive strength of 14MPa"]
[]
[null," Wall ties for blockwork"]
[]
[null,"Wall ties shall be polypropylene ties complying with BS76377. Ties for hollow walls shall be of sufficient length to allow not less than 75mm of each end to be built into the blockwork. Ties are to be spaced at intervals of not more than 1m in the horizontal direction and not more than 400mm staggered in the vertical direction except at openings, vertical joints or ends of walls where they are to be placed vertically above each other"]
[]
[null,"Blockwork"]
[]
[null,"Blockwork shall comply with SANS 10145 \"Concrete Masonry Construction\""]
[]
[null,"Surfaces to be plastered shall have joints raked out to a depth of at least 10mm to provide a key. Cavities of hollow walls shall be kept free of mortar droppings or other undesirable matter. Every second perpend of the bottom course of the external skin of hollow walls shall be left open as a weep hole"]
[]
[null,"Standard complementary blocks"]
[]
[null,"Descriptions of blockwork shall be deemed to include standard complementary blocks such as corner, three-quarter, half and quarter blocks required in the construction of corners, reveals, jambs, ends, etc to solid and hollow walls and for bonding as necessary"]
[]
[null,"DECORATIVE BLOCKS"]
[]
[null,"Blocks shall be of approved manufacture, sound, well burnt or cured and uniform and true in size, shape and colour"]
[]
[null,"BRICKWORK"]
[]
[null,"FOUNDATIONS (PROVISIONAL)"]
[]
[4.1,"Brickwork of NFX bricks (14MPa nominal compressive strength) in class I mortar"]
[]
["4.1.1","Piers","m³",1,{"v":2506.24305864,"d":"2,506.24"}]
[{"$nulls":4},0]
["4.1.2","L-shaped piers","m³",1,{"v":2545.4989460000006,"d":"2,545.50"}]
[{"$nulls":4},0]
["4.1.3","H-shaped piers","m³",1,{"v":2584.7548333600007,"d":"2,584.75"}]
[{"$nulls":4},0]
["4.1.4","One brick walls","m²",1,{"v":495.60557792000003,"d":"495.61"}]
[{"$nulls":4},0]
["4.1.5","One brick walls circular on plan","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.1.6","One and a half brick walls","m²",1,{"v":731.14090208,"d":"731.14"}]
[{"$nulls":4},0]
["4.1.7","One and a half brick wall circular on plan","m²",1,{"v":758.1293246400002,"d":"758.13"}]
[{"$nulls":4},0]
["4.1.8","One brick cavity walls","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.1.9","Two brick walls","m²",1,{"v":949.5017755200001,"d":"949.50"}]
[{"$nulls":4},0]
["4.1.10","Two brick walls circular on plan","m²",1,{"v":975.2634516000003,"d":"975.26"}]
[{"$nulls":4},0]
["4.2","Brickwork of concrete bricks (14MPa nominal compressive strength) in class I mortar",null,null,0]
[{"$nulls":4},0]
["4.2.1","Piers","m³",1,{"v":2506.24305864,"d":"2,506.24"}]
[{"$nulls":4},0]
["4.2.2","L-shaped piers","m³",1,{"v":2545.4989460000006,"d":"2,545.50"}]
[{"$nulls":4},0]
["4.2.3","H-shaped piers","m³",1,{"v":2584.7548333600007,"d":"2,584.75"}]
[{"$nulls":4},0]
["4.2.4","One brick walls","m²",1,{"v":495.60557792000003,"d":"495.61"}]
[{"$nulls":4},0]
["4.2.5","One brick walls circular on plan","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.2.6","One and a half brick walls","m²",1,{"v":731.14090208,"d":"731.14"}]
[{"$nulls":4},0]
["4.2.7","One and a half brick wall circular on plan","m²",1,{"v":758.1293246400002,"d":"758.13"}]
[{"$nulls":4},0]
["4.2.8","Two brick walls","m²",1,{"v":949.5017755200001,"d":"949.50"}]
[{"$nulls":4},0]
["4.2.9","Two brick walls circular on plan","m²",1,{"v":975.2634516000003,"d":"975.26"}]
[{"$nulls":4},0]
[null,"SUPERSTRUCTURE",null,null,0]
[{"$nulls":4},0]
["4.3","Brickwork of NFX bricks (14MPa nominal compressive strength) in class II mortar",null,null,0]
[{"$nulls":4},0]
["4.3.1","Piers","m³",1,{"v":2506.24305864,"d":"2,506.24"}]
[{"$nulls":4},0]
["4.3.2","L-shaped piers","m³",1,{"v":2545.4989460000006,"d":"2,545.50"}]
[{"$nulls":4},0]
["4.3.3","H-shaped piers","m³",1,{"v":2584.7548333600007,"d":"2,584.75"}]
[{"$nulls":4},0]
["4.3.4","50mm cut lining to concrete","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["4.3.5","50mm cut lining to concrete circular on plan","m²",1,{"v":188.91895792000003,"d":"188.92"}]
[{"$nulls":4},0]
["4.3.6","Brick-on-edge walls","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["4.3.7","Half brick walls","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.3.8","Half brick walls circular on plan","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["4.3.9","Half brick walls against existing surfaces","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.3.10","Half brick walls in beamfilling","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["4.3.11","Half brick walls in beamfilling circular on plan","m²",1,{"v":268.65747912000006,"d":"268.66"}]
[{"$nulls":4},0]
["4.3.12","Half brick lining to concrete columns","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.3.13","Half brick lining to concrete columns circular on plan","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["4.3.14","One brick walls","m²",1,{"v":495.60557792000003,"d":"495.61"}]
[{"$nulls":4},0]
["4.3.15","One brick walls circular on plan","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.3.16","One brick walls against existing surfaces","m²",1,{"v":495.60557792000003,"d":"495.61"}]
[{"$nulls":4},0]
["4.3.17","One brick walls in beamfilling","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.3.18","One brick walls in beamfilling circular on plan","m²",1,{"v":534.8614652800001,"d":"534.86"}]
[{"$nulls":4},0]
["4.3.19","280mm hollow walls of two half brick skins including wire ties","m²",1,{"v":527.5009864000001,"d":"527.50"}]
[{"$nulls":4},0]
["4.3.20","280mm hollow walls of two half brick skins including wire ties circular on plan","m²",1,{"v":542.2219441600001,"d":"542.22"}]
[{"$nulls":4},0]
["4.3.21","One and a half brick wall","m²",1,{"v":731.14090208,"d":"731.14"}]
[{"$nulls":4},0]
["4.3.22","One and a half brick wall circular on plan","m²",1,{"v":758.1293246400002,"d":"758.13"}]
[{"$nulls":4},0]
["4.3.23","390mm hollow walls of one half brick and one one brick skins including wire ties","m²",1,{"v":765.4898035200002,"d":"765.49"}]
[{"$nulls":4},0]
["4.3.24","390mm hollow walls of one half brick and one one brick skins including wire ties circular on plan","m²",1,{"v":785.1177472,"d":"785.12"}]
[{"$nulls":4},0]
["4.3.25","Two brick walls","m²",1,{"v":949.5017755200001,"d":"949.50"}]
[{"$nulls":4},0]
["4.3.26","Two brick walls circular on plan","m²",1,{"v":975.2634516000003,"d":"975.26"}]
[{"$nulls":4},0]
["4.3.27","Half brick kerb 170mm high","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["4.3.28","Half brick kerb 170mm high circular on plan","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["4.3.29","One brick kerb 170mm high","m",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["4.3.30","One brick kerb 170mm high circular on plan","m",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["4.4","Brickwork of concrete bricks (14MPa nominal compressive strength) in class II mortar",null,null,0]
[{"$nulls":4},0]
["4.4.1","Piers","m³",1,{"v":2506.24305864,"d":"2,506.24"}]
[{"$nulls":4},0]
["4.4.2","L-shaped piers","m³",1,{"v":2545.4989460000006,"d":"2,545.50"}]
[{"$nulls":4},0]
["4.4.3","H-shaped piers","m³",1,{"v":2584.7548333600007,"d":"2,584.75"}]
[{"$nulls":4},0]
["4.4.4","50mm cut lining to concrete","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["4.4.5","50mm cut lining to concrete circular on plan","m²",1,{"v":188.91895792000003,"d":"188.92"}]
[{"$nulls":4},0]
["4.4.6","Brick-on-edge walls","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["4.4.7","Half brick walls","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.4.8","Half brick walls circular on plan","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["4.4.9","Half brick walls against existing surfaces","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.4.10","Half brick walls in beamfilling","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["4.4.11","Half brick walls in beamfilling circular on plan","m²",1,{"v":268.65747912000006,"d":"268.66"}]
[{"$nulls":4},0]
["4.4.12","Half brick lining to concrete columns","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.4.13","Half brick lining to concrete columns circular on plan","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["4.4.14","One brick walls","m²",1,{"v":495.60557792000003,"d":"495.61"}]
[{"$nulls":4},0]
["4.4.15","One brick walls circular on plan","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.4.16","One brick walls against existing surfaces","m²",1,{"v":495.60557792000003,"d":"495.61"}]
[{"$nulls":4},0]
["4.4.17","One brick walls in beamfilling","m²",1,{"v":518.91376104,"d":"518.91"}]
[{"$nulls":4},0]
["4.4.18","One brick walls in beamfilling circular on plan","m²",1,{"v":534.8614652800001,"d":"534.86"}]
[{"$nulls":4},0]
["4.4.19","280mm hollow walls of two half brick skins including wire ties","m²",1,{"v":527.5009864000001,"d":"527.50"}]
[{"$nulls":4},0]
["4.4.20","280mm hollow walls of two half brick skins including wire ties circular on plan","m²",1,{"v":542.2219441600001,"d":"542.22"}]
[{"$nulls":4},0]
["4.4.21","One and a half brick wall","m²",1,{"v":731.14090208,"d":"731.14"}]
[{"$nulls":4},0]
["4.4.22","One and a half brick wall circular on plan","m²",1,{"v":758.1293246400002,"d":"758.13"}]
[{"$nulls":4},0]
["4.4.23","390mm hollow walls of one half brick and one one brick skins including wire ties","m²",1,{"v":765.4898035200002,"d":"765.49"}]
[{"$nulls":4},0]
["4.4.24","390mm hollow walls of one half brick and one one brick skins including wire ties circular on plan","m²",1,{"v":785.1177472,"d":"785.12"}]
[{"$nulls":4},0]
["4.4.25","Two brick walls","m²",1,{"v":949.5017755200001,"d":"949.50"}]
[{"$nulls":4},0]
["4.4.26","Two brick walls circular on plan","m²",1,{"v":975.2634516000003,"d":"975.26"}]
[{"$nulls":4},0]
["4.4.27","Half brick kerb 170mm high","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["4.4.28","Half brick kerb 170mm high circular on plan","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["4.4.29","One brick kerb 170mm high","m",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["4.4.30","One brick kerb 170mm high circular on plan","m",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
[null,"BRICKWORK SUNDRIES",null,null,0]
[{"$nulls":4},0]
[4.5,"Brickwork sundries",null,null,0]
[{"$nulls":4},0]
["4.5.1","Cutting toothings and bonding new brickwork to existing","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["4.5.2","Extra for building brickwork to battered face with each course set back 55mm","m²",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["4.5.3","Extra for building brickwork to battered face with sloping joints","m²",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["4.5.4","Extra for building brickwork to oversail face with each course projecting 55mm","m²",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["4.5.5","Splayed mortar fillet one course high in 50mm cavity","m",1,{"v":13.494211280000002,"d":"13.49"}]
[{"$nulls":4},0]
["4.5.6","Splayed mortar fillet two course high in 50mm cavity","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["4.5.7","Closing 50mm cavity of hollow wall vertically with brickwork half brick wide","m",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["4.5.8","Closing 50mm cavity of hollow wall horizontally with one course of brickwork","m",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["4.5.9","Closing 50mm cavity of hollow wall horizontally with two course of brickwork","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["4.5.10","Closing 50mm cavity at raking top of hollow wall with two course of brickwork","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
[4.6,"Reinforcing and stabilising brickwork",null,null,0]
[{"$nulls":4},0]
["4.6.1","Cutting out and removing one course half brickwall and  building in  1 x 110 x 75mm lintels in lengths not exceeding 3m ","m",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
["4.6.2","Cutting out and removing one course one brickwall and  building in  2 x 110 x 75mm lintels in lengths not exceeding 3m ","m",1,{"v":198.73292976000002,"d":"198.73"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[4.7,"Fair face to brickwork on horizontal stretcher bond pointed with flush horizontal and vertical joints",null,null,0]
[{"$nulls":4},0]
["4.7.1","Extra for fair face","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["4.7.2","Half brick walls pointed both sides","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.8","Fair face to brickwork on horizontal stretcher bond pointed with recessed horizontal and flush vertical joints",null,null,0]
[{"$nulls":4},0]
["4.8.1","Extra for fair face","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["4.8.2","Half brick walls pointed both sides","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.9","Fair face to brickwork on horizontal stretcher bond pointed with recessed horizontal and vertical joints",null,null,0]
[{"$nulls":4},0]
["4.9.1","Extra for fair face","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["4.9.2","Half brick walls pointed both sides","m²",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["4.10","Bagging of 1:3 cement and sand mixture",null,null,0]
[{"$nulls":4},0]
["4.10.1","On brick surfaces","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["4.10.2","On concrete surfaces including fins, irregularities","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["4.11","Cement wash of 1:3 liquid cement and sand mixture applied with a brush",null,null,0]
[{"$nulls":4},0]
["4.11.1","On brick surfaces","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["4.11.2","On concrete surfaces including fins, irregularities","m²",1,{"v":15.947704240000004,"d":"15.95"}]
[{"$nulls":4},0]
["4.12","Joint forming material in movement joints",null,null,0]
[{"$nulls":4},0]
["4.12.1","10mm Fibre board built in vertically between brick skins","m²",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["4.12.2","10mm Fibre board built in vertically through brick walls","m²",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["4.12.3","10mm Bitumen impregnated fibre board built in vertically between brick skins","m²",1,{"v":142.30259168000003,"d":"142.30"}]
[{"$nulls":4},0]
["4.12.4","10mm Bitumen impregnated fibre board built in vertically through brick walls","m²",1,{"v":142.30259168000003,"d":"142.30"}]
[{"$nulls":4},0]
["4.13","Steel bar reinforcement",null,null,0]
[{"$nulls":4},0]
["4.13.1","8mm diameter mild steel bar built in horizontally (0.395 kg/m)","kg",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["4.13.2","10mm diameter high tensile steel bar built in horizontally (0.617 kg/m)","Kg",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["4.14","Reinforcement to brickwork",null,null,0]
[{"$nulls":4},0]
["4.14.1","75mm wide brick force built in horizontally","m",1,{"v":1.2267464800000003,"d":"1.23"}]
[{"$nulls":4},0]
["4.14.2","150mm wide brick force built in horizontally","m",1,{"v":1.2267464800000003,"d":"1.23"}]
[{"$nulls":4},0]
["4.14.3","230mm wide brick force built in horizontally","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["4.15","Prestressed fabricated lintels",null,null,0]
[{"$nulls":4},0]
["4.15.1","110 x 75mm. lintels in lengths not exceeding 3m.","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["4.15.2","110 x 75mm. lintels in lengths exceeding 3m and not exceeding 4,5m","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["4.15.3","150 x 75mm. lintels in lengths not exceeding 3m","m",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["4.15.4","150 x 75mm. lintels in lengths exceeding 3m and not exceeding 4,5m","m",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["4.16","Galvanised wire ties etc",null,null,0]
[{"$nulls":4},0]
["4.16.1","4mm diameter roof tie 2m girth bent double with one end fixed to timber and other end built into brickwork","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["4.16.2","4mm diameter roof tie 2m girth bent double with one end fixed to timber and other end cast into concrete","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["4.16.3","4mm diameter butterfly ties fixed to brickwork","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["4.17","Galvanised hoop iron cramps, ties, etc.",null,null,0]
[{"$nulls":4},0]
["4.17.1","40 x 1,6mm \"Tibond\" wall tie strips shot pinned to concrete and with tie bent out and built into brickwork","no",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["4.17.2","30 x 1,6mm cramp 300mm long with two ends fixed to  brickwork","no",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["4.17.3","30 x 1,6mm cramp 500mm long with one end fixed to wood and other end built into brickwork","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["4.17.4","30 x 1,6mm wall tie 500mm long with one end cast into concrete and other end built into brickwork","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["4.17.5","30 x 1,6mm wall tie 500mm long with one end shot pinned to concrete and other end built into brickwork","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["4.17.6","30 x 1,6mm roof tie 1,5m long with one fixed to timber and other end built into brickwork","no",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["4.17.7","30 x 1,6mm roof tie 1,5m long with one fixed to timber and other end cast into concrete","no",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["4.17.8","30 x 1,6mm ceiling hanger 1m long with one fixed to timber and other end shot pinned to concrete","no",1,{"v":13.494211280000002,"d":"13.49"}]
[{"$nulls":4},0]
["4.18","Air bricks etc",null,null,0]
[{"$nulls":4},0]
["4.18.1","230 x 76mm clay vermin proof air brick","no",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["4.18.2","230 x 150mm clay vermin proof air brick","no",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["4.18.3","230 x 160mm cement air brick","no",1,{"v":11.040718320000003,"d":"11.04"}]
[{"$nulls":4},0]
[null,"FACE BRICKWORK",null,null,0]
[{"$nulls":4},0]
["4.19","Face brick pointed with recessed horizontal and vertical joints. (Allow P.C. amount of R3,200.00 per 1000 for supply and delivery)",null,null,0]
[{"$nulls":4},0]
["4.19.1","Extra over ordinary brickwork for face brickwork in foundations","m²",1,{"v":157.02354944000004,"d":"157.02"}]
[{"$nulls":4},0]
["4.19.2","Extra over ordinary brickwork for face brickwork in foundations circular on plan","m²",1,{"v":163.15728184000005,"d":"163.16"}]
[{"$nulls":4},0]
["4.19.3","Extra over ordinary brickwork for face brickwork","m²",1,{"v":157.02354944000004,"d":"157.02"}]
[{"$nulls":4},0]
["4.19.4","Extra over ordinary brickwork for face brickwork circular on plan","m²",1,{"v":163.15728184000005,"d":"163.16"}]
[{"$nulls":4},0]
["4.19.5","Extra over ordinary brickwork for face brickwork in soldier courses","m²",1,{"v":157.02354944000004,"d":"157.02"}]
[{"$nulls":4},0]
["4.19.6","Extra over ordinary brickwork for face brickwork in soldier courses circular on plan","m²",1,{"v":163.15728184000005,"d":"163.16"}]
[{"$nulls":4},0]
["4.19.7","50mm cut lining to concrete","m²",1,{"v":418.32054968000006,"d":"418.32"}]
[{"$nulls":4},0]
["4.19.8","50mm cut lining to concrete circular on plan","m²",1,{"v":431.81476096000006,"d":"431.81"}]
[{"$nulls":4},0]
["4.19.9","Half brick wall pointed both sides","m²",1,{"v":431.81476096000006,"d":"431.81"}]
[{"$nulls":4},0]
["4.19.10","One brick walls in English bond pointed both sides","m²",1,{"v":834.1876064000003,"d":"834.19"}]
[{"$nulls":4},0]
["4.19.11","Extra over brickwork for brick-on-flat header course band","m",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["4.19.12","Extra over brickwork for brick-on-edge header course band","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["4.19.13","Extra over brickwork for brick-on-end soldier course band","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["4.19.14","Extra over brickwork for brick-on-edge header course lintel","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["4.19.14a","Extra over brickwork for brick-on-edge header course window sill set sloping","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["4.19.15","Extra over brickwork for brick-on-edge header course lintel pointed one side and 110mm soffit","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["4.19.16","Extra over brickwork for brick-on-end soldier course lintel","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["4.19.17","Extra over brickwork for brick-on-edge soldier course lintel pointed one side and 110mm soffit","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["4.19.17a","Fair raking cutting","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.18","Fair splay cutting","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.19","Fair stepped cutting and fitting over treads and risers","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.20","Fair circular cutting","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.21","Fair cutting at squint quoin or birdsmouth angle","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.22","Fair cutting to both sides at mitred squint quoin or birdsmouth  angle","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.23","Cutting toothings and bonding new face brickwork to existing","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.19.24","Fair cutting and fitting around pipes not exceeding 100mm diameter","no",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["4.19.25","Fair cutting and fitting around pipes exceeding 100mm diameter  and not exceeding 200mm diameter","no",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
[null,"Cleaning of face brick walls",null,null,0]
[{"$nulls":4},0]
["4.19.26","Cleaning of Face Brick walls sugar soap or equally approved detergent","m2",1,{"v":40.12001066666667,"d":"40.12"}]
[{"$nulls":4},0]
["4.19.27","Steam cleaning of Face Brick walls","m2",1,{"v":50.150013333333355,"d":"50.15"}]
[{"$nulls":4},0]
[null,"HERITAGE BUILDINGS ONLY - \"Restore Old face brick in poor condition",null,null,0]
[{"$nulls":4},0]
["4.19.28","Patching and sealing of old face brick wall in bad condition","m2",1,{"v":52.07886000000001,"d":"52.08"}]
[{"$nulls":4},0]
["4.20","Brick-on-edge header course copings, sills etc. of face brick as described",null,null,0]
[{"$nulls":4},0]
["4.20.1","Coping on top of half brick wall","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["4.20.2","Coping on top of one brick wall","m",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["4.20.3","Coping on top of one and a half brick wall","m",1,{"v":145.98283112000004,"d":"145.98"}]
[{"$nulls":4},0]
["4.20.4","Coping on racking top of one brick wall","m",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["4.20.5","Coping on top of one brick wall circular on plan","m",1,{"v":100.59321136000001,"d":"100.59"}]
[{"$nulls":4},0]
["4.20.6","230mm wide sills set level and slightly projecting","m",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["4.20.7","230mm wide sills set sloping and slightly projecting","m",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["4.21","Fair arches, recesses, etc. of face brick as described",null,null,0]
[{"$nulls":4},0]
["4.21.1","Extra over brickwork for segmental arch in half brick wall 900mm span and 340mm high formed of brick-on-edge header course ring pointed on soffit and one side including centre","no",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["4.21.2","Extra over brickwork for segmental arch in one brick wall 900mm span and 340mm high formed of brick-on-edge header course rings pointed on soffit and both sides including centre","no",1,{"v":62.56407048000001,"d":"62.56"}]
[{"$nulls":4},0]
["4.21.3","Extra over brickwork for 900mm diameter semi-circular arch in one brick wall formed of  2 brick-on-edge header course rings pointed on soffit and both sides including centre","no",1,{"v":143.52933816000004,"d":"143.53"}]
[{"$nulls":4},0]
[null,"QUARRY TILES",null,null,0]
[{"$nulls":4},0]
["4.22","150x150x25mm quarry tiles on brickwork with continuous joints in both directions and pointed on all exposed surfaces",null,null,0]
[{"$nulls":4},0]
["4.22.1","150mm wide sill of one row of tiles set flat or sloping and slightly projecting","m",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["4.22.2","150mm wide bullnosed edge sill of one row of tiles set flat or sloping and slightly projecting","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["4.23","300 x 300 x 10mm quarry tiles with continuous joints in both directions flush pointed on all exposed surfaces",null,null,0]
[{"$nulls":4},0]
["4.23.1","Paving on 25mm thick mortar bed","m²",1,{"v":458.80318352000006,"d":"458.80"}]
[{"$nulls":4},0]
["4.23.2","Paving on average 50mm thick mortar bed to falls","m²",1,{"v":478.4311272000001,"d":"478.43"}]
[{"$nulls":4},0]
["4.23.3","Extra for 150mm wide band, margin, etc. in contrasting colour","m",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["4.23.4","Fair circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["4.23.5","300mm wide treads on 25mm thick mortar bed","m",1,{"v":160.70378888000002,"d":"160.70"}]
[{"$nulls":4},0]
["4.23.6","330mm wide treads with bullnosed edge on 25mm thick mortar bed","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["4.23.7","170mm high risers on 25mm mortar bed","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
[null,"NUTEC-CEMENT / FIBRE-CEMENT WINDOW SILLS",null,null,0]
[{"$nulls":4},0]
["4.24","Natural grey sills in single lengths bedded in class I mortar including metal fixing lugs etc",null,null,0]
[{"$nulls":4},0]
["4.24.1","15 x 150mm wide sills set flat and slightly projecting","m",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["4.24.2","15 x 200mm wide sills set sloping and slightly projecting","m",1,{"v":159.47704240000004,"d":"159.48"}]
[{"$nulls":4},0]
[null,"DECORATIVE BLOCKS",null,null,0]
[{"$nulls":4},0]
["4.25","400 x 400 x 100mm Concrete grille blocks in class II mortar pointed with flush joints pointed on both sides",null,null,0]
[{"$nulls":4},0]
["4.25.1","In walls","m²",1,{"v":278.4714509600001,"d":"278.47"}]
[{"$nulls":4},0]
[null,"GLASS BRICK WALLS",null,null,0]
[{"$nulls":4},0]
["4.26","190 x 190 x 80mm \"Ezylay System - Solaris Samba\" or equal and approved glass blocks bedded and jointed in slow-setting class I mortar with continuous joints in both directions pointed in tinted mortar both sides with flush horizontal and vertical joints",null,null,0]
[{"$nulls":4},0]
["4.26.1","80mm walls","m²",1,{"v":937.2343107200002,"d":"937.23"}]
[{"$nulls":4},0]
["4.26.2","80mm walls circular on plan","m²",1,{"v":945.82153608,"d":"945.82"}]
[{"$nulls":4},0]
["4.27","190 x 190 x 80mm \"Ezylay System - Solaris Light Diffusing\" or equal and approved glass blocks bedded and jointed in slow-setting class I mortar with continuous joints in both directions pointed in tinted mortar both sides with recessed horizontal and vertical joints",null,null,0]
[{"$nulls":4},0]
["4.27.1","80mm walls","m²",1,{"v":1066.0426911200002,"d":"1,066.04"}]
[{"$nulls":4},0]
["4.27.2","80mm walls circular on plan","m²",1,{"v":1074.6299164800002,"d":"1,074.63"}]
[{"$nulls":4},0]
["4.28","Sundries in glass block walls",null,null,0]
[{"$nulls":4},0]
["4.28.1","Two layers Type FV damp proof course horizontal slip joint below glass blocks","m²",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["4.28.2","10mm expanded polystyrene (density 33kg per m³) horizontal between top of glass blocks and structure","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["4.28.3","10mm expanded polystyrene (density 33kg per m³) vertically between glass blocks and structure","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["4.28.4","8mm diameter galvanised mild steel bar reinforcement horizontally and vertically","kg",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["4.29","Vanity Slabs to tops",null,null,0]
[{"$nulls":4},0]
["4.29.1","Granite slab 600mm wide","m",1,{"v":1429.27538,"d":"1,429.28"}]
[{"$nulls":4},0]
["4.29.2","Granite slab 900mm wide","m",1,{"v":1579.72542,"d":"1,579.73"}]
[{"$nulls":4},0]
["4.29.3","Open ended dog-leg shaped vanity basin 600mm wide at a 15deg angel with a 50 x 50 mm waste chanel, mounted on concealed steel angle brackets @ 7000mm centres. Inclusing a 600mm high splashback all made of granite","no",1,{"v":2571.5383760000004,"d":"2,571.54"}]
[{"$nulls":4},0]
["4.29.4","Extra over for cutting and opening of granite slab for stoves ","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["4.29.5","Extra over for cutting and opening of tap holes","no",1,{"v":92.00598600000001,"d":"92.01"}]
{"$rows_empty":16}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Waterproofing","index":4,"n_rows":230,"n_cols":7,"rows_kept":230,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 5"]
[]
[null,"WATERPROOFING"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Waterproofing to roofs, basements, etc shall be laid under a ten year guarantee. Waterproofing to roofs shall be laid to even falls to outlets etc with necessary ridges, hips and valleys. Description of sheet or membrane waterproofing shall be deemed to include additional labour to turn-ups and turndowns"]
[]
[null,"DAMP PROOFING OF WALLS AND FLOORS"]
[]
[5.1,"One layer of 375 micron \"Gundle plastic Brikgrip DPC\" embossed damp proof course"]
[]
["5.1.1","In walls","m²",1,{"v":32.3956352,"d":"32.40"}]
[{"$nulls":4},0]
[5.2,"One layer of 250 micron \"Gundle Plastic USB Green\" waterproofing sheeting sealed at laps with \"Gunplas Pressure Sensitive Tape\"",null,null,0]
[{"$nulls":4},0]
["5.2.1","Under surface beds","m²",1,{"v":22.86750720000001,"d":"22.87"}]
[{"$nulls":4},0]
["5.2.2","Vertically between walls","m²",1,{"v":22.86750720000001,"d":"22.87"}]
[{"$nulls":4},0]
[5.3,"One layer of 250 micron \"Gundle Plastic Hyperelastic Orange\" waterproofing sheeting sealed at laps with \"Superstik\" tape carried out strictly in accordance with the manufacturer's instructions",null,null,0]
[{"$nulls":4},0]
["5.3.1","Under surface beds","m²",1,{"v":53.3575168,"d":"53.36"}]
[{"$nulls":4},0]
["5.3.2","Vertically between walls","m²",1,{"v":53.3575168,"d":"53.36"}]
[{"$nulls":4},0]
[5.4,"Two coats \"Brickseal\" bitumen emulsion waterproof coating",null,null,0]
[{"$nulls":4},0]
["5.4.1","On concrete floors","m²",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["5.4.2","On concrete walls, columns and beams","m²",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["5.4.3","On concrete walls, columns and beams in foundations","m²",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["5.4.4","On brick walls","m²",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["5.4.5","On brick bagged walls","m²",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
[5.5,"Primer and two coats \"Durabit\" rubber bitumen emulsion waterproof coating",null,null,0]
[{"$nulls":4},0]
["5.5.1","On IBR, corrugated, etc. roof sheeting","m²",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["5.5.2","On concrete floors","m²",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["5.5.3","On concrete walls, columns and beams","m²",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["5.5.4","On concrete walls, columns and beams in foundations","m²",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["5.5.5","On brick walls","m²",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["5.5.6","On brick bagged walls","m²",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
[5.6,"Primer and three coats \"Durabit\" rubber bitumen emulsion waterproof coating and one coat \"Silvershield\" aluminium coating",null,null,0]
[{"$nulls":4},0]
["5.6.1","On concrete floors","m²",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["5.6.2","On concrete walls, columns and beams","m²",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["5.6.3","On concrete walls, columns and beams in foundations","m²",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["5.6.4","On brick walls","m²",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["5.6.5","On brick bagged walls","m²",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
[5.7,"4mm \"Derbigum SP4\" or equal and approved fully bonded waterproofing system carried out strictly in accordance with the manufacturer's instructions and under a Ten Year Insurance Backed Guarantee on materials and workmanship (On Concrete)",null,null,0]
[{"$nulls":4},0]
["5.7.1","On flat floors","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.2","On sloping floors","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.3","On flat roofs","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.4","On flat wooden panels,roofs, etc","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.5","On sloping roofs","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.7","On parapet walls","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.8","On tops and sides of invert beams","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.9","On bottom and sides of floor ducts, channels, etc","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.10","On bottom and sides of box gutters","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.11","On bottom and sides of planter boxes","m²",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["5.7.12","On internal surfaces of 450 x 450 x 450mm deep sump, catchpit, etc","no",1,{"v":228.67507200000006,"d":"228.68"}]
[{"$nulls":4},0]
["5.7.13","Sealing edge to brickwork or concrete","m",1,{"v":60.98001920000001,"d":"60.98"}]
[{"$nulls":4},0]
["5.7.14","Sealing edge to brickwork or concrete including trowelled mastic bead","m",1,{"v":93.37565440000003,"d":"93.38"}]
[{"$nulls":4},0]
["5.7.15","Flashing strip 200mm girth a turn-ups including sealing top edge into groove with mastic","m",1,{"v":93.37565440000003,"d":"93.38"}]
[{"$nulls":4},0]
["5.7.16","Additional membrane 200mm girth at internal and external angles","m",1,{"v":60.98001920000001,"d":"60.98"}]
[{"$nulls":4},0]
["5.7.17","Additional membrane 200mm girth at internal and external angles circular on plan including darts as necessary","m",1,{"v":60.98001920000001,"d":"60.98"}]
[{"$nulls":4},0]
["5.7.18","Additional membrane 200mm girth a turn-ups including flashing strip 200mm girth and sealing top edge into groove with mastic","m",1,{"v":93.37565440000003,"d":"93.38"}]
[{"$nulls":4},0]
["5.7.19","Type 40 bituminous fibreglass felt protection layer with coarse building sand blinding loose laid over horizontal waterproofing with 50mm wide side and end laps sealed with cold bituminous adhesive","m²",1,{"v":261.0707072,"d":"261.07"}]
[{"$nulls":4},0]
["5.7.20","30 x 30mm softwood timber triangular fillet","m",1,{"v":19.05625600000001,"d":"19.06"}]
[{"$nulls":4},0]
["5.7.21","50 x 50mm softwood timber triangular fillet","m",1,{"v":28.584384000000007,"d":"28.58"}]
[{"$nulls":4},0]
[null,"PROTECTIVE STONE DRESSING",null,null,0]
[{"$nulls":4},0]
[5.8,"20mm crusher stone dressing evenly spread with larger stones around outlets",null,null,0]
[{"$nulls":4},0]
["5.8.1","50mm thick on waterproofing to flat roofs","m²",1,{"v":47.64064000000001,"d":"47.64"}]
[{"$nulls":4},0]
[null,"PROTECTIVE ROOFING PAINT",null,null,0]
[{"$nulls":4},0]
[5.9,"Two coats bituminous aluminium paint",null,null,0]
[{"$nulls":4},0]
["5.9.1","On waterproofing to roofs","m²",1,{"v":51.451891200000006,"d":"51.45"}]
[{"$nulls":4},0]
["5.9.2","On waterproofing to box gutters","m²",1,{"v":51.451891200000006,"d":"51.45"}]
[{"$nulls":4},0]
[null,"JOINT SEALANTS, ETC.",null,null,0]
[{"$nulls":4},0]
[{"v":5.1,"d":"5.10"},"Silicone sealing compound including backing cord, bond breaker, primer, etc.",null,null,0]
[{"$nulls":4},0]
["5.10.1","6 x 12mm. in saw cut joints in concrete surface beds","m",1,{"v":51.451891200000006,"d":"51.45"}]
[{"$nulls":4},0]
["5.10.2","10 x 12mm. in expansion joints between concrete surface beds and brickwork including raking out joint filler as necessary","m",1,{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
["5.10.3","10 x 12mm. in vertical expansion joints between brickwork or concrete surfaces including raking out joint filler as necessary","m",1,{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
["5.10.4","10 x 12mm. in expansion joints in soffits raking out joint filler as necessary","m",1,{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
["5.10.5","10 x 12mm. in expansion joints in soffits raking out joint filler as necessary","m",1,{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
[5.11,"Clear silicon sealant",null,null,0]
[{"$nulls":4},0]
["5.11.1","Between glazed tiles and sanitary fittings","m",1,{"v":17.150630400000004,"d":"17.15"}]
[{"$nulls":4},0]
["5.11.2","\"The Works\" or equivalent wet surface sealant","m",1,{"v":102.90378240000001,"d":"102.90"}]
[{"$nulls":4},0]
[null,"EPOXY",null,null,0]
[{"$nulls":4},0]
[5.12,"\"EPOXY 319/20\" epoxy floor and wall coating applied in strict accordance with the manufacturer's instructions ",null,null,0]
[{"$nulls":4},0]
["5.12.1","On screeded floors","m²",1,{"v":123.86566400000002,"d":"123.87"}]
[{"$nulls":4},0]
["5.12.2","On screeded seating slabs","m²",1,{"v":123.86566400000002,"d":"123.87"}]
[{"$nulls":4},0]
["5.12.3","On plastered walls","m²",1,{"v":123.86566400000002,"d":"123.87"}]
[{"$nulls":4},0]
[5.13,"Primer and two coats \"Rubberising\"  bitumen emulsion waterproof coating",null,null,0]
[{"$nulls":4},0]
["5.13.1","On concrete floors","m²",1,{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
["5.13.2","On concrete walls, columns and beams","m²",1,{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
["5.13.3","On concrete walls, columns and beams in foundations","m²",1,{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
["5.13.4","On brick walls","m²",1,{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
["5.13.5","On brick bagged walls","m²",1,{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
[null,"Fibre Flex membrane free \"Flash Harry\" or equally approved waterproofing",null,null,0]
[{"$nulls":4},0]
["5.14.1","On flat roofs","m²",1,{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
["5.14.2","On flat wooden panels,roofs, etc","m²",1,{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
["5.14.3","On sloping roofs","m²",1,{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
["5.14.4","On sloping IBR roof sheeeting","m²",1,{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
["5.14.5","On walls","m²",1,{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
["5.14.6","On tops and sides of invert beams","m²",1,{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[5.15,"Bituminised heat-laminated layer of aluminium foil \"Slatex 2000\" or equivalent waterproofing to slate roofs",null,null,0]
[{"$nulls":4},0]
["5.15.1","On flat roofs","m²",1,{"v":199.93823795200007,"d":"199.94"}]
[{"$nulls":4},0]
["5.15.2","On sloping roofs","m²",1,{"v":199.93823795200007,"d":"199.94"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[5.16,"Two coats of one-component Siloxane \"abe-wall seal\" or equivalent waterporoofing repelent ",null,null,0]
[{"$nulls":4},0]
["5.16.1","On walls","m²",1,{"v":999.1766708480004,"d":"999.18"}]
[{"$nulls":4},0]
["5.16.2","On tops and sides of invert beams","m²",1,{"v":999.1766708480004,"d":"999.18"}]
[{"$nulls":4},0]
[5.17,"Bitumen emulsion \"abe-Flintkote 3\" or equivalent waterproofing",null,null,0]
[{"$nulls":4},0]
["5.17.1"," On concrete retaining walls","m²",1,{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
["5.17.2","On basements","m²",1,{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
["5.17.3"," On abutments","m²",1,{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
["5.17.4","On wingwalls","m²",1,{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
[5.18,"Three coats of two-component \"Vandex\" or equivalent waterporoofing repelent ",null,null,0]
[{"$nulls":4},0]
["5.18.1","On walls","m²",1,{"v":977.9814400000004,"d":"977.98"}]
[{"$nulls":4},0]
["5.18.2","On tops and sides of invert beams","m²",1,{"v":977.9814400000004,"d":"977.98"}]
{"$rows_empty":20}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Roof Covering","index":5,"n_rows":680,"n_cols":7,"rows_kept":680,"merged":[[0,4,0,6]],"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 6"]
[]
[null,"ROOF COVERINGS ETC."]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Straight cutting"]
[]
[null,"Description of all roof coverings are deemed to include for all straight cutting"]
[]
[]
[null,"TILES"]
[]
[6.1,"\"Marley Mendip\" or equal and approved profile M22 factory-coated through colour concrete roof tiles, size 420 x 332mm manufactured in accordance with SABS 542, of approved colour with matching fittings nailed and/or fixed with suitable non-corrosive clips as required to and including 38x50mm"]
[null,"sawn softwood battens at 320mm centres on an underlay of SABS approved \"Gundle\" white 250 micron plastic sheeting laid horizontally over trusses, with minimum overlap of 150mm and secured with non-corrosive clout nails to the trusses"]
[]
["6.1.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":222.04111288000004,"d":"222.04"}]
[{"$nulls":4},0]
["6.1.2","Side cladding at gable ends","m²",1,{"v":222.04111288000004,"d":"222.04"}]
[{"$nulls":4},0]
["6.1.3","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.1.4","Taper ridge tiles edge bedded and pointed in 1:3 cement/sand mortar tinted to match tile colour over 150mm wide DPC","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.1.5","Taper hip tiles edge bedded and pointed in 1:3 cement/sand mortar tinted to match tile colour over 150mm wide DPC","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.1.6","Verge capping tiles to match roofing tiles fixed with non-corrosive fixing accessories","m",1,{"v":256.39001432000003,"d":"256.39"}]
[{"$nulls":4},0]
["6.1.7","Purpose made tile to end ridge bedded and pointed in 1:3 cement mortar tinted to match existing colour","no",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["6.1.8","Purpose made tile to two-way intersection of ridge with hips bedded and pointed in 1:3 cement mortar tinted to match existing colour","no",1,{"v":150.88981704000003,"d":"150.89"}]
[{"$nulls":4},0]
["6.1.9","Open cut valley including cutting of tiles and waste to both sides forming a neat open channel of at least 100mm","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["6.1.10","Cutting and waste at abutments, parapets and verges","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.1.11","Making good and sealing loose tiles to roof","m",1,{"v":43.97770400000001,"d":"43.98"}]
[{"$nulls":4},0]
[6.2,"\"Harveytile\" 1675 x 397mm \"Tufftile\" Zincalume coated mild steel tile with stonecoat finish on one side fixed with serrated galvanized clout nails to and including 38 x 38mm sawn softwood batten at 369mm centres on an",null,null,0]
[null,"underlay of SABS approved \"Gundle\" white 250 micron plastic sheeting with 150mm lapped and sealed joints laid horizontally over and secured with non-corrosive clout nails to the trusses ",null,null,0]
[{"$nulls":4},0]
["6.2.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":244.24522416800002,"d":"244.25"}]
[{"$nulls":4},0]
["6.2.2","Side cladding to gables, etc","m²",1,{"v":244.24522416800002,"d":"244.25"}]
[{"$nulls":4},0]
["6.2.3","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.2.4","Square ridge tapered capping to match roofing tile","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.2.5","Angle ridge tapered capping to match roofing tile","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.2.6","Square hip tapered capping to match roofing tile","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.2.7","Angle hip tapered capping to match roofing tile","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.2.8","Gable tapered trim to match roofing tile","m",1,{"v":256.39001432000003,"d":"256.39"}]
[{"$nulls":4},0]
["6.2.9","Bargeboard serrated cover to match roofing tile ","m",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["6.2.10","Sidewall serrated flashing to match roofing tile","m",1,{"v":152.48458746400001,"d":"152.48"}]
[{"$nulls":4},0]
["6.2.11","Headwall flashing to match roofing tile","m",1,{"v":152.48458746400001,"d":"152.48"}]
[{"$nulls":4},0]
["6.2.12","Cover flashing to match roofing tile","m",1,{"v":152.48458746400001,"d":"152.48"}]
[{"$nulls":4},0]
["6.2.13","Hip end cap","no",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["6.2.14","Ridge end cap","no",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["6.2.15","Junction of ridge with two hip capping","no",1,{"v":150.88981704000003,"d":"150.89"}]
[{"$nulls":4},0]
["6.2.16","Junction of ridge with one ridge capping","no",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["6.2.17","Cutting and waste including bending edge of tiles up or down at abutments, parapets and verges","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["6.2.18","Cut valley including cutting of tiles and waste to both sides including bending edge of tiles down forming a neat 75mm open channel","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["6.2.19","Cut valley including cutting of tiles and waste to both sides including bending edge of tiles down forming a neat closed channel","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["6.2.20","Cut hip including cutting of tiles and waste to both sides including bending edge of tiles up forming a snug tapered fit","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.2.21","Making good and sealing loose tiles to roof","m",1,{"v":43.97770400000001,"d":"43.98"}]
[{"$nulls":4},0]
[6.3,"THATCH",null,null,0]
[{"$nulls":4},0]
[null,"User note",null,null,0]
[{"$nulls":4},0]
[null,"Grass in the Gauteng area suitable for thatch is the hyparrhenia species and is obtainable in lengths varying from 760 to 1020mm",null,null,0]
[{"$nulls":4},0]
[null,"The minimum density to which the above-mentioned grass should be compacted is 30kg/m2/150mm thickness",null,null,0]
[{"$nulls":4},0]
[null,"The fibre blanket usually consists of an interlay or an underlay of multilayered fire -retarded reinforced double-sided aluminium foil sheeting",null,null,0]
[{"$nulls":4},0]
[6.3,"150mm Thick thatch of hand cut grass of the hyparrhenia hirta species in lengths varying from 760 to 1020mm laid in bundles of suitable size, compacted to a minimum density of 30kg/m2/150mm thickness and fixed by means of suitable fixing rods interlaced through and ovet the bundles at not axceeding 600mm centres ans secured with tarred twine to and including eucalyptus battens CCa treated in accordance with SANS 457-2, varying in diameter from 20 to 40mm, spaced at maximum 300mm centres generally and at closer centres nearer to eaves, including a fire-retardent interlay of multi-layered reinforced double-sided aluminium foil sheeting in accordance with SANS 1381-4 with mass of not less than 272g/m2 and a Class I fire rating in accordance with SANS 0177-3",null,null,0]
[{"$nulls":4},0]
["6.3.1","Covering to general roof slopes","m²",1,{"v":284.60518336000007,"d":"284.61"}]
[{"$nulls":4},0]
["6.3.2","Covering to general roof slopes including a spreadlayer to exposed soffit","m²",1,{"v":284.60518336000007,"d":"284.61"}]
[{"$nulls":4},0]
["6.3.3","Coverings to dormers, turrets, etc","m²",1,{"v":284.60518336000007,"d":"284.61"}]
[{"$nulls":4},0]
["6.3.4","Ridges formed by extending covering above ridge level on the one roof slope, bending over and down on the opposite slope and fixing and securing as described for roof covering and repeating the process on the other roof slope including covering with galvanised wire bird netting 900mm girth and necessary additional fixing rods","m",1,{"v":176.65149312000005,"d":"176.65"}]
[{"$nulls":4},0]
["6.3.5","Purpose made continous glass fibre ridge capping of not less than 1.5mm thick material 1300mm girth and in suitable lengths, securely fixed to thatch with 75mm wire lapped and sealed heading joints including grass filling under","m",1,{"v":218.36087344000003,"d":"218.36"}]
[{"$nulls":4},0]
["6.3.6","Extra over ridge capping for purpose made angle piece","no",1,{"v":235.53532416000004,"d":"235.54"}]
[{"$nulls":4},0]
["6.3.7","Extra over ridge capping for purpose made curved returned end piece","no",1,{"v":235.53532416000004,"d":"235.54"}]
[{"$nulls":4},0]
[null,"PROFILED FIBRE-CEMENT SHEETING AND ACCESSORIES",null,null,0]
[{"$nulls":4},0]
[6.4,"\"Nutec Bigsix\" sheeting fixed to timber/steel purlins or rails",null,null,0]
[{"$nulls":4},0]
["6.4.1","Roof covering with pitch not exceeding 50 degrees with side and end laps sealed with 12 x 25mm closed cell impregnated polyurethane foam strips","m²",1,{"v":239.21556360000005,"d":"239.22"}]
[{"$nulls":4},0]
["6.4.2","Side cladding","m²",1,{"v":212.22714104000002,"d":"212.23"}]
[{"$nulls":4},0]
["6.4.3","Extra over roof covering for soaker flange sheet suitable for ventilator with throat size 850 x 460mm","no",1,{"v":570.4371132000002,"d":"570.44"}]
[{"$nulls":4},0]
["6.4.4","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.4.5","Side apron flashing","m",1,{"v":145.98283112000004,"d":"145.98"}]
[{"$nulls":4},0]
["6.4.6","End apron flashing","m",1,{"v":208.54690160000007,"d":"208.55"}]
[{"$nulls":4},0]
["6.4.7","Plain fixed angle ridge/hip capping flashing","m",1,{"v":231.85508472,"d":"231.86"}]
[{"$nulls":4},0]
["6.4.8","Plain adjustable ridge/hip capping flashing","m",1,{"v":311.5936059200001,"d":"311.59"}]
[{"$nulls":4},0]
["6.4.9","Fixed angle wide profile ridge sheets","m",1,{"v":231.85508472,"d":"231.86"}]
[{"$nulls":4},0]
["6.4.10","Close fitting adjustable ridge capping","m",1,{"v":247.80278896000002,"d":"247.80"}]
[{"$nulls":4},0]
["6.4.11","Fixed angle sawtooth ridge capping","m",1,{"v":231.85508472,"d":"231.86"}]
[{"$nulls":4},0]
["6.4.12","Adjustable sawtooth ridge capping","m",1,{"v":284.60518336000007,"d":"284.61"}]
[{"$nulls":4},0]
["6.4.13","Birdproofing","m",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["6.4.14","Eaves fillers","m",1,{"v":157.02354944000004,"d":"157.02"}]
[{"$nulls":4},0]
["6.4.15","Straight sill flashing","m",1,{"v":152.11656352,"d":"152.12"}]
[{"$nulls":4},0]
["6.4.16","U-flashing","m",1,{"v":154.57005648,"d":"154.57"}]
[{"$nulls":4},0]
["6.4.17","Hip and end cap","no",1,{"v":103.04670432000002,"d":"103.05"}]
[{"$nulls":4},0]
["6.4.18","Ridge end cap","no",1,{"v":103.04670432000002,"d":"103.05"}]
[{"$nulls":4},0]
["6.4.19","Junction of ridge with two hip cappings","no",1,{"v":207.32015512000004,"d":"207.32"}]
[{"$nulls":4},0]
[null,"PROFILED METAL SHEETING AND ACCESSORIES",null,null,0]
[{"$nulls":4},0]
[6.5,"0,58mm corrugated profile roll-formed Z275 spelter galvanised steel sheeting, in single lengths, fixed to timber/steel purlins or rails and 0,58mm galvanised sheet steel accessories",null,null,0]
[{"$nulls":4},0]
["6.5.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":272.33771856000004,"d":"272.34"}]
[{"$nulls":4},0]
["6.5.2","Roof covering with pitch not exceeding 50 degrees side laps seam stitched","m²",1,{"v":278.4714509600001,"d":"278.47"}]
[{"$nulls":4},0]
["6.5.3","Roof covering with pitch not exceeding 50 degrees side laps seal with 6 x 20mm closed cell impregnated polyurethane strips and seam stitched","m²",1,{"v":293.19240872,"d":"293.19"}]
[{"$nulls":4},0]
["6.5.4","Side cladding","m²",1,{"v":272.33771856000004,"d":"272.34"}]
[{"$nulls":4},0]
["6.5.5","Side cladding circular on plan to 3,0m radius","m²",1,{"v":272.33771856000004,"d":"272.34"}]
[{"$nulls":4},0]
["6.5.6","Roof covering and side cladding to dormers, turrets, etc","m²",1,{"v":272.33771856000004,"d":"272.34"}]
[{"$nulls":4},0]
["6.5.7","Extra over roof covering /side cladding for 1,25mm semi-opaque 90% light transmission \"Modek - Polycarbonate\" translucent panel","m²",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["6.5.8","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.5.9","Extra over roof covering for 20 degree crank to form ridge","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["6.5.10","Extra over roof covering for 110 degrees bullnose to form 450mm radius at edge","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["6.5.11","Ridge capping 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.5.12","Hip capping 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.5.13","Side wall flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.5.14","Head wall flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.5.15","Cover flashing 154mm girth","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["6.5.16","Gable trim 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.5.17","Apex flashing 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.5.18","Corner trim 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.5.19","Apron flashing 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.5.20","Drip flashing 154mm girth","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["6.5.21","Sill flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.5.22","Jamb flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.5.23","Narrow and broad flute closers ","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["6.5.24","Narrow and broad flute closers raking at valleys or hips ","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.5.25","Moulded narrow and broad rib polyethylene filler blocks","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.5.26","Moulded narrow and broad rib polyethylene filler blocks raking at valleys and hips","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.5.27","Making good roof sheeting by screwing and sealing of loose or missing  screws /nails. Sealing using waterproofing ","m2",1,{"v":37.61251000000001,"d":"37.61"}]
[{"$nulls":4},0]
[6.6,"0,58mm corrugated profile roll-formed Z275 spelter galvanised steel sheeting with \"Global-Sil\" finish on one side, in single lengths fixed to timber/steel purlins or rails and 0,58mm galvanised sheet steel accessories with \"Global-Sil\" finish on one side",null,null,0]
[{"$nulls":4},0]
["6.6.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["6.6.2","Roof covering with pitch not exceeding 50 degrees with side laps seam stitched","m²",1,{"v":318.9540848000001,"d":"318.95"}]
[{"$nulls":4},0]
["6.6.3","Roof covering with pitch not exceeding 50 degrees with side laps seal with 6 x 20mm closed cell impregnated polyurethane strips and seam stitched","m²",1,{"v":333.67504256,"d":"333.68"}]
[{"$nulls":4},0]
["6.6.4","Side cladding","m²",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["6.6.5","Side cladding circular on plan to 3,0m radius","m²",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["6.6.6","Roof covering and side cladding to dormers, turrets, etc","m²",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["6.6.7","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.6.8","Extra over roof covering for 20 degree crank to form ridge","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["6.6.9","Extra over roof covering for 110 degrees bullnose to form 450mm radius at edge","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["6.6.10","Ridge capping 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.6.11","Hip capping 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.6.12","Side wall flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.6.13","Head wall flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.6.14","Cover flashing 154mm girth","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["6.6.15","Gable trim 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.6.16","Apex flashing 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.6.17","Corner trim 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.6.18","Apron flashing 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.6.19","Drip flashing 154mm girth","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["6.6.20","Sill flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.6.21","Jamb flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.6.22","Narrow and broad flute closers ","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["6.6.23","Narrow and broad flute closers raking at valleys or hips ","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.6.24","Moulded narrow and broad rib polyethylene filler blocks","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.6.25","Moulded narrow and broad rib polyethylene filler blocks raking at valleys and hips","m",1,{"v":37.61251000000001,"d":"37.61"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.6.26","Making good roof sheeting by screwing and sealing of loose or missing  screws /nails. Sealing using waterproofing ","m2",1,{"v":40.50578000000001,"d":"40.51"}]
[{"$nulls":4},0]
[6.7,"0,58mm IBR profile Z275 spelter galvanised steel troughed sheeting, in single lengths fixed to timber/steel purlins or rails and 0,58mm galvanised sheet steel accessories",null,null,0]
[{"$nulls":4},0]
["6.7.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":268.65747912000006,"d":"268.66"}]
[{"$nulls":4},0]
["6.7.2","Roof covering with pitch not exceeding 50 degrees with side laps seam stitched","m²",1,{"v":276.017958,"d":"276.02"}]
[{"$nulls":4},0]
["6.7.3","Roof covering with pitch not exceeding 50 degrees with side laps seal with 6 x 20mm closed cell impregnated polyurethane strips and seam stitched","m²",1,{"v":289.5121692800001,"d":"289.51"}]
[{"$nulls":4},0]
["6.7.4","Side cladding","m²",1,{"v":268.65747912000006,"d":"268.66"}]
[{"$nulls":4},0]
["6.7.5","Side cladding circular on plan to 3,0m radius","m²",1,{"v":268.65747912000006,"d":"268.66"}]
[{"$nulls":4},0]
["6.7.6","Roof covering and side cladding to dormers, turrets, etc","m²",1,{"v":268.65747912000006,"d":"268.66"}]
[{"$nulls":4},0]
["6.7.7","Extra over roof covering /side cladding for 1,25mm semi-opaque 90% light transmission \"Modek - Polycarbonate\" translucent panel","m²",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["6.7.8","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.7.9","Extra over roof covering for 20 degree crank to form ridge","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["6.7.10","Extra over roof covering for 110 degrees bullnose to form 450mm radius at edge","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["6.7.11","Ridge capping 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.7.12","Hip capping 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.7.13","Side wall flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.7.14","Head wall flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.7.15","Cover flashing 154mm girth","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["6.7.16","Gable trim 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.7.17","Apex flashing 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.7.18","Corner trim 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.7.19","Apron flashing 462mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.7.20","Drip flashing 154mm girth","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["6.7.21","Sill flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.7.22","Jamb flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["6.7.23","Narrow and broad flute closers ","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["6.7.24","Narrow and broad flute closers raking at valleys or hips ","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.7.25","Moulded narrow and broad rib polyethylene filler blocks","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.7.26","Moulded narrow and broad rib polyethylene filler blocks raking at valleys and hips","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.7.27","Making good roof sheeting by screwing and sealing of loose or missing  screws /nails. Sealing using waterproofing ","m2",1,{"v":40.50578000000001,"d":"40.51"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[6.8,"0,58mm. IBR profile Z275 spelter galvanised steel troughed sheeting with \"Global-Sil\" finish on one side, in single lengths fixed to steel purlins or rails and 0,58mm galvanised sheet steel accessories with \"Global-Sil\" finish on one side",null,null,0]
[{"$nulls":4},0]
["6.8.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":309.14011296,"d":"309.14"}]
[{"$nulls":4},0]
["6.8.2","Roof covering with pitch not exceeding 50 degrees with side laps seam stitched","m²",1,{"v":314.0470988800001,"d":"314.05"}]
[{"$nulls":4},0]
["6.8.3","Roof covering with pitch not exceeding 50 degrees with side laps seal with 6 x 20mm closed cell impregnated polyurethane strips and seam stitched","m²",1,{"v":314.0470988800001,"d":"314.05"}]
[{"$nulls":4},0]
["6.8.3a","Side cladding","m²",1,{"v":309.14011296,"d":"309.14"}]
[{"$nulls":4},0]
["6.8.4","Side cladding circular on plan to 3,0m radius","m²",1,{"v":309.14011296,"d":"309.14"}]
[{"$nulls":4},0]
["6.8.5","Roof covering and side cladding to dormers, turrets, etc","m²",1,{"v":309.14011296,"d":"309.14"}]
[{"$nulls":4},0]
["6.8.6","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.8.7","Extra over roof covering for 20 degree crank to form ridge","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["6.8.9","Extra over roof covering for 110 degrees bullnose to form 450mm radius at edge","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["6.8.10","Ridge capping 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.8.11","Hip capping 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.8.12","Side wall flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.8.13","Head wall flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.8.14","Cover flashing 154mm girth","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["6.8.15","Gable trim 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.8.16","Apex flashing 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.8.17","Corner trim 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.8.18","Apron flashing 462mm girth","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.8.19","Drip flashing 154mm girth","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["6.8.20","Sill flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.8.21","Jamb flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.8.22","Narrow and broad flute closers ","m",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["6.8.23","Narrow and broad flute closers raking at valleys or hips ","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.8.24","Moulded narrow and broad rib polyethylene filler blocks","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["6.8.25","Moulded narrow and broad rib polyethylene filler blocks raking at valleys and hips","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.8.26","Making good roof sheeting by screwing and sealing of loose or missing  screws /nails. Sealing using waterproofing ","m2",1,{"v":40.50578000000001,"d":"40.51"}]
[{"$nulls":4},0]
[6.9,"0,6mm \"Klip-lok 700\"  Z275 spelter galvanised ribbed sheet steel in single lengths fixed to timber/steel purlins or rails and 0,58mm galvanised sheet steel accessories",null,null,0]
[{"$nulls":4},0]
["6.9.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":344.7157608800001,"d":"344.72"}]
[{"$nulls":4},0]
["6.9.2","Side cladding","m²",1,{"v":352.07623976,"d":"352.08"}]
[{"$nulls":4},0]
["6.9.3","Roof covering and side cladding to dormers, turrets, etc","m²",1,{"v":365.57045104,"d":"365.57"}]
[{"$nulls":4},0]
["6.9.4","Extra over roof covering /side cladding for 1,25mm semi-opaque 90% light transmission \"Modek - Polycarbonate\" translucent panel","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.9.5","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.9.6","Extra over roof covering for 20 degree crank to form ridge","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["6.9.7","Extra over roof covering for 110 degrees bullnose to form 450mm radius at edge","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["6.9.8","Ridge capping 550mm girth","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["6.9.9","Hip capping 550mm girth","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["6.9.10","Side wall flashing 408mm girth","m",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["6.9.11","Head wall flashing 375mm girth","m",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["6.9.12","Counter flashing 185mm girth","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["6.9.13","Gable trim 580mm girth","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["6.9.14","Apex flashing 550mm girth","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["6.9.15","Corner trim 616mm girth","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["6.9.16","Apron flashing 375mm girth","m",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["6.9.17","Drip flashing 231mm girth","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["6.9.18","Sill flashing 185mm girth","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["6.9.19","Jamb flashing 308mm girth","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
[{"v":6.1,"d":"6.10"},"0,6mm \"Klip-lok 700\"  Z275 spelter galvanised ribbed sheet steel with \"Global-Sil\" finish on one side, in single lengths fixed to timber/steel purlins or rails and 0,58mm galvanised sheet steel accessories with \"Global-Sil\" finish on one side",null,null,0]
[{"$nulls":4},0]
["6.10.1","Roof covering with pitch not exceeding 50 degrees","m²",1,{"v":397.46585952000004,"d":"397.47"}]
[{"$nulls":4},0]
["6.10.2","Side cladding","m²",1,{"v":403.5995919200001,"d":"403.60"}]
[{"$nulls":4},0]
["6.10.3","Roof covering and side cladding to dormers, turrets, etc","m²",1,{"v":418.32054968000006,"d":"418.32"}]
[{"$nulls":4},0]
["6.10.4","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.10.5","Extra over roof covering for 20 degree crank to form ridge","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["6.10.6","Extra over roof covering for 110 degrees bullnose to form 450mm radius at edge","m",1,{"v":170.51776072,"d":"170.52"}]
[{"$nulls":4},0]
["6.10.7","Ridge capping 550mm girth","m",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["6.10.8","Hip capping 550mm girth","m",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["6.10.9","Side wall flashing 408mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.10.10","Head wall flashing 375mm girth","m",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["6.10.11","Counter flashing 185mm girth","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["6.10.12","Gable trim 580mm girth","m",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["6.10.13","Apex flashing 550mm girth","m",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["6.10.14","Corner trim 616mm girth","m",1,{"v":105.50019728000004,"d":"105.50"}]
[{"$nulls":4},0]
["6.10.15","Apron flashing 375mm girth","m",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["6.10.16","Drip flashing 231mm girth","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["6.10.17","Sill flashing 185mm girth","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["6.10.18","Jamb flashing 308mm girth","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
[null,"ROOF VENTILATORS",null,null,0]
[{"$nulls":4},0]
[6.11,"\"Everite\"",null,null,0]
[{"$nulls":4},0]
["6.11.1","\"Nutec Ventair Product No. 760-270\" fibre-cement ventilator fixed on soaker flange sheet (soaker flange sheet elsewhere) including sealing strips, fixing accessories, etc","m",1,{"v":3577.19273568,"d":"3,577.19"}]
[{"$nulls":4},0]
["6.11.1","\"Ventco Firelight MKIII\" galvanised sheet metal multi-purpose ventilator 2,15m long fixed through profile roof sheeting to steel purlins including flashings, closers, sealing strips, etc","no",1,0]
[{"$nulls":4},0]
["6.11.2","\"Ventco Firelight MKIII\" galvanised sheet metal, with \"Global-Sil\" finish on one side, multi-purpose ventilator 2,15m long fixed through profile roof sheeting to steel purlins including flashings, closers, sealing strips, etc","no",1,0]
[{"$nulls":4},0]
[null,"ROOF AND WALL INSULATION",null,null,0]
[{"$nulls":4},0]
[6.12,"\"Sisalation RSA 420\" heavy industrial grade aluminium foil based insulation",null,null,0]
[{"$nulls":4},0]
["6.12.1","Insulation laid taut over purlins (at approximately 1800mm centres) and fixed concurrent with roof covering including galvanised steel straining wires","m²",1,{"v":30.668662000000005,"d":"30.67"}]
[{"$nulls":4},0]
[6.13,"\"Sisalation RSA 410\" residential grade glass fibre reinforced aluminium foil bonded insulation",null,null,0]
[{"$nulls":4},0]
["6.13.1","Insulation laid taut over rafters (at approximately 1200mm centres) and fixed concurrent with tiling battens, purlins, etc","m²",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"SHEET METAL FLASHINGS, LININGS, COPINGS, ETC.",null,null,0]
[{"$nulls":4},0]
[6.14,"0,58mm. galvanised sheet iron ",null,null,0]
[{"$nulls":4},0]
["6.14.1","Flashings","m²",1,{"v":158.25029592000004,"d":"158.25"}]
[{"$nulls":4},0]
["6.14.2","Stepped cover flashings","m²",1,{"v":158.25029592000004,"d":"158.25"}]
[{"$nulls":4},0]
["6.14.3","Stepped cover flashings to roof pitches exceeding 50 degrees","m²",1,{"v":158.25029592000004,"d":"158.25"}]
[{"$nulls":4},0]
["6.14.4","Soakers","m²",1,{"v":158.25029592000004,"d":"158.25"}]
[{"$nulls":4},0]
["6.14.5","Lining to valleys with riveted and soldered joints","m²",1,{"v":158.25029592000004,"d":"158.25"}]
[{"$nulls":4},0]
["6.14.6","Lining to box gutters with riveted and soldered joints","m²",1,{"v":158.25029592000004,"d":"158.25"}]
[{"$nulls":4},0]
["6.14.7","Copings with riveted and soldered joints attached with suitable clips at 500mm centres along both edges, riveted to coping and plugged to brickwork or concrete","m²",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["6.14.8","Antguards","m²",1,{"v":133.71536632000002,"d":"133.72"}]
[{"$nulls":4},0]
["6.14.9","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
[6.15,"0,58mm. galvanised sheet iron with \"Global-Sil\" finish on one side",null,null,0]
[{"$nulls":4},0]
["6.15.1","Flashings","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.2","Stepped cover flashings","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.3","Stepped cover flashings to roof pitches exceeding 50 degrees","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.4","Soakers","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.5","Lining to valleys with riveted and soldered joints","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.6","Lining to box gutters with riveted and soldered joints","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.7","Copings with riveted and soldered joints attached with suitable clips at 500mm centres along both edges, riveted to coping and plugged to brickwork or concrete","m²",1,{"v":206.09340864000004,"d":"206.09"}]
[{"$nulls":4},0]
["6.15.8","Antguards","m²",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["6.15.9","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
[null,"SLATES",null,null,0]
[{"$nulls":4},0]
["6.16.","420 X 330mm \"Marley Eternit\" slates or equally approved laid in single thickness with a headlap of 90mm on underlay of bituminous roofing felt in accordance with SANS 92 Type 60 faced with 0.1mm aluminium foil over half its width with 150mm head laps and with tops of slates nailed with galvanised steel clout nails to and including 38 x 25mm sawn softwood battens at 450mm centres",null,null,0]
[{"$nulls":4},0]
["6.16.1","Roof covering with pitches not exceeding 25 degrees","m²",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
["6.16.2","Roof covering with pitches not exceeding 25 degrees, circular across the fall to ?m radius","m²",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
[null,"Roof covering circular along the fall not exceeding 6m radius",null,null,0]
[{"$nulls":4},0]
["6.16.3","Roof covering to conical shape with a 25 degree pitch and aradius varying from ?m to ?m, including cutting slates to wedge shape","m²",1,{"v":465.5502891600001,"d":"465.55"}]
[{"$nulls":4},0]
["6.16.4","Side cladding to gables etc","m²",1,{"v":465.5502891600001,"d":"465.55"}]
[{"$nulls":4},0]
["6.16.5","Side cladding to gables etc circular on plan to ?m radius","m²",1,{"v":465.5502891600001,"d":"465.55"}]
[{"$nulls":4},0]
["6.16.6","Soft cladding to eaves overhangs etc","m²",1,{"v":465.5502891600001,"d":"465.55"}]
[{"$nulls":4},0]
["6.16.7","Roof covering in side cladding to dormers, turrets, etc","m²",1,{"v":464.9369159200001,"d":"464.94"}]
[{"$nulls":4},0]
["6.16.8","Circular cutting","m",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["6.16.9","Extra on roof covering for double course at eaves including fixing clips and 38 x 38mm softwood tilting fillet","m",1,{"v":91.08592614,"d":"91.09"}]
[{"$nulls":4},0]
["6.16.10","Close cut and mitred ridge including soakers of bituminous roofing felt in accordance with SANS 92 Type 60 and necessary additional battens","m",1,{"v":120.71185363200003,"d":"120.71"}]
[{"$nulls":4},0]
["6.16.11","Close cut and mitred valley including soakers of bituminous roofing felt in accordance with SANS 92 Type 60 and necessary additional battens","m",1,{"v":120.71185363200003,"d":"120.71"}]
[{"$nulls":4},0]
["6.16.12","Close cut and mitred vertical angle including soakers of bituminous roofing felt in accordance with SANS 92 Type 60 and necessary additional battens","m",1,{"v":120.71185363200003,"d":"120.71"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
["6.16.13","Making good and sealing slate tiles and shingles to roof","m2",1,{"v":63.65194,"d":"63.65"}]
[{"$nulls":4},0]
[null,"RAINWATER DISPOSAL",null,null,0]
[{"$nulls":4},0]
["6.17.","0,6mm Galvanised sheet iron",null,null,0]
[{"$nulls":4},0]
["6.17.1","125mm Half round eaves gutter with beaded front edge including fixing brackets","m",1,{"v":109.18043672000002,"d":"109.18"}]
[{"$nulls":4},0]
["6.17.2","Extra over 125mm half round eaves gutter for stopped end","no",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["6.17.3","Extra over 125mm half round eaves gutter for angle","no",1,{"v":94.45947896000001,"d":"94.46"}]
[{"$nulls":4},0]
["6.17.4","Extra over 125mm half round eaves gutter for outlet for 76mm diameter pipe","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["6.17.5","76mm diameter rainwater pipes","m",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.17.6","Extra over 76mm diameter rainwater pipe for bend","no",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["6.17.7","Extra over 76mm diameter rainwater pipe for shoe","no",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["6.17.8","100 x 125mm eaves gutter with beaded front edge including fixing brackets","m",1,{"v":118.99440856000004,"d":"118.99"}]
[{"$nulls":4},0]
["6.17.9","Extra over 100 x 125mm eaves gutter for stopped end","no",1,{"v":68.69780288,"d":"68.70"}]
[{"$nulls":4},0]
["6.17.10","Extra over 100 x 125mm eaves gutter for angle","no",1,{"v":94.45947896000001,"d":"94.46"}]
[{"$nulls":4},0]
["6.17.11","Extra over 100 x 125mm eaves gutter for 100 x 76mm outlet  ","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["6.17.12","Extra over 76mm diameter rainwater pipe for outlet","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["6.17.13","100 x 76mm rainwater pipes","m",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["6.17.14","Extra over 100 x 76mm rainwater pipe for soldered bend","no",1,{"v":53.97684512000001,"d":"53.98"}]
[{"$nulls":4},0]
["6.17.15","Extra over 100 x 76mm rainwater pipe for soldered shoe","no",1,{"v":53.97684512000001,"d":"53.98"}]
[{"$nulls":4},0]
[6.18,"Extruded Seamless Aluminium",null,null,0]
[{"$nulls":4},0]
["6.18.1","125 x 85mm OGEE eaves gutter ","m",1,{"v":123.90139448000001,"d":"123.90"}]
[{"$nulls":4},0]
["6.18.2","125 x 85mm eaves gutter stopped end","no",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["6.18.3","125 x 85mm eaves gutter mitre corner","no",1,{"v":107.95369024000001,"d":"107.95"}]
[{"$nulls":4},0]
["6.18.4","75 x 50mm eaves gutter outlet  ","no",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["6.18.5","75 x 50mm fluted rainwater pipe","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["6.18.6","75 x 50mm crimped rainwater pipe bend","no",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.18.7","75 x 50mm crimped rainwater pipe shoe","no",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
["6.18.8","150 x 125mm OGEE eaves gutter ","m",1,{"v":134.94211280000002,"d":"134.94"}]
[{"$nulls":4},0]
["6.18.9","150 x 125mm eaves gutter stopped end","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["6.18.10","150 x 125mm eaves gutter mitre corner","no",1,{"v":107.95369024000001,"d":"107.95"}]
[{"$nulls":4},0]
["6.18.11","100 x 75mm eaves gutter outlet  ","no",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["6.18.12","100 x 75mm fluted rainwater pipe","m",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["6.18.13","100 x 75mm crimped rainwater pipe bend","no",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["6.18.14","100 x 75mm crimped rainwater pipe shoe","no",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
[null,"REPLACE DAMAGED GUTTERS AND DOWNPIPES",null,null,0]
[{"$nulls":4},0]
[null,"Carefully cut and remove gutter and / or down pipe in damaged section, replace with new including gutter brackets, pipe clips, making water tight at joints, prepare and paint to match existing and leave in good working order.",null,null,0]
[{"$nulls":4},0]
[6.19,"0,6mm Galvanised Sheet Iron",null,null,0]
[{"$nulls":4},0]
["6.19.1","125mm Half round eaves gutter with beaded front edge","m",1,{"v":112.86067616000003,"d":"112.86"}]
[{"$nulls":4},0]
["6.19.2","125mm half round eaves gutter stopped end","no",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["6.19.3","125mm half round eaves gutter angle","no",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["6.19.4","125mm half round eaves gutter outlet for 76mm diameter pipe","no",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.19.5","76mm diameter rainwater pipe","m",1,{"v":87.09900008000002,"d":"87.10"}]
[{"$nulls":4},0]
["6.19.6","76mm diameter rainwater pipe bend","no",1,{"v":53.97684512000001,"d":"53.98"}]
[{"$nulls":4},0]
["6.19.7","76mm diameter rainwater pipe shoe","no",1,{"v":53.97684512000001,"d":"53.98"}]
[{"$nulls":4},0]
["6.19.8","100 x 125mm eaves gutter with beaded front edge","m",1,{"v":122.67464800000002,"d":"122.67"}]
[{"$nulls":4},0]
["6.19.9","100 x 125mm eaves gutter stopped end","no",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["6.19.10","100 x 125mm eaves gutter angle","no",1,{"v":98.1397184,"d":"98.14"}]
[{"$nulls":4},0]
["6.19.11","100 x 76mm eaves gutter outlet  ","no",1,{"v":83.41876064,"d":"83.42"}]
[{"$nulls":4},0]
["6.19.12","100 x 76mm rainwater pipe","m",1,{"v":94.45947896000001,"d":"94.46"}]
[{"$nulls":4},0]
["6.19.13","100 x 76mm rainwater pipe soldered bend","no",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["6.19.14","100 x 76mm rainwater pipe soldered shoe","no",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["6.20.","Sundries",null,null,0]
[{"$nulls":4},0]
["6.20.1","Replace or install new gutter bracket and / or pipe clip","no",1,{"v":20.1554446664,"d":"20.16"}]
[{"$nulls":4},0]
["6.20.2","Repair leaking joint to Galvanised Iron gutter and / or down pipe not exceeding 500mm girth","no",1,{"v":30.055288760000007,"d":"30.06"}]
[{"$nulls":4},0]
["6.20.3","Repair leaking joint to Aluminium gutter and / or down pipe not exceeding 500mm girth","no",1,{"v":30.055288760000007,"d":"30.06"}]
[{"$nulls":4},0]
["6.20.4","Repair leaking joint to Galvanised Iron down pipe not exceeding 350mm diameter","no",1,{"v":30.055288760000007,"d":"30.06"}]
[{"$nulls":4},0]
["6.20.5","Replace or install new 80 or 100mm Full-bore cast iron outlet grating","no",1,{"v":1884.7487569424004,"d":"1,884.75"}]
[]
[]
[]
[]
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Carpentry and Joinery","index":6,"n_rows":707,"n_cols":7,"rows_kept":707,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 7"]
[]
[null,"CARPENTRY AND JOINERY"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Particle board"]
[]
[null,"Particle board shall comply with the following specifications:"]
[null,"a)  SABS 1300 Particle board: exterior and flooring type"]
[null,"b)  SABS 1301 Particle board: interior type"]
[]
[null,"Joinery"]
[]
[null,"Description of frames shall be deemed to include frames, transoms, mullions, rails, etc"]
[]
[null,"Description of hardwood joinery shall be deemed to include pelleting of bolt holes"]
[]
[null,"Fixings"]
[]
[null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or shot pins to brickwork or concrete."]
[]
[null,"Decorative laminated finish"]
[]
[null,"Laminated finish shall be glued under pressure.  Edge strips shall be butt jointed at junctions with adjacent similar finish"]
[]
[null,"ROOFS, ETC"]
[]
[null,"Prefabricated timber roof construction complete, including battens, runners, bracing, hips, valleys, cleats, etc., designed, supplied and fixed complete"]
[]
[7.1,"Flat roof construction for rectangular shaped"]
[]
["7.1.1","Flat roof construction for rectangular shaped building with a 400mm overhang projection on both sides","m²",{"v":1,"d":"1.00"},{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
[7.2,"Pitched roof construction for rectangular shaped",null,null,0]
[{"$nulls":4},0]
["7.2.1","Mono pitch roof trusses for rectangular shaped building with a pitch not exceeding 270 and a 500mm eaves overhang projection on one side, erected in position complete","no",{"v":1,"d":"1.00"},{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.2.2","Double pitch roof trusses for rectangular shaped building with a pitch not exceeding 270 and a 500mm eaves overhang projection on one side, erected in position complete","no",{"v":1,"d":"1.00"},{"v":408.3561278000001,"d":"408.36"}]
[{"$nulls":4},0]
[7.3,"Sawn softwood grade 4",null,null,0]
[{"$nulls":4},0]
["7.3.1","38 x 38mm Battens","m",1,{"v":22.70707734480001,"d":"22.71"}]
[{"$nulls":4},0]
["7.3.2","38 x 76mm Tilting battens","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["7.3.3","38 x 76mm wall plates","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["7.3.4","38 x 76mm wall plates bolted","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["7.3.5","50 x 76mm bracing","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["7.3.6","50 x 76mm hangers","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["7.3.7","50 x 75mm purlins","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["7.3.8","50 x 50mm trimmers","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["7.3.9","38 x 152mm sprockets","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["7.3.10","38 x 114mm Ceiling joists in lengths not exceeding 2,4m","m",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["7.3.11","50 x 152mm Ceiling joists in lengths exceeding 2,4m and not exceeding 3,9m","m",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["7.3.12","38 x 114mm Rafters in lengths not exceeding 2,4m","m",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["7.3.13","50 x 152mm Rafters in lengths exceeding 2,4m and not exceeding 3,9m","m",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["7.3.14","76 x 152mm Rafters in lengths exceeding 3,9m and not exceeding 6,6m","m",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["7.3.15","38 x 114mm Bearers in lengths not exceeding 2,4mm","m",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["7.3.16","50 x 152mm Bearers in lengths exceeding 2,4mm and not exceeding 3,9mm","m",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["7.3.17","76 x 152mm Bearers in lengths exceeding 3,9m and not exceeding 6,6m","m",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
[7.4,"Sawn softwood grade 6",null,null,0]
[{"$nulls":4},0]
["7.4.1","76 x 228mm Rafters in lengths exceeding 3,9m and not exceeding 6,6m","m",1,{"v":198.73292976000002,"d":"198.73"}]
[{"$nulls":4},0]
["7.4.2","76  x 228mm Rafters in lengths exceeding 6,6m","m",1,{"v":211.00039456000007,"d":"211.00"}]
[{"$nulls":4},0]
["7.4.3","76  x 228mm Bearers in lengths exceeding 3,9m and not exceeding 6,6m","m",1,{"v":198.73292976000002,"d":"198.73"}]
[{"$nulls":4},0]
["7.4.4","76  x 228mm Bearers in lengths exceeding 6,6m","m",1,{"v":211.00039456000007,"d":"211.00"}]
[{"$nulls":4},0]
[7.5,"Wrought softwood grade 6",null,null,0]
[{"$nulls":4},0]
["7.5.1","76 x 228mm Rafters in lengths exceeding 3,9m and not exceeding 6,6m","m",1,{"v":279.69819744000006,"d":"279.70"}]
[{"$nulls":4},0]
["7.5.2","76  x 228mm Rafters in lengths exceeding 6,6m","m",1,{"v":293.19240872,"d":"293.19"}]
[{"$nulls":4},0]
["7.5.3","76  x 228mm Bearers in lengths exceeding 3,9m and not exceeding 6,6m","m",1,{"v":279.69819744000006,"d":"279.70"}]
[{"$nulls":4},0]
["7.5.4","76  x 228mm Bearers in lengths exceeding 6,6m","m",1,{"v":293.19240872,"d":"293.19"}]
[{"$nulls":4},0]
[7.6,"Sundries",null,null,0]
[{"$nulls":4},0]
["7.6.1","Two coats creosote on sawn timbers","m²",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["7.6.2","2.5 mm diameter galvanised wire tie 2m girth wrapped around rafter and purlin with ends tied together","no",1,{"v":13.494211280000002,"d":"13.49"}]
[{"$nulls":4},0]
["7.6.3","30 x 1,6mm galvanised hoop iron roof tie 1500mm girth with each end fixed to timber","no",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["7.6.4","4.5mm Diameter galvanised wire tie 1500mm girth with one end fied to timber and other end built into brickwork","no",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
[null,"EAVES, VERGES, ETC",null,null,0]
[{"$nulls":4},0]
[7.7,"Sawn softwood",null,null,0]
[{"$nulls":4},0]
["7.7.1","38 x 38mm Branders ","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["7.7.2","38 x 114mm Bearers","m",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["7.7.3","38 x 114mm Hangers","m",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
[7.8,"Wrought softwood",null,null,0]
[{"$nulls":4},0]
["7.8.1","Eaves soffit covering of 25 x 38mm slates at 60mm centres including galvanised wire bird mesh backing","m²",1,{"v":431.81476096000006,"d":"431.81"}]
[{"$nulls":4},0]
["7.8.2","Verge soffit covering of 25 x 38mm slates at 60mm centres including galvanised wire bird mesh backing","m²",1,{"v":431.81476096000006,"d":"431.81"}]
[{"$nulls":4},0]
[7.9,"Wrought Meranti",null,null,0]
[{"$nulls":4},0]
["7.9.1","Eaves soffit covering of 22 x 96mm tounged and grooved boarding ","m²",1,{"v":385.5541511992001,"d":"385.55"}]
[{"$nulls":4},0]
["7.9.2","38 x 38mm Branders","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["7.9.3","38 x 114mm Bearers","m",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["7.9.4","38 x 114mm Hangers","m",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["7.9.5","38 x 38mm Branders wrought on one surface","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["7.9.6"," 19mm Quadrant beads","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["7.9.7","10 x 20mm Beads","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["7.9.8"," 32mm Half round cover strips","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["7.9.9","10 x 32mm Cover strips","m",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["7.9.10","22 x 144mm Fascias and barge boards","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
[{"v":7.1,"d":"7.10"},"\"Everite\" high density plain Pressed Nutec-cement",null,null,0]
[{"$nulls":4},0]
["7.10.1","Eaves soffit covering of 4mm thick sheets (branders elsewhere) with H-type pressed steel jointing strips","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["7.10.2","Eaves soffit covering of 4mm thick sheets with H-type pressed steel jointing strips including 38 x 38mm sawn softwood brandering along edges, along centre and at 400mm centres across sheets","m²",1,{"v":125.12814096000002,"d":"125.13"}]
[{"$nulls":4},0]
["7.10.3","12 x 225mm fascias and barge boards including galvanised steel H-profile jointing strips","m",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
[null,"FLOORS",null,null,0]
[{"$nulls":4},0]
[7.11,"Sawn Softwood",null,null,0]
[{"$nulls":4},0]
["7.11.1","38 x 76mm Battens wired to concrete (wire ties elsewhere)","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["7.11.2","50 x 150mm Floor joists in lengths not exceeding 2.4m","m",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["7.11.3","50 x 150mm Floor joists in lengths exceeding 2.4m and not exceeding 3.9m","m",1,{"v":100.47053671200003,"d":"100.47"}]
[{"$nulls":4},0]
["7.11.4","50 x 150mm Floor joists in lengths exceeding 3.9m and not exceeding 6.6m","m",1,{"v":130.61169772560004,"d":"130.61"}]
[{"$nulls":4},0]
["7.11.5","50 x 150mm Floor joists in lengths exceeding 6.6m","m",1,{"v":169.79398029680002,"d":"169.79"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["7.11.6","76 x 152mm Bearers in lengths exceeding 3.9m and not exceeding 6.6m","m",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["7.11.7","76 x 152mm Bearers in lengths exceeding 6.6m","m",1,{"v":143.52933816000004,"d":"143.53"}]
[{"$nulls":4},0]
[7.12,"Wrought Softwood",null,null,0]
[{"$nulls":4},0]
["7.12.1","Flooring of 22 x 96mm tounged and grooved boarding ","m²",1,{"v":385.5541511992001,"d":"385.55"}]
[{"$nulls":4},0]
["7.12.2","Raking cutting","m",1,{"v":15.223923816800003,"d":"15.22"}]
[{"$nulls":4},0]
["7.12.3","Circular cutting","m",1,{"v":15.223923816800003,"d":"15.22"}]
[{"$nulls":4},0]
["7.12.4","22 x 170mm Risers with rebated top edge let into and including groove in treads","m",1,{"v":72.13269302400002,"d":"72.13"}]
[{"$nulls":4},0]
["7.12.5","22 x 300mm Treads with rounded front edge","m",1,{"v":127.36081955360002,"d":"127.36"}]
[{"$nulls":4},0]
[7.13,"Wire ties",null,null,0]
[{"$nulls":4},0]
["7.13.1","4mm Diameter galvanised wire tie 450mm girth bent double, embedded in concrete, bound around floor batten and twisted together including saw cuts","no",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
[null,"SKIRTINGS",null,null,0]
[{"$nulls":4},0]
[7.14,"Wrought Softwood",null,null,0]
[{"$nulls":4},0]
["7.14.1","19 x 70mm. skirting nailed","m",1,{"v":26.988422560000004,"d":"26.99"}]
[{"$nulls":4},0]
["7.14.2","19 x 70mm. skirting plugged","m",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["7.14.3","19 x 70mm. skirting stepped over treads and risers nailed","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["7.14.4","19 x 70mm. skirting stepped over treads and risers plugged","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["7.14.5","22 x 94mm. skirting nailed","m",1,{"v":33.12215496,"d":"33.12"}]
[{"$nulls":4},0]
["7.14.6","22 x 94mm. skirting plugged","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["7.14.7","19mm. quadrant bead nailed","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["7.14.8","32mm. quadrant bead nailed","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["7.14.9","19mm  Raking skirting 230mm high extreme with bottom edge stepped over treads and risers nailed","m",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["7.14.10","19mm  Raking skirting 230mm high extreme with bottom edge stepped over treads and risers plugged","m",1,{"v":52.75009864000002,"d":"52.75"}]
[{"$nulls":4},0]
[7.15,"Wrought Meranti",null,null,0]
[{"$nulls":4},0]
["7.15.1","19 x 70mm. skirting nailed","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["7.15.2","19 x 70mm. skirting plugged","m",1,{"v":44.162873280000014,"d":"44.16"}]
[{"$nulls":4},0]
["7.15.3","19 x 70mm. skirting stepped over treads and risers nailed","m",1,{"v":50.296605680000006,"d":"50.30"}]
[{"$nulls":4},0]
["7.15.4","19 x 70mm. skirting stepped over treads and risers plugged","m",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
["7.15.5","22 x 94mm. skirting nailed","m",1,{"v":53.97684512000001,"d":"53.98"}]
[{"$nulls":4},0]
["7.15.6","22 x 94mm. skirting plugged","m",1,{"v":56.43033808000001,"d":"56.43"}]
[{"$nulls":4},0]
["7.15.7","19mm. quadrant bead nailed","m",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
["7.15.8","32mm. quadrant bead nailed","m",1,{"v":33.12215496,"d":"33.12"}]
[{"$nulls":4},0]
["7.15.9","19mm  Raking skirting 230mm high extreme with bottom edge stepped over treads and risers nailed","m",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["7.15.10","19mm Raking skirting 230mm high extreme with bottom edge stepped over treads and risers plugged","m",1,{"v":94.45947896000001,"d":"94.46"}]
[{"$nulls":4},0]
[null,"HERITAGE SKIRTING AND ARCHITRAVES - \"Making good, patching, straightning and sealing of existing skirting to Heritage Buildings\" (Paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["7.15.11","70mm Skirting / Architraves / Dado Rails","m",1,{"v":57.86540000000001,"d":"57.87"}]
[{"$nulls":4},0]
["7.15.12","115mm Skirting / Architraves / Dado Rails","m",1,{"v":72.33175,"d":"72.33"}]
[{"$nulls":4},0]
["7.15.13","150mm Skirting / Architraves / Dado Rails","m",1,{"v":90.4146875,"d":"90.41"}]
[{"$nulls":4},0]
["7.15.14","170mm Skirting / Architraves / Dado Rails","m",1,{"v":113.018359375,"d":"113.02"}]
[{"$nulls":4},0]
["7.15.15","225mm Skirting / Architraves / Dado Rails","m",1,{"v":141.27294921875,"d":"141.27"}]
[{"$nulls":4},0]
[null,"DOORS, ETC",null,null,0]
[{"$nulls":4},0]
[7.16,"Wrought Meranti doors hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.16.1","44mm Framed batten door 900 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":1355.5548604000003,"d":"1,355.55"}]
[{"$nulls":4},0]
["7.16.2","44mm Framed batten door 813 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":1192.3975785600003,"d":"1,192.40"}]
[{"$nulls":4},0]
["7.16.3","44mm Framed batten door 813 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 150mm middle ledge and 44 x 225mm bottom ledge filled in with 22mm V-jointed one side boarding","no",1,{"v":1355.5548604000003,"d":"1,355.55"}]
[{"$nulls":4},0]
["7.16.4","44mm Framed batten door 813 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 150mm middle ledge and 44 x 225mm bottom ledge filled in with 22mm V-jointed one side boarding and 3mm sheet metal fixed to other side","no",1,{"v":1748.1137340000002,"d":"1,748.11"}]
[{"$nulls":4},0]
["7.16.5","44mm Framed batten door 762 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":1192.3975785600003,"d":"1,192.40"}]
[{"$nulls":4},0]
["7.16.6","44mm Framed batten double door 1616 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 150mm middle ledge and 44 x 225mm bottom ledge filled in with 22mm V-jointed one side boarding","no",1,{"v":2711.1097208000006,"d":"2,711.11"}]
[{"$nulls":4},0]
["7.16.7","44mm Double leaf framed batten door 1510 x 2032mm high of 44 x 100mm top rail, stiles and rebated meeting stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":2351.6730021600006,"d":"2,351.67"}]
[{"$nulls":4},0]
[null,"\"Swartland\"",null,null,0]
[{"$nulls":4},0]
["7.16.8","44mm \"Kayo 8\" Panel door 813 x 2032mm high ","no",1,{"v":1594.7704240000003,"d":"1,594.77"}]
[{"$nulls":4},0]
["7.16.9","44mm \"Kayo 8\" Panel rebated double door 1626 x 2032mm high ","no",1,{"v":3189.5408480000006,"d":"3,189.54"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[7.17,"Semi-solid flush door with 3,2mm. hardboard covering on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.17.1","40mm Door 900 x 2032mm. high ","no",1,{"v":463.71016944,"d":"463.71"}]
[{"$nulls":4},0]
["7.17.2","40mm Door 813 x 2032mm. high ","no",1,{"v":414.6403102400001,"d":"414.64"}]
[{"$nulls":4},0]
["7.17.3","40mm Door 762 x 2032mm. high ","no",1,{"v":414.6403102400001,"d":"414.64"}]
[{"$nulls":4},0]
["7.17.4","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":774.0770288800001,"d":"774.08"}]
[{"$nulls":4},0]
["7.17.5","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":774.0770288800001,"d":"774.08"}]
[{"$nulls":4},0]
["7.17.6","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":740.9548739200002,"d":"740.95"}]
[{"$nulls":4},0]
["7.17.7","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":774.0770288800001,"d":"774.08"}]
[{"$nulls":4},0]
["7.17.8","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":774.0770288800001,"d":"774.08"}]
[{"$nulls":4},0]
["7.17.9","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":740.9548739200002,"d":"740.95"}]
[{"$nulls":4},0]
["7.17.10","Extra for 300 x 450mm opening including natural anodised aluminium louvre unit","no",1,{"v":669.8035780800001,"d":"669.80"}]
[{"$nulls":4},0]
[7.18,"Semi-solid flush door with sapele veneer on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.18.1","40mm Door 900 x 2032mm. high ","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
["7.18.2","40mm Door 813 x 2032mm. high ","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
["7.18.3","40mm Door 762 x 2032mm. high ","no",1,{"v":669.8035780800002,"d":"669.80"}]
[{"$nulls":4},0]
["7.18.4","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":847.6818176800001,"d":"847.68"}]
[{"$nulls":4},0]
["7.18.5","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":847.6818176800001,"d":"847.68"}]
[{"$nulls":4},0]
["7.18.6","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":810.8794232800002,"d":"810.88"}]
[{"$nulls":4},0]
["7.18.7","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":847.6818176800001,"d":"847.68"}]
[{"$nulls":4},0]
["7.18.8","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":847.6818176800001,"d":"847.68"}]
[{"$nulls":4},0]
["7.18.9","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":810.8794232800002,"d":"810.88"}]
[{"$nulls":4},0]
["7.18.10","Extra for 300 x 450mm opening including natural anodised aluminium louvre unit","no",1,{"v":669.8035780800001,"d":"669.80"}]
[{"$nulls":4},0]
[7.19,"Solid flush door with 3,2mm. hardboard covering on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.19.1","40mm Door 900 x 2032mm. high ","no",1,{"v":840.4440134480001,"d":"840.44"}]
[{"$nulls":4},0]
["7.19.2","40mm Door 813 x 2032mm. high ","no",1,{"v":840.4440134480001,"d":"840.44"}]
[{"$nulls":4},0]
["7.19.3","40mm Door 762 x 2032mm. high ","no",1,{"v":840.4440134480001,"d":"840.44"}]
[{"$nulls":4},0]
["7.19.4","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":1424.1299886320003,"d":"1,424.13"}]
[{"$nulls":4},0]
["7.19.5","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":1424.1299886320003,"d":"1,424.13"}]
[{"$nulls":4},0]
["7.19.6","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":1376.2868759120001,"d":"1,376.29"}]
[{"$nulls":4},0]
["7.19.7","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":1424.1299886320003,"d":"1,424.13"}]
[{"$nulls":4},0]
["7.19.8","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":1424.1299886320003,"d":"1,424.13"}]
[{"$nulls":4},0]
["7.19.9","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":1376.2868759120001,"d":"1,376.29"}]
[{"$nulls":4},0]
["7.19.10","Extra for 300 x 450mm opening including natural anodised aluminium louvre unit","no",1,{"v":870.7446515040001,"d":"870.74"}]
[{"$nulls":4},0]
[{"v":7.2,"d":"7.20"},"Solid flush door with sapele veneer on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.20.1","40mm Door 900 x 2032mm. high ","no",1,{"v":918.5877642240001,"d":"918.59"}]
[{"$nulls":4},0]
["7.20.2","40mm Door 813 x 2032mm. high ","no",1,{"v":816.5224570880001,"d":"816.52"}]
[{"$nulls":4},0]
["7.20.3","40mm Door 762 x 2032mm. high ","no",1,{"v":816.5224570880001,"d":"816.52"}]
[{"$nulls":4},0]
["7.20.4","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":1564.4697859440003,"d":"1,564.47"}]
[{"$nulls":4},0]
["7.20.5","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":1564.4697859440003,"d":"1,564.47"}]
[{"$nulls":4},0]
["7.20.6","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":1510.2475915280004,"d":"1,510.25"}]
[{"$nulls":4},0]
["7.20.7","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":1564.4697859440003,"d":"1,564.47"}]
[{"$nulls":4},0]
["7.20.8","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":1564.4697859440003,"d":"1,564.47"}]
[{"$nulls":4},0]
["7.20.9","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":1510.2475915280004,"d":"1,510.25"}]
[{"$nulls":4},0]
["7.20.10","Extra for 300 x 450mm opening including natural anodised aluminium louvre unit","no",1,{"v":669.8035780800001,"d":"669.80"}]
[{"$nulls":4},0]
[null,"JOINERY SUNDRIES",null,null,0]
[{"$nulls":4},0]
[7.21,"Wrought Meranti or Softwood",null,null,0]
[{"$nulls":4},0]
["7.21.1","Slatted shelving, seats, etc of 22 x 96mm slats at 35mm centres","m²",1,{"v":385.5541511992001,"d":"385.55"}]
[{"$nulls":4},0]
["7.21.2","Install 813 x 2032mm timber door including furniture (door handle)","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["7.21.3","Install  door furniture (door handle)","no",1,{"v":118.38103532000002,"d":"118.38"}]
[{"$nulls":4},0]
[null,"Making good of existing doors (Patching and repairing where necessary, paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
[null,"Wrought Meranti doors hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.21.4","44mm Framed batten door 900 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
["7.21.5","44mm Framed batten door 813 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
["7.21.6","44mm Framed batten door 813 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 150mm middle ledge and 44 x 225mm bottom ledge filled in with 22mm V-jointed one side boarding","no",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
["7.21.7","44mm Framed batten door 813 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 150mm middle ledge and 44 x 225mm bottom ledge filled in with 22mm V-jointed one side boarding and 3mm sheet metal fixed to other side","no",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
["7.21.8","44mm Framed batten door 762 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
["7.21.9","44mm Framed batten double door 1616 x 2032mm high of 44 x 100mm top rail and stiles, 44 x 150mm middle ledge and 44 x 225mm bottom ledge filled in with 22mm V-jointed one side boarding","no",1,{"v":846.4550712000002,"d":"846.46"}]
[{"$nulls":4},0]
["7.21.10","44mm Double leaf framed batten door 1510 x 2032mm high of 44 x 100mm top rail, stiles and rebated meeting stiles, 44 x 100mm middle ledge and braces and 44 x 100mm bottom rail filled in with 70mm V-jointed one side boarding and covered on other side with 3,2mm plywood with veneer to match door let into and including rebates all round","no",1,{"v":846.4550712000002,"d":"846.46"}]
[{"$nulls":4},0]
[null,"ONLY IN HERITAGE BUILDINGS \"Making good of existing doors (Patching and repairing where necessary, paintwork elsewhere)\"",null,null,0]
[{"$nulls":4},0]
[null,"Wooden Heritage doors hung to wooden frames",null,null,0]
[{"$nulls":4},0]
["7.21.10a"," 762 x 2032mm high Single door","no",1,{"v":1058.068839,"d":"1,058.07"}]
[{"$nulls":4},0]
["7.21.10b","813 x 2032mm high Single door","no",1,{"v":1058.068839,"d":"1,058.07"}]
[{"$nulls":4},0]
["7.21.10c"," 900 x 2032mm high Single door","no",1,{"v":1058.068839,"d":"1,058.07"}]
[{"$nulls":4},0]
["7.21.10d"," 1200 x 2032mm high Single door","no",1,{"v":1100.3915925600004,"d":"1,100.39"}]
[{"$nulls":4},0]
["7.21.10e"," 1510 x 2032mm high Double door","no",1,{"v":1692.9101424,"d":"1,692.91"}]
[{"$nulls":4},0]
["7.21.10f"," 1616 x 2032mm high Double door","no",1,{"v":2116.137678,"d":"2,116.14"}]
[{"$nulls":4},0]
["7.21.10g"," 1810 x 2032mm high Double door","no",1,{"v":2370.07419936,"d":"2,370.07"}]
[{"$nulls":4},0]
[null,"\"Swartland\"",null,null,0]
[{"$nulls":4},0]
["7.21.11","44mm \"Kayo 8\" Panel door 813 x 2032mm high ","no",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
[null,"Making good of Semi-solid flush door with 3,2mm. hardboard covering on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.21.12","40mm Door 900 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.13","40mm Door 813 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.14","40mm Door 762 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.15","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.16","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.17","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.18","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.19","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.20","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
[null,"Making good of Semi-solid flush door with sapele veneer on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.21.21","40mm Door 900 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.22","40mm Door 813 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.23","40mm Door 762 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.24","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.25","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.26","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.27","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.28","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.29","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"Making good of Solid flush door with 3,2mm. hardboard covering on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.21.30","40mm Door 900 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.31","40mm Door 813 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.32","40mm Door 762 x 2032mm. high ","no",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["7.21.33","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.34","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.35","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.36","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.37","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["7.21.38","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"Making good of Solid flush door with sapele veneer on both sides hung to steel frames",null,null,0]
[{"$nulls":4},0]
["7.21.40","40mm Door 900 x 2032mm. high ","no",1,{"v":156.23658000000003,"d":"156.24"}]
[{"$nulls":4},0]
["7.21.41","40mm Door 813 x 2032mm. high ","no",1,{"v":156.23658000000003,"d":"156.24"}]
[{"$nulls":4},0]
["7.21.42","40mm Door 762 x 2032mm. high ","no",1,{"v":156.23658000000003,"d":"156.24"}]
[{"$nulls":4},0]
["7.21.43","40mm Double leaf door 1511 x 2032mm. high with rebated meeting styles","no",1,{"v":312.47316000000006,"d":"312.47"}]
[{"$nulls":4},0]
["7.21.44","40mm Double leaf door 1613 x 2032mm. high with rebated meeting styles","no",1,{"v":312.47316000000006,"d":"312.47"}]
[{"$nulls":4},0]
["7.21.45","40mm Double leaf door 1359 x 2032mm. high with rebated meeting styles","no",1,{"v":312.47316000000006,"d":"312.47"}]
[{"$nulls":4},0]
["7.21.46","40mm Double leaf door 1616 x 2032mm. high with flush meeting styles","no",1,{"v":312.47316000000006,"d":"312.47"}]
[{"$nulls":4},0]
["7.21.47","40mm Double leaf door 1511 x 2032mm. high with flush meeting styles","no",1,{"v":312.47316000000006,"d":"312.47"}]
[{"$nulls":4},0]
["7.21.48","40mm Double leaf door 1359 x 2032mm. high with flush meeting styles","no",1,{"v":312.47316000000006,"d":"312.47"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"FITTINGS",null,null,0]
[{"$nulls":4},0]
[null,"General",null,null,0]
[{"$nulls":4},0]
[null,"The following cupboards fittings have been measured as complete units i.e. the components of the units have not been separately measured.  The descriptions, therefore, of such units shall be ",null,null,0]
[null,"deemed to include all components, assembling, housing, notching, glueing, blocking, planting on and screwing with countersunk screws, edge strips, decorative plastic finish, glass, ironmongery, metalwork, paint or varnish finishes, etc",null,null,0]
[{"$nulls":4},0]
[7.22,"Kitchen cupboards etc with approved hinges, handles and telescopic drawer sliders",null,null,0]
[{"$nulls":4},0]
["7.22.1","Wall cupboard Type W300 - 300 x 300 x 720mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":496.485132,"d":"496.49"}]
[{"$nulls":4},0]
["7.22.2","Wall cupboard Type W450 - 450 x 300 x 720mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":607.5867000000001,"d":"607.59"}]
[{"$nulls":4},0]
["7.22.3","Wall cupboard Type W600 - 600 x 300 x 720mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":722.1601920000002,"d":"722.16"}]
[{"$nulls":4},0]
["7.22.4","Wall cupboard Type W750 - 750 x 300 x 720mm high with top, sides, bottom, division, shelf, back and double hinged door","no",1,{"v":827.4752200000001,"d":"827.48"}]
[{"$nulls":4},0]
["7.22.5","Wall cupboard Type W900 - 900 x 300 x 720mm high with top, sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":1006.8579600000002,"d":"1,006.86"}]
[{"$nulls":4},0]
["7.22.6","Wall cupboard Type W1200 - 1200 x 300 x 720mm high with top, sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":1295.027652,"d":"1,295.03"}]
[{"$nulls":4},0]
["7.22.7","Wall cupboard Type WCU600 (L shaped) - 600 x 300 x 720mm high with top, sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":945.5206360000001,"d":"945.52"}]
[{"$nulls":4},0]
["7.22.8","Wall cupboard Type WC300 (End display) - 300 x 300 x 720mm high with top, sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":496.485132,"d":"496.49"}]
[{"$nulls":4},0]
["7.22.9","Floor cupboard Type F300 - (without top) - 300 x 550 x 880mm high with sides, bottom, division, shelf, and single hinged door","no",1,{"v":737.2051960000001,"d":"737.21"}]
[{"$nulls":4},0]
["7.22.10","Floor cupboard Type F450 - (without top) - 450 x 550 x 880mm high with sides, bottom, division, shelf, and single hinged door","no",1,{"v":883.0260040000001,"d":"883.03"}]
[{"$nulls":4},0]
["7.22.11","Floor cupboard Type F600 - (without top) - 600 x 550 x 880mm high with sides, bottom, division, shelf, and single hinged door","no",1,{"v":1040.4198920000001,"d":"1,040.42"}]
[{"$nulls":4},0]
["7.22.12","Floor cupboard Type F750 - (without top) - 750 x 550 x 880mm high with sides, bottom, division, shelf, and double hinged doors","no",1,{"v":1254.5218720000003,"d":"1,254.52"}]
[{"$nulls":4},0]
["7.22.13","Floor cupboard Type F900 - (without top) - 900 x 550 x 880mm high with sides, bottom, division, shelf, and double hinged doors","no",1,{"v":1395.7134480000002,"d":"1,395.71"}]
[{"$nulls":4},0]
["7.22.14","Floor cupboard Type F1200 - (without top) - 1200 x 550 x 880mm high with sides, bottom, division, shelf, and double hinged doors","no",1,{"v":1702.4000680000004,"d":"1,702.40"}]
[{"$nulls":4},0]
["7.22.15","Floor cupboard Type F450/1 - (without top) - 450 x 550 x 880mm high with sides, bottom, division, shelf, and single hinged door, dividing framework and 1 drawer","no",1,{"v":970.9814120000002,"d":"970.98"}]
[{"$nulls":4},0]
["7.22.16","Floor cupboard Type F450/4 - (without top) - 450 x 550 x 880mm high with sides, bottom,  dividing framework and 4 drawers","no",1,{"v":1197.81378,"d":"1,197.81"}]
[{"$nulls":4},0]
["7.22.17","Floor cupboard Type F600/1 - (without top) - 600 x 550 x 880mm high with sides, bottom, division, shelf, and single hinged door, dividing framework and 1 drawer","no",1,{"v":1126.060684,"d":"1,126.06"}]
[{"$nulls":4},0]
["7.22.18","Floor cupboard Type F600/4 - (without top) - 600 x 550 x 880mm high with sides, bottom,  dividing framework and 4 drawers","no",1,{"v":1634.1188960000002,"d":"1,634.12"}]
[{"$nulls":4},0]
["7.22.19","Floor cupboard Type FCU900 (L shaped) - 900 x 300 x 880mm high with sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":2007.9293800000003,"d":"2,007.93"}]
[{"$nulls":4},0]
["7.22.20","Floor cupboard Type BC450 - 450 x 300 x 2095mm high with top, sides, bottom, division, 2 shelves, back and single hinged door","no",1,{"v":1930.389744,"d":"1,930.39"}]
[{"$nulls":4},0]
["7.22.21","Floor cupboard Type GC600 - 600 x 300 x 2095mm high with top, sides, bottom, division, 4 shelves, back and single hinged door","no",1,{"v":2445.391804,"d":"2,445.39"}]
[{"$nulls":4},0]
["7.22.22","Sink cupboard Type S900 - 900 x 550 x 880mm high with sides, bottom, division, shelf, back and double hinged doors (sink elsewhere)","no",1,{"v":1395.7134480000002,"d":"1,395.71"}]
[{"$nulls":4},0]
["7.22.23","Sink cupboard Type S1200 - 1200 x 550 x 880mm high with sides, bottom, division, shelf, back and double hinged doors (sink elsewhere)","no",1,{"v":1702.4000680000004,"d":"1,702.40"}]
[{"$nulls":4},0]
["7.22.24","Sink cupboard Type S1500 (double bowl) - 1500 x 550 x 880mm high with sides, bottom, division, shelf, back and double hinged doors (sink elsewhere)","no",1,{"v":2128.289412,"d":"2,128.29"}]
[{"$nulls":4},0]
[7.23,"32mm thick post formed (on one side) top with 0,6mm Decon Laminated in Artic Granite or similar",null,null,0]
[{"$nulls":4},0]
["7.23.1","600mm wide","m",1,{"v":266.18084000000005,"d":"266.18"}]
[{"$nulls":4},0]
["7.23.2","900mm wide","m",1,{"v":372.6531760000001,"d":"372.65"}]
[{"$nulls":4},0]
["7.23.3","Extra over for edge strip","m",1,{"v":10.415772,"d":"10.42"}]
[{"$nulls":4},0]
["7.23.4","Extra over for splay cutting","m",1,{"v":6.943848,"d":"6.94"}]
[{"$nulls":4},0]
[7.24,"Laminated Pine",null,null,0]
[{"$nulls":4},0]
["7.24.1","46 x 231mm Beam","m",1,{"v":131.21558104000002,"d":"131.22"}]
[{"$nulls":4},0]
["7.24.2","46 x 297mm Beam","m",1,{"v":168.71236024000004,"d":"168.71"}]
[{"$nulls":4},0]
["7.24.3","70 x 147mm Beam","m",1,{"v":127.0724184,"d":"127.07"}]
[{"$nulls":4},0]
["7.24.4","70 x 231mm Beam","m",1,{"v":199.68192231999998,"d":"199.68"}]
[{"$nulls":4},0]
["7.24.5","70 x 297mm Beam","m",1,{"v":256.7372067200001,"d":"256.74"}]
[{"$nulls":4},0]
["7.24.6","70 x 363mm Beam","m",1,{"v":313.78091803999996,"d":"313.78"}]
[{"$nulls":4},0]
[7.25,"Service Counters",null,null,0]
[{"$nulls":4},0]
["7.25.1","Plumtree melamine, Alpine finish, Size 750 x 1000mm high, in high impact PVC edged all round 32mm worktop including 2 x 2door lockable cupboards with two open spaces for chairs and cable outlets, 3 x open shelves, 2 x rounded corner unitt with min 3 x open front display shelves","no",1,{"v":3254.813019200001,"d":"3,254.81"}]
[{"$nulls":4},0]
["7.25.2","Four Tier open bag storage unit 450 x 1832 x 450mm deep (4 x pigeon holes per unit)","no",1,{"v":2018.5766136000002,"d":"2,018.58"}]
[{"$nulls":4},0]
["7.25.3","Library shelving unit 900 x 1200 x 300mm deep with adjustable shelves, 22mm \"Plumtree\" melamine","no",1,{"v":2265.4304100000004,"d":"2,265.43"}]
[{"$nulls":4},0]
["7.25.4","Adult - Computer/study bay 800 x 750 x 300mm deep with enclosed sides 800mm high with cable outlets","no",1,{"v":2151.3777066000007,"d":"2,151.38"}]
[{"$nulls":4},0]
["7.25.5","Water treated solid wood platform of 100 x 50mm continuous top and bottom rails, 100 x 100mm intermediate post at approximately 1200mm centres, 100 x 100mm cross-bracing, 100 x 30mm flat section floor slats, all bolted together with 100 x 10mm diameter stainless steel bolts","m2",1,{"v":3437.2047600000005,"d":"3,437.20"}]
[{"$nulls":4},0]
[7.26,"CUBICLES AND SHELVES",null,null,0]
[{"$nulls":4},0]
[null,"COJ cubicles",null,null,0]
[{"$nulls":4},0]
["7.26.1","Manufacture, supply and install: Interview Cubicles with 32mm thick Melamine wood grain \"Vancouver Maple\" or other colour board with 32 mm work-tops, vanity, tripple drawer units and edged all around in black hi-impact edging to suit. All new counters to include for plant-on black squares detail, counter holes for cables, two down lights, alluminium skirting as per drawing. (2.7m high x 1.4m wide). ","no",1,{"v":35979.195433060006,"d":"35,979.20"}]
[{"$nulls":4},0]
["7.26.2","Manufacture, supply and install new 2400 wide reception counter in 16mm thick Melamine wood grain \"Vancouver Maple\" or other colour melamine base unit, 32 mm work surface edged with 3 mm hi-impact polyurethane edging and includes for a single 3 drawer pedestal unit for storage, Maple vanity front and 10 mm tempered glass upper split level shelf top section on stainless steel posts.","no",1,{"v":17359.620000000003,"d":"17,359.62"}]
[{"$nulls":4},0]
["7.26.3","Manufacture, supply and install: 32mm thick Melamine wood grain door 813 x 2032mm. high for staff entrance plus 32mm panel around door 2700 high x 2000mm wide. Complete with hinges","no",1,{"v":3124.7316,"d":"3,124.73"}]
[{"$nulls":4},0]
["7.26.4","Manufacture, supply and install: 16mm thick Melamine wood grain tender box 500x500x12000mm with 32mm similar top. Complete with hinges, lock, pad lock with 450mm COJ Brushed Alluminium  logo and 100x450 \"Name logo's\" ","no",1,{"v":3457.4576500000003,"d":"3,457.46"}]
[{"$nulls":4},0]
[null,"Libraries shelves",null,null,0]
[{"$nulls":4},0]
["7.26.5","Elephant folio shelving 2000 x 900 x 650d fixed to the floor, 120mm spacing between shelves, in Mahogany. 2 - A.1.1.f.y shelving units 1800w x 1800h x 300d Addendum B Mahogany is adapted to manufacture these fixed Elephant folio shelving units.","no",1,{"v":7625.295832522,"d":"7,625.30"}]
[{"$nulls":4},0]
["7.26.6","Catalogue card storage boxes unit 1300 x 1870 x 370d fixed to the floor, 103mm spacing between shelves. 1 - A.1.1.f.y shelving unit 1800w x 1800h x 300d Addendum B Mahogany is adapted to manufacture this fixed storage unit.","no",1,{"v":7625.295832522,"d":"7,625.30"}]
[{"$nulls":4},0]
["7.26.7","10 - Drawer AO size map/plan filing cabinets, fixed to the floor, each unit includes the following: 1x 4 drawer metal unit, 1420w x 530h x 960d fixed on top of 1 x 6 drawer metal unit, 1420w x 740h x 960d and 1x  universal metal stand, all of the above cladded with Beech wood melamine, to match the existing furniture, total height per unit: 1520mm. ","no",1,{"v":36961.871442400006,"d":"36,961.87"}]
[{"$nulls":4},0]
["7.26.8","Single wall units 954w x 2000h x 466d, fixed to the floor fitted with 12x fixed shelves each, with 138mm(h) gaps between shelves, in Mahogany.13 - B.1.1.f.y Shelving units 1800 x 1500 x 300 Addendum B is adapted to manufacture these multi-shelf fixed units. (Equal angle colour matching aluminium is used to fix the shelving units to the floor.)","no",1,{"v":6367.64459969,"d":"6,367.64"}]
[{"$nulls":4},0]
["7.26.9","Single wall units 900 x 2000 x 300 fixed to the floor fitted with 4x adjustable shelves each, in Beechwood. 6 - A.1.1.c.y - Shelving units 900 x 1800 x 300 Addendum B Beechwood, is adapted to manufacture these fixed shelving units. (6x shelving units fixed behind the counter) (Equal angle colour matching aluminium is used to fix the shelving units to the floor.)","no",1,{"v":4249.377474970001,"d":"4,249.38"}]
[{"$nulls":4},0]
["7.26.10"," Counter 1500w x 750h x 500d single level, granite top 1500 x 500mm, Steel construction design to match the existing counters, 10mm clear polished glass paneling fitted with the vinylle logo as per existing units single level Rustenburg (colour) granite 1 - 1500 x 500 x 30mm, counter fixed to the floor.","no",1,{"v":11384.554526799999,"d":"11,384.55"}]
[{"$nulls":4},0]
["7.26.11","Double island units 1800 x 1500 x 660 fixed to the floor fitted with 8x lockable glass doors each, in Mahogany. 10 - B.1.2.c.y Shelving units 2700 x 1400 x 600. Addendum B Mahogany, is adapted to manufacture these fixed lockable shelving units.","no",1,{"v":15419.656425570001,"d":"15,419.66"}]
[{"$nulls":4},0]
["7.26.12","Double island units 900 x 1500 x 660 fixed to the floor fitted with 4x lockable glass doors each, in Mahogany. 10 - B.1.1.j.y Shelving units 2700 x 1500 x 300 Addendum B Mahogany, is adapted to manufacture these fixed lockable shelving units. (10 Rows of 2700mm(w) lockable shelving units)(Equal angle colour matching aluminium is used to the shelving units to the floor)fix ","no",1,{"v":9052.01182588,"d":"9,052.01"}]
[{"$nulls":4},0]
["7.26.13","Single wall units 450w x 2500h x 450d, fixed to the floor fitted with 10x fixed shelves each, with 450mm(h) gaps between shelves, in Melamine wood colour to match existing furniture. with 2mm PVC edging. (Equal angle colour matching aluminium is used to fix the shelving units to the floor.)","no",1,{"v":5287.647667360001,"d":"5,287.65"}]
[{"$nulls":4},0]
["7.26.14","Drawing pigeon hole 450w X 1100h X 800b, fixed to the floor in 16mm Melamine wood colour to match existing furniture","no",1,{"v":1180.4541600000002,"d":"1,180.45"}]
[{"$nulls":4},0]
[null,"ROLL-UP, RETRACTABLE SCREENS AND BLINDS",null,null,0]
[{"$nulls":4},0]
[7.27,"\"Windovert\" or equivalent blinds",null,null,0]
[{"$nulls":4},0]
[null,"Supply and install complete with colour co-ordinated ladder lace, cord, head and bottom rails, tilters, cord locks and installation brackets",null,null,0]
[{"$nulls":4},0]
["7.27.1","25mm Plain slatted venetian wooden window ","m2",1,{"v":565.923612,"d":"565.92"}]
[{"$nulls":4},0]
["7.27.2","25mm Perforated venetian wooden window blinds","m2",1,{"v":795.83441928,"d":"795.83"}]
[{"$nulls":4},0]
["7.27.3","50mm Plaswood venetian wooden window screen","m2",1,{"v":1626.0177400000005,"d":"1,626.02"}]
[{"$nulls":4},0]
["7.27.4","2300 x 1600mm high double leaf hinged bamboo screen with 100 x 35mm meranti frame","no",1,{"v":3124.7316,"d":"3,124.73"}]
[{"$nulls":4},0]
["7.27.5","63mm blade width vertical fabric venetian blinds","m2",1,{"v":421.8387660000001,"d":"421.84"}]
[{"$nulls":4},0]
["7.27.6","90mm blade width vertical fabric venetian blinds","m2",1,{"v":485.11458089999996,"d":"485.11"}]
[{"$nulls":4},0]
["7.27.7","127mm blade width vertical fabric venetian blinds","m2",1,{"v":548.3903958000001,"d":"548.39"}]
[{"$nulls":4},0]
["7.27.8","16mm blade width aluminium venetian blinds","m2",1,{"v":480.42748350000016,"d":"480.43"}]
[{"$nulls":4},0]
["7.27.9","25mm blade width aluminium venetian blinds","m2",1,{"v":552.4916060250001,"d":"552.49"}]
[{"$nulls":4},0]
["7.27.10","50mm blade width aluminium venetian blinds","m2",1,{"v":624.5557285500003,"d":"624.56"}]
[{"$nulls":4},0]
[7.28,"Fabric Screens",null,null,0]
[{"$nulls":4},0]
["7.28.1","\"Fabric Duke/Black Suede\" regis lined-in workwear 100% cotton with nine racer single tracks c/w cording sets","m2",1,{"v":666.8640157600001,"d":"666.86"}]
[{"$nulls":4},0]
["7.28.2","\"Fabric York Velvet\" regis lined-in workwear 100% cotton with nine racer single tracks c/w cording sets","m2",1,{"v":1186.14811536,"d":"1,186.15"}]
[{"$nulls":4},0]
[7.29,"Stage Screens",null,null,0]
[{"$nulls":4},0]
["7.29.1","\"Fabric Duke/Black Suede\" one valance plus two stage screws ,lined-in workwear 100% cotton glorius track with winch","m2",1,{"v":691.41051844,"d":"691.41"}]
[{"$nulls":4},0]
["7.29.2","\"Fabric York Velvet\" one valance plus two stage screws ,lined-in workwear 100% cotton glorius track with winch","m2",1,{"v":1010.6192110000001,"d":"1,010.62"}]
[{"$nulls":4},0]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
[{"v":7.3,"d":"7.30"},"Making good wooden floors",null,null,0]
[{"$nulls":4},0]
["7.30.1","Cleaning, sanding and sealing ordinary floors","m2",1,{"v":214.10198000000005,"d":"214.10"}]
[{"$nulls":4},0]
["7.30.2","Cleaning, sanding and sealing parquet floors","m2",1,{"v":289.327,"d":"289.33"}]
[{"$nulls":4},0]
["7.30.3","Replacing parquet floors","m2",1,{"v":1012.6445000000001,"d":"1,012.64"}]
{"$rows_empty":36}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Ceilings, Partitions etc.","index":7,"n_rows":508,"n_cols":7,"rows_kept":508,"merged":[[0,4,0,6]],"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 8"]
[]
[null,"CEILINGS, PARTITIONS AND ACCESS FLOORING"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Descriptions"]
[]
[null,"Items described as \"nailed\" shall be deemed to be fixed with hardened steel nails or pins or shot pinned to brickwork or concrete"]
[]
[null,"Items described as \"plugged\" shall be deemed to include screwing to fibre, plastic or metal plugs at not exceeding 600mm centres, and where described as \"bolted\" the bolts have been given elsewhere"]
[]
[null,"CEILINGS ETC"]
[]
[8.1,"\"Isotherm\" insulation"]
[]
["8.1.1","50mm insulation closely fitted and laid on top of brandering between roof trusses","m²",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
[null,"NAILED UP CEILINGS",null,null,0]
[{"$nulls":4},0]
[8.2,"6.4mm \"Rhino\" gypsum plasterboard with 32mm wrought softwood half round cover strip over joints",null,null,0]
[{"$nulls":4},0]
["8.2.1","Ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["8.2.2","Sloping ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.2.3","Vertical ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.2.4","Horizontal bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["8.2.5","Sloping bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.2.6","Vertical bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.2.7","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.2.8","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.2.9","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.2.10","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.2.11","Extra over ceiling for opening for 300 x 1200mm light fitting","no",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["8.2.12","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["8.2.13","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["8.2.14","Extra over ceiling for 600 x 600mm trap door of 38 x 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening on 20 x 20mm pressed steel angle","no",1,{"v":380.29140880000006,"d":"380.29"}]
[{"$nulls":4},0]
["8.2.15","Ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["8.2.16","Sloping ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["8.2.17","Vertical ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":114.70079588000002,"d":"114.70"}]
[{"$nulls":4},0]
[8.3,"6.4mm \"Rhino\" gypsum plasterboard with H-type pressed metal jointing strips",null,null,0]
[{"$nulls":4},0]
["8.3.1","Ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["8.3.2","Sloping ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.3.3","Vertical ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.3.4","Horizontal bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["8.3.5","Sloping bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.3.6","Vertical bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.3.7","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.3.8","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.3.9","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.3.10","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.3.11","Extra over ceiling for opening for 300 x 1200mm light fitting","no",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["8.3.12","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["8.3.13","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["8.3.14","Extra over ceiling for 600 x 600mm trap door of 38 x 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening on 20 x 20mm pressed steel angle","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["8.3.15","Ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["8.3.16","Sloping ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["8.3.17","Vertical ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":114.70079588000002,"d":"114.70"}]
[{"$nulls":4},0]
[8.4,"6.4mm \"Rhino\" gypsum plasterboard with 63mm wide strips of mesh scrim fixed over joints and  finished with gypsum skim plaster trowelled and sanded to a smooth polished surface",null,null,0]
[{"$nulls":4},0]
["8.4.1","Ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":190.14570440000003,"d":"190.15"}]
[{"$nulls":4},0]
["8.4.2","Sloping ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":196.2794368,"d":"196.28"}]
[{"$nulls":4},0]
["8.4.3","Vertical ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":196.2794368,"d":"196.28"}]
[{"$nulls":4},0]
["8.4.4","Horizontal bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["8.4.5","Sloping bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["8.4.6","Vertical bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["8.4.7","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.4.8","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.4.9","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.4.10","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.4.11","Extra over ceiling for opening for 300 x 1200mm light fitting","no",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["8.4.12","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["8.4.13","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["8.4.14","Extra over ceiling for 600 x 600mm trap door of 38 x 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening on 20 x 20mm pressed steel angle","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["8.4.15","Ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["8.4.16","Sloping ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["8.4.17","Vertical ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":114.70079588000002,"d":"114.70"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[8.5,"4mm \"Everite Cladit\" high density plain Pressed Nutec-cement boards with 32 x 10mm wrought softwood cover strip over joints",null,null,0]
[{"$nulls":4},0]
["8.5.1","Ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["8.5.2","Sloping ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.5.3","Vertical ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.5.4","Horizontal bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["8.5.5","Sloping bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.5.6","Vertical bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.5.7","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.5.8","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.5.9","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.5.10","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.5.11","Extra over ceiling for opening for 300 x 1200mm light fitting","no",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["8.5.12","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["8.5.13","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["8.5.14","Extra over ceiling for 600 x 600mm trap door of 38 x 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening on 20 x 20mm pressed steel angle","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["8.5.15","Ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["8.5.16","Sloping ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["8.5.17","Vertical ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":114.70079588000002,"d":"114.70"}]
[{"$nulls":4},0]
[8.6,"4mm \"Everite Cladit\" high density plain Pressed Nutec-cement boards with H-type pressed steel jointing strips",null,null,0]
[{"$nulls":4},0]
["8.6.1","Ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["8.6.2","Sloping ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.6.3","Vertical ceilings including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":147.20957760000005,"d":"147.21"}]
[{"$nulls":4},0]
["8.6.4","Horizontal bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["8.6.5","Sloping bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.6.6","Vertical bulkhead including 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":171.74450720000002,"d":"171.74"}]
[{"$nulls":4},0]
["8.6.7","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.6.8","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["9.6.9","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.6.10","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.6.11","Extra over ceiling for opening for 300 x 1200mm light fitting","no",1,{"v":29.441915520000006,"d":"29.44"}]
[{"$nulls":4},0]
["8.6.12","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["8.6.13","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":49.0698592,"d":"49.07"}]
[{"$nulls":4},0]
["8.6.14","Extra over ceiling for 600 x 600mm trap door of 38 x 50mm wrought softwood rebated framing with one 38 x 38mm sawn softwood cross brander covered with ceiling board and fitted flush in opening on 20 x 20mm pressed steel angle","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["8.6.15","Ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["8.6.16","Sloping ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["8.6.17","Vertical ceilings excluding 38 x 50mm sawn softwood brandering at 400mm centres","m²",1,{"v":114.70079588000002,"d":"114.70"}]
[{"$nulls":4},0]
[8.7,"Book Detection System Partition (Oak Melamine)",null,null,0]
[{"$nulls":4},0]
["8.7.1","Partition 1200 x 1800mm with wood","m²",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["8.7.2","Partition 1200 x 1800mm with glazing (Glazing measured else where)","m²",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
[null,"CORNICES, MOULDINGS AND ROSES",null,null,0]
[{"$nulls":4},0]
[8.8,"\"Rhino\" gypsum plasterboard cornice",null,null,0]
[{"$nulls":4},0]
["8.8.1","75mm standard coved cornice","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["8.8.2","125mm standard coved cornice","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
[8.9,"\"Rhino\" gypsum plasterboard decorative mouldings",null,null,0]
[{"$nulls":4},0]
["8.9.1","75mm standard coved cornice","m",1,{"v":34.96227468000001,"d":"34.96"}]
[{"$nulls":4},0]
["8.9.2","125mm standard coved cornice","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["8.9.3","155mm standard coved cornice","m",1,{"v":70.66059724800002,"d":"70.66"}]
[{"$nulls":4},0]
["8.9.4","225mm standard coved cornice","m",1,{"v":84.7927166976,"d":"84.79"}]
[{"$nulls":4},0]
[{"v":8.1,"d":"8.10"},"Polystyrene, Expanded Polystyrene (EPS) and Polyurethane decorative mouldings",null,null,0]
[{"$nulls":4},0]
["8.10.1","75mm standard coved cornice","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["8.10.2","125mm standard coved cornice","m",1,{"v":33.12215496,"d":"33.12"}]
[{"$nulls":4},0]
["8.10.3","155mm standard coved cornice","m",1,{"v":39.74658595200001,"d":"39.75"}]
[{"$nulls":4},0]
["8.10.4","225mm standard coved cornice","m",1,{"v":47.695903142400006,"d":"47.70"}]
[{"$nulls":4},0]
[8.11,"Wrought softwood",null,null,0]
[{"$nulls":4},0]
["8.11.1","20 x 65mm cornice","m",1,{"v":30.668662000000005,"d":"30.67"}]
[{"$nulls":4},0]
[null,"HERITAGE CORNICE AND MOULDINGS - \"Making good, patching, straightning and sealing of existing Cornice, Mouldings and soffits of verges to Heritage Buildings\" (Paintwork elsewhere)",null,null,0]
[{"$nulls":4},0]
["8.11.2","75mm Heritage Moulding cornice","m",1,{"v":26.039430000000007,"d":"26.04"}]
[{"$nulls":4},0]
["8.11.3","125mm Heritage Moulding cornice","m",1,{"v":41.663088,"d":"41.66"}]
[{"$nulls":4},0]
["8.11.4","155mm Heritage Moulding cornice","m",1,{"v":53.120437200000005,"d":"53.12"}]
[{"$nulls":4},0]
["8.11.5","225mm Heritage Moulding cornice","m",1,{"v":78.11829000000002,"d":"78.12"}]
[{"$nulls":4},0]
["8.11.6","Not exceeding 225mm girth Moulding cornice External with special bonding liquid","m",1,{"v":127.30388,"d":"127.30"}]
[{"$nulls":4},0]
["8.11.7","Exceeding 225mm and not exceeding 600mm girth Moulding cornice External with special bonding liquid","m",1,{"v":165.495044,"d":"165.50"}]
[{"$nulls":4},0]
["8.11.8","Restoring soffits of verges including mouldings","m2",1,{"v":368.60259800000006,"d":"368.60"}]
[{"$nulls":4},0]
[8.12,"SUSPENDED CEILINGS",null,null,0]
[{"$nulls":4},0]
["8.12.1","Electrical  light  fittings, diffusers, panels, etc generally are  \"lay  in\"  units  of  the  same dimensions as the suspension grid described  and  allowance  must  be  made  accordingly for their support  inclusive  of any flexibility in setting out that may be required (ceiling panels have not been deducted and pricing is to take cognisance thereof) ",null,null,0]
[null," ",null,null,0]
[8.13,"BPB Gypsum DonnCeil Gyprex White vinyl finished gypsum ceiling tiles size 1200 x 600mm x 12,5mm thick laid on and including SQ/T38 galvanised main tees, cross tees, hold-down ",null,null,0]
[null,"clips, wedges, etc., all suspended with galvanised hangers at hanger centres not exceeding 1200mm",null,null,0]
[{"$nulls":4},0]
["8.13.1","Ceiling suspended not exceeding 1m below concrete soffits","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.2","Ceiling suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.3","Sloping ceiling suspended not exceeding 1m below concrete soffits","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.4","Sloping ceiling suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.5","Ceiling suspended not exceeding 1m. below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.6","Ceiling suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.7","Sloping ceiling suspended not exceeding 1m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.8","Sloping ceiling suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.9","Ceilings suspended not exceeding 1m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.10","Ceilings suspended exceeding 1m and not exceeding 2m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.11","Sloping ceilings suspended not exceeding 1m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.12","Sloping ceilings suspended exceeding 1m and not exceeding 2m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.13","Horizontal bulkheads suspended not exceeding 1m below concrete soffits","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.14","Horizontal bulkheads suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.15","Horizontal bulkhead suspended not exceeding 1m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.16","Horizontal bulkhead suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.17","Sloping bulkheads suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":261.29700024000005,"d":"261.30"}]
[{"$nulls":4},0]
["8.13.18","Sloping bulkhead suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":264.97723968,"d":"264.98"}]
[{"$nulls":4},0]
["8.13.19","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.13.20","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.13.21","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.13.22","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.13.23","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["8.13.24","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":6.1337324,"d":"6.13"}]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
["8.13.25","Install 600 x 1200mm acoustic tile in existing suspended ceiling frame","m2",1,{"v":130.64850012000002,"d":"130.65"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[8.14,"Everite Nutec vinyl finished ceiling tiles size 1200 x 600mm x 6mm thick laid on and including SQ/T38 galvanised main tees, cross tees, hold-down clips, wedges, etc., all suspended with galvanised hangers at hanger centres not exceeding 1200mm",null,null,0]
[{"$nulls":4},0]
["8.14.1","Ceiling suspended not exceeding 1m below concrete soffits","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.2","Ceiling suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.3","Sloping ceiling suspended not exceeding 1m below concrete soffits","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.4","Sloping ceiling suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.5","Ceiling suspended not exceeding 1m. below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.6","Ceiling suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.7","Sloping ceiling suspended not exceeding 1m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.8","Sloping ceiling suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.9","Ceilings suspended not exceeding 1m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.10","Ceilings suspended exceeding 1m and not exceeding 2m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.11","Sloping ceilings suspended not exceeding 1m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.12","Sloping ceilings suspended exceeding 1m and not exceeding 2m below steel purlins at ± 1,8m centres (trusses at ± 6,0m centres)","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.13","Horizontal bulkheads suspended not exceeding 1m below concrete soffits","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.14","Horizontal bulkheads suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.15","Horizontal bulkhead suspended not exceeding 1m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.16","Horizontal bulkhead suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.17","Sloping bulkheads suspended exceeding 1m and not exceeding 2m below concrete soffits","m²",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["8.14.18","Sloping bulkhead suspended exceeding 1m and not exceeding 2m below timber/steel purlins at ± 1,4m centres (trusses at ± 1,0m centres)","m²",1,{"v":240.44231008000006,"d":"240.44"}]
[{"$nulls":4},0]
["8.14.19","Circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
["8.14.20","Opening for sprinkler head","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.14.21","Extra over ceiling for opening for 75mm diameter downlighter","no",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["8.14.22","Extra over ceiling for opening for 180mm diameter downlighter","no",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["8.14.23","Extra over ceiling for opening for 600 x 1200mm light fitting","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
["8.14.24","Extra over ceiling for 600 x 600mm opening for ventilation/air conditioning diffuser","no",1,{"v":6.1337324,"d":"6.13"}]
[{"$nulls":4},0]
[8.15,"Donn cornices to suspended ceilings",null,null,0]
[{"$nulls":4},0]
["8.15.1","47 x 35mm 'SM25' recessed shadowline cornice plugged (code LSM 25).","m",1,{"v":29.441915520000006,"d":"29.44"}]
[null," ",null,null,0]
["8.15.2","47 x 35mm 'SM25' recessed shadowline cornice plugged (code LSM 25) circular on plan","m",1,{"v":30.668662000000005,"d":"30.67"}]
[null," ",null,null,0]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
["8.15.3","Install 600 x 1200mm acoustic tile in existing suspended ceiling frame","no",1,{"v":164.41810461111118,"d":"164.42"}]
[{"$nulls":4},0]
["8.15.4","Vacuum cleaning of ceiling voids","m2",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
[null,"CEILING TILES TO Rhino / Gypsum Board ceiling",null,null,0]
[{"$nulls":4},0]
["8.15.5","500 x 500 Polystyrene Tile with wood finish","m2",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["8.15.6","500 x 500 Polystyrene Tile with Laminated finish","m2",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
[null,"PARTITIONS ETC.",null,null,0]
[{"$nulls":4},0]
[null,"Rhino-Drywall partition systems",null,null,0]
[{"$nulls":4},0]
[8.16,"BPB Gypsum GypRoc Standard - 40 db (½ hour fire rating) Ultrasteel Stud Drywall consisting of stud and track system with 51mm Drywall Ultrasteel studs positioned at 600mm centres fixed into 51mm wide top and bottom track clad on both sides with 12,5mm thick taper edged Rhinoboard fixed with 25mm Drywall screws at 220mm centres and all corners fixed with Drywall Corner beads and all joints to be taped and jointed as per manufacture's specifications.",null,null,0]
[{"$nulls":4},0]
["8.16.1","Partitioning 2100mm high with bottom track plugged and free top track ","m",1,{"v":494.3788314400001,"d":"494.38"}]
[{"$nulls":4},0]
["8.16.2","Partitioning  3000mm high with bottom track plugged and top track fixed to suspended ceiling tees","m",1,{"v":722.55367672,"d":"722.55"}]
[null," ",null,null,0]
["8.16.3","Partitioning  3000mm high with bottom track plugged and top track fixed to suspended ceiling tees circular on plan","m",1,{"v":722.55367672,"d":"722.55"}]
[{"$nulls":4},0]
["8.16.4","Partitioning  3600mm high with bottom track plugged and top track fixed to suspended ceiling tees","m",1,{"v":874.6702402400002,"d":"874.67"}]
[{"$nulls":4},0]
["8.16.5","Partitioning  3600mm high with bottom track plugged and top track fixed to suspended ceiling tees circular on plan","m",1,{"v":874.6702402400002,"d":"874.67"}]
[{"$nulls":4},0]
["8.16.6","Partition 3000mm high with top and bottom tracks plugged and glazing in lieu of boarding 1,1m high at 1,0m above floor level framed all round with \"Drywall\" aluminium glazing sections and divided into panels with aluminium mullions at 1,2m centres with each panel glazed with 4mm clear float glass including neoprene glazing gaskets (glass elsewhere)","m",1,{"v":1406.12922,"d":"1,406.13"}]
[{"$nulls":4},0]
["8.16.7","Extra over partition 2100mm. high for vertical abutment","no",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["8.16.8","Extra over partition 2100mm. high for corner","no",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["8.16.9","Extra over partition 2100mm. high for T - intersection","no",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
["8.16.10","Extra over partition 2100mm. high for fair end","no",1,{"v":149.66307056,"d":"149.66"}]
[{"$nulls":4},0]
["8.16.11","Extra over partition 3000mm. high for vertical abutment","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["8.16.12","Extra over partition 3000mm. high for corner","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["8.16.13","Extra over partition 3000mm. high for T - intersection","no",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["8.16.14","Extra over partition 3000mm. high for fair end","no",1,{"v":209.77364808000007,"d":"209.77"}]
[{"$nulls":4},0]
["8.16.15","Extra over partition 3600mm. high for vertical abutment","no",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["8.16.16","Extra over partition 3600mm. high for corner","no",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["8.16.17","Extra over partition 3600mm. high for T - intersection","no",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["8.16.18","Extra over partition 3600mm. high for fair end","no",1,{"v":249.02953544000002,"d":"249.03"}]
[{"$nulls":4},0]
["8.16.19","75mm Alluminium skirting","m",1,{"v":52.07886000000001,"d":"52.08"}]
[{"$nulls":4},0]
["8.16.20","Removal and riffiting of double sided partition with new alluminium top and bottom railtracks (Paint work elsewhere)","m",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
["8.16.21","Extra over alluminium frame into drywall partition for glass partition ","m",1,{"v":116.54091560000002,"d":"116.54"}]
[{"$nulls":4},0]
["8.16.22","Opening of existing partition for doors, windows, etc","m2",1,{"v":63.65194,"d":"63.65"}]
[{"$nulls":4},0]
[8.17,"Doors",null,null,0]
[{"$nulls":4},0]
["8.17.1","Extra over partition for 40mm semi-solid flush door 762 x 2032mm high with commercial veneer on both sides and hardwood edge strips to vertical edges hung to and including standard natural anodised aluminium door frame with one pair of 100mm nylon washered aluminium hinges and additional studding, trimming, etc ","no",1,{"v":964.2227332800003,"d":"964.22"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["8.17.2","Extra over partition for 40mm semi-solid flush door 813 x 2032mm high with commercial veneer on both sides and hardwood edge strips to vertical edges hung to and including standard natural anodised aluminium door frame with one pair of 100mm nylon washered aluminium hinges and additional studding, trimming, etc ","no",1,{"v":964.2227332800003,"d":"964.22"}]
[{"$nulls":4},0]
["8.17.3","Extra over partition for 40mm semi-solid flush double door 1510 x 2032mm high with commercial veneer on both sides and hardwood edge strips to vertical edges hung to and including standard natural anodised aluminium door frame with three pair of 100mm nylon washered aluminium hinges and additional studding, trimming, etc ","no",1,{"v":1503.9911844800006,"d":"1,503.99"}]
[{"$nulls":4},0]
["8.17.4","Extra over partition for 40mm semi-solid flush door 813 x 2032mm high with commercial veneer on both sides and hardwood edge strips to vertical edges hung to and including standard natural anodised aluminium door frame with one pair of 100mm nylon washered aluminium hinges and additional studding, trimming, etc","no",1,{"v":999.7983812000002,"d":"999.80"}]
["8.17.5","Extra over partition for 40mm semi-solid flush double door 1510 x 2032mm high with commercial veneer on both sides and hardwood edge strips to vertical edges hung to and including standard natural anodised aluminium door frame with three pair of 100mm nylon washered aluminium hinges and additional studding, trimming, etc ","no",1,{"v":1577.5959732800004,"d":"1,577.60"}]
[{"$nulls":4},0]
[8.18,"Insulation",null,null,0]
[{"$nulls":4},0]
["8.18.1","75mm Thick \"Isotherm\" thermal insulation blanket in cavity of partitioning","m²",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
[null,"TOILET PARTITIONS",null,null,0]
[{"$nulls":4},0]
[null,"Note :",null,null,0]
[{"$nulls":4},0]
[null,"All toilet partitions are to be manufactured in a one-piece construction.  No horizontal or vertical joints will be permitted",null,null,0]
[{"$nulls":4},0]
[8.19,"\"Vitraflex\" toilet partitioning with 20mm thick vitreous enamelled steel sheet faced particle board bonded panels and natural anodised aluminium edging and top rails including fixing components and standard ironmongery comprising of indicator bolts, coat ",null,null,0]
[{"$nulls":4},0]
["8.19.1","Partition 800 X 2000mm high","no",1,{"v":2208.143664,"d":"2,208.14"}]
[{"$nulls":4},0]
["8.19.2","Partition 900 X 2000mm high","no",1,{"v":2451.0394670400005,"d":"2,451.04"}]
[{"$nulls":4},0]
["8.19.3","Partition 1200 X 2000mm high","no",1,{"v":2817.8366645600004,"d":"2,817.84"}]
[{"$nulls":4},0]
["8.19.4","Partition 1800 X 2000mm high","no",1,{"v":3523.2158905600004,"d":"3,523.22"}]
[{"$nulls":4},0]
["8.19.5","Full stile 200 X 2000mm high","no",1,{"v":203.63991568000006,"d":"203.64"}]
[{"$nulls":4},0]
["8.19.6","Wall stile 105mm wide x 2000mm high","no",1,{"v":155.79680296000004,"d":"155.80"}]
[{"$nulls":4},0]
["8.19.7","End stile 140mm wide x 2000mm high","no",1,{"v":172.97125368000002,"d":"172.97"}]
[{"$nulls":4},0]
["8.19.8","Door 794 x 1800mm high","no",1,{"v":2208.143664,"d":"2,208.14"}]
{"$rows_empty":31}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Floor covering, etc.","index":8,"n_rows":392,"n_cols":7,"rows_kept":392,"merged":[[0,4,0,6]],"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 9"]
[]
[]
[null,"FLOOR COVERINGS, WALL LININGS, ETC."]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"FLOOR COVERINGS"]
[]
[null,"Laminated wooden floor"]
[]
[9.1,"8mm Brown Rhodesian teak mosaic wood floor boards or equally approved"]
[]
["9.1.1","On floors","m²",1,{"v":475.97763424,"d":"475.98"}]
[{"$nulls":4},0]
["9.1.2","On dished (sunken) floors ","m²",1,{"v":475.97763424000016,"d":"475.98"}]
[{"$nulls":4},0]
["9.1.3","On treads and risers of stepped floors","m²",1,{"v":457.57643704000003,"d":"457.58"}]
[{"$nulls":4},0]
["9.1.4","On treads and risers of stairs","m²",1,{"v":457.57643704000003,"d":"457.58"}]
[{"$nulls":4},0]
["9.1.5","On treads and risers of winding stairs","m²",1,{"v":457.57643704000003,"d":"457.58"}]
[{"$nulls":4},0]
["9.1.6","Margins and borders not exceeding 500mm wide","m",1,{"v":229.40159176000003,"d":"229.40"}]
[{"$nulls":4},0]
["9.1.7","Inserts 500mm wide of differing colour","m",1,{"v":229.40159176000003,"d":"229.40"}]
[{"$nulls":4},0]
["9.1.8","Circular cutting","m",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
[9.2,"8mm Brown Rhodesian teak mosaic wood  blocks or equally approved",null,null,0]
[{"$nulls":4},0]
["9.2.1","On floors","m²",1,{"v":475.97763424000016,"d":"475.98"}]
[{"$nulls":4},0]
["9.2.2","On dished (sunken) floors ","m²",1,{"v":475.97763424000016,"d":"475.98"}]
[{"$nulls":4},0]
["9.2.3","On treads and risers of stepped floors","m²",1,{"v":457.57643704000003,"d":"457.58"}]
[{"$nulls":4},0]
["9.2.4","On treads and risers of stairs","m²",1,{"v":457.57643704000003,"d":"457.58"}]
[{"$nulls":4},0]
["9.2.5","On treads and risers of winding stairs","m²",1,{"v":457.57643704000003,"d":"457.58"}]
[{"$nulls":4},0]
["9.2.6","Margins and borders not exceeding 500mm wide","m",1,{"v":229.40159176000003,"d":"229.40"}]
[{"$nulls":4},0]
["9.2.7","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":229.40159176000003,"d":"229.40"}]
[{"$nulls":4},0]
["9.2.8","Inserts 500mm wide of differing colour","m",1,{"v":229.40159176000003,"d":"229.40"}]
[{"$nulls":4},0]
["9.2.9","Circular cutting","m",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
["9.2.10","Sanding and sealing to floors","m²",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[9.3,"220 x 73 x 19mm Brown Rhodesian teak mosaic wood  blocks in herringbone pattern or equally approved",null,null,0]
[{"$nulls":4},0]
["9.3.1","On floors","m²",1,{"v":778.9840148000001,"d":"778.98"}]
[{"$nulls":4},0]
["9.3.2","On dished floors ","m²",1,{"v":778.9840148000001,"d":"778.98"}]
[{"$nulls":4},0]
["9.3.3","On treads and risers of stepped floors","m²",1,{"v":778.9840148000001,"d":"778.98"}]
[{"$nulls":4},0]
["9.3.4","On treads and risers of stairs","m²",1,{"v":778.9840148000001,"d":"778.98"}]
[{"$nulls":4},0]
["9.3.5","On treads and risers of winding stairs","m²",1,{"v":778.9840148000001,"d":"778.98"}]
[{"$nulls":4},0]
["9.3.6","Margins and borders not exceeding 500mm wide","m",1,{"v":392.5588736,"d":"392.56"}]
[{"$nulls":4},0]
["9.3.7","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":392.5588736,"d":"392.56"}]
[{"$nulls":4},0]
["9.3.8","Inserts 500mm wide of differing colour","m",1,{"v":392.5588736,"d":"392.56"}]
[{"$nulls":4},0]
["9.3.9","Circular cutting","m",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[9.4,"300 x 300 x 2,0mm \"Floorflex\" semi-flexible vinyl tiles",null,null,0]
[{"$nulls":4},0]
["9.4.1","On floors","m²",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
["9.4.2","On dished (sunken) floors ","m²",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
["9.4.3","On treads and risers of steps","m²",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
["9.4.4","On treads and risers of stairs","m²",1,{"v":126.35488744000003,"d":"126.35"}]
[{"$nulls":4},0]
["9.4.5","Margins and borders not exceeding 500mm wide","m",1,{"v":65.01756344,"d":"65.02"}]
[{"$nulls":4},0]
["9.4.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":65.01756344,"d":"65.02"}]
[{"$nulls":4},0]
["9.4.7","Inserts 150mm wide of differing colour","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["9.4.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.4.9","75mm Skirting","m",1,{"v":15.162586492800001,"d":"15.16"}]
[{"$nulls":4},0]
[9.5,"300 x 300 x 2,5mm \"Floorflex\" semi-flexible vinyl tiles",null,null,0]
[{"$nulls":4},0]
["9.5.1","On floors","m²",1,{"v":145.98283112000004,"d":"145.98"}]
[{"$nulls":4},0]
["9.5.2","On dished floors ","m²",1,{"v":145.98283112000004,"d":"145.98"}]
[{"$nulls":4},0]
["9.5.3","On treads and risers of stepped","m²",1,{"v":145.98283112000004,"d":"145.98"}]
[{"$nulls":4},0]
["9.5.4","On treads and risers of stairs","m²",1,{"v":145.98283112000004,"d":"145.98"}]
[{"$nulls":4},0]
["9.5.5","Margins and borders not exceeding 500mm wide","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["9.5.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["9.5.7","Inserts 150mm wide of differing colour","m",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["9.5.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.5.9","75mm Skirting","m",1,{"v":17.517939734400006,"d":"17.52"}]
[{"$nulls":4},0]
[9.6,"300 x 300 x 2,0mm \"Superflex\" fully-flexible vinyl tiles",null,null,0]
[{"$nulls":4},0]
["9.6.1","On floors","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["9.6.2","On dished (sunken) floors ","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["9.6.3","On treads and risers of steps","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["9.6.4","On treads and risers of stairs","m²",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["9.6.5","Margins and borders not exceeding 500mm wide","m",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["9.6.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["9.6.7","Inserts 150mm wide of differing colour","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["9.6.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.6.9","75mm Skirting","m",1,{"v":24.28958030400001,"d":"24.29"}]
[{"$nulls":4},0]
[9.7,"300 x 300 x 2,5mm \"Superflex\" fully-flexible vinyl tiles",null,null,0]
[{"$nulls":4},0]
["9.7.1","On floors","m²",1,{"v":251.48302840000005,"d":"251.48"}]
[{"$nulls":4},0]
["9.7.2","On dished (sunken) floors ","m²",1,{"v":251.48302840000005,"d":"251.48"}]
[{"$nulls":4},0]
["9.7.3","On treads and risers of steps","m²",1,{"v":251.48302840000005,"d":"251.48"}]
[{"$nulls":4},0]
["9.7.4","On treads and risers of stairs","m²",1,{"v":251.48302840000005,"d":"251.48"}]
[{"$nulls":4},0]
["9.7.5","Margins and borders not exceeding 500mm wide","m",1,{"v":127.58163392000003,"d":"127.58"}]
[{"$nulls":4},0]
["9.7.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":127.58163392000003,"d":"127.58"}]
[{"$nulls":4},0]
["9.7.7","Inserts 150mm wide of differing colour","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["9.7.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.13.7","75mm Skirting","m",1,{"v":30.177963408000007,"d":"30.18"}]
[{"$nulls":4},0]
[9.8,"2,0mm. \"Superflex\" fully flexible vinyl sheeting with welded joints",null,null,0]
[{"$nulls":4},0]
["9.8.1","On floors","m²",1,{"v":351.15617990000004,"d":"351.16"}]
[{"$nulls":4},0]
["9.8.2","On dished (sunken) floors ","m²",1,{"v":364.7730658280001,"d":"364.77"}]
[{"$nulls":4},0]
["9.8.3","On treads and risers of steps","m²",1,{"v":364.7730658280001,"d":"364.77"}]
[{"$nulls":4},0]
["9.8.4","On treads and risers of stairs","m²",1,{"v":364.7730658280001,"d":"364.77"}]
[{"$nulls":4},0]
["9.8.5","Margins and borders not exceeding 500mm wide","m",1,{"v":182.39266664640004,"d":"182.39"}]
[{"$nulls":4},0]
["9.8.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":182.39266664640004,"d":"182.39"}]
[{"$nulls":4},0]
["9.8.7","Inserts 150mm wide of differing colour","m",1,{"v":72.95461316560001,"d":"72.95"}]
[{"$nulls":4},0]
["9.8.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.13.7","75mm Skirting","m",1,{"v":42.10193919360001,"d":"42.10"}]
[{"$nulls":4},0]
["9.9.","2,5mm. \"Superflex\" fully flexible vinyl sheeting with welded joints",null,null,0]
[{"$nulls":4},0]
["9.9.1","On floors","m²",1,{"v":403.83267375120005,"d":"403.83"}]
[{"$nulls":4},0]
["9.9.2","On dished floors ","m²",1,{"v":417.32688503120005,"d":"417.33"}]
[{"$nulls":4},0]
["9.9.3","On treads and risers of steps","m²",1,{"v":417.32688503120005,"d":"417.33"}]
[{"$nulls":4},0]
["9.9.4","On treads and risers of stairs","m²",1,{"v":417.32688503120005,"d":"417.33"}]
[{"$nulls":4},0]
["9.9.5","Margins and borders not exceeding 500mm wide","m",1,{"v":208.66957624800003,"d":"208.67"}]
[{"$nulls":4},0]
["9.9.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":208.66957624800003,"d":"208.67"}]
[{"$nulls":4},0]
["9.9.7","Inserts 150mm wide of differing colour","m",1,{"v":83.4555630344,"d":"83.46"}]
[{"$nulls":4},0]
["9.9.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.9.9","75mm Skirting","m",1,{"v":48.43195103040001,"d":"48.43"}]
[{"$nulls":4},0]
[{"v":9.1,"d":"9.10"},"3,5mm. \"Industrial Floor\" flexible vinyl sheeting with welded joints",null,null,0]
[{"$nulls":4},0]
["9.10.1","On floors","m²",1,{"v":479.9277579056002,"d":"479.93"}]
[{"$nulls":4},0]
["9.10.2","On dished (sunken) floors ","m²",1,{"v":493.4219691856001,"d":"493.42"}]
[{"$nulls":4},0]
["9.10.3","On treads and risers of steps","m²",1,{"v":506.9161804656001,"d":"506.92"}]
[{"$nulls":4},0]
["9.10.4","On treads and risers of stairs","m²",1,{"v":506.9161804656001,"d":"506.92"}]
[{"$nulls":4},0]
["9.10.5","Margins and borders not exceeding 500mm wide","m",1,{"v":253.45809023280006,"d":"253.46"}]
[{"$nulls":4},0]
["9.10.6","Turn-ups over coves and up against walls not exceeding 500mm girth","m",1,{"v":253.45809023280006,"d":"253.46"}]
[{"$nulls":4},0]
["9.10.7","Inserts 150mm wide of differing colour","m",1,{"v":101.37832910720002,"d":"101.38"}]
[{"$nulls":4},0]
["9.10.8","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.10.9","75mm Skirting","m",1,{"v":57.55894484160001,"d":"57.56"}]
[{"$nulls":4},0]
[null,"3,5mm. \"Industrial Floor\" non - slip flexible vinyl sheeting with welded joints",null,null,0]
[{"$nulls":4},0]
["9.10.9","On floors","m²",1,{"v":494.64871566560015,"d":"494.65"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[9.11,"450 x 450 x 6.3mm stud pattern Eco range (Colour : dark grey) \"Tuff Seal\" interlocking heavy duty vinyl tiles laid in accordance with manufactures instructions ",null,null,0]
[{"$nulls":4},0]
["9.11.1","On floors","m²",1,{"v":472.29739480000006,"d":"472.30"}]
[{"$nulls":4},0]
["9.11.2","On dished (sunken) floors ","m²",1,{"v":472.29739480000006,"d":"472.30"}]
[{"$nulls":4},0]
["9.11.3","On treads and risers of steps","m²",1,{"v":472.29739480000006,"d":"472.30"}]
[{"$nulls":4},0]
["9.11.4","On treads and risers of stairs","m²",1,{"v":472.29739480000006,"d":"472.30"}]
[{"$nulls":4},0]
["9.11.5","Margins and borders not exceeding 450mm wide","m",1,{"v":142.30259168000003,"d":"142.30"}]
[{"$nulls":4},0]
["9.11.6","Circular cutting","m",1,{"v":9.813971840000002,"d":"9.81"}]
[{"$nulls":4},0]
["9.11.7","75mm Skirting","m",1,{"v":56.67568737600002,"d":"56.68"}]
[{"$nulls":4},0]
[9.12,"\"Belgotex Berber Point\" polypropylene needlepunch carpeting laid in accordance with SABS 0186-2000 fitting code of practice",null,null,0]
[{"$nulls":4},0]
["9.12.1","On floors","m²",1,{"v":333.06166932000014,"d":"333.06"}]
[{"$nulls":4},0]
["9.12.2","On dished (sunken) floors ","m²",1,{"v":349.7086190536,"d":"349.71"}]
[{"$nulls":4},0]
["9.12.3","On treads and risers of steps","m²",1,{"v":349.7086190536,"d":"349.71"}]
[{"$nulls":4},0]
["9.12.4","On treads and risers of stairs","m²",1,{"v":349.7086190536,"d":"349.71"}]
[{"$nulls":4},0]
["9.12.5","Margins and borders not exceeding 500mm wide","m",1,{"v":166.53083466000007,"d":"166.53"}]
[{"$nulls":4},0]
["9.12.6","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
[9.13,"\"Belgotex Berber Point 920 Nexus\" 500 x 500mm carpet tiles laid in accordance with SABS 0186-2000 fitting code of practice",null,null,0]
[{"$nulls":4},0]
["9.13.1","On floors","m²",1,{"v":333.06166932000014,"d":"333.06"}]
[{"$nulls":4},0]
["9.13.2","On dished floors ","m²",1,{"v":349.7086190536,"d":"349.71"}]
[{"$nulls":4},0]
["9.13.3","On treads and risers of steps","m²",1,{"v":349.7086190536,"d":"349.71"}]
[{"$nulls":4},0]
["9.13.4","On treads and risers of stairs","m²",1,{"v":349.7086190536,"d":"349.71"}]
[{"$nulls":4},0]
["9.13.5","Margins and borders not exceeding 500mm wide","m",1,{"v":166.53083466000007,"d":"166.53"}]
[{"$nulls":4},0]
["9.13.6","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
["9.13.7","75mm Skirting","m",1,{"v":39.89379552960001,"d":"39.89"}]
[{"$nulls":4},0]
[9.14,"Sundries",null,null,0]
[{"$nulls":4},0]
["9.14.1","Blue underfelt","m²",1,{"v":110.92241672160002,"d":"110.92"}]
[{"$nulls":4},0]
["9.14.2","Self-levelling screed","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["9.14.3","Aluminium metal door strips","m",1,{"v":59.49720428000002,"d":"59.50"}]
[{"$nulls":4},0]
["9.14.4","Steam cleaning to carpets","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
[null,"WALL LININGS",null,null,0]
[{"$nulls":4},0]
[9.15,"1,25mm. \"Superflex\" fully flexible vinyl sheeting with welded joints",null,null,0]
[{"$nulls":4},0]
["9.15.1","On walls","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["9.15.2","On circular walls","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["9.15.3","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
[9.16,"\"Belgotex Berber Heritage\" tufted carpeting glued on",null,null,0]
[{"$nulls":4},0]
["9.16.1","On walls","m²",1,{"v":333.06166932000014,"d":"333.06"}]
[{"$nulls":4},0]
["9.16.2","On circular walls","m²",1,{"v":333.06166932000014,"d":"333.06"}]
[{"$nulls":4},0]
["9.16.3","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
[9.17,"Architect approved sheet carpet (Cost Price R120.00/m², delivered on site, fixed with adhesive)",null,null,0]
[{"$nulls":4},0]
["9.17.1","On walls","m²",1,{"v":333.06166932000014,"d":"333.06"}]
[{"$nulls":4},0]
["9.17.2","On circular walls","m²",1,{"v":333.06166932000014,"d":"333.06"}]
[{"$nulls":4},0]
["9.17.3","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
[null,"SKIRTINGS, NOSINGS, ETC",null,null,0]
[{"$nulls":4},0]
[9.18,"\"Floorworx Extruda\"",null,null,0]
[{"$nulls":4},0]
["9.18.1","25mm MES25 edge strip","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["9.18.2","25 x 2.5mm MPT25 edge trim","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["9.18.3","70 x 10mm MCB70 vinyl skirting","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
["9.18.4","100 x 14mm MCB100 vinyl skirting","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["9.18.5","100 x 50mm MFE5 vinyl hospital skirting","m",1,{"v":53.97684512000001,"d":"53.98"}]
[{"$nulls":4},0]
["9.18.6","35 x 14mm MCF54 vinyl coved fillet","m",1,{"v":47.843112720000015,"d":"47.84"}]
[{"$nulls":4},0]
["9.18.7","75 x 10mm MSN100 vinyl stairnosing","m",1,{"v":58.88383104000001,"d":"58.88"}]
[{"$nulls":4},0]
[9.19,"\"Floorworx Protrim Mouldings\"",null,null,0]
[{"$nulls":4},0]
["9.19.1","82 x 11mm PTS082 skitring","m",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["9.19.2","16 x 16mm PTQ016 quarter round","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["9.19.3","66 x 17mm PTC066 chair rail","m",1,{"v":65.01756344,"d":"65.02"}]
[{"$nulls":4},0]
[{"v":9.2,"d":"9.20"},"\"Floorworx Intrad Wall and Corner Protection\" All to be installed strictly in accordance to manufacturer’s instructions",null,null,0]
[{"$nulls":4},0]
["9.20.1","Wall protector of 200 x 29mm TR200 high impact resistant uPVC extruded lip channel profile complete with 25mm wide uPVC brackets TRP200 at 400mm max. centres plugged to wall and uPVC joining blocks TRJ200 as required","m",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
["9.20.2","Extra over lip channel for uPVC external corner TRE200","no",1,{"v":127.58163392000003,"d":"127.58"}]
[{"$nulls":4},0]
["9.20.3","Extra over lip channel for uPVC stopend TRS200","no",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["9.20.4","Corner protector of 70 x 70 x 1.2mm thick CP1200 high impact resistant uPVC extruded angular profile","m",1,{"v":114.08742264000001,"d":"114.09"}]
[{"$nulls":4},0]
[null,"HANDRAILS",null,null,0]
[{"$nulls":4},0]
[9.21,"\"Floorworx Extruda\" vinyl handrails",null,null,0]
[{"$nulls":4},0]
["9.21.1","MHR1 handrail fitted over 40 x 6mm core rail","m",1,{"v":61.33732400000001,"d":"61.34"}]
[{"$nulls":4},0]
["9.21.2","MHR2 handrail fitted over 40 x 10mm core rail","m",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["9.21.3","MHR3 handrail fitted over 50 x 6mm core rail","m",1,{"v":78.51177472000002,"d":"78.51"}]
[{"$nulls":4},0]
["9.21.4","MHR4 handrail fitted over 50 x 10mm core rail","m",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
[null,"POLISH, SEALERS, ETC.",null,null,0]
[{"$nulls":4},0]
[9.22,"Polish, Sealers, etc",null,null,0]
[{"$nulls":4},0]
["9.22.1","2 coats wax polish on vinyl flooring","m²",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
["9.22.2","Strip and seal on vinyl flooring","m²",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
[null,"EXPANSION JOINTS",null,null,0]
[{"$nulls":4},0]
[9.23,"\"Floorworx Intrad Wall and Corner Protection\" All to be installed strictly in accordance to manufacturer’s instructions",null,null,0]
[{"$nulls":4},0]
["9.23.1","Floor expansion joint with aluminium extruded T-section profile profile complete with rubber plugged to wall, floors,etc TRJ200 as required","m",1,{"v":236.76207064000005,"d":"236.76"}]
[{"$nulls":4},0]
[null,"WALL COVERINGS (PAPERHANGING)",null,null,0]
[{"$nulls":4},0]
[9.24,"1,25mm. \"Superflex\" wall paper sheeting with welded joints",null,null,0]
[{"$nulls":4},0]
["9.24.1","On walls","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["9.24.2","On circular walls","m²",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
["9.24.3","Circular cutting","m",1,{"v":2.4534929600000006,"d":"2.45"}]
[{"$nulls":4},0]
[9.25,"HERITAGE BUILDINGS ; \"Rehabilitation of wooden floors, facades, and panels",null,null,0]
[{"$nulls":4},0]
["9.25.1","Rehabilitation of suspended wooden floor","m²",1,{"v":295.11354000000006,"d":"295.11"}]
[{"$nulls":4},0]
["9.25.2","Rehabilitation of wooden panels","m²",1,{"v":260.3943,"d":"260.39"}]
[{"$nulls":4},0]
["9.25.3","Rehabilitation of wooden facades","m²",1,{"v":260.3943,"d":"260.39"}]
[{"$nulls":4},0]
[]
[]
[]
[]
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Ironmongery","index":9,"n_rows":733,"n_cols":7,"rows_kept":733,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 10"]
[]
[null,"IRONMONGERY"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Finishers to ironmongery"]
[]
[null,"Where applicable finishes to ironmongery are indicated by suffixes in accordance with the following list :"]
[]
[null,"BS   Satin bronze lacquered"]
[null,"CH   Chromium plated"]
[null,"SC   Satin chromium plated"]
[null,"SE   Silver enamelled"]
[null,"GE   Grey enamelled"]
[null,"AS   Anodised silver"]
[null,"AB   Anodised bronze"]
[null,"AG   Anodised gold"]
[null,"ABL Anodised black"]
[null,"PB   Polished brass"]
[null,"PL   Polished and lacquered"]
[null,"PT   Epoxy coated"]
[null,"SD   Sanded"]
[]
[null,"HINGES, BOLTS, ETC."]
[]
[10.1,"\"Union\" or equal and approved fixed to timber"]
[]
["10.1.1","100mm steel hinge","no",1,{"v":55.548986240000005,"d":"55.55"}]
[{"$nulls":4},0]
["10.1.2","100mm Falling / Rising butt Hinge","no",1,{"v":142.42760071936004,"d":"142.43"}]
[{"$nulls":4},0]
["10.1.3","100mm brass hinge JH-BB-STD-2-SS","no",1,{"v":110.08799091200002,"d":"110.09"}]
[{"$nulls":4},0]
["10.1.4","100 x 100mm brass parliament hinge","no",1,{"v":363.5933644800001,"d":"363.59"}]
[{"$nulls":4},0]
["10.1.5","100mm brass barrel bolt","no",1,{"v":36.61183184000001,"d":"36.61"}]
[{"$nulls":4},0]
["10.1.6","100mm brass barrel bolt with keep fixed to metal","no",1,{"v":46.71164752000001,"d":"46.71"}]
[{"$nulls":4},0]
["10.1.7","100mm brass barrel bolt with keep let into concrete","no",1,{"v":46.71164752000001,"d":"46.71"}]
[{"$nulls":4},0]
["10.1.8","100mm Chrome plated brass barrel bolt","no",1,{"v":36.61183184000001,"d":"36.61"}]
[{"$nulls":4},0]
["10.1.9","100mm Chrome plated brass barrel bolt with keep fixed to metal","no",1,{"v":65.50588000000002,"d":"65.51"}]
[{"$nulls":4},0]
["10.1.10","100mm Chrome plated brass barrel bolt with keep let into concrete","no",1,{"v":65.50588000000002,"d":"65.51"}]
[{"$nulls":4},0]
["10.1.11","WC Anidised Silver bathroom indicator bolt Ref. AL809AS","no",1,{"v":1235.8336462361603,"d":"1,235.83"}]
[{"$nulls":4},0]
["10.1.12","WC chrome plated indicator bolt with keep fixed to metal. Ref. CZ80941CH","no",1,{"v":273.3616111948801,"d":"273.36"}]
[{"$nulls":4},0]
["10.1.13","WC chrome plated indicator Ref  SS5004-73SS  ","no",1,{"v":299.4595349120001,"d":"299.46"}]
[{"$nulls":4},0]
["10.1.14","Escutcheon on Rose Bathroom indicator SS5305-73SS ","no",1,{"v":244.8397317145601,"d":"244.84"}]
[{"$nulls":4},0]
["10.1.14a","Escutcheon Bathroom indicator PB5375-73CH (Chrome plated)","no",1,{"v":346.9892675020801,"d":"346.99"}]
[{"$nulls":4},0]
["10.1.15","Lockset IW2029/IW2030/IW2031/IW2047 for indicator bolt or CZ682TR / TL with 22314 indicator Lockset","no",1,0]
[{"$nulls":4},0]
["10.1.16","Heavy duty security door chain brass code V-WS6-EB","no",1,{"v":432.2721111040002,"d":"432.27"}]
[{"$nulls":4},0]
[10.2,"CATCHES, CABIN HOOKS, ETC",null,null,0]
[{"$nulls":4},0]
["10.2.1","Brass window catch to side hung sash  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.2","Brass window stay to side hung sash  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.3","Brass window  combination stay and fastener size 300mm Ref IW1260  ","no",1,{"v":145.18485040000002,"d":"145.18"}]
[{"$nulls":4},0]
["10.2.4","Brass window  fanlight stay and fastener size 300mm Ref IW1261  ","no",1,{"v":145.18485040000002,"d":"145.18"}]
[{"$nulls":4},0]
["10.2.5","Brass window sliding stays outwards size 300mm Ref IW1262  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.6","Brass window telescopic stays size 300mm Ref IW1263  ","no",1,{"v":145.18485040000002,"d":"145.18"}]
[{"$nulls":4},0]
["10.2.7","Brass window roller stay size 300mm Ref IW1263  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.8","Brass window casement stay  size 300mm Ref IW1265  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.9","Brass window sash hook with wooden stick Ref IW1271  ","no",1,{"v":296.68208560000005,"d":"296.68"}]
[{"$nulls":4},0]
["10.2.10","32mm Diameter polished hardwood longarm 2 600mm long with brass sash hook Ref \"IW 1271\" on one end, two broom clips each with 20 x 100 x 100mm wrought and chamfered hardwood block twice oiled and plugged and 20 x 70 x 70mm wrought and chamfered hardwood block with sinking twice oiled and plugged ","no",1,{"v":410.3050120000001,"d":"410.31"}]
[{"$nulls":4},0]
["10.2.11","Brass window sash lifts Ref IW1272  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.12","Brass window spring catch Ref IW1273  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.13","Brass window spring catch box Ref IW1274  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.14","Cupboard fastener IW 1266","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.15","Sash fastener IW 1267","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.16","Casement fastener IW 1269","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.2.17","Curved casement fastener IW 1270","no",1,{"v":87.11091024000002,"d":"87.11"}]
[{"$nulls":4},0]
["10.2.18","Casement fastener wedge plate IW 1277","no",1,{"v":87.11091024000002,"d":"87.11"}]
[{"$nulls":4},0]
["10.2.19","Dual screw/ sash window lock","no",1,{"v":170.43438960000003,"d":"170.43"}]
[{"$nulls":4},0]
["10.2.20","100mm Brass cabin hook and eye","no",1,{"v":83.32347936000002,"d":"83.32"}]
[{"$nulls":4},0]
["10.2.21","150mm Brass cabin hook and eye including 70 x 70 x 20mm chamfered hardwood block twice oiled and plugged","no",1,{"v":117.41035728,"d":"117.41"}]
[{"$nulls":4},0]
["10.2.22","150mm Chromium plated cabin hook and eye","no",1,{"v":40.39926272000001,"d":"40.40"}]
[{"$nulls":4},0]
["10.2.23","150mm Chromium plated cabin hook and eye including 70 x 70 x 20mm chamfered hardwood block twice oiled and plugged","no",1,{"v":75.74861760000002,"d":"75.75"}]
[{"$nulls":4},0]
["10.2.24","Brass window handle  ","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
[null,"LOCKS",null,null,0]
[{"$nulls":4},0]
[10.3,"\"Union\" or equal and approved fixed to timber",null,null,0]
[{"$nulls":4},0]
["10.3.1","Two lever lockset (2 Keys) with striking plate fixed to metal Ref. No. CZ682-24-95CH / SC. Lockset with lock, handles and keys, complete","no",1,{"v":515.7773871462401,"d":"515.78"}]
[{"$nulls":4},0]
["10.3.2","Three lever lockset (2 Keys) with striking plate fixed to metal Ref. CZ682-24-52CH / SC.  Lockset with lock, handles and keys, complete","no",1,{"v":619.7852890188802,"d":"619.79"}]
[{"$nulls":4},0]
["10.3.3","Four lever lockset (2 Keys) with striking plate fixed to metal Ref. CZ682-24-61CH.  Lockset with lock, handles and keys, complete","no",1,{"v":752.6180648422401,"d":"752.62"}]
[{"$nulls":4},0]
["10.3.4","Double cylinder lockset (2 Keys) with striking plate fixed to metal Ref. CZ682-05-222CH. Lockset with lock, handles and keys, complete","no",1,{"v":796.8552575206403,"d":"796.86"}]
[{"$nulls":4},0]
["10.3.5","Combination Bishop Furniture Ref. No. AL684-24-95AS with key hole with Two lever lockset 2295-76SS (2 Keys) with striking plate fixed to metal","no",1,{"v":965.6837764275202,"d":"965.68"}]
[{"$nulls":4},0]
["10.3.6","Combination Bishop Furniture Ref. No. AL684-24-95AS with key hole with Three lever lockset 2252-76SS (2 Keys) with striking plate fixed to metal","no",1,{"v":1065.6719516595203,"d":"1,065.67"}]
[{"$nulls":4},0]
["10.3.7","Combination Bishop Furniture Ref. No. AL684-24-95AS with key hole with Four lever lockset 2252-76SS (2 Keys) with striking plate fixed to metal","no",1,{"v":1065.6719516595203,"d":"1,065.67"}]
[{"$nulls":4},0]
["10.3.8","Combination Bishop Furniture Double cylinder Ref. No. AL684-05AS with key hole with Cylinder Euro lockset L-2209-78SS (2 Keys) with striking plate fixed to metal","no",1,{"v":1284.7571533900805,"d":"1,284.76"}]
[{"$nulls":4},0]
["10.3.9","Oval knob cylinder lockset (2 Keys) with striking plate fixed to metal Ref. AL684-05-222AS / IW2122","no",1,{"v":608.51389472,"d":"608.51"}]
[{"$nulls":4},0]
["10.3.10","Oval half knob cylinder lockset (2 Keys) with striking plate fixed to metal Ref. AL684-05-222AS / IW2122","no",1,{"v":597.1516020800002,"d":"597.15"}]
[{"$nulls":4},0]
["10.3.11","Cylinder deadlockset (2 Keys) with striking plate fixed to metal Ref. IW 2019","no",1,{"v":549.1774776000001,"d":"549.18"}]
[{"$nulls":4},0]
["10.3.12","Two lever lockset 2295-76SS (2 Keys) with striking plate fixed to metal","no",1,{"v":293.2986473472001,"d":"293.30"}]
[{"$nulls":4},0]
["10.3.13","Three lever lockset 2252-76SS (2 Keys) with striking plate fixed to metal","no",1,{"v":393.28682257920013,"d":"393.29"}]
[{"$nulls":4},0]
["10.3.14","Four lever lockset 22313-7615MMCH (2 Keys) with striking plate fixed to metal","no",1,{"v":393.28682257920013,"d":"393.29"}]
[{"$nulls":4},0]
["10.3.15","Rebated conversion set Ref No IW 2140  / UDY2900SS fixed to timber door","no",1,{"v":288.85472844800006,"d":"288.85"}]
[{"$nulls":4},0]
["10.3.16","Cylinder rim night latch Ref No 1022G Dimple keyway","no",1,{"v":621.3204610022401,"d":"621.32"}]
[{"$nulls":4},0]
["10.3.17","Union LX 3261 security gate lock box","no",1,{"v":578.2144476800001,"d":"578.21"}]
[{"$nulls":4},0]
["10.3.18","Master key","no",1,{"v":151.49723520000003,"d":"151.50"}]
[{"$nulls":4},0]
["10.3.19","Cylinder rim night latch Ref No 1022G-KB, KB502 keyway","no",1,{"v":410.6181062860801,"d":"410.62"}]
[{"$nulls":4},0]
["10.3.20","Union EP Cylinder upright lock Ref No L-2215-78SS/SL","no",1,{"v":286.3095748966401,"d":"286.31"}]
[{"$nulls":4},0]
["10.3.21","Union EP Knob Cylinder MKD SC Code: 2x19SCMKD","no",1,{"v":385.79275934464005,"d":"385.79"}]
[{"$nulls":4},0]
["10.3.22","Campus lockset 72mm centres Code SS6D67L-05CAM72 LH / RH","no",1,{"v":890.8037429760002,"d":"890.80"}]
[{"$nulls":4},0]
["10.3.23","52 Union Cylinder Cupboard lock (22/25/32/38mm), Code: 452-NP","no",1,{"v":431.1409317478401,"d":"431.14"}]
[{"$nulls":4},0]
["10.3.24","15CB Union Cylinder Cupboard drawer lock (22/25/32/38mm), Code: 415-64L/1 or 415-64R/1","no",1,{"v":46.943943280640006,"d":"46.94"}]
[{"$nulls":4},0]
["10.3.25","Union Rim Dimple key lock Code: 1x1SDD","no",1,{"v":235.74989760256003,"d":"235.75"}]
[{"$nulls":4},0]
["10.3.26","Union Cylinder Rim Lock GMKSC Code: 1x1SCGMK","no",1,{"v":396.61976175360013,"d":"396.62"}]
[{"$nulls":4},0]
["10.3.27","Container Double Glass door lock Code: M89100711R","no",1,{"v":1615.9705088000005,"d":"1,615.97"}]
[{"$nulls":4},0]
["10.3.28","Heavy duty Digital Rim lock with Over Keys, Code: MDL2735SC","no",1,{"v":1291.62502805248,"d":"1,291.63"}]
[{"$nulls":4},0]
["10.3.29","Heavy duty Escutcheons Code B-3G110-SS-P300","no",1,{"v":302.99447040000007,"d":"302.99"}]
[{"$nulls":4},0]
["10.3.30","Cam Locks 60 Series for cupboards and drawers K37/B44 KD, Code: LA1106R","no",1,{"v":54.993496377600025,"d":"54.99"}]
[{"$nulls":4},0]
["10.3.31","Cam Locks 60 Series for cupboards and drawers X44 DR KD, Code: LB7130R","no",1,{"v":58.073940160000014,"d":"58.07"}]
[{"$nulls":4},0]
["10.3.32","L&T locking handles 38mm Rose & 3PLD Code: LL3209R","no",1,{"v":134.32754854400002,"d":"134.33"}]
[{"$nulls":4},0]
["10.3.33","L&T locking handles T46 Re ATD Master C/P Code: LM1806R","no",1,{"v":175.49439725568007,"d":"175.49"}]
[{"$nulls":4},0]
["10.3.34","L&T locking handles K48 Lem Knob handle + 3PLD, Code LN2422/R","no",1,{"v":161.59705088000004,"d":"161.60"}]
[{"$nulls":4},0]
["10.3.35","Gate lock N201 Security lock with face plate, Code: LH4115/R","no",1,{"v":302.99447040000007,"d":"302.99"}]
[{"$nulls":4},0]
["10.3.36","Sliding door lock N201-1, Code: LH4145/R","no",1,{"v":222.19594496000002,"d":"222.20"}]
[{"$nulls":4},0]
["10.3.36a","Gate lock N888 Security lock with Cylinder and welded lock box, Code: LH8883","no",1,{"v":486.38692351744015,"d":"486.39"}]
[{"$nulls":4},0]
["10.3.36b","Locksmith to open Mortice lock and provide one key","no",1,{"v":209.02330800000001,"d":"209.02"}]
[{"$nulls":4},0]
["10.3.37","Locksmith to open Cylinder lock and provide one key","no",1,{"v":232.84362800000005,"d":"232.84"}]
[{"$nulls":4},0]
["10.3.38","Locksmith to open Cupboards, etc lock and provide one key","no",1,{"v":161.38266800000002,"d":"161.38"}]
[{"$nulls":4},0]
["10.3.39","Locksmith to open Mortice Cylinder lock and provide one key","no",1,{"v":232.84362800000005,"d":"232.84"}]
[{"$nulls":4},0]
["10.3.40","Locksmith to open Safe lock and provide one key","no",1,{"v":441.8669360000001,"d":"441.87"}]
[{"$nulls":4},0]
[10.4,"HANDLES, ETC.",null,null,0]
[{"$nulls":4},0]
[null,"\"IW\" or equal and approved fixed to timber",null,null,0]
[{"$nulls":4},0]
["10.4.1","\"UNION AL5D67-06AS\" OR \"IW 1324\" Dove pull handle for dead lock on 152 x 152mm backplate (One)","no",1,{"v":376.5211285504001,"d":"376.52"}]
[{"$nulls":4},0]
["10.4.6","Set of two \"IW 1320\" 300mm,25mm diameter Dove pull handles fixed back to back","no",1,{"v":738.5490216000001,"d":"738.55"}]
[{"$nulls":4},0]
["10.4.7","Set of two \"IW 1320\" 300mm,32mm diameter Dove pull handles fixed back to back","no",1,{"v":763.7985608000002,"d":"763.80"}]
[{"$nulls":4},0]
["10.4.8","Set of two lever handles Ref \"IW 1212/62/06\" fixed back to back","no",1,{"v":738.5490216000001,"d":"738.55"}]
[{"$nulls":4},0]
["10.4.9","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/62/06\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.10","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/62/05\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.11","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/62/13\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.12","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/62/24\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.13","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/63/06\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.14","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/63/05\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.15","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/63/13\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.16","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/63/24\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.17","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/66/06\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.18","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/66/05\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.19","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/66/13\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.20","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/66/24\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.21","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/67/06\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.22","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/67/05\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.23","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/67/13\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.24","Set of two lever handles with 3mm aluminium backplates Ref \"IW 1212/67/24\" fixed back to back","no",1,{"v":1129.9168792000003,"d":"1,129.92"}]
[{"$nulls":4},0]
["10.4.25","Euro profile IW2051 double cylinder lockset comprising IW1212/63/05 furniture and IW 2006 upright lockcase with striking plate","no",1,{"v":1243.5398056000004,"d":"1,243.54"}]
[{"$nulls":4},0]
["10.4.25a","Rebated conversion set","no",1,{"v":122.46026512000003,"d":"122.46"}]
[{"$nulls":4},0]
["10.4.25b","Aluminium Cupboard Pull handle Code: AL5123AS","no",1,{"v":96.95823052800004,"d":"96.96"}]
[{"$nulls":4},0]
["10.4.25c","Aluminium Hospital Pull handle Code: AL5510AS (One)","no",1,{"v":963.3810184524802,"d":"963.38"}]
[{"$nulls":4},0]
["10.4.25d","Aluminium 200 Pull handle BTB Code: AL5512-200BBAS (One)","no",1,{"v":313.34678147200003,"d":"313.35"}]
[{"$nulls":4},0]
["10.4.25e","Aluminium 300 Pull handle BTB Code: AL5512-300BBAS (One)","no",1,{"v":580.25461044736,"d":"580.25"}]
[{"$nulls":4},0]
["10.4.25f","Cedar Pull Handle Blank Code: AL5C63-06AS","no",1,{"v":298.6111503948801,"d":"298.61"}]
[{"$nulls":4},0]
["10.4.25g","Cedar Pull Handle on Back Plate LH/ RH Profile 152x152 Code: AL5C66L-05AS / AL5C66R-05AS","no",1,{"v":629.7639069107202,"d":"629.76"}]
[{"$nulls":4},0]
["10.4.25h","Cedar Pull Handle on Back Plate LH/ RH Profile 152x176 Code: AL5C67L-05AS  / AL5C67R-05AS","no",1,{"v":690.8273925120002,"d":"690.83"}]
[{"$nulls":4},0]
["10.4.25i","Stainless steel Dove Pull Handleon Back Plate LH / RH Key Hole 152x152 Plate Code: SS5D66L-24SS / SS5D66R-24SS","no",1,{"v":323.1941017600001,"d":"323.19"}]
[{"$nulls":4},0]
["10.4.25j","Stainless steel Dove Pull Handleon Back Plate LH / RH Key Hole 152x176 Plate Code: SS5D67L-24SS / SS5D67R-24SS","no",1,{"v":458.0872399820801,"d":"458.09"}]
[{"$nulls":4},0]
["10.4.25k","Flush Pull Handle Square - Wooden Sliding door, Code: 99004SS","no",1,{"v":103.62410887680002,"d":"103.62"}]
[{"$nulls":4},0]
["10.4.25l","Flush Pull Handle Radius - Wooden Sliding door, Code: SS5004SS","no",1,{"v":116.51147368448004,"d":"116.51"}]
[{"$nulls":4},0]
[null,"BOLTS",null,null,0]
[{"$nulls":4},0]
["10.4.26","Esco Rim lock night latch code EDY1033G","no",1,{"v":254.19216103424012,"d":"254.19"}]
[{"$nulls":4},0]
[null,"BATHROOM FITTINGS",null,null,0]
[{"$nulls":4},0]
[null,"\"IW\" or equal and approved fixed to timber",null,null,0]
[{"$nulls":4},0]
["10.4.27","Code IW7010SS surface mounted multi-roll (3)  toilet roll dispenser plugged","no",1,{"v":568.1146320000001,"d":"568.11"}]
[{"$nulls":4},0]
["10.4.28","Code IW7015SS wall mounted soap dispenser plugged","no",1,{"v":568.1146320000001,"d":"568.11"}]
[{"$nulls":4},0]
[null,"\"Bristell\" or equally approved",null,null,0]
[{"$nulls":4},0]
["10.4.29","32mm \"Bristell Type BGR1\" back grab rail 600mm long plugged","no",1,{"v":1181.6784345600004,"d":"1,181.68"}]
[{"$nulls":4},0]
["10.4.30","32mm \"Bristell Type BGR2A\" side grab rail 600mm long plugged","no",1,{"v":1127.3919252800004,"d":"1,127.39"}]
[{"$nulls":4},0]
[null,"SUNDRIES",null,null,0]
[{"$nulls":4},0]
[null,"\"IW\" or equal and approved fixed to timber",null,null,0]
[{"$nulls":4},0]
["10.4.31","Code No \"IW5002SC\" / Union CZ8731BP door stop plugged","no",1,{"v":72.94086884096001,"d":"72.94"}]
[{"$nulls":4},0]
["10.4.32","Code No \"IW5032AL\" / Union \"AL8253AS hat and coat hook with rubber tip","no",1,{"v":70.67851012864001,"d":"70.68"}]
[{"$nulls":4},0]
["10.4.33","Code No \"IW5042AL\" / Union \"AL8723AS hat and coat hook ","no",1,{"v":34.07677810432001,"d":"34.08"}]
[{"$nulls":4},0]
["10.4.34","Union code AL8254AS door stop 254/C91","no",1,{"v":208.056203008,"d":"208.06"}]
[{"$nulls":4},0]
["10.4.35","Union code AL8730AS door stop with rubber","no",1,{"v":135.41832863744006,"d":"135.42"}]
[{"$nulls":4},0]
["10.4.36","32mm Diameter polished hardwood longarm 2600mm long with brass pole hook on one end, two broom clips each with 20 x 100 x 100mm wrought and chamfered hardwood block twice oiled and plugged and 20 x 70 x 70mm wrought and chamfered hardwood block with sinking twice oiled and plugged (for opening windows)","no",1,{"v":410.3050120000001,"d":"410.31"}]
[{"$nulls":4},0]
[10.5,"PUSH PLATES \"Union\"",null,null,0]
[{"$nulls":4},0]
["10.5.1","200 x 800 x 2mm thick AL5089-200W aluminium push plate","no",1,{"v":339.60630224000005,"d":"339.61"}]
[{"$nulls":4},0]
["10.5.2","200 x 800 x 1,6mm thick SS5089-200W stainless steel push plate","no",1,{"v":465.8539982400001,"d":"465.85"}]
[{"$nulls":4},0]
["10.5.3","400 x 800 x 2mm thick AL5089-400W aluminium kick plate","no",1,{"v":604.7264638400002,"d":"604.73"}]
[{"$nulls":4},0]
["10.5.4","400 x 800 x 1,6mm thick SS5089-400W stainless steel kick plate","no",1,{"v":714.5619593600002,"d":"714.56"}]
[{"$nulls":4},0]
["10.5.5","152 x 76 Alluminium Push Plate Blank, Code: AL5063-06AS","no",1,{"v":117.54165488384001,"d":"117.54"}]
[{"$nulls":4},0]
["10.5.6","152 x 76 Alluminium Push Plate Keyhole, Code: AL5063-24AS","no",1,{"v":117.54165488384001,"d":"117.54"}]
[{"$nulls":4},0]
["10.5.7","152 x 152 Alluminium Push Plate Blank, Code: AL5066-06AS","no",1,{"v":155.79975667968003,"d":"155.80"}]
[{"$nulls":4},0]
["10.5.8","152 x 152 Alluminium Push Plate Keyhole, Code: AL5066-24AS","no",1,{"v":167.4549439744001,"d":"167.45"}]
[{"$nulls":4},0]
["10.5.9","152 x 152 Alluminium Push Plate LH / RH Bathroom, Code: AL5066TL-73AS / AL5066TR-73AS","no",1,{"v":590.9806146995202,"d":"590.98"}]
[{"$nulls":4},0]
["10.5.10","152 x 176 Alluminium Push Plate LH / RH Bathroom, Code: AL5067TL-73AS / AL5067TR-73AS","no",1,{"v":590.9806146995202,"d":"590.98"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"DOOR CLOSERS",null,null,0]
[{"$nulls":4},0]
[10.6,"\"Union\" fixed to timber",null,null,0]
[{"$nulls":4},0]
["10.6.1","\"Union\" Heavy duty regular arm door closer with bracket fixed to metal Ref. No DC 744 EN 1-6 RA DA Code: 744","no",1,{"v":6473.385961754881,"d":"6,473.39"}]
[{"$nulls":4},0]
["10.6.2","\"Union\" Heavy duty regular arm door closer with bracket fixed to metal Ref. No DC 744 EN 1-6 PA DA Code: 744P","no",1,{"v":6749.959314336001,"d":"6,749.96"}]
[{"$nulls":4},0]
["10.6.3","Heavy duty hold open arm door closer with bracket fixed to metal Ref. No DC 744 EN 1-6 HO DA, Code: 744HO","no",1,{"v":7972.428379473601,"d":"7,972.43"}]
[{"$nulls":4},0]
["10.6.4","Regular arm door closer with bracket fixed to metal Ref. No DC 777- EN 2-4 Code: 7770","no",1,{"v":959.9622308448,"d":"959.96"}]
[{"$nulls":4},0]
["10.6.5","Parallel arm door closer with bracket fixed to metal Ref. No DC 7772 OH EN 2-4, Code: 7772","no",1,{"v":1684.8007526592005,"d":"1,684.80"}]
[{"$nulls":4},0]
["10.6.6","Heavy duty double action floor spring Ref. NoFS 762 EN 3-6 HD DA TI, Code: 762 + with top centre Ref. No AC286 and bottom strap Ref. No AC278","no",1,{"v":15265.777977024962,"d":"15,265.78"}]
[{"$nulls":4},0]
["10.6.7","Heavy duty single action floor spring Ref. No FS 764 EN 3-6 HD LH TI Code: 764 + with top centre Ref. No AC286AS and bottom strap Ref. No AC278 (LH) or AC279 (RH)","no",1,{"v":15490.511500674564,"d":"15,490.51"}]
[{"$nulls":4},0]
["10.6.8","Regular duty double action floor spring Ref. No FS 749 EN 3 DA AL, CODE: 750 + with top centre Ref. No AC8 and bottom strap Ref. No AC115","no",1,{"v":8177.984878100802,"d":"8,177.98"}]
[{"$nulls":4},0]
["10.6.9","Regular duty single action floor spring Ref. No FS 754 EN 3 RH TI Code: 754 + with top centre Ref. No AC286CH and bottom strap Ref. No AC278 (RH) or AC279 (LH)","no",1,{"v":8891.741377160324,"d":"8,891.74"}]
[{"$nulls":4},0]
["10.6.10","Union Gate Closer Ref: 720 EN 2 Code: 720","no",1,{"v":3503.3735640000004,"d":"3,503.37"}]
[{"$nulls":4},0]
["10.6.11","Regular arm door closer with bracket fixed to metal Ref. No R&P CLOSER EN 2/3/4/SIL Code: DC120","no",1,{"v":791.2700594496,"d":"791.27"}]
[{"$nulls":4},0]
["10.6.12","Floor Springs Cam Action FS EN 3 Non HO, Code: DC420","no",1,{"v":6186.137104000001,"d":"6,186.14"}]
[{"$nulls":4},0]
[null,"SLIDING GEAR",null,null,0]
[{"$nulls":4},0]
[10.7,"\"UNION\" or equally approved",null,null,0]
[{"$nulls":4},0]
["10.7.1","Phantom sliding gear for silent doors up to 45kg width opening 610-915mm clinic cupboards Code: 27-792961","no",1,{"v":924.0119369318402,"d":"924.01"}]
[{"$nulls":4},0]
["10.7.2","Husky folding 25 for Folding doors up to 25kg maximum width 1200mm Kit Hf25/12 - 2 leaves","no",1,{"v":627.4409493043203,"d":"627.44"}]
[{"$nulls":4},0]
["10.7.3","Husky folding 25 for Folding doors up to 25kg maximum width 2400mm Kit Hf25/24 - 4 leaves","no",1,{"v":964.9565896985602,"d":"964.96"}]
[{"$nulls":4},0]
["10.7.4","Husky folding 40 for Folding doors up to 40kg maximum width 1500mm Kit Hf40/15 2 leaves","no",1,{"v":924.0119369318402,"d":"924.01"}]
[{"$nulls":4},0]
["10.7.5","Husky folding 40 for Folding doors up to 40kg maximum width 3000mm Kit Hf40/30 4 leaves","no",1,{"v":1559.1893450470407,"d":"1,559.19"}]
[{"$nulls":4},0]
["10.7.6","Senator kit for sliding doors up to 30kg for max 900mm opening width Ref 27-791065","no",1,{"v":437.3826178380801,"d":"437.38"}]
[{"$nulls":4},0]
["10.7.7","Marathon 55 kit for sliding doors up to 55kg for max 450-750mm opening width Ref 27-789400","no",1,{"v":621.9062503116801,"d":"621.91"}]
[{"$nulls":4},0]
["10.7.8","Marathon 55 kit for sliding doors up to 55kg for max 750-900mm opening width Ref 27-789431","no",1,{"v":693.8371375846402,"d":"693.84"}]
[{"$nulls":4},0]
["10.7.9","Marathon 55 kit for sliding doors up to 55kg for max 900-1050mm opening width Ref 27-789462","no",1,{"v":742.5182491622402,"d":"742.52"}]
[{"$nulls":4},0]
["10.7.10","Marathon 55 kit for sliding doors up to 55kg for max 1050-1200mm opening width Ref 27-789493","no",1,{"v":814.4491364352001,"d":"814.45"}]
[{"$nulls":4},0]
["10.7.11","Marathon 55 kit for sliding doors up to 55kg for max 1200-1500mm opening width Ref 27-790695","no",1,{"v":1015.8596607257602,"d":"1,015.86"}]
[{"$nulls":4},0]
["10.7.12","Loretto for Sliding cupboard doors up to 23kg - Bottom roller kit D4 - 2 leaves Max opening width 1200mm Ref 27-789280","no",1,{"v":703.1693672729601,"d":"703.17"}]
[{"$nulls":4},0]
["10.7.13","Loretto for Sliding cupboard doors up to 23kg - Bottom roller kit D5 - 2 leaves Max opening width 1500mm Ref 27-789314","no",1,{"v":758.6981538816002,"d":"758.70"}]
[{"$nulls":4},0]
["10.7.14","Loretto for Sliding cupboard doors up to 23kg - Bottom roller kit D6 - 2 leaves Max opening width 1800mm Ref 27-789345","no",1,{"v":821.0140166272002,"d":"821.01"}]
[{"$nulls":4},0]
["10.6.1","Phantom sliding gear set for single door with track 1,8m long fixed to wall including brackets, hangers, rollers, guides, stops, etc","no",1,0]
[{"$nulls":4},0]
["10.6.2","Husky 50 sliding gear set for double leaf door with track 3,2m long fixed to wall including brackets, hangers, rollers, guides, stops, etc","no",1,0]
[{"$nulls":4},0]
[null,"LETTERS, NAMEPLATES, ETC.",null,null,0]
[{"$nulls":4},0]
[10.8,"\"Union\"",null,null,0]
[{"$nulls":4},0]
["10.8.1","152  x 152 x 3mm aluminium plate anodised silver with male pictogram Ref. No. AL5063E-06ASE10","no",1,{"v":184.32163616000005,"d":"184.32"}]
[{"$nulls":4},0]
["10.8.2","152  x 152 x 3mm aluminium plate anodised silver with female pictogram Ref. No. AL5063E-06ASE11","no",1,{"v":184.32163616000005,"d":"184.32"}]
[{"$nulls":4},0]
["10.8.3","152  x 152 x 3mm aluminium plate anodised silver with paraplegic pictogram Ref. No. AL5066E-06ASE14","no",1,{"v":184.32163616000005,"d":"184.32"}]
[{"$nulls":4},0]
["10.8.4","152  x 152 x 3mm aluminium plate anodised silver with male and female pictogram Ref. No. AL5066E-06ASE12","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.5","152  x 152 x 3mm aluminium plate anodised silver with fire hydrant pictogram Ref. No. AL5066E-06ASE04","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.6","152  x 152 x 3mm aluminium plate anodised silver with fire hose reel pictogram Ref. No. AL5066E-06ASE05","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.7","152  x 152 x 3mm aluminium plate anodised silver with fire extinguisher pictogram Ref. No. AL5066E-06ASE06","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.8","152  x 152 x 3mm aluminium plate anodised silver with first aid pictogram Ref. No. IW6018","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.9","152  x 152 x 3mm aluminium plate anodised silver with shower pictogram Ref. No. IW6018","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.10","152  x 152 x 3mm aluminium plate anodised silver with shower pictogram Ref. No. IW6006","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.11","152  x 152 x 3mm aluminium plate anodised silver with tea room pictogram Ref. No. IW6006","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.12","152  x 152 x 3mm aluminium plate anodised silver with telephone pictogram Ref. No. IW6006","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.13","152  x 152 x 3mm aluminium plate anodised silver with man running left or right pictogram Ref. No. IW6012","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.14","152  x 152 x 3mm aluminium plate anodised silver with escape stair pictogram Ref. No. IW6013","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.15","152  x 152 x 3mm aluminium plate anodised silver with escape direction pictogram Ref. No. IW6014","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.16","152  x 152 x 3mm aluminium plate anodised silver with bucket and broom pictogram Ref. No. IW6011","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.17","152  x 152 x 3mm aluminium plate anodised silver with bbaby pictogram Ref. No. IW6004","no",1,{"v":186.84659008000003,"d":"186.85"}]
[{"$nulls":4},0]
["10.8.18","COJ Logo: Brushed alluminium 1000 x 800mm deep plugged with alluminium bolts with engraved letters","no",1,{"v":2524.953920000001,"d":"2,524.95"}]
[{"$nulls":4},0]
["10.8.19","COJ Logo: Brushed alluminium 500 x 300mm deep plugged with alluminium bolts  with engraved letters","no",1,{"v":1514.9723520000002,"d":"1,514.97"}]
[{"$nulls":4},0]
["10.8.20","1000 x 152 x 3mm brushed aluminium plate with engraved letters","m2",1,{"v":1262.4769600000004,"d":"1,262.48"}]
[{"$nulls":4},0]
["10.8.21","100  x 450 x 3mm aluminium plate anodised silver with Name Tags not exceeding 20 letters","no",1,{"v":363.5933644800001,"d":"363.59"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"PELMETS AND CERTAIN TRACKS",null,null,0]
[{"$nulls":4},0]
[10.9,"\"Kirsch\"",null,null,0]
[{"$nulls":4},0]
["10.9.1","Cheney pressed steel pelmet 120mm high with 150mm projection including  double track with 12 rollers per meter, brackets, returned ends, etc. plugged","m",1,{"v":109.83549552000002,"d":"109.84"}]
[{"$nulls":4},0]
["10.9.2","Regular duty C-profile double curtain  steel track for face fixing with 100mm projection including 14 rollers per meter, brackets, stopped ends, etc. plugged","m",1,{"v":124.35398056000002,"d":"124.35"}]
[{"$nulls":4},0]
["10.9.3","Heavy duty extruded aluminium double curtain  steel track for face fixing with 125mm projection including 14 rollers per meter, brackets, stopped ends, etc. plugged","no",1,{"v":138.87246560000006,"d":"138.87"}]
[{"$nulls":4},0]
["10.9.4","Forwin hospital cubicle track 1.0m below soffit including 12 gliders per meter, hangers, brackets, stopped ends, etc. plugged","no",1,{"v":212.09612928000007,"d":"212.10"}]
[{"$nulls":4},0]
["10.9.5","Extra for end plugged","no",1,{"v":73.22366368000002,"d":"73.22"}]
[{"$nulls":4},0]
["10.9.6","Extra for bend","no",1,{"v":73.22366368000002,"d":"73.22"}]
[{"$nulls":4},0]
["10.9.7","Extra for joint at bend","no",1,{"v":73.22366368000002,"d":"73.22"}]
[{"$nulls":4},0]
["10.8.1","Cheney pressed steel pelmet 120mm high with 150 projection including double curtain track with 12 rollers per meter, brackets, returned ends, etc plugged","m",1,0]
[{"$nulls":4},0]
["10.8.2","Regular duty C-profile double curtain steel track for face fixing with 100mm projection including 14 rollers per meter, brackets, stopped ends, etc plugged","m",1,0]
[{"$nulls":4},0]
["10.8.3","Heavy duty extruded aluminium double curtain track for face fixing with 125mm projection including 14 rollers per meter, brackets, stopped ends, etc plugged","m",1,0]
[{"$nulls":4},0]
["10.8.4","Forwin hospital cubicle track 1,0m below soffit including 12 gliders per meter, hangers, brackets, stopped ends, etc plugged","m",1,0]
[{"$nulls":4},0]
["10.8.5","Extra over hospital cubicle track for end plugged","no",1,0]
[{"$nulls":4},0]
["10.8.6","Extra over hospital cubicle track for bend","no",1,0]
[{"$nulls":4},0]
["10.8.7","Extra over hospital cubicle track for joint at bend","no",1,0]
[{"$nulls":4},0]
[null,"BATHROOM FITTINGS",null,null,0]
[{"$nulls":4},0]
[{"v":10.1,"d":"10.10"},"\"Halcast\"",null,null,0]
[{"$nulls":4},0]
["10.10.1","20mm Diameter chromium plated curtain or hanging rail 900mm long including end flange brackets Ref 374CH plugged","no",1,{"v":246.18300720000008,"d":"246.18"}]
[{"$nulls":4},0]
["10.10.2","20mm Diameter chromium plated towel rail 600mm long including end brackets Ref 261CH plugged","no",1,{"v":214.62108320000004,"d":"214.62"}]
[{"$nulls":4},0]
["10.10.3","20mm Diameter chromium plated towel rail 900mm long including end brackets Ref 261CH plugged","no",1,{"v":324.4565787200001,"d":"324.46"}]
[{"$nulls":4},0]
["10.10.4","Towel ring chromium plated Ref 165CH plugged","no",1,{"v":170.43438960000003,"d":"170.43"}]
[{"$nulls":4},0]
["10.10.5","Toilet roll holder chromium plated theft proof Ref 366SCH plugged","no",1,{"v":699.4122358400001,"d":"699.41"}]
[{"$nulls":4},0]
["10.10.6","Basket type soap dish chromium plated Ref  377CH","no",1,{"v":296.68208560000005,"d":"296.68"}]
[{"$nulls":4},0]
["10.9.1","20mm. diameter chromium plated curtain or hanging rail 900mm. Long including end flange brackets Ref. 374CH plugged","no",1,0]
[{"$nulls":4},0]
["10.9.2","20mm. diameter chromium plated towel rail 600mm. Long including end brackets Ref. 261CH plugged","no",1,0]
[{"$nulls":4},0]
["10.9.3","20mm. diameter chromium plated towel rail 900mm. Long including end brackets Ref. 261CH plugged","no",1,0]
[{"$nulls":4},0]
["10.9.4","Towel ring chromium plated Ref 165CH plugged","no",1,0]
[{"$nulls":4},0]
["10.9.5","Toilet roll holder chromium plated thief proof Ref. 366SCH plugged","no",1,0]
[{"$nulls":4},0]
["10.9.6","Basket type soap dish chromium plated Ref. 377CH plugged","no",1,0]
[{"$nulls":4},0]
[10.11,"\"Kwakuhle Hygiene\" of equal and approved",null,null,0]
[{"$nulls":4},0]
["10.11.1","Lockable and vandal resistant white powder coated metal roll holder Ref TR3W","no",1,{"v":699.4122358400001,"d":"699.41"}]
[{"$nulls":4},0]
["10.11.2","Lockable and vandal resistant white powder coated metal roll holder Ref TR2W","no",1,{"v":770.1109456000002,"d":"770.11"}]
[{"$nulls":4},0]
["10.11.3","Lockable and vandal resistant white powder coated metal roll holder Ref TR3CH","no",1,{"v":814.2976392000002,"d":"814.30"}]
[{"$nulls":4},0]
["10.11.4","Lockable and vandal resistant white powder coated metal roll holder Ref TR2CH","no",1,{"v":699.4122358400001,"d":"699.41"}]
[{"$nulls":4},0]
["10.11.5","ABS construction lockable Roll Control Paper Dispenser with viewing  window in colour white","no",1,{"v":1041.543492,"d":"1,041.54"}]
[{"$nulls":4},0]
["10.11.6","ABS construction lockable Reflex Paper Dispenser with viewing  window in colour white","no",1,{"v":1041.543492,"d":"1,041.54"}]
[{"$nulls":4},0]
["10.11.7","ABS construction Wastecare 40litre Multiliner Disposer wall mounted waste bin in colour white","no",1,{"v":435.5545512000001,"d":"435.55"}]
[{"$nulls":4},0]
["10.11.8","ABS construction 950ml Soap Dispenser in colour white","no",1,{"v":517.6155536000001,"d":"517.62"}]
[{"$nulls":4},0]
["10.11.9","Stainless steel 950ml vandal and theft resistant Soap Dispenser","no",1,{"v":991.0444136000001,"d":"991.04"}]
[{"$nulls":4},0]
["10.10.1","Lockable and vandal resistant white powder coated metal toilet roll holder Ref. TR3W plugged","no",1,0]
[{"$nulls":4},0]
["10.10.2","Lockable and vandal resistant  white powder coated metal toilet roll holder Ref. TR2W plugged","no",1,0]
[{"$nulls":4},0]
["10.10.3","Lockable and vandal resistant  chromium plated toilet roll holder Ref. TR3CH plugged","no",1,0]
[{"$nulls":4},0]
["10.10.4","Lockable and vandal resistant  chromium plated toilet roll holder Ref. TR2CH plugged","no",1,0]
[{"$nulls":4},0]
["10.10.5","ABS construction lockable Roll Control Paper Dispenser with viewing window in colour white","no",1,0]
[{"$nulls":4},0]
["10.10.6","ABS construction lockable Reflex Paper Dispenser with viewing window in colour white","no",1,0]
[{"$nulls":4},0]
["10.10.7","ABS construction Wastecare 40 litre Multiliner Disposer wall mounted waste bin in colour White","no",1,0]
[{"$nulls":4},0]
["10.10.8","ABS construction 950 ml Soap Dispenser in colour white","no",1,0]
[{"$nulls":4},0]
["10.10.9","Stainless steel 950 ml vandal and theft resistant Soap Dispenser","no",1,0]
[{"$nulls":4},0]
[10.12,"\"Chairman Industries\"",null,null,0]
[{"$nulls":4},0]
["10.12.1","32mm diameter stainless steel flushvalve back rail Ref. No. SR1","no",1,{"v":898.8835955200002,"d":"898.88"}]
[{"$nulls":4},0]
["10.12.2","32mm diameter stainless steel cistern back rail Ref. No. SR2","no",1,{"v":1074.3678929600003,"d":"1,074.37"}]
[{"$nulls":4},0]
["10.12.3","20mm diameter stainless steel door rail 300mm long Ref. No. SR3","no",1,{"v":555.4898624000002,"d":"555.49"}]
[{"$nulls":4},0]
["10.12.4","32mm diameter stainless steel dog leg side rail Ref. No. DL2","no",1,{"v":1127.3919252800004,"d":"1,127.39"}]
[{"$nulls":4},0]
["10.12.5","32mm diameter stainless steel dog leg with centre flange side rail Ref. No. DL3","no",1,{"v":1181.6784345600004,"d":"1,181.68"}]
[{"$nulls":4},0]
["10.12.6","19mm Diameter chromium plated towel rail 500mm long including end brackets plugged","no",1,{"v":302.99447040000007,"d":"302.99"}]
[{"$nulls":4},0]
["10.12.7","\"Bobrick\" B-4388 Surface mounted lockable multi-roll toilet tissue dispenser plugged","no",1,{"v":1249.8521904000004,"d":"1,249.85"}]
[{"$nulls":4},0]
["10.12.8","Wall mounted stainless steel dispenser Ref \"IW 7015\"","no",1,{"v":574.4270168000002,"d":"574.43"}]
[{"$nulls":4},0]
[10.13,"PADLOCKS",null,null,0]
[{"$nulls":4},0]
["10.13.1","30mm Brass Padlocks with 15mm Hardened Steel Shackle KD, Code: UN333000000000","no",1,{"v":169.26028602720007,"d":"169.26"}]
[{"$nulls":4},0]
["10.13.2","30mm Brass Padlocks with 32mm SS Long Shackle KD, Code: UN333002003200","no",1,{"v":176.83514778720004,"d":"176.84"}]
[{"$nulls":4},0]
["10.13.3","40mm Brass Padlocks with 20mm Hardened Steel Shackle KD, Code: UN334000000000","no",1,{"v":186.94758823680002,"d":"186.95"}]
[{"$nulls":4},0]
["10.13.4","40mm Brass Padlocks with 63mm SS Long Shackle KD, Code: UN334002006300","no",1,{"v":224.84083419120003,"d":"224.84"}]
[{"$nulls":4},0]
["10.13.5","50mm Brass Padlocks with 28mm Hardened Steel Shackle KD, Code: UN335000000000","no",1,{"v":296.4093905766401,"d":"296.41"}]
[{"$nulls":4},0]
["10.13.6","50mm Brass Padlocks with 63mm SS Long Shackle KD, Code: UN335002006300","no",1,{"v":328.4081316048,"d":"328.41"}]
[{"$nulls":4},0]
["10.13.7","Discus Padlock KD, Code: 400KATD","no",1,{"v":145.15328847600006,"d":"145.15"}]
[{"$nulls":4},0]
["10.13.8","78mm Brass Padlocks Concealed Hardened Steel Shackle KD Code: UN337800000000","no",1,{"v":671.9849238840002,"d":"671.98"}]
[{"$nulls":4},0]
["10.13.9","Padlock safety lockout device 6 Hole","no",1,{"v":94.31207881984002,"d":"94.31"}]
[{"$nulls":4},0]
["10.13.10","Gate Hasp Lock Classic Code: MCHBT-COM","no",1,{"v":5300.635764256,"d":"5,300.64"}]
[{"$nulls":4},0]
["10.13.11","Hercules Padlock3 Keys, B-1K57A","no",1,{"v":5268.316354080001,"d":"5,268.32"}]
[{"$nulls":4},0]
[10.14,"ESCAPE HARDWARE \"EMERGENCY\"",null,null,0]
[{"$nulls":4},0]
["10.14.1","Emergency exit lockset (2 Keys) with striking plate fixed to metal Ref. IW 2032","no",1,{"v":662.8004040000001,"d":"662.80"}]
[{"$nulls":4},0]
["10.14.2","Emergency exit lockset (2 Keys) with striking plate fixed to metal Ref. IW 2033","no",1,{"v":662.8004040000001,"d":"662.80"}]
[{"$nulls":4},0]
["10.14.3","Panic Latch push bar 900mm Code: J-881-SIL","no",1,{"v":2873.4177605913605,"d":"2,873.42"}]
[{"$nulls":4},0]
["10.14.4","Panic Latch push bar 1200mm Code: J-881-W-SIL","no",1,{"v":2974.8805089126404,"d":"2,974.88"}]
[{"$nulls":4},0]
["10.14.5","Panic Latch Touch Bar 900mm Code: J-881T-SIL","no",1,{"v":4292.1994680550415,"d":"4,292.20"}]
[{"$nulls":4},0]
["10.14.5a","Panic Latch push bar 1200mm Code: J-881T-W-SIL","no",1,{"v":4726.7137382400015,"d":"4,726.71"}]
[{"$nulls":4},0]
["10.14.6","Double panic bolt with pullman Latch Green 1940908NV","no",1,{"v":7790.745320160001,"d":"7,790.75"}]
[{"$nulls":4},0]
["10.14.7","Double panic bolt Push bar 900mm Code: J-883-SIL","no",1,{"v":7553.292341138401,"d":"7,553.29"}]
[{"$nulls":4},0]
["10.14.8","Double panic bolt Push bar 1200mm Code: J-883-W-SIL","no",1,{"v":8148.657538320002,"d":"8,148.66"}]
[{"$nulls":4},0]
["10.14.9","Audible Panic latch alarm exit device Code: 8420RED",null,1,{"v":14329.744734480004,"d":"14,329.74"}]
[{"$nulls":4},0]
["10.14.10","Outside acces device (OAD) for J-series & Tesa panic devices Lever handle Code: MMPS2SCPL","no",1,{"v":1131.1793561600002,"d":"1,131.18"}]
[{"$nulls":4},0]
["10.14.11","Outside acces device (OAD) for J-series panic devices Lever handle Code: J-885-SIL","no",1,{"v":1227.85479184896,"d":"1,227.85"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["10.17.1","Guardsman Baseline Locker 300 x 450 x 1800mm high Code GB004","no",1,0]
[{"$nulls":4},0]
["10.17.2","Extra for bolting lockers together","no",1,0]
[{"$nulls":4},0]
[null,"KITCHEN CUPBOARDS",null,null,0]
[{"$nulls":4},0]
[10.15,"\"Duracraft\" kitchen cupboards plugged",null,null,0]
[{"$nulls":4},0]
["10.15.1","Wall cupboard Type WHU300 - 300 x 300 x 800mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":747.3863603200001,"d":"747.39"}]
[{"$nulls":4},0]
["10.15.2","Wall cupboard Type WHU450 - 450 x 300 x 800mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":811.7726852800002,"d":"811.77"}]
[{"$nulls":4},0]
["10.15.3","Wall cupboard Type WHU525 - 525 x 300 x 800mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":934.2329504000003,"d":"934.23"}]
[{"$nulls":4},0]
["10.15.4","Wall cupboard Type WHU900 - 900 x 300 x 800mm high with top, sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":1329.3882388800002,"d":"1,329.39"}]
[{"$nulls":4},0]
["10.15.5","Wall cupboard Type WHU1200 - 1200 x 300 x 800mm high with top, sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":1622.2828936000005,"d":"1,622.28"}]
[{"$nulls":4},0]
["10.15.6","Wall cupboard Type WCU525 (corner unit) - 525 x 300 x 800mm high with top, sides, bottom, division, shelf, back and single hinged door","no",1,{"v":1227.1276051200005,"d":"1,227.13"}]
[{"$nulls":4},0]
["10.15.7","Floor cupboard Type BU300 - 300 x 530 x 875mm high with sides, bottom, division, shelf, and single hinged door (top elsewhere)","no",1,{"v":1109.7172478400003,"d":"1,109.72"}]
[{"$nulls":4},0]
["10.15.8","Floor cupboard Type BU450 - 450 x 530 x 875mm high with sides, bottom, division, shelf, and single hinged door (top elsewhere)","no",1,{"v":1181.6784345600004,"d":"1,181.68"}]
[{"$nulls":4},0]
["10.15.9","Floor cupboard Type BU525 - 525 x 530 x 875mm high with sides, bottom, division, shelf, and single hinged door (top elsewhere)","no",1,{"v":1271.3142987200004,"d":"1,271.31"}]
[{"$nulls":4},0]
["10.15.10","Floor cupboard Type BU900 - 900 x 530 x 875mm high with sides, bottom, division, shelf, and double hinged doors (top elsewhere)","no",1,{"v":2245.9465118400003,"d":"2,245.95"}]
[{"$nulls":4},0]
["10.15.11","Floor cupboard Type BU1200 - 1200 x 530 x 875mm high with sides, bottom, division, shelf, and double hinged doors (top elsewhere)","no",1,{"v":2695.3883096,"d":"2,695.39"}]
[{"$nulls":4},0]
["10.15.12","Floor cupboard Type BU450/1 - 450 x 530 x 875mm high with sides, bottom, division, shelf, and single hinged door, dividing framework and 1 drawer (top elsewhere)","no",1,{"v":1389.98713296,"d":"1,389.99"}]
[{"$nulls":4},0]
["10.15.13","Floor cupboard Type BU450/4 - 450 x 530 x 875mm high with sides, bottom, division framework and 4 drawer (top elsewhere)","no",1,{"v":2309.0703598400005,"d":"2,309.07"}]
[{"$nulls":4},0]
["10.15.14","Floor cupboard Type BCU825 (corner unit) - 825 x 530 x 875mm high with sides, bottom, division, shelf, back and double hinged doors","no",1,{"v":3302.639727360001,"d":"3,302.64"}]
[{"$nulls":4},0]
["10.15.15","Floor cupboard Type BB450 - 450 x 530 x 2160mm high with top, sides, bottom, division, 2 shelves, back and single hinged door","no",1,{"v":2225.7468804800005,"d":"2,225.75"}]
[{"$nulls":4},0]
["10.15.16","Sink cupboard Type HSU900 - 900 x 530 x 875mm high with sides, bottom, division, shelf, back and double hinged doors (sink elsewhere)","no",1,{"v":2527.4788739200003,"d":"2,527.48"}]
[{"$nulls":4},0]
["10.15.17","Sink cupboard Type HSU1200 - 1200 x 530 x 875mm high with sides, bottom, division, shelf, back and double hinged doors (sink elsewhere)","no",1,{"v":3281.177619040001,"d":"3,281.18"}]
[{"$nulls":4},0]
["10.15.18","Sink cupboard Type HSU1500 (double bowl) - 1500 x 530 x 875mm high with sides, bottom, division, shelf, back and double hinged doors (sink elsewhere)","no",1,{"v":5330.177725120002,"d":"5,330.18"}]
[{"$nulls":4},0]
["10.15.19","Extra over kitchen cupboards for Top \"T\" joints","no",1,{"v":78.27357152000002,"d":"78.27"}]
[{"$nulls":4},0]
["10.15.20","Extra over kitchen cupboards for filler piece","no",1,{"v":75.74861760000002,"d":"75.75"}]
[{"$nulls":4},0]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
["10.15.21","Sliding drawer rail 600mm long","m",1,{"v":78.90481000000003,"d":"78.90"}]
[{"$nulls":4},0]
["10.15.22","Steel drawer handle","no",1,{"v":75.74861760000002,"d":"75.75"}]
[{"$nulls":4},0]
["10.15.23","PVC drawer handle","no",1,{"v":61.230132560000015,"d":"61.23"}]
[{"$nulls":4},0]
["10.15.24","PVC drawer handle","no",1,{"v":61.230132560000015,"d":"61.23"}]
[{"$nulls":4},0]
["10.15.25","Cast Zinc Cupboard Pull Handle Code: CZ5105CH","no",1,{"v":100.99815680000003,"d":"101.00"}]
[{"$nulls":4},0]
["10.15.26","Cast Zinc Cupboard Push Button Catch Code: CZ51741CH","no",1,{"v":199.99655009536008,"d":"200.00"}]
[{"$nulls":4},0]
["10.15.27","Cast Zinc Locking Cupboard Catch Code: CZ5174CHKA","no",1,{"v":293.78343849984003,"d":"293.78"}]
[{"$nulls":4},0]
[10.16,"Turnstile and Locking Exit Gate",null,null,0]
[{"$nulls":4},0]
["10.16.1","Stainless steel one-way supermarket entrance turnstile","no",1,{"v":5494.804720704,"d":"5,494.80"}]
[{"$nulls":4},0]
["10.16.2","Single locking exit gate for M3501","no",1,{"v":16764.179056448,"d":"16,764.18"}]
[{"$nulls":4},0]
["10.16.3","Service and make good stainless steel one-way supermarket entrance turnstile","no",1,{"v":865.4279560800002,"d":"865.43"}]
[{"$nulls":4},0]
[10.17,"Infra-red beam system",null,null,0]
[{"$nulls":4},0]
["10.17.1","Infra-red beam system","no",1,{"v":8946.593476118403,"d":"8,946.59"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[null,"TOILET BINS",null,null,0]
[{"$nulls":4},0]
[null,"Stainless steel",null,null,0]
[{"$nulls":4},0]
[10.18,"\"FRANKE\" or equally approved",null,null,0]
[{"$nulls":4},0]
["10.18.1","Half moon wall mounted bin size 330 x 450 x 180mm","no",1,{"v":1807.3367663968002,"d":"1,807.34"}]
[{"$nulls":4},0]
["10.18.2","Wall mounted 430 grade brushed  one piece  with internal steel frame inside for disposable liner bin size 415 x 450 x 200mm","no",1,{"v":1156.1511504288003,"d":"1,156.15"}]
[{"$nulls":4},0]
["10.18.3","Wall mounted 430 grade brushed  one piece  with internal steel frame inside for disposable liner bin size 310 x 300 x 200mm","no",1,{"v":850.5054784128,"d":"850.51"}]
[{"$nulls":4},0]
[null,"Epoxy coated",null,null,0]
[{"$nulls":4},0]
[10.19,"\"FRANKE\" or equally approved",null,null,0]
[{"$nulls":4},0]
["10.19.1","Wall mounted mild steel  one piece  with internal steel frame inside for disposable liner bin size 415 x 450 x 200mm","no",1,{"v":690.8905163600001,"d":"690.89"}]
[{"$nulls":4},0]
["10.19.2","Wall mounted mild steel  one piece  with internal steel frame inside for disposable liner bin size 310 x 300 x 200mm","no",1,{"v":598.0100864128002,"d":"598.01"}]
{"$rows_empty":26}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Metalwork","index":10,"n_rows":677,"n_cols":7,"rows_kept":677,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 11"]
[]
[null,"METALWORK"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Descriptions"]
[]
[null,"Descriptions of bolts shall be deemed to include nuts and washers"]
[]
[null,"Descriptions of expansion anchors and bolts an chemical anchors and bolts shall be deemed to include nuts, washers and mortises in brickwork or concrete"]
[]
[null,"Metalwork described as \"holed for bolts(s)\" shall be deemed to exclude the bolts unless otherwise described"]
[]
[null,"STEEL HANDRAILS, BALUSTRADES, ETC"]
[]
[11.1,"Welded handrail to mild steel"]
[]
["11.1.1","80 x 40 x 2,0mm hollow section continuous rails with flat closed ends welded to bracket, formed of 25mm diameter bar 100mm girth once bent to 50mm internal radius, at approximately 1200mm centres each with 80mm diameter by 6mm thick plate twice holed for bolts ","m",1,{"v":674.7105640000001,"d":"674.71"}]
[{"$nulls":4},0]
["11.1.2","Extra over 80 x 40 x 2mm hollow section for mitred L-intersection","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.1.3","38 x 38 x 2,0mm hollow section continuous rails with flat closed ends welded to bracket, formed of 25mm diameter bar 100mm girth once bent to 50mm internal radius, at approximately 1200mm centres each with 80mm diameter by 6mm thick plate twice holed for bolts ","m",1,{"v":564.3033808000001,"d":"564.30"}]
[{"$nulls":4},0]
["11.1.4","Extra over 38 x 38 x 2mm hollow section for mitred L-intersection","no",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["11.1.5","76mm diameter 2,0mm hollow section continuous rails with flat closed ends welded to bracket, formed of 25mm diameter bar 100mm girth once bent to 50mm internal radius, at approximately 1200mm centres each with 80mm diameter by 6mm thick plate twice holed for bolts ","m",1,{"v":625.6407048,"d":"625.64"}]
[{"$nulls":4},0]
["11.1.6","Extra over 76mm pipe rail for bend to 200mm Internal radius","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.1.7","38mm diameter 2,0mm hollow section continuous rails with flat closed ends welded to bracket, formed of 25mm diameter bar 100mm girth once bent to 50mm internal radius, at approximately 1200mm centres each with 80mm diameter by 6mm thick plate twice holed for bolts ","m",1,{"v":564.3033808000001,"d":"564.30"}]
[{"$nulls":4},0]
["11.1.8","Extra over 38mm pipe rail for bend to 200mm Internal radius","no",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
["11.1.9","6mm expansion bolt","no",1,{"v":13.494211280000002,"d":"13.49"}]
[{"$nulls":4},0]
["11.1.10","8mm expansion bolt","no",1,{"v":15.334331000000002,"d":"15.33"}]
[{"$nulls":4},0]
["11.1.11","10mm expansion bolt","no",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["11.1.12","6mm expansion anchor with loose bolt","no",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["11.1.13","8mm expansion anchor with loose bolt","no",1,{"v":19.01457044,"d":"19.01"}]
[{"$nulls":4},0]
["11.1.14","10mm expansion anchor with loose bolt","no",1,{"v":20.85469016,"d":"20.85"}]
[{"$nulls":4},0]
["11.1.15","12mm expansion anchor with loose bolt","no",1,{"v":23.430857768000003,"d":"23.43"}]
[{"$nulls":4},0]
[11.2,"Welded balustrading to mild steel",null,null,0]
[{"$nulls":4},0]
["11.2.1","Raking balustrading to staircase or ramp of 80 x 40 x 2mm hollow section continuous top rail, 40 x 10mm flat section continuous bottom rail, 12mm square bar section intermediate balusters at 125mm centres between to and bottom rails and 38 x 38 x 2mm hollow section post at approximately 1200mm centres each with 120 x 50 x 8mm flat section base plate twice holed for bolts","m",1,{"v":740.9548739200002,"d":"740.95"}]
[{"$nulls":4},0]
["11.2.2","Extra over 80 x 40 x 2mm hollow section for mitred L-intersection","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.2.3","Raking balustrading to staircase or ramp of 50 x 10mm flat section continuous top rail, 40 x 10mm flat section continuous bottom rail, 12mm square bar section intermediate balusters at 125mm centres between to and bottom rails and 38 x 38 x 2mm hollow section post at approximately 1200mm centres each with 120 x 50 x 8mm flat section base plate twice holed for bolts","m",1,{"v":642.8151555200001,"d":"642.82"}]
[{"$nulls":4},0]
["11.2.4","Balustrading of 50 x 10mm flat section continuous top rail, 40 x 10mm flat section continuous bottom rail, 12mm square bar section intermediate balusters at 125mm centres between to and bottom rails and 38 x 38 x 2mm hollow section post at approximately 1200mm centres each with 120 x 50 x 8mm flat section base plate twice holed for bolts","m",1,{"v":685.7512823200001,"d":"685.75"}]
[{"$nulls":4},0]
["11.2.5","Extra over 50 x 10mm flat section for mitred L-intersection","no",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["11.2.6","M14mm expansion anchor bolt ","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.2.7","Vastrap Sheet 3mm","m2",1,{"v":897.1605923733331,"d":"897.16"}]
[{"$nulls":4},0]
["11.2.8","Channel 200 x 75mm","m",1,{"v":692.9187530871468,"d":"692.92"}]
[{"$nulls":4},0]
[11.3,"Welded balustrading to stainless steel",null,null,0]
[{"$nulls":4},0]
["11.3.1","Grade 304 stainless steel polished horizontal balustrading to walkways or landings comprising 90° top mounted stanchions at 1,5m centres with top and knee rails of straight tube, with 90° closure, all necessary bends and slip joints, the stanchions to be bolted in position with 45mm long M16 expanding bolts with nuts and washers and the sections of tube to be joined with slip joints and welded inside the stanchion balls.","m",1,0]
[{"$nulls":4},0]
["11.3.2","Grade 304 stainless steel polished raking balustrading to staircases comprising 30° step top mounted stanchions at 1,5m centres with top and knee rails of straight tube, with 30° closure, all necessary bends and slip joints, the stanchions to be bolted in position with 45mm long M16 expanding bolts with nuts and washers and the sections of tube to be joined with slip joints and welded inside the stanchion balls.","m",1,0]
[{"$nulls":4},0]
[null,"SUNDRY STEELWORK",null,null,0]
[{"$nulls":4},0]
[null,"Bolts",null,null,0]
[{"$nulls":4},0]
["11.3.1","Bolts(Provisional)","kg",1,{"v":128.80838040000003,"d":"128.81"}]
[{"$nulls":4},0]
[null,"Welded brick (lintel) bearers and framing",null,null,0]
[{"$nulls":4},0]
["11.3.2","Two 80 x 80 x 6mm angle section welded back-to-back with ends build into brickwork","kg",1,{"v":2.14680634,"d":"2.15"}]
[{"$nulls":4},0]
["11.3.3","25 x 25 x 2mm Hollow section framing","m",1,{"v":57.04371132000001,"d":"57.04"}]
[{"$nulls":4},0]
["11.3.4","Extra over 25 x 25mm hollow section for mitred L-section","no",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["11.3.5","76 x 76 x 3.5mm hollow section post with top welded to bearers and bottom welded to and including 150 x 150 x 6mm foot plate fout times holed for bolts",null,null,0]
[null,null,"m",1,{"v":99.36646488000001,"d":"99.37"}]
[11.4,"Bearers to brick linings, lintels, etc",null,null,0]
[{"$nulls":4},0]
["11.4.1","100 x 75 x 8mm angle section bearers and holed at 500mm centres for bolting to concrete","m",1,{"v":225.72135232000005,"d":"225.72"}]
[{"$nulls":4},0]
["11.4.2","100 x 75 x 8mm angle section bearers with 130 x 50 x 8mm flat section brackets welded on at 500mm centres and once holed for bolting to concrete","m",1,{"v":252.70977488000005,"d":"252.71"}]
[{"$nulls":4},0]
["11.4.3","M12/60L expansion bolt","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
[11.5,"Corner protectors",null,null,0]
[{"$nulls":4},0]
["11.5.1","60 x 60 x 6mm angle section corner protectors in varying lengths twice screwed to brickwork of concrete a 500mm centres","m",1,{"v":117.76766208000002,"d":"117.77"}]
[{"$nulls":4},0]
["11.5.2","40 x 40 x 2mm angle section corner protectors in varying lengths twice screwed to brickwork of concrete a 500mm centres","m",1,{"v":94.21412966400001,"d":"94.21"}]
[{"$nulls":4},0]
[null,"Welded guard,bump rails, etc",null,null,0]
[{"$nulls":4},0]
["11.5.2a","80 x 40 x 2,0mm hollow section continuous rails with flat closed ends welded to bracket, formed of 25mm diameter bar 100mm girth once bent to 50mm internal radius, at approximately 1200mm centres each with 80mm diameter by 6mm thick plate twice holed for bolts ","m",1,{"v":287.0586763200001,"d":"287.06"}]
[{"$nulls":4},0]
["11.5.3","Extra over 80 x 40 x 2mm hollow section for mitred L-intersection","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
["11.5.4","Repair chromium plated lifesaver's chair","no",1,{"v":1649.3606423600004,"d":"1,649.36"}]
[{"$nulls":4},0]
[11.6,"Welded bearers to benches, spectators seating, etc",null,null,0]
[{"$nulls":4},0]
["11.6.1","80 x 40 x 2,0mm hollow section continuous rails with flat closed ends welded to bracket, formed of 25mm diameter bar 100mm girth once bent to 50mm internal radius, at approximately 1200mm centres each with 80mm diameter by 6mm thick plate twice holed for bolts ","m",1,{"v":287.0586763200001,"d":"287.06"}]
[{"$nulls":4},0]
["11.6.2","Extra over 80 x 40 x 2mm hollow section for mitred L-intersection","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.6.3","70 x 70 x6mm Angle section cleat three times holed and bolted to brickwork or concrete at 300mm centres","m",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
["11.6.1","225 x 75 x 2,5mm cold formed channel 3000mm long with 220 x 70 x 3mm internal plate stiffeners at 1000mm centres, two 225 x 75 x 3mm end plates and three 220 x 50 x 5mm flat section twice holed for bolts and welded on  ","no",1,0]
[{"$nulls":4},0]
["11.6.2","170 x 50 x 2,5mm cold formed channel 3000mm long with 165 x 45 x 3mm internal plate stiffeners at 1000mm centres, two 170 x 50 x 3mm end plates and three 167 x 50 x 5mm flat section twice holed for bolts and welded on  ","no",1,0]
[{"$nulls":4},0]
["11.6.3","75 x 50 x 20 x 2mm lipped channel in varying lengths with two 57 x 50 x 3mm end plates and 50 x 50 x 5mm flat section once holed for bolts and welded on at 1000mm centres","m",1,0]
[{"$nulls":4},0]
["11.6.4","Extra over 80 x 40 x 2mm hollow section for mitred L-intersection","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.6.5","70 x 70 x6mm Angle section cleat three times holed and bolted to brickwork or concrete at 300mm centres","m",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
[11.7,"Welded framing to benches, spectators seating, etc",null,null,0]
[{"$nulls":4},0]
["11.7.1","70 x 70 x6mm Angle section cleat three times holed and bolted to brickwork or concrete at 300mm centres","m",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
["11.7.1","Triangular shaped frame 2300 x 2250mm high with 900mm extended leg formed of 50 x 50 x 5mm angle section frame including intermediate horizontal and vertical struts mitred and welded at angles and six times holed for bolts","no",1,0]
[{"$nulls":4},0]
["11.7.2","L-shaped bracket formed of 50 x 50 x 5mm angle section 900mm girth with 50mm splay cut ends mitred and welded at angles and four time holed for bolts including welding on to Triangular shaped frame (elsewhere measured)","no",1,0]
[{"$nulls":4},0]
["11.7.3","Triangular shaped bracket 460 x 330mm high formed of 50 x 50 x 5mm angle section and 40 x 40 x 5mm angle section diagonal frame mitred and welded at angles and 7 times hold for bolts","no",1,0]
[{"$nulls":4},0]
["11.7.4","M16/100L expansion bolts","no",1,0]
[{"$nulls":4},0]
["11.7.5","M12/25L with anti vandal shear nut","no",1,0]
[{"$nulls":4},0]
[11.8,"Welded bracing etc with flat section connecting plates bolted to steel",null,null,0]
[{"$nulls":4},0]
["11.8.1","80 x 40 x 2,0 hollow section continuous bracing with flat section connecting plate 100 x 100 x 2,0 mm bolted to steel","m",1,{"v":287.0586763200001,"d":"287.06"}]
[{"$nulls":4},0]
["11.8.1","30 x 30 x 3mm Angle section bracing","m",1,0]
[{"$nulls":4},0]
[null,"WELDED SCREENS, GATES, ETC",null,null,0]
[{"$nulls":4},0]
[11.9,"Screens and gates to doors",null,null,0]
[{"$nulls":4},0]
["11.9.1","50 x 76 x 3.5mm Hollow section framing","m",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
["11.9.2","Extra over 50 x 76mm hollow section for mitred and welded  L-intersection","m",1,{"v":99.36646488000001,"d":"99.37"}]
[{"$nulls":4},0]
["11.9.3","Hole through 50 x 76mm hollow section","no",1,{"v":5.520359160000002,"d":"5.52"}]
[{"$nulls":4},0]
["11.9.4","100mm M10 expansion bolt in brickwork","no",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["11.9.5","Single gate 810 x 2066mm high of 50 x 50 x2,5mm hollow section frame and two 50 x 50 x 2,5mm hollow section horizontal middle rails filled in with 20mm diameter solid vertical round bars at 89mm centres framed through middle rails and into framing and fitted with three suitable hinges welded to post and a \"Union\" LX 3261 security gate lock box between middle rails","no",1,{"v":2220.411128800001,"d":"2,220.41"}]
[{"$nulls":4},0]
["11.9.6","Double gate with two single leaves 1620 x 2066mm high of 50 x 50 x2,5mm hollow section frame and two 50 x 50 x 2,5mm hollow section horizontal middle rails filled in with 20mm diameter solid vertical round bars at 89mm centres framed through middle rails and into framing and fitted with six suitable hinges welded to posts and a \"Union\" LX 3261 security gate lock box between middle rails including conversion set.","no",1,{"v":4440.822257600002,"d":"4,440.82"}]
[{"$nulls":4},0]
["11.9.7","Steel wire expanded mesh burglar proofing not exceeding 1,0m² bolted to brickwork ","no",1,{"v":1447.5608464000002,"d":"1,447.56"}]
[{"$nulls":4},0]
["11.9.8","Steel wire expanded mesh burglar proofing exceeding 1,0m² and not exceeding 2,0m² bolted to brickwork ","no",1,{"v":1778.7823960000005,"d":"1,778.78"}]
[{"$nulls":4},0]
["11.9.10","Steel wire mesh burglar proofing exceeding 2,0m² and not exceeding 3,0m² bolted to brickwork ","no",1,{"v":2220.411128800001,"d":"2,220.41"}]
[{"$nulls":4},0]
["11.9.11","Steel round, square, etc burglar proofing not exceeding 1,0m² bolted to brickwork ","no",1,{"v":1447.5608464000002,"d":"1,447.56"}]
[{"$nulls":4},0]
["11.9.12","Steel round, square, etc burglar proofing exceeding 1,0m² and not exceeding 2,0m² bolted to brickwork ","no",1,{"v":1778.7823960000005,"d":"1,778.78"}]
[{"$nulls":4},0]
["11.9.13","Steel round, square, etc burglar proofing exceeding 2,0m² and not exceeding 3,0m² bolted to brickwork ","no",1,{"v":2220.411128800001,"d":"2,220.41"}]
[{"$nulls":4},0]
["11.9.14","Steel round, square, etc burglar proofing not exceeding 1,0m² welded to brickwork ","no",1,{"v":1447.5608464000002,"d":"1,447.56"}]
[{"$nulls":4},0]
["11.9.15","Steel round, square, etc burglar proofing exceeding 1,0m² and not exceeding 2,0m² welded to brickwork ","no",1,{"v":1778.7823960000005,"d":"1,778.78"}]
[{"$nulls":4},0]
["11.9.16","Steel round, square, etc burglar proofing exceeding 2,0m² and not exceeding 3,0m² welded to brickwork ","no",1,{"v":2220.411128800001,"d":"2,220.41"}]
[{"$nulls":4},0]
["11.9.17","Steel round, square, etc burglar proofing, perimeter fencing, 1800mm high  welded to steel  ","m",1,{"v":1625.439086,"d":"1,625.44"}]
[{"$nulls":4},0]
["11.9.18","Steel round, square, etc burglar proofing, perimeter fencing, 2100mm high  welded to steel  ","m",1,{"v":1787.9829946000002,"d":"1,787.98"}]
[{"$nulls":4},0]
[null,"RETRACTABLE SECURITY GATES AND SCREENS",null,null,0]
[{"$nulls":4},0]
[null,"\"TRELLIDOR\" or equally approved installed by a Trellidor installer for a 5-year warranty on workmanship and hardware",null,null,0]
[{"$nulls":4},0]
["11.9.18a","Security \"slamlock\" gate size 900 x 2032mm high","no",1,{"v":5246.192894800001,"d":"5,246.19"}]
[{"$nulls":4},0]
["11.9.18b","Security \"slamlock\" gate size 1150 x 2032mm high","no",1,{"v":6866.539825600001,"d":"6,866.54"}]
[{"$nulls":4},0]
["11.9.19","Security \"slamlock\" gate size 1300 x 2032mm high","no",1,{"v":7287.799937600001,"d":"7,287.80"}]
[{"$nulls":4},0]
["11.9.20","Security screen to openings not exceeding 5m2 ","m2",1,{"v":3015.306619067827,"d":"3,015.31"}]
[{"$nulls":4},0]
["11.9.20a","Security screen to openings exceeding 5m2 not exceeding 10m2 ","m2",1,{"v":3200.2947552069572,"d":"3,200.29"}]
[{"$nulls":4},0]
[null,"Making good screens and gates to doors, etc.",null,null,0]
[{"$nulls":4},0]
["11.9.21","Single gate 810 x 2066mm high of 50 x 50 x2,5mm hollow section frame and two 50 x 50 x 2,5mm hollow section horizontal middle rails filled in with 20mm diameter solid vertical round bars at 89mm centres framed through middle rails and into framing and fitted with three suitable hinges welded to post and a \"Union\" LX 3261 security gate lock box between middle rails","no",1,{"v":555.1027822000002,"d":"555.10"}]
[{"$nulls":4},0]
["11.9.22","Double gate with two single leaves 1620 x 2066mm high of 50 x 50 x2,5mm hollow section frame and two 50 x 50 x 2,5mm hollow section horizontal middle rails filled in with 20mm diameter solid vertical round bars at 89mm centres framed through middle rails and into framing and fitted with six suitable hinges welded to posts and a \"Union\" LX 3261 security gate lock box between middle rails including conversion set.","no",1,{"v":1110.2055644000004,"d":"1,110.21"}]
[{"$nulls":4},0]
["11.9.23","Burglar proofing 2066mm high of 50 x 50 x2,5mm hollow section frame and two 50 x 50 x 2,5mm hollow section horizontal middle rails filled in with 20mm diameter solid vertical round/square bars at 89mm centres framed through middle rails and into framing and bolted to brickwork, concrete, etc.","m",1,{"v":555.1027822000002,"d":"555.10"}]
[{"$nulls":4},0]
["11.9.24","Steel wire mesh burglar proofing  ","m2",1,{"v":346.9361720088001,"d":"346.94"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["11.9.1","Screen fencing 6,0m high formed of eleven 3.15mm galvanised straining wires passed through posts and tied to end posts covered with 50 x 2,5mm fully galvanised diamond mesh fixed with 1,6mm galvanised binding wire to straining wires, posts, rails, etc (framework elsewhere measured)","m",1,0]
[{"$nulls":4},0]
["11.9.2","76,2mm diameter 2,5mm thick pipe, rail, post, etc","m",1,0]
[{"$nulls":4},0]
["11.9.3","Extra over for closed end","no",1,0]
[{"$nulls":4},0]
["11.9.4","Extra over for mitred and welded L-intersection","no",1,0]
[{"$nulls":4},0]
["11.9.5","48,5mm diameter 2,5mm thick pipe, rail, post, etc","m",1,0]
[{"$nulls":4},0]
["11.9.6","Extra over for closed end","no",1,0]
[{"$nulls":4},0]
["11.9.7","Extra over for mitred and welded L-intersection","no",1,0]
[{"$nulls":4},0]
["11.9.8","Extra over post for closed end","no",1,0]
[{"$nulls":4},0]
["11.9.9","76,2mm diameter 2,5mm thick post 7,2m long with closed top end, 230 x 230 x 5mm base plate welded on and cast in 500 x 500 x 1000mm 20MPa/20mm concrete including excavations","no",1,0]
[{"$nulls":4},0]
[null,"PRESSED STEEL DOOR FRAMES",null,null,0]
[{"$nulls":4},0]
[{"v":11.1,"d":"11.10"},"1,2mm. Rebated frame suitable for half brick wall",null,null,0]
[{"$nulls":4},0]
["11.10.1","Frame for door size 762 x 2032mm. high","no",1,{"v":478.4311272000001,"d":"478.43"}]
[{"$nulls":4},0]
["11.10.2","Frame for door size 813 x 2032mm. high","no",1,{"v":478.4311272000001,"d":"478.43"}]
[{"$nulls":4},0]
["11.10.3","Frame for door size 900 x 2032mm. high","no",1,{"v":529.95447936,"d":"529.95"}]
[{"$nulls":4},0]
["11.10.4","Frame for double door size 1359 x 2032mm. high","no",1,{"v":540.9951976800002,"d":"541.00"}]
[{"$nulls":4},0]
["11.10.5","Frame for double door size 1511 x 2032mm. high","no",1,{"v":552.035916,"d":"552.04"}]
[{"$nulls":4},0]
["11.10.6","Frame for double door size 1613 x 2032mm. high","no",1,{"v":552.035916,"d":"552.04"}]
[{"$nulls":4},0]
[11.11,"1,2mm. Rebated frame suitable one brick wall",null,null,0]
[{"$nulls":4},0]
["11.11.1","Frame for door size 762 x 2032mm. high","no",1,{"v":682.07104288,"d":"682.07"}]
[{"$nulls":4},0]
["11.11.2","Frame for door size 813 x 2032mm. high","no",1,{"v":682.07104288,"d":"682.07"}]
[{"$nulls":4},0]
["11.11.3","Frame for door size 900 x 2032mm. high","no",1,{"v":753.2223387200002,"d":"753.22"}]
[{"$nulls":4},0]
["11.11.4","Frame for double door size 1359 x 2032mm. high","no",1,{"v":767.9432964800001,"d":"767.94"}]
[{"$nulls":4},0]
["11.11.5","Frame for double door size 1511 x 2032mm. high","no",1,{"v":783.8910007200002,"d":"783.89"}]
[{"$nulls":4},0]
["11.11.6","Frame for double door size 1613 x 2032mm. high","no",1,{"v":783.8910007200002,"d":"783.89"}]
[{"$nulls":4},0]
[null,"PRESSED STEEL CUPBOARD DOOR FRAMES",null,null,0]
[{"$nulls":4},0]
[11.12,"Standard cupboard door frame",null,null,0]
[{"$nulls":4},0]
["11.12.1","Frame for door size 762 x 2032mm. high","no",1,{"v":444.0822257600001,"d":"444.08"}]
[{"$nulls":4},0]
["11.12.2","Frame for door size 1511 x 2032mm. high","no",1,{"v":512.7800286400001,"d":"512.78"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["11.13.1","Type BV door 914 x 2134mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.13.2","Type CV door 1219 x 2134mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.13.3","Type HV door 1219 x 2438mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.13.4","Type YV double door 1524x 2438mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.13.5","Type YVV (vent top and bottom) double door 1524x 2438mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.13.6","Type DV double door 1830x 2438mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.13.7","Type DVV (vent top and bottom) double door 1830x 2438mm high with rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
[null,"STEEL WINDOWS, DOORS, ETC.",null,null,0]
[{"$nulls":4},0]
[11.13,"Standard residential windows with 10mm diameter mild steel burglar bars to opening sashes",null,null,0]
[{"$nulls":4},0]
["11.13.1","Window type NE1 size 533 x 654mm. high","no",1,{"v":437.94849336000004,"d":"437.95"}]
[{"$nulls":4},0]
["11.13.2","Window type NE2 size 1022 x 654mm. high","no",1,{"v":598.65228224,"d":"598.65"}]
[{"$nulls":4},0]
["11.13.3","Window type NE4 size 1511 x 654mm. high","no",1,{"v":962.9959868000002,"d":"963.00"}]
[{"$nulls":4},0]
["11.13.4","Window type NE11 size 2000 x 654mm. high","no",1,{"v":1039.05426856,"d":"1,039.05"}]
[{"$nulls":4},0]
["11.13.5","Window type E1H size 533 x 654mm. high","no",1,{"v":463.71016944,"d":"463.71"}]
[{"$nulls":4},0]
["11.13.6","Window type E2H size 1022 x 654mm. high","no",1,{"v":647.7221414400002,"d":"647.72"}]
[{"$nulls":4},0]
["11.13.7","Window type E4H size 1511 x 654mm. high","no",1,{"v":1035.3740291200002,"d":"1,035.37"}]
[{"$nulls":4},0]
["11.13.8","Window type E22 size 2000 x 654mm. high","no",1,{"v":1165.4091560000002,"d":"1,165.41"}]
[{"$nulls":4},0]
["11.13.9","Window type NC1 size 533 x 949mm. high","no",1,{"v":569.2103667200001,"d":"569.21"}]
[{"$nulls":4},0]
["11.13.10","Window type NC2 size 1022 x 949mm. high","no",1,{"v":775.3037753600003,"d":"775.30"}]
[{"$nulls":4},0]
["11.13.11","Window type NC4 size 1511 x 949mm. high","no",1,{"v":1269.6826068000003,"d":"1,269.68"}]
[{"$nulls":4},0]
["11.13.12","Window type NC11 size 2000 x 949mm. high","no",1,{"v":1350.6478744800002,"d":"1,350.65"}]
[{"$nulls":4},0]
["11.13.13","Window type C1H size 533 x 949mm. high","no",1,{"v":619.5069724000001,"d":"619.51"}]
[{"$nulls":4},0]
["11.13.14","Window type C2H size 1022 x 949mm. high","no",1,{"v":870.9900008000002,"d":"870.99"}]
[{"$nulls":4},0]
["11.13.15","Window type C4H size 1511 x 949mm. high","no",1,{"v":1414.4386914400002,"d":"1,414.44"}]
[{"$nulls":4},0]
["11.13.16","Window type ND1 size 533 x 1245mm. high","no",1,{"v":651.4023808800001,"d":"651.40"}]
[{"$nulls":4},0]
["11.13.17","Window type ND2 size 1022 x 1245mm. high","no",1,{"v":901.6586628000002,"d":"901.66"}]
[{"$nulls":4},0]
["11.13.18","Window type ND4 size 1511 x 1245mm. high","no",1,{"v":1467.1887900800002,"d":"1,467.19"}]
[{"$nulls":4},0]
["11.13.19","Window type ND11 size 2000 x 1245mm. high","no",1,{"v":1565.3285084800004,"d":"1,565.33"}]
[{"$nulls":4},0]
["11.13.20","Window type D1H size 533 x 1245mm. high","no",1,{"v":722.55367672,"d":"722.55"}]
[{"$nulls":4},0]
["11.13.21","Window type D2H size 1022 x 1245mm. high","no",1,{"v":1047.6414939200001,"d":"1,047.64"}]
[{"$nulls":4},0]
["11.13.22","Window type D4H size 1511 x 1245mm. high","no",1,{"v":1689.2299029600003,"d":"1,689.23"}]
[{"$nulls":4},0]
["11.13.23","Window type NCT1S size 533 x 949mm. high","no",1,{"v":517.6870145600001,"d":"517.69"}]
[{"$nulls":4},0]
["11.13.24","Window type NCTX7S size 1022 x 949mm. high","no",1,{"v":694.3385076800001,"d":"694.34"}]
[{"$nulls":4},0]
["11.13.25","Window type NCTX7S5 size 1511 x 949mm. high","no",1,{"v":916.3796205600001,"d":"916.38"}]
[{"$nulls":4},0]
["11.13.26","Window type TD7 size 1022 x 1245mm. high","no",1,{"v":1072.1764235200003,"d":"1,072.18"}]
[{"$nulls":4},0]
["11.13.27","Window type TD75 size 1511 x 1245mm. high","no",1,{"v":1339.6071561600002,"d":"1,339.61"}]
[{"$nulls":4},0]
["11.13.28","Window type TD57S8 size 2000 x 1559mm. high","no",1,{"v":1561.6482690400005,"d":"1,561.65"}]
[{"$nulls":4},0]
[11.14,"Standard medium universal doors, sidelights, etc",null,null,0]
[{"$nulls":4},0]
["11.14.1","Sidelight Type NSDAS, 800 x 2134mm high","no",1,{"v":929.8738318400002,"d":"929.87"}]
[{"$nulls":4},0]
["11.14.2","Door Type NDAS, 800 x 2134mm high","no",1,{"v":2702.5224954400005,"d":"2,702.52"}]
[{"$nulls":4},0]
["11.14.3","Double door Type NDDA, 1524 x 2134mm high","no",1,{"v":4336.5488068,"d":"4,336.55"}]
[{"$nulls":4},0]
["11.14.4","Sidelight Type SDASH, 800 x 2134mm high","no",1,{"v":1101.6183390400001,"d":"1,101.62"}]
[{"$nulls":4},0]
["11.14.5","Door Type DASH, 800 x 2134mm high","no",1,{"v":2974.8602140000007,"d":"2,974.86"}]
[{"$nulls":4},0]
["11.14.6","Double door Type DDAH, 1524 x 2134mm high","no",1,{"v":4529.148004160001,"d":"4,529.15"}]
[{"$nulls":4},0]
[null,"Combination doors and frames",null,null,0]
[{"$nulls":4},0]
["11.14.7","Door and frame size 813 x 2032mm. high","no",1,{"v":2281.748452800001,"d":"2,281.75"}]
[{"$nulls":4},0]
["11.14.8","Door and frame size 1626 x 2032mm. high","no",1,{"v":4115.182404484001,"d":"4,115.18"}]
[{"$nulls":4},0]
[null,"ALUMINIUM SHOPFRONTS COMPLETE WITH GLAZING, HANDLES AND ALL ACCESSORIES",null,null,0]
[{"$nulls":4},0]
[null,"SLIDING FOLDING DOORS",null,null,0]
[{"$nulls":4},0]
["11.14.9","4500-4800 x 2100mm Aluminium Folding door (Toughened Safety Glass) - 5+1 Panel ","no",1,{"v":47347.13911813601,"d":"47,347.14"}]
[{"$nulls":4},0]
["11.14.10","4500-4800 x 2700mm Aluminium Folding door (Toughened Safety Glass) - 5+1 Panel ","no",1,{"v":53412.05104060802,"d":"53,412.05"}]
[{"$nulls":4},0]
["11.14.11","5400-5700 x 2100mm Aluminium Folding door (Toughened Safety Glass) - 5+1 Panel ","no",1,{"v":50908.261474928004,"d":"50,908.26"}]
[{"$nulls":4},0]
["11.14.12","5400-5700 x 2700mm Aluminium Folding door (Toughened Safety Glass) - 5+1 Panel ","no",1,{"v":57406.95095272801,"d":"57,406.95"}]
[{"$nulls":4},0]
["11.14.13","5400-5700 x 2100mm Aluminium Folding door (Toughened Safety Glass) - 5+5 Panel ","no",1,{"v":67594.34442124002,"d":"67,594.34"}]
[{"$nulls":4},0]
["11.14.14","5400-5700 x 2700mm Aluminium Folding door (Toughened Safety Glass) - 5+5 Panel ","no",1,{"v":76231.62103762402,"d":"76,231.62"}]
[{"$nulls":4},0]
["11.14.14a","6300-6600 x 2100mm Aluminium Folding door (Toughened Safety Glass) - 5+5 Panel ","no",1,{"v":71134.73476252,"d":"71,134.73"}]
[{"$nulls":4},0]
["11.14.14b","6300-6600 x 2700mm Aluminium Folding door (Toughened Safety Glass) - 5+5 Panel ","no",1,{"v":80202.59939338402,"d":"80,202.60"}]
[{"$nulls":4},0]
[null,"ALUMINIUM SLIDING DOORS",null,null,0]
[{"$nulls":4},0]
["11.14.15","1800 x 2100 Aluminium sliding door (Standard 5mm glass) - Double Leaf","no",1,{"v":7980.59922564,"d":"7,980.60"}]
[{"$nulls":4},0]
["11.14.16","2400 x 2100 Aluminium sliding door (Standard 5mm glass) - Double Leaf","no",1,{"v":9436.133924160002,"d":"9,436.13"}]
[{"$nulls":4},0]
["11.14.17","3000 x 2100 Aluminium sliding door (Standard 5mm glass) - Double Leaf","no",1,{"v":11603.794954320003,"d":"11,603.79"}]
[{"$nulls":4},0]
["11.16.1","Type ALU louvered unit 900 x 745mmmm high with double rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.16.2","Type BLU louvered unit 1590 x 745mmmm high with double rebated frame suitable for one brick wall","no",1,0]
[{"$nulls":4},0]
["11.18.1","Single Pivot Door 890 - 920 x 1800mm high Code PD920 Colour white","no",1,0]
[{"$nulls":4},0]
["11.18.2","Single Pivot Door 830 - 860 x 1800mm high Code PD860 Colour white","no",1,0]
[{"$nulls":4},0]
["11.14.18","1800 x 2400 Aluminium sliding door (Safety glass) - Double Leaf","no",1,{"v":14041.953583320003,"d":"14,041.95"}]
[{"$nulls":4},0]
["11.14.19","2400 x 2400 Aluminium sliding door (Safety glass) - Double Leaf","no",1,{"v":16656.76370544,"d":"16,656.76"}]
[{"$nulls":4},0]
["11.14.20","3000 x 2400 Aluminium sliding door (Safety glass) - Double leaf","no",1,{"v":19264.213348680005,"d":"19,264.21"}]
[{"$nulls":4},0]
["11.14.21","3600 x 2400 Aluminium sliding door (Safety glass) - Four Leaf","no",1,{"v":27695.641905720007,"d":"27,695.64"}]
[{"$nulls":4},0]
["11.14.22","4200 x 2400 Aluminium sliding door (Safety glass) - Four Leaf","no",1,{"v":30288.370591200004,"d":"30,288.37"}]
[{"$nulls":4},0]
["11.14.23","6000 x 2400 Aluminium sliding door (Safety glass) - Four leaf","no",1,{"v":38268.96981684001,"d":"38,268.97"}]
[{"$nulls":4},0]
[null,"ALUMINIUM PANE DOORS ",null,null,0]
[{"$nulls":4},0]
["11.14.24","900 x 2100 Aluminium Single Door (Safety Glass)  - Single leaf","no",1,{"v":11784.126686880003,"d":"11,784.13"}]
[{"$nulls":4},0]
["11.14.25","1800 x 2100 Aluminium Doublee Door (Safety Glass)  - Double leaf","no",1,{"v":18369.91516476,"d":"18,369.92"}]
[{"$nulls":4},0]
["11.14.26","900 x 2400 Aluminium Single Door (Safety Glass)  - Single leaf","no",1,{"v":14871.847577040004,"d":"14,871.85"}]
[{"$nulls":4},0]
["11.14.27","1800 x 2400 Aluminium Double Door (Safety Glass)  - Double leaf","no",1,{"v":28915.641280080006,"d":"28,915.64"}]
[{"$nulls":4},0]
[null,"ALUMINIUM HINGE DOORS WITH MIDRAIL",null,null,0]
[{"$nulls":4},0]
["11.14.28","900 x 2100 Aluminium Hinge Door (Safety Glass)  - Single leaf","no",1,{"v":12551.45661012,"d":"12,551.46"}]
[{"$nulls":4},0]
["11.14.29","1800 x 2100 Aluminium Hinge Double Door (Safety Glass)  - Double leaf","no",1,{"v":19759.205553360003,"d":"19,759.21"}]
[{"$nulls":4},0]
["11.14.30","900 x 2400 Aluminium Hinge Door (Safety Glass)  - Single leaf","no",1,{"v":17935.64691084,"d":"17,935.65"}]
[{"$nulls":4},0]
["11.14.31","1800 x 2400 Aluminium Hinge Double Door (Safety Glass)  - Double leaf","no",1,{"v":30328.85322504001,"d":"30,328.85"}]
[{"$nulls":4},0]
[null,"ALUMINIUM SIDELIGHTS ",null,null,0]
[{"$nulls":4},0]
["11.14.32","600 x 2100 Aluminium Sidelight (Safety Glass)  - Large Pane","no",1,{"v":6985.094457120001,"d":"6,985.09"}]
[{"$nulls":4},0]
["11.14.33","900 x 2100 Aluminium Sidelight (Safety Glass)  - Large Pane","no",1,{"v":7524.24953508,"d":"7,524.25"}]
[{"$nulls":4},0]
["11.14.34","600 x 2400 Aluminium Sidelight (Safety Glass)  - Large Pane","no",1,{"v":7982.439345360001,"d":"7,982.44"}]
[{"$nulls":4},0]
["11.14.35","900 x 2400 Aluminium Sidelight (Safety Glass)  - Large Pane","no",1,{"v":8600.719571280002,"d":"8,600.72"}]
[{"$nulls":4},0]
["11.14.36","600 x 2100 Aluminium Sidelight (Safety Glass)  - With Midrail","no",1,{"v":7930.915993200002,"d":"7,930.92"}]
[{"$nulls":4},0]
["11.14.37","900 x 2100 Aluminium Sidelight (Safety Glass)  - With Midrail","no",1,{"v":8804.972860200001,"d":"8,804.97"}]
[{"$nulls":4},0]
["11.14.38","600 x 2400 Aluminium Sidelight (Safety Glass)  - With Midrail","no",1,{"v":15341.078105640003,"d":"15,341.08"}]
[{"$nulls":4},0]
["11.14.39","900 x 2400 Aluminium Sidelight (Safety Glass)  - With Midrail","no",1,{"v":16697.246339280002,"d":"16,697.25"}]
[{"$nulls":4},0]
["11.14.40","600 x 2100 Aluminium Sidelight (Safety Glass)  - With Vents","no",1,{"v":9213.479438040002,"d":"9,213.48"}]
[{"$nulls":4},0]
["11.14.41","900 x 2100 Aluminium Sidelight (Safety Glass)  - With Vents","no",1,{"v":10098.577023360003,"d":"10,098.58"}]
[{"$nulls":4},0]
["11.14.42","600 x 2400 Aluminium Sidelight (Safety Glass)  - With Vents","no",1,{"v":10516.2841998,"d":"10,516.28"}]
[{"$nulls":4},0]
["11.14.43","900 x 2400 Aluminium Sidelight (Safety Glass)  - With Vents","no",1,{"v":11432.663820360003,"d":"11,432.66"}]
[{"$nulls":4},0]
[null,"ALUMINIUM WINDOWS ",null,null,0]
[{"$nulls":4},0]
["11.14.44","600 x 600 Aluminium Window, Code: PT66(A3) - Top Hung Casement window","no",1,{"v":2284.2019457600004,"d":"2,284.20"}]
[{"$nulls":4},0]
["11.14.45","900 x 600 Aluminium Window, Code: PT96(A3) - Top Hung Casement window","no",1,{"v":2794.2831321440003,"d":"2,794.28"}]
[{"$nulls":4},0]
["11.14.46","1200 x 600 Aluminium Window, Code: PT126(A3) - Top Hung Casement window","no",1,{"v":3318.103879104,"d":"3,318.10"}]
[{"$nulls":4},0]
["11.14.47","600 x 900 Aluminium Window, Code: PT69(A3) - Top Hung Casement window","no",1,{"v":2988.3544252800007,"d":"2,988.35"}]
[{"$nulls":4},0]
["11.14.48","900 x 900 Aluminium Window, Code: PT99(A3) - Top Hung Casement window","no",1,{"v":3707.963910448,"d":"3,707.96"}]
[{"$nulls":4},0]
["11.14.49","1500 x 900 Aluminium Window, Code: PT159(A3) - Top Hung Casement window","no",1,{"v":4676.602931056001,"d":"4,676.60"}]
[{"$nulls":4},0]
["11.14.50","1800 x 1200 Aluminium Window, Code: PTT1812(A1) - Top Hung Casement window","no",1,{"v":7443.406942048,"d":"7,443.41"}]
[{"$nulls":4},0]
["11.14.51","1800 x 1500 Aluminium Window, Code: PTT1815(A3) - Top Hung Casement window","no",1,{"v":8123.51519056,"d":"8,123.52"}]
[{"$nulls":4},0]
["11.14.52","1800 x 1800 Aluminium Window, Code: DPTT1818(A3) - Top Hung Casement window","no",1,{"v":13045.712766912002,"d":"13,045.71"}]
[{"$nulls":4},0]
["11.14.53","2100 x 1200 Aluminium Window, Code: PTT2112(A1) - Top Hung Casement window","no",1,{"v":5832.443464512,"d":"5,832.44"}]
[{"$nulls":4},0]
["11.14.54","2100 x 1500 Aluminium Window, Code: PTT2115(A3) - Top Hung Casement window","no",1,{"v":7170.333175600001,"d":"7,170.33"}]
[{"$nulls":4},0]
["11.14.55","2400 x 1500 Aluminium Window, Code: PTT2415(A3) - Top Hung Casement window","no",1,{"v":7962.075353792001,"d":"7,962.08"}]
[{"$nulls":4},0]
["11.14.56","2400 x 1200 Aluminium Window, Code: DPTT2412(A1) - Top Hung Casement window","no",1,{"v":8156.146646928001,"d":"8,156.15"}]
[{"$nulls":4},0]
["11.14.57","1200 x 900 Aluminium Window, Code: SH129 - Side Hung Casement window","no",1,{"v":3318.103879104,"d":"3,318.10"}]
[{"$nulls":4},0]
["11.14.58","1500 x 900 Aluminium Window, Code: SH159 - Side Hung Casement window","no",1,{"v":3639.266107568001,"d":"3,639.27"}]
[{"$nulls":4},0]
["11.14.59","1800 x 1200 Aluminium, Code: SH1812 - Side Hung Casement window","no",1,{"v":4728.126283216001,"d":"4,728.13"}]
[{"$nulls":4},0]
["11.14.60","2100 x 1200 Aluminium, Code: SHH2112 - Side Hung Casement window","no",1,{"v":6725.514901952001,"d":"6,725.51"}]
[{"$nulls":4},0]
["11.14.61","1200 x 600 Aluminium, Code: HS126 - Horizontal Sliding window","no",1,{"v":3349.0178903999995,"d":"3,349.02"}]
[{"$nulls":4},0]
["11.14.62","1200 x 900 Aluminium, Code: HS129 - Horizontal Sliding window","no",1,{"v":3823.032730272,"d":"3,823.03"}]
[{"$nulls":4},0]
["11.14.63","1200 x 1200 Aluminium, Code: HS1212 - Horizontal Sliding window","no",1,{"v":4303.917350432001,"d":"4,303.92"}]
[{"$nulls":4},0]
["11.14.64","1800 x 600 Aluminium, Code: HS186 - Horizontal Sliding window","no",1,{"v":4260.981223632,"d":"4,260.98"}]
[{"$nulls":4},0]
["11.14.65","1800 x 900 Aluminium, Code: HS189 - Horizontal Sliding window","no",1,{"v":4803.693866383999,"d":"4,803.69"}]
[{"$nulls":4},0]
["11.14.66","1800 x 1200 Aluminium, Code: HS1812 - Horizontal Sliding window","no",1,{"v":5344.689064064,"d":"5,344.69"}]
[{"$nulls":4},0]
["11.14.67","2400 x 900 Aluminium, Code: HS249X - Horizontal Sliding window","no",1,{"v":7132.549384016001,"d":"7,132.55"}]
[{"$nulls":4},0]
["11.14.68","2400 x 1200 Aluminium, Code: HS2412X - Horizontal Sliding window","no",1,{"v":8020.468486240001,"d":"8,020.47"}]
[{"$nulls":4},0]
["11.14.69","900 x 900 Aluminium, Code: VS99 - Vertical Sliding window","no",1,{"v":4530.620099936001,"d":"4,530.62"}]
[{"$nulls":4},0]
["11.14.70","900 x 1200 Aluminium, Code: VS912 - Vertical Sliding window","no",1,{"v":4994.330269376001,"d":"4,994.33"}]
[{"$nulls":4},0]
["11.14.71","900 x 1500 Aluminium, Code: VS915 - Vertical Sliding window","no",1,{"v":5523.303351552001,"d":"5,523.30"}]
[{"$nulls":4},0]
["11.14.72","900 x 1800 Aluminium, Code: VS918 - Vertical Sliding window","no",1,{"v":6387.1782227680005,"d":"6,387.18"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["11.14.73","1200 x 1200 Aluminium, Code: VS1212 - Vertical Sliding window","no",1,{"v":5729.396760192,"d":"5,729.40"}]
[{"$nulls":4},0]
["11.14.74","1200 x 1800 Aluminium, Code: VS1218 - Vertical Sliding window","no",1,{"v":7352.382353232001,"d":"7,352.38"}]
[{"$nulls":4},0]
["11.14.75","900 x 2100 Aluminium, Code: VS912S9 - Vertical Sliding window","no",1,{"v":7470.8860632000005,"d":"7,470.89"}]
[{"$nulls":4},0]
["11.14.76","1200 x 2100 Aluminium, Code: VS1212S9 - Vertical Sliding window","no",1,{"v":8666.227833312001,"d":"8,666.23"}]
[{"$nulls":4},0]
[null,"STEEL ROLLER SHUTTERS ETC.",null,null,0]
[{"$nulls":4},0]
[11.15,"Galvanised roller shutters fixed to brickwork or concrete",null,null,0]
[{"$nulls":4},0]
["11.15.1","Manual pushup 76mm slatted roller shutter for 2440 x 2135mm high opening","no",1,{"v":4389.298905440001,"d":"4,389.30"}]
[{"$nulls":4},0]
["11.15.2","Manual pushup 76mm slatted roller shutter for 3000 x 2440mm high opening","no",1,{"v":5806.191089840001,"d":"5,806.19"}]
[{"$nulls":4},0]
[null,"Galvanized chain operated industrial roller shutter door with 75mm slats",null,null,0]
[{"$nulls":4},0]
["11.15.3","2750x2500mm High door","no",1,{"v":15153.99926744,"d":"15,154.00"}]
[{"$nulls":4},0]
[11.16,"Pre-painted Chromadek roller shutters fixed to brickwork or concrete",null,null,0]
[{"$nulls":4},0]
["11.16.1","Manual push-up 76mm slatted roller shutter for 2440 x 2135mm high opening","no",1,{"v":5097.1316244,"d":"5,097.13"}]
[{"$nulls":4},0]
["11.16.2","Manual pushup 76mm slatted roller shutter for 3000 x 2440mm high opening","no",1,{"v":6797.402245680001,"d":"6,797.40"}]
[{"$nulls":4},0]
["11.16.3","Extra over manual pushup roller shutter for electrically operated complete with one transmitter and battery back-up","no",1,{"v":3665.5184822400006,"d":"3,665.52"}]
[{"$nulls":4},0]
[null,"GRILLES",null,null,0]
[{"$nulls":4},0]
[11.17,"Aluminium grilles",null,null,0]
[{"$nulls":4},0]
["11.17.1","Grille size 400 x 300mm high","no",1,{"v":521.367254,"d":"521.37"}]
[{"$nulls":4},0]
[null,"Mild Steel grilles",null,null,0]
[{"$nulls":4},0]
["11.17.2","Grille size 400 x 300mm high","no",1,{"v":521.367254,"d":"521.37"}]
[{"$nulls":4},0]
["11.17.2","Grille size 600 x500mm high","no",1,{"v":790.0247331200001,"d":"790.02"}]
[{"$nulls":4},0]
["11.21.3","Type DS1 6mm record room door with 7-lever security key lock and 3-wheel combination lock , overall size 750 x 1870mm high with a mass of 130kg finished in rustproof undercoat for final painting by contractors.","no",1,0]
[{"$nulls":4},0]
["11.21.4","Type DS50/2 SABS Category 2 (Light Duty) strongroom door with 2 x 7-lever security key lock and 3-wheel combination lock , overall size 760 x 1860mm high with a mass of 480kg finished in rustproof undercoat for final painting by contractors.","no",1,0]
[{"$nulls":4},0]
["11.17.1","Grille size 400 x 300mm high","no",1,{"v":1908.8175228800003,"d":"1,908.82"}]
[{"$nulls":4},0]
["11.17.3","Grille size 600 x500mm high","no",1,{"v":790.0247331200001,"d":"790.02"}]
["11.22.2","Model RMS1 SABS Category 2 dropsafe with 2 x 7-lever security key lock and one key lock on deposit drawer, overall size 450 x 450 x 700mm high with a mass of 260Kg twice holed for and including bolting to floor",null,"no",{"v":1.2267464800000003,"d":"1.23"}]
[{"$nulls":4},0]
["11.17.2","Grille size 600 x500mm high",null,"no",{"v":1.2267464800000003,"d":"1.23"}]
[{"$nulls":4},0]
[null,"Gratings",null,null,0]
[{"$nulls":4},0]
[11.18,"Galvanised steel",null,null,0]
[{"$nulls":4},0]
["11.18.1","\"Open Ended System Mentis\" rectagrid grating size 3000x1000mm cut out where required to permit pipes,etc to pass through and bolted to concrete where required to permit pipes,etc to pass through and bolted to concrete surface bed","no",{"v":1,"d":"1.00"},{"v":4768.976941000001,"d":"4,768.98"}]
[{"$nulls":4},0]
[null,"Swimming Pool Ladder",null,null,0]
[{"$nulls":4},0]
[11.19,"Stainless Steel",null,null,0]
[{"$nulls":4},0]
["11.19.1","48mm Diameter, 500mm long stub pipe cast in concrete base, flush with paving for pool ladder stability","no",{"v":1,"d":"1.00"},{"v":134.94211280000002,"d":"134.94"}]
[{"$nulls":4},0]
["11.19.2","50mm Diameter dog-leg hollow chromium plated tube, 2.5mm thick three steps ladder with 132mm diameter, 5mm thick solid flange, twice holed and welded to top end of ladder.","no",{"v":1,"d":"1.00"},{"v":9750.585849378404,"d":"9,750.59"}]
[{"$nulls":4},0]
[null,"STARTING BLOCKS",null,null,0]
[{"$nulls":4},0]
[{"v":11.2,"d":"11.20"},"Stainless Steel",null,null,0]
[{"$nulls":4},0]
["11.20.1","Stainless steel \"Grade 316\" starting block","no",{"v":1,"d":"1.00"},{"v":17817.7075042528,"d":"17,817.71"}]
[{"$nulls":4},0]
[11.21,"Fibreglass",null,null,0]
[{"$nulls":4},0]
["11.21.1","Fibreglass starting block","no",{"v":1,"d":"1.00"},{"v":1987.3292976000005,"d":"1,987.33"}]
[{"$nulls":4},0]
[11.22,"Nameboards",null,null,0]
[{"$nulls":4},0]
["11.22.1","2500 x 1800 x 8mm Chromadek nameboard mounted to 50 x 50mm welded frame mounted on 2 x 75 x 3mm diameter hollow tube, with overall height of 2500mm, 500mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat.","no",{"v":1,"d":"1.00"},{"v":10181.995784000002,"d":"10,182.00"}]
[{"$nulls":4},0]
[null,"Lifesaver's Chair",null,null,0]
[{"$nulls":4},0]
[11.23,"Stainless Steel",null,null,0]
[{"$nulls":4},0]
["11.23.1","38mm Diameter tubular framework 2900mm overall height with plastic seat, overhead shade, platform and treads and rubber feet for ease of movement","no",{"v":1,"d":"1.00"},{"v":3303.6282706400007,"d":"3,303.63"}]
[{"$nulls":4},0]
["11.23.2","Three seater 1800 pool shade gazebo ","no",{"v":1,"d":"1.00"},{"v":3864.2514120000005,"d":"3,864.25"}]
[{"$nulls":4},0]
[null,"STEEL LOCKERS",null,null,0]
[{"$nulls":4},0]
[11.24,"\"Krost\" or equally approved",null,null,0]
[{"$nulls":4},0]
[null,"Epoxy coated",null,null,0]
[{"$nulls":4},0]
["11.24.1","18kg Single compartment unit size 1800 x 300 x 450m","no",{"v":1,"d":"1.00"},{"v":734.8211415200003,"d":"734.82"}]
[{"$nulls":4},0]
["11.24.2","19kg Two compartment unit size 1800 x 300 x 450m","no",{"v":1,"d":"1.00"},{"v":828.0538740000001,"d":"828.05"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["11.25.","STRUCTURAL STEEL COMPONENTS",null,null,0]
[{"$nulls":4},0]
["11.25.1","Columns, comprising channels welded to form box sections","t",1,{"v":28705.867632,"d":"28,705.87"}]
[{"$nulls":4},0]
["11.25.2","In roof trusses-sop primed lattice","t",1,{"v":28705.867632,"d":"28,705.87"}]
[{"$nulls":4},0]
["11.25.3","In purlins of cold formed lippde Z sections","t",1,{"v":28705.867632,"d":"28,705.87"}]
[{"$nulls":4},0]
["11.25.4","In bracing","t",1,{"v":28705.867632,"d":"28,705.87"}]
[{"$nulls":4},0]
["11.25.5","Tubular welded roof trusses","t",1,{"v":28705.867632,"d":"28,705.87"}]
[{"$nulls":4},0]
["11.10.6","In gutters","t",1,{"v":28705.867632,"d":"28,705.87"}]
[{"$nulls":4},0]
["11.22.2","Model RMS1 SABS Category 2 dropsafe with 2 x 7-lever security key lock and one key lock on deposit drawer, overall size 450 x 450 x 700mm high with a mass of 260Kg twice holed for and including bolting to floor","no",1,0]
[11.26,"TABLES",null,null,0]
[{"$nulls":4},0]
[null,"Stainless Steel",null,null,0]
[{"$nulls":4},0]
["11.26.1","\"Vulcan\" or equally approved",null,null,0]
[{"$nulls":4},0]
["11.26.2","Model \"SWB 1650\" table with splashback","no",1,{"v":5230.356292128001,"d":"5,230.36"}]
[{"$nulls":4},0]
["11.26.3","Model \"SWB 1840\" table with splashback","no",1,{"v":6014.737991440001,"d":"6,014.74"}]
[{"$nulls":4},0]
[11.27,"WASHING LINES",null,null,0]
[{"$nulls":4},0]
["11.27.1","4 x 8m lines Retractaline or equivalent Mounted Washing Line wall mounted both sides","no",1,{"v":1458.20808,"d":"1,458.21"}]
[{"$nulls":4},0]
["11.27.2","Compact Wall Mounted Washing line","no",1,{"v":2499.7852800000005,"d":"2,499.79"}]
[{"$nulls":4},0]
["11.27.3","Rotating Washing Line not exceeding 3m radius","no",1,{"v":3327.2605000000003,"d":"3,327.26"}]
[{"$nulls":4},0]
["11.27.4","2.0 m long Rectangular washing line 2m high off ground, made up of 2no x 2.4m (L)75mm dia galvinised steel post forming a \"T\" 600mm (W) cast in concrete, with 4no strains of 3mm straining wire or skie rope.","no",1,{"v":3726.53176,"d":"3,726.53"}]
[{"$nulls":4},0]
["11.27.5","4.0 m long Rectangular washing line 2m high off ground, made up of 2no x 2.4m (L)75mm dia galvinised steel post forming a \"T\" 600mm (W) cast in concrete, with 4no strains of 3mm straining wire or skie rope.","no",1,{"v":5589.797640000001,"d":"5,589.80"}]
{"$rows_empty":18}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Plastering","index":11,"n_rows":380,"n_cols":7,"rows_kept":380,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 12"]
[]
[null,"PLASTERING"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"SCREEDS"]
[]
[12.1,"Cement screeds wood floated on concrete"]
[]
["12.1.1","25mm. thick on floors and landings","m²",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["12.1.2","Average 40mm thick on floors to falls","m²",1,{"v":130.03512688,"d":"130.04"}]
[{"$nulls":4},0]
["12.1.3","Average 40mm thick on floors to falls and currents","m²",1,{"v":130.03512688,"d":"130.04"}]
[{"$nulls":4},0]
["12.1.4","25mm thick treads and risers of stairs ","m²",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
[null,"Cement screeds steel floated on concrete",null,null,0]
[{"$nulls":4},0]
["12.1.5","25mm. thick on floors and landings","m²",1,{"v":85.87225360000001,"d":"85.87"}]
[{"$nulls":4},0]
["12.1.6","Average 40mm thick on floors to falls","m²",1,{"v":130.03512688,"d":"130.04"}]
[{"$nulls":4},0]
["12.1.7","Average 40mm thick on floors to falls and currents","m²",1,{"v":130.03512688,"d":"130.04"}]
[{"$nulls":4},0]
["12.1.8","25mm thick treads and risers of stairs ","m²",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
[12.2,"Repairing superficial cracks in cement screeds on concrete or brick surfaces not exceeding 1mm wide by opening cracks, preparing and applying a suitable thick slurry finishing flush to match existing (floor finishers where applicable measured elsewhere)",null,null,0]
[{"$nulls":4},0]
["12.2.1","On horizontal top surfaces","m",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["12.2.2","On vertical surfaces","m",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["12.2.3","On treads and risers of stairs","m",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
[12.3,"Repairing cracks in cement screeds on concrete or brick surfaces exceeding 1mm wide by hacking up/off screeds 150mm wide on both sides of crack, preparing existing surface and laying new screeds on and including chicken mesh spiked to base finishing flush with existing surface to match existing  ",null,null,0]
[{"$nulls":4},0]
["12.3.1","On horizontal top surfaces","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["12.3.2","On vertical surfaces","m",1,{"v":39.25588736000001,"d":"39.26"}]
[{"$nulls":4},0]
["12.3.3","On treads and risers of stairs","m",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
[null,"GRANOLITHIC",null,null,0]
[{"$nulls":4},0]
[12.4,"Untinted granolithic on concrete",null,null,0]
[{"$nulls":4},0]
["12.4.1","25mm. thick on floors and landings","m²",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["12.4.2","Average 40mm thick on floors to falls","m²",1,{"v":136.16885928000002,"d":"136.17"}]
[{"$nulls":4},0]
["12.4.3","Average 40mm thick on floors to falls and currents","m²",1,{"v":136.16885928000002,"d":"136.17"}]
[{"$nulls":4},0]
["12.4.4","25mm thick treads and risers of stairs ","m²",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["12.4.5","25mm thick treads and risers of stairs including reeding ","m²",1,{"v":109.18043672000002,"d":"109.18"}]
[{"$nulls":4},0]
["12.4.6","25mm thick on narrow widths","m²",1,{"v":90.77923952,"d":"90.78"}]
[{"$nulls":4},0]
["12.4.7","Skirting 75mm high","m",1,{"v":12.2674648,"d":"12.27"}]
[{"$nulls":4},0]
["12.4.8","Skirting 75mm high stepped over treads and risers","m",1,{"v":18.401197200000006,"d":"18.40"}]
[{"$nulls":4},0]
["12.4.9","Skirting 75mm high average 150mm high racked over treads and risers","m",1,{"v":23.308183120000006,"d":"23.31"}]
[{"$nulls":4},0]
[12.5,"Repairing superficial cracks in untinted granolithic screeds on concrete or brick surfaces not exceeding 1mm wide by opening cracks, preparing and applying a suitable thick slurry finishing flush to match existing",null,null,0]
[{"$nulls":4},0]
["12.5.1","On horizontal top surfaces","m",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["12.5.2","On vertical surfaces","m",1,{"v":7.360478880000001,"d":"7.36"}]
[{"$nulls":4},0]
["12.5.3","On treads and risers of stairs","m",1,{"v":8.58722536,"d":"8.59"}]
[{"$nulls":4},0]
[12.6,"Repairing cracks in untinted granolithic screeds on concrete or brick surfaces exceeding 1mm wide by hacking up/off screeds 150mm wide on both sides of crack, preparing existing surface and laying new screeds on and including chicken mesh spiked to base finishing flush with existing surface to match existing  ",null,null,0]
[{"$nulls":4},0]
["12.6.1","On horizontal top surfaces","m",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
["12.6.2","On vertical surfaces","m",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
["12.6.3","On treads and risers of stairs","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
[12.7,"Sundries",null,null,0]
[{"$nulls":4},0]
["12.7.1","Fix in position steel/uPVC underfloor cable duct 150 x 30mm deep overall including levelling by means of wedges and mortar packing, securing in position whilst screeding and working screed around and under duct and junction boxes, to finish levels with floor finish (ducts supplied and places roughly in position by others)","m",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
[null,"INTERNAL PLASTER",null,null,0]
[{"$nulls":4},0]
[12.8,"Two coat cement plaster with gypsum finish on brickwork/concrete",null,null,0]
[{"$nulls":4},0]
["12.8.1","On walls ","m²",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["12.8.2","On walls in sunk/raised panels","m²",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["12.8.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":101.81995784000003,"d":"101.82"}]
[{"$nulls":4},0]
["12.8.4","On circular walls","m²",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["12.8.5","On narrow widths","m²",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
[12.9,"Cement plaster steel trowelled on brickwork/concrete",null,null,0]
[{"$nulls":4},0]
["12.9.1","On walls ","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.9.2","On walls in sunk/raised panels","m²",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["12.9.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["12.9.4","On circular walls","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.9.5","On narrow widths","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.9.6","On ceilings","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["12.9.7","On raking soffits of stairs","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["12.9.8","On projecting and isolated columns/beams","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
[{"v":12.1,"d":"12.10"},"Cement plaster wood floated on brickwork/concrete",null,null,0]
[{"$nulls":4},0]
["12.10.1","On walls ","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.10.2","On walls in sunk/raised panels","m²",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["12.10.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["12.10.4","On circular walls","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.10.5","On narrow widths","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.10.6","On ceilings","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["12.10.7","On raking soffits of stairs","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["12.10.8","On projecting and isolated columns/beams","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
[12.11,"Fine rough-cast plaster on brickwork/concrete",null,null,0]
[{"$nulls":4},0]
["12.11.1","On walls ","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.11.2","On walls in sunk/raised panels","m²",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["12.11.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":69.92454936000001,"d":"69.92"}]
[{"$nulls":4},0]
["12.11.4","On circular walls","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.11.5","On narrow widths","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
["12.11.6","On ceilings","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["12.11.7","On raking soffits of stairs","m²",1,{"v":74.83153528,"d":"74.83"}]
[{"$nulls":4},0]
["12.11.8","On projecting and isolated columns/beams","m²",1,{"v":66.24430992,"d":"66.24"}]
[{"$nulls":4},0]
[12.12,"Repairing cracks in internal cement plaster on concrete or brick surfaces exceeding 1mm wide by hacking off plaster 150mm wide on both sides of crack, preparing existing surface and applying new plaster on and including chicken mesh spiked to base finishing flush with existing surface (painting measured elsewhere)",null,null,0]
[{"$nulls":4},0]
["12.12.1","On horizontal top surfaces","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["12.12.2","On sloping top surfaces","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["12.12.3","On vertical surfaces","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["12.12.4","On vertical surfaces circular","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["12.12.5","On horizontal soffits","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["12.12.6","On horizontal soffits circular","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["12.12.7","On raking soffits","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["12.12.8","EXTERNAL PLASTER",null,null,0]
[{"$nulls":4},0]
[12.13,"Cement plaster on brickwork/concrete",null,null,0]
[{"$nulls":4},0]
["12.13.1","On walls ","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.13.2","On walls in sunk/raised panels","m²",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["12.13.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["12.13.4","On circular walls","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.13.5","On narrow widths","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.13.6","On ceilings","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["12.13.7","On raking soffits of stairs","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["12.13.8","On projecting and isolated columns/beams","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
[12.14,"Rough-cast plaster on brickwork/concrete",null,null,0]
[{"$nulls":4},0]
["12.14.1","On walls ","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.14.2","On walls in sunk/raised panels","m²",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["12.14.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":77.28502824,"d":"77.29"}]
[{"$nulls":4},0]
["12.14.4","On circular walls","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.14.5","On narrow widths","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.14.6","On ceilings","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["12.14.7","On raking soffits of stairs","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["12.14.8","On projecting and isolated columns/beams","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
[12.15,"Repairing cracks in external cement plaster on concrete or brick surfaces exceeding 1mm wide by hacking off plaster 150mm wide on both sides of crack, preparing existing surface and applying new plaster on and including chicken mesh spiked to base finishing flush with existing surface (painting measured elsewhere)",null,null,0]
[{"$nulls":4},0]
["12.15.1","On horizontal top surfaces","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["12.15.2","On sloping top surfaces","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["12.15.3","On vertical surfaces","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["12.15.4","On vertical surfaces circular","m",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
["12.15.5","On horizontal soffits","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["12.15.6","On horizontal soffits circular","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["12.15.7","On raking soffits","m",1,{"v":38.02914088,"d":"38.03"}]
[{"$nulls":4},0]
["12.15.8","SPECIALIST PLASTER WALL COVERINGS",null,null,0]
[{"$nulls":4},0]
[null,"All specialist plaster wall coverings are to be executed in strict accordance with the manufacturer's instructions",null,null,0]
[{"$nulls":4},0]
[12.16,"\"Gamma Zenith\" or equal and approved 2,5mm thick \"Striato Medium\" pure acrylic plasticised coating with trowel on finish on plaster",null,null,0]
[{"$nulls":4},0]
["12.16.1","On walls ","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.16.2","On walls in sunk/raised panels","m²",1,{"v":76.05828176,"d":"76.06"}]
[{"$nulls":4},0]
["12.16.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":76.05828176,"d":"76.06"}]
[{"$nulls":4},0]
["12.16.4","On circular walls","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.16.5","On narrow widths","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
["12.16.6","On ceilings","m²",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["12.16.7","On raking soffits of stairs","m²",1,{"v":84.64550712,"d":"84.65"}]
[{"$nulls":4},0]
["12.16.8","On projecting and isolated columns/beams","m²",1,{"v":72.37804232000002,"d":"72.38"}]
[{"$nulls":4},0]
[12.17,"Repairing cracks in \"Gumma Zenith\" or equal and approved 2,5mm thick \"Striato Medium\" pure acrylic plasticised coating with trowel on finish on plastered concrete or brick surfaces exceeding 1mm wide by carefully cutting out in sections using straight horizontal and/or vertical saw cuts, hacking up/off and removing plaster 150mm wide on both sides of crack, preparing existing surface and applying new cement plaster on and including chicken mesh spiked to base, and finishing flush with \"Gamma Zenith\" covering to match existing surface",null,null,0]
[{"$nulls":4},0]
["12.17.1","On horizontal top surfaces","m",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["12.17.2","On sloping top surfaces","m",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["12.17.3","On vertical surfaces","m",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["12.17.4","On vertical surfaces circular","m",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
["12.17.5","On horizontal soffits","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["12.17.6","On horizontal soffits circular","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["12.17.7","On raking soffits","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
[12.18,"\"Gamma Zenith\" or equal and approved 3,0mm thick \"Granitico\" pure acrylic plasticised coating with stone finish on plaster",null,null,0]
[{"$nulls":4},0]
["12.18.1","On walls ","m²",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["12.18.2","On walls in sunk/raised panels","m²",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["12.18.3","On walls between timber grounds (area of grounds not deducted)","m²",1,{"v":95.68622544000003,"d":"95.69"}]
[{"$nulls":4},0]
["12.18.4","On circular walls","m²",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["12.18.5","On narrow widths","m²",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
["12.18.6","On ceilings","m²",1,{"v":105.50019728000004,"d":"105.50"}]
[{"$nulls":4},0]
["12.18.7","On raking soffits of stairs","m²",1,{"v":105.50019728000004,"d":"105.50"}]
[{"$nulls":4},0]
["12.18.8","On projecting and isolated columns/beams","m²",1,{"v":92.00598600000001,"d":"92.01"}]
[{"$nulls":4},0]
[12.19,"Repairing cracks in \"Gumma Zenith\" or equal and approved 3,0mm thick \"Granitico\" pure acrylic plasticised coating with stone finish on plastered concrete or brick surfaces exceeding 1mm wide by carefully cutting out in sections using straight horizontal and/or vertical saw cuts, hacking up/off and removing plaster 150mm wide on both sides of crack, preparing existing surface and applying new cement plaster on and including chicken mesh spiked to base, and finishing flush with \"Gamma Zenith\" covering to match existing surface",null,null,0]
[{"$nulls":4},0]
["12.19.1","On horizontal top surfaces","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["12.19.2","On sloping top surfaces","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["12.19.3","On vertical surfaces","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["12.19.4","On vertical surfaces circular","m",1,{"v":57.65708456,"d":"57.66"}]
[{"$nulls":4},0]
["12.19.5","On horizontal soffits","m",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["12.19.6","On horizontal soffits circular","m",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
["12.19.7","On raking soffits","m",1,{"v":63.790816960000015,"d":"63.79"}]
[{"$nulls":4},0]
[{"v":12.2,"d":"12.20"},"Two coats gypsum plaster \"Rhinolite\" polished to a smooth finish",null,null,0]
[{"$nulls":4},0]
["12.20.1","Plaster","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.20.2","Plaster in patches","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.20.3","Gypsum plasterboard ceilings, bulkheads, etc","m²",1,{"v":134.94211280000002,"d":"134.94"}]
[{"$nulls":4},0]
["12.20.4","Gypsum plasterboard ceilings, bulkheads, etc in patches","m²",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["12.20.5","Gypsum plasterboard partitioning","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.20.6","Gypsum plasterboard partitioning in patches","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
[12.21,"Two coats gypsum plaster \"Rhinolite\" to a brushed finish",null,null,0]
[{"$nulls":4},0]
["12.21.1","Plaster","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.21.2","Plaster in patches","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.21.3","Gypsum plasterboard ceilings, bulkheads, etc","m²",1,{"v":134.94211280000002,"d":"134.94"}]
[{"$nulls":4},0]
["12.21.4","Gypsum plasterboard ceilings, bulkheads, etc in patches","m²",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["12.21.5","Gypsum plasterboard partitioning","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.21.6","Gypsum plasterboard partitioning in patches","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
[12.22,"Two coats gypsum plaster \"Rhinolite\" polished to a textured finish",null,null,0]
[{"$nulls":4},0]
["12.22.1","Plaster","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.22.2","Plaster in patches","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.22.3","Gypsum plasterboard ceilings, bulkheads, etc","m²",1,{"v":134.94211280000002,"d":"134.94"}]
[{"$nulls":4},0]
["12.22.4","Gypsum plasterboard ceilings, bulkheads, etc in patches","m²",1,{"v":138.62235224000003,"d":"138.62"}]
[{"$nulls":4},0]
["12.22.5","Gypsum plasterboard partitioning","m²",1,{"v":110.40718320000003,"d":"110.41"}]
[{"$nulls":4},0]
["12.22.6","Gypsum plasterboard partitioning in patches","m²",1,{"v":36.80239440000001,"d":"36.80"}]
[{"$nulls":4},0]
[null,"AIR GRATINGS",null,null,0]
[{"$nulls":4},0]
[12.23,"Air gratings",null,null,0]
[{"$nulls":4},0]
["12.23.1","110 x 150mm cast plaster or white plastic plain pattern air grating fixed with plaster face","no",1,{"v":19.627943680000005,"d":"19.63"}]
[{"$nulls":4},0]
[null,"CORNER PROTECTORS, DIVIDING STRIPS. ETC",null,null,0]
[{"$nulls":4},0]
[12.24,"Dividing strips",null,null,0]
[{"$nulls":4},0]
["12.24.1","30 x 3mm flat brass dividing strip between different floor finishes","m",1,{"v":88.32574656000003,"d":"88.33"}]
{"$rows_empty":25}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Tiling","index":12,"n_rows":283,"n_cols":12,"rows_kept":283,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 13"]
[]
[null,"TILING"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":9},1.06]
[]
[null,"Unless described as \"fixed with adhesive to plaster (plaster elsewhere)\" descriptions of tiling on brick or concrete walls, columns, etc shall be deemed to include 1:4 cement plaster backing and descriptions of tiling on concrete floors etc shall be deemed to include 1:3 plaster bedding"]
[]
[null,"WALL TILING"]
[]
[13.1,"300 x 600 x 10mm. white glazed ceramic tiles fixed with adhesive to plaster (plaster elsewhere)"]
[]
["13.1.1","On horizontal top surfaces","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["13.1.2","On sloping top surfaces","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["13.1.3","On vertical surfaces","m²",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["13.1.4","On vertical surfaces circular","m²",1,{"v":195.05269032000007,"d":"195.05"}]
[{"$nulls":4},0]
["13.1.5","On horizontal soffits","m²",1,{"v":195.05269032000007,"d":"195.05"}]
[{"$nulls":4},0]
["13.1.6","On narrow widths","m²",1,{"v":199.95967624000002,"d":"199.96"}]
[{"$nulls":4},0]
["13.1.7","Circular cutting","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
[13.2,"600 x 1200 x 10mm. white glazed Porceline tiles fixed with adhesive to plaster (plaster elsewhere) ",null,null,0]
[{"$nulls":4},0]
["13.2.1","On horizontal top surfaces","m²",1,{"v":214.68063400000003,"d":"214.68"}]
[{"$nulls":4},0]
["13.2.2","On sloping top surfaces","m²",1,{"v":214.68063400000003,"d":"214.68"}]
[{"$nulls":4},0]
["13.2.3","On vertical surfaces","m²",1,{"v":214.68063400000003,"d":"214.68"}]
[{"$nulls":4},0]
["13.2.4","On vertical surfaces circular","m²",1,{"v":226.94809880000008,"d":"226.95"}]
[{"$nulls":4},0]
["13.2.5","On horizontal soffits","m²",1,{"v":226.94809880000008,"d":"226.95"}]
[{"$nulls":4},0]
["13.2.6","On narrow widths","m²",1,{"v":231.85508472,"d":"231.86"}]
[{"$nulls":4},0]
["13.2.7","Circular cutting","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
[13.3,"Ceramic wall tiles (PC sum R85.00/m² for supply and delivery, excluding labour, waste and VAT) fixed with adhesive to plaster (plaster elsewhere) and flush pointed with tinted waterproof jointing compound ",null,null,0]
[{"$nulls":4},0]
["13.3.1","On horizontal top surfaces","m²",1,{"v":228.17484528000003,"d":"228.17"}]
[{"$nulls":4},0]
["13.3.2","On sloping top surfaces","m²",1,{"v":228.17484528000003,"d":"228.17"}]
[{"$nulls":4},0]
["13.3.3","On vertical surfaces","m²",1,{"v":228.17484528000003,"d":"228.17"}]
[{"$nulls":4},0]
["13.3.4","On vertical surfaces circular","m²",1,{"v":239.21556360000005,"d":"239.22"}]
[{"$nulls":4},0]
["13.3.5","On horizontal soffits","m²",1,{"v":239.21556360000005,"d":"239.22"}]
[{"$nulls":4},0]
["13.3.6","On narrow widths","m²",1,{"v":245.34929600000004,"d":"245.35"}]
[{"$nulls":4},0]
["13.3.7","Circular cutting","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
[null,"240x116x7.4mm White glazed ceramic tiles fixed with adhesive to plaster, screeds, etc",null,null,0]
[{"$nulls":4},0]
["13.3.7a","On walls","m2",{"v":1,"d":"1.00"},{"v":357.73154103280007,"d":"357.73"}]
[{"$nulls":4},0]
[null,"100x100x5mm \"Novodoma Mosaic\" sheet black shiny tiles fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.3.7b","On walls","m²",{"v":1,"d":"1.00"},{"v":434.3418587088001,"d":"434.34"}]
[{"$nulls":4},0]
["13.3.7b","Extra over for cross pattern","m²",{"v":1,"d":"1.00"},{"v":119.44830475760003,"d":"119.45"}]
[{"$nulls":4},0]
[null,"250x250x5mm \"Glass Mosaic B50-31-30-13\" sheet blue shiny tiles fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.3.7c","On walls","m²",{"v":1,"d":"1.00"},{"v":434.3295912440001,"d":"434.33"}]
[{"$nulls":4},0]
[null,"Code \"311200900\" White Glossy\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.3.7c","On walls","m²",{"v":1,"d":"1.00"},{"v":437.5313995568001,"d":"437.53"}]
[{"$nulls":4},0]
[null,"Code \"311200901\" White Glossy\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.3.7e","On walls","m²",{"v":1,"d":"1.00"},{"v":467.0959897248001,"d":"467.10"}]
[{"$nulls":4},0]
[null,"Code \"311200710\" Light Blue Glossy\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.3.7f","On walls","m²",{"v":1,"d":"1.00"},{"v":453.6753832336001,"d":"453.68"}]
[{"$nulls":4},0]
[null,"FLOOR TILING",null,null,0]
[{"$nulls":4},0]
[13.4,"Ceramic floor tiles (PC sum R125.00/m² for supply and delivery, excluding labour, waste and VAT) fixed with adhesive to bedding (bedding elsewhere) and flush pointed with tinted jointing compound ",null,null,0]
[{"$nulls":4},0]
["13.4.1","On horizontal top surfaces","m²",1,{"v":290.73891576,"d":"290.74"}]
[{"$nulls":4},0]
["13.4.2","On vertical surfaces","m²",1,{"v":290.73891576,"d":"290.74"}]
[{"$nulls":4},0]
["13.4.3","On narrow widths","m²",1,{"v":290.73891576,"d":"290.74"}]
[{"$nulls":4},0]
["13.4.4","On horizontal surfaces to falls and currents","m²",1,{"v":301.77963408000005,"d":"301.78"}]
[{"$nulls":4},0]
["13.4.5","On treads and risers of stairs","m²",1,{"v":310.3668594400001,"d":"310.37"}]
[{"$nulls":4},0]
["13.4.6","Skirtings 100mm high of stretcher course tiles ","m",1,{"v":34.34890144,"d":"34.35"}]
[{"$nulls":4},0]
["13.4.7","Skirtings exceeding 100mm high and not exceeding 150mm high of stretcher course tiles ","m",1,{"v":47.843112720000015,"d":"47.84"}]
[{"$nulls":4},0]
["13.4.8","Circular cutting","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
[null,"240x116x7.4mm White glazed ceramic tiles fixed with adhesive to plaster, screeds, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8a","On floors","m²",{"v":1,"d":"1.00"},{"v":357.73154103280007,"d":"357.73"}]
[{"$nulls":4},0]
["13.4.8b","100x100x5mm \"Novodoma Mosaic\" sheet black shiny tiles fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
[{"$nulls":4},0]
["13.4.8c1","In lanes","m",{"v":1,"d":"1.00"},{"v":69.63013020480001,"d":"69.63"}]
[{"$nulls":4},0]
["13.4.8c2","Extra over for cross pattern","m²",{"v":1,"d":"1.00"},{"v":119.44830475760003,"d":"119.45"}]
[{"$nulls":4},0]
["13.4.8d3","Extra over for \"City of Joburg\" logo pattern","m²",{"v":1,"d":"1.00"},{"v":266.4248005264,"d":"266.42"}]
[{"$nulls":4},0]
["13.4.8e","295x295x5mm \"Non Skid\" tiles Code Union Tile \"1W22WYEXSL\"",null,null,0]
[{"$nulls":4},0]
["13.4.8e1","On floors","m²",{"v":1,"d":"1.00"},{"v":434.3418587088001,"d":"434.34"}]
[{"$nulls":4},0]
["13.4.8e2","Tile Skirting","m²",{"v":1,"d":"1.00"},{"v":56.855349304981935,"d":"56.86"}]
[{"$nulls":4},0]
["13.4.8f","Code \"311200781\" Matt Glazed Azurblau\" (dark blue) size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8f1","On floors","m²",{"v":1,"d":"1.00"},{"v":493.0662127064001,"d":"493.07"}]
[{"$nulls":4},0]
["13.4.8f2","Tile Skirting","m²",{"v":1,"d":"1.00"},{"v":64.54236724326778,"d":"64.54"}]
[{"$nulls":4},0]
["13.4.8g","Code \"311200786\" Non-Slip Azurblau\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8g1","On floors","m²",{"v":1,"d":"1.00"},{"v":618.3538307088002,"d":"618.35"}]
[{"$nulls":4},0]
["13.4.8g2","Tile Skirting","m²",{"v":1,"d":"1.00"},{"v":80.94251643978194,"d":"80.94"}]
[{"$nulls":4},0]
["13.4.8h","Code \"311200710\" Light Blue Glossy\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8h1","On floors","m²",{"v":1,"d":"1.00"},{"v":453.6753832336001,"d":"453.68"}]
[{"$nulls":4},0]
["13.4.8h2","Tile Skirting","m²",{"v":1,"d":"1.00"},{"v":59.38610766527826,"d":"59.39"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["13.4.8i","Code \"311200716\" Light Blue Non-Slip\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8i1","On floors","m²",{"v":1,"d":"1.00"},{"v":1159.0791441632002,"d":"1,159.08"}]
[{"$nulls":4},0]
["13.4.8i2","Tile Skirting","m²",{"v":1,"d":"1.00"},{"v":151.7234599709629,"d":"151.72"}]
[{"$nulls":4},0]
["13.4.8j","Code \"663130690\" RP1 Small Grooved tile Beige\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8j1","On floors","m²",{"v":1,"d":"1.00"},{"v":1159.0791441632002,"d":"1,159.08"}]
[{"$nulls":4},0]
["13.4.8k","Code \"663130690-788\" RP3 Small Grooved Tile Safety Marking Beige + Azurblau\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8k1","On floors","m²",{"v":1,"d":"1.00"},{"v":3046.2077892768,"d":"3,046.21"}]
[{"$nulls":4},0]
["13.4.8.l","Code \"663130690-786\" Non-slip Beige Blue Nose Rounded Azurblau Matt - Raised End Edges\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8l1","On floors","m²",{"v":1,"d":"1.00"},{"v":3574.9600570864004,"d":"3,574.96"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["13.4.8m","Code \"311200906\" RHB Non-Slip White\" size 244x119mm fixed with adhesive to plaster, screed, etc",null,null,0]
[{"$nulls":4},0]
["13.4.8m1","On floors","m²",{"v":1,"d":"1.00"},{"v":549.3984110680001,"d":"549.40"}]
[{"$nulls":4},0]
[null,"CHANNELS",null,null,0]
[{"$nulls":4},0]
[13.5,"\"Vaal\" or equal and approved white glazed fireclay block channels bedded and jointed in 1:3 cement mortar and pointed with flush joints in 1:3 white cement mortar",null,null,0]
[{"$nulls":4},0]
["13.5.1","150 x 100mm block SCUM channels","m",1,{"v":772.8502824000002,"d":"772.85"}]
[{"$nulls":4},0]
["13.5.2","Extra over block channels for Fair end","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
["13.5.3","Extra over block channels for Stopped end","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
["13.5.4","Extra over block channels for Angle","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
["13.5.5","Extra over block channels for T-intersection","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
["13.5.6","Extra over block channels for X-intersection","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
["13.5.7","Extra over block channels for Outlet","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
["13.5.8","Extra over block channels for Stopped end with outlet","no",1,{"v":223.26785936000005,"d":"223.27"}]
[{"$nulls":4},0]
[null,"TOILET PAPER HOLDERS ETC ",null,null,0]
[{"$nulls":4},0]
[13.6,"\"Johnson\" or equal and approved white glazed ceramic",null,null,0]
[{"$nulls":4},0]
["13.6.1","150 x 150mm semi-recessed toilet paper holder","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
["13.6.2","150 x 150mm semi-recessed soap dish","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
[null,"POLISHED FLOORS",null,null,0]
[{"$nulls":4},0]
[13.7,"Grinding and polishing of concrete floor to \"HTC Superfloor\" or equivalent",null,null,0]
[{"$nulls":4},0]
["13.7.1","Floors not exceeding 500m2","m2",1,{"v":588.8383104000002,"d":"588.84"}]
[{"$nulls":4},0]
["13.7.2","Floors exceeding 500m2 and not exceeding 1000m2","m2",1,{"v":426.90777504,"d":"426.91"}]
[{"$nulls":4},0]
["13.7.3","Floors exceeding 1000m2 and not exceeding 2000m2","m2",1,{"v":412.18681728000007,"d":"412.19"}]
[{"$nulls":4},0]
["13.7.4","Floors exceeding 2000m2 and not exceeding 5000m2","m2",1,{"v":397.46585952000004,"d":"397.47"}]
[{"$nulls":4},0]
["13.7.5","Floors exceeding 5000m2 and not exceeding 10000m2","m2",1,{"v":382.7449017600001,"d":"382.74"}]
[{"$nulls":4},0]
["13.7.8","Floors exceeding 1000m2 and not exceeding 2000m2","m2",1,{"v":368.02394400000003,"d":"368.02"}]
[{"$nulls":4},0]
[13.8,"Grinding and polishing of concrete floor to \"HTC Superfloor\" in partitioned areas or equivalent",null,null,0]
[{"$nulls":4},0]
["13.8.1","Floors not exceeding 500m2","m2",1,{"v":647.7221414400002,"d":"647.72"}]
[{"$nulls":4},0]
["13.8.2","Floors exceeding 500m2 and not exceeding 1000m2","m2",1,{"v":485.79160608000007,"d":"485.79"}]
[{"$nulls":4},0]
["13.8.3","Floors exceeding 1000m2 and not exceeding 2000m2","m2",1,{"v":471.0706483200001,"d":"471.07"}]
[{"$nulls":4},0]
["13.8.4","Floors exceeding 2000m2 and not exceeding 5000m2","m2",1,{"v":456.34969056000006,"d":"456.35"}]
[{"$nulls":4},0]
["13.8.5","Floors exceeding 5000m2 and not exceeding 10000m2","m2",1,{"v":441.62873280000014,"d":"441.63"}]
[{"$nulls":4},0]
["13.8.6","Floors exceeding 1000m2 and not exceeding 2000m2","m2",1,{"v":426.90777504,"d":"426.91"}]
[{"$nulls":4},0]
[13.9,"\"HTC Twister\" Restoration deep clean",null,null,0]
[{"$nulls":4},0]
["13.9.1","Linoleum/vinyl","m2",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["13.9.2","Powerfloat concrete floor","m2",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
["13.9.3","Granite","m2",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["13.9.4","Marble","m2",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["13.9.5","Terrazo","m2",1,{"v":191.37245088000006,"d":"191.37"}]
[{"$nulls":4},0]
["13.10.","\"HTC Stain\" Resistance",null,null,0]
[{"$nulls":4},0]
["13.10.1","Single coat","m2",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
[13.11,"Cementation overlay",null,null,0]
[{"$nulls":4},0]
["13.11.1","Placement","m2",1,{"v":1317.5257195200002,"d":"1,317.53"}]
[{"$nulls":4},0]
["13.11.2","Door raising","no",1,{"v":250.25628192000005,"d":"250.26"}]
[{"$nulls":4},0]
[13.12,"Polished Porcelain  floor tiles (PC sum R189.00/m² for supply and delivery, excluding labour, waste and VAT) fixed with adhesive to bedding (bedding elsewhere) and flush pointed with tinted jointing compound ",null,null,0]
[{"$nulls":4},0]
["13.12.1","On horizontal top surfaces","m²",1,{"v":394.15595864,"d":"394.16"}]
[{"$nulls":4},0]
["13.12.2","On vertical surfaces","m²",1,{"v":394.15595864,"d":"394.16"}]
[{"$nulls":4},0]
["13.12.3","On narrow widths","m²",1,{"v":394.15595864,"d":"394.16"}]
[{"$nulls":4},0]
["13.12.4","On horizontal surfaces to falls and currents","m²",1,{"v":417.3368378800001,"d":"417.34"}]
[{"$nulls":4},0]
["13.12.5","On treads and risers of stairs","m²",1,{"v":417.3368378800001,"d":"417.34"}]
[{"$nulls":4},0]
["13.12.6","Skirtings 100mm high of stretcher course tiles ","m",1,{"v":41.73252648000001,"d":"41.73"}]
[{"$nulls":4},0]
["13.12.7","Skirtings exceeding 100mm high and not exceeding 150mm high of stretcher course tiles ","m",1,{"v":62.598789720000006,"d":"62.60"}]
[{"$nulls":4},0]
["13.12.8","Circular cutting","m",1,{"v":83.46505296000002,"d":"83.47"}]
{"$rows_empty":15}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Glazing","index":13,"n_rows":153,"n_cols":7,"rows_kept":153,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","Unit","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 14"]
[]
[]
[null,"GLAZING"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"GLAZING TO STEEL WITH PUTTY"]
[]
[14.1,"4mm. clear float glass"]
[]
["14.1.1","4mm Glass","m²",1,{"v":306.68662,"d":"306.69"}]
[{"$nulls":4},0]
["14.1.2","4mm Glass in cottage sashes","m²",1,{"v":337.35528200000005,"d":"337.36"}]
[{"$nulls":4},0]
["14.1.3","4mm Glass in shapes other than rectangular","m²",1,{"v":337.35528200000005,"d":"337.36"}]
[{"$nulls":4},0]
[14.2,"4mm. patterned glass",null,null,0]
[{"$nulls":4},0]
["14.2.1","4mm Glass","m²",1,{"v":398.69260600000007,"d":"398.69"}]
[{"$nulls":4},0]
["14.2.2","4mm Glass in cottage sashes","m²",1,{"v":438.56186660000003,"d":"438.56"}]
[{"$nulls":4},0]
["14.2.3","4mm Glass in shapes other than rectangular","m²",1,{"v":438.56186660000003,"d":"438.56"}]
[{"$nulls":4},0]
[14.3,"6.38mm clear toughened safety glass",null,null,0]
[{"$nulls":4},0]
["14.3.1","6.38mm Glass","m²",1,{"v":775.3037753600003,"d":"775.30"}]
[{"$nulls":4},0]
["14.3.2","6.38mm Glass in shapes other than rectangular","m²",1,{"v":853.81555008,"d":"853.82"}]
[{"$nulls":4},0]
[null,"GLAZING TO WOOD WITH PINNED ON BEADS (BEADS MEASURED ELSEWHERE)",null,null,0]
[{"$nulls":4},0]
[14.4,"4mm. clear float glass",null,null,0]
[{"$nulls":4},0]
["14.4.1","4mm Glass","m²",1,{"v":306.68662,"d":"306.69"}]
[{"$nulls":4},0]
["14.4.2","4mm Glass in cottage sashes","m²",1,{"v":337.35528200000005,"d":"337.36"}]
[{"$nulls":4},0]
["14.4.3","4mm Glass in shapes other than rectangular","m²",1,{"v":337.35528200000005,"d":"337.36"}]
[{"$nulls":4},0]
[14.5,"4mm. patterned glass",null,null,0]
[{"$nulls":4},0]
["14.5.1","4mm Glass","m²",1,{"v":398.69260600000007,"d":"398.69"}]
[{"$nulls":4},0]
["14.5.2","4mm Glass in cottage sashes","m²",1,{"v":438.56186660000003,"d":"438.56"}]
[{"$nulls":4},0]
["14.5.3","4mm Glass in shapes other than rectangular","m²",1,{"v":438.56186660000003,"d":"438.56"}]
[{"$nulls":4},0]
[14.6,"6.38mm clear toughened safety glass",null,null,0]
[{"$nulls":4},0]
["14.6.1","6.38mm Glass","m²",1,{"v":775.3037753600003,"d":"775.30"}]
[{"$nulls":4},0]
["14.6.2","6.38mm Glass in shapes other than rectangular","m²",1,{"v":853.81555008,"d":"853.82"}]
[{"$nulls":4},0]
[null,"GLAZING TO ALUMINIUM WITH CLIP ON BEADS (BEADS MEASURED ELSEWHERE)",null,null,0]
[{"$nulls":4},0]
[14.7,"4mm. clear float glass",null,null,0]
[{"$nulls":4},0]
["14.7.1","4mm Glass","m²",1,{"v":217.13412696000003,"d":"217.13"}]
[{"$nulls":4},0]
["14.7.2","4mm Glass in cottage sashes","m²",1,{"v":222.04111288000004,"d":"222.04"}]
[{"$nulls":4},0]
["14.7.3","4mm Glass in shapes other than rectangular","m²",1,{"v":244.12254952000004,"d":"244.12"}]
[{"$nulls":4},0]
[14.8,"4mm. patterned glass",null,null,0]
[{"$nulls":4},0]
["14.8.1","4mm Glass","m²",1,{"v":381.5181552800001,"d":"381.52"}]
[{"$nulls":4},0]
["14.8.2","4mm Glass in cottage sashes","m²",1,{"v":385.1983947200001,"d":"385.20"}]
[{"$nulls":4},0]
["14.8.3","4mm Glass in shapes other than rectangular","m²",1,{"v":423.2275356000001,"d":"423.23"}]
[{"$nulls":4},0]
[14.9,"6.38mm clear toughened safety glass",null,null,0]
[{"$nulls":4},0]
["14.9.1","6.38mm Glass","m²",1,{"v":775.3037753600003,"d":"775.30"}]
[{"$nulls":4},0]
["14.9.2","6.38mm Glass in shapes other than rectangular","m²",1,{"v":853.81555008,"d":"853.82"}]
[{"$nulls":4},0]
[null,"GLASS LOUVRE BLADES",null,null,0]
[{"$nulls":4},0]
[{"v":14.1,"d":"14.10"},"6mm Clear Glass Louvre Blades",null,null,0]
[{"$nulls":4},0]
["14.10.1","Louvre blades not exceeding 150mm wide with polished edges","m",1,{"v":214.68063400000003,"d":"214.68"}]
[{"$nulls":4},0]
[null,"GLASS IN TOPS, SHELVES, DOORS, MIRRORS, ETC.",null,null,0]
[{"$nulls":4},0]
[14.11,"5mm Silvered float glass copper backed mirrors with polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete ",null,null,0]
[{"$nulls":4},0]
["14.11.1","Mirror 300 x 300mm high with four screws","no",1,{"v":96.91297192000003,"d":"96.91"}]
[{"$nulls":4},0]
["14.11.2","Mirror 400 x 400mm high with four screws","no",1,{"v":142.30259168000003,"d":"142.30"}]
[{"$nulls":4},0]
["14.11.3","Mirror 400 x 600mm high with four screws","no",1,{"v":198.73292976000002,"d":"198.73"}]
[{"$nulls":4},0]
["14.11.4","Mirror size 400 x 600mm and screw fixing in recess to match existing ","m²",1,{"v":893.0714374400002,"d":"893.07"}]
[{"$nulls":4},0]
[14.12,"5mm Silvered float glass copper backed mirrors with 10mm bevelled and polished edges holed for and fixed with chromium plated dome capped mirror screws with rubber buffers to plugs in brickwork or concrete ",null,null,0]
[{"$nulls":4},0]
["14.12.1","Mirror 300 x 300mm high with four screws","no",1,{"v":182.78522552,"d":"182.79"}]
[{"$nulls":4},0]
["14.12.2","Mirror 400 x 400mm high with four screws","no",1,{"v":252.70977488000005,"d":"252.71"}]
[{"$nulls":4},0]
["14.12.3","Mirror 400 x 600mm high with four screws","no",1,{"v":339.80877496000005,"d":"339.81"}]
[{"$nulls":4},0]
["14.12.4","Mirror size and screw fixing in recess to match existing ","m²",1,{"v":1176.4498743200002,"d":"1,176.45"}]
[{"$nulls":4},0]
[null,"Sundries",null,null,0]
[{"$nulls":4},0]
[14.13,"Sandblasting",null,null,0]
[{"$nulls":4},0]
["14.13.1","To glazing","m²",1,{"v":435.4950004000001,"d":"435.50"}]
[{"$nulls":4},0]
[14.14,"Vinyl films and tinting",null,null,0]
[{"$nulls":4},0]
["14.14.1","Vinyl film to glazing","m²",1,{"v":435.4950004000001,"d":"435.50"}]
[{"$nulls":4},0]
["14.14.2","Vinyl film  including muriels to glazing","m²",1,{"v":1042.734508,"d":"1,042.73"}]
[{"$nulls":4},0]
[14.15,"Awnings",null,null,0]
[{"$nulls":4},0]
["14.15.1","Vinyl tinted awning including frame fixed to walls,concrete,wood,etc",null,null,0]
[null,"not exceeding 1200mm length","no",1,{"v":2760.1795800000004,"d":"2,760.18"}]
[{"$nulls":4},0]
["14.15.2","Vinyl tinted awning including frame fixed to walls,concrete,wood,etc",null,null,0]
[null,"exceeding 1200mm and not exceeding 2400mm length","no",1,{"v":4830.314265000001,"d":"4,830.31"}]
{"$rows_empty":21}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Painting","index":14,"n_rows":358,"n_cols":7,"rows_kept":358,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 15"]
[]
[null,"PAINTING"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Descriptions"]
[]
[null,"Description of paintwork shall be deemed to include for all cutting in"]
[]
[null,"Paint Specifications"]
[]
[null,"All painting shall be carried out in strict accordance with \"Plascon\" or equally approved specifications"]
[]
[null,"PAINTWORK, ETC. TO NEW WORK"]
[]
[null,"ON BRICKS OR QUARRY TILES"]
[]
[15.1,"Two coats solvent based UV resistant clear gloss acrylic brick dressing"]
[]
["15.1.1","On sills, thresholds, etc","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.1.2","On flush pointed face walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.1.3","On recessed pointed face walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
[null,"ON FLOATED PLASTER",null,null,0]
[{"$nulls":4},0]
[15.2,"One coat alkaline resistant plaster primer, one coat universal alkyd based undercoat and one coats alkyd based eggshell enamel paint",null,null,0]
[{"$nulls":4},0]
["15.2.1","On internal walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.3,"One coat alkaline resistant plaster primer and two coats superior acrylic PVA emulsion paint",null,null,0]
[{"$nulls":4},0]
["15.3.1","On internal walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.3.2","On ceilings","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.4,"One coat resin based bonding liquid two coats superior acrylic PVA emulsion paint",null,null,0]
[{"$nulls":4},0]
["15.4.1","On external walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
[15.5,"One coat resin based bonding liquid and two coats UV resistant water based mica and marble waterproof fine texture paint",null,null,0]
[{"$nulls":4},0]
["15.5.1","On external walls","m²",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
[null,"ON FAIR FACE BRICKWORK",null,null,0]
[{"$nulls":4},0]
[15.6,"One coat alkaline resistant plaster primer, one coat universal alkyd based undercoat and two coats superior acrylic PVA emulsion paint",null,null,0]
[{"$nulls":4},0]
["15.6.1","On internal walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.6.2","On external walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
[null,"0N PLASTER BOARD",null,null,0]
[{"$nulls":4},0]
[15.7,"One coat alkaline resistant plaster primer and two coats superior acrylic PVA emulsion paint",null,null,0]
[{"$nulls":4},0]
["15.7.1","On ceilings and cornices","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.7.2","On drywall partitions","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[null,"ON FIBRE-CEMENT",null,null,0]
[{"$nulls":4},0]
[15.8,"One coat resin based bonding liquid two full coats UV resistant water based acrylic roof paint",null,null,0]
[{"$nulls":4},0]
["15.8.1","On profiled roof sheets (measured on flat)","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.8.2","On fascias and barge boards","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.9,"One coat alkaline resistant plaster primer and two coats superior acrylic PVA emulsion paint",null,null,0]
[{"$nulls":4},0]
["15.9.1","On internal fibre cement ceilings including priming steel joints and nail heads with one coat zinc phosphate alkyd resin primer","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.9.2","On fascias and barge boards","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.9.3","On internal fibre cement sills not exceeding 300mm girth","m",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.9.4","On fascia and barge boards not exceeding 300mm girth","m",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[null,"ON METAL",null,null,0]
[{"$nulls":4},0]
[{"v":15.1,"d":"15.10"},"Spot prime defects in pre-primed surfaces with zinc chromate primer and apply one universal alkyd based undercoat and two coats alkyd based high gloss enamel paint",null,null,0]
[{"$nulls":4},0]
["15.10.1","On door frames","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.10.2","On recordroom and strongroom doors and frames","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.10.3","On window frames","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.10.4","On window frames with burglar bars","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.10.5","On gates, grilles, burglar screens, balustrades, steel palisade, etc (both sides measured over full flat area)","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.11,"One coat water based galvanised iron primer, one coat universal alkyd based undercoat and two coats alkyd based high gloss enamel paint",null,null,0]
[{"$nulls":4},0]
["15.11.1","On corrugated iron profile roof sheeting (measured on flat)","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.11.2","On IBR profile roof sheeting (measured on flat)","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.11.3","On eaves gutters","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.11.4","On rails, bars, pipes etc ","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["15.11.5","On eaves gutters/rainwater downpipes not exceeding 300mm girth","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
["15.11.6","On rails, bars, pipes etc not exceeding 300mm girth","m",1,{"v":28.215169040000006,"d":"28.22"}]
[{"$nulls":4},0]
[null,"ON WOOD",null,null,0]
[{"$nulls":4},0]
[15.12,"One coat wood primer, one universal alkyd based undercoat and two coats alkyd based eggshell enamel paint",null,null,0]
[{"$nulls":4},0]
["15.12.1","On boarded panelling","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.12.2","On boarded ceilings","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.12.3","On doors","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.12.4","On fittings","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.12.5","On roof timbers at eves and verges","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.12.6","Skirtings, rails, etc. not exceeding 300mm. girth","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
[15.13,"Three coats clear polyurethane suede varnish ",null,null,0]
[{"$nulls":4},0]
["15.13.1","On doors","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.13.2","Skirtings, rails, etc. not exceeding 300mm. girth","m",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
[null,"PAINTWORK, ETC. TO PREVIOUSLY PAINTED WORK",null,null,0]
[{"$nulls":4},0]
[null,"PREPARATORY WORK TO EXISTING WORK",null,null,0]
[{"$nulls":4},0]
[null,"Previously painted plastered surfaces",null,null,0]
[{"$nulls":4},0]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with suitable filler and finished smooth",null,null,0]
[{"$nulls":4},0]
[null,"Previously painted metal surfaces",null,null,0]
[{"$nulls":4},0]
[null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed down to bare metal",null,null,0]
[{"$nulls":4},0]
[null,"Previously painted wood surfaces",null,null,0]
[{"$nulls":4},0]
[null,"Surfaces shall be thoroughly cleaned down. Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth",null,null,0]
[{"$nulls":4},0]
[null,"ON BRICKS OR QUARRY TILES",null,null,0]
[{"$nulls":4},0]
[15.14,"Two coats solvent based UV resistant clear gloss acrylic brick dressing",null,null,0]
[{"$nulls":4},0]
["15.14.1","On sills, thresholds, etc","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.14.2","On flush pointed face walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.14.3","On recessed pointed face walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[null,"ON FLOATED PLASTER",null,null,0]
[{"$nulls":4},0]
[null,"One coat alkaline resistant plaster primer, one coat universal alkyd based undercoat and one coats alkyd based eggshell enamel paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.14.4","On internal walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.14.5","On columns","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.15,"One coat resin based bonding liquid two coats superior acrylic PVA emulsion paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.15.1","On internal walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.15.2","On external walls","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.15.3","On ceilings","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[null,"ON GAMMA ZENNITH",null,null,0]
[{"$nulls":4},0]
[15.16,"One coat resin based bonding liquid two coats superior glamour paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.16.1","On internal walls","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["15.16.2","On external walls","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
["15.16.3","On ceilings","m²",1,{"v":82.19201416000003,"d":"82.19"}]
[{"$nulls":4},0]
[null,"ON FAIR FACE BRICKWORK",null,null,0]
[{"$nulls":4},0]
[15.17,"One coat alkaline resistant plaster primer, one coat universal alkyd based undercoat and one coats alkyd based eggshell enamel paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.17.1","On internal walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
[15.18,"One coat resin based bonding liquid and two coats superior acrylic PVA emulsion paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.18.1","On internal walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.18.2","On external walls","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
[null,"0N PLASTER BOARD",null,null,0]
[{"$nulls":4},0]
[15.19,"One coat resin based bonding liquid and two coats superior acrylic PVA emulsion paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.19.1","On ceilings and cornices","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.19.2","On drywall partitions","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[null,"ON FIBRE-CEMENT",null,null,0]
[{"$nulls":4},0]
[{"v":15.2,"d":"15.20"},"One coat resin based bonding liquid and two full coats UV resistant water based acrylic roof paint on work in poor condition",null,null,0]
[{"$nulls":4},0]
["15.20.1","On profiled roof sheets (measured on flat)","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.20.2","On fascias and barge boards","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.21,"Two coats superior acrylic PVA emulsion paint on work in sound condition",null,null,0]
[{"$nulls":4},0]
["15.21.1","On internal fibre cement ceilings including priming steel joints and nail heads with one coat zinc phosphate alkyd resin primer","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.21.2","On fascias and barge boards","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.21.3","On internal fibre cement sills not exceeding 300mm girth","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["15.21.4","On fascia and barge boards not exceeding 300mm girth","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
[null,"ON METAL",null,null,0]
[{"$nulls":4},0]
[15.22,"Two coats alkyd based high gloss enamel paint on previously painted steel in sound condition",null,null,0]
[{"$nulls":4},0]
["15.22.1","On door frames","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.22.2","On recordroom,strongroom, combination doors and frames","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.22.3","On window frames","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.22.4","On window frames with burglar bars","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.22.5","On gates, grilles, burglar screens, balustrades, etc (both sides measured over full flat area)","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.22.6","On eaves gutters/rainwater downpipes not exceeding 300mm girth","m",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["15.22.7","On rails not exceeding 300mm girth","m",1,{"v":31.895408480000008,"d":"31.90"}]
[{"$nulls":4},0]
["15.22.8","On eaves gutters","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.22.9","On palisade fencing","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.23,"One coat water based galvanised iron primer, one coat Universal alkyd based undercoat and two coats alkyd based high gloss enamel paint on galvanised steel in poor condition (rusted)",null,null,0]
[{"$nulls":4},0]
["15.23.1","On corrugated iron profile roof sheeting (measured on flat)","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["15.23.2","On IBR profile roof sheeting (measured on flat)","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["15.23.3","On eaves gutters","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["15.23.4","On gates, grilles, burglar screens, balustrades, etc (both sides measured over full flat area)","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["15.23.5","On Steel Palisade (both sides measured over full flat area)","m²",1,{"v":79.73852120000002,"d":"79.74"}]
[{"$nulls":4},0]
["15.23.6","On rails, bars, pipes exceeding 300mm girth","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
["15.23.7","On eaves gutters/rainwater downpipes not exceeding 300mm girth","m",1,{"v":35.57564792000001,"d":"35.58"}]
[{"$nulls":4},0]
[null,"ON WOOD",null,null,0]
[{"$nulls":4},0]
[15.24,"Spot prime bare wood surfaces with wood primer and apply one universal alkyd based undercoat and two coats alkyd based eggshell enamel paint on previously painted surfaces in poor condition",null,null,0]
[{"$nulls":4},0]
["15.24.1","On doors","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.24.2","On fittings","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.24.3","Skirtings, rails, etc. not exceeding 300mm. girth","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["15.24.4","On roof timbers at eaves and verges","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.25,"Two coats alkyd based eggshell enamel paint on previously painted surfaces in sound condition",null,null,0]
[{"$nulls":4},0]
["15.25.1","On doors","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.25.2","On fittings","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
["15.25.3","Skirtings, rails, etc. not exceeding 300mm. girth","m",1,{"v":22.081436640000007,"d":"22.08"}]
[{"$nulls":4},0]
["15.25.4","On roof timbers at eves and verges","m²",1,{"v":67.47105640000001,"d":"67.47"}]
[{"$nulls":4},0]
[15.26,"Three coats clear polyurethane suede varnish ",null,null,0]
[{"$nulls":4},0]
["15.26.1","On doors","m²",1,{"v":73.60478880000002,"d":"73.60"}]
[{"$nulls":4},0]
["15.26.2","Skirtings, rails, etc. not exceeding 300mm. girth","m",1,{"v":25.761676080000004,"d":"25.76"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[15.27,"MURIELS AND PAINTINGS",null,null,0]
[{"$nulls":4},0]
["15.27.1","TOWNSHIP THEME: Customized two dimensional puzzle designed and the pieces set back and forth to give dimension - vivid colors are used. Materials: Puzzle pieces cut out of masonite board fixed onto wall.","m2",1,{"v":2948.2935256008363,"d":"2,948.29"}]
[{"$nulls":4},0]
["15.27.2","BEACH THEME: Individual bear figure activities on the beach set back and forth to create dimension on backing board. Materials: Masonite figures cut out and placed on masonite backing board. Acrylic formulated sand mixture to backing board.","m2",1,{"v":2473.4076755844167,"d":"2,473.41"}]
[{"$nulls":4},0]
["15.27.3","INSECT THEME: Insects on flowers and leafs in three dimension. Materials: Gupsym board backing with formulated\npastes to create dimension","m2",1,{"v":6046.107651428573,"d":"6,046.11"}]
[{"$nulls":4},0]
["15.27.4","SPACE THEME: Moon and planets in a dimensional space with\nastronaut. Materials: Gupsym board backing with formulated\npaste to create dimension.","m2",1,{"v":2621.341718243244,"d":"2,621.34"}]
[{"$nulls":4},0]
["15.27.5","ANCIENT THEME: figures (to be finalised) on dimensional Anciant\nCastledoing every day life. Materials: Masonite figures cut out to create dimension on a backing board","m2",1,{"v":2473.4076755844167,"d":"2,473.41"}]
[{"$nulls":4},0]
["15.27.6","PIRATE SHIPS AND UNDER SEA THEME: Dimensional Fighting battle ships above and sea life below - to be finalised. Materials: Masonite battle ships and sea cretures cut out and placed on backing boards","m2",1,{"v":2473.4076755844167,"d":"2,473.41"}]
[{"$nulls":4},0]
["15.27.7","BUTTERFLY / MOUSE THEME: Pictures of everyday life at home - bright colors to be used. Materials: Bold Acrylic colors on Masonite board, final coat using vanish, paint brushes and rollers, glue, pencils, etc","m2",1,{"v":1380.8402466557914,"d":"1,380.84"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["15.27.8","FLOWERS / BIRD THEME: Pictures of everyday life at home - bright colors to be used. Materials: Pastel collors colors on Masonite board, final coat using vanish, paint brushes and rollers, glue, pencils, etc","m2",1,{"v":1461.9258569948188,"d":"1,461.93"}]
[{"$nulls":4},0]
["15.27.9","BIG FIVE THEME: Pictures of everyday life at home - bright colors to be used. Materials: Pastel collors colors on Masonite board, final coat using vanish, paint brushes and rollers, glue, pencils, etc","m2",1,{"v":1461.9258569948188,"d":"1,461.93"}]
{"$rows_empty":45}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Ext. Works","index":15,"n_rows":787,"n_cols":7,"rows_kept":787,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 17"]
[]
[null,"EXTERNAL WORKS"]
[]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Descriptions"]
[]
[null,"For full descriptions and supplementary preambles applicable to this section, see also previous bills"]
[]
[null,"Nature of ground"]
[]
[null,"A soil investigation will be carried out on site by the engineer, and the report will be annexed to these bills of quantities.Descriptions of all excavations shall be deemed to include all ground conditions classified as \"earth\" described in the annexed report and where conditions of a more difficult character are indicated these are separately measured"]
[]
[null,"Carting away of excavated material"]
[]
[null,"Description of carting away of excavated material shall deemed to include loading of excavated material onto trucks directly from the excavtions, or alternatively, from stock piles situated on the building site."]
[]
[17.1,"Concrete pipes"]
[]
[null,"Pipes shall be jointed with ogee joints with rubber collars or socket and spigot joints with rubber rings"]
[]
[null,"uPVC pipes and fittings"]
[]
[null,"Sewer and drainage pipes and fittings shall be jointed and sealed with butyl rubber rings"]
[null,"Soil, waste and vent pipes and fittings shall be solvent weld jointed"]
[]
[null,"uPVC pressure pipes and fittings"]
[]
[null,"Pipes for water supply shall be of the class stated"]
[null,"Pipes of 40mm diameter and smaller shall be plain ended with solvent welded uPVC loose socket fittings"]
[]
[null,"Pipes of 50mm diameter and greater shall have sockets and spigots with push-in type integral rubber ring joints. Bens shall be uPVC and all other fittings shall be cast iron, all with similar push-in type joints with solvent welded uPVC loose socket fittings"]
[]
[null,"Exposed concrete surfaces"]
[]
[null,"Exposed surfaces of concrete stormwater channels, cover slabs, inspection eye marker slabs, gulley tops, cleaning eye tops, catchpits, inspection chambers, etc. shall be finished smooth with plaster"]
[]
[null,"Excavations"]
[]
[null,"No claim for rock excavation will be entertained unless the contractor has timeously notified the quantity surveyor thereof prior to backfilling"]
[]
[null,"\"Soft rock\" and \"hard rock\" shall be as defined in \"Earthworks\""]
[]
[null,"Laying, backfilling, bedding, etc. of pipes"]
[]
[null,"Pipes shall be laid and bedded and trenches shall be carefully backfilled in accordance with manufacturers' instructions"]
[]
[null,"The selection of the imported \"borrow pit\" pipe bending material for classB,C or flexible pipe beddings shall be done by the contractor, and all the tendered rates for the imported material shall be deemed to include for the necessary selection of material."]
[]
[null,"The selection of the imported \"borrow pit\" pipe bending material for classB,C or flexible pipe beddings shall be done by the contractor, and all the tendered rates for the imported material shall be deemed to include for the necessary selection of material."]
[]
[null,"Where no manufacturers' instructions exist, pipes shall be laid in accordance with clauses 5.1 and 5.2 of each of the following:"]
[]
[null,"SABS 1200                  L : Medium-pressure pipelines"]
[null,"                                 LD : Sewers"]
[null,"                                 LE : Stormwater drainage"]
[]
[null,"Pipe trenches, etc. shall be backfilled in accordance with clauses3, 5.5, 5.6, 5.7 and 7 of SABS 1200"]
[]
[null,"                                 LB : Bedding (Pipes)"]
[]
[null,"Unless otherwise described, bedding of rigid pipes shall be class B bedding"]
[]
[null,"Unless otherwise described, bedding of rigid pipes shall be class B bedding"]
[]
[null,"\"Densyl\" petrolatum anti-corrsion tape as manufactured by Denso SA (Pty) Ltd or equally approved"]
[]
[null,"Pipes to be taped shall be coated with the appropriate primer and the tape shall be applied with minimum 15mm lap per spiral unless otherwise described"]
[]
[null,"Couplings and fittings to pipes shall be taped in strict accordance with the manufacturers instructions, including all mastic tape \"Layflat\" sheeting, securing of same, etc."]
[]
[null,"Unless otherwise described, bedding of rigid pipes shall be class B bedding"]
[]
[null,"ALTERATIONS"]
[]
[null,"REMOVAL OF EXISTING WORK"]
[]
[17.1,"Taking out and removing road kerbs and surfacing"]
[]
["17.1.1","Break up and cart away tarmac paving and crusher run base 175mm thick bedding including concrete kerbs","m²",1,{"v":31.2575003104,"d":"31.26"}]
[{"$nulls":4},0]
["17.1.2","Precast concrete vertical kerbs with 150 x 150mm cat in-situ concrete apron along sides of existing road including necessary excavation, backfilling and compaction","m",1,{"v":10.42734508,"d":"10.43"}]
[{"$nulls":4},0]
["17.1.3","Lift up concrete, clay, etc. paving blocks and set aside for re-use","m²",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["17.1.4","Lift up concrete, clay, etc paving blocks, set aside and relay including 20mm sand bedding","m²",1,{"v":57.35039794000001,"d":"57.35"}]
[{"$nulls":4},0]
["17.1.6","Break down and cart away half brickwall 1.8m high with piers at 2m centres and cart away","m",1,{"v":208.51009920560006,"d":"208.51"}]
[{"$nulls":4},0]
["17.1.7","Break down and cart away one brickwall 1.8m high with piers at 3m centres and cart away","m",1,{"v":382.2787380976,"d":"382.28"}]
[{"$nulls":4},0]
["17.1.8","Break down and cart away one and half brickwall 1.8m high with piers at 3m centres and cart away","m",1,{"v":382.2787380976,"d":"382.28"}]
[{"$nulls":4},0]
[null,"LANDSCAPING",null,null,0]
[{"$nulls":4},0]
[17.2,"Preambles",null,null,0]
[{"$nulls":4},0]
["17.2.1","The accuracy of bulk earthworks and landscaping will be in accordance with SABS 1200D and SABS 1200DM Degree II",null,null,0]
[{"$nulls":4},0]
[null,"Topsoil, compost, lime and fertilizer",null,null,0]
[{"$nulls":4},0]
[17.3,"Excavate and preserve topsoil and deposit in stockpile",null,null,0]
[{"$nulls":4},0]
["17.3.1","Topsoil obtained from prescribed stock piles on site spread and levelled over the site for grass areas including slightly wetting and rolling with light roller","m3",1,{"v":97.30553079360001,"d":"97.31"}]
[{"$nulls":4},0]
["17.3.2","Topsoil obtained from prescribed stock piles on site spread and levelled over the site for grass areas including slightly wetting and rolling with light roller in plant beds, road islands, etc.","m²",1,{"v":76.46310809840001,"d":"76.46"}]
[{"$nulls":4},0]
[17.4,"Topsoil supplied by the contractor spread and levelled over the site for grass areas","m3",1,{"v":373.8509897800001,"d":"373.85"}]
[{"$nulls":4},0]
["17.4.1","Compost in plant boxes","m3",1,{"v":500.81925046000003,"d":"500.82"}]
[{"$nulls":4},0]
[17.5,"TREES",null,null,0]
[{"$nulls":4},0]
["17.5.1","Celtis africana (50l)","no",1,{"v":1104.071832,"d":"1,104.07"}]
[{"$nulls":4},0]
["17.5.2","Tanalith treated eucalyptus fencing 1200mm high","m",1,{"v":556.9429019200002,"d":"556.94"}]
[{"$nulls":4},0]
["17.5.3","Tanalith treated vertical lath (wood) handrails 1200mm high","m",1,{"v":384.2169975360001,"d":"384.22"}]
[{"$nulls":4},0]
[null,"GRASSING, GROUND COVERS, ETC.",null,null,0]
[{"$nulls":4},0]
[null,"\"Kikuyu\"",null,null,0]
[{"$nulls":4},0]
[17.6,"Roots in rows","m²",1,{"v":20.842422695200003,"d":"20.84"}]
[{"$nulls":4},0]
["17.6.1","Areas not exceeding 1000m2","m²",1,{"v":24.731209036800003,"d":"24.73"}]
[{"$nulls":4},0]
["17.6.2","Areas exceeding 1000m2","m²",1,{"v":23.553532416000003,"d":"23.55"}]
[{"$nulls":4},0]
["17.6.2","Hydroseeding (Hydraulic mulch seeding, hydro-mulching)","m²",1,{"v":51.52335216000001,"d":"51.52"}]
[{"$nulls":4},0]
[null,"EARTHWORKS, ROADWORKS, ETC",null,null,0]
[{"$nulls":4},0]
[17.7,"Site clearance",null,null,0]
[{"$nulls":4},0]
["17.7.1","Digging up and removing rubbish, debris, vegetation, hedges, shrubs and trees not exceeding 200mm girth, bush, etc.","m²",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
[null,"Bulk excavation, filling, etc",null,null,0]
[{"$nulls":4},0]
["17.7.2","On drywall partitions","m²",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
[17.8,"Open face excavation over sloping site",null,null,0]
[{"$nulls":4},0]
["17.8.1","Open face excavation to reduce levels under roads, parking areas, etc. (spoil measured elsewhere)","m3",1,{"v":60.110577520000014,"d":"60.11"}]
[{"$nulls":4},0]
[null,"Extra over bulk excavation in earth for excavation in",null,null,0]
[{"$nulls":4},0]
["17.8.2","Soft rock","m3",1,{"v":184.01197200000001,"d":"184.01"}]
[{"$nulls":4},0]
["17.8.3","Hard rock","m3",1,{"v":392.5588736,"d":"392.56"}]
[{"$nulls":4},0]
[17.9,"Extra over excavations for carting away",null,null,0]
[{"$nulls":4},0]
["17.9.1","Surplus material from excavations on site to a dumping site to be located by the contractor (100% of excavated material)","m3",1,{"v":40.48263384000001,"d":"40.48"}]
[{"$nulls":4},0]
[null,"Keeping excavations free of water",null,null,0]
[{"$nulls":4},0]
["17.9.2","Keeping excavations free of water","Item",1,{"v":1533.4331,"d":"1,533.43"}]
[{"$nulls":4},0]
[null,"Keeping excavations moist",null,null,0]
[{"$nulls":4},0]
["17.9.4","Extra over bulk or open face excavations to reduce levels under roads, parking areas, etc. (irrespective of depth) for keeping exposed or open excavation sides and bottoms","Item",1,{"v":1840.1197200000004,"d":"1,840.12"}]
[{"$nulls":4},0]
[{"v":17.1,"d":"17.10"},"Earthfilling supplied by the contractor under roads, parking areas, paving, etc. including all haul, selection, handling, etc (No designated borrow pit available)",null,null,0]
[{"$nulls":4},0]
[null,"Note:",null,null,0]
[null,"Road construction materials shall conform to the requirements of TRH 14: Guidelines for road construction materials",null,null,0]
[{"$nulls":4},0]
["17.10.1","Approved G7 material for use in backfilling under walkways, paths and islands in 150mm thick layers compacted to 90% Modified AASHTO density","m3",1,{"v":356.9832256800001,"d":"356.98"}]
[{"$nulls":4},0]
["17.10.2","Selected G6 type material compacted in 150mm layers to 93% Modified AASHTO density","m3",1,{"v":356.9832256800001,"d":"356.98"}]
[{"$nulls":4},0]
["17.10.3","150mm Sub-base layer G5 type material stabilized with 3% cement to obtain a C4 material compacted to 95% Modified AASHTO density","m3",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
[17.11,"Compaction of surfaces",null,null,0]
[{"$nulls":4},0]
["17.11.1","Compaction of ground surface under roads and parking areas including scarifying for a depth of 150mm, breaking down oversize material, addinng suitable material where necessary and compacting to 90% Mod AASHTO density","m²",1,{"v":7.973852120000002,"d":"7.97"}]
[{"$nulls":4},0]
[17.12,"Tests",null,null,0]
[{"$nulls":4},0]
["17.12.1","\"Modified AASHTO Density\" test to 93%","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
[17.13,"Soil poisoning (In confined areas)",null,null,0]
[{"$nulls":4},0]
["17.13.1","\"Trimex-S\" weedkiller mixed 30g/l water and applied at a rate of 1 litre/10m2 under road, parking and walkway paving","m²",1,{"v":55.20359160000002,"d":"55.20"}]
[{"$nulls":4},0]
[null,"Precast concrete block road surfacing",null,null,0]
[{"$nulls":4},0]
[null,"Paving is to be laid in accordance with SABS 1200 MJ, SABS 1058 and the Concrete Masonry Association's specifications",null,null,0]
[{"$nulls":4},0]
[null,"Paving is to be laid in herringbone pattern on 25mm (thickness after final compaction) clean river sand (preparation of ground or filling elsewhere)",null,null,0]
[{"$nulls":4},0]
[null,"Clean sand is to be swept into joints between roadstones",null,null,0]
[{"$nulls":4},0]
[null,"ASPHALT ",null,null,0]
[{"$nulls":4},0]
[17.14,"Tar Surfacing (Parking and walkways)",null,null,0]
[{"$nulls":4},0]
["17.14.1","Tar road resurfacing and making good","m²",1,{"v":211.61376780000006,"d":"211.61"}]
[{"$nulls":4},0]
["17.14.2","Tar road resurfacing and making good in bad condition","m²",1,{"v":282.15169040000006,"d":"282.15"}]
[{"$nulls":4},0]
["17.14.3","Saw-cutting asphalt(tar)","m",1,{"v":32.50878172,"d":"32.51"}]
[{"$nulls":4},0]
[null,"PAVING",null,null,0]
[{"$nulls":4},0]
[null,"Lifting up, setting aside and re-laying paving blocks including backfilling and 20mm bedding sand",null,null,0]
[{"$nulls":4},0]
["17.14.4","Precast concrete paving to falls","m²",1,{"v":88.76552360000001,"d":"88.77"}]
[{"$nulls":4},0]
[17.15,"450 x 450 x50mm precast concrete paving slabs laid on 50mm thick river sand bead including preparation of ground or filling",null,null,0]
[{"$nulls":4},0]
["17.15.1","Paving of slabs laid with butt joints","m²",1,{"v":219.58761992000004,"d":"219.59"}]
[{"$nulls":4},0]
["17.15.2","Paving of slabs laid with 10mm wide joints jointed with mortar and flush pointed","m²",1,{"v":228.17484528000003,"d":"228.17"}]
[{"$nulls":4},0]
["17.15.3","Fair circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
[null,"450 x 450 x50mm precast concrete paving slabs with exposed aggregate finish laid on 50mm thick river sand bead including preparation of ground or filling",null,null,0]
[{"$nulls":4},0]
["17.15.4","Paving of slabs laid with butt joints","m²",1,{"v":250.25628192000005,"d":"250.26"}]
[{"$nulls":4},0]
["17.15.5","Paving of slabs laid with 10mm wide joints jointed with mortar and flush pointed","m²",1,{"v":258.84350728000004,"d":"258.84"}]
[{"$nulls":4},0]
["17.15.6","Fair circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
[17.16,"60mm Standard grey \"Concor Double Zig-Zag\" interlocking roadstone paving or equally approved ",null,null,0]
[{"$nulls":4},0]
["17.16.1","Paving to roads, parking areas, etc. to slight falls","m²",1,{"v":165.6107748,"d":"165.61"}]
[{"$nulls":4},0]
["17.16.2","Circular cutting to pavers","m²",1,{"v":11.654091560000003,"d":"11.65"}]
[{"$nulls":4},0]
["17.16.3","Joint of new paving or concrete edge beam to existing paving including all cutting, waste, filling of openings with concrete, etc.","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["17.16.a","60mm Standard grey \"Concor Double Zig-Zag\" interlocking roadstone paving or equally approved (For low traffic-All inclusive trade) Including earthworks, 25mm thick river sand bed with sand  swept into joints including preparation of ground or filling etc",null,null,0]
[{"$nulls":4},0]
["17.16.1a","Paving to roads, parking areas, etc. to slight falls","m²",1,{"v":251.48302840000005,"d":"251.48"}]
[{"$nulls":4},0]
[17.17,"85mm Standard grey \"Concor Double Zig-Zag\" interlocking roadstone paving or equally approved",null,null,0]
[{"$nulls":4},0]
["17.17.1","Paving to roads, parking areas, etc. to slight falls","m²",1,{"v":177.87823960000006,"d":"177.88"}]
[{"$nulls":4},0]
["17.17.2","Circular cutting to pavers","m²",1,{"v":10.42734508,"d":"10.43"}]
[{"$nulls":4},0]
["17.17.3","Joint of new paving or concrete edge beam to existing paving including all cutting, waste, filling of openings with concrete, etc.","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
["17.17.4","Paving of 220 x 108.5 x 50mm thick \"Corobrik Tuscan Blend\" paving bricks with butt joints on 25mm thick river sand bed with sand and cement mixture swept into joints and hosed down including preparation of ground or filling",null,null,0]
[{"$nulls":4},0]
["17.17.4a","Paving in stretcher bond pattern","m²",1,{"v":208.54690160000007,"d":"208.55"}]
[{"$nulls":4},0]
["17.17.4b","Paving in stretcher bond pattern to falls","m²",1,{"v":208.54690160000007,"d":"208.55"}]
[{"$nulls":4},0]
["17.17.4c","Paving in herringboned bond pattern","m²",1,{"v":208.54690160000007,"d":"208.55"}]
[{"$nulls":4},0]
["17.17.4d","Paving in herringboned bond pattern to falls","m²",1,{"v":208.54690160000007,"d":"208.55"}]
[{"$nulls":4},0]
["17.17.4e","75mm wide brick-on-edge edging on 50mm thick mortar bed","m",1,{"v":24.5349296,"d":"24.53"}]
[{"$nulls":4},0]
["17.17.4f","110mm wide brick-on-end edging on 50mm thick mortar bed","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["17.17.4g","220mm wide brick-on-flat header course edging on 50mm thick mortar bed","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["17.17.4h","220mm wide brick-on-flat header course edging on 50mm thick mortar bed circular on plan","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["17.17.4i","220mm wide brick-on-edge header course edging on 50mm thick mortar bed","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["17.17.4j","220mm wide brick-on-edge header course edging on 50mm thick mortar bed circular on plan","m",1,{"v":46.61636624000001,"d":"46.62"}]
[{"$nulls":4},0]
["17.17.4k","170mm high brick-on-flat risers on 25mm thick mortar bed","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["17.17.4l","350mm wide treads of brick-on-flat header course and brick-on-flat stretcher course on 25mm thick mortar bed","m",1,{"v":52.75009864000002,"d":"52.75"}]
[{"$nulls":4},0]
["17.17.5","Paving of 200 x 100 x 50mm thick precast concrete \"Concor Bondbrick\" chamfered paving block with butt joints on 25mm thick river sand bed with sand  swept into joints including preparation of ground or filling",null,null,0]
[{"$nulls":4},0]
["17.17.5a","Paving in stretcher bond pattern","m²",1,{"v":180.33173256000003,"d":"180.33"}]
[{"$nulls":4},0]
["17.17.5b ","Paving in stretcher bond pattern to falls","m²",1,{"v":180.33173256000003,"d":"180.33"}]
[{"$nulls":4},0]
["17.17.5c","Paving in herringboned bond pattern","m²",1,{"v":180.33173256000003,"d":"180.33"}]
[{"$nulls":4},0]
["17.17.5d","Paving in herringboned bond pattern to falls","m²",1,{"v":180.33173256000003,"d":"180.33"}]
[{"$nulls":4},0]
["17.17.5e","100mm wide block-on-end edging on 50mm thick mortar bed","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["17.17.5f","200mm wide block-on-flat header course edging on 50mm thick mortar bed","m",1,{"v":41.70938032,"d":"41.71"}]
[{"$nulls":4},0]
["17.17.5g","200mm wide block-on-flat header course edging on 50mm thick mortar bed circular on plan","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["17.17.5h","200mm wide block-on-edge header course edging on 50mm thick mortar bed","m",1,{"v":45.38961976,"d":"45.39"}]
[{"$nulls":4},0]
["17.17.5i","200mm wide block-on-edge header course edging on 50mm thick mortar bed circular on plan","m",1,{"v":46.61636624000001,"d":"46.62"}]
[{"$nulls":4},0]
["17.17.5j","170mm high brick-on-flat risers on 25mm thick mortar bed","m",1,{"v":42.936126800000004,"d":"42.94"}]
[{"$nulls":4},0]
["17.17.5k","330mm wide treads of brick-on-flat header course and brick-on-flat stretcher course on 25mm thick mortar bed","m",1,{"v":52.75009864000002,"d":"52.75"}]
[{"$nulls":4},0]
["17.17.5l","Extra for contrasting colour blocks as marker lines","m",1,{"v":12.2674648,"d":"12.27"}]
[{"$nulls":4},0]
["17.17.6","Double zig-zag (shape S-A) interlocking precast concrete blocks complying with SABS 1058 laid with butt joints on 25mm thick river sand bed with sand swept into joints including preparation of ground or filling",null,null,0]
[{"$nulls":4},0]
["17.17.6a","Paving of 80mm thick blocks including edge blocks","m²",1,{"v":209.77364808000007,"d":"209.77"}]
[{"$nulls":4},0]
["17.17.6b","Paving of 80mm thick blocks including edge blocks to falls and cross falls","m²",1,{"v":209.77364808000007,"d":"209.77"}]
[{"$nulls":4},0]
["17.17.6c","Paving of 60mm thick blocks including edge blocks","m²",1,{"v":203.63991568000006,"d":"203.64"}]
[{"$nulls":4},0]
["17.17.6d","Paving of 60mm thick blocks including edge blocks to falls and cross falls","m²",1,{"v":203.63991568000006,"d":"203.64"}]
[{"$nulls":4},0]
["17.17.6e","Extra for contrasting colour blocks as marker lines","m",1,{"v":12.2674648,"d":"12.27"}]
[{"$nulls":4},0]
["17.17.6f","Fair circular cutting","m",1,{"v":4.906985920000001,"d":"4.91"}]
[{"$nulls":4},0]
[17.18,"Precast concrete finished smooth on exposed surfaces including bedding, jointing and pointing",null,null,0]
[{"$nulls":4},0]
["17.18.1","Vertical kerb (SABS 927 fig 7) 180 x 280mm high in 1 000mm sections with 13mm thick softboard expansion joints at 20 000mm centres complete with 250 x 180mm thick class 15Mpa/19mm unreinforced cast in-situ concrete continuous anchor block strip for the full length at back of kerbing including excavation, backfilling, etc.","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
["17.18.2","Vertical kerb (SABS 927 fig 7) 180 x 280mm high in 1 000mm sections with 13mm thick softboard expansion joints at 20 000mm centres complete with 250 x 180mm thick class 15Mpa/19mm unreinforced cast in-situ concrete continuous anchor block strip for the full length at back of kerbing, circular on plan to exceeding 4 000mm radius formed with short lengths of straight kerb including excavation, backfilling, etc.","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
["17.18.3","Vertical kerb (SABS 927 fig 7) 180 x 280mm high in 1 000mm sections with 13mm thick softboard expansion joints at 20 000mm centres complete with 250 x 180mm thick class 15Mpa/19mm unreinforced cast in-situ concrete continuous anchor block strip for the full length at back of kerbing, circular on plan to  not exceeding 4 000mm radius formed with short lengths (maximum 300mm long) of straight kerb including excavation, backfilling, etc.","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
["17.18.4","Semi-mountable kerb (SABS 927 fig 7 laid flat on back) 180 x 280mm high in 1000mm sections with 13mm thick softboard expansion joints at 20 000mm centres complete with 250 x 180mm thick class 15Mpa/19mm unreinforced cast in-situ concrete continuous anchor block strip for the full length at back of kerbing including excavation, backfilling, etc.","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
["17.18.5","Semi-mountable kerb (SABS 927 fig 7 laid flat on back) 180 x 280mm high in          1 000mm sections with 13mm thick softboard expansion joints at 20 000mm centres complete with 250 x 180mm thick class 15Mpa/19mm unreinforced cast in-situ concrete continuous anchor block strip for the full length at back of kerbing, circular on plan to exceeding 4 000mm radius formed with short lengths of straight kerb including excavation, backfilling, etc.","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
["17.18.6","Semi-mountable kerb (SABS 927 fig 7 laid flat on back) 180 x 280mm high in 1 000mm sections with 13mm thick softboard expansion joints at 20 000mm centres complete with 250 x 180mm thick class 15Mpa/19mm unreinforced cast in-situ concrete continuous anchor block strip for the full length at back of kerbing, circular on plan to not exceeding 4 000mm radius formed with short lengths (maximum 300mm long) of straight kerb including excavation, backfilling, etc.","m",1,{"v":153.34331,"d":"153.34"}]
[{"$nulls":4},0]
[17.19,"Sundries",null,null,0]
[{"$nulls":4},0]
["17.19.1","Joint of new fig 7 kerb to existing kerb, including all cutting","m",1,{"v":17.17445072,"d":"17.17"}]
[{"$nulls":4},0]
[{"v":17.2,"d":"17.20"},"SABS 731-1987 yellow or white roadmark paint on paving at a rate of 1 litre/m2",null,null,0]
[{"$nulls":4},0]
["17.20.1","Line 100mm wide","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["17.20.2","Line 100mm wide (RTM 1)","m",1,{"v":14.720957760000003,"d":"14.72"}]
[{"$nulls":4},0]
["17.20.3","Numeral or letter 400mm high","no",1,{"v":104.27345080000003,"d":"104.27"}]
[{"$nulls":4},0]
["17.20.4","Numeral or letter 1250mm high (GM7)","no",1,{"v":131.87524660000003,"d":"131.88"}]
[{"$nulls":4},0]
["17.20.5","Traffic arrow 1250 x 500mm wide extreme (G M4.1)","no",1,{"v":131.87524660000003,"d":"131.88"}]
[{"$nulls":4},0]
["17.20.6","Information sign for \"people with disability\" parking in 150mm wide lines","m2",1,{"v":135.53095111040003,"d":"135.53"}]
[{"$nulls":4},0]
["17.20.7","550 x 235 x 1600mm cast in-situ concrete dish channel","no",1,{"v":210.26434667200007,"d":"210.26"}]
[{"$nulls":4},0]
[null,"DRAINAGE",null,null,0]
[{"$nulls":4},0]
[null,"Stormwater drainage pipes",null,null,0]
[{"$nulls":4},0]
[17.21,"SABS 966 Class 9 uPVC pressure pipes, laid to falls on and including imported bedding for flexible pipes as SABS 1200LB, drawing LB-2(a) with bottom of trench compacted to 90% Modified AASHTO density (backfilling importation elsewhere measured)",null,null,0]
[{"$nulls":4},0]
["17.21.1","200mm Pipes laid in and including trenches not exceeding 1m deep","m",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["17.21.2","200mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",1,{"v":430.5880144800001,"d":"430.59"}]
[{"$nulls":4},0]
["17.21.3","200mm Pipes laid in and including trenches exceeding 2m and not exceeding 3m deep","m",1,{"v":559.7644188240001,"d":"559.76"}]
[{"$nulls":4},0]
[17.22,"SABS 966 Class 9 uPVC pressure pipes, laid to falls on and including imported bedding for flexible pipes as SABS 1200LB, drawing LB-2(a)  including backfilling with soil raft foundation material",null,null,0]
[{"$nulls":4},0]
["17.22.1","200mm Pipes laid in and including trenches not exceeding 1m deep","m",1,{"v":331.2215496,"d":"331.22"}]
[{"$nulls":4},0]
["17.22.2","200mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",1,{"v":430.5880144800001,"d":"430.59"}]
[{"$nulls":4},0]
["17.22.3","200mm Pipes laid in and including trenches exceeding 2m and not exceeding 3m deep","m",1,{"v":559.7644188240001,"d":"559.76"}]
[{"$nulls":4},0]
[17.23,"Plain ended cast iron pipes with SSN couplings, laid to falls on and including imported ClassB bedding for rigid pipes as SABS 1200LB drawing LB-1(b) with bottom of trench compacted to 90% Modified AASHTO density (backfilling importation measured elsewhere)",null,null,0]
[{"$nulls":4},0]
["17.23.1","200mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep in soil raft foundation","m",1,{"v":711.5129584000002,"d":"711.51"}]
[{"$nulls":4},0]
[17.24,"Extra over uPVC Class 9 pipes for fittings",null,null,0]
[{"$nulls":4},0]
["17.24.1","200mm Bend","no",1,{"v":693.7251344400001,"d":"693.73"}]
[{"$nulls":4},0]
["17.24.2","200mm Junction","no",1,{"v":747.0886063200003,"d":"747.09"}]
[{"$nulls":4},0]
["17.24.3","200mm SSN coupling","no",1,{"v":789.7793838240001,"d":"789.78"}]
[{"$nulls":4},0]
[17.25,"Grid inlets, kerb inlets, field inlets, catchpits, etc. (steel and cast iron gratings and covers elsewhere meaured)",null,null,0]
[{"$nulls":4},0]
["17.25.1","Grid inlet 500 x 500mm and exceeding 500mm and not exceeding 750mm deep internally","no",1,{"v":766.71655,"d":"766.72"}]
[{"$nulls":4},0]
["17.25.2","Grid inlet 500 x 500mm and exceeding 750mm and not exceeding 1000mm deep internally","no",1,{"v":924.9668459200002,"d":"924.97"}]
[{"$nulls":4},0]
["17.25.3","Grid inlet 500 x 500mm and exceeding 1000mm and not exceeding 1250mm deep internally","no",1,{"v":1081.9903953600003,"d":"1,081.99"}]
[{"$nulls":4},0]
["17.25.4","Grid inlet 500 x 500mm and exceeding 1250mm and not exceeding 1500mm deep internally","no",1,{"v":1266.1863793320003,"d":"1,266.19"}]
[{"$nulls":4},0]
["17.25.5","Grid inlet 500 x 500mm and exceeding 1500mm and not exceeding 1750mm deep internally","no",1,{"v":1481.4435841776,"d":"1,481.44"}]
[{"$nulls":4},0]
["17.25.6","Junction box 500 x 500mm and not exceeding 500mm with concrete slab over","no",1,{"v":705.379226,"d":"705.38"}]
[{"$nulls":4},0]
[17.26,"Heavy duty precast concrete circular inspection chambers including step irons, bases, etc (covers elsewhere)",null,null,0]
[{"$nulls":4},0]
["17.26.1","Inspection chamber 1000mm diameter exceeding 2 500mm and not exceeding 2 750mm deep internally (on top of existing stormwater pipe including altering benching, etc","no",1,{"v":4048.2633840000008,"d":"4,048.26"}]
[{"$nulls":4},0]
[17.27,"Covers, etc.",null,null,0]
[{"$nulls":4},0]
["17.27.1","450 x 450 x 79kg Medium duty cast iron flat stormwater grating and frame","no",1,{"v":1821.7185228000003,"d":"1,821.72"}]
[{"$nulls":4},0]
["17.27.2","550mm Diameter x 75kg type 4A single seal cast iron manhole cover and frame","no",1,{"v":1858.5209172000004,"d":"1,858.52"}]
[{"$nulls":4},0]
[17.28,"Sundries",null,null,0]
[{"$nulls":4},0]
["17.28.1","Approved G6 imported imported material to be supplied by the contractor for use in pipe bacfilling to trenches in 150mm thick layers compacted to 90% Modified AASHTO density","m3",1,{"v":306.68662,"d":"306.69"}]
[{"$nulls":4},0]
["17.28.2","Extra over trench excavations (irrespective of depth) for keeping exposed or open trench sides and bottoms wet at natural moisture conditions by adding or spraying of water for the whole duration of the trenching, pipe laying and backfill processes or construction duration","Item",1,{"v":141.07584520000003,"d":"141.08"}]
[{"$nulls":4},0]
[17.29,"Testing",null,null,0]
[{"$nulls":4},0]
["17.29.1","Testing stormwater drainage pipe system","Item",1,0]
[{"$nulls":4},0]
[null,"Soil drainage pipes",null,null,0]
[{"$nulls":4},0]
[{"v":17.3,"d":"17.30"},"SABS 791 Class 34 \"Mainlite\" uPVC pipes with rubber-ring seal couplings, laid to falls on and including imported bedding for flexible pipes as SABS 1200LB, drawing L-B2(a) with bottom of trench compacted to a minimum of 90% Modified AASHTO density (backfilling importation elsewhere measured)",null,null,0]
[{"$nulls":4},0]
["17.30.1","110mm Pipes laid in and including trenches not exceeding 1m ","m",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
["17.30.2","110mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep","m",1,{"v":253.93652136000006,"d":"253.94"}]
[{"$nulls":4},0]
[17.31,"SABS 791 Class 34 \"Mainlite\" uPVC pipes with rubber-ring seal couplings, laid to falls on and including imported bedding for flexible pipes as SABS 1200LB, drawing L-B2(a) including backfilling with soil raft foundation material",null,null,0]
[{"$nulls":4},0]
["17.31.1","110mm Pipes vertically or ramped to cleaning eyes, etc. (no excavation)","m",1,{"v":202.41316920000003,"d":"202.41"}]
[{"$nulls":4},0]
["17.31.2","110mm Pipes laid in and including trenches not exceeding 1m deep in soil raft foundation","m",1,{"v":232.77514458000005,"d":"232.78"}]
[{"$nulls":4},0]
["17.31.3","110mm Pipes laid in and including trenches exceeding 1m and not exceeding 2m deep in soil raft foundation","m",1,{"v":267.68834940080006,"d":"267.69"}]
[{"$nulls":4},0]
[17.32,"Extra over uPVC Class 34 pipes for fittings",null,null,0]
[{"$nulls":4},0]
["17.32.1","110mm Bend","no",1,{"v":220.81436640000007,"d":"220.81"}]
[{"$nulls":4},0]
["17.32.2","110mm Junction","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["17.32.3","110mm Access junction","no",1,{"v":316.5005918400001,"d":"316.50"}]
[{"$nulls":4},0]
["17.32.4","110mm x 50mm Reducer","no",1,{"v":294.4191552000001,"d":"294.42"}]
[{"$nulls":4},0]
["17.32.5","110mm x 50mm Reducing junction","no",1,{"v":312.8203524,"d":"312.82"}]
[{"$nulls":4},0]
["17.32.6","110mm SSN coupling","no",1,{"v":349.6227468,"d":"349.62"}]
[{"$nulls":4},0]
[17.33,"uPVC gulleys",null,null,0]
[{"$nulls":4},0]
["17.33.1","110mm Gulley complete with hopper head and grating, not exceeding  1 000mm deep","no",1,{"v":1214.4790152000003,"d":"1,214.48"}]
[{"$nulls":4},0]
[17.34,"Heavy duty precast concrete circular inspection chambers including step irons, bases, etc (covers elsewhere)",null,null,0]
[{"$nulls":4},0]
["17.34.1","Inspection chamber 1 000mm diameter exceeding 2 000mm deep internally","no",1,{"v":2392.1556360000004,"d":"2,392.16"}]
[{"$nulls":4},0]
[17.35,"Covers, etc",null,null,0]
[{"$nulls":4},0]
["17.35.1","550mm Diameter heavy duty precast concrete removable cover and frame","no",1,{"v":1343.2873956000003,"d":"1,343.29"}]
[{"$nulls":4},0]
["17.35.2","Lifting key for manhole cover","no",1,{"v":257.61676080000007,"d":"257.62"}]
[{"$nulls":4},0]
[null,"FENCING",null,null,0]
[{"$nulls":4},0]
[17.36,"Mild steel welded palisade fence including spot prime exposed metal surfaces and and two coats high gloss enamel paint",null,null,0]
["17.36.1","Palisade fence 1800mm high of 40 x 40 x 3mm angle section continuous top and bottom rails and 30 x 30 x 3mm angle section pickets with top end split and sharpened at average 150mm centres, welded to rails, rails welded 2200mm high posts of 76 x 76 x 5mm square tube with steel pyramid shaped capping on top at 2475mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":1044.4151506776002,"d":"1,044.42"}]
[{"$nulls":4},0]
["17.36.2","Palisade fence 2400mm high of 40 x 40 x 3mm angle section continuous top and bottom rails and 30 x 30 x 3mm angle section pickets with top end split and sharpened at average 150mm centres, welded to rails, rails welded 2600mm high posts of 76 x 76 x 5mm square tube with steel pyramid shaped capping on top at 2475mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean, neat and painted","m",1,{"v":1219.5700130920002,"d":"1,219.57"}]
[{"$nulls":4},0]
["17.36.3","Palisade pedestrian gate 900mm wide x 1800mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty hinges, secutity type locking device suitable for hand operated control, completely installed and painted","no",1,{"v":2643.638664400001,"d":"2,643.64"}]
[{"$nulls":4},0]
["17.36.4","Palisade fence vehicle sliding gate 6000mm wide x 1800mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, steel track cast in or bolted to and including concrete rail footing, secutity type locking device suitable for hand operated control rail, gate stops, gate guides, etc. completely installed and painted","no",1,{"v":15088.981704000002,"d":"15,088.98"}]
[{"$nulls":4},0]
["17.36.5","Palisade fence vehicle sliding gate 6000mm wide x 2400mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, steel track cast in or bolted to and including concrete rail footing, secutity type locking device suitable for hand operated control rail, gate stops, gate guides, etc. completely installed","no",1,{"v":17665.149312,"d":"17,665.15"}]
[{"$nulls":4},0]
["17.36.6","Palisade fence vehicle swing double gate 3000mm wide x 2400mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, etc. completely installed and painted","no",1,{"v":8243.736345600002,"d":"8,243.74"}]
[{"$nulls":4},0]
["17.36.7","Palisade fence vehicle swing double gate 6000mm wide x 1800mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, etc. completely installed and painted","no",1,{"v":14782.295084000001,"d":"14,782.30"}]
[{"$nulls":4},0]
["17.36.8","Palisade fence vehicle swing double gate 6000mm wide x 2400mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, etc. completely installed and painted","no",1,{"v":16487.472691200004,"d":"16,487.47"}]
[{"$nulls":4},0]
[17.38,"Making good complete",null,null,0]
[{"$nulls":4},0]
["17.38.1","Palisade pedestrian gate 900mm wide x 1800mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty hinges, secutity type locking device suitable for hand operated control ","no",1,{"v":395.6257398,"d":"395.63"}]
[{"$nulls":4},0]
["17.38.2","Palisade fence vehicle sliding gate 6000mm wide x 1800mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, secutity type locking device suitable for hand operated control rail, gate stops, gate guides, etc. ","no",1,{"v":3005.528876,"d":"3,005.53"}]
[{"$nulls":4},0]
["17.38.3","Palisade fence vehicle sliding gate 6000mm wide x 2400mm high overall, formed of 150 x 75 x 3mm thick hollow section frame, 100 x 75 x 3mm thick hollow section middle rail and cross bracing bars and with 25 x 25 x 2.5mm thick angle section spiked vertical bars at maximum 143mm centres welded to frame, middle rail and cross bracing bars complete with approved heavy duty castors, steel track cast in or bolted to and including concrete rail footing, secutity type locking device suitable for hand operated control rail, gate stops, gate guides, etc. completely installed","no",1,{"v":3005.528876,"d":"3,005.53"}]
[{"$nulls":4},0]
[17.39,"Concrete Palisade Fence",null,null,0]
[{"$nulls":4},0]
["17.39.1","Palisade fence 1800mm high of stacked slats, slid in-between 2300mm high posts of 110 x 70mm H-section post at 1500mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":837.4630195016001,"d":"837.46"}]
[{"$nulls":4},0]
["17.39.2","Palisade fence 2400mm high of stacked slats, slid in-between 2900mm high posts of 110 x 70mm H-section post at 1500mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":1004.9507164160002,"d":"1,004.95"}]
[{"$nulls":4},0]
[{"v":17.4,"d":"17.40"},"Precast Concrete  Fence",null,null,0]
[{"$nulls":4},0]
["17.40.1","Precast slatted fence 1800mm high of 110 x 70mm section continuous top and bottom rails and 140 x 70mm section with top end mitred at average 150mm centres, bolteded to rails, rails bolted 2200mm high posts of 140 x 140mm square post at 2475mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":713.5738924864,"d":"713.57"}]
[{"$nulls":4},0]
["17.40.2","Precast slatted fence 2400mm high of 110 x 70mm section continuous top and bottom rails and 140 x 70mm section with top end mitred at average 150mm centres, bolteded to rails, rails bolted 2200mm high posts of 140 x 140mm square post at 2475mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":891.9673656080003,"d":"891.97"}]
[{"$nulls":4},0]
["17.40.3","Precast slatted fence panel size 1500 x 300mm ","no",1,{"v":314.7095419792001,"d":"314.71"}]
[{"$nulls":4},0]
[17.41,"Diamond Wire Mesh ",null,null,0]
[{"$nulls":4},0]
["17.41.1","70 x 70mm Galvanised diamond wire mesh fence 1800mm high with seven horizontal strand wire of 2.9mm diameter fixed to posts, y-standards, droppers, etc with posts at 2475mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":713.5738924864,"d":"713.57"}]
[{"$nulls":4},0]
["17.41.2","70 x 70mm Galvanised diamond wire mesh fence 3600mm high with fourteen horizontal strand wire of 2.9mm diameter fixed to posts, y-standards, droppers, etc with posts at 2475mm centres with 500mm bottom ends cast into and including 15Mpa concrete footing in ground including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":1427.1477849728,"d":"1,427.15"}]
[{"$nulls":4},0]
["17.41.3","Post 2000 x 101 x 3mm hot dipped galvanised","no",1,{"v":480.8846201600001,"d":"480.88"}]
[{"$nulls":4},0]
["17.41.4","Stay 2000 x 48 x 2m hot dipped galvanised","no",1,{"v":225.72135232000005,"d":"225.72"}]
[{"$nulls":4},0]
["17.41.5","Y - standard 1850mm","no",1,{"v":96.23826135600001,"d":"96.24"}]
[{"$nulls":4},0]
["17.41.6","Droppers 1200mm","no",1,{"v":27.60179580000001,"d":"27.60"}]
[{"$nulls":4},0]
[null,"Diamond Wire Mesh 1.2m high for Low Cost Housing",null,null,0]
[{"$nulls":4},0]
["17.41.7","Wire mesh fencing shall be 1.2 m high formed of 50mm mesh chain link netting 2.5 mm diameter galvanised mild steel wire stained and secured to top and bottom rails and posts. Fencing shall be formed with three 4mm gauge strands of staining wire between 75 mm diameter posts inclusive of 38 mm tubular stays and intermediate rolled steel standards at approximately 3.65m. Corner posts shall have a minimum diameter of 75mm, 1.8m long for 1.2m high fencing and set 0.6 m deep in the ground with ends embedded in class “c” concrete. Stays shall have a minimum diameter of 38mm, 2.8mm thick. Stays shall also be neatly mitred and welded to corner and end posts. Corner posts are to be provided with two stays and end posts with one stay.","m",1,{"v":174.86923880000003,"d":"174.87"}]
[{"$nulls":4},0]
["17.41.8","Single pedestrian gate shall be 0.9 x 1.2 m high formed of 38mm diameter x 2.8 thick pipe framing all round complete with one 38mm diameter thick x 2.8 mm thick pipe horizontal brace all neatly mitred and welded at intersections, the gate with two strands of 4mm thick galvanised mild steel straining wire.","no",1,{"v":1735.9620000000002,"d":"1,735.96"}]
[{"$nulls":4},0]
["17.41.9","Single Vehicle gate shall be 3.2 x 1.2 m high formed of 38mm diameter x 2.8 thick pipe framing all round complete with one 38mm diameter thick x 2.8 mm thick pipe horizontal brace all neatly mitred and welded at intersections, the gate with two strands of 4mm thick galvanised mild steel straining wire.","no",1,{"v":3240.4624000000003,"d":"3,240.46"}]
[{"$nulls":4},0]
[17.42,"Razor barbed wire",null,null,0]
[{"$nulls":4},0]
["17.42.1","Razor Flat-wrap - To top or bottom of fence - not exceeding 6 strands","m",1,{"v":120.22115504000001,"d":"120.22"}]
[{"$nulls":4},0]
["17.42.2","Concertina Barbed Wire to top of fence","m",1,{"v":172.23520579200002,"d":"172.24"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[17.43,"Sundries",null,null,0]
[{"$nulls":4},0]
["17.43.1","40 x40 x 2mm angle section @ 2m, for razor barbed wire support at 500mm length","no",1,{"v":38.49530454240001,"d":"38.50"}]
[{"$nulls":4},0]
["17.43.2","Replace missing Steel Palisade fence Slats 1800mm high made of 30 x 30 x 3mm angle section pickets with top end split and sharpened, welded to top and bottom rails including painting on both sides","no",1,{"v":203.10755400000002,"d":"203.11"}]
[{"$nulls":4},0]
["17.43.2a","Replace missing Steel Palisade fence Slats 2400mm high made of 30 x 30 x 3mm angle section pickets with top end split and sharpened, welded to top and bottom rails including painting on both sides","no",1,{"v":270.81007200000005,"d":"270.81"}]
[{"$nulls":4},0]
["17.43.3","Fix pedestrian gate including lock, hinges, slats, etc","no",1,{"v":395.6257398,"d":"395.63"}]
[{"$nulls":4},0]
["17.43.4","Replace missing Concrete Palisade fence Slats 1800mm highmade of 110 x 70mm reinforced concrete ","no",1,{"v":225.72135232000005,"d":"225.72"}]
[{"$nulls":4},0]
["17.43.5","Replace missing Concrete Palisade fence Slats 2400mm highmade of 110 x 70mm reinforced concrete ","no",1,{"v":300.9618030933334,"d":"300.96"}]
[{"$nulls":4},0]
[17.44,"\"Betafence 3510\" galvanised wire panels with adhesion coat coating, minimum 200micron and PVC coated to a perfect and durable finish, minimum 60micron",null,null,0]
[{"$nulls":4},0]
["17.44.1","Panels 1988mm high fixed to 2600mm \"Bekafix Secure\" PVC coated post at 3050 centres including stainless steel mini spider brackets, M8 x 25 x 2mm bolts, M8 shear nuts and M8 x 50mm cup square and posts 600mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":1396.0374942400001,"d":"1,396.04"}]
[{"$nulls":4},0]
["17.44.1a","Panels 2376mm high fixed to 3000mm \"Bekafix Secure\" PVC coated post at 3050 centres including stainless steel mini spider brackets, M8 x 25 x 2mm bolts, M8 shear nuts and M8 x 50mm cup square and posts 600mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":3277.2743753924597,"d":"3,277.27"}]
[{"$nulls":4},0]
["17.44.2","Panels 6000mm high fixed to 2600mm \"Bekafix Secure\" PVC coated post at 3050 centres including stainless steel mini spider brackets, M8 x 25 x 2mm bolts, M8 shear nuts and M8 x 50mm cup square and posts 600mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat","m2",1,{"v":803.3717348224002,"d":"803.37"}]
[{"$nulls":4},0]
["17.44.3","PVC coated serrated strip 3000mm long, including backing plates fixed to top of panel","m2",1,{"v":803.3717348224002,"d":"803.37"}]
[{"$nulls":4},0]
[null,"Serrated strip 3000mm long, including backing platesfixed to top of panel","m",1,{"v":101.83222530480003,"d":"101.83"}]
[{"$nulls":4},0]
["17.44.4","Hot Dipped Galvanised serrated strip 3000mm long, including backing plates fixed to top of panel","m",1,{"v":88.25214177120002,"d":"88.25"}]
[{"$nulls":4},0]
["17.44.5","Swing gate \"Singleskin Flat\" wire 3.96mm diameter PVC RAL 7021 MTO 2000mm high x 1000mm wide","no",1,{"v":8249.870078000002,"d":"8,249.87"}]
[{"$nulls":4},0]
["17.44.6","Vehicle sliding gate \"Singleskin Flat\" wire 3.96mm diameter PVC RAL 7021 MTO 2000mm high x 6000mm wide","no",1,{"v":35461.90398637441,"d":"35,461.90"}]
[{"$nulls":4},0]
[17.45,"\"Betafence 3510\" galvanised wire panels with hot dipped galvanised coating, zincalu super coated to SANS 10244-2:2003 specification",null,null,0]
[{"$nulls":4},0]
["17.45.1","Panels 2000mm high fixed to 2600mm \"Bekafix Secure\" PVC coated post at 3050 centres including stainless steel mini spider brackets, M8 x 25 x 2mm bolts, M8 shear nuts and M8 x 50mm cup square and posts 600mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":1166.4518905080001,"d":"1,166.45"}]
[{"$nulls":4},0]
["17.45.1a","Panels 2376mm high fixed to 3000mm \"Bekafix Secure\" PVC coated post at 3050 centres including stainless steel mini spider brackets, M8 x 25 x 2mm bolts, M8 shear nuts and M8 x 50mm cup square and posts 600mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat","m",1,{"v":2345.9836950042622,"d":"2,345.98"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["17.45.2","Panels 6000mm high fixed to 2600mm \"Bekafix Secure\" PVC coated post at 3050 centres including stainless steel mini spider brackets, M8 x 25 x 2mm bolts, M8 shear nuts and M8 x 50mm cup square and posts 600mm bottom ends cast into and including 15MPa concrete footing in ground, including excavation, ramming, removal of spoil and leaving clean and neat","m2",1,{"v":670.3801489256001,"d":"670.38"}]
[{"$nulls":4},0]
["17.45.3","Hot Dipped Galvanised serrated strip 3000mm long, including backing plates fixed to top of panel","m",1,{"v":88.25214177120002,"d":"88.25"}]
[{"$nulls":4},0]
["17.45.4","Swing gate \"Singleskin Flat\" wire 3.96mm diameter PVC RAL 7021 MTO 2000mm high x 1000mm wide","no",1,{"v":6124.090172667201,"d":"6,124.09"}]
[{"$nulls":4},0]
["17.45.5","Vehicle sliding gate \"Singleskin Flat\" wire 3.96mm diameter PVC RAL 7021 MTO 2000mm high x 6000mm wide","no",1,{"v":23396.987297687203,"d":"23,396.99"}]
[{"$nulls":4},0]
[null,"CARPOTS WITH ROOF SHEETING TO SLIGHT FALLS",null,null,0]
[{"$nulls":4},0]
[17.46,"Carpots comprising the following: concrete foundations for columns to be 20Mpa concrete, 500 x 500 x 600mm deep including all excavations, backfilling, compaction, carting away, etc; columns 76 x 76 x 3mm hot rolled tubing with 150 x 150 x 3mm base plates and 200 x 70 x 6mm top flanges: columns 2600mm minimum height, beams; 76 x 76 x3mm hot rolled tubing with closed ends; beams bolted to columns with two 10 x 100mm bolts and nuts at each column; purlins; 150 x 75 x 20 x3mm hot rolled lipped channels bolted to cleats on beams with 0.5mm thick chromadek finished IBR profile roof sheeting; all steelwork cleaned with degreaser and painted with one each of red oxide and universal primer with two coats enamel paint",null,null,0]
[{"$nulls":4},0]
["17.46.1","Carpot comprising one bay, 2,5 x 5,0m on plan, including cutting of existing paving blocks around columns","no",1,{"v":6931.117612000001,"d":"6,931.12"}]
[{"$nulls":4},0]
["17.46.2","Range of carpots (one row) comprising two bays, each bay 2,5 x 5,0m on plan, with carpot structure stepped over sloping site if required, including cutting of existing paving blocks around columns","no",1,{"v":13169.123462800002,"d":"13,169.12"}]
[{"$nulls":4},0]
["17.46.3","Range of carpots (one row) comprising three bays, each bay 2,5 x 5,0m on plan, with carpot structure stepped over sloping site if required, including cutting of existing paving blocks around columns","no",1,{"v":19753.685194200003,"d":"19,753.69"}]
[{"$nulls":4},0]
["17.46.4","Range of carpots (one row) comprising four bays, each bay 2,5 x 5,0m on plan, with carpot structure stepped over sloping site if required, including cutting of existing paving blocks around columns","no",1,{"v":26338.246925600004,"d":"26,338.25"}]
[{"$nulls":4},0]
["17.46.5","Range of carpots (one row) comprising five bays, each bay 2,5 x 5,0m on plan, with carpot structure stepped over sloping site if required, including cutting of existing paving blocks around columns","no",1,{"v":32922.808657,"d":"32,922.81"}]
[{"$nulls":4},0]
["17.46.6","Range of carpots (one row) comprising six bays, each bay 2,5 x 5,0m on plan, with carpot structure stepped over sloping site if required, including cutting of existing paving blocks around columns","no",1,{"v":39507.370388400006,"d":"39,507.37"}]
[{"$nulls":4},0]
[null,"COURTS",null,null,0]
[{"$nulls":4},0]
[17.47,"Clay Courts \"NEW\"",null,null,0]
[{"$nulls":4},0]
["17.47.1","Volleyball, netball, basketball, multi-purpose courts including markings (earthworks measured elsewhere)","m2",1,{"v":398.69260600000007,"d":"398.69"}]
[{"$nulls":4},0]
[17.48,"Refurbishment of Clay Courts",null,null,0]
[{"$nulls":4},0]
["17.48.1","Volleyball, netball, basketball, multi-purpose courts including markings","m2",1,{"v":226.94809880000008,"d":"226.95"}]
[{"$nulls":4},0]
["17.48.2","Volleybal, netball, basketball, multi-purpose courts including markings in bad conditions","m2",1,{"v":226.94809880000008,"d":"226.95"}]
[{"$nulls":4},0]
[null,"GRADING",null,null,0]
[{"$nulls":4},0]
[17.49,"Grading of soccer fields",null,null,0]
[{"$nulls":4},0]
["17.49.1","Open face excavation to reduce levels ","m2",1,{"v":5.1768701456000015,"d":"5.18"}]
[{"$nulls":4},0]
[{"v":17.5,"d":"17.50"},"\"Enviro Outdoor Furniture\" or equally approved",null,null,0]
[{"$nulls":4},0]
["17.50.1","Plastic jungle gym combo","no",1,{"v":24370.2143501304,"d":"24,370.21"}]
[{"$nulls":4},0]
["17.50.2","Plastic two seater sleeper bench 1200mm with back and set in concrete base including all excavations and formwork","no",1,{"v":2695.7753898,"d":"2,695.78"}]
[{"$nulls":4},0]
["17.50.3","Plastic three seater sleeper bench 1800mm with back and set in concrete base including all excavations and formwork","no",1,{"v":3189.5408480000006,"d":"3,189.54"}]
[{"$nulls":4},0]
["17.50.4","Plastic five seater picnic set with open back bench and table set in concrete base including all excavations and formwork","no",1,{"v":5245.199924536001,"d":"5,245.20"}]
[{"$nulls":4},0]
["17.50.5","Plastic square swivel bin","no",1,{"v":1709.2749404432004,"d":"1,709.27"}]
[{"$nulls":4},0]
["17.50.6","Rubber playground flooring","m2",1,{"v":500.5125638400001,"d":"500.51"}]
[{"$nulls":4},0]
[17.51,"Steel seaters, poles, posts, etc.",null,null,0]
[{"$nulls":4},0]
[null,"Epoxy coated",null,null,0]
[{"$nulls":4},0]
["17.51.1","Four seater swing with A-frame Code \"S2 Junior\"","no",1,{"v":3986.9260600000002,"d":"3,986.93"}]
[{"$nulls":4},0]
["17.51.2","\"Tharad\" or equally approved three seater senior swing","no",1,{"v":12707.130738432003,"d":"12,707.13"}]
[{"$nulls":4},0]
["17.51.3","50mm diameter aluminium mini soccer goal posts set,size 1000 x 1500 x 1000m with nets","no",1,{"v":7286.874091200001,"d":"7,286.87"}]
[{"$nulls":4},0]
["17.51.4","\"Van Dyck\" or equally approved easy soccer outdoor carpeting secured with resin based glue to concrete surfaces","m2",1,{"v":552.035916,"d":"552.04"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[17.52,"\"Jungle Gym World\" or equally approved",null,null,0]
[{"$nulls":4},0]
["17.52.1","Code \"SP 3\" Ball throwing stand","no",1,{"v":558.1696484,"d":"558.17"}]
[{"$nulls":4},0]
["17.52.2"," Code \"JG3\" Toddler's Beginners","no",1,{"v":8771.237332,"d":"8,771.24"}]
[{"$nulls":4},0]
["17.52.3"," Code \"JG4\" Toddler's Advanced ","no",1,{"v":9568.622544000002,"d":"9,568.62"}]
[{"$nulls":4},0]
["17.52.4","Code \"JG 8\" Junior Jungle Gym","no",1,{"v":10366.007756000003,"d":"10,366.01"}]
[{"$nulls":4},0]
["17.52.5","Code \"JG 9\" Junior Jungle Gym","no",1,{"v":11641.824095200001,"d":"11,641.82"}]
[{"$nulls":4},0]
["17.52.6","Code \"JG 10\" Senior Jungle Gym","no",1,{"v":15150.319028000002,"d":"15,150.32"}]
[{"$nulls":4},0]
["17.52.7","Code \"JG 11\" Senior De Lux Jungle Gym","no",1,{"v":16745.089452000004,"d":"16,745.09"}]
[{"$nulls":4},0]
["17.52.8","Code \"JG 12\" Super Senior Jungle Gym","no",1,{"v":17904.364875600004,"d":"17,904.36"}]
[{"$nulls":4},0]
["17.52.9","Code \"JG 25 A\" No Tyre Tunnel","no",1,{"v":19137.245088000003,"d":"19,137.25"}]
[{"$nulls":4},0]
["17.52.10","Code \"JG 25 A\" With Tyre Tunnel","no",1,{"v":19995.967624,"d":"19,995.97"}]
[{"$nulls":4},0]
["17.52.11","Implanted Heavy Duty Junior Jungle Gym","no",1,{"v":15947.704240000001,"d":"15,947.70"}]
[{"$nulls":4},0]
["17.52.12","One Seater Implanted Swing","no",1,{"v":3986.9260600000002,"d":"3,986.93"}]
[{"$nulls":4},0]
["17.52.13","Two-Seater A-Frame Swing","no",1,{"v":3189.5408480000006,"d":"3,189.54"}]
[{"$nulls":4},0]
["17.52.14","Four-Seater A-Frame Swing","no",1,{"v":3986.9260600000002,"d":"3,986.93"}]
[{"$nulls":4},0]
["17.52.15","Four-Seater Implanted Swing","no",1,{"v":6379.081696000001,"d":"6,379.08"}]
[{"$nulls":4},0]
["17.52.16","Carousel Swing","no",1,{"v":7973.8521200000005,"d":"7,973.85"}]
[{"$nulls":4},0]
["17.52.17","See Saw Swing","no",1,{"v":3986.9260600000002,"d":"3,986.93"}]
[{"$nulls":4},0]
["17.52.18","Implanted Four Seat Swing","no",1,{"v":12758.163392000002,"d":"12,758.16"}]
[{"$nulls":4},0]
["17.52.19","Code \"SR 1\" Rocking Horse","no",1,{"v":797.3852120000001,"d":"797.39"}]
[{"$nulls":4},0]
["17.52.20","Code \"SR 2\" Four Seat Rocking Sleigh","no",1,{"v":3986.9260600000002,"d":"3,986.93"}]
[{"$nulls":4},0]
["17.52.21","Code \"HD Ssaw\" Implanted Four Seat See Saw","no",1,{"v":6379.081696000001,"d":"6,379.08"}]
[{"$nulls":4},0]
["17.52.22","Code \" HD SS\" Implanted Slide Stand with 5m steel slide","no",1,{"v":19137.245088000003,"d":"19,137.25"}]
[{"$nulls":4},0]
["17.52.23","Code \"SP 8B\" One soccer goal posts (pre-school)","no",1,{"v":1594.7704240000003,"d":"1,594.77"}]
[{"$nulls":4},0]
["17.52.24","Code \"SP 5B\" netball pole 2000mm high with ring and net","no",1,{"v":637.9081696000002,"d":"637.91"}]
[{"$nulls":4},0]
["17.52.25","Code \"SP 6B\" netball pole 3000mm high with ring and net","no",1,{"v":797.3852120000001,"d":"797.39"}]
[{"$nulls":4},0]
["17.52.26","Code \"SP 8A\" Soccer goal posts (pre-school)","no",1,{"v":3189.5408480000006,"d":"3,189.54"}]
[{"$nulls":4},0]
["17.52.27","Code \"SP 5A\" Netball posts set 2000mm high with ring and net","no",1,{"v":1275.8163392000004,"d":"1,275.82"}]
[{"$nulls":4},0]
["17.52.28","Code \"SP 6A\" netball pole 3000mm high with ring and net cast into concrete","no",1,{"v":1594.7704240000003,"d":"1,594.77"}]
[{"$nulls":4},0]
["17.52.29","Code \"SP1\" Basket and netball wall mounted ring","no",1,{"v":318.9540848000001,"d":"318.95"}]
[{"$nulls":4},0]
["17.52.30","Code \"SP2\" Basketball ring with 3000mm high stand and blocker","no",1,{"v":1275.8163392000004,"d":"1,275.82"}]
[{"$nulls":4},0]
["17.52.31","Code \"SP4\" Jogging barrel","no",1,{"v":1435.2933816000002,"d":"1,435.29"}]
[{"$nulls":4},0]
["17.52.32","Code \"SP7\" set of implant rugby posts (pre-school)","no",1,{"v":3189.5408480000006,"d":"3,189.54"}]
[{"$nulls":4},0]
[17.53,"\"Gimtrac\" or equally approved",null,null,0]
[{"$nulls":4},0]
["17.53.1","Code \"SOCC012\" 3000 x 2000 x 1000mm mini soccer goal post set","no",1,{"v":11387.2251307408,"d":"11,387.23"}]
[{"$nulls":4},0]
["17.53.2","Code \"SOCC012\" 1000 x 1500 x 1000mm Aluminium mini soccer goal post set","no",1,{"v":7894.113598800001,"d":"7,894.11"}]
[{"$nulls":4},0]
["17.53.3","Code \"SOCC012\" Five seater aluminium soccer shelter","no",1,{"v":41378.69853885121,"d":"41,378.70"}]
[{"$nulls":4},0]
[null,"PREFABRICATED SHELTERS",null,null,0]
[{"$nulls":4},0]
[17.54,"WENDY HUTS",null,null,0]
[{"$nulls":4},0]
["17.54.1","2400 X 2400mm \"Rock Hard\" wendy house with dune walls, galvanised roof including concrete surface bed","no",1,{"v":14432.672337200005,"d":"14,432.67"}]
[{"$nulls":4},0]
[null,"PHYSICAL BARRIERS",null,null,0]
[{"$nulls":4},0]
[17.55,"BOOM GATES",null,null,0]
[{"$nulls":4},0]
["17.55.1","Steel boom gates not exceeding 6000mm long","no",1,{"v":16432.526716360804,"d":"16,432.53"}]
[{"$nulls":4},0]
[17.56,"BOLLARDS",null,null,0]
[{"$nulls":4},0]
["17.56.1","200mm Diameter precast concrete bollards not exceeding 1500mm","no",1,{"v":561.7026782624,"d":"561.70"}]
[{"$nulls":4},0]
["17.56.2","200mm Diameter steel bollards with concrete infill not exceeding 1500mm","no",1,{"v":722.5046068608002,"d":"722.50"}]
[{"$nulls":4},0]
["17.56.3","400 x 400mm precast concrete dustbin not exceeding 1500mm high","m",1,{"v":1896.5500580800003,"d":"1,896.55"}]
[{"$nulls":4},0]
[17.57,"TIMBER RAILING",null,null,0]
[{"$nulls":4},0]
["17.57.1","Tanalith treated vertical lath (wood) handrails 1200mm high","m",1,{"v":384.2169975360001,"d":"384.22"}]
[{"$nulls":4},0]
[17.58,"RETAINING WALL BLOCKS",null,null,0]
[{"$nulls":4},0]
["17.58.1","Terraforce or Loffelstein or equally approved retaining wall blocks or equivalent retaining wall smooth finish closed face @ 9 blocks per m2. Including AG900 Bidum","m2",1,{"v":781.1829,"d":"781.18"}]
[{"$nulls":4},0]
["17.58.2","Terraforce or Loffelstein or equally approved retaining wall blocks or equivalent retaining wall smooth finish closed face @ 6.5 blocks per m2. Including AG900 Bidum. Earthworks elsewhere.","m2",1,{"v":598.90689,"d":"598.91"}]
[{"$nulls":4},0]
["17.58.3","Terraforce or Loffelstein or equally approved retaining wall blocks or equivalent retaining wall smooth finish closed face @ 9 blocks per m2. Including AG900 Bidum","m2",1,{"v":833.2617600000002,"d":"833.26"}]
[{"$nulls":4},0]
["17.58.4","Terraforce or Loffelstein or equally approved retaining wall blocks or equivalent retaining wall smooth finish closed face @ 6.5 blocks per m2. Including AG900 Bidum. Earthworks elsewhere.","m2",1,{"v":636.5194,"d":"636.52"}]
[{"$nulls":4},0]
[17.59,"GRASS  BLOCKS",null,null,0]
[{"$nulls":4},0]
["17.59.1","Loffelstein grass block or equivalent 600x400x120mm including earthworks @ 4.1 blocks per m2.","m2",1,{"v":332.147396,"d":"332.15"}]
{"$rows_empty":35}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Mechanical Works","index":16,"n_rows":209,"n_cols":7,"rows_kept":209,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 18"]
[]
[null,"MECHANICAL WORKS "]
[]
[null,"AIRC-CONDITIONING"]
[]
[]
[18.1,"INSPECTION AND MAINTENANCE"]
[]
["18,1,1","Major service (3 monthly inspection per unit)","No",1]
[]
["18,1,2","Adhoc Inspection","No",1,{"v":32.3956352,"d":"32.40"}]
[{"$nulls":4},0]
[18.2,"INSTALLATION",null,null,0]
[{"$nulls":4},0]
["18,2,1","Supply and installation 9000 BTU Air-Conditioning","No",1,{"v":22.86750720000001,"d":"22.87"}]
[{"$nulls":4},0]
["18,2,2","Supply and installation 18000 BTU Air-Conditioning","No",1,{"v":22.86750720000001,"d":"22.87"}]
[{"$nulls":4},0]
["18,2,3","Supply and installation 24000 BTU Air-Conditioning","No",1,0]
[{"$nulls":4},0]
[18.3,"REPAIR AND MAINTENANCE",null,null,{"v":53.3575168,"d":"53.36"}]
[{"$nulls":4},0]
["18,3,1","9000 BTU Air-conditioning"]
[null,"Replacement of Air-conditioning parts with the same specidfication as existing."]
[]
["18,3,1,1","Evaporator","No",1,0]
[{"$nulls":4},0]
["18,3,1,2","Condensor","No",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["18,3,1,3","Condensor fan","No",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["18,3,1,4","Gas system pipes","m",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["18,3,1,5","Compressor","No",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["18,3,1,6","Thermostat","No",1,{"v":24.773132800000006,"d":"24.77"}]
[{"$nulls":4},0]
["18,3,1,7","PC Board",null,null,0]
[{"$nulls":4},0]
["18,3,1,8","Regas","No",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["18,3,1,9","Air fliters","No",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["18,3,1,10","Electrical works per Air-conditioning","No",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
["18,3,1,11","Remote control ","No",1,{"v":57.168768000000014,"d":"57.17"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":57.168768000000014,"d":"57.17"}]
[]
[]
[]
[{"$nulls":4},0]
[{"$nulls":4},{"v":57.168768000000014,"d":"57.17"}]
["18,3,2","18000 BTU Air-conditioning",null,null,0]
[null,"Replacement of Air-conditioning parts with the same specidfication as existing.",null,null,0]
[{"$nulls":4},0]
["18,3,2,1","Evaporator","No",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["18,3,2,2","Condensor","No",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["18,3,2,3","Condensor fan","No",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["18,3,2,4","Gas system pipes","m",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["18,3,2,5","Compressor","No",1,{"v":156.26129920000002,"d":"156.26"}]
[{"$nulls":4},0]
["18,3,2,6","Thermostat","No",1,0]
[{"$nulls":4},0]
["18,3,2,7","PC Board",null,null,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["18,3,2,8","Regas","No",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["18,3,2,9","Air fliters","No",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["18,3,2,10","Electrical works per Air-conditioning","No",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["18,3,2,11","Remote control ","No",1,{"v":377.3138688000001,"d":"377.31"}]
[{"$nulls":4},0]
["18,3,3","24000 BTU Air-conditioning",null,null,{"v":377.3138688000001,"d":"377.31"}]
[null,"Replacement of Air-conditioning parts with the same specidfication as existing.",null,null,0]
[{"$nulls":4},{"v":377.3138688000001,"d":"377.31"}]
["18,3,3,1","Evaporator","No",1,0]
[{"$nulls":4},{"v":377.3138688000001,"d":"377.31"}]
["18,3,3,2","Condensor","No",1,0]
[{"$nulls":4},{"v":377.3138688000001,"d":"377.31"}]
["18,3,3,3","Condensor fan","No",1,0]
[{"$nulls":4},{"v":377.3138688000001,"d":"377.31"}]
["18,3,3,4","Gas system pipes","m",1,0]
[{"$nulls":4},{"v":228.67507200000006,"d":"228.68"}]
["18,3,3,5","Compressor","No",1,0]
[{"$nulls":4},{"v":60.98001920000001,"d":"60.98"}]
["18,3,3,6","Thermostat","No",1,0]
[{"$nulls":4},{"v":93.37565440000003,"d":"93.38"}]
["18,3,3,7","PC Board",null,null,0]
[{"$nulls":4},{"v":93.37565440000003,"d":"93.38"}]
["18,3,3,8","Regas","No",1,0]
[{"$nulls":4},{"v":60.98001920000001,"d":"60.98"}]
["18,3,3,9","Air fliters","No",1,0]
[{"$nulls":4},{"v":60.98001920000001,"d":"60.98"}]
["18,3,3,10","Electrical works per Air-conditioning","No",1,0]
[{"$nulls":4},{"v":93.37565440000003,"d":"93.38"}]
["18,3,3,11","Remote control ","No",1,0]
[{"$nulls":4},{"v":261.0707072,"d":"261.07"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":28.584384000000007,"d":"28.58"}]
[{"$nulls":4},0]
[null,"TOTAL CARRIED TO SUMMARY",null,null,0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":47.64064000000001,"d":"47.64"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":51.451891200000006,"d":"51.45"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":51.451891200000006,"d":"51.45"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":51.451891200000006,"d":"51.45"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":81.94190080000001,"d":"81.94"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":17.150630400000004,"d":"17.15"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":102.90378240000001,"d":"102.90"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":123.86566400000002,"d":"123.87"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":123.86566400000002,"d":"123.87"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":123.86566400000002,"d":"123.87"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":500.98897024000007,"d":"500.99"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":128.21049036800002,"d":"128.21"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":199.93823795200007,"d":"199.94"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":199.93823795200007,"d":"199.94"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":999.1766708480004,"d":"999.18"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":999.1766708480004,"d":"999.18"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":100.04534400000004,"d":"100.05"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},0]
[{"$nulls":4},{"v":977.9814400000004,"d":"977.98"}]
[{"$nulls":4},0]
[{"$nulls":4},{"v":977.9814400000004,"d":"977.98"}]

{"sheet":"Provisional Sums","index":17,"n_rows":258,"n_cols":7,"rows_kept":258,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 19"]
[]
[null,"NB:"]
[null,"ALL ITEMS CLAIMED FROM THIS BILL TO BE APPROVED BY GROUP HEAD STRATEGIC SUPPLY CHAIN MANAGEMENT (SSCM). 3 QUOTATIONS FROM LEGITIMATE SERVICE PROVIDERS. QUOTATIONS TO HAVE A COST BREAKDOWN"]
[]
[null,"PROVISIONAL SUMS, ETC."]
[null,"\"HOW TO IMPLEMENT PRIME COST\": THIS IS WHERE A SERVICE IS PROVIDED BY ANOTHER SERVICE PROVIDER. IN THIS CASE, THE MAIN CONTRACTOR SHALL BE ENTITLED TO CHARGE PROFITS AND ATTENDANCE"]
[null,"Tenderers are advised to study the \"Model Preambles for Trades 2008\" before pricing this schedule."]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"Works listed under the heading 'SPECIALIST SUB-CONTRACTORS\"  are works that will commence during the execution of various contracts and the contractor shall allow free access to the site for these specialist contractors.  The contractor shall prepare a programme in conjunction with these sub-contractors in order to complete the works successfully.  Payment to the specialist sub-contractor will be made via the contractor.  The estimated value of these works will vary between the different contracts.  However, the tenderer is to list his/her profit and attendance percentage in the rate column, if required"]
[]
[null,"SPECIALIST SUB-CONTRACTORS"]
[]
[16.1,"PREFABRICATED TIMBER ROOF TRUSSES"]
[]
["16.1.1","For the design, manufacture, delivery to site of prefabricated timber trusses and erection by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.1.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.1.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.2,"REHABILITATION OF SWIMMING POOLS"]
[]
["16.2.1","For the supply, installation  and commissioning of pool cleaning equipment by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.2.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.2.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.3,"STRUCTURAL STEELWORK"]
[]
["16.3.1","For the design, manufacture, delivery to site, repairs and maintenance of structural steelwork by an approved sub-contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.3.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.3.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.4,"PLUMBING AND DRAINLAYING"]
[]
["16.4.1","For the supply, delivery to site of plumbing, drainlaying, including rainwater disposal, sewerage disposal, sanitary fittings, sanitary plumbing, water and fire reticulation, etc and installation by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.4.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.4.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.5,"ELECTRICAL INSTALLATION"]
[]
["16.5.1","For the supply, delivery to site of the electrical reticulation including light fittings, etc and installed by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.5.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"}]
[]
["16.5.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"}]
[]
[16.6,"ART WORK AND SIGNAGE"]
[]
["16.6.1","For the design and installation of art work and/or signage by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.6.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.6.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.7,"ALUMINIUM SHOPFRONTS/CURTAIN WALLING"]
[]
["16.7.1","For the supply, delivery to site of aluminium shopfronts/curtain walling and installed by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.7.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.7.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.8,"SECURITY GATES, SCREENS, ROLLER SHUTTERS AND GRILLES"]
[]
["16.8.1","For the manufactured, delivered to site of security gates, screens, roller shutters and grilles and the erection by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.8.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.8.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.9,"STEEL ROLLER SHUTTER AND GRILLES"]
[]
["16.9.1","For the manufactured, delivered to site of steel roller shutters/grilles and the erection by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.9.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.9.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.10.","ELECTRIC, SOLAR WATER HEATING AND GENERATORS"]
[]
["16.10.1","For the design, supply, installation, commissioning and maintenance of electric, solar water heating system, generators involing, solar geysers, boiler, heat pumps, generator etc by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.10.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.10.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.11.","AIR CONDITIONING / VENTILATION / EXTRACTORS/ COOLING UNITS"]
[]
["16.11.1","For the design, manufactured, delivered to site of air conditioning/ventilation system and the erection by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.11.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.11.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.12.","FIRE DETECTION SYSTEMS"]
[]
["16.12.1","For the designed, supply, installation, commissioning, repair and maintenance of fire protection / prevention systems by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.12.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.12.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.13.","VANITY SLAB TOPS"]
[]
["16.13.1","For the supply, delivery to site and installation of granite vanity slab tops, etc an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.13.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.13.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.14.","MISCELLANEOUS"]
[]
["16.14.1","For any specialized miscellaneous items",{"$nulls":4},"To be advised where applicable"]
[]
["16.14.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.14.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.15.","CONCERETE SPALL REPAIRS"]
[]
["16.15.1","For concrete spall repairs / rehabilitation done by an approved  spall repair sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.15.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.15.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.16,"BIOMETRICS / ACCESS CONTROL"]
[]
["16.16.1","For the supply, installation, repairs and maintenance of biometrics / access control systems done by a specialist sub-contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.16.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.16.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.17,"BOOK DETECTION SYSTEMS FOR LIBRARIES"]
[]
["16.17.1","For the supply, commisioning, installation, repairs, maintenance of Book detection systems, book check units and hardware warranty systems done by a specialist sub-contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.17.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.17.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[16.18,"PRE-FABRICATED STRUCTURES"]
[]
["16.18.1","For the supply and installation pre-fabricated / stroke mobile structures / cottages supplied and installed by a specialist sub-contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.18.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.18.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.19.","LIFTS, ESCALATORS AND HOISTS"]
[]
["16.19.1","For the supply, installation, repair, servicing and warranty to lifts, escalators and hoistsinstalled by an accredited  specialist sub-contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.19.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.19.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.20.","PROFESSIONAL CONSULTING SERVICES (Not Exceeding R200,000.00 VAT inclusive)"]
[]
["16.20.1","For the designs, investigations, cost estimates, and project management servioces supplied by a proffesional accredited consultant, such as an Architect, Quantity Surveyor, Civil Engineer, Electrical Engineer, Structural Engineer, Fire Rational Engineer, Land Surveyor, etc",{"$nulls":4},"To be advised where applicable"]
[]
["16.20.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.20.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.21.","SHOPFITTING, CAPENTRY AND JOINERY"]
[]
["16.21.1","For the fabrication, and installation of shop fitting, capentry and joinery by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.21.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.21.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[]
["16.22.","SCAFFOLDING AND STRUCTURAL SUPPORT"]
[]
["16.22.1","For the erection of scaffolding and structural support for complex structures and high rise building exceeding nine storey high  by a licensed specialist contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.22.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.22.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
[]
["16.23.","FIRE DETECTION SYSTEMS"]
[]
["16.23.1","For the supply, installation, commissioning, repair and maintenance of book detection systems by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.23.2","Allow for profit (insert percent only in rate column)","%",null,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.23.3","Allow for attendance (insert percent only in rate column)","%",null,{"v":5,"d":"5.00"},null,"Rate only"]
[]
[]
["16.24.","SURVEILLANCE AND SECURITY EQUIPMENT "]
[]
["16.24.1","For the supply, installation, commissioning, repair and maintenance of Surveillance and security equipment including CCTV cameras by an approved sub contractor",{"$nulls":4},"To be advised where applicable"]
[]
["16.24.2","Allow for profit (insert percent only in rate column)","%",1,{"v":7.5,"d":"7.50"},null,"Rate only"]
[]
["16.24.3","Allow for attendance (insert percent only in rate column)","%",1,{"v":5,"d":"5.00"},null,"Rate only"]
{"$rows_empty":46}
[null,"TOTAL CARRIED TO SUMMARY",{"$nulls":4},"Rate only"]

{"sheet":"Inspection and Report","index":18,"n_rows":47,"n_cols":7,"rows_kept":47,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 20"]
[]
[null,"INSPECTION AND REPORT"]
[]
[null,"Carrying out detailed inspection and reporting to the Project Manager on roof covering defaults including ridges, hips, valleys, flashings, etc caused by cracks, breakages, dislodgement, failure, etc."]
[]
[19.1,"Roof area with pitch not exceeding 50 degrees and not exceeding 500m²"]
[]
["19.1.1","Thatch/Concrete or terra cotta tiles","item",1,{"v":1441.1293600000004,"d":"1,441.13"}]
[{"$nulls":4},0]
["19.1.2","Profiled fibre-cement sheeting","item",1,{"v":1310.1176,"d":"1,310.12"}]
[{"$nulls":4},0]
["19.1.3","Profiled metal sheeting","item",1,{"v":1179.1058400000004,"d":"1,179.11"}]
[{"$nulls":4},0]
[19.2,"Roof area with pitch not exceeding 50 degrees, exceeding 500m² and not exceeding 1000m²",null,null,0]
[{"$nulls":4},0]
["19.2.1","Concrete or terra cotta tiles","item",1,{"v":2358.211680000001,"d":"2,358.21"}]
[{"$nulls":4},0]
["19.2.2","Profiled fibre-cement sheeting","item",1,{"v":2185.51436,"d":"2,185.51"}]
[{"$nulls":4},0]
["19.2.3","Profiled metal sheeting","item",1,{"v":1965.1764,"d":"1,965.18"}]
[{"$nulls":4},0]
[19.3,"Roof area with pitch not exceeding 50 degrees, exceeding 1000m² and not exceeding 2000m²",null,null,0]
[{"$nulls":4},0]
["19.3.1","Concrete or terra cotta tiles","item",1,{"v":3930.3528,"d":"3,930.35"}]
[{"$nulls":4},0]
["19.3.2","Profiled fibre-cement sheeting","item",1,{"v":3644.5089600000006,"d":"3,644.51"}]
[{"$nulls":4},0]
["19.3.3","Profiled metal sheeting","item",1,{"v":3275.2940000000003,"d":"3,275.29"}]
[{"$nulls":4},0]
[19.4,"Roof area with pitch not exceeding 50 degrees and exceeding 2000m²",null,null,0]
[{"$nulls":4},0]
["19.4.1","Concrete or terra cotta tiles","item",1,{"v":5895.529200000001,"d":"5,895.53"}]
[{"$nulls":4},0]
["19.4.2","Profiled fibre-cement sheeting","item",1,{"v":5109.458640000001,"d":"5,109.46"}]
[{"$nulls":4},0]
["19.4.3","Profiled metal sheeting","item",1,{"v":4257.882200000001,"d":"4,257.88"}]
[]
[]
[]
[]
[]
[]
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"Miscellaneous Chargers","index":19,"n_rows":182,"n_cols":7,"rows_kept":182,"flags":["formulas_cached_only"]}
[]
["Item No.","Description","UNIT","QTY","JULY 2018 Rate","RATE","AMOUNT"]
[]
[null,"SCHEDULE No. 21"]
[]
[null,"MISCELLANEOUS CHARGERS - GENERAL BUILDING ITEMS"]
[]
[null,"SUPPLEMENTARY PREAMBLES"]
[]
[null,"General building services will be carried out at the discretion of The City of Johannesburg's Department Head and Project Managers."]
[]
[null,"Where general building services are required, and the value can not be ascertained in terms of the rates provided by the contractor in Schedules No. 1 to 17, this work will be executed in terms of the contract based on the rates hereunder."]
[]
["18.1.","Call-out Charge"]
[]
["18.1.1","Call-out charge (once off charge applicable to work under R30,00.00 VAT inclusive)","item",1,393.26]
[{"$nulls":4},0]
["18.1.1a","Call-out charge (once off charge applicable to an emergency call-out which takes place after hours, weekends and holidays)","item",1,{"v":561.8000000000001,"d":"561.80"}]
[{"$nulls":4},0]
["18.1.2","Preliminary and General (Works between R30,000.00 and R500,000.00  @ 7%) VAT exclusive","%",1,{"v":0.07,"d":"7%"},{"v":0.07,"d":"7%"},"Rate only"]
[{"$nulls":4},0]
["18.1.3","Preliminary and General (Works between R500,000.00 and R10 million @ 5%) VAT exclusive","%",1,{"v":0.05,"d":"5%"},{"v":0.05,"d":"5%"},"Rate only"]
[{"$nulls":4},0]
[null,"LABOUR RATES - LIMITED TO BILL NO.16 (For new items with no rates)",null,null,0]
[{"$nulls":4},0]
[null,"GENERAL BUILDING",null,null,0]
[{"$nulls":4},0]
["18.2.","Normal hours",null,null,0]
[{"$nulls":4},0]
["18.2.1","General Labour (R200 per day)","hr",1,28.09]
[{"$nulls":4},0]
["18.2.2","Semi Skilled (R280 per day)","hr",1,{"v":39.326,"d":"39.33"}]
[{"$nulls":4},0]
["18.2.3","Artisan (R360 per day)","hr",1,{"v":50.562000000000005,"d":"50.56"}]
[{"$nulls":4},0]
["18.2.4","Site Supervisor (R880 per day)","hr",1,{"v":123.59600000000002,"d":"123.60"}]
[{"$nulls":4},0]
["18.3.","After normal hours and Saturdays ",null,null,0]
[{"$nulls":4},0]
["18.3.1","General Labour","hr",1,{"v":42.135000000000005,"d":"42.14"}]
[{"$nulls":4},0]
["18.3.2","Semi Skilled ","hr",1,{"v":58.98900000000001,"d":"58.99"}]
[{"$nulls":4},0]
["18.3.3","Artisan ","hr",1,{"v":72.47220000000002,"d":"72.47"}]
[{"$nulls":4},0]
["18.3.4","Contracts Manager","hr",1,{"v":134.83200000000002,"d":"134.83"}]
[{"$nulls":4},0]
["18.4.","Extra over - Sundays and holidays (for eight hour shift)",null,null,0]
[{"$nulls":4},0]
["18.4.1","General Labour","hr",1,56.18]
[{"$nulls":4},0]
["18.4.2","Semi Skilled ","hr",1,{"v":78.652,"d":"78.65"}]
[{"$nulls":4},0]
["18.4.3","Artisan ","hr",1,{"v":96.62960000000001,"d":"96.63"}]
[{"$nulls":4},0]
["18.4.4","Contracts Manager","hr",1,{"v":179.77600000000004,"d":"179.78"}]
[{"$nulls":4},0]
["18.5.","SALARY TO THE COMMUNITY LIAISON OFFICE",null,null,0]
[{"$nulls":4},0]
["18.5.1","For the Community Liaison Officer (CLO) salary, including cell phone allowance. (For Projects exceeding R650,000.00 and a period of 3 months)","month",1,{"v":6179.8,"d":"6,179.80"}]
[{"$nulls":4},0]
["18.6.","SCAFFOLDING (To be used as directed by the Project Manager and to be deducted in whole or in part if not required)",null,null,0]
[{"$nulls":4},0]
["18.6.1","Scaffolding exceeding 3.6m high and not exceeding 10m wide in normal areas, 1-storey","day",1,{"v":319.52375,"d":"319.52"}]
[{"$nulls":4},0]
["18.6.2","Scaffolding exceeding 3.6m high and not exceeding 3m wide in confined areas, 1-storey","day",1,{"v":319.52375,"d":"319.52"}]
[{"$nulls":4},0]
["18.6.3","Scaffolding not exceeding 8m high not exceeding 10m wide (Single Tower) in normal areas, 2-storey","day",1,{"v":393.26000000000005,"d":"393.26"}]
[{"$nulls":4},0]
["18.6.4","Scaffolding not exceeding 8m high not exceeding 3m wide (Single Tower) in confined/restricted areas, 2-storey","day",1,{"v":393.26000000000005,"d":"393.26"}]
[{"$nulls":4},0]
["18.6.5","Scaffolding exceeding 12m high and exceeding 10m wide in normal areas 3- storey","day",1,{"v":511.23800000000006,"d":"511.24"}]
[{"$nulls":4},0]
["18.6.6","Scaffolding exceeding 12m high and exceeding 10m wide in normal areas - 3-storey","day",1,{"v":511.23800000000006,"d":"511.24"}]
[{"$nulls":4},0]
["18.6.7","Scaffolding exceeding 16m high  not exceeding 10m wide in normal areas, 4-storey","day",1,{"v":568.0422222222222,"d":"568.04"}]
[{"$nulls":4},0]
["18.6.8","Scaffolding exceeding 20m high  not exceeding 10m wide in normal areas, 5-storey","day",1,{"v":639.0475,"d":"639.05"}]
[{"$nulls":4},0]
["18.6.9","Scaffolding exceeding 24m high  not exceeding 10m wide in normal areas, 5-storey","day",1,730.34]
[{"$nulls":4},0]
["18.6.10","Scaffolding exceeding 28m high  not exceeding 10m wide in normal areas, 6-storey","day",1,{"v":852.0633333333334,"d":"852.06"}]
[{"$nulls":4},0]
["18.6.11","Scaffolding exceeding 32m high  not exceeding 10m wide in normal areas, 7-storey","day",1,{"v":1022.4760000000001,"d":"1,022.48"}]
[{"$nulls":4},0]
["18.6.12","Scaffolding exceeding 36m high  not exceeding 10m wide in normal areas, 8-storey","day",1,{"v":1278.095,"d":"1,278.10"}]
[{"$nulls":4},0]
[{"$nulls":4},0]
["18.8.","UNBLOCKING AND PUMPING",null,null,0]
[{"$nulls":4},0]
["18.8.1","Un-blocking of Drains and Manholes using sewer rods","hour",1,{"v":337.08000000000004,"d":"337.08"}]
[{"$nulls":4},0]
["18.8.2","Water ram 32mm to 50mm dia waste pipes ","hour",1,{"v":426.968,"d":"426.97"}]
[{"$nulls":4},0]
["18.8.3","Electro mechanical, spring cable machine from 50 to 150mm dia","hour",1,{"v":842.7,"d":"842.70"}]
[{"$nulls":4},0]
["18.8.4","Pumping out of non-contaminated water from basements or pools into raods, stormwater channels etc","hour",1,{"v":280.90000000000003,"d":"280.90"}]
[{"$nulls":4},0]
["18.8.5","Pumping out of contaminated water from basements into nearest sewer manholes","hour",1,{"v":303.372,"d":"303.37"}]
[{"$nulls":4},0]
["18.8.6","Disinfecting or Hygiene to contaminated areas, due to sewerage or other","m2",1,{"v":24.7192,"d":"24.72"}]
[{"$nulls":4},0]
["18.9.","PLANT HIRE",null,null,0]
[null,"Including miscellaneous items",null,null,0]
[{"$nulls":4},0]
["18.9.1","Concrete Mixer STD HD GX160 5HP - Drum volume 400L dry mix input 310L, Wet Mix output 260L","hour",1,{"v":275.1246960000001,"d":"275.12"}]
[{"$nulls":4},0]
["18.9.2","Concrete Saw 13HP GX350 - 13Hp petrol engine, push type, blade size350mm Diamond Blade","hour",1,{"v":225.10202400000006,"d":"225.10"}]
[{"$nulls":4},0]
["18.9.3","5kVa Generator ","hour",1,{"v":162.57368400000004,"d":"162.57"}]
[{"$nulls":4},0]
["18.9.4","10kVA Generator ","hour",1,{"v":225.10202400000006,"d":"225.10"}]
[{"$nulls":4},0]
["18.9.5","19 cfm Towable Compressor including miscellaneous","hour",1,{"v":437.6983800000001,"d":"437.70"}]
[{"$nulls":4},0]
["18.9.6","50mm Water pump","hour",1,{"v":187.58502000000001,"d":"187.59"}]
[{"$nulls":4},0]
["18.9.7","80mm Water Pump","hour",1,{"v":225.10202400000006,"d":"225.10"}]
[{"$nulls":4},0]
["18.9.8","Jolly Jumper / Rammer","hour",1,{"v":262.61902800000007,"d":"262.62"}]
[{"$nulls":4},0]
["18.9.9","Conrete breaker / hammer","hour",1,{"v":162.57368400000004,"d":"162.57"}]
[{"$nulls":4},0]
["18.9.10","Hydraulic Jack","hour",1,{"v":162.57368400000004,"d":"162.57"}]
[{"$nulls":4},0]
["18.9.11","Crane Truck 20ton","hour",1,{"v":562.7550600000001,"d":"562.76"}]
[{"$nulls":4},0]
["18.9.12","12000 l Water Truck","hour",1,{"v":475.21538400000014,"d":"475.22"}]
[{"$nulls":4},0]
["18.9.13","6m high mobile scaffolding","hour",1,{"v":162.57368400000004,"d":"162.57"}]
{"$rows_empty":51}
[null,"TOTAL CARRIED TO SUMMARY"]

{"sheet":"SUMMARY","index":20,"n_rows":52,"n_cols":5,"rows_kept":52,"flags":["formulas_cached_only"]}
[]
["Bill No.","SUMMARY","PAGE","AMOUNT","JULY 2018 Rate"]
[]
[1,"ALTERATIONS",30]
[]
[2,"EARTHWORKS",38]
[]
[3,"CONCRETE WORKS",52]
[]
[4,"MASONRY",64]
[]
[5,"WATERPROOFING",69,null,{"v":1441.1293600000004,"d":"1,441.13"}]
[{"$nulls":4},0]
[6,"ROOF COVERING",84,null,{"v":1310.1176,"d":"1,310.12"}]
[{"$nulls":4},0]
[7,"CARPENTRY AND JOINERY",104,null,{"v":1179.1058400000004,"d":"1,179.11"}]
[{"$nulls":4},0]
[8,"CEILING,PARTITION ",117,null,0]
[{"$nulls":4},0]
[9,"FLOOR COVERING",125,null,{"v":2358.211680000001,"d":"2,358.21"}]
[{"$nulls":4},0]
[10,"IRONMONGERY",141,null,{"v":2185.51436,"d":"2,185.51"}]
[{"$nulls":4},0]
[11,"METALWORKS",155,null,{"v":1965.1764,"d":"1,965.18"}]
[{"$nulls":4},0]
[12,"PLASTERING",163,null,0]
[{"$nulls":4},0]
[13,"TILING",169,null,{"v":3930.3528,"d":"3,930.35"}]
[{"$nulls":4},0]
[14,"GLAZING",172,null,{"v":3644.5089600000006,"d":"3,644.51"}]
[{"$nulls":4},0]
[15,"PAINTING",180,null,{"v":3275.2940000000003,"d":"3,275.29"}]
[{"$nulls":4},0]
[16,"EXTERNAL WORKS",201,null,0]
[{"$nulls":4},0]
[17,"MECHANICAL WORKS",203,null,{"v":5895.529200000001,"d":"5,895.53"}]
[{"$nulls":4},0]
[18,"PROVISIONAL SUMS",209,"Rate only",{"v":5109.458640000001,"d":"5,109.46"}]
[{"$nulls":4},0]
[19,"INSPECTION AND REPORTS",210,null,{"v":4257.882200000001,"d":"4,257.88"}]
[]
[20,"MISCELLANEOUS CHARGES",214]
{"$rows_empty":9}
[null,"TOTAL CARRIED TO FORM OF OFFER"]