{"text_format":"3","workbook":"xls","n_sheets":13,"sheets":["A.General","B.Site Clear","C.Earthworks","D.Concrete","E.Piping","F.Structural Steel","G.Mechanical","H.Instrumentation","I.Miscellaneous","J.Building","K.Roads","L. Day Works","Summary"],"not_rendered":{"external_links":1,"defined_names":20,"comments":23},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"A.General","index":0,"n_rows":58,"n_cols":9,"rows_kept":58,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[{"$nulls":3}," "," "]
[null,"ITEM No.","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"A",null,"SECTION A: GENERAL"]
[null,"A1","SANS 1200A","PRELIMINARY AND GENERAL "]
[null,"A2",8.3,"FIXED-CHARGE AND VALUE RELATED ITEMS"]
[null,"A3","8.3.1","Contractual Requirements","Sum",1]
[null,"A4","8.3.2","Establish Facilities on the Site :"]
[null,"A5","SANS 1200AB PSA 8.12","Facilities for Engineer"]
[null,"A6","8.3.2.1","Furnished office","No",1]
[null,"A7",null,"Carports","No",2]
[null,"A8",null,"Name boards","No",1]
[null,"A9","PSA 8.1","Provision of survey equipment and materials","Sum",1]
[null,"A10","PSA 8.13","Facilities for Contractor:"]
[null,"A11",null,"Offices and storage sheds","Sum",1]
[null,"A12",null,"Workshops","Sum",1]
[null,"A13",null,"Laboratories","Sum",1]
[null,"A14",null,"Ablution and latrine facilities","Sum",1]
[null,"A15",null,"Tools and equipment","Sum",1]
[null,"A16",null,"Water supplies, electrical power and communications","Sum",1]
[null,"A17","PSA 8.29","Dealing with water, including protection of the works during storm events for the complete project duration.","Sum",1]
[null,"A18",null,"Access","Sum",1]
[null,"A19",null,"Provision of lateral support to earthworks where required","Sum",1]
[null,"A20","8.3.3","Other fixed-charge obligations","Sum",1]
[null,"A21","8.3.4","Remove Engineer's and Contractor's Site establishment on completion","Sum",1]
[null,"A22",null,"Comply with the regulations as set forth by DEAT","Sum",1]
[]
[null,"A23",8.4,"TIME-RELATED ITEMS"]
[null,"A24","8.4.1","Contractual Requirements","No",1]
[null,"A25","8.4.2","Operate and maintain facilities on the Site:"]
[null,"A26","8.4.2.1","Facilities for Engineer (SANS 1200 AB):"]
[null,"A27",null,"Communications","Sum",1]
[null,"A28",null,"Site Travel","Sum",1]
[null,"A29",null,"Accommodation","Sum",1]
[null,"A30",null,"Survey assistant and material","Sum",1]
[null,"A31","8.4.2.2","Facilities for Contractor :"]
[null,"A32",null,"Offices and storage sheds","Sum",1]
[null,"A33",null,"Workshops","Sum",1]
[null,"A34",null,"Laboratories","Sum",1]
[null,"A35",null,"Accommodation","Sum",1]
[null,"A36",null,"Ablution and latrine facilities","Sum",1]
[null,"A37",null,"Tools and equipment","Sum",1]
[null,"A38",null,"Water supplies, electrical power and communications","Sum",1]
[null,"A39",null,"Dealing with water, including protection of the works during storm events for the complete project duration.","Sum",1]
[null,"A40",null,"Access","Sum",1]
[null,"A41","8.4.3","Supervision","Sum",1]
[null,"A42","8.4.4","Company and head office overhead costs","Sum",1]
[null,"A43","8.4.5","Other time-related obligations","Sum",1]
[null,"A44","8.8.4","Existing services",null," "]
[null,"A45",null,"Temporary protection of existing services","Sum",1]
[null,"A46",null,"Comply with the regulations as set forth by DEAT","Sum",1]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"B.Site Clear","index":1,"n_rows":16,"n_cols":9,"rows_kept":16,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No.","PAYMENT ","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"B","SANS 1200 C","SECTION B: SITE CLEARANCE"]
[null,"B1","PSC 8.2.1","CLEAR SITE"]
[null,"B2","8.2.1","Clear and grub Site","m²",12000,null," "," "]
[null,"B3","8.2.3","Remove and grub all trees and tree stumps regardless of girth:","No",40,null," "," "]
[null,"B4","8.2.10","Strip and remove topsoil to nominal depth of 150mm and stockpile for later re-use as directed by the engineer","m³",1800]
[null,"B5",null,"Clear and remove to spoil dence vegetation including trees up to 200mm in girth","m²",600]
[]
[{"$nulls":8}," "]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY",{"$nulls":4}," "]

{"sheet":"C.Earthworks","index":2,"n_rows":115,"n_cols":9,"rows_kept":115,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No.","PAYMENT ","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"C","SANS1200D","SECTION C: EARTHWORKS"]
[null,"C1","8.3.2","Bulk Excavation"]
[null,null,"PSD 8.3.6","Excavate in all materials to temporary stockpile, backfill to 96% Mod.AASHTO and dispose of surplus to spoil to: "]
[null,"C1.1",null,"Inlet Works ","m³",750]
[null,"C1.2",null,"Manholes","m³",100]
[null,"C1.3",null,"Blower House","m³",145]
[null,"C1.4",null,"Splitter Box","m³",50]
[null,"C1.5",null,"Bioreactors","m³",14040]
[null,"C1.6",null,"Clarifiers","m³",25200]
[null,"C1.7",null,"Sludge Sump","m³",270]
[null,"C1.8",null,"Sludge Pump Station Building","m³",270]
[null,"C1.9",null,"Sludge Pumps","m³",15]
[null,"C1.10",null,"RAS Sump","m³",45]
[null,"C1.11",null,"Scum Sump","m³",135]
[null,"C1.12",null,"New Chlorine Contact Tank","m³",1000]
[null,"C1.13",null,"Chlorine Building","m³",100]
[null,"C1.14",null,"Sludge Drying Beds","m³",4320]
[null,"C1.15",null,"Pipe Works Treches","m³",4500]
[]
[null,"C2",null,"Bulk excavation in all materials to temporary stockpile, and dispose of surplus to spoil for the formation of platforms to: "]
[null,"C2.1",null,"Blower House","m³",3400]
[null,"C2.2",null,"Sludge Pump Station Building","m³",3370]
[null,"C2.3",null,"Chlorine Building"]
[]
[null,"C3","8.3.3","Restricted Excavation"]
[{"$nulls":3},"Excavate in all materials to temporary stockpile, backfill to 96% Mod.AASHTO and dispose of surplus to spoil to: "]
[null,"C3.1",null,"Inlet Works ","m³",75]
[null,"C3.2",null,"Manholes","m³",10]
[null,"C3.3",null,"Blower House","m³",15]
[null,"C3.4",null,"Splitter Box","m³",5]
[null,"C3.5",null,"Bioreactors","m³",1405]
[null,"C3.6",null,"Clarifiers","m³",2520]
[null,"C3.7",null,"Sludge Sump","m³",27]
[null,"C3.8",null,"Sludge Pump Station Building","m³",27]
[null,"C3.9",null,"Sludge Pumps","m³",2]
[null,"C3.10",null,"RAS Sump","m³",5]
[null,"C3.11",null,"Scum Sump","m³",{"v":15,"d":"15.0"}]
[null,"C3.12",null,"New Chlorine Contact Tank","m³",100]
[null,"C3.13",null,"Chlorine Building","m³",10]
[null,"C3.14",null,"Sludge Drying Beds","m³",432]
[null,"C3.15",null,"Pipe Works Treches","m³",450]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"C4",null,"Recompact base of excavation to 95% Mod AASHTO. "]
[null,"C4.1",null,"Inlet Works ","m²",170]
[null,"C4.2",null,"Manholes","m²",55]
[null,"C4.3",null,"Blower House","m²",145]
[null,"C4.4",null,"Splitter Box","m²",50]
[null,"C4.5",null,"Bioreactors","m²",2340]
[null,"C4.6",null,"Clarifiers","m²",2965]
[null,"C4.7",null,"Sludge Sump","m²",80]
[null,"C4.8",null,"Sludge Pump Station Building","m²",180]
[null,"C4.9",null,"Sludge Pumps","m²",10]
[null,"C4.10",null,"RAS Sump","m²",30]
[null,"C4.11",null,"Scum Sump","m²",25]
[null,"C4.12",null,"New Chlorine Contact Tank","m²",250]
[null,"C4.13",null,"Chlorine Building","m²",65]
[null,"C4.14",null,"Sludge Drying Beds","m²",2880]
[null,"C4.15",null,"Pipe Works Treches","m²",2500]
[]
[null,"C5",null,"Backfill with selected material obtained locally and compact to 95% ModAASHTO "]
[null,"C5.1",null,"Inlet Works ","m³",290]
[null,"C5.2",null,"Manholes","m³",142]
[null,"C5.3",null,"Blower House","m³",60]
[null,"C5.4",null,"Splitter Box","m³",54]
[null,"C5.5",null,"Bioreactors","m³",627]
[null,"C5.6",null,"Clarifiers","m³",355]
[null,"C5.7",null,"Sludge Sump","m³",165]
[null,"C5.8",null,"Sludge Pump Station Building","m³",84]
[null,"C5.10",null,"RAS Sump","m³",63]
[null,"C5.11",null,"Scum Sump","m³",105]
[null,"C5.12",null,"New Chlorine Contact Tank","m³",110]
[null,"C5.13",null,"Chlorine Building","m³",70]
[null,"C5.14",null,"Sludge Drying Beds","m³",600]
[null,"C5.15",null,"Pipe Works Treches","m³",750]
[]
[null,"C6","8.3.5","Working Space:"]
[{"$nulls":3},"Extra excavation in soft material to provide working space for insertion and removal of formwork only, to vertical sides of concrete, backfill and compact to 95% Mod AASHTO density to:"]
[null,"C6.1",null,"Inlet Works ","m³",65]
[null,"C6.2",null,"Manholes","m³",80]
[null,"C6.3",null,"Blower House","m³",60]
[null,"C6.4",null,"Splitter Box","m³",30]
[null,"C6.5",null,"Bioreactors","m³",105]
[null,"C6.6",null,"Clarifiers","m³",60]
[null,"C6.7",null,"Sludge Sump","m³",120]
[null,"C6.8",null,"Sludge Pump Station Building","m³",60]
[null,"C6.10",null,"RAS Sump","m³",15]
[null,"C6.11",null,"Scum Sump","m³",25]
[null,"C6.12",null,"New Chlorine Contact Tank","m³",35]
[null,"C6.13",null,"Chlorine Building","m³",45]
[null,"C6.14",null,"Sludge Drying Beds","m³",400]
[null,"C6.15",null,"Pipe Works Treches","m³",1940]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"C7","8.3.3.2","Extra-over above items C1 - C6 inclusive for excavation in:"]
[null,"C7.1",null,"Hard rock material","m³",510]
[]
[null,"C8","8.3.8","Existing services"]
[null,null,"8.3.8.1","Location of existing services by:"]
[null,"C8.1",null,"a) Pipe or cable detection","Sum",1]
[{"$nulls":3},"b) Excavate by hand in soft material to expose                                               existing services","m³",50]
[null,null,"SANS 1200D 8.3.3","c) Hand excavation in restricted areas.","m³",50," "]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY",{"$nulls":4}," "]

{"sheet":"D.Concrete","index":3,"n_rows":441,"n_cols":9,"rows_kept":441,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"D","SANS 1200 G","SECTION D: CONCRETE (STRUCTURAL)"]
[null,"D1","8.2.1","ROUGH FORMWORK"]
[{"$nulls":3},"Formwork to produce a rough finish to:"]
[null,"D1.1",null,"Inlet Works"]
[null,"D.1.1.1",null,"Vertical sides of walls","m²",242]
[null,"D.1.1.2",null,"Rough circular vertical formwork to degritter cone","m²",29]
[]
[null,"D1.2",null,"Manholes"]
[null,"D.1.2.1",null,"Footings for benching","m²",100]
[]
[null,"D1.3",null,"Blower House"]
[null,"D1.3.1",null,"Bases","m²",16]
[null,"D1.3.2",null,"Ring Beam","m²",11]
[null,"D1.3.3",null,"Roof Slab Vertical Sides","m²",11]
[null,"D1.3.4",null,"Roof Slab Soffit","m²",11]
[null,"D1.3.5",null,"Pumps Plinths","m²",4]
[]
[null,"D1.4",null,"Splitter Box"]
[null,"D1.4.1",null,"Footings","m²",28]
[null,"D1.4.2",null,"Walls","m²",517]
[]
[null,"D1.5",null,"Bioreactors"]
[null,"D1.5.1",null,"Footings","m²",3]
[null,"D1.5.2",null,"Walls","m²",48]
[null,"D1.5.3",null,"Concrete Walkway","m²",48]
[]
[null,"D1.6",null,"Clarifiers"]
[null,"D1.6.1",null,"Footings","m²",17]
[null,"D1.6.2",null,"Walls","m²",185]
[null,"D1.6.3",null,"Base Slab","m²",185]
[]
[null,"D1.7",null,"Sludge Sump "]
[null,"D1.7.1",null,"Footings","m²",5]
[null,"D1.7.2",null,"Walls","m²",58]
[null,"D1.7.3",null,"Base Slab","m²",185]
[]
[null,"D1.8",null,"Sludge Pump Station Building"]
[null,"D1.8.1",null,"Bases","m²",16]
[null,"D1.8.2",null,"Ring Beam","m²",11]
[null,"D1.8.3",null,"Roof Slab Vertical Sides","m²",11]
[null,"D1.8.4",null,"Roof Slab Soffit","m²",11]
[]
[null,"D1.9",null,"Sludge Pumps Plinths"]
[null,"D1.9.1",null,"Pumps Plinths","m²",4]
[]
[null,"D1.10",null,"RAS Sump"]
[null,"D1.10.1",null,"Sides of base slab","m²",4]
[null,"D1.10.2",null,"Walls","m²",53]
[]
[null,"D1.11",null,"Scum Sump"]
[null,"D1.11.1",null,"Sides of base slab","m²",4]
[null,"D1.11.2",null,"Walls","m²",53]
[]
[null,"D1.12",null,"New Chlorine Contact Tank"]
[null,"D1.12.1",null,"Sides of base slab","m²",4]
[null,"D1.12.2",null,"Walls","m²",53]
[]
[null,"D1.13",null,"Chlorine Building"]
[null,"D1.13.1",null,"Bases","m²",4]
[null,"D1.13.2",null,"Ring Beam","m²",53]
[null,"D1.13.3",null,"Roof Slab Vertical Sides","m²",4]
[null,"D1.13.4",null,"Roof Slab Soffit","m²",53]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"D1.14",null,"Sludge Drying Beds"]
[null,"D1.14.1",null,"Sides of base slab","m²",4]
[null,"D1.14.2",null,"Walls","m²",53]
[]
[null,"D2","8.2.2","SMOOTH FORMWORK"]
[null,null,"PSG 4.5.1","Formwork, including cutting, small angle fillets not exceeding 20mm x 20mm etc., to produce a smooth finish as from a new steel shutter including filling imperfections with cement grout and rubbing down excrescences, etc., to:"]
[{"$nulls":3},"Sides of walls including forming openings as detailed on the drawings to"]
[null,"D2.1",null,"Inlet Works"]
[null,"D2.1.1",null,"Vertical to sides of walls","m²",274]
[null,"D2.1.2",null,"Smooth circular vertical formwork to degritter cone","m²",21]
[null,"D2.1.3",null,"Sides of base slabs","m²",35]
[null,"D2.1.4",null,"Sides of plinths / bases","m²",1]
[null,"D2.1.5",null,"Sides of suspended slabs","m²",6]
[]
[null,"D2.2",null,"Manholes"]
[null,"D2.2.1",null,"Smooth benching curved surface","m²",1370]
[]
[null,"D2.3",null,"Splitter Box"]
[null,"D2.3.1",null,"Vertical to sides of walls","m²",735]
[]
[null,"D2.4",null,"Bioreactors"]
[null,"D2.4.1",null,"Vertical to sides of walls","m²",48]
[]
[null,"D2.5",null,"Clarifier"]
[null,"D2.5.1",null,"Vertical to sides of walls","m²",653]
[null,"D2.5.2",null,"Circular Formwork to columns","m²",27]
[null,"D2.5.3",null,"Vertical to sides of walls of luanders","m²",27]
[null,"D2.5.4",null,"Horizontal suspended slabs of luanders","m²",27]
[]
[null,"D2.6",null,"RAS Sump "]
[null,"D2.6.1",null,"Vertical to sides of walls","m²",85]
[]
[null,"D2.7",null,"Scum Sump"]
[null,"D2.7.1",null,"Vertical to sides of walls","m²",70]
[]
[null,"D2.8",null,"New Chlorine Contact Tank"]
[null,"D2.8.1",null,"Vertical to sides of walls","m²",21]
[]
[null,"D.2.9","8.2.5","Narrow widths to up to 150mm wide"]
[null,"D2.9.1",null,"Inlet Works","m",19]
[null,"D2.9.2",null,"Bioreactors","m",154]
[null,"D2.9.3",null,"Clarifier","m",131]
[null,"D2.9.4",null,"RAS Sump","m",20]
[null,"D2.9.5",null,"Scum Sump"]
[]
[null,"D2.10","8.2.4","Smooth Horizontal formwork to Suspended slabs"," "]
[null,"D2.10.1",null,"Inlet Works","m²",22]
[null,"D2.10.2",null,"Bioreactors","m²",4]
[null,"D2.10.3",null,"Clarifiers","m²",80]
[null,"D2.10.3",null,"RAS Sump","m²",5]
[null,"D2.10.4",null,"Scum Sump","m²",25]
[]
[null,"D2.11",null,"Formation of chamfers on walls to:"]
[null,"D2.11.1",null,"Clarifier launder","m",92]
[null,"D2.11.2",null,"New Chlorine Contact Tank","m",8]
[null,"D2.11.3",null,"Bioreactors","m",92]
[null,"D2.11.4",null,"Clarifiers","m",8]
[null,"D2.11.5",null,"RAS Sump","m",92]
[null,"D2.11.6",null,"Scum Sump","m",8]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"D3","8.2.6","Box out holes"]
[null,"D3.1","8.2.6A","Small, circular, of diameter up to and including 0.35m"]
[{"$nulls":3},"Up to and including 0.35m deep"]
[null,"D3.1.1",null,"Inlet works","No","Rate Only",null,"Rate Only"]
[null,"D3.1.2",null,"Bioreactors","No",12]
[null,"D3.1.3",null,"Clarifiers","No",5]
[null,"D3.1.4",null,"Splitter Box","No",3]
[null,"D3.1.5",null,"RAS Sump","No",9]
[null,"D3.1.6",null,"Scum Sump ","No",3]
[null,"D3.1.7",null,"New Chlorine Contact Tank","No",4]
[null,"D3.1.8",null,"Sludge Drying Beds","No",42]
[]
[null,"D3.2","8.2.6C","Large, circular, of diameter over 0.35m up to and including 0.7m "]
[{"$nulls":3},"Up to and including 0.5m deep"]
[null,"D3.2.1",null,"Inlet works","No",8]
[null,"D3.2.2",null,"Bioreactors","No",2]
[null,"D3.2.3",null,"Clarifiers","No",3]
[null,"D3.2.4",null,"Splitter Box","No",1]
[null,"D3.2.5",null,"RAS Sump","No","Rate Only",null,"Rate Only"]
[null,"D3.2.6",null,"Scum Sump ","No","Rate Only",null,"Rate Only"]
[null,"D3.2.7",null,"New Chlorine Contact Tank","No","Rate Only",null,"Rate Only"]
[null,"D3.2.8",null,"Sludge Drying Beds","No","Rate Only",null,"Rate Only"]
[]
[null,"D3.4","PSG 8.1.2","REINFORCEMENT"]
[null,"D3.4.1","8.3.1","MILD STEEL BARS:"]
[null,"D3.4.1.1",null,"Inlet Works ","t",0.5]
[null,"D3.4.1.2",null,"Blower House","t",{"v":2,"d":"2.0"}]
[null,"D3.4.1.3",null,"Splitter Box","t",0.5]
[null,"D3.4.1.4",null,"Bioreactors","t",0.2]
[null,"D3.4.1.5",null,"Clarifiers","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.6",null,"Sludge Sump","t",0.5]
[null,"D3.4.1.7",null,"Sludge Pump Station Building","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.8",null,"RAS Sump","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.9",null,"Scum Sump","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.10",null,"New Chlorine Contact Tank","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.11",null,"Chlorine Building","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.12",null,"Sludge Drying Beds","t",{"v":1,"d":"1.0"}]
[null,"D3.4.1.13",null,"Pipe Works Thrust Blocks","t",{"v":1,"d":"1.0"}]
[]
[null,"D3.4.2","8.3.1","HIGH-TENSILE STEEL BARS:"]
[null,"D3.4.2.1",null,"Inlet Works ","t",10]
[null,"D3.4.2.2",null,"Blower House","t",143]
[null,"D3.4.2.3",null,"Splitter Box","t",43]
[null,"D3.4.2.4",null,"Bioreactors","t",48]
[null,"D3.4.2.5",null,"Clarifiers","t",3]
[null,"D3.4.2.6",null,"Sludge Sump","t",22]
[null,"D3.4.2.7",null,"Sludge Pump Station Building","t",4]
[null,"D3.4.2.8",null,"RAS Sump","t",3]
[null,"D3.4.2.9",null,"Scum Sump","t",5]
[null,"D3.4.2.10",null,"New Chlorine Contact Tank","t",1.5]
[null,"D3.4.2.11",null,"Chlorine Building","t",28]
[null,"D3.4.2.12",null,"Sludge Drying Beds","t",{"v":3,"d":"3.0"}]
[null,"D3.4.2.13",null,"Pipe Works Thrust Blocks","t",{"v":3,"d":"3.0"}]
[]
[null,"D3.4.3","8.3.2","MESH:"]
[{"$nulls":3},"High-tensile welded mesh reinforcement in standard sheet sizes (6.0 m x 2.4 m)"]
[null,"D3.4.3.1",null,"Mesh Ref. 193","t","RATE ONLY"]
[null,"D3.4.3.2",null,"Mesh Ref. 395","t",1]
[null,"D3.4.3.3",null,"Mesh Ref. 617","t",8]
[null,"D3.4.3.4",null,"Mesh Ref. 888","t",10]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"D4",null,"CONCRETE"]
[null,"D4.1","8.4.2","Blinding layer in 15MPa / 19mm concrete to:"]
[null,"D4.1.1",null,"Inlet Works ","m²",178]
[null,"D4.1.2",null,"Manholes","m²",1750]
[null,"D4.1.3",null,"Blower House","m²",347]
[null,"D4.1.4",null,"Splitter Box","m²",17]
[null,"D4.1.5",null,"Bioreactors","m²",278]
[null,"D4.1.6",null,"Clarifiers","m²",22]
[null,"D4.1.7",null,"Sludge Sump","m²",11]
[null,"D4.1.8",null,"Sludge Pump Station Building","m²",16]
[null,"D4.1.9",null,"RAS Sump","m²",16]
[null,"D4.1.10",null,"Scum Sump","m²",16]
[null,"D4.1.11",null,"New Chlorine Contact Tank","m²",16]
[null,"D4.1.12",null,"Chlorine Building","m²",16]
[null,"D4.1.13",null,"Sludge Drying Beds","m²",16]
[null,"D4.1.14",null,"Pipe Works Thrust Blocks","m²",16]
[]
[null,"D4.2",null,"Mass concrete encasement, class 15MPa/19mm to pipes of various sizes to:"]
[null,"D4.2.1",null,"Inlet works","m³",55]
[null,"D4.2.2",null,"Bioreactors","m³",65]
[null,"D4.2.3",null,"Clarifiers","m³",95]
[null,"D4.2.4",null,"Splitter Box","m³",5]
[null,"D4.2.5",null,"RAS Sump","m³",7]
[null,"D4.2.6",null,"Scum Sump ","m³",3]
[null,"D4.2.7",null,"New Chlorine Contact Tank","m³",10]
[null,"D4.2.8",null,"Sludge Drying Beds","m³",45]
[null,"D4.2.9",null,"Manholes ","m³",42]
[]
[null,"D4.3",null,"Screed applied to surfaces to produce a slope with a minimum thickness of 30mm to:"]
[null,"D4.3.1",null,"Inlet Works","m²",5]
[null,"D4.3.2",null,"Clarifier","m²",75]
[null,"D4.3.3",null,"Splitter Box","m²",{"v":1.5,"d":"2"}]
[null,"D4.3.4",null,"Bioreactors","m²",55]
[null,"D4.3.5",null,"RAS Sump","m²",5]
[null,"D4.3.6",null,"Scum Sump ","m²",{"v":1.5,"d":"2"}]
[null,"D4.3.7",null,"New Chlorine Contact Tank","m²",7]
[null,"D4.3.8",null,"Sludge Drying Beds","m²",75]
[]
[null,"D4.4",null,"Dry mortar (75mm Thick) to underside of:"]
[null,"D4.4.1",null,"Clarifiers","m²",200]
[]
[null,"D4.5",null,"No Fines concrete (10mm Thick) to:"]
[null,"D4.5.1",null,"Bioreactors","m³",25]
[]
[null,"D4.6",null,"Benching to: "]
[null,"D4.6.1",null,"Inlet Works","m³",3]
[null,"D4.6.2",null,"Clarifier","m³",86]
[]
[null,"D4.7","8.4.3","Strength concrete grade 30MPa / 19mm (with 30% PFA) to:"]
[null,"D.4.7.1",null,"Inlet Works:"]
[null,"D.4.7.1.1",null,"Floor slab","m³",33]
[null,"D.4.7.1.2",null,"Walls","m³",40]
[null,"D.4.7.1.3",null,"Suspended Slabs","m³",6]
[null,"D.4.7.1.4",null,"Degritter cone walls","m³",13]
[null,"D.4.7.1.5",null,"Bases","m³",1]
[]
[null,"D4.7.2",null,"Blower House"]
[null,"D4.7.2.1",null,"Ring Beam","m³",394]
[null,"D4.7.2.1",null,"Roof Slab","m³",542]
[null,"D4.7.2.1",null,"Pump Plinth","m³",1]
[null,"D4.7.2.1",null,"Floor Slabs","m³",191]
[]
[null,"D4.7.3",null,"Clarifiers"]
[null,"D4.7.3.1",null,"Vertical Walls","m³",38]
[null,"D4.7.3.2",null,"10 Degree Inclined Base slab","m³",129]
[null,"D4.7.3.3",null,"Launders","m³",115]
[null,"D4.7.3.4",null,"Outlet Chamber","m³",8]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"D4.7.4",null,"Bioreactors"]
[null,"D4.7.4.1",null,"Floor slabs","m³",790]
[null,"D4.7.4.2",null,"Vertical Walls","m³",450]
[null,"D4.7.4.3",null,"Walkway","m³",25]
[null,"D4.7.4.4",null,"Aerator Platforms","m³",20]
[null,"D4.7.4.5",null,"Outlet Chamber","m³",3]
[]
[null,"D4.7.5",null,"Splitter Box"]
[null,"D4.7.5.1",null,"Floor slab","m³",4]
[null,"D4.7.5.2",null,"Vertical Walls","m³",14]
[]
[null,"D4.7.6",null,"Sludge  Sump"]
[null,"D4.7.6.1",null,"Floors","m³",8]
[null,"D4.7.6.2",null,"Vertical Walls","m³",25]
[null,"D4.7.6.2",null,"Suspended Slabs","m³",8]
[]
[null,"D4.7.7",null,"Sludge Pump Station Building"]
[null,"D4.7.7.1",null,"Ring Beam","m³",6]
[null,"D4.7.7.2",null,"Roof Slab","m³",30]
[null,"D4.7.7.3",null,"Pump Plinth","m³",30]
[null,"D4.7.7.4",null,"Floor Slabs","m³",25]
[]
[null,"D4.7.8",null,"RAS Sump"]
[null,"D4.7.8.1",null,"Floors","m³",25]
[null,"D4.7.8.2",null,"Vertical Walls","m³",35]
[null,"D4.7.8.3",null,"Suspended Slabs","m³",25]
[]
[null,"D4.7.9",null,"New Chlorine Contact Tank"]
[null,"D4.7.9.1",null,"Floor Slabs","m³",8]
[null,"D4.7.9.2",null,"Vertical Walls","m³",11]
[null,"D4.7.9.3",null,"Walkway","m³",6]
[]
[null,"D4.7.10",null,"Chlorine Building"]
[null,"D4.7.10.1",null,"Ring Beam","m³",6]
[null,"D4.7.10.2",null,"Roof Slab","m³",30]
[null,"D4.7.10.4",null,"Floor Slabs","m³",21]
[]
[null,"D4.7.11",null,"Sludge Drying Beds"]
[null,"D4.7.11.1",null,"Floor slabs","m³",330]
[]
[null,"D5","8.4.4","FINISHES TO UNFORMED SURFACES"]
[null,"D5.1","8.4.4A      PSG 5.1.4","Wood float finish to top surface of floorslab and walls to:"]
[null,"D5.1.1",null,"Inlet Works ","m²",47]
[null,"D5.1.2",null,"Blower House","m²",15]
[null,"D5.1.3",null,"Splitter Box","m²",4]
[null,"D5.1.4",null,"Bioreactors","m²",250]
[null,"D5.1.5",null,"Clarifiers","m²",185]
[null,"D5.1.6",null,"Sludge Sump","m²",27]
[null,"D5.1.7",null,"RAS Sump","m²",5]
[null,"D5.1.8",null,"Scum Sump","m²",20]
[null,"D5.1.9",null,"New Chlorine Contact Tank","m²",5]
[null,"D5.1.10",null,"Sludge Drying Beds","m²",4]
[null,"D5.1.11",null,"Pipe Works Thrust Blocks","m²",25]
[]
[null,"D5.2","8.4.4B      PSG 5.4.2","Steel trowel finish to top surface of floorslab and walls to:"]
[null,"D5.2.1",null,"Inlet Works ","m²",47]
[null,"D5.2.2",null,"Blower House","m²",15]
[null,"D5.2.3",null,"Splitter Box","m²",4]
[null,"D5.2.4",null,"Bioreactors","m²",250]
[null,"D5.2.5",null,"Clarifiers","m²",185]
[null,"D5.2.6",null,"Sludge Sump","m²",27]
[null,"D5.2.7",null,"RAS Sump","m²",5]
[null,"D5.2.8",null,"Scum Sump","m²",20]
[null,"D5.2.9",null,"New Chlorine Contact Tank","m²",5]
[null,"D5.2.10",null,"Sludge Drying Beds","m²",4]
[null,"D5.2.11",null,"Pipe Works Thrust Blocks","m²",25]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"D5.3","8.4.4C      ","Powerfloat finish to top surface of floorslab to:"]
[null,"D5.3.1",null,"Sludge Pump Station Building","m²",1198]
[null,"D5.3.2",null,"Chlorine Building","m²",230]
[]
[null,"D6",null,"Supply and install 20x50mm MCC \"Servistrip AH205\" Hydrophilic water or similar approved at pipe entries / exits to:"]
[null,"D6.1",null,"Clarifier","m",60]
[]
[null,"D7",null,"12 x 12mm Polyurethane bead to seal  joints to:"]
[null,"D7.1",null,"Bioreactors","m",315]
[null,"D7.2",null,"Clarifier","m",216]
[]
[]
[null,"D8",null,"EXISTING WORKS"]
[null,"D8.1",null,"Tie-in of new pipelines into existing manholes. Rate to include for breaking into chamber, diversion of existing flows, patching with a non-shrink epoxy grout, hydrophilic waterbar \"SW20\" wrapped around pipe and any other requirements needed."]
[null,"D8.1.1",null,"500ND Spigot and Socket tie-in Existing Sewer Inlet","No",1]
[]
[null,"D8.2",null,"Seal existing pipe entry and exits to ensure a watertight structure. Rate to include formwork, concrete and any other requirements to ensure a watertight seal."]
[null,"D8.2.1",null,"500ND Spigot and Socket tie-in Existing Sewer Inlet","No",1]
[]
[null,"D9",null,"Manholes"]
[null,"D9.1","SANS 8.2.14 PSLD 3.5.2","Construct precast concrete manholes 1200mm internal diameter, complete including excavation, stabilized soil, 150mm base slabs with one layer mesh ref. 617,  backfilling, and precast concrete covers with type 4A replacement lid and all joints sealed, internal step irons, benching, and forming / sealing pipe entry/exit holes, up to 1.5m deep. "]
[null,"D9.1.1",null,"Up to 1.5m deep"," "," "]
[null,"D9.1.1.1",null,"Main Sewer Line to the Inlet Works","No",5]
[null,"D9.1.1.2",null,"RAS line","No",4]
[null,"D9.1.1.3",null,"Sludge Gravity Lines to the Sludge Sump","No",12]
[null,"D9.1.1.4",null,"Supenatant from Bioreactors to the Clarifiers line","No",3]
[null,"D9.1.1.5",null,"Treated Effluent to the Chlorine Contact Tank line","No",4]
[null,"D9.1.1.6",null,"Treated Effluent to the the pond line","No",2]
[null,"D9.1.1.7",null,"Gravity lin from sludge drying beds to Inlet Works","No",14]
[]
[null,"D9.1.2",null,"Extra over item C252 for increase in height: "]
[null,"D9.1.2.1",null,"From 1.5m - 2.0m","No",4]
[null,"D9.1.2.2",null,"From 2m - 2.5m","No",12]
[null,"D9.1.2.3",null,"2.5m and deeper","No",2]
[]
[null,"D10","8.8            PSG 8.4","CAST IN ITEMS"]
[null,"D10.1",null,"Labour component to position and cast-in or fix the following items in place"]
[null,"D10.1.1",null,"To inlet works:"]
[null,"D10.1.1.1",null,"Mechanical grit removal frame","No",2]
[null,"D10.1.1.2",null,"Manual bar screen frame","No",2]
[null,"D10.1.1.3",null,"Sluice gate frames for 1.2m wide channel","No",2]
[null,"D10.1.1.4",null,"Sluice gate frames for 0.75m wide channel","No",6]
[null,"D10.1.1.5",null,"Mechanical Screen","No",2]
[null,"D10.1.1.6",null,"Degritter ","No",2]
[]
[null,"D10.1.2",null,"To Clarifier:"]
[null,"D10.1.2.1",null,"M20 HD Bolts supplied by Mechanical bridge supplier","No",8]
[null,"D10.1.2.2",null,"50mm uPVC drainage pipes ","No",8]
[null,"D10.1.2.3",null,"Weir Plate to Launders","No",2]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"D10.2",null,"Supply deliver and install ball and tube handrailing, top mounted, Stainless steel grade 304, including all fixings, rivets, bends etc.",null," "]
[null,"D10.2.1",null,"To Bioreactors Walkways","m",144]
[null,"D10.2.2",null,"To Clarifiers Rotating Scrappers Walkway","m",46]
[null,"D10.2.3",null,"To Sludge Sump","m",9]
[null,"D10.2.4",null,"To Clhlorine Contact Tank","m",70]
[]
[null,"D10.3",null,"Supply deliver and install ball and tube handrailing, side mounted, Stainless steel grade 304, including all fixings, rivets, bends etc."]
[null,"D10.3.1",null,"To Inlet Works","m",90]
[]
[null,"D10.4",null,"Supply deliver and install ball and tube handrailing radiused at 1975mm, top mounted, stainless steel grade 304, including all fixings, rivets, bends etc."]
[null,"D10.4.1",null,"To Inlet Works","m",20]
[]
[null,"D10.5",null,"Supply, deliver and install chemical anchors including drilling, resin tubes, studs, nuts and washers of various diameters to suppliers specifications"]
[null,"D10.5.1",null,"M12","No",16]
[null,"D10.5.2",null,"M16","No",28]
[null,"D10.5.3",null,"M20","No",194]
[null,"D10.5.4",null,"M24","No",16]
[]
[null,"D10.6",null,"Supply, deliver and install cementitious non shrink grout (ABE - Duragrout 1000 or similar approved) to bolt pockets and under base plates"]
[null,"D10.6.1",null,"Inlet Works","m³",{"v":0.4,"d":"0.400"}]
[null,"D10.6.2",null,"To Clhlorine Contact Tank","m³",{"v":0.3,"d":"0.300"}]
[null,"D10.6.3",null,"To Bioreactors Walkways","m³",{"v":0.6,"d":"0.600"}]
[null,"D10.6.4",null,"To Sludge Sump","m³",0.015]
[]
[null,"D10.7",8.5,"JOINTS"]
[null,"D10.7.1",null,"Keyed expansion joints complete with 250mm Rear Guard \"S\" Waterbar or similar approved including Flexcell joint filler and polyurethane joint sealer: "]
[null,"D10.7.1.1",null,"Chlorine Contact Tank(Expansion Joint)","m",55]
[]
[null,"D10.7.2","PSG 8.2","Expansion joints complete with 200mm Rear Guard \"S\" Waterbar or similar approved including Flexcell joint filler and polyurethane joint sealer: "]
[null,"D10.7.1.1",null,"To Inlet Works","m",25]
[null,"D10.7.1.2",null,"Clarifier (Typical Section through Clarifier Wall)","m",40]
[null,"D10.7.1.3",null,"Clarifier (Floor Joints)","m",90]
[]
[null,"D10.7.3",null,"Formation of expansion joints complete with 150mm Rear Guard \"S\" Waterbar or similar approved including 12mm Flexcell joint filler and polyurethane joint sealer: "]
[null,"D10.7.3.1",null,"To Inlet Works","m",45]
[null,"D10.7.3.2",null,"Clarifier (Clarifier Wall)","m",154]
[null,"D10.7.3.3",null,"Clarifier (Floor  to Wall Joints)","m",88]
[null,"D10.7.3.2",null,"Bioreactors (Bioreactors Walls)","m",95]
[null,"D10.7.3.3",null,"Bioreactors (Floor  to Wall Joints)","m",128]
[]
[null,"D10.7.4","PSG 8.2","Formation of Key joints complete with 150mm Rear Guard \"R\" Waterbar or similar approved including polyurethane joint sealer: "]
[null,"D10.7.4.1",null,"To Bioreactors Walkways  (Floor Key Joint K.J.)","m",335]
[null,"D10.7.4.2",null,"Sludge Sump (Floor Key Joint)","m",35]
[]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"E.Piping","index":4,"n_rows":324,"n_cols":11,"rows_kept":324,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"E"," ","SECTION E: PIPELINES"]
[null,"E1","SANS 1200 DB","EARTHWORKS FOR PIPE TRENCHES:"]
[null,"E1.1","8.3.2","Excavate in all materials for trenches, backfill, compact to 93% Mod AASHTO and dispose of surplus material including selective stockpile and double handling of suitable granular material for pipe cradle and blanket for all pipes of nominal diameter, to a depth not exceeding 1.5m"]
[null,"E1.1.1",null,"750ND Spigot and Socket concrete pipe","m³","RATE ONLY",null,"RATE ONLY"]
[null,"E1.1.2",null,"600ND Spigot and Socket concrete pipe","m³","RATE ONLY",null,"RATE ONLY"]
[null,"E1.1.3",null,"500ND Spigot and Socket concrete pipe","m³",1300]
[null,"E1.1.4",null,"350ND Spigot and Socket concrete pipe","m³",555]
[null,"E1.1.5",null,"250OD mPVC Class 12","m³",675]
[null,"E1.1.6",null,"250OD mPVC Class 9","m³",925]
[null,"E1.1.7",null,"200OD mPVC Class 9","m³",330]
[null,"E1.1.8",null,"160OD mPVC Class 9","m³","RATE ONLY",null,"RATE ONLY"]
[null,"E1.1.9",null,"140OD mPVC Class 10","m³","RATE ONLY",null,"RATE ONLY"]
[null,"E1.1.10",null,"110OD mPVC Class 10","m³","RATE ONLY",null,"RATE ONLY"]
[null,"E1.1.11",null,"90OD HDPE Class10","m³","RATE ONLY",null,"RATE ONLY"]
[null,"E1.1.12",null,"80OD mPVC Class 9","m³","RATE ONLY",null,"RATE ONLY"]
[]
[null,"E1.2","8.3.2","Extra-over items E2 for deeper excavation in material"]
[null,"E1.2.1",null,"From 1.5m to 2m","m³",428]
[null,"E1.2.2",null,"Deeper than 2m","m³","RATE ONLY",null,"RATE ONLY"]
[]
[null,"E1.3","8.3.2.2","Rock "]
[null,"E1.3.1"," ","Extra over 5.2 for rock","m³",45]
[]
[null,"E2","SANS 1200 LB","Bedding (Pipes) "]
[null,"E2.1","8.2.2.3","Importation and placing of backfill and bedding materials from commercial sources and compact to 90% ModAASHTO for Class \"Flexible bedding: \""]
[null,"E2.1.1","PSLB 3.1","Selected granular material, for pipe cradle ","m³",139]
[null,"E2.1.2","PSLB 3.2","Selected fill blanket 300mm above and around pipe","m³",741]
[]
[null,"E3","SANS 1200LD","Medium Pressure Pipelines"]
[null,"E3.1"," ","Concrete Pipes"]
[null,"E3.1.1","8.2.1","Supply, lay, joint, bed (class C) and test Concrete Pressure pipes Class \"T2\""]
[]
[null,"E3.1.1.1",null,"500ND Spigot and Socket Concrete pipes","m",570]
[]
[null,"E3.1.2","8.2.1","Supply and deliver, lay, joint, bed (class C) and test Concrete pipes Class \"75D\":"]
[null,"E3.1.2.1",null,"750ND Spigot and Socket Concrete Pipes","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.1.2.2",null,"600ND Spigot and Socket Concrete Pipes","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.1.2.3",null,"350ND Spigot and Socket Concrete Pipes","m",245]
[null,"E3.1.2.4",null,"250ND Spigot and Socket Concrete Pipes","m","RATE ONLY",null,"RATE ONLY"]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"E3.2","8.2.5","mPVC Piping"]
[null,"E3.2.1",null,"Supply and deliver to site, lay, bed and test the following mPVC type pipes with integral couplings below ground"]
[null,"E3.2.1.1",null,"250mm OD mPVC class 12","m",300]
[null,"E3.2.1.2",null,"250mm OD mPVC class 9","m",410]
[null,"E3.2.1.3",null,"200mm OD mPVC class 9","m",200]
[null,"E3.2.1.4",null,"160mm OD mPVC class 9","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.2.1.5",null,"140mm OD mPVC class 9","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.2.1.6",null,"110mm OD mPVC class 9","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.2.1.7",null,"80mm OD mPVC class 9","m","RATE ONLY",null,"RATE ONLY"]
[]
[null,"E3.2.2",null,"Supply, deliver to site and install 160mm OD mPVC dewatering pipe together with endcap to prevent ingress of foreign matter to:"]
[null,"E44",null,"Clarifiers","m",45]
[]
[null,"E3.3",null,"HDPE Piping"]
[null,"E3.3.1",null,"Supply and deliver to site, lay, bed and test the following HDPE below ground. HDPE type piping shall be to SANS ISO 4427."]
[null,"E3.3.1.1",null,"160mm ND HDPE PE80 CLASS 10","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.3.1.2",null,"90mm ND HDPE PE80 CLASS 10","m","RATE ONLY",null,"RATE ONLY"]
[null,"E3.3.1.3",null,"90mm ND HDPE PE63 CLASS 10","m","RATE ONLY",null,"RATE ONLY"]
[]
[null,"E3.4",null,"Supply, deliver and install steel piping (6mm wall thickness minimum), flanged to SANS 1123 Table 1000/3. All pipework shall be fabricated in accordance with SANS 719. Rate to include Carboline epoxy lining internally and externally to a 0.3mm dry film thickness"]
[null,"E3.4.1",null,"350ND Steel Pipe"]
[null,"E3.4.1.1",null,"Clarifier centre column","m",7]
[]
[null,"E3.5",null,"Pipe Specials: Supply, deliver and install steel piping specials (6mm wall thickness minimum), flanged to SANS 1123 Table 1000/3. All pipework shall be fabricated in accordance with SANS 719. Rate to include Carboline epoxy lining internally and externally to a 0.3mm dry film thickness"]
[null,"E3.5.1",null,"Inlet Works"]
[null,"E3.5.1.1",null,"500ND Steel Bends"]
[null,"E3.5.1.1.1",null,"7 to 22.5 deg incl.","No","Rate Only"]
[null,"E3.5.1.1.2",null,"to 45 deg incl.","No","Rate Only"]
[null,"E3.5.1.1.3",null,"to 90 deg incl.","No",2]
[]
[null,"E3.5.2",null,"Biorectors"]
[null,"E3.5.2.1",null,"500ND Steel Bends"]
[null,"E3.5.2.1.1",null,"7 to 22.5 deg incl.","No","Rate Only"]
[null,"E3.5.2.1.2",null,"to 45 deg incl.","No","Rate Only"]
[null,"E3.5.2.1.3",null,"to 90 deg incl.","No",2]
[]
[null,"E3.5.3",null,"Inlet Works"]
[null,"E3.5.3.1",null,"350ND Steel Bends"]
[null,"E3.5.3.1.1",null,"7 to 22.5 deg incl.","No","Rate Only"]
[null,"E3.5.3.1.2",null,"to 45 deg incl.","No","Rate Only"]
[null,"E3.5.3.1.3",null,"to 90 deg incl.","No","Rate Only"]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"E60",null,"Couplings"]
[null,"E61",null,"Supply, deliver and install Viking Johnson flange adaptor to suit 500ND steel pipe "]
[null,"E62",null,"Biorectors","No",3]
[]
[null,"E63",null,"Valves"]
[null,"E64",null,"500NB PVC Non-return valves to:"]
[null,"E65",null,"Biorectors","No",3]
[]
[null,"E64",null,"350NB PVC Non-return valves to:"]
[null,"E65",null,"Clarifiers","No",3]
[null,"E66",null,"Cordrain piping as per \"Under Drain Detail\" on drawing 346617 / 005","m",51]
[null,"E67",null,"PUMPSTATIONS"]
[]
[null,"E68","SANS 1200L 8.2.1","All pipework shall be fabricated in accordance with SANS 62 medium class / SANS 719, with a Carboline epoxy finish internally and externally to a 0.3mm dry film thickness, and all  flanges to be fabricated to SANS 1123 - Table 1000/3 flat faced.  Rates shall include all jointing material, bolts, nuts, washers and gaskets to suit the pipe pressure rating."]
[null,"E69",null,"Existing Clarifier Scum Pumpstation - Line 24"]
[null,"E70",null,"Suction Pipework"]
[null,"E71",null,"PS1 - 80/50ND concentric reducer welded to 1000mm long x 80ND, final site measure (FSM), P.E spool piece. 50ND end flanged to suit pump suction.","No",2]
[null,"E72",null,"PS2 - 80ND, 90 Degree, P.E medium radius bend (MRB), one end welded to 5900mm long  x 80ND (FSM) spool piece, other end welded to PS1","No",2]
[null,"E73",null,"PS3 - 100/80ND bell mouth with 80ND end welded to PS2","No",2]
[null,"E74",null,"Delivery Pipework"]
[null,"E75",null,"PD1 - 80/50ND concentric reducer flanged both  ends. 50ND end flanged to suit pump delivery.","No",2]
[null,"E76",null,"PD2 - 500mm long x 80ND (FSM) spool piece, flanged both ends.","No",2]
[null,"E77",null,"PD3 - 80ND M.R.B, flanged both ends.","No",2]
[null,"E78",null,"PD4 - 1000mm long x 80ND (FSM)  spool piece, flanged both ends.","No",2]
[null,"E79",null,"PD5 - 80ND x 60 degree lateral, flanged all ends.","No",1]
[null,"E80",null,"PD6 - 80/50ND Tee piece, flanged all ends.","No",1]
[null,"E81",null,"PD7 - 80ND M.R.B, flanged both ends.","No",1]
[null,"E82",null,"PD8 - 2500mm long x 80ND (FSM) spool piece, flanged both ends.","No",1]
[null,"E83",null,"PD9 - 80ND M.R.B, flanged both ends.","No",1]
[null,"E84",null,"PD10 - Viking Johnson Flange Adaptor to suit 90ND HDPE PE63 Class 10.","No",1]
{"$rows_empty":15}
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"E85",null,"New Clarifier Scum Pumpstation - Line 35"]
[null,"E86",null,"Suction Pipework"]
[null,"E87",null,"PS4 - 80/50ND concentric reducer welded to 1000mm long x 80ND, final site measure (FSM), P.E spool piece. 50ND end flanged to suit pump suction.","No",2]
[null,"E88",null,"PS5 - 80ND, 90 Degree, P.E medium radius bend (MRB), one end welded to 2500mm long  x 80ND (FSM) spool piece, other end welded to PS4","No",2]
[null,"E89",null,"PS6 - 100/80ND bell mouth with 80ND end welded to PS5","No",2]
[null,"E90",null,"Delivery Pipework"]
[null,"E91",null,"PD11 - 80/50ND concentric reducer flanged both  ends. 50ND end flanged to suit pump delivery.","No",2]
[null,"E92",null,"PD12 - 500mm long x 80ND (FSM) spool piece, flanged both ends.","No",2]
[null,"E93",null,"PD13 - 80ND M.R.B, flanged both ends.","No",2]
[null,"E94",null,"PD14 - 1000mm long x 80ND (FSM)  spool piece, flanged both ends.","No",2]
[null,"E95",null,"PD15 - 80ND x 60 degree lateral, flanged all ends.","No",1]
[null,"E96",null,"PD16 - 80/50ND Tee piece, flanged all ends.","No",1]
[null,"E97",null,"PD17 - 80ND M.R.B, flanged both ends.","No",1]
[null,"E98",null,"PD18 - 2500mm long x 80ND (FSM) spool piece, flanged both ends.","No",1]
[null,"E99",null,"PD19 - 80ND M.R.B, flanged both ends.","No",1]
[null,"E100",null,"PD20 - Viking Johnson Flange Adaptor to suit 90ND HDPE PE80 Class 10 pipe.","No",1]
[]
[null,"E101",null,"Exist. Aerobic Reactor to WAS - Line 32"]
[null,"E102",null,"Suction Pipework"]
[null,"E103",null,"PS7 - 100/80ND concentric reducer welded to 1000mm long x 100ND (FSM) P.E spool piece. 80ND end flanged to suit pump suction.","No",2]
[null,"E104",null,"PS8 - 100ND, 90 Degree, P.E medium radius bend, one end welded to 4800mm long  x 100ND (FSM) spool piece, other end welded to PS7","No",2]
[null,"E105",null,"PS9 - 200/100ND bell mouth with 100ND end welded to PS8","No",2]
[null,"E106",null,"Delivery Pipework"]
[null,"E107",null,"PD21 - 125/80ND concentric reducer flanged both  ends. 50ND end flanged to suit pump delivery.","No",2,{"$nulls":4}," "]
[null,"E108",null,"PD22 - 500mm long x 125ND (FSM) spool piece, flanged both ends.","No",2]
[null,"E109",null,"PD23 - 125ND M.R.B, flanged both ends.","No",2]
[null,"E110",null,"PD24 - 1000mm long x 125ND (FSM)  spool piece, flanged both ends.","No",2]
[null,"E111",null,"PD25 - 125ND x 60 degree lateral, flanged all ends.","No",1]
[null,"E112",null,"PD26 - 125/50ND Tee piece, flanged all ends.","No",1]
[null,"E113",null,"PD27 - 125ND M.R.B, flanged both ends.","No",1]
[null,"E114",null,"PD28 - 2500mm long x 125ND (FSM) spool piece, flanged both ends.","No",1]
[null,"E115",null,"PD29 - 125ND M.R.B, flanged both ends.","No",1]
[null,"E116",null,"PD30 - Viking Johnson Flange Adaptor to suit 160ND HDPE PE80 Class 6 pipe.","No",1]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"E117",null,"New Aerobic Reactor to WAS - Line 33"]
[null,"E118",null,"Suction Pipework"]
[null,"E119",null,"PS10 - 100/80ND concentric reducer welded to 1000mm long x 100ND (FSM) P.E spool piece. 80ND end flanged to suit pump suction.","No",2]
[null,"E120",null,"PS11 - 100ND, 90 Degree, P.E medium radius bend, one end welded to 4800mm long  x 100ND (FSM) spool piece, other end welded to PS10","No",2]
[null,"E121",null,"PS12 - 200/100ND bell mouth with 100ND end welded to PS11","No",2]
[null,"E122",null,"Delivery Pipework"]
[null,"E123",null,"PD31 - 125/80ND concentric reducer flanged both  ends. 50ND end flanged to suit pump delivery.","No",2]
[null,"E124",null,"PD32 - 500mm long x 125ND (FSM) spool piece, flanged both ends.","No",2]
[null,"E125",null,"PD33 - 125ND M.R.B, flanged both ends.","No",2]
[null,"E126",null,"PD34 - 1000mm long x 125ND (FSM)  spool piece, flanged both ends.","No",2]
[null,"E127",null,"PD35 - 125ND x 60 degree lateral, flanged all ends.","No",1]
[null,"E128",null,"PD36 - 125/50ND Tee piece, flanged all ends.","No",1]
[null,"E129",null,"PD37 - 125ND M.R.B, flanged both ends.","No",1]
[null,"E130",null,"PD38 - 2500mm long x 125ND (FSM) spool piece, flanged both ends.","No",1]
[null,"E131",null,"PD39 - 125ND M.R.B, flanged both ends.","No",1]
[null,"E132",null,"PD40 - Viking Johnson Flange Adaptor to suit 160ND HDPE PE80 Class 6 pipe.","No",1]
[]
[null,"E133",null,"WAS to Filter Press - Line 27"]
[null,"E134",null,"Suction Pipework"]
[null,"E135",null,"PS13 - 100/80ND concentric reducer welded to 1000mm long x 100ND (FSM) P.E spool piece. 80ND end flanged to suit pump suction.","No",3]
[null,"E136",null,"PS14 - 100ND, 90 Degree, P.E medium radius bend, one end welded to 3300mm long  x 100ND (FSM) spool piece, other end welded to PS13","No",3]
[null,"E137",null,"PS15 - 200/100ND bell mouth with 100ND end welded to PS14","No",3]
[null,"E138",null,"Delivery Pipework"]
[null,"E139",null,"PD41 - 125/80 Concentric reducer, flanged both ends, 80NB end flanged to suit pump delivery flange","No",3]
[null,"E140",null,"PD42 - 125NB, 90 Degree Medium Radius Bends","No",5]
[null,"E141",null,"PD43 - 125NB, Medium Radius Sweep Tees","No",3]
[null,"E142",null,"PD44 - 125NB, 1215 long pipe, flanged both ends","No",2]
[null,"E143",null,"PD45 - 125/80 NB Tee, flanged all ends","No",1]
[null,"E144",null,"PD46 - 125NB pipe, 300mm long, flanged both ends","No",1]
[null,"E145",null,"PD47 - 125NB pipe, 2000mm F/F, Flanged both ends","No",1]
[null,"E146",null,"PD48 - Viking Johnson Flange Adaptor to suit 140OD mPVC, Class 10 pipe","No",1]
[null,"E147",null,"PD49 - Blank flange to suit 125NB steel line flanged to SABS 112-1977 table 1000/3","No",1]
[]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"E148",null,"RAS  to Aerator - Line 28"]
[null,"E149",null,"Suction Pipework"]
[null,"E150",null,"PS16 - 250/200ND concentric reducer welded to 350mm long x 250ND (FSM) P.E spool piece. 200ND end flanged to suit pump suction.","No",3]
[null,"E151",null,"PS17 - 250ND, 90 Degree, P.E medium radius bend, one end welded to 3650mm long  x 250ND (FSM) spool piece, other end welded to PS16","No",3]
[null,"E152",null,"PS18 - 250/350ND bell mouth with 250ND end welded to PS17","No",3]
[null,"E153",null,"Delivery Pipework"]
[null,"E154",null,"PD50 - 250/200ND concentric reducer flanged both  ends. 200ND end flanged to suit pump delivery.","No",3]
[null,"E155",null,"PD51 - 250ND M.R.B, flanged both ends.","No",5]
[null,"E156",null,"PD52 - 250NB, Medium Radius Sweep Tees","No",3]
[null,"E157",null,"PD53 - Blank flange to suit 250NB steel line flanged to SABS 112-1977 table 1000/3","No",1]
[null,"E158",null,"PD54 - 250NB, 780mm long pipe, flanged both ends","No",2]
[null,"E159",null,"PD55 - 250/100 NB Tee, flanged all ends","No",1]
[null,"E160",null,"PD56 - 250NB pipe, 2100mm F/F, Flanged both ends","No",1]
[null,"E161",null,"PD57 - Viking Johnson Flange Adaptor to suit 250ND mPVC, Class 9 pipe","No",1]
[]
[null,"E162",null,"Washwater Return - Line 29"]
[null,"E163",null,"Suction Pipework"]
[null,"E164",null,"PS19 - 100/80ND concentric reducer welded to 1000mm long x 100ND (FSM) P.E spool piece. 80ND end flanged to suit pump suction.","No",2]
[null,"E165",null,"PS20 - 100ND, 90 Degree, P.E medium radius bend, one end welded to 4800mm long  x 100ND (FSM) spool piece, other end welded to PS10","No",2]
[null,"E166",null,"PS21 - 200/100ND bell mouth with 100ND end welded to PS11","No",2]
[null,"E167",null,"Delivery Pipework"]
[null,"E168",null,"PD58 - 125/80ND concentric reducer flanged both  ends. 50ND end flanged to suit pump delivery.","No",2]
[null,"E169",null,"PD59 - 500mm long x 125ND (FSM) spool piece, flanged both ends.","No",2]
[null,"E170",null,"PD60 - 125ND M.R.B, flanged both ends.","No",2]
[null,"E171",null,"PD61 - 1000mm long x 125ND (FSM)  spool piece, flanged both ends.","No",2]
[null,"E172",null,"PD62 - 125ND x 60 degree lateral, flanged all ends.","No",1]
[null,"E173",null,"PD63 - 125/50ND Tee piece, flanged all ends.","No",1]
[null,"E174",null,"PD64 - 125ND M.R.B, flanged both ends.","No",1]
[null,"E175",null,"PD65 - 2500mm long x 125ND (FSM) spool piece, flanged both ends.","No",1]
[null,"E176",null,"PD66 - 125ND M.R.B, flanged both ends.","No",1]
[null,"E177",null,"PD67 - Viking Johnson Flange Adaptor to suit 160ND HDPE PE80 Class 6 pipe.","No",1]
[]
[]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[]
[null,"E178",null,"HDPE type piping shall be to SANS ISO 4427 SDR17 rating (PN 6,3). Compression type couplings and fittings shall be the Plasson type."]
[null,"E179",null,"Municipal Water"]
[null,"E180",null,"32mm OD - HDPE potable water supply pipe","m",200]
[null,"E181",null,"32mm HDPE 90 degree bends.","No",8]
[null,"E182",null,"32mm HDPE T-joints.","No",3]
[null,"E183",null,"Supply and install standpipe linked to municipal water supply.","No",3]
[]
[null,"E184",null,"Water Line to Chlorine Room"]
[null,"E185",null,"25nb galvanised nipple","No",3]
[null,"E186",null,"25nb galvanised elbow","No",2]
[null,"E187",null,"32 x 25nb galvanised reducing bush","No",2]
[null,"E188",null,"32mm Plasson Fitting","No",2]
[null,"E189",null,"32mm HDPE pipe","m",50]
[null,"E190",null,"40nb galvanised nipple","No",1]
[null,"E191",null,"40nb galvanised elbow","No",1]
[null,"E192",null,"50 x 40nb galvanised reducing bush","No",1]
[null,"E193",null,"50nb galvanised nipple","No",1]
[null,"E194",null,"50nb galvanised elbow","No",1]
[null,"E195",null,"50nb socket","No",1]
[]
[null,"E196",null,"Chlorine Dosing Pipe and Return"]
[null,"E197",null,"32mm OD uPVC pipe","m",5]
[null,"E198",null,"40mm OD uPVC Pipe","m",15]
[null,"E199",null,"32mm OD - 90 degree bends","No",2]
[null,"E200",null,"40mm OD - 90 degree bends","No",6]
[null,"E201",null,"Holderbats","No",12]
[]
[null,"E202",null,"Resilient seal valves"]
[null,"E203",null,"Double flanged fully encapulated gate resilient seal waterworks gate valves with clockwise closing non-rising spindles fitted with handwheels"]
[null,"E204",null,"400mm & ","No",1]
[null,"E205",null,"300mm & ","No",1]
[null,"E206",null,"200mm & ","No","RATE ONLY"]
[null,"E207",null,"160mm & ","No",3]
[null,"E208",null,"110mm & ","No",4]
[null,"E209",null,"50mm & ","No",3]
[]
[null,"E210",null,"Viking Johnson flange adaptor couplings to SANS 1123 Table 1600/3  with Denso protection for:"]
[null,"E211",null,"400mm & ","No",2]
[null,"E212",null,"300mm & ","No","RATE ONLY"]
[null,"E213",null,"200mm & ","No",5]
[null,"E214",null,"160mm & ","No","RATE ONLY"]
[null,"E215",null,"110mm & ","No","RATE ONLY"]
[]
[]
[]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"E216",null,"Viking Johnson type stepped coupling for steel to mPVC, working pressure up to 1600kPa with Denso protection"]
[null,"E217",null,"400mm & ","No",2]
[null,"E218",null,"300mm & ","No","RATE ONLY"]
[null,"E219",null,"200mm & ","No","RATE ONLY"]
[null,"E220",null,"160mm & ","No",3]
[null,"E221",null,"110mm & ","No","RATE ONLY"]
[]
[null,"E222",null,"76mm & HDPE Class 6 cable sleeve"]
[null,"E223",null,"Clarifier","m",30]
[]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"F.Structural Steel","index":5,"n_rows":47,"n_cols":9,"rows_kept":47,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"F"," ","SECTION F: STRUCTURAL STEEL"]
[null,"F1","SANS 1200 HA","Supply, fabrication, delivery, storage and erection of Hot Dipped Galvanised structural steelwork to SANS 1431, Grade 300WA complete with all the necessary cleats, brackets, gussets, packers etc. to:"]
[null,"F2",null,"Inlet Structure Canopy"]
[null,"F3",null,"a) Hot rolled column H sections at 23Kg/m","t",0.5]
[null,"F4",null,"b) Hot rolled I-sections at 31Kg/m","t",1.1]
[null,"F5",null,"b) Hot rolled I-sections at 41Kg/m","t",0.5]
[null,"F6",null,"c) Cold formed PFC purlins at 16Kg/m","t",{"v":1,"d":"1.0"}]
[null,"F7",null,"d) Base plates and sundry steelwork","t",0.3]
[null,"F8",null,"e) Hot rolled UB 356 x 171 x 45","t",0.5]
[]
[null,"F9",null,"Chlorine Room "]
[null,"F10",null,"a) Hot rolled column H sections at 46Kg/m","t",0.4]
[null,"F11",null,"b) Hot rolled I-sections at 45Kg/m","t",0.5]
[null,"F12",null,"d) Sundry steelwork","t",0.3]
[]
[null,"F13",null,"Blower Room "]
[null,"F14",null,"a) Hot rolled I-sections at 41Kg/m","t",{"v":1,"d":"1.0"}]
[null,"F15",null,"b) Sundry steelwork","t",0.3]
[]
[null,"F16",null,"STAIRCASES"]
[null,"F17",null,"Hot rolled PFC channels 200 x 75mm @ 24Kg/m","t",0.6]
[null,"F24",null,"800mm Wide H.D.G staircase with 300mm treads forming risers of 175mm as per drawing ?????"]
[null,"F25",null,"H.D.G 35 Degree, side mounted Stanchions ","No",8]
[null,"F26",null,"H.D.G, Vertical, side mounted stanchions","No",5]
[]
[null,"F27",null,"MISCELLANEOUS"]
[null,"F28",null,"Angle 60x60x6 with 300mm long lugs at 300mm crs","m",5]
[null,"F29",null,"Channel 120x55","m",7]
[null,"F30",null,"Flat bar 20x4.5","m",4]
[null,"F31",null,"Vastrap 4.5mm","m²",30]
[]
[null,"F32",null,"RAILS"]
[null,"F33",null,"Supply, deliver and cast in rails @ 40Kg/m for bin removal"]
[null,"F34",null,"Inlet Works","t",1.8]
[]
[null,"F35",null,"Supply, deliver and install M20 HD Bolts each supplied with one washer and two nuts, 400mm long with 75 x 75mm base plate welded to plain end"]
[null,"F36",null,"Inlet Works Canopy","No.",16]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"G.Mechanical","index":6,"n_rows":200,"n_cols":9,"rows_kept":200,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"G",null,"SECTION G: MECHANICAL "]
[null,"G1",null,"INLET WORKS"]
[null,"G2","PSXA","Supply & install Stainless steel mechanical screen with 3mm spacing's (Huber - Ro2 ROTAMAT Wedge Wire Screen OR similar approved) for approx.1200mm channel width x 800 mm channel depth, wired for local start / stop / reverse, with all necessary drives, cabling, fittings and fixings, driven by a 1.1kW drive unit","No",2]
[null,"G3","PSXE","Supply & install stainless steel, handwheel operated sluice gates, 1200mm (W) x 1800mm (D) to fit flush with channel wall (SAME or similar approved ), with all necessary fittings ","No",4]
[null,"G4",null,"Supply & install stainless steel, handwheel operated sluice gates, 900mm (W) x 1800mm (D), surface mounted (SAME or similar approved ), with all necessary fittings for inlet distribution box","No",2]
[null,"G5","PSXE","Supply & install stainless steel, handwheel operated sluice gates, 750mm (W) x 1800mm (D) to fit flush with channel wall (SAME or similar approved ), with all necessary fittings ","No",2]
[null,"G6",null,"Supply & install manual fine bar-screen, 15 mm spacing, MS galvanised, to fit approximate channel dimensions 2000mm(W) x 600mm(D), including purpose made hand rake, with all necessary fittings and fixtures ","No",1]
[null,"G7",null,"Supply & install manual coarse bar-screen, 100mm apertures, MS galvanised, to fit approximate channel dimensions 2600mm(W) x 18600mm(D), including purpose made hand rake, with all necessary fittings and fixtures ","No",1]
[null,"G8","PSXC","Supply and install Grit Classifier (Huber Coanda RoSF3e or similar approved) Stainless steel, with all necessary, drives, pipework, cabling and fittings for a fully functional system.","No",1]
[null,"G9","PSXB","Supply & install grit removal system for an ADWF of 18Ml/d (Huber Rotamat - Vormax Size 5 or similar approved). Grit removal system to be complete with all drives, airlift and all necessary pipework, cabling and fittings for a fully operational system.","No",1]
[null,"G10","PSXF","Supply, deliver, install and commission filter scrubber system for the inlet works. The rate to include filter media, pre-filters, extraction fans, exhaust stacks, valves, fittings and all ancillaries for a fully operational system","No",1]
[null,"G11",null,"Supply and fit 9 000mm length mechanical screenings conveyor, with all necessary piping, pipe specials, cabling and fittings.","No",1]
[null,"G12",null,"Supply and fit 5 000mm length grit screenings conveyor, with all necessary piping, pipe specials, cabling and fittings.","No",1]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G13",null,"New Aerator Basin"]
[null,"G14","PSXG","Supply and install Tilting Weir to fit an opening of 4500mm (W) x 1000mm (H) (Fulton or similar approved), including all end sealing plates, seals, support brackets, Fasteners and anchor bolts","No",2]
[null,"G15","PSXH","Supply, deliver and install fine bubble EPDM membrane disc diffuser aeration system type ABS, model 2940 PIK300 (or similar approved) including all non return ball valves, diffuser elements, connection sleeves, mounting brackets and all ancillaries for a fully operational system to suit an oxidation tank of 38x38m with an operating depth of 4.75m","No",2]
[null,"G16","PSXI","Supply, deliver and install centrifugal compressors (2 operational + 1 standby for aeration to both oxidation tanks), type ABS, model HST-Integral S9000-1-H (or similar approved), for a total average air flow requirement of 12180 Nm3/h, including all drives, guards, converters, master control units, backflow barriers and silencers and all ancillaries for a fully operational system","No",3]
[]
[null,"G22",null,"Clarifier"]
[null,"G23","PSXK","Supply, deliver and fit fixed bridge centre drive mechanicals (Bonfiglioli) for 28m internal diameter clarifier (Hallmark Echelon, or similar approved), including all motors, drives, sludge and scum collection, weirs, weir plates and scum baffle plates, handrailing and rectagrid walkway and all ancillaries for a fully operational system. All collection systems, weirs, weir and baffle plates, handrailing and rectagrid to be manufactured from Stainless Steel 304","No",1]
[null,"G24",null,"Supply & install stainless steel, handwheel operated sluice gates, 900mm (W) x 1800mm (D), surface mounted (SAME or similar approved ), with all necessary fittings for Clarifier distribution box","No",3]
[]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G25",null,"Filter Press Plant"]
[null,"G26",null,"Sludge Thickening and Dewatering Plant and Equipment"]
[null,"G27","PSXL","Supply, deliver, store, install and commission filter press plant (INENZO Supply or similar approved). Rate to include all necessary pipework, valves, electrical and instrumentation requirements, craneage, double handling and all sundries for a fully operational plant, for a flow rate of 85m3/hr and an operating frequency of 8 hrs/day."]
[null,"G28",null,"Design and Submission of drawings","Sum",1]
[null,"G29",null,"Setting out of works and checking feed pipework at battery limit ","Sum",1]
[null,"G30","PSXL","Belt thickener gravity table GTN 1600 (or similar approved) including feeding box, washing systems, belt tracking and tensioning systems, collection trays, scrapers and all requirements for a fully operational system.","No",2]
[null,"G31","PSXL","Belt Press BPF 1600 Bravo CMF (or similar approved) including washing systems, pressure, guide and tensioning rolls, belt tracking and tensioning systems, collection trays, scrapers and all requirements for a fully operational system.","No",2]
[null,"G32",null,"Supply and fit mechanicals for 9000mm H.D.G belt-press cake sludge conveyor, with all necessary piping, pipe specials, cabling and fittings for a fully operational system.","No",2]
[null,"G33",null,"Supply and fit mechanicals for 8000mm H.D.G screw conveyor, with all necessary piping, pipe specials, cabling and fittings for a fully operational system.","No",2]
[null,"G34",null,"Supply, deliver, store and install complete stairs, walkway and platform system. Rate to include all fixings and sundries and all requirements to comply with the relevant Health and Safety regulations, for a fully operational system.","Sum",1]
[]
[null,"G35",null,"Extra Over items G30 To G34 For double handling"," "]
[null,"G36",null,"Item G30","Sum",1]
[null,"G37",null,"Item G31","Sum",1]
[null,"G38",null,"Item G32","Sum",1]
[null,"G39",null,"Item G33","Sum",1]
[null,"G40",null,"Item G34","Sum",1]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G41",null,"Supply, deliver, store, install and commission Polyelectrolyte Dosing System (INENZO Supply or similar approved) including backup pump, valving and piping. Rate to include all necessary pipework, valves, double handling and all sundries for a fully operational system."]
[null,"G42",null,"Design and Submission of drawings","Sum",1]
[null,"G43",null,"Setting out of works and checking feed pipework at battery limit ","Sum",1]
[null,"G44",null,"Solution Dosing pumpset and ancillaries","No",1]
[null,"G45",null,"Make up water pipework, solution pipework, valves, supports and ancillaries","Sum",1]
[]
[null,"G46",null,"Extra-over Items G44 To G45 For double handling."]
[null,"G47",null,"Item G44","Sum",1]
[null,"G48",null,"Item G45","Sum",1]
[]
[null,"G49",null,"Supply, deliver, store, install and commission Sludge Feed and Distribution System (INENZO Supply or similar approved). Rate to include all necessary pipework, valves, supports, fittings and all ancillaries for a fully operational system."]
[null,"G50",null,"Design and Submission of drawings","Sum",1]
[null,"G51",null,"Setting out of works and checking feed pipework at battery limit ","Sum",1]
[null,"G52",null,"Sludge feed pipework within the battery limit of the filter press building","Sum",1]
[]
[null,"G53",null,"Extra-over Items G52 For double handling."]
[null,"G54",null,"Item G52","Sum",1]
[]
[null,"G55",null,"Supply, deliver, store, install and commission Washwater Piping and ancillaries (INENZO Supply or similar approved). Rate to include all necessary pipework, valves, solenoid valves, strainers, supports, fittings and all ancillaries for a fully operational system."]
[null,"G56",null,"Design and Submission of drawings","Sum",1]
[null,"G57",null,"Setting out of works and checking feed pipework at battery limit ","Sum",1]
[null,"G58",null,"Washwater Piping and ancillaries","Sum",1]
[]
[null,"G59",null,"Extra-over Item G58 For double handling."]
[null,"G60",null,"Washwater Piping and ancillaries","Sum",1]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G61",null,"Supply, deliver, store, install and commission Ventilation System and ancillaries (INENZO Supply or similar approved). Rate to include all necessary pipework, valves, filters, supports, fittings and all ancillaries for a fully operational system."]
[null,"G62",null,"Design and Submission of drawings","Sum",1]
[null,"G63",null,"Setting out of works and checking feed pipework at battery limit ","Sum",1]
[null,"G64",null,"Axial Flow Exhaust Fan","No",1]
[null,"G65",null,"Ducting, supports, dampers and ancillary equipment","Sum",1]
[]
[null,"G66",null,"Extra-over Items G64 To G65 For double handling."]
[null,"G67",null,"Axial Flow Exhaust Fan","Sum",1]
[null,"G68",null,"Ducting, supports, dampers and ancillary equipment","Sum",1]
[]
[null,"G69",null,"Sundries"]
[null,"G70",null,"Factory inspections of equipment","Sum",1]
[null,"G71",null,"Provision of A1 \"as built\" drawings configured for AUTOCAD including one CD with all relevant drawings attached","Sum",1]
[null,"G72",null,"Provision of one hardcopy of the operation and maintenance manuals including an electronic copy thereof.","Sum",1]
[]
[null,"G73",null,"Supply and deliver to site, install and commission in accordance with the supplier's / manufacturer's requirements slow speed mixers for solids suspension for a required thrust of 980N and a propeller speed of between 25 - 45 rpm. The rate to include all drives, shafts, guards, cabling and all fittings and fixtures for a fully operational system for:"]
[null,"G74",null,"WAS Sump","No",3]
[]
[null,"G75",null,"PUMPS"]
[null,"G76","PSXM","Supply and deliver to site, install and commission in accordance with the supplier's / manufacturer's requirements Surface mounted Gorman Rupp self-priming centrifugal type pumps, Model Super T2A3S-BFM vee belt driven, driven by 2.2Kw/4P/3PH/525V/IP55 electric motors, with a pumping capacity of 4l/s, a forward velocity of 1m/s, turning at 1550 r/min. The rate to include a common folded mild steel galvanized baseplate complete with vee belts, pulleys, guards and air release valves supplied loose for:"]
[null,"G77",null,"Scum Sump (1 operational + 1 Standby)","No",3]
[{"$nulls":5},6]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G78",null,"Supply and deliver to site, install and commission in accordance with the supplier's / manufacturer's requirements Surface mounted Gorman Rupp self-priming centrifugal type pumps, Model Super T2A3S-BFM vee belt driven, driven by 2.2Kw/4P/3PH/525V/IP55 electric motors, with a pumping capacity of 4l/s, a forward velocity of 1m/s, turning at 1380 r/min. The rate to include a common folded mild steel galvanized baseplate complete with vee belts, pulleys, guards and air release valves supplied loose for:"]
[null,"G79",null,"New Clarifier Scum Sump (1 Opper. + 1 Standby)","No",6]
[]
[null,"G80","PSXN","Supply and deliver to site, install and commission in accordance with the supplier's / manufacturer's requirements Surface mounted Gorman Rupp self-priming centrifugal type pumps, Model Super T3A3S-BFM vee belt driven, driven by 7.5Kw/4P/3PH/525V/IP55 electric motors, with a pumping capacity of 16.7l/s each, a forward velocity of 1.4m/s, turning at 1430 r/min. The rate to include a common folded mild steel galvanized baseplate complete with vee belts, pulleys, guards and air release valves supplied loose for:"]
[null,"G82",null,"New Aerator to WAS (1 Operat. + 1 Standby)","No",6]
[null,"G83",null,"Washwater Return (1 Operat. + 1 Standby)","No",6]
[]
[null,"G84",null,"Supply and deliver to site, install and commission in accordance with the supplier's / manufacturer's requirements Surface mounted Gorman Rupp self-priming centrifugal type pumps, Model Super T3A3S-BFM vee belt driven, driven by 3.0Kw/4P/3PH/525V/IP55 electric motors, with a pumping capacity of 13.9l/s each, a forward velocity of 1.14m/s, turning at 1040 r/min. The rate to include a common folded mild steel galvanized baseplate complete with vee belts, pulleys, guards and air release valves supplied loose for:"]
[null,"G85",null,"WAS to Filter Press (2 Opper. + 1 Standby)","No",6]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G86","PSXO","Supply and deliver to site, install and commission in accordance with the supplier's / manufacturer's requirements Surface mounted Gorman Rupp self-priming centrifugal type pumps, Model Super T8A3S-BFM vee belt driven, driven by 15.0Kw/4P/3PH/525V/IP55 electric motors, with a pumping capacity of 83.3l/s each, a forward velocity of 1.7m/s, turning at 790 r/min. The rate to include a common folded mild steel galvanized baseplate complete with vee belts, pulleys, guards and air release valves supplied loose for:"]
[null,"G87",null,"RAS to Aerator (2 Opper. + 1 Standby)","No",9]
[]
[null,"G88",null,"PUMPSTATIONS"]
[null,"G89",null,"Clarifier Scum - Line "]
[null,"G90",null,"80ND PN10 Single door Non Return Valve to SANS 144, S.G. Iron body, cover and door, cast iron hinge, 304 stainless steel hinge pin, double flanged with epoxy paint coating to 250 micron minimum.","No",6]
[null,"G91",null,"80ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",6]
[null,"G92",null,"50ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",3]
[null,"G93","PSXP","50ND PN10 ARV/Vacuum breaker, Stainless Steel AISI 304, double orifice, flanged studded inlet to SANS 1123 - Table 1000/3 (Ventomat RGX or similar approved)","No",3]
[]
[null,"G94",null,"New Clarifier Scum Sump - Line 35"]
[null,"G95",null,"80ND PN10 Single door Non Return Valve to SANS 144, S.G. Iron body, cover and door, cast iron hinge, 304 stainless steel hinge pin, double flanged with epoxy paint coating to 250 micron minimum.","No",6]
[null,"G96",null,"80ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",6]
[null,"G97",null,"50ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",3]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G98","PSXP","50ND PN10 ARV/Vacuum breaker, Stainless Steel AISI 304, double orifice, flanged studded inlet to SANS 1123 - Table 1000/3 (Ventomat RGX or similar approved)","No",3]
[]
[null,"G104",null,"New Aerator to WAS - Line 12"]
[null,"G105",null,"125ND PN10 Single door Non Return Valve to SANS 144, S.G. Iron body, cover and door, cast iron hinge, 304 stainless steel hinge pin, double flanged with epoxy paint coating to 250 micron minimum.","No",6]
[null,"G106",null,"125ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",6]
[null,"G107",null,"50ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",3]
[null,"G108","PSXP","50ND PN10 ARV/Vacuum breaker, Stainless Steel AISI 304, double orifice, flanged studded inlet to SANS 1123 - Table 1000/3 (Ventomat RGX or similar approved)","No",3]
[]
[null,"G109",null,"WAS to Filter Press - Line 27"]
[null,"G110",null,"125ND PN10 Single door Non Return Valve to SANS 144, S.G. Iron body, cover and door, cast iron hinge, 304 stainless steel hinge pin, double flanged with epoxy paint coating to 250 micron minimum.","No",9]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G111",null,"125ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",9]
[null,"G112",null,"50ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",3]
[null,"G113","PSXP","50ND PN10 ARV/Vacuum breaker, Stainless Steel AISI 304, double orifice, flanged studded inlet to SANS 1123 - Table 1000/3 (Ventomat RGX or similar approved)","No",3]
[]
[null,"G114",null,"RAS to Aerator - Line 11"]
[null,"G115",null,"250ND PN10 Single door Non Return Valve to SANS 144, S.G. Iron body, cover and door, cast iron hinge, 304 stainless steel hinge pin, double flanged with epoxy paint coating to 250 micron minimum.","No",9]
[null,"G116",null,"250ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",9]
[null,"G117",null,"100ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",3]
[null,"G118","PSXP","100ND PN10 ARV/Vacuum breaker, Stainless Steel AISI 304, double orifice, flanged studded inlet to SANS 1123 - Table 1000/3 (Ventomat RGX or similar approved)","No",3]
[]
[null,"G119",null,"Washwater Return - Line 29"]
[null,"G120",null,"125ND PN10 Single door Non Return Valve to SANS 144, S.G. Iron body, cover and door, cast iron hinge, 304 stainless steel hinge pin, double flanged with epoxy paint coating to 250 micron minimum.","No",6]
[null,"G121",null,"125ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",6]
[null,"G122",null,"50ND PN10 RSV gate valve, clockwise closing, non rising spindle, handwheel operated, S.G. Iron body and bonnet, fusion bonded epoxy coating internally and externally to minimum dry film thickness of 250micron to SANS 664","No",3]
[null,"G123",null,"50ND PN10 ARV/Vacuum breaker, Stainless Steel AISI 304, double orifice, flanged studded inlet to SANS 1123 - Table 1000/3 (Ventomat RGX or similar approved)","No",3]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"G124",null,"MISCELLANEOUS"]
[null,"G125",null,"Supply and deliver 5m3 skip on rollers for the removal of grit to specified site.","No",6]
[]
[null,"G126",null,"Manual chain hoist for a 2T lifting capacity"]
[null,"G127",null,"Chlorine Room Crawl Beam","No",1]
[]
[null,"G128",null,"Manual chain hoist for a 3T lifting capacity"]
[null,"G129",null,"Blower room crawl beam","No",1]
[]
[]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"H.Instrumentation","index":7,"n_rows":86,"n_cols":9,"rows_kept":86,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"H",null,"SECTION H: INSTRUMENTATION"]
[null,"H1",null,"FLOW METERS"]
[null,"H2","PSXD","Supply, deliver, install and calibrate flow meters as per the suppliers recommended installation method, complete with local indication and future transmission of data to an office located PLC/VDU."," "," "]
[null,"H3",null,"Feed lines to Aerators"," "," "]
[null,"H4",null,"Flow meter (Endress & Hauser or similar approved) for:","No",6]
[null,"H5",null,"Pipe Diameter -                    500ND"]
[null,"H6",null,"Pipe Material -                     Concrete"]
[null,"H7",null,"Flow Type -                         Gravity"]
[null,"H8",null,"Flow Rate -                          730 l/s (PWWF)"]
[null,"H9",null,"Pressure Rating -                SANS 1123 - 1000/3"]
[null,"H10",null,"Siting -                               Chamber below "]
[null,"H11",null,"Voltage Requirements -        240V"]
[null,"H12",null,"PLC / SCADA Link -             YES"]
[]
[null,"H13",null,"Supply, deliver, install and calibrate flow meters as per the suppliers recommended installation method, complete with local indication and future transmission of data to an office located PLC/VDU. The flow meter must be capable of being programmed to measure a predetermined flow upon which it will send a signal to the pump to switch off."]
[null,"H14",null,"Aerator to WAS"]
[null,"H15",null,"Flow meter (Endress & Hauser or similar approved) for:","No",6]
[null,"H16",null,"Pipe Diameter -                    125NB"]
[null,"H17",null,"Pipe Material -                     Steel, Epoxy Lined"]
[null,"H18",null,"Flow Type -                         Pumped"]
[null,"H19",null,"Flow Rate -                          20 l/s (PWWF)"]
[null,"H20",null,"Pressure Rating -                SANS 1123 - 1600/3"]
[null,"H21",null,"Siting -                               Above ground "]
[null,"H22",null,"Voltage Requirements -        240V"]
[null,"H23",null,"PLC / SCADA Link -             YES"]
[]
[null,"H24",null,"Supply, deliver, install and calibrate flow meters as per the suppliers recommended installation method, complete with local indication."]
[null,"H25",null,"Feed lines to Clarifiers"]
[null,"H26",null,"Flow meter (Endress & Hauser or similar approved) for","No",3]
[null,"H27",null,"Pipe Diameter -                    600ND"]
[null,"H28",null,"Pipe Material -                     Concrete"]
[null,"H29",null,"Flow Type -                         Gravity"]
[null,"H30",null,"Flow Rate -                         140 l/s (PWWF)"]
[null,"H31",null,"Pressure Rating -                SANS 1123 - 1000/3"]
[null,"H32",null,"Siting -                               Chamber below "]
[null,"H33",null,"Voltage Requirements -        240V"]
[null,"H34",null,"PLC / SCADA Link -             No"]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"H35",null,"Supply, deliver, install and calibrate flow meter as per the suppliers recommended installation method, complete with local indication and future transmission of data to an office located PLC/VDU."]
[null,"H36",null,"Final Effluent Discharge meter"]
[null,"H37",null,"Flow meter (Endress & Hauser or similar approved) for","No",2]
[null,"H38",null,"Pipe Diameter -              600ND"]
[null,"H39",null,"Pipe Material -               Concrete"]
[null,"H40",null,"Flow Type -                   Gravity"]
[null,"H41",null,"Flow Rate -                    730 l/s (PWWF)"]
[null,"H42",null,"Pressure Rating -           SANS 1123 - 1000/3"]
[null,"H43",null,"Siting -                          Chamber below ground"]
[null,"H44",null,"Voltage Requirements -   240V"]
[null,"H45",null,"PLC / SCADA Link -       Yes"]
[]
[null,"H46",null,"Supply, deliver, install and calibrate ultrasonic level controllers (Endress & Hauser or similar approved) as per the suppliers recommended installation method."]
[null,"H47",null,"Scum return to WAS","No",6]
[null,"H48",null,"WAS feed to Filter Press","No",3]
[null,"H49",null,"Return Activated Sludge to Aerator","No",3]
[]
[null,"H50",null,"Supply, deliver and install Disolved Oxygen meters. Royce Technologies or similar approved"]
[null,"H51",null,"New Aerator Basin","No",6]
[]
[null,"H52",null,"Supply, deliver and install Mixed Liquor Suspended Solids (MLSS) meters. Royce Technologies or similar approved"]
[null,"H53",null,"New Aerator Basin","No",2]
{"$rows_empty":11}
[{"$nulls":3}," "]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]
[{"$nulls":3}," "]

{"sheet":"I.Miscellaneous","index":8,"n_rows":62,"n_cols":9,"rows_kept":62,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"I",null,"SECTION I: MISCELLANEOUS"]
[null,"I1",null,"Supply, Deliver and apply two coats Bituminous paint to surfaces to act as a slip joint to:"]
[null,"I2"," ","Bioreactors","m²",1885]
[null,"I3",null,"Clarifier","m²",2]
[]
[null,"I4",null,"Drainage"]
[null,"I5",null,"19mm Stone to Clarifier Cordrain","m³",5]
[null,"I6",null,"U14 Biddum surround to Clarifier Cordrain","m²",46]
[]
[]
[null,"I9",null,"ODOUR CONTROL"]
[null,"I10",null,"Supply, deliver and fit Glassfibre Reinforced Polyester Sheeting \"Everite - Longspan B\" or similar approved, with a nominal mass of 2.4kg/m2 and of a clear colour permitting a light translucency of 85%. Rate to include for all drilling, fixing bolts, polyethylene soft washers with a steel cup washer backer, and spacers. All fixings to be stainless steel to:"]
[null,"I11",null,"Inlet Works","m²",120]
[]
[null,"I12",null,"Supply, deliver and install profiled filler panels along corrugated edges of sheeting for odour entrapment, to:"]
[null,"I13",null,"Inlet Works","m",80]
[]
[null,"I14",null,"250 Micron Polyethylene sheet to underside of floor slabs to:"]
[null,"I15",null,"Blower Room","m²",57]
[null,"I16",null,"Chlorine Room","m²",28]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"I19",null,"Two layers DPC placed on top of brickwork prior to casting concrete roof to form slip joint"]
[null,"I20",null,"Blower Room","m",35]
[null,"I21",null,"Chlorine Room","m",30]
[null,"I23",null,"Control Room","m",31]
[]
[null,"I24",null,"Supply, deliver and apply 4mm TORCHON water proofing membrane (EX ABE) to roof slabs:"]
[null,"I25",null,"Blower Room","m²",83]
[null,"I26",null,"Chlorine Room","m²",47]
[null,"I28",null,"Control Room","m²",64]
[]
[null,"I30",null,"Signage"]
[]
[null,"I31",null,"Supply and erect safety signage and name boards at motors and buildings. Signage to comply with clients specifications","Prov. Sum",1,null,{"v":10000,"d":"10,000"}]
[]
[null,"I32",null,"Health and Safety"]
[null,"I33",null,"Supply, deliver and install emergency eye wash and shower unit, linked to municipal water supply.","No",1]
[null,"I34",null,"Life rings and ropes","No",5]
[null,"I35",null,"Chlorine mask and filter","No",1]
[null,"I36",null,"Chlorine mask housing","No",1]
[]
[]
[null,"I40",null,"Supply, deliver and erect JOJO water tank for potable water storage, 5500l capacity x 1800mm diameter x 2300mm high. "]
[null,"I42",null,"Chlorine Contact Tank","No",1]
[]
[null,"I43",null,"Extra Over item I39 for erection at heights"]
[null,"I44",null,"1 to 2m","No","RATE ONLY"]
[null,"I45",null,"2 to 3m","No",1]
[null,"I46",null,"3m and over","No",1]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"J.Building","index":9,"n_rows":227,"n_cols":9,"rows_kept":227,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[null,null," "]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"J",null,"SECTION J: BUILDING  WORKS"]
[null,"J1",null,"Clear and grub Site"]
[null,"J2",null,"Chlorine Room","m²",70]
[null,"J3",null,"Blower Room","m²",120]
[]
[]
[]
[null,"J6",null,"Remove and grub all trees and tree stumps regardless of girth:"]
[null,"J7",null,"Chlorine Room","No",2]
[null,"J8",null,"Blower Room","No",3]
[]
[]
[]
[null,"J11",null,"Strip and remove topsoil to nominal depth of 150mm and stockpile for later re-use as directed by the engineer"]
[null,"J12",null,"Chlorine Room","m²",70]
[null,"J13",null,"Blower Room","m²",120]
[]
[]
[null,"J18",null,"Restricted excavation in all materials for strip footings cast against sides of excavation and compact insitu material to 95% ModAASHTO to:"]
[null,"J19",null,"Chlorine Room","m³",13]
[null,"J20",null,"Blower Room","m³",12]
[]
[]
[]
[null,"J23",null,"Restricted excavation in all materials for footings and bases and compact insitu material to 95% ModAASHTO to:"]
[]
[null,"J25",null,"Drain Sumps","m³",4]
[]
[]
[null,"J27",null,"FORMWORK"]
[null,"J28",null,"Smooth Formwork, including cutting, small angle fillets not exceeding 20mm x 20mm etc., to produce a smooth finish as from a new steel shutter including filling imperfections with cement grout and rubbing down excrescences, etc., to:"]
[null,"J29",null,"Sides of walls including forming openings as detailed on the drawings to"]
[null,"J30",null,"Dewatering Plant"]
[null,"J31",null,"Bases and Plinths","m²",44]
[null,"J32",null,"Drainage Sumps","m²",12]
[null,"J33",null,"Dewatering Plant Bases / plinths","m³",10]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[]
[null,"J34",null,"Smooth horizontal formwork to soffits of suspended slabs:"," "," "]
[null,"J35",null,"Blower Room","m²",85]
[null,"J36",null,"Chlorine Room","m²",48]
[]
[null,"J40",null,"Smooth formwork to sides of roof slabs up to and including 300mm"]
[null,"J41",null,"Blower Room","m",30]
[null,"J43",null,"Control Room","m",10]
[]
[null,"J45",null,"Smooth formwork to sides of apron slabs up to and including 150mm"]
[null,"J46",null,"Blower Room","m",45]
[]
[null,"J48",null,"Smooth vertical formwork to sides of columns and beams"]
[null,"J49",null,"Blower Room","m²",22]
[null,"J50",null,"Chlorine Room","m²",6]
[]
[null,"J51",null,"REINFORCEMENT"]
[null,"J52",null,"HIGH-TENSILE STEEL BARS:"]
[null,"J53",null,"Chlorine room ","t",1.5]
[null,"J58",null,"Control Room","t",2]
[]
[null,"J60",null,"High-tensile welded mesh reinforcement in standard sheet sizes (6.0 m x 2.4 m)"]
[null,"J61",null,"Chlorine room","t",0.3]
[null,"J64",null,"Blower Room","t",0.5]
[]
[null,"J65",null,"CONCRETE WORK"]
[null,"J66",null,"Blinding layer in 15MPa / 19mm concrete to:"," "," "]
[null,"J67",null,"Chlorine Room","m²",28]
[null,"J68",null,"Blower Room","m²",57]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"J72",null,"Strength concrete grade 20MPa/19mm (with 30% PFA) cast against sides of excavations for Strip footings to:"," "," "]
[null,"J73",null,"Chlorine Room","m³",5]
[null,"J74",null,"Blower Room","m³",6]
[]
[]
[]
[null,"J77",null,"Strength concrete grade 30MPa/19mm (with 30% PFA) to bases"]
[]
[null,"J79",null,"Drainage Sumps","m³",6]
[]
[]
[null,"J81",null,"Strength concrete grade 30MPa/19mm (with 30% PFA) for columns to:"]
[null,"J82",null,"Blower Room","m³",2]
[null,"J83",null,"Chlorine Room","m³",1]
[]
[null,"J84",null,"Strength concrete grade 30MPa/19mm (with 30% PFA) for beams to:"]
[null,"J85",null,"Blower Room","m³",1]
[null,"J86",null,"Chlorine Room","m³",1]
[]
[null,"J87",null,"Strength concrete grade 30MPa / 19mm (with 30% PFA) to floor slabs"]
[null,"J88",null,"Chlorine Room","m³",4]
[null,"J89",null,"Blower Room","m³",9]
[]
[]
[]
[null,"J92",null,"Strength concrete grade 30MPa / 19mm (with 30% PFA) to apron slabs to:"]
[null,"J93",null,"Blower Room","m³",3]
[]
[null,"J94",null,"Strength concrete grade 30MPa / 19mm (with 30% PFA) to roof slabs"]
[null,"J95",null,"Chlorine Room","m³",8]
[null,"J96",null,"Blower Room","m³",21]
[null,"J98",null,"Control Room","m³",17]
[]
[]
[null,"J100",null,"Screed 2:1 (Sand:Cement) ratio, average thickness 10mm, placed on existing concrete floors for levelling."]
[null,"J101",null,"Guard House","m²",42]
[]
[null,"J102",null,"Slushing to underside of suspended slabs to accept plaster"]
[null,"J103",null,"Blower Room","m²",85]
[null,"J104",null,"Chlorine Room","m²",48]
[null,"J106",null,"Control Room","m²",64]
[]
[]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"J108",null,"Wood float finish to top surface of slabs to:"]
[null,"J109",null,"Chlorine Room","m²",75]
[null,"J110",null,"Blower Room","m²",180]
[null,"J113",null,"Control Room","m²",64]
[]
[null,"J117",null,"BRICKWORK/BUILDING WORK"]
[null,"J118",null,"110mm wide brickwork to internal walls - Both faces plastered to:"]
[null,"J119",null,"Guard House","m²",15]
[null,"J120",null,"Control Room","m²",11]
[]
[null,"J121",null,"230mm wide brickwork - Both skins plastered to:"]
[null,"J122",null,"New Chlorine Contact Tank","m²",191]
[null,"J124",null,"Chlorine Room","m²",18]
[]
[null,"J128",null,"Cavity Walls"]
[null,"J129",null,"Construct cavity wall in stretcher bond with 50mm cavity between the faces, external skin face brick, internal skin stock, plastered and painted. Rate to include plastic wall ties at 1000mm c/c every fourth course, all pointing and nosing and 10MPa mortar."]
[null,"J131",null,"Blower Room","m²",152]
[null,"J132",null,"Chlorine Room","m²",110]
[null,"J133",null,"Control Room","m²",77]
[]
[null,"J138",null,"Plaster to underside of roof slabs to:"]
[null,"J139",null,"Blower Room","m²",85]
[null,"J140",null,"Chlorine Room","m²",48]
[null,"J141",null,"Guard House","m²",17]
[null,"J142",null,"Control Room","m²",64]
[]
[null,"J143",null,"Formation of 15mm half round drip channel along roof slab edges"]
[null,"J144",null,"Chlorine Room","m",30]
[null,"J145",null,"Blower Room","m",39]
[]
[null,"J148",null,"Isolation joints complete with 100 x 12mm Flexcell jointex filler (or similar approved) including polyurethane joint sealer: : "]
[null,"J149",null,"Dewatering Plant","m",370]
[]
[null,"J150",null,"25 x 5mm Saw cut joints complete with polyurethane joint sealer to : "]
[null,"J151",null,"Dewatering Plant","m",82]
[]
[null,"J152",null,"Supply, deliver and install IBR profiled polycarbonate sheeting with a 37mm profile depth, spanning 900mm,  including siscilation (Colour to be determined by Client). Rate to include all fixings and sundries for a fully installed system."]
[null,"J153",null,"Dewatering Plant roof sheeting","m²",315]
[null,"J154",null,"Dewatering Plant side cladding","m²",130]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[]
[null,"J163",null,"Supply and install:"]
[null,"J164",null,"125 x 100 x 0.8mm thick Galvanised sheet iron eaves gutter fixed with 40 x 5mm metal brackets"," "," "]
[null,"J165",null,"Blower Room","m",27]
[]
[null,"J168",null,"76mm Diameter galvanised sheet iron rainwater downpipe secured with holderbats to brickwork."," "," "]
[null,"J169",null,"Blower Room","m",15]
[]
[null,"J172",null,"Supply, deliver and install window type SS53 . Rate to include all fittings and glazing."," "," "]
[null,"J173",null,"Control Room","No",9]
[]
[null,"J174",null,"Supply, deliver and install windows Non open type, size 2000 x 600mm. Rate to include all fittings and glazing."]
[null,"J175",null,"Chlorine Room","No",2]
[null,"J176",null,"Blower Room","No",4]
[]
[null,"J177",null,"Supply, deliver and install windows type NG1, size 533 x 359mm. Rate to include all fittings and frosted glazing."]
[]
[null,"J179",null,"Control Room","No",1]
[]
[null,"J182",null,"Supply, deliver and install WC complete with cistern, seat, covers and fittings."]
[null,"J184",null,"Control Room","No",1]
[]
[null,"J185",null,"Supply, deliver and install wash hand basin complete with fittings."]
[]
[null,"J187",null,"Control Room","No",1]
[]
[null,"J190",null,"Precast concrete lintels above all openings and extending 230mm beyond openings on both sides"," "," "]
[null,"J191",null,"Chlorine Room","m",15]
[null,"J192",null,"Blower Room","m",24]
[]
[null,"J193",null,"Supply, deliver and install weatherproof Timber solid door 813(W) x 2032mm(H) including frame. Rate to include tying in of doorframe and all jointing / nosing required."," "," "]
[null,"J196",null,"Chlorine Room","No",1]
[null,"J197",null,"Control Room","No",1]
[]
[null,"J198",null,"Supply, deliver and install Internal hollow core timber door 813(W) x 2032mm(H) including frame and 300 x 300mm inspection window. Rate to include tying in of doorframe and all jointing / nosing required."]
[]
[null,"J200",null,"Guard House","No",2]
[null,"J201",null,"Control Room","No",1]
[]
[{"$nulls":3},"Total Carried Forward"]
[{"$nulls":3},"Total Brought Forward"]
[]
[null,"J202",null,"Supply, deliver and install WC cubical door including frame. Rate to include tying in of doorframe and all jointing / nosing required."]
[null,"J203",null,"Control Room","No",1]
[]
[]
[null,"J206",null,"Supply, deliver and install weatherproof double timber door and frame, 2200mm (W) x 3870mm (H) with internal panic bar to open both doors. Reliance or Brittex aluminium Panic bar, notched to accommodate crawl beam. Rate to include 2 OFF - 300 x 300 inspection windows, tying in of doorframe and all jointing / nosing required."]
[null,"J207",null,"Blower Room","No",3]
[null,"J208",null,"Chlorine Room","No",1]
[]
[null,"J215",null,"Supply, deliver and install gear operated galvanised roller shutter doors 3000 (H) x 3000mm (W), complete with all channels, guides, roller mechanisms, drive shafts, crank handles, endplates, gearbox and all fixings for a fully operational system."]
[null,"J216",null,"Dewatering plant","No",1]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"K.Roads","index":10,"n_rows":51,"n_cols":9,"rows_kept":51,"merged":[[5,7,5,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"K",null,"SECTION K: ROADWORKS"]
[null,"K1",null,"Bulk Excavation"]
[null,"K2","SANS 1200DM","Subgrade"]
[null,"K3","8.3.7","Excavate in all materials to temporary stockpile and dispose of surplus to spoil to: "," "," "]
[null,"K4",null,"Access Road","m³",700]
[]
[null,"K5"," ","Compact insitu material to 93% mod. AASHTO."]
[null,"K6",null,"Access Road","m²",860]
[]
[null,"K7","8.3.5","G7 material imported from commercial sources for the construction of 2 layers x 150mm thick Selected Sub Grade compacted to 93% mod. AASHTO"]
[null,"K8",null,"Access Road","m³",260]
[]
[null,"K9","SANS 1200ME","Subbase From Commercial Sources"]
[null,"K10","8.3.3","G5 material imported from commercial sources for the construction of 1 layer x 150mm thick Subbase compacted to 95% mod. AASHTO"]
[null,"K11",null,"Access Road","m³",130]
[]
[null,"K12","SANS 1200MFL","Base From Commercial Sources"]
[null,"K13",null,"G2 material imported from commercial sources for the construction of 1 layer x 150mm thick Base compacted to 98% mod. AASHTO"]
[null,"K14",null,"Access Road","m³",130]
[]
[null,"K15","SANS 1200MH","Bituminous Surfacing"]
[null,"K16","8.5.1","MC-30 cutback bitumen applied as prime coat, complying with the requirements of SANS 308, spray application at 0.9 l/m² applied at a maximum temperature of 80 oC."]
[null,"K17",null,"Access Road","m²",860]
[]
[null,"K18","8.5.4","35mm Premix applied to newly constructed road layers."]
[null,"K19",null,"Access Road","m²",860]
[]
[null,"K20","SANS 1200MK","Kerbing"]
[null,"K21",null,"450(W) x 75mm Thick soilcrete stabilised with 5% OPC for the bedding of kerbs"]
[null,"K22",null,"Access Road","m³",5]
[]
[null,"K23",null,"150(W) x 100mm (D) 20MPa/19mm Mass concrete placed as road edging between kerbs and wearing coarse."]
[null,"K24",null,"Access Road","m³",7]
[]
[null,"K25",null,"Supply, deliver, install and align 300 (W) x 150 (D), Fig 8, Mountable Kerbs to edge of pavement. Rate to include all jointing and backfilling against kerb upon completion of haunching."]
[null,"K26",null,"Radius up to 4m","m","RATE ONLY",null,"RATE ONLY"]
[null,"K27",null,"Radius 4m up to and including 20m","m",180]
[null,"K28",null,"Radius over 20m and straight","m",200]
[]
[null,"K29",null,"15MPa/19mm Mass concrete haunching to back face of kerbs at every joint."]
[null,"K30",null,"Access Road","m³",4]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"L. Day Works","index":11,"n_rows":67,"n_cols":9,"rows_kept":67,"merged":[[6,7,6,8]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
[{"$nulls":3},"LEPHALALE LOCAL MUNICIPALITY"]
[{"$nulls":3},"BILL OF QUANTITIES"]
[]
[]
[null,"ITEM No","PAYMENT","DESCRIPTION","UNIT","Qty","RATE","AMOUNT"]
[{"$nulls":7},"R","c"]
[null,"L",null,"Labour (including mark-up)"]
[]
[null,"L1",null,"a) Unskilled Labourer","hr",50]
[]
[null,"L2",null,"b) Semi Skilled Labourer","hr",70]
[]
[null,"L3",null,"Artisan","hr",50]
[]
[null,"L4",null,"Plumber","hr",50]
[]
[null,"L5",null,"Welder","hr",10]
[]
[null,"L6",null,"Bricklayer","hr",50]
[]
[null,"L7",null,"Carpenter","hr",50]
[]
[null,"L8",null,"Foreman : General","hr",12]
[]
[null,"L9",null,"Foreman : Concrete","hr",12]
[]
[null,"L10",null,"Foreman : Pipelaying","hr",12]
[]
[null,"L11",null,"Plant (including mark-up)"]
[{"$nulls":3},"(specify the capacity in each case)"]
[]
[null,"L12",null,"Tipper Truck"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L13",null,"Flat-bed Truck"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L14",null,"Front End loader"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L15",null,"LDV"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L16",null,"Motor Bulldozer"]
[{"$nulls":3},"..............D4.....................","hr",10]
[]
[null,"L17",null,"Motor Grader"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L18",null,"TLB"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L19",null,"Compactors"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L20",null,"Water Trailer"]
[{"$nulls":3},"...................................","hr",10]
[]
[null,"L21",null,"Materials to be used in dayworks"]
[null,"L22",null,"Materials as ordered by the Engineer","Prov",1,25000]
[{"$nulls":4},"Sum"]
[null,"L23",null,"% Mark Up Required …………………. %"]
[]
[]
[{"$nulls":3},"TOTALS CARRIED FORWARD TO SUMMARY"]

{"sheet":"Summary","index":12,"n_rows":27,"n_cols":3,"rows_kept":27,"merged":[[5,0,6,0],[5,1,6,1],[7,0,7,1]],"flags":["formulas_cached_only"]}
[]
["PAARL WASTE WATER TREATMENTWORKS PROPOSED UPGRADE"]
["LEPHALALE LOCAL MUNICIPALITY"]
["BILL OF QUANTITIES"]
[]
["Section No.","Description","Amount"]
[null,null,"R           C"]
["Summary to Schedule of Quantities"]
[]
["A","Preliminary and General"]
["B","Site Clearance "]
["C","Earthworks"]
["D","Concrete (structural)"]
["E","Pipework"]
["F","Structural Steelwork and Cladding"]
["G","Mechanical"]
["H","Instrumentation"]
["I","Miscellaneous"]
["J","Building Work"]
["K","Roads"]
["L","Dayworks"]
[]
[null,"Sub Total"]
[null,"ADD 15% VAT"]
[]
[]
[null,"Total Carried Forward to Form of Tender"]