{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["compliance to item description"],"read":"whole","date_system":"1900"}

{"sheet":"compliance to item description","index":0,"n_rows":57,"n_cols":5,"rows_kept":57}
["ANNEXURE H",null,null,"comply fully to item description"]
["I tem number","Description ","Text","yes","no"]
[61100266,"PLATE METAL;8 MM,1279 MM,3200 MM,3CR12","PLATE, METALLIC; THICKNESS: 8 MM, WIDTH: 1279 MM, LENGTH: 3200 MM, PLATE MATERIAL: STEEL BLACK, MATERIAL GRADE: 3CR12, FABRICATION"]
[null,null,"METHOD: HOT ROLLED; FOR WAGON FLOOR, CCL;"]
[null,null,"CUT TO THE TOLERANCE OF -1"]
[]
["368110266","PIPE METAL;PIPE SZ:OD 219 MM,LG:2.5 M","PIPE, METALLIC; PIPE SIZE: OD 219 MM, LENGTH: 2.5 M,"]
[null,null,"WALL THICKNESS: 6 MM,"]
[null,null,"PIPE MATERIAL: STEEL,"]
[null,null,"SURFACE TREATMENT: PAINTED,"]
[null,null,"END CONNECTION TYPE:"]
[null,null,"PLAIN; DRAWING NO: UTH655A007, A; CCL 1/3;"]
[null,null,"HANDBRAKE 3CR12"]
[]
["611000252","PLATE METAL;10 MM,2500 MM,1290 MM","PLATE, METALLIC;"]
[null,null,"THICKNESS: 10 MM,"]
[null,null,"WIDTH: 2500 MM,"]
[null,null,"LENGTH: 1290 MM,"]
[null,null,"MATERIAL GRADE: EN10088 3CR12; GENERAL:"]
[null,null,"MATERIAL CERTIFICATE TO"]
[null,null,"EN 10204 TYPE 3.1 TO BE SUPPLIED."]
[null,null,"NO RUST OR CORROSION ON THE SURFACE ALLOWED."]
[null,null,"FABRICATION METHOD: HOT ROLLED, SPECIAL FEATURES:"]
[null,null,"BLACK; FOR WAGON L & R STRENGTHENER CCL"]
[]
["914500578","PLATE METAL;4 MM,1500 MM,3300 MM","PLATE, METALLIC;"]
[null,null,"THICKNESS: 4 MM,"]
[null,null,"WIDTH: 1500 MM,"]
[null,null,"LENGTH: 3300 MM,"]
[null,null,"MATERIAL GRADE: EN 10088 3CR12;"]
[null,null,"GENERAL: MATERIAL CERTIFICATE TO"]
[null,null,"EN 10204 TYPE 3.1 TO BE SUPPLIED."]
[null,null,"NO RUST OR CORROSION ON THE SURFACE ALLOWED."]
[null,null,"FABRICATION METHOD: HOT ROLLED"]
[]
["6110000254","PLATE METAL;6 MM,1290 MM,2500 MM","PLATE, METALLIC;"]
[null,null,"THICKNESS: 6 MM,"]
[null,null,"WIDTH: 1290 MM,"]
[null,null,"LENGTH: 2500 MM,"]
[null,null,"MATERIAL GRADE: EN10088 3CR12;"]
[null,null,"GENERAL: MATERIAL CERTIFICATE TO"]
[null,null,"EN 10204 TYPE 3.1 TO BE SUPPLIED."]
[null,null,"NO RUST OR CORROSION ON THE SURFACE ALLOWED."]
[null,null,"FABRICATION METHOD: HOT ROLLED,"]
[null,null,"SPECIAL FEATURES: BLACK"]
[]
["611000257","PLATE METAL;4 MM,1500 MM,2454 MM,3CR12","PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2454 MM, PLATE MATERIAL: STEEL BLACK, MATERIAL GRADE: 3CR12, FABRICATION"]
[null,null,"METHOD: HOT ROLLED; FOR WAGON FLOOR; CCL;"]
[null,null,"PLEASE CUT TO THE TOLERANCE OF -1"]
[]
["6110000258","PLATE METAL;4 MM,1500 MM,2922 MM,3CR12","PLATE, METALLIC; THICKNESS: 4 MM, WIDTH: 1500 MM, LENGTH: 2922 MM, PLATE MATERIAL: STEEL BLACK, MATERIAL GRADE: 3CR12, FABRICATION"]
[null,null,"METHOD: HOT ROLLED; FOR WAGON FLOOR; CCL;"]
[null,null,"CUT TO THE TOLERANCE OF -1"]
[]
["6110000259","PLATE METAL;6 MM,1500 MM,3257 MM,3CR12","PLATE, METALLIC; THICKNESS: 6 MM, WIDTH: 1500 MM, LENGTH: 3257 MM, PLATE"]
[null,null,"MATERIAL: STEEL BLACK, MATERIAL GRADE: 3CR12, FABRICATION"]
[null,null,"METHOD: HOT ROLLED; CUT TO THE TOLERANCE OF -1"]