{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["SUMMARY BUILDINGS","PART H","GEN INSPECTION SHEET"],"not_rendered":{"external_links":6,"defined_names":167},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"SUMMARY BUILDINGS","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,9],[3,0,3,9],[4,0,4,9],[5,0,5,7],[6,0,6,7],[7,0,7,7],[8,0,8,7],[9,0,9,7],[10,0,10,7],[11,0,11,7],[12,0,12,7],[13,0,13,7],[14,0,14,7],[15,0,15,7],[16,0,16,7],[17,0,17,7],[18,0,18,7],[19,0,19,7],[20,0,20,7],[21,0,21,7],[22,0,22,3],[28,0,28,3],[36,0,36,7],[37,0,37,1]],"flags":["formulas_cached_only"]}
[]
[" BID RLM/DTIS/0020/2020/21 - SUMMARY\nELECTRICAL LABOUR:  ELECTRICAL INFRASTRUCTURE/CONSTRUCTION & MAINTENANCE (AS AND WHEN NEEDED)"]
[]
["WORKS ORDERS WILL BE ISSUED INDIVIDUALY AND WILL BE  BASED ON APPLICABLE UNIT RATES ONLY"]
["ALL IS TO BE RE-MEASURED PRIOR TO PAYMENT"]
[{"$nulls":8},"UNIT RATE AMOUNT (EXCL. VAT)","COMPARISON AMOUNT (EXCL. VAT)"]
["PART AA: TOTAL FOR PRELIMINARY & GENERAL ITEMS"]
["PART H: TOTAL BUILDING MAINTENANCE (LABOUR ONLY)"]
["PART H: TOTAL BUILDING CONSTRUCTION (PRICE PER SQUARE METER)"]
{"$rows_empty":10}
["SUB TOTAL "]
["ADD - 15% VAT"]
["TOTAL COMPARISON AMOUNTS ACCORDING TO BOQ"]
["UNIT RATE AMOUNT IN WORDS:"]
[]
[]
[]
[]
[]
["COMPARISON AMOUNT IN WORDS:"]
[]
[]
[]
[]
[]
[]
["                      % ANNUAL ESCALATION ON LABOUR EVERY 12 MONTHS AFTER CONTRACT COMMENCEMENT"]
[]
["SIGNATURE:",{"$nulls":4},"DATE:"]

{"sheet":"PART H","index":1,"n_rows":236,"n_cols":7,"rows_kept":236,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,9],[3,0,3,6],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[15,0,16,0],[29,0,33,0],[36,0,38,0],[43,0,45,0],[48,0,51,0],[58,1,58,3],[60,1,60,3],[61,2,62,2],[61,3,62,3],[61,4,62,4],[61,5,62,5],[61,6,62,6],[62,0,65,0],[70,0,73,0],[80,0,82,0],[90,0,92,0],[97,0,100,0],[106,0,108,0],[111,0,113,0],[119,1,119,3],[121,1,121,3],[122,2,123,2],[122,3,123,3],[122,4,123,4],[122,5,123,5],[122,6,123,6],[123,0,126,0],[134,0,136,0],[143,0,145,0],[149,0,151,0],[157,0,159,0],[162,0,165,0],[181,1,181,3],[182,1,182,3],[194,0,195,0],[194,2,195,2],[194,3,195,3],[194,4,195,4],[194,5,195,5],[194,6,195,6],[235,1,235,3]],"flags":["formulas_cached_only"]}
[" BID RLM/DTIS/0020/2020/21\nELECTRICAL LABOUR:  ELECTRICAL INFRASTRUCTURE/CONSTRUCTION & MAINTENANCE (AS AND WHEN NEEDED)"]
["PART H: BUILDING RELATED MAINTENANCE"]
["WORKS ORDERS WILL BE ISSUED INDIVIDUALY AND WILL BE  BASED ON APPLICABLE UNIT RATES ONLY"]
[" ALL IS TO BE RE-MEASURED PRIOR TO PAYMENT"]
["ITEM","DESCRIPTION","Unit","Each","Unit Rate  Labour ","Evaluation Quantity","Evaluation Total"]
[1,"INFRASTRUCTURE RELATED MAINTENANCE"]
[null,"Supply, delivery to site, installation and testing and commissioning of the following equipment."]
[]
[null,"Please note that the cost for material / equipment will not be remunerated "]
[null,"seperartely and must be included in the final price per item as below."]
[null,"Remuneration for all lifting and excavation equipment is to be included in "]
[null,"the labour rate."]
[null,"Travelling to and from site will be based on rates as per the day works rates "]
[null,"section"]
[]
[1.1,"Distribution Board Equipment"]
[null,"Delivery to site / Collect from RLM stores / remove / installation of the following distribution board equipment complete including labelling etc."]
["1.1.1","Single Phase Small frame MCCB’s – 2.5 to 10kA","No",1,null,10]
["1.1.2","Single Phase Earth Leakage Relay – 2.5 – 5kA","No",1,null,10]
["1.1.3","Three Phase Small frame MCCB’s – 2.5 to 10kA","No",1,null,10]
["1.1.4","Three Phase Earth Leakage Relay – 2.5 to 5kA","No",1,null,10]
["1.1.5","Medium frame 3 phase MCCB’s – 15 to 25kA","No",1,null,10]
["1.1.6","3 Phase Contactor – up to 100A rating","No",1,null,10]
["1.1.7","24hr timer","No",1,null,10]
["1.1.8","Indoor surge arrestor – 1.5 to 5kA","No",1,null,10]
["1.1.9","Photocell","No",1,null,10]
["1.1.10","Install DB Board (Flush / surface) Up to 12 Module","No",1,null,10]
["1.1.11","Install DB Board (Flush / surface) 13 to 24 Module","No",1,null,10]
["1.1.12","Install DB Board (Flush / surface) 25 to 36 Module","No",1,null,10]
[1.2,"Conduit"]
[null,"Delivery to site / Collect from RLM stores / remove / installation of the "]
[null,"following conduit  cast into concrete, build or chased into brickwork "]
[null,"including chasing or in ceiling voids complete with (couplings, saddles etc., "]
[null,"1.6mm draw wire supply & install)"]
["1.2.1","20-25mm dia","m",1,null,10]
["1.2.2","32 - 50mm dia","m",1,null,10]
[1.3,"Galvanized Draw boxes"]
[null,"Delivery to site / Collect from RLM stores / remove / installation of "]
[null,"galvanized outlet boxes cast into concrete or build/chased into brickwork"]
["1.3.1","100mm x 50mm x 50mm","No",1,null,10]
["1.3.2","100mm x 100mm x 50mm","No",1,null,10]
["1.3.3","150mm x 150mm x 100mm","No",1,null,10]
["1.3.4","60mm round","No",1,null,10]
[1.4,"Surface Extension Box"]
[null,"Delivery to site and installation of the following steel surface"]
[null,"mounted extension boxes complete"]
["1.4.1","100mm x 50mm x 50mm","No",1,null,10]
["1.4.2","100mm x 100mm x 50mm","No",1,null,10]
[1.5,"Wire Trunking & Cable Tray"]
[null,"Delivery to site / Collect from RLM stores / remove / installation of "]
[null,"galvanized steel wire trunking / medium duty cable tray complete including "]
[null,"bends, tees, knockouts, hangers etc."]
["1.5.1","O-Line PT38 Cable Tray (76 to 152mm)","m",1,null,10]
["1.5.2","O-Line PT38 Cable Tray (228 to 304mm)","m",1,null,10]
["1.5.3","O-Line PT38 Cable Tray (457 to 609mm)","m",1,null,10]
["1.5.4","O-Line OL8000 wiring channel","m",1,null,10]
["1.5.5","O-Line OL9000 wiring channel","m",1,null,10]
["1.5.6","PVC Ega Ducting (All sizes)","m",1,null,10]
[null,"TOTAL CARRIED FORWARD"]
[]
[null,"TOTAL BROUGHT FORWARD - PART H"]
["ITEM","DESCRIPTION","Unit","Each","Unit Rate  Labour ","Evaluation Quantity","Evaluation Total"]
[1.6,"Power skirting"]
[null,"Delivery to site / Collect from RLM stores / remove / installation of the "]
[null," following multi compartment power skirting in accordance with the "]
[null,"specification complete  including cover plates and the fixing thereof"]
["1.6.1","1-3 Compartment Power skirting","m",1,null,10]
["1.6.2","External elbow ","No",1,null,10]
["1.6.3","Internal elbow","No",1,null,10]
["1.6.4","End cap","No",1,null,10]
[1.7,"Copper Conductors"]
[null,"Delivery to site and installation of 600/1000V grade PVC insulated stranded"]
[null,"copper conductors drawn into conduits or power skirting including the"]
[null,"removal of existing wiring where applicable"]
["1.7.1","1.5mm sq.","m",1,null,100]
["1.7.2","2.5mm sq.","m",1,null,100]
["1.7.3","4.0mm sq.","m",1,null,100]
["1.7.4","6.0mm sq.","m",1,null,100]
["1.7.5","10.0mm sq.","m",1,null,100]
["1.7.6","16mm sq.","m",1,null,100]
[1.8,"Bare Copper Earth Wire"]
[null,"Deliver to site and installation of the following earth wire installed in the ground, sleeves or in cable trunking"]
[null,"LABOUR RATE"]
["1.8.1","16mm sq. BCEW","m",1,null,100]
["1.8.2","10mm sq. BCEW","m",11,null,100]
["1.8.3","6mm sq. BCEW","m",1,null,100]
["1.8.4","4mm sq. BCEW","m",1,null,100]
["1.8.5","2.5mm sq. BCEW","m",1,null,100]
["1.8.6","1.5mm sq. BCEW","m",1,null,100]
["1.8.7","Surfix (All sizes)","m",1,null,100]
[1.9,"Light switches"]
[null,"Delivery to site / Collection from RLM stores / remove / installation of"]
[null,"16A light switches mounted in conduit boxes complete with cover plates "]
["1.9.1","Single lever one way","No",1,null,10]
["1.9.2","Single lever two way","No",1,null,10]
["1.9.3","Two lever one way","No",1,null,10]
["1.9.4","Three lever one way","No",1,null,10]
[{"v":1.1,"d":"1.10"},"Switched Socket Outlets"]
[null,"Delivery to site / Collection from RLM stores / remove / installation of"]
[null,"16A 3 pin switched socket outlets with cover plates"]
[null,"Switched socket outlets mounted in outlet boxes / power skirting / pedestals"]
["1.10.1","Single 16A 3 pin","No",1,null,10]
["1.10.2","Double 16A 3 pin","No",1,null,10]
["1.10.3","Single watertight","No",1,null,10]
["1.10.4","Single 16A flat pin dedicated ","No",1,null,10]
["1.10.5","Double 16A flat pin dedicated ","No",1,null,10]
[1.11,"Isolators"]
[null,"Delivery to site / Collection from RLM stores / remove / installation of the "]
[null,"following isolators mounted in extension boxes complete "]
["1.11.1","30A 2P isolator","No",1,null,10]
["1.11.2","30A 4P isolator","No",1,null,10]
[1.12,"Luminaires"]
[null,"Delivery to site / Collection from RLM stores / remove / installation of the "]
[null,"following luminaires and fixing including"]
["1.12.1","Wall / Ceiling mounted / bulkhead / pendant luminaire","No",1,null,10]
["1.12.2","Recessed low voltage down lighter / PL down lighter","No",1,null,10]
["1.12.3","Surface / Recessed / open / close channel up to -1200mm fluorescent","No",1,null,10]
["1.12.4","Surface / Recessed/  open / close channel 1500mm to 1800mm fluorescent","No",1,null,10]
["1.12.5","Wall mounted floodlight","No",1,null,10]
[null,"TOTAL CARRIED FORWARD"]
[]
[null,"TOTAL BROUGHT FORWARD - PART H"]
["ITEM","DESCRIPTION","Unit","Each","Unit Rate  Labour ","Evaluation Quantity","Evaluation Total"]
[1.13,"Luminaires"]
[null,"Group replacement suitable to house Energy Efficiency LED type tubes"]
[null,"Delivery to site / Collection from RLM stores / remove old and install new "]
[null,"following luminaires and fixing including"]
["1.13.1","Surface / Recessed / open / close channel up to -1200mm fluorescent fitting ","units",1,null,10]
["1.13.2","Surface / Recessed / open / close channel 1500mm to 1800mm fluorescent fitting ","units",1,null,10]
["1.13.3","Re-wire (where necessary) of fluorescent fittings ","units",1,null,10]
["1.13.4","Attach all required labelling to conform to latest SABS standards to fluorescent fittings","units",1,null,10]
["1.13.5","Wall mounted floodlight fitting ","units",1,null,10]
["1.13.5b","Pole mounted floodlight fitting "]
["1.13.6","High Bay type light fitting ","units",1,null,10]
[1.14,"Replacement of Lamps / Globes"]
[null,"Delivery to site / Collection from RLM stores / remove old and installation "]
[null,"of the following new lamps to luminaires"]
["1.14.1","Up to 100W incandescent  / LED Replacement","No",1,null,10]
["1.14.2","Up to 36W Compact Fluorescent","No",1,null,10]
["1.14.3","50W 12V Dicroid","No",1,null,10]
["1.14.4","18W Fluorescent  / LED Replacement","No",1,null,10]
["1.14.5","36W Fluorescent  / LED Replacement","No",1,null,10]
["1.14.6","58W Fluorescent  / LED Replacement","No",1,null,10]
["1.14.7","Safe dispposal of bulbs / globes"]
[null,"Collection from site / Collection from RLM stores / and deliver to a duly"]
[null,"certified service profider that comply with all the stipulations set out:"]
[null,"A CERTIFICATE MUST BE ISSUED THAT SERVES TO CONFIRM THAT THE LAMP TYPES AND QUANTITIES AS SPESIFIED HEREUNDER HAVE BEEN CRUSHED, CONCEALED AND REMOVED FROM THE ABOVE SITE BY THE CRUSH TEAM IN ACCORDANCE WITH THE PROVISIONS OF THE ENVIROMENTAL CONSERVATION ACT NO. 73 1989, NATIONAL ENVIRONMENTAL MANAGEMENT ACT NO. 107 OF 1998, THE NATIONAL WATER ACT NO. 36 OF 1998, THE HEALTH ACT NO. 63 OF 1997, THE OCCUPATIONAL HEALTH AND SAFETY ACT NO. 85 OF 1993, THE NATIONAL TRAFFIC ACT NO. 93 OF 1996 AND TRANSPORTATION OF DANGEROUS SUBSTANCES BY ROAD – CHAPTER 8 OF THE NATIONAL ROAD ACT."]
["1.14.7.1","1 - 1000 Incandescent / down lighter bulbs - collection included","No",1,null,10]
["1.14.7.2","1 - 1000 fluerescent tubes / CFL bulbs - collection included","No",1,null,10]
[1.15,"Replacement of parts of luminaires"]
[null,"Delivery to site / Collection from RLM stores / remove old and installation "]
[null,"of the following equipment (testing of equipment included)"]
["1.15.1","60 / 100W incandescent lamp holders","No",1,null,10]
["1.15.2","Transformer for a 50W Dicroid lamp","No",1,null,10]
["1.15.3","Fluorescent ballast (36 and 58W)","No",1,null,10]
["1.15.4","Fluorescent starter (36 and 58W)","No",1,null,10]
["1.15.5","Fluorescent lamp holder","No",1,null,10]
[1.16,"Geysers"]
[null,"Delivery to site / Collection from RLM stores / remove old and installation "]
[null,"of the following equipment (testing of equipment included)"]
["1.16.1","Geyser element on all domestic geysers - 50 to 350 litres","No",1,null,10]
["1.16.2","Replacement of a thermostat on a geyser","No",1,null,10]
[1.17,"Generators"]
[null,"PREVENTATIVE MAINTENANCE: Monthly"]
[null,"Price to include traveling to and from various Generators Set locations "]
[null,"Monthly Generator maintenance as per attached Inspection Sheet. "]
[null,"The price must include the cost for investigation of a fault/problem and the "]
[null,"compiling and submission of a quotation if required in any extension in RTB"]
[null,"Any mechanical repairs to be done by Suitably qualified diesel mechanic "]
[null,"with applicable experience on Generators. "]
[null,"Attach a comprehensive Curriculum Vitae of mechanic (failure to adhere to "]
[null,"this requirement will disqualify the tenderer)"]
["1.17.1","Generator situated at: Civic Centre","Month",1,null,36]
["1.17.2","Generator situated at: Olympia Park","Month",1,null,36]
["1.17.3","Generator situated at: Mpheni House","Month",1,null,36]
["1.17.4","Generator situated at: Fire Brigade","Month",1,null,36]
["1.17.5","Generator situated at: Electrical Workshop","Month",1,null,36]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[null,"TOTAL BROUGHT FORWARD - PART H"]
[]
[2,"BUILDING INFRASTRUCTURE RELATED MAINTENANCE"]
[null,"Supply, delivery to site, construction, maintenance of the following equipment."]
[null,"ALL MATERIAL TO BE APPROVED PRIOR TO COMMENCEMENT OF WORK"]
[null,"Please note that the cost for material / equipment will not be remunerated "]
[null,"seperartely and must be include in the final price per square meter as below."]
[null,"Remuneration for all lifting and excavation equipment is to be included in "]
[null,"the labour rate."]
[null,"Travelling to and from site will be based on rates as per the day works rates "]
[null,"section"]
[]
[2.1,"DESCRIPTION","Unit","Each","Unit Rate  Labour ","Evaluation Quantity","Evaluation Total"]
[]
["2.1.1","Building Construction - Works - ONLY APPLICABLE TO SUBSTATIONS"]
["2.1.2","PRICE PER SQUARE METER/ CUBIC METER - ALL MATERIAL INCLUDED"]
["3.1.3","Concrete per cubic meter - foundations","Cubic m"]
["2.1.3","Concrete per square meter - floors","m2"]
["2.1.4","Building per square meter Single wall - 55 Bricks -  face brick","m2"]
["3.1.4","Building per square meter Single wall - 110 Bricks - Face brick","m2"]
["2.1.5","Building per square meter Single wall - 55 Bricks -  plaster brick","m2"]
["2.1.6","Building per square meter Single wall - 110 Bricks - plaster brick","m2"]
["3.1.5","Plastering per square meter - Walls","m2"]
["2.1.7","Ceilings per square meter complete with cornish","m2"]
["2.1.8","Installation of steel substation doors - Single","Each "]
["3.1.6","Installation of steel substation doors - Double","Each "]
["2.1.9","Paving per square meter around substations - including bedding","Each "]
["2.1.10","Demolishing and break up of concrete per square meter ","m2"]
["2.1.11","Removal and dumping of demolished concrete per square meter ","m2"]
["2.1.12","2.5 meter Clearvu fencing per running meter - Poles etc included.","m"]
["2.1.13","2.5 meter Clearvu fencing gate per running meter - Poles etc included.","m"]
["2.1.14","Painting of steel doors and sills per square meter - as per spec for steel","m2"]
["2.1.15","Painting of plastered walls per square meter - as per spec for for substations","m2"]
["2.1.16","Painting of concrete floor per square meter - as per spec for floors","m2"]
["2.1.17","Painting of roof per square meter - as per spec for steel roofs","m2"]
["2.1.18","Intallation of Concrete tile roof at 26 degrees - per sguare meter based on substation floor area with relevant trussers.","m2"]
["2.1.19","Intallation of Concrete tile roof at 26 degrees - per sguare meter based on substation floor area with relevant trussers. Lowest point 2.4 meter above floor.","m2"]
["2.1.20","Intallation of steel roof at 10 degrees - per sguare meter based on substation floor area with steel trussers. Lowest point 2.4 meter above floor.","m2"]
["2.1.21","Site rehabilitation per ton","Ton"]
[]
["2.1.22","Complete budget price for a 60m2 substation with 26 degree tile roof as per specification.","Total Cost"]
{"$rows_empty":7}
[null,"MARK UP ON UNDEFINED ITEMS TO FINALIZE THE WORK"]
[null,"PROVEN COST PLUS 15% MARK UP"]
[null,"BIDDER SIGNATURE: ________________________________________"]
[]
[null,"DATE:                         ________________________________________"]
[null,"PART H: TOTAL CARRIED FORWARD TO SUMMARY"]

{"sheet":"GEN INSPECTION SHEET","index":2,"n_rows":44,"n_cols":12,"rows_kept":44,"merged":[[0,0,0,9],[1,0,1,9],[2,0,2,9],[3,0,3,9],[4,0,4,9],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[13,3,13,4],[13,8,13,9],[13,11,13,12],[44,0,44,9],[45,0,45,9],[46,0,46,9],[47,0,47,9],[48,0,48,9],[49,0,49,9],[50,0,50,9],[51,0,51,9],[52,0,52,9],[53,0,53,9],[54,0,54,9],[55,0,55,9]],"flags":["formulas_cached_only"]}
[" BID RLM/DTIS/0020/2020/21\nELECTRICAL LABOUR:  ELECTRICAL INFRASTRUCTURE/CONSTRUCTION & MAINTENANCE\n (AS AND WHEN NEEDED)"]
["PART H: BUILDING RELATED MAINTENANCE"]
["ALL IS TO BE RE-MEASURED PRIOR TO PAYMENT"]
[]
["Generator maintenance as per attached check list (price is for monthly inspection per generator set each)"]
["Date:",{"$nulls":4},"Customer:"]
["Site:",{"$nulls":4},"Order No:"]
[]
["Engine Type:"]
["Engine OEM:"]
["Engine Model:"]
["Machine serial No.:"]
[]
[{"$nulls":3},"Checks",{"$nulls":4},"Checks",null,null,"Abnormal"]
[{"$nulls":3},"Normal","Abnormal",{"$nulls":3},"Normal","Abnormal"]
["Air Inlet Inspection",{"$nulls":4},"Turbo Charger Condition"]
["Air Filter",{"$nulls":4},"Crankcase Breather"]
["Oil Filter",{"$nulls":4},"Canopy/Plant room Condition"]
["Oil Leak",{"$nulls":4},"Check all Electrical Connection"]
["Oil Level",{"$nulls":4},"Check Panel Clean"]
["Fuel Filter - Prim/Sec",{"$nulls":4},"Check all Electrical Connections on motor"]
["Fuel Leak",{"$nulls":4},"Check that all Batteries are Connected"]
["Fuel Water Trap",{"$nulls":4},"Check that main contactor is energised"]
["Fuel Hoses",{"$nulls":4},"Check Battery charger:  charging voltage at batteries"]
["Radiator/Heat Exchanger",{"$nulls":4},"Check Electrical Fuel pump operating"]
["Coolant Level",{"$nulls":4},"Check if water jacket heater"]
["Jacket Water Heater \"ON\"",{"$nulls":4},"Check if lights working from gen made + main cell"]
["JWH Hoses (Replace Annually)",{"$nulls":4},"Controller on Auto"]
["Fan Belt Tension/Condition"]
["Fan Driver Pulley & Fan",{"$nulls":4},"ENGINE RUN/CHECKS"]
["Battery Condition",{"$nulls":4},"Simulate Low Oil Pressure"]
["Battery Electrolyte Level",{"$nulls":4},"Simulate High Engine Temperature"]
["Water Pump Condition",{"$nulls":4},"Simulate Low Water Level"]
[{"$nulls":5},"Simulate Low Fuel"]
[{"$nulls":5},"Check Charging Alternator"]
[]
[{"$nulls":5},"RECORD"]
[{"$nulls":5},"Battery Voltage"]
[{"$nulls":5},"Battery Voltage Drop"]
[{"$nulls":5},"Charging Current"]
[{"$nulls":5},"Max Demand Amps ",null,"R -","W -","B -"]
[{"$nulls":5},"Hour meter"]
[]
["Remarks:"]